<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<board>
<plain>
<text>8-bit Data
LED Bkout</text>
<text>8-bit Data
LED Bkout
Berzerkula.org</text>
<wire x1="3.81" y1="12.7" x2="3.81" y2="2.54" width="0" layer="20"/>
<wire x1="3.81" y1="2.54" x2="5.08" y2="1.27" width="0" layer="20" curve="90"/>
<wire x1="5.08" y1="1.27" x2="22.86" y2="1.27" width="0" layer="20"/>
<wire x1="22.86" y1="1.27" x2="24.13" y2="2.54" width="0" layer="20" curve="90"/>
<wire x1="24.13" y1="2.54" x2="24.13" y2="12.7" width="0" layer="20"/>
<wire x1="24.13" y1="12.7" x2="22.86" y2="13.97" width="0" layer="20" curve="90"/>
<wire x1="22.86" y1="13.97" x2="5.08" y2="13.97" width="0" layer="20"/>
<wire x1="5.08" y1="13.97" x2="3.81" y2="12.7" width="0" layer="20" curve="90"/>
<text>K</text>
<text>K</text>
<text>C.C.</text>
</plain>
<libraries>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1X01">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="led">
<description>&lt;b&gt;LEDs&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;br&gt;
Extended by Federico Battaglin &lt;author&gt;&amp;lt;federico.rd@fdpinternational.com&amp;gt;&lt;/author&gt; with DUOLED</description>
<packages>
<package name="CHIPLED_1206">
<description>&lt;b&gt;CHIPLED&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LG_LY N971.pdf</description>
</package>
</packages>
</library>
<library name="Resistor Array">
<description>&lt;h3&gt; PCBLayout.com - Frequently Used &lt;i&gt;Resistor Array&lt;/i&gt;&lt;/h3&gt;

Visit us at &lt;a href="http://www.PCBLayout.com"&gt;PCBLayout.com&lt;/a&gt; for quick and hassle-free PCB Layout/Manufacturing ordering experience.
&lt;BR&gt;
&lt;BR&gt;
This library has been generated by our experienced pcb layout engineers using current IPC and/or industry standards. We &lt;b&gt;believe&lt;/b&gt; the content to be accurate, complete and current. But, this content is provided as a courtesy and &lt;u&gt;user assumes all risk and responsiblity of it's usage&lt;/u&gt;.
&lt;BR&gt;
&lt;BR&gt;
Feel free to contact us at &lt;a href="mailto:Support@PCBLayout.com"&gt;Support@PCBLayout.com&lt;/a&gt; if you have any questions/concerns regarding any of our content or services.</description>
<packages>
<package name="EXB-E10C103J">
<description>10-Chiparray 4-Side Flat, 0.80 mm pitch, 4.00 X 2.10 X 0.55 mm body
&lt;p&gt;10-pin Chiparray 4-Side Flat package with 0.80 mm pitch with body size 4.00 X 2.10 X 0.55 mm&lt;/p&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="NEG1" library="pinhead" package="1X01" value="">
<attribute name="POPULARITY" value="64"/>
<attribute name="VALUE"/>
</element>
<element name="NEG2" library="pinhead" package="1X01" value="">
<attribute name="POPULARITY" value="64"/>
<attribute name="VALUE"/>
</element>
<element name="D7" library="pinhead" package="1X01" value="">
<attribute name="POPULARITY" value="64"/>
<attribute name="VALUE"/>
</element>
<element name="D6" library="pinhead" package="1X01" value="">
<attribute name="POPULARITY" value="64"/>
<attribute name="VALUE"/>
</element>
<element name="D5" library="pinhead" package="1X01" value="">
<attribute name="POPULARITY" value="64"/>
<attribute name="VALUE"/>
</element>
<element name="D4" library="pinhead" package="1X01" value="">
<attribute name="POPULARITY" value="64"/>
<attribute name="VALUE"/>
</element>
<element name="D3" library="pinhead" package="1X01" value="">
<attribute name="POPULARITY" value="64"/>
<attribute name="VALUE"/>
</element>
<element name="D2" library="pinhead" package="1X01" value="">
<attribute name="POPULARITY" value="64"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="pinhead" package="1X01" value="">
<attribute name="POPULARITY" value="64"/>
<attribute name="VALUE"/>
</element>
<element name="D0" library="pinhead" package="1X01" value="">
<attribute name="POPULARITY" value="64"/>
<attribute name="VALUE"/>
</element>
<element name="LED1" library="led" package="CHIPLED_1206" value="">
<attribute name="POPULARITY" value="28"/>
<attribute name="VALUE"/>
</element>
<element name="LED2" library="led" package="CHIPLED_1206" value="">
<attribute name="POPULARITY" value="28"/>
<attribute name="VALUE"/>
</element>
<element name="LED3" library="led" package="CHIPLED_1206" value="">
<attribute name="POPULARITY" value="28"/>
<attribute name="VALUE"/>
</element>
<element name="LED4" library="led" package="CHIPLED_1206" value="">
<attribute name="POPULARITY" value="28"/>
<attribute name="VALUE"/>
</element>
<element name="LED5" library="led" package="CHIPLED_1206" value="">
<attribute name="POPULARITY" value="28"/>
<attribute name="VALUE"/>
</element>
<element name="LED6" library="led" package="CHIPLED_1206" value="">
<attribute name="POPULARITY" value="28"/>
<attribute name="VALUE"/>
</element>
<element name="LED7" library="led" package="CHIPLED_1206" value="">
<attribute name="POPULARITY" value="28"/>
<attribute name="VALUE"/>
</element>
<element name="LED8" library="led" package="CHIPLED_1206" value="">
<attribute name="POPULARITY" value="28"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="Resistor Array" package="EXB-E10C103J" value="EXB-E10C103J">
<attribute name="CREATED_BY" value="PCBLayout.com"/>
<attribute name="DIGIKEY_PARTNO" value="U8103TR-ND"/>
<attribute name="MANUFACTURER" value="Panasonic Electronic Components"/>
<attribute name="MPN" value="EXB-E10C103J"/>
<attribute name="PACKAGE" value="1608"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="NEG1" pad="1"/>
<contactref element="NEG2" pad="1"/>
<contactref element="R1" pad="6"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="D7">
<contactref element="D7" pad="1"/>
<contactref element="LED8" pad="A"/>
</signal>
<signal name="D6">
<contactref element="D6" pad="1"/>
<contactref element="LED7" pad="A"/>
</signal>
<signal name="D5">
<contactref element="D5" pad="1"/>
<contactref element="LED6" pad="A"/>
</signal>
<signal name="D4">
<contactref element="D4" pad="1"/>
<contactref element="LED5" pad="A"/>
</signal>
<signal name="D3">
<contactref element="D3" pad="1"/>
<contactref element="LED4" pad="A"/>
</signal>
<signal name="D2">
<contactref element="D2" pad="1"/>
<contactref element="LED3" pad="A"/>
</signal>
<signal name="D1">
<contactref element="D1" pad="1"/>
<contactref element="LED2" pad="A"/>
</signal>
<signal name="D0">
<contactref element="D0" pad="1"/>
<contactref element="LED1" pad="A"/>
</signal>
<signal name="N$1">
<contactref element="LED1" pad="C"/>
<contactref element="R1" pad="10"/>
</signal>
<signal name="N$2">
<contactref element="LED2" pad="C"/>
<contactref element="R1" pad="9"/>
</signal>
<signal name="N$3">
<contactref element="LED3" pad="C"/>
<contactref element="R1" pad="8"/>
</signal>
<signal name="N$4">
<contactref element="LED4" pad="C"/>
<contactref element="R1" pad="7"/>
</signal>
<signal name="N$5">
<contactref element="LED5" pad="C"/>
<contactref element="R1" pad="5"/>
</signal>
<signal name="N$6">
<contactref element="LED6" pad="C"/>
<contactref element="R1" pad="4"/>
</signal>
<signal name="N$7">
<contactref element="LED7" pad="C"/>
<contactref element="R1" pad="3"/>
</signal>
<signal name="N$8">
<contactref element="LED8" pad="C"/>
<contactref element="R1" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
