<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<board>
<plain>
<wire x1="4.064" y1="22.098" x2="23.876" y2="22.098" width="0" layer="20"/>
<wire x1="23.876" y1="22.098" x2="26.416" y2="19.558" width="0" layer="20" curve="-90"/>
<wire x1="26.416" y1="19.558" x2="26.416" y2="1.27" width="0" layer="20"/>
<wire x1="26.416" y1="1.27" x2="23.876" y2="-1.27" width="0" layer="20" curve="-90"/>
<wire x1="23.876" y1="-1.27" x2="4.064" y2="-1.27" width="0" layer="20"/>
<wire x1="4.064" y1="-1.27" x2="1.524" y2="1.27" width="0" layer="20" curve="-90"/>
<wire x1="1.524" y1="1.27" x2="1.524" y2="19.558" width="0" layer="20"/>
<wire x1="1.524" y1="19.558" x2="4.064" y2="22.098" width="0" layer="20" curve="-90"/>
<text>A</text>
<text>B</text>
<text>C</text>
<text>D</text>
<text>E</text>
<text>F</text>
<text>G</text>
<text>DP</text>
<text>D1</text>
<text>D2</text>
<text>BERZERKULA ORG</text>
<text>7-Segment Breakout</text>
<text>BERZERKULA ORG</text>
<text>7-Segment Breakout</text>
</plain>
<libraries>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1X01">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="display-kingbright">
<description>&lt;b&gt;KINGBRIGHT Numeric Displays&lt;/b&gt;&lt;p&gt;
&lt;author&gt;librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DA56">
<description>&lt;b&gt;14.22mm (0.56INCH) DUAL DIGIT NUMERIC DISPLAYS&lt;/b&gt;&lt;p&gt;
Source: DA56-11SRWA.pdf</description>
</package>
</packages>
</library>
<library name="Resistor Array">
<description>&lt;h3&gt; PCBLayout.com - Frequently Used &lt;i&gt;Resistor Array&lt;/i&gt;&lt;/h3&gt;

Visit us at &lt;a href="http://www.PCBLayout.com"&gt;PCBLayout.com&lt;/a&gt; for quick and hassle-free PCB Layout/Manufacturing ordering experience.
&lt;BR&gt;
&lt;BR&gt;
This library has been generated by our experienced pcb layout engineers using current IPC and/or industry standards. We &lt;b&gt;believe&lt;/b&gt; the content to be accurate, complete and current. But, this content is provided as a courtesy and &lt;u&gt;user assumes all risk and responsiblity of it's usage&lt;/u&gt;.
&lt;BR&gt;
&lt;BR&gt;
Feel free to contact us at &lt;a href="mailto:Support@PCBLayout.com"&gt;Support@PCBLayout.com&lt;/a&gt; if you have any questions/concerns regarding any of our content or services.</description>
<packages>
<package name="EXB-2HV330JV">
<description>16-Chiparray 2-Side Convex, 0.50 mm pitch, 3.80 X 1.60 X 0.45 mm body
&lt;p&gt;16-pin Chiparray 2-Side Convex package with 0.50 mm pitch with body size 3.80 X 1.60 X 0.45 mm&lt;/p&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="JP1" library="pinhead" package="1X01" value="D1">
<attribute name="POPULARITY" value="64"/>
</element>
<element name="JP2" library="pinhead" package="1X01" value="D2">
<attribute name="POPULARITY" value="64"/>
</element>
<element name="LED1" library="display-kingbright" package="DA56" value="DC56-11SRWA">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</element>
<element name="R1" library="Resistor Array" package="EXB-2HV330JV" value="EXB-2HV330JV">
<attribute name="CREATED_BY" value="PCBLayout.com"/>
<attribute name="DIGIKEY_PARTNO" value="Y1330TR-ND"/>
<attribute name="MANUFACTURER" value="Panasonic Electronic Components"/>
<attribute name="MPN" value="EXB-2HV330JV"/>
<attribute name="PACKAGE" value="1506"/>
</element>
<element name="A" library="pinhead" package="1X01" value="">
<attribute name="POPULARITY" value="64"/>
<attribute name="VALUE"/>
</element>
<element name="B" library="pinhead" package="1X01" value="">
<attribute name="POPULARITY" value="64"/>
<attribute name="VALUE"/>
</element>
<element name="C" library="pinhead" package="1X01" value="">
<attribute name="POPULARITY" value="64"/>
<attribute name="VALUE"/>
</element>
<element name="D" library="pinhead" package="1X01" value="">
<attribute name="POPULARITY" value="64"/>
<attribute name="VALUE"/>
</element>
<element name="E" library="pinhead" package="1X01" value="">
<attribute name="POPULARITY" value="64"/>
<attribute name="VALUE"/>
</element>
<element name="F" library="pinhead" package="1X01" value="">
<attribute name="POPULARITY" value="64"/>
<attribute name="VALUE"/>
</element>
<element name="G" library="pinhead" package="1X01" value="">
<attribute name="POPULARITY" value="64"/>
<attribute name="VALUE"/>
</element>
<element name="DP" library="pinhead" package="1X01" value="">
<attribute name="POPULARITY" value="64"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="A">
<contactref element="R1" pad="1"/>
<contactref element="A" pad="1"/>
</signal>
<signal name="B">
<contactref element="R1" pad="2"/>
<contactref element="B" pad="1"/>
</signal>
<signal name="C">
<contactref element="R1" pad="3"/>
<contactref element="C" pad="1"/>
</signal>
<signal name="D">
<contactref element="R1" pad="4"/>
<contactref element="D" pad="1"/>
</signal>
<signal name="E">
<contactref element="R1" pad="5"/>
<contactref element="E" pad="1"/>
</signal>
<signal name="F">
<contactref element="R1" pad="6"/>
<contactref element="F" pad="1"/>
</signal>
<signal name="G">
<contactref element="R1" pad="7"/>
<contactref element="G" pad="1"/>
</signal>
<signal name="DP">
<contactref element="R1" pad="8"/>
<contactref element="DP" pad="1"/>
</signal>
<signal name="D1">
<contactref element="JP1" pad="1"/>
<contactref element="LED1" pad="14"/>
</signal>
<signal name="D2">
<contactref element="JP2" pad="1"/>
<contactref element="LED1" pad="13"/>
</signal>
<signal name="N$1">
<contactref element="LED1" pad="16"/>
<contactref element="R1" pad="16"/>
<contactref element="LED1" pad="11"/>
</signal>
<signal name="N$2">
<contactref element="LED1" pad="15"/>
<contactref element="R1" pad="15"/>
<contactref element="LED1" pad="10"/>
</signal>
<signal name="N$3">
<contactref element="LED1" pad="3"/>
<contactref element="R1" pad="14"/>
<contactref element="LED1" pad="8"/>
</signal>
<signal name="N$4">
<contactref element="LED1" pad="2"/>
<contactref element="R1" pad="13"/>
<contactref element="LED1" pad="6"/>
</signal>
<signal name="N$5">
<contactref element="LED1" pad="1"/>
<contactref element="R1" pad="12"/>
<contactref element="LED1" pad="5"/>
</signal>
<signal name="N$6">
<contactref element="LED1" pad="18"/>
<contactref element="R1" pad="11"/>
<contactref element="LED1" pad="12"/>
</signal>
<signal name="N$7">
<contactref element="LED1" pad="17"/>
<contactref element="R1" pad="10"/>
<contactref element="LED1" pad="7"/>
</signal>
<signal name="N$8">
<contactref element="LED1" pad="4"/>
<contactref element="R1" pad="9"/>
<contactref element="LED1" pad="9"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
