<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.1">
<drawing>
<library>
<description>Developed by element14 :&lt;br&gt;
element14 CAD Library consolidation.ulp
at 30/07/2012 12:23:11</description>
<packages>
<package name="DIP254P762X508-20">
</package>
<package name="SOIC127P1032X264-20N">
</package>
<package name="SOP65P640X110-20N">
</package>
<package name="DIP254P1524X483-28">
</package>
<package name="PLCC127P1245X1245X457-28N">
</package>
<package name="SOP65P640X110-24N">
</package>
<package name="QFP50P2200X2200X160-129N">
</package>
<package name="DIP254P1524X533-40">
</package>
<package name="SOT95P284X122-6N">
</package>
<package name="SOT95P285X120-6N">
</package>
<package name="DFN250X220X80-7N">
</package>
<package name="SOP65P490X109-8N">
</package>
<package name="SOP65P490X110-8N">
</package>
<package name="DIP254P762X508-8">
</package>
<package name="SOIC127P1032X264-14N">
</package>
<package name="DIP254P762X457-24">
</package>
<package name="SOP50P490X110-10N">
</package>
<package name="SOP50P490X109-10N">
</package>
<package name="SOIC127P600X175-8N">
</package>
<package name="SOIC127P620X175-8N">
</package>
<package name="SOP65P640X110-16N">
</package>
<package name="SOIC127P1030X265-28N">
</package>
<package name="SOP65P640X110-28N">
</package>
<package name="SOIC127P1032X265-24N">
</package>
<package name="SOIC127P1032X265-28N">
</package>
<package name="DFN220X250X80-7N">
</package>
<package name="SOP127P1032X265-24N">
</package>
<package name="QFP50P700X700X120-48N">
</package>
<package name="QFP50P900X900X120-48N">
</package>
<package name="BGA376C20X20127PX127P_279X279X">
</package>
<package name="QFP80P900X900X160-32N">
</package>
<package name="PLCC127P1753X1753X457-44N">
</package>
<package name="QFP80P1320X1320X245-44N">
</package>
<package name="SOIC127P1030X265-16N">
</package>
<package name="SOP65P770X200-28N">
</package>
<package name="SOT95P285X100-6N">
</package>
<package name="SOP65P640X110-14N">
</package>
<package name="QFN50P500X500X80-33N">
</package>
<package name="QFP50P1200DX1200X120-64N">
</package>
<package name="QFP50P1200X1200X120-64N">
</package>
<package name="QFN50P1000X1000X100-69N">
</package>
<package name="QFP80P900X900X145-64N">
</package>
<package name="QFN50P700X700X80-49N">
</package>
<package name="QFN50P900X900X80-61N">
</package>
<package name="QFN50P900X900X80-65N">
</package>
<package name="DIP254P762X508-16">
</package>
<package name="SOT95P285X90-6N">
</package>
<package name="QFP50P2200X2200X160-144N">
</package>
<package name="QFP50P900X900X160-48N">
</package>
<package name="QFN50P600X600X80-41N">
</package>
<package name="QFP50P900X900X160-49N">
</package>
<package name="QFP50P1400X1400X120-80N">
</package>
<package name="QFP50P1723X2323X315-128N">
</package>
<package name="SOIC127P600X175-16N">
</package>
<package name="SOIC127P600X175-14N">
</package>
<package name="DIP254P762X508-14">
</package>
<package name="QFN50P400X400X80-17N">
</package>
<package name="DFN300X300X80-9N">
</package>
<package name="DFN400X400X80-17N">
</package>
<package name="DFN400X300X80-15N">
</package>
<package name="SOIC127P620X175-16N">
</package>
<package name="PLCC127P991X991X457-20N">
</package>
<package name="DFN250X220X80-6N">
</package>
<package name="QFN50P550X1000X80-55N">
</package>
<package name="DFN400X300X80-14N">
</package>
<package name="SOIC127O620X175-8N">
</package>
<package name="SOP64P1035X274-48N">
</package>
<package name="QFP40P1600X1600X120-128N">
</package>
<package name="SOP50P800X110-48N">
</package>
<package name="SOP50P810X110-56N">
</package>
<package name="DFN600X600X80-33N">
</package>
<package name="SOP50P810X110-48N">
</package>
<package name="QFP50P1600X1600X120-100N">
</package>
<package name="SOT95P284X122-5N">
</package>
<package name="SOT95P284X119-5N">
</package>
<package name="SOIC127P600X175-8">
</package>
<package name="QFP50P500X500X80-33N">
</package>
<package name="QFN50P700X700X80-45N">
</package>
<package name="QFP50P1200X1200X145-64N">
</package>
<package name="SOP65P790X200-28N">
</package>
<package name="QFP50P1400X1400X140-80N">
</package>
<package name="QFP50P1400X1400X160-80N">
</package>
<package name="QFP50P1200X1200X120-64">
</package>
<package name="BGA196C14X14X100C_1500X1500X14">
</package>
<package name="SOIC127P62X175-8N">
</package>
<package name="QFN50P600X600X80-33N">
</package>
<package name="TO254P914X530-8P">
</package>
<package name="DIP254P760X508-14">
</package>
<package name="TO254P914X470-8P">
</package>
<package name="TO292P914X470-8P">
</package>
<package name="DIP245762X508-14">
</package>
<package name="DIP254762X508-8">
</package>
<package name="TO254P1435X457-3N">
</package>
<package name="TO254P470X1016X2222-3P">
</package>
<package name="TO254P1435X457-4N">
</package>
<package name="TO228P970X238-3N">
</package>
<package name="SOT230P696X180-4N">
</package>
<package name="DFN400X400X80-9N">
</package>
<package name="SOIC127P1041X200-10N">
</package>
<package name="TO292P939X470-10P">
</package>
<package name="SOIC127P1041X233-14N">
</package>
<package name="TO127P543X266-3P">
</package>
<package name="SOT95P285X120-5N">
</package>
<package name="DFN300X300X80-7N">
</package>
<package name="SOP65P490X110X8N">
</package>
<package name="TO127P254X495-3P">
</package>
<package name="SOP65P640X110-17N">
</package>
<package name="SOP65P640X110-21N">
</package>
<package name="SOT65P240X110-5N">
</package>
<package name="SOT65P210X110-5N">
</package>
<package name="SOIC127P620X168-9N">
</package>
<package name="SOIC127P600X168-9N">
</package>
<package name="TO127P1435X210-7N">
</package>
<package name="TO127P1435X210-8N">
</package>
<package name="SOP65P640X110-15N">
</package>
<package name="DFN400X400X80-11N">
</package>
<package name="SOP50P490X110-11N">
</package>
<package name="SOP65P490X110-9N">
</package>
<package name="DFN500X500X80-16N">
</package>
<package name="SOIC127P640X265-24N">
</package>
<package name="TO170X1435X457-6N">
</package>
<package name="TO170P1435X465-6N">
</package>
<package name="TO170P1435X457-6N">
</package>
<package name="TO170P470X1016X2092-5P">
</package>
<package name="TO170P1435X457-5N">
</package>
<package name="TO127P1435X457-7N">
</package>
<package name="TO127P1435X457-8N">
</package>
<package name="TO127P469X1016X2102-7P">
</package>
<package name="TO127P457X1016X2052-7P">
</package>
<package name="TO127P470X1016X1740-7P">
</package>
<package name="TO127O1435X465-7N">
</package>
<package name="TO170P1435X465-5N">
</package>
<package name="DFN400X400X80-15N">
</package>
<package name="DFN500X500X80-17N">
</package>
<package name="SOP65P640X175-21N">
</package>
<package name="QFN65P400X400X80-17N">
</package>
<package name="QFN400X400X80-25N">
</package>
<package name="SOT95P300X120-6N">
</package>
<package name="DFN600X500X100-15N">
</package>
<package name="DFN500X400X100-15N">
</package>
<package name="TO263127P1435X457-8N">
</package>
<package name="DFN500X600X100-15N">
</package>
<package name="DFN300X300X80-11N">
</package>
<package name="SOT95P300X120-5N">
</package>
<package name="SOT95P285X110-5N">
</package>
<package name="SOT65P285X120-5N">
</package>
<package name="SOP65P490X109-9N">
</package>
<package name="QFN50P400X400X80-25N">
</package>
<package name="BGA18C20PX364P5X7_161X180X60">
</package>
<package name="BGA20N40P4X5_161X201X60">
</package>
<package name="BGA12C3X4X40P_161X121X67">
</package>
<package name="BGA12N50P3X4_151X199X60">
</package>
<package name="SOT95P285X122-6N">
</package>
<package name="BGA14C43PX50P5X4_209X240X60">
</package>
<package name="DFN300X400X80-15N">
</package>
<package name="DIP254P1524X724-24">
</package>
<package name="SOT95P285X122-5N">
</package>
<package name="SOP50P490X109-11N">
</package>
<package name="SOP127P600X180-14N">
</package>
<package name="SOIC127P620X175-14N">
</package>
<package name="TO254P1435X464-4N">
</package>
<package name="TO254P482X1024X3124-3P">
</package>
<package name="SOT230P700X180-4N">
</package>
<package name="BGA10C50PX50P3X4_181X217X60">
</package>
<package name="BGA08C50PX50P3X3_166X181X60">
</package>
<package name="BGA09N50P3X3_195X195X60">
</package>
<package name="BGA8C3X3X50P_181X166X67">
</package>
<package name="DFN300X300X80-13N">
</package>
<package name="SOP65P640X110-29N">
</package>
<package name="SOT95P251X112-3N">
</package>
<package name="SOT95P263X110-3N">
</package>
<package name="BGA12N50P3X4_197X230X60">
</package>
<package name="BGA12C50P3X4_207X176X67">
</package>
<package name="BGA8C50PX50P3X3_192X192X60">
</package>
<package name="BGA10C50PX50P4X3_195X213X60">
</package>
<package name="QFN50P400X400X80-13N">
</package>
<package name="SOIC127P640X175-8N">
</package>
<package name="BGA12C3X4X40P_161X121X60">
</package>
<package name="BGA5C43PX50P3X2_105X138X60">
</package>
<package name="DFN50P300X300X80-9N">
</package>
<package name="BGA50PX43P3X3_148X110X67">
</package>
<package name="BGA12C3X550P_242X169X60">
</package>
<package name="AMP_LM3886T">
</package>
<package name="BGA49C7X7X50P_400X400X110">
</package>
<package name="QFN40P500X500X80-41N">
</package>
<package name="QFN65P200X200X80-9N">
</package>
<package name="BGA9C3X3X50P_146X146X60">
</package>
<package name="BGA9C40P3X3_140X140X60">
</package>
<package name="AMP_LM4702BTA">
</package>
<package name="AMP_LM4702CTA">
</package>
<package name="TO127P1435X464-8N">
</package>
<package name="TO97P1435X457-10N">
</package>
<package name="AMP_LM4765T">
</package>
<package name="AMP_LM4766T">
</package>
<package name="AMP_LM4766TF">
</package>
<package name="AMP_LM4780TA">
</package>
<package name="AMP_LM4781TA">
</package>
<package name="SOP50P490X110-8N">
</package>
<package name="BGA14C25PX43P7X5_225X204X67">
</package>
<package name="BGA25C5X5X50P_254X251X67">
</package>
<package name="BGA12C50P3X4_199X148X60">
</package>
<package name="BGA16C50P4X4_196X196X67">
</package>
<package name="BGA18C25P43P7X5_199X222X95">
</package>
<package name="BGA16C50P4X4_197X197X67">
</package>
<package name="BGA16C40P4X4_169X169X60">
</package>
<package name="BGA12C3X4X50P_200X150X67">
</package>
<package name="BGA25C50P5X5_300X300X110">
</package>
<package name="BGA25C40P5X5_200X200X67">
</package>
<package name="BGA16C50P4X4_200X200X60">
</package>
<package name="BGA20C50P4X5_251X199X675">
</package>
<package name="BGA20C50P4X5_251X202X67">
</package>
<package name="BGA14C50P4X4_197X197X67">
</package>
<package name="BGA20C50P4X5_272X220X67">
</package>
<package name="BGA36C50P6X6_305X305X65">
</package>
<package name="BGA36C50P6X6_351X325X72">
</package>
<package name="BGA36C6X650P_345X345X725">
</package>
<package name="BGA36C50P6X6_328X328X72">
</package>
<package name="BGA49C50P7X7_392X392X65">
</package>
<package name="BGA36C50P6X6_351X325X67">
</package>
<package name="BGA25C50P5X5_251X251X61">
</package>
<package name="BGA25C5X5X50P_272X272X60">
</package>
<package name="DFN80P400X400X80-11N">
</package>
<package name="TO97P1435X475-10N">
</package>
<package name="QFN50P500X500X80-29N">
</package>
<package name="MSOP50P490X110-10N">
</package>
<package name="QFN50P400X500X80-25N">
</package>
<package name="SOIC127P1032X265-14N">
</package>
<package name="SOT95P260X110-3N">
</package>
<package name="MUC10A">
</package>
<package name="SOIC127P1032X265-16N">
</package>
<package name="SOP127P620X168-9N">
</package>
<package name="SOT95P250X112-3N">
</package>
<package name="QFP50P1740X2340X340-128N">
</package>
<package name="SOT95P280X110-5N">
</package>
<package name="SOT95P284X110-5N">
</package>
<package name="DIOB_LMD18200T">
</package>
<package name="TO127P1435X465-6N">
</package>
<package name="AMP_LME49811TB">
</package>
<package name="AMP_LME49830TB">
</package>
<package name="BGA8C40P3X3_121X121X67">
</package>
<package name="BGA16C4X4X40P_161X161X67">
</package>
<package name="DFN250X300X80-9N">
</package>
<package name="QFN40P250X250X80-14N">
</package>
<package name="SOT95PX285X122-5N">
</package>
<package name="SOP635P600X172-16N">
</package>
<package name="QFP50P1000X1000X120-65N">
</package>
<package name="SOT65P240X110-6N">
</package>
<package name="SOT65P210X110-6N">
</package>
<package name="SOT95P284X120-6N">
</package>
<package name="SOP63P640X170-16N">
</package>
<package name="SOP65P640X170-16N">
</package>
<package name="SOP65P620X110-14N">
</package>
<package name="TO457P970X238-3N">
</package>
<package name="BGA4C2X2X50P_117X117X42">
</package>
<package name="BGA36C6X6X50P_345X345X67">
</package>
<package name="BGA16C4X450P_197X197X60">
</package>
<package name="BGA25C40P5X5_201X201X60">
</package>
<package name="SOT95P284X100-6N">
</package>
<package name="SOT95P284X120-5N">
</package>
<package name="BGA05C25PX433P3X3_93X110X50">
</package>
<package name="BGA5C50P2X3_110X93X57">
</package>
<package name="SOIC65P490X109-8N">
</package>
<package name="DFN329X292X80-7N">
</package>
<package name="DFN292X329X80-7N">
</package>
<package name="SOIC127P600X168-8N">
</package>
<package name="TO170P1436X210-6N">
</package>
<package name="TO17P1435X465-6N">
</package>
<package name="SOT150P696X180-5N">
</package>
<package name="TO228P1042X238-3N">
</package>
<package name="SOT15P696X180-5N">
</package>
<package name="SOP127P600X168-9N">
</package>
<package name="TO170P470X1016X2222-5P">
</package>
<package name="BGA25C5X5X50P_246X246X67">
</package>
<package name="QFN50P400X400X80-26N">
</package>
<package name="BGA36C5X5X50P_300X300X72">
</package>
<package name="BGA36C50P6X6_300X300X67">
</package>
<package name="DFN300X400X80-7N">
</package>
<package name="DFN300X200X80-9N">
</package>
<package name="BGA5C3X350P_146X100X675">
</package>
<package name="BGA5C3X3X50P_100X146X67">
</package>
<package name="BGA4C2X2X50P_129X101X60">
</package>
<package name="BGA4C2X2X50P_963X144X67">
</package>
<package name="BGA4C2X2X50P_96X144X67">
</package>
<package name="BGA5C3X3X50P_100X143X67">
</package>
<package name="BGA5C3X3X50P_100X438X67">
</package>
<package name="BGA9C3X340P_121X121X67">
</package>
<package name="BGA36C6X6X50P_300X300X65">
</package>
<package name="BGA4C2X2X50P_106X109X67">
</package>
<package name="BGA4C2X2X50P_109X106X67">
</package>
<package name="BGA5C3X3X50P_95X133X67">
</package>
<package name="BGA5C3X3X50P_133X95X67">
</package>
<package name="SOT95P280X120-5N">
</package>
<package name="QFP50P1600X1600X120-101N">
</package>
<package name="QFP80P900X900X145-32N">
</package>
<package name="BGA49C7X780P_700X700X150">
</package>
<package name="BGA196C14X14X100P_1500X1500X14">
</package>
<package name="BGA49C80P7X7_700X700X150">
</package>
<package name="BGA100C80P10X10_1000X1000X150">
</package>
</packages>
<symbols>
<symbol name="ADC0801LCN">
<pin name="VCC" direction="pwr"/>
<pin name="VIN+" direction="pwr"/>
<pin name="VREF/2" direction="pwr"/>
<pin name="~CS" direction="in"/>
<pin name="~RD" direction="in"/>
<pin name="~WR" direction="in"/>
<pin name="CLKR" direction="in"/>
<pin name="CLKIN" direction="in"/>
<pin name="VIN-" direction="pwr"/>
<pin name="DGND" direction="pas"/>
<pin name="AGND" direction="pas"/>
<pin name="~INTR" direction="out"/>
<pin name="DB0" direction="out"/>
<pin name="DB1" direction="out"/>
<pin name="DB2" direction="out"/>
<pin name="DB3" direction="out"/>
<pin name="DB4" direction="out"/>
<pin name="DB5" direction="out"/>
<pin name="DB6" direction="out"/>
<pin name="DB7" direction="out"/>
</symbol>
<symbol name="ADC0802LCN">
<pin name="VCC" direction="pwr"/>
<pin name="VIN+" direction="pwr"/>
<pin name="VREF/2" direction="pwr"/>
<pin name="~CS" direction="in"/>
<pin name="~RD" direction="in"/>
<pin name="~WR" direction="in"/>
<pin name="CLKR" direction="in"/>
<pin name="CLKIN" direction="in"/>
<pin name="VIN-" direction="pwr"/>
<pin name="DGND" direction="pas"/>
<pin name="AGND" direction="pas"/>
<pin name="~INTR" direction="out"/>
<pin name="DB0" direction="out"/>
<pin name="DB1" direction="out"/>
<pin name="DB2" direction="out"/>
<pin name="DB3" direction="out"/>
<pin name="DB4" direction="out"/>
<pin name="DB5" direction="out"/>
<pin name="DB6" direction="out"/>
<pin name="DB7" direction="out"/>
</symbol>
<symbol name="ADC0803LCN">
<pin name="VCC" direction="pwr"/>
<pin name="VIN+" direction="pwr"/>
<pin name="VREF/2" direction="in"/>
<pin name="CLK_IN" direction="in"/>
<pin name="CLK_R" direction="in"/>
<pin name="~CS" direction="in"/>
<pin name="~RD" direction="in"/>
<pin name="~WR" direction="in"/>
<pin name="~INTR" direction="in"/>
<pin name="VIN-" direction="pwr"/>
<pin name="AGND" direction="pas"/>
<pin name="DGND" direction="pas"/>
<pin name="DB0" direction="out"/>
<pin name="DB1" direction="out"/>
<pin name="DB2" direction="out"/>
<pin name="DB3" direction="out"/>
<pin name="DB4" direction="out"/>
<pin name="DB5" direction="out"/>
<pin name="DB6" direction="out"/>
<pin name="DB7" direction="out"/>
</symbol>
<symbol name="ADC0804LCN">
<pin name="VCC" direction="pwr"/>
<pin name="VIN(+)" direction="pwr"/>
<pin name="VREF/2" direction="in"/>
<pin name="CLK_IN" direction="in"/>
<pin name="CLK_R" direction="in"/>
<pin name="~CS" direction="in"/>
<pin name="~RD" direction="in"/>
<pin name="~WR" direction="in"/>
<pin name="~INTR" direction="in"/>
<pin name="VIN(-)" direction="pwr"/>
<pin name="DGND" direction="pas"/>
<pin name="AGND" direction="pas"/>
<pin name="DB0" direction="pas"/>
<pin name="DB1" direction="pas"/>
<pin name="DB2" direction="pas"/>
<pin name="DB3" direction="pas"/>
<pin name="DB4" direction="pas"/>
<pin name="DB5" direction="pas"/>
<pin name="DB6" direction="pas"/>
<pin name="DB7" direction="pas"/>
</symbol>
<symbol name="ADC0804LCWM">
<pin name="VCC" direction="pwr"/>
<pin name="VREF/2" direction="pwr"/>
<pin name="VIN+" direction="in"/>
<pin name="VIN-" direction="in"/>
<pin name="~CS" direction="in"/>
<pin name="~RD" direction="in"/>
<pin name="~WR" direction="in"/>
<pin name="CLKIN" direction="in"/>
<pin name="CLKR" direction="in"/>
<pin name="AGND" direction="pas"/>
<pin name="DGND" direction="pas"/>
<pin name="~INTR" direction="out"/>
<pin name="DB0" direction="out"/>
<pin name="DB1" direction="out"/>
<pin name="DB2" direction="out"/>
<pin name="DB3" direction="out"/>
<pin name="DB4" direction="out"/>
<pin name="DB5" direction="out"/>
<pin name="DB6" direction="out"/>
<pin name="DB7" direction="out"/>
</symbol>
<symbol name="ADC08060CIMT">
<pin name="VA_2" direction="pwr"/>
<pin name="VA_3" direction="pwr"/>
<pin name="VA" direction="pwr"/>
<pin name="CLOCK" direction="in"/>
<pin name="VIN" direction="in"/>
<pin name="VRT" direction="in"/>
<pin name="VRM" direction="pas"/>
<pin name="VRB" direction="in"/>
<pin name="PD" direction="in"/>
<pin name="DR_VD" direction="pwr"/>
<pin name="AGND_2" direction="pas"/>
<pin name="AGND_3" direction="pas"/>
<pin name="AGND_4" direction="pas"/>
<pin name="AGND" direction="pas"/>
<pin name="VIN_GND" direction="pas"/>
<pin name="DR_GND" direction="pas"/>
<pin name="D0" direction="out"/>
<pin name="D1" direction="out"/>
<pin name="D2" direction="out"/>
<pin name="D3" direction="out"/>
<pin name="D4" direction="out"/>
<pin name="D5" direction="out"/>
<pin name="D6" direction="out"/>
<pin name="D7" direction="out"/>
</symbol>
<symbol name="ADC0808CCN">
<pin name="VCC" direction="pwr"/>
<pin name="CLK" direction="in"/>
<pin name="VREF(+)" direction="pas"/>
<pin name="VREF(-)" direction="pas"/>
<pin name="START" direction="in"/>
<pin name="ALE" direction="in"/>
<pin name="EOC" direction="in"/>
<pin name="OUT_EN" direction="in"/>
<pin name="ADDC" direction="pas"/>
<pin name="ADDB" direction="pas"/>
<pin name="ADDA" direction="pas"/>
<pin name="IN0" direction="in"/>
<pin name="IN1" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="IN3" direction="in"/>
<pin name="IN4" direction="in"/>
<pin name="IN5" direction="in"/>
<pin name="IN6" direction="in"/>
<pin name="IN7" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="2_(1)" direction="pas"/>
<pin name="2_(2)" direction="pas"/>
<pin name="2_(3)" direction="pas"/>
<pin name="2_(4)" direction="pas"/>
<pin name="2_(5)" direction="pas"/>
<pin name="2_(6)" direction="pas"/>
<pin name="2_(7)" direction="pas"/>
<pin name="2_(8)" direction="pas"/>
</symbol>
<symbol name="ADC0808CCV">
<pin name="VCC" direction="pwr"/>
<pin name="START" direction="in"/>
<pin name="EOC" direction="in"/>
<pin name="OUTPUT_ENABLE" direction="in"/>
<pin name="CLOCK" direction="in"/>
<pin name="ALE" direction="in"/>
<pin name="VREF(+)" direction="in"/>
<pin name="VREF(-)" direction="in"/>
<pin name="IN_0" direction="in"/>
<pin name="IN_1" direction="in"/>
<pin name="IN_2" direction="in"/>
<pin name="IN_3" direction="in"/>
<pin name="IN_4" direction="in"/>
<pin name="IN_5" direction="in"/>
<pin name="IN_6" direction="in"/>
<pin name="IN_7" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="2_-8" direction="out"/>
<pin name="2_-1" direction="out"/>
<pin name="2_-2" direction="out"/>
<pin name="2_-3" direction="out"/>
<pin name="2_-4" direction="out"/>
<pin name="2_-5" direction="out"/>
<pin name="2_-6" direction="out"/>
<pin name="2_-7" direction="out"/>
<pin name="ADD_A"/>
<pin name="ADD_B"/>
<pin name="ADD_C"/>
</symbol>
<symbol name="ADC0809CCN">
<pin name="VCC" direction="pwr"/>
<pin name="CLK" direction="in"/>
<pin name="VREF(+)" direction="pas"/>
<pin name="VREF(-)" direction="pas"/>
<pin name="START" direction="in"/>
<pin name="ALE" direction="in"/>
<pin name="EOC" direction="in"/>
<pin name="OUT_EN" direction="in"/>
<pin name="ADDC" direction="pas"/>
<pin name="ADDB" direction="pas"/>
<pin name="ADDA" direction="pas"/>
<pin name="IN0" direction="in"/>
<pin name="IN1" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="IN3" direction="in"/>
<pin name="IN4" direction="in"/>
<pin name="IN5" direction="in"/>
<pin name="IN6" direction="in"/>
<pin name="IN7" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="2_(1)" direction="pas"/>
<pin name="2_(2)" direction="pas"/>
<pin name="2_(3)" direction="pas"/>
<pin name="2_(4)" direction="pas"/>
<pin name="2_(5)" direction="pas"/>
<pin name="2_(6)" direction="pas"/>
<pin name="2_(7)" direction="pas"/>
<pin name="2_(8)" direction="pas"/>
</symbol>
<symbol name="ADC0809CCV">
<pin name="VCC" direction="pwr"/>
<pin name="START" direction="in"/>
<pin name="EOC" direction="in"/>
<pin name="OUTPUT_ENABLE" direction="in"/>
<pin name="CLOCK" direction="in"/>
<pin name="ALE" direction="in"/>
<pin name="VREF(+)" direction="in"/>
<pin name="VREF(-)" direction="in"/>
<pin name="IN_0" direction="in"/>
<pin name="IN_1" direction="in"/>
<pin name="IN_2" direction="in"/>
<pin name="IN_3" direction="in"/>
<pin name="IN_4" direction="in"/>
<pin name="IN_5" direction="in"/>
<pin name="IN_6" direction="in"/>
<pin name="IN_7" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="2_-8" direction="out"/>
<pin name="2_-1" direction="out"/>
<pin name="2_-2" direction="out"/>
<pin name="2_-3" direction="out"/>
<pin name="2_-4" direction="out"/>
<pin name="2_-5" direction="out"/>
<pin name="2_-6" direction="out"/>
<pin name="2_-7" direction="out"/>
<pin name="ADD_A"/>
<pin name="ADD_B"/>
<pin name="ADD_C"/>
</symbol>
<symbol name="ADC08100CIMTC">
<pin name="DRVD" direction="pwr"/>
<pin name="VA_2" direction="pwr"/>
<pin name="VA_3" direction="pwr"/>
<pin name="VA" direction="pwr"/>
<pin name="CLK" direction="in"/>
<pin name="VRT" direction="in"/>
<pin name="PD" direction="in"/>
<pin name="VIN" direction="in"/>
<pin name="VRM" direction="pas"/>
<pin name="VRB" direction="in"/>
<pin name="AGND_2" direction="pas"/>
<pin name="AGND_3" direction="pas"/>
<pin name="AGND_4" direction="pas"/>
<pin name="AGND" direction="pas"/>
<pin name="VIN_GND" direction="pas"/>
<pin name="DR_GND" direction="pas"/>
<pin name="D0" direction="out"/>
<pin name="D1" direction="out"/>
<pin name="D2" direction="out"/>
<pin name="D3" direction="out"/>
<pin name="D4" direction="out"/>
<pin name="D5" direction="out"/>
<pin name="D6" direction="out"/>
<pin name="D7" direction="out"/>
</symbol>
<symbol name="ADC081500CIYB">
<pin name="VA_2" direction="pwr"/>
<pin name="VA_3" direction="pwr"/>
<pin name="VA_4" direction="pwr"/>
<pin name="VA_5" direction="pwr"/>
<pin name="VA_6" direction="pwr"/>
<pin name="VA_7" direction="pwr"/>
<pin name="VA_8" direction="pwr"/>
<pin name="VA_9" direction="pwr"/>
<pin name="VA_10" direction="pwr"/>
<pin name="VA_11" direction="pwr"/>
<pin name="VA" direction="pwr"/>
<pin name="VCMO" direction="in"/>
<pin name="CAL" direction="in"/>
<pin name="VBG" direction="in"/>
<pin name="PD" direction="in"/>
<pin name="REXT" direction="in"/>
<pin name="CALRUN" direction="in"/>
<pin name="FSR/ECE" direction="in"/>
<pin name="CALDLY/~SCS" direction="in"/>
<pin name="DCLK_RST" direction="in"/>
<pin name="CLK+" direction="in"/>
<pin name="CLK-" direction="in"/>
<pin name="DCLK-" direction="in"/>
<pin name="DCLK+" direction="in"/>
<pin name="VDR_2" direction="in"/>
<pin name="VDR_3" direction="in"/>
<pin name="VDR_4" direction="in"/>
<pin name="VDR_5" direction="in"/>
<pin name="VDR_6" direction="in"/>
<pin name="VDR_7" direction="in"/>
<pin name="VDR_8" direction="in"/>
<pin name="VDR" direction="in"/>
<pin name="VIN-" direction="in"/>
<pin name="VIN+" direction="in"/>
<pin name="TDIODE_P" direction="in"/>
<pin name="TDIODE_N" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC_6" direction="nc"/>
<pin name="NC_7" direction="nc"/>
<pin name="NC_8" direction="nc"/>
<pin name="NC_9" direction="nc"/>
<pin name="NC_10" direction="nc"/>
<pin name="NC_11" direction="nc"/>
<pin name="NC_12" direction="nc"/>
<pin name="NC_13" direction="nc"/>
<pin name="NC_14" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="DR_GND_2" direction="pas"/>
<pin name="DR_GND_3" direction="pas"/>
<pin name="DR_GND_4" direction="pas"/>
<pin name="DR_GND_5" direction="pas"/>
<pin name="DR_GND_6" direction="pas"/>
<pin name="DR_GND_7" direction="pas"/>
<pin name="DR_GND_8" direction="pas"/>
<pin name="DR_GND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="OUTV/SCLK" direction="out"/>
<pin name="OUT_EDGE/DDR/SDATA" direction="out"/>
<pin name="OR+" direction="out"/>
<pin name="OR-" direction="out"/>
<pin name="D0-" direction="out"/>
<pin name="D0+" direction="out"/>
<pin name="D1-" direction="out"/>
<pin name="D1+" direction="out"/>
<pin name="D2-" direction="out"/>
<pin name="D2+" direction="out"/>
<pin name="D3-" direction="out"/>
<pin name="D3+" direction="out"/>
<pin name="D4-" direction="out"/>
<pin name="D4+" direction="out"/>
<pin name="D5-" direction="out"/>
<pin name="D5+" direction="out"/>
<pin name="D6-" direction="out"/>
<pin name="D6+" direction="out"/>
<pin name="D7-" direction="out"/>
<pin name="D7+" direction="out"/>
<pin name="DD0-" direction="out"/>
<pin name="DD0+" direction="out"/>
<pin name="DD1-" direction="out"/>
<pin name="DD1+" direction="out"/>
<pin name="DD2-" direction="out"/>
<pin name="DD2+" direction="out"/>
<pin name="DD3-" direction="out"/>
<pin name="DD3+" direction="out"/>
<pin name="DD4-" direction="out"/>
<pin name="DD4+" direction="out"/>
<pin name="DD5-" direction="out"/>
<pin name="DD5+" direction="out"/>
<pin name="DD6-" direction="out"/>
<pin name="DD6+" direction="out"/>
<pin name="DD7-" direction="out"/>
<pin name="DD7+" direction="out"/>
<pin name="NC_15" direction="nc"/>
<pin name="NC_16" direction="nc"/>
<pin name="NC_17" direction="nc"/>
<pin name="NC_18" direction="nc"/>
<pin name="NC_19" direction="nc"/>
<pin name="NC_20" direction="nc"/>
<pin name="NC_21" direction="nc"/>
<pin name="NC_22" direction="nc"/>
<pin name="NC_23" direction="nc"/>
<pin name="NC_24" direction="nc"/>
<pin name="NC_25" direction="nc"/>
<pin name="NC_26" direction="nc"/>
<pin name="NC_27" direction="nc"/>
<pin name="NC_28" direction="nc"/>
<pin name="NC_29" direction="nc"/>
<pin name="NC_30" direction="nc"/>
<pin name="NC_31" direction="nc"/>
<pin name="NC_32" direction="nc"/>
<pin name="NC_33" direction="nc"/>
<pin name="NC_34" direction="nc"/>
<pin name="NC_35" direction="nc"/>
<pin name="NC_36" direction="nc"/>
<pin name="NC_37" direction="nc"/>
<pin name="NC_38" direction="nc"/>
<pin name="NC_39" direction="nc"/>
<pin name="NC_40" direction="nc"/>
<pin name="NC" direction="nc"/>
</symbol>
<symbol name="ADC0816CCN">
<pin name="VCC" direction="pwr"/>
<pin name="START" direction="in"/>
<pin name="COMPARATOR_IN" direction="in"/>
<pin name="EXPANSION_CONTROL" direction="in"/>
<pin name="EOC" direction="pas"/>
<pin name="OUTPUT_ENABLE" direction="in"/>
<pin name="CLOCK" direction="in"/>
<pin name="IN0" direction="in"/>
<pin name="IN1" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="IN3" direction="in"/>
<pin name="IN4" direction="in"/>
<pin name="IN5" direction="in"/>
<pin name="IN6" direction="in"/>
<pin name="IN7" direction="in"/>
<pin name="IN8" direction="in"/>
<pin name="IN9" direction="in"/>
<pin name="IN10" direction="in"/>
<pin name="IN11" direction="in"/>
<pin name="IN12" direction="in"/>
<pin name="IN13" direction="in"/>
<pin name="IN14" direction="in"/>
<pin name="IN15" direction="in"/>
<pin name="REF(-)" direction="in"/>
<pin name="REF(+)" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="2_-1" direction="out"/>
<pin name="2_-2" direction="out"/>
<pin name="2_-3" direction="out"/>
<pin name="2_-4" direction="out"/>
<pin name="2_-5" direction="out"/>
<pin name="2_-6" direction="out"/>
<pin name="2_-7" direction="out"/>
<pin name="2_-8" direction="out"/>
<pin name="ALE" direction="pas"/>
<pin name="ADD_D"/>
<pin name="ADD_C"/>
<pin name="ADD_B"/>
<pin name="ADD_A"/>
<pin name="MULTIPLEXER_OUT" direction="pas"/>
</symbol>
<symbol name="ADC0817CCN">
<pin name="VCC" direction="pwr"/>
<pin name="CLK" direction="in"/>
<pin name="START" direction="in"/>
<pin name="ALE" direction="in"/>
<pin name="EOC" direction="pas"/>
<pin name="OUT_EN" direction="in"/>
<pin name="ADD_A" direction="in"/>
<pin name="ADD_B" direction="in"/>
<pin name="ADD_C" direction="in"/>
<pin name="ADD_D" direction="in"/>
<pin name="REF(+)" direction="in"/>
<pin name="REF(-)" direction="in"/>
<pin name="IN0" direction="in"/>
<pin name="IN1" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="IN3" direction="in"/>
<pin name="IN4" direction="in"/>
<pin name="IN5" direction="in"/>
<pin name="IN6" direction="in"/>
<pin name="IN7" direction="in"/>
<pin name="IN8" direction="in"/>
<pin name="IN9" direction="in"/>
<pin name="IN10" direction="in"/>
<pin name="IN11" direction="in"/>
<pin name="IN12" direction="in"/>
<pin name="IN13" direction="in"/>
<pin name="IN14" direction="in"/>
<pin name="IN15" direction="in"/>
<pin name="COMPARATOR_IN" direction="in"/>
<pin name="EXPANSION_CONTROL" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="2_1" direction="out"/>
<pin name="2_2" direction="out"/>
<pin name="2_3" direction="out"/>
<pin name="2_4" direction="out"/>
<pin name="2_5" direction="out"/>
<pin name="2_6" direction="out"/>
<pin name="2_7" direction="out"/>
<pin name="2_8" direction="out"/>
<pin name="MULTIPLEXER_OUT" direction="out"/>
</symbol>
<symbol name="ADC081S021CIMF">
<pin name="VA" direction="pwr"/>
<pin name="VIN" direction="in"/>
<pin name="SCLK" direction="in"/>
<pin name="~CS" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="SDATA" direction="out"/>
</symbol>
<symbol name="ADC081S101CIMF">
<pin name="VA" direction="pwr"/>
<pin name="VIN" direction="in"/>
<pin name="SCLK" direction="in"/>
<pin name="~CS" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="SDATA" direction="out"/>
</symbol>
<symbol name="ADC081S101CISD">
<pin name="VA" direction="pwr"/>
<pin name="VIN" direction="in"/>
<pin name="SCLK" direction="in"/>
<pin name="~CS" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="SDATA" direction="out"/>
</symbol>
<symbol name="ADC08200CIMT">
<pin name="VA_2" direction="pwr"/>
<pin name="VA_3" direction="pwr"/>
<pin name="VA" direction="pwr"/>
<pin name="VIN" direction="pwr"/>
<pin name="CLK" direction="in"/>
<pin name="VDR" direction="pwr"/>
<pin name="VRM" direction="in"/>
<pin name="VRT" direction="in"/>
<pin name="VRB" direction="in"/>
<pin name="PD" direction="in"/>
<pin name="AGND_2" direction="pas"/>
<pin name="AGND_3" direction="pas"/>
<pin name="AGND_4" direction="pas"/>
<pin name="AGND" direction="pas"/>
<pin name="DR_GND" direction="pas"/>
<pin name="VIN_GND" direction="pas"/>
<pin name="D0" direction="out"/>
<pin name="D1" direction="out"/>
<pin name="D2" direction="out"/>
<pin name="D3" direction="out"/>
<pin name="D4" direction="out"/>
<pin name="D5" direction="out"/>
<pin name="D6" direction="out"/>
<pin name="D7" direction="out"/>
</symbol>
<symbol name="ADC0820CCN">
<pin name="VCC" direction="pwr"/>
<pin name="VIN" direction="in"/>
<pin name="~CS" direction="in"/>
<pin name="~WR~/RDY" direction="in"/>
<pin name="MODE" direction="in"/>
<pin name="~RD" direction="in"/>
<pin name="VREF(-)" direction="pwr"/>
<pin name="VREF(+)" direction="pwr"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="~OFL" direction="out"/>
<pin name="~INT" direction="pas"/>
<pin name="DB0" direction="out"/>
<pin name="DB1" direction="out"/>
<pin name="DB2" direction="out"/>
<pin name="DB3" direction="out"/>
<pin name="DB_4" direction="out"/>
<pin name="DB_5" direction="out"/>
<pin name="DB_6" direction="out"/>
<pin name="DB_7" direction="out"/>
</symbol>
<symbol name="ADC0820CCWM">
<pin name="VCC" direction="pwr"/>
<pin name="VIN" direction="pwr"/>
<pin name="~WR/RDY" direction="in"/>
<pin name="MODE" direction="in"/>
<pin name="~RD" direction="in"/>
<pin name="~INT" direction="in"/>
<pin name="~CS" direction="in"/>
<pin name="VREF(-)" direction="in"/>
<pin name="VREF(+)" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="DB0" direction="out"/>
<pin name="DB1" direction="out"/>
<pin name="DB2" direction="out"/>
<pin name="DB3" direction="out"/>
<pin name="DB4" direction="out"/>
<pin name="DB5" direction="out"/>
<pin name="DB6" direction="out"/>
<pin name="DB7" direction="out"/>
<pin name="~OFL" direction="out"/>
</symbol>
<symbol name="ADC082S021CIMM">
<pin name="VA" direction="pwr"/>
<pin name="~CS" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="IN1" direction="in"/>
<pin name="DIN" direction="in"/>
<pin name="SCLK" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="DOUT" direction="out"/>
</symbol>
<symbol name="ADC082S101CIMM">
<pin name="VA" direction="pwr"/>
<pin name="SCLK" direction="in"/>
<pin name="~CS" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="IN1" direction="in"/>
<pin name="DIN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="DOUT" direction="out"/>
</symbol>
<symbol name="ADC0831CCN">
<pin name="VCC" direction="pwr"/>
<pin name="CLK" direction="in"/>
<pin name="~CS" direction="in"/>
<pin name="VREF" direction="pwr"/>
<pin name="VIN+" direction="in"/>
<pin name="VIN-" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="DO" direction="out"/>
</symbol>
<symbol name="ADC0832CCN">
<pin name="VCC" direction="pwr"/>
<pin name="CLK" direction="in"/>
<pin name="~CS" direction="in"/>
<pin name="VREF" direction="pwr"/>
<pin name="VIN+" direction="in"/>
<pin name="VIN-" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="DO" direction="out"/>
</symbol>
<symbol name="ADC0834CCWM">
<pin name="VCC" direction="pwr"/>
<pin name="V+" direction="in"/>
<pin name="~CS" direction="in"/>
<pin name="CLK" direction="pas"/>
<pin name="DI" direction="in"/>
<pin name="CH0" direction="in"/>
<pin name="CH1" direction="in"/>
<pin name="CH2" direction="in"/>
<pin name="CH3" direction="in"/>
<pin name="VREF" direction="in"/>
<pin name="SARS" direction="pas"/>
<pin name="DGND" direction="pas"/>
<pin name="AGND" direction="pas"/>
<pin name="DO" direction="out"/>
</symbol>
<symbol name="ADC0838CCN">
<pin name="VCC" direction="pwr"/>
<pin name="VREF" direction="in"/>
<pin name="V+" direction="in"/>
<pin name="CLK" direction="in"/>
<pin name="~SE" direction="in"/>
<pin name="DI" direction="in"/>
<pin name="~CS" direction="in"/>
<pin name="CH0" direction="in"/>
<pin name="CH1" direction="in"/>
<pin name="CH2" direction="in"/>
<pin name="CH3" direction="in"/>
<pin name="CH4" direction="in"/>
<pin name="CH5" direction="in"/>
<pin name="CH6" direction="in"/>
<pin name="CH7" direction="in"/>
<pin name="COM" direction="in"/>
<pin name="DGND" direction="pas"/>
<pin name="AGND" direction="pas"/>
<pin name="D0" direction="out"/>
<pin name="SARS" direction="pas"/>
</symbol>
<symbol name="ADC0838CCWM">
<pin name="VCC" direction="pwr"/>
<pin name="V+" direction="in"/>
<pin name="CH0" direction="in"/>
<pin name="CH1" direction="in"/>
<pin name="CH2" direction="in"/>
<pin name="CH3" direction="in"/>
<pin name="CH4" direction="in"/>
<pin name="CH5" direction="in"/>
<pin name="CH6" direction="in"/>
<pin name="CH7" direction="in"/>
<pin name="COM" direction="pas"/>
<pin name="VREF" direction="in"/>
<pin name="~SE" direction="in"/>
<pin name="SARS" direction="in"/>
<pin name="CLK" direction="in"/>
<pin name="DI" direction="in"/>
<pin name="~CS" direction="in"/>
<pin name="DGND" direction="pas"/>
<pin name="AGND" direction="pas"/>
<pin name="DO" direction="out"/>
</symbol>
<symbol name="ADC0844CCN">
<pin name="VCC" direction="pwr"/>
<pin name="~RD" direction="in"/>
<pin name="~CS" direction="in"/>
<pin name="~WR" direction="in"/>
<pin name="~INTR" direction="in"/>
<pin name="VREF" direction="in"/>
<pin name="CH1" direction="in"/>
<pin name="CH2" direction="in"/>
<pin name="CH3" direction="in"/>
<pin name="CH4" direction="in"/>
<pin name="AGND" direction="pas"/>
<pin name="DGND" direction="pas"/>
<pin name="DB0/MA0" direction="out"/>
<pin name="DB1/MA1" direction="out"/>
<pin name="DB2/MA2" direction="out"/>
<pin name="DB3/MA3" direction="out"/>
<pin name="DB4" direction="out"/>
<pin name="DB5" direction="out"/>
<pin name="DB6" direction="out"/>
<pin name="DB7" direction="out"/>
</symbol>
<symbol name="ADC0848CCN">
<pin name="VCC" direction="pwr"/>
<pin name="VREF" direction="in"/>
<pin name="~RD" direction="in"/>
<pin name="~WR" direction="in"/>
<pin name="~CS" direction="in"/>
<pin name="~INTR" direction="in"/>
<pin name="CH1" direction="in"/>
<pin name="CH2" direction="in"/>
<pin name="CH3" direction="in"/>
<pin name="CH4" direction="in"/>
<pin name="CH5" direction="in"/>
<pin name="CH6" direction="in"/>
<pin name="CH7" direction="in"/>
<pin name="CH8" direction="in"/>
<pin name="AGND" direction="pas"/>
<pin name="DGND" direction="pas"/>
<pin name="DB0/MA0" direction="out"/>
<pin name="DB1/MA1" direction="out"/>
<pin name="DB2/MA2" direction="out"/>
<pin name="DB3/MA3" direction="out"/>
<pin name="DB4/MA4" direction="out"/>
<pin name="DB5" direction="out"/>
<pin name="DB6" direction="out"/>
<pin name="DB7" direction="out"/>
</symbol>
<symbol name="ADC0848CCV">
<pin name="VCC" direction="pwr"/>
<pin name="VREF" direction="in"/>
<pin name="~WR" direction="in"/>
<pin name="~CS" direction="in"/>
<pin name="~RD" direction="in"/>
<pin name="CH1" direction="in"/>
<pin name="CH2" direction="in"/>
<pin name="CH3" direction="in"/>
<pin name="CH4" direction="in"/>
<pin name="CH5" direction="in"/>
<pin name="CH6" direction="in"/>
<pin name="CH7" direction="in"/>
<pin name="CH8" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="AGND" direction="pas"/>
<pin name="DGND" direction="pas"/>
<pin name="~INTR" direction="out"/>
<pin name="DB7" direction="out"/>
<pin name="DB6" direction="out"/>
<pin name="DB5" direction="out"/>
<pin name="DB4/MA4" direction="out"/>
<pin name="DB3/MA3" direction="out"/>
<pin name="DB2/MA2" direction="out"/>
<pin name="DB1/MA1" direction="out"/>
<pin name="DB0/MA0" direction="out"/>
</symbol>
<symbol name="ADC084S021CIMM">
<pin name="VA" direction="pwr"/>
<pin name="SCLK" direction="in"/>
<pin name="~CS" direction="in"/>
<pin name="IN1" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="IN3" direction="in"/>
<pin name="IN4" direction="in"/>
<pin name="DIN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="DOUT" direction="out"/>
</symbol>
<symbol name="ADC084S051CIMM">
<pin name="VA" direction="pwr"/>
<pin name="~CS" direction="in"/>
<pin name="DIN" direction="in"/>
<pin name="SCLK" direction="in"/>
<pin name="IN1" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="IN3" direction="in"/>
<pin name="IN4" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="DOUT" direction="out"/>
</symbol>
<symbol name="ADC084S101CIMM">
<pin name="VA" direction="pwr"/>
<pin name="SCLK" direction="in"/>
<pin name="~CS" direction="in"/>
<pin name="IN1" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="IN4" direction="in"/>
<pin name="IN3" direction="in"/>
<pin name="DIN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="DOUT" direction="out"/>
</symbol>
<symbol name="ADC08500CIYB">
<pin name="VA_2" direction="pwr"/>
<pin name="VA_3" direction="pwr"/>
<pin name="VA_4" direction="pwr"/>
<pin name="VA_5" direction="pwr"/>
<pin name="VA_6" direction="pwr"/>
<pin name="VA_7" direction="pwr"/>
<pin name="VA_8" direction="pwr"/>
<pin name="VA_9" direction="pwr"/>
<pin name="VA_10" direction="pwr"/>
<pin name="VA_11" direction="pwr"/>
<pin name="VA" direction="pwr"/>
<pin name="VCMO" direction="in"/>
<pin name="CAL" direction="in"/>
<pin name="VBG" direction="in"/>
<pin name="PD" direction="in"/>
<pin name="REXT" direction="in"/>
<pin name="CALRUN" direction="in"/>
<pin name="FSR/ECE" direction="in"/>
<pin name="CALDLY/~SCS" direction="in"/>
<pin name="DCLK_RST" direction="in"/>
<pin name="CLK+" direction="in"/>
<pin name="CLK-" direction="in"/>
<pin name="DCLK-" direction="in"/>
<pin name="DCLK+" direction="in"/>
<pin name="VDR_2" direction="in"/>
<pin name="VDR_3" direction="in"/>
<pin name="VDR_4" direction="in"/>
<pin name="VDR_5" direction="in"/>
<pin name="VDR_6" direction="in"/>
<pin name="VDR_7" direction="in"/>
<pin name="VDR_8" direction="in"/>
<pin name="VDR" direction="in"/>
<pin name="VIN-" direction="in"/>
<pin name="VIN+" direction="in"/>
<pin name="TDIODE_P" direction="in"/>
<pin name="TDIODE_N" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC_6" direction="nc"/>
<pin name="NC_7" direction="nc"/>
<pin name="NC_8" direction="nc"/>
<pin name="NC_9" direction="nc"/>
<pin name="NC_10" direction="nc"/>
<pin name="NC_11" direction="nc"/>
<pin name="NC_12" direction="nc"/>
<pin name="NC_13" direction="nc"/>
<pin name="NC_14" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="DR_GND_2" direction="pas"/>
<pin name="DR_GND_3" direction="pas"/>
<pin name="DR_GND_4" direction="pas"/>
<pin name="DR_GND_5" direction="pas"/>
<pin name="DR_GND_6" direction="pas"/>
<pin name="DR_GND_7" direction="pas"/>
<pin name="DR_GND_8" direction="pas"/>
<pin name="DR_GND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="OUTV/SCLK" direction="out"/>
<pin name="OUT_EDGE/DDR/SDATA" direction="out"/>
<pin name="OR+" direction="out"/>
<pin name="OR-" direction="out"/>
<pin name="D0-" direction="out"/>
<pin name="D0+" direction="out"/>
<pin name="D1-" direction="out"/>
<pin name="D1+" direction="out"/>
<pin name="D2-" direction="out"/>
<pin name="D2+" direction="out"/>
<pin name="D3-" direction="out"/>
<pin name="D3+" direction="out"/>
<pin name="D4-" direction="out"/>
<pin name="D4+" direction="out"/>
<pin name="D5-" direction="out"/>
<pin name="D5+" direction="out"/>
<pin name="D6-" direction="out"/>
<pin name="D6+" direction="out"/>
<pin name="D7-" direction="out"/>
<pin name="D7+" direction="out"/>
<pin name="DD0-" direction="out"/>
<pin name="DD0+" direction="out"/>
<pin name="DD1-" direction="out"/>
<pin name="DD1+" direction="out"/>
<pin name="DD2-" direction="out"/>
<pin name="DD2+" direction="out"/>
<pin name="DD3-" direction="out"/>
<pin name="DD3+" direction="out"/>
<pin name="DD4-" direction="out"/>
<pin name="DD4+" direction="out"/>
<pin name="DD5-" direction="out"/>
<pin name="DD5+" direction="out"/>
<pin name="DD6-" direction="out"/>
<pin name="DD6+" direction="out"/>
<pin name="DD7-" direction="out"/>
<pin name="DD7+" direction="out"/>
<pin name="NC_15" direction="nc"/>
<pin name="NC_16" direction="nc"/>
<pin name="NC_17" direction="nc"/>
<pin name="NC_18" direction="nc"/>
<pin name="NC_19" direction="nc"/>
<pin name="NC_20" direction="nc"/>
<pin name="NC_21" direction="nc"/>
<pin name="NC_22" direction="nc"/>
<pin name="NC_23" direction="nc"/>
<pin name="NC_24" direction="nc"/>
<pin name="NC_25" direction="nc"/>
<pin name="NC_26" direction="nc"/>
<pin name="NC_27" direction="nc"/>
<pin name="NC_28" direction="nc"/>
<pin name="NC_29" direction="nc"/>
<pin name="NC_30" direction="nc"/>
<pin name="NC_31" direction="nc"/>
<pin name="NC_32" direction="nc"/>
<pin name="NC_33" direction="nc"/>
<pin name="NC_34" direction="nc"/>
<pin name="NC_35" direction="nc"/>
<pin name="NC_36" direction="nc"/>
<pin name="NC_37" direction="nc"/>
<pin name="NC_38" direction="nc"/>
<pin name="NC_39" direction="nc"/>
<pin name="NC_40" direction="nc"/>
<pin name="NC" direction="nc"/>
</symbol>
<symbol name="ADC08831IM">
<pin name="VCC" direction="pwr"/>
<pin name="VIN+" direction="in"/>
<pin name="VIN-" direction="in"/>
<pin name="VREF_IN" direction="in"/>
<pin name="~CS" direction="in"/>
<pin name="CLK" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="DO" direction="out"/>
</symbol>
<symbol name="ADC08832IM">
<pin name="VCC(VREF)" direction="pwr"/>
<pin name="CH0" direction="in"/>
<pin name="CH1" direction="in"/>
<pin name="CLK" direction="in"/>
<pin name="~CS" direction="in"/>
<pin name="DI" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="DO" direction="out"/>
</symbol>
<symbol name="ADC088S022CIMT">
<pin name="VA" direction="pwr"/>
<pin name="VD" direction="pwr"/>
<pin name="~CS" direction="in"/>
<pin name="DIN" direction="in"/>
<pin name="SCLK" direction="in"/>
<pin name="IN0" direction="in"/>
<pin name="IN1" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="IN3" direction="in"/>
<pin name="IN4" direction="in"/>
<pin name="IN5" direction="in"/>
<pin name="IN6" direction="in"/>
<pin name="IN7" direction="in"/>
<pin name="AGND" direction="pas"/>
<pin name="DGND" direction="pas"/>
<pin name="DOUT" direction="out"/>
</symbol>
<symbol name="ADC088S102CIMT">
<pin name="VA" direction="pwr"/>
<pin name="VD" direction="pwr"/>
<pin name="SCLK" direction="in"/>
<pin name="~CS" direction="in"/>
<pin name="IN0" direction="in"/>
<pin name="IN1" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="IN3" direction="in"/>
<pin name="IN4" direction="in"/>
<pin name="IN5" direction="in"/>
<pin name="IN6" direction="in"/>
<pin name="IN7" direction="in"/>
<pin name="DIN" direction="in"/>
<pin name="AGND" direction="pas"/>
<pin name="DGND" direction="pas"/>
<pin name="DOUT" direction="out"/>
</symbol>
<symbol name="ADC08D1000CIYB">
<pin name="VA_2" direction="pwr"/>
<pin name="VA_3" direction="pwr"/>
<pin name="VA_4" direction="pwr"/>
<pin name="VA_5" direction="pwr"/>
<pin name="VA_6" direction="pwr"/>
<pin name="VA_7" direction="pwr"/>
<pin name="VA_8" direction="pwr"/>
<pin name="VA_9" direction="pwr"/>
<pin name="VA_10" direction="pwr"/>
<pin name="VA_11" direction="pwr"/>
<pin name="VA" direction="pwr"/>
<pin name="VCMO" direction="in"/>
<pin name="CAL" direction="in"/>
<pin name="VBG" direction="in"/>
<pin name="PD" direction="in"/>
<pin name="REXT" direction="in"/>
<pin name="CALRUN" direction="in"/>
<pin name="FSR/ECE" direction="in"/>
<pin name="CALDLY/DES/~SCS" direction="in"/>
<pin name="DCLK_RST" direction="in"/>
<pin name="CLK+" direction="in"/>
<pin name="CLK-" direction="in"/>
<pin name="DCLK-" direction="in"/>
<pin name="DCLK+" direction="in"/>
<pin name="VDR_2" direction="in"/>
<pin name="VDR_3" direction="in"/>
<pin name="VDR_4" direction="in"/>
<pin name="VDR_5" direction="in"/>
<pin name="VDR_6" direction="in"/>
<pin name="VDR_7" direction="in"/>
<pin name="VDR_8" direction="in"/>
<pin name="VDR" direction="in"/>
<pin name="TDIODE_P" direction="in"/>
<pin name="TDIODE_N" direction="in"/>
<pin name="VIN-" direction="in"/>
<pin name="VIN+" direction="in"/>
<pin name="VINQ+" direction="in"/>
<pin name="VINQ-" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="DR_GND_2" direction="pas"/>
<pin name="DR_GND_3" direction="pas"/>
<pin name="DR_GND_4" direction="pas"/>
<pin name="DR_GND_5" direction="pas"/>
<pin name="DR_GND_6" direction="pas"/>
<pin name="DR_GND_7" direction="pas"/>
<pin name="DR_GND_8" direction="pas"/>
<pin name="DR_GND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="OUTV/SCLK" direction="out"/>
<pin name="OUT_EDGE/DDR/SDATA" direction="out"/>
<pin name="OR+" direction="out"/>
<pin name="OR-" direction="out"/>
<pin name="DI0-" direction="out"/>
<pin name="DI0+" direction="out"/>
<pin name="DI1-" direction="out"/>
<pin name="DI1+" direction="out"/>
<pin name="DI2-" direction="out"/>
<pin name="DI2+" direction="out"/>
<pin name="DI3-" direction="out"/>
<pin name="DI3+" direction="out"/>
<pin name="DI4-" direction="out"/>
<pin name="DI4+" direction="out"/>
<pin name="DI5-" direction="out"/>
<pin name="DI5+" direction="out"/>
<pin name="DI6-" direction="out"/>
<pin name="DI6+" direction="out"/>
<pin name="DI7-" direction="out"/>
<pin name="DI7+" direction="out"/>
<pin name="DID0-" direction="out"/>
<pin name="DID0+" direction="out"/>
<pin name="DID1-" direction="out"/>
<pin name="DID1+" direction="out"/>
<pin name="DID2-" direction="out"/>
<pin name="DID2+" direction="out"/>
<pin name="DID3-" direction="out"/>
<pin name="DID3+" direction="out"/>
<pin name="DID4-" direction="out"/>
<pin name="DID4+" direction="out"/>
<pin name="DID5-" direction="out"/>
<pin name="DID5+" direction="out"/>
<pin name="DID6-" direction="out"/>
<pin name="DID6+" direction="out"/>
<pin name="DID7-" direction="out"/>
<pin name="DID7+" direction="out"/>
<pin name="DQD0+" direction="out"/>
<pin name="DQD0-" direction="out"/>
<pin name="DQD1+" direction="out"/>
<pin name="DQD1-" direction="out"/>
<pin name="DQD2+" direction="out"/>
<pin name="DQD2-" direction="out"/>
<pin name="DQD3+" direction="out"/>
<pin name="DQD3-" direction="out"/>
<pin name="DQD4+" direction="out"/>
<pin name="DQD4-" direction="out"/>
<pin name="DQD5+" direction="out"/>
<pin name="DQD5-" direction="out"/>
<pin name="DQD6+" direction="out"/>
<pin name="DQD6-" direction="out"/>
<pin name="DQD7+" direction="out"/>
<pin name="DQD7-" direction="out"/>
<pin name="DQ0+" direction="out"/>
<pin name="DQ0-" direction="out"/>
<pin name="DQ1-" direction="out"/>
<pin name="DQ1+" direction="out"/>
<pin name="DQ2+" direction="out"/>
<pin name="DQ2-" direction="out"/>
<pin name="DQ3+" direction="out"/>
<pin name="DQ3-" direction="out"/>
<pin name="DQ4+" direction="out"/>
<pin name="DQ4-" direction="out"/>
<pin name="DQ5+" direction="out"/>
<pin name="DQ5-" direction="out"/>
<pin name="DQ6+" direction="out"/>
<pin name="DQ6-" direction="out"/>
<pin name="DQ7+" direction="out"/>
<pin name="DQ7-" direction="out"/>
<pin name="PDQ" direction="in"/>
</symbol>
<symbol name="ADC08D1500CIYB">
<pin name="VA_2" direction="pwr"/>
<pin name="VA_3" direction="pwr"/>
<pin name="VA_4" direction="pwr"/>
<pin name="VA_5" direction="pwr"/>
<pin name="VA_6" direction="pwr"/>
<pin name="VA_7" direction="pwr"/>
<pin name="VA_8" direction="pwr"/>
<pin name="VA_9" direction="pwr"/>
<pin name="VA_10" direction="pwr"/>
<pin name="VA_11" direction="pwr"/>
<pin name="VA" direction="pwr"/>
<pin name="VCMO" direction="in"/>
<pin name="CAL" direction="in"/>
<pin name="VBG" direction="in"/>
<pin name="PD" direction="in"/>
<pin name="REXT" direction="in"/>
<pin name="CALRUN" direction="in"/>
<pin name="FSR/ECE" direction="in"/>
<pin name="CALDLY/DES/~SCS" direction="in"/>
<pin name="DCLK_RST" direction="in"/>
<pin name="CLK+" direction="in"/>
<pin name="CLK-" direction="in"/>
<pin name="DCLK-" direction="in"/>
<pin name="DCLK+" direction="in"/>
<pin name="VDR_2" direction="in"/>
<pin name="VDR_3" direction="in"/>
<pin name="VDR_4" direction="in"/>
<pin name="VDR_5" direction="in"/>
<pin name="VDR_6" direction="in"/>
<pin name="VDR_7" direction="in"/>
<pin name="VDR_8" direction="in"/>
<pin name="VDR" direction="in"/>
<pin name="TDIODE_P" direction="in"/>
<pin name="TDIODE_N" direction="in"/>
<pin name="VINI-" direction="in"/>
<pin name="VINI+" direction="in"/>
<pin name="VINQ+" direction="in"/>
<pin name="VINQ-" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="DR_GND_2" direction="pas"/>
<pin name="DR_GND_3" direction="pas"/>
<pin name="DR_GND_4" direction="pas"/>
<pin name="DR_GND_5" direction="pas"/>
<pin name="DR_GND_6" direction="pas"/>
<pin name="DR_GND_7" direction="pas"/>
<pin name="DR_GND_8" direction="pas"/>
<pin name="DR_GND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="OUTV/SCLK" direction="out"/>
<pin name="OUT_EDGE/DDR/SDATA" direction="out"/>
<pin name="OR+" direction="out"/>
<pin name="OR-" direction="out"/>
<pin name="DI0-" direction="out"/>
<pin name="DI0+" direction="out"/>
<pin name="DI1-" direction="out"/>
<pin name="DI1+" direction="out"/>
<pin name="DI2-" direction="out"/>
<pin name="DI2+" direction="out"/>
<pin name="DI3-" direction="out"/>
<pin name="DI3+" direction="out"/>
<pin name="DI4-" direction="out"/>
<pin name="DI4+" direction="out"/>
<pin name="DI5-" direction="out"/>
<pin name="DI5+" direction="out"/>
<pin name="DI6-" direction="out"/>
<pin name="DI6+" direction="out"/>
<pin name="DI7-" direction="out"/>
<pin name="DI7+" direction="out"/>
<pin name="DID0-" direction="out"/>
<pin name="DID0+" direction="out"/>
<pin name="DID1-" direction="out"/>
<pin name="DID1+" direction="out"/>
<pin name="DID2-" direction="out"/>
<pin name="DID2+" direction="out"/>
<pin name="DID3-" direction="out"/>
<pin name="DID3+" direction="out"/>
<pin name="DID4-" direction="out"/>
<pin name="DID4+" direction="out"/>
<pin name="DID5-" direction="out"/>
<pin name="DID5+" direction="out"/>
<pin name="DID6-" direction="out"/>
<pin name="DID6+" direction="out"/>
<pin name="DID7-" direction="out"/>
<pin name="DID7+" direction="out"/>
<pin name="DQD0+" direction="out"/>
<pin name="DQD0-" direction="out"/>
<pin name="DQD1+" direction="out"/>
<pin name="DQD1-" direction="out"/>
<pin name="DQD2+" direction="out"/>
<pin name="DQD2-" direction="out"/>
<pin name="DQD3+" direction="out"/>
<pin name="DQD3-" direction="out"/>
<pin name="DQD4+" direction="out"/>
<pin name="DQD4-" direction="out"/>
<pin name="DQD5+" direction="out"/>
<pin name="DQD5-" direction="out"/>
<pin name="DQD6+" direction="out"/>
<pin name="DQD6-" direction="out"/>
<pin name="DQD7+" direction="out"/>
<pin name="DQD7-" direction="out"/>
<pin name="DQ0+" direction="out"/>
<pin name="DQ0-" direction="out"/>
<pin name="DQ1-" direction="out"/>
<pin name="DQ1+" direction="out"/>
<pin name="DQ2+" direction="out"/>
<pin name="DQ2-" direction="out"/>
<pin name="DQ3+" direction="out"/>
<pin name="DQ3-" direction="out"/>
<pin name="DQ4+" direction="out"/>
<pin name="DQ4-" direction="out"/>
<pin name="DQ5+" direction="out"/>
<pin name="DQ5-" direction="out"/>
<pin name="DQ6+" direction="out"/>
<pin name="DQ6-" direction="out"/>
<pin name="DQ7+" direction="out"/>
<pin name="DQ7-" direction="out"/>
<pin name="PDQ" direction="in"/>
</symbol>
<symbol name="ADC08D500CIYB">
<pin name="VA_2" direction="pwr"/>
<pin name="VA_3" direction="pwr"/>
<pin name="VA_4" direction="pwr"/>
<pin name="VA_5" direction="pwr"/>
<pin name="VA_6" direction="pwr"/>
<pin name="VA_7" direction="pwr"/>
<pin name="VA_8" direction="pwr"/>
<pin name="VA_9" direction="pwr"/>
<pin name="VA_10" direction="pwr"/>
<pin name="VA_11" direction="pwr"/>
<pin name="VA" direction="pwr"/>
<pin name="VCMO" direction="in"/>
<pin name="CAL" direction="in"/>
<pin name="VBG" direction="in"/>
<pin name="PD" direction="in"/>
<pin name="REXT" direction="in"/>
<pin name="CALRUN" direction="in"/>
<pin name="FSR/ECE" direction="in"/>
<pin name="CALDLY/DES/~SCS" direction="in"/>
<pin name="DCLK_RST" direction="in"/>
<pin name="CLK+" direction="in"/>
<pin name="CLK-" direction="in"/>
<pin name="DCLK-" direction="in"/>
<pin name="DCLK+" direction="in"/>
<pin name="VDR_2" direction="in"/>
<pin name="VDR_3" direction="in"/>
<pin name="VDR_4" direction="in"/>
<pin name="VDR_5" direction="in"/>
<pin name="VDR_6" direction="in"/>
<pin name="VDR_7" direction="in"/>
<pin name="VDR_8" direction="in"/>
<pin name="VDR" direction="in"/>
<pin name="TDIODE_P" direction="in"/>
<pin name="TDIODE_N" direction="in"/>
<pin name="VINI-" direction="in"/>
<pin name="VINI+" direction="in"/>
<pin name="VINQ+" direction="in"/>
<pin name="VINQ-" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="DR_GND_2" direction="pas"/>
<pin name="DR_GND_3" direction="pas"/>
<pin name="DR_GND_4" direction="pas"/>
<pin name="DR_GND_5" direction="pas"/>
<pin name="DR_GND_6" direction="pas"/>
<pin name="DR_GND_7" direction="pas"/>
<pin name="DR_GND_8" direction="pas"/>
<pin name="DR_GND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="OUTV/SCLK" direction="out"/>
<pin name="OUT_EDGE/DDR/SDATA" direction="out"/>
<pin name="OR+" direction="out"/>
<pin name="OR-" direction="out"/>
<pin name="DI0-" direction="out"/>
<pin name="DI0+" direction="out"/>
<pin name="DI1-" direction="out"/>
<pin name="DI1+" direction="out"/>
<pin name="DI2-" direction="out"/>
<pin name="DI2+" direction="out"/>
<pin name="DI3-" direction="out"/>
<pin name="DI3+" direction="out"/>
<pin name="DI4-" direction="out"/>
<pin name="DI4+" direction="out"/>
<pin name="DI5-" direction="out"/>
<pin name="DI5+" direction="out"/>
<pin name="DI6-" direction="out"/>
<pin name="DI6+" direction="out"/>
<pin name="DI7-" direction="out"/>
<pin name="DI7+" direction="out"/>
<pin name="DID0-" direction="out"/>
<pin name="DID0+" direction="out"/>
<pin name="DID1-" direction="out"/>
<pin name="DID1+" direction="out"/>
<pin name="DID2-" direction="out"/>
<pin name="DID2+" direction="out"/>
<pin name="DID3-" direction="out"/>
<pin name="DID3+" direction="out"/>
<pin name="DID4-" direction="out"/>
<pin name="DID4+" direction="out"/>
<pin name="DID5-" direction="out"/>
<pin name="DID5+" direction="out"/>
<pin name="DID6-" direction="out"/>
<pin name="DID6+" direction="out"/>
<pin name="DID7-" direction="out"/>
<pin name="DID7+" direction="out"/>
<pin name="DQD0+" direction="out"/>
<pin name="DQD0-" direction="out"/>
<pin name="DQD1+" direction="out"/>
<pin name="DQD1-" direction="out"/>
<pin name="DQD2+" direction="out"/>
<pin name="DQD2-" direction="out"/>
<pin name="DQD3+" direction="out"/>
<pin name="DQD3-" direction="out"/>
<pin name="DQD4+" direction="out"/>
<pin name="DQD4-" direction="out"/>
<pin name="DQD5+" direction="out"/>
<pin name="DQD5-" direction="out"/>
<pin name="DQD6+" direction="out"/>
<pin name="DQD6-" direction="out"/>
<pin name="DQD7+" direction="out"/>
<pin name="DQD7-" direction="out"/>
<pin name="DQ0+" direction="out"/>
<pin name="DQ0-" direction="out"/>
<pin name="DQ1-" direction="out"/>
<pin name="DQ1+" direction="out"/>
<pin name="DQ2+" direction="out"/>
<pin name="DQ2-" direction="out"/>
<pin name="DQ3+" direction="out"/>
<pin name="DQ3-" direction="out"/>
<pin name="DQ4+" direction="out"/>
<pin name="DQ4-" direction="out"/>
<pin name="DQ5+" direction="out"/>
<pin name="DQ5-" direction="out"/>
<pin name="DQ6+" direction="out"/>
<pin name="DQ6-" direction="out"/>
<pin name="DQ7+" direction="out"/>
<pin name="DQ7-" direction="out"/>
<pin name="PDQ" direction="in"/>
</symbol>
<symbol name="ADC08L060CIMT">
<pin name="VA_2" direction="pwr"/>
<pin name="VA_3" direction="pwr"/>
<pin name="VA" direction="pwr"/>
<pin name="DR_VD" direction="pas"/>
<pin name="VIN" direction="in"/>
<pin name="PD" direction="in"/>
<pin name="CLOCK" direction="in"/>
<pin name="VRM" direction="pas"/>
<pin name="VRT" direction="in"/>
<pin name="VRB" direction="in"/>
<pin name="AGND_2" direction="pas"/>
<pin name="AGND_3" direction="pas"/>
<pin name="AGND_4" direction="pas"/>
<pin name="AGND" direction="pas"/>
<pin name="VIN_GND" direction="pas"/>
<pin name="DR_GND" direction="pas"/>
<pin name="D0" direction="out"/>
<pin name="D1" direction="out"/>
<pin name="D2" direction="out"/>
<pin name="D3" direction="out"/>
<pin name="D4" direction="out"/>
<pin name="D5" direction="out"/>
<pin name="D6" direction="out"/>
<pin name="D7" direction="out"/>
</symbol>
<symbol name="ADC10064CIWM">
<pin name="AVCC" direction="pwr"/>
<pin name="DVCC" direction="pwr"/>
<pin name="~CS" direction="in"/>
<pin name="S0" direction="in"/>
<pin name="S1" direction="in"/>
<pin name="VREF-" direction="in"/>
<pin name="VREF+" direction="in"/>
<pin name="VIN0" direction="in"/>
<pin name="VIN1" direction="in"/>
<pin name="VIN2" direction="in"/>
<pin name="VIN3" direction="in"/>
<pin name="~S/H" direction="in"/>
<pin name="~RD" direction="in"/>
<pin name="SPEED_ADJ" direction="pas"/>
<pin name="N.C." direction="nc"/>
<pin name="AGND" direction="pas"/>
<pin name="DGND" direction="pas"/>
<pin name="~INT" direction="out"/>
<pin name="DB0" direction="out"/>
<pin name="DB1" direction="out"/>
<pin name="DB2" direction="out"/>
<pin name="DB3" direction="out"/>
<pin name="DB4" direction="out"/>
<pin name="DB5" direction="out"/>
<pin name="DB6" direction="out"/>
<pin name="DB7" direction="out"/>
<pin name="DB8" direction="out"/>
<pin name="DB9" direction="out"/>
</symbol>
<symbol name="ADC10065CIMT">
<pin name="VDDA_2" direction="pwr"/>
<pin name="VDDA_3" direction="pwr"/>
<pin name="VDDA" direction="pwr"/>
<pin name="VDDIO" direction="pwr"/>
<pin name="CLK" direction="pas"/>
<pin name="IRS" direction="pas"/>
<pin name="VCOM" direction="pas"/>
<pin name="VREF" direction="in"/>
<pin name="VREFT" direction="in"/>
<pin name="VREFB" direction="in"/>
<pin name="VIN-" direction="in"/>
<pin name="VIN+" direction="in"/>
<pin name="DF" direction="in"/>
<pin name="STDBY" direction="pas"/>
<pin name="VSSA_2" direction="pas"/>
<pin name="VSSA_3" direction="pas"/>
<pin name="VSSA" direction="pas"/>
<pin name="VSSIO" direction="pas"/>
<pin name="D0" direction="out"/>
<pin name="D1" direction="out"/>
<pin name="D2" direction="out"/>
<pin name="D3" direction="out"/>
<pin name="D4" direction="out"/>
<pin name="D5" direction="out"/>
<pin name="D6" direction="out"/>
<pin name="D7" direction="out"/>
<pin name="D8" direction="out"/>
<pin name="D9" direction="out"/>
</symbol>
<symbol name="ADC10080CIMT">
<pin name="VDDA_2" direction="pwr"/>
<pin name="VDDA_3" direction="pwr"/>
<pin name="VDDA" direction="pwr"/>
<pin name="VDDIO" direction="pwr"/>
<pin name="CLK" direction="in"/>
<pin name="VCOM" direction="in"/>
<pin name="IRS" direction="in"/>
<pin name="DF" direction="in"/>
<pin name="VREF" direction="in"/>
<pin name="STDBY" direction="in"/>
<pin name="VREFT" direction="in"/>
<pin name="VREFB" direction="in"/>
<pin name="VIN-" direction="in"/>
<pin name="VIN+" direction="in"/>
<pin name="VSSA_2" direction="pas"/>
<pin name="VSSA_3" direction="pas"/>
<pin name="VSSA" direction="pas"/>
<pin name="VSSIO" direction="pas"/>
<pin name="D0" direction="out"/>
<pin name="D1" direction="out"/>
<pin name="D2" direction="out"/>
<pin name="D3" direction="out"/>
<pin name="D4" direction="out"/>
<pin name="D5" direction="out"/>
<pin name="D6" direction="out"/>
<pin name="D7" direction="out"/>
<pin name="D8" direction="out"/>
<pin name="D9" direction="out"/>
</symbol>
<symbol name="ADC10154CIWM">
<pin name="DV+" direction="pwr"/>
<pin name="AV+" direction="pwr"/>
<pin name="~CS" direction="in"/>
<pin name="CLK" direction="in"/>
<pin name="~RD" direction="in"/>
<pin name="~WR" direction="in"/>
<pin name="CH0" direction="in"/>
<pin name="CH1" direction="in"/>
<pin name="CH2" direction="in"/>
<pin name="CH3" direction="in"/>
<pin name="VREF_OUT" direction="pas"/>
<pin name="VREF+" direction="in"/>
<pin name="VREF-" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="DGND" direction="pas"/>
<pin name="~INT" direction="out"/>
<pin name="DB0" direction="out"/>
<pin name="DB1" direction="out"/>
<pin name="DB2" direction="out"/>
<pin name="DB3" direction="out"/>
<pin name="DB4" direction="out"/>
<pin name="DB5" direction="out"/>
<pin name="DB6" direction="out"/>
<pin name="DB7" direction="out"/>
</symbol>
<symbol name="ADC10158CIWM">
<pin name="AV+" direction="pwr"/>
<pin name="DV+" direction="pwr"/>
<pin name="VREF+" direction="in"/>
<pin name="VREF-" direction="in"/>
<pin name="CLK" direction="in"/>
<pin name="~WR" direction="in"/>
<pin name="~RD" direction="in"/>
<pin name="~CS" direction="in"/>
<pin name="CH0" direction="in"/>
<pin name="CH1" direction="in"/>
<pin name="CH2" direction="in"/>
<pin name="CH3" direction="in"/>
<pin name="CH4" direction="in"/>
<pin name="CH5" direction="in"/>
<pin name="CH6" direction="in"/>
<pin name="CH7" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="DGND" direction="pas"/>
<pin name="~INT" direction="out"/>
<pin name="VREFOUT" direction="out"/>
<pin name="DB0(MA0)"/>
<pin name="DB1(MA1)"/>
<pin name="DB2(MA2)"/>
<pin name="DB3(MA3)"/>
<pin name="DB4(MA4)"/>
<pin name="DB5(U/~S)"/>
<pin name="DB6(8/~10)"/>
<pin name="DB7(L/~R)"/>
</symbol>
<symbol name="ADC101S021CIMF">
<pin name="VA" direction="pwr"/>
<pin name="SCLK" direction="in"/>
<pin name="~CS" direction="in"/>
<pin name="VIN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="SDATA" direction="out"/>
</symbol>
<symbol name="ADC101S021CISD">
<pin name="VA" direction="pwr"/>
<pin name="SCLK" direction="in"/>
<pin name="~CS" direction="in"/>
<pin name="VIN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="SDATA" direction="out"/>
</symbol>
<symbol name="ADC101S051CIMF">
<pin name="VA" direction="pwr"/>
<pin name="VIN" direction="in"/>
<pin name="SCLK" direction="in"/>
<pin name="~CS" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="SDATA" direction="out"/>
</symbol>
<symbol name="ADC101S051CISD">
<pin name="VA" direction="pwr"/>
<pin name="SCLK" direction="in"/>
<pin name="~CS" direction="in"/>
<pin name="VIN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="SDATA" direction="out"/>
</symbol>
<symbol name="ADC101S101CIMF">
<pin name="VDD" direction="pwr"/>
<pin name="VIN" direction="in"/>
<pin name="SCLK" direction="in"/>
<pin name="~CS" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="SDATA" direction="out"/>
</symbol>
<symbol name="ADC102S021CIMM">
<pin name="VA" direction="pwr"/>
<pin name="SCLK" direction="in"/>
<pin name="~CS" direction="in"/>
<pin name="DIN" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="IN1" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="DOUT" direction="out"/>
</symbol>
<symbol name="ADC102S101CIMM">
<pin name="VA" direction="pwr"/>
<pin name="SCLK" direction="in"/>
<pin name="~CS" direction="in"/>
<pin name="DIN" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="IN1" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="DOUT" direction="out"/>
</symbol>
<symbol name="ADC104S021CIMM">
<pin name="VA" direction="pwr"/>
<pin name="~CS" direction="in"/>
<pin name="SCLK" direction="in"/>
<pin name="DIN" direction="in"/>
<pin name="IN1" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="IN3" direction="in"/>
<pin name="IN4" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="DOUT" direction="out"/>
</symbol>
<symbol name="ADC104S051CIMM">
<pin name="VA" direction="pwr"/>
<pin name="~CS" direction="in"/>
<pin name="SCLK" direction="in"/>
<pin name="DIN" direction="in"/>
<pin name="IN1" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="IN3" direction="in"/>
<pin name="IN4" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="DOUT" direction="out"/>
</symbol>
<symbol name="ADC104S101CIMM">
<pin name="VA" direction="pwr"/>
<pin name="~CS" direction="in"/>
<pin name="SCLK" direction="in"/>
<pin name="DIN" direction="in"/>
<pin name="IN1" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="IN3" direction="in"/>
<pin name="IN4" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="DOUT" direction="out"/>
</symbol>
<symbol name="ADC10664CIWM">
<pin name="D_VCC" direction="pwr"/>
<pin name="AVCC" direction="pwr"/>
<pin name="SPEED_ADJ" direction="in"/>
<pin name="~S/H" direction="in"/>
<pin name="~RD" direction="in"/>
<pin name="~CS" direction="in"/>
<pin name="S0" direction="in"/>
<pin name="S1" direction="in"/>
<pin name="VREF-" direction="in"/>
<pin name="VREF+" direction="in"/>
<pin name="VIN0" direction="in"/>
<pin name="VIN1" direction="in"/>
<pin name="VIN2" direction="in"/>
<pin name="VIN3" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="AGND" direction="pas"/>
<pin name="DGND" direction="pas"/>
<pin name="~INT" direction="out"/>
<pin name="DB0" direction="out"/>
<pin name="DB1" direction="out"/>
<pin name="DB2" direction="out"/>
<pin name="DB3" direction="out"/>
<pin name="DB4" direction="out"/>
<pin name="DB5" direction="out"/>
<pin name="DB6" direction="out"/>
<pin name="DB7" direction="out"/>
<pin name="DB8" direction="out"/>
<pin name="DB9" direction="out"/>
</symbol>
<symbol name="ADC10738CIWM">
<pin name="DV+" direction="pwr"/>
<pin name="AV+" direction="pwr"/>
<pin name="CH0" direction="in"/>
<pin name="CH1" direction="in"/>
<pin name="CH2" direction="in"/>
<pin name="CH3" direction="in"/>
<pin name="CH4" direction="in"/>
<pin name="CH5" direction="in"/>
<pin name="CH6" direction="in"/>
<pin name="CH7" direction="in"/>
<pin name="VREF+" direction="in"/>
<pin name="VREF-" direction="in"/>
<pin name="SARS" direction="pas"/>
<pin name="CLK" direction="in"/>
<pin name="DI" direction="in"/>
<pin name="~CS" direction="in"/>
<pin name="VREF_OUT" direction="pas"/>
<pin name="COM" direction="in"/>
<pin name="PD" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="DGND" direction="pas"/>
<pin name="AGND" direction="pas"/>
<pin name="DO" direction="out"/>
</symbol>
<symbol name="ADC108S022CIMT">
<pin name="VA" direction="pwr"/>
<pin name="VD" direction="pwr"/>
<pin name="~CS" direction="in"/>
<pin name="DIN" direction="in"/>
<pin name="SCLK" direction="in"/>
<pin name="IN0" direction="in"/>
<pin name="IN1" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="IN3" direction="in"/>
<pin name="IN4" direction="in"/>
<pin name="IN5" direction="in"/>
<pin name="IN6" direction="in"/>
<pin name="IN7" direction="in"/>
<pin name="AGND" direction="pas"/>
<pin name="DGND" direction="pas"/>
<pin name="DOUT" direction="out"/>
</symbol>
<symbol name="ADC108S052CIMT">
<pin name="VA" direction="pwr"/>
<pin name="VD" direction="pwr"/>
<pin name="~CS" direction="in"/>
<pin name="DIN" direction="in"/>
<pin name="SCLK" direction="in"/>
<pin name="IN0" direction="in"/>
<pin name="IN1" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="IN3" direction="in"/>
<pin name="IN4" direction="in"/>
<pin name="IN5" direction="in"/>
<pin name="IN6" direction="in"/>
<pin name="IN7" direction="in"/>
<pin name="AGND" direction="pas"/>
<pin name="DGND" direction="pas"/>
<pin name="DOUT" direction="out"/>
</symbol>
<symbol name="ADC108S102CIMT">
<pin name="VA" direction="pwr"/>
<pin name="VD" direction="pwr"/>
<pin name="~CS" direction="in"/>
<pin name="DIN" direction="in"/>
<pin name="SCLK" direction="in"/>
<pin name="IN0" direction="in"/>
<pin name="IN1" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="IN3" direction="in"/>
<pin name="IN4" direction="in"/>
<pin name="IN5" direction="in"/>
<pin name="IN6" direction="in"/>
<pin name="IN7" direction="in"/>
<pin name="AGND" direction="pas"/>
<pin name="DGND" direction="pas"/>
<pin name="DOUT" direction="out"/>
</symbol>
<symbol name="ADC10D020CIVS">
<pin name="VA_2" direction="pwr"/>
<pin name="VA" direction="pwr"/>
<pin name="VD" direction="pwr"/>
<pin name="VDR_2" direction="pwr"/>
<pin name="VDR" direction="pwr"/>
<pin name="VREF" direction="in"/>
<pin name="OS" direction="in"/>
<pin name="OC" direction="in"/>
<pin name="OF" direction="in"/>
<pin name="CLK" direction="in"/>
<pin name="PD" direction="in"/>
<pin name="STDBY" direction="in"/>
<pin name="GAIN" direction="in"/>
<pin name="Q+" direction="in"/>
<pin name="Q-" direction="in"/>
<pin name="I-" direction="in"/>
<pin name="I+" direction="in"/>
<pin name="VRP" direction="pas"/>
<pin name="VRN" direction="pas"/>
<pin name="VCMO" direction="pas"/>
<pin name="DR_GND_2" direction="pas"/>
<pin name="DR_GND" direction="pas"/>
<pin name="AGND_2" direction="pas"/>
<pin name="AGND_3" direction="pas"/>
<pin name="DGND" direction="pas"/>
<pin name="AGND_4" direction="pas"/>
<pin name="AGND" direction="pas"/>
<pin name="I/~Q" direction="out"/>
<pin name="I0" direction="out"/>
<pin name="I1" direction="out"/>
<pin name="I2" direction="out"/>
<pin name="I3" direction="out"/>
<pin name="I4" direction="out"/>
<pin name="I5" direction="out"/>
<pin name="I6" direction="out"/>
<pin name="I7" direction="out"/>
<pin name="I8" direction="out"/>
<pin name="I9" direction="out"/>
<pin name="Q0" direction="out"/>
<pin name="Q1" direction="out"/>
<pin name="Q2" direction="out"/>
<pin name="Q3" direction="out"/>
<pin name="Q4" direction="out"/>
<pin name="Q5" direction="out"/>
<pin name="Q6" direction="out"/>
<pin name="Q7" direction="out"/>
<pin name="Q8" direction="out"/>
<pin name="Q9" direction="out"/>
</symbol>
<symbol name="ADC10D040CIVS">
<pin name="VA_2" direction="pwr"/>
<pin name="VA" direction="pwr"/>
<pin name="VD" direction="pwr"/>
<pin name="VDR_2" direction="pwr"/>
<pin name="VDR" direction="pwr"/>
<pin name="CLK" direction="in"/>
<pin name="PD" direction="pwr"/>
<pin name="VREF" direction="in"/>
<pin name="VRP" direction="pas"/>
<pin name="OS" direction="in"/>
<pin name="VRN" direction="pas"/>
<pin name="OC" direction="pas"/>
<pin name="STBY" direction="pwr"/>
<pin name="GAIN" direction="in"/>
<pin name="Q+" direction="in"/>
<pin name="Q-" direction="in"/>
<pin name="I-" direction="in"/>
<pin name="I+" direction="in"/>
<pin name="AGND_2" direction="pas"/>
<pin name="AGND_3" direction="pas"/>
<pin name="DGND" direction="pas"/>
<pin name="AGND_4" direction="pas"/>
<pin name="AGND" direction="pas"/>
<pin name="DR_GND_2" direction="pas"/>
<pin name="DR_GND" direction="pas"/>
<pin name="I0" direction="out"/>
<pin name="I1" direction="out"/>
<pin name="I2" direction="out"/>
<pin name="I3" direction="out"/>
<pin name="I4" direction="out"/>
<pin name="I5" direction="out"/>
<pin name="I6" direction="out"/>
<pin name="I7" direction="out"/>
<pin name="I8" direction="out"/>
<pin name="I9" direction="out"/>
<pin name="Q0" direction="out"/>
<pin name="Q1" direction="out"/>
<pin name="Q2" direction="out"/>
<pin name="Q3" direction="out"/>
<pin name="Q4" direction="out"/>
<pin name="Q5" direction="out"/>
<pin name="Q6" direction="out"/>
<pin name="Q7" direction="out"/>
<pin name="Q8" direction="out"/>
<pin name="Q9" direction="out"/>
<pin name="I/~Q" direction="out"/>
<pin name="OF" direction="pas"/>
<pin name="VCMO" direction="out"/>
</symbol>
<symbol name="ADC10D1000CCMLS_1">
<pin name="VA_2" direction="pwr"/>
<pin name="VA_3" direction="pwr"/>
<pin name="VA_4" direction="pwr"/>
<pin name="VA_5" direction="pwr"/>
<pin name="VA_6" direction="pwr"/>
<pin name="VA_7" direction="pwr"/>
<pin name="VA_8" direction="pwr"/>
<pin name="VDR_2" direction="pwr"/>
<pin name="VDR_3" direction="pwr"/>
<pin name="VDR_4" direction="pwr"/>
<pin name="VDR_5" direction="pwr"/>
<pin name="VDR_6" direction="pwr"/>
<pin name="VDR" direction="pwr"/>
<pin name="VA_9" direction="pwr"/>
<pin name="VA" direction="pwr"/>
<pin name="VBG" direction="pwr"/>
<pin name="VE_2" direction="pwr"/>
<pin name="VE_3" direction="pwr"/>
<pin name="VE" direction="pwr"/>
<pin name="SCLK" direction="in"/>
<pin name="SDI" direction="in"/>
<pin name="SDO" direction="out"/>
<pin name="DI0+" direction="out"/>
<pin name="DI0-" direction="out"/>
<pin name="DI1+" direction="out"/>
<pin name="DI1-" direction="out"/>
<pin name="DI2+" direction="out"/>
<pin name="DI2-" direction="out"/>
<pin name="DI3+" direction="out"/>
<pin name="DI3-" direction="out"/>
<pin name="DI4+" direction="out"/>
<pin name="RTRIM+" direction="pas"/>
<pin name="REXT+" direction="pas"/>
<pin name="RTRIM-" direction="pas"/>
<pin name="REXT-" direction="pas"/>
<pin name="TPM" direction="in"/>
<pin name="~ECE" direction="in"/>
<pin name="NDM" direction="in"/>
<pin name="~SCSB" direction="in"/>
<pin name="CAL" direction="in"/>
<pin name="VBIASI_2" direction="pwr"/>
<pin name="VBIASI" direction="pwr"/>
<pin name="VBIASQ" direction="pwr"/>
<pin name="CALRUN" direction="out"/>
<pin name="GNDE_2" direction="pas"/>
<pin name="GNDE_3" direction="pas"/>
<pin name="GNDE" direction="pas"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GNDTC" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDDR_2" direction="pas"/>
<pin name="GNDDR_3" direction="pas"/>
<pin name="GNDDR_4" direction="pas"/>
<pin name="GNDDR_5" direction="pas"/>
<pin name="GNDDR_6" direction="pas"/>
<pin name="GNDDR_7" direction="pas"/>
<pin name="GNDDR_8" direction="pas"/>
<pin name="GNDDR_9" direction="pas"/>
<pin name="GNDDR_10" direction="pas"/>
<pin name="GNDDR_11" direction="pas"/>
<pin name="GNDDR_12" direction="pas"/>
<pin name="GNDDR_13" direction="pas"/>
<pin name="GNDDR_14" direction="pas"/>
<pin name="GNDDR_15" direction="pas"/>
<pin name="GNDDR" direction="pas"/>
<pin name="DID0+" direction="out"/>
<pin name="DID0-" direction="out"/>
<pin name="DID1+" direction="out"/>
<pin name="DID1-" direction="out"/>
<pin name="DID2+" direction="out"/>
<pin name="DID2-" direction="out"/>
<pin name="DID3+" direction="out"/>
<pin name="DID3-" direction="out"/>
<pin name="DID4+" direction="out"/>
<pin name="DID4-" direction="out"/>
<pin name="DID5+" direction="out"/>
<pin name="DID5-" direction="out"/>
<pin name="DID6+" direction="out"/>
<pin name="DID6-" direction="out"/>
<pin name="DID7+" direction="out"/>
<pin name="DID7-" direction="out"/>
<pin name="DID8+" direction="out"/>
<pin name="DID8-" direction="out"/>
<pin name="DID9+" direction="out"/>
<pin name="DID9-" direction="out"/>
<pin name="TDIODE+" direction="pas"/>
<pin name="TDIODE-" direction="pas"/>
</symbol>
<symbol name="ADC10D1000CCMLS_2">
<pin name="VINI+" direction="in"/>
<pin name="VINQ+" direction="in"/>
<pin name="VINI-" direction="in"/>
<pin name="VINQ-" direction="in"/>
<pin name="VDR_2" direction="pwr"/>
<pin name="VDR_3" direction="pwr"/>
<pin name="VDR_4" direction="pwr"/>
<pin name="VDR_5" direction="pwr"/>
<pin name="VDR_6" direction="pwr"/>
<pin name="VDR" direction="pwr"/>
<pin name="VTC_2" direction="pwr"/>
<pin name="VTC_3" direction="pwr"/>
<pin name="VTC_4" direction="pwr"/>
<pin name="VTC_5" direction="pwr"/>
<pin name="VTC_6" direction="pwr"/>
<pin name="VTC_7" direction="pwr"/>
<pin name="VTC_8" direction="pwr"/>
<pin name="VTC_9" direction="pwr"/>
<pin name="VTC_10" direction="pwr"/>
<pin name="VTC_11" direction="pwr"/>
<pin name="VTC_12" direction="pwr"/>
<pin name="VTC_13" direction="pwr"/>
<pin name="VTC_14" direction="pwr"/>
<pin name="VTC" direction="pwr"/>
<pin name="VA_2" direction="pwr"/>
<pin name="VA_3" direction="pwr"/>
<pin name="VA_4" direction="pwr"/>
<pin name="VA_5" direction="pwr"/>
<pin name="VA_6" direction="pwr"/>
<pin name="VA" direction="pwr"/>
<pin name="PDI" direction="in"/>
<pin name="CLK+" direction="in"/>
<pin name="DI4-" direction="out"/>
<pin name="DI5+" direction="out"/>
<pin name="DI5-" direction="out"/>
<pin name="DI6+" direction="out"/>
<pin name="DI6-" direction="out"/>
<pin name="DI7+" direction="out"/>
<pin name="DI7-" direction="out"/>
<pin name="DI8+" direction="out"/>
<pin name="DI8-" direction="out"/>
<pin name="DI9+" direction="out"/>
<pin name="DI9-" direction="out"/>
<pin name="VBIASI_2" direction="pwr"/>
<pin name="VBIASQ_2" direction="pwr"/>
<pin name="VBIASI" direction="pwr"/>
<pin name="VBIASQ_3" direction="pwr"/>
<pin name="VBIASQ" direction="pwr"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDTC_2" direction="pas"/>
<pin name="GNDTC_3" direction="pas"/>
<pin name="GNDTC_4" direction="pas"/>
<pin name="GNDTC_5" direction="pas"/>
<pin name="GNDTC_6" direction="pas"/>
<pin name="GNDTC_7" direction="pas"/>
<pin name="GNDTC_8" direction="pas"/>
<pin name="GNDTC_9" direction="pas"/>
<pin name="GNDTC_10" direction="pas"/>
<pin name="GNDTC_11" direction="pas"/>
<pin name="GNDTC_12" direction="pas"/>
<pin name="GNDTC" direction="pas"/>
<pin name="GNDDR_2" direction="pas"/>
<pin name="GNDDR_3" direction="pas"/>
<pin name="GNDDR_4" direction="pas"/>
<pin name="GNDDR" direction="pas"/>
<pin name="DCLKI+" direction="out"/>
<pin name="DCLKQ+" direction="out"/>
<pin name="DCLKI-" direction="out"/>
<pin name="DCLKQ-" direction="out"/>
<pin name="RCOUT1-" direction="out"/>
<pin name="ORI+" direction="out"/>
<pin name="ORQ+" direction="out"/>
<pin name="ORI-" direction="out"/>
<pin name="ORQ-" direction="out"/>
<pin name="DQD2-" direction="out"/>
<pin name="DQ1-" direction="out"/>
<pin name="DQ3+" direction="out"/>
<pin name="DQ3-" direction="out"/>
<pin name="DQ4+" direction="out"/>
<pin name="DQ4-" direction="out"/>
<pin name="DQ5+" direction="out"/>
<pin name="DQ5-" direction="out"/>
<pin name="DQ6+" direction="out"/>
<pin name="DQ6-" direction="out"/>
<pin name="DQ7+" direction="out"/>
<pin name="DQ7-" direction="out"/>
<pin name="DQ8+" direction="out"/>
<pin name="DQ8-" direction="out"/>
<pin name="DQ9+" direction="out"/>
<pin name="DQ9-" direction="out"/>
</symbol>
<symbol name="ADC10D1000CCMLS_3">
<pin name="VA_2" direction="pwr"/>
<pin name="VA_3" direction="pwr"/>
<pin name="VA" direction="pwr"/>
<pin name="VE_2" direction="pwr"/>
<pin name="VE_3" direction="pwr"/>
<pin name="VE" direction="pwr"/>
<pin name="VDR_2" direction="pwr"/>
<pin name="VDR_3" direction="pwr"/>
<pin name="VDR_4" direction="pwr"/>
<pin name="VDR" direction="pwr"/>
<pin name="RCLK+" direction="in"/>
<pin name="RCLK-" direction="in"/>
<pin name="PDQ" direction="in"/>
<pin name="FSR" direction="in"/>
<pin name="CLK-" direction="in"/>
<pin name="DCLK_RST+" direction="in"/>
<pin name="DCLK_RST-" direction="in"/>
<pin name="DDRPH" direction="in"/>
<pin name="RSV" direction="pas"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND_11" direction="pas"/>
<pin name="GND_12" direction="pas"/>
<pin name="GND_13" direction="pas"/>
<pin name="GND_14" direction="pas"/>
<pin name="GND_15" direction="pas"/>
<pin name="GND_16" direction="pas"/>
<pin name="GND_17" direction="pas"/>
<pin name="GND_18" direction="pas"/>
<pin name="GND_19" direction="pas"/>
<pin name="GND_20" direction="pas"/>
<pin name="GND_21" direction="pas"/>
<pin name="GND_22" direction="pas"/>
<pin name="GND_23" direction="pas"/>
<pin name="GND_24" direction="pas"/>
<pin name="GND_25" direction="pas"/>
<pin name="GND_26" direction="pas"/>
<pin name="GND_27" direction="pas"/>
<pin name="GND_28" direction="pas"/>
<pin name="GND_29" direction="pas"/>
<pin name="GND_30" direction="pas"/>
<pin name="GND_31" direction="pas"/>
<pin name="GND_32" direction="pas"/>
<pin name="GND_33" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDE_2" direction="pas"/>
<pin name="GNDE_3" direction="pas"/>
<pin name="GNDE" direction="pas"/>
<pin name="GNDDR_2" direction="pas"/>
<pin name="GNDDR_3" direction="pas"/>
<pin name="GNDDR_4" direction="pas"/>
<pin name="GNDDR_5" direction="pas"/>
<pin name="GNDDR_6" direction="pas"/>
<pin name="GNDDR_7" direction="pas"/>
<pin name="GNDDR_8" direction="pas"/>
<pin name="GNDDR_9" direction="pas"/>
<pin name="GNDDR_10" direction="pas"/>
<pin name="GNDDR_11" direction="pas"/>
<pin name="GNDDR_12" direction="pas"/>
<pin name="GNDDR_13" direction="pas"/>
<pin name="GNDDR" direction="pas"/>
<pin name="RCOUT1+" direction="out"/>
<pin name="RCOUT2+" direction="out"/>
<pin name="RCOUT2-" direction="out"/>
<pin name="DQ0+" direction="out"/>
<pin name="DQD0+" direction="out"/>
<pin name="DQD0-" direction="out"/>
<pin name="DQ0-" direction="out"/>
<pin name="DQ1+" direction="out"/>
<pin name="DQD1+" direction="out"/>
<pin name="DQD1-" direction="out"/>
<pin name="DQ2+" direction="out"/>
<pin name="DQD2+" direction="out"/>
<pin name="DQ2-" direction="out"/>
<pin name="DQD3+" direction="out"/>
<pin name="DQD3-" direction="out"/>
<pin name="DQD4+" direction="out"/>
<pin name="DQD4-" direction="out"/>
<pin name="DQD5+" direction="out"/>
<pin name="DQD5-" direction="out"/>
<pin name="DQD6+" direction="out"/>
<pin name="DQD6-" direction="out"/>
<pin name="DQD7+" direction="out"/>
<pin name="DQD7-" direction="out"/>
<pin name="DQD8+" direction="out"/>
<pin name="DQD8-" direction="out"/>
<pin name="DQD9+" direction="out"/>
<pin name="DQD9-" direction="out"/>
</symbol>
<symbol name="ADC10D1000CCMLS_4">
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND_11" direction="pas"/>
<pin name="GND_12" direction="pas"/>
<pin name="GND_13" direction="pas"/>
<pin name="GND_14" direction="pas"/>
<pin name="GND_15" direction="pas"/>
<pin name="GND_16" direction="pas"/>
<pin name="GND_17" direction="pas"/>
<pin name="GND_18" direction="pas"/>
<pin name="GND_19" direction="pas"/>
<pin name="GND_20" direction="pas"/>
<pin name="GND_21" direction="pas"/>
<pin name="GND_22" direction="pas"/>
<pin name="GND_23" direction="pas"/>
<pin name="GND_24" direction="pas"/>
<pin name="GND_25" direction="pas"/>
<pin name="GND_26" direction="pas"/>
<pin name="GND_27" direction="pas"/>
<pin name="GND_28" direction="pas"/>
<pin name="GND_29" direction="pas"/>
<pin name="GND_30" direction="pas"/>
<pin name="GND_31" direction="pas"/>
<pin name="GND_32" direction="pas"/>
<pin name="GND_33" direction="pas"/>
<pin name="GND_34" direction="pas"/>
<pin name="GND_35" direction="pas"/>
<pin name="GND_36" direction="pas"/>
<pin name="GND_37" direction="pas"/>
<pin name="GND_38" direction="pas"/>
<pin name="GND_39" direction="pas"/>
<pin name="GND_40" direction="pas"/>
<pin name="GND_41" direction="pas"/>
<pin name="GND_42" direction="pas"/>
<pin name="GND_43" direction="pas"/>
<pin name="GND_44" direction="pas"/>
<pin name="GND_45" direction="pas"/>
<pin name="GND_46" direction="pas"/>
<pin name="GND_47" direction="pas"/>
<pin name="GND_48" direction="pas"/>
<pin name="GND_49" direction="pas"/>
<pin name="GND_50" direction="pas"/>
<pin name="GND_51" direction="pas"/>
<pin name="GND_52" direction="pas"/>
<pin name="GND_53" direction="pas"/>
<pin name="GND_54" direction="pas"/>
<pin name="GND_55" direction="pas"/>
<pin name="GND_56" direction="pas"/>
<pin name="GND_57" direction="pas"/>
<pin name="GND_58" direction="pas"/>
<pin name="GND_59" direction="pas"/>
<pin name="GND_60" direction="pas"/>
<pin name="GND_61" direction="pas"/>
<pin name="GND_62" direction="pas"/>
<pin name="GND_63" direction="pas"/>
<pin name="GND_64" direction="pas"/>
<pin name="GND_65" direction="pas"/>
<pin name="GND_66" direction="pas"/>
<pin name="GND_67" direction="pas"/>
<pin name="GND_68" direction="pas"/>
<pin name="GND_69" direction="pas"/>
<pin name="GND_70" direction="pas"/>
<pin name="GND_71" direction="pas"/>
<pin name="GND_72" direction="pas"/>
<pin name="GND_73" direction="pas"/>
<pin name="GND_74" direction="pas"/>
<pin name="GND_75" direction="pas"/>
<pin name="GND_76" direction="pas"/>
<pin name="GND_77" direction="pas"/>
<pin name="GND_78" direction="pas"/>
<pin name="GND_79" direction="pas"/>
<pin name="GND_80" direction="pas"/>
<pin name="GND_81" direction="pas"/>
<pin name="GND_82" direction="pas"/>
<pin name="GND_83" direction="pas"/>
<pin name="GND_84" direction="pas"/>
<pin name="GND_85" direction="pas"/>
<pin name="GND_86" direction="pas"/>
<pin name="GND_87" direction="pas"/>
<pin name="GND_88" direction="pas"/>
<pin name="GND_89" direction="pas"/>
<pin name="GND_90" direction="pas"/>
<pin name="GND_91" direction="pas"/>
<pin name="GND_92" direction="pas"/>
<pin name="GND_93" direction="pas"/>
<pin name="GND" direction="pas"/>
</symbol>
<symbol name="ADC1173CIMTC">
<pin name="AVDD_2" direction="pwr"/>
<pin name="DVDD_2" direction="pwr"/>
<pin name="AVDD_3" direction="pwr"/>
<pin name="AVDD" direction="pwr"/>
<pin name="DVDD" direction="pwr"/>
<pin name="VIN" direction="pwr"/>
<pin name="~OE" direction="in"/>
<pin name="CLK" direction="in"/>
<pin name="VRB" direction="pas"/>
<pin name="VRTS" direction="in"/>
<pin name="VRT" direction="in"/>
<pin name="AVSS_2" direction="pas"/>
<pin name="AVSS" direction="pas"/>
<pin name="VRBS" direction="pas"/>
<pin name="DVSS_2" direction="pas"/>
<pin name="DVSS" direction="pas"/>
<pin name="D0" direction="out"/>
<pin name="D1" direction="out"/>
<pin name="D2" direction="out"/>
<pin name="D3" direction="out"/>
<pin name="D4" direction="out"/>
<pin name="D5" direction="out"/>
<pin name="D6" direction="out"/>
<pin name="D7" direction="out"/>
</symbol>
<symbol name="ADC12010CIVY">
<pin name="VA_2" direction="pwr"/>
<pin name="VA_3" direction="pwr"/>
<pin name="VA" direction="pwr"/>
<pin name="VD" direction="pwr"/>
<pin name="VDR" direction="pwr"/>
<pin name="~OE" direction="in"/>
<pin name="CLK" direction="in"/>
<pin name="VIN+" direction="in"/>
<pin name="VIN-" direction="in"/>
<pin name="VREF" direction="in"/>
<pin name="PD" direction="in"/>
<pin name="VRN" direction="pas"/>
<pin name="VRP" direction="pas"/>
<pin name="VRM" direction="pas"/>
<pin name="AGND_2" direction="pas"/>
<pin name="DR_GND" direction="pas"/>
<pin name="AGND_3" direction="pas"/>
<pin name="DGND_2" direction="pas"/>
<pin name="AGND" direction="pas"/>
<pin name="DGND" direction="pas"/>
<pin name="D0" direction="out"/>
<pin name="D1" direction="out"/>
<pin name="D2" direction="out"/>
<pin name="D3" direction="out"/>
<pin name="D4" direction="out"/>
<pin name="D5" direction="out"/>
<pin name="D6" direction="out"/>
<pin name="D7" direction="out"/>
<pin name="D8" direction="out"/>
<pin name="D9" direction="out"/>
<pin name="D10" direction="out"/>
<pin name="D11" direction="out"/>
</symbol>
<symbol name="ADC12020CIVY">
<pin name="VA_2" direction="pwr"/>
<pin name="VA_3" direction="pwr"/>
<pin name="VA" direction="pwr"/>
<pin name="VD" direction="pwr"/>
<pin name="VDR" direction="pwr"/>
<pin name="~OE" direction="in"/>
<pin name="CLK" direction="in"/>
<pin name="VIN+" direction="in"/>
<pin name="VIN-" direction="in"/>
<pin name="VREF" direction="in"/>
<pin name="PD" direction="in"/>
<pin name="VRN" direction="pas"/>
<pin name="VRP" direction="pas"/>
<pin name="VRM" direction="pas"/>
<pin name="AGND_2" direction="pas"/>
<pin name="DR_GND" direction="pas"/>
<pin name="AGND_3" direction="pas"/>
<pin name="DGND_2" direction="pas"/>
<pin name="AGND" direction="pas"/>
<pin name="DGND" direction="pas"/>
<pin name="D0" direction="out"/>
<pin name="D1" direction="out"/>
<pin name="D2" direction="out"/>
<pin name="D3" direction="out"/>
<pin name="D4" direction="out"/>
<pin name="D5" direction="out"/>
<pin name="D6" direction="out"/>
<pin name="D7" direction="out"/>
<pin name="D8" direction="out"/>
<pin name="D9" direction="out"/>
<pin name="D10" direction="out"/>
<pin name="D11" direction="out"/>
</symbol>
<symbol name="ADC12038CIWM">
<pin name="VA+" direction="pwr"/>
<pin name="VD+" direction="pwr"/>
<pin name="VREF-" direction="in"/>
<pin name="VREF+" direction="in"/>
<pin name="SCLK" direction="in"/>
<pin name="CCLK" direction="in"/>
<pin name="CH0" direction="in"/>
<pin name="CH1" direction="in"/>
<pin name="CH2" direction="in"/>
<pin name="CH3" direction="in"/>
<pin name="CH4" direction="in"/>
<pin name="CH5" direction="in"/>
<pin name="CH6" direction="in"/>
<pin name="CH7" direction="in"/>
<pin name="COM" direction="pas"/>
<pin name="A/DIN1" direction="in"/>
<pin name="A/DIN2" direction="in"/>
<pin name="PD" direction="pwr"/>
<pin name="~CONV" direction="in"/>
<pin name="~CS" direction="in"/>
<pin name="DI" direction="in"/>
<pin name="AGND" direction="pas"/>
<pin name="DGND" direction="pas"/>
<pin name="MUXOUT1" direction="out"/>
<pin name="MUXOUT2" direction="out"/>
<pin name="EOC" direction="out"/>
<pin name="DO" direction="out"/>
<pin name="~DOR" direction="out"/>
</symbol>
<symbol name="ADC12040CIVY">
<pin name="VA_2" direction="pwr"/>
<pin name="VD" direction="pwr"/>
<pin name="VA_3" direction="pwr"/>
<pin name="VA" direction="pwr"/>
<pin name="VREF" direction="in"/>
<pin name="VDR" direction="pwr"/>
<pin name="VIN+" direction="in"/>
<pin name="VIN-" direction="in"/>
<pin name="VRN" direction="in"/>
<pin name="VRP" direction="in"/>
<pin name="VRM" direction="in"/>
<pin name="PD" direction="in"/>
<pin name="CLK" direction="in"/>
<pin name="~OE" direction="in"/>
<pin name="DGND_2" direction="pas"/>
<pin name="AGND_2" direction="pas"/>
<pin name="AGND_3" direction="pas"/>
<pin name="AGND" direction="pas"/>
<pin name="DGND" direction="pas"/>
<pin name="DR_GND" direction="pas"/>
<pin name="D0" direction="out"/>
<pin name="D1" direction="out"/>
<pin name="D2" direction="out"/>
<pin name="D3" direction="out"/>
<pin name="D4" direction="out"/>
<pin name="D5" direction="out"/>
<pin name="D6" direction="out"/>
<pin name="D7" direction="out"/>
<pin name="D8" direction="out"/>
<pin name="D9" direction="out"/>
<pin name="D10" direction="out"/>
<pin name="D11" direction="out"/>
</symbol>
<symbol name="ADC12048CIV">
<pin name="VA+" direction="pwr"/>
<pin name="VD+_2" direction="pwr"/>
<pin name="VD+" direction="pwr"/>
<pin name="VREF+" direction="in"/>
<pin name="VREF-" direction="in"/>
<pin name="~RD" direction="in"/>
<pin name="~CS" direction="in"/>
<pin name="COM" direction="in"/>
<pin name="CLK" direction="in"/>
<pin name="~WR" direction="in"/>
<pin name="CH0" direction="in"/>
<pin name="CH1" direction="in"/>
<pin name="CH2" direction="in"/>
<pin name="CH3" direction="in"/>
<pin name="CH4" direction="in"/>
<pin name="CH5" direction="in"/>
<pin name="CH7" direction="in"/>
<pin name="CH6" direction="in"/>
<pin name="ADCIN-" direction="in"/>
<pin name="ADCIN+" direction="in"/>
<pin name="WMODE" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="AGND" direction="pas"/>
<pin name="DGND_2" direction="pas"/>
<pin name="DGND" direction="pas"/>
<pin name="~RDY" direction="out"/>
<pin name="~STDBY" direction="out"/>
<pin name="MUXOUT-" direction="out"/>
<pin name="MUXOUT+" direction="out"/>
<pin name="SYNC"/>
<pin name="D0"/>
<pin name="D1"/>
<pin name="D2"/>
<pin name="D3"/>
<pin name="D4"/>
<pin name="D5"/>
<pin name="D6"/>
<pin name="D7"/>
<pin name="D8"/>
<pin name="D9"/>
<pin name="D10"/>
<pin name="D11"/>
<pin name="D12"/>
</symbol>
<symbol name="ADC12048CIVF">
<pin name="VA+" direction="pwr"/>
<pin name="VD+_2" direction="pwr"/>
<pin name="VD+" direction="pwr"/>
<pin name="CH0" direction="in"/>
<pin name="CH1" direction="in"/>
<pin name="CH2" direction="in"/>
<pin name="CH3" direction="in"/>
<pin name="CH4" direction="in"/>
<pin name="CH5" direction="in"/>
<pin name="CH6" direction="in"/>
<pin name="CH7" direction="in"/>
<pin name="VREF-" direction="in"/>
<pin name="VREF+" direction="in"/>
<pin name="ADCIN-" direction="in"/>
<pin name="ADCIN+" direction="in"/>
<pin name="COM" direction="in"/>
<pin name="WMODE" direction="in"/>
<pin name="CLK" direction="in"/>
<pin name="~WR" direction="in"/>
<pin name="~RD" direction="in"/>
<pin name="~CS" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="AGND" direction="pas"/>
<pin name="DGND_2" direction="pas"/>
<pin name="DGND" direction="pas"/>
<pin name="MUXOUT_-" direction="out"/>
<pin name="MUXOUT+" direction="out"/>
<pin name="~RDY" direction="out"/>
<pin name="~STDBY" direction="out"/>
<pin name="SYNC"/>
<pin name="D0"/>
<pin name="D1"/>
<pin name="D2"/>
<pin name="D3"/>
<pin name="D4"/>
<pin name="D5"/>
<pin name="D6"/>
<pin name="D7"/>
<pin name="D8"/>
<pin name="D9"/>
<pin name="D10"/>
<pin name="D11"/>
<pin name="D12"/>
</symbol>
<symbol name="ADC12130CIWM">
<pin name="VA+" direction="pwr"/>
<pin name="VD+" direction="pwr"/>
<pin name="SCLK" direction="in"/>
<pin name="CCLK" direction="in"/>
<pin name="CH0" direction="in"/>
<pin name="CH1" direction="in"/>
<pin name="COM" direction="in"/>
<pin name="EOC" direction="in"/>
<pin name="~CS" direction="in"/>
<pin name="DI" direction="in"/>
<pin name="~CONV" direction="in"/>
<pin name="VREF-" direction="in"/>
<pin name="VREF+" direction="in"/>
<pin name="DGND" direction="pas"/>
<pin name="~DOR" direction="out"/>
<pin name="DO" direction="out"/>
</symbol>
<symbol name="ADC12138CIMSA">
<pin name="VD+" direction="pwr"/>
<pin name="VA+" direction="pwr"/>
<pin name="SCLK" direction="in"/>
<pin name="CCLK" direction="in"/>
<pin name="CH0" direction="in"/>
<pin name="CH1" direction="in"/>
<pin name="CH2" direction="in"/>
<pin name="CH3" direction="in"/>
<pin name="CH4" direction="in"/>
<pin name="CH5" direction="in"/>
<pin name="CH6" direction="in"/>
<pin name="CH7" direction="in"/>
<pin name="COM" direction="in"/>
<pin name="A/DIN1" direction="in"/>
<pin name="A/DIN2" direction="in"/>
<pin name="VREF-" direction="in"/>
<pin name="VREF+" direction="in"/>
<pin name="PD" direction="in"/>
<pin name="DI" direction="in"/>
<pin name="~CONV" direction="in"/>
<pin name="~CS" direction="in"/>
<pin name="DGND" direction="pas"/>
<pin name="AGND" direction="pas"/>
<pin name="MUXOUT1" direction="out"/>
<pin name="MUXOUT2" direction="out"/>
<pin name="EOC" direction="out"/>
<pin name="DO" direction="out"/>
<pin name="~DOR" direction="out"/>
</symbol>
<symbol name="ADC12138CIWM">
<pin name="VA+" direction="pwr"/>
<pin name="VD+" direction="pwr"/>
<pin name="SCLK" direction="in"/>
<pin name="CCLK" direction="in"/>
<pin name="VREF+" direction="in"/>
<pin name="VREF-" direction="in"/>
<pin name="CH0" direction="in"/>
<pin name="CH1" direction="in"/>
<pin name="CH2" direction="in"/>
<pin name="CH3" direction="in"/>
<pin name="CH4" direction="in"/>
<pin name="CH5" direction="in"/>
<pin name="CH6" direction="in"/>
<pin name="CH7" direction="in"/>
<pin name="COM" direction="in"/>
<pin name="A/DIN1" direction="in"/>
<pin name="A/DIN2" direction="in"/>
<pin name="PD" direction="in"/>
<pin name="~CONV" direction="in"/>
<pin name="~CS" direction="in"/>
<pin name="DI" direction="in"/>
<pin name="DGND" direction="pas"/>
<pin name="AGND" direction="pas"/>
<pin name="MUXOUT1" direction="out"/>
<pin name="MUXOUT2" direction="out"/>
<pin name="EOC" direction="out"/>
<pin name="~DOR" direction="out"/>
<pin name="DO" direction="out"/>
</symbol>
<symbol name="ADC121C021CIMK">
<pin name="VA" direction="pwr"/>
<pin name="SCL" direction="in"/>
<pin name="VIN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="ALERT" direction="out"/>
<pin name="SDA"/>
</symbol>
<symbol name="ADC121C027CIMK">
<pin name="VA" direction="pwr"/>
<pin name="ADDR" direction="in"/>
<pin name="SCL" direction="in"/>
<pin name="VIN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="SDA"/>
</symbol>
<symbol name="ADC121S021CIMF">
<pin name="VA" direction="pwr"/>
<pin name="VIN" direction="in"/>
<pin name="SCLK" direction="in"/>
<pin name="~CS" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="SDATA" direction="out"/>
</symbol>
<symbol name="ADC121S021CISD">
<pin name="VA" direction="pwr"/>
<pin name="VIN" direction="in"/>
<pin name="SCLK" direction="in"/>
<pin name="~CS" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="SDATA" direction="out"/>
</symbol>
<symbol name="ADC121S051CIMF">
<pin name="VA" direction="pwr"/>
<pin name="SCLK" direction="in"/>
<pin name="~CS" direction="in"/>
<pin name="VIN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="SDATA" direction="out"/>
</symbol>
<symbol name="ADC121S101CIMF">
<pin name="VDD" direction="pwr"/>
<pin name="VIN" direction="in"/>
<pin name="SCLK" direction="in"/>
<pin name="~CS" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="SDATA" direction="out"/>
</symbol>
<symbol name="ADC121S101CISD">
<pin name="VA" direction="pwr"/>
<pin name="VIN" direction="in"/>
<pin name="SCLK" direction="in"/>
<pin name="~CS" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="SDATA" direction="out"/>
<pin name="THERMAL_PAD" direction="pas"/>
</symbol>
<symbol name="ADC121S625CIMM">
<pin name="+VA" direction="pwr"/>
<pin name="+IN" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="VREF" direction="in"/>
<pin name="SCLK" direction="in"/>
<pin name="~CS" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="DOUT" direction="out"/>
</symbol>
<symbol name="ADC122S021CIMM">
<pin name="VA" direction="pwr"/>
<pin name="~CS" direction="in"/>
<pin name="SCLK" direction="in"/>
<pin name="DIN" direction="in"/>
<pin name="IN1" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="DOUT" direction="out"/>
</symbol>
<symbol name="ADC122S051CIMM">
<pin name="VA" direction="pwr"/>
<pin name="~CS" direction="in"/>
<pin name="SCLK" direction="in"/>
<pin name="DIN" direction="in"/>
<pin name="IN1" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="DOUT" direction="out"/>
</symbol>
<symbol name="ADC122S101CIMM">
<pin name="VA" direction="pwr"/>
<pin name="DIN" direction="in"/>
<pin name="SCLK" direction="in"/>
<pin name="~CS" direction="in"/>
<pin name="IN1" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="DOUT" direction="out"/>
</symbol>
<symbol name="ADC122S706CIMT">
<pin name="VA" direction="pwr"/>
<pin name="VD" direction="pwr"/>
<pin name="VREF" direction="pwr"/>
<pin name="~CS" direction="in"/>
<pin name="CHA-" direction="in"/>
<pin name="CHA+" direction="in"/>
<pin name="CHB-" direction="in"/>
<pin name="CHB+" direction="in"/>
<pin name="DUAL" direction="in"/>
<pin name="SCLK" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="DOUTA" direction="out"/>
<pin name="DOUTB" direction="out"/>
</symbol>
<symbol name="ADC124S021CIMM">
<pin name="VA" direction="pwr"/>
<pin name="~CS" direction="in"/>
<pin name="SCLK" direction="in"/>
<pin name="DIN" direction="in"/>
<pin name="IN1" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="IN3" direction="in"/>
<pin name="IN4" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="DOUT" direction="out"/>
</symbol>
<symbol name="ADC124S051CIMM">
<pin name="VA" direction="pwr"/>
<pin name="~CS" direction="in"/>
<pin name="SCLK" direction="in"/>
<pin name="DIN" direction="in"/>
<pin name="IN1" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="IN3" direction="in"/>
<pin name="IN4" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="DOUT" direction="out"/>
</symbol>
<symbol name="ADC124S101CIMM">
<pin name="VA" direction="pwr"/>
<pin name="~CS" direction="in"/>
<pin name="SCLK" direction="in"/>
<pin name="DIN" direction="in"/>
<pin name="IN1" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="IN3" direction="in"/>
<pin name="IN4" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="DOUT" direction="out"/>
</symbol>
<symbol name="ADC128S022CIMT">
<pin name="VA" direction="pwr"/>
<pin name="VD" direction="pwr"/>
<pin name="~CS" direction="in"/>
<pin name="DIN" direction="in"/>
<pin name="SCLK" direction="in"/>
<pin name="IN0" direction="in"/>
<pin name="IN1" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="IN3" direction="in"/>
<pin name="IN4" direction="in"/>
<pin name="IN5" direction="in"/>
<pin name="IN6" direction="in"/>
<pin name="IN7" direction="in"/>
<pin name="AGND" direction="pas"/>
<pin name="DGND" direction="pas"/>
<pin name="DOUT" direction="out"/>
</symbol>
<symbol name="ADC128S052CIMT">
<pin name="VA" direction="pwr"/>
<pin name="VD" direction="pwr"/>
<pin name="~CS" direction="in"/>
<pin name="DIN" direction="in"/>
<pin name="SCLK" direction="in"/>
<pin name="IN0" direction="in"/>
<pin name="IN1" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="IN3" direction="in"/>
<pin name="IN4" direction="in"/>
<pin name="IN5" direction="in"/>
<pin name="IN6" direction="in"/>
<pin name="IN7" direction="in"/>
<pin name="AGND" direction="pas"/>
<pin name="DGND" direction="pas"/>
<pin name="DOUT" direction="out"/>
</symbol>
<symbol name="ADC128S102CIMT">
<pin name="VA" direction="pwr"/>
<pin name="VD" direction="pwr"/>
<pin name="~CS" direction="in"/>
<pin name="DIN" direction="in"/>
<pin name="SCLK" direction="in"/>
<pin name="IN0" direction="in"/>
<pin name="IN1" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="IN3" direction="in"/>
<pin name="IN4" direction="in"/>
<pin name="IN5" direction="in"/>
<pin name="IN6" direction="in"/>
<pin name="IN7" direction="in"/>
<pin name="AGND" direction="pas"/>
<pin name="DGND" direction="pas"/>
<pin name="DOUT" direction="out"/>
</symbol>
<symbol name="ADC12C105CISQ">
<pin name="VA_2" direction="pwr"/>
<pin name="VA_3" direction="pwr"/>
<pin name="VA" direction="pwr"/>
<pin name="VRN" direction="in"/>
<pin name="VRP" direction="in"/>
<pin name="VDR" direction="in"/>
<pin name="CLK" direction="in"/>
<pin name="PD" direction="in"/>
<pin name="DRDY" direction="pas"/>
<pin name="VREF" direction="in"/>
<pin name="OF/DCS" direction="pas"/>
<pin name="VCMO" direction="in"/>
<pin name="VIN+" direction="in"/>
<pin name="VIN-" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="AGND_2" direction="pas"/>
<pin name="AGND_3" direction="pas"/>
<pin name="AGND" direction="pas"/>
<pin name="DRGND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="D0" direction="out"/>
<pin name="D1" direction="out"/>
<pin name="D2" direction="out"/>
<pin name="D3" direction="out"/>
<pin name="D4" direction="out"/>
<pin name="D5" direction="out"/>
<pin name="D6" direction="out"/>
<pin name="D7" direction="out"/>
<pin name="D8" direction="out"/>
<pin name="D9" direction="out"/>
<pin name="D10" direction="out"/>
<pin name="D11(MSB)" direction="out"/>
</symbol>
<symbol name="ADC12D040CIVS">
<pin name="VA_2" direction="pwr"/>
<pin name="VA_3" direction="pwr"/>
<pin name="VA_4" direction="pwr"/>
<pin name="VA_5" direction="pwr"/>
<pin name="VA" direction="pwr"/>
<pin name="VD_2" direction="pwr"/>
<pin name="VD" direction="pwr"/>
<pin name="VDR_2" direction="pwr"/>
<pin name="VDR" direction="pwr"/>
<pin name="~INT~/_EXT_REF" direction="in"/>
<pin name="~OEA" direction="in"/>
<pin name="~OEB" direction="in"/>
<pin name="CLK" direction="in"/>
<pin name="VREF" direction="in"/>
<pin name="OF" direction="in"/>
<pin name="PD" direction="in"/>
<pin name="VIN_A+" direction="in"/>
<pin name="VIN_A-" direction="in"/>
<pin name="VINB+" direction="in"/>
<pin name="VINB-" direction="in"/>
<pin name="VRM_A" direction="in"/>
<pin name="VRM_B" direction="in"/>
<pin name="VRN_A" direction="in"/>
<pin name="VRN_B" direction="in"/>
<pin name="VRP_A" direction="in"/>
<pin name="VRP_B" direction="in"/>
<pin name="AGND_2" direction="pas"/>
<pin name="AGND_3" direction="pas"/>
<pin name="AGND_4" direction="pas"/>
<pin name="AGND_5" direction="pas"/>
<pin name="AGND_6" direction="pas"/>
<pin name="AGND_7" direction="pas"/>
<pin name="AGND" direction="pas"/>
<pin name="DGND_2" direction="pas"/>
<pin name="DGND" direction="pas"/>
<pin name="DR_GND_2" direction="pas"/>
<pin name="DR_GND_3" direction="pas"/>
<pin name="DR_GND_4" direction="pas"/>
<pin name="DR_GND_5" direction="pas"/>
<pin name="DR_GND" direction="pas"/>
<pin name="DA0" direction="out"/>
<pin name="DA1" direction="out"/>
<pin name="DA2" direction="out"/>
<pin name="DA3" direction="out"/>
<pin name="DA4" direction="out"/>
<pin name="DA5" direction="out"/>
<pin name="DA6" direction="out"/>
<pin name="DA7" direction="out"/>
<pin name="DA8" direction="out"/>
<pin name="DA9" direction="out"/>
<pin name="DA10" direction="out"/>
<pin name="DA11" direction="out"/>
<pin name="DB0" direction="out"/>
<pin name="DB1" direction="out"/>
<pin name="DB2" direction="out"/>
<pin name="DB3" direction="out"/>
<pin name="DB4" direction="out"/>
<pin name="DB5" direction="out"/>
<pin name="DB6" direction="out"/>
<pin name="DB7" direction="out"/>
<pin name="DB8" direction="out"/>
<pin name="DB9" direction="out"/>
<pin name="DB10" direction="out"/>
<pin name="DB11" direction="out"/>
</symbol>
<symbol name="ADC12DL040CIVS">
<pin name="VA_2" direction="pwr"/>
<pin name="VA_3" direction="pwr"/>
<pin name="VA_4" direction="pwr"/>
<pin name="VA_5" direction="pwr"/>
<pin name="VA" direction="pwr"/>
<pin name="VD_2" direction="pwr"/>
<pin name="VD" direction="pwr"/>
<pin name="VDR_2" direction="pwr"/>
<pin name="VDR" direction="pwr"/>
<pin name="MULTIPLEX" direction="in"/>
<pin name="VREF" direction="in"/>
<pin name="DF/DCS" direction="in"/>
<pin name="~OEA" direction="in"/>
<pin name="~OEB" direction="in"/>
<pin name="PD" direction="in"/>
<pin name="CLK" direction="in"/>
<pin name="VRN_A" direction="pwr"/>
<pin name="VRP_A" direction="pwr"/>
<pin name="VRP_B" direction="in"/>
<pin name="VRM_A" direction="pwr"/>
<pin name="VRM_B" direction="in"/>
<pin name="VIN_A+" direction="pwr"/>
<pin name="VIN_A-" direction="pwr"/>
<pin name="VIN_B-" direction="in"/>
<pin name="VRN_B" direction="in"/>
<pin name="VINB+" direction="in"/>
<pin name="DR_GND_2" direction="pas"/>
<pin name="DR_GND" direction="pas"/>
<pin name="DR_GND_3" direction="pas"/>
<pin name="DR_GND_4" direction="pas"/>
<pin name="DR_GND_5" direction="pas"/>
<pin name="DGND_2" direction="pas"/>
<pin name="DGND" direction="pas"/>
<pin name="AGND_2" direction="pas"/>
<pin name="AGND_3" direction="pas"/>
<pin name="AGND_4" direction="pas"/>
<pin name="AGND_5" direction="pas"/>
<pin name="AGND_6" direction="pas"/>
<pin name="AGND_7" direction="pas"/>
<pin name="AGND" direction="pas"/>
<pin name="DA0" direction="out"/>
<pin name="DA1" direction="out"/>
<pin name="DA2" direction="out"/>
<pin name="DA3" direction="out"/>
<pin name="DA4" direction="out"/>
<pin name="DA5" direction="out"/>
<pin name="DA6" direction="out"/>
<pin name="DA7" direction="out"/>
<pin name="DA8" direction="out"/>
<pin name="DA9" direction="out"/>
<pin name="DA10" direction="out"/>
<pin name="DA11" direction="out"/>
<pin name="DB0/ABB" direction="out"/>
<pin name="DB1" direction="out"/>
<pin name="DB2" direction="out"/>
<pin name="DB3" direction="out"/>
<pin name="DB4" direction="out"/>
<pin name="DB5" direction="out"/>
<pin name="DB6" direction="out"/>
<pin name="DB7" direction="out"/>
<pin name="DB8" direction="out"/>
<pin name="DB9" direction="out"/>
<pin name="DB10" direction="out"/>
<pin name="DB11" direction="out"/>
</symbol>
<symbol name="ADC12DL065CIVS">
<pin name="VA_2" direction="pwr"/>
<pin name="VA_3" direction="pwr"/>
<pin name="VA_4" direction="pwr"/>
<pin name="VA_5" direction="pwr"/>
<pin name="VA" direction="pwr"/>
<pin name="VD_2" direction="pwr"/>
<pin name="VD" direction="pwr"/>
<pin name="VDR_2" direction="pwr"/>
<pin name="VDR" direction="pwr"/>
<pin name="MULTIPLEX" direction="in"/>
<pin name="VREF" direction="in"/>
<pin name="DF/DCS" direction="in"/>
<pin name="~OEA" direction="in"/>
<pin name="~OEB" direction="in"/>
<pin name="PD" direction="in"/>
<pin name="CLK" direction="in"/>
<pin name="VRN_A" direction="pwr"/>
<pin name="VRP_A" direction="pwr"/>
<pin name="VRP_B" direction="in"/>
<pin name="VRM_A" direction="pwr"/>
<pin name="VRM_B" direction="in"/>
<pin name="VIN_A+" direction="pwr"/>
<pin name="VIN_A-" direction="pwr"/>
<pin name="VIN_B-" direction="in"/>
<pin name="VRN_B" direction="in"/>
<pin name="VINB+" direction="in"/>
<pin name="DR_GND_2" direction="pas"/>
<pin name="DR_GND" direction="pas"/>
<pin name="DR_GND_3" direction="pas"/>
<pin name="DR_GND_4" direction="pas"/>
<pin name="DR_GND_5" direction="pas"/>
<pin name="DGND_2" direction="pas"/>
<pin name="DGND" direction="pas"/>
<pin name="AGND_2" direction="pas"/>
<pin name="AGND_3" direction="pas"/>
<pin name="AGND_4" direction="pas"/>
<pin name="AGND_5" direction="pas"/>
<pin name="AGND_6" direction="pas"/>
<pin name="AGND_7" direction="pas"/>
<pin name="AGND" direction="pas"/>
<pin name="DA0" direction="out"/>
<pin name="DA1" direction="out"/>
<pin name="DA2" direction="out"/>
<pin name="DA3" direction="out"/>
<pin name="DA4" direction="out"/>
<pin name="DA5" direction="out"/>
<pin name="DA6" direction="out"/>
<pin name="DA7" direction="out"/>
<pin name="DA8" direction="out"/>
<pin name="DA9" direction="out"/>
<pin name="DA10" direction="out"/>
<pin name="DA11" direction="out"/>
<pin name="DB0/ABB" direction="out"/>
<pin name="DB1" direction="out"/>
<pin name="DB2" direction="out"/>
<pin name="DB3" direction="out"/>
<pin name="DB4" direction="out"/>
<pin name="DB5" direction="out"/>
<pin name="DB6" direction="out"/>
<pin name="DB7" direction="out"/>
<pin name="DB8" direction="out"/>
<pin name="DB9" direction="out"/>
<pin name="DB10" direction="out"/>
<pin name="DB11" direction="out"/>
</symbol>
<symbol name="ADC12DL066CIVS">
<pin name="VA_2" direction="pwr"/>
<pin name="VA_3" direction="pwr"/>
<pin name="VA_4" direction="pwr"/>
<pin name="VA_5" direction="pwr"/>
<pin name="VA" direction="pwr"/>
<pin name="VD_2" direction="pwr"/>
<pin name="VD" direction="pwr"/>
<pin name="VDR_2" direction="pwr"/>
<pin name="VDR" direction="pwr"/>
<pin name="~INT/EXT_REF" direction="in"/>
<pin name="VREF" direction="in"/>
<pin name="OF" direction="in"/>
<pin name="~OEA" direction="in"/>
<pin name="~OEB" direction="in"/>
<pin name="PD" direction="in"/>
<pin name="CLK" direction="in"/>
<pin name="VRN_A" direction="pwr"/>
<pin name="VRP_A" direction="pwr"/>
<pin name="VRP_B" direction="in"/>
<pin name="VRM_A" direction="pwr"/>
<pin name="VRM_B" direction="in"/>
<pin name="VIN_A+" direction="pwr"/>
<pin name="VIN_A-" direction="pwr"/>
<pin name="VIN_B-" direction="in"/>
<pin name="VRN_B" direction="in"/>
<pin name="VINB+" direction="in"/>
<pin name="DR_GND_2" direction="pas"/>
<pin name="DR_GND" direction="pas"/>
<pin name="DR_GND_3" direction="pas"/>
<pin name="DR_GND_4" direction="pas"/>
<pin name="DR_GND_5" direction="pas"/>
<pin name="DGND_2" direction="pas"/>
<pin name="DGND" direction="pas"/>
<pin name="AGND_2" direction="pas"/>
<pin name="AGND_3" direction="pas"/>
<pin name="AGND_4" direction="pas"/>
<pin name="AGND_5" direction="pas"/>
<pin name="AGND_6" direction="pas"/>
<pin name="AGND_7" direction="pas"/>
<pin name="AGND" direction="pas"/>
<pin name="DA0" direction="out"/>
<pin name="DA1" direction="out"/>
<pin name="DA2" direction="out"/>
<pin name="DA3" direction="out"/>
<pin name="DA4" direction="out"/>
<pin name="DA5" direction="out"/>
<pin name="DA6" direction="out"/>
<pin name="DA7" direction="out"/>
<pin name="DA8" direction="out"/>
<pin name="DA9" direction="out"/>
<pin name="DA10" direction="out"/>
<pin name="DA11" direction="out"/>
<pin name="DB0/ABB" direction="out"/>
<pin name="DB1" direction="out"/>
<pin name="DB2" direction="out"/>
<pin name="DB3" direction="out"/>
<pin name="DB4" direction="out"/>
<pin name="DB5" direction="out"/>
<pin name="DB6" direction="out"/>
<pin name="DB7" direction="out"/>
<pin name="DB8" direction="out"/>
<pin name="DB9" direction="out"/>
<pin name="DB10" direction="out"/>
<pin name="DB11" direction="out"/>
</symbol>
<symbol name="ADC12DL080CIVS">
<pin name="VA_2" direction="pwr"/>
<pin name="VA_3" direction="pwr"/>
<pin name="VA_4" direction="pwr"/>
<pin name="VA_5" direction="pwr"/>
<pin name="VA" direction="pwr"/>
<pin name="VD_2" direction="pwr"/>
<pin name="VD" direction="pwr"/>
<pin name="VDR_2" direction="in"/>
<pin name="VDR" direction="in"/>
<pin name="VIN_B-" direction="in"/>
<pin name="VINB+" direction="in"/>
<pin name="VRM_B" direction="in"/>
<pin name="VRP_B" direction="in"/>
<pin name="VRN_B" direction="in"/>
<pin name="VRN_A" direction="in"/>
<pin name="VRP_A" direction="in"/>
<pin name="VRM_A" direction="in"/>
<pin name="VIN_A+" direction="in"/>
<pin name="VIN_A-" direction="in"/>
<pin name="CLK" direction="in"/>
<pin name="VREF" direction="in"/>
<pin name="PD" direction="in"/>
<pin name="REFSEL/DCS" direction="in"/>
<pin name="~OEB/DRDY" direction="in"/>
<pin name="OF/DOEN" direction="in"/>
<pin name="~OEA/OF" direction="in"/>
<pin name="DGND_2" direction="pas"/>
<pin name="DGND" direction="pas"/>
<pin name="DRGND_2" direction="pas"/>
<pin name="DRGND_3" direction="pas"/>
<pin name="DRGND_4" direction="pas"/>
<pin name="DRGND_5" direction="pas"/>
<pin name="DRGND" direction="pas"/>
<pin name="AGND_2" direction="pas"/>
<pin name="AGND_3" direction="pas"/>
<pin name="AGND_4" direction="pas"/>
<pin name="AGND_5" direction="pas"/>
<pin name="AGND_6" direction="pas"/>
<pin name="AGND_7" direction="pas"/>
<pin name="AGND" direction="pas"/>
<pin name="(LSB)DA0" direction="out"/>
<pin name="DA1" direction="out"/>
<pin name="DA2" direction="out"/>
<pin name="DA3" direction="out"/>
<pin name="DA4" direction="out"/>
<pin name="DA5" direction="out"/>
<pin name="DA6" direction="out"/>
<pin name="DA7" direction="out"/>
<pin name="DA8" direction="out"/>
<pin name="DA9" direction="out"/>
<pin name="DA10" direction="out"/>
<pin name="DA11(MSB)" direction="out"/>
<pin name="DB0(LSB)" direction="out"/>
<pin name="DB1" direction="out"/>
<pin name="DB2" direction="out"/>
<pin name="DB3" direction="out"/>
<pin name="DB4" direction="out"/>
<pin name="DB5" direction="out"/>
<pin name="DB6" direction="out"/>
<pin name="DB7" direction="out"/>
<pin name="DB8" direction="out"/>
<pin name="DB9" direction="out"/>
<pin name="DB10" direction="out"/>
<pin name="DB11(MSB)" direction="out"/>
</symbol>
<symbol name="ADC12EU050CIPLQ">
<pin name="VA_2" direction="pwr"/>
<pin name="VA_3" direction="pwr"/>
<pin name="VA_4" direction="pwr"/>
<pin name="VA_5" direction="pwr"/>
<pin name="VA_6" direction="pwr"/>
<pin name="VA_7" direction="pwr"/>
<pin name="VA_8" direction="pwr"/>
<pin name="VA" direction="pwr"/>
<pin name="VD_2" direction="pwr"/>
<pin name="VD_3" direction="pwr"/>
<pin name="VD_4" direction="pwr"/>
<pin name="VD" direction="pwr"/>
<pin name="VDR_2" direction="pwr"/>
<pin name="VDR_3" direction="pwr"/>
<pin name="VDR" direction="pwr"/>
<pin name="CLK+_(SE)" direction="in"/>
<pin name="CLK-" direction="in"/>
<pin name="SCLK" direction="in"/>
<pin name="DCAP" direction="in"/>
<pin name="~RST" direction="in"/>
<pin name="SLEEP" direction="in"/>
<pin name="~SSEL" direction="in"/>
<pin name="SDATA"/>
<pin name="RREF" direction="pas"/>
<pin name="VREFB" direction="pwr"/>
<pin name="VREFT" direction="pwr"/>
<pin name="VIN0+" direction="in"/>
<pin name="VIN0-" direction="in"/>
<pin name="VIN1+" direction="in"/>
<pin name="VIN1-" direction="in"/>
<pin name="VIN2+" direction="in"/>
<pin name="VIN2-" direction="in"/>
<pin name="VIN3+" direction="in"/>
<pin name="VIN3-" direction="in"/>
<pin name="VIN4+" direction="in"/>
<pin name="VIN4-" direction="in"/>
<pin name="VIN5+" direction="in"/>
<pin name="VIN5-" direction="in"/>
<pin name="VIN6+" direction="in"/>
<pin name="VIN6-" direction="in"/>
<pin name="VIN7+" direction="in"/>
<pin name="VIN7-" direction="in"/>
<pin name="DGND_2" direction="pas"/>
<pin name="DGND_3" direction="pas"/>
<pin name="DGND_4" direction="pas"/>
<pin name="DGND_5" direction="pas"/>
<pin name="DGND_6" direction="pas"/>
<pin name="DGND" direction="pas"/>
<pin name="AGND" direction="pas"/>
<pin name="DO0+" direction="out"/>
<pin name="DO0-" direction="out"/>
<pin name="DO1+" direction="out"/>
<pin name="DO1-" direction="out"/>
<pin name="DO2+" direction="out"/>
<pin name="DO2-" direction="out"/>
<pin name="DO3+" direction="out"/>
<pin name="DO3-" direction="out"/>
<pin name="DO4+" direction="out"/>
<pin name="DO4-" direction="out"/>
<pin name="DO5+" direction="out"/>
<pin name="DO5-" direction="out"/>
<pin name="DO6+" direction="out"/>
<pin name="DO6-" direction="out"/>
<pin name="DO7+" direction="out"/>
<pin name="DO7-" direction="out"/>
<pin name="BCLK+" direction="out"/>
<pin name="BCLK-" direction="out"/>
<pin name="WCLK+" direction="out"/>
<pin name="WCLK-" direction="out"/>
</symbol>
<symbol name="ADC12L063CIVY">
<pin name="VA_2" direction="pwr"/>
<pin name="VA_3" direction="pwr"/>
<pin name="VA" direction="pwr"/>
<pin name="VD" direction="pwr"/>
<pin name="VDR" direction="pwr"/>
<pin name="CLK" direction="in"/>
<pin name="~OE" direction="in"/>
<pin name="VREF" direction="in"/>
<pin name="PD" direction="in"/>
<pin name="VRN" direction="in"/>
<pin name="VRP" direction="in"/>
<pin name="VRM" direction="in"/>
<pin name="VIN+" direction="in"/>
<pin name="VIN-" direction="in"/>
<pin name="AGND_2" direction="pas"/>
<pin name="AGND_3" direction="pas"/>
<pin name="AGND" direction="pas"/>
<pin name="DGND_2" direction="pas"/>
<pin name="DGND" direction="pas"/>
<pin name="DR_GND" direction="pas"/>
<pin name="D0" direction="out"/>
<pin name="D1" direction="out"/>
<pin name="D2" direction="out"/>
<pin name="D3" direction="out"/>
<pin name="D4" direction="out"/>
<pin name="D5" direction="out"/>
<pin name="D6" direction="out"/>
<pin name="D7" direction="out"/>
<pin name="D8" direction="out"/>
<pin name="D9" direction="out"/>
<pin name="D10" direction="out"/>
<pin name="D11" direction="out"/>
</symbol>
<symbol name="ADC12L066CIVY">
<pin name="VA_2" direction="pwr"/>
<pin name="VA_3" direction="pwr"/>
<pin name="VA" direction="pwr"/>
<pin name="VD" direction="pwr"/>
<pin name="VDR" direction="pwr"/>
<pin name="VREF" direction="in"/>
<pin name="PD" direction="in"/>
<pin name="CLK" direction="in"/>
<pin name="~OE" direction="in"/>
<pin name="VIN+" direction="in"/>
<pin name="VIN-" direction="in"/>
<pin name="VRN" direction="in"/>
<pin name="VRP" direction="in"/>
<pin name="VRM" direction="in"/>
<pin name="AGND_2" direction="pas"/>
<pin name="AGND_3" direction="pas"/>
<pin name="AGND" direction="pas"/>
<pin name="DGND_2" direction="pas"/>
<pin name="DGND" direction="pas"/>
<pin name="DR_GND" direction="pas"/>
<pin name="D0" direction="out"/>
<pin name="D1" direction="out"/>
<pin name="D2" direction="out"/>
<pin name="D3" direction="out"/>
<pin name="D4" direction="out"/>
<pin name="D5" direction="out"/>
<pin name="D6" direction="out"/>
<pin name="D7" direction="out"/>
<pin name="D8" direction="out"/>
<pin name="D9" direction="out"/>
<pin name="D10" direction="out"/>
<pin name="D11" direction="out"/>
</symbol>
<symbol name="ADC12L080CIVY">
<pin name="VA_2" direction="pwr"/>
<pin name="VA_3" direction="pwr"/>
<pin name="VA" direction="pwr"/>
<pin name="VD" direction="pwr"/>
<pin name="CLK" direction="in"/>
<pin name="VREF" direction="in"/>
<pin name="PD" direction="in"/>
<pin name="VDR" direction="pwr"/>
<pin name="OF" direction="in"/>
<pin name="VRN" direction="in"/>
<pin name="VRP" direction="in"/>
<pin name="VRM" direction="in"/>
<pin name="VIN+" direction="in"/>
<pin name="VIN-" direction="in"/>
<pin name="DGND_2" direction="pas"/>
<pin name="DGND" direction="pas"/>
<pin name="AGND_2" direction="pas"/>
<pin name="AGND_3" direction="pas"/>
<pin name="AGND" direction="pas"/>
<pin name="DR_GND" direction="pas"/>
<pin name="D0" direction="out"/>
<pin name="D1" direction="out"/>
<pin name="D2" direction="out"/>
<pin name="D3" direction="out"/>
<pin name="D4" direction="out"/>
<pin name="D5" direction="out"/>
<pin name="D6" direction="out"/>
<pin name="D7" direction="out"/>
<pin name="D8" direction="out"/>
<pin name="D9" direction="out"/>
<pin name="D10" direction="out"/>
<pin name="D11" direction="out"/>
</symbol>
<symbol name="ADC14155CISQ">
<pin name="VA_2" direction="pwr"/>
<pin name="VA_3" direction="pwr"/>
<pin name="VA_4" direction="pwr"/>
<pin name="VA_5" direction="pwr"/>
<pin name="VA_6" direction="pwr"/>
<pin name="VA_7" direction="pwr"/>
<pin name="VA" direction="pwr"/>
<pin name="VD" direction="pwr"/>
<pin name="VDR_2" direction="pwr"/>
<pin name="VDR_3" direction="pwr"/>
<pin name="VDR" direction="pwr"/>
<pin name="VIN-" direction="in"/>
<pin name="VIN+" direction="in"/>
<pin name="PD" direction="in"/>
<pin name="CLK_SEL/DF" direction="in"/>
<pin name="CLK+" direction="in"/>
<pin name="CLK-" direction="in"/>
<pin name="AGND_2" direction="pas"/>
<pin name="AGND_3" direction="pas"/>
<pin name="AGND_4" direction="pas"/>
<pin name="AGND_5" direction="pas"/>
<pin name="AGND_6" direction="pas"/>
<pin name="AGND_7" direction="pas"/>
<pin name="AGND" direction="pas"/>
<pin name="DGND" direction="pas"/>
<pin name="DRGND_2" direction="pas"/>
<pin name="DRGND_3" direction="pas"/>
<pin name="DRGND" direction="pas"/>
<pin name="(LSB)D0" direction="out"/>
<pin name="D1" direction="out"/>
<pin name="D2" direction="out"/>
<pin name="D3" direction="out"/>
<pin name="D4" direction="out"/>
<pin name="D5" direction="out"/>
<pin name="D6" direction="out"/>
<pin name="D7" direction="out"/>
<pin name="D8" direction="out"/>
<pin name="D9" direction="out"/>
<pin name="D10" direction="out"/>
<pin name="D11" direction="out"/>
<pin name="D12" direction="out"/>
<pin name="D13(MSB)" direction="out"/>
<pin name="OVR" direction="pas"/>
<pin name="DRDY" direction="pas"/>
<pin name="VRP" direction="pas"/>
<pin name="VRN" direction="pas"/>
<pin name="VRM" direction="pas"/>
<pin name="VREF" direction="pas"/>
</symbol>
<symbol name="ADC14C080CISQ">
<pin name="VA_2" direction="pwr"/>
<pin name="VA_3" direction="pwr"/>
<pin name="VA" direction="pwr"/>
<pin name="CLK" direction="in"/>
<pin name="OF/DCS" direction="in"/>
<pin name="VDR" direction="pwr"/>
<pin name="DRDY" direction="in"/>
<pin name="PD" direction="in"/>
<pin name="VREF" direction="in"/>
<pin name="VCMO" direction="in"/>
<pin name="VIN+" direction="in"/>
<pin name="VIN-" direction="in"/>
<pin name="VRN" direction="in"/>
<pin name="VRP" direction="in"/>
<pin name="AGND_2" direction="pas"/>
<pin name="AGND_3" direction="pas"/>
<pin name="AGND" direction="pas"/>
<pin name="DRGND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="D0" direction="out"/>
<pin name="D1" direction="out"/>
<pin name="D2" direction="out"/>
<pin name="D3" direction="out"/>
<pin name="D4" direction="out"/>
<pin name="D5" direction="out"/>
<pin name="D6" direction="out"/>
<pin name="D7" direction="out"/>
<pin name="D8" direction="out"/>
<pin name="D9" direction="out"/>
<pin name="D10" direction="out"/>
<pin name="D11" direction="out"/>
<pin name="D12" direction="out"/>
<pin name="D13(MSB)" direction="out"/>
</symbol>
<symbol name="ADC14C105CISQ">
<pin name="VA_2" direction="pwr"/>
<pin name="VA_3" direction="pwr"/>
<pin name="VA" direction="pwr"/>
<pin name="CLK" direction="in"/>
<pin name="OF/DCS" direction="in"/>
<pin name="VDR" direction="pwr"/>
<pin name="DRDY" direction="in"/>
<pin name="PD" direction="in"/>
<pin name="VREF" direction="in"/>
<pin name="VCMO" direction="in"/>
<pin name="VRN" direction="in"/>
<pin name="VRP" direction="in"/>
<pin name="VIN+" direction="in"/>
<pin name="VIN-" direction="in"/>
<pin name="AGND_2" direction="pas"/>
<pin name="AGND_3" direction="pas"/>
<pin name="AGND" direction="pas"/>
<pin name="DRGND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="D0" direction="out"/>
<pin name="D1" direction="out"/>
<pin name="D2" direction="out"/>
<pin name="D3" direction="out"/>
<pin name="D4" direction="out"/>
<pin name="D5" direction="out"/>
<pin name="D6" direction="out"/>
<pin name="D7" direction="out"/>
<pin name="D8" direction="out"/>
<pin name="D9" direction="out"/>
<pin name="D10" direction="out"/>
<pin name="D11" direction="out"/>
<pin name="D12" direction="out"/>
<pin name="D13(MSB)" direction="out"/>
</symbol>
<symbol name="ADC14DS080CISQ">
<pin name="VA_2" direction="pwr"/>
<pin name="VA_3" direction="pwr"/>
<pin name="VA_4" direction="pwr"/>
<pin name="VA_5" direction="pwr"/>
<pin name="VA" direction="pwr"/>
<pin name="VDR_2" direction="pwr"/>
<pin name="VDR_3" direction="pwr"/>
<pin name="VDR_4" direction="pwr"/>
<pin name="VDR" direction="pwr"/>
<pin name="CLK" direction="in"/>
<pin name="SCLK" direction="in"/>
<pin name="WAM" direction="in"/>
<pin name="DLL_LOCK" direction="in"/>
<pin name="DLC" direction="in"/>
<pin name="SCSB" direction="in"/>
<pin name="SPI_EN" direction="in"/>
<pin name="VREF" direction="in"/>
<pin name="OF/DCS" direction="in"/>
<pin name="PD_A" direction="in"/>
<pin name="PD_B" direction="in"/>
<pin name="TEST" direction="in"/>
<pin name="RESET_DLL" direction="in"/>
<pin name="LVDS_BIAS" direction="in"/>
<pin name="VRNB" direction="in"/>
<pin name="VRPB" direction="in"/>
<pin name="VRPA" direction="in"/>
<pin name="VRNA" direction="in"/>
<pin name="VCMOA" direction="in"/>
<pin name="VCMOB" direction="in"/>
<pin name="VINA-" direction="in"/>
<pin name="VINA+" direction="in"/>
<pin name="VINB+" direction="in"/>
<pin name="VINB-" direction="in"/>
<pin name="N/C_2" direction="nc"/>
<pin name="N/C_3" direction="nc"/>
<pin name="N/C_4" direction="nc"/>
<pin name="N/C" direction="nc"/>
<pin name="DRGND_2" direction="pas"/>
<pin name="DRGND_3" direction="pas"/>
<pin name="DRGND" direction="pas"/>
<pin name="AGND_2" direction="pas"/>
<pin name="AGND_3" direction="pas"/>
<pin name="AGND_4" direction="pas"/>
<pin name="AGND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="SD0_A-" direction="out"/>
<pin name="SD0_A+" direction="out"/>
<pin name="SD0_B-" direction="out"/>
<pin name="SD0_B+" direction="out"/>
<pin name="SD1_A-" direction="out"/>
<pin name="SD1_A+" direction="out"/>
<pin name="SD1_B-" direction="out"/>
<pin name="SD1_B+" direction="out"/>
<pin name="OUTCLK-" direction="out"/>
<pin name="OUTCLK+" direction="out"/>
<pin name="FRAME-" direction="out"/>
<pin name="FRAME+" direction="out"/>
<pin name="ORA" direction="out"/>
<pin name="ORB" direction="in"/>
<pin name="SDO" direction="out"/>
<pin name="SDI" direction="in"/>
</symbol>
<symbol name="ADC14DS105CISQ">
<pin name="VA_2" direction="pwr"/>
<pin name="VA_3" direction="pwr"/>
<pin name="VA_4" direction="pwr"/>
<pin name="VA_5" direction="pwr"/>
<pin name="VA" direction="pwr"/>
<pin name="VDR_2" direction="pwr"/>
<pin name="VDR_3" direction="pwr"/>
<pin name="VDR_4" direction="pwr"/>
<pin name="VDR" direction="pwr"/>
<pin name="CLK" direction="in"/>
<pin name="SCLK" direction="in"/>
<pin name="WAM" direction="in"/>
<pin name="DLL_LOCK" direction="in"/>
<pin name="DLC" direction="in"/>
<pin name="SCSB" direction="in"/>
<pin name="SPI_EN" direction="in"/>
<pin name="VREF" direction="in"/>
<pin name="OF/DCS" direction="in"/>
<pin name="PD_A" direction="in"/>
<pin name="PD_B" direction="in"/>
<pin name="TEST" direction="in"/>
<pin name="RESET_DLL" direction="in"/>
<pin name="LVDS_BIAS" direction="in"/>
<pin name="VRNB" direction="in"/>
<pin name="VRPB" direction="in"/>
<pin name="VRPA" direction="in"/>
<pin name="VRNA" direction="in"/>
<pin name="VCMOA" direction="in"/>
<pin name="VCMOB" direction="in"/>
<pin name="VINA-" direction="in"/>
<pin name="VINA+" direction="in"/>
<pin name="VINB+" direction="in"/>
<pin name="VINB-" direction="in"/>
<pin name="N/C_2" direction="nc"/>
<pin name="N/C_3" direction="nc"/>
<pin name="N/C_4" direction="nc"/>
<pin name="N/C" direction="nc"/>
<pin name="DRGND_2" direction="pas"/>
<pin name="DRGND_3" direction="pas"/>
<pin name="DRGND" direction="pas"/>
<pin name="AGND_2" direction="pas"/>
<pin name="AGND_3" direction="pas"/>
<pin name="AGND_4" direction="pas"/>
<pin name="AGND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="SD0_A-" direction="out"/>
<pin name="SD0_A+" direction="out"/>
<pin name="SD0_B-" direction="out"/>
<pin name="SD0_B+" direction="out"/>
<pin name="SD1_A-" direction="out"/>
<pin name="SD1_A+" direction="out"/>
<pin name="SD1_B-" direction="out"/>
<pin name="SD1_B+" direction="out"/>
<pin name="OUTCLK-" direction="out"/>
<pin name="OUTCLK+" direction="out"/>
<pin name="FRAME-" direction="out"/>
<pin name="FRAME+" direction="out"/>
<pin name="ORA" direction="out"/>
<pin name="ORB" direction="in"/>
<pin name="SDO" direction="out"/>
<pin name="SDI" direction="in"/>
</symbol>
<symbol name="ADC14L020CIVY">
<pin name="VA_2" direction="pwr"/>
<pin name="VA" direction="pwr"/>
<pin name="VD" direction="pwr"/>
<pin name="VDR" direction="pwr"/>
<pin name="CLK" direction="in"/>
<pin name="DF/DCS" direction="pas"/>
<pin name="PD" direction="in"/>
<pin name="VIN-" direction="in"/>
<pin name="VIN+" direction="in"/>
<pin name="VREF" direction="in"/>
<pin name="VRM" direction="pas"/>
<pin name="VRN" direction="pas"/>
<pin name="VRP" direction="pas"/>
<pin name="AGND_2" direction="pas"/>
<pin name="AGND_3" direction="pas"/>
<pin name="AGND" direction="pas"/>
<pin name="DGND" direction="pas"/>
<pin name="DRGND" direction="pas"/>
<pin name="(LSB)D0" direction="out"/>
<pin name="D1" direction="out"/>
<pin name="D2" direction="out"/>
<pin name="D3" direction="out"/>
<pin name="D4" direction="out"/>
<pin name="D5" direction="out"/>
<pin name="D6" direction="out"/>
<pin name="D7" direction="out"/>
<pin name="D8" direction="out"/>
<pin name="D9" direction="out"/>
<pin name="D10" direction="out"/>
<pin name="D11" direction="out"/>
<pin name="D12" direction="out"/>
<pin name="D13" direction="out"/>
</symbol>
<symbol name="ADC14L040CIVY">
<pin name="VA_2" direction="pwr"/>
<pin name="VA" direction="pwr"/>
<pin name="VD" direction="pwr"/>
<pin name="VDR" direction="pwr"/>
<pin name="CLK" direction="in"/>
<pin name="DF/DCS" direction="pas"/>
<pin name="PD" direction="in"/>
<pin name="VIN-" direction="in"/>
<pin name="VIN+" direction="in"/>
<pin name="VREF" direction="in"/>
<pin name="VRM" direction="pas"/>
<pin name="VRN" direction="pas"/>
<pin name="VRP" direction="pas"/>
<pin name="AGND_2" direction="pas"/>
<pin name="AGND_3" direction="pas"/>
<pin name="AGND" direction="pas"/>
<pin name="DGND" direction="pas"/>
<pin name="DRGND" direction="pas"/>
<pin name="(LSB)D0" direction="out"/>
<pin name="D1" direction="out"/>
<pin name="D2" direction="out"/>
<pin name="D3" direction="out"/>
<pin name="D4" direction="out"/>
<pin name="D5" direction="out"/>
<pin name="D6" direction="out"/>
<pin name="D7" direction="out"/>
<pin name="D8" direction="out"/>
<pin name="D9" direction="out"/>
<pin name="D10" direction="out"/>
<pin name="D11" direction="out"/>
<pin name="D12" direction="out"/>
<pin name="D13" direction="out"/>
</symbol>
<symbol name="ADC16V130CISQ">
<pin name="VIN-" direction="in"/>
<pin name="VIN+" direction="in"/>
<pin name="VA3.0_2" direction="pwr"/>
<pin name="VA3.0_3" direction="pwr"/>
<pin name="VA3.0" direction="pwr"/>
<pin name="VA1.8_2" direction="pwr"/>
<pin name="VA1.8" direction="pwr"/>
<pin name="VAD1.8" direction="pwr"/>
<pin name="PD" direction="in"/>
<pin name="CLK_SEL/DF" direction="in"/>
<pin name="CLK+" direction="in"/>
<pin name="CLK-" direction="in"/>
<pin name="VREF" direction="pwr"/>
<pin name="VRP_2" direction="pwr"/>
<pin name="VRP" direction="pwr"/>
<pin name="VRM" direction="pas"/>
<pin name="VRN_2" direction="pwr"/>
<pin name="VRN" direction="pwr"/>
<pin name="VDR_2" direction="pwr"/>
<pin name="VDR" direction="pwr"/>
<pin name="AGND_2" direction="pas"/>
<pin name="AGND_3" direction="pas"/>
<pin name="AGND_4" direction="pas"/>
<pin name="AGND_5" direction="pas"/>
<pin name="AGND_6" direction="pas"/>
<pin name="AGND_7" direction="pas"/>
<pin name="AGND" direction="pas"/>
<pin name="DRGND_2" direction="pas"/>
<pin name="DRGND" direction="pas"/>
<pin name="D0+" direction="out"/>
<pin name="D0-" direction="out"/>
<pin name="D1+" direction="out"/>
<pin name="D1-" direction="out"/>
<pin name="D2+" direction="out"/>
<pin name="D2-" direction="out"/>
<pin name="D3+" direction="out"/>
<pin name="D3-" direction="out"/>
<pin name="D4+" direction="out"/>
<pin name="D4-" direction="out"/>
<pin name="D5+" direction="out"/>
<pin name="OR+" direction="out"/>
<pin name="D5-" direction="out"/>
<pin name="OR-" direction="out"/>
<pin name="D6+" direction="out"/>
<pin name="D6-" direction="out"/>
<pin name="D7+" direction="out"/>
<pin name="D7-" direction="out"/>
<pin name="D8+" direction="out"/>
<pin name="D8-" direction="out"/>
<pin name="D9+" direction="out"/>
<pin name="D9-" direction="out"/>
<pin name="D10+" direction="out"/>
<pin name="D10-" direction="out"/>
<pin name="D11+" direction="out"/>
<pin name="D11-" direction="out"/>
<pin name="D12+" direction="out"/>
<pin name="D12-" direction="out"/>
<pin name="D13+" direction="out"/>
<pin name="D13-" direction="out"/>
<pin name="D14+" direction="out"/>
<pin name="D14-" direction="out"/>
<pin name="D15+" direction="out"/>
<pin name="D15-" direction="out"/>
<pin name="OUTCLK-" direction="out"/>
<pin name="OUTCLK+" direction="out"/>
</symbol>
<symbol name="ADC78H89CIMT">
<pin name="AVDD" direction="pwr"/>
<pin name="DVDD" direction="pwr"/>
<pin name="~CS" direction="in"/>
<pin name="DIN" direction="in"/>
<pin name="SCLK" direction="in"/>
<pin name="AIN1" direction="in"/>
<pin name="AIN2" direction="in"/>
<pin name="AIN3" direction="in"/>
<pin name="AIN4" direction="in"/>
<pin name="AIN5" direction="in"/>
<pin name="AIN6" direction="in"/>
<pin name="AIN7" direction="in"/>
<pin name="AIN8" direction="in"/>
<pin name="AGND" direction="pas"/>
<pin name="DGND" direction="pas"/>
<pin name="DOUT" direction="out"/>
</symbol>
<symbol name="ADC78H90CIMT">
<pin name="AVDD" direction="pwr"/>
<pin name="DVDD" direction="pwr"/>
<pin name="AIN1" direction="in"/>
<pin name="AIN2" direction="in"/>
<pin name="AIN3" direction="in"/>
<pin name="AIN4" direction="in"/>
<pin name="AIN5" direction="in"/>
<pin name="AIN6" direction="in"/>
<pin name="AIN7" direction="in"/>
<pin name="AIN8" direction="in"/>
<pin name="~CS" direction="in"/>
<pin name="DIN" direction="in"/>
<pin name="SCLK" direction="in"/>
<pin name="AGND" direction="pas"/>
<pin name="DGND" direction="pas"/>
<pin name="DOUT" direction="out"/>
</symbol>
<symbol name="CLC001AJE-TR13">
<pin name="VDD" direction="pwr"/>
<pin name="VBB" direction="pwr"/>
<pin name="VIN+" direction="in"/>
<pin name="VIN-" direction="in"/>
<pin name="RREF" direction="pas"/>
<pin name="VSS" direction="pwr"/>
<pin name="SDO" direction="out"/>
<pin name="~SDO" direction="out"/>
</symbol>
<symbol name="CLC001AJE">
<pin name="VDD" direction="pwr"/>
<pin name="VBB" direction="pwr"/>
<pin name="VIN+" direction="in"/>
<pin name="VIN-" direction="in"/>
<pin name="RREF" direction="pas"/>
<pin name="VSS" direction="pas"/>
<pin name="SDO" direction="out"/>
<pin name="~SDO" direction="out"/>
</symbol>
<symbol name="CLC020BCQ">
<pin name="VDD_2" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="VDDO" direction="pwr"/>
<pin name="VDDOD" direction="pwr"/>
<pin name="VDDSD" direction="pwr"/>
<pin name="D0" direction="in"/>
<pin name="D1" direction="in"/>
<pin name="D2" direction="in"/>
<pin name="D3" direction="in"/>
<pin name="D4" direction="in"/>
<pin name="D5" direction="in"/>
<pin name="D6" direction="in"/>
<pin name="D7" direction="in"/>
<pin name="D8" direction="in"/>
<pin name="D9" direction="in"/>
<pin name="PCLK" direction="in"/>
<pin name="LOCK_DETECT" direction="in"/>
<pin name="TPG_EN" direction="in"/>
<pin name="RREF" direction="in"/>
<pin name="~SYNC_DET_EN" direction="in"/>
<pin name="VSS_2" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="VSSO" direction="pwr"/>
<pin name="VSSSD" direction="pwr"/>
<pin name="VSSOD" direction="pwr"/>
<pin name="SDO" direction="out"/>
<pin name="~SDO" direction="out"/>
<pin name="TEST_OUT" direction="out"/>
</symbol>
<symbol name="CLC021AVGZ-3.3">
<pin name="RESET" direction="in"/>
<pin name="NRZ/~NRZI" direction="in"/>
<pin name="VSS_2" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="VDD_2" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="EDH_FORCE" direction="in"/>
<pin name="~EDH_ENABLE" direction="in"/>
<pin name="~SMPTE_MODE" direction="in"/>
<pin name="N/C_2" direction="nc"/>
<pin name="D0" direction="in"/>
<pin name="D1" direction="in"/>
<pin name="D2" direction="in"/>
<pin name="D3" direction="in"/>
<pin name="D4" direction="in"/>
<pin name="D5" direction="in"/>
<pin name="D6" direction="in"/>
<pin name="D7" direction="in"/>
<pin name="D8" direction="in"/>
<pin name="D9" direction="in"/>
<pin name="PCLK" direction="in"/>
<pin name="VSSO" direction="pwr"/>
<pin name="VDDO" direction="pwr"/>
<pin name="TPG_ENB" direction="in"/>
<pin name="VSSOD_2" direction="pwr"/>
<pin name="VSSOD" direction="pwr"/>
<pin name="VDDOD_2" direction="pwr"/>
<pin name="VDDOD_3" direction="pwr"/>
<pin name="N/C" direction="nc"/>
<pin name="RREF" direction="in"/>
<pin name="VDDOD" direction="pwr"/>
<pin name="VSSSD" direction="pwr"/>
<pin name="VDDSD" direction="pwr"/>
<pin name="~SYNC.~DET.~ENB" direction="in"/>
<pin name="TEST_OUT" direction="out"/>
<pin name="H/LFB0" direction="out"/>
<pin name="V/LFB1" direction="out"/>
<pin name="F/LFB2" direction="out"/>
<pin name="LOCK_DET" direction="out"/>
<pin name="SDO" direction="out"/>
<pin name="~SDO" direction="out"/>
<pin name="NSP" direction="out"/>
<pin name="ANC" direction="out"/>
<pin name="PAL/~NTSC" direction="out"/>
</symbol>
<symbol name="CLC021AVGZ-5.0">
<pin name="RESET" direction="in"/>
<pin name="NRZ/~NRZI" direction="in"/>
<pin name="VSS_2" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="VDD_2" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="EDH_FORCE" direction="in"/>
<pin name="~EDH_ENABLE" direction="in"/>
<pin name="~SMPTE_MODE" direction="in"/>
<pin name="N/C_2" direction="nc"/>
<pin name="D0" direction="in"/>
<pin name="D1" direction="in"/>
<pin name="D2" direction="in"/>
<pin name="D3" direction="in"/>
<pin name="D4" direction="in"/>
<pin name="D5" direction="in"/>
<pin name="D6" direction="in"/>
<pin name="D7" direction="in"/>
<pin name="D8" direction="in"/>
<pin name="D9" direction="in"/>
<pin name="PCLK" direction="in"/>
<pin name="VSSO" direction="pwr"/>
<pin name="VDDO" direction="pwr"/>
<pin name="TPG_ENB" direction="in"/>
<pin name="VSSOD_2" direction="pwr"/>
<pin name="VSSOD" direction="pwr"/>
<pin name="VDDOD_2" direction="pwr"/>
<pin name="VDDOD_3" direction="pwr"/>
<pin name="N/C" direction="nc"/>
<pin name="RREF" direction="in"/>
<pin name="VDDOD" direction="pwr"/>
<pin name="VSSSD" direction="pwr"/>
<pin name="VDDSD" direction="pwr"/>
<pin name="~SYNC.~DET.~ENB" direction="in"/>
<pin name="TEST_OUT" direction="out"/>
<pin name="H/LFB0" direction="out"/>
<pin name="V/LFB1" direction="out"/>
<pin name="F/LFB2" direction="out"/>
<pin name="LOCK_DET" direction="out"/>
<pin name="SDO" direction="out"/>
<pin name="~SDO" direction="out"/>
<pin name="NSP" direction="out"/>
<pin name="ANC" direction="out"/>
<pin name="PAL/~NTSC" direction="out"/>
</symbol>
<symbol name="DAC0808LCN">
<pin name="VCC" direction="pwr"/>
<pin name="VEE" direction="pwr"/>
<pin name="VREF(+)" direction="in"/>
<pin name="VREF(-)" direction="in"/>
<pin name="COMP" direction="pas"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="A5" direction="in"/>
<pin name="A6" direction="in"/>
<pin name="A7" direction="in"/>
<pin name="A8" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="IO" direction="out"/>
</symbol>
<symbol name="DAC081S101CIMM">
<pin name="VA" direction="pwr"/>
<pin name="SCLK" direction="in"/>
<pin name="~SYNC" direction="in"/>
<pin name="DIN" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="DAC082S085CIMM">
<pin name="VA" direction="pwr"/>
<pin name="SCLK" direction="in"/>
<pin name="~SYNC" direction="in"/>
<pin name="VREFIN" direction="in"/>
<pin name="DIN" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="VOUTA" direction="out"/>
<pin name="VOUTB" direction="out"/>
</symbol>
<symbol name="DAC0832LCN">
<pin name="VCC" direction="pwr"/>
<pin name="VREF" direction="in"/>
<pin name="~CS" direction="in"/>
<pin name="~WR1" direction="in"/>
<pin name="~WR2" direction="in"/>
<pin name="RFB" direction="pas"/>
<pin name="~XFER" direction="in"/>
<pin name="DI0" direction="in"/>
<pin name="DI1" direction="in"/>
<pin name="DI2" direction="in"/>
<pin name="DI3" direction="in"/>
<pin name="DI4" direction="in"/>
<pin name="DI5" direction="in"/>
<pin name="DI6" direction="in"/>
<pin name="DI7" direction="in"/>
<pin name="ILE(BYTE1/~BYTE2)" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IOUT1" direction="out"/>
<pin name="IOUT2" direction="out"/>
</symbol>
<symbol name="DAC084S085CIMM">
<pin name="VA" direction="pwr"/>
<pin name="SCLK" direction="in"/>
<pin name="~SYNC" direction="in"/>
<pin name="VREFIN" direction="in"/>
<pin name="DIN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUTA" direction="out"/>
<pin name="VOUTB" direction="out"/>
<pin name="VOUTC" direction="out"/>
<pin name="VOUTD" direction="out"/>
</symbol>
<symbol name="DAC101S101CIMM">
<pin name="VA" direction="pwr"/>
<pin name="SCLK" direction="in"/>
<pin name="~SYNC" direction="in"/>
<pin name="DIN" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="DAC108S085CIMT">
<pin name="VA" direction="pwr"/>
<pin name="SCLK" direction="in"/>
<pin name="~SYNC" direction="in"/>
<pin name="VREF1" direction="in"/>
<pin name="VREF2" direction="in"/>
<pin name="DIN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="DOUT" direction="out"/>
<pin name="VOUTA" direction="out"/>
<pin name="VOUTB" direction="pwr"/>
<pin name="VOUTC" direction="pas"/>
<pin name="VOUTD" direction="in"/>
<pin name="VOUTE" direction="out"/>
<pin name="VOUTF" direction="out"/>
<pin name="VOUTG" direction="out"/>
<pin name="VOUTH" direction="out"/>
</symbol>
<symbol name="DAC121S101CIMK">
<pin name="VA" direction="pwr"/>
<pin name="SCLK" direction="in"/>
<pin name="~SYNC" direction="in"/>
<pin name="DIN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="DAC128S085CIMT">
<pin name="VA" direction="pwr"/>
<pin name="SCLK" direction="in"/>
<pin name="~SYNC" direction="in"/>
<pin name="DIN" direction="in"/>
<pin name="VREF1" direction="in"/>
<pin name="VREF2" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="DOUT" direction="out"/>
<pin name="VOUTA" direction="out"/>
<pin name="VOUTB" direction="out"/>
<pin name="VOUTC" direction="out"/>
<pin name="VOUTD" direction="out"/>
<pin name="VOUTE" direction="out"/>
<pin name="VOUTF" direction="out"/>
<pin name="VOUTG" direction="out"/>
<pin name="VOUTH" direction="out"/>
</symbol>
<symbol name="DP83816AVNG_A">
<pin name="IAUXVDD_2" direction="pwr"/>
<pin name="IAUXVDD" direction="pwr"/>
<pin name="PCIVDD" direction="pwr"/>
<pin name="AUXVDD_2" direction="pwr"/>
<pin name="AUXVDD_3" direction="pwr"/>
<pin name="AUXVDD_4" direction="pwr"/>
<pin name="AUXVDD_5" direction="pwr"/>
<pin name="AUXVDD_6" direction="pwr"/>
<pin name="AUXVDD" direction="pwr"/>
<pin name="RXCLK" direction="in"/>
<pin name="TXCLK" direction="in"/>
<pin name="PCICLK" direction="in"/>
<pin name="VREF" direction="in"/>
<pin name="RXD0/MA6"/>
<pin name="RXD1/MA7"/>
<pin name="RXD2/MA8"/>
<pin name="RXD3/MA9"/>
<pin name="RXER/MA10"/>
<pin name="RXDV/MA11"/>
<pin name="X1" direction="in"/>
<pin name="C1" direction="pas"/>
<pin name="COL/MA16" direction="in"/>
<pin name="CRS" direction="in"/>
<pin name="MDIO"/>
<pin name="REGEN" direction="nc"/>
<pin name="RSTN" direction="in"/>
<pin name="TPRDM" direction="in"/>
<pin name="GNTN" direction="in"/>
<pin name="TPRDP" direction="in"/>
<pin name="RESERVED_2" direction="nc"/>
<pin name="RESERVED" direction="nc"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="VSS_2" direction="pas"/>
<pin name="VSS_3" direction="pas"/>
<pin name="VSS_4" direction="pas"/>
<pin name="VSS_5" direction="pas"/>
<pin name="VSS_6" direction="pas"/>
<pin name="VSS_7" direction="pas"/>
<pin name="VSS_8" direction="pas"/>
<pin name="VSS_9" direction="pas"/>
<pin name="VSS_10" direction="pas"/>
<pin name="VSS_11" direction="pas"/>
<pin name="VSS_12" direction="pas"/>
<pin name="VSS_13" direction="pas"/>
<pin name="VSS_14" direction="pas"/>
<pin name="VSS" direction="pas"/>
<pin name="MDC" direction="out"/>
<pin name="RXOE" direction="out"/>
<pin name="X2" direction="out"/>
<pin name="TXEN" direction="out"/>
<pin name="REQN" direction="out"/>
<pin name="MA3/EEDI" direction="out"/>
<pin name="MA4/EECLK" direction="out"/>
<pin name="MA5" direction="out"/>
<pin name="TXD0/MA12" direction="out"/>
<pin name="TXD1/MA13" direction="out"/>
<pin name="TXD2/MA14" direction="out"/>
<pin name="TXD3/MA15" direction="out"/>
<pin name="TPTDM" direction="out"/>
<pin name="TPTDP" direction="out"/>
<pin name="PMEN/CLKRUNN"/>
<pin name="INTAN" direction="out"/>
<pin name="AD31"/>
<pin name="AD30"/>
<pin name="AD29"/>
<pin name="AD28"/>
<pin name="AD27"/>
<pin name="AD26"/>
</symbol>
<symbol name="DP83816AVNG_B">
<pin name="PCIVDD_2" direction="pwr"/>
<pin name="PCIVDD_3" direction="pwr"/>
<pin name="PCIVDD_4" direction="pwr"/>
<pin name="AUXVDD" direction="pwr"/>
<pin name="3VAUX" direction="in"/>
<pin name="FRAMEN"/>
<pin name="IRDYN"/>
<pin name="IDSEL" direction="in"/>
<pin name="TRDYN"/>
<pin name="PCIVDD" direction="pwr"/>
<pin name="DEVSELN"/>
<pin name="STOPN"/>
<pin name="PERRN"/>
<pin name="SERRN"/>
<pin name="PAR"/>
<pin name="PWRGOOD" direction="in"/>
<pin name="RESERVED" direction="nc"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="VSS_2" direction="pas"/>
<pin name="VSS_3" direction="pas"/>
<pin name="VSS_4" direction="pas"/>
<pin name="VSS_5" direction="pas"/>
<pin name="VSS" direction="pas"/>
<pin name="CBEN2"/>
<pin name="CBEN3"/>
<pin name="CBEN1"/>
<pin name="CBEN0"/>
<pin name="AD0"/>
<pin name="AD1"/>
<pin name="AD2"/>
<pin name="AD3"/>
<pin name="AD4"/>
<pin name="AD5"/>
<pin name="AD6"/>
<pin name="AD7"/>
<pin name="AD8"/>
<pin name="AD9"/>
<pin name="AD10"/>
<pin name="AD11"/>
<pin name="AD12"/>
<pin name="AD13"/>
<pin name="AD14"/>
<pin name="AD15"/>
<pin name="AD16"/>
<pin name="AD17"/>
<pin name="AD18"/>
<pin name="AD19"/>
<pin name="AD20"/>
<pin name="AD21"/>
<pin name="AD22"/>
<pin name="AD23"/>
<pin name="AD24"/>
<pin name="AD25"/>
<pin name="EESEL" direction="out"/>
<pin name="MCSN" direction="out"/>
<pin name="MRDN" direction="out"/>
<pin name="MWRN" direction="out"/>
<pin name="MD1/CFGDISN"/>
<pin name="MD0"/>
<pin name="MD2"/>
<pin name="MD3"/>
<pin name="MD4/EEDO"/>
<pin name="MD5"/>
<pin name="MD6"/>
<pin name="MD7"/>
<pin name="MA0/LEDACTN" direction="out"/>
<pin name="MA1/LED10N" direction="out"/>
<pin name="MA2/LED100N" direction="out"/>
</symbol>
<symbol name="DP83848CVV">
<pin name="AVDD33" direction="pwr"/>
<pin name="IOVDD3" direction="pwr"/>
<pin name="IOVDD33" direction="pwr"/>
<pin name="TX_EN" direction="in"/>
<pin name="TXD_0" direction="in"/>
<pin name="TXD_1" direction="in"/>
<pin name="TXD_2" direction="in"/>
<pin name="TXD_3/SNI_MODE" direction="in"/>
<pin name="PWR_DOWN/INT" direction="in"/>
<pin name="PFBIN1" direction="in"/>
<pin name="PFBIN2" direction="in"/>
<pin name="RBIAS" direction="in"/>
<pin name="RESET_N" direction="in"/>
<pin name="MDC" direction="in"/>
<pin name="X1" direction="in"/>
<pin name="AGND_2" direction="pas"/>
<pin name="AGND" direction="pas"/>
<pin name="DGND" direction="pas"/>
<pin name="IOGND_2" direction="pas"/>
<pin name="IOGND" direction="pas"/>
<pin name="RD-"/>
<pin name="RD+"/>
<pin name="TD-"/>
<pin name="TD+"/>
<pin name="RESERVED_2"/>
<pin name="RESERVED_3"/>
<pin name="RESERVED_4"/>
<pin name="RESERVED_5"/>
<pin name="RESERVED_6"/>
<pin name="RESERVED_7"/>
<pin name="RESERVED"/>
<pin name="COL/PHYAD0" direction="out"/>
<pin name="RXD_0/PHYAD1" direction="out"/>
<pin name="RXD_1/PHYAD2" direction="out"/>
<pin name="RXD_2/PHYAD3" direction="out"/>
<pin name="RXD_3/PHYAD4" direction="out"/>
<pin name="X2" direction="out"/>
<pin name="MDIO"/>
<pin name="PFBOUT" direction="out"/>
<pin name="RX_CLK" direction="out"/>
<pin name="TX_CLK" direction="out"/>
<pin name="25MHZ_OUT" direction="out"/>
<pin name="LED_ACT/COL/AN_" direction="out"/>
<pin name="LED_SPEED/AN1" direction="out"/>
<pin name="LED_LINK/AN0" direction="out"/>
<pin name="RX_ER/MDIX_EN" direction="out"/>
<pin name="RX_DV/MII_MODE" direction="out"/>
<pin name="CRS/CRS_DV/LED_CFG" direction="out"/>
</symbol>
<symbol name="DP83848HSQ">
<pin name="AVDD33" direction="pwr"/>
<pin name="IOVDD33" direction="pwr"/>
<pin name="IO_VDD33" direction="pwr"/>
<pin name="X1" direction="in"/>
<pin name="PFBIN1" direction="in"/>
<pin name="PFBIN2" direction="in"/>
<pin name="RBIAS" direction="in"/>
<pin name="RESET_N" direction="in"/>
<pin name="MDC" direction="in"/>
<pin name="TX_EN" direction="in"/>
<pin name="TXD_0" direction="in"/>
<pin name="TXD_1" direction="in"/>
<pin name="TXD_2" direction="in"/>
<pin name="TXD_3" direction="in"/>
<pin name="IOGND" direction="pas"/>
<pin name="AGND_2" direction="pas"/>
<pin name="DGND" direction="pas"/>
<pin name="AGND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="RX_CLK" direction="out"/>
<pin name="TX_CLK" direction="out"/>
<pin name="X2" direction="out"/>
<pin name="RD-"/>
<pin name="RD+"/>
<pin name="TD_-"/>
<pin name="TD_+"/>
<pin name="RESERVED_2"/>
<pin name="RESERVED_3"/>
<pin name="RESERVED"/>
<pin name="COL/PHYAD0" direction="out"/>
<pin name="RXD_0/PHYAD1" direction="out"/>
<pin name="RXD_1/PHYAD2" direction="out"/>
<pin name="RXD_2/PHYAD3" direction="out"/>
<pin name="RXD_3/PHYAD4" direction="out"/>
<pin name="MDIO"/>
<pin name="PFBOUT" direction="out"/>
<pin name="25MHZ_OUT" direction="out"/>
<pin name="LED_LINK/AN0" direction="out"/>
<pin name="RX_DV/MII_MODE" direction="out"/>
<pin name="CRS/CRS_DV/LED_CFG" direction="out"/>
<pin name="RX_ER/MDIX_EN" direction="out"/>
</symbol>
<symbol name="DP83848MSQ">
<pin name="AVDD33" direction="pwr"/>
<pin name="IOVDD33" direction="pwr"/>
<pin name="IO_VDD33" direction="pwr"/>
<pin name="TX_CLK" direction="out"/>
<pin name="TX_EN" direction="in"/>
<pin name="X1" direction="in"/>
<pin name="TXD_0" direction="in"/>
<pin name="TXD_1" direction="in"/>
<pin name="TXD_2" direction="in"/>
<pin name="TXD_3" direction="in"/>
<pin name="RD-"/>
<pin name="RD+"/>
<pin name="TD_-"/>
<pin name="TD_+"/>
<pin name="PFBIN1" direction="in"/>
<pin name="PFBIN2" direction="in"/>
<pin name="RBIAS" direction="in"/>
<pin name="RESET_N" direction="in"/>
<pin name="MDC" direction="in"/>
<pin name="RESERVED_2"/>
<pin name="RESERVED_3"/>
<pin name="RESERVED"/>
<pin name="GND" direction="pas"/>
<pin name="AGND_2" direction="pas"/>
<pin name="AGND" direction="pas"/>
<pin name="DGND" direction="pas"/>
<pin name="IOGND" direction="pwr"/>
<pin name="X2" direction="out"/>
<pin name="MDIO"/>
<pin name="PFBOUT" direction="out"/>
<pin name="RX_CLK" direction="out"/>
<pin name="25MHZ_OUT" direction="out"/>
<pin name="LED_LINK/AN0"/>
<pin name="RX_DVMI_MODE" direction="out"/>
<pin name="RX_ER/MDIX_EN" direction="out"/>
<pin name="COL/PHYAD0" direction="out"/>
<pin name="RXD_0/PHYAD1" direction="out"/>
<pin name="RXD_1/PHYAD2" direction="out"/>
<pin name="RXD_2/PHYAD3" direction="out"/>
<pin name="RXD_3/PHYAD4" direction="out"/>
<pin name="CRS/CRS_DV/LED_CFG" direction="out"/>
</symbol>
<symbol name="DP83848TSQ">
<pin name="AVDD33" direction="pwr"/>
<pin name="IOVDD33" direction="pwr"/>
<pin name="IO_VDD33" direction="pwr"/>
<pin name="X1" direction="in"/>
<pin name="PFBIN1" direction="in"/>
<pin name="PFBIN2" direction="in"/>
<pin name="RBIAS" direction="in"/>
<pin name="RESET_N" direction="in"/>
<pin name="MDC" direction="in"/>
<pin name="TX_EN" direction="in"/>
<pin name="TXD_0" direction="in"/>
<pin name="TXD_1" direction="in"/>
<pin name="TXD_2" direction="in"/>
<pin name="TXD_3" direction="in"/>
<pin name="IOGND" direction="pas"/>
<pin name="AGND_2" direction="pas"/>
<pin name="DGND" direction="pas"/>
<pin name="AGND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="RX_CLK" direction="out"/>
<pin name="TX_CLK" direction="out"/>
<pin name="X2" direction="out"/>
<pin name="RD-"/>
<pin name="RD+"/>
<pin name="TD_-"/>
<pin name="TD_+"/>
<pin name="RESERVED_2"/>
<pin name="RESERVED_3"/>
<pin name="RESERVED"/>
<pin name="COL/PHYAD0" direction="out"/>
<pin name="RXD_0/PHYAD1" direction="out"/>
<pin name="RXD_1/PHYAD2" direction="out"/>
<pin name="RXD_2/PHYAD3" direction="out"/>
<pin name="RXD_3/PHYAD4" direction="out"/>
<pin name="MDIO"/>
<pin name="PFBOUT" direction="out"/>
<pin name="25MHZ_OUT" direction="out"/>
<pin name="LED_LINK/AN0" direction="out"/>
<pin name="RX_DV/MII_MODE" direction="out"/>
<pin name="CRS/CRS_DV/LED_CFG" direction="out"/>
<pin name="RX_ER/MDIX_EN" direction="out"/>
</symbol>
<symbol name="DP83848VYB">
<pin name="IOVDD33_2" direction="pwr"/>
<pin name="IOVDD33" direction="pwr"/>
<pin name="AVDD33" direction="pwr"/>
<pin name="TDI" direction="in"/>
<pin name="MDC" direction="in"/>
<pin name="RESET" direction="in"/>
<pin name="X1" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="TMS" direction="in"/>
<pin name="TRST" direction="in"/>
<pin name="TXD_0" direction="in"/>
<pin name="TXD_1" direction="in"/>
<pin name="TXD_2" direction="in"/>
<pin name="TXD_3/SNI_MODE" direction="in"/>
<pin name="TX_EN" direction="in"/>
<pin name="PFBIN1" direction="in"/>
<pin name="PFBIN2" direction="in"/>
<pin name="PWR_DOWN/INT" direction="in"/>
<pin name="IOGND_2" direction="pas"/>
<pin name="IOGND" direction="pas"/>
<pin name="AGND_2" direction="pas"/>
<pin name="AGND" direction="pas"/>
<pin name="DGND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="X2" direction="out"/>
<pin name="TDO" direction="out"/>
<pin name="MDIO"/>
<pin name="TX_CLK" direction="out"/>
<pin name="RX_CLK" direction="out"/>
<pin name="TD+"/>
<pin name="TD-"/>
<pin name="RD+"/>
<pin name="RD-"/>
<pin name="RXD_0/PHYAD1" direction="out"/>
<pin name="RXD_1/PHYAD2" direction="out"/>
<pin name="RXD_2/PHYAD3" direction="out"/>
<pin name="RXD_3/PHYAD4" direction="out"/>
<pin name="RESERVED_2"/>
<pin name="RESERVED"/>
<pin name="RBIAS" direction="in"/>
<pin name="PFBOUT" direction="out"/>
<pin name="25MHZ_OUT" direction="out"/>
<pin name="COL/PHYAD0" direction="out"/>
<pin name="LED_ACT/COL/AN_EN" direction="out"/>
<pin name="CRS/CRS_DV/LED_CFG" direction="out"/>
<pin name="LED_SPEED/AN1" direction="out"/>
<pin name="LED_LINK/AN0" direction="out"/>
<pin name="RX_ER/MDIX_EN" direction="out"/>
<pin name="RX_DV/MII_MODE" direction="out"/>
</symbol>
<symbol name="DP83848YB">
<pin name="IOVDD33_2" direction="pwr"/>
<pin name="AVDD33" direction="pwr"/>
<pin name="IOVDD33" direction="pas"/>
<pin name="TCK" direction="in"/>
<pin name="TX_EN" direction="in"/>
<pin name="TXD_0" direction="in"/>
<pin name="TXD_1" direction="in"/>
<pin name="TXD_2" direction="in"/>
<pin name="TXD_3/SNI_MODE" direction="in"/>
<pin name="PWR_DOWN/INT" direction="in"/>
<pin name="TMS" direction="in"/>
<pin name="TRST" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="RD-"/>
<pin name="RD+"/>
<pin name="TD-"/>
<pin name="TD+"/>
<pin name="PFBIN1" direction="in"/>
<pin name="PFBIN2" direction="in"/>
<pin name="PFBOUT" direction="out"/>
<pin name="RBIAS" direction="in"/>
<pin name="RESET_N" direction="in"/>
<pin name="MDC" direction="in"/>
<pin name="X1" direction="in"/>
<pin name="RESERVED_2"/>
<pin name="RESERVED"/>
<pin name="EP" direction="pas"/>
<pin name="AGND_2" direction="pas"/>
<pin name="AGND" direction="pas"/>
<pin name="DGND" direction="pas"/>
<pin name="IOGND_2" direction="pas"/>
<pin name="IOGND" direction="pas"/>
<pin name="X2" direction="out"/>
<pin name="TX_CLK" direction="out"/>
<pin name="RX_CLK" direction="out"/>
<pin name="TDO" direction="out"/>
<pin name="MDIO"/>
<pin name="25MHZ_OUT" direction="out"/>
<pin name="LED_ACT/COL/AN_EN" direction="out"/>
<pin name="LED_SPEED/AN1" direction="out"/>
<pin name="LED_LINK/AN0" direction="out"/>
<pin name="RX_DV/MII_MODE" direction="out"/>
<pin name="CRS/CRS_DV/LED_CFG" direction="out"/>
<pin name="RX_ER/MDIX_EN" direction="out"/>
<pin name="COL/PHYAD0" direction="out"/>
<pin name="RXD_0/PHYAD1" direction="out"/>
<pin name="RXD_1/PHYAD2" direction="out"/>
<pin name="RXD_2/PHYAD3" direction="out"/>
<pin name="RXD_3/PHYAD4" direction="out"/>
</symbol>
<symbol name="DP83849CVS">
<pin name="ANA33VDD" direction="pwr"/>
<pin name="IOVDD1" direction="pwr"/>
<pin name="IOVDD2" direction="pwr"/>
<pin name="IOVDD3" direction="pwr"/>
<pin name="IOVDD4" direction="pwr"/>
<pin name="X1" direction="in"/>
<pin name="MDC" direction="in"/>
<pin name="RBIAS" direction="in"/>
<pin name="PFBIN1" direction="in"/>
<pin name="PFBIN2" direction="in"/>
<pin name="PFBIN3" direction="in"/>
<pin name="PFBIN4" direction="in"/>
<pin name="RESET_N" direction="in"/>
<pin name="PWRDOWN_INT_A" direction="in"/>
<pin name="PWRDOWN_INT_B" direction="in"/>
<pin name="TXD0_A" direction="in"/>
<pin name="TXD1_A" direction="in"/>
<pin name="TXD2_A" direction="in"/>
<pin name="TXD3_A/SNI_MODE_A" direction="in"/>
<pin name="TXD3_B/SNI_MODE_B" direction="in"/>
<pin name="TXD2_B" direction="in"/>
<pin name="TX_EN_A" direction="in"/>
<pin name="TXD0_B" direction="in"/>
<pin name="TXD1_B" direction="in"/>
<pin name="TX_EN_B" direction="in"/>
<pin name="RX_DV_B/MII_MODE_B" direction="in"/>
<pin name="CDGND1" direction="pas"/>
<pin name="IOGND1" direction="pas"/>
<pin name="IOGND2" direction="pas"/>
<pin name="CDGND2" direction="pas"/>
<pin name="ANAGND1" direction="pas"/>
<pin name="ANAGND2" direction="pas"/>
<pin name="ANAGND3" direction="pas"/>
<pin name="ANAGND4" direction="pas"/>
<pin name="IOGND3" direction="pas"/>
<pin name="IOGND4" direction="pas"/>
<pin name="COREGND1" direction="pas"/>
<pin name="COREGND2" direction="pas"/>
<pin name="MDIO"/>
<pin name="PFBOUT" direction="out"/>
<pin name="CLK2MAC" direction="out"/>
<pin name="X2" direction="out"/>
<pin name="COL_A" direction="out"/>
<pin name="COL_B" direction="out"/>
<pin name="RXD2_B" direction="out"/>
<pin name="CRS_A/CRS_DV_A/LED_CFG_A" direction="out"/>
<pin name="RX_ER_A/MDIX_EN_A" direction="out"/>
<pin name="RX_CLK_A" direction="out"/>
<pin name="RXD0_A/PHYAD1" direction="out"/>
<pin name="RXD1_A/PHYAD2" direction="out"/>
<pin name="RXD2_A/CLK2MAC_DIS" direction="out"/>
<pin name="RXD3_A/ED_EN_A" direction="out"/>
<pin name="RXD3_B/ED_EN_B" direction="out"/>
<pin name="LED_LINK_A/AN0_A"/>
<pin name="LED_SPEED_A/AN1_A"/>
<pin name="TPRDM_A"/>
<pin name="TPRDP_A"/>
<pin name="TPTDM_A"/>
<pin name="TPTDP_A"/>
<pin name="TPTDP_B"/>
<pin name="TPTDM_B"/>
<pin name="TPRDP_B"/>
<pin name="TPRDM_B"/>
<pin name="LED_ACT/LED_COL/AN_EN_A"/>
<pin name="LED_ACT/LED_COL/AN_EN_B"/>
<pin name="LED_SPEED_B/AN1_B"/>
<pin name="LED_LINK_B/AN0_B"/>
<pin name="RXD0_B/PHYAD3" direction="out"/>
<pin name="RXD1_B/PHYAD4" direction="out"/>
<pin name="RX_DV_A/MII_MODE_A" direction="out"/>
<pin name="RX_ER_B/MDIX_EN_B" direction="out"/>
<pin name="CRS_B/CRS_DV_B/LED_CFG_B" direction="out"/>
<pin name="TX_CLK_A" direction="out"/>
<pin name="TX_CLK_B" direction="out"/>
<pin name="RX_CLK_B" direction="out"/>
<pin name="RESERVED_2"/>
<pin name="RESERVED_3"/>
<pin name="RESERVED_4"/>
<pin name="RESERVED_5"/>
<pin name="RESERVED"/>
</symbol>
<symbol name="DP83865DVH_A">
<pin name="VDD_SEL_STRAP" direction="pwr"/>
<pin name="IO_VDD_2" direction="pwr"/>
<pin name="IO_VDD_3" direction="pwr"/>
<pin name="IO_VDD_4" direction="pwr"/>
<pin name="IO_VDD_5" direction="pwr"/>
<pin name="IO_VDD_6" direction="pwr"/>
<pin name="IO_VDD_7" direction="pwr"/>
<pin name="IO_VDD_8" direction="pwr"/>
<pin name="IO_VDD" direction="pwr"/>
<pin name="CORE_VDD_2" direction="pwr"/>
<pin name="CORE_VDD_3" direction="pwr"/>
<pin name="CORE_VDD_4" direction="pwr"/>
<pin name="CORE_VDD_5" direction="pwr"/>
<pin name="CORE_VDD_6" direction="pwr"/>
<pin name="CORE_VDD" direction="pwr"/>
<pin name="TCK" direction="in"/>
<pin name="~RESET" direction="in"/>
<pin name="~TRST" direction="in"/>
<pin name="TMS" direction="in"/>
<pin name="TX_ER" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="PHYADDR1_STRAP"/>
<pin name="PHYADDR3_STRAP"/>
<pin name="ACTIVITY_LED_/_SPEED0_STRAP"/>
<pin name="DUPLEX_LED_/_PHYADDR0_STRAP"/>
<pin name="NON_IEEE_STRAP"/>
<pin name="LINK10_LED_/_RLED/SPEED1_STRAP"/>
<pin name="LINK100_LED_/_DUPLEX_STRAP"/>
<pin name="LINK1000_LED_/_AN_EN_STRAP"/>
<pin name="TX_TCLK_/_MAN_MDIX_STRAP"/>
<pin name="TX_CLK/RGMII_SEL1" direction="in"/>
<pin name="TX_EN/TXEN_ER" direction="in"/>
<pin name="RESERVED_2" direction="pas"/>
<pin name="RESERVED" direction="pas"/>
<pin name="VSS_2" direction="pas"/>
<pin name="VSS_3" direction="pas"/>
<pin name="VSS_4" direction="pas"/>
<pin name="VSS_5" direction="pas"/>
<pin name="VSS_6" direction="pas"/>
<pin name="VSS_7" direction="pas"/>
<pin name="VSS_8" direction="pas"/>
<pin name="VSS_9" direction="pas"/>
<pin name="VSS_10" direction="pas"/>
<pin name="VSS_11" direction="pas"/>
<pin name="VSS_12" direction="pas"/>
<pin name="VSS_13" direction="pas"/>
<pin name="VSS_14" direction="pas"/>
<pin name="VSS" direction="pas"/>
<pin name="TDO" direction="out"/>
<pin name="PHYADDR2_STRAP"/>
<pin name="CRS/RGMII_SEL0" direction="out"/>
<pin name="RX_ER/RXDV_ER" direction="out"/>
<pin name="COL/CLK_MAC_FREQ" direction="out"/>
<pin name="RX_DV/RCK" direction="out"/>
<pin name="RX_CLK" direction="out"/>
<pin name="RXD0/RX0" direction="out"/>
<pin name="RXD1/RX1" direction="out"/>
<pin name="RXD2/RX2" direction="out"/>
<pin name="RXD3/RX3" direction="out"/>
<pin name="RXD4" direction="out"/>
<pin name="RXD5" direction="out"/>
<pin name="RXD6" direction="out"/>
<pin name="RXD7" direction="out"/>
<pin name="~INTERRUPT" direction="out"/>
</symbol>
<symbol name="DP83865DVH_B">
<pin name="IO_VDD_2" direction="pwr"/>
<pin name="IO_VDD_3" direction="pwr"/>
<pin name="IO_VDD_4" direction="pwr"/>
<pin name="IO_VDD" direction="pwr"/>
<pin name="CORE_VDD_2" direction="pwr"/>
<pin name="CORE_VDD" direction="pwr"/>
<pin name="1V8_AVDD1_2" direction="pwr"/>
<pin name="1V8_AVDD1_3" direction="pwr"/>
<pin name="1V8_AVDD1_4" direction="pwr"/>
<pin name="1V8_AVDD1_5" direction="pwr"/>
<pin name="1V8_AVDD1" direction="pwr"/>
<pin name="1V8_AVDD2" direction="pwr"/>
<pin name="1V8_AVDD3" direction="pwr"/>
<pin name="2V5_AVDD2" direction="pwr"/>
<pin name="2V5_AVDD1" direction="pwr"/>
<pin name="GTX_CLK/TCK" direction="in"/>
<pin name="CLK_IN" direction="in"/>
<pin name="MAC_CLK_EN_STRAP" direction="in"/>
<pin name="MULTI_EN_STRAP_/_TX_TRIGGER"/>
<pin name="MDIB_P"/>
<pin name="MDIC_P"/>
<pin name="MDID_P"/>
<pin name="MDIC_N"/>
<pin name="MDID_N"/>
<pin name="MDC"/>
<pin name="MDIO"/>
<pin name="TXD4" direction="in"/>
<pin name="TXD5" direction="in"/>
<pin name="TXD6" direction="in"/>
<pin name="TXD7" direction="in"/>
<pin name="TXD0/TX0" direction="in"/>
<pin name="TXD1/TX1" direction="in"/>
<pin name="TXD2/TX2" direction="in"/>
<pin name="TXD3/TX3" direction="in"/>
<pin name="MDIX_EN_STRAP"/>
<pin name="RESERVED" direction="pas"/>
<pin name="VSS_2" direction="pas"/>
<pin name="VSS_3" direction="pas"/>
<pin name="VSS_4" direction="pas"/>
<pin name="VSS_5" direction="pas"/>
<pin name="VSS_6" direction="pas"/>
<pin name="VSS_7" direction="pas"/>
<pin name="VSS_8" direction="pas"/>
<pin name="VSS_9" direction="pas"/>
<pin name="VSS_10" direction="pas"/>
<pin name="VSS_11" direction="pas"/>
<pin name="VSS_12" direction="pas"/>
<pin name="VSS_13" direction="pas"/>
<pin name="VSS_14" direction="pas"/>
<pin name="VSS_15" direction="pas"/>
<pin name="VSS_16" direction="pas"/>
<pin name="VSS_17" direction="pas"/>
<pin name="VSS_18" direction="pas"/>
<pin name="VSS_19" direction="pas"/>
<pin name="VSS_20" direction="pas"/>
<pin name="VSS_21" direction="pas"/>
<pin name="VSS" direction="pas"/>
<pin name="CLK_OUT" direction="out"/>
<pin name="CLK_TO_MAC" direction="out"/>
<pin name="PHYADDR4_STRAP"/>
<pin name="BG_REF" direction="in"/>
<pin name="MDIA_N"/>
<pin name="MDIA_P"/>
<pin name="MDIB_N"/>
</symbol>
<symbol name="DS08MB200TSQ">
<pin name="VDD_2" direction="pwr"/>
<pin name="VDD_3" direction="pwr"/>
<pin name="VDD_4" direction="pwr"/>
<pin name="VDD_5" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="ENL_1" direction="in"/>
<pin name="ENL_0" direction="in"/>
<pin name="ENA_1" direction="in"/>
<pin name="ENB_1" direction="in"/>
<pin name="ENA_0" direction="in"/>
<pin name="ENB_0" direction="in"/>
<pin name="LI_1-" direction="in"/>
<pin name="LI_1+" direction="in"/>
<pin name="LI_0-" direction="in"/>
<pin name="LI_0+" direction="in"/>
<pin name="MUX_S1" direction="in"/>
<pin name="MUX_S0" direction="in"/>
<pin name="SIA_1+" direction="in"/>
<pin name="SIA_1-" direction="in"/>
<pin name="SIB_1+" direction="in"/>
<pin name="SIB_1-" direction="in"/>
<pin name="SIB_0-" direction="in"/>
<pin name="SIB_0+" direction="in"/>
<pin name="SIA_0-" direction="in"/>
<pin name="SIA_0+" direction="in"/>
<pin name="N/C_2" direction="nc"/>
<pin name="N/C_3" direction="nc"/>
<pin name="N/C_4" direction="nc"/>
<pin name="N/C_5" direction="nc"/>
<pin name="N/C_6" direction="nc"/>
<pin name="N/C_7" direction="nc"/>
<pin name="N/C" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="DAP" direction="pas"/>
<pin name="SOA_1+" direction="out"/>
<pin name="SOA_1-" direction="out"/>
<pin name="SOB_1+" direction="out"/>
<pin name="SOB_1-" direction="out"/>
<pin name="SOB_0-" direction="out"/>
<pin name="SOB_0+" direction="out"/>
<pin name="SOA_0-" direction="out"/>
<pin name="SOA_0+" direction="out"/>
<pin name="LO_0-" direction="out"/>
<pin name="LO_0+" direction="out"/>
<pin name="LO_1+" direction="out"/>
<pin name="LO_1-" direction="out"/>
</symbol>
<symbol name="DS10BR254TSQ">
<pin name="VDD_2" direction="pwr"/>
<pin name="VDD_3" direction="pwr"/>
<pin name="VDD_4" direction="pwr"/>
<pin name="VDD_5" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="IN1+" direction="in"/>
<pin name="IN1-" direction="in"/>
<pin name="IN2+" direction="in"/>
<pin name="IN2-" direction="in"/>
<pin name="SEL_IN" direction="in"/>
<pin name="~PWDN0" direction="in"/>
<pin name="~PWDN1" direction="in"/>
<pin name="~PWDN2" direction="in"/>
<pin name="~PWDN3" direction="in"/>
<pin name="~PWDN" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC_6" direction="nc"/>
<pin name="NC_7" direction="nc"/>
<pin name="NC_8" direction="nc"/>
<pin name="NC_9" direction="nc"/>
<pin name="NC_10" direction="nc"/>
<pin name="NC_11" direction="nc"/>
<pin name="NC_12" direction="nc"/>
<pin name="NC_13" direction="nc"/>
<pin name="NC_14" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="OUT0+" direction="out"/>
<pin name="OUT0-" direction="out"/>
<pin name="OUT1+" direction="out"/>
<pin name="OUT1-" direction="out"/>
<pin name="OUT2+" direction="out"/>
<pin name="OUT2-" direction="out"/>
<pin name="OUT3+" direction="out"/>
<pin name="OUT3-" direction="out"/>
<pin name="~LOS1" direction="out"/>
<pin name="~LOS2" direction="out"/>
</symbol>
<symbol name="DS10CP152QMA">
<pin name="VCC" direction="pwr"/>
<pin name="SEL0" direction="in"/>
<pin name="SEL1" direction="in"/>
<pin name="EN0" direction="in"/>
<pin name="EN1" direction="in"/>
<pin name="IN0+" direction="in"/>
<pin name="IN0-" direction="in"/>
<pin name="IN1+" direction="in"/>
<pin name="IN1-" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="OUT0+" direction="out"/>
<pin name="OUT0-" direction="out"/>
<pin name="OUT1+" direction="out"/>
<pin name="OUT1-" direction="out"/>
</symbol>
<symbol name="DS10CP152TMA">
<pin name="VCC" direction="pwr"/>
<pin name="SEL0" direction="in"/>
<pin name="SEL1" direction="in"/>
<pin name="EN0" direction="in"/>
<pin name="EN1" direction="in"/>
<pin name="IN0+" direction="in"/>
<pin name="IN0-" direction="in"/>
<pin name="IN1+" direction="in"/>
<pin name="IN1-" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="OUT0+" direction="out"/>
<pin name="OUT0-" direction="out"/>
<pin name="OUT1+" direction="out"/>
<pin name="OUT1-" direction="out"/>
</symbol>
<symbol name="DS10CP154ATSQ">
<pin name="VDD_2" direction="pwr"/>
<pin name="VDD_3" direction="pwr"/>
<pin name="VDD_4" direction="pwr"/>
<pin name="VDD_5" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="IN0+" direction="in"/>
<pin name="IN0-" direction="in"/>
<pin name="IN1+" direction="in"/>
<pin name="IN1-" direction="in"/>
<pin name="IN2+" direction="in"/>
<pin name="IN2-" direction="in"/>
<pin name="IN3-" direction="in"/>
<pin name="IN3+" direction="in"/>
<pin name="EN_SMB" direction="in"/>
<pin name="~PWDN" direction="in"/>
<pin name="S30" direction="in"/>
<pin name="S31" direction="in"/>
<pin name="S10/ADDR0"/>
<pin name="S11/ADDR1"/>
<pin name="S20/ADDR2"/>
<pin name="S21/ADDR3"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC_6" direction="nc"/>
<pin name="NC_7" direction="nc"/>
<pin name="NC_8" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="OUT0+" direction="out"/>
<pin name="OUT0-" direction="out"/>
<pin name="OUT1+" direction="out"/>
<pin name="OUT1-" direction="out"/>
<pin name="OUT2+" direction="out"/>
<pin name="OUT2-" direction="out"/>
<pin name="OUT3+" direction="out"/>
<pin name="OUT3-" direction="out"/>
<pin name="S00/SCL"/>
<pin name="S01/SDA"/>
</symbol>
<symbol name="DS14185WM">
<pin name="V+" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="RIN1" direction="in"/>
<pin name="RIN2" direction="in"/>
<pin name="RIN3" direction="in"/>
<pin name="RIN4" direction="in"/>
<pin name="RIN5" direction="in"/>
<pin name="DIN1" direction="in"/>
<pin name="DIN2" direction="in"/>
<pin name="DIN3" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="GND" direction="pas"/>
<pin name="DOUT1" direction="out"/>
<pin name="DOUT2" direction="out"/>
<pin name="DOUT3" direction="out"/>
<pin name="ROUT5" direction="out"/>
<pin name="ROUT4" direction="out"/>
<pin name="ROUT3" direction="out"/>
<pin name="ROUT2" direction="out"/>
<pin name="ROUT1" direction="out"/>
</symbol>
<symbol name="DS1487M">
<pin name="VCC" direction="pwr"/>
<pin name="RE*" direction="in"/>
<pin name="DE" direction="in"/>
<pin name="DI" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="A"/>
<pin name="B"/>
<pin name="RO" direction="out"/>
</symbol>
<symbol name="DS14C232CM">
<pin name="VCC" direction="pwr"/>
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
<pin name="C1+" direction="pas"/>
<pin name="C1-" direction="pas"/>
<pin name="C2+" direction="pas"/>
<pin name="C2-" direction="pas"/>
<pin name="RIN1" direction="in"/>
<pin name="RIN2" direction="in"/>
<pin name="DIN2" direction="in"/>
<pin name="DIN1" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="DOUT1" direction="out"/>
<pin name="DOUT2" direction="out"/>
<pin name="ROUT1" direction="out"/>
<pin name="ROUT2" direction="out"/>
</symbol>
<symbol name="DS14C232CN">
<pin name="V+" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="C1+" direction="pas"/>
<pin name="C1-" direction="pas"/>
<pin name="C2+" direction="pas"/>
<pin name="C2-" direction="pas"/>
<pin name="DIN1" direction="in"/>
<pin name="DIN2" direction="in"/>
<pin name="RIN1" direction="in"/>
<pin name="RIN2" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="GND" direction="pas"/>
<pin name="ROUT1" direction="out"/>
<pin name="ROUT2" direction="out"/>
<pin name="DOUT1" direction="out"/>
<pin name="DOUT2" direction="out"/>
</symbol>
<symbol name="DS14C232TM">
<pin name="VCC" direction="pwr"/>
<pin name="V+" direction="pwr"/>
<pin name="C1+" direction="pas"/>
<pin name="C1-" direction="pas"/>
<pin name="C2+" direction="pas"/>
<pin name="C2-" direction="pas"/>
<pin name="RIN1" direction="in"/>
<pin name="RIN2" direction="in"/>
<pin name="DIN1" direction="in"/>
<pin name="DIN2" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="GND" direction="pas"/>
<pin name="ROUT1" direction="out"/>
<pin name="ROUT2" direction="out"/>
<pin name="DOUT1" direction="out"/>
<pin name="DOUT2" direction="out"/>
</symbol>
<symbol name="DS14C335MSA">
<pin name="VCC" direction="pwr"/>
<pin name="V+" direction="pwr"/>
<pin name="C1-" direction="pas"/>
<pin name="C1+" direction="pas"/>
<pin name="C2+" direction="pas"/>
<pin name="C2-" direction="pas"/>
<pin name="C3-" direction="pas"/>
<pin name="C3+" direction="pas"/>
<pin name="SD" direction="in"/>
<pin name="DIN1" direction="in"/>
<pin name="DIN2" direction="in"/>
<pin name="DIN3" direction="in"/>
<pin name="RIN5" direction="in"/>
<pin name="RIN1" direction="in"/>
<pin name="RIN2" direction="in"/>
<pin name="RIN3" direction="in"/>
<pin name="RIN4" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="ROUT1" direction="out"/>
<pin name="ROUT2" direction="out"/>
<pin name="ROUT3" direction="out"/>
<pin name="ROUT4" direction="out"/>
<pin name="ROUT5" direction="out"/>
<pin name="DOUT1" direction="out"/>
<pin name="DOUT2" direction="out"/>
<pin name="DOUT3" direction="out"/>
</symbol>
<symbol name="DS14C535MSA">
<pin name="VCC" direction="pwr"/>
<pin name="V+" direction="pwr"/>
<pin name="C1+" direction="pas"/>
<pin name="C1-" direction="pas"/>
<pin name="C2-" direction="pas"/>
<pin name="C2+" direction="pas"/>
<pin name="SD" direction="in"/>
<pin name="DIN1" direction="in"/>
<pin name="DIN2" direction="in"/>
<pin name="DIN3" direction="in"/>
<pin name="RIN5" direction="in"/>
<pin name="RIN1" direction="in"/>
<pin name="RIN2" direction="in"/>
<pin name="RIN3" direction="in"/>
<pin name="RIN4" direction="in"/>
<pin name="N/C_2" direction="nc"/>
<pin name="N/C" direction="nc"/>
<pin name="V-" direction="pwr"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="ROUT1" direction="out"/>
<pin name="ROUT2" direction="out"/>
<pin name="ROUT3" direction="out"/>
<pin name="ROUT4" direction="out"/>
<pin name="ROUT5" direction="out"/>
<pin name="DOUT1" direction="out"/>
<pin name="DOUT2" direction="out"/>
<pin name="DOUT3" direction="out"/>
</symbol>
<symbol name="DS14C88M">
<pin name="V+" direction="pwr"/>
<pin name="INA" direction="in"/>
<pin name="IN_B1" direction="in"/>
<pin name="IN_B2" direction="in"/>
<pin name="IN_C1" direction="in"/>
<pin name="IN_C2" direction="in"/>
<pin name="IN_D1" direction="in"/>
<pin name="IN_D2" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="GND" direction="pas"/>
<pin name="OUT_A" direction="out"/>
<pin name="OUT_B" direction="out"/>
<pin name="OUT_C" direction="out"/>
<pin name="OUT_D" direction="out"/>
</symbol>
<symbol name="DS14C88N">
<pin name="V+" direction="pwr"/>
<pin name="IN_A" direction="in"/>
<pin name="IN_B1" direction="in"/>
<pin name="IN_B2" direction="in"/>
<pin name="IN_C1" direction="in"/>
<pin name="IN_C2" direction="in"/>
<pin name="IN_D1" direction="in"/>
<pin name="IN_D2" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="GND" direction="pas"/>
<pin name="OUT_A" direction="out"/>
<pin name="OUT_B" direction="out"/>
<pin name="OUT_C" direction="out"/>
<pin name="OUT_D" direction="out"/>
</symbol>
<symbol name="DS14C89AM">
<pin name="VCC" direction="pwr"/>
<pin name="INA" direction="in"/>
<pin name="INB" direction="in"/>
<pin name="INC" direction="nc"/>
<pin name="IND" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
<pin name="OUTC" direction="out"/>
<pin name="OUTD" direction="out"/>
</symbol>
<symbol name="DS14C89AN">
<pin name="VCC" direction="pwr"/>
<pin name="INA" direction="in"/>
<pin name="INB" direction="in"/>
<pin name="INC" direction="nc"/>
<pin name="IND" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
<pin name="OUTC" direction="out"/>
<pin name="OUTD" direction="out"/>
</symbol>
<symbol name="DS15BR400TVS">
<pin name="VDD_2" direction="pwr"/>
<pin name="VDD_3" direction="pwr"/>
<pin name="VDD_4" direction="pwr"/>
<pin name="VDD_5" direction="pwr"/>
<pin name="VDD_6" direction="pwr"/>
<pin name="VDD_7" direction="pwr"/>
<pin name="VDD_8" direction="pwr"/>
<pin name="VDD_9" direction="pwr"/>
<pin name="VDD_10" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="PEM" direction="in"/>
<pin name="~PWDN" direction="in"/>
<pin name="IN0+" direction="in"/>
<pin name="IN0-" direction="in"/>
<pin name="IN1+" direction="in"/>
<pin name="IN1-" direction="in"/>
<pin name="IN2+" direction="in"/>
<pin name="IN2-" direction="in"/>
<pin name="IN3+" direction="in"/>
<pin name="IN3-" direction="in"/>
<pin name="N/C_2" direction="nc"/>
<pin name="N/C_3" direction="nc"/>
<pin name="N/C_4" direction="nc"/>
<pin name="N/C_5" direction="nc"/>
<pin name="N/C_6" direction="nc"/>
<pin name="N/C_7" direction="pas"/>
<pin name="N/C_8" direction="nc"/>
<pin name="N/C_9" direction="nc"/>
<pin name="N/C_10" direction="nc"/>
<pin name="N/C" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="OUT0-" direction="out"/>
<pin name="OUT0+" direction="out"/>
<pin name="OUT1-" direction="out"/>
<pin name="OUT1+" direction="out"/>
<pin name="OUT2-" direction="out"/>
<pin name="OUT2+" direction="out"/>
<pin name="OUT3-" direction="out"/>
<pin name="OUT3+" direction="out"/>
</symbol>
<symbol name="DS15EA101SQ">
<pin name="VCC_2" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="~EN" direction="in"/>
<pin name="IN+" direction="in"/>
<pin name="IN-" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="CAP+" direction="pas"/>
<pin name="CAP-" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="LOS" direction="out"/>
<pin name="OUT+" direction="out"/>
<pin name="OUT-" direction="out"/>
</symbol>
<symbol name="DS15MB200TSQ">
<pin name="VDD_2" direction="pwr"/>
<pin name="VDD_3" direction="pwr"/>
<pin name="VDD_4" direction="pwr"/>
<pin name="VDD_5" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="ENL_1" direction="in"/>
<pin name="ENL_0" direction="in"/>
<pin name="ENA_1" direction="in"/>
<pin name="ENB_1" direction="in"/>
<pin name="ENB_0" direction="in"/>
<pin name="ENA_0" direction="in"/>
<pin name="PREL_0" direction="in"/>
<pin name="PREL_1" direction="in"/>
<pin name="PREA_1" direction="in"/>
<pin name="PREA_0" direction="in"/>
<pin name="PREB_1" direction="in"/>
<pin name="PREB_0" direction="in"/>
<pin name="LI_1+" direction="in"/>
<pin name="LI_1-" direction="in"/>
<pin name="LI_0-" direction="in"/>
<pin name="LI_0+" direction="in"/>
<pin name="SOA_1+" direction="out"/>
<pin name="SOA_1-" direction="out"/>
<pin name="SIA_0-" direction="in"/>
<pin name="SIA_0+" direction="in"/>
<pin name="SIA_1+" direction="in"/>
<pin name="SIA_1-" direction="in"/>
<pin name="SIB_1+" direction="in"/>
<pin name="SIB_1-" direction="in"/>
<pin name="SIB_0-" direction="in"/>
<pin name="SIB_0+" direction="in"/>
<pin name="SOB_1+" direction="out"/>
<pin name="SOB_1-" direction="out"/>
<pin name="MUX_S1" direction="in"/>
<pin name="MUX_S0" direction="in"/>
<pin name="N/C" direction="nc"/>
<pin name="DAP" direction="pas"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="LO_1+" direction="out"/>
<pin name="LO_1-" direction="out"/>
<pin name="LO_0-" direction="out"/>
<pin name="LO_0+" direction="out"/>
<pin name="SOB_0-" direction="out"/>
<pin name="SOB_0+" direction="out"/>
<pin name="SOA_0-" direction="out"/>
<pin name="SOA_0+" direction="out"/>
</symbol>
<symbol name="DS16EV5110SQ">
<pin name="VDD_2" direction="pwr"/>
<pin name="VDD_3" direction="pwr"/>
<pin name="VDD_4" direction="pwr"/>
<pin name="VDD_5" direction="pwr"/>
<pin name="VDD_6" direction="pwr"/>
<pin name="VDD_7" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="EN" direction="in"/>
<pin name="FEB" direction="in"/>
<pin name="C_IN-" direction="in"/>
<pin name="C_IN+" direction="in"/>
<pin name="D_IN0-" direction="in"/>
<pin name="D_IN0+" direction="in"/>
<pin name="D_IN1-" direction="in"/>
<pin name="D_IN1+" direction="in"/>
<pin name="D_IN2-" direction="in"/>
<pin name="D_IN2+" direction="in"/>
<pin name="SDA" direction="in"/>
<pin name="SDC" direction="in"/>
<pin name="CS" direction="in"/>
<pin name="BST_0" direction="in"/>
<pin name="BST_1" direction="in"/>
<pin name="BST_2" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="C_OUT-" direction="out"/>
<pin name="C_OUT+" direction="out"/>
<pin name="D_OUT0-" direction="out"/>
<pin name="D_OUT0+" direction="out"/>
<pin name="D_OUT1-" direction="out"/>
<pin name="D_OUT1+" direction="out"/>
<pin name="D_OUT2-" direction="out"/>
<pin name="D_OUT2+" direction="out"/>
<pin name="SD" direction="out"/>
<pin name="RESERVE_2" direction="pas"/>
<pin name="RESERVE_3" direction="pas"/>
<pin name="RESERVE_4" direction="pas"/>
<pin name="RESERVE_5" direction="pas"/>
<pin name="RESERVE_6" direction="pas"/>
<pin name="RESERVE_7" direction="pas"/>
<pin name="RESERVE_8" direction="pas"/>
<pin name="RESERVE_9" direction="pas"/>
<pin name="RESERVE_10" direction="pas"/>
<pin name="RESERVE" direction="pas"/>
</symbol>
<symbol name="DS16F95AJA">
<pin name="VCC" direction="pwr"/>
<pin name="~RE" direction="in"/>
<pin name="DE" direction="in"/>
<pin name="DI" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="RO" direction="out"/>
<pin name="A"/>
<pin name="B"/>
</symbol>
<symbol name="DS22EV5110SQ">
<pin name="VDD_2" direction="pwr"/>
<pin name="VDD_3" direction="pwr"/>
<pin name="VDD_4" direction="pwr"/>
<pin name="VDD_5" direction="pwr"/>
<pin name="VDD_6" direction="pwr"/>
<pin name="VDD_7" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="VOD_CRL" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="LOCK" direction="in"/>
<pin name="SD" direction="in"/>
<pin name="C_IN-" direction="in"/>
<pin name="C_IN+" direction="in"/>
<pin name="D_IN0-" direction="in"/>
<pin name="D_IN0+" direction="in"/>
<pin name="D_IN1-" direction="in"/>
<pin name="DIN1+" direction="in"/>
<pin name="D_IN2-" direction="in"/>
<pin name="D_IN2+" direction="in"/>
<pin name="DE0" direction="in"/>
<pin name="DE1" direction="in"/>
<pin name="EQ0" direction="in"/>
<pin name="EQ1" direction="in"/>
<pin name="EQ2" direction="in"/>
<pin name="LFP" direction="in"/>
<pin name="LFN" direction="in"/>
<pin name="BYPASS" direction="in"/>
<pin name="RESRV_2" direction="nc"/>
<pin name="RESRV_3" direction="nc"/>
<pin name="RESRV_4" direction="nc"/>
<pin name="RESRV_5" direction="nc"/>
<pin name="RESRV_6" direction="nc"/>
<pin name="RESRV_7" direction="nc"/>
<pin name="RESRV" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="D_OUT2+" direction="out"/>
<pin name="D_OUT2-" direction="out"/>
<pin name="D_OUT1+" direction="out"/>
<pin name="D_OUT1-" direction="out"/>
<pin name="D_OUT0+" direction="out"/>
<pin name="D_OUT0-" direction="out"/>
<pin name="C_OUT+" direction="out"/>
<pin name="C_OUT-" direction="out"/>
</symbol>
<symbol name="DS25BR101TSD">
<pin name="VCC" direction="pwr"/>
<pin name="EQ" direction="in"/>
<pin name="PE" direction="in"/>
<pin name="IN+" direction="in"/>
<pin name="IN-" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="OUT+" direction="out"/>
<pin name="OUT-" direction="out"/>
</symbol>
<symbol name="DS25BR204TSQ">
<pin name="VDD_2" direction="pwr"/>
<pin name="VDD_3" direction="pwr"/>
<pin name="VDD_4" direction="pwr"/>
<pin name="VDD_5" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="~PWDN" direction="in"/>
<pin name="~PWDN0" direction="in"/>
<pin name="~PWDN1" direction="in"/>
<pin name="~PWDN2" direction="in"/>
<pin name="~PWDN3" direction="in"/>
<pin name="EQ1" direction="in"/>
<pin name="EQ2" direction="in"/>
<pin name="IN1-" direction="in"/>
<pin name="IN1+" direction="in"/>
<pin name="IN2-" direction="in"/>
<pin name="IN2+" direction="in"/>
<pin name="PE0" direction="in"/>
<pin name="PE1" direction="in"/>
<pin name="PE2" direction="in"/>
<pin name="PE3" direction="in"/>
<pin name="SEL_IN" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC_6" direction="nc"/>
<pin name="NC_7" direction="nc"/>
<pin name="NC_8" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="~LOS1" direction="out"/>
<pin name="~LOS2" direction="out"/>
<pin name="OUT0-" direction="out"/>
<pin name="OUT0+" direction="out"/>
<pin name="OUT1-" direction="out"/>
<pin name="OUT1+" direction="out"/>
<pin name="OUT2-" direction="out"/>
<pin name="OUT2+" direction="out"/>
<pin name="OUT3-" direction="out"/>
<pin name="OUT3+" direction="out"/>
</symbol>
<symbol name="DS25BR400TSQ">
<pin name="VCC_2" direction="pwr"/>
<pin name="VCC_3" direction="pwr"/>
<pin name="VCC_4" direction="pwr"/>
<pin name="VCC_5" direction="pwr"/>
<pin name="VCC_6" direction="pwr"/>
<pin name="VCC_7" direction="pwr"/>
<pin name="VCC_8" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="~EQA" direction="in"/>
<pin name="~EQB" direction="in"/>
<pin name="RSV" direction="pas"/>
<pin name="PREA_1" direction="in"/>
<pin name="PREA_0" direction="in"/>
<pin name="PREB_0" direction="in"/>
<pin name="PREB_1" direction="in"/>
<pin name="IA_0-" direction="in"/>
<pin name="IA_0+" direction="in"/>
<pin name="IA_1+" direction="in"/>
<pin name="IA_1-" direction="in"/>
<pin name="IA_2-" direction="in"/>
<pin name="IA_2+" direction="in"/>
<pin name="IA_3+" direction="in"/>
<pin name="IA_3-" direction="in"/>
<pin name="IB_0+" direction="in"/>
<pin name="IB_0-" direction="in"/>
<pin name="IB_1-" direction="in"/>
<pin name="IB_1+" direction="in"/>
<pin name="IB_2+" direction="in"/>
<pin name="IB_2-" direction="in"/>
<pin name="IB_3-" direction="in"/>
<pin name="IB_3+" direction="in"/>
<pin name="~LB0" direction="in"/>
<pin name="~LB1" direction="in"/>
<pin name="~LB2" direction="in"/>
<pin name="~LB3" direction="in"/>
<pin name="EP" direction="pas"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="OB_1+" direction="out"/>
<pin name="OB_1-" direction="out"/>
<pin name="OB_2-" direction="out"/>
<pin name="OB_2+" direction="out"/>
<pin name="OB_3+" direction="out"/>
<pin name="OB_3-" direction="out"/>
<pin name="OA_3-" direction="out"/>
<pin name="OA_3+" direction="out"/>
<pin name="OA_2+" direction="out"/>
<pin name="OA_2-" direction="out"/>
<pin name="OA_1-" direction="out"/>
<pin name="OA_1+" direction="out"/>
<pin name="OA_0+" direction="out"/>
<pin name="OA_0-" direction="out"/>
<pin name="OB_0-" direction="out"/>
<pin name="OB_0+" direction="out"/>
</symbol>
<symbol name="DS25BR440TSQ">
<pin name="VDD_2" direction="pwr"/>
<pin name="VDD_3" direction="pwr"/>
<pin name="VDD_4" direction="pwr"/>
<pin name="VDD_5" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="IN0+" direction="in"/>
<pin name="IN0-" direction="in"/>
<pin name="IN1+" direction="in"/>
<pin name="IN1-" direction="in"/>
<pin name="IN2+" direction="in"/>
<pin name="IN2-" direction="in"/>
<pin name="IN3+" direction="in"/>
<pin name="IN3-" direction="in"/>
<pin name="EQ0" direction="in"/>
<pin name="EQ1" direction="in"/>
<pin name="EQ2" direction="in"/>
<pin name="EQ3" direction="in"/>
<pin name="PE0" direction="in"/>
<pin name="PE1" direction="in"/>
<pin name="PE2" direction="in"/>
<pin name="PE3" direction="in"/>
<pin name="~PWDN0" direction="in"/>
<pin name="~PWDN1" direction="in"/>
<pin name="~PWDN2" direction="in"/>
<pin name="~PWDN3" direction="in"/>
<pin name="~PWDN" direction="in"/>
<pin name="NC" direction="pas"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="OUT0+" direction="out"/>
<pin name="OUT0-" direction="out"/>
<pin name="OUT1+" direction="out"/>
<pin name="OUT1-" direction="out"/>
<pin name="OUT2+" direction="out"/>
<pin name="OUT2-" direction="out"/>
<pin name="OUT3+" direction="out"/>
<pin name="OUT3-" direction="out"/>
<pin name="~LOS0" direction="out"/>
<pin name="~LOS1" direction="out"/>
<pin name="~LOS2" direction="out"/>
<pin name="~LOS3" direction="out"/>
</symbol>
<symbol name="DS25CP102QSQ">
<pin name="VDD" direction="pwr"/>
<pin name="PE" direction="in"/>
<pin name="EN0" direction="in"/>
<pin name="EN1" direction="in"/>
<pin name="EQ" direction="in"/>
<pin name="SEL0" direction="in"/>
<pin name="SEL1" direction="in"/>
<pin name="IN0+" direction="in"/>
<pin name="IN0-" direction="in"/>
<pin name="IN1+" direction="in"/>
<pin name="IN1-" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="OUT0+" direction="out"/>
<pin name="OUT0-" direction="out"/>
<pin name="OUT1+" direction="out"/>
<pin name="OUT1-" direction="out"/>
</symbol>
<symbol name="DS25CP102TSQ">
<pin name="VDD" direction="pwr"/>
<pin name="PE" direction="in"/>
<pin name="EN0" direction="in"/>
<pin name="EN1" direction="in"/>
<pin name="EQ" direction="in"/>
<pin name="SEL0" direction="in"/>
<pin name="SEL1" direction="in"/>
<pin name="IN0+" direction="in"/>
<pin name="IN0-" direction="in"/>
<pin name="IN1+" direction="in"/>
<pin name="IN1-" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="OUT0+" direction="out"/>
<pin name="OUT0-" direction="out"/>
<pin name="OUT1+" direction="out"/>
<pin name="OUT1-" direction="out"/>
</symbol>
<symbol name="DS25CP104ATSQ">
<pin name="VDD_2" direction="pwr"/>
<pin name="VDD_3" direction="pwr"/>
<pin name="VDD_4" direction="pwr"/>
<pin name="VDD_5" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="EN_SMB" direction="in"/>
<pin name="S00/SCL" direction="in"/>
<pin name="S01/SDA" direction="in"/>
<pin name="EQ0" direction="in"/>
<pin name="EQ1" direction="in"/>
<pin name="EQ2" direction="in"/>
<pin name="EQ3" direction="in"/>
<pin name="PE0" direction="in"/>
<pin name="PE1" direction="in"/>
<pin name="PE2" direction="in"/>
<pin name="PE3" direction="in"/>
<pin name="S30" direction="in"/>
<pin name="S31" direction="in"/>
<pin name="S10/ADDR0" direction="in"/>
<pin name="S11/ADDR1" direction="in"/>
<pin name="S20/ADDR2" direction="in"/>
<pin name="S21/ADDR3" direction="in"/>
<pin name="IN0+" direction="in"/>
<pin name="IN0-" direction="in"/>
<pin name="IN1+" direction="in"/>
<pin name="IN1-" direction="in"/>
<pin name="IN2+" direction="in"/>
<pin name="IN2-" direction="in"/>
<pin name="IN3+" direction="in"/>
<pin name="IN3-" direction="in"/>
<pin name="~PWDN" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="OUT0+" direction="out"/>
<pin name="OUT0-" direction="out"/>
<pin name="OUT1+" direction="out"/>
<pin name="OUT1-" direction="out"/>
<pin name="OUT2+" direction="out"/>
<pin name="OUT2-" direction="out"/>
<pin name="OUT3+" direction="out"/>
<pin name="OUT3-" direction="out"/>
</symbol>
<symbol name="DS25CP152QSQ">
<pin name="VCC" direction="pwr"/>
<pin name="EN0" direction="in"/>
<pin name="EN1" direction="in"/>
<pin name="SEL0" direction="in"/>
<pin name="SEL1" direction="in"/>
<pin name="IN0+" direction="in"/>
<pin name="IN0-" direction="in"/>
<pin name="IN1+" direction="in"/>
<pin name="IN1-" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="OUT0+" direction="out"/>
<pin name="OUT0-" direction="out"/>
<pin name="OUT1+" direction="out"/>
<pin name="OUT1-" direction="out"/>
</symbol>
<symbol name="DS25CP152TSQ">
<pin name="VCC" direction="pwr"/>
<pin name="EN0" direction="in"/>
<pin name="EN1" direction="in"/>
<pin name="SEL0" direction="in"/>
<pin name="SEL1" direction="in"/>
<pin name="IN0+" direction="in"/>
<pin name="IN0-" direction="in"/>
<pin name="IN1+" direction="in"/>
<pin name="IN1-" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="OUT0+" direction="out"/>
<pin name="OUT0-" direction="out"/>
<pin name="OUT1+" direction="out"/>
<pin name="OUT1-" direction="out"/>
</symbol>
<symbol name="DS25MB200TSQ">
<pin name="VCC_2" direction="pwr"/>
<pin name="VCC_3" direction="pwr"/>
<pin name="VCC_4" direction="pwr"/>
<pin name="VCC_5" direction="pwr"/>
<pin name="VCC_6" direction="pwr"/>
<pin name="VCC_7" direction="pwr"/>
<pin name="VCC_8" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="LI_0+" direction="in"/>
<pin name="LI_0-" direction="in"/>
<pin name="PREL1" direction="in"/>
<pin name="PREL0" direction="in"/>
<pin name="MUX_S1" direction="in"/>
<pin name="MUX_S0" direction="in"/>
<pin name="SIA_1-" direction="in"/>
<pin name="SIA_1+" direction="in"/>
<pin name="SIB_1-" direction="in"/>
<pin name="SIB_1+" direction="in"/>
<pin name="LIB1A" direction="in"/>
<pin name="LIB1B" direction="in"/>
<pin name="PRES1" direction="in"/>
<pin name="PRES0" direction="in"/>
<pin name="LI_1+" direction="in"/>
<pin name="LI_1-" direction="in"/>
<pin name="RSV" direction="in"/>
<pin name="SIA_0-" direction="in"/>
<pin name="SIA_0+" direction="in"/>
<pin name="SIB_0-" direction="in"/>
<pin name="SIB_0+" direction="in"/>
<pin name="EP" direction="pas"/>
<pin name="GND_2" direction="pwr"/>
<pin name="GND_3" direction="pwr"/>
<pin name="GND_4" direction="pwr"/>
<pin name="GND_5" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="SOA_0-" direction="out"/>
<pin name="SOA_0+" direction="out"/>
<pin name="SOA_1-" direction="out"/>
<pin name="SOA_1+" direction="out"/>
<pin name="SOB_0-" direction="out"/>
<pin name="SOB_0+" direction="out"/>
<pin name="SOB_1-" direction="out"/>
<pin name="SOB_1+" direction="out"/>
<pin name="LO_0+" direction="out"/>
<pin name="LO_0-" direction="out"/>
<pin name="LO_1+" direction="out"/>
<pin name="LO_1-" direction="out"/>
<pin name="LB0A" direction="pas"/>
<pin name="LB0B" direction="pas"/>
</symbol>
<symbol name="DS26C31TM">
<pin name="5V" direction="pwr"/>
<pin name="EN" direction="in"/>
<pin name="~EN" direction="in"/>
<pin name="IN_A" direction="in"/>
<pin name="IN_B" direction="in"/>
<pin name="IN_C" direction="in"/>
<pin name="IN_D" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUTA+" direction="out"/>
<pin name="OUTA-" direction="out"/>
<pin name="OUTB-" direction="out"/>
<pin name="OUTB+" direction="out"/>
<pin name="OUTC+" direction="out"/>
<pin name="OUTC-" direction="out"/>
<pin name="OUTD-" direction="out"/>
<pin name="OUTD+" direction="out"/>
</symbol>
<symbol name="DS26C31TN">
<pin name="5V" direction="pwr"/>
<pin name="EN" direction="in"/>
<pin name="~EN" direction="in"/>
<pin name="IN_A" direction="in"/>
<pin name="IN_B" direction="in"/>
<pin name="IN_C" direction="in"/>
<pin name="IN_D" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="CHANNEL_A_OUT_2" direction="out"/>
<pin name="CHANNEL_A_OUT" direction="out"/>
<pin name="CHANNEL_B_OUT_2" direction="out"/>
<pin name="CHANNEL_B_OUT" direction="out"/>
<pin name="CHANNEL_C_OUT_2" direction="out"/>
<pin name="CHANNEL_C_OUT" direction="out"/>
<pin name="CHANNEL_D_OUT_2" direction="out"/>
<pin name="CHANNEL_D_OUT" direction="out"/>
</symbol>
<symbol name="DS26C32ATM">
<pin name="VCC" direction="pwr"/>
<pin name="~EN" direction="in"/>
<pin name="EN_A" direction="in"/>
<pin name="-IN_A" direction="in"/>
<pin name="+IN_A" direction="in"/>
<pin name="+IN_B" direction="in"/>
<pin name="-IN_B" direction="in"/>
<pin name="+IN_C" direction="in"/>
<pin name="-IN_C" direction="in"/>
<pin name="-IN_D" direction="in"/>
<pin name="+IN_D" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT_A" direction="out"/>
<pin name="OUT_C" direction="out"/>
<pin name="OUT_D" direction="out"/>
<pin name="OUT_B" direction="out"/>
</symbol>
<symbol name="DS26LS31CM">
<pin name="5V" direction="pwr"/>
<pin name="EN" direction="in"/>
<pin name="~EN" direction="in"/>
<pin name="IN_A" direction="in"/>
<pin name="IN_B" direction="in"/>
<pin name="IN_C" direction="in"/>
<pin name="IN_D" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT_A2" direction="out"/>
<pin name="OUT_A1" direction="out"/>
<pin name="OUT_B1" direction="out"/>
<pin name="OUT_B2" direction="out"/>
<pin name="OUT_C2" direction="out"/>
<pin name="OUT_C1" direction="out"/>
<pin name="OUT_D1" direction="out"/>
<pin name="OUT_D2" direction="out"/>
</symbol>
<symbol name="DS26LS31CN">
<pin name="5V" direction="pwr"/>
<pin name="EN" direction="in"/>
<pin name="~EN" direction="in"/>
<pin name="IN_A" direction="in"/>
<pin name="IN_B" direction="in"/>
<pin name="IN_C" direction="in"/>
<pin name="IN_D" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="CHANNEL_A_OUT_2" direction="out"/>
<pin name="CHANNEL_A_OUT" direction="out"/>
<pin name="CHANNEL_B_OUT_2" direction="out"/>
<pin name="CHANNEL_B_OUT" direction="out"/>
<pin name="CHANNEL_C_OUT_2" direction="out"/>
<pin name="CHANNEL_C_OUT" direction="out"/>
<pin name="CHANNEL_D_OUT_2" direction="out"/>
<pin name="CHANNEL_D_OUT" direction="out"/>
</symbol>
<symbol name="DS26LS32ACM">
<pin name="VCC" direction="pwr"/>
<pin name="~EN" direction="in"/>
<pin name="EN_A" direction="in"/>
<pin name="-IN_A" direction="in"/>
<pin name="+IN_A" direction="in"/>
<pin name="+IN_B" direction="in"/>
<pin name="-IN_B" direction="in"/>
<pin name="+IN_C" direction="in"/>
<pin name="-IN_C" direction="in"/>
<pin name="-IN_D" direction="in"/>
<pin name="+IN_D" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT_A" direction="out"/>
<pin name="OUT_C" direction="out"/>
<pin name="OUT_D" direction="out"/>
<pin name="OUT_B" direction="out"/>
</symbol>
<symbol name="DS26LS32ACN">
<pin name="VCC" direction="pwr"/>
<pin name="EN_A" direction="in"/>
<pin name="~EN" direction="in"/>
<pin name="-IN_A" direction="in"/>
<pin name="+IN_A" direction="in"/>
<pin name="+IN_B" direction="in"/>
<pin name="-IN_B" direction="in"/>
<pin name="+IN_C" direction="in"/>
<pin name="-IN_C" direction="in"/>
<pin name="-IN_D" direction="in"/>
<pin name="+IN_D" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT_A" direction="out"/>
<pin name="OUT_C" direction="out"/>
<pin name="OUT_D" direction="out"/>
<pin name="OUT_B" direction="out"/>
</symbol>
<symbol name="DS26LS32CM">
<pin name="VCC" direction="pwr"/>
<pin name="~EN" direction="in"/>
<pin name="EN_A" direction="in"/>
<pin name="-IN_A" direction="in"/>
<pin name="+IN_A" direction="in"/>
<pin name="+IN_B" direction="in"/>
<pin name="-IN_B" direction="in"/>
<pin name="+IN_C" direction="in"/>
<pin name="-IN_C" direction="in"/>
<pin name="-IN_D" direction="in"/>
<pin name="+IN_D" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT_A" direction="out"/>
<pin name="OUT_C" direction="out"/>
<pin name="OUT_D" direction="out"/>
<pin name="OUT_B" direction="out"/>
</symbol>
<symbol name="DS26LS32CN">
<pin name="VCC" direction="pwr"/>
<pin name="EN_A" direction="in"/>
<pin name="~EN" direction="in"/>
<pin name="-IN_A" direction="in"/>
<pin name="+IN_A" direction="in"/>
<pin name="+IN_B" direction="in"/>
<pin name="-IN_B" direction="in"/>
<pin name="+IN_C" direction="in"/>
<pin name="-IN_C" direction="in"/>
<pin name="-IN_D" direction="in"/>
<pin name="+IN_D" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT_A" direction="out"/>
<pin name="OUT_C" direction="out"/>
<pin name="OUT_D" direction="out"/>
<pin name="OUT_B" direction="out"/>
</symbol>
<symbol name="DS32ELX0124SQ">
<pin name="VDD25_2" direction="pwr"/>
<pin name="VDD25_3" direction="pwr"/>
<pin name="VDD33_2" direction="pwr"/>
<pin name="VDD25" direction="pwr"/>
<pin name="VDD33_3" direction="pwr"/>
<pin name="VDD33_4" direction="pwr"/>
<pin name="VDD33" direction="pwr"/>
<pin name="VDDPLL" direction="pwr"/>
<pin name="RXIN0-" direction="in"/>
<pin name="RXIN0+" direction="in"/>
<pin name="RXIN1-" direction="in"/>
<pin name="RXIN1+" direction="in"/>
<pin name="~DC_B" direction="in"/>
<pin name="~RS" direction="in"/>
<pin name="~RESET" direction="in"/>
<pin name="~LOCK" direction="pas"/>
<pin name="LF_CP" direction="pas"/>
<pin name="LF_REF" direction="pas"/>
<pin name="SCK" direction="in"/>
<pin name="SDA"/>
<pin name="SMB_CS" direction="in"/>
<pin name="GPIO0"/>
<pin name="GPIO1"/>
<pin name="GPIO2"/>
<pin name="LT_EN" direction="in"/>
<pin name="RX_MUX_SEL" direction="in"/>
<pin name="VOD_CTRL" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC_6" direction="nc"/>
<pin name="NC_7" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="RXCLKOUT-" direction="out"/>
<pin name="RXCLKOUT+" direction="out"/>
<pin name="RXOUT0-" direction="out"/>
<pin name="RXOUT0+" direction="out"/>
<pin name="RXOUT1-" direction="out"/>
<pin name="RXOUT1+" direction="out"/>
<pin name="RXOUT2-" direction="out"/>
<pin name="RXOUT2+" direction="out"/>
<pin name="RXOUT3-" direction="out"/>
<pin name="RXOUT3+" direction="out"/>
<pin name="RXOUT4-" direction="out"/>
<pin name="RXOUT4+" direction="out"/>
<pin name="TXOUT-" direction="out"/>
<pin name="TXOUT+" direction="out"/>
</symbol>
<symbol name="DS32ELX0421SQ">
<pin name="VDD33_2" direction="pwr"/>
<pin name="VDD33" direction="pwr"/>
<pin name="VDD25_2" direction="pwr"/>
<pin name="VDD25_3" direction="pwr"/>
<pin name="VDD25_4" direction="pwr"/>
<pin name="VDD25_5" direction="pwr"/>
<pin name="VDD25" direction="pwr"/>
<pin name="VDDPLL" direction="pwr"/>
<pin name="TXCLKIN-" direction="in"/>
<pin name="TXCLKIN+" direction="in"/>
<pin name="SCK" direction="in"/>
<pin name="TXOUT1_EN" direction="in"/>
<pin name="VOD_CTRL" direction="in"/>
<pin name="TXIN0-" direction="in"/>
<pin name="TXIN0+" direction="in"/>
<pin name="TXIN1-" direction="in"/>
<pin name="TXIN1+" direction="in"/>
<pin name="TXIN2-" direction="in"/>
<pin name="TXIN2+" direction="in"/>
<pin name="TXIN3-" direction="in"/>
<pin name="TXIN3+" direction="in"/>
<pin name="TXIN4-" direction="in"/>
<pin name="TXIN4+" direction="in"/>
<pin name="LF_CP" direction="in"/>
<pin name="LF_REF" direction="in"/>
<pin name="~RS" direction="in"/>
<pin name="~DC_B" direction="in"/>
<pin name="~RESET" direction="in"/>
<pin name="SDA"/>
<pin name="SMB_CS" direction="in"/>
<pin name="DE-EMP0" direction="in"/>
<pin name="DE-EMP1" direction="in"/>
<pin name="RSVD" direction="in"/>
<pin name="GPIO0"/>
<pin name="GPIO1"/>
<pin name="GPIO2"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC_6" direction="nc"/>
<pin name="NC_7" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="TXOUT0-_2" direction="out"/>
<pin name="TXOUT0+" direction="out"/>
<pin name="TXOUT0-" direction="out"/>
<pin name="TXOUT1+" direction="out"/>
<pin name="~LOCK" direction="out"/>
</symbol>
<symbol name="DS32EV100SD">
<pin name="VDD" direction="pwr"/>
<pin name="IN+" direction="in"/>
<pin name="IN-" direction="in"/>
<pin name="BST_0" direction="in"/>
<pin name="BST_1" direction="in"/>
<pin name="BST_2" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pwr"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="OUT+" direction="out"/>
<pin name="OUT-" direction="out"/>
</symbol>
<symbol name="DS32EV400SQ">
<pin name="VDD_2" direction="pwr"/>
<pin name="VDD_3" direction="pwr"/>
<pin name="VDD_4" direction="pwr"/>
<pin name="VDD_5" direction="pwr"/>
<pin name="VDD_6" direction="pwr"/>
<pin name="VDD_7" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="EN0" direction="in"/>
<pin name="EN1" direction="in"/>
<pin name="EN2" direction="in"/>
<pin name="EN3" direction="in"/>
<pin name="IN_0+" direction="in"/>
<pin name="IN_0-" direction="in"/>
<pin name="IN_1+" direction="in"/>
<pin name="IN_1-" direction="in"/>
<pin name="IN_2+" direction="in"/>
<pin name="IN_2-" direction="in"/>
<pin name="IN_3+" direction="in"/>
<pin name="IN_3-" direction="in"/>
<pin name="SDC"/>
<pin name="FEB" direction="in"/>
<pin name="CS" direction="in"/>
<pin name="SDA"/>
<pin name="BST_0" direction="in"/>
<pin name="BST_1" direction="in"/>
<pin name="BST_2" direction="in"/>
<pin name="RESERVE_2" direction="nc"/>
<pin name="RESERVE_3" direction="nc"/>
<pin name="RESERVE_4" direction="nc"/>
<pin name="RESERVE" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="OUT_0+" direction="out"/>
<pin name="OUT_0-" direction="out"/>
<pin name="OUT_1+" direction="out"/>
<pin name="OUT_1-" direction="out"/>
<pin name="OUT_2+" direction="out"/>
<pin name="OUT_2-" direction="out"/>
<pin name="OUT_3+" direction="out"/>
<pin name="OUT_3-" direction="out"/>
<pin name="SD0" direction="out"/>
<pin name="SD1" direction="out"/>
<pin name="SD2" direction="out"/>
<pin name="SD3" direction="out"/>
</symbol>
<symbol name="DS3486M">
<pin name="VCC" direction="pwr"/>
<pin name="TRI_STATE_CONTROL_A/C" direction="pas"/>
<pin name="TRI_STATE_CONTROL_B/D" direction="pas"/>
<pin name="IN_A" direction="in"/>
<pin name="IN_A_2" direction="in"/>
<pin name="IN_B" direction="in"/>
<pin name="IN_B_2" direction="in"/>
<pin name="IN_C" direction="in"/>
<pin name="IN_C_2" direction="in"/>
<pin name="IN_D" direction="in"/>
<pin name="IN_D_2" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT_A" direction="out"/>
<pin name="OUT_B" direction="out"/>
<pin name="OUT_C" direction="out"/>
<pin name="OUT_D" direction="out"/>
</symbol>
<symbol name="DS34C86TM">
<pin name="VCC" direction="pwr"/>
<pin name="EN_A/C" direction="in"/>
<pin name="EN_B/D" direction="in"/>
<pin name="-IN_A" direction="in"/>
<pin name="+IN_A" direction="in"/>
<pin name="+IN_B" direction="in"/>
<pin name="-IN_B" direction="in"/>
<pin name="+IN_C" direction="in"/>
<pin name="-IN_C" direction="in"/>
<pin name="-IN_D" direction="in"/>
<pin name="+IN_D" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT_A" direction="out"/>
<pin name="OUT_B" direction="out"/>
<pin name="OUT_C" direction="out"/>
<pin name="OUT_D" direction="out"/>
</symbol>
<symbol name="DS34C87TM">
<pin name="VCC" direction="pwr"/>
<pin name="A/B_CTRL" direction="in"/>
<pin name="C/D_CTRL" direction="in"/>
<pin name="INA" direction="in"/>
<pin name="INB" direction="in"/>
<pin name="INC" direction="in"/>
<pin name="IND" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUTA" direction="out"/>
<pin name="~OUTA" direction="out"/>
<pin name="~OUTB" direction="out"/>
<pin name="OUTB" direction="out"/>
<pin name="OUTC" direction="out"/>
<pin name="~OUTC" direction="out"/>
<pin name="~OUTD" direction="out"/>
<pin name="OUTD" direction="out"/>
</symbol>
<symbol name="DS34LV86TM">
<pin name="VCC" direction="pwr"/>
<pin name="EN_2" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="RI1-" direction="in"/>
<pin name="RI1+" direction="in"/>
<pin name="RI2+" direction="in"/>
<pin name="RI2-" direction="in"/>
<pin name="RI3-" direction="in"/>
<pin name="RI3+" direction="in"/>
<pin name="RI4+" direction="in"/>
<pin name="RI4-" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="RO1" direction="out"/>
<pin name="RO2" direction="out"/>
<pin name="RO3" direction="out"/>
<pin name="RO4" direction="out"/>
</symbol>
<symbol name="DS34LV87TM">
<pin name="VCC" direction="pwr"/>
<pin name="EN_2" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="DI1" direction="in"/>
<pin name="DI2" direction="in"/>
<pin name="DI3" direction="in"/>
<pin name="DI4" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="DO1+" direction="out"/>
<pin name="DO1-" direction="out"/>
<pin name="DO2-" direction="out"/>
<pin name="DO2+" direction="out"/>
<pin name="DO3+" direction="out"/>
<pin name="DO3-" direction="out"/>
<pin name="DO4-" direction="out"/>
<pin name="DO4+" direction="out"/>
</symbol>
<symbol name="DS36276M">
<pin name="VCC" direction="pwr"/>
<pin name="~RE" direction="in"/>
<pin name="DE" direction="in"/>
<pin name="DI" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="DO/RI"/>
<pin name="~DO/~RI"/>
<pin name="RO" direction="out"/>
</symbol>
<symbol name="DS36277TM">
<pin name="VCC" direction="pwr"/>
<pin name="~RE" direction="in"/>
<pin name="~DE" direction="in"/>
<pin name="DI" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="DO/RI"/>
<pin name="~DO/~RI"/>
<pin name="RO" direction="out"/>
</symbol>
<symbol name="DS3691M">
<pin name="VCC" direction="pwr"/>
<pin name="MODE_SEL" direction="in"/>
<pin name="IN_A" direction="in"/>
<pin name="IN_B/DISABLE" direction="in"/>
<pin name="IN_C/DISABLE" direction="in"/>
<pin name="IN_D" direction="in"/>
<pin name="RISE_TIME_CTRL_A" direction="in"/>
<pin name="RISE_TIME_CTRL_B" direction="in"/>
<pin name="RISE_TIME_CTRL_C" direction="in"/>
<pin name="RISE_TIME_CTRL_D" direction="in"/>
<pin name="VEE" direction="pwr"/>
<pin name="GND" direction="pas"/>
<pin name="OUT_D" direction="out"/>
<pin name="OUT_C" direction="out"/>
<pin name="OUT_B" direction="out"/>
<pin name="OUT_A" direction="out"/>
</symbol>
<symbol name="DS36950V">
<pin name="VCC" direction="pwr"/>
<pin name="~REC" direction="in"/>
<pin name="~RE4" direction="in"/>
<pin name="DE1" direction="in"/>
<pin name="DE2" direction="in"/>
<pin name="DE3" direction="in"/>
<pin name="DE4" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="DR1"/>
<pin name="DR2"/>
<pin name="DR3"/>
<pin name="DR4"/>
<pin name="OA1"/>
<pin name="OA2"/>
<pin name="OA3"/>
<pin name="OA4"/>
<pin name="OB1"/>
<pin name="OB2"/>
<pin name="OB3"/>
<pin name="OB4"/>
</symbol>
<symbol name="DS3695AM">
<pin name="VCC" direction="pwr"/>
<pin name="~RE" direction="in"/>
<pin name="DE" direction="in"/>
<pin name="DI" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="DO/RI"/>
<pin name="~DO/~RI"/>
<pin name="RO" direction="out"/>
</symbol>
<symbol name="DS3695ATM">
<pin name="VCC" direction="pwr"/>
<pin name="~RE" direction="in"/>
<pin name="DE" direction="in"/>
<pin name="DI" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="DO/RI"/>
<pin name="~DO/~RI"/>
<pin name="RO" direction="out"/>
</symbol>
<symbol name="DS3695N">
<pin name="VCC" direction="pwr"/>
<pin name="~RE" direction="in"/>
<pin name="DE" direction="in"/>
<pin name="DI" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="RO" direction="out"/>
<pin name="DO/RI"/>
<pin name="~DO/~RI"/>
</symbol>
<symbol name="DS3695TN">
<pin name="VCC" direction="pwr"/>
<pin name="~RE" direction="in"/>
<pin name="DE" direction="in"/>
<pin name="DI" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="DO/RI"/>
<pin name="~DO/~RI"/>
<pin name="RO" direction="out"/>
</symbol>
<symbol name="DS36C200M">
<pin name="VCC" direction="pwr"/>
<pin name="DE" direction="in"/>
<pin name="~RE" direction="in"/>
<pin name="DI/R01"/>
<pin name="DI/R02"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="DO/RI2+"/>
<pin name="DO/RI2-"/>
<pin name="DO/RI1-"/>
<pin name="DO/RI1+"/>
</symbol>
<symbol name="DS36C278M">
<pin name="VCC" direction="pwr"/>
<pin name="~RE" direction="in"/>
<pin name="DE" direction="in"/>
<pin name="DI" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="DO/RI"/>
<pin name="~DO/~RI"/>
<pin name="RO" direction="out"/>
</symbol>
<symbol name="DS36C278TM">
<pin name="VCC" direction="pwr"/>
<pin name="~RE" direction="in"/>
<pin name="DE" direction="in"/>
<pin name="DI" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="DO/RI"/>
<pin name="~DO/~RI"/>
<pin name="RO" direction="out"/>
</symbol>
<symbol name="DS36C279M">
<pin name="VCC" direction="pwr"/>
<pin name="~RE" direction="in"/>
<pin name="DE" direction="in"/>
<pin name="DI" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="DO/RI"/>
<pin name="~DO/~RI"/>
<pin name="RO" direction="out"/>
</symbol>
<symbol name="DS36C280TM">
<pin name="VCC" direction="pwr"/>
<pin name="SR" direction="in"/>
<pin name="DE/~RE" direction="in"/>
<pin name="DI" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="DO/RI"/>
<pin name="~DO/~RI"/>
<pin name="RO" direction="out"/>
</symbol>
<symbol name="DS38EP100SD">
<pin name="IOA+"/>
<pin name="IOA-"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="EP" direction="nc"/>
<pin name="IOB+"/>
<pin name="IOB-"/>
</symbol>
<symbol name="DS42BR400TSQ">
<pin name="VCC_2" direction="pwr"/>
<pin name="VCC_3" direction="pwr"/>
<pin name="VCC_4" direction="pwr"/>
<pin name="VCC_5" direction="pwr"/>
<pin name="VCC_6" direction="pwr"/>
<pin name="VCC_7" direction="pwr"/>
<pin name="VCC_8" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="~EQA" direction="in"/>
<pin name="~EQB" direction="in"/>
<pin name="RSV" direction="in"/>
<pin name="IA_1+" direction="in"/>
<pin name="IA_1-" direction="in"/>
<pin name="IA_2-" direction="in"/>
<pin name="IA_2+" direction="in"/>
<pin name="IA_3+" direction="in"/>
<pin name="IA_3-" direction="in"/>
<pin name="IB_3-" direction="in"/>
<pin name="IB_3+" direction="in"/>
<pin name="IB_1-" direction="in"/>
<pin name="IB_1+" direction="in"/>
<pin name="IB_2+" direction="in"/>
<pin name="IB_2-" direction="in"/>
<pin name="PREA_1" direction="in"/>
<pin name="PREA_0" direction="in"/>
<pin name="PREB_0" direction="in"/>
<pin name="PREB_1" direction="in"/>
<pin name="~LB0" direction="in"/>
<pin name="~LB1" direction="in"/>
<pin name="~LB2" direction="in"/>
<pin name="~LB3" direction="in"/>
<pin name="IB_0+" direction="in"/>
<pin name="IB_0-" direction="in"/>
<pin name="IA_0-" direction="in"/>
<pin name="IA_0+" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="OA_0+" direction="out"/>
<pin name="OA_0-" direction="out"/>
<pin name="OA_1-" direction="out"/>
<pin name="OA_1+" direction="out"/>
<pin name="OA_2+" direction="out"/>
<pin name="OA_2-" direction="out"/>
<pin name="OA_3-" direction="out"/>
<pin name="OA_3+" direction="out"/>
<pin name="OB_0-" direction="out"/>
<pin name="OB_0+" direction="out"/>
<pin name="OB_1+" direction="out"/>
<pin name="OB_1-" direction="out"/>
<pin name="OB_2-" direction="out"/>
<pin name="OB_2+" direction="out"/>
<pin name="OB_3+" direction="out"/>
<pin name="OB_3-" direction="out"/>
</symbol>
<symbol name="DS481TM">
<pin name="VCC" direction="pwr"/>
<pin name="~RE" direction="in"/>
<pin name="DE" direction="in"/>
<pin name="DI" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="A" direction="out"/>
<pin name="B" direction="out"/>
<pin name="RO" direction="out"/>
</symbol>
<symbol name="DS485M">
<pin name="VCC" direction="pwr"/>
<pin name="~RE" direction="in"/>
<pin name="DE" direction="in"/>
<pin name="DI" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="A"/>
<pin name="B"/>
<pin name="RO" direction="out"/>
</symbol>
<symbol name="DS485N">
<pin name="VCC" direction="pwr"/>
<pin name="~RE" direction="in"/>
<pin name="DE" direction="in"/>
<pin name="DI" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="A"/>
<pin name="B"/>
<pin name="RO" direction="out"/>
</symbol>
<symbol name="DS50EV401SQ">
<pin name="VDD_2" direction="pwr"/>
<pin name="VDD_3" direction="pwr"/>
<pin name="VDD_4" direction="pwr"/>
<pin name="VDD_5" direction="pwr"/>
<pin name="VDD_6" direction="pwr"/>
<pin name="VDD_7" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="EN0" direction="in"/>
<pin name="EN1" direction="in"/>
<pin name="EN2" direction="in"/>
<pin name="EN3" direction="in"/>
<pin name="MODE" direction="in"/>
<pin name="IN_0+" direction="in"/>
<pin name="IN_0-" direction="in"/>
<pin name="IN_1+" direction="in"/>
<pin name="IN_1-" direction="in"/>
<pin name="IN_2+" direction="in"/>
<pin name="IN_2-" direction="in"/>
<pin name="IN_3+" direction="in"/>
<pin name="IN_3-" direction="in"/>
<pin name="RESERV_2" direction="nc"/>
<pin name="RESERV_3" direction="nc"/>
<pin name="RESERV_4" direction="nc"/>
<pin name="RESERV_5" direction="nc"/>
<pin name="RESERV_6" direction="nc"/>
<pin name="RESERV_7" direction="nc"/>
<pin name="RESERV_8" direction="nc"/>
<pin name="RESERV_9" direction="nc"/>
<pin name="RESERV_10" direction="nc"/>
<pin name="RESERV" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="OUT_0+" direction="out"/>
<pin name="OUT_0-" direction="out"/>
<pin name="OUT_1+" direction="out"/>
<pin name="OUT_1-" direction="out"/>
<pin name="OUT_2+" direction="out"/>
<pin name="OUT_2-" direction="out"/>
<pin name="OUT_3+" direction="out"/>
<pin name="OUT_3-" direction="out"/>
<pin name="SD0" direction="out"/>
<pin name="SD1" direction="out"/>
<pin name="SD2" direction="out"/>
<pin name="SD3" direction="out"/>
</symbol>
<symbol name="DS50PCI401SQ">
<pin name="VDD_2" direction="pwr"/>
<pin name="VDD_3" direction="pwr"/>
<pin name="VDD_4" direction="pwr"/>
<pin name="VDD_5" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="IA_0-" direction="in"/>
<pin name="IA_0+" direction="in"/>
<pin name="IA_1-" direction="in"/>
<pin name="IA_1+" direction="in"/>
<pin name="IA_2-" direction="in"/>
<pin name="IA_2+" direction="in"/>
<pin name="IA_3-" direction="in"/>
<pin name="IA_3+" direction="in"/>
<pin name="IB_0-" direction="in"/>
<pin name="IB_0+" direction="in"/>
<pin name="IB_1-" direction="in"/>
<pin name="IB_1+" direction="in"/>
<pin name="IB_2-" direction="in"/>
<pin name="IB_2+" direction="in"/>
<pin name="IB_3-" direction="in"/>
<pin name="IB_3+" direction="in"/>
<pin name="DEMA1/SCL" direction="in"/>
<pin name="~PRSNT" direction="in"/>
<pin name="DEMB0/AD1" direction="in"/>
<pin name="DEMB1/AD0" direction="in"/>
<pin name="ENRXDET" direction="in"/>
<pin name="ENSMB" direction="in"/>
<pin name="EQA0" direction="in"/>
<pin name="EQA1" direction="in"/>
<pin name="EQB0/AD3" direction="in"/>
<pin name="EQB1/AD2" direction="in"/>
<pin name="RATE" direction="in"/>
<pin name="RXDETA" direction="in"/>
<pin name="RXDETB" direction="in"/>
<pin name="SD_TH" direction="in"/>
<pin name="TXIDLEA" direction="in"/>
<pin name="TXIDLEB" direction="in"/>
<pin name="EP" direction="pas"/>
<pin name="DEMA0/SDA"/>
<pin name="OA_0-" direction="out"/>
<pin name="OA_0+" direction="out"/>
<pin name="OA_1-" direction="out"/>
<pin name="OA_1+" direction="out"/>
<pin name="OA_2-" direction="out"/>
<pin name="OA_2+" direction="out"/>
<pin name="OA_3-" direction="out"/>
<pin name="OA_3+" direction="out"/>
<pin name="OB_0-" direction="out"/>
<pin name="OB_0+" direction="out"/>
<pin name="OB_1-" direction="out"/>
<pin name="OB_1+" direction="out"/>
<pin name="OB_2-" direction="out"/>
<pin name="OB_2+" direction="out"/>
<pin name="OB_3-" direction="out"/>
<pin name="OB_3+" direction="out"/>
</symbol>
<symbol name="DS64BR401SQE">
<pin name="VDD_2" direction="pwr"/>
<pin name="VDD_3" direction="pwr"/>
<pin name="VDD_4" direction="pwr"/>
<pin name="VDD_5" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="VOD0" direction="pwr"/>
<pin name="VOD1" direction="pwr"/>
<pin name="IA_0+" direction="in"/>
<pin name="IA_0-" direction="in"/>
<pin name="IA_1+" direction="in"/>
<pin name="IA_1-" direction="in"/>
<pin name="IA_2+" direction="in"/>
<pin name="IA_2-" direction="in"/>
<pin name="IA_3+" direction="in"/>
<pin name="IA_3-" direction="in"/>
<pin name="IB_0-" direction="in"/>
<pin name="IB_0+" direction="in"/>
<pin name="IB_1-" direction="in"/>
<pin name="IB_1+" direction="in"/>
<pin name="IB_2-" direction="in"/>
<pin name="IB_2+" direction="in"/>
<pin name="IB_3-" direction="in"/>
<pin name="IB_3+" direction="in"/>
<pin name="EQA1" direction="in"/>
<pin name="EQA0" direction="in"/>
<pin name="RATE" direction="in"/>
<pin name="TXIDLEA" direction="in"/>
<pin name="TXIDLEB" direction="in"/>
<pin name="SD_TH" direction="in"/>
<pin name="ENSMB" direction="in"/>
<pin name="PWDN" direction="in"/>
<pin name="EQB0/AD3" direction="in"/>
<pin name="EQB1/AD2" direction="in"/>
<pin name="DEMA0/SDA" direction="in"/>
<pin name="DEMA1/SCL" direction="in"/>
<pin name="DEMB0/AD1" direction="in"/>
<pin name="DEMB1/AD0" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="EP" direction="pas"/>
<pin name="OB_0+" direction="out"/>
<pin name="OB_0-" direction="out"/>
<pin name="OB_1+" direction="out"/>
<pin name="OB_1-" direction="out"/>
<pin name="OB_2+" direction="out"/>
<pin name="OB_2-" direction="out"/>
<pin name="OB_3+" direction="out"/>
<pin name="OB_3-" direction="out"/>
<pin name="OA_3-" direction="out"/>
<pin name="OA_3+" direction="out"/>
<pin name="OA_2-" direction="out"/>
<pin name="OA_2+" direction="out"/>
<pin name="OA_1-" direction="out"/>
<pin name="OA_1+" direction="out"/>
<pin name="OA_0-" direction="out"/>
<pin name="OA_0+" direction="out"/>
</symbol>
<symbol name="DS64EV100SD">
<pin name="VDD" direction="pwr"/>
<pin name="IN+" direction="in"/>
<pin name="IN-" direction="in"/>
<pin name="BST_0" direction="in"/>
<pin name="BST_1" direction="in"/>
<pin name="BST_2" direction="in"/>
<pin name="NC" direction="pas"/>
<pin name="GND_2" direction="pwr"/>
<pin name="GND_3" direction="pwr"/>
<pin name="GND_4" direction="pwr"/>
<pin name="GND_5" direction="pwr"/>
<pin name="GND_6" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="OUT+" direction="out"/>
<pin name="OUT-" direction="out"/>
</symbol>
<symbol name="DS64EV400SQ">
<pin name="VDD_2" direction="pwr"/>
<pin name="VDD_3" direction="pwr"/>
<pin name="VDD_4" direction="pwr"/>
<pin name="VDD_5" direction="pwr"/>
<pin name="VDD_6" direction="pwr"/>
<pin name="VDD_7" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="EN0" direction="in"/>
<pin name="EN1" direction="in"/>
<pin name="EN2" direction="in"/>
<pin name="EN3" direction="in"/>
<pin name="BST_0" direction="in"/>
<pin name="BST_1" direction="in"/>
<pin name="BST_2" direction="in"/>
<pin name="CS" direction="in"/>
<pin name="SDC" direction="in"/>
<pin name="FEB" direction="in"/>
<pin name="SDA"/>
<pin name="IN_0+" direction="in"/>
<pin name="IN_0-" direction="in"/>
<pin name="IN_1+" direction="in"/>
<pin name="IN_1-" direction="in"/>
<pin name="IN_2-" direction="in"/>
<pin name="IN_2+" direction="in"/>
<pin name="IN_3+" direction="in"/>
<pin name="IN_3-" direction="in"/>
<pin name="RESERV_2" direction="nc"/>
<pin name="RESERV_3" direction="nc"/>
<pin name="RESERV_4" direction="nc"/>
<pin name="RESERV" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="SD0" direction="out"/>
<pin name="SD1" direction="out"/>
<pin name="SD2" direction="out"/>
<pin name="SD3" direction="out"/>
<pin name="OUT_0-" direction="out"/>
<pin name="OUT_0+" direction="out"/>
<pin name="OUT_1+" direction="out"/>
<pin name="OUT_1-" direction="out"/>
<pin name="OUT_2-" direction="out"/>
<pin name="OUT_2+" direction="out"/>
<pin name="OUT_3+" direction="out"/>
<pin name="OUT_3-" direction="out"/>
</symbol>
<symbol name="DS75176BM">
<pin name="VCC" direction="pwr"/>
<pin name="~RE" direction="in"/>
<pin name="DE" direction="in"/>
<pin name="DI" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="RO" direction="out"/>
<pin name="DO/RI"/>
<pin name="~DO/~RI"/>
</symbol>
<symbol name="DS75176BN">
<pin name="VCC" direction="pwr"/>
<pin name="~RE" direction="in"/>
<pin name="DE" direction="in"/>
<pin name="DI" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="DO/RI"/>
<pin name="~DO/~RI"/>
<pin name="RO" direction="out"/>
</symbol>
<symbol name="DS75176BTM">
<pin name="VCC" direction="pwr"/>
<pin name="~RE" direction="in"/>
<pin name="DE" direction="in"/>
<pin name="DI" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="RO" direction="out"/>
<pin name="DO/RI"/>
<pin name="~DO/~RI"/>
</symbol>
<symbol name="DS75176BTN">
<pin name="VCC" direction="pwr"/>
<pin name="~RE" direction="in"/>
<pin name="DE" direction="in"/>
<pin name="DI" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="DO/RI"/>
<pin name="~DO/~RI"/>
<pin name="RO" direction="out"/>
</symbol>
<symbol name="DS80EP100SD">
<pin name="IOA+"/>
<pin name="IOA-"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="EP" direction="nc"/>
<pin name="IOB+"/>
<pin name="IOB-"/>
</symbol>
<symbol name="DS8921M">
<pin name="VCC" direction="pwr"/>
<pin name="DI" direction="in"/>
<pin name="RI-" direction="in"/>
<pin name="RI+" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="DO-" direction="out"/>
<pin name="DO+" direction="out"/>
<pin name="RO" direction="out"/>
</symbol>
<symbol name="DS8921N">
<pin name="VCC" direction="pwr"/>
<pin name="DI" direction="in"/>
<pin name="RI+" direction="in"/>
<pin name="RI-" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="RO" direction="out"/>
<pin name="DO-" direction="out"/>
<pin name="DO+" direction="out"/>
</symbol>
<symbol name="DS8922AM">
<pin name="VCC" direction="pwr"/>
<pin name="~EN1" direction="in"/>
<pin name="~EN2" direction="in"/>
<pin name="DI1" direction="in"/>
<pin name="DI2" direction="in"/>
<pin name="RI2+" direction="in"/>
<pin name="RI2-" direction="in"/>
<pin name="RI1-" direction="in"/>
<pin name="RI1+" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="RO1" direction="out"/>
<pin name="RO2" direction="out"/>
<pin name="DO2+" direction="out"/>
<pin name="DO2-" direction="out"/>
<pin name="DO1-" direction="out"/>
<pin name="DO1+" direction="out"/>
</symbol>
<symbol name="DS8923AM">
<pin name="VCC" direction="pwr"/>
<pin name="~DEN" direction="in"/>
<pin name="~REN" direction="in"/>
<pin name="DI1" direction="in"/>
<pin name="DI2" direction="in"/>
<pin name="RI2+" direction="in"/>
<pin name="RI2-" direction="in"/>
<pin name="RI1-" direction="in"/>
<pin name="RI1+" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="RO1" direction="out"/>
<pin name="RO2" direction="out"/>
<pin name="DO2+" direction="out"/>
<pin name="DO2-" direction="out"/>
<pin name="DO1-" direction="out"/>
<pin name="DO1+" direction="out"/>
</symbol>
<symbol name="DS8923AN">
<pin name="VCC" direction="pwr"/>
<pin name="~DEN" direction="in"/>
<pin name="~REN" direction="in"/>
<pin name="DI1" direction="in"/>
<pin name="DI2" direction="in"/>
<pin name="RI2+" direction="in"/>
<pin name="RI2-" direction="in"/>
<pin name="RI1-" direction="in"/>
<pin name="RI1+" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="RO1" direction="out"/>
<pin name="RO2" direction="out"/>
<pin name="DO2+" direction="out"/>
<pin name="DO2-" direction="out"/>
<pin name="DO1-" direction="out"/>
<pin name="DO1+" direction="out"/>
</symbol>
<symbol name="DS89C387TMEA">
<pin name="VCC" direction="pwr"/>
<pin name="EN_A,C" direction="in"/>
<pin name="EN_B,D" direction="in"/>
<pin name="EN_I,K" direction="in"/>
<pin name="EN_E,G" direction="in"/>
<pin name="EN_F,H" direction="in"/>
<pin name="EN_J,L" direction="in"/>
<pin name="DI_A" direction="in"/>
<pin name="DI_B" direction="in"/>
<pin name="DI_C" direction="in"/>
<pin name="DI_D" direction="in"/>
<pin name="DI_E" direction="in"/>
<pin name="DI_G" direction="in"/>
<pin name="DI_H" direction="in"/>
<pin name="DI_J" direction="in"/>
<pin name="DI_I" direction="in"/>
<pin name="DI_K" direction="in"/>
<pin name="DI_L" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="DO_A" direction="out"/>
<pin name="DO*_A" direction="out"/>
<pin name="DO*_C" direction="out"/>
<pin name="DO_C" direction="out"/>
<pin name="DO_E" direction="out"/>
<pin name="DO*_E" direction="out"/>
<pin name="DO*_G" direction="out"/>
<pin name="DO_G" direction="out"/>
<pin name="DO_I" direction="out"/>
<pin name="DO*_I" direction="out"/>
<pin name="DO*_K" direction="out"/>
<pin name="DO_K" direction="out"/>
<pin name="DO_L" direction="out"/>
<pin name="DO*_L" direction="out"/>
<pin name="DO*_J" direction="out"/>
<pin name="DO_J" direction="out"/>
<pin name="DO_H" direction="out"/>
<pin name="DO*_H" direction="out"/>
<pin name="DO*_F" direction="out"/>
<pin name="DO_F" direction="out"/>
<pin name="DI_F" direction="in"/>
<pin name="DO_D" direction="out"/>
<pin name="DO*_D" direction="out"/>
<pin name="DO*_B" direction="out"/>
<pin name="DO_B" direction="out"/>
</symbol>
<symbol name="DS90C031BTM">
<pin name="VCC" direction="pwr"/>
<pin name="EN" direction="in"/>
<pin name="~EN" direction="in"/>
<pin name="DIN1" direction="in"/>
<pin name="DIN2" direction="in"/>
<pin name="DIN3" direction="in"/>
<pin name="DIN4" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="DOUT1+" direction="out"/>
<pin name="DOUT1-" direction="out"/>
<pin name="DOUT2-" direction="out"/>
<pin name="DOUT2+" direction="out"/>
<pin name="DOUT3+" direction="out"/>
<pin name="DOUT3-" direction="out"/>
<pin name="DOUT4-" direction="out"/>
<pin name="DOUT4+" direction="out"/>
</symbol>
<symbol name="DS90C031TM">
<pin name="VCC" direction="pwr"/>
<pin name="EN" direction="in"/>
<pin name="~EN" direction="in"/>
<pin name="DIN1" direction="in"/>
<pin name="DIN2" direction="in"/>
<pin name="DIN3" direction="in"/>
<pin name="DIN4" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="DOUT1+" direction="out"/>
<pin name="DOUT1-" direction="out"/>
<pin name="DOUT2-" direction="out"/>
<pin name="DOUT2+" direction="out"/>
<pin name="DOUT3+" direction="out"/>
<pin name="DOUT3-" direction="out"/>
<pin name="DOUT4-" direction="out"/>
<pin name="DOUT4+" direction="out"/>
</symbol>
<symbol name="DS90C032BTM">
<pin name="VCC" direction="pwr"/>
<pin name="EN" direction="in"/>
<pin name="~EN" direction="in"/>
<pin name="RIN1-" direction="in"/>
<pin name="RIN1+" direction="in"/>
<pin name="RIN2+" direction="in"/>
<pin name="RIN2-" direction="in"/>
<pin name="RIN3+" direction="in"/>
<pin name="RIN3-" direction="in"/>
<pin name="RIN4+" direction="in"/>
<pin name="RIN4-" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="ROUT1" direction="out"/>
<pin name="ROUT2" direction="out"/>
<pin name="ROUT3" direction="out"/>
<pin name="ROUT4" direction="out"/>
</symbol>
<symbol name="DS90C032TM">
<pin name="VCC" direction="pwr"/>
<pin name="EN" direction="in"/>
<pin name="~EN" direction="in"/>
<pin name="RIN1-" direction="in"/>
<pin name="RIN1+" direction="in"/>
<pin name="RIN2+" direction="in"/>
<pin name="RIN2-" direction="in"/>
<pin name="RIN3+" direction="in"/>
<pin name="RIN3-" direction="in"/>
<pin name="RIN4+" direction="in"/>
<pin name="RIN4-" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="ROUT1" direction="out"/>
<pin name="ROUT2" direction="out"/>
<pin name="ROUT3" direction="out"/>
<pin name="ROUT4" direction="out"/>
</symbol>
<symbol name="DS90C124QVS">
<pin name="VDDPR0" direction="pwr"/>
<pin name="VDDPR1" direction="pwr"/>
<pin name="VDDR0" direction="pwr"/>
<pin name="VDDR1" direction="pwr"/>
<pin name="VDDOR1" direction="pwr"/>
<pin name="VDDOR2" direction="pwr"/>
<pin name="VDDOR3" direction="pwr"/>
<pin name="VDDIR" direction="pwr"/>
<pin name="REN" direction="in"/>
<pin name="RCLK" direction="in"/>
<pin name="RIN+" direction="in"/>
<pin name="RIN-" direction="in"/>
<pin name="RRFB" direction="in"/>
<pin name="RPWDNB" direction="in"/>
<pin name="RESRVD" direction="in"/>
<pin name="VSSR1" direction="pas"/>
<pin name="VSSR0" direction="pas"/>
<pin name="VSSIR" direction="pas"/>
<pin name="VSSPR1" direction="pas"/>
<pin name="VSSPR0" direction="pas"/>
<pin name="VSSOR1" direction="pas"/>
<pin name="VSSOR2" direction="pas"/>
<pin name="VSSOR3" direction="pas"/>
<pin name="ROUT[0]" direction="out"/>
<pin name="ROUT[1]" direction="out"/>
<pin name="ROUT[2]" direction="out"/>
<pin name="ROUT[3]" direction="out"/>
<pin name="ROUT[4]" direction="out"/>
<pin name="ROUT[5]" direction="out"/>
<pin name="ROUT[6]" direction="out"/>
<pin name="ROUT[7]" direction="out"/>
<pin name="ROUT[8]" direction="out"/>
<pin name="ROUT[9]" direction="out"/>
<pin name="ROUT[10]" direction="out"/>
<pin name="ROUT[11]" direction="out"/>
<pin name="ROUT[12]" direction="out"/>
<pin name="ROUT[13]" direction="out"/>
<pin name="ROUT[14]" direction="out"/>
<pin name="ROUT[15]" direction="out"/>
<pin name="ROUT[16]" direction="out"/>
<pin name="ROUT[17]" direction="out"/>
<pin name="ROUT[18]" direction="out"/>
<pin name="ROUT[19]" direction="out"/>
<pin name="ROUT[20]" direction="out"/>
<pin name="ROUT[21]" direction="out"/>
<pin name="ROUT[22]" direction="out"/>
<pin name="LOCK" direction="out"/>
<pin name="ROUT[23]" direction="out"/>
</symbol>
<symbol name="DS90C241QVS">
<pin name="VDDL" direction="pwr"/>
<pin name="VDDT" direction="pwr"/>
<pin name="VDDIT" direction="pwr"/>
<pin name="VDDDR" direction="pwr"/>
<pin name="VDDPT1" direction="pwr"/>
<pin name="VDDPT0" direction="pwr"/>
<pin name="TCLK" direction="in"/>
<pin name="PRE" direction="in"/>
<pin name="DEN" direction="in"/>
<pin name="TPWDNB" direction="in"/>
<pin name="DCBOFF" direction="in"/>
<pin name="TRFB" direction="in"/>
<pin name="DCAOFF" direction="in"/>
<pin name="RESRVD" direction="pas"/>
<pin name="VODSEL" direction="in"/>
<pin name="DIN0" direction="in"/>
<pin name="DIN1" direction="in"/>
<pin name="DIN2" direction="in"/>
<pin name="DIN3" direction="in"/>
<pin name="DIN4" direction="in"/>
<pin name="DIN5" direction="in"/>
<pin name="DIN6" direction="in"/>
<pin name="DIN7" direction="in"/>
<pin name="DIN8" direction="in"/>
<pin name="DIN9" direction="in"/>
<pin name="DIN10" direction="in"/>
<pin name="DIN11" direction="in"/>
<pin name="DIN12" direction="in"/>
<pin name="DIN13" direction="in"/>
<pin name="DIN14" direction="in"/>
<pin name="DIN15" direction="in"/>
<pin name="DIN16" direction="in"/>
<pin name="DIN17" direction="in"/>
<pin name="DIN18" direction="in"/>
<pin name="DIN19" direction="in"/>
<pin name="DIN20" direction="in"/>
<pin name="DIN21" direction="in"/>
<pin name="DIN22" direction="in"/>
<pin name="DIN23" direction="in"/>
<pin name="VSS" direction="pas"/>
<pin name="VSSL" direction="pas"/>
<pin name="VSST" direction="pas"/>
<pin name="VSSDR" direction="pas"/>
<pin name="VSSPT0" direction="pas"/>
<pin name="VSSPT1" direction="pas"/>
<pin name="VSSIT" direction="pas"/>
<pin name="DOUT-" direction="out"/>
<pin name="DOUT+" direction="out"/>
</symbol>
<symbol name="DS90C3201VS_A">
<pin name="VDDI" direction="pwr"/>
<pin name="VDDL_2" direction="pwr"/>
<pin name="VDDL_3" direction="pwr"/>
<pin name="VDDL" direction="pwr"/>
<pin name="VDDP1" direction="pwr"/>
<pin name="VDDP0" direction="pwr"/>
<pin name="VDDE1" direction="pwr"/>
<pin name="VDDT0" direction="pwr"/>
<pin name="PWDNB" direction="in"/>
<pin name="TCLKIN" direction="in"/>
<pin name="S2CLK" direction="in"/>
<pin name="S2DAT"/>
<pin name="RFB" direction="in"/>
<pin name="MODE0" direction="in"/>
<pin name="MODE1" direction="in"/>
<pin name="RESRVD" direction="in"/>
<pin name="TXEB0" direction="in"/>
<pin name="TXEB1" direction="in"/>
<pin name="TXEB2" direction="in"/>
<pin name="TXEB3" direction="in"/>
<pin name="TXEB4" direction="in"/>
<pin name="TXEB5" direction="in"/>
<pin name="TXEB6" direction="in"/>
<pin name="TXEA0" direction="in"/>
<pin name="TXEA1" direction="in"/>
<pin name="TXEA2" direction="in"/>
<pin name="TXEA3" direction="in"/>
<pin name="TXEA4" direction="in"/>
<pin name="TXEA5" direction="in"/>
<pin name="TXEA6" direction="in"/>
<pin name="TXEC3" direction="in"/>
<pin name="TXEC4" direction="in"/>
<pin name="TXEC5" direction="in"/>
<pin name="TXEC6" direction="in"/>
<pin name="VSSL_2" direction="pwr"/>
<pin name="VSSL_3" direction="pas"/>
<pin name="VSSL" direction="pas"/>
<pin name="VSSI" direction="pas"/>
<pin name="VSSP1" direction="pas"/>
<pin name="VSSE1" direction="pas"/>
<pin name="VSSP0" direction="pas"/>
<pin name="VSST0" direction="pas"/>
<pin name="TXEA+" direction="out"/>
<pin name="TXEA-" direction="out"/>
<pin name="TXOA+" direction="out"/>
<pin name="TXOA-" direction="out"/>
<pin name="TXOB+" direction="out"/>
<pin name="TXOB-" direction="out"/>
<pin name="TXEB+" direction="out"/>
<pin name="TXEB-" direction="out"/>
<pin name="TXOC+" direction="out"/>
<pin name="TXOC-" direction="out"/>
<pin name="TXEC+" direction="out"/>
<pin name="TXEC-" direction="out"/>
<pin name="TXOD+" direction="out"/>
<pin name="TXOD-" direction="out"/>
<pin name="TXED+" direction="out"/>
<pin name="TXED-" direction="out"/>
<pin name="TXOE+" direction="out"/>
<pin name="TXOE-" direction="out"/>
<pin name="TXEE+" direction="out"/>
<pin name="TXEE-" direction="out"/>
<pin name="TCLKOUT+" direction="out"/>
<pin name="TCLKOUT-" direction="out"/>
</symbol>
<symbol name="DS90C3201VS_B">
<pin name="VDDO0" direction="pwr"/>
<pin name="VDDT2" direction="pwr"/>
<pin name="VDDT3" direction="pwr"/>
<pin name="VDDT1" direction="pwr"/>
<pin name="VDDO1" direction="pwr"/>
<pin name="VDDE0" direction="pwr"/>
<pin name="TXOE0" direction="in"/>
<pin name="TXOE1" direction="in"/>
<pin name="TXOE2" direction="in"/>
<pin name="TXOE3" direction="in"/>
<pin name="TXOE4" direction="in"/>
<pin name="TXOE5" direction="in"/>
<pin name="TXOE6" direction="in"/>
<pin name="TXOD0" direction="in"/>
<pin name="TXOD1" direction="in"/>
<pin name="TXOD2" direction="in"/>
<pin name="TXOD3" direction="in"/>
<pin name="TXOD4" direction="in"/>
<pin name="TXOD5" direction="in"/>
<pin name="TXOD6" direction="in"/>
<pin name="TXOC0" direction="in"/>
<pin name="TXOC1" direction="in"/>
<pin name="TXOC2" direction="in"/>
<pin name="TXOC3" direction="in"/>
<pin name="TXOC4" direction="in"/>
<pin name="TXOC5" direction="in"/>
<pin name="TXOC6" direction="in"/>
<pin name="TXOB0" direction="in"/>
<pin name="TXOB1" direction="in"/>
<pin name="TXOB2" direction="in"/>
<pin name="TXOB3" direction="in"/>
<pin name="TXOB4" direction="in"/>
<pin name="TXOB5" direction="in"/>
<pin name="TXOB6" direction="in"/>
<pin name="TXOA0" direction="in"/>
<pin name="TXOA1" direction="in"/>
<pin name="TXOA2" direction="in"/>
<pin name="TXOA3" direction="in"/>
<pin name="TXOA4" direction="in"/>
<pin name="TXOA5" direction="in"/>
<pin name="TXOA6" direction="in"/>
<pin name="TXEE0" direction="in"/>
<pin name="TXEE1" direction="in"/>
<pin name="TXEE2" direction="in"/>
<pin name="TXEE3" direction="in"/>
<pin name="TXEE4" direction="in"/>
<pin name="TXEE5" direction="in"/>
<pin name="TXEE6" direction="in"/>
<pin name="TXED0" direction="in"/>
<pin name="TXED1" direction="in"/>
<pin name="TXED2" direction="in"/>
<pin name="TXED3" direction="in"/>
<pin name="TXED4" direction="in"/>
<pin name="TXED5" direction="in"/>
<pin name="TXED6" direction="in"/>
<pin name="TXEC0" direction="in"/>
<pin name="TXEC1" direction="in"/>
<pin name="TXEC2" direction="in"/>
<pin name="VSST1" direction="pas"/>
<pin name="VSST2" direction="pas"/>
<pin name="VSSO1" direction="pas"/>
<pin name="VSSE0" direction="pas"/>
<pin name="VSSO0" direction="pas"/>
<pin name="VSST3" direction="pas"/>
</symbol>
<symbol name="DS90C3202VS_A">
<pin name="VDDR0" direction="pwr"/>
<pin name="VDDP1" direction="pwr"/>
<pin name="VDD1" direction="pwr"/>
<pin name="VDDP0" direction="pwr"/>
<pin name="VDDR1" direction="pwr"/>
<pin name="VDD0" direction="pwr"/>
<pin name="VDD2" direction="pwr"/>
<pin name="VDD3" direction="pwr"/>
<pin name="S2CLK" direction="in"/>
<pin name="PWDNB" direction="in"/>
<pin name="S2DAT"/>
<pin name="VSS0" direction="pas"/>
<pin name="VSS1" direction="pas"/>
<pin name="VSSR0" direction="pas"/>
<pin name="VSS2" direction="pas"/>
<pin name="VSS3" direction="pwr"/>
<pin name="VSS4" direction="pas"/>
<pin name="VSSR1" direction="pas"/>
<pin name="VSSP1" direction="pas"/>
<pin name="VSSP0" direction="pas"/>
<pin name="RXEE0" direction="out"/>
<pin name="RCLKOUT" direction="out"/>
<pin name="RXOE0" direction="out"/>
<pin name="RXEE1" direction="out"/>
<pin name="RXOE1" direction="out"/>
<pin name="RXEE2" direction="out"/>
<pin name="RXOE2" direction="out"/>
<pin name="RXEE3" direction="out"/>
<pin name="RXOE3" direction="out"/>
<pin name="RXEE4" direction="out"/>
<pin name="RXOE4" direction="out"/>
<pin name="RXEE5" direction="out"/>
<pin name="RXOE5" direction="out"/>
<pin name="RXEE6" direction="out"/>
<pin name="RXOE6" direction="out"/>
<pin name="RXED0" direction="out"/>
<pin name="RXOD0" direction="out"/>
<pin name="RXED1" direction="out"/>
<pin name="RXED2" direction="out"/>
<pin name="RXED3" direction="out"/>
<pin name="RXED4" direction="out"/>
<pin name="RXED5" direction="out"/>
<pin name="RXED6" direction="out"/>
<pin name="RXEC0" direction="out"/>
<pin name="RXEC1" direction="out"/>
<pin name="RXEC2" direction="out"/>
<pin name="RXEC3" direction="out"/>
<pin name="RXEC4" direction="out"/>
<pin name="RXEC5" direction="out"/>
<pin name="RXEC6" direction="out"/>
<pin name="RXEB0" direction="out"/>
<pin name="RXEB1" direction="out"/>
<pin name="RXEB2" direction="out"/>
<pin name="RXEB3" direction="out"/>
<pin name="RXEB4" direction="out"/>
<pin name="RXEB5" direction="out"/>
<pin name="RXEB6" direction="out"/>
<pin name="RXEA0" direction="out"/>
<pin name="RXEA1" direction="out"/>
<pin name="RXEA2" direction="out"/>
<pin name="RXEA3" direction="out"/>
<pin name="RXEA4" direction="out"/>
<pin name="RXEA5" direction="out"/>
<pin name="RXEA6" direction="out"/>
</symbol>
<symbol name="DS90C3202VS_B">
<pin name="VDD4" direction="pwr"/>
<pin name="VDDR2" direction="pwr"/>
<pin name="VDD5" direction="pwr"/>
<pin name="VDDL_2" direction="pwr"/>
<pin name="VDDL_3" direction="pwr"/>
<pin name="VDDL" direction="pwr"/>
<pin name="RCLKIN-" direction="in"/>
<pin name="RCLKIN+" direction="in"/>
<pin name="MODE1" direction="in"/>
<pin name="MODE0" direction="in"/>
<pin name="RESRVD" direction="in"/>
<pin name="RFB" direction="in"/>
<pin name="RXEA+" direction="in"/>
<pin name="RXEA-" direction="in"/>
<pin name="RXOA-" direction="in"/>
<pin name="RXOA+" direction="in"/>
<pin name="RXOA0" direction="out"/>
<pin name="RXOB-" direction="in"/>
<pin name="RXEB-" direction="in"/>
<pin name="RXEB+" direction="in"/>
<pin name="RXOB+" direction="in"/>
<pin name="RXEC-" direction="in"/>
<pin name="RXOC-" direction="in"/>
<pin name="RXOC+" direction="in"/>
<pin name="RXEC+" direction="in"/>
<pin name="RXED-" direction="in"/>
<pin name="RXOD-" direction="in"/>
<pin name="RXOD+" direction="in"/>
<pin name="RXED+" direction="in"/>
<pin name="RXOE-" direction="in"/>
<pin name="RXEE+" direction="in"/>
<pin name="RXOE+" direction="in"/>
<pin name="RXEE-" direction="in"/>
<pin name="VSS5" direction="pas"/>
<pin name="VSSL_2" direction="pas"/>
<pin name="VSSL_3" direction="pas"/>
<pin name="VSSL" direction="pas"/>
<pin name="VSSR2" direction="pwr"/>
<pin name="RXOD1" direction="out"/>
<pin name="RXOD2" direction="out"/>
<pin name="RXOD3" direction="out"/>
<pin name="RXOD4" direction="out"/>
<pin name="RXOD5" direction="out"/>
<pin name="RXOD6" direction="out"/>
<pin name="RXOC0" direction="out"/>
<pin name="RXOC1" direction="out"/>
<pin name="RXOC2" direction="out"/>
<pin name="RXOC3" direction="out"/>
<pin name="RXOC4" direction="out"/>
<pin name="RXOC5" direction="out"/>
<pin name="RXOC6" direction="out"/>
<pin name="RXOB0" direction="out"/>
<pin name="RXOB1" direction="out"/>
<pin name="RXOB2" direction="out"/>
<pin name="RXOB3" direction="out"/>
<pin name="RXOB4" direction="out"/>
<pin name="RXOB5" direction="out"/>
<pin name="RXOB6" direction="out"/>
<pin name="RXOA1" direction="out"/>
<pin name="RXOA2" direction="out"/>
<pin name="RXOA3" direction="out"/>
<pin name="RXOA4" direction="out"/>
<pin name="RXOA5" direction="out"/>
<pin name="RXOA6" direction="out"/>
</symbol>
<symbol name="DS90C402M">
<pin name="VCC" direction="pwr"/>
<pin name="RI1+" direction="in"/>
<pin name="RI1-" direction="in"/>
<pin name="RI2+" direction="in"/>
<pin name="RI2-" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="RO1" direction="out"/>
<pin name="RO2" direction="out"/>
</symbol>
<symbol name="DS90CF364AMTD">
<pin name="VCC_2" direction="pwr"/>
<pin name="VCC_3" direction="pwr"/>
<pin name="VCC_4" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="LVDSVCC" direction="pwr"/>
<pin name="PLLVCC" direction="pwr"/>
<pin name="RXCLKIN-" direction="in"/>
<pin name="RXCLKIN+" direction="in"/>
<pin name="RXIN0-" direction="in"/>
<pin name="RXIN0+" direction="in"/>
<pin name="RXIN1-" direction="in"/>
<pin name="RXIN1+" direction="in"/>
<pin name="RXIN2-" direction="in"/>
<pin name="RXIN2+" direction="in"/>
<pin name="~PWRDWN" direction="pwr"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="LVDSGND_2" direction="pas"/>
<pin name="PLLGND_2" direction="pas"/>
<pin name="LVDSGND_3" direction="pas"/>
<pin name="PLLGND" direction="pas"/>
<pin name="LVDSGND" direction="pas"/>
<pin name="RXCLKOUT" direction="out"/>
<pin name="RXOUT0" direction="out"/>
<pin name="RXOUT1" direction="out"/>
<pin name="RXOUT2" direction="out"/>
<pin name="RXOUT3" direction="out"/>
<pin name="RXOUT4" direction="out"/>
<pin name="RXOUT5" direction="out"/>
<pin name="RXOUT6" direction="out"/>
<pin name="RXOUT7" direction="out"/>
<pin name="RXOUT8" direction="out"/>
<pin name="RXOUT9" direction="out"/>
<pin name="RXOUT10" direction="out"/>
<pin name="RXOUT11" direction="out"/>
<pin name="RXOUT12" direction="out"/>
<pin name="RXOUT13" direction="out"/>
<pin name="RXOUT14" direction="out"/>
<pin name="RXOUT15" direction="out"/>
<pin name="RXOUT16" direction="out"/>
<pin name="RXOUT17" direction="out"/>
<pin name="RXOUT18" direction="out"/>
<pin name="RXOUT19" direction="out"/>
<pin name="RXOUT20" direction="out"/>
</symbol>
<symbol name="DS90CF384AMTD">
<pin name="VCC_2" direction="pwr"/>
<pin name="VCC_3" direction="pwr"/>
<pin name="VCC_4" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="PLL_VCC" direction="pwr"/>
<pin name="LVDS_VCC" direction="pwr"/>
<pin name="RXCLKIN-" direction="in"/>
<pin name="RXCLKIN+" direction="in"/>
<pin name="RXIN0-" direction="in"/>
<pin name="RXIN0+" direction="in"/>
<pin name="RXIN1-" direction="in"/>
<pin name="RXIN1+" direction="in"/>
<pin name="RXIN2-" direction="in"/>
<pin name="RXIN2+" direction="in"/>
<pin name="RXIN3-" direction="in"/>
<pin name="RXIN3+" direction="in"/>
<pin name="~PWR_DOWN" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="PLL_GND_2" direction="pas"/>
<pin name="PLL_GND" direction="pas"/>
<pin name="LVDS_GND_2" direction="pas"/>
<pin name="LVDS_GND_3" direction="pas"/>
<pin name="LVDS_GND" direction="pas"/>
<pin name="RXCLK_OUT" direction="out"/>
<pin name="RXOUT0" direction="out"/>
<pin name="RXOUT1" direction="out"/>
<pin name="RXOUT2" direction="out"/>
<pin name="RXOUT3" direction="out"/>
<pin name="RXOUT4" direction="out"/>
<pin name="RXOUT5" direction="out"/>
<pin name="RXOUT6" direction="out"/>
<pin name="RXOUT7" direction="out"/>
<pin name="RXOUT8" direction="out"/>
<pin name="RXOUT9" direction="out"/>
<pin name="RXOUT10" direction="out"/>
<pin name="RXOUT11" direction="out"/>
<pin name="RXOUT12" direction="out"/>
<pin name="RXOUT13" direction="out"/>
<pin name="RXOUT14" direction="out"/>
<pin name="RXOUT15" direction="out"/>
<pin name="RXOUT16" direction="out"/>
<pin name="RXOUT17" direction="out"/>
<pin name="RXOUT18" direction="out"/>
<pin name="RXOUT19" direction="out"/>
<pin name="RXOUT20" direction="out"/>
<pin name="RXOUT21" direction="out"/>
<pin name="RXOUT22" direction="out"/>
<pin name="RXOUT23" direction="out"/>
<pin name="RXOUT24" direction="out"/>
<pin name="RXOUT25" direction="out"/>
<pin name="RXOUT26" direction="out"/>
<pin name="RXOUT27" direction="out"/>
</symbol>
<symbol name="DS90CP04TLQ">
<pin name="VDD_2" direction="pwr"/>
<pin name="VDD_3" direction="pwr"/>
<pin name="VDD_4" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="SEL0" direction="in"/>
<pin name="SCLK" direction="in"/>
<pin name="SI/SEL1" direction="in"/>
<pin name="LOAD" direction="in"/>
<pin name="MODE" direction="in"/>
<pin name="IN4-" direction="in"/>
<pin name="IN4+" direction="in"/>
<pin name="IN3-" direction="in"/>
<pin name="IN3+" direction="in"/>
<pin name="IN2-" direction="in"/>
<pin name="IN2+" direction="in"/>
<pin name="IN1-" direction="in"/>
<pin name="IN1+" direction="in"/>
<pin name="EP" direction="pas"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="CSO" direction="out"/>
<pin name="RSO" direction="out"/>
<pin name="RSCLK" direction="out"/>
<pin name="CSCLK" direction="out"/>
<pin name="OUT1+" direction="out"/>
<pin name="OUT1-" direction="out"/>
<pin name="OUT2+" direction="out"/>
<pin name="OUT2-" direction="out"/>
<pin name="OUT3+" direction="out"/>
<pin name="OUT3-" direction="out"/>
<pin name="OUT4+" direction="out"/>
<pin name="OUT4-" direction="out"/>
</symbol>
<symbol name="DS90CP22M-8">
<pin name="VCC" direction="pwr"/>
<pin name="EN1" direction="in"/>
<pin name="EN0" direction="in"/>
<pin name="SEL1" direction="in"/>
<pin name="SEL0" direction="in"/>
<pin name="IN0+" direction="in"/>
<pin name="IN0-" direction="in"/>
<pin name="IN1+" direction="in"/>
<pin name="IN1-" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="OUT0-" direction="out"/>
<pin name="OUT0+" direction="out"/>
<pin name="OUT1-" direction="out"/>
<pin name="OUT1+" direction="out"/>
</symbol>
<symbol name="DS90CP22MT">
<pin name="VCC" direction="pwr"/>
<pin name="EN1" direction="in"/>
<pin name="EN0" direction="in"/>
<pin name="SEL1" direction="in"/>
<pin name="SEL0" direction="in"/>
<pin name="IN0+" direction="in"/>
<pin name="IN0-" direction="in"/>
<pin name="IN1+" direction="in"/>
<pin name="IN1-" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="OUT1-" direction="out"/>
<pin name="OUT1+" direction="out"/>
<pin name="OUT0-" direction="out"/>
<pin name="OUT0+" direction="out"/>
</symbol>
<symbol name="DS90CR215MTD">
<pin name="VCC_2" direction="pwr"/>
<pin name="VCC_3" direction="pwr"/>
<pin name="VCC_4" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="PLL_VCC" direction="pwr"/>
<pin name="LVDS_VCC" direction="pwr"/>
<pin name="TXCLK_IN" direction="in"/>
<pin name="~PWRDWN" direction="in"/>
<pin name="TXIN0" direction="in"/>
<pin name="TXIN1" direction="in"/>
<pin name="TXIN2" direction="in"/>
<pin name="TXIN3" direction="in"/>
<pin name="TXIN4" direction="in"/>
<pin name="TXIN5" direction="in"/>
<pin name="TXIN6" direction="in"/>
<pin name="TXIN7" direction="in"/>
<pin name="TXIN8" direction="in"/>
<pin name="TXIN9" direction="in"/>
<pin name="TXIN10" direction="in"/>
<pin name="TXIN11" direction="in"/>
<pin name="TXIN12" direction="in"/>
<pin name="TXIN13" direction="in"/>
<pin name="TXIN14" direction="in"/>
<pin name="TXIN15" direction="in"/>
<pin name="TXIN16" direction="in"/>
<pin name="TXIN17" direction="in"/>
<pin name="TXIN18" direction="in"/>
<pin name="TXIN19" direction="in"/>
<pin name="TXIN20" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="PLL_GND_2" direction="pas"/>
<pin name="PLL_GND" direction="pas"/>
<pin name="LVDS_GND_2" direction="pas"/>
<pin name="LVDS_GND_3" direction="pas"/>
<pin name="LVDS_GND" direction="pas"/>
<pin name="TXCLK_OUT+" direction="out"/>
<pin name="TXCLK_OUT-" direction="out"/>
<pin name="TXOUT2+" direction="out"/>
<pin name="TXOUT2-" direction="out"/>
<pin name="TXOUT1+" direction="out"/>
<pin name="TXOUT1-" direction="out"/>
<pin name="TXOUT0+" direction="out"/>
<pin name="TXOUT0-" direction="out"/>
</symbol>
<symbol name="DS90CR216AMTD">
<pin name="VCC_2" direction="pwr"/>
<pin name="VCC_3" direction="pwr"/>
<pin name="VCC_4" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="LVDSVCC" direction="pwr"/>
<pin name="PLLVCC" direction="pwr"/>
<pin name="RXCLKIN-" direction="in"/>
<pin name="RXCLKIN+" direction="in"/>
<pin name="RXIN0-" direction="in"/>
<pin name="RXIN0+" direction="in"/>
<pin name="RXIN1-" direction="in"/>
<pin name="RXIN1+" direction="in"/>
<pin name="RXIN2-" direction="in"/>
<pin name="RXIN2+" direction="in"/>
<pin name="~PWRDWN" direction="pwr"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="LVDSGND_2" direction="pas"/>
<pin name="PLLGND_2" direction="pas"/>
<pin name="LVDSGND_3" direction="pas"/>
<pin name="PLLGND" direction="pas"/>
<pin name="LVDSGND" direction="pas"/>
<pin name="RXCLKOUT" direction="out"/>
<pin name="RXOUT0" direction="out"/>
<pin name="RXOUT1" direction="out"/>
<pin name="RXOUT2" direction="out"/>
<pin name="RXOUT3" direction="out"/>
<pin name="RXOUT4" direction="out"/>
<pin name="RXOUT5" direction="out"/>
<pin name="RXOUT6" direction="out"/>
<pin name="RXOUT7" direction="out"/>
<pin name="RXOUT8" direction="out"/>
<pin name="RXOUT9" direction="out"/>
<pin name="RXOUT10" direction="out"/>
<pin name="RXOUT11" direction="out"/>
<pin name="RXOUT12" direction="out"/>
<pin name="RXOUT13" direction="out"/>
<pin name="RXOUT14" direction="out"/>
<pin name="RXOUT15" direction="out"/>
<pin name="RXOUT16" direction="out"/>
<pin name="RXOUT17" direction="out"/>
<pin name="RXOUT18" direction="out"/>
<pin name="RXOUT19" direction="out"/>
<pin name="RXOUT20" direction="out"/>
</symbol>
<symbol name="DS90CR217MTD">
<pin name="VCC_2" direction="pwr"/>
<pin name="VCC_3" direction="pwr"/>
<pin name="VCC_4" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="PLL_VCC" direction="pwr"/>
<pin name="TXCLK_IN" direction="in"/>
<pin name="~PWRDWN" direction="in"/>
<pin name="TXIN0" direction="in"/>
<pin name="TXIN1" direction="in"/>
<pin name="TXIN2" direction="in"/>
<pin name="TXIN3" direction="in"/>
<pin name="TXIN4" direction="in"/>
<pin name="TXIN5" direction="in"/>
<pin name="TXIN6" direction="in"/>
<pin name="TXIN7" direction="in"/>
<pin name="TXIN8" direction="in"/>
<pin name="TXIN9" direction="in"/>
<pin name="TXIN10" direction="in"/>
<pin name="TXIN11" direction="in"/>
<pin name="TXIN12" direction="in"/>
<pin name="TXIN13" direction="in"/>
<pin name="TXIN14" direction="in"/>
<pin name="TXIN15" direction="in"/>
<pin name="TXIN16" direction="in"/>
<pin name="TXIN17" direction="in"/>
<pin name="TXIN18" direction="in"/>
<pin name="TXIN19" direction="in"/>
<pin name="TXIN20" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="PLL_GND_2" direction="pas"/>
<pin name="PLL_GND" direction="pas"/>
<pin name="LVDS_GND_2" direction="pas"/>
<pin name="LVDS_GND_3" direction="pas"/>
<pin name="LVDS_VCC" direction="pwr"/>
<pin name="LVDS_GND" direction="pas"/>
<pin name="TXCLK_OUT+" direction="out"/>
<pin name="TXCLK_OUT-" direction="out"/>
<pin name="TXOUT2+" direction="out"/>
<pin name="TXOUT2-" direction="out"/>
<pin name="TXOUT1+" direction="out"/>
<pin name="TXOUT1-" direction="out"/>
<pin name="TXOUT0+" direction="out"/>
<pin name="TXOUT0-" direction="out"/>
</symbol>
<symbol name="DS90CR218AMTD">
<pin name="VCC_2" direction="pwr"/>
<pin name="VCC_3" direction="pwr"/>
<pin name="VCC_4" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="PLLVCC" direction="pwr"/>
<pin name="LVDSVCC" direction="pwr"/>
<pin name="RXCLKIN-" direction="in"/>
<pin name="RXCLKIN+" direction="in"/>
<pin name="~PWRDWN" direction="pwr"/>
<pin name="RXCLKOUT" direction="out"/>
<pin name="RXIN0-" direction="in"/>
<pin name="RXIN0+" direction="in"/>
<pin name="RXIN1-" direction="in"/>
<pin name="RXIN1+" direction="in"/>
<pin name="RXIN2-" direction="in"/>
<pin name="RXIN2+" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="PLLGND_2" direction="pas"/>
<pin name="PLLGND" direction="pas"/>
<pin name="LVDSGND_2" direction="pas"/>
<pin name="LVDSGND_3" direction="pas"/>
<pin name="LVDSGND" direction="pas"/>
<pin name="RXOUT0" direction="out"/>
<pin name="RXOUT1" direction="out"/>
<pin name="RXOUT2" direction="out"/>
<pin name="RXOUT3" direction="out"/>
<pin name="RXOUT4" direction="out"/>
<pin name="RXOUT5" direction="out"/>
<pin name="RXOUT6" direction="out"/>
<pin name="RXOUT7" direction="out"/>
<pin name="RXOUT8" direction="out"/>
<pin name="RXOUT9" direction="out"/>
<pin name="RXOUT10" direction="out"/>
<pin name="RXOUT11" direction="out"/>
<pin name="RXOUT12" direction="out"/>
<pin name="RXOUT13" direction="out"/>
<pin name="RXOUT14" direction="out"/>
<pin name="RXOUT15" direction="out"/>
<pin name="RXOUT16" direction="out"/>
<pin name="RXOUT17" direction="out"/>
<pin name="RXOUT18" direction="out"/>
<pin name="RXOUT19" direction="out"/>
<pin name="RXOUT20" direction="out"/>
</symbol>
<symbol name="DS90CR285MTD">
<pin name="VCC_2" direction="pwr"/>
<pin name="VCC_3" direction="pwr"/>
<pin name="VCC_4" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="PLL_VCC" direction="pwr"/>
<pin name="LVDS_VCC" direction="pwr"/>
<pin name="TXCLK_IN" direction="in"/>
<pin name="~PWRDWN" direction="pas"/>
<pin name="TXIN0" direction="in"/>
<pin name="TXIN1" direction="in"/>
<pin name="TXIN2" direction="in"/>
<pin name="TXIN3" direction="in"/>
<pin name="TXIN4" direction="in"/>
<pin name="TXIN5" direction="in"/>
<pin name="TXIN6" direction="in"/>
<pin name="TXIN7" direction="in"/>
<pin name="TXIN8" direction="in"/>
<pin name="TXIN9" direction="in"/>
<pin name="TXIN10" direction="in"/>
<pin name="TXIN11" direction="in"/>
<pin name="TXIN12" direction="in"/>
<pin name="TXIN13" direction="in"/>
<pin name="TXIN14" direction="in"/>
<pin name="TXIN15" direction="in"/>
<pin name="TXIN16" direction="in"/>
<pin name="TXIN17" direction="in"/>
<pin name="TXIN18" direction="in"/>
<pin name="TXIN19" direction="in"/>
<pin name="TXIN20" direction="in"/>
<pin name="TXIN21" direction="in"/>
<pin name="TXIN22" direction="in"/>
<pin name="TXIN23" direction="in"/>
<pin name="TXIN24" direction="in"/>
<pin name="TXIN25" direction="in"/>
<pin name="TXIN26" direction="in"/>
<pin name="TXIN27" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="LVDS_GND_2" direction="pas"/>
<pin name="LVDS_GND_3" direction="pas"/>
<pin name="LVDS_GND" direction="pas"/>
<pin name="PLL_GND_2" direction="pas"/>
<pin name="PLL_GND" direction="pas"/>
<pin name="TXOUT0+" direction="out"/>
<pin name="TXOUT0-" direction="out"/>
<pin name="TXOUT1+" direction="out"/>
<pin name="TXOUT1-" direction="out"/>
<pin name="TXOUT2+" direction="out"/>
<pin name="TXOUT2-" direction="out"/>
<pin name="TXOUT3+" direction="out"/>
<pin name="TXOUT3-" direction="out"/>
<pin name="TXCLKOUT+" direction="out"/>
<pin name="TXCLKOUT-" direction="out"/>
</symbol>
<symbol name="DS90CR286AQMT">
<pin name="VCC_2" direction="pwr"/>
<pin name="VCC_3" direction="pwr"/>
<pin name="VCC_4" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="LVDS_VCC" direction="pwr"/>
<pin name="PLL_VCC" direction="pwr"/>
<pin name="RXCLKIN+" direction="in"/>
<pin name="RXCLKIN-" direction="in"/>
<pin name="~PWR_DOWN" direction="in"/>
<pin name="RXIN0+" direction="in"/>
<pin name="RXIN0-" direction="in"/>
<pin name="RXIN1+" direction="in"/>
<pin name="RXIN1-" direction="in"/>
<pin name="RXIN2+" direction="in"/>
<pin name="RXIN2-" direction="in"/>
<pin name="RXIN3+" direction="in"/>
<pin name="RXIN3-" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="LVDS_GND_2" direction="pas"/>
<pin name="LVDS_GND_3" direction="pas"/>
<pin name="PLL_GND_2" direction="pas"/>
<pin name="PLL_GND" direction="pas"/>
<pin name="LVDS_GND" direction="pwr"/>
<pin name="RXCLK_OUT" direction="out"/>
<pin name="RXOUT0" direction="out"/>
<pin name="RXOUT1" direction="out"/>
<pin name="RXOUT2" direction="out"/>
<pin name="RXOUT3" direction="out"/>
<pin name="RXOUT4" direction="out"/>
<pin name="RXOUT5" direction="out"/>
<pin name="RXOUT6" direction="out"/>
<pin name="RXOUT7" direction="out"/>
<pin name="RXOUT8" direction="out"/>
<pin name="RXOUT9" direction="out"/>
<pin name="RXOUT10" direction="out"/>
<pin name="RXOUT11" direction="out"/>
<pin name="RXOUT12" direction="out"/>
<pin name="RXOUT13" direction="out"/>
<pin name="RXOUT14" direction="out"/>
<pin name="RXOUT15" direction="out"/>
<pin name="RXOUT16" direction="out"/>
<pin name="RXOUT17" direction="out"/>
<pin name="RXOUT18" direction="out"/>
<pin name="RXOUT19" direction="out"/>
<pin name="RXOUT20" direction="out"/>
<pin name="RXOUT21" direction="out"/>
<pin name="RXOUT22" direction="out"/>
<pin name="RXOUT23" direction="out"/>
<pin name="RXOUT24" direction="out"/>
<pin name="RXOUT25" direction="out"/>
<pin name="RXOUT26" direction="out"/>
<pin name="RXOUT27" direction="out"/>
</symbol>
<symbol name="DS90CR287MTD">
<pin name="VCC_2" direction="pwr"/>
<pin name="VCC_3" direction="pwr"/>
<pin name="VCC_4" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="PLL_VCC" direction="pwr"/>
<pin name="LVDS_VCC" direction="pwr"/>
<pin name="TXCLK_IN" direction="in"/>
<pin name="~PWR~_~DWN" direction="in"/>
<pin name="TXIN0" direction="in"/>
<pin name="TXIN1" direction="in"/>
<pin name="TXIN2" direction="in"/>
<pin name="TXIN3" direction="in"/>
<pin name="TXIN4" direction="in"/>
<pin name="TXIN5" direction="in"/>
<pin name="TXIN6" direction="in"/>
<pin name="TXIN7" direction="in"/>
<pin name="TXIN8" direction="in"/>
<pin name="TXIN9" direction="in"/>
<pin name="TXIN10" direction="in"/>
<pin name="TXIN11" direction="in"/>
<pin name="TXIN12" direction="in"/>
<pin name="TXIN13" direction="in"/>
<pin name="TXIN14" direction="in"/>
<pin name="TXIN15" direction="in"/>
<pin name="TXIN16" direction="in"/>
<pin name="TXIN17" direction="in"/>
<pin name="TXIN18" direction="in"/>
<pin name="TXIN19" direction="in"/>
<pin name="TXIN20" direction="in"/>
<pin name="TXIN21" direction="in"/>
<pin name="TXIN22" direction="in"/>
<pin name="TXIN23" direction="in"/>
<pin name="TXIN24" direction="in"/>
<pin name="TXIN25" direction="in"/>
<pin name="TXIN26" direction="in"/>
<pin name="TXIN27" direction="in"/>
<pin name="PLL_GND_2" direction="pas"/>
<pin name="PLL_GND" direction="pas"/>
<pin name="LVDS_GND_2" direction="pas"/>
<pin name="LVDS_GND_3" direction="pas"/>
<pin name="LVDS_GND" direction="pas"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="TXOUT0+" direction="out"/>
<pin name="TXOUT0-" direction="out"/>
<pin name="TXOUT1+" direction="out"/>
<pin name="TXOUT1-" direction="out"/>
<pin name="TXOUT2+" direction="out"/>
<pin name="TXOUT2-" direction="out"/>
<pin name="TXOUT3+" direction="out"/>
<pin name="TXOUT3-" direction="out"/>
<pin name="TXCLKOUT+" direction="out"/>
<pin name="TXCLKOUT-" direction="out"/>
</symbol>
<symbol name="DS90CR288AMTD">
<pin name="LVDSVCC" direction="pwr"/>
<pin name="PLLVCC" direction="pwr"/>
<pin name="VCC_2" direction="pwr"/>
<pin name="VCC_3" direction="pwr"/>
<pin name="VCC_4" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="RXIN0-" direction="in"/>
<pin name="RXIN0+" direction="in"/>
<pin name="RXIN1-" direction="in"/>
<pin name="RXIN1+" direction="in"/>
<pin name="RXIN2-" direction="in"/>
<pin name="RXIN2+" direction="in"/>
<pin name="RXIN3-" direction="in"/>
<pin name="RXIN3+" direction="in"/>
<pin name="RXCLKIN-" direction="in"/>
<pin name="RXCLKIN+" direction="in"/>
<pin name="~PWRDN" direction="pas"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="PLLGND_2" direction="pas"/>
<pin name="PLLGND" direction="pwr"/>
<pin name="LVDSGND_2" direction="pas"/>
<pin name="LVDSGND_3" direction="pas"/>
<pin name="LVDSGND" direction="pas"/>
<pin name="RXCLK_OUT" direction="out"/>
<pin name="RXOUT0" direction="out"/>
<pin name="RXOUT1" direction="out"/>
<pin name="RXOUT2" direction="out"/>
<pin name="RXOUT3" direction="out"/>
<pin name="RXOUT4" direction="out"/>
<pin name="RXOUT5" direction="out"/>
<pin name="RXOUT6" direction="out"/>
<pin name="RXOUT7" direction="out"/>
<pin name="RXOUT8" direction="out"/>
<pin name="RXOUT9" direction="out"/>
<pin name="RXOUT10" direction="out"/>
<pin name="RXOUT11" direction="out"/>
<pin name="RXOUT12" direction="out"/>
<pin name="RXOUT13" direction="out"/>
<pin name="RXOUT14" direction="out"/>
<pin name="RXOUT15" direction="out"/>
<pin name="RXOUT16" direction="out"/>
<pin name="RXOUT17" direction="out"/>
<pin name="RXOUT18" direction="out"/>
<pin name="RXOUT19" direction="out"/>
<pin name="RXOUT20" direction="out"/>
<pin name="RXOUT21" direction="out"/>
<pin name="RXOUT22" direction="out"/>
<pin name="RXOUT23" direction="out"/>
<pin name="RXOUT24" direction="out"/>
<pin name="RXOUT25" direction="out"/>
<pin name="RXOUT26" direction="out"/>
<pin name="RXOUT27" direction="out"/>
</symbol>
<symbol name="DS90CR482VS">
<pin name="VCC_2" direction="pwr"/>
<pin name="VCC_3" direction="pwr"/>
<pin name="VCC_4" direction="pwr"/>
<pin name="VCC_5" direction="pwr"/>
<pin name="VCC_6" direction="pwr"/>
<pin name="VCC_7" direction="pwr"/>
<pin name="VCC_8" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="LVDSVCC_2" direction="pwr"/>
<pin name="LVDSVCC" direction="pwr"/>
<pin name="PLLVCC" direction="pwr"/>
<pin name="DESKEW" direction="in"/>
<pin name="PLLSEL" direction="in"/>
<pin name="~PD" direction="in"/>
<pin name="RXCLKP" direction="in"/>
<pin name="RXCLKM" direction="in"/>
<pin name="RXIN0P" direction="in"/>
<pin name="RXIN1P" direction="in"/>
<pin name="RXINP2" direction="in"/>
<pin name="RXINP3" direction="in"/>
<pin name="RXINP4" direction="in"/>
<pin name="RXINP5" direction="in"/>
<pin name="RXINP6" direction="in"/>
<pin name="RXINP7" direction="in"/>
<pin name="RXIN0M" direction="in"/>
<pin name="RXIN1M" direction="in"/>
<pin name="RXINM2" direction="in"/>
<pin name="RXINM3" direction="in"/>
<pin name="RXINM4" direction="in"/>
<pin name="RXINM5" direction="in"/>
<pin name="RXINM6" direction="in"/>
<pin name="RXINM7" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC_6" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pwr"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND" direction="pwr"/>
<pin name="LVDSGND_2" direction="pas"/>
<pin name="LVDSGND_3" direction="pas"/>
<pin name="LVDSGND" direction="pas"/>
<pin name="PLLGND_2" direction="pas"/>
<pin name="PLLGND" direction="pas"/>
<pin name="RXOUT0" direction="out"/>
<pin name="RXOUT1" direction="out"/>
<pin name="RXOUT2" direction="out"/>
<pin name="RXOUT3" direction="out"/>
<pin name="RXOUT4" direction="out"/>
<pin name="RXOUT5" direction="out"/>
<pin name="RXOUT6" direction="out"/>
<pin name="RXOUT7" direction="out"/>
<pin name="RXOUT8" direction="out"/>
<pin name="RXOUT9" direction="out"/>
<pin name="RXOUT10" direction="out"/>
<pin name="RXOUT11" direction="out"/>
<pin name="RXOUT12" direction="out"/>
<pin name="RXOUT13" direction="out"/>
<pin name="RXOUT14" direction="out"/>
<pin name="RXOUT15" direction="out"/>
<pin name="RXOUT16" direction="out"/>
<pin name="RXOUT17" direction="out"/>
<pin name="RXOUT18" direction="out"/>
<pin name="RXOUT19" direction="out"/>
<pin name="RXOUT20" direction="out"/>
<pin name="RXOUT21" direction="out"/>
<pin name="RXOUT22" direction="out"/>
<pin name="RXOUT23" direction="out"/>
<pin name="RXOUT24" direction="out"/>
<pin name="RXOUT25" direction="out"/>
<pin name="RXOUT26" direction="out"/>
<pin name="RXOUT27" direction="out"/>
<pin name="RXOUT28" direction="out"/>
<pin name="RXOUT29" direction="out"/>
<pin name="RXOUT30" direction="out"/>
<pin name="RXOUT31" direction="out"/>
<pin name="RXOUT32" direction="out"/>
<pin name="RXOUT33" direction="out"/>
<pin name="RXOUT34" direction="out"/>
<pin name="RXOUT35" direction="out"/>
<pin name="RXOUT36" direction="out"/>
<pin name="RXOUT37" direction="out"/>
<pin name="RXOUT38" direction="out"/>
<pin name="RXOUT39" direction="out"/>
<pin name="RXOUT40" direction="out"/>
<pin name="RXOUT41" direction="out"/>
<pin name="RXOUT42" direction="out"/>
<pin name="RXOUT43" direction="out"/>
<pin name="RXOUT44" direction="out"/>
<pin name="RXOUT45" direction="out"/>
<pin name="RXOUT46" direction="out"/>
<pin name="RXOUT47" direction="out"/>
<pin name="RXCLKOUT" direction="out"/>
</symbol>
<symbol name="DS90CR483AVJD">
<pin name="VCC_2" direction="pwr"/>
<pin name="VCC_3" direction="pwr"/>
<pin name="VCC_4" direction="pwr"/>
<pin name="VCC_5" direction="pwr"/>
<pin name="VCC_6" direction="pwr"/>
<pin name="VCC_7" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="PLLVCC_2" direction="pwr"/>
<pin name="PLLVCC" direction="pwr"/>
<pin name="LVDSVCC_2" direction="pwr"/>
<pin name="LVDSVCC_3" direction="pwr"/>
<pin name="LVDSVCC" direction="pwr"/>
<pin name="PRE" direction="in"/>
<pin name="~PD" direction="in"/>
<pin name="TXCLKIN" direction="in"/>
<pin name="TXCLKM" direction="in"/>
<pin name="PLLSEL" direction="in"/>
<pin name="TXCLKP" direction="in"/>
<pin name="DS_OPT" direction="in"/>
<pin name="TXIN0" direction="in"/>
<pin name="TXIN1" direction="in"/>
<pin name="TXIN2" direction="in"/>
<pin name="TXIN3" direction="in"/>
<pin name="TXIN4" direction="in"/>
<pin name="TXIN5" direction="in"/>
<pin name="TXIN6" direction="in"/>
<pin name="TXIN7" direction="in"/>
<pin name="TXIN8" direction="in"/>
<pin name="TXIN9" direction="in"/>
<pin name="TXIN10" direction="in"/>
<pin name="TXIN11" direction="in"/>
<pin name="TXIN12" direction="in"/>
<pin name="TXIN13" direction="in"/>
<pin name="TXIN14" direction="in"/>
<pin name="TXIN15" direction="in"/>
<pin name="TXIN16" direction="in"/>
<pin name="TXIN17" direction="in"/>
<pin name="TXIN18" direction="in"/>
<pin name="TXIN19" direction="in"/>
<pin name="TXIN20" direction="in"/>
<pin name="TXIN21" direction="in"/>
<pin name="TXIN22" direction="in"/>
<pin name="TXIN23" direction="in"/>
<pin name="TXIN24" direction="in"/>
<pin name="TXIN25" direction="in"/>
<pin name="TXIN26" direction="in"/>
<pin name="TXIN27" direction="in"/>
<pin name="TXIN28" direction="in"/>
<pin name="TXIN29" direction="in"/>
<pin name="TXIN30" direction="in"/>
<pin name="TXIN31" direction="in"/>
<pin name="TXIN32" direction="in"/>
<pin name="TXIN33" direction="in"/>
<pin name="TXIN34" direction="in"/>
<pin name="TXIN35" direction="in"/>
<pin name="TXIN36" direction="in"/>
<pin name="TXIN37" direction="in"/>
<pin name="TXIN38" direction="in"/>
<pin name="TXIN39" direction="in"/>
<pin name="TXIN40" direction="in"/>
<pin name="TXIN41" direction="in"/>
<pin name="TXIN42" direction="in"/>
<pin name="TXIN43" direction="in"/>
<pin name="TXIN44" direction="in"/>
<pin name="TXIN45" direction="in"/>
<pin name="TXIN46" direction="in"/>
<pin name="TXIN47" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="PLLGND_2" direction="pas"/>
<pin name="PLLGND_3" direction="pas"/>
<pin name="PLLGND" direction="pas"/>
<pin name="LVDSGND_2" direction="pas"/>
<pin name="LVDSGND_3" direction="pas"/>
<pin name="LVDSGND_4" direction="pas"/>
<pin name="LVDSGND" direction="pas"/>
<pin name="TXOUTM0" direction="out"/>
<pin name="TXOUTM1" direction="out"/>
<pin name="TXOUTM2" direction="out"/>
<pin name="TXOUTM3" direction="out"/>
<pin name="TXOUTM4" direction="out"/>
<pin name="TXOUTM5" direction="out"/>
<pin name="TXOUTM6" direction="out"/>
<pin name="TXOUTM7" direction="out"/>
<pin name="TXOUTP0" direction="out"/>
<pin name="TXOUTP1" direction="out"/>
<pin name="TXOUTP2" direction="out"/>
<pin name="TXOUTP3" direction="out"/>
<pin name="TXOUTP4" direction="out"/>
<pin name="TXOUTP5" direction="out"/>
<pin name="TXOUTP6" direction="out"/>
<pin name="TXOUTP7" direction="out"/>
<pin name="BAL" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC" direction="nc"/>
</symbol>
<symbol name="DS90CR484AVJD">
<pin name="VCC_2" direction="pwr"/>
<pin name="VCC_3" direction="pwr"/>
<pin name="VCC_4" direction="pwr"/>
<pin name="VCC_5" direction="pwr"/>
<pin name="VCC_6" direction="pwr"/>
<pin name="VCC_7" direction="pwr"/>
<pin name="VCC_8" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="PLLVCC" direction="pwr"/>
<pin name="LVDSVCC_2" direction="pwr"/>
<pin name="LVDSVCC" direction="pwr"/>
<pin name="RXCLKP" direction="in"/>
<pin name="RXCLKM" direction="in"/>
<pin name="~PD" direction="in"/>
<pin name="DESKEW" direction="in"/>
<pin name="PLLSEL" direction="in"/>
<pin name="RXINP0" direction="in"/>
<pin name="RXINM0" direction="in"/>
<pin name="RXINP1" direction="in"/>
<pin name="RXINM1" direction="in"/>
<pin name="RXINP2" direction="in"/>
<pin name="RXINM2" direction="in"/>
<pin name="RXINP3" direction="in"/>
<pin name="RXINM3" direction="in"/>
<pin name="RXINP4" direction="in"/>
<pin name="RXINM4" direction="in"/>
<pin name="RXINP5" direction="in"/>
<pin name="RXINM5" direction="in"/>
<pin name="RXINP6" direction="in"/>
<pin name="RXINM6" direction="in"/>
<pin name="RXINP7" direction="in"/>
<pin name="RXINM7" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC_6" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pwr"/>
<pin name="GND_5" direction="pwr"/>
<pin name="GND_6" direction="pwr"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="PLLGND_2" direction="pas"/>
<pin name="LVDSGND_2" direction="pas"/>
<pin name="LVDSGND_3" direction="pas"/>
<pin name="LVDSGND" direction="pas"/>
<pin name="PLLGND" direction="pas"/>
<pin name="RXCLKOUT" direction="out"/>
<pin name="RXOUT0" direction="out"/>
<pin name="RXOUT1" direction="out"/>
<pin name="RXOUT2" direction="out"/>
<pin name="RXOUT3" direction="out"/>
<pin name="RXOUT4" direction="out"/>
<pin name="RXOUT5" direction="out"/>
<pin name="RXOUT6" direction="out"/>
<pin name="RXOUT7" direction="out"/>
<pin name="RXOUT8" direction="out"/>
<pin name="RXOUT9" direction="out"/>
<pin name="RXOUT10" direction="out"/>
<pin name="RXOUT11" direction="out"/>
<pin name="RXOUT12" direction="out"/>
<pin name="RXOUT13" direction="out"/>
<pin name="RXOUT14" direction="out"/>
<pin name="RXOUT15" direction="out"/>
<pin name="RXOUT16" direction="out"/>
<pin name="RXOUT17" direction="out"/>
<pin name="RXOUT18" direction="out"/>
<pin name="RXOUT19" direction="out"/>
<pin name="RXOUT20" direction="out"/>
<pin name="RXOUT21" direction="out"/>
<pin name="RXOUT22" direction="out"/>
<pin name="RXOUT23" direction="out"/>
<pin name="RXOUT24" direction="out"/>
<pin name="RXOUT25" direction="out"/>
<pin name="RXOUT26" direction="out"/>
<pin name="RXOUT27" direction="out"/>
<pin name="RXOUT28" direction="out"/>
<pin name="RXOUT29" direction="out"/>
<pin name="RXOUT30" direction="out"/>
<pin name="RXOUT31" direction="out"/>
<pin name="RXOUT32" direction="out"/>
<pin name="RXOUT33" direction="out"/>
<pin name="RXOUT34" direction="out"/>
<pin name="RXOUT35" direction="out"/>
<pin name="RXOUT36" direction="out"/>
<pin name="RXOUT37" direction="out"/>
<pin name="RXOUT38" direction="out"/>
<pin name="RXOUT39" direction="out"/>
<pin name="RXOUT40" direction="out"/>
<pin name="RXOUT41" direction="out"/>
<pin name="RXOUT42" direction="out"/>
<pin name="RXOUT43" direction="out"/>
<pin name="RXOUT44" direction="out"/>
<pin name="RXOUT45" direction="out"/>
<pin name="RXOUT46" direction="out"/>
<pin name="RXOUT47" direction="out"/>
</symbol>
<symbol name="DS90CR485VS">
<pin name="VCC_2" direction="pwr"/>
<pin name="VCC_3" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="VCC3" direction="pwr"/>
<pin name="PLLVCC_2" direction="pwr"/>
<pin name="PLLVCC" direction="pwr"/>
<pin name="LVDSVCC_2" direction="pwr"/>
<pin name="LVDSVCC_3" direction="pwr"/>
<pin name="LVDSVCC_4" direction="pwr"/>
<pin name="LVDSVCC" direction="pwr"/>
<pin name="CLK1P" direction="in"/>
<pin name="PRE" direction="in"/>
<pin name="CLK1M" direction="in"/>
<pin name="PLLSEL" direction="in"/>
<pin name="PRBS_EN" direction="in"/>
<pin name="PAT_SEL" direction="in"/>
<pin name="CLKIN" direction="in"/>
<pin name="TSEN" direction="in"/>
<pin name="DS_OPT" direction="in"/>
<pin name="BAL" direction="in"/>
<pin name="~PD" direction="in"/>
<pin name="CON1" direction="in"/>
<pin name="CON2" direction="in"/>
<pin name="CON3" direction="in"/>
<pin name="CON4" direction="in"/>
<pin name="CON5" direction="in"/>
<pin name="CON6" direction="in"/>
<pin name="CON7" direction="in"/>
<pin name="CON8" direction="in"/>
<pin name="TEST1" direction="in"/>
<pin name="TEST2" direction="in"/>
<pin name="D0" direction="in"/>
<pin name="D1" direction="in"/>
<pin name="D2" direction="in"/>
<pin name="D3" direction="in"/>
<pin name="D4" direction="in"/>
<pin name="D5" direction="in"/>
<pin name="D6" direction="in"/>
<pin name="D7" direction="in"/>
<pin name="D8" direction="in"/>
<pin name="D9" direction="in"/>
<pin name="D10" direction="in"/>
<pin name="D11" direction="in"/>
<pin name="D12" direction="in"/>
<pin name="D13" direction="in"/>
<pin name="D14" direction="in"/>
<pin name="D15" direction="in"/>
<pin name="D16" direction="in"/>
<pin name="D17" direction="in"/>
<pin name="D18" direction="in"/>
<pin name="D19" direction="in"/>
<pin name="D20" direction="in"/>
<pin name="D21" direction="in"/>
<pin name="D22" direction="in"/>
<pin name="D23" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GND3" direction="pas"/>
<pin name="PLLGND_2" direction="pas"/>
<pin name="PLLGND_3" direction="pas"/>
<pin name="PLLGND" direction="pas"/>
<pin name="LVDSGND_2" direction="pas"/>
<pin name="LVDSGND_3" direction="pas"/>
<pin name="LVDSGND_4" direction="pas"/>
<pin name="LVDSGND_5" direction="pas"/>
<pin name="LVDSGND" direction="pas"/>
<pin name="TXOUT0P" direction="out"/>
<pin name="TXOUT0M" direction="out"/>
<pin name="TXOUT1P" direction="out"/>
<pin name="TXOUT1M" direction="out"/>
<pin name="TXOUT2P" direction="out"/>
<pin name="TXOUT2M" direction="out"/>
<pin name="TXOUT3P" direction="out"/>
<pin name="TXOUT3M" direction="out"/>
<pin name="TXOUT4P" direction="out"/>
<pin name="TXOUT4M" direction="out"/>
<pin name="TXOUT5P" direction="out"/>
<pin name="TXOUT5M" direction="out"/>
<pin name="TXOUT6P" direction="out"/>
<pin name="TXOUT6M" direction="out"/>
<pin name="TXOUT7P" direction="out"/>
<pin name="TXOUT7M" direction="out"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC_6" direction="nc"/>
<pin name="NC_7" direction="nc"/>
<pin name="NC_8" direction="nc"/>
<pin name="NC_9" direction="nc"/>
<pin name="NC_10" direction="nc"/>
<pin name="NC_11" direction="nc"/>
<pin name="NC_12" direction="nc"/>
<pin name="NC_13" direction="nc"/>
<pin name="NC_14" direction="nc"/>
<pin name="NC" direction="nc"/>
</symbol>
<symbol name="DS90CR486VS">
<pin name="VCC_2" direction="pwr"/>
<pin name="VCC_3" direction="pwr"/>
<pin name="VCC_4" direction="pwr"/>
<pin name="VCC_5" direction="pwr"/>
<pin name="VCC_6" direction="pwr"/>
<pin name="VCC_7" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="PLLVCC" direction="pwr"/>
<pin name="LVDSVCC_2" direction="pwr"/>
<pin name="LVDSVCC" direction="pwr"/>
<pin name="~PD" direction="in"/>
<pin name="DESKEW" direction="in"/>
<pin name="PLLSEL" direction="in"/>
<pin name="CON1" direction="in"/>
<pin name="RXCLKP" direction="in"/>
<pin name="RXCLKM" direction="in"/>
<pin name="RXIN0M" direction="in"/>
<pin name="RXIN0P" direction="in"/>
<pin name="RXIN1P" direction="in"/>
<pin name="RXIN1M" direction="in"/>
<pin name="RXINP2" direction="in"/>
<pin name="RXINM2" direction="in"/>
<pin name="RXINP3" direction="in"/>
<pin name="RXINM3" direction="in"/>
<pin name="RXINP4" direction="in"/>
<pin name="RXINM4" direction="in"/>
<pin name="RXINP5" direction="in"/>
<pin name="RXINM5" direction="in"/>
<pin name="RXINP6" direction="in"/>
<pin name="RXINM6" direction="in"/>
<pin name="RXINP7" direction="in"/>
<pin name="RXINM7" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC_6" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="PLLGND_2" direction="pas"/>
<pin name="PLLGND" direction="pas"/>
<pin name="LVDSGND_2" direction="pas"/>
<pin name="LVDSGND_3" direction="pas"/>
<pin name="LVDSGND" direction="pas"/>
<pin name="RXOUT0" direction="out"/>
<pin name="RXOUT1" direction="out"/>
<pin name="RXOUT2" direction="out"/>
<pin name="RXOUT3" direction="out"/>
<pin name="RXOUT4" direction="out"/>
<pin name="RXOUT5" direction="out"/>
<pin name="RXOUT6" direction="out"/>
<pin name="RXOUT7" direction="out"/>
<pin name="RXOUT8" direction="out"/>
<pin name="RXOUT9" direction="out"/>
<pin name="RXOUT10" direction="out"/>
<pin name="RXOUT11" direction="out"/>
<pin name="RXOUT12" direction="out"/>
<pin name="RXOUT13" direction="out"/>
<pin name="RXOUT14" direction="out"/>
<pin name="RXOUT15" direction="out"/>
<pin name="RXOUT16" direction="out"/>
<pin name="RXOUT17" direction="out"/>
<pin name="RXOUT18" direction="out"/>
<pin name="RXOUT19" direction="out"/>
<pin name="RXOUT20" direction="out"/>
<pin name="RXOUT21" direction="out"/>
<pin name="RXOUT22" direction="out"/>
<pin name="RXOUT23" direction="out"/>
<pin name="RXOUT24" direction="out"/>
<pin name="RXOUT25" direction="out"/>
<pin name="RXOUT26" direction="out"/>
<pin name="RXOUT27" direction="out"/>
<pin name="RXOUT28" direction="out"/>
<pin name="RXOUT29" direction="out"/>
<pin name="RXOUT30" direction="out"/>
<pin name="RXOUT31" direction="out"/>
<pin name="RXOUT32" direction="out"/>
<pin name="RXOUT33" direction="out"/>
<pin name="RXOUT34" direction="out"/>
<pin name="RXOUT35" direction="out"/>
<pin name="RXOUT36" direction="out"/>
<pin name="RXOUT37" direction="out"/>
<pin name="RXOUT38" direction="out"/>
<pin name="RXOUT39" direction="out"/>
<pin name="RXOUT40" direction="out"/>
<pin name="RXOUT41" direction="out"/>
<pin name="RXOUT42" direction="out"/>
<pin name="RXOUT43" direction="out"/>
<pin name="RXOUT44" direction="out"/>
<pin name="RXOUT45" direction="out"/>
<pin name="RXOUT46" direction="out"/>
<pin name="RXOUT47" direction="out"/>
<pin name="RXCLKOUT" direction="out"/>
</symbol>
<symbol name="DS90LT012AHMF">
<pin name="VDD" direction="pwr"/>
<pin name="IN+" direction="in"/>
<pin name="IN-" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="TTLOUT" direction="out"/>
</symbol>
<symbol name="DS90LT012AQMF">
<pin name="VDD" direction="pwr"/>
<pin name="IN+" direction="in"/>
<pin name="IN-" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="TTLOUT" direction="out"/>
</symbol>
<symbol name="DS90LT012ATMF">
<pin name="VDD" direction="pwr"/>
<pin name="IN+" direction="in"/>
<pin name="IN-" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="TTL_OUT" direction="out"/>
</symbol>
<symbol name="DS90LV001TLD">
<pin name="VCC" direction="pwr"/>
<pin name="EN" direction="in"/>
<pin name="IN-" direction="in"/>
<pin name="IN+" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="EP" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="OUT+" direction="out"/>
<pin name="OUT-" direction="out"/>
</symbol>
<symbol name="DS90LV001TM">
<pin name="VCC" direction="pwr"/>
<pin name="EN" direction="in"/>
<pin name="IN_-" direction="in"/>
<pin name="IN+" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="OUT+" direction="out"/>
<pin name="OUT-" direction="out"/>
</symbol>
<symbol name="DS90LV004TVS">
<pin name="VDD_2" direction="pwr"/>
<pin name="VDD_3" direction="pwr"/>
<pin name="VDD_4" direction="pwr"/>
<pin name="VDD_5" direction="pwr"/>
<pin name="VDD_6" direction="pwr"/>
<pin name="VDD_7" direction="pwr"/>
<pin name="VDD_8" direction="pwr"/>
<pin name="VDD_9" direction="pwr"/>
<pin name="VDD_10" direction="pwr"/>
<pin name="VDD_11" direction="pwr"/>
<pin name="VDD_12" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="~PWDN" direction="pwr"/>
<pin name="PEM0" direction="in"/>
<pin name="PEM1" direction="in"/>
<pin name="IN0+" direction="in"/>
<pin name="IN0-" direction="in"/>
<pin name="IN1+" direction="in"/>
<pin name="IN1-" direction="in"/>
<pin name="IN2+" direction="in"/>
<pin name="IN2-" direction="in"/>
<pin name="IN3+" direction="in"/>
<pin name="IN3-" direction="in"/>
<pin name="N/C_2" direction="nc"/>
<pin name="N/C_3" direction="nc"/>
<pin name="N/C_4" direction="nc"/>
<pin name="N/C_5" direction="nc"/>
<pin name="N/C" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND_11" direction="pas"/>
<pin name="GND_12" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="OUT0-" direction="out"/>
<pin name="OUT0+" direction="out"/>
<pin name="OUT1-" direction="out"/>
<pin name="OUT1+" direction="out"/>
<pin name="OUT2+" direction="out"/>
<pin name="OUT2-" direction="out"/>
<pin name="OUT3-" direction="out"/>
<pin name="OUT3+" direction="out"/>
</symbol>
<symbol name="DS90LV011AHMF">
<pin name="VDD" direction="pwr"/>
<pin name="TTL_IN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT-" direction="out"/>
<pin name="OUT+" direction="out"/>
</symbol>
<symbol name="DS90LV011AQMF">
<pin name="VDD" direction="pwr"/>
<pin name="TTL_IN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT-" direction="out"/>
<pin name="OUT+" direction="out"/>
</symbol>
<symbol name="DS90LV011ATMF">
<pin name="VDD" direction="pwr"/>
<pin name="TTL_IN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT-" direction="out"/>
<pin name="OUT+" direction="out"/>
</symbol>
<symbol name="DS90LV012ATMF">
<pin name="VDD" direction="pwr"/>
<pin name="IN+" direction="in"/>
<pin name="IN-" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="TTLOUT" direction="out"/>
</symbol>
<symbol name="DS90LV017ATM">
<pin name="VCC" direction="pwr"/>
<pin name="DI1" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="DO1+" direction="out"/>
<pin name="DO1-" direction="out"/>
</symbol>
<symbol name="DS90LV018ATM">
<pin name="VCC" direction="pwr"/>
<pin name="RIN1+" direction="in"/>
<pin name="RIN1-" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="ROUT1" direction="out"/>
</symbol>
<symbol name="DS90LV019TM">
<pin name="VCC" direction="pwr"/>
<pin name="DE" direction="in"/>
<pin name="~RE" direction="in"/>
<pin name="DIN" direction="in"/>
<pin name="RI-" direction="in"/>
<pin name="RI+" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="ROUT" direction="out"/>
<pin name="DO-" direction="out"/>
<pin name="DO+" direction="out"/>
</symbol>
<symbol name="DS90LV019TMTC">
<pin name="VCC" direction="pwr"/>
<pin name="DE" direction="in"/>
<pin name="~RE" direction="in"/>
<pin name="DIN" direction="in"/>
<pin name="RI-" direction="in"/>
<pin name="RI+" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="ROUT" direction="out"/>
<pin name="DO-" direction="out"/>
<pin name="DO+" direction="out"/>
</symbol>
<symbol name="DS90LV027AQMA">
<pin name="VCC" direction="pwr"/>
<pin name="DI1" direction="in"/>
<pin name="DI2" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="DO+1" direction="out"/>
<pin name="DO-1" direction="out"/>
<pin name="DO+2" direction="out"/>
<pin name="DO-2" direction="out"/>
</symbol>
<symbol name="DS90LV027ATM">
<pin name="VCC" direction="pwr"/>
<pin name="DI1" direction="in"/>
<pin name="DI2" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="DO+1" direction="out"/>
<pin name="DO-1" direction="out"/>
<pin name="DO-2" direction="out"/>
<pin name="DO+2" direction="out"/>
</symbol>
<symbol name="DS90LV028AHM">
<pin name="VCC" direction="pwr"/>
<pin name="RIN1-" direction="in"/>
<pin name="RIN1+" direction="in"/>
<pin name="RIN2+" direction="in"/>
<pin name="RIN2-" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="ROUT1" direction="out"/>
<pin name="ROUT2" direction="out"/>
</symbol>
<symbol name="DS90LV028AQMA">
<pin name="VCC" direction="pwr"/>
<pin name="RIN1-" direction="in"/>
<pin name="RIN1+" direction="in"/>
<pin name="RIN2+" direction="in"/>
<pin name="RIN2-" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="ROUT1" direction="out"/>
<pin name="ROUT2" direction="out"/>
</symbol>
<symbol name="DS90LV028ATM">
<pin name="VCC" direction="pwr"/>
<pin name="RIN1-" direction="in"/>
<pin name="RIN1+" direction="in"/>
<pin name="RIN2+" direction="in"/>
<pin name="RIN2-" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="ROUT1" direction="out"/>
<pin name="ROUT2" direction="out"/>
</symbol>
<symbol name="DS90LV031ATM">
<pin name="VCC" direction="pwr"/>
<pin name="EN" direction="in"/>
<pin name="~EN" direction="in"/>
<pin name="DIN1" direction="in"/>
<pin name="DIN2" direction="in"/>
<pin name="DIN3" direction="in"/>
<pin name="DIN4" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="DOUT1+" direction="out"/>
<pin name="DOUT1-" direction="out"/>
<pin name="DOUT2-" direction="out"/>
<pin name="DOUT2+" direction="out"/>
<pin name="DOUT3+" direction="out"/>
<pin name="DOUT3-" direction="out"/>
<pin name="DOUT4-" direction="out"/>
<pin name="DOUT4+" direction="out"/>
</symbol>
<symbol name="DS90LV031ATMTC">
<pin name="VCC" direction="pwr"/>
<pin name="EN" direction="in"/>
<pin name="~EN" direction="in"/>
<pin name="DIN1" direction="in"/>
<pin name="DIN2" direction="in"/>
<pin name="DIN3" direction="in"/>
<pin name="DIN4" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="DOUT1+" direction="out"/>
<pin name="DOUT1-" direction="out"/>
<pin name="DOUT2-" direction="out"/>
<pin name="DOUT2+" direction="out"/>
<pin name="DOUT3+" direction="out"/>
<pin name="DOUT3-" direction="out"/>
<pin name="DOUT4-" direction="out"/>
<pin name="DOUT4+" direction="out"/>
</symbol>
<symbol name="DS90LV032ATM">
<pin name="VCC" direction="pwr"/>
<pin name="EN" direction="in"/>
<pin name="~EN" direction="in"/>
<pin name="RIN1-" direction="in"/>
<pin name="RIN1+" direction="in"/>
<pin name="RIN2+" direction="in"/>
<pin name="RIN2-" direction="in"/>
<pin name="RIN3-" direction="in"/>
<pin name="RIN3+" direction="in"/>
<pin name="RIN4+" direction="in"/>
<pin name="RIN4-" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="ROUT1" direction="out"/>
<pin name="ROUT2" direction="out"/>
<pin name="ROUT3" direction="out"/>
<pin name="ROUT4" direction="out"/>
</symbol>
<symbol name="DS90LV032ATMTC">
<pin name="VCC" direction="pwr"/>
<pin name="EN" direction="in"/>
<pin name="~EN" direction="in"/>
<pin name="RIN1-" direction="in"/>
<pin name="RIN1+" direction="in"/>
<pin name="RIN2+" direction="in"/>
<pin name="RIN2-" direction="in"/>
<pin name="RIN3-" direction="in"/>
<pin name="RIN3+" direction="in"/>
<pin name="RIN4+" direction="in"/>
<pin name="RIN4-" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="ROUT1" direction="out"/>
<pin name="ROUT2" direction="out"/>
<pin name="ROUT3" direction="out"/>
<pin name="ROUT4" direction="out"/>
</symbol>
<symbol name="DS90LV047ATM">
<pin name="VCC" direction="pwr"/>
<pin name="EN" direction="in"/>
<pin name="~EN" direction="in"/>
<pin name="DIN1" direction="in"/>
<pin name="DIN2" direction="in"/>
<pin name="DIN3" direction="in"/>
<pin name="DIN4" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="DOUT1+" direction="out"/>
<pin name="DOUT1-" direction="out"/>
<pin name="DOUT2-" direction="out"/>
<pin name="DOUT2+" direction="out"/>
<pin name="DOUT3+" direction="out"/>
<pin name="DOUT3-" direction="out"/>
<pin name="DOUT4-" direction="out"/>
<pin name="DOUT4+" direction="out"/>
</symbol>
<symbol name="DS90LV047ATMTC">
<pin name="VCC" direction="pwr"/>
<pin name="EN" direction="in"/>
<pin name="*EN" direction="in"/>
<pin name="DIN1" direction="in"/>
<pin name="DIN2" direction="in"/>
<pin name="DIN3" direction="in"/>
<pin name="DIN4" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="DOUT4-" direction="out"/>
<pin name="DOUT4+" direction="out"/>
<pin name="DOUT3+" direction="out"/>
<pin name="DOUT3-" direction="out"/>
<pin name="DOUT2-" direction="out"/>
<pin name="DOUT2+" direction="out"/>
<pin name="DOUT1+" direction="out"/>
<pin name="DOUT1-" direction="out"/>
</symbol>
<symbol name="DS90LV048ATM">
<pin name="VCC" direction="pwr"/>
<pin name="~EN" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="RIN1-" direction="in"/>
<pin name="RIN1+" direction="in"/>
<pin name="RIN2+" direction="in"/>
<pin name="RIN2-" direction="in"/>
<pin name="RIN3-" direction="in"/>
<pin name="RIN3+" direction="in"/>
<pin name="RIN4+" direction="in"/>
<pin name="RIN4-" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="ROUT1" direction="out"/>
<pin name="ROUT2" direction="out"/>
<pin name="ROUT3" direction="out"/>
<pin name="ROUT4" direction="out"/>
</symbol>
<symbol name="DS90LV048ATMTC">
<pin name="VCC" direction="pwr"/>
<pin name="RIN1-" direction="in"/>
<pin name="RIN1+" direction="in"/>
<pin name="RIN2+" direction="in"/>
<pin name="RIN2-" direction="in"/>
<pin name="RIN3-" direction="in"/>
<pin name="RIN3+" direction="in"/>
<pin name="RIN4+" direction="in"/>
<pin name="RIN4-" direction="in"/>
<pin name="~EN" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="ROUT1" direction="out"/>
<pin name="ROUT2" direction="out"/>
<pin name="ROUT3" direction="out"/>
<pin name="ROUT4" direction="out"/>
</symbol>
<symbol name="DS90LV049HMT">
<pin name="RIN1-" direction="in"/>
<pin name="RIN1+" direction="in"/>
<pin name="RIN2+" direction="in"/>
<pin name="RIN2-" direction="in"/>
<pin name="DIN1" direction="in"/>
<pin name="DIN2" direction="in"/>
<pin name="EN" direction="pas"/>
<pin name="~EN" direction="pas"/>
<pin name="VDD" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="DOUT2-" direction="out"/>
<pin name="DOUT2+" direction="out"/>
<pin name="DOUT1+" direction="out"/>
<pin name="DOUT1-" direction="out"/>
<pin name="ROUT2" direction="out"/>
<pin name="ROUT1" direction="out"/>
</symbol>
<symbol name="DS90LV049QMT">
<pin name="RIN1-" direction="in"/>
<pin name="RIN1+" direction="in"/>
<pin name="RIN2+" direction="in"/>
<pin name="RIN2-" direction="in"/>
<pin name="DIN1" direction="in"/>
<pin name="DIN2" direction="in"/>
<pin name="EN" direction="pas"/>
<pin name="~EN" direction="pas"/>
<pin name="VDD" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="DOUT2-" direction="out"/>
<pin name="DOUT2+" direction="out"/>
<pin name="DOUT1+" direction="out"/>
<pin name="DOUT1-" direction="out"/>
<pin name="ROUT2" direction="out"/>
<pin name="ROUT1" direction="out"/>
</symbol>
<symbol name="DS90LV049TMT">
<pin name="VDD" direction="pwr"/>
<pin name="~EN" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="RIN1-" direction="in"/>
<pin name="RIN1+" direction="in"/>
<pin name="RIN2-" direction="in"/>
<pin name="RIN2+" direction="in"/>
<pin name="DIN1" direction="in"/>
<pin name="DIN2" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="ROUT1" direction="out"/>
<pin name="ROUT2" direction="out"/>
<pin name="DOUT1+" direction="out"/>
<pin name="DOUT1-" direction="out"/>
<pin name="DOUT2+" direction="out"/>
<pin name="DOUT2-" direction="out"/>
</symbol>
<symbol name="DS90LV110ATMT">
<pin name="VDD_2" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="EN" direction="in"/>
<pin name="IN+" direction="in"/>
<pin name="IN-" direction="in"/>
<pin name="VSS_2" direction="pwr"/>
<pin name="VSS_3" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="OUT1+" direction="out"/>
<pin name="OUT1-" direction="out"/>
<pin name="OUT2+" direction="out"/>
<pin name="OUT2-" direction="out"/>
<pin name="OUT3-" direction="out"/>
<pin name="OUT3+" direction="out"/>
<pin name="OUT4-" direction="out"/>
<pin name="OUT4+" direction="out"/>
<pin name="OUT5-" direction="out"/>
<pin name="OUT5+" direction="out"/>
<pin name="OUT6-" direction="out"/>
<pin name="OUT6+" direction="out"/>
<pin name="OUT7-" direction="out"/>
<pin name="OUT7+" direction="out"/>
<pin name="OUT8-" direction="out"/>
<pin name="OUT8+" direction="out"/>
<pin name="OUT9+" direction="out"/>
<pin name="OUT9-" direction="out"/>
<pin name="OUT10+" direction="out"/>
<pin name="OUT10-" direction="out"/>
</symbol>
<symbol name="DS90LV110TMTC">
<pin name="VDD_2" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="EN" direction="in"/>
<pin name="IN+" direction="in"/>
<pin name="IN-" direction="in"/>
<pin name="VSS_2" direction="pwr"/>
<pin name="VSS_3" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="OUT1+" direction="out"/>
<pin name="OUT1-" direction="out"/>
<pin name="OUT2+" direction="out"/>
<pin name="OUT2-" direction="out"/>
<pin name="OUT3-" direction="out"/>
<pin name="OUT3+" direction="out"/>
<pin name="OUT4-" direction="out"/>
<pin name="OUT4+" direction="out"/>
<pin name="OUT5-" direction="out"/>
<pin name="OUT5+" direction="out"/>
<pin name="OUT6-" direction="out"/>
<pin name="OUT6+" direction="out"/>
<pin name="OUT7-" direction="out"/>
<pin name="OUT7+" direction="out"/>
<pin name="OUT8-" direction="out"/>
<pin name="OUT8+" direction="out"/>
<pin name="OUT9+" direction="out"/>
<pin name="OUT9-" direction="out"/>
<pin name="OUT10+" direction="out"/>
<pin name="OUT10-" direction="out"/>
</symbol>
<symbol name="DS90LV804TSQ">
<pin name="VDD_2" direction="pwr"/>
<pin name="VDD_3" direction="pwr"/>
<pin name="VDD_4" direction="pwr"/>
<pin name="VDD_5" direction="pwr"/>
<pin name="VDD_6" direction="pwr"/>
<pin name="VDD_7" direction="pwr"/>
<pin name="VDD_8" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="EN" direction="in"/>
<pin name="IN0+" direction="in"/>
<pin name="IN0-" direction="in"/>
<pin name="IN1+" direction="in"/>
<pin name="IN1-" direction="in"/>
<pin name="IN2+" direction="in"/>
<pin name="IN2-" direction="in"/>
<pin name="IN3+" direction="in"/>
<pin name="IN3-" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="EPAD" direction="pas"/>
<pin name="OUT0-" direction="out"/>
<pin name="OUT0+" direction="out"/>
<pin name="OUT1-" direction="out"/>
<pin name="OUT1+" direction="out"/>
<pin name="OUT2-" direction="out"/>
<pin name="OUT2+" direction="out"/>
<pin name="OUT3-" direction="out"/>
<pin name="OUT3+" direction="out"/>
</symbol>
<symbol name="DS90UR124QVS">
<pin name="VDD_2" direction="pwr"/>
<pin name="VDD_3" direction="pwr"/>
<pin name="VDD_4" direction="pwr"/>
<pin name="VDD_5" direction="pwr"/>
<pin name="VDD_6" direction="pwr"/>
<pin name="VDD_7" direction="pwr"/>
<pin name="VDD_8" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="RIN+" direction="in"/>
<pin name="RIN-" direction="in"/>
<pin name="REN" direction="in"/>
<pin name="RRFB" direction="in"/>
<pin name="RAOFF" direction="in"/>
<pin name="SLEW" direction="in"/>
<pin name="BISTM" direction="in"/>
<pin name="PTOSEL" direction="in"/>
<pin name="BISTEN" direction="in"/>
<pin name="RPWDNB" direction="in"/>
<pin name="RES0_2" direction="in"/>
<pin name="RES0_3" direction="in"/>
<pin name="RES0_4" direction="in"/>
<pin name="RES0_5" direction="in"/>
<pin name="RES0_6" direction="in"/>
<pin name="RES0_7" direction="in"/>
<pin name="RES0_8" direction="in"/>
<pin name="RES0_9" direction="in"/>
<pin name="RES0_10" direction="in"/>
<pin name="RES0_11" direction="in"/>
<pin name="RES0" direction="in"/>
<pin name="VSS_2" direction="pwr"/>
<pin name="VSS_3" direction="pwr"/>
<pin name="VSS_4" direction="pwr"/>
<pin name="VSS_5" direction="pwr"/>
<pin name="VSS_6" direction="pwr"/>
<pin name="VSS_7" direction="pwr"/>
<pin name="VSS_8" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="ROUT0" direction="out"/>
<pin name="ROUT1" direction="out"/>
<pin name="ROUT2" direction="out"/>
<pin name="ROUT3" direction="out"/>
<pin name="ROUT4" direction="out"/>
<pin name="ROUT5" direction="out"/>
<pin name="ROUT6" direction="out"/>
<pin name="ROUT7" direction="out"/>
<pin name="ROUT8" direction="out"/>
<pin name="ROUT9" direction="out"/>
<pin name="ROUT10" direction="out"/>
<pin name="ROUT11" direction="out"/>
<pin name="ROUT12" direction="out"/>
<pin name="ROUT13" direction="out"/>
<pin name="ROUT14" direction="out"/>
<pin name="ROUT15" direction="out"/>
<pin name="ROUT16" direction="out"/>
<pin name="ROUT17" direction="out"/>
<pin name="ROUT18" direction="out"/>
<pin name="ROUT19" direction="out"/>
<pin name="ROUT20" direction="out"/>
<pin name="ROUT21" direction="out"/>
<pin name="ROUT22" direction="out"/>
<pin name="ROUT23" direction="out"/>
<pin name="RCLK" direction="out"/>
<pin name="LOCK" direction="out"/>
<pin name="PASS" direction="out"/>
</symbol>
<symbol name="DS90UR241QVS">
<pin name="VDD_2" direction="pwr"/>
<pin name="VDD_3" direction="pwr"/>
<pin name="VDD_4" direction="pwr"/>
<pin name="VDD_5" direction="pwr"/>
<pin name="VDD_6" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="DEN" direction="in"/>
<pin name="PRE" direction="in"/>
<pin name="TRFB" direction="in"/>
<pin name="RES0_2" direction="in"/>
<pin name="RES0_3" direction="in"/>
<pin name="RES0" direction="in"/>
<pin name="TCLK" direction="in"/>
<pin name="TPWDNB" direction="in"/>
<pin name="VODSEL" direction="in"/>
<pin name="RAOFF" direction="in"/>
<pin name="DIN0" direction="in"/>
<pin name="DIN1" direction="in"/>
<pin name="DIN2" direction="in"/>
<pin name="DIN3" direction="in"/>
<pin name="DIN4" direction="in"/>
<pin name="DIN5" direction="in"/>
<pin name="DIN6" direction="in"/>
<pin name="DIN7" direction="in"/>
<pin name="DIN8" direction="in"/>
<pin name="DIN9" direction="in"/>
<pin name="DIN10" direction="in"/>
<pin name="DIN11" direction="in"/>
<pin name="DIN12" direction="in"/>
<pin name="DIN13" direction="in"/>
<pin name="DIN14" direction="in"/>
<pin name="DIN15" direction="in"/>
<pin name="DIN16" direction="in"/>
<pin name="DIN17" direction="in"/>
<pin name="DIN18" direction="in"/>
<pin name="DIN19" direction="in"/>
<pin name="DIN20" direction="in"/>
<pin name="DIN21" direction="in"/>
<pin name="DIN22" direction="in"/>
<pin name="DIN23" direction="in"/>
<pin name="VSS_2" direction="pwr"/>
<pin name="VSS_3" direction="pwr"/>
<pin name="VSS_4" direction="pwr"/>
<pin name="VSS_5" direction="pwr"/>
<pin name="VSS_6" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="DOUT+" direction="out"/>
<pin name="DOUT-" direction="out"/>
</symbol>
<symbol name="DS91C176TMA">
<pin name="VCC" direction="pwr"/>
<pin name="DE" direction="in"/>
<pin name="~RE" direction="in"/>
<pin name="R" direction="out"/>
<pin name="D" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="A"/>
<pin name="B"/>
</symbol>
<symbol name="DS91C180TMA">
<pin name="VCC_2" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="~RE" direction="in"/>
<pin name="DE" direction="in"/>
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="D" direction="in"/>
<pin name="NC_2" direction="pas"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="R" direction="out"/>
<pin name="Y" direction="out"/>
<pin name="Z" direction="out"/>
</symbol>
<symbol name="DS91D176TMA">
<pin name="VCC" direction="pwr"/>
<pin name="~RE" direction="in"/>
<pin name="DE" direction="in"/>
<pin name="D" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="R" direction="out"/>
<pin name="A"/>
<pin name="B"/>
</symbol>
<symbol name="DS91D180TMA">
<pin name="VCC_2" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="~RE" direction="in"/>
<pin name="DE" direction="in"/>
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="D" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="R" direction="out"/>
<pin name="Y" direction="out"/>
<pin name="Z" direction="out"/>
</symbol>
<symbol name="DS91M040TSQ">
<pin name="VDD_2" direction="pwr"/>
<pin name="VDD_3" direction="pwr"/>
<pin name="VDD_4" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="FSEN1" direction="in"/>
<pin name="FSEN2" direction="in"/>
<pin name="MDE" direction="in"/>
<pin name="DE0" direction="in"/>
<pin name="DE1" direction="in"/>
<pin name="DE2" direction="in"/>
<pin name="DE3" direction="in"/>
<pin name="DI0" direction="in"/>
<pin name="DI1" direction="in"/>
<pin name="DI2" direction="in"/>
<pin name="DI3" direction="in"/>
<pin name="~RE0" direction="in"/>
<pin name="~RE1" direction="in"/>
<pin name="~RE2" direction="in"/>
<pin name="~RE3" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="A0"/>
<pin name="A1"/>
<pin name="A2"/>
<pin name="A3"/>
<pin name="B0"/>
<pin name="B1"/>
<pin name="B2"/>
<pin name="B3"/>
<pin name="RO0" direction="out"/>
<pin name="RO1" direction="out"/>
<pin name="RO2" direction="out"/>
<pin name="RO3" direction="out"/>
</symbol>
<symbol name="DS91M047TMA">
<pin name="VDD" direction="pwr"/>
<pin name="~DE" direction="in"/>
<pin name="DE" direction="in"/>
<pin name="DI0" direction="in"/>
<pin name="DI1" direction="in"/>
<pin name="DI2" direction="in"/>
<pin name="DI3" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="A0"/>
<pin name="A1"/>
<pin name="A2"/>
<pin name="A3"/>
<pin name="B0"/>
<pin name="B1"/>
<pin name="B2"/>
<pin name="B3"/>
</symbol>
<symbol name="DS91M124TMA">
<pin name="VDD" direction="pwr"/>
<pin name="DEO" direction="in"/>
<pin name="DE1" direction="in"/>
<pin name="DE2" direction="in"/>
<pin name="DE3" direction="in"/>
<pin name="DI" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="A0" direction="out"/>
<pin name="A1" direction="out"/>
<pin name="A2" direction="out"/>
<pin name="A3" direction="out"/>
<pin name="B0" direction="out"/>
<pin name="B1" direction="out"/>
<pin name="B2" direction="out"/>
<pin name="B3" direction="out"/>
</symbol>
<symbol name="DS91M125TMA">
<pin name="VDD" direction="pwr"/>
<pin name="DEO" direction="in"/>
<pin name="DE1" direction="in"/>
<pin name="DE2" direction="in"/>
<pin name="DE3" direction="in"/>
<pin name="DI+" direction="in"/>
<pin name="DI-" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="A0" direction="out"/>
<pin name="A1" direction="out"/>
<pin name="A2" direction="out"/>
<pin name="A3" direction="out"/>
<pin name="B0" direction="out"/>
<pin name="B1" direction="out"/>
<pin name="B2" direction="out"/>
<pin name="B3" direction="out"/>
</symbol>
<symbol name="DS92001TMA">
<pin name="VCC" direction="pwr"/>
<pin name="EN" direction="in"/>
<pin name="IN_" direction="in"/>
<pin name="IN+" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="OUT+" direction="out"/>
<pin name="OUT-" direction="out"/>
</symbol>
<symbol name="DS92CK16TMTC">
<pin name="VCC_2" direction="pwr"/>
<pin name="VCC_3" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="VCCA" direction="pwr"/>
<pin name="~OE" direction="in"/>
<pin name="~DE" direction="in"/>
<pin name="CRDCLKIN" direction="in"/>
<pin name="CLKI/O+" direction="in"/>
<pin name="CLKI/O-" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDA_2" direction="pas"/>
<pin name="GNDA" direction="pas"/>
<pin name="CLKOUT5" direction="out"/>
<pin name="CLKOUT4" direction="out"/>
<pin name="CLKOUT3" direction="out"/>
<pin name="CLKOUT2" direction="out"/>
<pin name="CLKOUT1" direction="out"/>
<pin name="CLKOUT0" direction="out"/>
</symbol>
<symbol name="DS92LV010ATM">
<pin name="VCC" direction="pwr"/>
<pin name="DE" direction="in"/>
<pin name="DIN" direction="in"/>
<pin name="~RE" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="DO-/RI-"/>
<pin name="DO+/RI+"/>
<pin name="ROUT" direction="out"/>
</symbol>
<symbol name="DS92LV040ATLQA">
<pin name="VCC_2" direction="pwr"/>
<pin name="VCC_3" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="AVCC_2" direction="pwr"/>
<pin name="AVCC_3" direction="pwr"/>
<pin name="AVCC_4" direction="pwr"/>
<pin name="AVCC" direction="pwr"/>
<pin name="DE12" direction="in"/>
<pin name="DE34" direction="in"/>
<pin name="~RE12" direction="in"/>
<pin name="~RE34" direction="in"/>
<pin name="DO1-/RIN1-"/>
<pin name="DO1+/RIN1+"/>
<pin name="DO2-/RIN2-"/>
<pin name="DO2+/RIN2+"/>
<pin name="DO3-/RIN3-"/>
<pin name="DO3+/RIN3+"/>
<pin name="DO4-/RIN4-"/>
<pin name="DO4+/RIN4+"/>
<pin name="DIN1" direction="in"/>
<pin name="DIN2" direction="in"/>
<pin name="DIN3" direction="in"/>
<pin name="DIN4" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC_6" direction="nc"/>
<pin name="NC_7" direction="nc"/>
<pin name="NC_8" direction="nc"/>
<pin name="NC_9" direction="nc"/>
<pin name="NC_10" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="EP" direction="pas"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="AGND_2" direction="pas"/>
<pin name="AGND_3" direction="pas"/>
<pin name="AGND" direction="pwr"/>
<pin name="RO1" direction="out"/>
<pin name="RO2" direction="out"/>
<pin name="RO3" direction="out"/>
<pin name="RO4" direction="out"/>
</symbol>
<symbol name="DS92LV090ATVEH">
<pin name="VCC_2" direction="pwr"/>
<pin name="VCC_3" direction="pwr"/>
<pin name="VCC_4" direction="pwr"/>
<pin name="VCC_5" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="AVCC_2" direction="pwr"/>
<pin name="AVCC_3" direction="pwr"/>
<pin name="AVCC_4" direction="pwr"/>
<pin name="AVCC_5" direction="pwr"/>
<pin name="AVCC" direction="pwr"/>
<pin name="DIN0" direction="in"/>
<pin name="DIN1" direction="in"/>
<pin name="DIN2" direction="in"/>
<pin name="DIN3" direction="in"/>
<pin name="DIN4" direction="in"/>
<pin name="DIN5" direction="in"/>
<pin name="DIN6" direction="in"/>
<pin name="DIN7" direction="in"/>
<pin name="DIN8" direction="in"/>
<pin name="DE" direction="in"/>
<pin name="~RE" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="AGND_2" direction="pas"/>
<pin name="AGND_3" direction="pas"/>
<pin name="AGND_4" direction="pas"/>
<pin name="AGND_5" direction="pas"/>
<pin name="AGND" direction="pas"/>
<pin name="DO0-/RO0-"/>
<pin name="DO0+/RO0+"/>
<pin name="DO1-/RIN1-"/>
<pin name="DO1+/RIN1+"/>
<pin name="DO2-/RIN2-"/>
<pin name="DO2+/RIN2+"/>
<pin name="DO3-/RIN3-"/>
<pin name="DO3+/RIN3+"/>
<pin name="DO4-/RIN4-"/>
<pin name="DO4+/RIN4+"/>
<pin name="DO5-/RIN5-"/>
<pin name="DO5+/RIN5+"/>
<pin name="DO6-/RIN6-"/>
<pin name="DO6+/RIN6+"/>
<pin name="DO7-/RIN7-"/>
<pin name="DO7+/RIN7+"/>
<pin name="DO8+/RO8+"/>
<pin name="DO8-/RIN8-"/>
<pin name="RO0" direction="out"/>
<pin name="RO1" direction="out"/>
<pin name="RO2" direction="out"/>
<pin name="RO3" direction="out"/>
<pin name="RO4" direction="out"/>
<pin name="RO5" direction="out"/>
<pin name="RO6" direction="out"/>
<pin name="RO7" direction="out"/>
<pin name="RO8" direction="out"/>
</symbol>
<symbol name="DS92LV1021AMSA">
<pin name="AVCC_2" direction="pwr"/>
<pin name="AVCC" direction="pwr"/>
<pin name="DVCC_2" direction="pwr"/>
<pin name="DVCC" direction="pwr"/>
<pin name="SYNC1" direction="in"/>
<pin name="SYNC2" direction="in"/>
<pin name="DEN" direction="in"/>
<pin name="TCLK" direction="in"/>
<pin name="~PWRDN" direction="in"/>
<pin name="TCLK_R~/~F" direction="in"/>
<pin name="DIN0" direction="in"/>
<pin name="DIN1" direction="in"/>
<pin name="DIN2" direction="in"/>
<pin name="DIN3" direction="in"/>
<pin name="DIN4" direction="in"/>
<pin name="DIN5" direction="in"/>
<pin name="DIN6" direction="in"/>
<pin name="DIN7" direction="in"/>
<pin name="DIN8" direction="in"/>
<pin name="DIN9" direction="in"/>
<pin name="AGND_2" direction="pas"/>
<pin name="AGND_3" direction="pas"/>
<pin name="AGND_4" direction="pas"/>
<pin name="AGND" direction="pas"/>
<pin name="DGND_2" direction="pas"/>
<pin name="DGND" direction="pas"/>
<pin name="D0-" direction="out"/>
<pin name="DO+" direction="out"/>
</symbol>
<symbol name="DS92LV1023EMQ">
<pin name="AVCC_2" direction="pwr"/>
<pin name="AVCC" direction="pwr"/>
<pin name="DVCC_2" direction="pwr"/>
<pin name="DVCC" direction="pwr"/>
<pin name="DIN0" direction="in"/>
<pin name="DIN1" direction="in"/>
<pin name="DIN2" direction="in"/>
<pin name="DIN3" direction="in"/>
<pin name="DIN4" direction="in"/>
<pin name="DIN5" direction="in"/>
<pin name="DIN6" direction="in"/>
<pin name="DIN7" direction="in"/>
<pin name="DIN8" direction="in"/>
<pin name="DIN9" direction="in"/>
<pin name="SYNC1" direction="in"/>
<pin name="SYNC2" direction="in"/>
<pin name="TCLK" direction="in"/>
<pin name="TCLK_R~/~F" direction="in"/>
<pin name="DEN" direction="in"/>
<pin name="~PWRDN" direction="in"/>
<pin name="AGND_2" direction="pas"/>
<pin name="AGND_3" direction="pas"/>
<pin name="AGND_4" direction="pas"/>
<pin name="AGND" direction="pas"/>
<pin name="DGND_2" direction="pas"/>
<pin name="DGND" direction="pas"/>
<pin name="D0-" direction="out"/>
<pin name="DO+" direction="out"/>
</symbol>
<symbol name="DS92LV1212AMSA">
<pin name="AVCC_2" direction="pwr"/>
<pin name="AVCC" direction="pwr"/>
<pin name="DVCC_2" direction="pwr"/>
<pin name="DVCC" direction="pwr"/>
<pin name="RCLK" direction="in"/>
<pin name="RCLK_R~/~F" direction="in"/>
<pin name="REFCLK" direction="in"/>
<pin name="~PWRDN" direction="in"/>
<pin name="REN" direction="in"/>
<pin name="RI+" direction="in"/>
<pin name="RI-" direction="in"/>
<pin name="AGND_2" direction="pas"/>
<pin name="AGND_3" direction="pas"/>
<pin name="AGND" direction="pas"/>
<pin name="DGND_2" direction="pas"/>
<pin name="DGND_3" direction="pas"/>
<pin name="DGND" direction="pas"/>
<pin name="~LOCK" direction="out"/>
<pin name="ROUT0" direction="out"/>
<pin name="ROUT1" direction="out"/>
<pin name="ROUT2" direction="out"/>
<pin name="ROUT3" direction="out"/>
<pin name="ROUT4" direction="out"/>
<pin name="ROUT5" direction="out"/>
<pin name="ROUT6" direction="out"/>
<pin name="ROUT7" direction="out"/>
<pin name="ROUT8" direction="out"/>
<pin name="ROUT9" direction="out"/>
</symbol>
<symbol name="DS92LV1224TMSA">
<pin name="AVCC_2" direction="pwr"/>
<pin name="AVCC" direction="pwr"/>
<pin name="DVCC_2" direction="pwr"/>
<pin name="DVCC" direction="pwr"/>
<pin name="RCLK_R/~F" direction="in"/>
<pin name="RCLK" direction="in"/>
<pin name="REFCLK" direction="in"/>
<pin name="REN" direction="in"/>
<pin name="~LOCK" direction="in"/>
<pin name="RI+" direction="in"/>
<pin name="RI-" direction="in"/>
<pin name="~PWRDN" direction="in"/>
<pin name="DGND_2" direction="pas"/>
<pin name="DGND_3" direction="pas"/>
<pin name="DGND" direction="pas"/>
<pin name="AGND_2" direction="pas"/>
<pin name="AGND_3" direction="pas"/>
<pin name="AGND" direction="pas"/>
<pin name="ROUT9" direction="out"/>
<pin name="ROUT8" direction="out"/>
<pin name="ROUT7" direction="out"/>
<pin name="ROUT6" direction="out"/>
<pin name="ROUT5" direction="out"/>
<pin name="ROUT4" direction="out"/>
<pin name="ROUT3" direction="out"/>
<pin name="ROUT2" direction="out"/>
<pin name="ROUT1" direction="out"/>
<pin name="ROUT0" direction="out"/>
</symbol>
<symbol name="DS92LV16TVHG">
<pin name="AVDD_2" direction="pwr"/>
<pin name="AVDD_3" direction="pwr"/>
<pin name="AVDD_4" direction="pwr"/>
<pin name="AVDD" direction="pwr"/>
<pin name="PVDD_2" direction="pwr"/>
<pin name="PVDD_3" direction="pwr"/>
<pin name="DVDD_2" direction="pwr"/>
<pin name="DVDD_3" direction="pwr"/>
<pin name="DVDD_4" direction="pwr"/>
<pin name="DVDD_5" direction="pwr"/>
<pin name="DVDD_6" direction="pwr"/>
<pin name="DVDD" direction="pwr"/>
<pin name="PVDD_4" direction="pwr"/>
<pin name="TCLK" direction="in"/>
<pin name="RCLK" direction="in"/>
<pin name="REFCLK" direction="in"/>
<pin name="RIN+" direction="in"/>
<pin name="RIN-" direction="in"/>
<pin name="REN" direction="in"/>
<pin name="~RPWDN" direction="in"/>
<pin name="~TPWDN" direction="in"/>
<pin name="CONFIG1" direction="pas"/>
<pin name="CONFIG2" direction="pas"/>
<pin name="DEN" direction="in"/>
<pin name="SYNC" direction="in"/>
<pin name="DIN0" direction="in"/>
<pin name="DIN1" direction="in"/>
<pin name="DIN2" direction="in"/>
<pin name="DIN3" direction="in"/>
<pin name="DIN4" direction="in"/>
<pin name="DIN5" direction="in"/>
<pin name="DIN6" direction="in"/>
<pin name="DIN7" direction="in"/>
<pin name="DIN8" direction="in"/>
<pin name="DIN9" direction="in"/>
<pin name="DIN10" direction="in"/>
<pin name="DIN11" direction="in"/>
<pin name="DIN12" direction="in"/>
<pin name="DIN13" direction="in"/>
<pin name="DIN14" direction="in"/>
<pin name="DIN15" direction="in"/>
<pin name="AGND_2" direction="pas"/>
<pin name="AGND_3" direction="pas"/>
<pin name="AGND_4" direction="pas"/>
<pin name="AGND" direction="pas"/>
<pin name="PGND_2" direction="pas"/>
<pin name="PGND_3" direction="pas"/>
<pin name="DGND_2" direction="pas"/>
<pin name="DGND_3" direction="pas"/>
<pin name="DGND_4" direction="pas"/>
<pin name="DGND_5" direction="pas"/>
<pin name="DGND_6" direction="pas"/>
<pin name="DGND_7" direction="pas"/>
<pin name="PGND_4" direction="pas"/>
<pin name="DGND_8" direction="pas"/>
<pin name="DGND_9" direction="pas"/>
<pin name="DGND" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="DO+" direction="out"/>
<pin name="DO-" direction="out"/>
<pin name="ROUT0" direction="out"/>
<pin name="ROUT1" direction="out"/>
<pin name="ROUT2" direction="out"/>
<pin name="ROUT3" direction="out"/>
<pin name="ROUT4" direction="out"/>
<pin name="ROUT5" direction="out"/>
<pin name="ROUT6" direction="out"/>
<pin name="ROUT7" direction="out"/>
<pin name="~LOCK" direction="out"/>
<pin name="ROUT8" direction="out"/>
<pin name="ROUT9" direction="out"/>
<pin name="ROUT10" direction="out"/>
<pin name="ROUT11" direction="out"/>
<pin name="ROUT12" direction="out"/>
<pin name="ROUT13" direction="out"/>
<pin name="ROUT14" direction="out"/>
<pin name="ROUT15" direction="out"/>
<pin name="PVDD" direction="pwr"/>
<pin name="LINE_LE" direction="in"/>
<pin name="LOCAL_LE" direction="in"/>
</symbol>
<symbol name="DS92LV18TVV">
<pin name="AVDD_2" direction="pwr"/>
<pin name="AVDD_3" direction="pwr"/>
<pin name="AVDD_4" direction="pwr"/>
<pin name="AVDD" direction="pwr"/>
<pin name="DVDD_2" direction="pwr"/>
<pin name="DVDD_3" direction="pwr"/>
<pin name="DVDD_4" direction="pwr"/>
<pin name="DVDD_5" direction="pwr"/>
<pin name="DVDD" direction="pwr"/>
<pin name="PVDD_2" direction="pwr"/>
<pin name="PVDD_3" direction="pwr"/>
<pin name="PVDD_4" direction="pwr"/>
<pin name="PVDD" direction="pwr"/>
<pin name="TCLK" direction="in"/>
<pin name="~RPWDN" direction="in"/>
<pin name="REN" direction="in"/>
<pin name="REFCLKK" direction="in"/>
<pin name="DEN" direction="in"/>
<pin name="~TPWDN" direction="in"/>
<pin name="SYNC" direction="in"/>
<pin name="RCLK" direction="in"/>
<pin name="LOCAL_LE" direction="in"/>
<pin name="LINE_LE" direction="in"/>
<pin name="RIN+" direction="in"/>
<pin name="RIN-" direction="in"/>
<pin name="DIN0" direction="in"/>
<pin name="DIN1" direction="in"/>
<pin name="DIN2" direction="in"/>
<pin name="DIN3" direction="in"/>
<pin name="DIN4" direction="in"/>
<pin name="DIN5" direction="in"/>
<pin name="DIN6" direction="in"/>
<pin name="DIN7" direction="in"/>
<pin name="DIN8" direction="in"/>
<pin name="DIN9" direction="in"/>
<pin name="DIN10" direction="in"/>
<pin name="DIN11" direction="in"/>
<pin name="DIN12" direction="in"/>
<pin name="DIN13" direction="in"/>
<pin name="DIN14" direction="in"/>
<pin name="DIN16" direction="in"/>
<pin name="DIN15" direction="in"/>
<pin name="DIN17" direction="in"/>
<pin name="DGND_2" direction="pas"/>
<pin name="DGND_3" direction="pas"/>
<pin name="DGND_4" direction="pas"/>
<pin name="DGND_5" direction="pas"/>
<pin name="DGND_6" direction="pas"/>
<pin name="DGND_7" direction="pas"/>
<pin name="DGND_8" direction="pas"/>
<pin name="DGND" direction="pas"/>
<pin name="AGND_2" direction="pas"/>
<pin name="AGND_3" direction="pas"/>
<pin name="AGND_4" direction="pas"/>
<pin name="AGND" direction="pas"/>
<pin name="PGND_2" direction="pas"/>
<pin name="PGND_3" direction="pas"/>
<pin name="PGND_4" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="ROUT0" direction="out"/>
<pin name="ROUT1" direction="out"/>
<pin name="ROUT2" direction="out"/>
<pin name="ROUT3" direction="out"/>
<pin name="ROUT4" direction="out"/>
<pin name="ROUT5" direction="out"/>
<pin name="ROUT6" direction="out"/>
<pin name="ROUT7" direction="out"/>
<pin name="ROUT8" direction="out"/>
<pin name="ROUT9" direction="out"/>
<pin name="ROUT10" direction="out"/>
<pin name="ROUT11" direction="out"/>
<pin name="ROUT12" direction="out"/>
<pin name="ROUT13" direction="out"/>
<pin name="ROUT14" direction="out"/>
<pin name="ROUT15" direction="out"/>
<pin name="ROUT16" direction="out"/>
<pin name="ROUT17" direction="out"/>
<pin name="~LOCK" direction="out"/>
<pin name="DO+" direction="out"/>
<pin name="DO-" direction="out"/>
</symbol>
<symbol name="DS92LV3222TVS">
<pin name="VDD_2" direction="pwr"/>
<pin name="VDD_3" direction="pwr"/>
<pin name="VDD_4" direction="pwr"/>
<pin name="VDD_5" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="VDDA" direction="pwr"/>
<pin name="VDDPLL_2" direction="pwr"/>
<pin name="VDDPLL_3" direction="pwr"/>
<pin name="VDDPLL" direction="pwr"/>
<pin name="RXIN0+" direction="in"/>
<pin name="RXIN0-" direction="in"/>
<pin name="RXIN1+" direction="in"/>
<pin name="RXIN1-" direction="in"/>
<pin name="PDB" direction="in"/>
<pin name="R_FB" direction="in"/>
<pin name="REN" direction="in"/>
<pin name="RSVD" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="VSS_2" direction="pwr"/>
<pin name="VSS_3" direction="pwr"/>
<pin name="VSS_4" direction="pwr"/>
<pin name="VSS_5" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="VSSA" direction="pwr"/>
<pin name="VSSPLL_2" direction="pwr"/>
<pin name="VSSPLL_3" direction="pwr"/>
<pin name="VSSPLL" direction="pwr"/>
<pin name="LOCK" direction="out"/>
<pin name="RXCLKOUT" direction="out"/>
<pin name="RXOUT0" direction="out"/>
<pin name="RXOUT1" direction="out"/>
<pin name="RXOUT16" direction="out"/>
<pin name="RXOUT17" direction="out"/>
<pin name="RXOUT18" direction="out"/>
<pin name="RXOUT19" direction="out"/>
<pin name="RXOUT20" direction="out"/>
<pin name="RXOUT21" direction="out"/>
<pin name="RXOUT22" direction="out"/>
<pin name="RXOUT23" direction="out"/>
<pin name="RXOUT24" direction="out"/>
<pin name="RXOUT25" direction="out"/>
<pin name="RXOUT26" direction="out"/>
<pin name="RXOUT27" direction="out"/>
<pin name="RXOUT28" direction="out"/>
<pin name="RXOUT29" direction="out"/>
<pin name="RXOUT30" direction="out"/>
<pin name="RXOUT31" direction="out"/>
<pin name="RXOUT2" direction="out"/>
<pin name="RXOUT3" direction="out"/>
<pin name="RXOUT4" direction="out"/>
<pin name="RXOUT5" direction="out"/>
<pin name="RXOUT6" direction="out"/>
<pin name="RXOUT7" direction="out"/>
<pin name="RXOUT8" direction="out"/>
<pin name="RXOUT9" direction="out"/>
<pin name="RXOUT10" direction="out"/>
<pin name="RXOUT11" direction="out"/>
<pin name="RXOUT12" direction="out"/>
<pin name="RXOUT13" direction="out"/>
<pin name="RXOUT14" direction="out"/>
<pin name="RXOUT15" direction="out"/>
</symbol>
<symbol name="DS92LV3241TVS">
<pin name="VDD_2" direction="pwr"/>
<pin name="VDD_3" direction="pwr"/>
<pin name="VDD_4" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="VDDA" direction="pwr"/>
<pin name="VDDPLL_2" direction="pwr"/>
<pin name="VDDPLL" direction="pwr"/>
<pin name="IOVDD" direction="pwr"/>
<pin name="MODE" direction="in"/>
<pin name="PDB" direction="in"/>
<pin name="PRE" direction="in"/>
<pin name="R_FB" direction="in"/>
<pin name="BISTEN" direction="in"/>
<pin name="RSVD" direction="in"/>
<pin name="TXCLKIN" direction="in"/>
<pin name="VSEL" direction="in"/>
<pin name="TXIN0" direction="in"/>
<pin name="TXIN1" direction="in"/>
<pin name="TXIN2" direction="in"/>
<pin name="TXIN3" direction="in"/>
<pin name="TXIN4" direction="in"/>
<pin name="TXIN5" direction="in"/>
<pin name="TXIN6" direction="in"/>
<pin name="TXIN7" direction="in"/>
<pin name="TXIN8" direction="in"/>
<pin name="TXIN9" direction="in"/>
<pin name="TXIN10" direction="in"/>
<pin name="TXIN11" direction="in"/>
<pin name="TXIN12" direction="in"/>
<pin name="TXIN13" direction="in"/>
<pin name="TXIN14" direction="in"/>
<pin name="TXIN15" direction="in"/>
<pin name="TXIN16" direction="in"/>
<pin name="TXIN17" direction="in"/>
<pin name="TXIN18" direction="in"/>
<pin name="TXIN19" direction="in"/>
<pin name="TXIN20" direction="in"/>
<pin name="TXIN21" direction="in"/>
<pin name="TXIN22" direction="in"/>
<pin name="TXIN23" direction="in"/>
<pin name="TXIN24" direction="in"/>
<pin name="TXIN25" direction="in"/>
<pin name="TXIN26" direction="in"/>
<pin name="TXIN27" direction="in"/>
<pin name="TXIN28" direction="in"/>
<pin name="TXIN29" direction="in"/>
<pin name="TXIN30" direction="in"/>
<pin name="TXIN31" direction="in"/>
<pin name="IOVSS" direction="pwr"/>
<pin name="VSS_2" direction="pwr"/>
<pin name="VSS_3" direction="pwr"/>
<pin name="VSS_4" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="VSSA" direction="pwr"/>
<pin name="VSSPLL_2" direction="pwr"/>
<pin name="VSSPLL" direction="pwr"/>
<pin name="TXOUT0+" direction="out"/>
<pin name="TXOUT1+" direction="out"/>
<pin name="TXOUT2+" direction="out"/>
<pin name="TXOUT3+" direction="out"/>
<pin name="TXOUT0-" direction="out"/>
<pin name="TXOUT1-" direction="out"/>
<pin name="TXOUT2-" direction="out"/>
<pin name="TXOUT3-" direction="out"/>
</symbol>
<symbol name="DS92LV3242TVS">
<pin name="VDD_2" direction="pwr"/>
<pin name="VDD_3" direction="pwr"/>
<pin name="VDD_4" direction="pwr"/>
<pin name="VDD_5" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="VDDA" direction="pwr"/>
<pin name="VDDPLL_2" direction="pwr"/>
<pin name="VDDPLL_3" direction="pwr"/>
<pin name="VDDPLL" direction="pwr"/>
<pin name="PDB" direction="in"/>
<pin name="R_FB" direction="in"/>
<pin name="REN" direction="in"/>
<pin name="RSVD" direction="in"/>
<pin name="RXIN0+" direction="in"/>
<pin name="RXIN1+" direction="in"/>
<pin name="RXIN2+" direction="in"/>
<pin name="RXIN3+" direction="in"/>
<pin name="RXIN0-" direction="in"/>
<pin name="RXIN1-" direction="in"/>
<pin name="RXIN2-" direction="in"/>
<pin name="RXIN3-" direction="in"/>
<pin name="VSS_2" direction="pwr"/>
<pin name="VSS_3" direction="pwr"/>
<pin name="VSS_4" direction="pwr"/>
<pin name="VSS_5" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="VSSA" direction="pwr"/>
<pin name="VSSPLL_2" direction="pwr"/>
<pin name="VSSPLL_3" direction="pwr"/>
<pin name="VSSPLL" direction="pwr"/>
<pin name="LOCK" direction="out"/>
<pin name="RXCLKOUT" direction="out"/>
<pin name="RXOUT0" direction="out"/>
<pin name="RXOUT1" direction="out"/>
<pin name="RXOUT2" direction="out"/>
<pin name="RXOUT3" direction="out"/>
<pin name="RXOUT4" direction="out"/>
<pin name="RXOUT5" direction="out"/>
<pin name="RXOUT6" direction="out"/>
<pin name="RXOUT7" direction="out"/>
<pin name="RXOUT8" direction="out"/>
<pin name="RXOUT9" direction="out"/>
<pin name="RXOUT10" direction="out"/>
<pin name="RXOUT11" direction="out"/>
<pin name="RXOUT12" direction="out"/>
<pin name="RXOUT13" direction="out"/>
<pin name="RXOUT14" direction="out"/>
<pin name="RXOUT15" direction="out"/>
<pin name="RXOUT16" direction="out"/>
<pin name="RXOUT17" direction="out"/>
<pin name="RXOUT18" direction="out"/>
<pin name="RXOUT19" direction="out"/>
<pin name="RXOUT20" direction="out"/>
<pin name="RXOUT21" direction="out"/>
<pin name="RXOUT22" direction="out"/>
<pin name="RXOUT23" direction="out"/>
<pin name="RXOUT24" direction="out"/>
<pin name="RXOUT25" direction="out"/>
<pin name="RXOUT26" direction="out"/>
<pin name="RXOUT27" direction="out"/>
<pin name="RXOUT28" direction="out"/>
<pin name="RXOUT29" direction="out"/>
<pin name="RXOUT30" direction="out"/>
<pin name="RXOUT31" direction="out"/>
</symbol>
<symbol name="DS92LV8028TUF_A">
<pin name="AVDD_2" direction="pwr"/>
<pin name="AVDD_3" direction="pwr"/>
<pin name="AVDD_4" direction="pwr"/>
<pin name="AVDD_5" direction="pwr"/>
<pin name="AVDD_6" direction="pwr"/>
<pin name="AVDD_7" direction="pwr"/>
<pin name="AVDD_8" direction="pwr"/>
<pin name="AVDD_9" direction="pwr"/>
<pin name="AVDD" direction="pwr"/>
<pin name="DVDD_2" direction="pwr"/>
<pin name="DVDD_3" direction="pwr"/>
<pin name="DVDD_4" direction="pwr"/>
<pin name="DVDD_5" direction="pwr"/>
<pin name="DVDD_6" direction="pwr"/>
<pin name="DVDD_7" direction="pwr"/>
<pin name="DVDD_8" direction="pwr"/>
<pin name="DVDD_9" direction="pwr"/>
<pin name="DVDD_10" direction="pwr"/>
<pin name="DVDD_11" direction="pwr"/>
<pin name="DVDD_12" direction="pwr"/>
<pin name="DVDD_13" direction="pwr"/>
<pin name="DVDD_14" direction="pwr"/>
<pin name="DVDD" direction="pwr"/>
<pin name="PVDD_2" direction="pwr"/>
<pin name="PVDD" direction="pwr"/>
<pin name="BIST_SEL_2" direction="in"/>
<pin name="BIST_SEL_3" direction="in"/>
<pin name="BIST_SEL_4" direction="in"/>
<pin name="BIST_ACT" direction="in"/>
<pin name="BIST_SEL" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="TMS" direction="in"/>
<pin name="TRSTN" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="TCLK" direction="in"/>
<pin name="DIN0&lt;0&gt;" direction="in"/>
<pin name="DIN0&lt;1&gt;" direction="in"/>
<pin name="DIN0&lt;2&gt;" direction="in"/>
<pin name="DIN0&lt;3&gt;" direction="in"/>
<pin name="DIN0&lt;4&gt;" direction="in"/>
<pin name="DIN6&lt;7&gt;" direction="in"/>
<pin name="DIN7&lt;1&gt;" direction="in"/>
<pin name="DIN7&lt;2&gt;" direction="in"/>
<pin name="DIN7&lt;3&gt;" direction="in"/>
<pin name="DIN7&lt;4&gt;" direction="in"/>
<pin name="DIN7&lt;5&gt;" direction="in"/>
<pin name="DIN7&lt;6&gt;" direction="in"/>
<pin name="DIN7&lt;7&gt;" direction="in"/>
<pin name="DIN7&lt;8&gt;" direction="in"/>
<pin name="DIN7&lt;9&gt;" direction="in"/>
<pin name="NC1" direction="nc"/>
<pin name="NC11" direction="nc"/>
<pin name="NC12" direction="nc"/>
<pin name="PGND_2" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="DGND_2" direction="pas"/>
<pin name="DGND_3" direction="pas"/>
<pin name="DGND_4" direction="pas"/>
<pin name="DGND_5" direction="pas"/>
<pin name="DGND_6" direction="pas"/>
<pin name="DGND_7" direction="pas"/>
<pin name="DGND_8" direction="pas"/>
<pin name="DGND_9" direction="pas"/>
<pin name="DGND_10" direction="pas"/>
<pin name="DGND_11" direction="pas"/>
<pin name="DGND_12" direction="pas"/>
<pin name="DGND_13" direction="pas"/>
<pin name="DGND_14" direction="pas"/>
<pin name="DGND_15" direction="pas"/>
<pin name="DGND_16" direction="pas"/>
<pin name="DGND_17" direction="pas"/>
<pin name="DGND" direction="pas"/>
<pin name="AGND_2" direction="pas"/>
<pin name="AGND_3" direction="pas"/>
<pin name="AGND_4" direction="pas"/>
<pin name="AGND_5" direction="pas"/>
<pin name="AGND_6" direction="pas"/>
<pin name="AGND_7" direction="pas"/>
<pin name="AGND_8" direction="pas"/>
<pin name="AGND_9" direction="pas"/>
<pin name="AGND" direction="pas"/>
<pin name="TDO" direction="out"/>
<pin name="DOUT0+" direction="out"/>
<pin name="DOUT1+" direction="out"/>
<pin name="DOUT2+" direction="out"/>
<pin name="DOUT3+" direction="out"/>
<pin name="DOUT4+" direction="out"/>
<pin name="DOUT5-" direction="out"/>
<pin name="DOUT6-" direction="out"/>
<pin name="DOUT7-" direction="out"/>
<pin name="DOUT0-" direction="out"/>
<pin name="DOUT1-" direction="out"/>
<pin name="DOUT2-" direction="out"/>
<pin name="DOUT3-" direction="out"/>
<pin name="DOUT4-" direction="out"/>
<pin name="DOUT5+" direction="out"/>
<pin name="DOUT6+" direction="out"/>
<pin name="DOUT7+" direction="out"/>
</symbol>
<symbol name="DS92LV8028TUF_B">
<pin name="DVDD" direction="pwr"/>
<pin name="DIN0&lt;5&gt;" direction="in"/>
<pin name="DIN0&lt;6&gt;" direction="in"/>
<pin name="DIN0&lt;7&gt;" direction="in"/>
<pin name="DIN0&lt;8&gt;" direction="in"/>
<pin name="DIN0&lt;9&gt;" direction="in"/>
<pin name="DIN1&lt;0&gt;" direction="in"/>
<pin name="DIN1&lt;1&gt;" direction="in"/>
<pin name="DIN1&lt;2&gt;" direction="in"/>
<pin name="DIN1&lt;3&gt;" direction="in"/>
<pin name="DIN1&lt;4&gt;" direction="in"/>
<pin name="DIN1&lt;5&gt;" direction="in"/>
<pin name="DIN1&lt;6&gt;" direction="in"/>
<pin name="DIN1&lt;7&gt;" direction="in"/>
<pin name="DIN1&lt;8&gt;" direction="in"/>
<pin name="DIN1&lt;9&gt;" direction="in"/>
<pin name="DIN2&lt;0&gt;" direction="in"/>
<pin name="DIN2&lt;1&gt;" direction="in"/>
<pin name="DIN2&lt;2&gt;" direction="in"/>
<pin name="DIN2&lt;3&gt;" direction="in"/>
<pin name="DIN2&lt;4&gt;" direction="in"/>
<pin name="DIN2&lt;5&gt;" direction="in"/>
<pin name="DIN2&lt;6&gt;" direction="in"/>
<pin name="DIN2&lt;7&gt;" direction="in"/>
<pin name="DIN2&lt;8&gt;" direction="in"/>
<pin name="DIN2&lt;9&gt;" direction="in"/>
<pin name="DIN3&lt;0&gt;" direction="in"/>
<pin name="DIN3&lt;2&gt;" direction="in"/>
<pin name="DIN3&lt;1&gt;" direction="in"/>
<pin name="DIN3&lt;3&gt;" direction="in"/>
<pin name="DIN3&lt;4&gt;" direction="in"/>
<pin name="DIN3&lt;5&gt;" direction="in"/>
<pin name="DIN3&lt;6&gt;" direction="in"/>
<pin name="DIN3&lt;7&gt;" direction="in"/>
<pin name="DIN3&lt;8&gt;" direction="in"/>
<pin name="DIN3&lt;9&gt;" direction="in"/>
<pin name="DIN4&lt;0&gt;" direction="in"/>
<pin name="DIN4&lt;1&gt;" direction="in"/>
<pin name="DIN4&lt;2&gt;" direction="in"/>
<pin name="DIN4&lt;3&gt;" direction="in"/>
<pin name="DIN4&lt;4&gt;" direction="in"/>
<pin name="DIN4&lt;5&gt;" direction="in"/>
<pin name="DIN4&lt;6&gt;" direction="in"/>
<pin name="DIN4&lt;7&gt;" direction="in"/>
<pin name="DIN4&lt;8&gt;" direction="in"/>
<pin name="DIN4&lt;9&gt;" direction="in"/>
<pin name="DIN5&lt;0&gt;" direction="in"/>
<pin name="DIN5&lt;1&gt;" direction="in"/>
<pin name="DIN5&lt;2&gt;" direction="in"/>
<pin name="DIN5&lt;3&gt;" direction="in"/>
<pin name="DIN5&lt;4&gt;" direction="in"/>
<pin name="DIN5&lt;5&gt;" direction="in"/>
<pin name="DIN5&lt;6&gt;" direction="in"/>
<pin name="DIN5&lt;7&gt;" direction="in"/>
<pin name="DIN5&lt;8&gt;" direction="in"/>
<pin name="DIN5&lt;9&gt;" direction="in"/>
<pin name="DIN6&lt;0&gt;" direction="in"/>
<pin name="DIN6&lt;1&gt;" direction="in"/>
<pin name="DIN6&lt;2&gt;" direction="in"/>
<pin name="DIN6&lt;3&gt;" direction="in"/>
<pin name="DIN6&lt;4&gt;" direction="in"/>
<pin name="DIN6&lt;5&gt;" direction="in"/>
<pin name="DIN6&lt;6&gt;" direction="in"/>
<pin name="DIN6&lt;8&gt;" direction="in"/>
<pin name="DIN6&lt;9&gt;" direction="in"/>
<pin name="DIN7&lt;0&gt;" direction="in"/>
<pin name="DEN" direction="in"/>
<pin name="~MS_PWDN" direction="in"/>
<pin name="SYNC&lt;0&gt;" direction="in"/>
<pin name="SYNC&lt;1&gt;" direction="in"/>
<pin name="SYNC&lt;2&gt;" direction="in"/>
<pin name="SYNC&lt;3&gt;" direction="in"/>
<pin name="SYNC&lt;4&gt;" direction="in"/>
<pin name="SYNC&lt;5&gt;" direction="in"/>
<pin name="SYNC&lt;6&gt;" direction="in"/>
<pin name="SYNC&lt;7&gt;" direction="in"/>
<pin name="~PWDN&lt;0&gt;" direction="in"/>
<pin name="~PWDN&lt;1&gt;" direction="in"/>
<pin name="~PWDN&lt;2&gt;" direction="in"/>
<pin name="~PWDN&lt;3&gt;" direction="in"/>
<pin name="~PWDN&lt;4&gt;" direction="in"/>
<pin name="~PWDN&lt;5&gt;" direction="in"/>
<pin name="~PWDN&lt;6&gt;" direction="in"/>
<pin name="~PWDN&lt;7&gt;" direction="in"/>
<pin name="DGND_2" direction="pas"/>
<pin name="DGND_3" direction="pas"/>
<pin name="DGND_4" direction="pas"/>
<pin name="DGND_5" direction="pas"/>
<pin name="DGND" direction="pas"/>
<pin name="NC2" direction="nc"/>
<pin name="NC3" direction="nc"/>
<pin name="NC4" direction="nc"/>
<pin name="NC5" direction="nc"/>
<pin name="NC7" direction="nc"/>
<pin name="NC6" direction="nc"/>
<pin name="NC8" direction="nc"/>
<pin name="NC9" direction="nc"/>
<pin name="NC10" direction="nc"/>
</symbol>
<symbol name="DS96174CN">
<pin name="VCC" direction="pwr"/>
<pin name="E1,2" direction="in"/>
<pin name="E3,4" direction="in"/>
<pin name="1A" direction="in"/>
<pin name="2A" direction="in"/>
<pin name="3A" direction="in"/>
<pin name="4A" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="1Y" direction="out"/>
<pin name="1Z" direction="out"/>
<pin name="2Y" direction="out"/>
<pin name="2Z" direction="out"/>
<pin name="3Y" direction="out"/>
<pin name="3Z" direction="out"/>
<pin name="4Y" direction="out"/>
<pin name="4Z" direction="out"/>
</symbol>
<symbol name="DS96175CN">
<pin name="VCC" direction="pwr"/>
<pin name="E1,2" direction="in"/>
<pin name="E3,4" direction="in"/>
<pin name="1A" direction="in"/>
<pin name="2A" direction="in"/>
<pin name="1B" direction="in"/>
<pin name="2B" direction="in"/>
<pin name="3A" direction="in"/>
<pin name="3B" direction="in"/>
<pin name="4A" direction="in"/>
<pin name="4B" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="1Y" direction="out"/>
<pin name="2Y" direction="out"/>
<pin name="3Y" direction="out"/>
<pin name="4Y" direction="out"/>
</symbol>
<symbol name="DS96176CN">
<pin name="VCC" direction="pwr"/>
<pin name="~RE" direction="in"/>
<pin name="DE" direction="in"/>
<pin name="DI" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="RO" direction="out"/>
<pin name="A"/>
<pin name="B"/>
</symbol>
<symbol name="DS9637ACM">
<pin name="VCC" direction="pwr"/>
<pin name="-INA" direction="in"/>
<pin name="+INA" direction="in"/>
<pin name="-INB" direction="in"/>
<pin name="+INB" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="DS9638CM">
<pin name="VCC" direction="pwr"/>
<pin name="INA" direction="in"/>
<pin name="INB" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUTA" direction="out"/>
<pin name="OUT~A" direction="out"/>
<pin name="OUTB" direction="out"/>
<pin name="OUT~B" direction="out"/>
</symbol>
<symbol name="DS99R421QSQ">
<pin name="VDDD" direction="pwr"/>
<pin name="VDDP1" direction="pwr"/>
<pin name="VDDP0" direction="pwr"/>
<pin name="VDDDR" direction="pwr"/>
<pin name="VDDSER" direction="pwr"/>
<pin name="VDDDES" direction="pwr"/>
<pin name="VDDIN" direction="pwr"/>
<pin name="OS0" direction="in"/>
<pin name="OS1" direction="in"/>
<pin name="OS2" direction="in"/>
<pin name="RXIN0-" direction="in"/>
<pin name="RXIN0+" direction="in"/>
<pin name="RXIN1-" direction="in"/>
<pin name="RXIN1+" direction="in"/>
<pin name="RXIN2-" direction="in"/>
<pin name="RXIN2+" direction="in"/>
<pin name="RESRVD_2" direction="in"/>
<pin name="RESRVD_3" direction="in"/>
<pin name="RESRVD_4" direction="in"/>
<pin name="RESRVD" direction="in"/>
<pin name="RXCLKIN-" direction="in"/>
<pin name="RXCLKIN+" direction="in"/>
<pin name="PRE" direction="in"/>
<pin name="DEN" direction="in"/>
<pin name="PWDNB" direction="in"/>
<pin name="BISTEN" direction="in"/>
<pin name="VODSEL" direction="in"/>
<pin name="VSSD" direction="pwr"/>
<pin name="VSSP0" direction="pwr"/>
<pin name="VSSP1" direction="pwr"/>
<pin name="VSSDR" direction="pwr"/>
<pin name="VSSDES" direction="pwr"/>
<pin name="VSSIN" direction="pwr"/>
<pin name="VSSSER" direction="pwr"/>
<pin name="DOUT+" direction="out"/>
<pin name="DOUT-" direction="out"/>
</symbol>
<symbol name="LF147J">
<pin name="V+" direction="pwr"/>
<pin name="-IN1-" direction="in"/>
<pin name="+IN1" direction="in"/>
<pin name="+IN2" direction="in"/>
<pin name="-IN2" direction="in"/>
<pin name="-IN3" direction="in"/>
<pin name="+IN3" direction="in"/>
<pin name="+IN4" direction="in"/>
<pin name="-IN4" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT1" direction="out"/>
<pin name="OUT2" direction="out"/>
<pin name="OUT3" direction="out"/>
<pin name="OUT4" direction="out"/>
</symbol>
<symbol name="LF156H">
<pin name="+IN" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
<pin name="NC" direction="pas"/>
<pin name="BALANCE_2" direction="pas"/>
<pin name="BALANCE" direction="pas"/>
<pin name="OUTPUT" direction="out"/>
</symbol>
<symbol name="LF347BN">
<pin name="V+" direction="pwr"/>
<pin name="-IN1" direction="in"/>
<pin name="+IN1" direction="in"/>
<pin name="+IN2" direction="in"/>
<pin name="-IN2" direction="in"/>
<pin name="-IN3" direction="in"/>
<pin name="+IN3" direction="in"/>
<pin name="+IN4" direction="in"/>
<pin name="-IN4" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT1" direction="out"/>
<pin name="OUT2" direction="out"/>
<pin name="OUT3" direction="out"/>
<pin name="OUT4" direction="out"/>
</symbol>
<symbol name="LF347M">
<pin name="V+" direction="pwr"/>
<pin name="-IN1" direction="in"/>
<pin name="+IN1" direction="in"/>
<pin name="+IN2" direction="in"/>
<pin name="-IN2" direction="in"/>
<pin name="-IN3" direction="in"/>
<pin name="+IN3" direction="in"/>
<pin name="+IN4" direction="in"/>
<pin name="-IN4" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT1" direction="out"/>
<pin name="OUT2" direction="out"/>
<pin name="OUT3" direction="out"/>
<pin name="OUT4" direction="out"/>
</symbol>
<symbol name="LF347N">
<pin name="V+" direction="pwr"/>
<pin name="IN1-" direction="in"/>
<pin name="IN1+" direction="in"/>
<pin name="IN2+" direction="in"/>
<pin name="IN2-" direction="in"/>
<pin name="IN3-" direction="in"/>
<pin name="IN3+" direction="in"/>
<pin name="IN4+" direction="in"/>
<pin name="IN4-" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT1" direction="out"/>
<pin name="OUT2" direction="out"/>
<pin name="OUT3" direction="out"/>
<pin name="OUT4" direction="out"/>
</symbol>
<symbol name="LF353M">
<pin name="V+" direction="pwr"/>
<pin name="POSA" direction="in"/>
<pin name="NEGA" direction="in"/>
<pin name="POSB" direction="in"/>
<pin name="NEGB" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="LF353N">
<pin name="V+" direction="pwr"/>
<pin name="NEGA" direction="in"/>
<pin name="POSA" direction="in"/>
<pin name="POSB" direction="in"/>
<pin name="NEGB" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="LF356H">
<pin name="-INA" direction="in"/>
<pin name="+INA" direction="in"/>
<pin name="BALANCE_2" direction="in"/>
<pin name="BALANCE" direction="in"/>
<pin name="V+" direction="in"/>
<pin name="V-" direction="pas"/>
<pin name="NC" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LF356M">
<pin name="V+" direction="pwr"/>
<pin name="-IN" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="BAL_2" direction="in"/>
<pin name="BAL" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LF356N">
<pin name="V+" direction="pas"/>
<pin name="IN_2" direction="in"/>
<pin name="IN" direction="in"/>
<pin name="OFS_2" direction="pas"/>
<pin name="OFS" direction="pas"/>
<pin name="NC" direction="nc"/>
<pin name="V-" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LF411ACN">
<pin name="V+" direction="pwr"/>
<pin name="+IN" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="BALANCE_2" direction="pas"/>
<pin name="BALANCE" direction="pas"/>
<pin name="N/C" direction="nc"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LF411CN">
<pin name="V+" direction="pwr"/>
<pin name="+IN" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="BALANCE_2" direction="pas"/>
<pin name="BALANCE" direction="pas"/>
<pin name="N/C" direction="nc"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LF412ACN">
<pin name="V+" direction="pwr"/>
<pin name="POSA" direction="in"/>
<pin name="POSB" direction="in"/>
<pin name="NEGA" direction="in"/>
<pin name="NEGB" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="LF412CN">
<pin name="V+" direction="pwr"/>
<pin name="POS_A" direction="in"/>
<pin name="NEG_A" direction="in"/>
<pin name="POS_B" direction="in"/>
<pin name="NEG_B" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT_A" direction="out"/>
<pin name="OUT_B" direction="out"/>
</symbol>
<symbol name="LF412MH">
<pin name="-INA" direction="in"/>
<pin name="+INA" direction="in"/>
<pin name="-INB" direction="in"/>
<pin name="+INB" direction="in"/>
<pin name="V+" direction="pas"/>
<pin name="V-" direction="pas"/>
<pin name="OUTB" direction="out"/>
<pin name="OUTA" direction="out"/>
</symbol>
<symbol name="LF442ACN">
<pin name="V+" direction="pwr"/>
<pin name="POSA" direction="in"/>
<pin name="POSB" direction="in"/>
<pin name="NEGA" direction="in"/>
<pin name="NEGB" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="LF442AMH">
<pin name="-INA" direction="in"/>
<pin name="+INA" direction="in"/>
<pin name="-INB" direction="in"/>
<pin name="+INB" direction="in"/>
<pin name="V+" direction="pas"/>
<pin name="V-" direction="pas"/>
<pin name="OUTB" direction="out"/>
<pin name="OUTA" direction="out"/>
</symbol>
<symbol name="LF442CN">
<pin name="V+" direction="pwr"/>
<pin name="POS_A" direction="in"/>
<pin name="NEG_A" direction="in"/>
<pin name="POS_B" direction="in"/>
<pin name="NEG_B" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT_A" direction="out"/>
<pin name="OUT_B" direction="out"/>
</symbol>
<symbol name="LF444ACN">
<pin name="V+" direction="pwr"/>
<pin name="IN1-" direction="in"/>
<pin name="IN1+" direction="in"/>
<pin name="IN2+" direction="in"/>
<pin name="IN2-" direction="in"/>
<pin name="IN3-" direction="in"/>
<pin name="IN3+" direction="in"/>
<pin name="IN4+" direction="in"/>
<pin name="IN4-" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT1" direction="out"/>
<pin name="OUT2" direction="out"/>
<pin name="OUT3" direction="out"/>
<pin name="OUT4" direction="out"/>
</symbol>
<symbol name="LF444CM">
<pin name="V+" direction="pwr"/>
<pin name="IN1-" direction="in"/>
<pin name="IN1+" direction="in"/>
<pin name="IN2+" direction="in"/>
<pin name="IN2-" direction="in"/>
<pin name="IN3-" direction="in"/>
<pin name="IN3+" direction="in"/>
<pin name="IN4+" direction="in"/>
<pin name="IN4-" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT1" direction="out"/>
<pin name="OUT2" direction="out"/>
<pin name="OUT3" direction="out"/>
<pin name="OUT4" direction="out"/>
</symbol>
<symbol name="LF444CN">
<pin name="V+" direction="pwr"/>
<pin name="IN1+" direction="in"/>
<pin name="IN1-" direction="in"/>
<pin name="IN2+" direction="in"/>
<pin name="IN2-" direction="in"/>
<pin name="IN3+" direction="in"/>
<pin name="IN3-" direction="in"/>
<pin name="IN4+" direction="in"/>
<pin name="IN4-" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT_1" direction="out"/>
<pin name="OUT_2" direction="out"/>
<pin name="OUT_3" direction="out"/>
<pin name="OUT_4" direction="out"/>
</symbol>
<symbol name="LM101AH">
<pin name="-INA" direction="in"/>
<pin name="+INA" direction="in"/>
<pin name="BALANCE_2" direction="in"/>
<pin name="BALANCE" direction="in"/>
<pin name="V+" direction="in"/>
<pin name="V-" direction="pas"/>
<pin name="COMP" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM101AHLQMLV">
<pin name="+IN" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
<pin name="COMPENSATION" direction="pas"/>
<pin name="BALANCE_2" direction="pas"/>
<pin name="BALANCE" direction="pas"/>
<pin name="OUTPUT" direction="out"/>
</symbol>
<symbol name="LM101AJLQMLV">
<pin name="V+" direction="pwr"/>
<pin name="-IN" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="BAL/COMP" direction="pas"/>
<pin name="BAL" direction="in"/>
<pin name="COMP" direction="pas"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM1084IS-12">
<pin name="IN" direction="pwr"/>
<pin name="ADJ/GND" direction="pas"/>
<pin name="OUT" direction="out"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LM1084IS-3.3">
<pin name="IN" direction="pwr"/>
<pin name="ADJ/GND" direction="pas"/>
<pin name="OUT" direction="out"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LM1084IS-5.0">
<pin name="IN" direction="pwr"/>
<pin name="ADJ/GND" direction="pas"/>
<pin name="OUT" direction="out"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LM1084IT-3.3">
<pin name="VIN" direction="in"/>
<pin name="ADJ/GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LM1084IT-5.0">
<pin name="IN" direction="in"/>
<pin name="ADJ/GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM1085IS-12">
<pin name="IN" direction="pwr"/>
<pin name="ADJ/GND" direction="pas"/>
<pin name="OUT" direction="out"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LM1085IS-3.3">
<pin name="IN" direction="pwr"/>
<pin name="ADJ/GND" direction="pas"/>
<pin name="OUT" direction="out"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LM1085IS-5.0">
<pin name="IN" direction="pwr"/>
<pin name="ADJ/GND" direction="pas"/>
<pin name="OUT" direction="out"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LM1085IT-3.3">
<pin name="VIN" direction="in"/>
<pin name="ADJ/GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LM1085IT-5.0">
<pin name="VIN" direction="in"/>
<pin name="ADJ/GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LM1085IT-ADJ">
<pin name="IN" direction="in"/>
<pin name="ADJ/GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM1086CS-2.5">
<pin name="IN" direction="pwr"/>
<pin name="ADJ/GND" direction="pas"/>
<pin name="OUT" direction="out"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LM1086CT-3.3">
<pin name="IN" direction="in"/>
<pin name="ADJ/GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM1086CT-5.0">
<pin name="VIN" direction="in"/>
<pin name="ADJ/GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LM1086CT-ADJ">
<pin name="IN" direction="in"/>
<pin name="ADJ/GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM1086IT-3.3">
<pin name="VIN" direction="in"/>
<pin name="ADJ/GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LM1086IT-5.0">
<pin name="VIN" direction="in"/>
<pin name="ADJ/GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LM10CLN">
<pin name="V+" direction="pwr"/>
<pin name="BALANCE" direction="in"/>
<pin name="REFERENCE_FEED_BACK" direction="pas"/>
<pin name="OP_AMP_IN+" direction="in"/>
<pin name="OP_AMP_IN-" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="REFERENCE_OUT" direction="out"/>
<pin name="OP_AMP_OUT" direction="out"/>
</symbol>
<symbol name="LM10CN">
<pin name="V+" direction="pwr"/>
<pin name="BALANCE" direction="in"/>
<pin name="REFERENCE_FEED_BACK" direction="pas"/>
<pin name="OP_AMP_IN+" direction="in"/>
<pin name="OP_AMP_IN-" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="REFERENCE_OUT" direction="out"/>
<pin name="OP_AMP_OUT" direction="out"/>
</symbol>
<symbol name="LM10CWM">
<pin name="V+" direction="pwr"/>
<pin name="BAL" direction="in"/>
<pin name="REF_FEEDBACK" direction="in"/>
<pin name="OP_AMP_IN-" direction="in"/>
<pin name="OP_AMP_IN+" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC_6" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="V-" direction="pwr"/>
<pin name="REF_OUT" direction="out"/>
<pin name="OP_AMP_OUT" direction="out"/>
</symbol>
<symbol name="LM1117DT-1.8">
<pin name="ADJ_/_GND" direction="pwr"/>
<pin name="VIN" direction="in"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LM1117DT-2.5">
<pin name="ADJ_/_GND" direction="pwr"/>
<pin name="VIN" direction="in"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LM1117DT-3.3">
<pin name="ADJ_/_GND" direction="pwr"/>
<pin name="VIN" direction="in"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LM1117DT-5.0">
<pin name="ADJ_/_GND" direction="pwr"/>
<pin name="VIN" direction="in"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LM1117DT-ADJ">
<pin name="ADJ_/_GND" direction="pwr"/>
<pin name="VIN" direction="in"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LM1117IDT-3.3">
<pin name="ADJ_/_GND" direction="pwr"/>
<pin name="VIN" direction="in"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LM1117IDT-5.0">
<pin name="ADJ_/_GND" direction="pwr"/>
<pin name="VIN" direction="in"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LM1117IMP-3.3">
<pin name="VIN" direction="in"/>
<pin name="ADJ/GND" direction="pas"/>
<pin name="VOUT_2" direction="out"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LM1117IMP-5.0">
<pin name="VIN" direction="in"/>
<pin name="ADJ/GND" direction="pas"/>
<pin name="VOUT_2" direction="out"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LM1117LD-1.8">
<pin name="VIN_2" direction="in"/>
<pin name="VIN_3" direction="in"/>
<pin name="VIN" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="ADJ/GND" direction="pas"/>
<pin name="VOUT_2" direction="out"/>
<pin name="VOUT_3" direction="out"/>
<pin name="VOUT_4" direction="out"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LM1117LD-3.3">
<pin name="VIN_2" direction="in"/>
<pin name="VIN_3" direction="in"/>
<pin name="VIN" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="ADJ/GND" direction="pas"/>
<pin name="VOUT_2" direction="out"/>
<pin name="VOUT_3" direction="out"/>
<pin name="VOUT_4" direction="out"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LM1117MP-1.8">
<pin name="VIN" direction="in"/>
<pin name="ADJ/GND" direction="pas"/>
<pin name="VOUT_2" direction="out"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LM1117MP-2.5">
<pin name="IN" direction="in"/>
<pin name="ADJ/GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM1117MP-3.3">
<pin name="IN" direction="in"/>
<pin name="ADJ/GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM1117MP-5.0">
<pin name="IN" direction="in"/>
<pin name="ADJ/GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM1117MP-ADJ">
<pin name="IN" direction="in"/>
<pin name="ADJ/GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM1117S-ADJ">
<pin name="IN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="ADJ/GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM1117T-2.5">
<pin name="IN" direction="in"/>
<pin name="ADJ/GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM1117T-3.3">
<pin name="IN" direction="in"/>
<pin name="ADJ/GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM1117T-5.0">
<pin name="IN" direction="in"/>
<pin name="ADJ/GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM1117T-ADJ">
<pin name="IN" direction="in"/>
<pin name="ADJ/GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM111H">
<pin name="+IN" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="BALANCE/STROBE" direction="in"/>
<pin name="BALANCE" direction="in"/>
<pin name="V+" direction="pas"/>
<pin name="V-" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM111HLQMLV">
<pin name="+IN" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="+V" direction="pas"/>
<pin name="V-" direction="pwr"/>
<pin name="GND" direction="pas"/>
<pin name="OUTPUT" direction="out"/>
<pin name="BALANCE" direction="in"/>
<pin name="BALANCE/STROBE" direction="in"/>
</symbol>
<symbol name="LM111J-8">
<pin name="VCC+" direction="pwr"/>
<pin name="IN+" direction="in"/>
<pin name="IN-" direction="in"/>
<pin name="BALANCE" direction="pas"/>
<pin name="BAL/STRB" direction="pas"/>
<pin name="VCC-" direction="pwr"/>
<pin name="EMIT_OUT" direction="out"/>
<pin name="COL_OUT" direction="out"/>
</symbol>
<symbol name="LM111J-8LQMLV">
<pin name="V+" direction="pwr"/>
<pin name="+IN" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="BAL" direction="in"/>
<pin name="BAL/STROBE" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM111WGLQMLV">
<pin name="V+" direction="pwr"/>
<pin name="+IN" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="BAL" direction="pas"/>
<pin name="BAL/STROBE" direction="pas"/>
<pin name="V-" direction="pwr"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM119H">
<pin name="+IN_2" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="-IN_2" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="V+" direction="pas"/>
<pin name="V-" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GND2" direction="pas"/>
<pin name="OUT_2" direction="out"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM124AJRLQMLV">
<pin name="V+" direction="pwr"/>
<pin name="-IN1" direction="in"/>
<pin name="+IN1" direction="in"/>
<pin name="+IN2" direction="in"/>
<pin name="-IN2" direction="in"/>
<pin name="-IN3" direction="in"/>
<pin name="+IN3" direction="in"/>
<pin name="+IN4" direction="in"/>
<pin name="-IN4" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT1" direction="out"/>
<pin name="OUT2" direction="out"/>
<pin name="OUT3" direction="out"/>
<pin name="OUT4" direction="out"/>
</symbol>
<symbol name="LM124AJRQMLV">
<pin name="V+" direction="pwr"/>
<pin name="-IN1" direction="in"/>
<pin name="+IN1" direction="in"/>
<pin name="+IN2" direction="in"/>
<pin name="-IN2" direction="in"/>
<pin name="-IN3" direction="in"/>
<pin name="+IN3" direction="in"/>
<pin name="+IN4" direction="in"/>
<pin name="-IN4" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT1" direction="out"/>
<pin name="OUT2" direction="out"/>
<pin name="OUT3" direction="out"/>
<pin name="OUT4" direction="out"/>
</symbol>
<symbol name="LM124AWGRLQMLV">
<pin name="V+" direction="pwr"/>
<pin name="+IN1" direction="in"/>
<pin name="-IN1" direction="in"/>
<pin name="+IN2" direction="in"/>
<pin name="-IN2" direction="in"/>
<pin name="+IN3" direction="in"/>
<pin name="-IN3" direction="in"/>
<pin name="+IN4" direction="in"/>
<pin name="-IN4" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT1" direction="out"/>
<pin name="OUT2" direction="out"/>
<pin name="OUT3" direction="out"/>
<pin name="OUT4" direction="out"/>
</symbol>
<symbol name="LM124AWGRQMLV">
<pin name="V+" direction="pwr"/>
<pin name="+IN1" direction="in"/>
<pin name="-IN1" direction="in"/>
<pin name="+IN2" direction="in"/>
<pin name="-IN2" direction="in"/>
<pin name="+IN3" direction="in"/>
<pin name="-IN3" direction="in"/>
<pin name="+IN4" direction="in"/>
<pin name="-IN4" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT1" direction="out"/>
<pin name="OUT2" direction="out"/>
<pin name="OUT3" direction="out"/>
<pin name="OUT4" direction="out"/>
</symbol>
<symbol name="LM124J">
<pin name="V+" direction="pwr"/>
<pin name="IN1-" direction="in"/>
<pin name="IN1+" direction="in"/>
<pin name="IN2+" direction="in"/>
<pin name="IN2-" direction="in"/>
<pin name="IN3-" direction="in"/>
<pin name="IN3+" direction="in"/>
<pin name="IN4+" direction="in"/>
<pin name="IN4-" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT1" direction="out"/>
<pin name="OUT2" direction="out"/>
<pin name="OUT3" direction="out"/>
<pin name="OUT4" direction="out"/>
</symbol>
<symbol name="LM12H458CIV">
<pin name="VA+" direction="pwr"/>
<pin name="VD+" direction="pwr"/>
<pin name="~RD" direction="in"/>
<pin name="~WR" direction="in"/>
<pin name="~CS" direction="in"/>
<pin name="ALE" direction="in"/>
<pin name="CLK" direction="in"/>
<pin name="SYNC" direction="in"/>
<pin name="BW" direction="in"/>
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="IN0" direction="in"/>
<pin name="IN1" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="IN3" direction="in"/>
<pin name="IN4(MUXOUT-)" direction="in"/>
<pin name="IN5(MUXOUT+)" direction="in"/>
<pin name="IN6(S/H_IN-)" direction="in"/>
<pin name="IN7(S/H_IN+)" direction="in"/>
<pin name="VREF-" direction="in"/>
<pin name="VREF+" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="D0"/>
<pin name="D1"/>
<pin name="D2"/>
<pin name="D3"/>
<pin name="D4"/>
<pin name="D5"/>
<pin name="D6"/>
<pin name="D7"/>
<pin name="D8"/>
<pin name="D9"/>
<pin name="D10"/>
<pin name="D11"/>
<pin name="D12"/>
<pin name="D13"/>
<pin name="D14"/>
<pin name="D15"/>
<pin name="~INT" direction="out"/>
<pin name="DMARQ" direction="out"/>
<pin name="VREFOUT" direction="out"/>
</symbol>
<symbol name="LM135H">
<pin name="ADJ" direction="in"/>
<pin name="-VE" direction="pas"/>
<pin name="+VE" direction="pwr"/>
</symbol>
<symbol name="LM13700M">
<pin name="V+" direction="pwr"/>
<pin name="+IN_2" direction="in"/>
<pin name="-IN_2" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="DIODE_BIAS_2" direction="in"/>
<pin name="DIODE_BIAS" direction="in"/>
<pin name="BUFFER_IN_2" direction="in"/>
<pin name="BUFFER_IN" direction="in"/>
<pin name="AMP_BIAS_IN_2" direction="in"/>
<pin name="AMP_BIAS_IN" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="BUFFER_OUT_2" direction="out"/>
<pin name="BUFFER_OUT" direction="out"/>
<pin name="OUT_2" direction="out"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM13700N">
<pin name="V+" direction="pwr"/>
<pin name="+IN_2" direction="in"/>
<pin name="-IN_2" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="DIODE_BIAS_2" direction="in"/>
<pin name="DIODE_BIAS" direction="in"/>
<pin name="BUFFER_IN_2" direction="in"/>
<pin name="BUFFER_IN" direction="in"/>
<pin name="AMP_BIAS_IN_2" direction="in"/>
<pin name="AMP_BIAS_IN" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="BUFFER_OUT_2" direction="out"/>
<pin name="BUFFER_OUT" direction="out"/>
<pin name="OUT_2" direction="out"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM139AJRLQMLV">
<pin name="V+" direction="pwr"/>
<pin name="-IN1" direction="in"/>
<pin name="+IN1" direction="in"/>
<pin name="-IN2" direction="in"/>
<pin name="+IN2" direction="in"/>
<pin name="-IN3" direction="in"/>
<pin name="+IN3" direction="in"/>
<pin name="-IN4" direction="in"/>
<pin name="+IN4" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT1" direction="out"/>
<pin name="OUT2" direction="out"/>
<pin name="OUT3" direction="out"/>
<pin name="OUT4" direction="out"/>
</symbol>
<symbol name="LM139AJRQMLV">
<pin name="V+" direction="pwr"/>
<pin name="-IN1" direction="in"/>
<pin name="+IN1" direction="in"/>
<pin name="-IN2" direction="in"/>
<pin name="+IN2" direction="in"/>
<pin name="-IN3" direction="in"/>
<pin name="+IN3" direction="in"/>
<pin name="-IN4" direction="in"/>
<pin name="+IN4" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT1" direction="out"/>
<pin name="OUT2" direction="out"/>
<pin name="OUT3" direction="out"/>
<pin name="OUT4" direction="out"/>
</symbol>
<symbol name="LM139AWGRQMLV">
<pin name="V+" direction="pwr"/>
<pin name="-IN1" direction="in"/>
<pin name="+IN1" direction="in"/>
<pin name="-IN2" direction="in"/>
<pin name="+IN2" direction="in"/>
<pin name="-IN3" direction="in"/>
<pin name="+IN3" direction="in"/>
<pin name="-IN4" direction="in"/>
<pin name="+IN4" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT2" direction="out"/>
<pin name="OUT1" direction="out"/>
<pin name="OUT4" direction="out"/>
<pin name="OUT3" direction="out"/>
</symbol>
<symbol name="LM139J">
<pin name="V+" direction="pwr"/>
<pin name="-IN1" direction="in"/>
<pin name="+IN1" direction="in"/>
<pin name="-IN2" direction="in"/>
<pin name="+IN2" direction="in"/>
<pin name="-IN3" direction="in"/>
<pin name="+IN3" direction="in"/>
<pin name="-IN4" direction="in"/>
<pin name="+IN4" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT1" direction="out"/>
<pin name="OUT2" direction="out"/>
<pin name="OUT3" direction="out"/>
<pin name="OUT4" direction="out"/>
</symbol>
<symbol name="LM1458M">
<pin name="V+" direction="pwr"/>
<pin name="NEG_INA" direction="in"/>
<pin name="POS_INA" direction="in"/>
<pin name="POS_INB" direction="in"/>
<pin name="NEG_INB" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="LM1458N">
<pin name="V+" direction="pwr"/>
<pin name="POS_A" direction="in"/>
<pin name="NEG_A" direction="in"/>
<pin name="POS_B" direction="in"/>
<pin name="NEG_B" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT_A" direction="out"/>
<pin name="OUT_B" direction="out"/>
</symbol>
<symbol name="LM148J">
<pin name="V+" direction="pwr"/>
<pin name="-IN1" direction="in"/>
<pin name="+IN1" direction="in"/>
<pin name="+IN2" direction="in"/>
<pin name="-IN2" direction="in"/>
<pin name="-IN3" direction="in"/>
<pin name="+IN3" direction="in"/>
<pin name="+IN4" direction="in"/>
<pin name="-IN4" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT1" direction="out"/>
<pin name="OUT2" direction="out"/>
<pin name="OUT3" direction="out"/>
<pin name="OUT4" direction="out"/>
</symbol>
<symbol name="LM1558H">
<pin name="-INA" direction="in"/>
<pin name="+INA" direction="in"/>
<pin name="-INB" direction="in"/>
<pin name="+INB" direction="in"/>
<pin name="V+" direction="pas"/>
<pin name="V-" direction="pas"/>
<pin name="OUTB" direction="out"/>
<pin name="OUTA" direction="out"/>
</symbol>
<symbol name="LM158AH">
<pin name="-INA" direction="in"/>
<pin name="+INA" direction="in"/>
<pin name="-INB" direction="in"/>
<pin name="+INB" direction="in"/>
<pin name="V+" direction="pas"/>
<pin name="V-" direction="pas"/>
<pin name="OUTB" direction="out"/>
<pin name="OUTA" direction="out"/>
</symbol>
<symbol name="LM158H">
<pin name="-INA" direction="in"/>
<pin name="+INA" direction="in"/>
<pin name="-INB" direction="in"/>
<pin name="+INB" direction="in"/>
<pin name="V+" direction="pas"/>
<pin name="V-" direction="pas"/>
<pin name="OUTB" direction="out"/>
<pin name="OUTA" direction="out"/>
</symbol>
<symbol name="LM158J">
<pin name="V+" direction="pwr"/>
<pin name="POSA" direction="in"/>
<pin name="POSB" direction="in"/>
<pin name="NEGA" direction="in"/>
<pin name="NEGB" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="LM1770SMF">
<pin name="VIN" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="LG" direction="out"/>
<pin name="HG" direction="out"/>
</symbol>
<symbol name="LM1770TMF">
<pin name="VIN" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="LG" direction="out"/>
<pin name="HG" direction="out"/>
</symbol>
<symbol name="LM1770UMF">
<pin name="VIN" direction="pwr"/>
<pin name="FB" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="LG" direction="out"/>
<pin name="HG" direction="out"/>
</symbol>
<symbol name="LM1771SMM">
<pin name="VIN_2" direction="pwr"/>
<pin name="VIN" direction="pwr"/>
<pin name="FB" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="HG" direction="out"/>
<pin name="LG" direction="out"/>
</symbol>
<symbol name="LM1771SSD">
<pin name="VIN" direction="pwr"/>
<pin name="FB" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="HG" direction="out"/>
<pin name="LG" direction="out"/>
</symbol>
<symbol name="LM1771TMM">
<pin name="VIN_2" direction="pwr"/>
<pin name="VIN" direction="pwr"/>
<pin name="EN" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="HG" direction="out"/>
<pin name="LG" direction="out"/>
</symbol>
<symbol name="LM1771UMM">
<pin name="VIN_2" direction="pwr"/>
<pin name="VIN" direction="pwr"/>
<pin name="FB" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="HG" direction="out"/>
<pin name="LG" direction="out"/>
</symbol>
<symbol name="LM193AH">
<pin name="-INA" direction="in"/>
<pin name="+INA" direction="in"/>
<pin name="-INB" direction="in"/>
<pin name="+INB" direction="in"/>
<pin name="V+" direction="pas"/>
<pin name="V-" direction="pas"/>
<pin name="OUTB" direction="out"/>
<pin name="OUTA" direction="out"/>
</symbol>
<symbol name="LM193AJ-QMLV">
<pin name="V+" direction="pwr"/>
<pin name="NEGA" direction="in"/>
<pin name="POSA" direction="in"/>
<pin name="POSB" direction="in"/>
<pin name="NEGB" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="LM193H">
<pin name="-INA" direction="in"/>
<pin name="+INA" direction="in"/>
<pin name="-INB" direction="in"/>
<pin name="+INB" direction="in"/>
<pin name="V+" direction="pas"/>
<pin name="V-" direction="pas"/>
<pin name="OUTB" direction="out"/>
<pin name="OUTA" direction="out"/>
</symbol>
<symbol name="LM19CIZ">
<pin name="+VS" direction="pwr"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LM20123MH">
<pin name="VCC" direction="pwr"/>
<pin name="FB" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="SS/TRK" direction="in"/>
<pin name="COMP" direction="in"/>
<pin name="AVIN" direction="in"/>
<pin name="PVIN_2" direction="in"/>
<pin name="PVIN" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="PGND_2" direction="pas"/>
<pin name="AGND" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="PGOOD" direction="out"/>
<pin name="SW_2" direction="out"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM20124MH">
<pin name="VCC" direction="pwr"/>
<pin name="FB" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="SS/TRK" direction="in"/>
<pin name="COMP" direction="in"/>
<pin name="AVIN" direction="in"/>
<pin name="PVIN_2" direction="in"/>
<pin name="PVIN" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="PGND_2" direction="pas"/>
<pin name="AGND" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="PGOOD" direction="out"/>
<pin name="SW_2" direction="out"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM20125MH">
<pin name="VCC" direction="pwr"/>
<pin name="FB" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="SS/TRK" direction="in"/>
<pin name="COMP" direction="in"/>
<pin name="AVIN" direction="in"/>
<pin name="PVIN_2" direction="in"/>
<pin name="PVIN" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="PGND_2" direction="pas"/>
<pin name="AGND" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="PGOOD" direction="out"/>
<pin name="SW_2" direction="out"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM20133MH">
<pin name="VCC" direction="pwr"/>
<pin name="FB" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="SS/TRK" direction="in"/>
<pin name="COMP" direction="in"/>
<pin name="AVIN" direction="in"/>
<pin name="PVIN_2" direction="in"/>
<pin name="PVIN" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="PGND_2" direction="pas"/>
<pin name="AGND" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="PGOOD" direction="out"/>
<pin name="SW_2" direction="out"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM20134MH">
<pin name="VCC" direction="pwr"/>
<pin name="FB" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="SS/TRK" direction="in"/>
<pin name="COMP" direction="in"/>
<pin name="AVIN" direction="in"/>
<pin name="PVIN_2" direction="in"/>
<pin name="PVIN" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="PGND_2" direction="pas"/>
<pin name="AGND" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="PGOOD" direction="out"/>
<pin name="SW_2" direction="out"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM20136MH">
<pin name="AVIN" direction="pwr"/>
<pin name="PVIN_2" direction="pwr"/>
<pin name="PVIN" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="COMP" direction="pas"/>
<pin name="EN" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="SS/TRK" direction="in"/>
<pin name="SYNC" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="AGND" direction="pas"/>
<pin name="PGND_2" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="EP" direction="pas"/>
<pin name="PGOOD" direction="out"/>
<pin name="SW_2" direction="out"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM20143MH">
<pin name="VCC" direction="pwr"/>
<pin name="FB" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="SS/TRK" direction="in"/>
<pin name="COMP" direction="in"/>
<pin name="RT" direction="in"/>
<pin name="AVIN" direction="in"/>
<pin name="PVIN_2" direction="in"/>
<pin name="PVIN" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="AGND" direction="pas"/>
<pin name="PGND_2" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="PGOOD" direction="out"/>
<pin name="SW_2" direction="out"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM20144MH">
<pin name="VCC" direction="pwr"/>
<pin name="FB" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="SS/TRK" direction="in"/>
<pin name="COMP" direction="in"/>
<pin name="RT" direction="in"/>
<pin name="AVIN" direction="in"/>
<pin name="PVIN_2" direction="in"/>
<pin name="PVIN" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="AGND" direction="pas"/>
<pin name="PGND_2" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="PGOOD" direction="out"/>
<pin name="SW_2" direction="out"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM20145MH">
<pin name="VCC" direction="pwr"/>
<pin name="FB" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="SS/TRK" direction="in"/>
<pin name="COMP" direction="in"/>
<pin name="RT" direction="in"/>
<pin name="AVIN" direction="in"/>
<pin name="PVIN_2" direction="in"/>
<pin name="PVIN" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="AGND" direction="pas"/>
<pin name="PGND_2" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="PGOOD" direction="out"/>
<pin name="SW_2" direction="out"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM20146MH">
<pin name="AVIN" direction="pwr"/>
<pin name="PVIN_2" direction="pwr"/>
<pin name="PVIN" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="COMP" direction="pas"/>
<pin name="EN" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="SS/TRK" direction="in"/>
<pin name="RT" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="AGND" direction="pas"/>
<pin name="PGND_2" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="EP" direction="pas"/>
<pin name="PGOOD" direction="out"/>
<pin name="SW_2" direction="out"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM20154MH">
<pin name="VCC" direction="pwr"/>
<pin name="AVIN" direction="in"/>
<pin name="PVIN_2" direction="in"/>
<pin name="PVIN" direction="in"/>
<pin name="SS/TRK" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="AGND" direction="pas"/>
<pin name="PGND_2" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="SYNCOUT" direction="out"/>
<pin name="PGOOD" direction="out"/>
<pin name="COMP" direction="out"/>
<pin name="SW_2" direction="out"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM20242MH">
<pin name="VCC" direction="pwr"/>
<pin name="SS/TRK" direction="in"/>
<pin name="BOOT" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="RT" direction="in"/>
<pin name="VIN_2" direction="in"/>
<pin name="VIN_3" direction="in"/>
<pin name="VIN_4" direction="in"/>
<pin name="VIN" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="AGND" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="COMP" direction="out"/>
<pin name="PGOOD" direction="out"/>
<pin name="SW_2" direction="out"/>
<pin name="SW_3" direction="out"/>
<pin name="SW_4" direction="out"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM20323MH">
<pin name="VCC" direction="pwr"/>
<pin name="SS/TRK" direction="in"/>
<pin name="BOOT" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="VIN_2" direction="in"/>
<pin name="VIN_3" direction="in"/>
<pin name="VIN_4" direction="in"/>
<pin name="VIN" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="AGND" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="COMP" direction="out"/>
<pin name="PGOOD" direction="out"/>
<pin name="SW_2" direction="out"/>
<pin name="SW_3" direction="out"/>
<pin name="SW_4" direction="out"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM20333MH">
<pin name="VCC" direction="pwr"/>
<pin name="SS/TRK" direction="in"/>
<pin name="BOOT" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="SYNC" direction="in"/>
<pin name="VIN_2" direction="in"/>
<pin name="VIN_3" direction="in"/>
<pin name="VIN_4" direction="in"/>
<pin name="VIN" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="AGND" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="COMP" direction="out"/>
<pin name="PGOOD" direction="out"/>
<pin name="SW_2" direction="out"/>
<pin name="SW_3" direction="out"/>
<pin name="SW_4" direction="out"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM20343MH">
<pin name="VCC" direction="pwr"/>
<pin name="SS/TRK" direction="in"/>
<pin name="BOOT" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="RT" direction="in"/>
<pin name="VIN_2" direction="in"/>
<pin name="VIN_3" direction="in"/>
<pin name="VIN_4" direction="in"/>
<pin name="VIN" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="AGND" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="COMP" direction="out"/>
<pin name="PGOOD" direction="out"/>
<pin name="SW_2" direction="out"/>
<pin name="SW_3" direction="out"/>
<pin name="SW_4" direction="out"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM20BIM7">
<pin name="V+" direction="pwr"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VO" direction="out"/>
</symbol>
<symbol name="LM20CIM7">
<pin name="V+" direction="pwr"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VO" direction="out"/>
</symbol>
<symbol name="LM224J">
<pin name="V+" direction="pwr"/>
<pin name="-IN1" direction="in"/>
<pin name="+IN1" direction="in"/>
<pin name="+IN2" direction="in"/>
<pin name="-IN2" direction="in"/>
<pin name="-IN3" direction="in"/>
<pin name="+IN3" direction="in"/>
<pin name="+IN4_2" direction="in"/>
<pin name="+IN4" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT1" direction="out"/>
<pin name="OUT2" direction="out"/>
<pin name="OUT3" direction="out"/>
<pin name="OUT4" direction="out"/>
</symbol>
<symbol name="LM22670MR-5.0">
<pin name="VIN" direction="pwr"/>
<pin name="RT/SYNC" direction="in"/>
<pin name="BOOT" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM22670MR-ADJ">
<pin name="VIN" direction="pwr"/>
<pin name="BOOT" direction="pwr"/>
<pin name="EN" direction="in"/>
<pin name="RT/SYNC" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="EPAD" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM22670TJ-5.0">
<pin name="VIN" direction="pwr"/>
<pin name="RT/SYNC" direction="in"/>
<pin name="BOOT" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM22670TJ-ADJ">
<pin name="VIN" direction="pwr"/>
<pin name="RT/SYNC" direction="in"/>
<pin name="BOOT" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM22671MR-ADJ">
<pin name="VIN" direction="in"/>
<pin name="RT/SYNC" direction="in"/>
<pin name="BOOT" direction="in"/>
<pin name="SS" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM22672MR-ADJ">
<pin name="VIN" direction="in"/>
<pin name="RT/SYNC" direction="in"/>
<pin name="BOOT" direction="in"/>
<pin name="SS" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM22673MR-ADJ">
<pin name="VIN" direction="pwr"/>
<pin name="BOOT" direction="pwr"/>
<pin name="SS" direction="in"/>
<pin name="IADJ" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="EPAD" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM22673TJ-ADJ">
<pin name="VIN" direction="pwr"/>
<pin name="IADJ" direction="in"/>
<pin name="BOOT" direction="in"/>
<pin name="SS" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM22674MR-ADJ">
<pin name="VIN" direction="pwr"/>
<pin name="BOOT" direction="pwr"/>
<pin name="EN" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="EPAD" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM22675MR-ADJ">
<pin name="VIN" direction="pwr"/>
<pin name="BOOT" direction="pwr"/>
<pin name="EN" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM22676MR-ADJ">
<pin name="VIN" direction="pwr"/>
<pin name="BOOT" direction="pwr"/>
<pin name="EN" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="EPAD" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM22676TJ-ADJ">
<pin name="VIN" direction="pwr"/>
<pin name="EN" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="BOOT" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM22677TJ-ADJ">
<pin name="VIN" direction="pwr"/>
<pin name="EN" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="BOOT" direction="in"/>
<pin name="RT/SYNC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM22678TJ-ADJ">
<pin name="VIN" direction="pwr"/>
<pin name="EN" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="BOOT" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM22679TJ-ADJ">
<pin name="VIN" direction="pwr"/>
<pin name="SS" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="BOOT" direction="in"/>
<pin name="IADJ" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM22680MR-ADJ">
<pin name="VIN" direction="pwr"/>
<pin name="EN" direction="in"/>
<pin name="SS" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="BOOT" direction="in"/>
<pin name="~RT/SYNC" direction="in"/>
<pin name="EP" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM239J">
<pin name="V+" direction="pwr"/>
<pin name="-IN1" direction="in"/>
<pin name="+IN1" direction="in"/>
<pin name="-IN2" direction="in"/>
<pin name="+IN2" direction="in"/>
<pin name="-IN3" direction="in"/>
<pin name="+IN3" direction="in"/>
<pin name="-IN4" direction="in"/>
<pin name="+IN4" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT1" direction="out"/>
<pin name="OUT2" direction="out"/>
<pin name="OUT3" direction="out"/>
<pin name="OUT4" direction="out"/>
</symbol>
<symbol name="LM25005MH">
<pin name="VCC" direction="pwr"/>
<pin name="VIN_2" direction="in"/>
<pin name="VIN" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="SS" direction="in"/>
<pin name="RT" direction="in"/>
<pin name="SD" direction="in"/>
<pin name="IS_2" direction="in"/>
<pin name="IS" direction="in"/>
<pin name="PRE" direction="in"/>
<pin name="BST" direction="in"/>
<pin name="RAMP" direction="in"/>
<pin name="SYNC" direction="in"/>
<pin name="COMP" direction="in"/>
<pin name="AGND" direction="pas"/>
<pin name="PGND_2" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="OUT" direction="out"/>
<pin name="SW_2" direction="out"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM25007MM">
<pin name="VCC" direction="pwr"/>
<pin name="VIN" direction="pwr"/>
<pin name="BST" direction="pas"/>
<pin name="FEEDBACK" direction="in"/>
<pin name="RCL" direction="in"/>
<pin name="RON" direction="in"/>
<pin name="RTN" direction="pas"/>
<pin name="SWITCH" direction="out"/>
</symbol>
<symbol name="LM25007SD">
<pin name="VCC" direction="pwr"/>
<pin name="VIN" direction="in"/>
<pin name="BST" direction="in"/>
<pin name="RCL" direction="in"/>
<pin name="RTN" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="RON" direction="in"/>
<pin name="EPAD" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM25010MH">
<pin name="VCC" direction="pwr"/>
<pin name="VIN" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="SS" direction="in"/>
<pin name="BST" direction="in"/>
<pin name="RTN" direction="in"/>
<pin name="ISEN" direction="in"/>
<pin name="RON/SD" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="SGND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM25010SD">
<pin name="VCC" direction="pwr"/>
<pin name="VIN" direction="in"/>
<pin name="RTN" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="BST" direction="in"/>
<pin name="SS" direction="in"/>
<pin name="ISEN" direction="in"/>
<pin name="RON/SD" direction="in"/>
<pin name="SGND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM25011MY">
<pin name="VIN" direction="pwr"/>
<pin name="FB" direction="in"/>
<pin name="RT" direction="in"/>
<pin name="CSG" direction="in"/>
<pin name="BST" direction="in"/>
<pin name="CS" direction="in"/>
<pin name="SS" direction="in"/>
<pin name="SGND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="PGD" direction="out"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM25037MT">
<pin name="VCC" direction="pwr"/>
<pin name="VIN" direction="in"/>
<pin name="SS" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="CS" direction="in"/>
<pin name="UVLO" direction="in"/>
<pin name="RAMP" direction="in"/>
<pin name="COMP" direction="in"/>
<pin name="RES" direction="in"/>
<pin name="REF" direction="in"/>
<pin name="RT1" direction="in"/>
<pin name="RT2" direction="in"/>
<pin name="AGND" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="LM25037QMT">
<pin name="VCC" direction="pwr"/>
<pin name="RAMP" direction="in"/>
<pin name="RES" direction="in"/>
<pin name="UVLO" direction="in"/>
<pin name="REF" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="CS" direction="in"/>
<pin name="SS" direction="in"/>
<pin name="RT1" direction="in"/>
<pin name="RT2" direction="in"/>
<pin name="VIN" direction="in"/>
<pin name="AGND" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
<pin name="COMP" direction="out"/>
</symbol>
<symbol name="LM25061PMM-1">
<pin name="VIN" direction="pwr"/>
<pin name="SENSE" direction="in"/>
<pin name="TIMER" direction="in"/>
<pin name="PWR" direction="in"/>
<pin name="UVLO/EN" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="GATE" direction="out"/>
<pin name="PGD" direction="out"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM25061PMM-2">
<pin name="VIN" direction="pwr"/>
<pin name="SENSE" direction="in"/>
<pin name="TIMER" direction="in"/>
<pin name="PWR" direction="in"/>
<pin name="UVLO/EN" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="GATE" direction="out"/>
<pin name="PGD" direction="out"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM25069PMM-1">
<pin name="VIN" direction="pwr"/>
<pin name="SENSE" direction="in"/>
<pin name="TIMER" direction="in"/>
<pin name="PWR" direction="in"/>
<pin name="UVLO/EN" direction="in"/>
<pin name="OVLO" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="GATE" direction="out"/>
<pin name="PGD" direction="out"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM25069PMM-2">
<pin name="VIN" direction="pwr"/>
<pin name="SENSE" direction="in"/>
<pin name="TIMER" direction="in"/>
<pin name="PWR" direction="in"/>
<pin name="UVLO/EN" direction="in"/>
<pin name="OVLO" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="GATE" direction="out"/>
<pin name="PGD" direction="out"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM25085AMM">
<pin name="VIN" direction="pwr"/>
<pin name="ADJ" direction="in"/>
<pin name="ISEN" direction="in"/>
<pin name="RT" direction="in"/>
<pin name="FB"/>
<pin name="GND" direction="pas"/>
<pin name="PGATE" direction="out"/>
<pin name="VCC" direction="out"/>
</symbol>
<symbol name="LM25085AMY">
<pin name="VCC" direction="pwr"/>
<pin name="ADJ" direction="in"/>
<pin name="ISEN" direction="in"/>
<pin name="RT" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="VIN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="PGATE" direction="out"/>
</symbol>
<symbol name="LM25085ASD">
<pin name="VCC" direction="pwr"/>
<pin name="ADJ" direction="in"/>
<pin name="ISEN" direction="in"/>
<pin name="RT" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="VIN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="PGATE" direction="out"/>
</symbol>
<symbol name="LM25085QMY">
<pin name="VCC" direction="pwr"/>
<pin name="ADJ" direction="in"/>
<pin name="RT" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="ISEN" direction="in"/>
<pin name="VIN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="PGATE" direction="out"/>
</symbol>
<symbol name="LM25085SD">
<pin name="VCC" direction="pwr"/>
<pin name="ADJ" direction="in"/>
<pin name="ISEN" direction="in"/>
<pin name="RT" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="VIN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="PGATE" direction="out"/>
</symbol>
<symbol name="LM25088MH-1">
<pin name="VCC" direction="pwr"/>
<pin name="CSG" direction="in"/>
<pin name="RAMP" direction="in"/>
<pin name="DITH" direction="in"/>
<pin name="BOOT" direction="in"/>
<pin name="CS" direction="in"/>
<pin name="RT/SYNC" direction="in"/>
<pin name="SS" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="HG" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="VIN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="SW" direction="out"/>
<pin name="OUT" direction="out"/>
<pin name="COMP" direction="out"/>
</symbol>
<symbol name="LM25088MH-2">
<pin name="VCC" direction="pwr"/>
<pin name="CSG" direction="in"/>
<pin name="RAMP" direction="in"/>
<pin name="DITH" direction="in"/>
<pin name="BOOT" direction="in"/>
<pin name="CS" direction="in"/>
<pin name="RT/SYNC" direction="in"/>
<pin name="SS" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="HG" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="VIN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="SW" direction="out"/>
<pin name="OUT" direction="out"/>
<pin name="COMP" direction="out"/>
</symbol>
<symbol name="LM25115AMT">
<pin name="VCC" direction="pwr"/>
<pin name="VBIAS" direction="in"/>
<pin name="CS" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="HS" direction="in"/>
<pin name="HB" direction="in"/>
<pin name="TRK/SS" direction="in"/>
<pin name="RAMP" direction="in"/>
<pin name="SYNC" direction="in"/>
<pin name="AGND" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="COMP" direction="out"/>
<pin name="VOUT" direction="out"/>
<pin name="CO" direction="out"/>
<pin name="LO" direction="out"/>
<pin name="HO" direction="out"/>
</symbol>
<symbol name="LM25115MT">
<pin name="VCC" direction="pwr"/>
<pin name="VBIAS" direction="in"/>
<pin name="CS" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="HS" direction="in"/>
<pin name="HB" direction="in"/>
<pin name="SS" direction="in"/>
<pin name="RAMP" direction="in"/>
<pin name="SYNC" direction="in"/>
<pin name="AGND" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="COMP" direction="out"/>
<pin name="VOUT" direction="out"/>
<pin name="CO" direction="out"/>
<pin name="LO" direction="out"/>
<pin name="HO" direction="out"/>
</symbol>
<symbol name="LM25115SD">
<pin name="VCC" direction="pwr"/>
<pin name="VBIAS" direction="in"/>
<pin name="CS" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="HS" direction="in"/>
<pin name="HB" direction="in"/>
<pin name="SS" direction="in"/>
<pin name="RAMP" direction="in"/>
<pin name="SYNC" direction="in"/>
<pin name="AGND" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="THER_PAD" direction="pas"/>
<pin name="COMP" direction="out"/>
<pin name="CO" direction="out"/>
<pin name="LO" direction="out"/>
<pin name="HO" direction="out"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LM25574MT">
<pin name="VCC" direction="pwr"/>
<pin name="VIN" direction="pwr"/>
<pin name="BST" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="IS" direction="in"/>
<pin name="PRE" direction="in"/>
<pin name="RAMP" direction="in"/>
<pin name="RT" direction="in"/>
<pin name="SD" direction="in"/>
<pin name="SS" direction="in"/>
<pin name="SW" direction="pas"/>
<pin name="AGND" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="COMP" direction="out"/>
<pin name="OUT" direction="out"/>
<pin name="SYNC"/>
</symbol>
<symbol name="LM25574QMT">
<pin name="VCC" direction="pwr"/>
<pin name="SD" direction="in"/>
<pin name="IS" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="SS" direction="in"/>
<pin name="RT" direction="in"/>
<pin name="PRE" direction="in"/>
<pin name="BST" direction="in"/>
<pin name="SYNC" direction="in"/>
<pin name="RAMP" direction="in"/>
<pin name="VIN" direction="in"/>
<pin name="PGND" direction="pas"/>
<pin name="AGND" direction="pas"/>
<pin name="COMP" direction="out"/>
<pin name="OUT" direction="out"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM25575MH">
<pin name="VCC" direction="pwr"/>
<pin name="VIN" direction="pwr"/>
<pin name="SD" direction="in"/>
<pin name="RT" direction="in"/>
<pin name="IS" direction="in"/>
<pin name="SS" direction="in"/>
<pin name="SW" direction="pas"/>
<pin name="BST" direction="in"/>
<pin name="PRE" direction="pas"/>
<pin name="SYNC"/>
<pin name="RAMP" direction="in"/>
<pin name="EP" direction="pas"/>
<pin name="AGND" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="COMP" direction="out"/>
<pin name="FB" direction="out"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM25575QMH">
<pin name="VCC" direction="pwr"/>
<pin name="VIN" direction="in"/>
<pin name="SYNC" direction="in"/>
<pin name="COMP" direction="in"/>
<pin name="RAMP" direction="in"/>
<pin name="PRE" direction="in"/>
<pin name="BST" direction="in"/>
<pin name="SD" direction="in"/>
<pin name="IS" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="SS" direction="in"/>
<pin name="RT" direction="in"/>
<pin name="AGND" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="SW" direction="out"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM25576MH">
<pin name="VCC" direction="pwr"/>
<pin name="VIN_2" direction="pwr"/>
<pin name="VIN" direction="pwr"/>
<pin name="SYNC"/>
<pin name="RAMP" direction="in"/>
<pin name="RT" direction="in"/>
<pin name="SD" direction="in"/>
<pin name="SS" direction="in"/>
<pin name="IS_2" direction="in"/>
<pin name="IS" direction="in"/>
<pin name="SW_2" direction="pas"/>
<pin name="SW" direction="pas"/>
<pin name="PRE" direction="pas"/>
<pin name="BST" direction="in"/>
<pin name="EP" direction="pas"/>
<pin name="AGND" direction="pas"/>
<pin name="PGND_2" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="COMP" direction="out"/>
<pin name="OUT" direction="out"/>
<pin name="FB" direction="out"/>
</symbol>
<symbol name="LM25576QMH">
<pin name="VCC" direction="pwr"/>
<pin name="SYNC" direction="in"/>
<pin name="COMP" direction="in"/>
<pin name="RAMP" direction="in"/>
<pin name="BST" direction="in"/>
<pin name="PRE" direction="in"/>
<pin name="SS" direction="in"/>
<pin name="SD" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="RT" direction="in"/>
<pin name="IS_2" direction="in"/>
<pin name="IS" direction="in"/>
<pin name="VIN_2" direction="in"/>
<pin name="VIN" direction="in"/>
<pin name="AGND" direction="pas"/>
<pin name="PGND_2" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="OUT" direction="out"/>
<pin name="SW_2" direction="out"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM2575M-5.0">
<pin name="VIN_2" direction="pwr"/>
<pin name="VIN" direction="pwr"/>
<pin name="FB" direction="in"/>
<pin name="ON/OFF" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC_6" direction="nc"/>
<pin name="NC_7" direction="nc"/>
<pin name="NC_8" direction="nc"/>
<pin name="NC_9" direction="nc"/>
<pin name="NC_10" direction="nc"/>
<pin name="NC_11" direction="nc"/>
<pin name="NC_12" direction="nc"/>
<pin name="NC_13" direction="nc"/>
<pin name="NC_14" direction="nc"/>
<pin name="NC_15" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="PWR_GND_2" direction="pas"/>
<pin name="PWR_GND" direction="pas"/>
<pin name="SIG_GND" direction="pas"/>
<pin name="OUT_2" direction="out"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM2575N-5.0">
<pin name="VIN" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="ON/OFF" direction="pas"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC_6" direction="nc"/>
<pin name="NC_7" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM2575S-12">
<pin name="VIN" direction="pwr"/>
<pin name="FB" direction="in"/>
<pin name="~ON/OFF" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM2575S-15">
<pin name="VIN" direction="in"/>
<pin name="~ON~/OFF" direction="pas"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
<pin name="FB"/>
</symbol>
<symbol name="LM2575S-3.3">
<pin name="VIN" direction="pwr"/>
<pin name="COMP" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM2575S-5.0">
<pin name="VIN" direction="pwr"/>
<pin name="COMP" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM2575S-ADJ">
<pin name="VIN" direction="pwr"/>
<pin name="COMP" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM2575T-12">
<pin name="VIN" direction="in"/>
<pin name="ON/OFF" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="FB" direction="in"/>
<pin name="OUTPUT" direction="out"/>
</symbol>
<symbol name="LM2575T-15">
<pin name="VIN" direction="in"/>
<pin name="ON/OFF" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="FB" direction="in"/>
<pin name="OUTPUT" direction="out"/>
</symbol>
<symbol name="LM2575T-3.3">
<pin name="VIN" direction="in"/>
<pin name="ON/OFF" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="FB" direction="in"/>
<pin name="OUTPUT" direction="out"/>
</symbol>
<symbol name="LM2575T-5.0">
<pin name="VIN" direction="in"/>
<pin name="ON/OFF" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="FB" direction="in"/>
<pin name="OUTPUT" direction="out"/>
</symbol>
<symbol name="LM2575T-ADJ">
<pin name="VIN" direction="in"/>
<pin name="ON/OFF" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="FB" direction="in"/>
<pin name="OUTPUT" direction="out"/>
</symbol>
<symbol name="LM2585S-12">
<pin name="VIN" direction="pwr"/>
<pin name="COMP" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM2585S-3.3">
<pin name="VIN" direction="pwr"/>
<pin name="COMP" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM2585S-5.0">
<pin name="VIN" direction="pwr"/>
<pin name="COMP" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM2585S-ADJ">
<pin name="VIN" direction="pwr"/>
<pin name="COMP" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM2585T-3.3">
<pin name="VIN" direction="in"/>
<pin name="FEEDBACK" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="SWITCH" direction="out"/>
<pin name="COMP" direction="in"/>
</symbol>
<symbol name="LM2585T-5.0">
<pin name="VIN" direction="in"/>
<pin name="FEEDBACK" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="SWITCH" direction="out"/>
<pin name="COMP" direction="in"/>
</symbol>
<symbol name="LM2585T-ADJ">
<pin name="VIN" direction="in"/>
<pin name="FEEDBACK" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="SWITCH" direction="out"/>
<pin name="COMP" direction="in"/>
</symbol>
<symbol name="LM2586S-5.0">
<pin name="VIN" direction="pwr"/>
<pin name="FREQ.ADJ._ON/~OFF" direction="in"/>
<pin name="COMP" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="FREQ_SYNC" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="SWITCH" direction="out"/>
</symbol>
<symbol name="LM2586S-ADJ">
<pin name="VIN" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="COMP" direction="in"/>
<pin name="FREQ_SYNC" direction="in"/>
<pin name="FREQ_ADJ_OR_ON/~OFF" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM2586T-3.3">
<pin name="COMP" direction="pas"/>
<pin name="FEEDBACK" direction="pas"/>
<pin name="VIN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="SWITCH" direction="out"/>
<pin name="SYNC" direction="pas"/>
<pin name="FREQ_ADJ_OR_ON/~OFF" direction="pas"/>
</symbol>
<symbol name="LM2586T-5.0">
<pin name="COMP" direction="pas"/>
<pin name="FEEDBACK" direction="pas"/>
<pin name="VIN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="SWITCH" direction="out"/>
<pin name="SYNC" direction="pas"/>
<pin name="FREQ_ADJ_OR_ON/~OFF" direction="pas"/>
</symbol>
<symbol name="LM2586T-ADJ">
<pin name="COMP" direction="pas"/>
<pin name="FEEDBACK" direction="pas"/>
<pin name="VIN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="SWITCH" direction="out"/>
<pin name="SYNC" direction="pas"/>
<pin name="FREQ_ADJ_OR_ON/~OFF" direction="pas"/>
</symbol>
<symbol name="LM2587S-3.3">
<pin name="VIN" direction="pwr"/>
<pin name="FB" direction="in"/>
<pin name="~ON/OFF" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM2587S-5.0">
<pin name="VIN" direction="pwr"/>
<pin name="COMP" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM2587S-ADJ">
<pin name="VIN" direction="pwr"/>
<pin name="COMP" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM2587T-12">
<pin name="VIN" direction="in"/>
<pin name="COMP" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="SW" direction="out"/>
<pin name="FB" direction="pas"/>
</symbol>
<symbol name="LM2587T-3.3">
<pin name="VIN" direction="in"/>
<pin name="COMP" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="SW" direction="out"/>
<pin name="FB" direction="pas"/>
</symbol>
<symbol name="LM2587T-5.0">
<pin name="VIN" direction="in"/>
<pin name="COMP" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="SW" direction="out"/>
<pin name="FB" direction="pas"/>
</symbol>
<symbol name="LM2587T-ADJ">
<pin name="VIN" direction="in"/>
<pin name="COMP" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="SW" direction="out"/>
<pin name="FB" direction="pas"/>
</symbol>
<symbol name="LM2588S-12">
<pin name="VIN" direction="pwr"/>
<pin name="FREQ.ADJ._ON/~OFF" direction="in"/>
<pin name="COMP" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="FREQ_SYNC" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="SWITCH" direction="out"/>
</symbol>
<symbol name="LM2588S-5.0">
<pin name="VIN" direction="pwr"/>
<pin name="FREQ.ADJ._ON/~OFF" direction="in"/>
<pin name="COMP" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="FREQ_SYNC" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="SWITCH" direction="out"/>
</symbol>
<symbol name="LM2588S-ADJ">
<pin name="VIN" direction="pwr"/>
<pin name="FREQ.ADJ._ON/~OFF" direction="in"/>
<pin name="COMP" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="FREQ_SYNC" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="SWITCH" direction="out"/>
</symbol>
<symbol name="LM2588T-5.0">
<pin name="VIN" direction="in"/>
<pin name="COMPENSATION" direction="in"/>
<pin name="FB" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="FRQ-SYNC" direction="pas"/>
<pin name="FRQ-ADJ-ON/OFF" direction="pas"/>
<pin name="SWITCH" direction="out"/>
</symbol>
<symbol name="LM2588T-ADJ">
<pin name="VIN" direction="in"/>
<pin name="COMPENSATION" direction="in"/>
<pin name="FB" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="FRQ-SYNC" direction="pas"/>
<pin name="FRQ-ADJ-ON/OFF" direction="pas"/>
<pin name="SWITCH" direction="out"/>
</symbol>
<symbol name="LM258H">
<pin name="-INA" direction="in"/>
<pin name="+INA" direction="in"/>
<pin name="-INB" direction="in"/>
<pin name="+INB" direction="in"/>
<pin name="V+" direction="pas"/>
<pin name="V-" direction="pas"/>
<pin name="OUTB" direction="out"/>
<pin name="OUTA" direction="out"/>
</symbol>
<symbol name="LM2590HVS-3.3">
<pin name="VIN" direction="in"/>
<pin name="DELAY" direction="in"/>
<pin name="~SD/SS" direction="in"/>
<pin name="FLAG" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM2590HVS-5.0">
<pin name="VIN" direction="in"/>
<pin name="DELAY" direction="in"/>
<pin name="~SD/SS" direction="in"/>
<pin name="FLAG" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM2590HVS-ADJ">
<pin name="VIN" direction="in"/>
<pin name="DELAY" direction="in"/>
<pin name="~SD/SS" direction="in"/>
<pin name="FLAG" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM2590HVT-3.3">
<pin name="VIN" direction="in"/>
<pin name="FLAG" direction="pas"/>
<pin name="*SD-SS" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="DELAY" direction="in"/>
<pin name="FEEDBACK" direction="in"/>
<pin name="OUTPUT" direction="out"/>
</symbol>
<symbol name="LM2590HVT-5.0">
<pin name="VIN" direction="in"/>
<pin name="FLAG" direction="pas"/>
<pin name="*SD-SS" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="DELAY" direction="in"/>
<pin name="FEEDBACK" direction="in"/>
<pin name="OUTPUT" direction="out"/>
</symbol>
<symbol name="LM2590HVT-ADJ">
<pin name="VIN" direction="in"/>
<pin name="FLAG" direction="pas"/>
<pin name="*SD-SS" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="DELAY" direction="in"/>
<pin name="FEEDBACK" direction="in"/>
<pin name="OUTPUT" direction="out"/>
</symbol>
<symbol name="LM2591HVS-3.3">
<pin name="VIN" direction="pwr"/>
<pin name="FB" direction="in"/>
<pin name="~ON/OFF" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM2591HVS-5.0">
<pin name="VIN" direction="pwr"/>
<pin name="FB" direction="in"/>
<pin name="~ON/OFF" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM2591HVS-ADJ">
<pin name="VIN" direction="pwr"/>
<pin name="FB" direction="in"/>
<pin name="~ON/OFF" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM2591HVT-3.3">
<pin name="*ON-OFF" direction="in"/>
<pin name="VIN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="FEEDBACK" direction="in"/>
<pin name="OUTPUT" direction="out"/>
</symbol>
<symbol name="LM2591HVT-5.0">
<pin name="VIN" direction="in"/>
<pin name="FB" direction="pas"/>
<pin name="~ON~/OFF" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="OUTPUT" direction="out"/>
</symbol>
<symbol name="LM2591HVT-ADJ">
<pin name="VIN" direction="in"/>
<pin name="FB" direction="pas"/>
<pin name="~ON~/OFF" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="OUTPUT" direction="out"/>
</symbol>
<symbol name="LM2592HVS-3.3">
<pin name="VIN" direction="pwr"/>
<pin name="FB" direction="in"/>
<pin name="~ON/OFF" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM2592HVS-5.0">
<pin name="VIN" direction="pwr"/>
<pin name="FB" direction="in"/>
<pin name="~ON/OFF" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM2592HVS-ADJ">
<pin name="VIN" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="~ON/OFF" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM2592HVT-3.3">
<pin name="VIN" direction="in"/>
<pin name="FB" direction="pas"/>
<pin name="~ON~/OFF" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="OUTPUT" direction="out"/>
</symbol>
<symbol name="LM2592HVT-5.0">
<pin name="VIN" direction="in"/>
<pin name="FB" direction="pas"/>
<pin name="~ON~/OFF" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="OUTPUT" direction="out"/>
</symbol>
<symbol name="LM2592HVT-ADJ">
<pin name="VIN" direction="in"/>
<pin name="FB" direction="pas"/>
<pin name="~ON~/OFF" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="OUTPUT" direction="out"/>
</symbol>
<symbol name="LM2593HVS-3.3">
<pin name="VIN" direction="in"/>
<pin name="DELAY" direction="in"/>
<pin name="~SD/SS" direction="in"/>
<pin name="FLAG" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM2593HVS-5.0">
<pin name="VIN" direction="in"/>
<pin name="DELAY" direction="in"/>
<pin name="~SD/SS" direction="in"/>
<pin name="FLAG" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM2593HVS-ADJ">
<pin name="VIN" direction="in"/>
<pin name="DELAY" direction="in"/>
<pin name="~SD/SS" direction="in"/>
<pin name="FLAG" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM2593HVT-3.3">
<pin name="VIN" direction="in"/>
<pin name="FLAG" direction="pas"/>
<pin name="*SD-SS" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="DELAY" direction="in"/>
<pin name="FEEDBACK" direction="in"/>
<pin name="OUTPUT" direction="out"/>
</symbol>
<symbol name="LM2593HVT-5.0">
<pin name="VIN" direction="in"/>
<pin name="FLAG" direction="pas"/>
<pin name="*SD-SS" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="DELAY" direction="in"/>
<pin name="FEEDBACK" direction="in"/>
<pin name="OUTPUT" direction="out"/>
</symbol>
<symbol name="LM2593HVT-ADJ">
<pin name="VIN" direction="in"/>
<pin name="FLAG" direction="pas"/>
<pin name="*SD-SS" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="DELAY" direction="in"/>
<pin name="FEEDBACK" direction="in"/>
<pin name="OUTPUT" direction="out"/>
</symbol>
<symbol name="LM2594HVM-12">
<pin name="VIN" direction="pwr"/>
<pin name="FB" direction="in"/>
<pin name="~ON/OFF" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="OUTPUT" direction="out"/>
</symbol>
<symbol name="LM2594HVM-3.3">
<pin name="VIN" direction="pwr"/>
<pin name="FB" direction="in"/>
<pin name="~ON~/OFF" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM2594HVM-5.0">
<pin name="VIN" direction="pwr"/>
<pin name="FB" direction="in"/>
<pin name="~ON~/OFF" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM2594HVM-ADJ">
<pin name="VIN" direction="in"/>
<pin name="~ON/OFF" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM2594HVN-12">
<pin name="VIN" direction="pwr"/>
<pin name="FB" direction="in"/>
<pin name="~ON~/OFF" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM2594HVN-3.3">
<pin name="VIN" direction="pwr"/>
<pin name="FB" direction="in"/>
<pin name="~ON~/OFF" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM2594HVN-5.0">
<pin name="VIN" direction="pwr"/>
<pin name="FB" direction="in"/>
<pin name="~ON~/OFF" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM2594HVN-ADJ">
<pin name="VIN" direction="pwr"/>
<pin name="FB" direction="in"/>
<pin name="~ON~/OFF" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM2594M-12">
<pin name="VIN" direction="pwr"/>
<pin name="FB" direction="in"/>
<pin name="~ON~/OFF" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM2594M-3.3">
<pin name="VIN" direction="pwr"/>
<pin name="FB" direction="in"/>
<pin name="ON/OFF" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM2594M-5.0">
<pin name="VIN" direction="pwr"/>
<pin name="FB" direction="in"/>
<pin name="ON/OFF" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM2594M-ADJ">
<pin name="VIN" direction="pwr"/>
<pin name="FB" direction="in"/>
<pin name="ON/OFF" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM2594N-12">
<pin name="VIN" direction="pwr"/>
<pin name="FB" direction="in"/>
<pin name="~ON~/OFF" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM2594N-3.3">
<pin name="VIN" direction="pwr"/>
<pin name="FB" direction="in"/>
<pin name="~ON~/OFF" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM2594N-5.0">
<pin name="VIN" direction="pwr"/>
<pin name="FB" direction="in"/>
<pin name="~ON~/OFF" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM2594N-ADJ">
<pin name="VIN" direction="pwr"/>
<pin name="FB" direction="in"/>
<pin name="~ON~/OFF" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM2595S-12">
<pin name="VIN" direction="pwr"/>
<pin name="FB" direction="in"/>
<pin name="~ON/OFF" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM2595S-3.3">
<pin name="VIN" direction="pwr"/>
<pin name="FB" direction="in"/>
<pin name="~ON/OFF" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM2595S-5.0">
<pin name="VIN" direction="pwr"/>
<pin name="FB" direction="in"/>
<pin name="~ON/OFF" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM2595S-ADJ">
<pin name="VIN" direction="pwr"/>
<pin name="FB" direction="in"/>
<pin name="~ON~/OFF" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM2595T-12">
<pin name="VIN" direction="in"/>
<pin name="~ON~/OFF" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="FB" direction="pas"/>
<pin name="OUTOUT" direction="out"/>
</symbol>
<symbol name="LM2595T-3.3">
<pin name="VIN" direction="in"/>
<pin name="~ON~/OFF" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="FB" direction="pas"/>
<pin name="OUTOUT" direction="out"/>
</symbol>
<symbol name="LM2595T-5.0">
<pin name="VIN" direction="in"/>
<pin name="~ON~/OFF" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="FB" direction="pas"/>
<pin name="OUTOUT" direction="out"/>
</symbol>
<symbol name="LM2595T-ADJ">
<pin name="VIN" direction="in"/>
<pin name="~ON~/OFF" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="FB" direction="pas"/>
<pin name="OUTOUT" direction="out"/>
</symbol>
<symbol name="LM2596S-12">
<pin name="VIN" direction="in"/>
<pin name="~ON~/OFF" direction="pas"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
<pin name="FB"/>
</symbol>
<symbol name="LM2596S-3.3">
<pin name="VIN" direction="pwr"/>
<pin name="FB" direction="in"/>
<pin name="~ON~/OFF" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM2596S-5.0">
<pin name="VIN" direction="pwr"/>
<pin name="FB" direction="in"/>
<pin name="~ON~/OFF" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM2596T-12">
<pin name="*ON-OFF" direction="in"/>
<pin name="VIN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="FEEDBACK" direction="in"/>
<pin name="OUTPUT" direction="out"/>
</symbol>
<symbol name="LM2596T-3.3">
<pin name="*ON-OFF" direction="in"/>
<pin name="VIN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="FEEDBACK" direction="in"/>
<pin name="OUTPUT" direction="out"/>
</symbol>
<symbol name="LM2596T-5.0">
<pin name="*ON-OFF" direction="in"/>
<pin name="VIN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="FEEDBACK" direction="in"/>
<pin name="OUTPUT" direction="out"/>
</symbol>
<symbol name="LM2597HVM-12">
<pin name="VIN" direction="pwr"/>
<pin name="B/S" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="~SD/SS" direction="in"/>
<pin name="DELAY" direction="in"/>
<pin name="ERROR_FLAG" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM2597HVM-3.3">
<pin name="VIN" direction="pwr"/>
<pin name="ERR_FLOG" direction="pas"/>
<pin name="DELAY" direction="pas"/>
<pin name="B/S" direction="pwr"/>
<pin name="FB" direction="in"/>
<pin name="~SD/SS" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM2597HVM-5.0">
<pin name="VIN" direction="pwr"/>
<pin name="B/S" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="~SD/SS" direction="in"/>
<pin name="DELAY" direction="in"/>
<pin name="ERROR_FLAG" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM2597HVM-ADJ">
<pin name="VIN" direction="pwr"/>
<pin name="B/S" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="~SD/SS" direction="in"/>
<pin name="DELAY" direction="in"/>
<pin name="ERROR_FLAG" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM2597HVN-ADJ">
<pin name="VIN" direction="pwr"/>
<pin name="B/S" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="~SD/SS" direction="in"/>
<pin name="DELAY" direction="in"/>
<pin name="ERROR_FLAG" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM2597M-12">
<pin name="VIN" direction="pwr"/>
<pin name="B/S" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="~SD/SS" direction="in"/>
<pin name="DELAY" direction="in"/>
<pin name="ERROR_FLAG" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM2597M-3.3">
<pin name="VIN" direction="pwr"/>
<pin name="ERROR_FLAG" direction="pas"/>
<pin name="DELAY" direction="pas"/>
<pin name="B/S" direction="pas"/>
<pin name="FB" direction="pas"/>
<pin name="~SD/SS" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="OUTPUT" direction="out"/>
</symbol>
<symbol name="LM2597M-5.0">
<pin name="VIN" direction="pwr"/>
<pin name="ERROR_FLAG" direction="pas"/>
<pin name="DELAY" direction="pas"/>
<pin name="B/S" direction="pas"/>
<pin name="FB" direction="pas"/>
<pin name="~SD/SS" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="OUTPUT" direction="out"/>
</symbol>
<symbol name="LM2597M-ADJ">
<pin name="VIN" direction="pwr"/>
<pin name="ERROR_FLAG" direction="pas"/>
<pin name="DELAY" direction="pas"/>
<pin name="B/S" direction="pas"/>
<pin name="FB" direction="pas"/>
<pin name="~SD/SS" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="OUTPUT" direction="out"/>
</symbol>
<symbol name="LM2597N-12">
<pin name="VIN" direction="pwr"/>
<pin name="B/S" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="~SD/SS" direction="in"/>
<pin name="DELAY" direction="in"/>
<pin name="ERROR_FLAG" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM2597N-3.3">
<pin name="VIN" direction="pwr"/>
<pin name="B/S" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="~SD/SS" direction="in"/>
<pin name="DELAY" direction="in"/>
<pin name="ERROR_FLAG" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM2597N-5.0">
<pin name="VIN" direction="pwr"/>
<pin name="B/S" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="~SD/SS" direction="in"/>
<pin name="DELAY" direction="in"/>
<pin name="ERROR_FLAG" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM2597N-ADJ">
<pin name="VIN" direction="pwr"/>
<pin name="B/S" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="~SD/SS" direction="in"/>
<pin name="DELAY" direction="in"/>
<pin name="ERROR_FLAG" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM2598S-3.3">
<pin name="VIN" direction="in"/>
<pin name="DELAY" direction="in"/>
<pin name="~SD/SS" direction="in"/>
<pin name="FLAG" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM2598S-5.0">
<pin name="VIN" direction="in"/>
<pin name="DELAY" direction="in"/>
<pin name="~SD/SS" direction="in"/>
<pin name="FLAG" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM2598S-ADJ">
<pin name="VIN" direction="in"/>
<pin name="DELAY" direction="in"/>
<pin name="~SD/SS" direction="in"/>
<pin name="FLAG" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM2598T-3.3">
<pin name="VIN" direction="in"/>
<pin name="FLAG" direction="pas"/>
<pin name="*SD-SS" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="DELAY" direction="in"/>
<pin name="FEEDBACK" direction="in"/>
<pin name="OUTPUT" direction="out"/>
</symbol>
<symbol name="LM2598T-5.0">
<pin name="VIN" direction="in"/>
<pin name="FLAG" direction="pas"/>
<pin name="*SD-SS" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="DELAY" direction="in"/>
<pin name="FEEDBACK" direction="in"/>
<pin name="OUTPUT" direction="out"/>
</symbol>
<symbol name="LM2598T-ADJ">
<pin name="VIN" direction="in"/>
<pin name="FLAG" direction="pas"/>
<pin name="*SD-SS" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="DELAY" direction="in"/>
<pin name="FEEDBACK" direction="in"/>
<pin name="OUTPUT" direction="out"/>
</symbol>
<symbol name="LM2599S-12">
<pin name="VIN" direction="in"/>
<pin name="DELAY" direction="in"/>
<pin name="~SD/SS" direction="in"/>
<pin name="FLAG" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM2599S-3.3">
<pin name="VIN" direction="in"/>
<pin name="DELAY" direction="in"/>
<pin name="~SD/SS" direction="in"/>
<pin name="FLAG" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM2599S-5.0">
<pin name="VIN" direction="in"/>
<pin name="DELAY" direction="in"/>
<pin name="~SD/SS" direction="in"/>
<pin name="FLAG" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM2599S-ADJ">
<pin name="VIN" direction="in"/>
<pin name="DELAY" direction="in"/>
<pin name="~SD/SS" direction="in"/>
<pin name="FLAG" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM2599T-12">
<pin name="VIN" direction="in"/>
<pin name="FLAG" direction="pas"/>
<pin name="*SD-SS" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="DELAY" direction="in"/>
<pin name="FEEDBACK" direction="in"/>
<pin name="OUTPUT" direction="out"/>
</symbol>
<symbol name="LM2599T-3.3">
<pin name="VIN" direction="in"/>
<pin name="FLAG" direction="pas"/>
<pin name="*SD-SS" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="DELAY" direction="in"/>
<pin name="FEEDBACK" direction="in"/>
<pin name="OUTPUT" direction="out"/>
</symbol>
<symbol name="LM2599T-5.0">
<pin name="VIN" direction="in"/>
<pin name="FLAG" direction="pas"/>
<pin name="*SD-SS" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="DELAY" direction="in"/>
<pin name="FEEDBACK" direction="in"/>
<pin name="OUTPUT" direction="out"/>
</symbol>
<symbol name="LM2599T-ADJ">
<pin name="VIN" direction="in"/>
<pin name="FLAG" direction="pas"/>
<pin name="*SD-SS" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="DELAY" direction="in"/>
<pin name="FEEDBACK" direction="in"/>
<pin name="OUTPUT" direction="out"/>
</symbol>
<symbol name="LM26001MXA">
<pin name="VDD" direction="pwr"/>
<pin name="EN" direction="in"/>
<pin name="SS" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="FREQ" direction="in"/>
<pin name="FPWM" direction="in"/>
<pin name="SYNC" direction="in"/>
<pin name="VBIAS" direction="in"/>
<pin name="BOOT" direction="in"/>
<pin name="VIN_2" direction="pwr"/>
<pin name="VIN" direction="pwr"/>
<pin name="GND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="PGOOD" direction="out"/>
<pin name="COMP" direction="out"/>
<pin name="SW_2" direction="out"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM26001QMXA">
<pin name="VDD" direction="pwr"/>
<pin name="VIN_2" direction="in"/>
<pin name="VIN" direction="in"/>
<pin name="FREQ" direction="in"/>
<pin name="FPWM" direction="in"/>
<pin name="SYNC" direction="in"/>
<pin name="VBIAS" direction="in"/>
<pin name="COMP" direction="in"/>
<pin name="BOOT" direction="pas"/>
<pin name="EN" direction="in"/>
<pin name="SS" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="EP" direction="pas"/>
<pin name="PGOOD" direction="out"/>
<pin name="SW_2" direction="out"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM26003MH">
<pin name="VDD" direction="pwr"/>
<pin name="VIN_2" direction="pwr"/>
<pin name="VIN_3" direction="pwr"/>
<pin name="VIN" direction="pwr"/>
<pin name="AVIN" direction="pwr"/>
<pin name="FREQ" direction="in"/>
<pin name="VBIAS" direction="in"/>
<pin name="FPWM" direction="in"/>
<pin name="SYNC" direction="in"/>
<pin name="BOOT" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="SS" direction="in"/>
<pin name="EPAD" direction="pas"/>
<pin name="AGND" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="PGOOD" direction="out"/>
<pin name="COMP" direction="out"/>
<pin name="SW_2" direction="out"/>
<pin name="SW_3" direction="out"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM26003QMH">
<pin name="VDD" direction="pwr"/>
<pin name="VIN_2" direction="pwr"/>
<pin name="VIN_3" direction="pwr"/>
<pin name="VIN" direction="pwr"/>
<pin name="AVIN" direction="pwr"/>
<pin name="FREQ" direction="in"/>
<pin name="VBIAS" direction="in"/>
<pin name="FPWM" direction="in"/>
<pin name="SYNC" direction="in"/>
<pin name="BOOT" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="SS" direction="in"/>
<pin name="EPAD" direction="pas"/>
<pin name="AGND" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="PGOOD" direction="out"/>
<pin name="COMP" direction="out"/>
<pin name="SW_2" direction="out"/>
<pin name="SW_3" direction="out"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM2611AMF">
<pin name="VIN" direction="pwr"/>
<pin name="NFB" direction="pas"/>
<pin name="~SHDN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM2611BMF">
<pin name="VIN" direction="pwr"/>
<pin name="NFB" direction="in"/>
<pin name="~SHDN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM2621MM">
<pin name="VDD" direction="pwr"/>
<pin name="FB" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="FREQ" direction="in"/>
<pin name="BOOT" direction="in"/>
<pin name="PGND" direction="pas"/>
<pin name="SGND" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM2622MM-ADJ">
<pin name="VIN" direction="pwr"/>
<pin name="FB" direction="in"/>
<pin name="VC" direction="in"/>
<pin name="~SHDN" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="SW" direction="out"/>
<pin name="FSLCT" direction="out"/>
</symbol>
<symbol name="LM2623AMM">
<pin name="VDD" direction="pwr"/>
<pin name="FB" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="FREQ" direction="in"/>
<pin name="BOOT" direction="in"/>
<pin name="PGND" direction="pas"/>
<pin name="SGND" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM2623LD">
<pin name="VDD" direction="pwr"/>
<pin name="FREQ" direction="in"/>
<pin name="BOOT" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="SGND" direction="pas"/>
<pin name="PGND_2" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="SW_2" direction="out"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM2623MM">
<pin name="VDD" direction="pwr"/>
<pin name="FB" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="FREQ" direction="in"/>
<pin name="BOOT" direction="in"/>
<pin name="PGND" direction="pas"/>
<pin name="SGND" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM26400YMH">
<pin name="PVIN_2" direction="pwr"/>
<pin name="PVIN_3" direction="pwr"/>
<pin name="PVIN_4" direction="pwr"/>
<pin name="PVIN" direction="pwr"/>
<pin name="AVIN" direction="pwr"/>
<pin name="FB1" direction="in"/>
<pin name="FB2" direction="in"/>
<pin name="SS1" direction="in"/>
<pin name="SS2" direction="in"/>
<pin name="EN1" direction="in"/>
<pin name="EN2" direction="in"/>
<pin name="BST1" direction="in"/>
<pin name="BST2" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="SW1" direction="out"/>
<pin name="SW2" direction="out"/>
</symbol>
<symbol name="LM26400YSD">
<pin name="AVIN" direction="pwr"/>
<pin name="PVIN_2" direction="pwr"/>
<pin name="PVIN_3" direction="pwr"/>
<pin name="PVIN_4" direction="pwr"/>
<pin name="PVIN" direction="pwr"/>
<pin name="FB1" direction="in"/>
<pin name="FB2" direction="in"/>
<pin name="SS1" direction="in"/>
<pin name="SS2" direction="in"/>
<pin name="EN1" direction="in"/>
<pin name="EN2" direction="in"/>
<pin name="BST1" direction="in"/>
<pin name="BST2" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="SW1" direction="out"/>
<pin name="SW2" direction="out"/>
</symbol>
<symbol name="LM2640MTC-ADJ">
<pin name="IN" direction="pwr"/>
<pin name="2NDFB/~FPWM" direction="in"/>
<pin name="ON/~OFF1" direction="in"/>
<pin name="ON/~OFF2" direction="in"/>
<pin name="~SD" direction="in"/>
<pin name="SYNC" direction="in"/>
<pin name="REF" direction="in"/>
<pin name="SS1" direction="in"/>
<pin name="SS2" direction="in"/>
<pin name="FB1" direction="in"/>
<pin name="FB2" direction="in"/>
<pin name="COMP1" direction="in"/>
<pin name="COMP2" direction="in"/>
<pin name="CBOOT1" direction="in"/>
<pin name="CBOOT2" direction="in"/>
<pin name="CSL1" direction="in"/>
<pin name="CSL2" direction="in"/>
<pin name="LIN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="CSH1" direction="out"/>
<pin name="CSH2" direction="pas"/>
<pin name="SW1" direction="out"/>
<pin name="SW2" direction="out"/>
<pin name="HDRV1" direction="out"/>
<pin name="HDRV2" direction="out"/>
<pin name="LDRV1" direction="out"/>
<pin name="LDRV2" direction="out"/>
</symbol>
<symbol name="LM26420XMH">
<pin name="VIND1_2" direction="pwr"/>
<pin name="VIND1" direction="pwr"/>
<pin name="VIND2_2" direction="pwr"/>
<pin name="VIND2" direction="pwr"/>
<pin name="VINC" direction="pwr"/>
<pin name="EN1" direction="in"/>
<pin name="EN2" direction="in"/>
<pin name="FB1" direction="in"/>
<pin name="FB2" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="PGND_2" direction="pas"/>
<pin name="PGND_3" direction="pas"/>
<pin name="PGND_4" direction="pas"/>
<pin name="AGND" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="PGND1_2" direction="pas"/>
<pin name="PGND1" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="SW1" direction="out"/>
<pin name="SW2" direction="out"/>
</symbol>
<symbol name="LM26420XSQ">
<pin name="VIND1_2" direction="pwr"/>
<pin name="VIND1" direction="pwr"/>
<pin name="VIND2_2" direction="pwr"/>
<pin name="VIND2" direction="pwr"/>
<pin name="VINDC" direction="pwr"/>
<pin name="FB1" direction="in"/>
<pin name="FB2" direction="in"/>
<pin name="EN1" direction="in"/>
<pin name="EN2" direction="in"/>
<pin name="AGND" direction="pas"/>
<pin name="PGND1" direction="pas"/>
<pin name="PGND2" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="SW1" direction="out"/>
<pin name="SW2" direction="out"/>
<pin name="FG1" direction="out"/>
<pin name="FG2" direction="out"/>
</symbol>
<symbol name="LM26420YMH">
<pin name="VIND1_2" direction="pwr"/>
<pin name="VIND1" direction="pwr"/>
<pin name="VIND2_2" direction="pwr"/>
<pin name="VIND2" direction="pwr"/>
<pin name="VINC" direction="pwr"/>
<pin name="EN1" direction="in"/>
<pin name="EN2" direction="in"/>
<pin name="FB1" direction="in"/>
<pin name="FB2" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="PGND_2" direction="pas"/>
<pin name="PGND_3" direction="pas"/>
<pin name="PGND_4" direction="pas"/>
<pin name="AGND" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="PGND1_2" direction="pas"/>
<pin name="PGND1" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="SW1" direction="out"/>
<pin name="SW2" direction="out"/>
</symbol>
<symbol name="LM26420YSQ">
<pin name="VIND1_2" direction="pwr"/>
<pin name="VIND1" direction="pwr"/>
<pin name="VIND2_2" direction="pwr"/>
<pin name="VIND2" direction="pwr"/>
<pin name="VINC" direction="pwr"/>
<pin name="FB1" direction="in"/>
<pin name="FB2" direction="in"/>
<pin name="EN1" direction="in"/>
<pin name="EN2" direction="in"/>
<pin name="AGND" direction="pas"/>
<pin name="PGND1" direction="pas"/>
<pin name="PGND2" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="SW1" direction="out"/>
<pin name="SW2" direction="out"/>
<pin name="FG1" direction="out"/>
<pin name="FG2" direction="out"/>
</symbol>
<symbol name="LM2642MTC">
<pin name="VDD1" direction="pwr"/>
<pin name="VDD2" direction="pwr"/>
<pin name="VIN" direction="pwr"/>
<pin name="VLIN5" direction="pwr"/>
<pin name="CBOOT1" direction="in"/>
<pin name="CBOOT2" direction="in"/>
<pin name="COMP1" direction="in"/>
<pin name="COMP2" direction="in"/>
<pin name="FB1" direction="in"/>
<pin name="FB2" direction="in"/>
<pin name="ILIM1" direction="in"/>
<pin name="ILIM2" direction="in"/>
<pin name="KS1" direction="in"/>
<pin name="KS2" direction="in"/>
<pin name="ON/SS1" direction="in"/>
<pin name="ON/SS2" direction="in"/>
<pin name="RSENS2" direction="in"/>
<pin name="RSNS1" direction="in"/>
<pin name="SW1" direction="pas"/>
<pin name="SW2" direction="pas"/>
<pin name="UVDELAY" direction="in"/>
<pin name="PGND" direction="pas"/>
<pin name="SGND" direction="pas"/>
<pin name="HDRV1" direction="out"/>
<pin name="HDRV2" direction="out"/>
<pin name="LDRV1" direction="out"/>
<pin name="LDRV2" direction="out"/>
<pin name="PGOOD1" direction="out"/>
</symbol>
<symbol name="LM2647MTC">
<pin name="VDD" direction="pwr"/>
<pin name="SENSE1" direction="in"/>
<pin name="SENSE2" direction="in"/>
<pin name="COMP1" direction="in"/>
<pin name="COMP2" direction="in"/>
<pin name="ILIM1" direction="in"/>
<pin name="ILIM2" direction="in"/>
<pin name="BOOT1" direction="in"/>
<pin name="BOOT2" direction="in"/>
<pin name="FB1" direction="in"/>
<pin name="FB2" direction="in"/>
<pin name="SS1" direction="in"/>
<pin name="SS2" direction="in"/>
<pin name="FREQ" direction="in"/>
<pin name="FPWM" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="V5" direction="in"/>
<pin name="VIN" direction="in"/>
<pin name="SGND" direction="pas"/>
<pin name="PGND1" direction="pas"/>
<pin name="PGND2" direction="pas"/>
<pin name="HDRV1" direction="out"/>
<pin name="HDRV2" direction="out"/>
<pin name="LDRV1" direction="out"/>
<pin name="LDRV2" direction="out"/>
<pin name="SW1" direction="out"/>
<pin name="SW2" direction="out"/>
<pin name="PGOOD" direction="out"/>
</symbol>
<symbol name="LM26480SQ-AA">
<pin name="AVDD" direction="pwr"/>
<pin name="VIN1" direction="pwr"/>
<pin name="VIN2" direction="pwr"/>
<pin name="SYNC" direction="in"/>
<pin name="FB1" direction="in"/>
<pin name="FB2" direction="in"/>
<pin name="FBL1" direction="in"/>
<pin name="FBL2" direction="in"/>
<pin name="ENSW1" direction="in"/>
<pin name="ENSW2" direction="in"/>
<pin name="ENLDO1" direction="in"/>
<pin name="ENLDO2" direction="in"/>
<pin name="VINLDO1" direction="in"/>
<pin name="VINLDO2" direction="in"/>
<pin name="VINLDO12" direction="in"/>
<pin name="GND_SW1" direction="pas"/>
<pin name="GND_SW2" direction="pas"/>
<pin name="GND_L" direction="pas"/>
<pin name="GND_C" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="LDO1" direction="out"/>
<pin name="LDO2" direction="out"/>
<pin name="SW1" direction="out"/>
<pin name="SW2" direction="out"/>
<pin name="NPOR" direction="out"/>
</symbol>
<symbol name="LM2650M-ADJ">
<pin name="VDD" direction="pwr"/>
<pin name="VIN" direction="pwr"/>
<pin name="PVIN_2" direction="pwr"/>
<pin name="PVIN" direction="pwr"/>
<pin name="FREQ_ADJ" direction="pas"/>
<pin name="SD" direction="in"/>
<pin name="SS" direction="pas"/>
<pin name="FB" direction="in"/>
<pin name="SUB_2" direction="pas"/>
<pin name="SUB" direction="pas"/>
<pin name="BOOT" direction="pwr"/>
<pin name="COMP" direction="in"/>
<pin name="SYNC" direction="in"/>
<pin name="SLEEP_LOGIC" direction="in"/>
<pin name="SLEEP_OUT_ADJ" direction="pas"/>
<pin name="SLEEP_IN_ADJ" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="PGND_2" direction="pas"/>
<pin name="PGND_3" direction="pas"/>
<pin name="PGND_4" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="SW_2" direction="out"/>
<pin name="SW" direction="out"/>
<pin name="EA_OUT" direction="out"/>
</symbol>
<symbol name="LM2651MTC-1.8">
<pin name="VIN_2" direction="in"/>
<pin name="VIN_3" direction="in"/>
<pin name="VIN" direction="in"/>
<pin name="~SD(SS)" direction="in"/>
<pin name="VCB" direction="pas"/>
<pin name="COMP" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="AVIN" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="AGND_2" direction="pas"/>
<pin name="AGND" direction="pas"/>
<pin name="PGND_2" direction="pas"/>
<pin name="PGND_3" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="SW_2" direction="out"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM2651MTC-3.3">
<pin name="VIN_2" direction="in"/>
<pin name="VIN_3" direction="in"/>
<pin name="VIN" direction="in"/>
<pin name="~SD(SS)" direction="in"/>
<pin name="VCB" direction="pas"/>
<pin name="COMP" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="AVIN" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="AGND_2" direction="pas"/>
<pin name="AGND" direction="pas"/>
<pin name="PGND_2" direction="pas"/>
<pin name="PGND_3" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="SW_2" direction="out"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM2651MTC-ADJ">
<pin name="VIN_2" direction="pwr"/>
<pin name="VIN_3" direction="pwr"/>
<pin name="VIN" direction="pwr"/>
<pin name="AVIN" direction="in"/>
<pin name="COMP" direction="pas"/>
<pin name="VCB" direction="pas"/>
<pin name="~SD/SS" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="AGND_2" direction="pas"/>
<pin name="AGND" direction="pas"/>
<pin name="PGND_2" direction="pas"/>
<pin name="PGND_3" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="SW_2" direction="out"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM2653MTC-ADJ">
<pin name="VIN_2" direction="in"/>
<pin name="VIN_3" direction="in"/>
<pin name="VIN" direction="in"/>
<pin name="~SD(SS)" direction="in"/>
<pin name="VCB" direction="pas"/>
<pin name="COMP" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="LDELAY" direction="in"/>
<pin name="AVIN" direction="in"/>
<pin name="AGND" direction="pas"/>
<pin name="PGND_2" direction="pas"/>
<pin name="PGND_3" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="PGOOD" direction="out"/>
<pin name="SW_2" direction="out"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM2655MTC-3.3">
<pin name="PVIN_2" direction="pwr"/>
<pin name="PVIN_3" direction="pwr"/>
<pin name="PVIN_4" direction="pwr"/>
<pin name="PVIN_5" direction="pwr"/>
<pin name="PVIN_6" direction="pwr"/>
<pin name="PVIN" direction="pwr"/>
<pin name="~SD(SS)" direction="in"/>
<pin name="LDELAY" direction="in"/>
<pin name="COMP" direction="in"/>
<pin name="VCB" direction="pas"/>
<pin name="LDR" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="AVIN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="SW_2" direction="out"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM2655MTC-ADJ">
<pin name="PVIN_2" direction="pwr"/>
<pin name="PVIN_3" direction="pwr"/>
<pin name="PVIN_4" direction="pwr"/>
<pin name="PVIN_5" direction="pwr"/>
<pin name="PVIN_6" direction="pwr"/>
<pin name="PVIN" direction="pwr"/>
<pin name="~SD(SS)" direction="in"/>
<pin name="LDELAY" direction="in"/>
<pin name="COMP" direction="in"/>
<pin name="VCB" direction="pas"/>
<pin name="LDR" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="AVIN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="SW_2" direction="out"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM2660M">
<pin name="V+" direction="pwr"/>
<pin name="FC" direction="in"/>
<pin name="LV" direction="in"/>
<pin name="OSC" direction="in"/>
<pin name="CAP+" direction="in"/>
<pin name="CAP-" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM2660MM">
<pin name="V+" direction="pwr"/>
<pin name="CAP+" direction="in"/>
<pin name="CAP-" direction="in"/>
<pin name="OSC" direction="in"/>
<pin name="FC" direction="in"/>
<pin name="LV" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM2662M">
<pin name="V+" direction="pwr"/>
<pin name="FC" direction="in"/>
<pin name="LV" direction="in"/>
<pin name="OSC" direction="in"/>
<pin name="CAP+" direction="in"/>
<pin name="CAP-" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM2663M">
<pin name="V+" direction="pwr"/>
<pin name="CAP+" direction="in"/>
<pin name="CAP-" direction="in"/>
<pin name="SD" direction="in"/>
<pin name="LV" direction="in"/>
<pin name="OSC" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM2664M6">
<pin name="V+" direction="pwr"/>
<pin name="CAP-" direction="in"/>
<pin name="CAP+" direction="in"/>
<pin name="~SD" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM2665M6">
<pin name="V+" direction="pwr"/>
<pin name="SD" direction="in"/>
<pin name="CAP+" direction="in"/>
<pin name="CAP-" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM2670S-12">
<pin name="IN" direction="pwr"/>
<pin name="C_BOOST" direction="pas"/>
<pin name="ON/~OFF" direction="in"/>
<pin name="SYNC" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="SW_OUT" direction="out"/>
</symbol>
<symbol name="LM2670S-3.3">
<pin name="IN" direction="pwr"/>
<pin name="C_BOOST" direction="pas"/>
<pin name="ON/~OFF" direction="in"/>
<pin name="SYNC" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="SW_OUT" direction="out"/>
</symbol>
<symbol name="LM2670S-5.0">
<pin name="IN" direction="pwr"/>
<pin name="C_BOOST" direction="pas"/>
<pin name="ON/~OFF" direction="in"/>
<pin name="SYNC" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="SW_OUT" direction="out"/>
</symbol>
<symbol name="LM2670S-ADJ">
<pin name="IN" direction="pwr"/>
<pin name="C_BOOST" direction="pas"/>
<pin name="ON/~OFF" direction="in"/>
<pin name="SYNC" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="SW_OUT" direction="out"/>
</symbol>
<symbol name="LM2670SD-12">
<pin name="VIN_2" direction="pwr"/>
<pin name="VIN" direction="pwr"/>
<pin name="CB" direction="in"/>
<pin name="SYNC" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="ON/OFF" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="VSW_2" direction="out"/>
<pin name="VSW_3" direction="out"/>
<pin name="VSW" direction="out"/>
</symbol>
<symbol name="LM2670SD-ADJ">
<pin name="VIN_2" direction="pwr"/>
<pin name="VIN" direction="pwr"/>
<pin name="CB" direction="in"/>
<pin name="SYNC" direction="nc"/>
<pin name="FB" direction="in"/>
<pin name="ON/~OFF" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="VSW_2" direction="out"/>
<pin name="VSW_3" direction="out"/>
<pin name="VSW" direction="out"/>
</symbol>
<symbol name="LM2670T-ADJ">
<pin name="INPUT" direction="out"/>
<pin name="C_BOOST" direction="pas"/>
<pin name="*ON-OFF" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="SYNC" direction="in"/>
<pin name="FEEDBACK" direction="in"/>
<pin name="SW_OUTPUT" direction="in"/>
</symbol>
<symbol name="LM2671M-12">
<pin name="VIN" direction="pwr"/>
<pin name="CB" direction="in"/>
<pin name="SS" direction="in"/>
<pin name="SYNC" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="ON/~OFF" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM2671M-3.3">
<pin name="VIN" direction="pwr"/>
<pin name="CB" direction="in"/>
<pin name="SS" direction="in"/>
<pin name="SYNC" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="ON/~OFF" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM2671M-5.0">
<pin name="VIN" direction="pwr"/>
<pin name="CB" direction="in"/>
<pin name="SS" direction="in"/>
<pin name="SYNC" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="ON/~OFF" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM2671M-ADJ">
<pin name="VIN" direction="pwr"/>
<pin name="CB" direction="in"/>
<pin name="SS" direction="in"/>
<pin name="SYNC" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="ON/~OFF" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM2671N-3.3">
<pin name="VIN" direction="pwr"/>
<pin name="CB" direction="in"/>
<pin name="SS" direction="in"/>
<pin name="SYNC" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="ON/~OFF" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM2671N-5.0">
<pin name="VIN" direction="pwr"/>
<pin name="CB" direction="in"/>
<pin name="SS" direction="in"/>
<pin name="SYNC" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="ON/~OFF" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM2671N-ADJ">
<pin name="VIN" direction="pwr"/>
<pin name="CB" direction="in"/>
<pin name="SS" direction="in"/>
<pin name="SYNC" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="ON/~OFF" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM2672M-12">
<pin name="VIN" direction="pwr"/>
<pin name="CB" direction="in"/>
<pin name="SS" direction="in"/>
<pin name="SYNC" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="ON/~OFF" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VSW" direction="out"/>
</symbol>
<symbol name="LM2672M-3.3">
<pin name="VIN" direction="pwr"/>
<pin name="SYNC" direction="pas"/>
<pin name="VSW" direction="pas"/>
<pin name="SS" direction="pas"/>
<pin name="CB" direction="pas"/>
<pin name="FB" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="ON/~OFF" direction="pas"/>
</symbol>
<symbol name="LM2672M-5.0">
<pin name="VIN" direction="pwr"/>
<pin name="SYNC" direction="pas"/>
<pin name="VSW" direction="pas"/>
<pin name="SS" direction="pas"/>
<pin name="CB" direction="pas"/>
<pin name="FB" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="ON/~OFF" direction="pas"/>
</symbol>
<symbol name="LM2672M-ADJ">
<pin name="VIN" direction="pwr"/>
<pin name="CB" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="SS" direction="in"/>
<pin name="SYNC" direction="in"/>
<pin name="ON/~OFF" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VSW" direction="out"/>
</symbol>
<symbol name="LM2672N-3.3">
<pin name="VIN" direction="pwr"/>
<pin name="CB" direction="in"/>
<pin name="SS" direction="in"/>
<pin name="SYNC" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="ON/~OFF" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VSW" direction="out"/>
</symbol>
<symbol name="LM2672N-5.0">
<pin name="VIN" direction="pwr"/>
<pin name="CB" direction="in"/>
<pin name="SS" direction="in"/>
<pin name="SYNC" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="ON/~OFF" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VSW" direction="out"/>
</symbol>
<symbol name="LM2672N-ADJ">
<pin name="VIN" direction="pwr"/>
<pin name="CB" direction="in"/>
<pin name="SS" direction="in"/>
<pin name="SYNC" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="ON/~OFF" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VSW" direction="out"/>
</symbol>
<symbol name="LM2673S-12">
<pin name="VIN" direction="pwr"/>
<pin name="BOOST" direction="in"/>
<pin name="CL_ADJ" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="SS" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="TAB" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM2673S-3.3">
<pin name="IN" direction="pwr"/>
<pin name="FB" direction="in"/>
<pin name="SS" direction="in"/>
<pin name="C_BOOST" direction="in"/>
<pin name="CURRENT_ADJ" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="SW_OUT" direction="out"/>
</symbol>
<symbol name="LM2673S-5.0">
<pin name="IN" direction="pwr"/>
<pin name="FB" direction="in"/>
<pin name="SS" direction="in"/>
<pin name="C_BOOST" direction="in"/>
<pin name="CURRENT_ADJ" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="SW_OUT" direction="out"/>
</symbol>
<symbol name="LM2673S-ADJ">
<pin name="IN" direction="pwr"/>
<pin name="FB" direction="in"/>
<pin name="SS" direction="in"/>
<pin name="C_BOOST" direction="in"/>
<pin name="CURRENT_ADJ" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="SW_OUT" direction="out"/>
</symbol>
<symbol name="LM2673SD-3.3">
<pin name="VIN_2" direction="in"/>
<pin name="VIN" direction="in"/>
<pin name="BOOST" direction="pas"/>
<pin name="NC_2" direction="pas"/>
<pin name="CL_ADJ" direction="pas"/>
<pin name="FB" direction="pas"/>
<pin name="THER.PAD" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="NC_3" direction="pas"/>
<pin name="NC_4" direction="pas"/>
<pin name="NC" direction="pas"/>
<pin name="SW_2" direction="out"/>
<pin name="SW_3" direction="out"/>
<pin name="SW" direction="out"/>
<pin name="SS" direction="pas"/>
</symbol>
<symbol name="LM2673SD-5.0">
<pin name="VIN_2" direction="in"/>
<pin name="VIN" direction="in"/>
<pin name="BOOST" direction="pas"/>
<pin name="CL_ADJ" direction="pas"/>
<pin name="FB" direction="pas"/>
<pin name="THER_PAD" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="NC_2" direction="pas"/>
<pin name="NC_3" direction="pas"/>
<pin name="NC_4" direction="pas"/>
<pin name="NC" direction="pas"/>
<pin name="SW_2" direction="out"/>
<pin name="SW_3" direction="out"/>
<pin name="SW" direction="out"/>
<pin name="SS" direction="pas"/>
</symbol>
<symbol name="LM2673SD-ADJ">
<pin name="VIN_2" direction="in"/>
<pin name="VIN" direction="in"/>
<pin name="BOOST" direction="pas"/>
<pin name="CL_ADJ" direction="pas"/>
<pin name="FB" direction="pas"/>
<pin name="THER_PAD" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="NC_2" direction="pas"/>
<pin name="NC_3" direction="pas"/>
<pin name="NC_4" direction="pas"/>
<pin name="NC" direction="pas"/>
<pin name="SW_2" direction="out"/>
<pin name="SW_3" direction="out"/>
<pin name="SW" direction="out"/>
<pin name="SS" direction="pas"/>
</symbol>
<symbol name="LM2673T-12">
<pin name="VIN" direction="in"/>
<pin name="BOOST" direction="pas"/>
<pin name="CL_ADJ" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="FB" direction="pas"/>
<pin name="SS" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM2673T-3.3">
<pin name="INPUT" direction="pas"/>
<pin name="C_BOOST" direction="pas"/>
<pin name="SOFTSTART" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="CURRENT_ADJ" direction="in"/>
<pin name="FEEDBACK" direction="in"/>
<pin name="SW_OUTPUT" direction="out"/>
</symbol>
<symbol name="LM2673T-5.0">
<pin name="VIN" direction="in"/>
<pin name="BOOST" direction="pas"/>
<pin name="CL_ADJ" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="FB" direction="pas"/>
<pin name="SS" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM2673T-ADJ">
<pin name="VIN" direction="in"/>
<pin name="BOOST" direction="pas"/>
<pin name="CL_ADJ" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="FB" direction="pas"/>
<pin name="SS" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM2674LD-3.3">
<pin name="VIN" direction="pwr"/>
<pin name="ON/OFF" direction="in"/>
<pin name="CB" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC_6" direction="nc"/>
<pin name="NC_7" direction="nc"/>
<pin name="NC_8" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="VSW_2" direction="out"/>
<pin name="VSW" direction="out"/>
</symbol>
<symbol name="LM2674LD-ADJ">
<pin name="VIN" direction="pwr"/>
<pin name="ON/OFF" direction="in"/>
<pin name="CB" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC_6" direction="nc"/>
<pin name="NC_7" direction="nc"/>
<pin name="NC_8" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="VSW_2" direction="out"/>
<pin name="VSW" direction="out"/>
</symbol>
<symbol name="LM2674M-12">
<pin name="VIN" direction="in"/>
<pin name="CB" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="ON/~OFF" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="VSW" direction="out"/>
</symbol>
<symbol name="LM2674M-3.3">
<pin name="VIN" direction="pwr"/>
<pin name="ON/~OFF" direction="in"/>
<pin name="CB" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="VSW" direction="out"/>
</symbol>
<symbol name="LM2674M-5.0">
<pin name="VIN" direction="pwr"/>
<pin name="CB" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="ON/~OFF" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="VSW" direction="out"/>
</symbol>
<symbol name="LM2674M-ADJ">
<pin name="VIN" direction="pwr"/>
<pin name="CB" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="ON/~OFF" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="VSW" direction="out"/>
</symbol>
<symbol name="LM2674N-3.3">
<pin name="VIN" direction="pwr"/>
<pin name="ON/~OFF" direction="in"/>
<pin name="CB" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="VSW" direction="out"/>
</symbol>
<symbol name="LM2674N-5.0">
<pin name="VIN" direction="pwr"/>
<pin name="ON/~OFF" direction="in"/>
<pin name="CB" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="VSW" direction="out"/>
</symbol>
<symbol name="LM2674N-ADJ">
<pin name="VIN" direction="pwr"/>
<pin name="ON/~OFF" direction="in"/>
<pin name="CB" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="VSW" direction="out"/>
</symbol>
<symbol name="LM2675LD-5.0">
<pin name="VIN" direction="pwr"/>
<pin name="ON/OFF" direction="in"/>
<pin name="CB" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC_6" direction="nc"/>
<pin name="NC_7" direction="nc"/>
<pin name="NC_8" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="VSW_2" direction="out"/>
<pin name="VSW" direction="out"/>
</symbol>
<symbol name="LM2675LD-ADJ">
<pin name="BOOST" direction="pas"/>
<pin name="VIN" direction="in"/>
<pin name="FB" direction="pas"/>
<pin name="ON/~OFF" direction="pas"/>
<pin name="EP" direction="pas"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="NC_2" direction="pas"/>
<pin name="NC_3" direction="pas"/>
<pin name="NC_4" direction="pas"/>
<pin name="NC_5" direction="pas"/>
<pin name="NC_6" direction="pas"/>
<pin name="NC_7" direction="pas"/>
<pin name="NC_8" direction="pas"/>
<pin name="NC" direction="pas"/>
<pin name="SW_2" direction="out"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM2675M-12">
<pin name="VIN" direction="in"/>
<pin name="BOOST" direction="pas"/>
<pin name="ON/~OFF" direction="pas"/>
<pin name="FB" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="NC_2" direction="pas"/>
<pin name="NC" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM2675M-3.3">
<pin name="VIN" direction="pwr"/>
<pin name="CB" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="ON/~OFF" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="VSW" direction="out"/>
</symbol>
<symbol name="LM2675M-5.0">
<pin name="VIN" direction="pwr"/>
<pin name="CB" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="ON/~OFF" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="VSW" direction="out"/>
</symbol>
<symbol name="LM2675M-ADJ">
<pin name="VIN" direction="pwr"/>
<pin name="CB" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="ON/~OFF" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="VSW" direction="out"/>
</symbol>
<symbol name="LM2675N-12">
<pin name="BOOST" direction="pas"/>
<pin name="VIN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="NC_2" direction="pas"/>
<pin name="NC" direction="pas"/>
<pin name="FB" direction="pas"/>
<pin name="ON/~OFF" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM2675N-3.3">
<pin name="BOOST" direction="pas"/>
<pin name="VIN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="NC_2" direction="pas"/>
<pin name="NC" direction="pas"/>
<pin name="FB" direction="pas"/>
<pin name="ON/~OFF" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM2675N-5.0">
<pin name="BOOST" direction="pas"/>
<pin name="VIN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="NC_2" direction="pas"/>
<pin name="NC" direction="pas"/>
<pin name="FB" direction="pas"/>
<pin name="ON/~OFF" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM2675N-ADJ">
<pin name="BOOST" direction="pas"/>
<pin name="VIN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="NC_2" direction="pas"/>
<pin name="NC" direction="pas"/>
<pin name="FB" direction="pas"/>
<pin name="ON/~OFF" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM2676S-12">
<pin name="VIN" direction="in"/>
<pin name="BOOST" direction="pas"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="N.C." direction="pas"/>
<pin name="FB" direction="pas"/>
<pin name="ON/~OFF" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM2676S-3.3">
<pin name="VIN" direction="in"/>
<pin name="BOOST" direction="pas"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="N.C." direction="pas"/>
<pin name="FB" direction="pas"/>
<pin name="ON/~OFF" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM2676S-5.0">
<pin name="VIN" direction="in"/>
<pin name="BOOST" direction="pas"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="N.C." direction="pas"/>
<pin name="FB" direction="pas"/>
<pin name="ON/~OFF" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM2676S-ADJ">
<pin name="VIN" direction="in"/>
<pin name="BOOST" direction="pas"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="N.C." direction="pas"/>
<pin name="FB" direction="pas"/>
<pin name="ON/~OFF" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM2676SD-12">
<pin name="VIN_2" direction="in"/>
<pin name="VIN" direction="in"/>
<pin name="BOOST" direction="pas"/>
<pin name="FB" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="EP" direction="pas"/>
<pin name="NC_2" direction="pas"/>
<pin name="NC_3" direction="pas"/>
<pin name="NC_4" direction="pas"/>
<pin name="NC_5" direction="pas"/>
<pin name="NC" direction="pas"/>
<pin name="ON/~OFF" direction="pas"/>
<pin name="SW_2" direction="out"/>
<pin name="SW_3" direction="out"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM2676SD-3.3">
<pin name="VIN_2" direction="in"/>
<pin name="VIN" direction="in"/>
<pin name="BOOST" direction="pas"/>
<pin name="FB" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="EP" direction="pas"/>
<pin name="NC_2" direction="pas"/>
<pin name="NC_3" direction="pas"/>
<pin name="NC_4" direction="pas"/>
<pin name="NC_5" direction="pas"/>
<pin name="NC" direction="pas"/>
<pin name="ON/~OFF" direction="pas"/>
<pin name="SW_2" direction="out"/>
<pin name="SW_3" direction="out"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM2676SD-5.0">
<pin name="VIN_2" direction="pwr"/>
<pin name="VIN" direction="pwr"/>
<pin name="CD" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="ON/~OFF" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="VSW_2" direction="out"/>
<pin name="VSW_3" direction="out"/>
<pin name="VSW" direction="out"/>
</symbol>
<symbol name="LM2676SD-ADJ">
<pin name="VIN_2" direction="in"/>
<pin name="VIN" direction="in"/>
<pin name="BOOST" direction="pas"/>
<pin name="FB" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="EP" direction="pas"/>
<pin name="NC_2" direction="pas"/>
<pin name="NC_3" direction="pas"/>
<pin name="NC_4" direction="pas"/>
<pin name="NC_5" direction="pas"/>
<pin name="NC" direction="pas"/>
<pin name="ON/~OFF" direction="pas"/>
<pin name="SW_2" direction="out"/>
<pin name="SW_3" direction="out"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM2676T-12">
<pin name="VIN" direction="in"/>
<pin name="BOOST" direction="pas"/>
<pin name="ON/OFF" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="NC" direction="nc"/>
<pin name="FB" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM2676T-3.3">
<pin name="VIN" direction="in"/>
<pin name="BOOST" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="N.C." direction="pas"/>
<pin name="ON/~OFF" direction="pas"/>
<pin name="FB" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM2676T-5.0">
<pin name="VIN" direction="in"/>
<pin name="BOOST" direction="pas"/>
<pin name="ON/OFF" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="NC" direction="nc"/>
<pin name="FB" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM2676T-ADJ">
<pin name="VIN" direction="in"/>
<pin name="BOOST" direction="pas"/>
<pin name="ON/OFF" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="NC" direction="nc"/>
<pin name="FB" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM2677S-12">
<pin name="VIN" direction="in"/>
<pin name="BOOST" direction="pas"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="SYNC" direction="pas"/>
<pin name="FB" direction="pas"/>
<pin name="ON/~OFF" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM2677S-3.3">
<pin name="VIN" direction="in"/>
<pin name="BOOST" direction="pas"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="SYNC" direction="pas"/>
<pin name="FB" direction="pas"/>
<pin name="ON/~OFF" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM2677S-5.0">
<pin name="VIN" direction="in"/>
<pin name="BOOST" direction="pas"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="SYNC" direction="pas"/>
<pin name="FB" direction="pas"/>
<pin name="ON/~OFF" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM2677S-ADJ">
<pin name="VIN" direction="in"/>
<pin name="BOOST" direction="pas"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="SYNC" direction="pas"/>
<pin name="FB" direction="pas"/>
<pin name="ON/~OFF" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM2677SD-3.3">
<pin name="VIN_2" direction="in"/>
<pin name="VIN" direction="in"/>
<pin name="BOOST" direction="pas"/>
<pin name="FB" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="EP" direction="pas"/>
<pin name="NC_2" direction="pas"/>
<pin name="NC_3" direction="pas"/>
<pin name="NC_4" direction="pas"/>
<pin name="NC" direction="pas"/>
<pin name="SYNC" direction="pas"/>
<pin name="ON/~OFF" direction="pas"/>
<pin name="SW_2" direction="out"/>
<pin name="SW_3" direction="out"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM2677SD-ADJ">
<pin name="VIN_2" direction="in"/>
<pin name="VIN" direction="in"/>
<pin name="BOOST" direction="pas"/>
<pin name="FB" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="EP" direction="pas"/>
<pin name="NC_2" direction="pas"/>
<pin name="NC_3" direction="pas"/>
<pin name="NC_4" direction="pas"/>
<pin name="NC" direction="pas"/>
<pin name="SYNC" direction="pas"/>
<pin name="ON/~OFF" direction="pas"/>
<pin name="SW_2" direction="out"/>
<pin name="SW_3" direction="out"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM2677T-3.3">
<pin name="VIN" direction="in"/>
<pin name="BOOST" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="SYNC" direction="pas"/>
<pin name="ON/~OFF" direction="pas"/>
<pin name="FB" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM2677T-5.0">
<pin name="VIN" direction="in"/>
<pin name="BOOST" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="SYNC" direction="pas"/>
<pin name="ON/~OFF" direction="pas"/>
<pin name="FB" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM2677T-ADJ">
<pin name="VIN" direction="in"/>
<pin name="BOOST" direction="pas"/>
<pin name="SS" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="SYNC" direction="pas"/>
<pin name="FB" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM2678S-12">
<pin name="VIN" direction="in"/>
<pin name="BOOST" direction="pas"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="N.C." direction="pas"/>
<pin name="FB" direction="pas"/>
<pin name="ON/~OFF" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM2678S-3.3">
<pin name="VIN" direction="in"/>
<pin name="BOOST" direction="pas"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="N.C." direction="pas"/>
<pin name="FB" direction="pas"/>
<pin name="ON/~OFF" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM2678S-5.0">
<pin name="VIN" direction="in"/>
<pin name="BOOST" direction="pas"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="N.C." direction="pas"/>
<pin name="FB" direction="pas"/>
<pin name="ON/~OFF" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM2678S-ADJ">
<pin name="VIN" direction="pwr"/>
<pin name="FB" direction="in"/>
<pin name="C_BOOST" direction="in"/>
<pin name="ON/~OFF" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="SW_IN" direction="out"/>
</symbol>
<symbol name="LM2678SD-5.0">
<pin name="VIN_2" direction="in"/>
<pin name="VIN" direction="in"/>
<pin name="BOOST" direction="pas"/>
<pin name="FB" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="EP" direction="pas"/>
<pin name="NC_2" direction="pas"/>
<pin name="NC_3" direction="pas"/>
<pin name="NC_4" direction="pas"/>
<pin name="NC_5" direction="pas"/>
<pin name="NC" direction="pas"/>
<pin name="ON/~OFF" direction="pas"/>
<pin name="SW_2" direction="out"/>
<pin name="SW_3" direction="out"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM2678SD-ADJ">
<pin name="VIN_2" direction="in"/>
<pin name="VIN" direction="in"/>
<pin name="BOOST" direction="pas"/>
<pin name="FB" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="EP" direction="pas"/>
<pin name="NC_2" direction="pas"/>
<pin name="NC_3" direction="pas"/>
<pin name="NC_4" direction="pas"/>
<pin name="NC_5" direction="pas"/>
<pin name="NC" direction="pas"/>
<pin name="ON/~OFF" direction="pas"/>
<pin name="SW_2" direction="out"/>
<pin name="SW_3" direction="out"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM2678T-12">
<pin name="VIN" direction="in"/>
<pin name="BOOST" direction="pas"/>
<pin name="SS" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="NC" direction="nc"/>
<pin name="FB" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM2678T-3.3">
<pin name="VIN" direction="in"/>
<pin name="BOOST" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="N.C." direction="pas"/>
<pin name="ON/~OFF" direction="pas"/>
<pin name="FB" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM2678T-5.0">
<pin name="VIN" direction="in"/>
<pin name="BOOST" direction="pas"/>
<pin name="SS" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="NC" direction="nc"/>
<pin name="FB" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM2678T-ADJ">
<pin name="VIN" direction="in"/>
<pin name="BOOST" direction="pas"/>
<pin name="SS" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="NC" direction="nc"/>
<pin name="FB" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM2679S-12">
<pin name="VIN" direction="in"/>
<pin name="BOOST" direction="pas"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="CURRENT_ADJ" direction="pas"/>
<pin name="FB" direction="pas"/>
<pin name="SOFTSTART" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM2679S-3.3">
<pin name="VIN" direction="in"/>
<pin name="BOOST" direction="pas"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="CURRENT_ADJ" direction="pas"/>
<pin name="FB" direction="pas"/>
<pin name="SOFTSTART" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM2679S-5.0">
<pin name="VIN" direction="pwr"/>
<pin name="SS" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="C__BOOST" direction="in"/>
<pin name="CURRENT_ADJ" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="SW_OUT" direction="out"/>
</symbol>
<symbol name="LM2679S-ADJ">
<pin name="VIN" direction="pwr"/>
<pin name="SS" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="C__BOOST" direction="in"/>
<pin name="CURRENT_ADJ" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="SW_OUT" direction="out"/>
</symbol>
<symbol name="LM2679SD-5.0">
<pin name="VIN_2" direction="in"/>
<pin name="VIN" direction="in"/>
<pin name="BOOST" direction="pas"/>
<pin name="FB" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="EP" direction="pas"/>
<pin name="NC_2" direction="pas"/>
<pin name="NC_3" direction="pas"/>
<pin name="NC_4" direction="pas"/>
<pin name="CURRENT_ADJ" direction="pas"/>
<pin name="NC" direction="pas"/>
<pin name="SOFTSTART" direction="pas"/>
<pin name="SW_2" direction="out"/>
<pin name="SW_3" direction="out"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM2679SD-ADJ">
<pin name="VIN_2" direction="in"/>
<pin name="VIN" direction="in"/>
<pin name="BOOST" direction="pas"/>
<pin name="FB" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="EP" direction="pas"/>
<pin name="NC_2" direction="pas"/>
<pin name="NC_3" direction="pas"/>
<pin name="NC_4" direction="pas"/>
<pin name="CURRENT_ADJ" direction="pas"/>
<pin name="NC" direction="pas"/>
<pin name="SOFTSTART" direction="pas"/>
<pin name="SW_2" direction="out"/>
<pin name="SW_3" direction="out"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM2679T-12">
<pin name="VIN" direction="in"/>
<pin name="BOOST" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="CURRENT_ADJ" direction="pas"/>
<pin name="SOFTSTART" direction="pas"/>
<pin name="FB" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM2679T-3.3">
<pin name="VIN" direction="in"/>
<pin name="BOOST" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="CURRENT_ADJ" direction="pas"/>
<pin name="SOFTSTART" direction="pas"/>
<pin name="FB" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM2679T-5.0">
<pin name="VIN" direction="in"/>
<pin name="BOOST" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="CURRENT_ADJ" direction="pas"/>
<pin name="SOFTSTART" direction="pas"/>
<pin name="FB" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM2679T-ADJ">
<pin name="VIN" direction="in"/>
<pin name="BOOST" direction="pas"/>
<pin name="CL_ADJ" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="FB" direction="pas"/>
<pin name="SS" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM2682MM">
<pin name="VIN" direction="in"/>
<pin name="C1-_" direction="pas"/>
<pin name="C1+" direction="pas"/>
<pin name="C2-_" direction="pas"/>
<pin name="C2+" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="NC" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LM2687MM">
<pin name="VIN" direction="pwr"/>
<pin name="CAP+" direction="pas"/>
<pin name="CAP-" direction="pas"/>
<pin name="~SD" direction="in"/>
<pin name="VFB" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VNEG" direction="out"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LM2694MT">
<pin name="VCC" direction="pwr"/>
<pin name="VIN" direction="pwr"/>
<pin name="BOOST" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="ISEN" direction="in"/>
<pin name="RON/SD" direction="in"/>
<pin name="SS" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="RTN" direction="pas"/>
<pin name="SGND" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM2694SD">
<pin name="VIN" direction="in"/>
<pin name="BOOST" direction="pas"/>
<pin name="RTN" direction="pas"/>
<pin name="VCC" direction="pas"/>
<pin name="EP" direction="pas"/>
<pin name="SGND" direction="pas"/>
<pin name="FB" direction="pas"/>
<pin name="SS" direction="pas"/>
<pin name="RON/SD" direction="pas"/>
<pin name="ISEN" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM2695MH">
<pin name="VIN" direction="in"/>
<pin name="BST" direction="pas"/>
<pin name="ISEN" direction="pas"/>
<pin name="RTN" direction="pas"/>
<pin name="VCC" direction="pas"/>
<pin name="SGND" direction="pas"/>
<pin name="EP" direction="pas"/>
<pin name="NC_2" direction="pas"/>
<pin name="NC_3" direction="pas"/>
<pin name="NC_4" direction="pas"/>
<pin name="NC" direction="pas"/>
<pin name="FB" direction="pas"/>
<pin name="SS" direction="pas"/>
<pin name="RON/SD" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM2696MXA">
<pin name="PVIN_2" direction="pwr"/>
<pin name="PVIN_3" direction="pwr"/>
<pin name="PVIN" direction="pwr"/>
<pin name="AVIN" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="SD" direction="in"/>
<pin name="SS" direction="in"/>
<pin name="RON" direction="in"/>
<pin name="BOOT" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="SW_2" direction="out"/>
<pin name="SW_3" direction="out"/>
<pin name="SW" direction="out"/>
<pin name="EXTVCC" direction="out"/>
<pin name="PGOOD" direction="out"/>
</symbol>
<symbol name="LM2698MM-ADJ">
<pin name="VC" direction="pas"/>
<pin name="VIN" direction="in"/>
<pin name="FB" direction="pas"/>
<pin name="~SD" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="NC" direction="pas"/>
<pin name="FSLCT" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM26CIM5-PHA">
<pin name="V+" direction="pwr"/>
<pin name="HYST" direction="in"/>
<pin name="VTEMP" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="~OS" direction="out"/>
</symbol>
<symbol name="LM26CIM5-RPA">
<pin name="V+" direction="pwr"/>
<pin name="HYST" direction="in"/>
<pin name="~OS" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VTEMP" direction="out"/>
</symbol>
<symbol name="LM26CIM5-SHA">
<pin name="V+" direction="pwr"/>
<pin name="HYST" direction="in"/>
<pin name="VTEMP" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="~OS" direction="out"/>
</symbol>
<symbol name="LM26CIM5-SPA">
<pin name="V+" direction="pwr"/>
<pin name="HYST" direction="in"/>
<pin name="VTEMP" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="~OS" direction="out"/>
</symbol>
<symbol name="LM26CIM5-TPA">
<pin name="V+" direction="pwr"/>
<pin name="HYST" direction="in"/>
<pin name="~OS" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VTEMP" direction="out"/>
</symbol>
<symbol name="LM26CIM5-VHA">
<pin name="V+" direction="pwr"/>
<pin name="HYST" direction="in"/>
<pin name="VTEMP" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OS/~OS" direction="out"/>
</symbol>
<symbol name="LM26CIM5-VPA">
<pin name="V+" direction="pwr"/>
<pin name="HYST" direction="in"/>
<pin name="VTEMP" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OS/~OS" direction="out"/>
</symbol>
<symbol name="LM26CIM5-XPA">
<pin name="V+" direction="pwr"/>
<pin name="HYST" direction="in"/>
<pin name="~OS" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VTEMP" direction="out"/>
</symbol>
<symbol name="LM26CIM5-YHA">
<pin name="V+" direction="pwr"/>
<pin name="HYST" direction="in"/>
<pin name="VTEMP" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OS/~OS" direction="out"/>
</symbol>
<symbol name="LM2700LD-ADJ">
<pin name="VIN" direction="pwr"/>
<pin name="VC" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="~SHDN" direction="in"/>
<pin name="FSLCT" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="AGND" direction="pas"/>
<pin name="PGND_2" direction="pas"/>
<pin name="PGND_3" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="SW_2" direction="out"/>
<pin name="SW_3" direction="out"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM2700MT-ADJ">
<pin name="VIN" direction="pwr"/>
<pin name="VC" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="~SHDN" direction="in"/>
<pin name="FSLCT" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="AGND" direction="pas"/>
<pin name="PGND_2" direction="pas"/>
<pin name="PGND_3" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="SW_2" direction="out"/>
<pin name="SW_3" direction="out"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM2703MF-ADJ">
<pin name="VIN" direction="pwr"/>
<pin name="SW" direction="in"/>
<pin name="~SHDN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="FB" direction="out"/>
</symbol>
<symbol name="LM2704MF-ADJ">
<pin name="VIN" direction="pwr"/>
<pin name="FB" direction="in"/>
<pin name="~SHDN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM2705MF-ADJ">
<pin name="VIN" direction="pwr"/>
<pin name="FB" direction="in"/>
<pin name="~SHDN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM27213SQ">
<pin name="VDD" direction="pwr"/>
<pin name="PVDD" direction="pwr"/>
<pin name="CBOOT" direction="in"/>
<pin name="SRCK" direction="in"/>
<pin name="ILIM" direction="in"/>
<pin name="VREF" direction="in"/>
<pin name="CMP" direction="in"/>
<pin name="CMPREF" direction="in"/>
<pin name="SS" direction="in"/>
<pin name="ILIMREF" direction="in"/>
<pin name="CLK_EN" direction="in"/>
<pin name="STP_CPU" direction="in"/>
<pin name="DE_EN" direction="in"/>
<pin name="XPOK" direction="in"/>
<pin name="SENSE" direction="in"/>
<pin name="VBOOT" direction="in"/>
<pin name="V1R7" direction="in"/>
<pin name="SLP" direction="in"/>
<pin name="VOVP" direction="in"/>
<pin name="VSLP" direction="in"/>
<pin name="VRON" direction="in"/>
<pin name="P_Z0" direction="in"/>
<pin name="P_Z1" direction="in"/>
<pin name="P_Z2" direction="in"/>
<pin name="VID5" direction="in"/>
<pin name="VID4" direction="in"/>
<pin name="VID3" direction="in"/>
<pin name="VID2" direction="in"/>
<pin name="VID1" direction="in"/>
<pin name="VID0" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC_6" direction="nc"/>
<pin name="NC_7" direction="nc"/>
<pin name="NC_8" direction="nc"/>
<pin name="NC_9" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="DGND" direction="pas"/>
<pin name="SGND" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="HG" direction="out"/>
<pin name="LG" direction="nc"/>
<pin name="SW" direction="out"/>
<pin name="VDAC" direction="out"/>
<pin name="VSTP" direction="out"/>
<pin name="PGOOD" direction="out"/>
</symbol>
<symbol name="LM27222M">
<pin name="VCC" direction="pwr"/>
<pin name="CB" direction="in"/>
<pin name="IN" direction="in"/>
<pin name="LEN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="SW" direction="out"/>
<pin name="HG" direction="out"/>
<pin name="LG" direction="out"/>
</symbol>
<symbol name="LM2727MTC">
<pin name="VCC" direction="pwr"/>
<pin name="BOOT" direction="pwr"/>
<pin name="~SD" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="FREQ" direction="in"/>
<pin name="HG" direction="in"/>
<pin name="ISEN" direction="in"/>
<pin name="LG" direction="in"/>
<pin name="SS" direction="in"/>
<pin name="PGND_2" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="SGND" direction="pas"/>
<pin name="EAO" direction="out"/>
<pin name="PWGD" direction="out"/>
</symbol>
<symbol name="LM27313XMF">
<pin name="VIN" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="~SHDN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM2731XMF">
<pin name="VIN" direction="pwr"/>
<pin name="~SD" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM2731YMF">
<pin name="VIN" direction="pwr"/>
<pin name="~SD" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM2733XMF">
<pin name="VIN" direction="pwr"/>
<pin name="~SD" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM2733YMF">
<pin name="VIN" direction="pwr"/>
<pin name="~SD" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM27341MY">
<pin name="AVIN" direction="pwr"/>
<pin name="PVIN_2" direction="pwr"/>
<pin name="PVIN" direction="pwr"/>
<pin name="FB" direction="in"/>
<pin name="BOOST" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="SYNC" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="EP" direction="pas"/>
<pin name="SW_2" direction="out"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM27341QMY">
<pin name="AVIN" direction="pwr"/>
<pin name="PVIN_2" direction="pwr"/>
<pin name="PVIN" direction="pwr"/>
<pin name="FB" direction="in"/>
<pin name="BOOST" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="SYNC" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="EP" direction="pas"/>
<pin name="SW_2" direction="out"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM27341SD">
<pin name="AVIN" direction="pwr"/>
<pin name="PVIN_2" direction="pwr"/>
<pin name="PVIN" direction="pwr"/>
<pin name="FB" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="BOOST" direction="in"/>
<pin name="SYNC" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="EP" direction="pas"/>
<pin name="SW_2" direction="out"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM27342MY">
<pin name="AVIN" direction="pwr"/>
<pin name="PVIN_2" direction="pwr"/>
<pin name="PVIN" direction="pwr"/>
<pin name="FB" direction="in"/>
<pin name="BOOST" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="SYNC" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="EP" direction="pas"/>
<pin name="SW_2" direction="out"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM27342QMY">
<pin name="AVIN" direction="pwr"/>
<pin name="PVIN_2" direction="pwr"/>
<pin name="PVIN" direction="pwr"/>
<pin name="FB" direction="in"/>
<pin name="BOOST" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="SYNC" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="EP" direction="pas"/>
<pin name="SW_2" direction="out"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM27342SD">
<pin name="AVIN" direction="pwr"/>
<pin name="PVIN_2" direction="pwr"/>
<pin name="PVIN" direction="pwr"/>
<pin name="FB" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="BOOST" direction="in"/>
<pin name="SYNC" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="EP" direction="pas"/>
<pin name="SW_2" direction="out"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM2734XMK">
<pin name="VIN" direction="in"/>
<pin name="BOOST" direction="pas"/>
<pin name="FB" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="EN" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM2734XQMK">
<pin name="VIN" direction="pwr"/>
<pin name="BST" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM2734YMK">
<pin name="VIN" direction="pwr"/>
<pin name="EN" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="BOOST" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM2734YQMK">
<pin name="VIN" direction="pwr"/>
<pin name="BST" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM2734ZQSD">
<pin name="VIN" direction="pwr"/>
<pin name="EN" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="BOOST" direction="pas"/>
<pin name="SW" direction="pwr"/>
<pin name="FB" direction="in"/>
<pin name="DAP" direction="pwr"/>
</symbol>
<symbol name="LM2735XMF">
<pin name="VIN" direction="pwr"/>
<pin name="EN" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="SW" direction="pwr"/>
<pin name="FB" direction="in"/>
</symbol>
<symbol name="LM2735XMY">
<pin name="VIN" direction="pwr"/>
<pin name="EN" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="PGND" direction="pas"/>
<pin name="AGND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM2735XQMF">
<pin name="VIN" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM2735XSD">
<pin name="VIN" direction="pwr"/>
<pin name="EN" direction="in"/>
<pin name="PGND" direction="pwr"/>
<pin name="AGND" direction="pwr"/>
<pin name="FB" direction="in"/>
<pin name="DAP" direction="pwr"/>
<pin name="SW" direction="pwr"/>
</symbol>
<symbol name="LM2735YMF">
<pin name="VIN" direction="pwr"/>
<pin name="EN" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="FB" direction="in"/>
<pin name="SW" direction="pwr"/>
</symbol>
<symbol name="LM2735YMY">
<pin name="VIN" direction="pwr"/>
<pin name="EN" direction="in"/>
<pin name="PGND" direction="pwr"/>
<pin name="AGND" direction="pwr"/>
<pin name="NC_2" direction="pas"/>
<pin name="NC" direction="pas"/>
<pin name="FB" direction="in"/>
<pin name="DAP" direction="pwr"/>
<pin name="SW" direction="pwr"/>
</symbol>
<symbol name="LM2735YQMF">
<pin name="VIN" direction="pwr"/>
<pin name="EN" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM2735YSD">
<pin name="VIN" direction="pwr"/>
<pin name="EN" direction="in"/>
<pin name="PGND" direction="pwr"/>
<pin name="AGND" direction="pwr"/>
<pin name="FB" direction="in"/>
<pin name="DAP" direction="pwr"/>
<pin name="SW" direction="pwr"/>
</symbol>
<symbol name="LM2736XMK">
<pin name="VIN" direction="in"/>
<pin name="BOOST" direction="pas"/>
<pin name="FB" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="EN" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM2736YMK">
<pin name="VIN" direction="pwr"/>
<pin name="EN" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="BOOST" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM2737MTC">
<pin name="BOOT" direction="pas"/>
<pin name="LG" direction="out"/>
<pin name="ISEN" direction="pas"/>
<pin name="VCC" direction="pas"/>
<pin name="PGND_2" direction="pas"/>
<pin name="SGND" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="EAO" direction="pas"/>
<pin name="SS" direction="pas"/>
<pin name="FB" direction="pas"/>
<pin name="FREQ" direction="pas"/>
<pin name="EN" direction="pas"/>
<pin name="HG" direction="out"/>
<pin name="PWGD" direction="pas"/>
</symbol>
<symbol name="LM2738XMY">
<pin name="VCC" direction="pwr"/>
<pin name="IN" direction="in"/>
<pin name="BST" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM2738XSD">
<pin name="IN" direction="pwr"/>
<pin name="EN" direction="in"/>
<pin name="VCC" direction="pwr"/>
<pin name="EP" direction="pwr"/>
<pin name="GND_2" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="BST" direction="pas"/>
<pin name="SW" direction="pwr"/>
<pin name="FB" direction="in"/>
</symbol>
<symbol name="LM2738YMY">
<pin name="VCC" direction="pwr"/>
<pin name="IN" direction="in"/>
<pin name="BST" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM2738YSD">
<pin name="IN" direction="pwr"/>
<pin name="EN" direction="in"/>
<pin name="VCC" direction="pwr"/>
<pin name="EP" direction="pwr"/>
<pin name="GND_2" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="BST" direction="pas"/>
<pin name="SW" direction="pwr"/>
<pin name="FB" direction="in"/>
</symbol>
<symbol name="LM2742MTC">
<pin name="BOOT" direction="pas"/>
<pin name="LG" direction="pas"/>
<pin name="ISEN" direction="pas"/>
<pin name="VCC" direction="pas"/>
<pin name="PGND_2" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="SGND" direction="pas"/>
<pin name="EAO" direction="pas"/>
<pin name="SS" direction="pas"/>
<pin name="FB" direction="pas"/>
<pin name="FREQ" direction="pas"/>
<pin name="~SD" direction="pas"/>
<pin name="HG" direction="out"/>
<pin name="PWGD" direction="pas"/>
</symbol>
<symbol name="LM2743MTC">
<pin name="VCC" direction="pwr"/>
<pin name="BOOT" direction="pwr"/>
<pin name="~SD" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="FREQ" direction="in"/>
<pin name="HG" direction="in"/>
<pin name="ISEN" direction="in"/>
<pin name="LG" direction="in"/>
<pin name="SS/TRACK" direction="in"/>
<pin name="PGND_2" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="SGND" direction="pas"/>
<pin name="EAO" direction="out"/>
<pin name="PWGD" direction="out"/>
</symbol>
<symbol name="LM2745MTC">
<pin name="VCC" direction="pwr"/>
<pin name="BOOT" direction="pwr"/>
<pin name="LG" direction="in"/>
<pin name="HG" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="~SD" direction="in"/>
<pin name="ISEN" direction="in"/>
<pin name="SS/TRACK" direction="in"/>
<pin name="FREQ/SYNC" direction="in"/>
<pin name="PGND_2" direction="pas"/>
<pin name="SGND" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="PGOOD" direction="out"/>
<pin name="EAO" direction="out"/>
</symbol>
<symbol name="LM2747MTC">
<pin name="BOOT" direction="pas"/>
<pin name="LG" direction="pas"/>
<pin name="ISEN" direction="pas"/>
<pin name="VCC" direction="pas"/>
<pin name="PGND_2" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="SGND" direction="pas"/>
<pin name="EAO" direction="pas"/>
<pin name="SS/TRACK" direction="pas"/>
<pin name="FB" direction="pas"/>
<pin name="FREQ/SYNC" direction="pas"/>
<pin name="~SD" direction="pas"/>
<pin name="HG" direction="out"/>
<pin name="PWGD" direction="pas"/>
</symbol>
<symbol name="LM2750LD-5.0">
<pin name="VIN_2" direction="in"/>
<pin name="VIN" direction="in"/>
<pin name="C+" direction="out"/>
<pin name="C-" direction="pas"/>
<pin name="FB" direction="pas"/>
<pin name="SD" direction="pas"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT_2" direction="out"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LM2750LD-ADJ">
<pin name="VIN_2" direction="in"/>
<pin name="VIN" direction="in"/>
<pin name="C+" direction="out"/>
<pin name="C-" direction="pas"/>
<pin name="FB" direction="pas"/>
<pin name="SD" direction="pas"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT_2" direction="out"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LM2750SD-5.0">
<pin name="VIN_2" direction="in"/>
<pin name="VIN" direction="in"/>
<pin name="C+" direction="out"/>
<pin name="C-" direction="pas"/>
<pin name="FB" direction="pas"/>
<pin name="SD" direction="pas"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT_2" direction="out"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LM2750SD-ADJ">
<pin name="VIN_2" direction="in"/>
<pin name="VIN" direction="in"/>
<pin name="C+" direction="out"/>
<pin name="C-" direction="pas"/>
<pin name="FB" direction="pas"/>
<pin name="SD" direction="pas"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT_2" direction="out"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LM2751SD-A">
<pin name="VIN" direction="pas"/>
<pin name="CS0" direction="pas"/>
<pin name="C1-" direction="in"/>
<pin name="C2+" direction="in"/>
<pin name="C2-" direction="pas"/>
<pin name="CS1" direction="pas"/>
<pin name="EN" direction="pas"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="in"/>
<pin name="VOUT" direction="out"/>
<pin name="C1+" direction="pas"/>
</symbol>
<symbol name="LM2751SD-B">
<pin name="VIN" direction="pas"/>
<pin name="CS0" direction="pas"/>
<pin name="C1-" direction="in"/>
<pin name="C2+" direction="in"/>
<pin name="C2-" direction="pas"/>
<pin name="CS1" direction="pas"/>
<pin name="EN" direction="pas"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="in"/>
<pin name="VOUT" direction="out"/>
<pin name="C1+" direction="pas"/>
</symbol>
<symbol name="LM2753SD">
<pin name="C1+" direction="pas"/>
<pin name="VIN" direction="out"/>
<pin name="C1-" direction="pas"/>
<pin name="FLASH" direction="pas"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="EP" direction="pas"/>
<pin name="EN" direction="pas"/>
<pin name="IOUT" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LM2754SQ">
<pin name="C1+" direction="pas"/>
<pin name="C1-" direction="pas"/>
<pin name="NC_2" direction="pas"/>
<pin name="C2-" direction="pas"/>
<pin name="NC" direction="pas"/>
<pin name="C2+" direction="pas"/>
<pin name="VIN" direction="in"/>
<pin name="VINSW_2" direction="pas"/>
<pin name="VINSW" direction="pas"/>
<pin name="ISET1" direction="pas"/>
<pin name="ISET2" direction="pas"/>
<pin name="D1" direction="pas"/>
<pin name="EP" direction="pas"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GNDSW" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="D2" direction="pas"/>
<pin name="D3" direction="pas"/>
<pin name="D4" direction="pas"/>
<pin name="SEL" direction="pas"/>
<pin name="TX" direction="pas"/>
<pin name="T/F" direction="pas"/>
<pin name="EN" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LM2755TM">
<pin name="VIN" direction="pwr"/>
<pin name="C1+" direction="in"/>
<pin name="C1-" direction="in"/>
<pin name="C2-" direction="in"/>
<pin name="C2+" direction="in"/>
<pin name="VIO" direction="in"/>
<pin name="SCL" direction="in"/>
<pin name="ADDR" direction="in"/>
<pin name="SDIO" direction="in"/>
<pin name="ISET" direction="in"/>
<pin name="HWEN" direction="in"/>
<pin name="SYNC" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="POUT" direction="out"/>
<pin name="ID1" direction="out"/>
<pin name="ID2" direction="out"/>
<pin name="ID3" direction="out"/>
</symbol>
<symbol name="LM2756TM">
<pin name="VIN" direction="pwr"/>
<pin name="C1+" direction="in"/>
<pin name="C1-" direction="in"/>
<pin name="C2+" direction="in"/>
<pin name="C2-" direction="in"/>
<pin name="HWEN" direction="in"/>
<pin name="SDIO"/>
<pin name="SCL" direction="in"/>
<pin name="ISET" direction="in"/>
<pin name="GND_2" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="VOUT" direction="pwr"/>
<pin name="D1A" direction="pas"/>
<pin name="D2A" direction="pas"/>
<pin name="D3A" direction="pas"/>
<pin name="D4A" direction="pas"/>
<pin name="D53" direction="pas"/>
<pin name="D62" direction="pas"/>
<pin name="D1B" direction="pas"/>
<pin name="D1C" direction="pas"/>
</symbol>
<symbol name="LM2757TM">
<pin name="VIN_2" direction="pwr"/>
<pin name="VIN" direction="pwr"/>
<pin name="C1+" direction="in"/>
<pin name="C1-" direction="in"/>
<pin name="C2+" direction="in"/>
<pin name="C2-" direction="in"/>
<pin name="M0" direction="in"/>
<pin name="M1" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LM2758TL">
<pin name="VIN" direction="pwr"/>
<pin name="ISET" direction="in"/>
<pin name="C1+" direction="in"/>
<pin name="C1-" direction="in"/>
<pin name="C2+" direction="in"/>
<pin name="C2-" direction="in"/>
<pin name="SGND" direction="pwr"/>
<pin name="PGND" direction="pwr"/>
<pin name="LED-" direction="pas"/>
<pin name="EN1" direction="in"/>
<pin name="EN2" direction="in"/>
<pin name="CPOUT" direction="pwr"/>
</symbol>
<symbol name="LM2765M6">
<pin name="V+" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="CAP-_" direction="pas"/>
<pin name="SD" direction="pas"/>
<pin name="VOUT" direction="out"/>
<pin name="CAP+" direction="pas"/>
</symbol>
<symbol name="LM2766M6">
<pin name="V+" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="CAP-_" direction="pas"/>
<pin name="SD" direction="pas"/>
<pin name="VOUT" direction="out"/>
<pin name="CAP+" direction="pas"/>
</symbol>
<symbol name="LM2767M5">
<pin name="V+" direction="pwr"/>
<pin name="CAP-" direction="in"/>
<pin name="CAP+" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LM2771SD">
<pin name="EN" direction="in"/>
<pin name="C1+" direction="pas"/>
<pin name="C1-" direction="pas"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="VOUT_2" direction="out"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LM2794TL">
<pin name="C1+" direction="pas"/>
<pin name="C2+" direction="pas"/>
<pin name="~SD" direction="pas"/>
<pin name="C1-_" direction="pas"/>
<pin name="BRGT" direction="pas"/>
<pin name="ISET" direction="pas"/>
<pin name="VIN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="D4" direction="pas"/>
<pin name="C2-_" direction="pas"/>
<pin name="D1" direction="pas"/>
<pin name="D2" direction="pas"/>
<pin name="D3" direction="pas"/>
<pin name="POUT" direction="out"/>
</symbol>
<symbol name="LM27951SD">
<pin name="C2+" direction="pas"/>
<pin name="C1+" direction="pas"/>
<pin name="D4" direction="pas"/>
<pin name="D3" direction="pas"/>
<pin name="D2" direction="pas"/>
<pin name="D1" direction="pas"/>
<pin name="VIN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="EP" direction="pas"/>
<pin name="ISET" direction="pas"/>
<pin name="EN" direction="pas"/>
<pin name="PWM" direction="pas"/>
<pin name="C2-" direction="pas"/>
<pin name="C1-" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LM27952SD">
<pin name="C2+" direction="pas"/>
<pin name="C1+" direction="pas"/>
<pin name="D4" direction="pas"/>
<pin name="D3" direction="pas"/>
<pin name="D2" direction="pas"/>
<pin name="D1" direction="pas"/>
<pin name="VIN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="EP" direction="pas"/>
<pin name="ISET" direction="pas"/>
<pin name="EN" direction="pas"/>
<pin name="PWM" direction="pas"/>
<pin name="C2-" direction="pas"/>
<pin name="C1-" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LM27964SQ-C">
<pin name="SCL" direction="pas"/>
<pin name="SDIO" direction="pas"/>
<pin name="ISETB" direction="pas"/>
<pin name="D1B" direction="pas"/>
<pin name="D2B" direction="pas"/>
<pin name="DKEY" direction="pas"/>
<pin name="VIO" direction="pas"/>
<pin name="VIN" direction="in"/>
<pin name="ISETK" direction="pas"/>
<pin name="ISETA" direction="pas"/>
<pin name="EP" direction="pas"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="NC_2" direction="pas"/>
<pin name="NC" direction="pas"/>
<pin name="D4A" direction="pas"/>
<pin name="D3A" direction="pas"/>
<pin name="D2A" direction="pas"/>
<pin name="D1A" direction="pas"/>
<pin name="C1_2" direction="pas"/>
<pin name="C2_2" direction="pas"/>
<pin name="C2" direction="pas"/>
<pin name="C1" direction="pas"/>
<pin name="POUT" direction="out"/>
</symbol>
<symbol name="LM27964SQ-I">
<pin name="SCL" direction="pas"/>
<pin name="SDIO" direction="pas"/>
<pin name="ISETB" direction="pas"/>
<pin name="D1B" direction="pas"/>
<pin name="D2B" direction="pas"/>
<pin name="DKEY" direction="pas"/>
<pin name="VIO" direction="pas"/>
<pin name="VIN" direction="in"/>
<pin name="ISETK" direction="pas"/>
<pin name="ISETA" direction="pas"/>
<pin name="EP" direction="pas"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="NC_2" direction="pas"/>
<pin name="NC" direction="pas"/>
<pin name="D4A" direction="pas"/>
<pin name="D3A" direction="pas"/>
<pin name="D2A" direction="pas"/>
<pin name="D1A" direction="pas"/>
<pin name="C1_2" direction="pas"/>
<pin name="C2_2" direction="pas"/>
<pin name="C2" direction="pas"/>
<pin name="C1" direction="pas"/>
<pin name="POUT" direction="out"/>
</symbol>
<symbol name="LM27965SQ">
<pin name="SCL" direction="pas"/>
<pin name="SDIO" direction="pas"/>
<pin name="D1C" direction="pas"/>
<pin name="D1B" direction="pas"/>
<pin name="D2B" direction="pas"/>
<pin name="D3B" direction="pas"/>
<pin name="VIO" direction="pas"/>
<pin name="VIN" direction="in"/>
<pin name="*RESET" direction="pas"/>
<pin name="D5A" direction="pas"/>
<pin name="ISET" direction="pas"/>
<pin name="EP" direction="pas"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="NC_2" direction="pas"/>
<pin name="NC" direction="pas"/>
<pin name="D4A" direction="pas"/>
<pin name="D3A" direction="pas"/>
<pin name="D2A" direction="pas"/>
<pin name="D1A" direction="pas"/>
<pin name="C1_2" direction="pas"/>
<pin name="C2_2" direction="pas"/>
<pin name="C2" direction="pas"/>
<pin name="C1" direction="pas"/>
<pin name="POUT" direction="out"/>
</symbol>
<symbol name="LM27966SQ">
<pin name="SCL" direction="pas"/>
<pin name="SDIO" direction="pas"/>
<pin name="DAUX" direction="pas"/>
<pin name="VIO" direction="pas"/>
<pin name="VIN" direction="in"/>
<pin name="*RESET" direction="pas"/>
<pin name="D5" direction="pas"/>
<pin name="ISET" direction="pas"/>
<pin name="EP" direction="pas"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="NC_2" direction="pas"/>
<pin name="NC_3" direction="pas"/>
<pin name="NC_4" direction="pas"/>
<pin name="NC_5" direction="pas"/>
<pin name="NC" direction="pas"/>
<pin name="D4" direction="pas"/>
<pin name="D3" direction="pas"/>
<pin name="D2" direction="pas"/>
<pin name="D1" direction="pas"/>
<pin name="C1_2" direction="pas"/>
<pin name="C2_2" direction="pas"/>
<pin name="C2" direction="pas"/>
<pin name="C1" direction="pas"/>
<pin name="POUT" direction="out"/>
</symbol>
<symbol name="LM2825HN-ADJ">
<pin name="VIN_2" direction="in"/>
<pin name="VIN_3" direction="in"/>
<pin name="VIN_4" direction="in"/>
<pin name="VIN_5" direction="in"/>
<pin name="VIN_6" direction="in"/>
<pin name="VIN" direction="in"/>
<pin name="SS/~SD_2" direction="pas"/>
<pin name="SS/~SD" direction="pas"/>
<pin name="ADJ" direction="pas"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="NC_2" direction="pas"/>
<pin name="NC_3" direction="pas"/>
<pin name="NC_4" direction="pas"/>
<pin name="NC_5" direction="pas"/>
<pin name="NC" direction="pas"/>
<pin name="VOUT_2" direction="out"/>
<pin name="VOUT_3" direction="out"/>
<pin name="VOUT_4" direction="out"/>
<pin name="VOUT_5" direction="out"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LM2825N-12">
<pin name="IN_2" direction="in"/>
<pin name="IN_3" direction="in"/>
<pin name="IN_4" direction="in"/>
<pin name="IN_5" direction="in"/>
<pin name="IN_6" direction="in"/>
<pin name="IN" direction="in"/>
<pin name="ADJ" direction="pas"/>
<pin name="~SD/SOFT_START" direction="pas"/>
<pin name="~SD/SOFT_START_2" direction="pas"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="OUT_2" direction="out"/>
<pin name="OUT_3" direction="out"/>
<pin name="OUT_4" direction="out"/>
<pin name="OUT_5" direction="out"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM2825N-3.3">
<pin name="IN_2" direction="in"/>
<pin name="IN_3" direction="in"/>
<pin name="IN_4" direction="in"/>
<pin name="IN_5" direction="in"/>
<pin name="IN_6" direction="in"/>
<pin name="IN" direction="in"/>
<pin name="ADJ" direction="pas"/>
<pin name="~SD/SOFT_2" direction="pas"/>
<pin name="~SD/SOFT" direction="pas"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="OUT_2" direction="out"/>
<pin name="OUT_3" direction="out"/>
<pin name="OUT_4" direction="out"/>
<pin name="OUT_5" direction="out"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM2825N-5.0">
<pin name="IN_2" direction="in"/>
<pin name="IN_3" direction="in"/>
<pin name="IN_4" direction="in"/>
<pin name="IN_5" direction="in"/>
<pin name="IN_6" direction="in"/>
<pin name="IN" direction="in"/>
<pin name="ADJ" direction="pas"/>
<pin name="~SD/SOFT_2" direction="pas"/>
<pin name="~SD/SOFT" direction="pas"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="OUT_2" direction="out"/>
<pin name="OUT_3" direction="out"/>
<pin name="OUT_4" direction="out"/>
<pin name="OUT_5" direction="out"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM2825N-ADJ">
<pin name="IN_2" direction="in"/>
<pin name="IN_3" direction="in"/>
<pin name="IN_4" direction="in"/>
<pin name="IN_5" direction="in"/>
<pin name="IN_6" direction="in"/>
<pin name="IN" direction="in"/>
<pin name="ADJ" direction="pas"/>
<pin name="~SD/SOFT_2" direction="pas"/>
<pin name="~SD/SOFT" direction="pas"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="OUT_2" direction="out"/>
<pin name="OUT_3" direction="out"/>
<pin name="OUT_4" direction="out"/>
<pin name="OUT_5" direction="out"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM2830XMF">
<pin name="VIN" direction="pwr"/>
<pin name="FB" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM2831XMF">
<pin name="VIN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="FB" direction="pas"/>
<pin name="EN" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM2831XSD">
<pin name="VINA" direction="in"/>
<pin name="VIND" direction="in"/>
<pin name="FB" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="EP" direction="pas"/>
<pin name="EN" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM2831YMF">
<pin name="EN" direction="pas"/>
<pin name="VIN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="FB" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM2831YSD">
<pin name="FB" direction="pas"/>
<pin name="VIND" direction="in"/>
<pin name="VINA" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="EN" direction="pas"/>
<pin name="EP" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM2831ZMF">
<pin name="VIN" direction="pwr"/>
<pin name="FB" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM2831ZSD">
<pin name="VINA" direction="in"/>
<pin name="VIND" direction="in"/>
<pin name="FB" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="EP" direction="pas"/>
<pin name="EN" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM2832XMY">
<pin name="VINA" direction="pwr"/>
<pin name="VIND" direction="pwr"/>
<pin name="EN" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM2832XSD">
<pin name="VINA" direction="in"/>
<pin name="VIND" direction="in"/>
<pin name="FB" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="EP" direction="pas"/>
<pin name="EN" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM2832YMY">
<pin name="VIND" direction="in"/>
<pin name="VINA" direction="in"/>
<pin name="EN" direction="pas"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="EP" direction="pas"/>
<pin name="FB" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM2832YSD">
<pin name="VINA" direction="in"/>
<pin name="VIND" direction="in"/>
<pin name="FB" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="EP" direction="pas"/>
<pin name="EN" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM2832ZMY">
<pin name="VIND" direction="in"/>
<pin name="VINA" direction="in"/>
<pin name="EN" direction="pas"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="EP" direction="pas"/>
<pin name="FB" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM2833XMY">
<pin name="VINC" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="SGND" direction="pas"/>
<pin name="NC" direction="nc"/>
<pin name="FB" direction="in"/>
<pin name="PGND" direction="pas"/>
<pin name="EP" direction="pas"/>
<pin name="SW_2" direction="in"/>
<pin name="SW" direction="in"/>
<pin name="VIND_2" direction="in"/>
<pin name="VIND" direction="in"/>
</symbol>
<symbol name="LM2833XSD">
<pin name="VINC" direction="pwr"/>
<pin name="VIND_2" direction="in"/>
<pin name="VIND" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="SGND" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="EP" direction="pas"/>
<pin name="SW_2" direction="out"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM2833ZMY">
<pin name="VINC" direction="pwr"/>
<pin name="VIND_2" direction="in"/>
<pin name="VIND" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="SGND" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="EP" direction="pas"/>
<pin name="SW_2" direction="out"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM2833ZSD">
<pin name="VINC" direction="pwr"/>
<pin name="VIND_2" direction="in"/>
<pin name="VIND" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="SGND" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="EP" direction="pas"/>
<pin name="SW_2" direction="out"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM2841XMK-ADJL">
<pin name="VIN" direction="in"/>
<pin name="CB" direction="in"/>
<pin name="*SHDN" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM2841YMK-ADJL">
<pin name="VIN" direction="in"/>
<pin name="CB" direction="in"/>
<pin name="*SHDN" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM2842XMK-ADJL">
<pin name="VIN" direction="in"/>
<pin name="CB" direction="in"/>
<pin name="*SHDN" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM2842YMK-ADJL">
<pin name="VIN" direction="in"/>
<pin name="CB" direction="in"/>
<pin name="*SHDN" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM2852XMXA-0.8">
<pin name="AVIN" direction="in"/>
<pin name="PVIN_2" direction="in"/>
<pin name="PVIN" direction="in"/>
<pin name="EN" direction="pas"/>
<pin name="SS" direction="pas"/>
<pin name="NC_2" direction="pas"/>
<pin name="PGND_2" direction="pas"/>
<pin name="SGND" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="NC_3" direction="pas"/>
<pin name="NC" direction="pas"/>
<pin name="SW_2" direction="out"/>
<pin name="SW" direction="out"/>
<pin name="SNS" direction="pas"/>
<pin name="EP" direction="pas"/>
</symbol>
<symbol name="LM2852XMXA-1.0">
<pin name="AVIN" direction="in"/>
<pin name="PVIN_2" direction="in"/>
<pin name="PVIN" direction="in"/>
<pin name="EN" direction="pas"/>
<pin name="SS" direction="pas"/>
<pin name="NC_2" direction="pas"/>
<pin name="PGND_2" direction="pas"/>
<pin name="SGND" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="NC_3" direction="pas"/>
<pin name="NC" direction="pas"/>
<pin name="SW_2" direction="out"/>
<pin name="SW" direction="out"/>
<pin name="SNS" direction="pas"/>
<pin name="EP" direction="pas"/>
</symbol>
<symbol name="LM2852XMXA-1.2">
<pin name="AVIN" direction="in"/>
<pin name="PVIN_2" direction="in"/>
<pin name="PVIN" direction="in"/>
<pin name="EN" direction="pas"/>
<pin name="SS" direction="pas"/>
<pin name="NC_2" direction="pas"/>
<pin name="PGND_2" direction="pas"/>
<pin name="SGND" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="NC_3" direction="pas"/>
<pin name="NC" direction="pas"/>
<pin name="SW_2" direction="out"/>
<pin name="SW" direction="out"/>
<pin name="SNS" direction="pas"/>
<pin name="EP" direction="pas"/>
</symbol>
<symbol name="LM2852XMXA-1.5">
<pin name="AVIN" direction="in"/>
<pin name="PVIN_2" direction="in"/>
<pin name="PVIN" direction="in"/>
<pin name="EN" direction="pas"/>
<pin name="SS" direction="pas"/>
<pin name="NC_2" direction="pas"/>
<pin name="PGND_2" direction="pas"/>
<pin name="SGND" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="NC_3" direction="pas"/>
<pin name="NC" direction="pas"/>
<pin name="SW_2" direction="out"/>
<pin name="SW" direction="out"/>
<pin name="SNS" direction="pas"/>
<pin name="EP" direction="pas"/>
</symbol>
<symbol name="LM2852XMXA-1.8">
<pin name="AVIN" direction="in"/>
<pin name="PVIN_2" direction="in"/>
<pin name="PVIN" direction="in"/>
<pin name="EN" direction="pas"/>
<pin name="SS" direction="pas"/>
<pin name="NC_2" direction="pas"/>
<pin name="PGND_2" direction="pas"/>
<pin name="SGND" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="NC_3" direction="pas"/>
<pin name="NC" direction="pas"/>
<pin name="SW_2" direction="out"/>
<pin name="SW" direction="out"/>
<pin name="SNS" direction="pas"/>
<pin name="EP" direction="pas"/>
</symbol>
<symbol name="LM2852XMXA-2.5">
<pin name="AVIN" direction="in"/>
<pin name="PVIN_2" direction="in"/>
<pin name="PVIN" direction="in"/>
<pin name="EN" direction="pas"/>
<pin name="SS" direction="pas"/>
<pin name="NC_2" direction="pas"/>
<pin name="PGND_2" direction="pas"/>
<pin name="SGND" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="NC_3" direction="pas"/>
<pin name="NC" direction="pas"/>
<pin name="SW_2" direction="out"/>
<pin name="SW" direction="out"/>
<pin name="SNS" direction="pas"/>
<pin name="EP" direction="pas"/>
</symbol>
<symbol name="LM2852XMXA-3.0">
<pin name="AVIN" direction="in"/>
<pin name="PVIN_2" direction="in"/>
<pin name="PVIN" direction="in"/>
<pin name="EN" direction="pas"/>
<pin name="SS" direction="pas"/>
<pin name="NC_2" direction="pas"/>
<pin name="PGND_2" direction="pas"/>
<pin name="SGND" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="NC_3" direction="pas"/>
<pin name="NC" direction="pas"/>
<pin name="SW_2" direction="out"/>
<pin name="SW" direction="out"/>
<pin name="SNS" direction="pas"/>
<pin name="EP" direction="pas"/>
</symbol>
<symbol name="LM2852XMXA-3.3">
<pin name="AVIN" direction="in"/>
<pin name="PVIN_2" direction="in"/>
<pin name="PVIN" direction="in"/>
<pin name="EN" direction="pas"/>
<pin name="SS" direction="pas"/>
<pin name="NC_2" direction="pas"/>
<pin name="PGND_2" direction="pas"/>
<pin name="SGND" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="NC_3" direction="pas"/>
<pin name="NC" direction="pas"/>
<pin name="SW_2" direction="out"/>
<pin name="SW" direction="out"/>
<pin name="SNS" direction="pas"/>
<pin name="EP" direction="pas"/>
</symbol>
<symbol name="LM2852YMXA-1.0">
<pin name="AVIN" direction="in"/>
<pin name="PVIN_2" direction="in"/>
<pin name="PVIN" direction="in"/>
<pin name="EN" direction="pas"/>
<pin name="SS" direction="pas"/>
<pin name="NC_2" direction="pas"/>
<pin name="PGND_2" direction="pas"/>
<pin name="SGND" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="NC_3" direction="pas"/>
<pin name="NC" direction="pas"/>
<pin name="SW_2" direction="out"/>
<pin name="SW" direction="out"/>
<pin name="SNS" direction="pas"/>
<pin name="EP" direction="pas"/>
</symbol>
<symbol name="LM2852YMXA-1.2">
<pin name="AVIN" direction="in"/>
<pin name="PVIN_2" direction="in"/>
<pin name="PVIN" direction="in"/>
<pin name="EN" direction="pas"/>
<pin name="SS" direction="pas"/>
<pin name="NC_2" direction="pas"/>
<pin name="PGND_2" direction="pas"/>
<pin name="SGND" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="NC_3" direction="pas"/>
<pin name="NC" direction="pas"/>
<pin name="SW_2" direction="out"/>
<pin name="SW" direction="out"/>
<pin name="SNS" direction="pas"/>
<pin name="EP" direction="pas"/>
</symbol>
<symbol name="LM2852YMXA-1.3">
<pin name="AVIN" direction="in"/>
<pin name="PVIN_2" direction="in"/>
<pin name="PVIN" direction="in"/>
<pin name="EN" direction="pas"/>
<pin name="SS" direction="pas"/>
<pin name="NC_2" direction="pas"/>
<pin name="PGND_2" direction="pas"/>
<pin name="SGND" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="NC_3" direction="pas"/>
<pin name="NC" direction="pas"/>
<pin name="SW_2" direction="out"/>
<pin name="SW" direction="out"/>
<pin name="SNS" direction="pas"/>
<pin name="EP" direction="pas"/>
</symbol>
<symbol name="LM2852YMXA-1.8">
<pin name="AVIN" direction="in"/>
<pin name="PVIN_2" direction="in"/>
<pin name="PVIN" direction="in"/>
<pin name="EN" direction="pas"/>
<pin name="SS" direction="pas"/>
<pin name="NC_2" direction="pas"/>
<pin name="PGND_2" direction="pas"/>
<pin name="SGND" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="NC_3" direction="pas"/>
<pin name="NC" direction="pas"/>
<pin name="SW_2" direction="out"/>
<pin name="SW" direction="out"/>
<pin name="SNS" direction="pas"/>
<pin name="EP" direction="pas"/>
</symbol>
<symbol name="LM2852YMXA-2.5">
<pin name="AVIN" direction="in"/>
<pin name="PVIN_2" direction="in"/>
<pin name="PVIN" direction="in"/>
<pin name="EN" direction="pas"/>
<pin name="SS" direction="pas"/>
<pin name="NC_2" direction="pas"/>
<pin name="PGND_2" direction="pas"/>
<pin name="SGND" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="NC_3" direction="pas"/>
<pin name="NC" direction="pas"/>
<pin name="SW_2" direction="out"/>
<pin name="SW" direction="out"/>
<pin name="SNS" direction="pas"/>
<pin name="EP" direction="pas"/>
</symbol>
<symbol name="LM2852YMXA-3.0">
<pin name="AVIN" direction="in"/>
<pin name="PVIN_2" direction="in"/>
<pin name="PVIN" direction="in"/>
<pin name="EN" direction="pas"/>
<pin name="SS" direction="pas"/>
<pin name="NC_2" direction="pas"/>
<pin name="PGND_2" direction="pas"/>
<pin name="SGND" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="NC_3" direction="pas"/>
<pin name="NC" direction="pas"/>
<pin name="SW_2" direction="out"/>
<pin name="SW" direction="out"/>
<pin name="SNS" direction="pas"/>
<pin name="EP" direction="pas"/>
</symbol>
<symbol name="LM2852YMXA-3.3">
<pin name="AVIN" direction="in"/>
<pin name="PVIN_2" direction="in"/>
<pin name="PVIN" direction="in"/>
<pin name="EN" direction="pas"/>
<pin name="SS" direction="pas"/>
<pin name="NC_2" direction="pas"/>
<pin name="PGND_2" direction="pas"/>
<pin name="SGND" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="NC_3" direction="pas"/>
<pin name="NC" direction="pas"/>
<pin name="SW_2" direction="out"/>
<pin name="SW" direction="out"/>
<pin name="SNS" direction="pas"/>
<pin name="EP" direction="pas"/>
</symbol>
<symbol name="LM2853MH-0.8">
<pin name="AVIN" direction="in"/>
<pin name="PVIN_2" direction="in"/>
<pin name="PVIN" direction="in"/>
<pin name="EN" direction="pas"/>
<pin name="SS" direction="pas"/>
<pin name="NC_2" direction="pas"/>
<pin name="PGND_2" direction="pas"/>
<pin name="SGND" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="NC_3" direction="pas"/>
<pin name="NC" direction="pas"/>
<pin name="SW_2" direction="out"/>
<pin name="SW" direction="out"/>
<pin name="SNS" direction="pas"/>
<pin name="EP" direction="pas"/>
</symbol>
<symbol name="LM2853MH-1.0">
<pin name="AVIN" direction="in"/>
<pin name="PVIN_2" direction="in"/>
<pin name="PVIN" direction="in"/>
<pin name="EN" direction="pas"/>
<pin name="SS" direction="pas"/>
<pin name="NC_2" direction="pas"/>
<pin name="PGND_2" direction="pas"/>
<pin name="SGND" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="NC_3" direction="pas"/>
<pin name="NC" direction="pas"/>
<pin name="SW_2" direction="out"/>
<pin name="SW" direction="out"/>
<pin name="SNS" direction="pas"/>
<pin name="EP" direction="pas"/>
</symbol>
<symbol name="LM2853MH-1.2">
<pin name="AVIN" direction="in"/>
<pin name="PVIN_2" direction="in"/>
<pin name="PVIN" direction="in"/>
<pin name="EN" direction="pas"/>
<pin name="SS" direction="pas"/>
<pin name="NC_2" direction="pas"/>
<pin name="PGND_2" direction="pas"/>
<pin name="SGND" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="NC_3" direction="pas"/>
<pin name="NC" direction="pas"/>
<pin name="SW_2" direction="out"/>
<pin name="SW" direction="out"/>
<pin name="SNS" direction="pas"/>
<pin name="EP" direction="pas"/>
</symbol>
<symbol name="LM2853MH-1.5">
<pin name="AVIN" direction="in"/>
<pin name="PVIN_2" direction="in"/>
<pin name="PVIN" direction="in"/>
<pin name="EN" direction="pas"/>
<pin name="SS" direction="pas"/>
<pin name="NC_2" direction="pas"/>
<pin name="PGND_2" direction="pas"/>
<pin name="SGND" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="NC_3" direction="pas"/>
<pin name="NC" direction="pas"/>
<pin name="SW_2" direction="out"/>
<pin name="SW" direction="out"/>
<pin name="SNS" direction="pas"/>
<pin name="EP" direction="pas"/>
</symbol>
<symbol name="LM2853MH-1.8">
<pin name="AVIN" direction="in"/>
<pin name="PVIN_2" direction="in"/>
<pin name="PVIN" direction="in"/>
<pin name="EN" direction="pas"/>
<pin name="SS" direction="pas"/>
<pin name="NC_2" direction="pas"/>
<pin name="PGND_2" direction="pas"/>
<pin name="SGND" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="NC_3" direction="pas"/>
<pin name="NC" direction="pas"/>
<pin name="SW_2" direction="out"/>
<pin name="SW" direction="out"/>
<pin name="SNS" direction="pas"/>
<pin name="EP" direction="pas"/>
</symbol>
<symbol name="LM2853MH-2.5">
<pin name="AVIN" direction="in"/>
<pin name="PVIN_2" direction="in"/>
<pin name="PVIN" direction="in"/>
<pin name="EN" direction="pas"/>
<pin name="SS" direction="pas"/>
<pin name="NC_2" direction="pas"/>
<pin name="PGND_2" direction="pas"/>
<pin name="SGND" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="NC_3" direction="pas"/>
<pin name="NC" direction="pas"/>
<pin name="SW_2" direction="out"/>
<pin name="SW" direction="out"/>
<pin name="SNS" direction="pas"/>
<pin name="EP" direction="pas"/>
</symbol>
<symbol name="LM2853MH-3.0">
<pin name="AVIN" direction="in"/>
<pin name="PVIN_2" direction="in"/>
<pin name="PVIN" direction="in"/>
<pin name="EN" direction="pas"/>
<pin name="SS" direction="pas"/>
<pin name="NC_2" direction="pas"/>
<pin name="PGND_2" direction="pas"/>
<pin name="SGND" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="NC_3" direction="pas"/>
<pin name="NC" direction="pas"/>
<pin name="SW_2" direction="out"/>
<pin name="SW" direction="out"/>
<pin name="SNS" direction="pas"/>
<pin name="EP" direction="pas"/>
</symbol>
<symbol name="LM2853MH-3.3">
<pin name="AVIN" direction="in"/>
<pin name="PVIN_2" direction="in"/>
<pin name="PVIN" direction="in"/>
<pin name="EN" direction="pas"/>
<pin name="SS" direction="pas"/>
<pin name="NC_2" direction="pas"/>
<pin name="PGND_2" direction="pas"/>
<pin name="SGND" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="NC_3" direction="pas"/>
<pin name="NC" direction="pas"/>
<pin name="SW_2" direction="out"/>
<pin name="SW" direction="out"/>
<pin name="SNS" direction="pas"/>
<pin name="EP" direction="pas"/>
</symbol>
<symbol name="LM2854MH-1000">
<pin name="PVIN_2" direction="pwr"/>
<pin name="PVIN_3" direction="pwr"/>
<pin name="PVIN" direction="pwr"/>
<pin name="AVIN" direction="pwr"/>
<pin name="EN" direction="in"/>
<pin name="SS" direction="pas"/>
<pin name="NC_2" direction="pas"/>
<pin name="NC_3" direction="pas"/>
<pin name="NC" direction="pas"/>
<pin name="SW_2" direction="pwr"/>
<pin name="SW" direction="pwr"/>
<pin name="FB" direction="in"/>
<pin name="AGND" direction="pwr"/>
<pin name="PGND_2" direction="pwr"/>
<pin name="PGND_3" direction="pwr"/>
<pin name="PGND" direction="pwr"/>
<pin name="EP" direction="pwr"/>
</symbol>
<symbol name="LM2854MH-500">
<pin name="PVIN_2" direction="pwr"/>
<pin name="PVIN_3" direction="pwr"/>
<pin name="PVIN" direction="pwr"/>
<pin name="AVIN" direction="pwr"/>
<pin name="FB" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="SS" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="AGND" direction="pas"/>
<pin name="PGND_2" direction="pas"/>
<pin name="PGND_3" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="SW_2" direction="out"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM2901M">
<pin name="VCC" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="-INA" direction="in"/>
<pin name="+INA_" direction="in"/>
<pin name="-INB" direction="in"/>
<pin name="+INB" direction="in"/>
<pin name="-INC" direction="in"/>
<pin name="+INC" direction="in"/>
<pin name="-IND" direction="in"/>
<pin name="+IND" direction="in"/>
<pin name="OUTD" direction="out"/>
<pin name="OUTC" direction="out"/>
<pin name="OUTB" direction="out"/>
<pin name="OUTA" direction="out"/>
</symbol>
<symbol name="LM2901N">
<pin name="VCC" direction="pas"/>
<pin name="-INA" direction="in"/>
<pin name="+INA_" direction="in"/>
<pin name="-INB" direction="in"/>
<pin name="+INB" direction="in"/>
<pin name="-INC" direction="in"/>
<pin name="+INC" direction="in"/>
<pin name="-IND" direction="in"/>
<pin name="+IND" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUTD" direction="out"/>
<pin name="OUTC" direction="out"/>
<pin name="OUTB" direction="out"/>
<pin name="OUTA" direction="out"/>
</symbol>
<symbol name="LM2902M">
<pin name="V+" direction="pwr"/>
<pin name="IN1-" direction="in"/>
<pin name="IN1+" direction="in"/>
<pin name="IN2+" direction="in"/>
<pin name="IN2-" direction="in"/>
<pin name="IN3-" direction="in"/>
<pin name="IN3+" direction="in"/>
<pin name="IN4-" direction="in"/>
<pin name="IN4+" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT1" direction="out"/>
<pin name="OUT2" direction="out"/>
<pin name="OUT3" direction="out"/>
<pin name="OUT4" direction="out"/>
</symbol>
<symbol name="LM2902N">
<pin name="-INA" direction="in"/>
<pin name="+INA_" direction="in"/>
<pin name="-INB" direction="in"/>
<pin name="+INB" direction="in"/>
<pin name="-INC" direction="in"/>
<pin name="+INC" direction="in"/>
<pin name="-IND" direction="in"/>
<pin name="+IND" direction="in"/>
<pin name="V+" direction="pas"/>
<pin name="V-" direction="pas"/>
<pin name="OUTD" direction="out"/>
<pin name="OUTC" direction="out"/>
<pin name="OUTB" direction="out"/>
<pin name="OUTA" direction="out"/>
</symbol>
<symbol name="LM2903M">
<pin name="-INA" direction="in"/>
<pin name="+INA" direction="in"/>
<pin name="+INB" direction="in"/>
<pin name="-INB" direction="in"/>
<pin name="V+" direction="pas"/>
<pin name="V-" direction="pas"/>
<pin name="OUTB" direction="out"/>
<pin name="OUTA" direction="out"/>
</symbol>
<symbol name="LM2903N">
<pin name="+INA" direction="in"/>
<pin name="-INA" direction="in"/>
<pin name="+INB" direction="in"/>
<pin name="-INB" direction="in"/>
<pin name="V+" direction="pas"/>
<pin name="V-" direction="pas"/>
<pin name="OUTB" direction="out"/>
<pin name="OUTA" direction="out"/>
</symbol>
<symbol name="LM2904M">
<pin name="-INA" direction="in"/>
<pin name="+INA" direction="in"/>
<pin name="+INB" direction="in"/>
<pin name="-INB" direction="in"/>
<pin name="VCC" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="OUTB" direction="out"/>
<pin name="OUTA" direction="out"/>
</symbol>
<symbol name="LM2904N">
<pin name="+INA" direction="in"/>
<pin name="-INA" direction="in"/>
<pin name="+INB" direction="in"/>
<pin name="-INB" direction="in"/>
<pin name="VCC" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="OUTB" direction="out"/>
<pin name="OUTA" direction="out"/>
</symbol>
<symbol name="LM2931AT-5.0">
<pin name="IN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM2931AZ-5.0">
<pin name="IN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM2931CT">
<pin name="IN" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="ADJ" direction="in"/>
<pin name="ON/OFF" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM2931T-5.0">
<pin name="IN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM2931Z-5.0">
<pin name="IN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM2937ES-10">
<pin name="VIN" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="VOUT" direction="out"/>
<pin name="TAB" direction="pas"/>
</symbol>
<symbol name="LM2937ES-12">
<pin name="VIN" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="VOUT" direction="out"/>
<pin name="TAB" direction="pas"/>
</symbol>
<symbol name="LM2937ES-15">
<pin name="VIN" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="VOUT" direction="out"/>
<pin name="TAB" direction="pas"/>
</symbol>
<symbol name="LM2937ES-5.0">
<pin name="VIN" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="VOUT" direction="out"/>
<pin name="TAB" direction="pas"/>
</symbol>
<symbol name="LM2937ES-8.0">
<pin name="VIN" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="VOUT" direction="out"/>
<pin name="TAB" direction="pas"/>
</symbol>
<symbol name="LM2937ET-10">
<pin name="VIN" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LM2937ET-12">
<pin name="IN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM2937ET-15">
<pin name="IN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM2937ET-5.0">
<pin name="IN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM2937ET-8.0">
<pin name="IN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM2937IMP-10">
<pin name="VIN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="GND_(TAB)" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LM2937IMP-12">
<pin name="VIN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="GND_(TAB)" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LM2937IMP-15">
<pin name="VIN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="GND_(TAB)" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LM2937IMP-5.0">
<pin name="VIN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="GND_(TAB)" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LM2937IMP-8.0">
<pin name="VIN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="GND_(TAB)" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LM293H">
<pin name="-INA" direction="in"/>
<pin name="+INA" direction="in"/>
<pin name="-INB" direction="in"/>
<pin name="+INB" direction="in"/>
<pin name="V+" direction="pas"/>
<pin name="V-" direction="pas"/>
<pin name="OUTB" direction="out"/>
<pin name="OUTA" direction="out"/>
</symbol>
<symbol name="LM2940CS-5.0">
<pin name="IN" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM2940CS-9.0">
<pin name="IN" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM2940CT-12">
<pin name="IN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM2940CT-15">
<pin name="IN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM2940CT-5.0">
<pin name="IN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM2940IMP-5.0">
<pin name="VIN" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LM2940S-5.0">
<pin name="IN" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM2940T-10.0">
<pin name="IN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM2940T-12.0">
<pin name="IN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM2940T-5.0">
<pin name="IN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM2940T-8.0">
<pin name="IN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM2940T-9.0">
<pin name="IN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM2941CT">
<pin name="IN" direction="in"/>
<pin name="ADJ" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="ON/OFF" direction="in"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM2941LD">
<pin name="IN" direction="in"/>
<pin name="ON/OFF" direction="pas"/>
<pin name="ADJ" direction="pas"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM2941S">
<pin name="IN" direction="in"/>
<pin name="ADJ" direction="pas"/>
<pin name="ON/OFF" direction="pas"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM2990S-12">
<pin name="IN" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM2990T-12">
<pin name="IN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM2990T-15">
<pin name="IN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM2990T-5.0">
<pin name="IN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM3000SQ">
<pin name="VDD" direction="in"/>
<pin name="VIN" direction="pwr"/>
<pin name="VDR" direction="in"/>
<pin name="FREQ/SYNC" direction="in"/>
<pin name="ILIM1" direction="in"/>
<pin name="ILIM2" direction="in"/>
<pin name="COMP1" direction="in"/>
<pin name="COMP2" direction="in"/>
<pin name="VCB1" direction="in"/>
<pin name="VCB2" direction="in"/>
<pin name="EN1" direction="in"/>
<pin name="EN2" direction="in"/>
<pin name="TRK1" direction="in"/>
<pin name="TRK2" direction="in"/>
<pin name="SS1" direction="in"/>
<pin name="SS2" direction="in"/>
<pin name="FB1" direction="in"/>
<pin name="FB2" direction="in"/>
<pin name="SGND" direction="pas"/>
<pin name="PGND1" direction="pas"/>
<pin name="PGND2" direction="pas"/>
<pin name="EA1_GND" direction="pas"/>
<pin name="EA2_GND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="CLKOUT" direction="out"/>
<pin name="PGOOD1" direction="out"/>
<pin name="PGOOD2" direction="out"/>
<pin name="LG2" direction="out"/>
<pin name="LG1" direction="out"/>
<pin name="VSW1" direction="out"/>
<pin name="VSW2" direction="out"/>
<pin name="HG1" direction="out"/>
<pin name="HG2" direction="out"/>
</symbol>
<symbol name="LM301AH">
<pin name="-INA" direction="in"/>
<pin name="+INA" direction="in"/>
<pin name="BALANCE_2" direction="in"/>
<pin name="BALANCE" direction="in"/>
<pin name="V+" direction="in"/>
<pin name="V-" direction="pas"/>
<pin name="COMP" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM301AN">
<pin name="V+" direction="pwr"/>
<pin name="BAL/COMP" direction="pas"/>
<pin name="BAL" direction="pas"/>
<pin name="COMP" direction="pas"/>
<pin name="+IN" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM3100MH">
<pin name="VCC" direction="pwr"/>
<pin name="VIN_2" direction="in"/>
<pin name="VIN" direction="in"/>
<pin name="SS" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="BST" direction="in"/>
<pin name="TST" direction="in"/>
<pin name="RON" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC_6" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="PGND_2" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="SW_2" direction="out"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM3102MH">
<pin name="VCC" direction="pwr"/>
<pin name="FB" direction="in"/>
<pin name="BST" direction="in"/>
<pin name="RON" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="SS" direction="in"/>
<pin name="VIN_2" direction="in"/>
<pin name="VIN" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC_6" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="AGND" direction="pas"/>
<pin name="PGND_2" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="SW_2" direction="out"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM3103MH">
<pin name="VCC" direction="pwr"/>
<pin name="VIN_2" direction="in"/>
<pin name="VIN" direction="in"/>
<pin name="SS" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="RON" direction="in"/>
<pin name="BST" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="AGND" direction="pas"/>
<pin name="PGND_2" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="SW_2" direction="out"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM311H">
<pin name="-INA" direction="in"/>
<pin name="+INA" direction="in"/>
<pin name="-INB" direction="in"/>
<pin name="+INB" direction="in"/>
<pin name="V+" direction="pas"/>
<pin name="V-" direction="pas"/>
<pin name="OUTB" direction="out"/>
<pin name="OUTA" direction="out"/>
</symbol>
<symbol name="LM311M">
<pin name="V+" direction="pwr"/>
<pin name="IN2" direction="in"/>
<pin name="IN3" direction="in"/>
<pin name="BAL" direction="pas"/>
<pin name="BAL/STROBE" direction="pas"/>
<pin name="V-" direction="pwr"/>
<pin name="GND1" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM311N">
<pin name="V+" direction="pwr"/>
<pin name="IN2" direction="in"/>
<pin name="IN3" direction="in"/>
<pin name="BAL" direction="pas"/>
<pin name="BAL/STROBE" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM3150MH">
<pin name="VCC" direction="pwr"/>
<pin name="VIN" direction="in"/>
<pin name="BST" direction="in"/>
<pin name="RON" direction="in"/>
<pin name="ILIM" direction="in"/>
<pin name="SS" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="SGND_2" direction="pas"/>
<pin name="SGND" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="LG" direction="out"/>
<pin name="HG" direction="out"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM318M">
<pin name="V+" direction="pwr"/>
<pin name="+IN" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="BAL/COMP1" direction="pas"/>
<pin name="COMP2" direction="pas"/>
<pin name="BAL/COMP3" direction="pas"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM318N">
<pin name="V+" direction="pwr"/>
<pin name="BAL/COMP1" direction="pas"/>
<pin name="COMP2" direction="pas"/>
<pin name="BAL/COMP3" direction="pas"/>
<pin name="-IN" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM319AM">
<pin name="V+" direction="pwr"/>
<pin name="+IN" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="+IN2" direction="in"/>
<pin name="-IN2" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="V-" direction="pwr"/>
<pin name="GND1" direction="pas"/>
<pin name="GND2" direction="pas"/>
<pin name="OUT1" direction="out"/>
<pin name="OUT2" direction="out"/>
</symbol>
<symbol name="LM319M">
<pin name="V+" direction="pwr"/>
<pin name="+IN" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="+IN2" direction="in"/>
<pin name="-IN2" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="V-" direction="pwr"/>
<pin name="GND1" direction="pas"/>
<pin name="GND2" direction="pas"/>
<pin name="OUT1" direction="out"/>
<pin name="OUT2" direction="out"/>
</symbol>
<symbol name="LM319N">
<pin name="V+" direction="pwr"/>
<pin name="+IN" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="+IN2" direction="in"/>
<pin name="-IN2" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="V-" direction="pwr"/>
<pin name="GND1" direction="pas"/>
<pin name="GND2" direction="pas"/>
<pin name="OUT1" direction="out"/>
<pin name="OUT2" direction="out"/>
</symbol>
<symbol name="LM3200TL">
<pin name="PVIN" direction="in"/>
<pin name="VCON" direction="pas"/>
<pin name="BYP" direction="pas"/>
<pin name="VDD" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="SGND" direction="pas"/>
<pin name="FB" direction="pas"/>
<pin name="SW" direction="out"/>
<pin name="EN" direction="pas"/>
<pin name="BYPOUT" direction="pas"/>
</symbol>
<symbol name="LM3203TL">
<pin name="PVIN" direction="in"/>
<pin name="VCON" direction="pas"/>
<pin name="BYP" direction="pas"/>
<pin name="VDD" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="SGND" direction="pas"/>
<pin name="FB" direction="pas"/>
<pin name="SW" direction="out"/>
<pin name="EN" direction="pas"/>
<pin name="BYPOUT" direction="pas"/>
</symbol>
<symbol name="LM3205SD-2">
<pin name="VDD" direction="pwr"/>
<pin name="PVIN_2" direction="in"/>
<pin name="PVIN" direction="in"/>
<pin name="VCON" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="PGND_2" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="SGND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM3205TL">
<pin name="PVIN" direction="in"/>
<pin name="VDD" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="SGND" direction="pas"/>
<pin name="EN" direction="pas"/>
<pin name="VCON" direction="pas"/>
<pin name="FB" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM3207TL">
<pin name="PVIN" direction="in"/>
<pin name="SW" direction="out"/>
<pin name="VCON" direction="pas"/>
<pin name="ENLDO" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="SGND" direction="pas"/>
<pin name="EN" direction="pas"/>
<pin name="FB" direction="pas"/>
<pin name="LDO" direction="out"/>
</symbol>
<symbol name="LM3208TL">
<pin name="VDD" direction="pwr"/>
<pin name="PVIN" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="VCON" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="PGND" direction="pas"/>
<pin name="SGND" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM3211MT-ADJ">
<pin name="VIN" direction="in"/>
<pin name="VSW" direction="pas"/>
<pin name="~SHDN" direction="pas"/>
<pin name="FSLCT" direction="pas"/>
<pin name="GMA1-IN" direction="in"/>
<pin name="GMA2-IN" direction="in"/>
<pin name="GMA3-IN" direction="in"/>
<pin name="GMA4-IN" direction="in"/>
<pin name="VS+" direction="pas"/>
<pin name="VC" direction="pas"/>
<pin name="AGND" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="NC_2" direction="pas"/>
<pin name="NC" direction="pas"/>
<pin name="GMA4-OUT" direction="out"/>
<pin name="GMA3-OUT" direction="out"/>
<pin name="GMA2-OUT" direction="out"/>
<pin name="GMA1-OUT" direction="out"/>
<pin name="SS" direction="pas"/>
<pin name="FB" direction="pas"/>
</symbol>
<symbol name="LM321MF">
<pin name="V+" direction="pwr"/>
<pin name="+IN" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM3224MM-ADJ">
<pin name="VIN" direction="pwr"/>
<pin name="VC" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="SS" direction="in"/>
<pin name="~SHDN" direction="in"/>
<pin name="FSLCT" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM324AM">
<pin name="V+" direction="pwr"/>
<pin name="-IN1" direction="in"/>
<pin name="+IN1" direction="in"/>
<pin name="+IN2" direction="in"/>
<pin name="-IN2" direction="in"/>
<pin name="-IN3" direction="in"/>
<pin name="+IN3" direction="in"/>
<pin name="+IN4" direction="in"/>
<pin name="-IN4" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT1" direction="out"/>
<pin name="OUT2" direction="out"/>
<pin name="OUT3" direction="out"/>
<pin name="OUT4" direction="out"/>
</symbol>
<symbol name="LM324AN">
<pin name="V+" direction="pas"/>
<pin name="+INA_" direction="in"/>
<pin name="-INA" direction="in"/>
<pin name="+INB" direction="in"/>
<pin name="-INB" direction="in"/>
<pin name="+INC" direction="in"/>
<pin name="-INC" direction="in"/>
<pin name="+IND" direction="in"/>
<pin name="-IND" direction="in"/>
<pin name="V-" direction="pas"/>
<pin name="OUTD" direction="out"/>
<pin name="OUTC" direction="out"/>
<pin name="OUTB" direction="out"/>
<pin name="OUTA" direction="out"/>
</symbol>
<symbol name="LM324M">
<pin name="V+" direction="pwr"/>
<pin name="-IN1" direction="in"/>
<pin name="+IN1" direction="in"/>
<pin name="+IN2" direction="in"/>
<pin name="-IN2" direction="in"/>
<pin name="-IN3" direction="in"/>
<pin name="+IN3" direction="in"/>
<pin name="+IN4" direction="in"/>
<pin name="-IN4" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT1" direction="out"/>
<pin name="OUT2" direction="out"/>
<pin name="OUT3" direction="out"/>
<pin name="OUT4" direction="out"/>
</symbol>
<symbol name="LM324MT">
<pin name="V+" direction="pwr"/>
<pin name="-IN1" direction="in"/>
<pin name="+IN1" direction="in"/>
<pin name="+IN2" direction="in"/>
<pin name="-IN2" direction="in"/>
<pin name="-IN3" direction="in"/>
<pin name="+IN3" direction="in"/>
<pin name="+IN4" direction="in"/>
<pin name="-IN4" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT1" direction="out"/>
<pin name="OUT2" direction="out"/>
<pin name="OUT3" direction="out"/>
<pin name="OUT4" direction="out"/>
</symbol>
<symbol name="LM324N">
<pin name="V+" direction="pas"/>
<pin name="+INA_" direction="in"/>
<pin name="-INA" direction="in"/>
<pin name="+INB" direction="in"/>
<pin name="-INB" direction="in"/>
<pin name="+INC" direction="in"/>
<pin name="-INC" direction="in"/>
<pin name="+IND" direction="in"/>
<pin name="-IND" direction="in"/>
<pin name="V-" direction="pas"/>
<pin name="OUTD" direction="out"/>
<pin name="OUTC" direction="out"/>
<pin name="OUTB" direction="out"/>
<pin name="OUTA" direction="out"/>
</symbol>
<symbol name="LM3310SQ">
<pin name="VDD" direction="pwr"/>
<pin name="~SHDN" direction="in"/>
<pin name="FREQ" direction="in"/>
<pin name="VFLK" direction="in"/>
<pin name="VDPM" direction="in"/>
<pin name="NEG" direction="in"/>
<pin name="POS" direction="in"/>
<pin name="VGH" direction="in"/>
<pin name="SS" direction="in"/>
<pin name="VC" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="CE" direction="in"/>
<pin name="RE" direction="in"/>
<pin name="AVIN" direction="in"/>
<pin name="VIN" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="AGND" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="VGHM" direction="out"/>
<pin name="OUT" direction="out"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM334Z">
<pin name="V+" direction="pwr"/>
<pin name="R" direction="in"/>
<pin name="V-" direction="out"/>
</symbol>
<symbol name="LM339AM">
<pin name="V+" direction="pwr"/>
<pin name="-IN1" direction="in"/>
<pin name="+IN1" direction="in"/>
<pin name="-IN2" direction="in"/>
<pin name="+IN2" direction="in"/>
<pin name="-IN3" direction="in"/>
<pin name="+IN3" direction="in"/>
<pin name="-IN4" direction="in"/>
<pin name="+IN4" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT1" direction="out"/>
<pin name="OUT2" direction="out"/>
<pin name="OUT3" direction="out"/>
<pin name="OUT4" direction="out"/>
</symbol>
<symbol name="LM339M">
<pin name="V+" direction="pwr"/>
<pin name="-IN1" direction="in"/>
<pin name="+IN1" direction="in"/>
<pin name="-IN2" direction="in"/>
<pin name="+IN2" direction="in"/>
<pin name="-IN3" direction="in"/>
<pin name="+IN3" direction="in"/>
<pin name="-IN4" direction="in"/>
<pin name="+IN4" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT1" direction="out"/>
<pin name="OUT2" direction="out"/>
<pin name="OUT3" direction="out"/>
<pin name="OUT4" direction="out"/>
</symbol>
<symbol name="LM339N">
<pin name="V+" direction="pwr"/>
<pin name="-IN1" direction="in"/>
<pin name="+IN1" direction="in"/>
<pin name="-IN2" direction="in"/>
<pin name="+IN2" direction="in"/>
<pin name="-IN3" direction="in"/>
<pin name="+IN3" direction="in"/>
<pin name="-IN4" direction="in"/>
<pin name="+IN4" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT1" direction="out"/>
<pin name="OUT2" direction="out"/>
<pin name="OUT3" direction="out"/>
<pin name="OUT4" direction="out"/>
</symbol>
<symbol name="LM3401MM">
<pin name="VIN" direction="pwr"/>
<pin name="CS" direction="in"/>
<pin name="ILIM" direction="in"/>
<pin name="DIM" direction="in"/>
<pin name="HYS" direction="in"/>
<pin name="SNS" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="HG" direction="out"/>
</symbol>
<symbol name="LM3402HVMM">
<pin name="VCC" direction="pwr"/>
<pin name="VIN" direction="pwr"/>
<pin name="BOOT" direction="pas"/>
<pin name="CS" direction="in"/>
<pin name="DIM" direction="in"/>
<pin name="RON" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="SWITCH" direction="out"/>
</symbol>
<symbol name="LM3402HVMR">
<pin name="VCC" direction="pwr"/>
<pin name="VIN" direction="in"/>
<pin name="BOOT" direction="in"/>
<pin name="RON" direction="in"/>
<pin name="DIM" direction="in"/>
<pin name="CS" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM3402MM">
<pin name="VCC" direction="pwr"/>
<pin name="VIN" direction="pwr"/>
<pin name="BOOT" direction="pas"/>
<pin name="CS" direction="in"/>
<pin name="DIM" direction="in"/>
<pin name="RON" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="SWITCH" direction="out"/>
</symbol>
<symbol name="LM3402MR">
<pin name="VCC" direction="pwr"/>
<pin name="VIN" direction="in"/>
<pin name="BOOT" direction="in"/>
<pin name="RON" direction="in"/>
<pin name="DIM" direction="in"/>
<pin name="CS" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM3404HVMA">
<pin name="VCC" direction="pwr"/>
<pin name="BOOT" direction="in"/>
<pin name="DIM" direction="in"/>
<pin name="CS" direction="in"/>
<pin name="RON" direction="in"/>
<pin name="VIN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM3404MA">
<pin name="VCC" direction="pwr"/>
<pin name="VIN" direction="in"/>
<pin name="BOOT" direction="in"/>
<pin name="DIM" direction="in"/>
<pin name="RON" direction="in"/>
<pin name="CS" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM3405AXMK">
<pin name="VIN" direction="pwr"/>
<pin name="EN/DIM" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="BST" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM3405AXMY">
<pin name="VIN" direction="pwr"/>
<pin name="FB" direction="in"/>
<pin name="BOOST" direction="in"/>
<pin name="EN/DIM" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM3405XMK">
<pin name="VIN" direction="pwr"/>
<pin name="EN/DIM" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="BST" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM3406HVMH">
<pin name="VCC" direction="pwr"/>
<pin name="VIN_2" direction="in"/>
<pin name="VIN" direction="in"/>
<pin name="VINS" direction="in"/>
<pin name="BOOT" direction="in"/>
<pin name="DIM" direction="in"/>
<pin name="RON" direction="in"/>
<pin name="COMP" direction="in"/>
<pin name="CS" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="VOUT" direction="out"/>
<pin name="SW_2" direction="out"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM3406MH">
<pin name="VCC" direction="pwr"/>
<pin name="VIN_2" direction="in"/>
<pin name="VIN" direction="in"/>
<pin name="VINS" direction="in"/>
<pin name="BOOT" direction="in"/>
<pin name="DIM" direction="in"/>
<pin name="RON" direction="in"/>
<pin name="COMP" direction="in"/>
<pin name="CS" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="VOUT" direction="out"/>
<pin name="SW_2" direction="out"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM3407MY">
<pin name="VCC" direction="pwr"/>
<pin name="VIN" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="FS" direction="in"/>
<pin name="ISNS" direction="in"/>
<pin name="DIM" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="LX" direction="out"/>
</symbol>
<symbol name="LM3409HVMY">
<pin name="VCC" direction="pwr"/>
<pin name="VIN" direction="pwr"/>
<pin name="COFF" direction="in"/>
<pin name="CSN" direction="in"/>
<pin name="CSP" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="IADJ" direction="in"/>
<pin name="UVLO" direction="in"/>
<pin name="EP" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="PGATE" direction="out"/>
</symbol>
<symbol name="LM3409MY">
<pin name="VCC" direction="pwr"/>
<pin name="VIN" direction="pwr"/>
<pin name="COFF" direction="in"/>
<pin name="CSN" direction="in"/>
<pin name="CSP" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="IADJ" direction="in"/>
<pin name="UVLO" direction="in"/>
<pin name="EP" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="PGATE" direction="out"/>
</symbol>
<symbol name="LM3410XMF">
<pin name="VIN" direction="pwr"/>
<pin name="FB" direction="in"/>
<pin name="DIM" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM3410XMY">
<pin name="VIN" direction="pwr"/>
<pin name="DIM" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="AGND" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM3410XSD">
<pin name="VIN" direction="pwr"/>
<pin name="DIM" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="PGND" direction="pas"/>
<pin name="AGND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM3410YMF">
<pin name="VIN" direction="pwr"/>
<pin name="FB" direction="in"/>
<pin name="DIM" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM3410YMY">
<pin name="VIN" direction="pwr"/>
<pin name="DIM" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="AGND" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM3410YSD">
<pin name="VIN" direction="pwr"/>
<pin name="DIM" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="PGND" direction="pas"/>
<pin name="AGND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM3421MH">
<pin name="VCC" direction="pwr"/>
<pin name="VIN" direction="in"/>
<pin name="CSH" direction="in"/>
<pin name="RPD" direction="in"/>
<pin name="RCT" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="IS" direction="in"/>
<pin name="HSP" direction="in"/>
<pin name="HSN" direction="in"/>
<pin name="NDIM" direction="in"/>
<pin name="OVP" direction="in"/>
<pin name="COMP" direction="in"/>
<pin name="AGND" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="DDRV" direction="out"/>
<pin name="GATE" direction="out"/>
</symbol>
<symbol name="LM3423MH">
<pin name="VCC" direction="pwr"/>
<pin name="VIN" direction="in"/>
<pin name="CSH" direction="in"/>
<pin name="RPD" direction="in"/>
<pin name="RCT" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="IS" direction="in"/>
<pin name="HSP" direction="in"/>
<pin name="HSN" direction="in"/>
<pin name="NDIM" direction="in"/>
<pin name="OVP" direction="in"/>
<pin name="COMP" direction="in"/>
<pin name="AGND" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="DDRV" direction="out"/>
<pin name="GATE" direction="out"/>
</symbol>
<symbol name="LM3424MH">
<pin name="VCC" direction="pwr"/>
<pin name="VIN" direction="pwr"/>
<pin name="VS" direction="pwr"/>
<pin name="COMP" direction="pas"/>
<pin name="CSH" direction="pas"/>
<pin name="DDRV" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="HSN" direction="in"/>
<pin name="HSP" direction="in"/>
<pin name="IS" direction="in"/>
<pin name="NDIM" direction="in"/>
<pin name="OVP" direction="in"/>
<pin name="RT" direction="pas"/>
<pin name="SLOPE" direction="in"/>
<pin name="SS" direction="in"/>
<pin name="TGAIN" direction="in"/>
<pin name="TREF" direction="in"/>
<pin name="TSENSE" direction="in"/>
<pin name="DAP" direction="pas"/>
<pin name="GATE" direction="out"/>
<pin name="GND" direction="out"/>
</symbol>
<symbol name="LM3424QMH">
<pin name="VCC" direction="pwr"/>
<pin name="NDIM" direction="in"/>
<pin name="TREF" direction="in"/>
<pin name="OVP" direction="in"/>
<pin name="HSP" direction="in"/>
<pin name="HSN" direction="in"/>
<pin name="CSH" direction="in"/>
<pin name="TGAIN" direction="in"/>
<pin name="TSENSE" direction="in"/>
<pin name="SLOPE" direction="in"/>
<pin name="RT" direction="in"/>
<pin name="VS" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="SS" direction="in"/>
<pin name="IS" direction="in"/>
<pin name="VIN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="COMP" direction="out"/>
<pin name="GATE" direction="out"/>
<pin name="DDRV" direction="out"/>
</symbol>
<symbol name="LM3429MH">
<pin name="VCC" direction="pwr"/>
<pin name="VIN" direction="pwr"/>
<pin name="COMP" direction="pas"/>
<pin name="CSH" direction="in"/>
<pin name="HSN" direction="in"/>
<pin name="HSP" direction="in"/>
<pin name="IS" direction="in"/>
<pin name="NDIM" direction="in"/>
<pin name="OVP" direction="in"/>
<pin name="RCT" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="AGND" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="DAP" direction="pas"/>
<pin name="GATE" direction="out"/>
</symbol>
<symbol name="LM3430SD">
<pin name="VCC" direction="pwr"/>
<pin name="VIN" direction="in"/>
<pin name="CS" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="SS" direction="in"/>
<pin name="COMP" direction="in"/>
<pin name="VDHC" direction="in"/>
<pin name="UVLO" direction="in"/>
<pin name="RT/SYNC" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM3431AMH">
<pin name="VCC" direction="pwr"/>
<pin name="VIN" direction="pwr"/>
<pin name="CS" direction="in"/>
<pin name="FF" direction="in"/>
<pin name="SC" direction="in"/>
<pin name="RT" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="DLY" direction="in"/>
<pin name="DIM" direction="in"/>
<pin name="ILIM" direction="in"/>
<pin name="AFB" direction="in"/>
<pin name="REF" direction="in"/>
<pin name="CFB" direction="in"/>
<pin name="COMP" direction="in"/>
<pin name="THM" direction="in"/>
<pin name="MODE/F" direction="in"/>
<pin name="SS/SH" direction="in"/>
<pin name="REFIN" direction="in"/>
<pin name="LEDOFF" direction="in"/>
<pin name="SNS1" direction="in"/>
<pin name="SNS2" direction="in"/>
<pin name="SNS3" direction="in"/>
<pin name="SGND" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="LG" direction="out"/>
<pin name="NDRV1" direction="out"/>
<pin name="NDRV2" direction="out"/>
<pin name="NDRV3" direction="out"/>
</symbol>
<symbol name="LM3431AQMH">
<pin name="VCC" direction="pwr"/>
<pin name="ILIM" direction="in"/>
<pin name="SS/SH" direction="in"/>
<pin name="MODE/F" direction="in"/>
<pin name="REFIN" direction="in"/>
<pin name="SNS1" direction="in"/>
<pin name="SNS2" direction="in"/>
<pin name="SNS3" direction="in"/>
<pin name="CS" direction="in"/>
<pin name="FF" direction="in"/>
<pin name="RT" direction="in"/>
<pin name="REF" direction="in"/>
<pin name="DLY" direction="in"/>
<pin name="THM" direction="in"/>
<pin name="DIM" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="VIN" direction="in"/>
<pin name="SGND" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="AFB" direction="out"/>
<pin name="CFB" direction="out"/>
<pin name="COMP" direction="in"/>
<pin name="LEDOFF" direction="out"/>
<pin name="LG" direction="out"/>
<pin name="SC" direction="out"/>
<pin name="NDRV1" direction="out"/>
<pin name="NDRV2" direction="out"/>
<pin name="NDRV3" direction="out"/>
</symbol>
<symbol name="LM3431MH">
<pin name="VCC" direction="pwr"/>
<pin name="ILIM" direction="in"/>
<pin name="SS/SH" direction="in"/>
<pin name="MODE/F" direction="in"/>
<pin name="REFIN" direction="in"/>
<pin name="SNS1" direction="in"/>
<pin name="SNS2" direction="in"/>
<pin name="SNS3" direction="in"/>
<pin name="CS" direction="in"/>
<pin name="FF" direction="in"/>
<pin name="RT" direction="in"/>
<pin name="REF" direction="in"/>
<pin name="DLY" direction="in"/>
<pin name="THM" direction="in"/>
<pin name="DIM" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="VIN" direction="in"/>
<pin name="SGND" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="AFB" direction="out"/>
<pin name="CFB" direction="out"/>
<pin name="COMP" direction="in"/>
<pin name="LEDOFF" direction="out"/>
<pin name="LG" direction="out"/>
<pin name="SC" direction="out"/>
<pin name="NDRV1" direction="out"/>
<pin name="NDRV2" direction="out"/>
<pin name="NDRV3" direction="out"/>
</symbol>
<symbol name="LM3431QMH">
<pin name="VCC" direction="pwr"/>
<pin name="ILIM" direction="in"/>
<pin name="SS/SH" direction="in"/>
<pin name="MODE/F" direction="in"/>
<pin name="REFIN" direction="in"/>
<pin name="SNS1" direction="in"/>
<pin name="SNS2" direction="in"/>
<pin name="SNS3" direction="in"/>
<pin name="CS" direction="in"/>
<pin name="FF" direction="in"/>
<pin name="RT" direction="in"/>
<pin name="REF" direction="in"/>
<pin name="DLY" direction="in"/>
<pin name="THM" direction="in"/>
<pin name="DIM" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="VIN" direction="in"/>
<pin name="SGND" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="AFB" direction="out"/>
<pin name="CFB" direction="out"/>
<pin name="COMP" direction="in"/>
<pin name="LEDOFF" direction="out"/>
<pin name="LG" direction="out"/>
<pin name="SC" direction="out"/>
<pin name="NDRV1" direction="out"/>
<pin name="NDRV2" direction="out"/>
<pin name="NDRV3" direction="out"/>
</symbol>
<symbol name="LM3432MH">
<pin name="VCC" direction="pwr"/>
<pin name="VIN" direction="pwr"/>
<pin name="EN" direction="in"/>
<pin name="DIM" direction="in"/>
<pin name="MODE" direction="in"/>
<pin name="IREF" direction="in"/>
<pin name="CDHC" direction="in"/>
<pin name="FAULTB" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC_6" direction="nc"/>
<pin name="NC_7" direction="nc"/>
<pin name="NC_8" direction="nc"/>
<pin name="NC_9" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="AGND" direction="pas"/>
<pin name="PGND_2" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="IOUT1" direction="out"/>
<pin name="IOUT2" direction="out"/>
<pin name="IOUT3" direction="out"/>
<pin name="IOUT4" direction="out"/>
<pin name="IOUT5" direction="out"/>
<pin name="IOUT6" direction="out"/>
<pin name="OTMB" direction="out"/>
<pin name="VDHC" direction="out"/>
</symbol>
<symbol name="LM3433SQ">
<pin name="VCC" direction="pwr"/>
<pin name="SS" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="LS" direction="in"/>
<pin name="HS" direction="in"/>
<pin name="TON" direction="in"/>
<pin name="ADJ" direction="in"/>
<pin name="BST" direction="in"/>
<pin name="BST2" direction="in"/>
<pin name="CSN" direction="in"/>
<pin name="CSP" direction="in"/>
<pin name="COMP" direction="in"/>
<pin name="DIMR" direction="in"/>
<pin name="DIM" direction="in"/>
<pin name="VIN" direction="pwr"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="VEE" direction="pwr"/>
<pin name="CGND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="DIMO" direction="out"/>
<pin name="LO" direction="out"/>
<pin name="HO" direction="out"/>
</symbol>
<symbol name="LM3445MM">
<pin name="VCC" direction="pwr"/>
<pin name="BLDR" direction="in"/>
<pin name="COFF" direction="in"/>
<pin name="FLTR1" direction="in"/>
<pin name="FLTR2" direction="in"/>
<pin name="GATE" direction="in"/>
<pin name="ISNS" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="ASNS" direction="out"/>
<pin name="DIM"/>
</symbol>
<symbol name="LM346M">
<pin name="V+" direction="pwr"/>
<pin name="SET_A,B,D" direction="in"/>
<pin name="SET_C" direction="in"/>
<pin name="-INA" direction="in"/>
<pin name="+INA" direction="in"/>
<pin name="+INB" direction="in"/>
<pin name="-INB" direction="in"/>
<pin name="-INC" direction="in"/>
<pin name="+INC" direction="in"/>
<pin name="+IND" direction="in"/>
<pin name="-IND" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
<pin name="OUTC" direction="out"/>
<pin name="OUTD" direction="out"/>
</symbol>
<symbol name="LM3475MF">
<pin name="VIN" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="PGATE" direction="out"/>
</symbol>
<symbol name="LM3477MM">
<pin name="VIN" direction="pwr"/>
<pin name="FB" direction="in"/>
<pin name="DR" direction="in"/>
<pin name="CB" direction="in"/>
<pin name="ISEN" direction="in"/>
<pin name="COMP/~SD" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM3478MM">
<pin name="VIN" direction="pwr"/>
<pin name="FB" direction="in"/>
<pin name="FA/SD" direction="pas"/>
<pin name="COMP" direction="in"/>
<pin name="ISEN" direction="in"/>
<pin name="AGND" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="DR" direction="out"/>
</symbol>
<symbol name="LM3478QMM">
<pin name="VIN" direction="pwr"/>
<pin name="ISENS" direction="in"/>
<pin name="COMP" direction="in"/>
<pin name="DR" direction="in"/>
<pin name="FA/SD" direction="in"/>
<pin name="AGND" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="FB" direction="out"/>
</symbol>
<symbol name="LM3480IM3-12">
<pin name="IN" direction="pwr"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM3480IM3-15">
<pin name="IN" direction="pwr"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM3480IM3-3.3">
<pin name="IN" direction="pwr"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM3480IM3-5.0">
<pin name="IN" direction="pwr"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM3481MM">
<pin name="VCC" direction="pwr"/>
<pin name="FB" direction="in"/>
<pin name="UVLO" direction="in"/>
<pin name="COMP" direction="in"/>
<pin name="ISEN" direction="in"/>
<pin name="FA/SYNC/SD" direction="in"/>
<pin name="VIN" direction="in"/>
<pin name="AGND" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="DR" direction="out"/>
</symbol>
<symbol name="LM3485MM">
<pin name="VIN" direction="pwr"/>
<pin name="ISENSE" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="ADJ" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="PWRGND" direction="pas"/>
<pin name="PGATE" direction="out"/>
</symbol>
<symbol name="LM3488MM">
<pin name="VIN" direction="pwr"/>
<pin name="FB" direction="in"/>
<pin name="ISEN" direction="in"/>
<pin name="COMP" direction="in"/>
<pin name="FA/SYNC/SD" direction="in"/>
<pin name="AGND" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="DR" direction="out"/>
</symbol>
<symbol name="LM3488QMM">
<pin name="VIN" direction="pwr"/>
<pin name="ISENS" direction="in"/>
<pin name="COMP" direction="in"/>
<pin name="DR" direction="in"/>
<pin name="FA/SYNC/SD" direction="in"/>
<pin name="AGND" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="FB" direction="out"/>
</symbol>
<symbol name="LM3489MM">
<pin name="VIN" direction="pwr"/>
<pin name="ADJ" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="ISENSE" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="PGATE" direction="out"/>
</symbol>
<symbol name="LM3489QMM">
<pin name="VIN" direction="pwr"/>
<pin name="ISENSE" direction="in"/>
<pin name="ADJ" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="PGND" direction="pas"/>
<pin name="PGATE" direction="out"/>
</symbol>
<symbol name="LM348M">
<pin name="V+" direction="pwr"/>
<pin name="-IN1" direction="in"/>
<pin name="+IN1" direction="in"/>
<pin name="+IN2" direction="in"/>
<pin name="-IN2" direction="in"/>
<pin name="-IN3" direction="in"/>
<pin name="+IN3" direction="in"/>
<pin name="+IN4" direction="in"/>
<pin name="-IN4" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT1" direction="out"/>
<pin name="OUT2" direction="out"/>
<pin name="OUT3" direction="out"/>
<pin name="OUT4" direction="out"/>
</symbol>
<symbol name="LM34910SD">
<pin name="VCC" direction="pwr"/>
<pin name="VIN" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="SS" direction="in"/>
<pin name="BST" direction="in"/>
<pin name="ISEN" direction="in"/>
<pin name="RTN" direction="in"/>
<pin name="SD/RON" direction="in"/>
<pin name="SGND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM34917ATL">
<pin name="VIN_2" direction="pwr"/>
<pin name="VIN" direction="pwr"/>
<pin name="RON/SD" direction="in"/>
<pin name="SS" direction="in"/>
<pin name="RTN" direction="pwr"/>
<pin name="SGND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="BST" direction="in"/>
<pin name="SW_2" direction="pwr"/>
<pin name="SW" direction="pwr"/>
<pin name="ISEN" direction="in"/>
<pin name="FB" direction="in"/>
</symbol>
<symbol name="LM34930TL">
<pin name="VCC" direction="pwr"/>
<pin name="VIN_2" direction="pwr"/>
<pin name="VIN" direction="pwr"/>
<pin name="BST" direction="in"/>
<pin name="RT" direction="in"/>
<pin name="SW_2" direction="in"/>
<pin name="SW" direction="in"/>
<pin name="SS" direction="in"/>
<pin name="NOV" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="FB" direction="out"/>
<pin name="ISEN" direction="pas"/>
</symbol>
<symbol name="LM3495MTC">
<pin name="VIN" direction="pwr"/>
<pin name="FB" direction="in"/>
<pin name="CSL" direction="in"/>
<pin name="SNS" direction="in"/>
<pin name="~FPWM" direction="in"/>
<pin name="BOOST" direction="in"/>
<pin name="TRACK" direction="in"/>
<pin name="ILIM" direction="in"/>
<pin name="FREQ/SYNC" direction="in"/>
<pin name="COMP/~SD" direction="in"/>
<pin name="VLIN5" direction="in"/>
<pin name="SGND" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="HG" direction="out"/>
<pin name="LG" direction="out"/>
<pin name="SW/CSH" direction="out"/>
</symbol>
<symbol name="LM3500TL-16">
<pin name="AGND" direction="pas"/>
<pin name="SHDN" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="VIN" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="VOUT" direction="out"/>
<pin name="VSW" direction="in"/>
<pin name="GND" direction="pas"/>
</symbol>
<symbol name="LM3500TL-21">
<pin name="AGND" direction="pas"/>
<pin name="SHDN" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="VIN" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="VOUT" direction="out"/>
<pin name="VSW" direction="in"/>
<pin name="GND" direction="pas"/>
</symbol>
<symbol name="LM3501TL-16">
<pin name="VIN" direction="in"/>
<pin name="SHDN" direction="in"/>
<pin name="CNTRL" direction="nc"/>
<pin name="AGND" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="FB" direction="in"/>
<pin name="VOUT" direction="out"/>
<pin name="VSW" direction="in"/>
</symbol>
<symbol name="LM3501TL-21">
<pin name="VIN" direction="in"/>
<pin name="SHDN" direction="in"/>
<pin name="CNTRL" direction="nc"/>
<pin name="AGND" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="FB" direction="in"/>
<pin name="VOUT" direction="out"/>
<pin name="VSW" direction="in"/>
</symbol>
<symbol name="LM3502ITL-16">
<pin name="VIN" direction="in"/>
<pin name="CNTRL" direction="in"/>
<pin name="EN1" direction="in"/>
<pin name="EN2" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="PGND" direction="pas"/>
<pin name="AGND" direction="pas"/>
<pin name="VOUT2" direction="out"/>
<pin name="VOUT1" direction="out"/>
<pin name="SW" direction="in"/>
</symbol>
<symbol name="LM3502ITL-25">
<pin name="VIN" direction="in"/>
<pin name="CNTRL" direction="in"/>
<pin name="EN1" direction="in"/>
<pin name="EN2" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="PGND" direction="pas"/>
<pin name="AGND" direction="pas"/>
<pin name="VOUT2" direction="out"/>
<pin name="VOUT1" direction="out"/>
<pin name="SW" direction="in"/>
</symbol>
<symbol name="LM3502ITL-35">
<pin name="VIN" direction="in"/>
<pin name="CNTRL" direction="in"/>
<pin name="EN1" direction="in"/>
<pin name="EN2" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="PGND" direction="pas"/>
<pin name="AGND" direction="pas"/>
<pin name="VOUT2" direction="out"/>
<pin name="VOUT1" direction="out"/>
<pin name="SW" direction="in"/>
</symbol>
<symbol name="LM3502ITL-44">
<pin name="VIN" direction="in"/>
<pin name="CNTRL" direction="in"/>
<pin name="EN1" direction="in"/>
<pin name="EN2" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="PGND" direction="pas"/>
<pin name="AGND" direction="pas"/>
<pin name="VOUT2" direction="out"/>
<pin name="VOUT1" direction="out"/>
<pin name="SW" direction="in"/>
</symbol>
<symbol name="LM3502SQ-16">
<pin name="SW_2" direction="out"/>
<pin name="SW" direction="out"/>
<pin name="FB" direction="pas"/>
<pin name="VIN" direction="in"/>
<pin name="AGND" direction="pas"/>
<pin name="PGND_2" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="NC_2" direction="pas"/>
<pin name="NC_3" direction="pas"/>
<pin name="NC_4" direction="pas"/>
<pin name="NC" direction="pas"/>
<pin name="CNTRL" direction="pas"/>
<pin name="EN1" direction="pas"/>
<pin name="EN2" direction="pas"/>
<pin name="VOUT2" direction="out"/>
<pin name="VOUT1" direction="out"/>
<pin name="EP" direction="pas"/>
</symbol>
<symbol name="LM3502SQ-25">
<pin name="SW_2" direction="out"/>
<pin name="SW" direction="out"/>
<pin name="FB" direction="pas"/>
<pin name="VIN" direction="in"/>
<pin name="AGND" direction="pas"/>
<pin name="PGND_2" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="NC_2" direction="pas"/>
<pin name="NC_3" direction="pas"/>
<pin name="NC_4" direction="pas"/>
<pin name="NC" direction="pas"/>
<pin name="CNTRL" direction="pas"/>
<pin name="EN1" direction="pas"/>
<pin name="EN2" direction="pas"/>
<pin name="VOUT2" direction="out"/>
<pin name="VOUT1" direction="out"/>
<pin name="EP" direction="pas"/>
</symbol>
<symbol name="LM3502SQ-35">
<pin name="SW_2" direction="out"/>
<pin name="SW" direction="out"/>
<pin name="FB" direction="pas"/>
<pin name="VIN" direction="in"/>
<pin name="AGND" direction="pas"/>
<pin name="PGND_2" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="NC_2" direction="pas"/>
<pin name="NC_3" direction="pas"/>
<pin name="NC_4" direction="pas"/>
<pin name="NC" direction="pas"/>
<pin name="CNTRL" direction="pas"/>
<pin name="EN1" direction="pas"/>
<pin name="EN2" direction="pas"/>
<pin name="VOUT2" direction="out"/>
<pin name="VOUT1" direction="out"/>
<pin name="EP" direction="pas"/>
</symbol>
<symbol name="LM3502SQ-44">
<pin name="SW_2" direction="out"/>
<pin name="SW" direction="out"/>
<pin name="FB" direction="pas"/>
<pin name="VIN" direction="in"/>
<pin name="AGND" direction="pas"/>
<pin name="PGND_2" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="NC_2" direction="pas"/>
<pin name="NC_3" direction="pas"/>
<pin name="NC_4" direction="pas"/>
<pin name="NC" direction="pas"/>
<pin name="CNTRL" direction="pas"/>
<pin name="EN1" direction="pas"/>
<pin name="EN2" direction="pas"/>
<pin name="VOUT2" direction="out"/>
<pin name="VOUT1" direction="out"/>
<pin name="EP" direction="pas"/>
</symbol>
<symbol name="LM3503ITL-16">
<pin name="VIN" direction="in"/>
<pin name="CNTRL" direction="in"/>
<pin name="EN1" direction="in"/>
<pin name="EN2" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="PGND" direction="pas"/>
<pin name="AGND" direction="pas"/>
<pin name="VOUT2" direction="out"/>
<pin name="VOUT1" direction="out"/>
<pin name="SW" direction="in"/>
</symbol>
<symbol name="LM3503ITL-25">
<pin name="VIN" direction="in"/>
<pin name="CNTRL" direction="in"/>
<pin name="EN1" direction="in"/>
<pin name="EN2" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="PGND" direction="pas"/>
<pin name="AGND" direction="pas"/>
<pin name="VOUT2" direction="out"/>
<pin name="VOUT1" direction="out"/>
<pin name="SW" direction="in"/>
</symbol>
<symbol name="LM3503ITL-35">
<pin name="VIN" direction="in"/>
<pin name="CNTRL" direction="in"/>
<pin name="EN1" direction="in"/>
<pin name="EN2" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="PGND" direction="pas"/>
<pin name="AGND" direction="pas"/>
<pin name="VOUT2" direction="out"/>
<pin name="VOUT1" direction="out"/>
<pin name="SW" direction="in"/>
</symbol>
<symbol name="LM3503ITL-44">
<pin name="VIN" direction="in"/>
<pin name="CNTRL" direction="in"/>
<pin name="EN1" direction="in"/>
<pin name="EN2" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="PGND" direction="pas"/>
<pin name="AGND" direction="pas"/>
<pin name="VOUT2" direction="out"/>
<pin name="VOUT1" direction="out"/>
<pin name="SW" direction="in"/>
</symbol>
<symbol name="LM3503SQ-16">
<pin name="VIN" direction="pwr"/>
<pin name="FB" direction="in"/>
<pin name="SW_2" direction="in"/>
<pin name="SW" direction="in"/>
<pin name="CNTRL" direction="in"/>
<pin name="EN1" direction="in"/>
<pin name="EN2" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="AGND" direction="pas"/>
<pin name="PGND_2" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="HEAT_PAD" direction="pas"/>
<pin name="VOUT1" direction="out"/>
<pin name="VOUT2" direction="out"/>
</symbol>
<symbol name="LM3503SQ-25">
<pin name="VIN" direction="pwr"/>
<pin name="FB" direction="in"/>
<pin name="SW_2" direction="in"/>
<pin name="SW" direction="in"/>
<pin name="CNTRL" direction="in"/>
<pin name="EN1" direction="in"/>
<pin name="EN2" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="AGND" direction="pas"/>
<pin name="PGND_2" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="HEAT_PAD" direction="pas"/>
<pin name="VOUT1" direction="out"/>
<pin name="VOUT2" direction="out"/>
</symbol>
<symbol name="LM3503SQ-35">
<pin name="VIN" direction="pwr"/>
<pin name="FB" direction="in"/>
<pin name="SW_2" direction="in"/>
<pin name="SW" direction="in"/>
<pin name="CNTRL" direction="in"/>
<pin name="EN1" direction="in"/>
<pin name="EN2" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="AGND" direction="pas"/>
<pin name="PGND_2" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="HEAT_PAD" direction="pas"/>
<pin name="VOUT1" direction="out"/>
<pin name="VOUT2" direction="out"/>
</symbol>
<symbol name="LM3503SQ-44">
<pin name="VIN" direction="pwr"/>
<pin name="FB" direction="in"/>
<pin name="SW_2" direction="in"/>
<pin name="SW" direction="in"/>
<pin name="CNTRL" direction="in"/>
<pin name="EN1" direction="in"/>
<pin name="EN2" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="AGND" direction="pas"/>
<pin name="PGND_2" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="HEAT_PAD" direction="pas"/>
<pin name="VOUT1" direction="out"/>
<pin name="VOUT2" direction="out"/>
</symbol>
<symbol name="LM3519MK-20">
<pin name="VIN" direction="pwr"/>
<pin name="EN" direction="in"/>
<pin name="LED_RTN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="SW" direction="out"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LM3525M-H">
<pin name="IN" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="FLAG" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="OUT_2" direction="out"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM3525M-L">
<pin name="IN" direction="in"/>
<pin name="~EN" direction="in"/>
<pin name="FLAG" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="OUT_2" direction="out"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM3526M-H">
<pin name="IN" direction="pwr"/>
<pin name="FLAGA" direction="in"/>
<pin name="FLAGB" direction="in"/>
<pin name="ENA" direction="in"/>
<pin name="ENB" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="LM3526M-L">
<pin name="IN" direction="pwr"/>
<pin name="FLAGA" direction="in"/>
<pin name="FLAGB" direction="in"/>
<pin name="~ENA" direction="in"/>
<pin name="~ENB" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="LM3528TME">
<pin name="IN" direction="pwr"/>
<pin name="SUB/FB" direction="in"/>
<pin name="OVP" direction="in"/>
<pin name="VIO" direction="in"/>
<pin name="SCL" direction="in"/>
<pin name="SET" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="HWEN/PGEN/GPIO"/>
<pin name="MAIN" direction="in"/>
<pin name="GPIO1"/>
<pin name="SDA"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM3544M-L">
<pin name="IN1" direction="pwr"/>
<pin name="IN2" direction="pwr"/>
<pin name="~EN1" direction="in"/>
<pin name="~EN2" direction="in"/>
<pin name="~EN3" direction="in"/>
<pin name="~EN4" direction="in"/>
<pin name="FLAG1" direction="in"/>
<pin name="FLAG2" direction="in"/>
<pin name="FLAG3" direction="in"/>
<pin name="FLAG4" direction="in"/>
<pin name="GND1" direction="pas"/>
<pin name="GND2" direction="pas"/>
<pin name="OUT1" direction="out"/>
<pin name="OUT2" direction="out"/>
<pin name="OUT3" direction="out"/>
<pin name="OUT4" direction="out"/>
</symbol>
<symbol name="LM3551SD">
<pin name="VIN" direction="pwr"/>
<pin name="FET-T" direction="in"/>
<pin name="FET-F" direction="in"/>
<pin name="VC" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="SD" direction="in"/>
<pin name="SS" direction="in"/>
<pin name="OVP" direction="in"/>
<pin name="FTO" direction="in"/>
<pin name="T/F" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="AGND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM3552SD">
<pin name="VIN" direction="pwr"/>
<pin name="FET-T" direction="in"/>
<pin name="FET-F" direction="in"/>
<pin name="VC" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="SS" direction="in"/>
<pin name="OVP" direction="in"/>
<pin name="FTO" direction="in"/>
<pin name="T/F" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="AGND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM3553SD">
<pin name="VIN" direction="pwr"/>
<pin name="SCL" direction="in"/>
<pin name="FEN" direction="in"/>
<pin name="ISET" direction="in"/>
<pin name="OVP" direction="in"/>
<pin name="VIO" direction="in"/>
<pin name="TX" direction="in"/>
<pin name="D1" direction="in"/>
<pin name="D2" direction="in"/>
<pin name="EPAD" direction="pas"/>
<pin name="SW" direction="out"/>
<pin name="M/F"/>
<pin name="SDA"/>
</symbol>
<symbol name="LM3557SD-2">
<pin name="VIN" direction="pwr"/>
<pin name="EN" direction="in"/>
<pin name="OVP" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="SW1" direction="out"/>
<pin name="SW2" direction="out"/>
</symbol>
<symbol name="LM358AM">
<pin name="V+" direction="pwr"/>
<pin name="NEGA" direction="in"/>
<pin name="POSA" direction="in"/>
<pin name="POSB" direction="in"/>
<pin name="NEGB" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="LM358AN">
<pin name="V+" direction="pwr"/>
<pin name="NEG_A" direction="in"/>
<pin name="POS_A" direction="in"/>
<pin name="POS_B" direction="in"/>
<pin name="NEG_B" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="LM358M">
<pin name="V+" direction="pwr"/>
<pin name="NEGA" direction="in"/>
<pin name="POSA" direction="in"/>
<pin name="POSB" direction="in"/>
<pin name="NEGB" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="LM358N">
<pin name="V+" direction="pwr"/>
<pin name="NEG_A" direction="in"/>
<pin name="POS_A" direction="in"/>
<pin name="POS_B" direction="in"/>
<pin name="NEG_B" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="LM359M">
<pin name="V+" direction="pwr"/>
<pin name="ISET_(IN)" direction="in"/>
<pin name="-INA" direction="in"/>
<pin name="+INA" direction="in"/>
<pin name="+INB" direction="in"/>
<pin name="-INB" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND_A" direction="pas"/>
<pin name="GND_B" direction="pas"/>
<pin name="ISET_(OUT)" direction="out"/>
<pin name="VOUTA" direction="out"/>
<pin name="VOUTB" direction="out"/>
<pin name="COMP_A" direction="out"/>
<pin name="COMP_B" direction="out"/>
</symbol>
<symbol name="LM35AH">
<pin name="+VS" direction="pwr"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LM35CAH">
<pin name="+VS" direction="pwr"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LM35CAZ">
<pin name="+VS" direction="pwr"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LM35CZ">
<pin name="+VS" direction="pwr"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LM35DM">
<pin name="+VS" direction="pwr"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LM35DZ">
<pin name="+VS" direction="pwr"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LM360M">
<pin name="V+" direction="pwr"/>
<pin name="IN1" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="V-" direction="pwr"/>
<pin name="GND" direction="pas"/>
<pin name="OUT1" direction="out"/>
<pin name="OUT2" direction="out"/>
</symbol>
<symbol name="LM361M">
<pin name="+IN" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="V-" direction="pas"/>
<pin name="V+" direction="pas"/>
<pin name="VCC" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="NC_2" direction="pas"/>
<pin name="NC_3" direction="pas"/>
<pin name="NC_4" direction="pas"/>
<pin name="NC" direction="pas"/>
<pin name="STROBE2" direction="pas"/>
<pin name="STROBE1" direction="pas"/>
<pin name="OUT-" direction="out"/>
<pin name="OUT+" direction="out"/>
</symbol>
<symbol name="LM361N">
<pin name="VCC" direction="pwr"/>
<pin name="V+" direction="pwr"/>
<pin name="IN1" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="STRB1" direction="pas"/>
<pin name="STRB2" direction="pas"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT1" direction="out"/>
<pin name="OUT2" direction="out"/>
</symbol>
<symbol name="LM3668SD-2833">
<pin name="VDD" direction="pwr"/>
<pin name="PVIN" direction="in"/>
<pin name="VSEL" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="MODE/SYNC" direction="in"/>
<pin name="SW1" direction="in"/>
<pin name="SW2" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="PGND" direction="pas"/>
<pin name="SGND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LM3670MF-1.2">
<pin name="VIN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="EN" direction="pas"/>
<pin name="FB" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM3670MF-1.8">
<pin name="VIN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="EN" direction="pas"/>
<pin name="FB" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM3670MF-3.3">
<pin name="VIN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="EN" direction="pas"/>
<pin name="FB" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM3670MF-ADJ">
<pin name="VIN" direction="pwr"/>
<pin name="EN" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM3671MF-1.2">
<pin name="VIN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="EN" direction="pas"/>
<pin name="FB" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM3671MF-1.25">
<pin name="VIN" direction="pwr"/>
<pin name="EN" direction="in"/>
<pin name="SW" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="FB"/>
</symbol>
<symbol name="LM3671MF-1.5">
<pin name="VIN" direction="pwr"/>
<pin name="EN" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM3671MF-1.8">
<pin name="VIN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="EN" direction="pas"/>
<pin name="FB" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM3671MF-1.875">
<pin name="VIN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="EN" direction="pas"/>
<pin name="FB" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM3671MF-2.5">
<pin name="VIN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="EN" direction="pas"/>
<pin name="FB" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM3671MF-3.3">
<pin name="VIN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="EN" direction="pas"/>
<pin name="FB" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM3671MF-ADJ">
<pin name="VIN" direction="pwr"/>
<pin name="EN" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM3671TL-1.2">
<pin name="VIN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="SW" direction="pas"/>
<pin name="EN" direction="pas"/>
<pin name="FB" direction="pas"/>
</symbol>
<symbol name="LM3671TL-1.8">
<pin name="VIN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="SW" direction="pas"/>
<pin name="EN" direction="pas"/>
<pin name="FB" direction="pas"/>
</symbol>
<symbol name="LM3671TL-3.3">
<pin name="VIN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="SW" direction="pas"/>
<pin name="EN" direction="pas"/>
<pin name="FB" direction="pas"/>
</symbol>
<symbol name="LM3673TL-1.2">
<pin name="VIN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="SW" direction="pas"/>
<pin name="EN" direction="pas"/>
<pin name="FB" direction="pas"/>
</symbol>
<symbol name="LM3673TL-1.5">
<pin name="VIN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="SW" direction="pas"/>
<pin name="EN" direction="pas"/>
<pin name="FB" direction="pas"/>
</symbol>
<symbol name="LM3673TL-ADJ">
<pin name="VIN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="SW" direction="pas"/>
<pin name="EN" direction="pas"/>
<pin name="FB" direction="pas"/>
</symbol>
<symbol name="LM3674MF-1.2">
<pin name="VIN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="EN" direction="pas"/>
<pin name="FB" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM3674MF-1.5">
<pin name="VIN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="EN" direction="pas"/>
<pin name="FB" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM3674MF-1.8">
<pin name="VIN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="EN" direction="pas"/>
<pin name="FB" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM3674MF-1.875">
<pin name="VIN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="EN" direction="pas"/>
<pin name="FB" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM3674MF-2.8">
<pin name="VIN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="EN" direction="pas"/>
<pin name="FB" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM3674MF-ADJ">
<pin name="VIN" direction="pwr"/>
<pin name="EN" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM3676SD-1.5">
<pin name="VIN" direction="in"/>
<pin name="PGND" direction="pas"/>
<pin name="SW" direction="out"/>
<pin name="MODE" direction="pas"/>
<pin name="FB" direction="pas"/>
<pin name="EN" direction="pas"/>
<pin name="NC" direction="pas"/>
<pin name="SGND" direction="pas"/>
<pin name="ANY" direction="pas"/>
</symbol>
<symbol name="LM3676SD-1.8">
<pin name="VIN" direction="in"/>
<pin name="PGND" direction="pas"/>
<pin name="SW" direction="out"/>
<pin name="MODE" direction="pas"/>
<pin name="FB" direction="pas"/>
<pin name="EN" direction="pas"/>
<pin name="NC" direction="pas"/>
<pin name="SGND" direction="pas"/>
<pin name="ANY" direction="pas"/>
</symbol>
<symbol name="LM3676SD-3.3">
<pin name="VIN" direction="in"/>
<pin name="PGND" direction="pas"/>
<pin name="SW" direction="out"/>
<pin name="MODE" direction="pas"/>
<pin name="FB" direction="pas"/>
<pin name="EN" direction="pas"/>
<pin name="NC" direction="pas"/>
<pin name="SGND" direction="pas"/>
<pin name="ANY" direction="pas"/>
</symbol>
<symbol name="LM3676SD-ADJ">
<pin name="VIN" direction="in"/>
<pin name="PGND" direction="pas"/>
<pin name="SW" direction="out"/>
<pin name="MODE" direction="pas"/>
<pin name="FB" direction="pas"/>
<pin name="EN" direction="pas"/>
<pin name="NC" direction="pas"/>
<pin name="SGND" direction="pas"/>
<pin name="ANY" direction="pas"/>
</symbol>
<symbol name="LM3677TL-ADJ">
<pin name="VIN" direction="pwr"/>
<pin name="EN" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM3686TLE-AAEF">
<pin name="VIN_LILO" direction="pwr"/>
<pin name="VIN_LDO" direction="pwr"/>
<pin name="FB_DCDC" direction="in"/>
<pin name="VBATT" direction="in"/>
<pin name="EN_LILO" direction="in"/>
<pin name="EN_LDO" direction="in"/>
<pin name="EN_DCDC" direction="in"/>
<pin name="PGND" direction="pas"/>
<pin name="QGND" direction="pas"/>
<pin name="SW" direction="out"/>
<pin name="VOUT_LDO" direction="out"/>
<pin name="VOUT_LILO" direction="out"/>
</symbol>
<symbol name="LM3704YCMM-308">
<pin name="VCC" direction="pwr"/>
<pin name="~MR" direction="in"/>
<pin name="PFI" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="~LLO" direction="out"/>
<pin name="~PFO" direction="out"/>
<pin name="~RESET" direction="out"/>
</symbol>
<symbol name="LM3710XQMM-308">
<pin name="VCC" direction="pwr"/>
<pin name="~MR" direction="in"/>
<pin name="PFI" direction="in"/>
<pin name="WDI" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="~LLO" direction="out"/>
<pin name="~PFO" direction="out"/>
<pin name="~RESET" direction="out"/>
</symbol>
<symbol name="LM3724EM5-3.08">
<pin name="VCC" direction="pwr"/>
<pin name="~MR" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="~RESET" direction="pas"/>
</symbol>
<symbol name="LM3724EM5-4.63">
<pin name="VCC" direction="pwr"/>
<pin name="~MR" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="~RESET" direction="pas"/>
</symbol>
<symbol name="LM3724IM5-2.32">
<pin name="VCC" direction="pwr"/>
<pin name="~MR" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="~RESET" direction="out"/>
</symbol>
<symbol name="LM3724IM5-3.08">
<pin name="VCC" direction="pwr"/>
<pin name="~MR" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="~RESET" direction="pas"/>
</symbol>
<symbol name="LM3724IM5-4.63">
<pin name="VCC" direction="pwr"/>
<pin name="~MR" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="~RESET" direction="out"/>
</symbol>
<symbol name="LM3743MM-1000">
<pin name="VCC" direction="pwr"/>
<pin name="ILIM" direction="in"/>
<pin name="LGATE" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="SS/TRACK" direction="in"/>
<pin name="SW" direction="in"/>
<pin name="HGATE" direction="in"/>
<pin name="BOOT" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="COMP/EN" direction="out"/>
</symbol>
<symbol name="LM3753SQ">
<pin name="VDD" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="~FAULT" direction="in"/>
<pin name="CS1" direction="in"/>
<pin name="CS2" direction="in"/>
<pin name="BOOT1" direction="pas"/>
<pin name="BOOT2" direction="in"/>
<pin name="IAVE" direction="in"/>
<pin name="NBASE" direction="pas"/>
<pin name="ILIM" direction="in"/>
<pin name="COMP" direction="in"/>
<pin name="VDIF" direction="in"/>
<pin name="FREQ" direction="in"/>
<pin name="SYNC" direction="in"/>
<pin name="CSM" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="SS" direction="in"/>
<pin name="PH" direction="in"/>
<pin name="SNSM" direction="in"/>
<pin name="SNSP" direction="in"/>
<pin name="VIN" direction="in"/>
<pin name="SGND" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="LG1" direction="out"/>
<pin name="LG2" direction="out"/>
<pin name="HG1" direction="out"/>
<pin name="HG2" direction="out"/>
<pin name="SW1" direction="out"/>
<pin name="SW2" direction="out"/>
<pin name="PGOOD" direction="out"/>
<pin name="SYNCOUT" direction="out"/>
</symbol>
<symbol name="LM3754SQ">
<pin name="VDD" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="~FAULT" direction="in"/>
<pin name="CS1" direction="in"/>
<pin name="CS2" direction="in"/>
<pin name="BOOT1" direction="pas"/>
<pin name="BOOT2" direction="in"/>
<pin name="IAVE" direction="in"/>
<pin name="NBASE" direction="pas"/>
<pin name="ILIM" direction="in"/>
<pin name="COMP" direction="in"/>
<pin name="VDIF" direction="in"/>
<pin name="FREQ" direction="in"/>
<pin name="SYNC" direction="in"/>
<pin name="CSM" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="SS" direction="in"/>
<pin name="PH" direction="in"/>
<pin name="SNSM" direction="in"/>
<pin name="SNSP" direction="in"/>
<pin name="VIN" direction="in"/>
<pin name="SGND" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="LG1" direction="out"/>
<pin name="LG2" direction="out"/>
<pin name="HG1" direction="out"/>
<pin name="HG2" direction="out"/>
<pin name="SW1" direction="out"/>
<pin name="SW2" direction="out"/>
<pin name="PGOOD" direction="out"/>
<pin name="SYNCOUT" direction="out"/>
</symbol>
<symbol name="LM3880MF-1AB">
<pin name="VCC" direction="pwr"/>
<pin name="EN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="FLAG1" direction="out"/>
<pin name="FLAG2" direction="out"/>
<pin name="FLAG3" direction="out"/>
</symbol>
<symbol name="LM3881MM">
<pin name="VCC" direction="pwr"/>
<pin name="EN" direction="in"/>
<pin name="TADJ" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="INV" direction="out"/>
<pin name="FLAG1" direction="out"/>
<pin name="FLAG2" direction="out"/>
<pin name="FLAG3" direction="out"/>
</symbol>
<symbol name="LM3886T">
<pin name="VIN-" direction="in"/>
<pin name="VIN+" direction="in"/>
<pin name="MUTE" direction="in"/>
<pin name="V+_2" direction="pwr"/>
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="NC_2" direction="pas"/>
<pin name="NC_3" direction="pas"/>
<pin name="NC" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM3886TF">
<pin name="VIN-" direction="in"/>
<pin name="VIN+" direction="in"/>
<pin name="MUTE" direction="in"/>
<pin name="V+_2" direction="pwr"/>
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="NC_2" direction="pas"/>
<pin name="NC_3" direction="pas"/>
<pin name="NC" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM392M">
<pin name="V+" direction="pwr"/>
<pin name="POS_A" direction="in"/>
<pin name="NEG_A" direction="in"/>
<pin name="NEG_B" direction="in"/>
<pin name="POS_B" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT_A" direction="out"/>
<pin name="OUT_B" direction="out"/>
</symbol>
<symbol name="LM392N">
<pin name="V+" direction="pwr"/>
<pin name="POA_A" direction="in"/>
<pin name="NEG_A" direction="in"/>
<pin name="POS_B" direction="in"/>
<pin name="NEG_B" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT_A" direction="out"/>
<pin name="OUT_B" direction="out"/>
</symbol>
<symbol name="LM393M">
<pin name="V+" direction="pwr"/>
<pin name="NEGA" direction="in"/>
<pin name="POSA" direction="in"/>
<pin name="NEGB" direction="in"/>
<pin name="POSB" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="LM393N">
<pin name="V+" direction="pwr"/>
<pin name="POA_A" direction="in"/>
<pin name="NEG_A" direction="in"/>
<pin name="POS_B" direction="in"/>
<pin name="NEG_B" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT_A" direction="out"/>
<pin name="OUT_B" direction="out"/>
</symbol>
<symbol name="LM3940IMP-3.3">
<pin name="IN" direction="pwr"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM3940IS-3.3">
<pin name="IN" direction="pwr"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM3940IT-3.3">
<pin name="IN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM397MF">
<pin name="VS" direction="pwr"/>
<pin name="VIN-" direction="in"/>
<pin name="VIN+" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM4120AIM5-1.8">
<pin name="VIN" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="REF" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LM4120AIM5-2.0">
<pin name="VIN" direction="pwr"/>
<pin name="REF" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LM4120AIM5-2.5">
<pin name="VIN" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="REF" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LM4120AIM5-3.0">
<pin name="VIN" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="REF" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LM4120AIM5-3.3">
<pin name="VIN" direction="pwr"/>
<pin name="REF" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LM4120AIM5-4.1">
<pin name="VIN" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="REF" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LM4120AIM5-5.0">
<pin name="VIN" direction="pwr"/>
<pin name="REF" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LM4120IM5-1.8">
<pin name="VIN" direction="pwr"/>
<pin name="REF" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LM4120IM5-2.0">
<pin name="VIN" direction="pwr"/>
<pin name="REF" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LM4120IM5-3.0">
<pin name="VIN" direction="pwr"/>
<pin name="REF" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LM4120IM5-3.3">
<pin name="VIN" direction="pwr"/>
<pin name="REF" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LM4120IM5-4.1">
<pin name="VIN" direction="pwr"/>
<pin name="REF" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LM4120IM5-5.0">
<pin name="VIN" direction="pwr"/>
<pin name="REF" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LM4132AMF-2.5">
<pin name="VIN" direction="pwr"/>
<pin name="EN" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="VREF" direction="out"/>
</symbol>
<symbol name="LM4132BMF-4.1">
<pin name="VIN" direction="pwr"/>
<pin name="EN" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="VREF" direction="out"/>
</symbol>
<symbol name="LM4132CMF-2.5">
<pin name="VIN" direction="pwr"/>
<pin name="EN" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="VREF" direction="out"/>
</symbol>
<symbol name="LM4132DMF-4.1">
<pin name="VIN" direction="pwr"/>
<pin name="EN" direction="in"/>
<pin name="N/C" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="VREF" direction="out"/>
</symbol>
<symbol name="LM4132EMF-2.5">
<pin name="VIN" direction="pwr"/>
<pin name="EN" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="VREF" direction="out"/>
</symbol>
<symbol name="LM4132EMF-3.0">
<pin name="VIN" direction="pwr"/>
<pin name="EN" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="VREF" direction="out"/>
</symbol>
<symbol name="LM4140ACM-1.0">
<pin name="VIN" direction="pwr"/>
<pin name="EN" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VREF" direction="out"/>
</symbol>
<symbol name="LM4140ACM-1.2">
<pin name="VIN" direction="pwr"/>
<pin name="EN" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VREF" direction="out"/>
</symbol>
<symbol name="LM4140ACM-2.0">
<pin name="VIN" direction="pwr"/>
<pin name="EN" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VREF" direction="out"/>
</symbol>
<symbol name="LM4140ACM-2.5">
<pin name="VIN" direction="pwr"/>
<pin name="EN" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VREF" direction="out"/>
</symbol>
<symbol name="LM4140ACM-4.1">
<pin name="VIN" direction="pwr"/>
<pin name="EN" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VREF" direction="out"/>
</symbol>
<symbol name="LM4140BCM-1.0">
<pin name="VIN" direction="pwr"/>
<pin name="EN" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VREF" direction="out"/>
</symbol>
<symbol name="LM4140BCM-2.5">
<pin name="VIN" direction="pwr"/>
<pin name="EN" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VREF" direction="out"/>
</symbol>
<symbol name="LM4140BCM-4.1">
<pin name="VIN" direction="pwr"/>
<pin name="EN" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VREF" direction="out"/>
</symbol>
<symbol name="LM4140CCM-1.0">
<pin name="VIN" direction="pwr"/>
<pin name="EN" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VREF" direction="out"/>
</symbol>
<symbol name="LM4140CCM-1.2">
<pin name="VIN" direction="pwr"/>
<pin name="EN" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VREF" direction="out"/>
</symbol>
<symbol name="LM4140CCM-2.0">
<pin name="VIN" direction="pwr"/>
<pin name="EN" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VREF" direction="out"/>
</symbol>
<symbol name="LM4140CCM-2.5">
<pin name="VIN" direction="pwr"/>
<pin name="EN" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VREF" direction="out"/>
</symbol>
<symbol name="LM4140CCM-4.1">
<pin name="VIN" direction="pwr"/>
<pin name="EN" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VREF" direction="out"/>
</symbol>
<symbol name="LM4250CM">
<pin name="V+" direction="pwr"/>
<pin name="QUISCENT_ISET" direction="in"/>
<pin name="OFFSETNULL_2" direction="in"/>
<pin name="OFFSETNULL" direction="in"/>
<pin name="NEG" direction="in"/>
<pin name="POS" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM4250CN">
<pin name="V+" direction="pwr"/>
<pin name="POS" direction="in"/>
<pin name="NEG" direction="in"/>
<pin name="OFFSET_NULL" direction="pas"/>
<pin name="OFFSET_NULL_2" direction="pas"/>
<pin name="QUIESCENT_CURRENT_SET" direction="pas"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM4308GR">
<pin name="VDD" direction="pwr"/>
<pin name="VDDA" direction="pwr"/>
<pin name="VDDIO_2" direction="pwr"/>
<pin name="VDDIO" direction="pwr"/>
<pin name="AD" direction="in"/>
<pin name="PD" direction="in"/>
<pin name="WR" direction="in"/>
<pin name="TM" direction="in"/>
<pin name="RD" direction="in"/>
<pin name="WO" direction="in"/>
<pin name="ERR" direction="in"/>
<pin name="M/S" direction="in"/>
<pin name="CS1" direction="in"/>
<pin name="CS2" direction="in"/>
<pin name="DDN_S/DCN_M"/>
<pin name="DCN_S/DDN_M"/>
<pin name="RDS0/PLLCON0" direction="in"/>
<pin name="RDS1/PLLCON1" direction="in"/>
<pin name="VSSA" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="VSSIO_2" direction="pwr"/>
<pin name="VSSIO_3" direction="pwr"/>
<pin name="VSSIO_4" direction="pwr"/>
<pin name="VSSIO_5" direction="pwr"/>
<pin name="VSSIO_6" direction="pwr"/>
<pin name="VSSIO_7" direction="pwr"/>
<pin name="VSSIO_8" direction="pwr"/>
<pin name="VSSIO_9" direction="pwr"/>
<pin name="VSSIO" direction="pwr"/>
<pin name="DCP_S/DDP_M"/>
<pin name="DDP_S/DCP_M"/>
<pin name="D0"/>
<pin name="D1"/>
<pin name="D2"/>
<pin name="D3"/>
<pin name="D4"/>
<pin name="D5"/>
<pin name="D6"/>
<pin name="D7"/>
<pin name="D8"/>
<pin name="D9"/>
<pin name="D10"/>
<pin name="D11"/>
<pin name="D12"/>
<pin name="D13"/>
<pin name="D14"/>
<pin name="D15"/>
<pin name="D16"/>
<pin name="D17"/>
</symbol>
<symbol name="LM4308SQ">
<pin name="VDD" direction="pwr"/>
<pin name="VDDA" direction="pwr"/>
<pin name="VDDIO_2" direction="pwr"/>
<pin name="VDDIO" direction="pwr"/>
<pin name="~CS~1" direction="in"/>
<pin name="~CS~2" direction="in"/>
<pin name="~WR" direction="in"/>
<pin name="~PD" direction="in"/>
<pin name="TM" direction="in"/>
<pin name="~RD" direction="in"/>
<pin name="M/~S" direction="in"/>
<pin name="ERR" direction="in"/>
<pin name="CLK/WO" direction="in"/>
<pin name="PLLCON0/RDS0" direction="in"/>
<pin name="PLLCON1/RDS1" direction="in"/>
<pin name="DDP/DCP"/>
<pin name="DDN/DCN"/>
<pin name="DCP/DDP" direction="in"/>
<pin name="DCN/DDN" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="VSSA" direction="pwr"/>
<pin name="EPAD" direction="pas"/>
<pin name="D0"/>
<pin name="AD"/>
<pin name="D1"/>
<pin name="D2"/>
<pin name="D3"/>
<pin name="D6"/>
<pin name="D4"/>
<pin name="D5"/>
<pin name="D7"/>
<pin name="D8"/>
<pin name="D9"/>
<pin name="D10"/>
<pin name="D11"/>
<pin name="D12"/>
<pin name="D13"/>
<pin name="D14"/>
<pin name="D15"/>
<pin name="D16"/>
<pin name="D17"/>
</symbol>
<symbol name="LM432MA">
<pin name="VS" direction="pwr"/>
<pin name="AIN-" direction="in"/>
<pin name="AIN+" direction="in"/>
<pin name="BIN+" direction="in"/>
<pin name="BIN-" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="AOUT" direction="out"/>
<pin name="BOUT" direction="out"/>
</symbol>
<symbol name="LM4510SD">
<pin name="VIN" direction="pwr"/>
<pin name="EN" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="SS" direction="in"/>
<pin name="COMP" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="PGND" direction="pas"/>
<pin name="AGND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="SW" direction="out"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LM4562HA">
<pin name="-INA" direction="in"/>
<pin name="+INA" direction="in"/>
<pin name="-INB" direction="in"/>
<pin name="+INB" direction="in"/>
<pin name="V+" direction="pas"/>
<pin name="V-" direction="pas"/>
<pin name="OUTB" direction="out"/>
<pin name="OUTA" direction="out"/>
</symbol>
<symbol name="LM4562MA">
<pin name="V+" direction="pwr"/>
<pin name="POS_A" direction="in"/>
<pin name="POS_B" direction="in"/>
<pin name="NEG_A" direction="in"/>
<pin name="NEG_B" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT_A" direction="out"/>
<pin name="OUT_B" direction="out"/>
</symbol>
<symbol name="LM4562NA">
<pin name="V+" direction="pwr"/>
<pin name="POS_A" direction="in"/>
<pin name="NEG_A" direction="in"/>
<pin name="POS_B" direction="in"/>
<pin name="NEG_B" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT_A" direction="out"/>
<pin name="OUT_B" direction="out"/>
</symbol>
<symbol name="LM4570LQ">
<pin name="VDD" direction="pwr"/>
<pin name="IN" direction="in"/>
<pin name="REF1" direction="in"/>
<pin name="REF2" direction="in"/>
<pin name="SHDN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="HEAT_PAD" direction="pas"/>
<pin name="VO1" direction="out"/>
<pin name="VO2" direction="out"/>
</symbol>
<symbol name="LM45BIM3">
<pin name="+VS" direction="pwr"/>
<pin name="GND" direction="pas"/>
<pin name="VO" direction="out"/>
</symbol>
<symbol name="LM45CIM3">
<pin name="+VS" direction="pwr"/>
<pin name="GND" direction="pas"/>
<pin name="VO" direction="out"/>
</symbol>
<symbol name="LM4667MM">
<pin name="VDD" direction="pwr"/>
<pin name="~SD" direction="pas"/>
<pin name="GAINSELECT" direction="pas"/>
<pin name="IN-" direction="in"/>
<pin name="IN+" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VO1" direction="out"/>
<pin name="VO2" direction="out"/>
</symbol>
<symbol name="LM4670ITL">
<pin name="VDD" direction="pwr"/>
<pin name="PVDD" direction="pwr"/>
<pin name="IN+" direction="pwr"/>
<pin name="IN-" direction="in"/>
<pin name="~SHDN" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VO1" direction="out"/>
<pin name="VO2" direction="out"/>
</symbol>
<symbol name="LM4670SD">
<pin name="VDD" direction="pwr"/>
<pin name="~SHDN" direction="pas"/>
<pin name="IN-" direction="in"/>
<pin name="IN+" direction="in"/>
<pin name="EP" direction="pas"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VO1" direction="out"/>
<pin name="VO2" direction="out"/>
</symbol>
<symbol name="LM4673SD">
<pin name="VDD" direction="pwr"/>
<pin name="PVDD" direction="pwr"/>
<pin name="IN-" direction="in"/>
<pin name="IN+" direction="in"/>
<pin name="~SD" direction="pas"/>
<pin name="EP" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VO1" direction="out"/>
<pin name="VO2" direction="out"/>
</symbol>
<symbol name="LM4673TM">
<pin name="VDD" direction="pwr"/>
<pin name="PVDD_2" direction="pwr"/>
<pin name="PVDD" direction="pwr"/>
<pin name="IN+" direction="in"/>
<pin name="IN-" direction="in"/>
<pin name="~SD" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="VO1" direction="out"/>
</symbol>
<symbol name="LM4675SD">
<pin name="VDD" direction="pwr"/>
<pin name="PVDD" direction="pwr"/>
<pin name="IN+" direction="in"/>
<pin name="IN-" direction="in"/>
<pin name="~SHDN" direction="in"/>
<pin name="HEAT_PAD" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VO1" direction="out"/>
<pin name="VO2" direction="out"/>
</symbol>
<symbol name="LM4702BTA">
<pin name="IN2+" direction="pas"/>
<pin name="IN2-" direction="in"/>
<pin name="IN1+" direction="in"/>
<pin name="IN1-" direction="in"/>
<pin name="COMP1" direction="pas"/>
<pin name="COMP2" direction="pas"/>
<pin name="VCC+_2" direction="pas"/>
<pin name="VCC+" direction="pas"/>
<pin name="VEE-" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="SINK2" direction="pas"/>
<pin name="SOURCE2" direction="pas"/>
<pin name="MUTE" direction="pas"/>
<pin name="SOURCE1" direction="pas"/>
<pin name="SINK1" direction="pas"/>
</symbol>
<symbol name="LM4702CTA">
<pin name="IN2+" direction="pas"/>
<pin name="IN2-" direction="in"/>
<pin name="IN1+" direction="in"/>
<pin name="IN1-" direction="in"/>
<pin name="COMP1" direction="pas"/>
<pin name="COMP2" direction="pas"/>
<pin name="VCC+_2" direction="pas"/>
<pin name="VCC+" direction="pas"/>
<pin name="VEE-" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="SINK2" direction="pas"/>
<pin name="SOURCE2" direction="pas"/>
<pin name="MUTE" direction="pas"/>
<pin name="SOURCE1" direction="pas"/>
<pin name="SINK1" direction="pas"/>
</symbol>
<symbol name="LM4752TS">
<pin name="VCC" direction="pwr"/>
<pin name="BIAS" direction="pas"/>
<pin name="INA" direction="in"/>
<pin name="INB" direction="in"/>
<pin name="TAB" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="LM4755TS">
<pin name="MUTE" direction="pas"/>
<pin name="BIAS" direction="pas"/>
<pin name="INA" direction="in"/>
<pin name="INB" direction="in"/>
<pin name="VCC" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="TAB" direction="pas"/>
<pin name="NC" direction="pas"/>
<pin name="OUTB" direction="out"/>
<pin name="OUTA" direction="out"/>
</symbol>
<symbol name="LM4765T">
<pin name="+IN_A" direction="in"/>
<pin name="-IN_A" direction="in"/>
<pin name="-IN_B" direction="in"/>
<pin name="+IN_B" direction="in"/>
<pin name="MUTE_A" direction="pas"/>
<pin name="MUTE_B" direction="pas"/>
<pin name="VCCA" direction="pas"/>
<pin name="VCC_B" direction="pas"/>
<pin name="VEE" direction="pas"/>
<pin name="GND_B" direction="pas"/>
<pin name="GND_A" direction="pas"/>
<pin name="STANDBY_B" direction="pas"/>
<pin name="STANDBY_A" direction="pas"/>
<pin name="OUTB" direction="out"/>
<pin name="OUTA" direction="out"/>
</symbol>
<symbol name="LM4766T">
<pin name="-IN_A" direction="in"/>
<pin name="+IN_A" direction="in"/>
<pin name="-IN_B" direction="in"/>
<pin name="+IN_B" direction="in"/>
<pin name="MUTE_A" direction="pas"/>
<pin name="MUTE_B" direction="pas"/>
<pin name="VCC_A" direction="pas"/>
<pin name="VCC_B" direction="pas"/>
<pin name="VEE" direction="pas"/>
<pin name="GND_A" direction="pas"/>
<pin name="GND_B" direction="pas"/>
<pin name="NC_2" direction="pas"/>
<pin name="NC" direction="pas"/>
<pin name="OUTB" direction="out"/>
<pin name="OUTA" direction="out"/>
</symbol>
<symbol name="LM4766TF">
<pin name="+IN_A" direction="in"/>
<pin name="-IN_A" direction="in"/>
<pin name="+IN_B" direction="in"/>
<pin name="-IN_B" direction="in"/>
<pin name="MUTE_A" direction="pas"/>
<pin name="MUTE_B" direction="pas"/>
<pin name="VCC_A" direction="pas"/>
<pin name="VCC_B" direction="pas"/>
<pin name="VEE" direction="pas"/>
<pin name="GND_A" direction="pas"/>
<pin name="GND_B" direction="pas"/>
<pin name="NC_2" direction="pas"/>
<pin name="NC" direction="pas"/>
<pin name="OUTB" direction="out"/>
<pin name="OUTA" direction="out"/>
</symbol>
<symbol name="LM4780TA">
<pin name="-IN_A" direction="in"/>
<pin name="+IN_A" direction="in"/>
<pin name="-IN_B" direction="in"/>
<pin name="+IN_B" direction="in"/>
<pin name="MUTE_A" direction="pas"/>
<pin name="MUTE_B" direction="pas"/>
<pin name="V+_2" direction="pas"/>
<pin name="V+_3" direction="pas"/>
<pin name="V+_4" direction="pas"/>
<pin name="V+_5" direction="pas"/>
<pin name="V+" direction="pas"/>
<pin name="V-_2" direction="pas"/>
<pin name="V-_3" direction="pas"/>
<pin name="V-_4" direction="pas"/>
<pin name="V-_5" direction="pas"/>
<pin name="V-" direction="pas"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="NC_2" direction="pas"/>
<pin name="NC_3" direction="pas"/>
<pin name="NC_4" direction="pas"/>
<pin name="NC_5" direction="pas"/>
<pin name="NC_6" direction="pas"/>
<pin name="NC_7" direction="pas"/>
<pin name="NC" direction="pas"/>
<pin name="OUT_B" direction="out"/>
<pin name="OUT_A" direction="out"/>
</symbol>
<symbol name="LM4781TA">
<pin name="V+_2" direction="pas"/>
<pin name="V+_3" direction="pas"/>
<pin name="V+" direction="pas"/>
<pin name="MUTE1" direction="pas"/>
<pin name="MUTE2" direction="pas"/>
<pin name="MUTE3" direction="pas"/>
<pin name="IN1-" direction="in"/>
<pin name="IN1+" direction="in"/>
<pin name="IN2-" direction="in"/>
<pin name="IN2+" direction="in"/>
<pin name="IN3-" direction="in"/>
<pin name="IN3+" direction="in"/>
<pin name="V-_2" direction="pas"/>
<pin name="V-_3" direction="pas"/>
<pin name="V-" direction="pas"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="NC_2" direction="pas"/>
<pin name="NC_3" direction="pas"/>
<pin name="NC_4" direction="pas"/>
<pin name="NC_5" direction="pas"/>
<pin name="NC_6" direction="pas"/>
<pin name="NC" direction="pas"/>
<pin name="OUT3" direction="out"/>
<pin name="OUT2" direction="out"/>
<pin name="OUT1" direction="out"/>
</symbol>
<symbol name="LM4808M">
<pin name="VDD" direction="pwr"/>
<pin name="IN_A-" direction="in"/>
<pin name="IN_A+" direction="in"/>
<pin name="IN_B+" direction="in"/>
<pin name="IN_B-" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT_A" direction="out"/>
<pin name="OUT_B" direction="out"/>
</symbol>
<symbol name="LM4808MM">
<pin name="VDD" direction="pwr"/>
<pin name="IN_A_+" direction="in"/>
<pin name="IN_A_-" direction="in"/>
<pin name="IN_B+" direction="in"/>
<pin name="IN_B-" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT_A" direction="out"/>
<pin name="OUT_B" direction="out"/>
</symbol>
<symbol name="LM4809MM">
<pin name="VDD" direction="pwr"/>
<pin name="BYPASS" direction="in"/>
<pin name="~SHDN" direction="in"/>
<pin name="VIN_1" direction="in"/>
<pin name="VIN2" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT1" direction="out"/>
<pin name="VOUT2" direction="out"/>
</symbol>
<symbol name="LM48100QMH">
<pin name="VDD" direction="pwr"/>
<pin name="I2CVDD" direction="pwr"/>
<pin name="IN1" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="SCL" direction="in"/>
<pin name="ADR" direction="in"/>
<pin name="BIAS" direction="in"/>
<pin name="~FAULT" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="PVDD" direction="pwr"/>
<pin name="EPAD" direction="pas"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
<pin name="SDA"/>
</symbol>
<symbol name="LM4811LD">
<pin name="VDD" direction="pwr"/>
<pin name="BYPASS" direction="in"/>
<pin name="SHDN" direction="in"/>
<pin name="CLK" direction="in"/>
<pin name="UP/DN" direction="in"/>
<pin name="VIN1" direction="in"/>
<pin name="VIN2" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT1" direction="out"/>
<pin name="VOUT2" direction="out"/>
</symbol>
<symbol name="LM4811MM">
<pin name="VDD" direction="pwr"/>
<pin name="CLK" direction="in"/>
<pin name="BYPASS" direction="in"/>
<pin name="UP/DN" direction="in"/>
<pin name="SHDN" direction="in"/>
<pin name="VIN1" direction="in"/>
<pin name="VIN2" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT1" direction="out"/>
<pin name="VOUT2" direction="out"/>
</symbol>
<symbol name="LM4838MT">
<pin name="VDD_2" direction="pwr"/>
<pin name="VDD_3" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="SHDN" direction="in"/>
<pin name="MODE" direction="in"/>
<pin name="MUTE" direction="in"/>
<pin name="DC_VOL" direction="in"/>
<pin name="GAIN_SELECT" direction="in"/>
<pin name="LEFT_IN" direction="in"/>
<pin name="RIGHT_IN" direction="in"/>
<pin name="BEEP_IN" direction="in"/>
<pin name="RIGHT_DOCK" direction="in"/>
<pin name="LEFT_DOCK_" direction="in"/>
<pin name="RIGHT_GAIN_1" direction="in"/>
<pin name="RIGHT_GAIN_2" direction="in"/>
<pin name="LEFT_GAIN_2" direction="in"/>
<pin name="LEFT_GAIN_1" direction="in"/>
<pin name="HP_SENSE" direction="in"/>
<pin name="BYPASS" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="LEFT_OUT_+" direction="out"/>
<pin name="LEFT_OUT_-" direction="out"/>
<pin name="RIGHT_OUT_-" direction="out"/>
<pin name="RIGHT_OUT_+" direction="out"/>
</symbol>
<symbol name="LM48413TL">
<pin name="VDD" direction="pwr"/>
<pin name="PVDD" direction="pwr"/>
<pin name="~SD" direction="in"/>
<pin name="3DEN" direction="in"/>
<pin name="3DR+" direction="in"/>
<pin name="3DR-" direction="in"/>
<pin name="3DL-" direction="in"/>
<pin name="3DL+" direction="in"/>
<pin name="INL-" direction="in"/>
<pin name="INL+" direction="in"/>
<pin name="INR-" direction="in"/>
<pin name="INR+" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="OUTLA" direction="out"/>
<pin name="OUTLB" direction="out"/>
<pin name="OUTRA" direction="out"/>
<pin name="OUTRB" direction="out"/>
</symbol>
<symbol name="LM4846TL">
<pin name="VDD_2" direction="pwr"/>
<pin name="VDD_3" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="I2CSPI_VDD" direction="pwr"/>
<pin name="I2CSPI_SEL" direction="in"/>
<pin name="RHP3D1" direction="in"/>
<pin name="RHP3D2" direction="in"/>
<pin name="LHP3D1" direction="in"/>
<pin name="LHP3D2" direction="in"/>
<pin name="SCL" direction="in"/>
<pin name="ID_ENB" direction="in"/>
<pin name="PHONE_IN" direction="in"/>
<pin name="CBYPASS" direction="pwr"/>
<pin name="RIN" direction="in"/>
<pin name="LIN" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="SDA"/>
<pin name="VOC" direction="out"/>
<pin name="MONO-" direction="out"/>
<pin name="MONO+" direction="out"/>
<pin name="ROUT" direction="out"/>
<pin name="LOUT" direction="out"/>
</symbol>
<symbol name="LM48556TL">
<pin name="PVDD" direction="pwr"/>
<pin name="SVDD" direction="pwr"/>
<pin name="~SD" direction="in"/>
<pin name="C1N" direction="pas"/>
<pin name="C1P" direction="pas"/>
<pin name="IN-" direction="in"/>
<pin name="IN+" direction="in"/>
<pin name="CPVSS" direction="pas"/>
<pin name="SVSS" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="OUT-" direction="out"/>
<pin name="OUT+" direction="out"/>
</symbol>
<symbol name="LM48557TL">
<pin name="PVDD" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="I2CVDD" direction="pwr"/>
<pin name="SCL" direction="in"/>
<pin name="SDA" direction="in"/>
<pin name="VCM" direction="in"/>
<pin name="C1N" direction="in"/>
<pin name="C1P" direction="pas"/>
<pin name="~RESET" direction="in"/>
<pin name="IN+" direction="in"/>
<pin name="IN-" direction="in"/>
<pin name="SGND" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="CPVSS" direction="out"/>
<pin name="OUT-" direction="out"/>
<pin name="OUT+" direction="out"/>
</symbol>
<symbol name="LM4855ITL">
<pin name="LIN" direction="in"/>
<pin name="RIN" direction="in"/>
<pin name="DATA" direction="pas"/>
<pin name="PHONE_IN_IHS" direction="in"/>
<pin name="PHONE_IN_IHF" direction="in"/>
<pin name="ENB" direction="pas"/>
<pin name="BYPASS" direction="pas"/>
<pin name="CLOCK" direction="pas"/>
<pin name="VDD_2" direction="pas"/>
<pin name="VDD" direction="pas"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="SPKR_OUT+" direction="out"/>
<pin name="SPKR_OUT-" direction="out"/>
<pin name="LOUT+" direction="out"/>
<pin name="LOUT-" direction="out"/>
<pin name="ROUT-" direction="out"/>
<pin name="ROUT+" direction="out"/>
</symbol>
<symbol name="LM4865M">
<pin name="VDD" direction="pwr"/>
<pin name="-VIN" direction="in"/>
<pin name="BYPASS" direction="pas"/>
<pin name="HPSENSE" direction="pas"/>
<pin name="DC_VOL/~SD" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VO1" direction="out"/>
<pin name="VO2" direction="out"/>
</symbol>
<symbol name="LM4871M">
<pin name="VDD" direction="pwr"/>
<pin name="SHUTDOWN" direction="in"/>
<pin name="BYPASS" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="V01" direction="out"/>
<pin name="V02" direction="out"/>
</symbol>
<symbol name="LM4875M">
<pin name="VDD" direction="pwr"/>
<pin name="-VIN" direction="in"/>
<pin name="BYPASS" direction="pas"/>
<pin name="HPSENSE" direction="pas"/>
<pin name="DC_VOL/~SD" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VO1" direction="out"/>
<pin name="VO2" direction="out"/>
</symbol>
<symbol name="LM4875MM">
<pin name="VDD" direction="pwr"/>
<pin name="-VIN" direction="in"/>
<pin name="BYPASS" direction="in"/>
<pin name="HPSENSE" direction="in"/>
<pin name="DC_VOL/~SD" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VO1" direction="out"/>
<pin name="VO2" direction="out"/>
</symbol>
<symbol name="LM4876M">
<pin name="VDD" direction="pwr"/>
<pin name="~SHUTDOWN" direction="in"/>
<pin name="BYPASS" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="V01" direction="out"/>
<pin name="V02" direction="out"/>
</symbol>
<symbol name="LM4881MM">
<pin name="VDD" direction="pwr"/>
<pin name="VIN_A" direction="in"/>
<pin name="VIN_B" direction="in"/>
<pin name="BYPASS" direction="in"/>
<pin name="SHUTDOWN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT_A_2" direction="out"/>
<pin name="OUT_A" direction="out"/>
</symbol>
<symbol name="LM48821TL">
<pin name="IN_A+" direction="in"/>
<pin name="IN_A-" direction="in"/>
<pin name="IN_B+" direction="in"/>
<pin name="IN_B-" direction="in"/>
<pin name="CCP-" direction="in"/>
<pin name="CCP+" direction="in"/>
<pin name="SDA" direction="in"/>
<pin name="SCL" direction="in"/>
<pin name="I2CVDD" direction="pwr"/>
<pin name="PGND" direction="pas"/>
<pin name="SGND" direction="pas"/>
<pin name="PVDD" direction="pwr"/>
<pin name="SVDD" direction="pwr"/>
<pin name="VOA" direction="out"/>
<pin name="VOB" direction="out"/>
<pin name="VSS" direction="pwr"/>
</symbol>
<symbol name="LM48823TL">
<pin name="I2CVDD" direction="pwr"/>
<pin name="PVDD" direction="pwr"/>
<pin name="SVDD" direction="pwr"/>
<pin name="INA" direction="in"/>
<pin name="INB" direction="in"/>
<pin name="BYPASS" direction="pas"/>
<pin name="C1P" direction="in"/>
<pin name="C1N" direction="in"/>
<pin name="SDA" direction="in"/>
<pin name="SCL" direction="in"/>
<pin name="~RESET" direction="in"/>
<pin name="SGND" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
<pin name="VSS" direction="pwr"/>
</symbol>
<symbol name="LM48824TM">
<pin name="HPVDD" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="SDA" direction="in"/>
<pin name="SCL" direction="in"/>
<pin name="INL-" direction="in"/>
<pin name="INL+" direction="in"/>
<pin name="INR-" direction="in"/>
<pin name="INR+" direction="in"/>
<pin name="C1P" direction="pas"/>
<pin name="C1N" direction="pas"/>
<pin name="SW" direction="pas"/>
<pin name="COM" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUTL" direction="out"/>
<pin name="OUTR" direction="out"/>
<pin name="HPVSS" direction="out"/>
</symbol>
<symbol name="LM48860TL">
<pin name="VDD" direction="pwr"/>
<pin name="~SD_LC" direction="in"/>
<pin name="~SD_RC" direction="in"/>
<pin name="CCP+" direction="in"/>
<pin name="CCP-" direction="in"/>
<pin name="RIN" direction="in"/>
<pin name="LIN" direction="in"/>
<pin name="PGND" direction="pas"/>
<pin name="SGND" direction="pas"/>
<pin name="VSS(CP)" direction="pwr"/>
<pin name="LOUT" direction="out"/>
<pin name="ROUT" direction="out"/>
</symbol>
<symbol name="LM4889MA">
<pin name="VDD" direction="pwr"/>
<pin name="~SHDN" direction="in"/>
<pin name="BYPASS" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VO1" direction="out"/>
<pin name="VO2" direction="out"/>
</symbol>
<symbol name="LM4889MM">
<pin name="VDD" direction="pwr"/>
<pin name="~SHDN" direction="in"/>
<pin name="BYPASS" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VO1" direction="out"/>
<pin name="VO2" direction="out"/>
</symbol>
<symbol name="LM49100GR">
<pin name="VDDCP" direction="pwr"/>
<pin name="VDDLS_2" direction="pwr"/>
<pin name="VDDHP" direction="pwr"/>
<pin name="VDDLS" direction="pwr"/>
<pin name="VDD12C" direction="pwr"/>
<pin name="RIN" direction="in"/>
<pin name="LIN" direction="in"/>
<pin name="MIN+" direction="in"/>
<pin name="MIN-" direction="in"/>
<pin name="BYPASS" direction="pas"/>
<pin name="SDA" direction="in"/>
<pin name="C1P" direction="pas"/>
<pin name="SCL" direction="in"/>
<pin name="C1N" direction="pas"/>
<pin name="ADDR" direction="in"/>
<pin name="VSSCP" direction="pwr"/>
<pin name="VSSHP" direction="pwr"/>
<pin name="AGND" direction="pas"/>
<pin name="GNDCP" direction="pas"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="LS+" direction="out"/>
<pin name="LS-" direction="out"/>
<pin name="HPR" direction="out"/>
<pin name="HPL" direction="out"/>
</symbol>
<symbol name="LM49101TM">
<pin name="VDDHP" direction="pwr"/>
<pin name="I2CVDD" direction="pwr"/>
<pin name="VDDCP" direction="pwr"/>
<pin name="VDDLS" direction="pwr"/>
<pin name="SCL" direction="in"/>
<pin name="SDA" direction="in"/>
<pin name="BYPASS_IN-" direction="in"/>
<pin name="BIAS" direction="pwr"/>
<pin name="C1N" direction="pas"/>
<pin name="BYPASS_IN+" direction="in"/>
<pin name="C1P" direction="pas"/>
<pin name="HW_RESET" direction="in"/>
<pin name="LIN" direction="in"/>
<pin name="MIN-" direction="in"/>
<pin name="MIN+" direction="in"/>
<pin name="RIN" direction="in"/>
<pin name="VSSCP" direction="pwr"/>
<pin name="GND_2" direction="pas"/>
<pin name="CPGND" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="HPGND" direction="pas"/>
<pin name="HPL" direction="out"/>
<pin name="HPR" direction="out"/>
<pin name="MONO-" direction="out"/>
<pin name="MONO+" direction="out"/>
</symbol>
<symbol name="LM4910MM">
<pin name="VDD" direction="pwr"/>
<pin name="IN_1" direction="in"/>
<pin name="IN_2" direction="in"/>
<pin name="~SD" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VO1" direction="out"/>
<pin name="VO2" direction="out"/>
<pin name="VO3" direction="out"/>
</symbol>
<symbol name="LM49120TL">
<pin name="VDD_2" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="I2CVDD" direction="pwr"/>
<pin name="SCL" direction="in"/>
<pin name="SDA" direction="in"/>
<pin name="MONO_IN+" direction="in"/>
<pin name="MONO_IN-" direction="in"/>
<pin name="RIN" direction="in"/>
<pin name="LIN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="MONO+" direction="out"/>
<pin name="MONO-" direction="out"/>
<pin name="ROUT" direction="out"/>
<pin name="LOUT" direction="out"/>
<pin name="BYPASS" direction="pas"/>
<pin name="VOC" direction="out"/>
</symbol>
<symbol name="LM49151TL">
<pin name="I2CVDD" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="LSVDD" direction="pwr"/>
<pin name="BYPASS" direction="pwr"/>
<pin name="SDA" direction="in"/>
<pin name="SCL" direction="in"/>
<pin name="SET" direction="pas"/>
<pin name="INL" direction="in"/>
<pin name="INR" direction="in"/>
<pin name="INM-" direction="in"/>
<pin name="INM+" direction="in"/>
<pin name="CPN" direction="pas"/>
<pin name="CPP" direction="pas"/>
<pin name="HPR" direction="out"/>
<pin name="HPL" direction="out"/>
<pin name="CPVSS" direction="out"/>
<pin name="GND" direction="pas"/>
<pin name="CPGND" direction="pas"/>
<pin name="LSOUT-" direction="out"/>
<pin name="LSOUT+" direction="out"/>
</symbol>
<symbol name="LM4916MM">
<pin name="VDD" direction="pwr"/>
<pin name="IN_A" direction="in"/>
<pin name="IN_B" direction="in"/>
<pin name="SD" direction="in"/>
<pin name="MUTE" direction="in"/>
<pin name="BYPASS" direction="in"/>
<pin name="~SE/BTL" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOA" direction="out"/>
<pin name="VOB" direction="out"/>
</symbol>
<symbol name="LM49200TL">
<pin name="VDD" direction="pwr"/>
<pin name="I2CVDD" direction="pwr"/>
<pin name="SCL" direction="in"/>
<pin name="SDA" direction="in"/>
<pin name="LIN" direction="in"/>
<pin name="MIN-" direction="in"/>
<pin name="MIN+" direction="in"/>
<pin name="RIN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="CPGND" direction="pas"/>
<pin name="BIAS" direction="out"/>
<pin name="VSSCP" direction="pwr"/>
<pin name="HPL" direction="out"/>
<pin name="HPR" direction="out"/>
<pin name="C1N" direction="out"/>
<pin name="C1P" direction="out"/>
<pin name="LOUT-" direction="out"/>
<pin name="LOUT+" direction="out"/>
<pin name="ROUT-" direction="out"/>
<pin name="ROUT+" direction="out"/>
</symbol>
<symbol name="LM4920TL">
<pin name="+AVDD" direction="pwr"/>
<pin name="-AVDD" direction="pwr"/>
<pin name="CPVDD" direction="pwr"/>
<pin name="L_IN" direction="in"/>
<pin name="R_IN" direction="in"/>
<pin name="CCP+" direction="in"/>
<pin name="CCP-" direction="in"/>
<pin name="SD_RC" direction="in"/>
<pin name="SD_LC" direction="in"/>
<pin name="SGND" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="R_OUT" direction="out"/>
<pin name="L_OUT" direction="out"/>
<pin name="VCP_OUT" direction="out"/>
</symbol>
<symbol name="LM4921ITL">
<pin name="AVDD" direction="pwr"/>
<pin name="DVDD" direction="pwr"/>
<pin name="VDDX" direction="pwr"/>
<pin name="I2S-CLK"/>
<pin name="SPI_CLK" direction="in"/>
<pin name="I2S-LRCLK"/>
<pin name="MCLK/XTAL_IN" direction="in"/>
<pin name="SPI_EN" direction="in"/>
<pin name="I2S_DATA" direction="in"/>
<pin name="SPI_DATA" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GNDD" direction="pas"/>
<pin name="AGND" direction="pas"/>
<pin name="GNDX" direction="pas"/>
<pin name="BYPASS"/>
<pin name="XTAL_OUT" direction="out"/>
<pin name="NC_OPEN" direction="out"/>
<pin name="HP_R" direction="out"/>
<pin name="HP-L" direction="out"/>
</symbol>
<symbol name="LM4923LQ">
<pin name="VDD" direction="pwr"/>
<pin name="IN-" direction="in"/>
<pin name="IN+" direction="in"/>
<pin name="SD" direction="in"/>
<pin name="BYPASS" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="VO+" direction="out"/>
<pin name="VO-" direction="out"/>
</symbol>
<symbol name="LM49250RL">
<pin name="VDD" direction="pwr"/>
<pin name="VDD(CP)" direction="pwr"/>
<pin name="VDD(LS)" direction="pwr"/>
<pin name="I2CVDD" direction="pwr"/>
<pin name="~RESET" direction="in"/>
<pin name="SCL" direction="in"/>
<pin name="SDA" direction="in"/>
<pin name="RIN+" direction="in"/>
<pin name="RIN-" direction="in"/>
<pin name="LIN+" direction="in"/>
<pin name="LIN-" direction="in"/>
<pin name="MIN+" direction="in"/>
<pin name="MIN-" direction="in"/>
<pin name="BYPASS" direction="pas"/>
<pin name="ADR" direction="in"/>
<pin name="L3D2" direction="pas"/>
<pin name="L3D1" direction="pas"/>
<pin name="R3D2" direction="in"/>
<pin name="CCP-" direction="pas"/>
<pin name="VSS(CP)" direction="pwr"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pwr"/>
<pin name="GND(CP)" direction="pas"/>
<pin name="GND(LS)" direction="pas"/>
<pin name="GND(HP)" direction="pas"/>
<pin name="RLS+" direction="out"/>
<pin name="RLS-" direction="out"/>
<pin name="LLS+" direction="out"/>
<pin name="LLS-" direction="out"/>
<pin name="EP+" direction="out"/>
<pin name="EP-" direction="out"/>
<pin name="HPR" direction="out"/>
<pin name="HPL" direction="out"/>
<pin name="CCP+" direction="pas"/>
<pin name="R3D1" direction="out"/>
<pin name="VO(LDO)" direction="out"/>
</symbol>
<symbol name="LM49321RL">
<pin name="AVDD_2" direction="pwr"/>
<pin name="DVDD" direction="pwr"/>
<pin name="AVDD" direction="pwr"/>
<pin name="I/O_VDD" direction="pwr"/>
<pin name="PLL_VDD" direction="pwr"/>
<pin name="I2C_VDD" direction="pwr"/>
<pin name="MCLK" direction="in"/>
<pin name="I2S_CLK"/>
<pin name="SCL/SCK" direction="in"/>
<pin name="I2S_WS"/>
<pin name="ADDR/ENB" direction="in"/>
<pin name="MODE" direction="in"/>
<pin name="SDA/SDI"/>
<pin name="I2S_SDATA" direction="in"/>
<pin name="LIN" direction="in"/>
<pin name="RIN" direction="in"/>
<pin name="PLL_IN" direction="in"/>
<pin name="DIFF-" direction="in"/>
<pin name="DIFF+" direction="in"/>
<pin name="BYPASS" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="AGND_2" direction="pas"/>
<pin name="AGND_3" direction="pas"/>
<pin name="DGND" direction="pwr"/>
<pin name="AGND" direction="pas"/>
<pin name="PLL_GND" direction="pas"/>
<pin name="LS+" direction="out"/>
<pin name="LS-" direction="out"/>
<pin name="EP+" direction="out"/>
<pin name="EP-" direction="out"/>
<pin name="CHP" direction="out"/>
<pin name="LHP" direction="out"/>
<pin name="RHP" direction="out"/>
<pin name="PLL_OUT" direction="out"/>
<pin name="GPIO" direction="out"/>
</symbol>
<symbol name="LM49350RL">
<pin name="LS_VDD" direction="pwr"/>
<pin name="D_VDD" direction="pwr"/>
<pin name="A_VDD" direction="in"/>
<pin name="I/O_VDD" direction="pwr"/>
<pin name="PORT1_CLK"/>
<pin name="PORT2_SDI" direction="in"/>
<pin name="PORT1_SDI" direction="in"/>
<pin name="LEFT_MIC+" direction="in"/>
<pin name="LEFT_MIC-" direction="in"/>
<pin name="RIGHT_MIC+" direction="in"/>
<pin name="RIGHT_MIC-" direction="in"/>
<pin name="AUX_L" direction="in"/>
<pin name="AUX_R" direction="in"/>
<pin name="MCLK" direction="in"/>
<pin name="SCL" direction="in"/>
<pin name="CP+" direction="in"/>
<pin name="CP-" direction="in"/>
<pin name="DGND" direction="pas"/>
<pin name="AGND" direction="pas"/>
<pin name="LSGND" direction="pas"/>
<pin name="HP_VSS" direction="pwr"/>
<pin name="LS+" direction="out"/>
<pin name="LS-" direction="out"/>
<pin name="HPR" direction="out"/>
<pin name="HPL" direction="out"/>
<pin name="GPIO"/>
<pin name="SDA"/>
<pin name="AUX_OUT+" direction="out"/>
<pin name="AUX_OUT-" direction="out"/>
<pin name="VREF_FLT"/>
<pin name="MIC_BIAS" direction="out"/>
<pin name="PORT1_SDO" direction="out"/>
<pin name="PORT1_SYNC"/>
<pin name="PORT2_CLK"/>
<pin name="PORT2_SYNC"/>
<pin name="PORT2_SDO" direction="out"/>
</symbol>
<symbol name="LM49352RL">
<pin name="DVDD" direction="pwr"/>
<pin name="IOVDD" direction="pwr"/>
<pin name="AVDD" direction="pwr"/>
<pin name="HPVDD" direction="pwr"/>
<pin name="LSVDD" direction="pwr"/>
<pin name="SCL" direction="in"/>
<pin name="MCLK" direction="in"/>
<pin name="SDA"/>
<pin name="MONO+" direction="in"/>
<pin name="MIC+" direction="in"/>
<pin name="DAC/REF"/>
<pin name="ADC/REF" direction="in"/>
<pin name="AUXR" direction="in"/>
<pin name="AUXL" direction="in"/>
<pin name="PORT2/SYNC"/>
<pin name="PORT2/SDI" direction="in"/>
<pin name="PORT2/SDO"/>
<pin name="PORT2/CLK"/>
<pin name="LSGND" direction="pas"/>
<pin name="AGND" direction="pas"/>
<pin name="DGND" direction="pas"/>
<pin name="PORT1/CLK"/>
<pin name="PORT1/SDI"/>
<pin name="LS-" direction="out"/>
<pin name="LS+" direction="out"/>
<pin name="HPL" direction="out"/>
<pin name="HPR" direction="out"/>
<pin name="MIC-" direction="in"/>
<pin name="MONO-" direction="in"/>
<pin name="PORT1/SYNC"/>
<pin name="PORT1/SDO"/>
<pin name="EP-" direction="out"/>
<pin name="EP+" direction="out"/>
<pin name="CP+"/>
<pin name="CP-"/>
<pin name="HPVSS" direction="pwr"/>
</symbol>
<symbol name="LM4935RL">
<pin name="A_VDD" direction="pwr"/>
<pin name="LS_VDD_2" direction="pwr"/>
<pin name="BB_VDD" direction="pwr"/>
<pin name="LS_VDD" direction="pwr"/>
<pin name="PLL_VDD" direction="pwr"/>
<pin name="D_VDD" direction="pwr"/>
<pin name="EXT_MIC" direction="in"/>
<pin name="INT_MIC_POS" direction="in"/>
<pin name="MCLK" direction="in"/>
<pin name="SDA"/>
<pin name="SCL" direction="in"/>
<pin name="EP_POS" direction="out"/>
<pin name="INT_MIC_NEG" direction="in"/>
<pin name="BYPASS"/>
<pin name="TEST_MODE/~CS" direction="in"/>
<pin name="PLL_FILT"/>
<pin name="AUX_R" direction="in"/>
<pin name="GPIO_2"/>
<pin name="VREF_FLT"/>
<pin name="AUX_L" direction="in"/>
<pin name="SPI_MODE" direction="in"/>
<pin name="MIC_DET" direction="in"/>
<pin name="CPI_NEG" direction="in"/>
<pin name="CPI_POS" direction="in"/>
<pin name="I2S_SDI" direction="in"/>
<pin name="VSAR2" direction="in"/>
<pin name="VSAR1" direction="in"/>
<pin name="LS_VSS" direction="pwr"/>
<pin name="PLL_VSS" direction="pwr"/>
<pin name="D_VSS" direction="pwr"/>
<pin name="A_VSS" direction="pwr"/>
<pin name="EP_NEG" direction="out"/>
<pin name="HP_R" direction="out"/>
<pin name="EXT_BIAS" direction="out"/>
<pin name="INT_BIAS" direction="out"/>
<pin name="HP_L" direction="out"/>
<pin name="GPIO_1"/>
<pin name="HP_VMID"/>
<pin name="HP_VMID_FB"/>
<pin name="IRQ" direction="out"/>
<pin name="I2S_SDO" direction="out"/>
<pin name="CPO_NEG" direction="out"/>
<pin name="AUX_OUT_NEG" direction="out"/>
<pin name="I2S_WS"/>
<pin name="I2S_CLK"/>
<pin name="LS_POS" direction="out"/>
<pin name="LS_NEG" direction="out"/>
<pin name="CPO_POS" direction="out"/>
<pin name="AUX_OUT_POS" direction="out"/>
</symbol>
<symbol name="LM4936MH">
<pin name="VDD_2" direction="pwr"/>
<pin name="VDD_3" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="I2C/SPI_SELECT" direction="in"/>
<pin name="ID/CE" direction="in"/>
<pin name="SCL/CLK" direction="in"/>
<pin name="SPA/DATA"/>
<pin name="I2C/SPI_VDD" direction="pwr"/>
<pin name="BYPASS" direction="in"/>
<pin name="HP_SENSES" direction="in"/>
<pin name="RIGHT_IN" direction="in"/>
<pin name="BEEP_IN" direction="in"/>
<pin name="LEFT_IN" direction="in"/>
<pin name="LEFT_DOCK" direction="pas"/>
<pin name="RIGHT_DOCK" direction="pas"/>
<pin name="LEFT_GAIN2" direction="in"/>
<pin name="LEFT_GAIN1" direction="in"/>
<pin name="RIGHT_GAIN1" direction="in"/>
<pin name="RIGHT_GAIN2" direction="in"/>
<pin name="EP" direction="pas"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="LEFT_OUT+" direction="out"/>
<pin name="LEFT_OUT-" direction="out"/>
<pin name="RIGHT_OUT-" direction="out"/>
<pin name="RIGHT_OUT+" direction="out"/>
</symbol>
<symbol name="LM4937RL">
<pin name="I2C_VDD" direction="pwr"/>
<pin name="PLLVDD" direction="pwr"/>
<pin name="DVDD" direction="pwr"/>
<pin name="AVDD_2" direction="pwr"/>
<pin name="AVDD" direction="pwr"/>
<pin name="VDDIO" direction="pwr"/>
<pin name="LIN" direction="in"/>
<pin name="RIN" direction="in"/>
<pin name="I2S_SDATA" direction="in"/>
<pin name="I2S_CLK" direction="in"/>
<pin name="I2S_WS" direction="in"/>
<pin name="SDA/SDI" direction="in"/>
<pin name="SCL/SCK" direction="in"/>
<pin name="ADDR/ENB" direction="in"/>
<pin name="MODE" direction="in"/>
<pin name="DIFF-" direction="in"/>
<pin name="DIFF+" direction="in"/>
<pin name="PLL_IN" direction="in"/>
<pin name="MCLK" direction="in"/>
<pin name="BYPASS" direction="pas"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="DGND" direction="pas"/>
<pin name="AGND_2" direction="pas"/>
<pin name="AGND_3" direction="pas"/>
<pin name="AGND" direction="pas"/>
<pin name="PLLGND" direction="pas"/>
<pin name="LS+" direction="out"/>
<pin name="LS-" direction="out"/>
<pin name="EP+" direction="out"/>
<pin name="EP-" direction="out"/>
<pin name="CHP" direction="out"/>
<pin name="LHP" direction="out"/>
<pin name="RHP" direction="out"/>
<pin name="PLL_OUT" direction="out"/>
<pin name="GPIO" direction="out"/>
</symbol>
<symbol name="LM4937TL">
<pin name="I2C_VDD" direction="pwr"/>
<pin name="PLLVDD" direction="pwr"/>
<pin name="DVDD" direction="pwr"/>
<pin name="AVDD_2" direction="pwr"/>
<pin name="AVDD" direction="pwr"/>
<pin name="VDDIO" direction="pwr"/>
<pin name="LIN" direction="in"/>
<pin name="RIN" direction="in"/>
<pin name="I2S_SDATA" direction="in"/>
<pin name="I2S_CLK" direction="in"/>
<pin name="I2S_WS" direction="in"/>
<pin name="SDA/SDI" direction="in"/>
<pin name="SCL/SCK" direction="in"/>
<pin name="ADDR/ENB" direction="in"/>
<pin name="MODE" direction="in"/>
<pin name="DIFF-" direction="in"/>
<pin name="DIFF+" direction="in"/>
<pin name="PLL_IN" direction="in"/>
<pin name="MCLK" direction="in"/>
<pin name="BYPASS" direction="pas"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="DGND" direction="pas"/>
<pin name="AGND_2" direction="pas"/>
<pin name="AGND_3" direction="pas"/>
<pin name="AGND" direction="pas"/>
<pin name="PLLGND" direction="pas"/>
<pin name="LS+" direction="out"/>
<pin name="LS-" direction="out"/>
<pin name="EP+" direction="out"/>
<pin name="EP-" direction="out"/>
<pin name="CHP" direction="out"/>
<pin name="LHP" direction="out"/>
<pin name="RHP" direction="out"/>
<pin name="PLL_OUT" direction="out"/>
<pin name="GPIO" direction="out"/>
</symbol>
<symbol name="LM4938MH">
<pin name="VDD_2" direction="pwr"/>
<pin name="VDD_3" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="SHDN" direction="in"/>
<pin name="MODE" direction="in"/>
<pin name="MUTE" direction="in"/>
<pin name="DC_VOL" direction="in"/>
<pin name="BYPASS" direction="in"/>
<pin name="GAINSELECT" direction="in"/>
<pin name="HP_SENSES" direction="in"/>
<pin name="RIGHT_DOCK" direction="in"/>
<pin name="RIGHT_IN" direction="in"/>
<pin name="BEEP_IN" direction="in"/>
<pin name="LEFT_IN" direction="in"/>
<pin name="LEFT_DOCK" direction="in"/>
<pin name="LEFT_GAIN1" direction="in"/>
<pin name="LEFT_GAIN2" direction="in"/>
<pin name="RIGHT_GAIN1" direction="in"/>
<pin name="RIGHT_GAIN2" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="LEFT_OUT+" direction="out"/>
<pin name="LEFT_OUT-" direction="out"/>
<pin name="RIGHT_OUT-" direction="out"/>
<pin name="RIGHT_OUT+" direction="out"/>
</symbol>
<symbol name="LM49450SQ">
<pin name="VDD" direction="pwr"/>
<pin name="DVDD" direction="pwr"/>
<pin name="IOVDD" direction="pwr"/>
<pin name="LSVDD_2" direction="pwr"/>
<pin name="LSVDD" direction="pwr"/>
<pin name="HPVDD" direction="pwr"/>
<pin name="CPVDD" direction="pwr"/>
<pin name="INL" direction="in"/>
<pin name="INR" direction="in"/>
<pin name="I2S_CLK" direction="in"/>
<pin name="I2S_WS" direction="in"/>
<pin name="I2S_SDI" direction="in"/>
<pin name="SDA" direction="in"/>
<pin name="SCL" direction="in"/>
<pin name="MCLK" direction="in"/>
<pin name="REF" direction="pas"/>
<pin name="HPS" direction="in"/>
<pin name="BYPASS" direction="pas"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="DGND" direction="pas"/>
<pin name="HPGND" direction="pas"/>
<pin name="LLS+" direction="out"/>
<pin name="LLS-" direction="out"/>
<pin name="RLS+" direction="out"/>
<pin name="RLS-" direction="out"/>
<pin name="HPL" direction="out"/>
<pin name="HPR" direction="out"/>
<pin name="C1P" direction="pas"/>
<pin name="C1N" direction="pas"/>
<pin name="HPVSS" direction="pwr"/>
<pin name="CPGND" direction="pas"/>
<pin name="LSGND" direction="pas"/>
</symbol>
<symbol name="LM4947TL">
<pin name="AVDD_2" direction="pwr"/>
<pin name="LSVDD" direction="pwr"/>
<pin name="I2CVDD" direction="pwr"/>
<pin name="AVDD" direction="pwr"/>
<pin name="LHP3D1" direction="in"/>
<pin name="LHP3D2" direction="in"/>
<pin name="RHP3D1" direction="in"/>
<pin name="RHP3D2" direction="in"/>
<pin name="RIN1" direction="in"/>
<pin name="LIN2" direction="in"/>
<pin name="RIN2" direction="in"/>
<pin name="LIN1" direction="in"/>
<pin name="ADDR" direction="pwr"/>
<pin name="SDA" direction="in"/>
<pin name="MIN+" direction="in"/>
<pin name="MIN-" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="SCL" direction="in"/>
<pin name="CBYPASS" direction="pas"/>
<pin name="VOC" direction="out"/>
<pin name="RHP" direction="out"/>
<pin name="LS-" direction="out"/>
<pin name="LS+" direction="out"/>
<pin name="LHP" direction="out"/>
</symbol>
<symbol name="LM4949TL">
<pin name="VDD" direction="pwr"/>
<pin name="VDDLS_2" direction="pwr"/>
<pin name="VDDHP" direction="pwr"/>
<pin name="VDDLS" direction="pwr"/>
<pin name="I2CVDD" direction="pwr"/>
<pin name="SCL" direction="in"/>
<pin name="SDA" direction="in"/>
<pin name="ADR" direction="in"/>
<pin name="BYPASS" direction="in"/>
<pin name="RIN-" direction="in"/>
<pin name="RIN+" direction="in"/>
<pin name="MIN+" direction="in"/>
<pin name="MIN-" direction="in"/>
<pin name="LIN-" direction="in"/>
<pin name="LIN+" direction="in"/>
<pin name="HPGND" direction="pas"/>
<pin name="GNDLS" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="LLS+" direction="out"/>
<pin name="LLS-" direction="out"/>
<pin name="HPR" direction="out"/>
<pin name="HPL" direction="out"/>
<pin name="RLS-" direction="out"/>
<pin name="RLS+" direction="out"/>
<pin name="VOC" direction="out"/>
</symbol>
<symbol name="LM4950TS">
<pin name="VDD" direction="pwr"/>
<pin name="~SHDN" direction="in"/>
<pin name="BYPASS" direction="in"/>
<pin name="VINA" direction="in"/>
<pin name="VINB" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GND(TAB)" direction="pas"/>
<pin name="VOUTA" direction="out"/>
<pin name="VOUTB" direction="out"/>
</symbol>
<symbol name="LM4951SD">
<pin name="VDD" direction="pwr"/>
<pin name="VIN" direction="in"/>
<pin name="BYPASS" direction="in"/>
<pin name="~SHDN" direction="in"/>
<pin name="CCHG" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="VO-" direction="out"/>
<pin name="VO+" direction="out"/>
</symbol>
<symbol name="LM4952TS">
<pin name="VDD" direction="pwr"/>
<pin name="~SHDN" direction="in"/>
<pin name="BYPASS" direction="in"/>
<pin name="-VINA" direction="in"/>
<pin name="-VINB" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VOUTA" direction="out"/>
<pin name="VOUTB" direction="out"/>
<pin name="DC_VOL" direction="out"/>
</symbol>
<symbol name="LM4953SD">
<pin name="AVDD" direction="pwr"/>
<pin name="CPVDD" direction="pwr"/>
<pin name="SD" direction="in"/>
<pin name="CCP+" direction="in"/>
<pin name="CCP-" direction="in"/>
<pin name="VIN" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="AVSS" direction="pwr"/>
<pin name="PGND" direction="pas"/>
<pin name="SGND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="VCP_OUT" direction="out"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="LM4960SQ">
<pin name="VDD" direction="pwr"/>
<pin name="FB" direction="in"/>
<pin name="VAMP" direction="in"/>
<pin name="BYPASS" direction="in"/>
<pin name="REG_SHDN" direction="in"/>
<pin name="AMP_SHDN" direction="in"/>
<pin name="VIN_A" direction="nc"/>
<pin name="VIN_B" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC_6" direction="nc"/>
<pin name="NC_7" direction="nc"/>
<pin name="NC_8" direction="nc"/>
<pin name="NC_9" direction="nc"/>
<pin name="NC_10" direction="nc"/>
<pin name="NC_11" direction="nc"/>
<pin name="NC_12" direction="nc"/>
<pin name="NC_13" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="SW" direction="out"/>
<pin name="VOUT_A" direction="out"/>
<pin name="VOUT_B" direction="out"/>
</symbol>
<symbol name="LM4961LQ">
<pin name="VDD" direction="pwr"/>
<pin name="BYPASS" direction="in"/>
<pin name="BAND-SW" direction="in"/>
<pin name="CCHG" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="VAMP" direction="in"/>
<pin name="SW" direction="out"/>
<pin name="BW1" direction="in"/>
<pin name="BW2" direction="in"/>
<pin name="SHDN1" direction="in"/>
<pin name="SHDN2" direction="in"/>
<pin name="VIN" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC_6" direction="nc"/>
<pin name="NC_7" direction="nc"/>
<pin name="NC_8" direction="nc"/>
<pin name="NC_9" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="SW-OUT" direction="out"/>
<pin name="VOUT-" direction="out"/>
<pin name="VOUT+" direction="out"/>
</symbol>
<symbol name="LM4970SD">
<pin name="VDD" direction="pwr"/>
<pin name="I2CVDD" direction="pwr"/>
<pin name="SCL" direction="in"/>
<pin name="FILT" direction="in"/>
<pin name="SDA" direction="in"/>
<pin name="ADR" direction="in"/>
<pin name="MIN" direction="in"/>
<pin name="LIN" direction="in"/>
<pin name="RIN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="LGND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="LED1" direction="out"/>
<pin name="LED2" direction="out"/>
<pin name="LED3" direction="out"/>
</symbol>
<symbol name="LM5000SD-3">
<pin name="VIN" direction="pwr"/>
<pin name="COMP" direction="in"/>
<pin name="~SHDN" direction="in"/>
<pin name="TEST" direction="in"/>
<pin name="BYP" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="SS" direction="in"/>
<pin name="FS" direction="in"/>
<pin name="AGND" direction="pas"/>
<pin name="PGND_2" direction="pas"/>
<pin name="PGND_3" direction="pas"/>
<pin name="PGND_4" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="SW_2" direction="out"/>
<pin name="SW_3" direction="out"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM5000SD-6">
<pin name="VIN" direction="pwr"/>
<pin name="COMP" direction="in"/>
<pin name="~SHDN" direction="in"/>
<pin name="TEST" direction="in"/>
<pin name="BYP" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="SS" direction="in"/>
<pin name="FS" direction="in"/>
<pin name="AGND" direction="pas"/>
<pin name="PGND_2" direction="pas"/>
<pin name="PGND_3" direction="pas"/>
<pin name="PGND_4" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="SW_2" direction="out"/>
<pin name="SW_3" direction="out"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM5001MA">
<pin name="VCC" direction="pwr"/>
<pin name="VIN" direction="pwr"/>
<pin name="EN" direction="in"/>
<pin name="RT" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="SW" direction="out"/>
<pin name="COMP" direction="out"/>
</symbol>
<symbol name="LM5002MA">
<pin name="VCC" direction="pwr"/>
<pin name="VIN" direction="pwr"/>
<pin name="EN" direction="in"/>
<pin name="RT" direction="in"/>
<pin name="FB"/>
<pin name="GND" direction="pas"/>
<pin name="SW" direction="out"/>
<pin name="COMP" direction="out"/>
</symbol>
<symbol name="LM5005MH">
<pin name="VCC" direction="pwr"/>
<pin name="VIN_2" direction="in"/>
<pin name="VIN" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="SS" direction="in"/>
<pin name="RT" direction="in"/>
<pin name="SD" direction="in"/>
<pin name="IS_2" direction="in"/>
<pin name="IS" direction="in"/>
<pin name="PRE" direction="in"/>
<pin name="BST" direction="in"/>
<pin name="RAMP" direction="in"/>
<pin name="SYNC" direction="in"/>
<pin name="COMP" direction="in"/>
<pin name="AGND" direction="pas"/>
<pin name="PGND_2" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="OUT" direction="out"/>
<pin name="SW_2" direction="out"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM5007MM">
<pin name="VCC" direction="pwr"/>
<pin name="VIN" direction="pwr"/>
<pin name="BST" direction="pas"/>
<pin name="RCL" direction="pas"/>
<pin name="FEEDBACK" direction="in"/>
<pin name="RON" direction="in"/>
<pin name="RTN" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM5007SD">
<pin name="VCC" direction="pwr"/>
<pin name="BST" direction="in"/>
<pin name="RCL" direction="in"/>
<pin name="RTN" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="RON" direction="in"/>
<pin name="VIN" direction="in"/>
<pin name="EPAD" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM5008AMM">
<pin name="VIN" direction="pwr"/>
<pin name="BST" direction="pas"/>
<pin name="RT/SD" direction="in"/>
<pin name="RCL" direction="in"/>
<pin name="RTN" direction="pas"/>
<pin name="SW" direction="pas"/>
<pin name="FB"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="LM5008ASD">
<pin name="VCC" direction="pwr"/>
<pin name="BST" direction="in"/>
<pin name="RCL" direction="in"/>
<pin name="RTN" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="RT/SD" direction="in"/>
<pin name="VIN" direction="in"/>
<pin name="EPAD" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM5008MM">
<pin name="VCC" direction="pwr"/>
<pin name="VIN" direction="pwr"/>
<pin name="BST" direction="pas"/>
<pin name="RCL" direction="pas"/>
<pin name="FEEDBACK" direction="in"/>
<pin name="RON" direction="in"/>
<pin name="RTN" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM5008SDC">
<pin name="VCC" direction="pwr"/>
<pin name="BST" direction="in"/>
<pin name="RCL" direction="in"/>
<pin name="RTN" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="RON/SD" direction="in"/>
<pin name="VIN" direction="in"/>
<pin name="EPAD" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM5009AMM">
<pin name="VIN" direction="pwr"/>
<pin name="BST" direction="pas"/>
<pin name="RT/SD" direction="in"/>
<pin name="RCL" direction="in"/>
<pin name="RTN" direction="pas"/>
<pin name="SW" direction="pas"/>
<pin name="FB"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="LM5009ASD">
<pin name="VCC" direction="pwr"/>
<pin name="BST" direction="in"/>
<pin name="RCL" direction="in"/>
<pin name="RTN" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="RT/SD" direction="in"/>
<pin name="VIN" direction="in"/>
<pin name="EPAD" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM5009MM">
<pin name="VCC" direction="pwr"/>
<pin name="VIN" direction="pwr"/>
<pin name="BST" direction="pas"/>
<pin name="RCL" direction="pas"/>
<pin name="FEEDBACK" direction="in"/>
<pin name="SD/RON" direction="in"/>
<pin name="RTN" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM5009SDC">
<pin name="VCC" direction="pwr"/>
<pin name="BST" direction="in"/>
<pin name="RCL" direction="in"/>
<pin name="RTN" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="RON/SD" direction="in"/>
<pin name="VIN" direction="in"/>
<pin name="EPAD" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM5010AMH">
<pin name="VCC" direction="pwr"/>
<pin name="VIN" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="SS" direction="in"/>
<pin name="BST" direction="in"/>
<pin name="ISEN" direction="in"/>
<pin name="RTN" direction="in"/>
<pin name="RON/SD" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="SGND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM5010AQ0MH">
<pin name="VCC" direction="pwr"/>
<pin name="VIN" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="SS" direction="in"/>
<pin name="BST" direction="in"/>
<pin name="ISEN" direction="in"/>
<pin name="RON/SD" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="SGND" direction="pas"/>
<pin name="RTN" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM5010AQ1MH">
<pin name="VCC" direction="pwr"/>
<pin name="RON/SD" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="BST" direction="in"/>
<pin name="SS" direction="in"/>
<pin name="ISEN" direction="in"/>
<pin name="RTN" direction="in"/>
<pin name="VIN" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="SGND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM5010ASD">
<pin name="VCC" direction="pwr"/>
<pin name="BST" direction="in"/>
<pin name="ISEN" direction="in"/>
<pin name="RTN" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="SS" direction="in"/>
<pin name="SD/RON" direction="in"/>
<pin name="VIN" direction="in"/>
<pin name="SGND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM5010MH">
<pin name="VCC" direction="pwr"/>
<pin name="BST" direction="in"/>
<pin name="ISEN" direction="in"/>
<pin name="SD/RON" direction="in"/>
<pin name="RTN" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="SS" direction="in"/>
<pin name="VIN" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="SGND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM5010SD">
<pin name="VCC" direction="pwr"/>
<pin name="VIN" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="SS" direction="in"/>
<pin name="BST" direction="in"/>
<pin name="RTN" direction="in"/>
<pin name="ISEN" direction="in"/>
<pin name="SD/RON" direction="in"/>
<pin name="SGND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM5020MM-1">
<pin name="VCC" direction="pwr"/>
<pin name="VIN" direction="in"/>
<pin name="CS" direction="in"/>
<pin name="RT/SYNC" direction="in"/>
<pin name="SS" direction="in"/>
<pin name="UVLO" direction="pas"/>
<pin name="VFB" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="COMP" direction="out"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM5020MM-2">
<pin name="VCC" direction="pwr"/>
<pin name="VIN" direction="in"/>
<pin name="CS" direction="in"/>
<pin name="RT/SYNC" direction="in"/>
<pin name="SS" direction="in"/>
<pin name="UVLO" direction="pas"/>
<pin name="VFB" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="COMP" direction="out"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM5020SD-1">
<pin name="VCC" direction="pwr"/>
<pin name="FB" direction="in"/>
<pin name="RT/SYNC" direction="in"/>
<pin name="COMP" direction="in"/>
<pin name="UVLO" direction="in"/>
<pin name="CS" direction="in"/>
<pin name="SS" direction="in"/>
<pin name="VIN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM5021MM-1">
<pin name="VCC" direction="pwr"/>
<pin name="VIN" direction="in"/>
<pin name="COMP" direction="in"/>
<pin name="CS" direction="in"/>
<pin name="RT" direction="in"/>
<pin name="SS" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM5021MM-2">
<pin name="VCC" direction="pwr"/>
<pin name="VIN" direction="in"/>
<pin name="COMP" direction="in"/>
<pin name="CS" direction="in"/>
<pin name="RT" direction="in"/>
<pin name="SS" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM5022MM">
<pin name="VCC" direction="pwr"/>
<pin name="VIN" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="CS" direction="in"/>
<pin name="SS" direction="in"/>
<pin name="COMP" direction="in"/>
<pin name="UVLO" direction="in"/>
<pin name="RT/SYNC" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM5025AMTC">
<pin name="VCC" direction="pwr"/>
<pin name="VIN" direction="in"/>
<pin name="RAMP" direction="in"/>
<pin name="TIME" direction="in"/>
<pin name="SYNC" direction="in"/>
<pin name="COMP" direction="in"/>
<pin name="UVLO" direction="in"/>
<pin name="REF" direction="in"/>
<pin name="SS" direction="in"/>
<pin name="RT" direction="in"/>
<pin name="CS1" direction="in"/>
<pin name="CS2" direction="in"/>
<pin name="PGND" direction="pas"/>
<pin name="AGND" direction="pas"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="LM5025ASD">
<pin name="VCC" direction="pwr"/>
<pin name="VIN" direction="in"/>
<pin name="CS1" direction="in"/>
<pin name="CS2" direction="in"/>
<pin name="RT" direction="in"/>
<pin name="SS" direction="in"/>
<pin name="REF" direction="in"/>
<pin name="COMP" direction="in"/>
<pin name="SYNC" direction="in"/>
<pin name="UVLO" direction="in"/>
<pin name="RAMP" direction="in"/>
<pin name="PGND" direction="pas"/>
<pin name="AGND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
<pin name="TIME" direction="out"/>
</symbol>
<symbol name="LM5025BSD">
<pin name="VCC" direction="pwr"/>
<pin name="RAMP" direction="in"/>
<pin name="TIME" direction="in"/>
<pin name="UVLO" direction="in"/>
<pin name="SYNC" direction="in"/>
<pin name="REF" direction="in"/>
<pin name="COMP" direction="in"/>
<pin name="SS" direction="in"/>
<pin name="RT" direction="in"/>
<pin name="CS1" direction="in"/>
<pin name="CS2" direction="in"/>
<pin name="VIN" direction="in"/>
<pin name="PGND" direction="pas"/>
<pin name="AGND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="OUT_A" direction="out"/>
<pin name="OUT_B" direction="out"/>
</symbol>
<symbol name="LM5025MTC">
<pin name="VCC" direction="pwr"/>
<pin name="VIN" direction="in"/>
<pin name="CS1" direction="in"/>
<pin name="CS2" direction="in"/>
<pin name="TIME" direction="in"/>
<pin name="RAMP" direction="in"/>
<pin name="COMP" direction="in"/>
<pin name="SYNC" direction="in"/>
<pin name="UVLO" direction="in"/>
<pin name="REF" direction="in"/>
<pin name="SS" direction="in"/>
<pin name="RT" direction="in"/>
<pin name="PGND" direction="pas"/>
<pin name="AGND" direction="pas"/>
<pin name="OUT_A" direction="out"/>
<pin name="OUT_B" direction="out"/>
</symbol>
<symbol name="LM5025SD">
<pin name="VCC" direction="pwr"/>
<pin name="VIN" direction="in"/>
<pin name="SYNC" direction="in"/>
<pin name="COMP" direction="in"/>
<pin name="UVLO" direction="pas"/>
<pin name="TIME" direction="in"/>
<pin name="RAMP" direction="in"/>
<pin name="REF" direction="in"/>
<pin name="CS1" direction="in"/>
<pin name="CS2" direction="in"/>
<pin name="SS" direction="in"/>
<pin name="RT" direction="in"/>
<pin name="PGND" direction="pas"/>
<pin name="AGND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="OUT_A" direction="out"/>
<pin name="OUT_B" direction="out"/>
</symbol>
<symbol name="LM5026MT">
<pin name="VCC" direction="pwr"/>
<pin name="VIN" direction="in"/>
<pin name="REF" direction="in"/>
<pin name="CS" direction="in"/>
<pin name="SS" direction="in"/>
<pin name="RT" direction="in"/>
<pin name="RES" direction="in"/>
<pin name="DCL" direction="in"/>
<pin name="COMP" direction="in"/>
<pin name="UVLO" direction="in"/>
<pin name="TIME" direction="in"/>
<pin name="SYNC" direction="in"/>
<pin name="PGND" direction="pas"/>
<pin name="AGND" direction="pas"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="LM5026SD">
<pin name="VCC" direction="pwr"/>
<pin name="VIN" direction="in"/>
<pin name="UVLO" direction="in"/>
<pin name="TIME" direction="in"/>
<pin name="SYNC" direction="in"/>
<pin name="COMP" direction="in"/>
<pin name="RES" direction="in"/>
<pin name="REF" direction="in"/>
<pin name="DCL" direction="in"/>
<pin name="CS" direction="in"/>
<pin name="SS" direction="in"/>
<pin name="RT" direction="in"/>
<pin name="PGND" direction="pas"/>
<pin name="AGND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="LM5027MH">
<pin name="VCC" direction="pwr"/>
<pin name="VIN" direction="in"/>
<pin name="TIME1" direction="in"/>
<pin name="TIME2" direction="in"/>
<pin name="TIME3" direction="in"/>
<pin name="RAMP" direction="in"/>
<pin name="COMP" direction="in"/>
<pin name="SSSR" direction="in"/>
<pin name="OTP" direction="in"/>
<pin name="REF" direction="in"/>
<pin name="UVLO" direction="in"/>
<pin name="RES" direction="in"/>
<pin name="CS" direction="in"/>
<pin name="SS" direction="in"/>
<pin name="RT" direction="in"/>
<pin name="AGND" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
<pin name="OUTSR" direction="out"/>
</symbol>
<symbol name="LM5030MM">
<pin name="VCC" direction="pwr"/>
<pin name="VIN" direction="pwr"/>
<pin name="VFB" direction="in"/>
<pin name="CS" direction="in"/>
<pin name="RT" direction="in"/>
<pin name="SS" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="COMP" direction="out"/>
<pin name="OUT1" direction="out"/>
<pin name="OUT2" direction="out"/>
</symbol>
<symbol name="LM5030SD">
<pin name="VCC" direction="pwr"/>
<pin name="VIN" direction="in"/>
<pin name="VFB" direction="in"/>
<pin name="COMP" direction="in"/>
<pin name="CS" direction="in"/>
<pin name="RT" direction="in"/>
<pin name="SS" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="OUT1" direction="out"/>
<pin name="OUT2" direction="out"/>
</symbol>
<symbol name="LM5032MTC">
<pin name="VCC" direction="pwr"/>
<pin name="VIN" direction="in"/>
<pin name="RT/SYNC" direction="in"/>
<pin name="UVLO" direction="in"/>
<pin name="DCL" direction="in"/>
<pin name="RES" direction="in"/>
<pin name="COMP1" direction="in"/>
<pin name="COMP2" direction="in"/>
<pin name="CS1" direction="in"/>
<pin name="CS2" direction="in"/>
<pin name="SS1" direction="in"/>
<pin name="SS2" direction="in"/>
<pin name="GND1" direction="pas"/>
<pin name="GND2" direction="pas"/>
<pin name="OUT1" direction="out"/>
<pin name="OUT2" direction="out"/>
</symbol>
<symbol name="LM5033MM">
<pin name="VCC" direction="pwr"/>
<pin name="VIN" direction="in"/>
<pin name="CS" direction="in"/>
<pin name="SS" direction="in"/>
<pin name="REF" direction="in"/>
<pin name="COMP" direction="in"/>
<pin name="RT/SYNC" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT1" direction="out"/>
<pin name="OUT2" direction="out"/>
</symbol>
<symbol name="LM5033SD">
<pin name="VCC" direction="pwr"/>
<pin name="REF" direction="in"/>
<pin name="COMP" direction="in"/>
<pin name="SS" direction="in"/>
<pin name="CS" direction="in"/>
<pin name="RT/SYNC" direction="in"/>
<pin name="VIN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="OUT1" direction="out"/>
<pin name="OUT2" direction="out"/>
</symbol>
<symbol name="LM5034MTC">
<pin name="VIN" direction="pwr"/>
<pin name="COMP1" direction="in"/>
<pin name="COMP2" direction="in"/>
<pin name="CS1" direction="in"/>
<pin name="CS2" direction="in"/>
<pin name="SS1" direction="in"/>
<pin name="SS2" direction="in"/>
<pin name="OVLP" direction="in"/>
<pin name="UVLO" direction="in"/>
<pin name="RES" direction="in"/>
<pin name="DCL" direction="in"/>
<pin name="RT/SYNC" direction="in"/>
<pin name="GND1" direction="pas"/>
<pin name="GND2" direction="pas"/>
<pin name="VCC1" direction="out"/>
<pin name="VCC2" direction="out"/>
<pin name="AC1" direction="out"/>
<pin name="AC2" direction="out"/>
<pin name="OUT1" direction="out"/>
<pin name="OUT2" direction="out"/>
</symbol>
<symbol name="LM5035AMH">
<pin name="VCC" direction="pwr"/>
<pin name="VIN" direction="in"/>
<pin name="HB" direction="in"/>
<pin name="HS" direction="in"/>
<pin name="CS" direction="in"/>
<pin name="SS" direction="in"/>
<pin name="RT" direction="in"/>
<pin name="OVP" direction="in"/>
<pin name="DLY" direction="in"/>
<pin name="REF" direction="in"/>
<pin name="RES" direction="in"/>
<pin name="UVLO" direction="in"/>
<pin name="COMP" direction="in"/>
<pin name="RAMP" direction="in"/>
<pin name="PGND" direction="pas"/>
<pin name="AGND" direction="pwr"/>
<pin name="EPAD" direction="pas"/>
<pin name="LO" direction="out"/>
<pin name="HO" direction="out"/>
<pin name="SR1" direction="out"/>
<pin name="SR2" direction="out"/>
</symbol>
<symbol name="LM5035ASQ">
<pin name="VCC" direction="pwr"/>
<pin name="VIN" direction="in"/>
<pin name="COMP" direction="in"/>
<pin name="RAMP" direction="in"/>
<pin name="UVLO" direction="in"/>
<pin name="OVP" direction="in"/>
<pin name="DLY" direction="in"/>
<pin name="RES" direction="in"/>
<pin name="REF" direction="in"/>
<pin name="HS" direction="in"/>
<pin name="HB" direction="in"/>
<pin name="RT" direction="in"/>
<pin name="CS" direction="in"/>
<pin name="SS" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="AGND" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="HO" direction="out"/>
<pin name="LO" direction="out"/>
<pin name="SR1" direction="out"/>
<pin name="SR2" direction="out"/>
</symbol>
<symbol name="LM5035BMH">
<pin name="VCC" direction="pwr"/>
<pin name="HS" direction="in"/>
<pin name="HB" direction="in"/>
<pin name="RAMP" direction="in"/>
<pin name="UVLO" direction="in"/>
<pin name="DLY" direction="in"/>
<pin name="COMP" direction="in"/>
<pin name="REF" direction="in"/>
<pin name="OVP" direction="in"/>
<pin name="RES" direction="in"/>
<pin name="CS" direction="in"/>
<pin name="RT" direction="in"/>
<pin name="SS" direction="in"/>
<pin name="VIN" direction="in"/>
<pin name="PGND" direction="pas"/>
<pin name="AGND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="HO" direction="out"/>
<pin name="LO" direction="out"/>
<pin name="SR1" direction="out"/>
<pin name="SR2" direction="out"/>
</symbol>
<symbol name="LM5035BSQ">
<pin name="VCC" direction="pwr"/>
<pin name="VIN" direction="in"/>
<pin name="COMP" direction="in"/>
<pin name="RAMP" direction="in"/>
<pin name="UVLO" direction="in"/>
<pin name="OVP" direction="in"/>
<pin name="DLY" direction="in"/>
<pin name="RES" direction="in"/>
<pin name="REF" direction="in"/>
<pin name="HS" direction="in"/>
<pin name="HB" direction="in"/>
<pin name="RT" direction="in"/>
<pin name="CS" direction="in"/>
<pin name="SS" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="AGND" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="HO" direction="out"/>
<pin name="LO" direction="out"/>
<pin name="SR1" direction="out"/>
<pin name="SR2" direction="out"/>
</symbol>
<symbol name="LM5035CMH">
<pin name="VCC" direction="pwr"/>
<pin name="HS" direction="in"/>
<pin name="HB" direction="in"/>
<pin name="RAMP" direction="in"/>
<pin name="UVLO" direction="in"/>
<pin name="DLY" direction="in"/>
<pin name="COMP" direction="in"/>
<pin name="REF" direction="in"/>
<pin name="OVP" direction="in"/>
<pin name="RES" direction="in"/>
<pin name="CS" direction="in"/>
<pin name="RT" direction="in"/>
<pin name="SS" direction="in"/>
<pin name="VIN" direction="in"/>
<pin name="PGND" direction="pas"/>
<pin name="AGND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="HO" direction="out"/>
<pin name="LO" direction="out"/>
<pin name="SR1" direction="out"/>
<pin name="SR2" direction="out"/>
</symbol>
<symbol name="LM5035CSQ">
<pin name="VCC" direction="pwr"/>
<pin name="VIN" direction="in"/>
<pin name="COMP" direction="in"/>
<pin name="RAMP" direction="in"/>
<pin name="UVLO" direction="in"/>
<pin name="OVP" direction="in"/>
<pin name="DLY" direction="in"/>
<pin name="RES" direction="in"/>
<pin name="REF" direction="in"/>
<pin name="HS" direction="in"/>
<pin name="HB" direction="in"/>
<pin name="RT" direction="in"/>
<pin name="CS" direction="in"/>
<pin name="SS" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="AGND" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="HO" direction="out"/>
<pin name="LO" direction="out"/>
<pin name="SR1" direction="out"/>
<pin name="SR2" direction="out"/>
</symbol>
<symbol name="LM5035MH">
<pin name="VCC" direction="pwr"/>
<pin name="HS" direction="in"/>
<pin name="HB" direction="in"/>
<pin name="RAMP" direction="in"/>
<pin name="UVLO" direction="in"/>
<pin name="DLY" direction="in"/>
<pin name="COMP" direction="in"/>
<pin name="REF" direction="in"/>
<pin name="OVP" direction="in"/>
<pin name="RES" direction="in"/>
<pin name="CS" direction="in"/>
<pin name="RT" direction="in"/>
<pin name="SS" direction="in"/>
<pin name="VIN" direction="in"/>
<pin name="PGND" direction="pas"/>
<pin name="AGND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="HO" direction="out"/>
<pin name="LO" direction="out"/>
<pin name="SR1" direction="out"/>
<pin name="SR2" direction="out"/>
</symbol>
<symbol name="LM5035SQ">
<pin name="VCC" direction="pwr"/>
<pin name="VIN" direction="in"/>
<pin name="COMP" direction="in"/>
<pin name="RAMP" direction="in"/>
<pin name="UVLO" direction="in"/>
<pin name="OVP" direction="in"/>
<pin name="DLY" direction="in"/>
<pin name="RES" direction="in"/>
<pin name="REF" direction="in"/>
<pin name="HS" direction="in"/>
<pin name="HB" direction="in"/>
<pin name="RT" direction="in"/>
<pin name="CS" direction="in"/>
<pin name="SS" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="AGND" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="HO" direction="out"/>
<pin name="LO" direction="out"/>
<pin name="SR1" direction="out"/>
<pin name="SR2" direction="out"/>
</symbol>
<symbol name="LM5041AMTC">
<pin name="VCC" direction="pwr"/>
<pin name="VIN" direction="pwr"/>
<pin name="CS" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="SS" direction="in"/>
<pin name="TIME" direction="in"/>
<pin name="RT" direction="in"/>
<pin name="UVLO" direction="in"/>
<pin name="PGND" direction="pas"/>
<pin name="AGND" direction="pas"/>
<pin name="HD" direction="out"/>
<pin name="LD" direction="out"/>
<pin name="PUSH" direction="out"/>
<pin name="PULL" direction="out"/>
<pin name="COMP" direction="out"/>
<pin name="REF" direction="out"/>
</symbol>
<symbol name="LM5041BMTC">
<pin name="VCC" direction="pwr"/>
<pin name="VIN" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="CS" direction="in"/>
<pin name="SS" direction="in"/>
<pin name="RT" direction="in"/>
<pin name="REF" direction="in"/>
<pin name="TIME" direction="in"/>
<pin name="UVLO" direction="in"/>
<pin name="PGND" direction="pas"/>
<pin name="AGND" direction="pas"/>
<pin name="PUSH" direction="out"/>
<pin name="PULL" direction="out"/>
<pin name="COMP" direction="out"/>
<pin name="HD" direction="out"/>
<pin name="LD" direction="out"/>
</symbol>
<symbol name="LM5041MTC">
<pin name="VCC" direction="pwr"/>
<pin name="VIN" direction="pwr"/>
<pin name="FB" direction="in"/>
<pin name="CS" direction="in"/>
<pin name="SS" direction="in"/>
<pin name="TIME" direction="in"/>
<pin name="RT" direction="in"/>
<pin name="UVLO" direction="in"/>
<pin name="PGND" direction="pas"/>
<pin name="AGND" direction="pas"/>
<pin name="HD" direction="out"/>
<pin name="LD" direction="out"/>
<pin name="REF" direction="out"/>
<pin name="COMP" direction="out"/>
<pin name="PUSH" direction="out"/>
<pin name="PULL" direction="out"/>
</symbol>
<symbol name="LM5041SD">
<pin name="VCC" direction="pwr"/>
<pin name="VIN" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="CS" direction="in"/>
<pin name="SS" direction="in"/>
<pin name="RT" direction="in"/>
<pin name="REF" direction="in"/>
<pin name="TIME" direction="in"/>
<pin name="UVLO" direction="in"/>
<pin name="PGND" direction="pas"/>
<pin name="AGND" direction="pas"/>
<pin name="THER_PAD" direction="pas"/>
<pin name="PUSH" direction="out"/>
<pin name="PULL" direction="out"/>
<pin name="COMP" direction="out"/>
<pin name="HD" direction="out"/>
<pin name="LD" direction="out"/>
</symbol>
<symbol name="LM5060Q1MM">
<pin name="VIN" direction="pwr"/>
<pin name="EN" direction="in"/>
<pin name="SENSE" direction="in"/>
<pin name="OVP" direction="in"/>
<pin name="UVLO" direction="in"/>
<pin name="TIMER" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GATE" direction="out"/>
<pin name="OUT" direction="out"/>
<pin name="NPGD" direction="out"/>
</symbol>
<symbol name="LM5067MM-1">
<pin name="VCC" direction="pwr"/>
<pin name="UVLO/EN" direction="in"/>
<pin name="OVLO" direction="in"/>
<pin name="TIMER" direction="in"/>
<pin name="SEN" direction="in"/>
<pin name="PWR" direction="in"/>
<pin name="VEE" direction="pwr"/>
<pin name="PGD" direction="out"/>
<pin name="OUT" direction="out"/>
<pin name="GATE" direction="out"/>
</symbol>
<symbol name="LM5067MM-2">
<pin name="VCC" direction="pwr"/>
<pin name="UVLO/EN" direction="in"/>
<pin name="OVLO" direction="in"/>
<pin name="TIMER" direction="in"/>
<pin name="SEN" direction="in"/>
<pin name="PWR" direction="in"/>
<pin name="VEE" direction="pwr"/>
<pin name="PGD" direction="out"/>
<pin name="OUT" direction="out"/>
<pin name="GATE" direction="out"/>
</symbol>
<symbol name="LM5067MW-1">
<pin name="VCC" direction="pwr"/>
<pin name="TIMER" direction="in"/>
<pin name="SENSE" direction="in"/>
<pin name="UVLO/EN" direction="in"/>
<pin name="OVLO" direction="in"/>
<pin name="PWR" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="VEE" direction="pwr"/>
<pin name="GATE" direction="out"/>
<pin name="OUT" direction="out"/>
<pin name="PGD" direction="out"/>
</symbol>
<symbol name="LM5068MM-1">
<pin name="VDD" direction="pwr"/>
<pin name="OV" direction="in"/>
<pin name="UV" direction="in"/>
<pin name="PWRGD" direction="in"/>
<pin name="SENSE" direction="in"/>
<pin name="TIMER" direction="in"/>
<pin name="VEE" direction="pwr"/>
<pin name="GATE" direction="out"/>
</symbol>
<symbol name="LM5068MM-2">
<pin name="VDD" direction="pwr"/>
<pin name="POWERGOOD" direction="in"/>
<pin name="OV" direction="in"/>
<pin name="UV" direction="in"/>
<pin name="SENSE" direction="in"/>
<pin name="TIMER" direction="in"/>
<pin name="VEE" direction="pwr"/>
<pin name="GATE" direction="out"/>
</symbol>
<symbol name="LM5068MM-3">
<pin name="VDD" direction="pwr"/>
<pin name="POWERGOOD" direction="in"/>
<pin name="OV" direction="in"/>
<pin name="UV" direction="in"/>
<pin name="SENSE" direction="in"/>
<pin name="TIMER" direction="in"/>
<pin name="VEE" direction="pwr"/>
<pin name="GATE" direction="out"/>
</symbol>
<symbol name="LM5068MM-4">
<pin name="VDD" direction="pwr"/>
<pin name="POWERGOOD" direction="in"/>
<pin name="OV" direction="in"/>
<pin name="UV" direction="in"/>
<pin name="SENSE" direction="in"/>
<pin name="TIMER" direction="in"/>
<pin name="VEE" direction="pwr"/>
<pin name="GATE" direction="out"/>
</symbol>
<symbol name="LM5069MM-1">
<pin name="VIN" direction="pwr"/>
<pin name="SENSE" direction="in"/>
<pin name="UVLO" direction="in"/>
<pin name="OVLO" direction="in"/>
<pin name="TMR" direction="in"/>
<pin name="PWR" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="PGD" direction="out"/>
<pin name="OUT" direction="out"/>
<pin name="GATE" direction="out"/>
</symbol>
<symbol name="LM5069MM-2">
<pin name="VIN" direction="pwr"/>
<pin name="SENSE" direction="in"/>
<pin name="UVLO" direction="pas"/>
<pin name="OVLO" direction="pas"/>
<pin name="TIMER" direction="pas"/>
<pin name="PWR" direction="pwr"/>
<pin name="GND" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="OUT" direction="out"/>
<pin name="GATE" direction="out"/>
</symbol>
<symbol name="LM5070MTC-50">
<pin name="VCC" direction="pwr"/>
<pin name="VIN" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="CS" direction="in"/>
<pin name="RT" direction="in"/>
<pin name="SS" direction="in"/>
<pin name="RTN" direction="in"/>
<pin name="RCLP" direction="in"/>
<pin name="UVLO" direction="in"/>
<pin name="RSIG" direction="in"/>
<pin name="ARTN" direction="in"/>
<pin name="COMP" direction="in"/>
<pin name="RCLASS" direction="in"/>
<pin name="UVLORTN" direction="in"/>
<pin name="VEE" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM5070MTC-80">
<pin name="VCC" direction="pwr"/>
<pin name="VIN" direction="in"/>
<pin name="RSIG" direction="in"/>
<pin name="RCLASS" direction="in"/>
<pin name="UVLO" direction="in"/>
<pin name="UVLORTN" direction="in"/>
<pin name="RCLP" direction="in"/>
<pin name="RTN" direction="in"/>
<pin name="ARTN" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="COMP" direction="in"/>
<pin name="CS" direction="in"/>
<pin name="RT" direction="in"/>
<pin name="SS" direction="in"/>
<pin name="VEE" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM5070SD-80">
<pin name="VCC" direction="pwr"/>
<pin name="VIN" direction="in"/>
<pin name="RSIG" direction="in"/>
<pin name="RCLASS" direction="in"/>
<pin name="UVLO" direction="in"/>
<pin name="UVLORTN" direction="in"/>
<pin name="RCLP" direction="in"/>
<pin name="RTN" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="COMP" direction="in"/>
<pin name="CS" direction="in"/>
<pin name="RT" direction="in"/>
<pin name="SS" direction="in"/>
<pin name="ARTN" direction="in"/>
<pin name="VEE" direction="pwr"/>
<pin name="EPAD" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM5071MT-50">
<pin name="VCC" direction="pwr"/>
<pin name="VIN" direction="in"/>
<pin name="RSIG" direction="in"/>
<pin name="RCLASS" direction="in"/>
<pin name="AUX" direction="in"/>
<pin name="UVLO" direction="in"/>
<pin name="UVLO_RTN" direction="in"/>
<pin name="RTN" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="COMP" direction="in"/>
<pin name="CS" direction="in"/>
<pin name="RT" direction="in"/>
<pin name="SS" direction="in"/>
<pin name="ARTN" direction="in"/>
<pin name="VEE" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM5071MT-80">
<pin name="VCC" direction="pwr"/>
<pin name="VIN" direction="in"/>
<pin name="RSIG" direction="in"/>
<pin name="RCLASS" direction="in"/>
<pin name="AUX" direction="in"/>
<pin name="UVLO" direction="in"/>
<pin name="UVLO_RTN" direction="in"/>
<pin name="RTN" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="COMP" direction="in"/>
<pin name="CS" direction="in"/>
<pin name="RT" direction="in"/>
<pin name="SS" direction="in"/>
<pin name="ARTN" direction="in"/>
<pin name="VEE" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM5072MH-50">
<pin name="VCC" direction="pwr"/>
<pin name="VIN" direction="pwr"/>
<pin name="RT" direction="pas"/>
<pin name="CS" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="SS" direction="pas"/>
<pin name="RCLASS" direction="pas"/>
<pin name="ICL_FAUX" direction="pas"/>
<pin name="DCCL" direction="pas"/>
<pin name="RAUX" direction="in"/>
<pin name="RTN" direction="pas"/>
<pin name="NPGOOD" direction="pas"/>
<pin name="EP" direction="pas"/>
<pin name="ARTN" direction="pas"/>
<pin name="VEE" direction="pwr"/>
<pin name="OUT" direction="out"/>
<pin name="COMP" direction="out"/>
</symbol>
<symbol name="LM5072MH-80">
<pin name="VCC" direction="pwr"/>
<pin name="VIN" direction="pwr"/>
<pin name="RT" direction="pas"/>
<pin name="CS" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="SS" direction="pas"/>
<pin name="RCLASS" direction="pas"/>
<pin name="ICL_FAUX" direction="pas"/>
<pin name="DCCL" direction="pas"/>
<pin name="RAUX" direction="in"/>
<pin name="RTN" direction="pas"/>
<pin name="NPGOOD" direction="pas"/>
<pin name="EP" direction="pas"/>
<pin name="ARTN" direction="pas"/>
<pin name="VEE" direction="pwr"/>
<pin name="OUT" direction="out"/>
<pin name="COMP" direction="out"/>
</symbol>
<symbol name="LM5085MY">
<pin name="VCC" direction="pwr"/>
<pin name="VIN" direction="in"/>
<pin name="ADJ" direction="in"/>
<pin name="ISEN" direction="in"/>
<pin name="RT" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="EPAD" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="PGATE" direction="out"/>
</symbol>
<symbol name="LM5085QMY">
<pin name="VCC" direction="pwr"/>
<pin name="VIN" direction="in"/>
<pin name="ADJ" direction="in"/>
<pin name="ISEN" direction="in"/>
<pin name="RT" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="EPAD" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="PGATE" direction="out"/>
</symbol>
<symbol name="LM5085SD">
<pin name="VCC" direction="pwr"/>
<pin name="VIN" direction="in"/>
<pin name="ADJ" direction="in"/>
<pin name="ISEN" direction="in"/>
<pin name="RT" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="EP" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="PGATE" direction="out"/>
</symbol>
<symbol name="LM5088MH-1">
<pin name="VCC" direction="pwr"/>
<pin name="VIN" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="DITH" direction="in"/>
<pin name="SS" direction="in"/>
<pin name="CSG" direction="in"/>
<pin name="RAMP" direction="in"/>
<pin name="CS" direction="in"/>
<pin name="RT" direction="in"/>
<pin name="COMP" direction="in"/>
<pin name="BOOT" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="OUT" direction="out"/>
<pin name="SW" direction="out"/>
<pin name="HG" direction="out"/>
</symbol>
<symbol name="LM5088MH-2">
<pin name="VCC" direction="pwr"/>
<pin name="VIN" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="DITH" direction="in"/>
<pin name="SS" direction="in"/>
<pin name="CSG" direction="in"/>
<pin name="RAMP" direction="in"/>
<pin name="CS" direction="in"/>
<pin name="RT" direction="in"/>
<pin name="COMP" direction="in"/>
<pin name="BOOT" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="OUT" direction="out"/>
<pin name="SW" direction="out"/>
<pin name="HG" direction="out"/>
</symbol>
<symbol name="LM50BIM3">
<pin name="+VS" direction="pwr"/>
<pin name="GND" direction="pas"/>
<pin name="VO" direction="out"/>
</symbol>
<symbol name="LM50CIM3">
<pin name="+VS" direction="pwr"/>
<pin name="GND" direction="pas"/>
<pin name="VO" direction="out"/>
</symbol>
<symbol name="LM5100AM">
<pin name="VDD" direction="pwr"/>
<pin name="HS" direction="pas"/>
<pin name="HB" direction="pas"/>
<pin name="HI" direction="in"/>
<pin name="LI" direction="in"/>
<pin name="VSS" direction="pas"/>
<pin name="HO" direction="out"/>
<pin name="LO" direction="out"/>
</symbol>
<symbol name="LM5101AM">
<pin name="VDD" direction="pwr"/>
<pin name="HS" direction="pas"/>
<pin name="HB" direction="pas"/>
<pin name="HI" direction="in"/>
<pin name="LI" direction="in"/>
<pin name="VSS" direction="pas"/>
<pin name="HO" direction="out"/>
<pin name="LO" direction="out"/>
</symbol>
<symbol name="LM5101ASD">
<pin name="VDD" direction="pwr"/>
<pin name="HB" direction="in"/>
<pin name="HS" direction="in"/>
<pin name="HI" direction="in"/>
<pin name="LI" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="VSS" direction="pwr"/>
<pin name="EPAD" direction="pas"/>
<pin name="HO" direction="out"/>
<pin name="LO" direction="out"/>
</symbol>
<symbol name="LM5101BMA">
<pin name="VDD" direction="pwr"/>
<pin name="HS" direction="in"/>
<pin name="HB" direction="in"/>
<pin name="LI" direction="in"/>
<pin name="HI" direction="in"/>
<pin name="VSS" direction="pas"/>
<pin name="LO" direction="out"/>
<pin name="HO" direction="out"/>
</symbol>
<symbol name="LM5101CMA">
<pin name="VDD" direction="pwr"/>
<pin name="HS" direction="in"/>
<pin name="HB" direction="in"/>
<pin name="LI" direction="in"/>
<pin name="HI" direction="in"/>
<pin name="VSS" direction="pas"/>
<pin name="LO" direction="out"/>
<pin name="HO" direction="out"/>
</symbol>
<symbol name="LM5102SD">
<pin name="VDD" direction="pwr"/>
<pin name="HI" direction="in"/>
<pin name="LI" direction="in"/>
<pin name="HB" direction="pas"/>
<pin name="HS" direction="pas"/>
<pin name="RT1" direction="pas"/>
<pin name="RT2" direction="pas"/>
<pin name="EP" direction="pas"/>
<pin name="VSS" direction="pas"/>
<pin name="HO" direction="out"/>
<pin name="LO" direction="out"/>
</symbol>
<symbol name="LM5104M">
<pin name="VDD" direction="pwr"/>
<pin name="HS" direction="pas"/>
<pin name="HB" direction="pas"/>
<pin name="RT" direction="in"/>
<pin name="LI" direction="in"/>
<pin name="VSS" direction="pas"/>
<pin name="HO" direction="out"/>
<pin name="LO" direction="out"/>
</symbol>
<symbol name="LM5105SD">
<pin name="VDD" direction="pwr"/>
<pin name="EN" direction="in"/>
<pin name="IN" direction="in"/>
<pin name="HB" direction="pas"/>
<pin name="HS" direction="pas"/>
<pin name="RDT" direction="pas"/>
<pin name="NC" direction="nc"/>
<pin name="EP" direction="pas"/>
<pin name="VSS" direction="pas"/>
<pin name="HO" direction="out"/>
<pin name="LO" direction="out"/>
</symbol>
<symbol name="LM5106MM">
<pin name="VDD" direction="pwr"/>
<pin name="IN" direction="in"/>
<pin name="HB" direction="in"/>
<pin name="HS" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="RDT" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="VSS" direction="pwr"/>
<pin name="HO" direction="out"/>
<pin name="LO" direction="out"/>
</symbol>
<symbol name="LM5107MA">
<pin name="VDD" direction="pwr"/>
<pin name="HB" direction="in"/>
<pin name="HI" direction="in"/>
<pin name="LI" direction="in"/>
<pin name="HS" direction="in"/>
<pin name="VSS" direction="pwr"/>
<pin name="LO" direction="out"/>
<pin name="HO" direction="out"/>
</symbol>
<symbol name="LM5109BMA">
<pin name="VDD" direction="pwr"/>
<pin name="HI" direction="in"/>
<pin name="LI" direction="in"/>
<pin name="HS" direction="in"/>
<pin name="HB" direction="in"/>
<pin name="VSS" direction="pwr"/>
<pin name="LO" direction="out"/>
<pin name="HO" direction="out"/>
</symbol>
<symbol name="LM5110-1M">
<pin name="VCC" direction="pwr"/>
<pin name="VEE" direction="pwr"/>
<pin name="~SHDN" direction="in"/>
<pin name="IN_A" direction="in"/>
<pin name="IN_B" direction="in"/>
<pin name="IN_REF" direction="pas"/>
<pin name="OUT_A" direction="out"/>
<pin name="OUT_B" direction="out"/>
</symbol>
<symbol name="LM5110-2M">
<pin name="VCC" direction="pwr"/>
<pin name="VEE" direction="pwr"/>
<pin name="~SHDN" direction="in"/>
<pin name="IN_A" direction="in"/>
<pin name="IN_B" direction="in"/>
<pin name="IN_REF" direction="pas"/>
<pin name="OUT_A" direction="out"/>
<pin name="OUT_B" direction="out"/>
</symbol>
<symbol name="LM5111-1M">
<pin name="VCC" direction="pwr"/>
<pin name="IN_A" direction="in"/>
<pin name="IN_B" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="VEE" direction="pwr"/>
<pin name="OUT_A" direction="out"/>
<pin name="OUT_B" direction="out"/>
</symbol>
<symbol name="LM5111-1MY">
<pin name="VCC" direction="pwr"/>
<pin name="IN_A" direction="in"/>
<pin name="IN_B" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="EP" direction="pas"/>
<pin name="VEE" direction="pwr"/>
<pin name="OUT_B" direction="out"/>
<pin name="OUT_A" direction="out"/>
</symbol>
<symbol name="LM5111-2MY">
<pin name="VCC" direction="pwr"/>
<pin name="IN_A" direction="in"/>
<pin name="IN_B" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="EP" direction="pas"/>
<pin name="VEE" direction="pwr"/>
<pin name="OUT_B" direction="out"/>
<pin name="OUT_A" direction="out"/>
</symbol>
<symbol name="LM5111-4M">
<pin name="VCC" direction="pwr"/>
<pin name="INA" direction="in"/>
<pin name="INB" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="VEE" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="LM5112MY">
<pin name="VCC" direction="pwr"/>
<pin name="IN" direction="in"/>
<pin name="IN_B" direction="in"/>
<pin name="IN_REF" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="VEE" direction="pwr"/>
<pin name="EPAD" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM5115MTC">
<pin name="VCC" direction="pwr"/>
<pin name="VBIAS" direction="pwr"/>
<pin name="CS" direction="in"/>
<pin name="HS" direction="in"/>
<pin name="SS" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="HB" direction="in"/>
<pin name="RAMP" direction="in"/>
<pin name="SYNC" direction="in"/>
<pin name="AGND" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="CO" direction="out"/>
<pin name="HO" direction="out"/>
<pin name="LO" direction="out"/>
<pin name="COMP" direction="out"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LM5115SD">
<pin name="VCC" direction="pwr"/>
<pin name="RAMP" direction="in"/>
<pin name="VBIAS" direction="in"/>
<pin name="SYNC" direction="in"/>
<pin name="CS" direction="in"/>
<pin name="SS" direction="in"/>
<pin name="HB" direction="in"/>
<pin name="HS" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="AGND" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="COMP" direction="out"/>
<pin name="VOUT" direction="out"/>
<pin name="CO" direction="out"/>
<pin name="HO" direction="out"/>
<pin name="LO" direction="out"/>
</symbol>
<symbol name="LM5118MH">
<pin name="VCC" direction="pwr"/>
<pin name="VCCX" direction="pwr"/>
<pin name="VIN" direction="pwr"/>
<pin name="EN" direction="in"/>
<pin name="HB" direction="pwr"/>
<pin name="HS" direction="in"/>
<pin name="RT" direction="in"/>
<pin name="SS" direction="in"/>
<pin name="CS" direction="in"/>
<pin name="SYNC" direction="in"/>
<pin name="RAMP" direction="in"/>
<pin name="UVLO" direction="pas"/>
<pin name="CSG" direction="in"/>
<pin name="PGND" direction="pas"/>
<pin name="AGND" direction="pas"/>
<pin name="FB"/>
<pin name="LO" direction="out"/>
<pin name="HO" direction="out"/>
<pin name="COMP" direction="out"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LM5118Q1MH">
<pin name="VCC" direction="pwr"/>
<pin name="VCCX" direction="pwr"/>
<pin name="SYNC" direction="in"/>
<pin name="UVLO" direction="in"/>
<pin name="RAMP" direction="in"/>
<pin name="CS" direction="in"/>
<pin name="RT" direction="in"/>
<pin name="CSG" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="SS" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="HB" direction="in"/>
<pin name="HS" direction="in"/>
<pin name="VIN" direction="in"/>
<pin name="AGND" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="VOUT" direction="out"/>
<pin name="COMP" direction="in"/>
<pin name="LO" direction="out"/>
<pin name="HO" direction="out"/>
</symbol>
<symbol name="LM5574MT">
<pin name="VCC" direction="pwr"/>
<pin name="VIN" direction="in"/>
<pin name="SD" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="IS" direction="in"/>
<pin name="SS" direction="in"/>
<pin name="RT" direction="in"/>
<pin name="PRE" direction="in"/>
<pin name="BST" direction="in"/>
<pin name="RAMP" direction="in"/>
<pin name="SYNC" direction="in"/>
<pin name="COMP" direction="in"/>
<pin name="PGND" direction="pas"/>
<pin name="AGND" direction="pas"/>
<pin name="OUT" direction="out"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM5574QMT">
<pin name="VCC" direction="pwr"/>
<pin name="PRE" direction="in"/>
<pin name="RAMP" direction="in"/>
<pin name="BST" direction="in"/>
<pin name="SYNC" direction="in"/>
<pin name="SD" direction="in"/>
<pin name="SS" direction="in"/>
<pin name="IS" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="RT" direction="in"/>
<pin name="VIN" direction="in"/>
<pin name="AGND" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="COMP" direction="out"/>
<pin name="OUT" direction="out"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM5575MH">
<pin name="VCC" direction="pwr"/>
<pin name="VIN" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="SD" direction="in"/>
<pin name="RT" direction="in"/>
<pin name="IS" direction="in"/>
<pin name="SS" direction="in"/>
<pin name="PRE" direction="in"/>
<pin name="BST" direction="in"/>
<pin name="SYNC" direction="in"/>
<pin name="RAMP" direction="in"/>
<pin name="COMP" direction="in"/>
<pin name="AGND" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="OUT" direction="out"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM5575QMH">
<pin name="VCC" direction="pwr"/>
<pin name="IS" direction="in"/>
<pin name="SD" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="RT" direction="in"/>
<pin name="SS" direction="in"/>
<pin name="SYNC" direction="in"/>
<pin name="COMP" direction="in"/>
<pin name="PRE" direction="in"/>
<pin name="RAMP" direction="in"/>
<pin name="BST" direction="in"/>
<pin name="VIN" direction="in"/>
<pin name="AGND" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="EP" direction="pas"/>
<pin name="OUT" direction="out"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM5576MH">
<pin name="VCC" direction="pwr"/>
<pin name="VIN_2" direction="pwr"/>
<pin name="VIN" direction="pwr"/>
<pin name="SYNC"/>
<pin name="RAMP" direction="in"/>
<pin name="SD" direction="in"/>
<pin name="SS" direction="in"/>
<pin name="RT" direction="in"/>
<pin name="IS_2" direction="in"/>
<pin name="IS" direction="in"/>
<pin name="SW_2" direction="pas"/>
<pin name="SW" direction="pas"/>
<pin name="PRE" direction="pas"/>
<pin name="BST" direction="in"/>
<pin name="EP" direction="pas"/>
<pin name="AGND" direction="pas"/>
<pin name="PGND_2" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="COMP" direction="out"/>
<pin name="OUT" direction="out"/>
<pin name="FB" direction="out"/>
</symbol>
<symbol name="LM5576QMH">
<pin name="VCC" direction="pwr"/>
<pin name="SS" direction="in"/>
<pin name="SD" direction="in"/>
<pin name="IS_2" direction="in"/>
<pin name="IS" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="RT" direction="in"/>
<pin name="RAMP" direction="in"/>
<pin name="SYNC" direction="in"/>
<pin name="PRE" direction="in"/>
<pin name="BST" direction="in"/>
<pin name="VIN_2" direction="in"/>
<pin name="VIN" direction="in"/>
<pin name="PGND_2" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="AGND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="COMP" direction="out"/>
<pin name="OUT" direction="out"/>
<pin name="SW_2" direction="out"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LM5642MH">
<pin name="VDD1" direction="pwr"/>
<pin name="VDD2" direction="pwr"/>
<pin name="VIN" direction="in"/>
<pin name="VLIN5" direction="in"/>
<pin name="SYNC" direction="in"/>
<pin name="UVDELAY" direction="in"/>
<pin name="FB1" direction="in"/>
<pin name="FB2" direction="in"/>
<pin name="KS1" direction="in"/>
<pin name="KS2" direction="in"/>
<pin name="ILIM1" direction="in"/>
<pin name="ILIM2" direction="in"/>
<pin name="ON/SS1" direction="in"/>
<pin name="ON/SS2" direction="in"/>
<pin name="RSNS1" direction="in"/>
<pin name="RSNS2" direction="in"/>
<pin name="CBOOT1" direction="in"/>
<pin name="CBOOT2" direction="in"/>
<pin name="PGND" direction="pas"/>
<pin name="SGND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="HDRV1" direction="out"/>
<pin name="HDRV2" direction="out"/>
<pin name="LDRV1" direction="out"/>
<pin name="LDRV2" direction="out"/>
<pin name="COMP1" direction="out"/>
<pin name="COMP2" direction="out"/>
<pin name="SW1" direction="out"/>
<pin name="SW2" direction="out"/>
</symbol>
<symbol name="LM5642MTC">
<pin name="VDD1" direction="pwr"/>
<pin name="VDD2" direction="pwr"/>
<pin name="VLIN5" direction="pwr"/>
<pin name="VIN" direction="pwr"/>
<pin name="CBOOT1" direction="pas"/>
<pin name="CBOOT2" direction="pas"/>
<pin name="FB1" direction="in"/>
<pin name="FB2" direction="in"/>
<pin name="ILIM1" direction="in"/>
<pin name="ILIM2" direction="in"/>
<pin name="KS1" direction="in"/>
<pin name="KS2" direction="in"/>
<pin name="ON/SS1" direction="in"/>
<pin name="ON/SS2" direction="in"/>
<pin name="SW1" direction="pas"/>
<pin name="SW2" direction="pas"/>
<pin name="RSENS2" direction="in"/>
<pin name="RSNS1" direction="in"/>
<pin name="SYNC" direction="in"/>
<pin name="UVDELAY" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="SGND" direction="pas"/>
<pin name="COMP1" direction="out"/>
<pin name="COMP2" direction="out"/>
<pin name="HDRV1" direction="out"/>
<pin name="HDRV2" direction="out"/>
<pin name="LDRV1" direction="out"/>
<pin name="LDRV2" direction="out"/>
</symbol>
<symbol name="LM5642XMH">
<pin name="VDD1" direction="pwr"/>
<pin name="VDD2" direction="pwr"/>
<pin name="SYNC" direction="in"/>
<pin name="UVDELAY" direction="in"/>
<pin name="VLIN5" direction="in"/>
<pin name="VIN" direction="in"/>
<pin name="ILIM1" direction="in"/>
<pin name="ILIM2" direction="in"/>
<pin name="ON/SS1" direction="in"/>
<pin name="ON/SS2" direction="in"/>
<pin name="FB1" direction="in"/>
<pin name="FB2" direction="in"/>
<pin name="KS1" direction="in"/>
<pin name="KS2" direction="in"/>
<pin name="RSNS1" direction="in"/>
<pin name="RSNS2" direction="in"/>
<pin name="CBOOT1" direction="in"/>
<pin name="CBOOT2" direction="in"/>
<pin name="PGND" direction="pas"/>
<pin name="SGND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="COMP1" direction="out"/>
<pin name="COMP2" direction="out"/>
<pin name="LDRV1" direction="out"/>
<pin name="LDRV2" direction="out"/>
<pin name="HDRV1" direction="out"/>
<pin name="HDRV2" direction="out"/>
<pin name="SW1" direction="out"/>
<pin name="SW2" direction="out"/>
</symbol>
<symbol name="LM5642XMT">
<pin name="VDD1" direction="pwr"/>
<pin name="VDD2" direction="pwr"/>
<pin name="SYNC" direction="in"/>
<pin name="VLIN5" direction="in"/>
<pin name="UVDELAY" direction="pas"/>
<pin name="KS1" direction="in"/>
<pin name="KS2" direction="in"/>
<pin name="FB1" direction="in"/>
<pin name="FB2" direction="in"/>
<pin name="ON/SS1" direction="in"/>
<pin name="ON/SS2" direction="in"/>
<pin name="COMP1" direction="in"/>
<pin name="COMP2" direction="in"/>
<pin name="ILIM1" direction="in"/>
<pin name="ILIM2" direction="in"/>
<pin name="RSNS1" direction="in"/>
<pin name="RSNS2" direction="in"/>
<pin name="CBOOT1" direction="in"/>
<pin name="CBOOT2" direction="in"/>
<pin name="VIN" direction="in"/>
<pin name="SGND" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="SW1" direction="out"/>
<pin name="SW2" direction="out"/>
<pin name="LDRV1" direction="out"/>
<pin name="LDRV2" direction="out"/>
<pin name="HDRV1" direction="out"/>
<pin name="HDRV2" direction="out"/>
</symbol>
<symbol name="LM56BIM">
<pin name="V+" direction="pwr"/>
<pin name="VT1" direction="in"/>
<pin name="VT2" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VREF" direction="out"/>
<pin name="VTEMP" direction="out"/>
<pin name="OUT1" direction="out"/>
<pin name="OUT2" direction="out"/>
</symbol>
<symbol name="LM56BIMM">
<pin name="V+" direction="pwr"/>
<pin name="VT1" direction="in"/>
<pin name="VT2" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VREF" direction="out"/>
<pin name="VTEMP" direction="out"/>
<pin name="OUT1" direction="out"/>
<pin name="OUT2" direction="out"/>
</symbol>
<symbol name="LM56CIM">
<pin name="V+" direction="pwr"/>
<pin name="VT1" direction="in"/>
<pin name="VT2" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VREF" direction="out"/>
<pin name="VTEMP" direction="out"/>
<pin name="OUT1" direction="out"/>
<pin name="OUT2" direction="out"/>
</symbol>
<symbol name="LM56CIMM">
<pin name="V+" direction="pwr"/>
<pin name="VT1" direction="in"/>
<pin name="VT2" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VREF" direction="out"/>
<pin name="VTEMP" direction="out"/>
<pin name="OUT1" direction="out"/>
<pin name="OUT2" direction="out"/>
</symbol>
<symbol name="LM60BIM3">
<pin name="+VS" direction="pwr"/>
<pin name="GND" direction="pas"/>
<pin name="VO" direction="out"/>
</symbol>
<symbol name="LM60BIZ">
<pin name="+VS" direction="pwr"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LM60CIM3">
<pin name="+VS" direction="pwr"/>
<pin name="GND" direction="pas"/>
<pin name="VO" direction="out"/>
</symbol>
<symbol name="LM60CIZ">
<pin name="+VS" direction="pwr"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LM611CM">
<pin name="V+" direction="pwr"/>
<pin name="+IN" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="FB" direction="pas"/>
<pin name="ANODE" direction="pas"/>
<pin name="CATHODE" direction="pas"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC_6" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM6132AIM">
<pin name="V+" direction="pwr"/>
<pin name="-INA" direction="in"/>
<pin name="+INA" direction="in"/>
<pin name="+INB" direction="in"/>
<pin name="-INB" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="LM6132BIM">
<pin name="V+" direction="pwr"/>
<pin name="-INA" direction="in"/>
<pin name="+INA" direction="in"/>
<pin name="+INB" direction="in"/>
<pin name="-INB" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="LM6132BIN">
<pin name="+V" direction="pwr"/>
<pin name="+INA" direction="in"/>
<pin name="-INA" direction="in"/>
<pin name="+INB" direction="in"/>
<pin name="-INB" direction="in"/>
<pin name="-V" direction="pwr"/>
<pin name="OUT_A" direction="out"/>
<pin name="OUT_B" direction="out"/>
</symbol>
<symbol name="LM6134AIM">
<pin name="V+" direction="pwr"/>
<pin name="+INA" direction="in"/>
<pin name="-INA" direction="in"/>
<pin name="+INB" direction="in"/>
<pin name="-INB" direction="in"/>
<pin name="+INC" direction="in"/>
<pin name="-INC" direction="in"/>
<pin name="+IND" direction="in"/>
<pin name="-IND" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
<pin name="OUTC" direction="out"/>
<pin name="OUTD" direction="out"/>
</symbol>
<symbol name="LM6134BIM">
<pin name="V+" direction="pwr"/>
<pin name="+INA" direction="in"/>
<pin name="-INA" direction="in"/>
<pin name="+INB" direction="in"/>
<pin name="-INB" direction="in"/>
<pin name="+INC" direction="in"/>
<pin name="-INC" direction="in"/>
<pin name="+IND" direction="in"/>
<pin name="-IND" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
<pin name="OUTC" direction="out"/>
<pin name="OUTD" direction="out"/>
</symbol>
<symbol name="LM6134BIN">
<pin name="V+" direction="pwr"/>
<pin name="+INA" direction="in"/>
<pin name="-INA" direction="in"/>
<pin name="+INB" direction="in"/>
<pin name="-INB" direction="in"/>
<pin name="+INC" direction="in"/>
<pin name="-INC" direction="in"/>
<pin name="+IND" direction="in"/>
<pin name="-IND" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
<pin name="OUTC" direction="out"/>
<pin name="OUTD" direction="out"/>
</symbol>
<symbol name="LM613IWM">
<pin name="V+" direction="pwr"/>
<pin name="FB" direction="in"/>
<pin name="+COMP1" direction="in"/>
<pin name="-COMP1" direction="in"/>
<pin name="+OPAMP2" direction="in"/>
<pin name="-OPAMP2" direction="in"/>
<pin name="+OPAMP3" direction="in"/>
<pin name="-OPAMP3" direction="in"/>
<pin name="+COMP4" direction="in"/>
<pin name="-COMP4" direction="in"/>
<pin name="V-" direction="pas"/>
<pin name="OUT1" direction="out"/>
<pin name="OUT2" direction="out"/>
<pin name="OUT3" direction="out"/>
<pin name="OUT4" direction="out"/>
<pin name="CATHODE" direction="pas"/>
</symbol>
<symbol name="LM6142AIM">
<pin name="V+" direction="pwr"/>
<pin name="-INA" direction="in"/>
<pin name="+INA" direction="in"/>
<pin name="+INB" direction="in"/>
<pin name="-INB" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="LM6142BIM">
<pin name="V+" direction="pwr"/>
<pin name="-INA" direction="in"/>
<pin name="+INA" direction="in"/>
<pin name="+INB" direction="in"/>
<pin name="-INB" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="LM6142BIN">
<pin name="V+" direction="pwr"/>
<pin name="+INA" direction="in"/>
<pin name="-INA" direction="in"/>
<pin name="-INB" direction="in"/>
<pin name="+INB" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="LM6144AIM">
<pin name="V+" direction="pwr"/>
<pin name="-INA" direction="in"/>
<pin name="+INA" direction="in"/>
<pin name="+INB" direction="in"/>
<pin name="-INB" direction="in"/>
<pin name="-INC" direction="in"/>
<pin name="+INC" direction="in"/>
<pin name="+IND" direction="in"/>
<pin name="-IND" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
<pin name="OUTC" direction="out"/>
<pin name="OUTD" direction="out"/>
</symbol>
<symbol name="LM6144BIM">
<pin name="V+" direction="pwr"/>
<pin name="-INA" direction="in"/>
<pin name="+INA" direction="in"/>
<pin name="+INB" direction="in"/>
<pin name="-INB" direction="in"/>
<pin name="-INC" direction="in"/>
<pin name="+INC" direction="in"/>
<pin name="+IND" direction="in"/>
<pin name="-IND" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
<pin name="OUTC" direction="out"/>
<pin name="OUTD" direction="out"/>
</symbol>
<symbol name="LM6144BIN">
<pin name="V+" direction="pwr"/>
<pin name="+INA" direction="in"/>
<pin name="-INA" direction="in"/>
<pin name="+INB" direction="in"/>
<pin name="-INB" direction="in"/>
<pin name="+INC" direction="in"/>
<pin name="-INC" direction="in"/>
<pin name="+IND" direction="in"/>
<pin name="-IND" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
<pin name="OUTC" direction="out"/>
<pin name="OUTD" direction="out"/>
</symbol>
<symbol name="LM614CWM">
<pin name="V+" direction="pwr"/>
<pin name="FB" direction="in"/>
<pin name="-INA" direction="in"/>
<pin name="+INA" direction="in"/>
<pin name="+INB" direction="in"/>
<pin name="-INB" direction="in"/>
<pin name="-INC" direction="in"/>
<pin name="+INC" direction="in"/>
<pin name="+IND" direction="in"/>
<pin name="-IND" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="CATHODE" direction="pas"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
<pin name="OUTC" direction="out"/>
<pin name="OUTD" direction="out"/>
</symbol>
<symbol name="LM614IWM">
<pin name="V+" direction="pwr"/>
<pin name="FB" direction="in"/>
<pin name="-INA" direction="in"/>
<pin name="+INA" direction="in"/>
<pin name="+INB" direction="in"/>
<pin name="-INB" direction="in"/>
<pin name="-INC" direction="in"/>
<pin name="+INC" direction="in"/>
<pin name="+IND" direction="in"/>
<pin name="-IND" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="CATHODE" direction="pas"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
<pin name="OUTC" direction="out"/>
<pin name="OUTD" direction="out"/>
</symbol>
<symbol name="LM6152ACM">
<pin name="V+" direction="pwr"/>
<pin name="-INA" direction="in"/>
<pin name="+INA" direction="in"/>
<pin name="+INB" direction="in"/>
<pin name="-INB" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="LM6152BCM">
<pin name="V+" direction="pwr"/>
<pin name="-INA" direction="in"/>
<pin name="+INA" direction="in"/>
<pin name="+INB" direction="in"/>
<pin name="-INB" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="LM6154BCM">
<pin name="V+" direction="pwr"/>
<pin name="-INA" direction="in"/>
<pin name="+INA" direction="in"/>
<pin name="+INB" direction="in"/>
<pin name="-INB" direction="in"/>
<pin name="-INC" direction="in"/>
<pin name="+INC" direction="in"/>
<pin name="+IND" direction="in"/>
<pin name="-IND" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
<pin name="OUTC" direction="out"/>
<pin name="OUTD" direction="out"/>
</symbol>
<symbol name="LM6171AIM">
<pin name="V+" direction="pwr"/>
<pin name="-IN" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM6171BIM">
<pin name="V+" direction="pwr"/>
<pin name="+IN" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="N/C_2" direction="nc"/>
<pin name="N/C_3" direction="nc"/>
<pin name="N/C" direction="nc"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM6171BIN">
<pin name="V+" direction="pwr"/>
<pin name="+IN" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="N/C_2" direction="nc"/>
<pin name="N/C_3" direction="nc"/>
<pin name="N/C" direction="nc"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM6172AMJFQMLV">
<pin name="V+" direction="pwr"/>
<pin name="-NEGA" direction="in"/>
<pin name="+POSA" direction="in"/>
<pin name="+POSB" direction="in"/>
<pin name="-NEGB" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="LM6172IM">
<pin name="V+" direction="pwr"/>
<pin name="INVERTING_INPUT_A" direction="in"/>
<pin name="INVERTING_INPUT_B" direction="in"/>
<pin name="NON_INVERTING_INPUT_A" direction="in"/>
<pin name="NON_INVERTING_INPUT_B" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="LM6172IN">
<pin name="V+" direction="pwr"/>
<pin name="POS_A" direction="in"/>
<pin name="POS_B" direction="in"/>
<pin name="NEG_A" direction="in"/>
<pin name="NEG_B" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="LM6181IM-8">
<pin name="V+" direction="pwr"/>
<pin name="NEG" direction="in"/>
<pin name="POS" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM6181IN">
<pin name="V+" direction="pwr"/>
<pin name="+IN" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="N/C_2" direction="nc"/>
<pin name="N/C_3" direction="nc"/>
<pin name="N/C" direction="nc"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM61BIM3">
<pin name="+VS" direction="pwr"/>
<pin name="GND" direction="pas"/>
<pin name="VO" direction="out"/>
</symbol>
<symbol name="LM61CIM3">
<pin name="+VS" direction="pwr"/>
<pin name="GND" direction="pas"/>
<pin name="VO" direction="out"/>
</symbol>
<symbol name="LM6211MF">
<pin name="V+" direction="pwr"/>
<pin name="IN+" direction="in"/>
<pin name="IN-" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LM62BIM3">
<pin name="+VS" direction="pwr"/>
<pin name="GND" direction="pas"/>
<pin name="VO" direction="out"/>
</symbol>
<symbol name="LM63CIMA">
<pin name="VDD" direction="pwr"/>
<pin name="SMBCLK" direction="pas"/>
<pin name="D+" direction="in"/>
<pin name="D-" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="SMBDAT"/>
<pin name="PWM" direction="out"/>
<pin name="~ALERT/TACH"/>
</symbol>
<symbol name="LM6511IM">
<pin name="V+" direction="pwr"/>
<pin name="POS_A" direction="in"/>
<pin name="NEG_A" direction="in"/>
<pin name="OFS" direction="in"/>
<pin name="BAL/STRB" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM6584MT">
<pin name="V+" direction="pwr"/>
<pin name="-INA" direction="in"/>
<pin name="+INA" direction="in"/>
<pin name="+INB" direction="in"/>
<pin name="-INB" direction="in"/>
<pin name="-INC" direction="in"/>
<pin name="+INC" direction="in"/>
<pin name="+IND" direction="in"/>
<pin name="-IND" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
<pin name="OUTC" direction="out"/>
<pin name="OUTD" direction="out"/>
</symbol>
<symbol name="LM6588MA">
<pin name="V+" direction="pwr"/>
<pin name="-INA" direction="in"/>
<pin name="+INA" direction="in"/>
<pin name="-INB" direction="in"/>
<pin name="+INB" direction="in"/>
<pin name="-INC" direction="in"/>
<pin name="+INC" direction="in"/>
<pin name="-IND" direction="in"/>
<pin name="+IND" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
<pin name="OUTC" direction="out"/>
<pin name="OUTD" direction="out"/>
</symbol>
<symbol name="LM70CIMM-3">
<pin name="V+" direction="pwr"/>
<pin name="~CS" direction="in"/>
<pin name="SC" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="SI/O"/>
</symbol>
<symbol name="LM70CIMM-5">
<pin name="V+" direction="pwr"/>
<pin name="SC" direction="in"/>
<pin name="~CS" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="SI/O"/>
</symbol>
<symbol name="LM7121IM">
<pin name="V+" direction="pwr"/>
<pin name="IN-" direction="in"/>
<pin name="IN+" direction="in"/>
<pin name="N/C_2" direction="nc"/>
<pin name="N/C" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTPUT" direction="out"/>
</symbol>
<symbol name="LM7171AIM">
<pin name="V+" direction="pwr"/>
<pin name="-IN" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM7171BIM">
<pin name="V+" direction="pwr"/>
<pin name="-IN" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM7171BIN">
<pin name="V+" direction="pwr"/>
<pin name="+IN" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="N/C_2" direction="nc"/>
<pin name="N/C_3" direction="nc"/>
<pin name="N/C" direction="nc"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM71CIMF">
<pin name="V+" direction="pwr"/>
<pin name="SC" direction="in"/>
<pin name="~CS" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="SI/O"/>
</symbol>
<symbol name="LM7301IM">
<pin name="V+" direction="pwr"/>
<pin name="IN-" direction="in"/>
<pin name="IN+" direction="in"/>
<pin name="N/C_2" direction="nc"/>
<pin name="N/C" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTPUT" direction="out"/>
</symbol>
<symbol name="LM7301IM5">
<pin name="V+" direction="pwr"/>
<pin name="POS" direction="in"/>
<pin name="NEG" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM7321MA">
<pin name="V+" direction="pwr"/>
<pin name="IN-" direction="in"/>
<pin name="IN+" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM7321MF">
<pin name="V+" direction="pwr"/>
<pin name="-IN" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM7322MA">
<pin name="V+" direction="pwr"/>
<pin name="INA-" direction="in"/>
<pin name="INA+" direction="in"/>
<pin name="INB+" direction="in"/>
<pin name="INB-" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="LM7322MM">
<pin name="V+" direction="pwr"/>
<pin name="INA-" direction="in"/>
<pin name="INA+" direction="in"/>
<pin name="INB+" direction="in"/>
<pin name="INB-" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="LM7332MA">
<pin name="V+" direction="pwr"/>
<pin name="INA-" direction="in"/>
<pin name="INA+" direction="in"/>
<pin name="INB+" direction="in"/>
<pin name="INB-" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="LM7341MF">
<pin name="V+" direction="pwr"/>
<pin name="POS" direction="in"/>
<pin name="NEG" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM7372IMA">
<pin name="V+" direction="pwr"/>
<pin name="-IN_2" direction="in"/>
<pin name="+IN_2" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC_6" direction="nc"/>
<pin name="NC_7" direction="nc"/>
<pin name="NC_8" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="LM7372MR">
<pin name="V+" direction="pwr"/>
<pin name="-INA" direction="in"/>
<pin name="+INA" direction="in"/>
<pin name="+INB" direction="in"/>
<pin name="-INB" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="EPAD" direction="pas"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="LM73CIMK-0">
<pin name="VDD" direction="pwr"/>
<pin name="ADDR" direction="in"/>
<pin name="SMBCLK" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="~ALERT" direction="out"/>
<pin name="SMBDAT" direction="out"/>
</symbol>
<symbol name="LM73CIMK-1">
<pin name="VDD" direction="pwr"/>
<pin name="ADDR" direction="in"/>
<pin name="SMBCLK" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="~ALERT" direction="out"/>
<pin name="SMBDAT" direction="out"/>
</symbol>
<symbol name="LM741CH">
<pin name="-INA" direction="in"/>
<pin name="+INA" direction="in"/>
<pin name="OFFSET_NULL" direction="in"/>
<pin name="OFFSET_NULL_2" direction="in"/>
<pin name="V+" direction="in"/>
<pin name="V-" direction="pas"/>
<pin name="NC" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM741CN">
<pin name="V+" direction="pwr"/>
<pin name="POS" direction="in"/>
<pin name="NEG" direction="in"/>
<pin name="OFFSET_NULL" direction="pas"/>
<pin name="OFFSET_NULL_2" direction="pas"/>
<pin name="NC" direction="nc"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM741H">
<pin name="-INA" direction="in"/>
<pin name="+INA" direction="in"/>
<pin name="OFFSET_NULL" direction="in"/>
<pin name="OFFSET_NULL_2" direction="in"/>
<pin name="V+" direction="in"/>
<pin name="V-" direction="pas"/>
<pin name="NC" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM75AIM">
<pin name="+VS" direction="pwr"/>
<pin name="SCL" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A0" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="SDA"/>
<pin name="O.S." direction="out"/>
</symbol>
<symbol name="LM76CHM-5">
<pin name="VS+" direction="pwr"/>
<pin name="SDA"/>
<pin name="SCL" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A0" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="T_CRIT_A" direction="out"/>
<pin name="INT" direction="out"/>
</symbol>
<symbol name="LM77CIMM-3">
<pin name="+VS" direction="pwr"/>
<pin name="SDA"/>
<pin name="SCL" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A0" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="INT" direction="out"/>
<pin name="T_CRIT_A" direction="out"/>
</symbol>
<symbol name="LM78L05ACM">
<pin name="VIN" direction="pwr"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LM809M3-2.63">
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pas"/>
<pin name="~RESET" direction="out"/>
</symbol>
<symbol name="LM809M3-2.93">
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pas"/>
<pin name="~RESET" direction="out"/>
</symbol>
<symbol name="LM809M3-3.08">
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pas"/>
<pin name="~RESET" direction="out"/>
</symbol>
<symbol name="LM809M3-4.63">
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pas"/>
<pin name="~RESET" direction="out"/>
</symbol>
<symbol name="LM8261M5">
<pin name="V+" direction="pwr"/>
<pin name="NEG" direction="in"/>
<pin name="POS" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM8262MM">
<pin name="V+" direction="pwr"/>
<pin name="+INA" direction="in"/>
<pin name="-INA" direction="in"/>
<pin name="+INB" direction="in"/>
<pin name="-INB" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="LM8272MM">
<pin name="V+" direction="pwr"/>
<pin name="+INA" direction="in"/>
<pin name="-INA" direction="in"/>
<pin name="+INB" direction="in"/>
<pin name="-INB" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="LM833N">
<pin name="+VCC" direction="pwr"/>
<pin name="+INA" direction="in"/>
<pin name="-INA" direction="in"/>
<pin name="+INB" direction="in"/>
<pin name="-INB" direction="in"/>
<pin name="-VEE" direction="pwr"/>
<pin name="OUT_A" direction="out"/>
<pin name="OUT_B" direction="out"/>
</symbol>
<symbol name="LM8364BALMF20">
<pin name="IN" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="~RESET" direction="out"/>
</symbol>
<symbol name="LM8365BALMF27">
<pin name="IN" direction="in"/>
<pin name="CD" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="~RESET" direction="out"/>
</symbol>
<symbol name="LM86CIMM">
<pin name="VDD" direction="pwr"/>
<pin name="D+" direction="pas"/>
<pin name="D-" direction="pas"/>
<pin name="T_CRIT_A" direction="pas"/>
<pin name="SMBCLK" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="~ALERT" direction="out"/>
<pin name="SMBDATA"/>
</symbol>
<symbol name="LM9036M-5.0">
<pin name="VIN" direction="pwr"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LM9036MM-3.3">
<pin name="VIN" direction="pwr"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LM9076BMA-5.0">
<pin name="VIN" direction="in"/>
<pin name="CDELAY" direction="pas"/>
<pin name="SD" direction="pas"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="~RESET" direction="out"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LM9076S-3.3">
<pin name="VIN" direction="in"/>
<pin name="~RESET" direction="in"/>
<pin name="CDELAY" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LM9076S-5.0">
<pin name="VIN" direction="in"/>
<pin name="~RESET" direction="in"/>
<pin name="CDELAY" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LM92CIM">
<pin name="VS+" direction="pwr"/>
<pin name="SCL" direction="in"/>
<pin name="T_CRIT_A" direction="in"/>
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="SDA"/>
<pin name="INT" direction="out"/>
</symbol>
<symbol name="LM94021BIMG">
<pin name="VDD" direction="pwr"/>
<pin name="GS0" direction="in"/>
<pin name="GS1" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM94022BIMG">
<pin name="VDD" direction="pwr"/>
<pin name="GS0" direction="in"/>
<pin name="GS1" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LM94022QBIMG">
<pin name="VDD" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="OUT" direction="out"/>
<pin name="GSO" direction="in"/>
<pin name="GS1" direction="in"/>
</symbol>
<symbol name="LM95071CIMF">
<pin name="VDD" direction="pwr"/>
<pin name="SC" direction="in"/>
<pin name="~CS" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="SI/O"/>
</symbol>
<symbol name="LM95214CISD">
<pin name="VDD" direction="pwr"/>
<pin name="SMBCLK" direction="in"/>
<pin name="A0" direction="in"/>
<pin name="D-" direction="in"/>
<pin name="D1+" direction="in"/>
<pin name="D2+" direction="in"/>
<pin name="D3+" direction="in"/>
<pin name="D4+" direction="in"/>
<pin name="NC" direction="in"/>
<pin name="EP" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="SMBDAT"/>
<pin name="~TCRIT1" direction="out"/>
<pin name="~TCRIT2" direction="out"/>
<pin name="~TCRIT3" direction="out"/>
</symbol>
<symbol name="LM95231CIMM">
<pin name="VDD" direction="pwr"/>
<pin name="SMBCLK" direction="in"/>
<pin name="D1+" direction="in"/>
<pin name="D1-" direction="in"/>
<pin name="D2+" direction="in"/>
<pin name="D2-" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="SMBDAT"/>
</symbol>
<symbol name="LM95233CISD">
<pin name="VDD" direction="pwr"/>
<pin name="SMBCLK" direction="in"/>
<pin name="A0" direction="in"/>
<pin name="D-" direction="in"/>
<pin name="D1+" direction="in"/>
<pin name="D2+" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="EP" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="~TCRIT1" direction="out"/>
<pin name="~TCRIT2" direction="out"/>
<pin name="~TCRIT3" direction="out"/>
<pin name="SMBDAT"/>
</symbol>
<symbol name="LM95234CISD">
<pin name="VDD" direction="pwr"/>
<pin name="SMBCLK" direction="in"/>
<pin name="A0" direction="in"/>
<pin name="D-" direction="in"/>
<pin name="D1+" direction="in"/>
<pin name="D3+" direction="in"/>
<pin name="D4+" direction="in"/>
<pin name="D2+" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="EP" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="~TCRIT1" direction="out"/>
<pin name="~TCRIT2" direction="out"/>
<pin name="~TCRIT3" direction="out"/>
<pin name="SMBDAT"/>
</symbol>
<symbol name="LM95235CIMM">
<pin name="VDD" direction="pwr"/>
<pin name="SMBCLK" direction="in"/>
<pin name="D-" direction="in"/>
<pin name="~T_CRIT" direction="out"/>
<pin name="GND" direction="pas"/>
<pin name="D+" direction="out"/>
<pin name="~OS/A0"/>
<pin name="SMBDAT"/>
</symbol>
<symbol name="LM95235DIMM">
<pin name="VDD" direction="pwr"/>
<pin name="SMBCLK" direction="in"/>
<pin name="D-" direction="in"/>
<pin name="~T_CRIT" direction="out"/>
<pin name="GND" direction="pas"/>
<pin name="D+" direction="out"/>
<pin name="~OS/A0"/>
<pin name="SMBDAT"/>
</symbol>
<symbol name="LM95235EIMM">
<pin name="VDD" direction="pwr"/>
<pin name="SMBCLK" direction="in"/>
<pin name="D-" direction="in"/>
<pin name="~T_CRIT" direction="out"/>
<pin name="GND" direction="pas"/>
<pin name="D+" direction="out"/>
<pin name="~OS/A0"/>
<pin name="SMBDAT"/>
</symbol>
<symbol name="LM95235QEIMM">
<pin name="VDD" direction="pwr"/>
<pin name="D+" direction="in"/>
<pin name="D-" direction="in"/>
<pin name="SMBCLK" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="SMBDAT"/>
<pin name="~OS~/A0"/>
<pin name="~T_CRIT" direction="out"/>
</symbol>
<symbol name="LM95245CIMM">
<pin name="VDD" direction="pwr"/>
<pin name="SMBCLK" direction="in"/>
<pin name="D+" direction="in"/>
<pin name="D-" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="~T_CRIT" direction="out"/>
<pin name="~OS~/A0" direction="out"/>
<pin name="SMBDAT"/>
</symbol>
<symbol name="LM97593VH_A">
<pin name="VD_2" direction="pwr"/>
<pin name="VD_3" direction="pwr"/>
<pin name="VD_4" direction="pwr"/>
<pin name="VD" direction="pwr"/>
<pin name="VA_2" direction="pwr"/>
<pin name="VA_3" direction="pwr"/>
<pin name="VA_4" direction="pwr"/>
<pin name="VA_5" direction="pwr"/>
<pin name="VA" direction="pwr"/>
<pin name="VDR_2" direction="pwr"/>
<pin name="VDR_3" direction="pwr"/>
<pin name="VDR" direction="pwr"/>
<pin name="VD18" direction="pwr"/>
<pin name="VINA-" direction="in"/>
<pin name="VINA+" direction="in"/>
<pin name="VINB+" direction="in"/>
<pin name="VINB-" direction="in"/>
<pin name="REFSEL/DCS" direction="in"/>
<pin name="VREF" direction="in"/>
<pin name="D7"/>
<pin name="D6"/>
<pin name="PD" direction="in"/>
<pin name="CK" direction="in"/>
<pin name="~MR" direction="in"/>
<pin name="~SI" direction="in"/>
<pin name="~WR" direction="in"/>
<pin name="~RD" direction="in"/>
<pin name="~CE" direction="in"/>
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="A5" direction="in"/>
<pin name="A6" direction="in"/>
<pin name="A7" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="AGND_2" direction="pas"/>
<pin name="AGND_3" direction="pas"/>
<pin name="AGND_4" direction="pas"/>
<pin name="AGND_5" direction="pas"/>
<pin name="DGND_2" direction="pas"/>
<pin name="AGND_6" direction="pas"/>
<pin name="AGND" direction="pas"/>
<pin name="DGND_3" direction="pas"/>
<pin name="DGND_4" direction="pas"/>
<pin name="DRGND_2" direction="pas"/>
<pin name="DGND" direction="pas"/>
<pin name="DRGND_3" direction="pas"/>
<pin name="DRGND" direction="pas"/>
<pin name="D18GND_2" direction="pas"/>
<pin name="D18GND" direction="pas"/>
<pin name="VCOMA_2" direction="out"/>
<pin name="VRPA" direction="out"/>
<pin name="VRNA" direction="out"/>
<pin name="VRNB" direction="out"/>
<pin name="VRPB" direction="out"/>
<pin name="VCOMA" direction="out"/>
<pin name="BGAIN2" direction="out"/>
<pin name="BGAIN1" direction="out"/>
<pin name="BGAIN0" direction="out"/>
<pin name="~BSTROBE" direction="out"/>
</symbol>
<symbol name="LM97593VH_B">
<pin name="VDR_2" direction="pwr"/>
<pin name="VDR_3" direction="pwr"/>
<pin name="VDR_4" direction="pwr"/>
<pin name="VDR_5" direction="pwr"/>
<pin name="VDR" direction="pwr"/>
<pin name="VD18_2" direction="pwr"/>
<pin name="VD18_3" direction="pwr"/>
<pin name="VD18_4" direction="pwr"/>
<pin name="VD18" direction="pwr"/>
<pin name="SCK_IN" direction="in"/>
<pin name="POUT_SEL2" direction="in"/>
<pin name="POUT_SEL1" direction="in"/>
<pin name="POUT_SEL0" direction="in"/>
<pin name="~POUT_EN" direction="in"/>
<pin name="D0"/>
<pin name="D1"/>
<pin name="D2"/>
<pin name="D3"/>
<pin name="D4"/>
<pin name="D5"/>
<pin name="SCK" direction="out"/>
<pin name="SFS" direction="out"/>
<pin name="TDI" direction="in"/>
<pin name="TMS" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="~TRST" direction="in"/>
<pin name="~SCAN_EN" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="DRGND_2" direction="pas"/>
<pin name="DRGND_3" direction="pas"/>
<pin name="DRGND_4" direction="pas"/>
<pin name="DRGND_5" direction="pas"/>
<pin name="DRGND" direction="pas"/>
<pin name="D18GND_2" direction="pas"/>
<pin name="D18GND_3" direction="pas"/>
<pin name="D18GND_4" direction="pas"/>
<pin name="D18GND_5" direction="pas"/>
<pin name="D18GND" direction="pas"/>
<pin name="RDY" direction="out"/>
<pin name="BOUT" direction="out"/>
<pin name="AOUT" direction="out"/>
<pin name="POUT0" direction="out"/>
<pin name="POUT1" direction="out"/>
<pin name="POUT2" direction="out"/>
<pin name="POUT3" direction="out"/>
<pin name="POUT4" direction="out"/>
<pin name="POUT5" direction="out"/>
<pin name="POUT6" direction="out"/>
<pin name="POUT7" direction="out"/>
<pin name="POUT8" direction="out"/>
<pin name="POUT9" direction="out"/>
<pin name="POUT10" direction="out"/>
<pin name="POUT11" direction="out"/>
<pin name="POUT12" direction="out"/>
<pin name="POUT13" direction="out"/>
<pin name="POUT14" direction="out"/>
<pin name="POUT15" direction="out"/>
<pin name="~ASTROBE" direction="out"/>
<pin name="AGAIN0" direction="out"/>
<pin name="AGAIN1" direction="out"/>
<pin name="AGAIN2" direction="out"/>
<pin name="TDO" direction="out"/>
</symbol>
<symbol name="LM98714BCMT">
<pin name="SH_R" direction="in"/>
<pin name="INCLK+" direction="in"/>
<pin name="INCLK-" direction="in"/>
<pin name="OSR" direction="in"/>
<pin name="OSG" direction="in"/>
<pin name="OSB" direction="in"/>
<pin name="~SEN" direction="in"/>
<pin name="SCLK" direction="in"/>
<pin name="SDIO"/>
<pin name="~RESET" direction="in"/>
<pin name="VCLP" direction="pwr"/>
<pin name="VA_2" direction="pwr"/>
<pin name="VA_3" direction="pwr"/>
<pin name="VA" direction="pwr"/>
<pin name="VR" direction="pwr"/>
<pin name="VD" direction="pwr"/>
<pin name="VC" direction="pwr"/>
<pin name="SH" direction="out"/>
<pin name="CLK_1" direction="out"/>
<pin name="CLK_2" direction="out"/>
<pin name="CLK_3" direction="out"/>
<pin name="CLK4" direction="out"/>
<pin name="CLK5" direction="out"/>
<pin name="CLK6" direction="out"/>
<pin name="CLK7" direction="out"/>
<pin name="CLK8" direction="out"/>
<pin name="CLK9" direction="out"/>
<pin name="CLKOUT/CLK10" direction="out"/>
<pin name="DOUT0/TXOUT0-" direction="out"/>
<pin name="DOUT1/TXOUT0+" direction="out"/>
<pin name="DOUT2/TXOUT1-" direction="out"/>
<pin name="DOUT3/TXOUT1+" direction="out"/>
<pin name="DOUT4/TXOUT2-" direction="out"/>
<pin name="DOUT5/TXOUT2+" direction="out"/>
<pin name="DOUT6/TXCLK-" direction="out"/>
<pin name="DOUT7/TXCLK+" direction="out"/>
<pin name="VREFB" direction="out"/>
<pin name="VREFT" direction="out"/>
<pin name="DVB" direction="out"/>
<pin name="AGND_2" direction="pwr"/>
<pin name="AGND_3" direction="pwr"/>
<pin name="AGND_4" direction="pwr"/>
<pin name="AGND_5" direction="pwr"/>
<pin name="AGND_6" direction="pwr"/>
<pin name="AGND" direction="pwr"/>
<pin name="DGND_2" direction="pwr"/>
<pin name="DGND_3" direction="pwr"/>
<pin name="DGND" direction="pwr"/>
</symbol>
<symbol name="LM98722CCMT">
<pin name="PHIC2" direction="out"/>
<pin name="PHIC1" direction="out"/>
<pin name="SH1" direction="out"/>
<pin name="CE" direction="in"/>
<pin name="CAL" direction="in"/>
<pin name="*RESET" direction="in"/>
<pin name="SH_R" direction="in"/>
<pin name="SDI" direction="in"/>
<pin name="SDO" direction="out"/>
<pin name="SCLK" direction="in"/>
<pin name="*SEN" direction="in"/>
<pin name="VA_2" direction="pwr"/>
<pin name="VA_3" direction="pwr"/>
<pin name="VREFB" direction="out"/>
<pin name="VREFT" direction="out"/>
<pin name="VA_4" direction="pwr"/>
<pin name="VCLP"/>
<pin name="VA" direction="pwr"/>
<pin name="IBIAS" direction="out"/>
<pin name="OSR" direction="in"/>
<pin name="OSG" direction="in"/>
<pin name="OSB" direction="in"/>
<pin name="CPOFILT2" direction="pas"/>
<pin name="DGND_2" direction="pwr"/>
<pin name="DGND_3" direction="pwr"/>
<pin name="DGND" direction="pwr"/>
<pin name="AGND_2" direction="pwr"/>
<pin name="AGND_3" direction="pwr"/>
<pin name="AGND_4" direction="pwr"/>
<pin name="AGND_5" direction="pwr"/>
<pin name="AGND" direction="pwr"/>
<pin name="SH5" direction="out"/>
<pin name="SH4" direction="out"/>
<pin name="PHIB2" direction="out"/>
<pin name="PHIB1" direction="out"/>
<pin name="VC_2" direction="pwr"/>
<pin name="PHIA2" direction="out"/>
<pin name="PHIA1" direction="out"/>
<pin name="CP" direction="out"/>
<pin name="RS" direction="out"/>
<pin name="SH3" direction="out"/>
<pin name="CLKOUT/SH2" direction="out"/>
<pin name="VC" direction="pwr"/>
<pin name="VD" direction="pwr"/>
<pin name="DOUT0/TXOUT0-" direction="out"/>
<pin name="DOUT1/TXOUT0+" direction="out"/>
<pin name="DOUT2/TXOUT1-" direction="out"/>
<pin name="DOUT3/TXOUT1+" direction="out"/>
<pin name="DOUT4/TXOUT2-" direction="out"/>
<pin name="DOUT5/TXOUT2+" direction="out"/>
<pin name="DOUT6/TXCLK-" direction="out"/>
<pin name="DOUT7/TXCLK+" direction="out"/>
<pin name="INCLK-" direction="in"/>
<pin name="INCLK+" direction="in"/>
<pin name="DVB" direction="pas"/>
<pin name="CPOFILT1" direction="pas"/>
</symbol>
<symbol name="LM98725CCMT">
<pin name="PHIC2" direction="out"/>
<pin name="PHIC1" direction="out"/>
<pin name="SH1" direction="out"/>
<pin name="CE" direction="in"/>
<pin name="CAL" direction="in"/>
<pin name="*RESET" direction="in"/>
<pin name="SH_R" direction="in"/>
<pin name="SDI" direction="in"/>
<pin name="SDO" direction="out"/>
<pin name="SCLK" direction="in"/>
<pin name="*SEN" direction="in"/>
<pin name="VA_2" direction="pwr"/>
<pin name="VA_3" direction="pwr"/>
<pin name="VREFB" direction="out"/>
<pin name="VREFT" direction="out"/>
<pin name="VA_4" direction="pwr"/>
<pin name="VCLP"/>
<pin name="VA" direction="pwr"/>
<pin name="IBIAS" direction="out"/>
<pin name="OSR" direction="in"/>
<pin name="OSG" direction="in"/>
<pin name="OSB" direction="in"/>
<pin name="CPOFILT2" direction="pas"/>
<pin name="DGND_2" direction="pwr"/>
<pin name="DGND_3" direction="pwr"/>
<pin name="DGND" direction="pwr"/>
<pin name="AGND_2" direction="pwr"/>
<pin name="AGND_3" direction="pwr"/>
<pin name="AGND_4" direction="pwr"/>
<pin name="AGND_5" direction="pwr"/>
<pin name="AGND" direction="pwr"/>
<pin name="SH5" direction="out"/>
<pin name="SH4" direction="out"/>
<pin name="PHIB2" direction="out"/>
<pin name="PHIB1" direction="out"/>
<pin name="VC_2" direction="pwr"/>
<pin name="PHIA2" direction="out"/>
<pin name="PHIA1" direction="out"/>
<pin name="CP" direction="out"/>
<pin name="RS" direction="out"/>
<pin name="SH3" direction="out"/>
<pin name="CLKOUT/SH2" direction="out"/>
<pin name="VC" direction="pwr"/>
<pin name="VD" direction="pwr"/>
<pin name="DOUT0/TXOUT0-" direction="out"/>
<pin name="DOUT1/TXOUT0+" direction="out"/>
<pin name="DOUT2/TXOUT1-" direction="out"/>
<pin name="DOUT3/TXOUT1+" direction="out"/>
<pin name="DOUT4/TXOUT2-" direction="out"/>
<pin name="DOUT5/TXOUT2+" direction="out"/>
<pin name="DOUT6/TXCLK-" direction="out"/>
<pin name="DOUT7/TXCLK+" direction="out"/>
<pin name="INCLK-" direction="in"/>
<pin name="INCLK+" direction="in"/>
<pin name="DVB" direction="pas"/>
<pin name="CPOFILT1" direction="pas"/>
</symbol>
<symbol name="LM99CIMM">
<pin name="VDD" direction="pwr"/>
<pin name="SMBCLK" direction="in"/>
<pin name="SMBDATA"/>
<pin name="D+" direction="in"/>
<pin name="D-" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="~T_CRIT_A" direction="out"/>
<pin name="~ALERT" direction="out"/>
</symbol>
<symbol name="LMC6001AIN">
<pin name="V+" direction="pwr"/>
<pin name="NEG" direction="in"/>
<pin name="POS" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LMC6001BIN">
<pin name="V+" direction="pwr"/>
<pin name="NEG" direction="in"/>
<pin name="POS" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LMC6024IM">
<pin name="V+" direction="pwr"/>
<pin name="NEG1" direction="in"/>
<pin name="POS1" direction="in"/>
<pin name="NEG2" direction="in"/>
<pin name="POS2" direction="in"/>
<pin name="NEG3" direction="in"/>
<pin name="POS3" direction="in"/>
<pin name="NEG4" direction="in"/>
<pin name="POS4" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT1" direction="out"/>
<pin name="OUT2" direction="out"/>
<pin name="OUT3" direction="out"/>
<pin name="OUT4" direction="out"/>
</symbol>
<symbol name="LMC6032IM">
<pin name="V+" direction="pwr"/>
<pin name="POSA" direction="in"/>
<pin name="POSB" direction="in"/>
<pin name="NEGA" direction="in"/>
<pin name="NEGB" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="LMC6032IN">
<pin name="V+" direction="pwr"/>
<pin name="POSA" direction="in"/>
<pin name="POSB" direction="in"/>
<pin name="NEGA" direction="in"/>
<pin name="NEGB" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="LMC6034IM">
<pin name="V+" direction="pwr"/>
<pin name="POS1" direction="in"/>
<pin name="POS2" direction="in"/>
<pin name="POS3" direction="in"/>
<pin name="POS4" direction="in"/>
<pin name="NEG1" direction="in"/>
<pin name="NEG2" direction="in"/>
<pin name="NEG3" direction="in"/>
<pin name="NEG4" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT1" direction="out"/>
<pin name="OUTB" direction="out"/>
<pin name="OUTC" direction="out"/>
<pin name="OUTD" direction="out"/>
</symbol>
<symbol name="LMC6035IM">
<pin name="V+" direction="pwr"/>
<pin name="NEGA" direction="in"/>
<pin name="NEGB" direction="in"/>
<pin name="POSA" direction="in"/>
<pin name="POSB" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="LMC6035IMM">
<pin name="V+" direction="pwr"/>
<pin name="POSA" direction="in"/>
<pin name="POSB" direction="in"/>
<pin name="NEGA" direction="in"/>
<pin name="NEGB" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="LMC6036IM">
<pin name="V+" direction="pwr"/>
<pin name="-INA" direction="in"/>
<pin name="+INA" direction="in"/>
<pin name="+INB" direction="in"/>
<pin name="-INB" direction="in"/>
<pin name="-INC" direction="in"/>
<pin name="+INC" direction="in"/>
<pin name="+IND" direction="in"/>
<pin name="-IND" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
<pin name="OUTC" direction="out"/>
<pin name="OUTD" direction="out"/>
</symbol>
<symbol name="LMC6041AIM">
<pin name="V+" direction="pwr"/>
<pin name="NEG" direction="in"/>
<pin name="POS" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LMC6041IM">
<pin name="V+" direction="pwr"/>
<pin name="NEG" direction="in"/>
<pin name="POS" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LMC6041IN">
<pin name="V+" direction="pwr"/>
<pin name="NEG" direction="in"/>
<pin name="POS" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LMC6042AIM">
<pin name="V+" direction="pwr"/>
<pin name="NEGA" direction="in"/>
<pin name="NEGB" direction="in"/>
<pin name="POSA" direction="in"/>
<pin name="POSB" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="LMC6042IM">
<pin name="V+" direction="pwr"/>
<pin name="NEGA" direction="in"/>
<pin name="NEGB" direction="in"/>
<pin name="POSA" direction="in"/>
<pin name="POSB" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="LMC6042IN">
<pin name="V+" direction="pwr"/>
<pin name="POS_A" direction="in"/>
<pin name="NEG_A" direction="in"/>
<pin name="POS_B" direction="in"/>
<pin name="NEG_B" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT_A" direction="out"/>
<pin name="OUT_B" direction="out"/>
</symbol>
<symbol name="LMC6044IM">
<pin name="V+" direction="pwr"/>
<pin name="NEG1" direction="in"/>
<pin name="NEG2" direction="in"/>
<pin name="NEG3" direction="in"/>
<pin name="NEG4" direction="in"/>
<pin name="POS1" direction="in"/>
<pin name="POS2" direction="in"/>
<pin name="POS3" direction="in"/>
<pin name="POS4" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT1" direction="out"/>
<pin name="OUTB" direction="out"/>
<pin name="OUTC" direction="out"/>
<pin name="OUTD" direction="out"/>
</symbol>
<symbol name="LMC6044IN">
<pin name="V+" direction="pwr"/>
<pin name="POS_1" direction="in"/>
<pin name="NEG_1" direction="in"/>
<pin name="POS_2" direction="in"/>
<pin name="NEG_2" direction="in"/>
<pin name="POS_3" direction="in"/>
<pin name="NEG_3" direction="in"/>
<pin name="POS_4" direction="in"/>
<pin name="NEG_4" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT_1" direction="out"/>
<pin name="OUT_2" direction="out"/>
<pin name="OUT_3" direction="out"/>
<pin name="OUT_4" direction="out"/>
</symbol>
<symbol name="LMC6061AIM">
<pin name="V+" direction="pwr"/>
<pin name="NEGA" direction="in"/>
<pin name="NEGB" direction="in"/>
<pin name="POSA" direction="in"/>
<pin name="POSB" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="LMC6061IM">
<pin name="V+" direction="pwr"/>
<pin name="NEGA" direction="in"/>
<pin name="NEGB" direction="in"/>
<pin name="POSA" direction="in"/>
<pin name="POSB" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="LMC6062AIM">
<pin name="V+" direction="pwr"/>
<pin name="NEGA" direction="in"/>
<pin name="NEGB" direction="in"/>
<pin name="POSA" direction="in"/>
<pin name="POSB" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="LMC6062IM">
<pin name="V+" direction="pwr"/>
<pin name="NEGA" direction="in"/>
<pin name="NEGB" direction="in"/>
<pin name="POSA" direction="in"/>
<pin name="POSB" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="LMC6062IN">
<pin name="V+" direction="pwr"/>
<pin name="POS_A" direction="in"/>
<pin name="NEG_A" direction="in"/>
<pin name="POS_B" direction="in"/>
<pin name="NEG_B" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT_A" direction="out"/>
<pin name="OUT_B" direction="out"/>
</symbol>
<symbol name="LMC6064AIM">
<pin name="V+" direction="pwr"/>
<pin name="NEG1" direction="in"/>
<pin name="NEG2" direction="in"/>
<pin name="NEG3" direction="in"/>
<pin name="NEG4" direction="in"/>
<pin name="POS1" direction="in"/>
<pin name="POS2" direction="in"/>
<pin name="POS3" direction="in"/>
<pin name="POS4" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT1" direction="out"/>
<pin name="OUT2" direction="out"/>
<pin name="OUT3" direction="out"/>
<pin name="OUTD" direction="out"/>
</symbol>
<symbol name="LMC6064IM">
<pin name="V+" direction="pwr"/>
<pin name="NEG1" direction="in"/>
<pin name="NEG2" direction="in"/>
<pin name="NEG3" direction="in"/>
<pin name="NEG4" direction="in"/>
<pin name="POS1" direction="in"/>
<pin name="POS2" direction="in"/>
<pin name="POS3" direction="in"/>
<pin name="POS4" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT1" direction="out"/>
<pin name="OUT2" direction="out"/>
<pin name="OUT3" direction="out"/>
<pin name="OUTD" direction="out"/>
</symbol>
<symbol name="LMC6064IN">
<pin name="V+" direction="pwr"/>
<pin name="POS1" direction="in"/>
<pin name="POS2" direction="in"/>
<pin name="POS3" direction="in"/>
<pin name="POS4" direction="in"/>
<pin name="NEG1" direction="in"/>
<pin name="NEG2" direction="in"/>
<pin name="NEG3" direction="in"/>
<pin name="NEG4" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT1" direction="out"/>
<pin name="OUT2" direction="out"/>
<pin name="OUT3" direction="out"/>
<pin name="OUT4" direction="out"/>
</symbol>
<symbol name="LMC6081AIM">
<pin name="V+" direction="pwr"/>
<pin name="NEG" direction="in"/>
<pin name="POS" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="LMC6081IM">
<pin name="V+" direction="pwr"/>
<pin name="NEG" direction="in"/>
<pin name="POS" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="LMC6081IN">
<pin name="V+" direction="pwr"/>
<pin name="NEG" direction="in"/>
<pin name="POS" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="V-" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LMC6082AIM">
<pin name="V+" direction="pwr"/>
<pin name="NEGA" direction="in"/>
<pin name="NEGB" direction="in"/>
<pin name="POSA" direction="in"/>
<pin name="POSB" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="LMC6082AIN">
<pin name="V+" direction="pwr"/>
<pin name="POS_A" direction="in"/>
<pin name="NEG_A" direction="in"/>
<pin name="POS_B" direction="in"/>
<pin name="NEG_B" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT_A" direction="out"/>
<pin name="OUT_B" direction="out"/>
</symbol>
<symbol name="LMC6082IM">
<pin name="V+" direction="pwr"/>
<pin name="NEGA" direction="in"/>
<pin name="NEGB" direction="in"/>
<pin name="POSA" direction="in"/>
<pin name="POSB" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="LMC6082IN">
<pin name="V+" direction="pwr"/>
<pin name="NEGA" direction="in"/>
<pin name="POSA" direction="in"/>
<pin name="POSB" direction="in"/>
<pin name="NEGB" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="LMC6084AIM">
<pin name="V+" direction="pwr"/>
<pin name="POS1" direction="in"/>
<pin name="POS2" direction="in"/>
<pin name="POS3" direction="in"/>
<pin name="POS4" direction="in"/>
<pin name="NEG1" direction="in"/>
<pin name="NEG2" direction="in"/>
<pin name="NEG3" direction="in"/>
<pin name="NEG4" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT1" direction="out"/>
<pin name="OUT2" direction="out"/>
<pin name="OUT3" direction="out"/>
<pin name="OUT4" direction="out"/>
</symbol>
<symbol name="LMC6084IM">
<pin name="V+" direction="pwr"/>
<pin name="NEG1" direction="in"/>
<pin name="NEG2" direction="in"/>
<pin name="NEG3" direction="in"/>
<pin name="NEG4" direction="in"/>
<pin name="POS1" direction="in"/>
<pin name="POS2" direction="in"/>
<pin name="POS3" direction="in"/>
<pin name="POS4" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT1" direction="out"/>
<pin name="OUT2" direction="out"/>
<pin name="OUT3" direction="out"/>
<pin name="OUTD" direction="out"/>
</symbol>
<symbol name="LMC6442AIM">
<pin name="V+" direction="pwr"/>
<pin name="-INA" direction="in"/>
<pin name="+INA" direction="in"/>
<pin name="+INB" direction="in"/>
<pin name="-INB" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="LMC6442IN">
<pin name="V+" direction="pwr"/>
<pin name="-INA" direction="in"/>
<pin name="+INA" direction="in"/>
<pin name="+INB" direction="in"/>
<pin name="-INB" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="LMC6462AIM">
<pin name="V+" direction="pwr"/>
<pin name="-INA" direction="in"/>
<pin name="+INA" direction="in"/>
<pin name="+INB" direction="in"/>
<pin name="-INB" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="LMC6462AIN">
<pin name="V+" direction="pwr"/>
<pin name="IN_A-" direction="in"/>
<pin name="IN_A+" direction="in"/>
<pin name="IN_B+" direction="in"/>
<pin name="IN_B-" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT_A" direction="out"/>
<pin name="OUT_B" direction="out"/>
</symbol>
<symbol name="LMC6462BIM">
<pin name="V+" direction="pwr"/>
<pin name="-INA" direction="in"/>
<pin name="+INA" direction="in"/>
<pin name="+INB" direction="in"/>
<pin name="-INB" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="LMC6462BIN">
<pin name="V+" direction="pwr"/>
<pin name="INA+" direction="in"/>
<pin name="INA-" direction="in"/>
<pin name="INB-" direction="in"/>
<pin name="INB+" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="LMC6464AIM">
<pin name="V+" direction="pwr"/>
<pin name="+INA" direction="in"/>
<pin name="-INA" direction="in"/>
<pin name="+INB" direction="in"/>
<pin name="-INB" direction="in"/>
<pin name="+INC" direction="in"/>
<pin name="-INC" direction="in"/>
<pin name="+IND" direction="in"/>
<pin name="-IND" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
<pin name="OUTC" direction="out"/>
<pin name="OUTD" direction="out"/>
</symbol>
<symbol name="LMC6464BIM">
<pin name="V+" direction="pwr"/>
<pin name="+INA" direction="in"/>
<pin name="-INA" direction="in"/>
<pin name="+INB" direction="in"/>
<pin name="-INB" direction="in"/>
<pin name="+INC" direction="in"/>
<pin name="-INC" direction="in"/>
<pin name="+IND" direction="in"/>
<pin name="-IND" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
<pin name="OUTC" direction="out"/>
<pin name="OUTD" direction="out"/>
</symbol>
<symbol name="LMC6464BIN">
<pin name="V+" direction="pwr"/>
<pin name="INA+" direction="in"/>
<pin name="INA-" direction="in"/>
<pin name="INB+" direction="in"/>
<pin name="INB-" direction="in"/>
<pin name="INC+" direction="in"/>
<pin name="INC-" direction="in"/>
<pin name="IND+" direction="in"/>
<pin name="IND-" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
<pin name="OUTC" direction="out"/>
<pin name="OUTD" direction="out"/>
</symbol>
<symbol name="LMC6482AIM">
<pin name="V+" direction="pwr"/>
<pin name="NEGA" direction="in"/>
<pin name="POSA" direction="in"/>
<pin name="POSB" direction="in"/>
<pin name="NEGB" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="LMC6482AIN">
<pin name="V+" direction="pwr"/>
<pin name="POS_A" direction="in"/>
<pin name="POS_B" direction="in"/>
<pin name="NEG_A" direction="in"/>
<pin name="NEG_B" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT_A" direction="out"/>
<pin name="OUT_B" direction="out"/>
</symbol>
<symbol name="LMC6482IM">
<pin name="V+" direction="pwr"/>
<pin name="NEGA" direction="in"/>
<pin name="POSA" direction="in"/>
<pin name="POSB" direction="in"/>
<pin name="NEGB" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="LMC6482IMM">
<pin name="V+" direction="pwr"/>
<pin name="NEGA" direction="in"/>
<pin name="NEGB" direction="in"/>
<pin name="POSA" direction="in"/>
<pin name="POSB" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="LMC6482IN">
<pin name="V+" direction="pwr"/>
<pin name="POSA" direction="in"/>
<pin name="NEGA" direction="in"/>
<pin name="POSB" direction="in"/>
<pin name="NEGB" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="LMC6484AIM">
<pin name="V+" direction="pwr"/>
<pin name="NEG1" direction="in"/>
<pin name="NEG2" direction="in"/>
<pin name="NEG3" direction="in"/>
<pin name="NEG4" direction="in"/>
<pin name="POS1" direction="in"/>
<pin name="POS2" direction="in"/>
<pin name="POS3" direction="in"/>
<pin name="POS4" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT1" direction="out"/>
<pin name="OUT2" direction="out"/>
<pin name="OUT3" direction="out"/>
<pin name="OUTD" direction="out"/>
</symbol>
<symbol name="LMC6484AIN">
<pin name="V+" direction="pwr"/>
<pin name="POS_1" direction="in"/>
<pin name="NEG_1" direction="in"/>
<pin name="POS_2" direction="in"/>
<pin name="NEG_2" direction="in"/>
<pin name="POS_3" direction="in"/>
<pin name="NEG_3" direction="in"/>
<pin name="POS_4" direction="in"/>
<pin name="NEG_4" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT_1" direction="out"/>
<pin name="OUT_2" direction="out"/>
<pin name="OUT_3" direction="out"/>
<pin name="OUT_4" direction="out"/>
</symbol>
<symbol name="LMC6484IM">
<pin name="V+" direction="pwr"/>
<pin name="NEG1" direction="in"/>
<pin name="NEG2" direction="in"/>
<pin name="NEG3" direction="in"/>
<pin name="NEG4" direction="in"/>
<pin name="POS1" direction="in"/>
<pin name="POS2" direction="in"/>
<pin name="POS3" direction="in"/>
<pin name="POS4" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT1" direction="out"/>
<pin name="OUT2" direction="out"/>
<pin name="OUT3" direction="out"/>
<pin name="OUTD" direction="out"/>
</symbol>
<symbol name="LMC6484IN">
<pin name="V+" direction="pwr"/>
<pin name="POS1" direction="in"/>
<pin name="POS2" direction="in"/>
<pin name="POS3" direction="in"/>
<pin name="POS4" direction="in"/>
<pin name="NEG1" direction="in"/>
<pin name="NEG2" direction="in"/>
<pin name="NEG3" direction="in"/>
<pin name="NEG4" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT1" direction="out"/>
<pin name="OUT2" direction="out"/>
<pin name="OUT3" direction="out"/>
<pin name="OUT4" direction="out"/>
</symbol>
<symbol name="LMC6492AEM">
<pin name="V+" direction="pwr"/>
<pin name="-INA" direction="in"/>
<pin name="+INA" direction="in"/>
<pin name="+INB" direction="in"/>
<pin name="-INB" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="LMC6492BEM">
<pin name="V+" direction="pwr"/>
<pin name="-INA" direction="in"/>
<pin name="+INA" direction="in"/>
<pin name="+INB" direction="in"/>
<pin name="-INB" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="LMC6494AEM">
<pin name="V+" direction="pwr"/>
<pin name="+INA" direction="in"/>
<pin name="-INA" direction="in"/>
<pin name="+INB" direction="in"/>
<pin name="-INB" direction="in"/>
<pin name="+INC" direction="in"/>
<pin name="-INC" direction="in"/>
<pin name="+IND" direction="in"/>
<pin name="-IND" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
<pin name="OUTC" direction="out"/>
<pin name="OUTD" direction="out"/>
</symbol>
<symbol name="LMC6494BEM">
<pin name="V+" direction="pwr"/>
<pin name="+INA" direction="in"/>
<pin name="-INA" direction="in"/>
<pin name="+INB" direction="in"/>
<pin name="-INB" direction="in"/>
<pin name="+INC" direction="in"/>
<pin name="-INC" direction="in"/>
<pin name="+IND" direction="in"/>
<pin name="-IND" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
<pin name="OUTC" direction="out"/>
<pin name="OUTD" direction="out"/>
</symbol>
<symbol name="LMC6572AIM">
<pin name="V+" direction="pwr"/>
<pin name="NEGA" direction="in"/>
<pin name="NEGB" direction="in"/>
<pin name="POSA" direction="in"/>
<pin name="POSB" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="LMC6572BIM">
<pin name="V+" direction="pwr"/>
<pin name="NEGA" direction="in"/>
<pin name="NEGB" direction="in"/>
<pin name="POSA" direction="in"/>
<pin name="POSB" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="LMC6574AIM">
<pin name="V+" direction="pwr"/>
<pin name="IN1+" direction="in"/>
<pin name="IN1-" direction="in"/>
<pin name="IN2+" direction="in"/>
<pin name="IN2-" direction="in"/>
<pin name="IN3+" direction="in"/>
<pin name="IN3-" direction="in"/>
<pin name="IN4+" direction="in"/>
<pin name="IN4-" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT1" direction="out"/>
<pin name="OUT2" direction="out"/>
<pin name="OUT3" direction="out"/>
<pin name="OUT4" direction="out"/>
</symbol>
<symbol name="LMC6574BIM">
<pin name="V+" direction="pwr"/>
<pin name="IN1+" direction="in"/>
<pin name="IN1-" direction="in"/>
<pin name="IN2+" direction="in"/>
<pin name="IN2-" direction="in"/>
<pin name="IN3+" direction="in"/>
<pin name="IN3-" direction="in"/>
<pin name="IN4+" direction="in"/>
<pin name="IN4-" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT1" direction="out"/>
<pin name="OUT2" direction="out"/>
<pin name="OUT3" direction="out"/>
<pin name="OUT4" direction="out"/>
</symbol>
<symbol name="LMC660AIM">
<pin name="V+" direction="pwr"/>
<pin name="IN1+" direction="in"/>
<pin name="IN1-" direction="in"/>
<pin name="IN2+" direction="in"/>
<pin name="IN2-" direction="in"/>
<pin name="IN3+" direction="in"/>
<pin name="IN3-" direction="in"/>
<pin name="IN4+" direction="in"/>
<pin name="IN4-" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT1" direction="out"/>
<pin name="OUT2" direction="out"/>
<pin name="OUT3" direction="out"/>
<pin name="OUT4" direction="out"/>
</symbol>
<symbol name="LMC660AIN">
<pin name="V+" direction="pwr"/>
<pin name="POS_1" direction="in"/>
<pin name="NEG_1" direction="in"/>
<pin name="POS_2" direction="in"/>
<pin name="NEG_2" direction="in"/>
<pin name="POS_3" direction="in"/>
<pin name="NEG_3" direction="in"/>
<pin name="POS_4" direction="in"/>
<pin name="NEG_4" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT_1" direction="out"/>
<pin name="OUT_2" direction="out"/>
<pin name="OUT_3" direction="out"/>
<pin name="OUT_4" direction="out"/>
</symbol>
<symbol name="LMC660CM">
<pin name="V+" direction="pwr"/>
<pin name="IN1+" direction="in"/>
<pin name="IN1-" direction="in"/>
<pin name="IN2+" direction="in"/>
<pin name="IN2-" direction="in"/>
<pin name="IN3+" direction="in"/>
<pin name="IN3-" direction="in"/>
<pin name="IN4+" direction="in"/>
<pin name="IN4-" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT1" direction="out"/>
<pin name="OUT2" direction="out"/>
<pin name="OUT3" direction="out"/>
<pin name="OUT4" direction="out"/>
</symbol>
<symbol name="LMC660CN">
<pin name="V+" direction="pwr"/>
<pin name="POS_1" direction="in"/>
<pin name="NEG_1" direction="in"/>
<pin name="POS_2" direction="in"/>
<pin name="NEG_2" direction="in"/>
<pin name="POS_3" direction="in"/>
<pin name="NEG_3" direction="in"/>
<pin name="POS_4" direction="in"/>
<pin name="NEG_4" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT_1" direction="out"/>
<pin name="OUT_2" direction="out"/>
<pin name="OUT_3" direction="out"/>
<pin name="OUT_4" direction="out"/>
</symbol>
<symbol name="LMC662AIM">
<pin name="V+" direction="pwr"/>
<pin name="NEGA" direction="in"/>
<pin name="NEGB" direction="in"/>
<pin name="POSA" direction="in"/>
<pin name="POSB" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="LMC662AIN">
<pin name="V+" direction="pwr"/>
<pin name="POS_A" direction="in"/>
<pin name="NEG_A" direction="in"/>
<pin name="POS_B" direction="in"/>
<pin name="NEG_B" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT_A" direction="out"/>
<pin name="OUT_B" direction="out"/>
</symbol>
<symbol name="LMC662CM">
<pin name="V+" direction="pwr"/>
<pin name="NEGA" direction="in"/>
<pin name="NEGB" direction="in"/>
<pin name="POSA" direction="in"/>
<pin name="POSB" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="LMC662CN">
<pin name="V+" direction="pwr"/>
<pin name="POS_A" direction="in"/>
<pin name="NEG_A" direction="in"/>
<pin name="POS_B" direction="in"/>
<pin name="NEG_B" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT_A" direction="out"/>
<pin name="OUT_B" direction="out"/>
</symbol>
<symbol name="LMC6762AIM">
<pin name="V+" direction="pwr"/>
<pin name="-INA" direction="in"/>
<pin name="+INA" direction="in"/>
<pin name="+INB" direction="in"/>
<pin name="-INB" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="LMC6762BIM">
<pin name="V+" direction="pwr"/>
<pin name="-INA" direction="in"/>
<pin name="+INA" direction="in"/>
<pin name="+INB" direction="in"/>
<pin name="-INB" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="LMC6772AIM">
<pin name="V+" direction="pwr"/>
<pin name="-INA" direction="in"/>
<pin name="+INA" direction="in"/>
<pin name="+INB" direction="in"/>
<pin name="-INB" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="LMC6772AIMM">
<pin name="V+" direction="pwr"/>
<pin name="IN_A-" direction="in"/>
<pin name="IN_A+" direction="in"/>
<pin name="IN_B+" direction="in"/>
<pin name="IN_B-" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="LMC6772BIM">
<pin name="V+" direction="pwr"/>
<pin name="-INA" direction="in"/>
<pin name="+INA" direction="in"/>
<pin name="+INB" direction="in"/>
<pin name="-INB" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="LMC6772BIN">
<pin name="VCC" direction="pwr"/>
<pin name="IN_A+" direction="in"/>
<pin name="IN_A-" direction="in"/>
<pin name="IN_B+" direction="in"/>
<pin name="IN_B-" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT_A" direction="out"/>
<pin name="OUT_B" direction="out"/>
</symbol>
<symbol name="LMC6772QMM">
<pin name="V+" direction="pwr"/>
<pin name="IN_A-" direction="in"/>
<pin name="IN_A+" direction="in"/>
<pin name="IN_B+" direction="in"/>
<pin name="IN_B-" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="LMC7101AIM5">
<pin name="V+" direction="pwr"/>
<pin name="POS" direction="in"/>
<pin name="NEG" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LMC7101BIM5">
<pin name="OUT" direction="out"/>
<pin name="V+" direction="pas"/>
<pin name="+IN" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="V-" direction="pas"/>
</symbol>
<symbol name="LMC7101QM5">
<pin name="V+" direction="pwr"/>
<pin name="POS" direction="in"/>
<pin name="NEG" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LMC7111BIM5">
<pin name="V+" direction="pwr"/>
<pin name="POS" direction="in"/>
<pin name="NEG" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LMC7211AIM">
<pin name="V+" direction="pwr"/>
<pin name="NEG" direction="in"/>
<pin name="POS" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LMC7211AIM5">
<pin name="V+" direction="pwr"/>
<pin name="POS" direction="in"/>
<pin name="NEG" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LMC7211BIM">
<pin name="V+" direction="pwr"/>
<pin name="NEG" direction="in"/>
<pin name="POS" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LMC7211BIM5">
<pin name="V+" direction="pwr"/>
<pin name="POS" direction="in"/>
<pin name="NEG" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LMC7215IM">
<pin name="V+" direction="pwr"/>
<pin name="NEG" direction="in"/>
<pin name="POS" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LMC7215IM5">
<pin name="V+" direction="pwr"/>
<pin name="POS" direction="in"/>
<pin name="NEG" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LMC7221AIM">
<pin name="V+" direction="pwr"/>
<pin name="NEG" direction="in"/>
<pin name="POS" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LMC7221AIM5">
<pin name="V+" direction="pwr"/>
<pin name="POS" direction="in"/>
<pin name="NEG" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LMC7221BIM">
<pin name="V+" direction="pwr"/>
<pin name="NEG" direction="in"/>
<pin name="POS" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LMC7221BIM5">
<pin name="V+" direction="pwr"/>
<pin name="POS" direction="in"/>
<pin name="NEG" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LMC7225IM5">
<pin name="V+" direction="pwr"/>
<pin name="POS" direction="in"/>
<pin name="NEG" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LMC8101MM">
<pin name="V+" direction="pwr"/>
<pin name="NEG" direction="in"/>
<pin name="POS" direction="in"/>
<pin name="SL" direction="pas"/>
<pin name="SD" direction="pas"/>
<pin name="NC" direction="nc"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LMD18200T">
<pin name="BOOTSTRAP1" direction="in"/>
<pin name="DIRECTION_IN" direction="in"/>
<pin name="BRAKE_IN" direction="in"/>
<pin name="PWM_IN" direction="in"/>
<pin name="BOOTSTRAP2" direction="in"/>
<pin name="VS_POWER_SUPPLY" direction="pwr"/>
<pin name="GND" direction="pas"/>
<pin name="CURR_SENSE_OUT" direction="out"/>
<pin name="THERM_OUT" direction="out"/>
<pin name="OUTPUT2" direction="out"/>
<pin name="OUTPUT1" direction="in"/>
</symbol>
<symbol name="LME49600TS">
<pin name="VIN" direction="in"/>
<pin name="BW" direction="pas"/>
<pin name="VCC" direction="pwr"/>
<pin name="VOUT" direction="out"/>
<pin name="VEE" direction="pwr"/>
</symbol>
<symbol name="LME49713HA">
<pin name="+IN" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
<pin name="NC_2" direction="pas"/>
<pin name="NC_3" direction="pas"/>
<pin name="NC" direction="pas"/>
<pin name="OUTPUT" direction="out"/>
</symbol>
<symbol name="LME49713MA">
<pin name="V+" direction="pwr"/>
<pin name="+IN" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTPUT" direction="out"/>
</symbol>
<symbol name="LME49721MA">
<pin name="VSS" direction="pwr"/>
<pin name="+IN_A" direction="in"/>
<pin name="-IN_A" direction="in"/>
<pin name="+IN_B" direction="in"/>
<pin name="-IN_B" direction="in"/>
<pin name="VDD" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="LME49722MA">
<pin name="V+" direction="pwr"/>
<pin name="POSA" direction="in"/>
<pin name="NEGA" direction="in"/>
<pin name="POSB" direction="in"/>
<pin name="NEGB" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="LME49723MA">
<pin name="V+" direction="pwr"/>
<pin name="POSA" direction="in"/>
<pin name="NEGA" direction="in"/>
<pin name="POSB" direction="in"/>
<pin name="NEGB" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="LME49724MR">
<pin name="VCC" direction="pwr"/>
<pin name="EN" direction="in"/>
<pin name="VIN-" direction="in"/>
<pin name="VIN+" direction="in"/>
<pin name="VOCM" direction="pas"/>
<pin name="EP" direction="pas"/>
<pin name="VEE" direction="pwr"/>
<pin name="VOUT-" direction="out"/>
<pin name="VOUT+" direction="out"/>
</symbol>
<symbol name="LME49725MA">
<pin name="V+" direction="pwr"/>
<pin name="POSA" direction="in"/>
<pin name="NEGA" direction="in"/>
<pin name="POSB" direction="in"/>
<pin name="NEGB" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="LME49726MY">
<pin name="VDD" direction="pwr"/>
<pin name="POSA" direction="in"/>
<pin name="NEGA" direction="in"/>
<pin name="POSB" direction="in"/>
<pin name="NEGB" direction="in"/>
<pin name="EP" direction="pas"/>
<pin name="VSS" direction="pwr"/>
<pin name="OUT_A" direction="out"/>
<pin name="OUT_B" direction="out"/>
</symbol>
<symbol name="LME49743MT">
<pin name="V+" direction="pwr"/>
<pin name="+IN1" direction="in"/>
<pin name="-IN1" direction="in"/>
<pin name="+IN2" direction="in"/>
<pin name="-IN2" direction="in"/>
<pin name="+IN3" direction="in"/>
<pin name="-IN3" direction="in"/>
<pin name="+IN4" direction="in"/>
<pin name="-IN4" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT1" direction="out"/>
<pin name="OUT2" direction="out"/>
<pin name="OUT3" direction="out"/>
<pin name="OUT4" direction="out"/>
</symbol>
<symbol name="LME49811TB">
<pin name="SD" direction="pas"/>
<pin name="IN+" direction="in"/>
<pin name="IN-" direction="in"/>
<pin name="COMP" direction="pas"/>
<pin name="VCC+" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC_6" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="VEE-" direction="pwr"/>
<pin name="SINK" direction="out"/>
<pin name="SOURCE" direction="out"/>
</symbol>
<symbol name="LME49830TB">
<pin name="MUTE" direction="pas"/>
<pin name="IN+" direction="in"/>
<pin name="IN-" direction="in"/>
<pin name="COMP" direction="pas"/>
<pin name="+VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="BASE_M" direction="nc"/>
<pin name="BASE_P" direction="nc"/>
<pin name="OSENSE" direction="nc"/>
<pin name="-VEE" direction="pwr"/>
<pin name="P_OUT" direction="out"/>
<pin name="N_OUT" direction="out"/>
</symbol>
<symbol name="LME49860NA">
<pin name="V+" direction="pwr"/>
<pin name="POS_A" direction="in"/>
<pin name="NEG_A" direction="in"/>
<pin name="POS_B" direction="in"/>
<pin name="NEG_B" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT_A" direction="out"/>
<pin name="OUT_B" direction="out"/>
</symbol>
<symbol name="LME49870MA">
<pin name="V+" direction="pwr"/>
<pin name="+IN" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="V-" direction="pwr"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LMH0001SQ">
<pin name="SDI" direction="in"/>
<pin name="~SDI" direction="in"/>
<pin name="RREF" direction="in"/>
<pin name="VCC" direction="pwr"/>
<pin name="SDO" direction="out"/>
<pin name="~SDO" direction="out"/>
<pin name="NC_2" direction="pas"/>
<pin name="NC_3" direction="pas"/>
<pin name="NC_4" direction="pas"/>
<pin name="NC_5" direction="pas"/>
<pin name="NC_6" direction="pas"/>
<pin name="NC_7" direction="pas"/>
<pin name="NC_8" direction="pas"/>
<pin name="NC_9" direction="pas"/>
<pin name="NC" direction="pas"/>
<pin name="DAP" direction="pwr"/>
<pin name="VEE" direction="pwr"/>
</symbol>
<symbol name="LMH0002MA">
<pin name="VCC" direction="pwr"/>
<pin name="SDI" direction="in"/>
<pin name="~SDI" direction="in"/>
<pin name="RREF" direction="in"/>
<pin name="VEE" direction="pwr"/>
<pin name="SD/~HD" direction="out"/>
<pin name="~SDO" direction="out"/>
<pin name="SDO" direction="out"/>
</symbol>
<symbol name="LMH0002SQ">
<pin name="SDI" direction="in"/>
<pin name="~SDI" direction="in"/>
<pin name="RREF" direction="in"/>
<pin name="SD-HD" direction="pas"/>
<pin name="VCC" direction="pwr"/>
<pin name="SDO" direction="out"/>
<pin name="~SDO" direction="out"/>
<pin name="NC_2" direction="pas"/>
<pin name="NC_3" direction="pas"/>
<pin name="NC_4" direction="pas"/>
<pin name="NC_5" direction="pas"/>
<pin name="NC_6" direction="pas"/>
<pin name="NC_7" direction="pas"/>
<pin name="NC_8" direction="pas"/>
<pin name="NC" direction="pas"/>
<pin name="DAP" direction="pwr"/>
<pin name="VEE" direction="pwr"/>
</symbol>
<symbol name="LMH0024MA">
<pin name="VCC_2" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="CLI" direction="pas"/>
<pin name="BYPASS" direction="pas"/>
<pin name="SDI" direction="in"/>
<pin name="~SDI" direction="in"/>
<pin name="AEC+" direction="pas"/>
<pin name="AEC-" direction="pas"/>
<pin name="NC" direction="nc"/>
<pin name="VEE_2" direction="pwr"/>
<pin name="VEE_3" direction="pwr"/>
<pin name="VEE_4" direction="pwr"/>
<pin name="VEE" direction="pwr"/>
<pin name="~SDO" direction="out"/>
<pin name="SDO" direction="out"/>
<pin name="MUTE" direction="pas"/>
</symbol>
<symbol name="LMH0026MH">
<pin name="VCC" direction="pwr"/>
<pin name="VCCO_2" direction="pwr"/>
<pin name="VCCO" direction="pwr"/>
<pin name="SDI" direction="in"/>
<pin name="RSVD" direction="in"/>
<pin name="~SDI" direction="in"/>
<pin name="SCO_EN" direction="in"/>
<pin name="~O/PMUTE" direction="in"/>
<pin name="BP/~AUTO-BP" direction="in"/>
<pin name="XTALIN/EXTCLK" direction="in"/>
<pin name="LF1" direction="in"/>
<pin name="LF2" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="EPAD" direction="pas"/>
<pin name="XTALOUT" direction="out"/>
<pin name="LOCKDET" direction="out"/>
<pin name="SCO/SDO2" direction="out"/>
<pin name="~SCO/SDO2" direction="out"/>
<pin name="SDO" direction="out"/>
<pin name="~SDO" direction="out"/>
<pin name="SD" direction="out"/>
</symbol>
<symbol name="LMH0030VS">
<pin name="VDDD_2" direction="pwr"/>
<pin name="VDDD" direction="pwr"/>
<pin name="VDDZ" direction="pwr"/>
<pin name="VDDLS" direction="pwr"/>
<pin name="VDDIO" direction="pwr"/>
<pin name="VDDPLLD" direction="pwr"/>
<pin name="VDDSD" direction="pwr"/>
<pin name="VDDPLLA" direction="pwr"/>
<pin name="ACLK" direction="in"/>
<pin name="VCLK" direction="in"/>
<pin name="IO0"/>
<pin name="IO1"/>
<pin name="DV0" direction="in"/>
<pin name="DV1" direction="in"/>
<pin name="DV2" direction="in"/>
<pin name="DV3" direction="in"/>
<pin name="DV4" direction="in"/>
<pin name="DV5" direction="in"/>
<pin name="DV6" direction="in"/>
<pin name="DV7" direction="in"/>
<pin name="DV8" direction="in"/>
<pin name="DV9" direction="in"/>
<pin name="DV10" direction="in"/>
<pin name="DV11" direction="in"/>
<pin name="DV12" direction="in"/>
<pin name="DV13" direction="in"/>
<pin name="DV14" direction="in"/>
<pin name="DV15" direction="in"/>
<pin name="DV16" direction="in"/>
<pin name="DV17" direction="in"/>
<pin name="DV18" direction="in"/>
<pin name="DV19" direction="in"/>
<pin name="RESET" direction="in"/>
<pin name="RD/~WR" direction="in"/>
<pin name="ANC/~CTRL" direction="in"/>
<pin name="RREFPRE" direction="in"/>
<pin name="RREFLVL" direction="in"/>
<pin name="VSSD_2" direction="pwr"/>
<pin name="VSSSD_2" direction="pwr"/>
<pin name="VSSD_3" direction="pwr"/>
<pin name="VSSSD" direction="pwr"/>
<pin name="VSSLS" direction="pwr"/>
<pin name="VSSD" direction="pwr"/>
<pin name="VSSPLLD" direction="pwr"/>
<pin name="VSSIO" direction="pwr"/>
<pin name="VSSPLLA" direction="pwr"/>
<pin name="IO2"/>
<pin name="IO3"/>
<pin name="IO4"/>
<pin name="IO5"/>
<pin name="IO6"/>
<pin name="IO7"/>
<pin name="AD0"/>
<pin name="AD1"/>
<pin name="AD2"/>
<pin name="AD3"/>
<pin name="AD4"/>
<pin name="AD5"/>
<pin name="AD6"/>
<pin name="AD7"/>
<pin name="AD8"/>
<pin name="AD9"/>
<pin name="SDO" direction="out"/>
<pin name="~SDO" direction="out"/>
</symbol>
<symbol name="LMH0031VS">
<pin name="AD9"/>
<pin name="AD8"/>
<pin name="AD7"/>
<pin name="AD6"/>
<pin name="AD5"/>
<pin name="VSSD_2" direction="pwr"/>
<pin name="AD4"/>
<pin name="AD3"/>
<pin name="AD2"/>
<pin name="AD1"/>
<pin name="AD0"/>
<pin name="ACLK" direction="pas"/>
<pin name="IO7"/>
<pin name="IO6"/>
<pin name="IO5"/>
<pin name="IO4"/>
<pin name="IO3"/>
<pin name="IO2"/>
<pin name="VSSIO_2" direction="pwr"/>
<pin name="DV19" direction="out"/>
<pin name="DV18" direction="out"/>
<pin name="DV17" direction="out"/>
<pin name="DV16" direction="out"/>
<pin name="DV15" direction="pas"/>
<pin name="VDDIO_2" direction="pwr"/>
<pin name="DV14" direction="out"/>
<pin name="DV13" direction="out"/>
<pin name="DV12" direction="out"/>
<pin name="DV11" direction="out"/>
<pin name="DV10" direction="out"/>
<pin name="VDDD_2" direction="pwr"/>
<pin name="VDDD_3" direction="pwr"/>
<pin name="VDDD" direction="pwr"/>
<pin name="VDDPLL" direction="pwr"/>
<pin name="VSSPLL" direction="pwr"/>
<pin name="VSSD_3" direction="pwr"/>
<pin name="VSSD" direction="pwr"/>
<pin name="DV9" direction="out"/>
<pin name="DV8" direction="out"/>
<pin name="DV7" direction="out"/>
<pin name="DV6" direction="out"/>
<pin name="DV5" direction="out"/>
<pin name="DV4" direction="out"/>
<pin name="DV3" direction="out"/>
<pin name="DV2" direction="out"/>
<pin name="DV1" direction="out"/>
<pin name="DV0" direction="out"/>
<pin name="IO1"/>
<pin name="IO0"/>
<pin name="VSSIO_3" direction="pwr"/>
<pin name="VDDIO" direction="pwr"/>
<pin name="RESET" direction="pas"/>
<pin name="VCLK" direction="pas"/>
<pin name="RREF" direction="pas"/>
<pin name="RBB" direction="pas"/>
<pin name="VSSSI" direction="pwr"/>
<pin name="SDI_2" direction="in"/>
<pin name="SDI" direction="in"/>
<pin name="VDDSI" direction="pwr"/>
<pin name="VSSIO" direction="pwr"/>
<pin name="XTALI/EXT" direction="pas"/>
<pin name="XTALO" direction="pas"/>
<pin name="ANC/CTRL" direction="pas"/>
<pin name="RD/WR" direction="pas"/>
</symbol>
<symbol name="LMH0034MA">
<pin name="VCC_2" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="CLI" direction="pas"/>
<pin name="BYPASS" direction="pas"/>
<pin name="SDI" direction="in"/>
<pin name="~SDI" direction="in"/>
<pin name="AEC+" direction="pas"/>
<pin name="AEC-" direction="pas"/>
<pin name="MUTEREF" direction="pas"/>
<pin name="VEE_2" direction="pwr"/>
<pin name="VEE_3" direction="pwr"/>
<pin name="VEE_4" direction="pwr"/>
<pin name="VEE" direction="pwr"/>
<pin name="~SDO" direction="out"/>
<pin name="SDO" direction="out"/>
<pin name="MUTE/~CD"/>
</symbol>
<symbol name="LMH0036SQ">
<pin name="VCC_2" direction="pwr"/>
<pin name="VCC_3" direction="pwr"/>
<pin name="VCC_4" direction="pwr"/>
<pin name="VCC_5" direction="pwr"/>
<pin name="VCC_6" direction="pwr"/>
<pin name="VCC_7" direction="pwr"/>
<pin name="VCC_8" direction="pwr"/>
<pin name="VCC_9" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="SEL0" direction="in"/>
<pin name="SEL1" direction="in"/>
<pin name="SCO_EN" direction="in"/>
<pin name="XTALIN/EXTCLK" direction="in"/>
<pin name="BPASS/~AUTOBYPSS" direction="in"/>
<pin name="~O/PMUTE" direction="in"/>
<pin name="LOCKDET" direction="pas"/>
<pin name="LF1" direction="pas"/>
<pin name="LF2" direction="pas"/>
<pin name="SDI0" direction="in"/>
<pin name="~SDI0" direction="in"/>
<pin name="SDI1" direction="in"/>
<pin name="~SDI1" direction="in"/>
<pin name="SDI2" direction="in"/>
<pin name="~SDI2" direction="in"/>
<pin name="SDI3" direction="in"/>
<pin name="~SDI3" direction="in"/>
<pin name="RSVD" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="EP" direction="pwr"/>
<pin name="VEE_2" direction="pwr"/>
<pin name="VEE_3" direction="pwr"/>
<pin name="VEE_4" direction="pwr"/>
<pin name="VEE_5" direction="pwr"/>
<pin name="VEE_6" direction="pwr"/>
<pin name="VEE_7" direction="pwr"/>
<pin name="VEE_8" direction="pwr"/>
<pin name="VEE_9" direction="pwr"/>
<pin name="VEE_10" direction="pwr"/>
<pin name="VEE_11" direction="pwr"/>
<pin name="VEE_12" direction="pwr"/>
<pin name="VEE_13" direction="pwr"/>
<pin name="VEE_14" direction="pwr"/>
<pin name="VEE" direction="pwr"/>
<pin name="SD" direction="out"/>
<pin name="XTALOUT" direction="out"/>
<pin name="SCO/SDO2" direction="out"/>
<pin name="~SCO/SDO2" direction="out"/>
<pin name="SDO" direction="out"/>
<pin name="~SDO" direction="out"/>
</symbol>
<symbol name="LMH0041SQ">
<pin name="VDD2V5_2" direction="pwr"/>
<pin name="VDD2V5_3" direction="pwr"/>
<pin name="VDD2V5" direction="pwr"/>
<pin name="VDD3V3_2" direction="pwr"/>
<pin name="VDD3V3_3" direction="pwr"/>
<pin name="VDD3V3_4" direction="pwr"/>
<pin name="VDD3V3" direction="pwr"/>
<pin name="VDDPLL" direction="pwr"/>
<pin name="RXCLK-" direction="in"/>
<pin name="RXCLK+" direction="in"/>
<pin name="RSET" direction="in"/>
<pin name="SCK" direction="in"/>
<pin name="RXIN0+" direction="in"/>
<pin name="RXIN0-" direction="in"/>
<pin name="RXIN1-" direction="in"/>
<pin name="RXIN1+" direction="in"/>
<pin name="RX0-" direction="in"/>
<pin name="RX0+" direction="in"/>
<pin name="RX1-" direction="in"/>
<pin name="RX1+" direction="in"/>
<pin name="RX2-" direction="in"/>
<pin name="RX2+" direction="in"/>
<pin name="RX3-" direction="in"/>
<pin name="RX3+" direction="in"/>
<pin name="RX4-" direction="in"/>
<pin name="RX4+" direction="in"/>
<pin name="RX_MUX_SEL" direction="in"/>
<pin name="LOOPTHRU_EN" direction="in"/>
<pin name="SDA"/>
<pin name="SMB_CS" direction="in"/>
<pin name="~RESET" direction="in"/>
<pin name="DVB_ASI" direction="in"/>
<pin name="LF_CP" direction="in"/>
<pin name="LF_REF" direction="in"/>
<pin name="RSVD_H" direction="in"/>
<pin name="DNC" direction="nc"/>
<pin name="EP" direction="pas"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="TXOUT-" direction="out"/>
<pin name="TXOUT+" direction="out"/>
<pin name="~LOCK" direction="out"/>
<pin name="GPIO_0"/>
<pin name="GPIO_1"/>
<pin name="GPIO_2"/>
</symbol>
<symbol name="LMH0044SQ">
<pin name="VCC_2" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="SDI" direction="in"/>
<pin name="~SDI" direction="in"/>
<pin name="MUTE" direction="pas"/>
<pin name="AEC+" direction="pas"/>
<pin name="~CD" direction="pas"/>
<pin name="AEC-" direction="pas"/>
<pin name="BYPASS" direction="pas"/>
<pin name="MUTEREF" direction="pas"/>
<pin name="EP" direction="pas"/>
<pin name="VEE_2" direction="pwr"/>
<pin name="VEE_3" direction="pwr"/>
<pin name="VEE_4" direction="pwr"/>
<pin name="VEE" direction="pwr"/>
<pin name="~SDO" direction="out"/>
<pin name="SDO" direction="out"/>
</symbol>
<symbol name="LMH0046MH">
<pin name="VCCO_2" direction="pwr"/>
<pin name="VCCO" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="SCO_EN" direction="in"/>
<pin name="BP/~AUTO-BP" direction="in"/>
<pin name="RATE0" direction="in"/>
<pin name="RATE1" direction="in"/>
<pin name="~OPMUTE" direction="in"/>
<pin name="XTAL_IN/EXT_CLK" direction="in"/>
<pin name="LF1" direction="pas"/>
<pin name="LF2" direction="pas"/>
<pin name="SDI" direction="in"/>
<pin name="~SDI" direction="in"/>
<pin name="VEE" direction="pas"/>
<pin name="SD/~HD" direction="out"/>
<pin name="LOCK_DET" direction="out"/>
<pin name="SCO/SDO2" direction="out"/>
<pin name="~SCO/~SDO2" direction="out"/>
<pin name="XTAL_OUT" direction="out"/>
<pin name="SDO" direction="out"/>
<pin name="~SDO" direction="out"/>
</symbol>
<symbol name="LMH0050SQ">
<pin name="VDD2V5_2" direction="pwr"/>
<pin name="VDD2V5_3" direction="pwr"/>
<pin name="VDD2V5_4" direction="pwr"/>
<pin name="VDD3V3_2" direction="pwr"/>
<pin name="VDD2V5_5" direction="pwr"/>
<pin name="VDD2V5" direction="pwr"/>
<pin name="VDD3V3" direction="pwr"/>
<pin name="VDDPLL" direction="pwr"/>
<pin name="TXCLK-" direction="in"/>
<pin name="TXCLK+" direction="in"/>
<pin name="RSET" direction="in"/>
<pin name="SCK" direction="in"/>
<pin name="TX0-" direction="in"/>
<pin name="TX0+" direction="in"/>
<pin name="TX1-" direction="in"/>
<pin name="TX1+" direction="in"/>
<pin name="TX2-" direction="in"/>
<pin name="TX2+" direction="in"/>
<pin name="TX3-" direction="in"/>
<pin name="TX3+" direction="in"/>
<pin name="TX4-" direction="in"/>
<pin name="TX4+" direction="in"/>
<pin name="SDA"/>
<pin name="~RESET" direction="in"/>
<pin name="SMB_CS" direction="in"/>
<pin name="DVB_ASI" direction="in"/>
<pin name="LF_CP" direction="in"/>
<pin name="LF_REF" direction="in"/>
<pin name="RSVD_H_2" direction="in"/>
<pin name="RSVD_H" direction="in"/>
<pin name="DNC_2" direction="nc"/>
<pin name="DNC" direction="nc"/>
<pin name="EP" direction="pas"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="~LOCK" direction="out"/>
<pin name="GPIO_0"/>
<pin name="GPIO_1"/>
<pin name="GPIO_2"/>
<pin name="TXOUT+" direction="out"/>
<pin name="TXOUT-" direction="out"/>
</symbol>
<symbol name="LMH0051SQ">
<pin name="VDD2V5_2" direction="pwr"/>
<pin name="VDD2V5_3" direction="pwr"/>
<pin name="VDD3V3_2" direction="pwr"/>
<pin name="VDD2V5" direction="pwr"/>
<pin name="VDD3V3_3" direction="pwr"/>
<pin name="VDD3V3_4" direction="pwr"/>
<pin name="VDDPLL" direction="pwr"/>
<pin name="VDD3V3" direction="pwr"/>
<pin name="RXIN0-" direction="in"/>
<pin name="RXIN0+" direction="in"/>
<pin name="RXIN1-" direction="in"/>
<pin name="RXIN1+" direction="in"/>
<pin name="RX0-" direction="in"/>
<pin name="RX0+" direction="in"/>
<pin name="RX1-" direction="in"/>
<pin name="RX1+" direction="in"/>
<pin name="RX2-" direction="in"/>
<pin name="RX2+" direction="in"/>
<pin name="RX3-" direction="in"/>
<pin name="RX3+" direction="in"/>
<pin name="RX4-" direction="in"/>
<pin name="RX4+" direction="in"/>
<pin name="RXCLK-" direction="in"/>
<pin name="RXCLK+" direction="in"/>
<pin name="RX_MUX_SEL" direction="in"/>
<pin name="SCK" direction="in"/>
<pin name="SDA"/>
<pin name="SMB_CS" direction="in"/>
<pin name="~RESET" direction="in"/>
<pin name="RSVD_H" direction="in"/>
<pin name="DVB_ASI" direction="in"/>
<pin name="RSET" direction="in"/>
<pin name="LF_REF" direction="pas"/>
<pin name="LF_CP" direction="pas"/>
<pin name="NC" direction="nc"/>
<pin name="DNC_2" direction="nc"/>
<pin name="DNC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="~LOCK" direction="out"/>
<pin name="GPIO_0"/>
<pin name="GPIO_1"/>
<pin name="GPIO_2"/>
</symbol>
<symbol name="LMH0070SQE">
<pin name="VDD2V5_2" direction="pwr"/>
<pin name="VDD2V5_3" direction="pwr"/>
<pin name="VDD2V5_4" direction="pwr"/>
<pin name="VDD3V3_2" direction="pwr"/>
<pin name="VDD2V5_5" direction="pwr"/>
<pin name="VDD2V5" direction="pwr"/>
<pin name="VDD3V3" direction="pwr"/>
<pin name="VDDPLL" direction="pwr"/>
<pin name="TXCLK-" direction="in"/>
<pin name="TXCLK+" direction="in"/>
<pin name="RSET" direction="in"/>
<pin name="SCK" direction="in"/>
<pin name="TX0-" direction="in"/>
<pin name="TX0+" direction="in"/>
<pin name="TX1-" direction="in"/>
<pin name="TX1+" direction="in"/>
<pin name="TX2-" direction="in"/>
<pin name="TX2+" direction="in"/>
<pin name="TX3-" direction="in"/>
<pin name="TX3+" direction="in"/>
<pin name="TX4-" direction="in"/>
<pin name="TX4+" direction="in"/>
<pin name="SDA"/>
<pin name="~RESET" direction="in"/>
<pin name="SMB_CS" direction="in"/>
<pin name="DVB_ASI" direction="in"/>
<pin name="LF_CP" direction="in"/>
<pin name="LF_REF" direction="in"/>
<pin name="RSVD_H_2" direction="in"/>
<pin name="RSVD_H" direction="in"/>
<pin name="DNC_2" direction="nc"/>
<pin name="DNC" direction="nc"/>
<pin name="EP" direction="pas"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="~LOCK" direction="out"/>
<pin name="GPIO_0"/>
<pin name="GPIO_1"/>
<pin name="GPIO_2"/>
<pin name="TXOUT+" direction="out"/>
<pin name="TXOUT-" direction="out"/>
</symbol>
<symbol name="LMH0071SQE">
<pin name="VDD2V5_2" direction="pwr"/>
<pin name="VDD2V5_3" direction="pwr"/>
<pin name="VDD2V5" direction="pwr"/>
<pin name="VDD3V3_2" direction="pwr"/>
<pin name="VDD3V3_3" direction="pwr"/>
<pin name="VDD3V3_4" direction="pwr"/>
<pin name="VDD3V3" direction="pwr"/>
<pin name="VDDPLL" direction="pwr"/>
<pin name="RXCLK-" direction="in"/>
<pin name="RXCLK+" direction="in"/>
<pin name="RSET" direction="in"/>
<pin name="SCK" direction="in"/>
<pin name="RXIN0+" direction="in"/>
<pin name="RXIN0-" direction="in"/>
<pin name="RXIN1-" direction="in"/>
<pin name="RXIN1+" direction="in"/>
<pin name="RX0-" direction="in"/>
<pin name="RX0+" direction="in"/>
<pin name="RX1-" direction="in"/>
<pin name="RX1+" direction="in"/>
<pin name="RX2-" direction="in"/>
<pin name="RX2+" direction="in"/>
<pin name="RX3-" direction="in"/>
<pin name="RX3+" direction="in"/>
<pin name="RX4-" direction="in"/>
<pin name="RX4+" direction="in"/>
<pin name="RX_MUX_SEL" direction="in"/>
<pin name="LOOPTHRU_EN" direction="in"/>
<pin name="SDA"/>
<pin name="SMB_CS" direction="in"/>
<pin name="~RESET" direction="in"/>
<pin name="DVB_ASI" direction="in"/>
<pin name="LF_CP" direction="in"/>
<pin name="LF_REF" direction="in"/>
<pin name="RSVD_H" direction="in"/>
<pin name="DNC" direction="nc"/>
<pin name="EP" direction="pas"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="TXOUT-" direction="out"/>
<pin name="TXOUT+" direction="out"/>
<pin name="~LOCK" direction="out"/>
<pin name="GPIO_0"/>
<pin name="GPIO_1"/>
<pin name="GPIO_2"/>
</symbol>
<symbol name="LMH0202MT">
<pin name="VCC1" direction="pwr"/>
<pin name="VCC2" direction="pwr"/>
<pin name="SD~/~HD1" direction="pas"/>
<pin name="SD~/~HD2" direction="pas"/>
<pin name="RREF1" direction="pas"/>
<pin name="RREF2" direction="pas"/>
<pin name="SDI1" direction="in"/>
<pin name="~SDI1" direction="in"/>
<pin name="SDI2" direction="in"/>
<pin name="~SDI2" direction="in"/>
<pin name="VEE1" direction="pwr"/>
<pin name="VEE2" direction="pwr"/>
<pin name="~SDO2" direction="out"/>
<pin name="SDO2" direction="out"/>
<pin name="~SDO1" direction="out"/>
<pin name="SDO1" direction="out"/>
</symbol>
<symbol name="LMH0302SQE">
<pin name="VCC" direction="pwr"/>
<pin name="EN" direction="in"/>
<pin name="SD/~HD" direction="in"/>
<pin name="SDI" direction="in"/>
<pin name="RREF" direction="pas"/>
<pin name="~SDI" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC_6" direction="nc"/>
<pin name="NC_7" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="VEE_2" direction="pas"/>
<pin name="VEE" direction="pwr"/>
<pin name="SDO" direction="out"/>
<pin name="~SDO" direction="out"/>
</symbol>
<symbol name="LMH0303SQE">
<pin name="VCC" direction="pwr"/>
<pin name="EN" direction="in"/>
<pin name="SD/~HD" direction="in"/>
<pin name="SDI" direction="in"/>
<pin name="RREF" direction="pas"/>
<pin name="~SDI" direction="in"/>
<pin name="SCL" direction="nc"/>
<pin name="SDA" direction="nc"/>
<pin name="~RSTI" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="VEE_2" direction="pas"/>
<pin name="VEE" direction="pwr"/>
<pin name="SDO" direction="out"/>
<pin name="~SDO" direction="out"/>
<pin name="~RSTO" direction="out"/>
<pin name="~FAULT" direction="out"/>
</symbol>
<symbol name="LMH0307GR">
<pin name="VCC" direction="pwr"/>
<pin name="EN" direction="in"/>
<pin name="SDI" direction="in"/>
<pin name="SCL" direction="in"/>
<pin name="RREF_2" direction="pas"/>
<pin name="RREF" direction="pas"/>
<pin name="~RSTI" direction="in"/>
<pin name="~SDI" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="VEE_2" direction="pwr"/>
<pin name="VEE_3" direction="pwr"/>
<pin name="VEE_4" direction="pwr"/>
<pin name="VEE_5" direction="pwr"/>
<pin name="VEE_6" direction="pwr"/>
<pin name="VEE" direction="pwr"/>
<pin name="~RSTO" direction="out"/>
<pin name="~FAULT" direction="out"/>
<pin name="SD/~HD" direction="out"/>
<pin name="SDO0" direction="out"/>
<pin name="~SDO0" direction="out"/>
<pin name="~SDO1" direction="out"/>
<pin name="SDO1" direction="out"/>
<pin name="SDA"/>
</symbol>
<symbol name="LMH0307SQE">
<pin name="VCC" direction="pwr"/>
<pin name="EN" direction="in"/>
<pin name="SD/~HD" direction="in"/>
<pin name="SDI" direction="in"/>
<pin name="RREF" direction="pas"/>
<pin name="~SDI" direction="in"/>
<pin name="SCL" direction="nc"/>
<pin name="SDA" direction="nc"/>
<pin name="~RSTI" direction="in"/>
<pin name="VEE_2" direction="pas"/>
<pin name="VEE" direction="pwr"/>
<pin name="SDO" direction="out"/>
<pin name="~SDO" direction="out"/>
<pin name="~SDO1" direction="out"/>
<pin name="SDO1" direction="out"/>
<pin name="~RSTO" direction="out"/>
<pin name="~FAULT" direction="out"/>
</symbol>
<symbol name="LMH0340SQE">
<pin name="VDD2V5_2" direction="pwr"/>
<pin name="VDD2V5_3" direction="pwr"/>
<pin name="VDD2V5_4" direction="pwr"/>
<pin name="VDD3V3_2" direction="pwr"/>
<pin name="VDD2V5_5" direction="pwr"/>
<pin name="VDD2V5" direction="pwr"/>
<pin name="VDD3V3" direction="pwr"/>
<pin name="VDDPLL" direction="pwr"/>
<pin name="TXCLK-" direction="in"/>
<pin name="TXCLK+" direction="in"/>
<pin name="RSET" direction="in"/>
<pin name="SCK" direction="in"/>
<pin name="TX0-" direction="in"/>
<pin name="TX0+" direction="in"/>
<pin name="TX1-" direction="in"/>
<pin name="TX1+" direction="in"/>
<pin name="TX2-" direction="in"/>
<pin name="TX2+" direction="in"/>
<pin name="TX3-" direction="in"/>
<pin name="TX3+" direction="in"/>
<pin name="TX4-" direction="in"/>
<pin name="TX4+" direction="in"/>
<pin name="SDA"/>
<pin name="~RESET" direction="in"/>
<pin name="SMB_CS" direction="in"/>
<pin name="DVB_ASI" direction="in"/>
<pin name="LF_CP" direction="in"/>
<pin name="LF_REF" direction="in"/>
<pin name="RSVD_H_2" direction="in"/>
<pin name="RSVD_H" direction="in"/>
<pin name="DNC_2" direction="nc"/>
<pin name="DNC" direction="nc"/>
<pin name="EP" direction="pas"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="~LOCK" direction="out"/>
<pin name="GPIO_0"/>
<pin name="GPIO_1"/>
<pin name="GPIO_2"/>
<pin name="TXOUT+" direction="out"/>
<pin name="TXOUT-" direction="out"/>
</symbol>
<symbol name="LMH0341SQE">
<pin name="VDD2V5_2" direction="pwr"/>
<pin name="VDD2V5_3" direction="pwr"/>
<pin name="VDD2V5" direction="pwr"/>
<pin name="VDD3V3_2" direction="pwr"/>
<pin name="VDD3V3_3" direction="pwr"/>
<pin name="VDD3V3_4" direction="pwr"/>
<pin name="VDD3V3" direction="pwr"/>
<pin name="VDDPLL" direction="pwr"/>
<pin name="RXCLK-" direction="in"/>
<pin name="RXCLK+" direction="in"/>
<pin name="RSET" direction="in"/>
<pin name="SCK" direction="in"/>
<pin name="RXIN0+" direction="in"/>
<pin name="RXIN0-" direction="in"/>
<pin name="RXIN1-" direction="in"/>
<pin name="RXIN1+" direction="in"/>
<pin name="RX0-" direction="in"/>
<pin name="RX0+" direction="in"/>
<pin name="RX1-" direction="in"/>
<pin name="RX1+" direction="in"/>
<pin name="RX2-" direction="in"/>
<pin name="RX2+" direction="in"/>
<pin name="RX3-" direction="in"/>
<pin name="RX3+" direction="in"/>
<pin name="RX4-" direction="in"/>
<pin name="RX4+" direction="in"/>
<pin name="RX_MUX_SEL" direction="in"/>
<pin name="LOOPTHRU_EN" direction="in"/>
<pin name="SDA"/>
<pin name="SMB_CS" direction="in"/>
<pin name="~RESET" direction="in"/>
<pin name="DVB_ASI" direction="in"/>
<pin name="LF_CP" direction="in"/>
<pin name="LF_REF" direction="in"/>
<pin name="RSVD_H" direction="in"/>
<pin name="DNC" direction="nc"/>
<pin name="EP" direction="pas"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="TXOUT-" direction="out"/>
<pin name="TXOUT+" direction="out"/>
<pin name="~LOCK" direction="out"/>
<pin name="GPIO_0"/>
<pin name="GPIO_1"/>
<pin name="GPIO_2"/>
</symbol>
<symbol name="LMH0344GR">
<pin name="VCC_2" direction="pwr"/>
<pin name="VCC_3" direction="pwr"/>
<pin name="VCC_4" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="~CD" direction="in"/>
<pin name="AEC+" direction="in"/>
<pin name="AEC-" direction="in"/>
<pin name="MUTEREF" direction="in"/>
<pin name="~SDI" direction="in"/>
<pin name="BYPASS" direction="in"/>
<pin name="SDI" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC_6" direction="nc"/>
<pin name="NC_7" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="VEE_2" direction="pwr"/>
<pin name="VEE_3" direction="pwr"/>
<pin name="VEE_4" direction="pwr"/>
<pin name="VEE" direction="pas"/>
<pin name="~SDO" direction="out"/>
<pin name="SDO" direction="out"/>
<pin name="MUTE" direction="out"/>
</symbol>
<symbol name="LMH0344SQ">
<pin name="VCC_2" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="SDI" direction="in"/>
<pin name="~SDI" direction="in"/>
<pin name="~CD" direction="pas"/>
<pin name="AEC+" direction="pas"/>
<pin name="AEC-" direction="pas"/>
<pin name="MUTEREF" direction="in"/>
<pin name="BYPASS" direction="in"/>
<pin name="VEE_2" direction="pwr"/>
<pin name="VEE_3" direction="pwr"/>
<pin name="VEE_4" direction="pwr"/>
<pin name="VEE" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="SDO" direction="out"/>
<pin name="~SDO" direction="out"/>
<pin name="MUTE" direction="out"/>
</symbol>
<symbol name="LMH0346MH">
<pin name="VCC" direction="pwr"/>
<pin name="VCCO_2" direction="pwr"/>
<pin name="VCCO" direction="pwr"/>
<pin name="SCO_EN" direction="in"/>
<pin name="RATE0" direction="in"/>
<pin name="RATE1" direction="in"/>
<pin name="~OP_MUTE" direction="in"/>
<pin name="BP/~AUTO-BP" direction="in"/>
<pin name="XTAL_IN/EXT_CLK" direction="in"/>
<pin name="LF1" direction="pas"/>
<pin name="LF2" direction="pas"/>
<pin name="SDI" direction="in"/>
<pin name="~SDI" direction="in"/>
<pin name="VEE" direction="pas"/>
<pin name="XTAL_OUT" direction="out"/>
<pin name="SD/~HD" direction="out"/>
<pin name="LOCK_DET" direction="out"/>
<pin name="SCO/SDO2" direction="out"/>
<pin name="~SCO/~SDO2" direction="out"/>
<pin name="SDO" direction="out"/>
<pin name="~SDO" direction="out"/>
</symbol>
<symbol name="LMH0356SQ">
<pin name="VCC_2" direction="pwr"/>
<pin name="VCC_3" direction="pwr"/>
<pin name="VCC_4" direction="pwr"/>
<pin name="VCC_5" direction="pwr"/>
<pin name="VCC_6" direction="pwr"/>
<pin name="VCC_7" direction="pwr"/>
<pin name="VCC_8" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="ENABLE" direction="in"/>
<pin name="SCO_EN" direction="in"/>
<pin name="XTALIN/EXTCLK" direction="in"/>
<pin name="SEL0" direction="in"/>
<pin name="SEL1" direction="in"/>
<pin name="BP/~AUTO-BP" direction="in"/>
<pin name="~O/PMUTE" direction="in"/>
<pin name="LOCKDET" direction="pas"/>
<pin name="RATE0" direction="in"/>
<pin name="RATE1" direction="in"/>
<pin name="LF1" direction="pas"/>
<pin name="LF2" direction="pas"/>
<pin name="SDI0" direction="in"/>
<pin name="~SDI0" direction="in"/>
<pin name="SDI1" direction="in"/>
<pin name="~SDI1" direction="in"/>
<pin name="SDI2" direction="in"/>
<pin name="~SDI2" direction="in"/>
<pin name="SDI3" direction="in"/>
<pin name="~SDI3" direction="in"/>
<pin name="EP" direction="pas"/>
<pin name="VEE_2" direction="pwr"/>
<pin name="VEE_3" direction="pwr"/>
<pin name="VEE_4" direction="pwr"/>
<pin name="VEE_5" direction="pwr"/>
<pin name="VEE_6" direction="pwr"/>
<pin name="VEE_7" direction="pwr"/>
<pin name="VEE_8" direction="pwr"/>
<pin name="VEE_9" direction="pwr"/>
<pin name="VEE_10" direction="pwr"/>
<pin name="VEE_11" direction="pwr"/>
<pin name="VEE_12" direction="pwr"/>
<pin name="VEE_13" direction="pwr"/>
<pin name="VEE_14" direction="pwr"/>
<pin name="VEE" direction="pwr"/>
<pin name="SD/~HD" direction="out"/>
<pin name="SCO/SDO2" direction="out"/>
<pin name="~SCO/~SDO2" direction="out"/>
<pin name="SDO" direction="out"/>
<pin name="~SDO" direction="out"/>
<pin name="XTALOUT" direction="out"/>
</symbol>
<symbol name="LMH1251MT">
<pin name="VCC_2" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="HSYNC_IN" direction="in"/>
<pin name="VSYNC_IN" direction="in"/>
<pin name="REXT" direction="in"/>
<pin name="RIN" direction="in"/>
<pin name="GIN" direction="in"/>
<pin name="BIN" direction="in"/>
<pin name="PR_IN" direction="in"/>
<pin name="PB_IN" direction="in"/>
<pin name="Y" direction="in"/>
<pin name="~Y" direction="in"/>
<pin name="PWR_SAV" direction="in"/>
<pin name="SD/HD_SEL" direction="in"/>
<pin name="AUTO/MANUAL_DETECT_SELECT" direction="in"/>
<pin name="IN_SEL" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VSYNC_OUT" direction="out"/>
<pin name="HSYNC_OUT" direction="out"/>
<pin name="BOUT" direction="out"/>
<pin name="GOUT" direction="out"/>
<pin name="ROUT" direction="out"/>
</symbol>
<symbol name="LMH1982SQ">
<pin name="VDD_2" direction="pwr"/>
<pin name="VDD_3" direction="pwr"/>
<pin name="VDD_4" direction="pwr"/>
<pin name="VDD_5" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="DVDD" direction="pwr"/>
<pin name="SCL" direction="in"/>
<pin name="VC_FREERUN" direction="in"/>
<pin name="HREF_A" direction="in"/>
<pin name="HREF_B" direction="in"/>
<pin name="VREF_A" direction="in"/>
<pin name="VREF_B" direction="in"/>
<pin name="REF_SEL" direction="in"/>
<pin name="VCXO" direction="in"/>
<pin name="~I2C_EN" direction="in"/>
<pin name="~GENLOCK" direction="in"/>
<pin name="~RESET" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="~HD_CLK" direction="out"/>
<pin name="HD_CLK" direction="out"/>
<pin name="~SD_CLK" direction="out"/>
<pin name="SD_CLK" direction="out"/>
<pin name="NO_LOCK" direction="out"/>
<pin name="NO_REF" direction="out"/>
<pin name="LPF" direction="out"/>
<pin name="SDA"/>
<pin name="TOF" direction="out"/>
</symbol>
<symbol name="LMH2180SD">
<pin name="VDD" direction="pwr"/>
<pin name="EN1" direction="in"/>
<pin name="EN2" direction="in"/>
<pin name="IN1" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="VSS" direction="pwr"/>
<pin name="EPAD" direction="pas"/>
<pin name="OUT1" direction="out"/>
<pin name="OUT2" direction="out"/>
</symbol>
<symbol name="LMH2180TM">
<pin name="VDD" direction="pwr"/>
<pin name="EN1" direction="in"/>
<pin name="EN2" direction="in"/>
<pin name="IN1" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="VSS" direction="pwr"/>
<pin name="OUT1" direction="out"/>
<pin name="OUT2" direction="out"/>
</symbol>
<symbol name="LMH2180YD">
<pin name="VDD" direction="pwr"/>
<pin name="IN1" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="EN1" direction="in"/>
<pin name="EN2" direction="in"/>
<pin name="VSS" direction="pwr"/>
<pin name="EPAD" direction="pas"/>
<pin name="OUT2" direction="out"/>
<pin name="OUT1" direction="out"/>
</symbol>
<symbol name="LMH2190TM-38">
<pin name="VBAT" direction="in"/>
<pin name="SCL" direction="in"/>
<pin name="SCLK_IN" direction="in"/>
<pin name="ENABLE" direction="in"/>
<pin name="CLK1" direction="in"/>
<pin name="CLK2" direction="in"/>
<pin name="CLK3" direction="in"/>
<pin name="CLK4" direction="in"/>
<pin name="SCLK_REQ" direction="in"/>
<pin name="CLK_REQ1" direction="in"/>
<pin name="CLK_REQ2" direction="in"/>
<pin name="CLK_REQ3" direction="in"/>
<pin name="CLK_REQ4" direction="in"/>
<pin name="VSS" direction="pwr"/>
<pin name="VOUT" direction="out"/>
<pin name="SDA"/>
</symbol>
<symbol name="LMH6321MR">
<pin name="V+" direction="pwr"/>
<pin name="EF" direction="in"/>
<pin name="CL" direction="in"/>
<pin name="VIN" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="V-" direction="pwr"/>
<pin name="GND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LMH6321TS">
<pin name="V+" direction="pwr"/>
<pin name="VIN" direction="in"/>
<pin name="EF" direction="in"/>
<pin name="CL" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="V-" direction="pwr"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LMH6502MA">
<pin name="V+_2" direction="pwr"/>
<pin name="V+" direction="pwr"/>
<pin name="+VIN" direction="in"/>
<pin name="-VIN" direction="in"/>
<pin name="I-" direction="in"/>
<pin name="VG" direction="in"/>
<pin name="VREF" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="V-_2" direction="pwr"/>
<pin name="V-" direction="pwr"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
<pin name="+RG" direction="out"/>
<pin name="-RG" direction="out"/>
</symbol>
<symbol name="LMH6503MA">
<pin name="V+_2" direction="pwr"/>
<pin name="V+" direction="pwr"/>
<pin name="+VIN" direction="in"/>
<pin name="-VIN" direction="in"/>
<pin name="I-" direction="in"/>
<pin name="VG" direction="in"/>
<pin name="VREF" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="V-_2" direction="pwr"/>
<pin name="V-" direction="pwr"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
<pin name="+RG" direction="out"/>
<pin name="-RG" direction="out"/>
</symbol>
<symbol name="LMH6503MT">
<pin name="V+_2" direction="pwr"/>
<pin name="V+" direction="pwr"/>
<pin name="+VIN" direction="in"/>
<pin name="-VIN" direction="in"/>
<pin name="I-" direction="in"/>
<pin name="VG" direction="in"/>
<pin name="VREF" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="V-_2" direction="pwr"/>
<pin name="V-" direction="pwr"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
<pin name="+RG" direction="out"/>
<pin name="-RG" direction="out"/>
</symbol>
<symbol name="LMH6505MA">
<pin name="V+" direction="pwr"/>
<pin name="I-" direction="in"/>
<pin name="VG" direction="in"/>
<pin name="VIN" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
<pin name="RG" direction="out"/>
</symbol>
<symbol name="LMH6505MM">
<pin name="V+" direction="pwr"/>
<pin name="VIN" direction="in"/>
<pin name="VG" direction="pwr"/>
<pin name="RG" direction="pas"/>
<pin name="I-" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LMH6514SQE">
<pin name="V+" direction="pwr"/>
<pin name="LOAD+" direction="pas"/>
<pin name="LOAD-" direction="pas"/>
<pin name="IN-" direction="in"/>
<pin name="IN+" direction="in"/>
<pin name="GAIN0" direction="in"/>
<pin name="GAIN1" direction="in"/>
<pin name="GAIN2" direction="in"/>
<pin name="LATCH" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="OUT+" direction="out"/>
<pin name="OUT-" direction="out"/>
</symbol>
<symbol name="LMH6518SQ">
<pin name="VCC_2" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="~CS" direction="in"/>
<pin name="SCLK" direction="in"/>
<pin name="VCM" direction="in"/>
<pin name="VCM_AUX" direction="in"/>
<pin name="IN-" direction="in"/>
<pin name="IN+" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="OUT_AUX+" direction="out"/>
<pin name="OUT_AUX-" direction="out"/>
<pin name="OUT+" direction="out"/>
<pin name="OUT-" direction="out"/>
<pin name="SDIO"/>
<pin name="VDD" direction="pwr"/>
</symbol>
<symbol name="LMH6550MA">
<pin name="V+" direction="pwr"/>
<pin name="+IN" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="VCM" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="+OUT" direction="out"/>
<pin name="-OUT" direction="out"/>
</symbol>
<symbol name="LMH6551MA">
<pin name="V+" direction="pwr"/>
<pin name="+IN" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="VCM" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="V-" direction="pwr"/>
<pin name="+OUT" direction="out"/>
<pin name="-OUT" direction="out"/>
</symbol>
<symbol name="LMH6551MM">
<pin name="V+" direction="pwr"/>
<pin name="+IN" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="VCM" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="V-" direction="pwr"/>
<pin name="+OUT" direction="out"/>
<pin name="-OUT" direction="out"/>
</symbol>
<symbol name="LMH6552SD">
<pin name="V+" direction="pwr"/>
<pin name="EN" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="VCM" direction="in"/>
<pin name="EP" direction="pas"/>
<pin name="V-" direction="pwr"/>
<pin name="+OUT" direction="out"/>
<pin name="-OUT" direction="out"/>
</symbol>
<symbol name="LMH6553MR_1">
<pin name="IN-" direction="in"/>
<pin name="VCM" direction="in"/>
<pin name="V+" direction="pwr"/>
<pin name="OUT+" direction="out"/>
<pin name="OUT-" direction="out"/>
<pin name="V-" direction="pwr"/>
<pin name="VCLAMP" direction="pas"/>
<pin name="IN+" direction="in"/>
</symbol>
<symbol name="LMH6553MR_2">
<pin name="DAP" direction="pas"/>
</symbol>
<symbol name="LMH6553SD">
<pin name="V+" direction="pwr"/>
<pin name="+IN" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="DAP" direction="pas"/>
<pin name="V-" direction="pwr"/>
<pin name="VCM" direction="out"/>
<pin name="VCLAMP" direction="out"/>
<pin name="+OUT" direction="out"/>
<pin name="-OUT" direction="out"/>
</symbol>
<symbol name="LMH6554LEE">
<pin name="V+_2" direction="pwr"/>
<pin name="V+" direction="pwr"/>
<pin name="VEN" direction="in"/>
<pin name="IN-" direction="in"/>
<pin name="IN+" direction="in"/>
<pin name="V-_2" direction="pwr"/>
<pin name="V-" direction="pwr"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="OUT+" direction="out"/>
<pin name="OUT-" direction="out"/>
<pin name="FB+" direction="out"/>
<pin name="VCM" direction="out"/>
<pin name="FB-" direction="out"/>
</symbol>
<symbol name="LMH6555SQ">
<pin name="VCC_2" direction="pwr"/>
<pin name="VCC_3" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="VIN+" direction="pwr"/>
<pin name="VIN-" direction="pwr"/>
<pin name="VCM_REF" direction="pas"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="DAP" direction="pas"/>
<pin name="VOUT+" direction="out"/>
<pin name="VOUT-" direction="out"/>
</symbol>
<symbol name="LMH6559MA">
<pin name="V+" direction="pwr"/>
<pin name="IN" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="VEE" direction="pwr"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LMH6559MF">
<pin name="IN" direction="in"/>
<pin name="V+" direction="pas"/>
<pin name="V-" direction="pas"/>
<pin name="NC" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LMH6570MA">
<pin name="V+" direction="pwr"/>
<pin name="IN0" direction="in"/>
<pin name="IN1" direction="in"/>
<pin name="SEL" direction="in"/>
<pin name="SD" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LMH6572MQ">
<pin name="R0" direction="in"/>
<pin name="G0" direction="in"/>
<pin name="B0" direction="in"/>
<pin name="R1" direction="in"/>
<pin name="G1" direction="in"/>
<pin name="B1" direction="in"/>
<pin name="V+" direction="pas"/>
<pin name="V-_2" direction="pas"/>
<pin name="V-" direction="pas"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="OUTB" direction="out"/>
<pin name="OUTG" direction="out"/>
<pin name="OUTR" direction="out"/>
<pin name="~EN" direction="pas"/>
<pin name="SEL" direction="pas"/>
</symbol>
<symbol name="LMH6574MA">
<pin name="V+" direction="pwr"/>
<pin name="IN0" direction="in"/>
<pin name="IN1" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="IN3" direction="in"/>
<pin name="~EN" direction="in"/>
<pin name="SD" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LMH6583YA">
<pin name="VCC_2" direction="pwr"/>
<pin name="VCC_3" direction="pwr"/>
<pin name="VCC_4" direction="pwr"/>
<pin name="VCC_5" direction="pwr"/>
<pin name="VCC_6" direction="pwr"/>
<pin name="VCC_7" direction="pwr"/>
<pin name="VCC_8" direction="pwr"/>
<pin name="VCC_9" direction="pwr"/>
<pin name="VCC_10" direction="pwr"/>
<pin name="VCC_11" direction="pwr"/>
<pin name="VCC_12" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="CLK" direction="in"/>
<pin name="CFG" direction="in"/>
<pin name="RST" direction="in"/>
<pin name="MODE" direction="in"/>
<pin name="BCST" direction="in"/>
<pin name="~CS" direction="in"/>
<pin name="DIN" direction="in"/>
<pin name="IN0" direction="in"/>
<pin name="IN1" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="IN3" direction="in"/>
<pin name="IN4" direction="in"/>
<pin name="IN5" direction="in"/>
<pin name="IN6" direction="in"/>
<pin name="IN7" direction="in"/>
<pin name="IN8" direction="in"/>
<pin name="IN9" direction="in"/>
<pin name="IN10" direction="in"/>
<pin name="IN11" direction="in"/>
<pin name="IN12" direction="in"/>
<pin name="IN13" direction="in"/>
<pin name="IN14" direction="in"/>
<pin name="IN15" direction="in"/>
<pin name="VEE_2" direction="pwr"/>
<pin name="VEE_3" direction="pwr"/>
<pin name="VEE_4" direction="pwr"/>
<pin name="VEE_5" direction="pwr"/>
<pin name="VEE_6" direction="pwr"/>
<pin name="VEE_7" direction="pwr"/>
<pin name="VEE_8" direction="pwr"/>
<pin name="VEE_9" direction="pwr"/>
<pin name="VEE_10" direction="pwr"/>
<pin name="VEE_11" direction="pwr"/>
<pin name="VEE_12" direction="pwr"/>
<pin name="VEE" direction="pwr"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pwr"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="OUT0" direction="out"/>
<pin name="OUT1" direction="out"/>
<pin name="OUT2" direction="out"/>
<pin name="OUT3" direction="out"/>
<pin name="OUT4" direction="out"/>
<pin name="OUT5" direction="out"/>
<pin name="OUT6" direction="out"/>
<pin name="OUT7" direction="out"/>
<pin name="DOUT" direction="out"/>
</symbol>
<symbol name="LMH6601MG">
<pin name="V+" direction="pwr"/>
<pin name="~SD" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LMH6601QMG">
<pin name="-IN" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="*SD" direction="in"/>
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pas"/>
<pin name="OUTPUT" direction="out"/>
</symbol>
<symbol name="LMH6609MA">
<pin name="V+" direction="pwr"/>
<pin name="-IN" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="NC_2" direction="in"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LMH6609MF">
<pin name="V+" direction="pwr"/>
<pin name="+IN" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LMH6611MK">
<pin name="V+" direction="pwr"/>
<pin name="IN+" direction="in"/>
<pin name="IN-" direction="in"/>
<pin name="~DIS" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LMH6612MA">
<pin name="V+" direction="pwr"/>
<pin name="-INB" direction="in"/>
<pin name="+INB" direction="in"/>
<pin name="+INA" direction="in"/>
<pin name="-INA" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT_A" direction="out"/>
<pin name="OUT_B" direction="out"/>
</symbol>
<symbol name="LMH6618MK">
<pin name="V+" direction="pwr"/>
<pin name="IN+" direction="in"/>
<pin name="IN-" direction="in"/>
<pin name="~DIS" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LMH6619MA">
<pin name="V+" direction="pwr"/>
<pin name="-INB" direction="in"/>
<pin name="+INB" direction="in"/>
<pin name="+INA" direction="in"/>
<pin name="-INA" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT_A" direction="out"/>
<pin name="OUT_B" direction="out"/>
</symbol>
<symbol name="LMH6622MA">
<pin name="V+" direction="pwr"/>
<pin name="+INA" direction="in"/>
<pin name="-INA" direction="in"/>
<pin name="+INB" direction="in"/>
<pin name="-INB" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="LMH6622MM">
<pin name="V+" direction="pwr"/>
<pin name="IN_A-" direction="in"/>
<pin name="IN_A+" direction="in"/>
<pin name="IN_B+" direction="in"/>
<pin name="IN_B-" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT_A" direction="out"/>
<pin name="OUT_B" direction="out"/>
</symbol>
<symbol name="LMH6624MA">
<pin name="V+" direction="pwr"/>
<pin name="-INA" direction="in"/>
<pin name="+INA" direction="in"/>
<pin name="-INB" direction="in"/>
<pin name="+INB" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="LMH6624MF">
<pin name="V+" direction="pwr"/>
<pin name="+IN" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LMH6626MA">
<pin name="V+" direction="pwr"/>
<pin name="-INA" direction="in"/>
<pin name="+INA" direction="in"/>
<pin name="-INB" direction="in"/>
<pin name="+INB" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="LMH6626MM">
<pin name="V+" direction="pwr"/>
<pin name="INA+" direction="in"/>
<pin name="INA-" direction="in"/>
<pin name="INB-" direction="in"/>
<pin name="INB+" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="LMH6628MA">
<pin name="+VCC" direction="pwr"/>
<pin name="VIN1" direction="in"/>
<pin name="VIN2" direction="in"/>
<pin name="VNON-INV1" direction="in"/>
<pin name="VNON-INV2" direction="in"/>
<pin name="-VCC" direction="pwr"/>
<pin name="VOUT1" direction="out"/>
<pin name="VOUT2" direction="out"/>
</symbol>
<symbol name="LMH6639MA">
<pin name="V+" direction="pwr"/>
<pin name="~SD" direction="in"/>
<pin name="IN-" direction="in"/>
<pin name="IN+" direction="in"/>
<pin name="N/C_2" direction="nc"/>
<pin name="N/C" direction="nc"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTPUT" direction="out"/>
</symbol>
<symbol name="LMH6639MF">
<pin name="V+" direction="pwr"/>
<pin name="~SD" direction="pas"/>
<pin name="+IN" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LMH6640MF">
<pin name="V+" direction="pwr"/>
<pin name="+IN" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LMH6642MA">
<pin name="V+" direction="pwr"/>
<pin name="IN-" direction="in"/>
<pin name="IN+" direction="in"/>
<pin name="N/C_2" direction="nc"/>
<pin name="N/C_3" direction="nc"/>
<pin name="N/C" direction="nc"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LMH6642MF">
<pin name="V+" direction="pwr"/>
<pin name="IN+" direction="in"/>
<pin name="IN-" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LMH6643MA">
<pin name="V+" direction="pwr"/>
<pin name="-INA" direction="in"/>
<pin name="-INB" direction="in"/>
<pin name="+INA" direction="in"/>
<pin name="+INB" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="LMH6643MM">
<pin name="V+" direction="pwr"/>
<pin name="IN_A-" direction="in"/>
<pin name="IN_A+" direction="in"/>
<pin name="IN_B+" direction="in"/>
<pin name="IN_B-" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT_A" direction="out"/>
<pin name="OUT_B" direction="out"/>
</symbol>
<symbol name="LMH6644MA">
<pin name="V+" direction="pwr"/>
<pin name="-INA" direction="in"/>
<pin name="+INA" direction="in"/>
<pin name="+INB" direction="in"/>
<pin name="-INB" direction="in"/>
<pin name="-INC" direction="in"/>
<pin name="+INC" direction="in"/>
<pin name="+IND" direction="in"/>
<pin name="-IND" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
<pin name="OUTC" direction="out"/>
<pin name="OUTD" direction="out"/>
</symbol>
<symbol name="LMH6644MT">
<pin name="V+" direction="pwr"/>
<pin name="-INA" direction="in"/>
<pin name="+INA" direction="in"/>
<pin name="+INB" direction="in"/>
<pin name="-INB" direction="in"/>
<pin name="-INC" direction="in"/>
<pin name="+INC" direction="in"/>
<pin name="+IND" direction="in"/>
<pin name="-IND" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
<pin name="OUTC" direction="out"/>
<pin name="OUTD" direction="out"/>
</symbol>
<symbol name="LMH6645MA">
<pin name="V+" direction="pwr"/>
<pin name="-IN" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LMH6645MF">
<pin name="V+" direction="pwr"/>
<pin name="+IN" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LMH6646MA">
<pin name="V+" direction="pwr"/>
<pin name="+INA" direction="in"/>
<pin name="-INA" direction="in"/>
<pin name="+INB" direction="in"/>
<pin name="-INB" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="LMH6646MM">
<pin name="V+" direction="pwr"/>
<pin name="INA+" direction="in"/>
<pin name="INA-" direction="in"/>
<pin name="INB-" direction="in"/>
<pin name="INB+" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="LMH6647MA">
<pin name="V+" direction="pwr"/>
<pin name="SD" direction="pas"/>
<pin name="+IN" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LMH6647MF">
<pin name="V-" direction="pwr"/>
<pin name="~SD" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="V+" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LMH6654MA">
<pin name="V+" direction="pwr"/>
<pin name="-IN" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LMH6654MF">
<pin name="V+" direction="pwr"/>
<pin name="+IN" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LMH6655MA">
<pin name="V+" direction="pwr"/>
<pin name="+INA" direction="in"/>
<pin name="-INA" direction="in"/>
<pin name="-INB" direction="in"/>
<pin name="+INB" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="LMH6655MM">
<pin name="V+" direction="pwr"/>
<pin name="IN_A-" direction="in"/>
<pin name="IN_A+" direction="in"/>
<pin name="IN_B+" direction="in"/>
<pin name="IN_B-" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT_A" direction="out"/>
<pin name="OUT_B" direction="out"/>
</symbol>
<symbol name="LMH6657MF">
<pin name="V+" direction="pwr"/>
<pin name="IN+" direction="in"/>
<pin name="IN-" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LMH6657MG">
<pin name="V+" direction="pwr"/>
<pin name="+IN" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LMH6658MA">
<pin name="V+" direction="pwr"/>
<pin name="-INA" direction="in"/>
<pin name="+INA" direction="in"/>
<pin name="-INB" direction="in"/>
<pin name="+INB" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="LMH6658MM">
<pin name="V+" direction="pwr"/>
<pin name="INA+" direction="in"/>
<pin name="INA-" direction="in"/>
<pin name="INB+" direction="in"/>
<pin name="INB-" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="LMH6672MA">
<pin name="V+" direction="pwr"/>
<pin name="-INA" direction="in"/>
<pin name="+INA" direction="in"/>
<pin name="-INB" direction="in"/>
<pin name="+INB" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="LMH6672MR">
<pin name="V+" direction="pwr"/>
<pin name="-INA" direction="in"/>
<pin name="+INA" direction="in"/>
<pin name="+INB" direction="in"/>
<pin name="-INB" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="EPAD" direction="pas"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="LMH6682MA">
<pin name="V+" direction="pwr"/>
<pin name="+INA" direction="in"/>
<pin name="-INA" direction="in"/>
<pin name="+INB" direction="in"/>
<pin name="-INB" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT_A" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="LMH6682MM">
<pin name="V+" direction="pwr"/>
<pin name="INA+" direction="in"/>
<pin name="INA-" direction="in"/>
<pin name="INB-" direction="in"/>
<pin name="INB+" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="LMH6683MA">
<pin name="V+" direction="pwr"/>
<pin name="+IN1" direction="in"/>
<pin name="-IN1" direction="in"/>
<pin name="+IN2" direction="in"/>
<pin name="-IN2" direction="in"/>
<pin name="+IN3" direction="in"/>
<pin name="-IN3" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT1" direction="out"/>
<pin name="OUT2" direction="out"/>
<pin name="OUT3" direction="out"/>
</symbol>
<symbol name="LMH6702JFQMLV">
<pin name="+VCC" direction="pwr"/>
<pin name="VNON-INV" direction="in"/>
<pin name="VINV" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="-VCC" direction="pwr"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LMH6702MA">
<pin name="V+" direction="pwr"/>
<pin name="IN-" direction="in"/>
<pin name="IN+" direction="in"/>
<pin name="N/C_2" direction="nc"/>
<pin name="N/C_3" direction="nc"/>
<pin name="N/C" direction="nc"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LMH6702MF">
<pin name="V+" direction="pwr"/>
<pin name="+IN" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LMH6703MA">
<pin name="VS+" direction="pwr"/>
<pin name="~SD" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="N/C_2" direction="nc"/>
<pin name="N/C" direction="nc"/>
<pin name="VS-" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LMH6703MF">
<pin name="V-" direction="pwr"/>
<pin name="~SD" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="V+" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LMH6704MA">
<pin name="VS+" direction="pwr"/>
<pin name="~DIS" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="N/C_2" direction="nc"/>
<pin name="N/C" direction="nc"/>
<pin name="VS-" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LMH6714MA">
<pin name="V+" direction="pwr"/>
<pin name="+IN" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LMH6714MF">
<pin name="V+" direction="pwr"/>
<pin name="IN+" direction="in"/>
<pin name="IN-" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LMH6715MA">
<pin name="+VCC" direction="pwr"/>
<pin name="VIN1" direction="in"/>
<pin name="VIN2" direction="in"/>
<pin name="VNON-INV1" direction="in"/>
<pin name="VNON-INV2" direction="in"/>
<pin name="-VCC" direction="pwr"/>
<pin name="VOUT1" direction="out"/>
<pin name="VOUT2" direction="out"/>
</symbol>
<symbol name="LMH6720MA">
<pin name="V+" direction="pwr"/>
<pin name="~SD" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LMH6720MF">
<pin name="V+" direction="pwr"/>
<pin name="+IN" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="~SD" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LMH6722MA">
<pin name="V+" direction="pwr"/>
<pin name="-INA" direction="in"/>
<pin name="+INA" direction="in"/>
<pin name="+INB" direction="in"/>
<pin name="-INB" direction="in"/>
<pin name="-INC" direction="in"/>
<pin name="+INC" direction="in"/>
<pin name="+IND" direction="in"/>
<pin name="-IND" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
<pin name="OUTC" direction="out"/>
<pin name="OUTD" direction="out"/>
</symbol>
<symbol name="LMH6722QSD">
<pin name="V+" direction="pwr"/>
<pin name="-INA" direction="in"/>
<pin name="+INA" direction="in"/>
<pin name="+INB" direction="in"/>
<pin name="-INB" direction="in"/>
<pin name="-INC" direction="in"/>
<pin name="+INC" direction="in"/>
<pin name="+IND" direction="in"/>
<pin name="-IND" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="THER_PAD" direction="pas"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
<pin name="OUTC" direction="out"/>
<pin name="OUTD" direction="out"/>
</symbol>
<symbol name="LMH6722SD">
<pin name="V+" direction="pwr"/>
<pin name="-INA" direction="in"/>
<pin name="+INA" direction="in"/>
<pin name="+INB" direction="in"/>
<pin name="-INB" direction="in"/>
<pin name="-INC" direction="in"/>
<pin name="+INC" direction="in"/>
<pin name="+IND" direction="in"/>
<pin name="-IND" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="THER_PAD" direction="pas"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
<pin name="OUTC" direction="out"/>
<pin name="OUTD" direction="out"/>
</symbol>
<symbol name="LMH6723MA">
<pin name="V+" direction="pwr"/>
<pin name="-IN" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LMH6723MF">
<pin name="V+" direction="pwr"/>
<pin name="IN+" direction="in"/>
<pin name="IN-" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LMH6724MA">
<pin name="V+" direction="pwr"/>
<pin name="-INA" direction="in"/>
<pin name="+INA" direction="in"/>
<pin name="+INB" direction="in"/>
<pin name="-INB" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="LMH6732MF">
<pin name="V+" direction="pwr"/>
<pin name="+IN" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="RP" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LMH6733MQ">
<pin name="VS+_2" direction="pwr"/>
<pin name="VS+" direction="pwr"/>
<pin name="~DIS_A" direction="in"/>
<pin name="~DIS_B" direction="in"/>
<pin name="~DIS_C" direction="in"/>
<pin name="-INA" direction="in"/>
<pin name="+INA" direction="in"/>
<pin name="-INB" direction="in"/>
<pin name="+INB" direction="in"/>
<pin name="-INC" direction="in"/>
<pin name="+INC" direction="in"/>
<pin name="VS-_2" direction="pwr"/>
<pin name="VS-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
<pin name="OUTC" direction="out"/>
</symbol>
<symbol name="LMH6738MQ">
<pin name="VS+_2" direction="pwr"/>
<pin name="VS+" direction="pwr"/>
<pin name="-INA" direction="in"/>
<pin name="+INA" direction="in"/>
<pin name="+INB" direction="in"/>
<pin name="-INB" direction="in"/>
<pin name="-INC" direction="in"/>
<pin name="+INC" direction="in"/>
<pin name="~DIS_A" direction="in"/>
<pin name="~DIS_B" direction="in"/>
<pin name="~DIS_C" direction="in"/>
<pin name="VS-_2" direction="pwr"/>
<pin name="VS-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
<pin name="OUTC" direction="out"/>
</symbol>
<symbol name="LMH6739MQ">
<pin name="VS+_2" direction="pwr"/>
<pin name="VS+" direction="pwr"/>
<pin name="~DISA" direction="in"/>
<pin name="~DISB" direction="in"/>
<pin name="~DISC" direction="in"/>
<pin name="-INA" direction="in"/>
<pin name="+INA" direction="in"/>
<pin name="-INB" direction="in"/>
<pin name="+INB" direction="in"/>
<pin name="-INC" direction="in"/>
<pin name="+INC" direction="in"/>
<pin name="VS-_2" direction="in"/>
<pin name="VS-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
<pin name="OUTC" direction="out"/>
</symbol>
<symbol name="LMH7220MG">
<pin name="VCC" direction="pwr"/>
<pin name="IN-" direction="in"/>
<pin name="IN+" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT_~Q" direction="out"/>
<pin name="OUT_Q" direction="out"/>
</symbol>
<symbol name="LMH7220MK">
<pin name="V-" direction="pwr"/>
<pin name="-IN" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="VCC" direction="pwr"/>
<pin name="OUT_~Q" direction="out"/>
<pin name="OUT_Q" direction="out"/>
</symbol>
<symbol name="LMH7322SQ">
<pin name="VCCO" direction="pwr"/>
<pin name="VCCIA" direction="pwr"/>
<pin name="VCCIB" direction="pwr"/>
<pin name="VCCOA" direction="pwr"/>
<pin name="VCCOB_2" direction="pwr"/>
<pin name="VCCOB" direction="pwr"/>
<pin name="RFREFA" direction="in"/>
<pin name="RFREFB" direction="in"/>
<pin name="RHYSA" direction="in"/>
<pin name="RHYSB" direction="in"/>
<pin name="-INA" direction="in"/>
<pin name="+INA" direction="in"/>
<pin name="+INB" direction="in"/>
<pin name="-INB" direction="in"/>
<pin name="LEA" direction="in"/>
<pin name="~LEA" direction="in"/>
<pin name="~LEB" direction="in"/>
<pin name="LEB" direction="in"/>
<pin name="VEEA" direction="pwr"/>
<pin name="VEEB" direction="pwr"/>
<pin name="EPAD" direction="pas"/>
<pin name="QA" direction="out"/>
<pin name="~QA" direction="out"/>
<pin name="~QB" direction="out"/>
<pin name="QB" direction="out"/>
</symbol>
<symbol name="LMH7324SQ">
<pin name="VCCIA" direction="pwr"/>
<pin name="VCCIB" direction="pwr"/>
<pin name="VCCIC" direction="pwr"/>
<pin name="VCCOA" direction="pwr"/>
<pin name="VCCID" direction="pwr"/>
<pin name="VCCOB" direction="pwr"/>
<pin name="VCCOC" direction="pwr"/>
<pin name="VCCOD" direction="pwr"/>
<pin name="INA+" direction="in"/>
<pin name="INA-" direction="in"/>
<pin name="INB-" direction="in"/>
<pin name="INB+" direction="in"/>
<pin name="INC+" direction="in"/>
<pin name="INC-" direction="in"/>
<pin name="IND+" direction="in"/>
<pin name="IND-" direction="in"/>
<pin name="VEEA_2" direction="pwr"/>
<pin name="VEEB_2" direction="pwr"/>
<pin name="VEEB" direction="pwr"/>
<pin name="VEEC_2" direction="pwr"/>
<pin name="VEEC" direction="pwr"/>
<pin name="VEED_2" direction="pwr"/>
<pin name="VEED" direction="pwr"/>
<pin name="VEEA" direction="pwr"/>
<pin name="DAP" direction="pas"/>
<pin name="~QA" direction="out"/>
<pin name="~QB" direction="out"/>
<pin name="~QC" direction="out"/>
<pin name="~QD" direction="out"/>
<pin name="QA" direction="out"/>
<pin name="QB" direction="out"/>
<pin name="QC" direction="out"/>
<pin name="QD" direction="out"/>
</symbol>
<symbol name="LMK01000ISQ">
<pin name="VCC1" direction="pwr"/>
<pin name="VCC2" direction="pwr"/>
<pin name="VCC3" direction="pwr"/>
<pin name="VCC4" direction="pwr"/>
<pin name="VCC5" direction="pwr"/>
<pin name="VCC6" direction="pwr"/>
<pin name="VCC7" direction="pwr"/>
<pin name="VCC8" direction="pwr"/>
<pin name="VCC9" direction="pwr"/>
<pin name="VCC10" direction="pwr"/>
<pin name="VCC11" direction="pwr"/>
<pin name="VCC12" direction="pwr"/>
<pin name="VCC13" direction="pwr"/>
<pin name="VCC14" direction="pwr"/>
<pin name="CLKIN0" direction="in"/>
<pin name="~CLKIN0" direction="in"/>
<pin name="CLKIN1" direction="in"/>
<pin name="~CLKIN1" direction="in"/>
<pin name="CLKUWIRE" direction="in"/>
<pin name="DATAUWIRE" direction="in"/>
<pin name="LEUWIRE" direction="in"/>
<pin name="GOE" direction="in"/>
<pin name="~SYNC" direction="in"/>
<pin name="BIAS" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pwr"/>
<pin name="EPAD" direction="pas"/>
<pin name="CLKOUT0" direction="out"/>
<pin name="~CLKOUT0" direction="out"/>
<pin name="CLKOUT1" direction="out"/>
<pin name="~CLKOUT1" direction="out"/>
<pin name="CLKOUT2" direction="out"/>
<pin name="~CLKOUT2" direction="out"/>
<pin name="CLKOUT3" direction="out"/>
<pin name="~CLKOUT3" direction="out"/>
<pin name="CLKOUT4" direction="out"/>
<pin name="~CLKOUT4" direction="out"/>
<pin name="CLKOUT5" direction="out"/>
<pin name="~CLKOUT5" direction="out"/>
<pin name="CLKOUT6" direction="out"/>
<pin name="~CLKOUT6" direction="out"/>
<pin name="CLKOUT7" direction="out"/>
<pin name="~CLKOUT7" direction="out"/>
<pin name="TEST" direction="out"/>
</symbol>
<symbol name="LMK01010ISQ">
<pin name="VCC1" direction="pwr"/>
<pin name="VCC2" direction="pwr"/>
<pin name="VCC3" direction="pwr"/>
<pin name="VCC4" direction="pwr"/>
<pin name="VCC5" direction="pwr"/>
<pin name="VCC6" direction="pwr"/>
<pin name="VCC7" direction="pwr"/>
<pin name="VCC8" direction="pwr"/>
<pin name="VCC9" direction="pwr"/>
<pin name="VCC10" direction="pwr"/>
<pin name="VCC11" direction="pwr"/>
<pin name="VCC12" direction="pwr"/>
<pin name="VCC13" direction="pwr"/>
<pin name="VCC14" direction="pwr"/>
<pin name="CLKIN0" direction="in"/>
<pin name="~CLKIN0" direction="in"/>
<pin name="CLKIN1" direction="in"/>
<pin name="~CLKIN1" direction="in"/>
<pin name="CLKUWIRE" direction="in"/>
<pin name="DATAUWIRE" direction="in"/>
<pin name="LEUWIRE" direction="in"/>
<pin name="GOE" direction="in"/>
<pin name="~SYNC" direction="in"/>
<pin name="BIAS" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pwr"/>
<pin name="EPAD" direction="pas"/>
<pin name="CLKOUT0" direction="out"/>
<pin name="~CLKOUT0" direction="out"/>
<pin name="CLKOUT1" direction="out"/>
<pin name="~CLKOUT1" direction="out"/>
<pin name="CLKOUT2" direction="out"/>
<pin name="~CLKOUT2" direction="out"/>
<pin name="CLKOUT3" direction="out"/>
<pin name="~CLKOUT3" direction="out"/>
<pin name="CLKOUT4" direction="out"/>
<pin name="~CLKOUT4" direction="out"/>
<pin name="CLKOUT5" direction="out"/>
<pin name="~CLKOUT5" direction="out"/>
<pin name="CLKOUT6" direction="out"/>
<pin name="~CLKOUT6" direction="out"/>
<pin name="CLKOUT7" direction="out"/>
<pin name="~CLKOUT7" direction="out"/>
<pin name="TEST" direction="out"/>
</symbol>
<symbol name="LMK02000ISQ">
<pin name="VCC1" direction="pwr"/>
<pin name="VCC2" direction="pwr"/>
<pin name="VCC3" direction="pwr"/>
<pin name="VCC4" direction="pwr"/>
<pin name="VCC5" direction="pwr"/>
<pin name="VCC6" direction="pwr"/>
<pin name="VCC7" direction="pwr"/>
<pin name="VCC8" direction="pwr"/>
<pin name="VCC9" direction="pwr"/>
<pin name="VCC10" direction="pwr"/>
<pin name="VCC11" direction="pwr"/>
<pin name="VCC12" direction="pwr"/>
<pin name="VCC13" direction="pwr"/>
<pin name="VCC14" direction="pwr"/>
<pin name="CLKIN" direction="in"/>
<pin name="~CLKIN" direction="in"/>
<pin name="FIN" direction="in"/>
<pin name="~FIN" direction="in"/>
<pin name="LDOBYP1" direction="in"/>
<pin name="LDOBYP2" direction="in"/>
<pin name="CLKUWIRE" direction="in"/>
<pin name="DATAUWIRE" direction="in"/>
<pin name="LEUWIRE" direction="in"/>
<pin name="GOE" direction="in"/>
<pin name="~SYNC" direction="in"/>
<pin name="BIAS" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pwr"/>
<pin name="EPAD" direction="pas"/>
<pin name="CLKOUT0" direction="out"/>
<pin name="~CLKOUT0" direction="out"/>
<pin name="CLKOUT1" direction="out"/>
<pin name="~CLKOUT1" direction="out"/>
<pin name="CLKOUT2" direction="out"/>
<pin name="~CLKOUT2" direction="out"/>
<pin name="CLKOUT3" direction="out"/>
<pin name="~CLKOUT3" direction="out"/>
<pin name="CLKOUT4" direction="out"/>
<pin name="~CLKOUT4" direction="out"/>
<pin name="CLKOUT5" direction="out"/>
<pin name="~CLKOUT5" direction="out"/>
<pin name="CLKOUT6" direction="out"/>
<pin name="~CLKOUT6" direction="out"/>
<pin name="CLKOUT7" direction="out"/>
<pin name="~CLKOUT7" direction="out"/>
<pin name="LD" direction="out"/>
<pin name="CPOUT" direction="out"/>
</symbol>
<symbol name="LMK02002ISQ">
<pin name="VCC1" direction="pwr"/>
<pin name="VCC2" direction="pwr"/>
<pin name="VCC3" direction="pwr"/>
<pin name="VCC4" direction="pwr"/>
<pin name="VCC5" direction="pwr"/>
<pin name="VCC6" direction="pwr"/>
<pin name="VCC7" direction="pwr"/>
<pin name="VCC8" direction="pwr"/>
<pin name="VCC9" direction="pwr"/>
<pin name="VCC10" direction="pwr"/>
<pin name="VCC11" direction="pwr"/>
<pin name="VCC12" direction="pwr"/>
<pin name="VCC13" direction="pwr"/>
<pin name="VCC14" direction="pwr"/>
<pin name="CLKIN" direction="in"/>
<pin name="~CLKIN" direction="in"/>
<pin name="FIN" direction="in"/>
<pin name="~FIN" direction="in"/>
<pin name="LDOBYP1" direction="in"/>
<pin name="LDOBYP2" direction="in"/>
<pin name="CLKUWIRE" direction="in"/>
<pin name="DATAUWIRE" direction="in"/>
<pin name="LEUWIRE" direction="in"/>
<pin name="GOE" direction="in"/>
<pin name="~SYNC" direction="in"/>
<pin name="BIAS" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC_6" direction="nc"/>
<pin name="NC_7" direction="nc"/>
<pin name="NC_8" direction="nc"/>
<pin name="NC_9" direction="nc"/>
<pin name="NC_10" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pwr"/>
<pin name="EPAD" direction="pas"/>
<pin name="CLKOUT0" direction="out"/>
<pin name="~CLKOUT0" direction="out"/>
<pin name="CLKOUT1" direction="out"/>
<pin name="~CLKOUT1" direction="out"/>
<pin name="CLKOUT2" direction="out"/>
<pin name="~CLKOUT2" direction="out"/>
<pin name="CLKOUT3" direction="out"/>
<pin name="~CLKOUT3" direction="out"/>
<pin name="LD" direction="out"/>
<pin name="CPOUT" direction="out"/>
</symbol>
<symbol name="LMK03000CISQ">
<pin name="VCC1" direction="pwr"/>
<pin name="VCC2" direction="pwr"/>
<pin name="VCC3" direction="pwr"/>
<pin name="VCC4" direction="pwr"/>
<pin name="VCC5" direction="pwr"/>
<pin name="VCC6" direction="pwr"/>
<pin name="VCC7" direction="pwr"/>
<pin name="VCC8" direction="pwr"/>
<pin name="VCC9" direction="pwr"/>
<pin name="VCC10" direction="pwr"/>
<pin name="VCC11" direction="pwr"/>
<pin name="VCC12" direction="pwr"/>
<pin name="VCC13" direction="pwr"/>
<pin name="VCC14" direction="pwr"/>
<pin name="OSCIN_2" direction="in"/>
<pin name="OSCIN" direction="in"/>
<pin name="LDOBYP1" direction="in"/>
<pin name="LDOBYP2" direction="in"/>
<pin name="CLKUWIRE" direction="in"/>
<pin name="DATAUWIRE" direction="in"/>
<pin name="LEUWIRE" direction="in"/>
<pin name="GOE" direction="in"/>
<pin name="~SYNC" direction="in"/>
<pin name="BIAS" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pwr"/>
<pin name="EPAD" direction="pas"/>
<pin name="~CLKOUT0" direction="out"/>
<pin name="CLKOUT0" direction="out"/>
<pin name="CLKOUT1" direction="out"/>
<pin name="~CLKOUT1" direction="out"/>
<pin name="CLKOUT2" direction="out"/>
<pin name="~CLKOUT2" direction="out"/>
<pin name="CLKOUT3" direction="out"/>
<pin name="~CLKOUT3" direction="out"/>
<pin name="CLKOUT4" direction="out"/>
<pin name="~CLKOUT4" direction="out"/>
<pin name="CLKOUT5" direction="out"/>
<pin name="~CLKOUT5" direction="out"/>
<pin name="CLKOUT6" direction="out"/>
<pin name="~CLKOUT6" direction="out"/>
<pin name="CLKOUT7" direction="out"/>
<pin name="~CLKOUT7" direction="out"/>
<pin name="LD" direction="out"/>
<pin name="CPOUT" direction="out"/>
<pin name="FOUT" direction="out"/>
</symbol>
<symbol name="LMK03000DISQ">
<pin name="VCC1" direction="pwr"/>
<pin name="VCC2" direction="pwr"/>
<pin name="VCC3" direction="pwr"/>
<pin name="VCC4" direction="pwr"/>
<pin name="VCC5" direction="pwr"/>
<pin name="VCC6" direction="pwr"/>
<pin name="VCC7" direction="pwr"/>
<pin name="VCC8" direction="pwr"/>
<pin name="VCC9" direction="pwr"/>
<pin name="VCC10" direction="pwr"/>
<pin name="VCC11" direction="pwr"/>
<pin name="VCC12" direction="pwr"/>
<pin name="VCC13" direction="pwr"/>
<pin name="VCC14" direction="pwr"/>
<pin name="CLKUWIRE" direction="in"/>
<pin name="DATAUWIRE" direction="in"/>
<pin name="LEUWIRE" direction="in"/>
<pin name="~SYNC" direction="in"/>
<pin name="BIAS" direction="in"/>
<pin name="GOE" direction="in"/>
<pin name="OSCIN" direction="in"/>
<pin name="~OSCIN" direction="in"/>
<pin name="LDOBYP1" direction="in"/>
<pin name="LDOBYP2" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="LD" direction="out"/>
<pin name="CPOUT" direction="out"/>
<pin name="FOUT" direction="out"/>
<pin name="CLKOUT0" direction="out"/>
<pin name="~CLKOUT0+" direction="out"/>
<pin name="CLKOUT1" direction="out"/>
<pin name="~CLKOUT1" direction="out"/>
<pin name="CLKOUT2" direction="out"/>
<pin name="~CLKOUT2" direction="out"/>
<pin name="CLKOUT3" direction="out"/>
<pin name="~CLKOUT3" direction="out"/>
<pin name="CLKOUT4" direction="out"/>
<pin name="~CLKOUT4" direction="out"/>
<pin name="CLKOUT5" direction="out"/>
<pin name="~CLKOUT5" direction="out"/>
<pin name="CLKOUT6" direction="out"/>
<pin name="~CLKOUT6" direction="out"/>
<pin name="CLKOUT7" direction="out"/>
<pin name="~CLKOUT7" direction="out"/>
</symbol>
<symbol name="LMK03000ISQ">
<pin name="VCC1" direction="pwr"/>
<pin name="VCC2" direction="pwr"/>
<pin name="VCC3" direction="pwr"/>
<pin name="VCC4" direction="pwr"/>
<pin name="VCC5" direction="pwr"/>
<pin name="VCC6" direction="pwr"/>
<pin name="VCC7" direction="pwr"/>
<pin name="VCC8" direction="pwr"/>
<pin name="VCC9" direction="pwr"/>
<pin name="VCC10" direction="pwr"/>
<pin name="VCC11" direction="pwr"/>
<pin name="VCC12" direction="pwr"/>
<pin name="VCC13" direction="pwr"/>
<pin name="VCC14" direction="pwr"/>
<pin name="CLKUWIRE" direction="in"/>
<pin name="DATAUWIRE" direction="in"/>
<pin name="LEUWIRE" direction="in"/>
<pin name="~SYNC" direction="in"/>
<pin name="BIAS" direction="in"/>
<pin name="GOE" direction="in"/>
<pin name="OSCIN" direction="in"/>
<pin name="~OSCIN" direction="in"/>
<pin name="LDOBYP1" direction="in"/>
<pin name="LDOBYP2" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="LD" direction="out"/>
<pin name="CPOUT" direction="out"/>
<pin name="FOUT" direction="out"/>
<pin name="CLKOUT0" direction="out"/>
<pin name="~CLKOUT0+" direction="out"/>
<pin name="CLKOUT1" direction="out"/>
<pin name="~CLKOUT1" direction="out"/>
<pin name="CLKOUT2" direction="out"/>
<pin name="~CLKOUT2" direction="out"/>
<pin name="CLKOUT3" direction="out"/>
<pin name="~CLKOUT3" direction="out"/>
<pin name="CLKOUT4" direction="out"/>
<pin name="~CLKOUT4" direction="out"/>
<pin name="CLKOUT5" direction="out"/>
<pin name="~CLKOUT5" direction="out"/>
<pin name="CLKOUT6" direction="out"/>
<pin name="~CLKOUT6" direction="out"/>
<pin name="CLKOUT7" direction="out"/>
<pin name="~CLKOUT7" direction="out"/>
</symbol>
<symbol name="LMK03001CISQ">
<pin name="VCC1" direction="pwr"/>
<pin name="VCC2" direction="pwr"/>
<pin name="VCC3" direction="pwr"/>
<pin name="VCC4" direction="pwr"/>
<pin name="VCC5" direction="pwr"/>
<pin name="VCC6" direction="pwr"/>
<pin name="VCC7" direction="pwr"/>
<pin name="VCC8" direction="pwr"/>
<pin name="VCC9" direction="pwr"/>
<pin name="VCC10" direction="pwr"/>
<pin name="VCC11" direction="pwr"/>
<pin name="VCC12" direction="pwr"/>
<pin name="VCC13" direction="pwr"/>
<pin name="VCC14" direction="pwr"/>
<pin name="CLKUWIRE" direction="in"/>
<pin name="DATAUWIRE" direction="in"/>
<pin name="LEUWIRE" direction="in"/>
<pin name="~SYNC" direction="in"/>
<pin name="BIAS" direction="in"/>
<pin name="GOE" direction="in"/>
<pin name="OSCIN" direction="in"/>
<pin name="~OSCIN" direction="in"/>
<pin name="LDOBYP1" direction="in"/>
<pin name="LDOBYP2" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="LD" direction="out"/>
<pin name="CPOUT" direction="out"/>
<pin name="FOUT" direction="out"/>
<pin name="CLKOUT0" direction="out"/>
<pin name="~CLKOUT0+" direction="out"/>
<pin name="CLKOUT1" direction="out"/>
<pin name="~CLKOUT1" direction="out"/>
<pin name="CLKOUT2" direction="out"/>
<pin name="~CLKOUT2" direction="out"/>
<pin name="CLKOUT3" direction="out"/>
<pin name="~CLKOUT3" direction="out"/>
<pin name="CLKOUT4" direction="out"/>
<pin name="~CLKOUT4" direction="out"/>
<pin name="CLKOUT5" direction="out"/>
<pin name="~CLKOUT5" direction="out"/>
<pin name="CLKOUT6" direction="out"/>
<pin name="~CLKOUT6" direction="out"/>
<pin name="CLKOUT7" direction="out"/>
<pin name="~CLKOUT7" direction="out"/>
</symbol>
<symbol name="LMK03001DISQ">
<pin name="VCC1" direction="pwr"/>
<pin name="VCC2" direction="pwr"/>
<pin name="VCC3" direction="pwr"/>
<pin name="VCC4" direction="pwr"/>
<pin name="VCC5" direction="pwr"/>
<pin name="VCC6" direction="pwr"/>
<pin name="VCC7" direction="pwr"/>
<pin name="VCC8" direction="pwr"/>
<pin name="VCC9" direction="pwr"/>
<pin name="VCC10" direction="pwr"/>
<pin name="VCC11" direction="pwr"/>
<pin name="VCC12" direction="pwr"/>
<pin name="VCC13" direction="pwr"/>
<pin name="VCC14" direction="pwr"/>
<pin name="CLKUWIRE" direction="in"/>
<pin name="DATAUWIRE" direction="in"/>
<pin name="LEUWIRE" direction="in"/>
<pin name="~SYNC" direction="in"/>
<pin name="BIAS" direction="in"/>
<pin name="GOE" direction="in"/>
<pin name="OSCIN" direction="in"/>
<pin name="~OSCIN" direction="in"/>
<pin name="LDOBYP1" direction="in"/>
<pin name="LDOBYP2" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="LD" direction="out"/>
<pin name="CPOUT" direction="out"/>
<pin name="FOUT" direction="out"/>
<pin name="CLKOUT0" direction="out"/>
<pin name="~CLKOUT0+" direction="out"/>
<pin name="CLKOUT1" direction="out"/>
<pin name="~CLKOUT1" direction="out"/>
<pin name="CLKOUT2" direction="out"/>
<pin name="~CLKOUT2" direction="out"/>
<pin name="CLKOUT3" direction="out"/>
<pin name="~CLKOUT3" direction="out"/>
<pin name="CLKOUT4" direction="out"/>
<pin name="~CLKOUT4" direction="out"/>
<pin name="CLKOUT5" direction="out"/>
<pin name="~CLKOUT5" direction="out"/>
<pin name="CLKOUT6" direction="out"/>
<pin name="~CLKOUT6" direction="out"/>
<pin name="CLKOUT7" direction="out"/>
<pin name="~CLKOUT7" direction="out"/>
</symbol>
<symbol name="LMK03001ISQ">
<pin name="VCC1" direction="pwr"/>
<pin name="VCC2" direction="pwr"/>
<pin name="VCC3" direction="pwr"/>
<pin name="VCC4" direction="pwr"/>
<pin name="VCC5" direction="pwr"/>
<pin name="VCC6" direction="pwr"/>
<pin name="VCC7" direction="pwr"/>
<pin name="VCC8" direction="pwr"/>
<pin name="VCC9" direction="pwr"/>
<pin name="VCC10" direction="pwr"/>
<pin name="VCC11" direction="pwr"/>
<pin name="VCC12" direction="pwr"/>
<pin name="VCC13" direction="pwr"/>
<pin name="VCC14" direction="pwr"/>
<pin name="CLKUWIRE" direction="in"/>
<pin name="DATAUWIRE" direction="in"/>
<pin name="LEUWIRE" direction="in"/>
<pin name="~SYNC" direction="in"/>
<pin name="BIAS" direction="in"/>
<pin name="GOE" direction="in"/>
<pin name="OSCIN" direction="in"/>
<pin name="~OSCIN" direction="in"/>
<pin name="LDOBYP1" direction="in"/>
<pin name="LDOBYP2" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="LD" direction="out"/>
<pin name="CPOUT" direction="out"/>
<pin name="FOUT" direction="out"/>
<pin name="CLKOUT0" direction="out"/>
<pin name="~CLKOUT0+" direction="out"/>
<pin name="CLKOUT1" direction="out"/>
<pin name="~CLKOUT1" direction="out"/>
<pin name="CLKOUT2" direction="out"/>
<pin name="~CLKOUT2" direction="out"/>
<pin name="CLKOUT3" direction="out"/>
<pin name="~CLKOUT3" direction="out"/>
<pin name="CLKOUT4" direction="out"/>
<pin name="~CLKOUT4" direction="out"/>
<pin name="CLKOUT5" direction="out"/>
<pin name="~CLKOUT5" direction="out"/>
<pin name="CLKOUT6" direction="out"/>
<pin name="~CLKOUT6" direction="out"/>
<pin name="CLKOUT7" direction="out"/>
<pin name="~CLKOUT7" direction="out"/>
</symbol>
<symbol name="LMK03033CISQ">
<pin name="VCC1" direction="pwr"/>
<pin name="VCC2" direction="pwr"/>
<pin name="VCC3" direction="pwr"/>
<pin name="VCC4" direction="pwr"/>
<pin name="VCC5" direction="pwr"/>
<pin name="VCC6" direction="pwr"/>
<pin name="VCC7" direction="pwr"/>
<pin name="VCC8" direction="pwr"/>
<pin name="VCC9" direction="pwr"/>
<pin name="VCC10" direction="pwr"/>
<pin name="VCC11" direction="pwr"/>
<pin name="VCC12" direction="pwr"/>
<pin name="VCC13" direction="pwr"/>
<pin name="VCC14" direction="pwr"/>
<pin name="OSCIN" direction="in"/>
<pin name="~OSCIN" direction="in"/>
<pin name="GOE" direction="in"/>
<pin name="~SYNC" direction="in"/>
<pin name="BIAS" direction="in"/>
<pin name="CLKUWIRE" direction="in"/>
<pin name="DATAUWIRE" direction="in"/>
<pin name="LEUWIRE" direction="in"/>
<pin name="LDOBYP1" direction="pas"/>
<pin name="LDOBYP2" direction="pas"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="DAP" direction="pas"/>
<pin name="LD" direction="out"/>
<pin name="FOUT" direction="out"/>
<pin name="CPOUT" direction="out"/>
<pin name="CLKOUT0" direction="out"/>
<pin name="~CLKOUT0" direction="out"/>
<pin name="CLKOUT1" direction="out"/>
<pin name="~CLKOUT1" direction="out"/>
<pin name="CLKOUT2" direction="out"/>
<pin name="~CLKOUT2" direction="out"/>
<pin name="CLKOUT3" direction="out"/>
<pin name="~CLKOUT3" direction="out"/>
<pin name="CLKOUT4" direction="out"/>
<pin name="~CLKOUT4" direction="out"/>
<pin name="CLKOUT5" direction="out"/>
<pin name="~CLKOUT5" direction="out"/>
<pin name="CLKOUT6" direction="out"/>
<pin name="~CLKOUT6" direction="out"/>
<pin name="CLKOUT7" direction="out"/>
<pin name="~CLKOUT7" direction="out"/>
</symbol>
<symbol name="LMK04000BISQE">
<pin name="VCC1" direction="pwr"/>
<pin name="VCC2" direction="pwr"/>
<pin name="VCC3" direction="pwr"/>
<pin name="VCC4" direction="pwr"/>
<pin name="VCC5" direction="pwr"/>
<pin name="VCC6" direction="pwr"/>
<pin name="VCC7" direction="pwr"/>
<pin name="VCC8" direction="pwr"/>
<pin name="VCC9" direction="pwr"/>
<pin name="VCC10" direction="pwr"/>
<pin name="VCC11" direction="pwr"/>
<pin name="VCC12" direction="pwr"/>
<pin name="VCC13" direction="pwr"/>
<pin name="VCC14" direction="pwr"/>
<pin name="~CLKIN0" direction="in"/>
<pin name="~CLKIN1" direction="in"/>
<pin name="~OSCIN" direction="in"/>
<pin name="~SYNC" direction="in"/>
<pin name="BIAS" direction="in"/>
<pin name="CLKIN0" direction="in"/>
<pin name="CLKIN1" direction="in"/>
<pin name="CLKUWIRE" direction="in"/>
<pin name="DATAUWIRE" direction="in"/>
<pin name="DLD_BYP" direction="pas"/>
<pin name="GOE" direction="in"/>
<pin name="LDOBYP1" direction="pas"/>
<pin name="LDOBYP2" direction="pas"/>
<pin name="LEUWIRE" direction="in"/>
<pin name="OSCIN" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="HEAT_TAB" direction="pas"/>
<pin name="~CLKOUT0" direction="out"/>
<pin name="~CLKOUT1" direction="out"/>
<pin name="~CLKOUT2" direction="out"/>
<pin name="~CLKOUT3" direction="out"/>
<pin name="~CLKOUT4" direction="out"/>
<pin name="CLKOUT0" direction="out"/>
<pin name="CLKOUT1" direction="out"/>
<pin name="CLKOUT2" direction="out"/>
<pin name="CLKOUT3" direction="out"/>
<pin name="CLKOUT4" direction="out"/>
<pin name="CPOUT1" direction="out"/>
<pin name="CPOUT2" direction="out"/>
<pin name="FOUT" direction="out"/>
<pin name="LD" direction="out"/>
<pin name="CLKIN0_LOS" direction="out"/>
<pin name="CLKIN1_LOS" direction="out"/>
</symbol>
<symbol name="LMK04001BISQE">
<pin name="VCC1" direction="pwr"/>
<pin name="VCC2" direction="pwr"/>
<pin name="VCC3" direction="pwr"/>
<pin name="VCC4" direction="pwr"/>
<pin name="VCC5" direction="pwr"/>
<pin name="VCC6" direction="pwr"/>
<pin name="VCC7" direction="pwr"/>
<pin name="VCC8" direction="pwr"/>
<pin name="VCC9" direction="pwr"/>
<pin name="VCC10" direction="pwr"/>
<pin name="VCC11" direction="pwr"/>
<pin name="VCC12" direction="pwr"/>
<pin name="VCC13" direction="pwr"/>
<pin name="VCC14" direction="pwr"/>
<pin name="~CLKIN0" direction="in"/>
<pin name="~CLKIN1" direction="in"/>
<pin name="~OSCIN" direction="in"/>
<pin name="~SYNC" direction="in"/>
<pin name="BIAS" direction="in"/>
<pin name="CLKIN0" direction="in"/>
<pin name="CLKIN1" direction="in"/>
<pin name="CLKUWIRE" direction="in"/>
<pin name="DATAUWIRE" direction="in"/>
<pin name="DLD_BYP" direction="pas"/>
<pin name="GOE" direction="in"/>
<pin name="LDOBYP1" direction="pas"/>
<pin name="LDOBYP2" direction="pas"/>
<pin name="LEUWIRE" direction="in"/>
<pin name="OSCIN" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="HEAT_TAB" direction="pas"/>
<pin name="~CLKOUT0" direction="out"/>
<pin name="~CLKOUT1" direction="out"/>
<pin name="~CLKOUT2" direction="out"/>
<pin name="~CLKOUT3" direction="out"/>
<pin name="~CLKOUT4" direction="out"/>
<pin name="CLKOUT0" direction="out"/>
<pin name="CLKOUT1" direction="out"/>
<pin name="CLKOUT2" direction="out"/>
<pin name="CLKOUT3" direction="out"/>
<pin name="CLKOUT4" direction="out"/>
<pin name="CPOUT1" direction="out"/>
<pin name="CPOUT2" direction="out"/>
<pin name="FOUT" direction="out"/>
<pin name="LD" direction="out"/>
<pin name="CLKIN0_LOS" direction="out"/>
<pin name="CLKIN1_LOS" direction="out"/>
</symbol>
<symbol name="LMK04002BISQE">
<pin name="VCC1" direction="pwr"/>
<pin name="VCC2" direction="pwr"/>
<pin name="VCC3" direction="pwr"/>
<pin name="VCC4" direction="pwr"/>
<pin name="VCC5" direction="pwr"/>
<pin name="VCC6" direction="pwr"/>
<pin name="VCC7" direction="pwr"/>
<pin name="VCC8" direction="pwr"/>
<pin name="VCC9" direction="pwr"/>
<pin name="VCC10" direction="pwr"/>
<pin name="VCC11" direction="pwr"/>
<pin name="VCC12" direction="pwr"/>
<pin name="VCC13" direction="pwr"/>
<pin name="VCC14" direction="pwr"/>
<pin name="~CLKIN0" direction="in"/>
<pin name="~CLKIN1" direction="in"/>
<pin name="~OSCIN" direction="in"/>
<pin name="~SYNC" direction="in"/>
<pin name="BIAS" direction="in"/>
<pin name="CLKIN0" direction="in"/>
<pin name="CLKIN1" direction="in"/>
<pin name="CLKUWIRE" direction="in"/>
<pin name="DATAUWIRE" direction="in"/>
<pin name="DLD_BYP" direction="pas"/>
<pin name="GOE" direction="in"/>
<pin name="LDOBYP1" direction="pas"/>
<pin name="LDOBYP2" direction="pas"/>
<pin name="LEUWIRE" direction="in"/>
<pin name="OSCIN" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="HEAT_TAB" direction="pas"/>
<pin name="~CLKOUT0" direction="out"/>
<pin name="~CLKOUT1" direction="out"/>
<pin name="~CLKOUT2" direction="out"/>
<pin name="~CLKOUT3" direction="out"/>
<pin name="~CLKOUT4" direction="out"/>
<pin name="CLKOUT0" direction="out"/>
<pin name="CLKOUT1" direction="out"/>
<pin name="CLKOUT2" direction="out"/>
<pin name="CLKOUT3" direction="out"/>
<pin name="CLKOUT4" direction="out"/>
<pin name="CPOUT1" direction="out"/>
<pin name="CPOUT2" direction="out"/>
<pin name="FOUT" direction="out"/>
<pin name="LD" direction="out"/>
<pin name="CLKIN0_LOS" direction="out"/>
<pin name="CLKIN1_LOS" direction="out"/>
</symbol>
<symbol name="LMK04010BISQE">
<pin name="VCC1" direction="pwr"/>
<pin name="VCC2" direction="pwr"/>
<pin name="VCC3" direction="pwr"/>
<pin name="VCC4" direction="pwr"/>
<pin name="VCC5" direction="pwr"/>
<pin name="VCC6" direction="pwr"/>
<pin name="VCC7" direction="pwr"/>
<pin name="VCC8" direction="pwr"/>
<pin name="VCC9" direction="pwr"/>
<pin name="VCC10" direction="pwr"/>
<pin name="VCC11" direction="pwr"/>
<pin name="VCC12" direction="pwr"/>
<pin name="VCC13" direction="pwr"/>
<pin name="VCC14" direction="pwr"/>
<pin name="~CLKIN0" direction="in"/>
<pin name="~CLKIN1" direction="in"/>
<pin name="~OSCIN" direction="in"/>
<pin name="~SYNC" direction="in"/>
<pin name="BIAS" direction="in"/>
<pin name="CLKIN0" direction="in"/>
<pin name="CLKIN1" direction="in"/>
<pin name="CLKUWIRE" direction="in"/>
<pin name="DATAUWIRE" direction="in"/>
<pin name="DLD_BYP" direction="pas"/>
<pin name="GOE" direction="in"/>
<pin name="LDOBYP1" direction="pas"/>
<pin name="LDOBYP2" direction="pas"/>
<pin name="LEUWIRE" direction="in"/>
<pin name="OSCIN" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="HEAT_TAB" direction="pas"/>
<pin name="~CLKOUT0" direction="out"/>
<pin name="~CLKOUT1" direction="out"/>
<pin name="~CLKOUT2" direction="out"/>
<pin name="~CLKOUT3" direction="out"/>
<pin name="~CLKOUT4" direction="out"/>
<pin name="CLKOUT0" direction="out"/>
<pin name="CLKOUT1" direction="out"/>
<pin name="CLKOUT2" direction="out"/>
<pin name="CLKOUT3" direction="out"/>
<pin name="CLKOUT4" direction="out"/>
<pin name="CPOUT1" direction="out"/>
<pin name="CPOUT2" direction="out"/>
<pin name="FOUT" direction="out"/>
<pin name="LD" direction="out"/>
<pin name="CLKIN0_LOS" direction="out"/>
<pin name="CLKIN1_LOS" direction="out"/>
</symbol>
<symbol name="LMK04011BISQE">
<pin name="VCC1" direction="pwr"/>
<pin name="VCC2" direction="pwr"/>
<pin name="VCC3" direction="pwr"/>
<pin name="VCC4" direction="pwr"/>
<pin name="VCC5" direction="pwr"/>
<pin name="VCC6" direction="pwr"/>
<pin name="VCC7" direction="pwr"/>
<pin name="VCC8" direction="pwr"/>
<pin name="VCC9" direction="pwr"/>
<pin name="VCC10" direction="pwr"/>
<pin name="VCC11" direction="pwr"/>
<pin name="VCC12" direction="pwr"/>
<pin name="VCC13" direction="pwr"/>
<pin name="VCC14" direction="pwr"/>
<pin name="~CLKIN0" direction="in"/>
<pin name="~CLKIN1" direction="in"/>
<pin name="~OSCIN" direction="in"/>
<pin name="~SYNC" direction="in"/>
<pin name="BIAS" direction="in"/>
<pin name="CLKIN0" direction="in"/>
<pin name="CLKIN1" direction="in"/>
<pin name="CLKUWIRE" direction="in"/>
<pin name="DATAUWIRE" direction="in"/>
<pin name="DLD_BYP" direction="pas"/>
<pin name="GOE" direction="in"/>
<pin name="LDOBYP1" direction="pas"/>
<pin name="LDOBYP2" direction="pas"/>
<pin name="LEUWIRE" direction="in"/>
<pin name="OSCIN" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="HEAT_TAB" direction="pas"/>
<pin name="~CLKOUT0" direction="out"/>
<pin name="~CLKOUT1" direction="out"/>
<pin name="~CLKOUT2" direction="out"/>
<pin name="~CLKOUT3" direction="out"/>
<pin name="~CLKOUT4" direction="out"/>
<pin name="CLKOUT0" direction="out"/>
<pin name="CLKOUT1" direction="out"/>
<pin name="CLKOUT2" direction="out"/>
<pin name="CLKOUT3" direction="out"/>
<pin name="CLKOUT4" direction="out"/>
<pin name="CPOUT1" direction="out"/>
<pin name="CPOUT2" direction="out"/>
<pin name="FOUT" direction="out"/>
<pin name="LD" direction="out"/>
<pin name="CLKIN0_LOS" direction="out"/>
<pin name="CLKIN1_LOS" direction="out"/>
</symbol>
<symbol name="LMK04031BISQE">
<pin name="VCC1" direction="pwr"/>
<pin name="VCC2" direction="pwr"/>
<pin name="VCC3" direction="pwr"/>
<pin name="VCC4" direction="pwr"/>
<pin name="VCC5" direction="pwr"/>
<pin name="VCC6" direction="pwr"/>
<pin name="VCC7" direction="pwr"/>
<pin name="VCC8" direction="pwr"/>
<pin name="VCC9" direction="pwr"/>
<pin name="VCC10" direction="pwr"/>
<pin name="VCC11" direction="pwr"/>
<pin name="VCC12" direction="pwr"/>
<pin name="VCC13" direction="pwr"/>
<pin name="VCC14" direction="pwr"/>
<pin name="~CLKIN0" direction="in"/>
<pin name="~CLKIN1" direction="in"/>
<pin name="~OSCIN" direction="in"/>
<pin name="~SYNC" direction="in"/>
<pin name="BIAS" direction="in"/>
<pin name="CLKIN0" direction="in"/>
<pin name="CLKIN1" direction="in"/>
<pin name="CLKUWIRE" direction="in"/>
<pin name="DATAUWIRE" direction="in"/>
<pin name="DLD_BYP" direction="pas"/>
<pin name="GOE" direction="in"/>
<pin name="LDOBYP1" direction="pas"/>
<pin name="LDOBYP2" direction="pas"/>
<pin name="LEUWIRE" direction="in"/>
<pin name="OSCIN" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="HEAT_TAB" direction="pas"/>
<pin name="~CLKOUT0" direction="out"/>
<pin name="~CLKOUT1" direction="out"/>
<pin name="~CLKOUT2" direction="out"/>
<pin name="~CLKOUT3" direction="out"/>
<pin name="~CLKOUT4" direction="out"/>
<pin name="CLKOUT0" direction="out"/>
<pin name="CLKOUT1" direction="out"/>
<pin name="CLKOUT2" direction="out"/>
<pin name="CLKOUT3" direction="out"/>
<pin name="CLKOUT4" direction="out"/>
<pin name="CPOUT1" direction="out"/>
<pin name="CPOUT2" direction="out"/>
<pin name="FOUT" direction="out"/>
<pin name="LD" direction="out"/>
<pin name="CLKIN0_LOS" direction="out"/>
<pin name="CLKIN1_LOS" direction="out"/>
</symbol>
<symbol name="LMK04033BISQE">
<pin name="VCC1" direction="pwr"/>
<pin name="VCC2" direction="pwr"/>
<pin name="VCC3" direction="pwr"/>
<pin name="VCC4" direction="pwr"/>
<pin name="VCC5" direction="pwr"/>
<pin name="VCC6" direction="pwr"/>
<pin name="VCC7" direction="pwr"/>
<pin name="VCC8" direction="pwr"/>
<pin name="VCC9" direction="pwr"/>
<pin name="VCC10" direction="pwr"/>
<pin name="VCC11" direction="pwr"/>
<pin name="VCC12" direction="pwr"/>
<pin name="VCC13" direction="pwr"/>
<pin name="VCC14" direction="pwr"/>
<pin name="~CLKIN0" direction="in"/>
<pin name="~CLKIN1" direction="in"/>
<pin name="~OSCIN" direction="in"/>
<pin name="~SYNC" direction="in"/>
<pin name="BIAS" direction="in"/>
<pin name="CLKIN0" direction="in"/>
<pin name="CLKIN1" direction="in"/>
<pin name="CLKUWIRE" direction="in"/>
<pin name="DATAUWIRE" direction="in"/>
<pin name="DLD_BYP" direction="pas"/>
<pin name="GOE" direction="in"/>
<pin name="LDOBYP1" direction="pas"/>
<pin name="LDOBYP2" direction="pas"/>
<pin name="LEUWIRE" direction="in"/>
<pin name="OSCIN" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="HEAT_TAB" direction="pas"/>
<pin name="~CLKOUT0" direction="out"/>
<pin name="~CLKOUT1" direction="out"/>
<pin name="~CLKOUT2" direction="out"/>
<pin name="~CLKOUT3" direction="out"/>
<pin name="~CLKOUT4" direction="out"/>
<pin name="CLKOUT0" direction="out"/>
<pin name="CLKOUT1" direction="out"/>
<pin name="CLKOUT2" direction="out"/>
<pin name="CLKOUT3" direction="out"/>
<pin name="CLKOUT4" direction="out"/>
<pin name="CPOUT1" direction="out"/>
<pin name="CPOUT2" direction="out"/>
<pin name="FOUT" direction="out"/>
<pin name="LD" direction="out"/>
<pin name="CLKIN0_LOS" direction="out"/>
<pin name="CLKIN1_LOS" direction="out"/>
</symbol>
<symbol name="LMP2011MA">
<pin name="V+" direction="pwr"/>
<pin name="-VIN" direction="in"/>
<pin name="+VIN" direction="in"/>
<pin name="N/C_2" direction="nc"/>
<pin name="N/C_3" direction="nc"/>
<pin name="N/C" direction="nc"/>
<pin name="V-" direction="pwr"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LMP2011MF">
<pin name="V+" direction="pwr"/>
<pin name="VIN+" direction="in"/>
<pin name="VIN-" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LMP2012MA">
<pin name="V+" direction="pwr"/>
<pin name="-VIN" direction="in"/>
<pin name="+VIN" direction="in"/>
<pin name="N/C_2" direction="nc"/>
<pin name="N/C_3" direction="nc"/>
<pin name="N/C" direction="nc"/>
<pin name="V-" direction="pwr"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LMP2012MM">
<pin name="V+" direction="pwr"/>
<pin name="INA+" direction="in"/>
<pin name="INA-" direction="in"/>
<pin name="INB-" direction="in"/>
<pin name="INB+" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="LMP2014MT">
<pin name="V+" direction="pwr"/>
<pin name="-INA" direction="in"/>
<pin name="+INA" direction="in"/>
<pin name="+INB" direction="in"/>
<pin name="-INB" direction="in"/>
<pin name="-INC" direction="in"/>
<pin name="+INC" direction="in"/>
<pin name="+IND" direction="in"/>
<pin name="-IND" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
<pin name="OUTC" direction="out"/>
<pin name="OUTD" direction="out"/>
</symbol>
<symbol name="LMP2015MA">
<pin name="V+" direction="pwr"/>
<pin name="VIN+" direction="in"/>
<pin name="VIN-" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="V-" direction="pwr"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LMP2015MF">
<pin name="V+" direction="pwr"/>
<pin name="VIN+" direction="in"/>
<pin name="VIN-" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LMP2016MA">
<pin name="V+" direction="pwr"/>
<pin name="VIN-" direction="in"/>
<pin name="VIN+" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="V-" direction="pwr"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LMP2016MM">
<pin name="V+" direction="pwr"/>
<pin name="INA+" direction="in"/>
<pin name="INA-" direction="in"/>
<pin name="INB-" direction="in"/>
<pin name="INB+" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="LMP2021MA">
<pin name="V+" direction="pwr"/>
<pin name="IN-" direction="in"/>
<pin name="IN+" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LMP2021MF">
<pin name="V+" direction="pwr"/>
<pin name="IN+" direction="in"/>
<pin name="IN-" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LMP2022MA">
<pin name="V+" direction="pwr"/>
<pin name="IN+" direction="in"/>
<pin name="IN-" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LMP2231AMA">
<pin name="V+" direction="pwr"/>
<pin name="VIN-" direction="in"/>
<pin name="VIN+" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="N/C_2" direction="nc"/>
<pin name="N/C" direction="nc"/>
<pin name="V-" direction="pwr"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LMP2231AMF">
<pin name="V+" direction="pwr"/>
<pin name="IN+" direction="in"/>
<pin name="IN-" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LMP2232AMA">
<pin name="V+" direction="pwr"/>
<pin name="INA-" direction="in"/>
<pin name="INA+" direction="in"/>
<pin name="INB-" direction="in"/>
<pin name="INB+" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="LMP2234AMA">
<pin name="V+" direction="pwr"/>
<pin name="INA-" direction="in"/>
<pin name="INA+" direction="in"/>
<pin name="INB+" direction="in"/>
<pin name="INB-" direction="in"/>
<pin name="INC-" direction="in"/>
<pin name="INC+" direction="in"/>
<pin name="IND-" direction="in"/>
<pin name="IND+" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
<pin name="OUTC" direction="out"/>
<pin name="OUTD" direction="out"/>
</symbol>
<symbol name="LMP2234AMT">
<pin name="V+" direction="pwr"/>
<pin name="INA-" direction="in"/>
<pin name="INA+" direction="in"/>
<pin name="INB-" direction="in"/>
<pin name="INB+" direction="in"/>
<pin name="INC-" direction="in"/>
<pin name="INC+" direction="in"/>
<pin name="IND+" direction="in"/>
<pin name="IND-" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
<pin name="OUTC" direction="out"/>
<pin name="OUTD" direction="out"/>
</symbol>
<symbol name="LMP7300MA">
<pin name="V+" direction="pwr"/>
<pin name="+IN" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="HYSP" direction="in"/>
<pin name="HYST" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
<pin name="REF" direction="out"/>
</symbol>
<symbol name="LMP7701MF">
<pin name="V+" direction="pwr"/>
<pin name="IN+" direction="in"/>
<pin name="IN-" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LMP7702MA">
<pin name="V+" direction="pwr"/>
<pin name="INA-" direction="in"/>
<pin name="INA+" direction="in"/>
<pin name="INB-" direction="in"/>
<pin name="INB+" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="LMP7702MM">
<pin name="V+" direction="pwr"/>
<pin name="INA+" direction="in"/>
<pin name="INA-" direction="in"/>
<pin name="INB-" direction="in"/>
<pin name="INB+" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="LMP7704MA">
<pin name="V+" direction="pwr"/>
<pin name="INA-" direction="in"/>
<pin name="INA+" direction="in"/>
<pin name="INB+" direction="in"/>
<pin name="INB-" direction="in"/>
<pin name="INC+" direction="in"/>
<pin name="INC-" direction="in"/>
<pin name="IND+" direction="in"/>
<pin name="IND-" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
<pin name="OUTC" direction="out"/>
<pin name="OUTD" direction="out"/>
</symbol>
<symbol name="LMP7704MT">
<pin name="V+" direction="pwr"/>
<pin name="-INA" direction="in"/>
<pin name="+INA" direction="in"/>
<pin name="+INB" direction="in"/>
<pin name="-INB" direction="in"/>
<pin name="-INC" direction="in"/>
<pin name="+INC" direction="in"/>
<pin name="+IND" direction="in"/>
<pin name="-IND" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
<pin name="OUTC" direction="out"/>
<pin name="OUTD" direction="out"/>
</symbol>
<symbol name="LMP7707MA">
<pin name="V+" direction="pwr"/>
<pin name="IN-" direction="in"/>
<pin name="IN+" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LMP7708MA">
<pin name="V+" direction="pwr"/>
<pin name="+INA" direction="in"/>
<pin name="-INA" direction="in"/>
<pin name="-INB" direction="in"/>
<pin name="+INB" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="LMP7708MM">
<pin name="V+" direction="pwr"/>
<pin name="+INA" direction="in"/>
<pin name="-INA" direction="in"/>
<pin name="+INB" direction="in"/>
<pin name="-INB" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="LMP7709MA">
<pin name="V+" direction="pwr"/>
<pin name="INA-" direction="in"/>
<pin name="INA+" direction="in"/>
<pin name="INB+" direction="in"/>
<pin name="INB-" direction="in"/>
<pin name="INC+" direction="in"/>
<pin name="INC-" direction="in"/>
<pin name="IND+" direction="in"/>
<pin name="IND-" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
<pin name="OUTC" direction="out"/>
<pin name="OUTD" direction="out"/>
</symbol>
<symbol name="LMP7709MT">
<pin name="V+" direction="pwr"/>
<pin name="INA+" direction="in"/>
<pin name="INA-" direction="in"/>
<pin name="INB+" direction="in"/>
<pin name="INB-" direction="in"/>
<pin name="INC-" direction="in"/>
<pin name="INC+" direction="in"/>
<pin name="IND-" direction="in"/>
<pin name="IND+" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
<pin name="OUTC" direction="out"/>
<pin name="OUTD" direction="out"/>
</symbol>
<symbol name="LMP7711MK">
<pin name="V+" direction="pwr"/>
<pin name="+IN" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT_" direction="out"/>
</symbol>
<symbol name="LMP7712MM">
<pin name="V+" direction="pwr"/>
<pin name="-INA" direction="in"/>
<pin name="+INA" direction="in"/>
<pin name="+INB" direction="in"/>
<pin name="-INB" direction="in"/>
<pin name="ENA" direction="in"/>
<pin name="ENB" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="LMP7715MF">
<pin name="V+" direction="pwr"/>
<pin name="IN+" direction="in"/>
<pin name="IN-" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LMP7716MM">
<pin name="V+" direction="pwr"/>
<pin name="INA+" direction="in"/>
<pin name="INA-" direction="in"/>
<pin name="INB-" direction="in"/>
<pin name="INB+" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="LMP7716QMM">
<pin name="V+" direction="pwr"/>
<pin name="INA+" direction="in"/>
<pin name="INA-" direction="in"/>
<pin name="INB-" direction="in"/>
<pin name="INB+" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="LMP7717MA">
<pin name="V+" direction="pwr"/>
<pin name="-INA" direction="in"/>
<pin name="+INA" direction="in"/>
<pin name="-INB" direction="in"/>
<pin name="+INB" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT_A" direction="out"/>
<pin name="OUT_B" direction="out"/>
</symbol>
<symbol name="LMP7717MF">
<pin name="V+" direction="pwr"/>
<pin name="+IN" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LMP7718MA">
<pin name="V-" direction="pwr"/>
<pin name="INA-" direction="in"/>
<pin name="INA+" direction="in"/>
<pin name="INB-" direction="in"/>
<pin name="INB+" direction="in"/>
<pin name="V+" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="LMP7718MM">
<pin name="V+" direction="pwr"/>
<pin name="+INA" direction="in"/>
<pin name="-INA" direction="in"/>
<pin name="+INB" direction="in"/>
<pin name="-INB" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="LMP7721MA">
<pin name="V+" direction="pwr"/>
<pin name="IN+" direction="in"/>
<pin name="IN-" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="V-" direction="pwr"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LMP7731MA">
<pin name="V+" direction="pwr"/>
<pin name="IN-" direction="in"/>
<pin name="IN+" direction="in"/>
<pin name="N/C_2" direction="in"/>
<pin name="N/C_3" direction="nc"/>
<pin name="N/C" direction="nc"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LMP7731MF">
<pin name="V+" direction="pwr"/>
<pin name="+IN" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LMP7732MA">
<pin name="V+" direction="pwr"/>
<pin name="+INA" direction="in"/>
<pin name="-INA" direction="in"/>
<pin name="-INB" direction="in"/>
<pin name="+INB" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="LMP7732MM">
<pin name="V+" direction="pwr"/>
<pin name="+INA" direction="in"/>
<pin name="-INA" direction="in"/>
<pin name="+INB" direction="in"/>
<pin name="-INB" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="LMP8100MA">
<pin name="V+" direction="pwr"/>
<pin name="SCK" direction="in"/>
<pin name="SDI" direction="in"/>
<pin name="~CS" direction="in"/>
<pin name="GRT1" direction="pas"/>
<pin name="GRT2" direction="pas"/>
<pin name="IN+" direction="pwr"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="V-" direction="pwr"/>
<pin name="DGND" direction="pas"/>
<pin name="VOUT" direction="out"/>
<pin name="SDO" direction="out"/>
</symbol>
<symbol name="LMP8601MA">
<pin name="VS" direction="pwr"/>
<pin name="OFFSET" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LMP8601QMA">
<pin name="VS" direction="pwr"/>
<pin name="OFFSET" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LMP8602MA">
<pin name="VS" direction="pwr"/>
<pin name="OFFSET" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LMP8602MM">
<pin name="VS" direction="pwr"/>
<pin name="-IN" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
<pin name="OFFSET"/>
</symbol>
<symbol name="LMP8603MA">
<pin name="VS" direction="pwr"/>
<pin name="OFFSET" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LMP8603MM">
<pin name="VS" direction="pwr"/>
<pin name="-IN" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
<pin name="OFFSET"/>
</symbol>
<symbol name="LMP8645MK">
<pin name="V+" direction="pwr"/>
<pin name="RG" direction="in"/>
<pin name="IN+" direction="in"/>
<pin name="IN-" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LMS1487ECM">
<pin name="VCC" direction="pwr"/>
<pin name="~RE" direction="in"/>
<pin name="DE" direction="in"/>
<pin name="DI" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="A" direction="out"/>
<pin name="B" direction="out"/>
<pin name="RO" direction="out"/>
</symbol>
<symbol name="LMS1487ECNA">
<pin name="VCC" direction="pwr"/>
<pin name="~RE" direction="in"/>
<pin name="DE" direction="in"/>
<pin name="DI" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="RO" direction="out"/>
<pin name="A"/>
<pin name="B"/>
</symbol>
<symbol name="LMS1587CS-1.5">
<pin name="IN" direction="pwr"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LMS1587CS-3.3">
<pin name="IN" direction="pwr"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LMS1587CT-3.3">
<pin name="VIN" direction="in"/>
<pin name="ADJ/GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LMS1587CT-ADJ">
<pin name="VIN" direction="in"/>
<pin name="ADJ/GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LMS1587IS-1.5">
<pin name="IN" direction="pwr"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LMS1587IS-3.3">
<pin name="IN" direction="pwr"/>
<pin name="ADJ/GND" direction="pas"/>
<pin name="OUT" direction="out"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LMS1587IS-ADJ">
<pin name="IN" direction="pwr"/>
<pin name="ADJ" direction="pas"/>
<pin name="OUT" direction="out"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LMS33460MG">
<pin name="VIN" direction="pwr"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="~VOUT" direction="out"/>
</symbol>
<symbol name="LMS8117ADT-3.3">
<pin name="VIN" direction="pwr"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LMS8117AMP-1.8">
<pin name="IN" direction="pwr"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LMS8117AMP-3.3">
<pin name="IN" direction="pwr"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LMS8117AMP-ADJ">
<pin name="IN" direction="pwr"/>
<pin name="ADJ" direction="pas"/>
<pin name="OUT" direction="out"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LMV1032URX-25">
<pin name="VCC" direction="pwr"/>
<pin name="INPUT" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUTPUT" direction="out"/>
</symbol>
<symbol name="LMV1088RL">
<pin name="I2CVDD" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="PE" direction="in"/>
<pin name="REF" direction="in"/>
<pin name="ADR" direction="in"/>
<pin name="SCL" direction="in"/>
<pin name="CAL" direction="in"/>
<pin name="LPF" direction="in"/>
<pin name="T1" direction="in"/>
<pin name="T2" direction="in"/>
<pin name="T3" direction="in"/>
<pin name="T4" direction="in"/>
<pin name="T5" direction="in"/>
<pin name="T6" direction="in"/>
<pin name="T7" direction="in"/>
<pin name="T8" direction="in"/>
<pin name="MIC1-" direction="in"/>
<pin name="MIC1+" direction="in"/>
<pin name="MIC2-" direction="in"/>
<pin name="MIC2+" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC_6" direction="nc"/>
<pin name="NC_7" direction="nc"/>
<pin name="NC_8" direction="nc"/>
<pin name="NC_9" direction="nc"/>
<pin name="NC_10" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="SDA"/>
<pin name="OUT" direction="out"/>
<pin name="MICBIAS" direction="out"/>
</symbol>
<symbol name="LMV1089RL">
<pin name="I2CVDD" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="PE" direction="in"/>
<pin name="REF" direction="in"/>
<pin name="ADR" direction="in"/>
<pin name="SCL" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="CAL" direction="in"/>
<pin name="LPF-" direction="in"/>
<pin name="LPF+" direction="in"/>
<pin name="M1_UNP" direction="in"/>
<pin name="M2_UNP" direction="in"/>
<pin name="GA0" direction="in"/>
<pin name="GA1" direction="in"/>
<pin name="GB0" direction="in"/>
<pin name="GB1" direction="in"/>
<pin name="T5" direction="in"/>
<pin name="T7" direction="in"/>
<pin name="MIC1-" direction="in"/>
<pin name="MIC1+" direction="in"/>
<pin name="MIC2-" direction="in"/>
<pin name="MIC2+" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC_6" direction="nc"/>
<pin name="NC_7" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="OUT+" direction="out"/>
<pin name="OUT-" direction="out"/>
<pin name="SDA"/>
<pin name="MICBIAS" direction="out"/>
</symbol>
<symbol name="LMV1089VY">
<pin name="VDD" direction="pwr"/>
<pin name="12CVDD" direction="pwr"/>
<pin name="MIC_BIAS" direction="in"/>
<pin name="PE" direction="in"/>
<pin name="CAL" direction="in"/>
<pin name="ADR" direction="in"/>
<pin name="SCL" direction="in"/>
<pin name="REF" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="T5" direction="in"/>
<pin name="T7" direction="in"/>
<pin name="MIC1+" direction="in"/>
<pin name="MIC1-" direction="in"/>
<pin name="MIC2+" direction="in"/>
<pin name="MIC2-" direction="in"/>
<pin name="LPF+" direction="in"/>
<pin name="LPF-" direction="in"/>
<pin name="GA0" direction="in"/>
<pin name="GA1" direction="in"/>
<pin name="GB0" direction="in"/>
<pin name="GB1" direction="in"/>
<pin name="M1_UNP" direction="in"/>
<pin name="M2_UNP" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="OUT-" direction="out"/>
<pin name="OUT+" direction="out"/>
<pin name="SDA"/>
</symbol>
<symbol name="LMV1090TL">
<pin name="VDD" direction="pwr"/>
<pin name="I2CVDD" direction="pwr"/>
<pin name="MIC1-" direction="in"/>
<pin name="MIC1+" direction="in"/>
<pin name="MIC2-" direction="in"/>
<pin name="MIC2+" direction="in"/>
<pin name="LPF+" direction="in"/>
<pin name="LPF-" direction="in"/>
<pin name="REF" direction="in"/>
<pin name="MICBIAS" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="SCL" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT+" direction="in"/>
<pin name="OUT-" direction="out"/>
<pin name="SDA"/>
</symbol>
<symbol name="LMV1091TM">
<pin name="VDD" direction="pwr"/>
<pin name="LPF+" direction="in"/>
<pin name="LPF-" direction="in"/>
<pin name="~SD" direction="in"/>
<pin name="GA0" direction="in"/>
<pin name="GA1" direction="in"/>
<pin name="GA2" direction="in"/>
<pin name="GA3" direction="in"/>
<pin name="GB0" direction="in"/>
<pin name="GB1" direction="in"/>
<pin name="GB2" direction="in"/>
<pin name="MIC1-" direction="in"/>
<pin name="MIC1+" direction="in"/>
<pin name="MIC2-" direction="in"/>
<pin name="MIC2+" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="MIC_BIAS" direction="out"/>
<pin name="MODE0" direction="in"/>
<pin name="MODE1" direction="in"/>
<pin name="MUTE1" direction="in"/>
<pin name="MUTE2" direction="in"/>
<pin name="REF" direction="in"/>
<pin name="OUT-" direction="out"/>
<pin name="OUT+" direction="out"/>
</symbol>
<symbol name="LMV112SD">
<pin name="VDD" direction="pwr"/>
<pin name="IN1" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="EN1" direction="in"/>
<pin name="EN2" direction="in"/>
<pin name="VSS" direction="pwr"/>
<pin name="EPAD" direction="pas"/>
<pin name="OUT1" direction="out"/>
<pin name="OUT2" direction="out"/>
</symbol>
<symbol name="LMV116MF">
<pin name="V+" direction="pwr"/>
<pin name="+IN" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LMV118MF">
<pin name="V+" direction="pwr"/>
<pin name="SD" direction="in"/>
<pin name="+IN_" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LMV2011MA">
<pin name="V+" direction="pwr"/>
<pin name="-VIN" direction="in"/>
<pin name="+VIN" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LMV2011MF">
<pin name="V+" direction="pwr"/>
<pin name="VIN+" direction="in"/>
<pin name="VIN-" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LMV301MG">
<pin name="V+" direction="pwr"/>
<pin name="+IN" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LMV321M5">
<pin name="V+" direction="pwr"/>
<pin name="+IN" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LMV321M7">
<pin name="V+" direction="pwr"/>
<pin name="+IN" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LMV324M">
<pin name="V+" direction="pwr"/>
<pin name="INA+" direction="in"/>
<pin name="INA-" direction="in"/>
<pin name="INB+" direction="in"/>
<pin name="INB-" direction="in"/>
<pin name="INC+" direction="in"/>
<pin name="INC-" direction="in"/>
<pin name="IND+" direction="in"/>
<pin name="IND-" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
<pin name="OUTC" direction="out"/>
<pin name="OUTD" direction="out"/>
</symbol>
<symbol name="LMV324MT">
<pin name="V+" direction="pwr"/>
<pin name="-INA" direction="in"/>
<pin name="+INA" direction="in"/>
<pin name="+INB" direction="in"/>
<pin name="-INB" direction="in"/>
<pin name="-INC" direction="in"/>
<pin name="+INC" direction="in"/>
<pin name="+IND" direction="in"/>
<pin name="-IND" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
<pin name="OUTC" direction="out"/>
<pin name="OUTD" direction="out"/>
</symbol>
<symbol name="LMV331M5">
<pin name="V+" direction="pwr"/>
<pin name="+IN" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LMV331M7">
<pin name="V+" direction="pwr"/>
<pin name="+IN" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LMV339M">
<pin name="V+" direction="pwr"/>
<pin name="INA-" direction="in"/>
<pin name="INA+" direction="in"/>
<pin name="INB-" direction="in"/>
<pin name="INB+" direction="in"/>
<pin name="INC-" direction="in"/>
<pin name="INC+" direction="in"/>
<pin name="IND-" direction="in"/>
<pin name="IND+" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
<pin name="OUTC" direction="out"/>
<pin name="OUTD" direction="out"/>
</symbol>
<symbol name="LMV339MT">
<pin name="V+" direction="pwr"/>
<pin name="-INA" direction="in"/>
<pin name="+INA" direction="in"/>
<pin name="-INB" direction="in"/>
<pin name="+INB" direction="in"/>
<pin name="-INC" direction="in"/>
<pin name="+INC" direction="in"/>
<pin name="+IND" direction="in"/>
<pin name="-IND" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
<pin name="OUTC" direction="out"/>
<pin name="OUTD" direction="out"/>
</symbol>
<symbol name="LMV341MG">
<pin name="V+" direction="pwr"/>
<pin name="~SHDN" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LMV342MA">
<pin name="V+" direction="pwr"/>
<pin name="-INA" direction="in"/>
<pin name="+INA" direction="in"/>
<pin name="+INB" direction="in"/>
<pin name="-INB" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="LMV342MM">
<pin name="V+" direction="pwr"/>
<pin name="-INA" direction="in"/>
<pin name="+INA" direction="in"/>
<pin name="+INB" direction="in"/>
<pin name="-INB" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="LMV344MA">
<pin name="V+" direction="pwr"/>
<pin name="-INA" direction="in"/>
<pin name="+INA" direction="in"/>
<pin name="+INB" direction="in"/>
<pin name="-INB" direction="in"/>
<pin name="-INC" direction="in"/>
<pin name="+INC" direction="in"/>
<pin name="+IND" direction="in"/>
<pin name="-IND" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
<pin name="OUTC" direction="out"/>
<pin name="OUTD" direction="out"/>
</symbol>
<symbol name="LMV344MT">
<pin name="V+" direction="pwr"/>
<pin name="-INA" direction="in"/>
<pin name="+INA" direction="in"/>
<pin name="+INB" direction="in"/>
<pin name="-INB" direction="in"/>
<pin name="-INC" direction="in"/>
<pin name="+INC" direction="in"/>
<pin name="+IND" direction="in"/>
<pin name="-IND" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
<pin name="OUTC" direction="out"/>
<pin name="OUTD" direction="out"/>
</symbol>
<symbol name="LMV358M">
<pin name="V+" direction="pwr"/>
<pin name="INA-" direction="in"/>
<pin name="INA+" direction="in"/>
<pin name="INB+" direction="in"/>
<pin name="INB-" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT_A" direction="out"/>
<pin name="OUT_B" direction="out"/>
</symbol>
<symbol name="LMV358MM">
<pin name="V+" direction="pwr"/>
<pin name="INA+" direction="in"/>
<pin name="INA-" direction="in"/>
<pin name="INB-" direction="in"/>
<pin name="INB+" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="LMV393M">
<pin name="V+" direction="pwr"/>
<pin name="IN_A-" direction="in"/>
<pin name="IN_B-" direction="in"/>
<pin name="IN_A+" direction="in"/>
<pin name="IN_B+" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="LMV393MM">
<pin name="V+" direction="pwr"/>
<pin name="INA+" direction="in"/>
<pin name="INA-" direction="in"/>
<pin name="INB-" direction="in"/>
<pin name="INB+" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="LMV431ACM5">
<pin name="ANODE" direction="pas"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="REF" direction="in"/>
<pin name="CATHODE" direction="pas"/>
</symbol>
<symbol name="LMV431BIMF">
<pin name="REF" direction="pas"/>
<pin name="ANODE" direction="pas"/>
<pin name="CATHODE" direction="pas"/>
</symbol>
<symbol name="LMV431CM5">
<pin name="REF" direction="in"/>
<pin name="ANODE" direction="pas"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="CATHODE" direction="pas"/>
</symbol>
<symbol name="LMV431IM5">
<pin name="ANODE" direction="pas"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="REF" direction="in"/>
<pin name="CATHODE" direction="pas"/>
</symbol>
<symbol name="LMV551MF">
<pin name="V+" direction="pwr"/>
<pin name="+IN" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LMV551MG">
<pin name="V+" direction="pwr"/>
<pin name="+IN" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LMV552MM">
<pin name="V+" direction="pwr"/>
<pin name="-INA" direction="in"/>
<pin name="+INA" direction="in"/>
<pin name="+INB" direction="in"/>
<pin name="-INB" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="LMV554MT">
<pin name="V+" direction="pwr"/>
<pin name="INA+" direction="in"/>
<pin name="INA-" direction="in"/>
<pin name="INB+" direction="in"/>
<pin name="INB-" direction="in"/>
<pin name="INC-" direction="in"/>
<pin name="INC+" direction="in"/>
<pin name="IND+" direction="in"/>
<pin name="IND-" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
<pin name="OUTC" direction="out"/>
<pin name="OUTD" direction="out"/>
</symbol>
<symbol name="LMV651MF">
<pin name="V+" direction="pwr"/>
<pin name="IN+" direction="in"/>
<pin name="IN-" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LMV651MG">
<pin name="V+" direction="pwr"/>
<pin name="+IN" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LMV652MM">
<pin name="V+" direction="pwr"/>
<pin name="INA-" direction="in"/>
<pin name="INA+" direction="in"/>
<pin name="INB-" direction="in"/>
<pin name="INB+" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="LMV654MT">
<pin name="V+" direction="pwr"/>
<pin name="-INA" direction="in"/>
<pin name="+INA" direction="in"/>
<pin name="+INB" direction="in"/>
<pin name="-INB" direction="in"/>
<pin name="-INC" direction="in"/>
<pin name="+INC" direction="in"/>
<pin name="+IND" direction="in"/>
<pin name="-IND" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
<pin name="OUTC" direction="out"/>
<pin name="OUTD" direction="out"/>
</symbol>
<symbol name="LMV710M5">
<pin name="V+" direction="pwr"/>
<pin name="IN+" direction="in"/>
<pin name="IN-" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LMV712MM">
<pin name="V+" direction="pwr"/>
<pin name="INA-" direction="in"/>
<pin name="INA+" direction="in"/>
<pin name="INB+" direction="in"/>
<pin name="INB-" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
<pin name="SDA"/>
<pin name="SDB"/>
</symbol>
<symbol name="LMV716MM">
<pin name="V+" direction="pwr"/>
<pin name="INA+" direction="in"/>
<pin name="INA-" direction="in"/>
<pin name="INB-" direction="in"/>
<pin name="INB+" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="LMV7219M5">
<pin name="V+" direction="pwr"/>
<pin name="NEG" direction="in"/>
<pin name="POS" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LMV7219M7">
<pin name="V+" direction="pwr"/>
<pin name="POS" direction="in"/>
<pin name="NEG" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LMV721M5">
<pin name="V+" direction="pwr"/>
<pin name="VIN+" direction="in"/>
<pin name="VIN-" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LMV721M7">
<pin name="V+" direction="pwr"/>
<pin name="VIN+" direction="in"/>
<pin name="VIN-" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LMV722M">
<pin name="V+" direction="pwr"/>
<pin name="-INA" direction="in"/>
<pin name="+INA" direction="in"/>
<pin name="+INB" direction="in"/>
<pin name="-INB" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="LMV722MM">
<pin name="V+" direction="pwr"/>
<pin name="+INA" direction="in"/>
<pin name="-INA" direction="in"/>
<pin name="-INB" direction="in"/>
<pin name="+INB" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="LMV7235M5">
<pin name="V+" direction="pwr"/>
<pin name="POS" direction="in"/>
<pin name="NEG" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LMV7235M7">
<pin name="V+" direction="pwr"/>
<pin name="POS" direction="in"/>
<pin name="NEG" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LMV7239M5">
<pin name="V+" direction="pwr"/>
<pin name="NEG" direction="in"/>
<pin name="POS" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LMV7239M7">
<pin name="V+" direction="pwr"/>
<pin name="POS" direction="in"/>
<pin name="NEG" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LMV7271MF">
<pin name="V+" direction="pwr"/>
<pin name="+IN" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LMV7271MG">
<pin name="V+" direction="pwr"/>
<pin name="+IN" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LMV7275MF">
<pin name="V+" direction="pwr"/>
<pin name="+IN" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LMV7275MG">
<pin name="V+" direction="pwr"/>
<pin name="+IN" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LMV7291MG">
<pin name="V+" direction="pwr"/>
<pin name="+IN" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LMV751M5">
<pin name="V+" direction="pwr"/>
<pin name="VIN+" direction="in"/>
<pin name="VIN-" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LMV761MA">
<pin name="V+" direction="pwr"/>
<pin name="-IN" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="~SD" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LMV761MF">
<pin name="V-" direction="pwr"/>
<pin name="~SD" direction="in"/>
<pin name="IN+" direction="in"/>
<pin name="IN-" direction="in"/>
<pin name="V+" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LMV762MA">
<pin name="V+" direction="pwr"/>
<pin name="IN_A-" direction="in"/>
<pin name="IN_A+" direction="in"/>
<pin name="IN_B+" direction="in"/>
<pin name="IN_B-" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT_A" direction="out"/>
<pin name="OUT_B" direction="out"/>
</symbol>
<symbol name="LMV762MM">
<pin name="V+" direction="pwr"/>
<pin name="INA-" direction="in"/>
<pin name="INA+" direction="in"/>
<pin name="INB-" direction="in"/>
<pin name="INB+" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="LMV771MG">
<pin name="V+" direction="pwr"/>
<pin name="+IN" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LMV772MA">
<pin name="V+" direction="pwr"/>
<pin name="-INA" direction="in"/>
<pin name="+INA" direction="in"/>
<pin name="+INB" direction="in"/>
<pin name="-INB" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="LMV772MM">
<pin name="V+" direction="pwr"/>
<pin name="INA-" direction="in"/>
<pin name="INA+" direction="in"/>
<pin name="INB-" direction="in"/>
<pin name="INB+" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="LMV774MT">
<pin name="V+" direction="pwr"/>
<pin name="-INA" direction="in"/>
<pin name="+INA" direction="in"/>
<pin name="+INB" direction="in"/>
<pin name="-INB" direction="in"/>
<pin name="-INC" direction="in"/>
<pin name="+INC" direction="in"/>
<pin name="+IND" direction="in"/>
<pin name="-IND" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
<pin name="OUTC" direction="out"/>
<pin name="OUTD" direction="out"/>
</symbol>
<symbol name="LMV791MK">
<pin name="V+" direction="pwr"/>
<pin name="EN" direction="in"/>
<pin name="IN+" direction="in"/>
<pin name="IN-" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LMV792MM">
<pin name="V+" direction="pwr"/>
<pin name="ENA" direction="in"/>
<pin name="ENB" direction="in"/>
<pin name="INA-" direction="in"/>
<pin name="INA+" direction="in"/>
<pin name="INB+" direction="in"/>
<pin name="INB-" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="LMV793MA">
<pin name="V+" direction="pwr"/>
<pin name="+IN" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LMV793MF">
<pin name="V+" direction="pwr"/>
<pin name="+IN" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LMV794MA">
<pin name="V+" direction="pwr"/>
<pin name="+IN" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LMV794MM">
<pin name="V+" direction="pwr"/>
<pin name="INA+" direction="in"/>
<pin name="INA-" direction="in"/>
<pin name="INB-" direction="in"/>
<pin name="INB+" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="LMV796MF">
<pin name="V+" direction="pwr"/>
<pin name="+IN" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LMV797MM">
<pin name="V+" direction="pwr"/>
<pin name="INA+" direction="in"/>
<pin name="INA-" direction="in"/>
<pin name="INB-" direction="in"/>
<pin name="INB+" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="LMV821M5">
<pin name="V+" direction="pwr"/>
<pin name="+IN" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LMV821M7">
<pin name="V+" direction="pwr"/>
<pin name="+IN" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LMV822M">
<pin name="V+" direction="pwr"/>
<pin name="-IN_A" direction="in"/>
<pin name="+IN_A" direction="in"/>
<pin name="+IN_B" direction="in"/>
<pin name="-IN_B" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="LMV822MM">
<pin name="V+" direction="pwr"/>
<pin name="INA+" direction="in"/>
<pin name="INA-" direction="in"/>
<pin name="INB-" direction="in"/>
<pin name="INB+" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="LMV824M">
<pin name="V+" direction="pwr"/>
<pin name="-INA" direction="in"/>
<pin name="+INA" direction="in"/>
<pin name="+INB" direction="in"/>
<pin name="-INB" direction="in"/>
<pin name="-INC" direction="in"/>
<pin name="+INC" direction="in"/>
<pin name="+IND" direction="in"/>
<pin name="-IND" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
<pin name="OUTC" direction="out"/>
<pin name="OUTD" direction="out"/>
</symbol>
<symbol name="LMV824MT">
<pin name="V+" direction="pwr"/>
<pin name="INA+" direction="in"/>
<pin name="INA-" direction="in"/>
<pin name="INB+" direction="in"/>
<pin name="INB-" direction="in"/>
<pin name="INC-" direction="in"/>
<pin name="INC+" direction="in"/>
<pin name="IND+" direction="in"/>
<pin name="IND-" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
<pin name="OUTC" direction="out"/>
<pin name="OUTD" direction="out"/>
</symbol>
<symbol name="LMV831MG">
<pin name="V-" direction="pwr"/>
<pin name="IN-" direction="in"/>
<pin name="IN+" direction="in"/>
<pin name="V+" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LMV832MM">
<pin name="V+" direction="pwr"/>
<pin name="INA-" direction="in"/>
<pin name="INA+" direction="in"/>
<pin name="INB-" direction="in"/>
<pin name="INB+" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="LMV834MT">
<pin name="V+" direction="pwr"/>
<pin name="INA-" direction="in"/>
<pin name="INA+" direction="in"/>
<pin name="INB-" direction="in"/>
<pin name="INB+" direction="in"/>
<pin name="INC-" direction="in"/>
<pin name="INC+" direction="in"/>
<pin name="IND-" direction="in"/>
<pin name="IND+" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
<pin name="OUTC" direction="out"/>
<pin name="OUTD" direction="out"/>
</symbol>
<symbol name="LMV841MG">
<pin name="V+" direction="pwr"/>
<pin name="+IN" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LMV842MA">
<pin name="V+" direction="pwr"/>
<pin name="IN_A+" direction="in"/>
<pin name="IN_A-" direction="in"/>
<pin name="INB-" direction="in"/>
<pin name="INB+" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="LMV842MM">
<pin name="V+" direction="pwr"/>
<pin name="INA+" direction="in"/>
<pin name="INA-" direction="in"/>
<pin name="INB-" direction="in"/>
<pin name="INB+" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="LMV842QMA">
<pin name="V+" direction="pwr"/>
<pin name="IN_A+" direction="in"/>
<pin name="IN_A-" direction="in"/>
<pin name="INB-" direction="in"/>
<pin name="INB+" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="LMV842QMM">
<pin name="V+" direction="pwr"/>
<pin name="INA+" direction="in"/>
<pin name="INA-" direction="in"/>
<pin name="INB-" direction="in"/>
<pin name="INB+" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="LMV844MA">
<pin name="V+" direction="pwr"/>
<pin name="-INA" direction="in"/>
<pin name="+INA" direction="in"/>
<pin name="+INB" direction="in"/>
<pin name="-INB" direction="in"/>
<pin name="-INC" direction="in"/>
<pin name="+INC" direction="in"/>
<pin name="+IND" direction="in"/>
<pin name="-IND" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
<pin name="OUTC" direction="out"/>
<pin name="OUTD" direction="out"/>
</symbol>
<symbol name="LMV844MT">
<pin name="V+" direction="pwr"/>
<pin name="-INA" direction="in"/>
<pin name="+INA" direction="in"/>
<pin name="+INB" direction="in"/>
<pin name="-INB" direction="in"/>
<pin name="-INC" direction="in"/>
<pin name="+INC" direction="in"/>
<pin name="+IND" direction="in"/>
<pin name="-IND" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
<pin name="OUTC" direction="out"/>
<pin name="OUTD" direction="out"/>
</symbol>
<symbol name="LMV844QMA">
<pin name="V+" direction="pwr"/>
<pin name="-INA" direction="in"/>
<pin name="+INA" direction="in"/>
<pin name="+INB" direction="in"/>
<pin name="-INB" direction="in"/>
<pin name="-INC" direction="in"/>
<pin name="+INC" direction="in"/>
<pin name="+IND" direction="in"/>
<pin name="-IND" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
<pin name="OUTC" direction="out"/>
<pin name="OUTD" direction="out"/>
</symbol>
<symbol name="LMV851MG">
<pin name="V+" direction="pwr"/>
<pin name="+IN" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LMV852MM">
<pin name="V+" direction="pwr"/>
<pin name="INA+" direction="in"/>
<pin name="INA-" direction="in"/>
<pin name="INB-" direction="in"/>
<pin name="INB+" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="LMV854MT">
<pin name="V+" direction="pwr"/>
<pin name="INA-" direction="in"/>
<pin name="INA+" direction="in"/>
<pin name="INB+" direction="in"/>
<pin name="INB-" direction="in"/>
<pin name="INC-" direction="in"/>
<pin name="INC+" direction="in"/>
<pin name="IND+" direction="in"/>
<pin name="IND-" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
<pin name="OUTC" direction="out"/>
<pin name="OUTD" direction="out"/>
</symbol>
<symbol name="LMV861MG">
<pin name="V+" direction="pwr"/>
<pin name="IN+" direction="in"/>
<pin name="IN-" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LMV862MM">
<pin name="V+" direction="pwr"/>
<pin name="INA+" direction="in"/>
<pin name="INA-" direction="in"/>
<pin name="INB-" direction="in"/>
<pin name="INB+" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="LMV931MF">
<pin name="V+" direction="pwr"/>
<pin name="+IN" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LMV931MG">
<pin name="V+" direction="pwr"/>
<pin name="IN+" direction="in"/>
<pin name="IN-" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LMV932MA">
<pin name="V+" direction="pwr"/>
<pin name="-INA" direction="in"/>
<pin name="+INA" direction="in"/>
<pin name="+INB" direction="in"/>
<pin name="-INB" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="LMV932MM">
<pin name="V+" direction="pwr"/>
<pin name="IN_A-" direction="in"/>
<pin name="IN_A+" direction="in"/>
<pin name="IN_B+" direction="in"/>
<pin name="IN_B-" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT_A" direction="out"/>
<pin name="OUT_B" direction="out"/>
</symbol>
<symbol name="LMV934MA">
<pin name="V+" direction="pwr"/>
<pin name="-INA" direction="in"/>
<pin name="+INA" direction="in"/>
<pin name="+INB" direction="in"/>
<pin name="-INB" direction="in"/>
<pin name="-INC" direction="in"/>
<pin name="+INC" direction="in"/>
<pin name="+IND" direction="in"/>
<pin name="-IND" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
<pin name="OUTC" direction="out"/>
<pin name="OUTD" direction="out"/>
</symbol>
<symbol name="LMV934MT">
<pin name="V+" direction="pwr"/>
<pin name="INA-" direction="in"/>
<pin name="INA+" direction="in"/>
<pin name="INB+" direction="in"/>
<pin name="INB-" direction="in"/>
<pin name="INC-" direction="in"/>
<pin name="INC+" direction="in"/>
<pin name="IND+" direction="in"/>
<pin name="IND-" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
<pin name="OUTC" direction="out"/>
<pin name="OUTD" direction="out"/>
</symbol>
<symbol name="LMV951MK">
<pin name="V+" direction="pwr"/>
<pin name="+IN" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="SD" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LMV981MF">
<pin name="VDD" direction="pwr"/>
<pin name="+IN" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="~SHDN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LMV981MG">
<pin name="VDD" direction="pwr"/>
<pin name="~SHDN" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LMV982MM">
<pin name="V+" direction="pwr"/>
<pin name="~SHDN_A" direction="in"/>
<pin name="~SHDN_B" direction="in"/>
<pin name="-INA" direction="in"/>
<pin name="+INA" direction="in"/>
<pin name="+INB" direction="in"/>
<pin name="-INB" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="LP2902M">
<pin name="V+" direction="pwr"/>
<pin name="-INA" direction="in"/>
<pin name="+INA" direction="in"/>
<pin name="+INB" direction="in"/>
<pin name="-INB" direction="in"/>
<pin name="-INC" direction="in"/>
<pin name="+INC" direction="in"/>
<pin name="+IND" direction="in"/>
<pin name="-IND" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
<pin name="OUTC" direction="out"/>
<pin name="OUTD" direction="out"/>
</symbol>
<symbol name="LP2951ACM">
<pin name="IN" direction="in"/>
<pin name="SEN" direction="pas"/>
<pin name="SD" direction="in"/>
<pin name="~ERR" direction="out"/>
<pin name="VTAP" direction="pas"/>
<pin name="FB" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LP2951ACN">
<pin name="IN" direction="pwr"/>
<pin name="SEN" direction="in"/>
<pin name="SD" direction="in"/>
<pin name="~ERROR" direction="in"/>
<pin name="VTAP" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LP2951ACSD-3.3">
<pin name="IN" direction="in"/>
<pin name="SEN"/>
<pin name="SD" direction="pas"/>
<pin name="~ERR" direction="pas"/>
<pin name="VTAP" direction="pas"/>
<pin name="FB" direction="pas"/>
<pin name="DAP" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LP2951CMM">
<pin name="IN" direction="pwr"/>
<pin name="VTAP" direction="pas"/>
<pin name="FB" direction="in"/>
<pin name="SHDN" direction="in"/>
<pin name="SENSE" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
<pin name="~ERROR" direction="out"/>
</symbol>
<symbol name="LP2951CSD-3.3">
<pin name="IN" direction="in"/>
<pin name="VTAP" direction="in"/>
<pin name="SEN" direction="in"/>
<pin name="SD" direction="in"/>
<pin name="~ERR" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LP2951CSD">
<pin name="IN" direction="in"/>
<pin name="VTAP" direction="in"/>
<pin name="SEN" direction="in"/>
<pin name="SD" direction="in"/>
<pin name="~ERR" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LP2952IM">
<pin name="REF" direction="pwr"/>
<pin name="V_TAP" direction="pas"/>
<pin name="FB" direction="in"/>
<pin name="IN" direction="in"/>
<pin name="SEN" direction="in"/>
<pin name="~SD" direction="in"/>
<pin name="~ERR" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LP2980AIM5-3.0">
<pin name="VIN" direction="pwr"/>
<pin name="ON/OFF" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP2980AIM5-3.3">
<pin name="VIN" direction="pwr"/>
<pin name="ON/OFF" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP2980AIM5-5.0">
<pin name="VIN" direction="pwr"/>
<pin name="ON/OFF" direction="in"/>
<pin name="N/C" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP2980IM5-3.0">
<pin name="VIN" direction="pwr"/>
<pin name="ON/OFF" direction="in"/>
<pin name="N/C" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP2980IM5-3.3">
<pin name="VIN" direction="pwr"/>
<pin name="ON/OFF" direction="in"/>
<pin name="N/C" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP2980IM5-5.0">
<pin name="VIN" direction="pwr"/>
<pin name="ON/OFF" direction="in"/>
<pin name="N/C" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP2982AIM5-3.0">
<pin name="VIN" direction="pwr"/>
<pin name="ON/~OFF" direction="in"/>
<pin name="BYPASS" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP2982AIM5-3.3">
<pin name="VIN" direction="pwr"/>
<pin name="ON/~OFF" direction="in"/>
<pin name="BYPASS" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP2982AIM5-5.0">
<pin name="VIN" direction="pwr"/>
<pin name="ON/~OFF" direction="in"/>
<pin name="BYPASS" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP2982IM5-3.3">
<pin name="VIN" direction="pwr"/>
<pin name="ON/~OFF" direction="in"/>
<pin name="BYPASS" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP2982IM5-5.0">
<pin name="VIN" direction="pwr"/>
<pin name="ON/OFF" direction="in"/>
<pin name="BYPASS" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP2985AIM5-2.5">
<pin name="VIN" direction="pwr"/>
<pin name="ON/OFF" direction="in"/>
<pin name="BYPASS" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP2985AIM5-2.7">
<pin name="VIN" direction="pwr"/>
<pin name="ON/OFF" direction="in"/>
<pin name="BP" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP2985AIM5-2.8">
<pin name="VIN" direction="pwr"/>
<pin name="ON/OFF" direction="in"/>
<pin name="BP" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP2985AIM5-3.0">
<pin name="VIN" direction="pwr"/>
<pin name="ON/OFF" direction="in"/>
<pin name="BYPASS" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP2985AIM5-3.3">
<pin name="VIN" direction="pwr"/>
<pin name="ON/OFF" direction="in"/>
<pin name="BYPASS" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP2985AIM5-3.6">
<pin name="VIN" direction="pwr"/>
<pin name="ON/OFF" direction="in"/>
<pin name="BP" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP2985AIM5-3.8">
<pin name="VIN" direction="pwr"/>
<pin name="ON/OFF" direction="in"/>
<pin name="BP" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP2985AIM5-4.0">
<pin name="VIN" direction="pwr"/>
<pin name="ON/OFF" direction="in"/>
<pin name="BP" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP2985AIM5-4.5">
<pin name="VIN" direction="pwr"/>
<pin name="ON/OFF" direction="in"/>
<pin name="BP" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP2985AIM5-5.0">
<pin name="VIN" direction="pwr"/>
<pin name="ON/OFF" direction="in"/>
<pin name="BY_PASS" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP2985AIM5-6.1">
<pin name="VIN" direction="pwr"/>
<pin name="ON/OFF" direction="in"/>
<pin name="BP" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP2985AITP-2.8">
<pin name="VIN" direction="in"/>
<pin name="ON-OFF" direction="pas"/>
<pin name="BP" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP2985AITP-3.3">
<pin name="VIN" direction="in"/>
<pin name="ON-OFF" direction="pas"/>
<pin name="BP" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP2985AITP-5.0">
<pin name="VIN" direction="pwr"/>
<pin name="ON/OFF" direction="in"/>
<pin name="BYPASS" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP2985IM5-2.5">
<pin name="VIN" direction="pwr"/>
<pin name="ON/OFF" direction="in"/>
<pin name="BYPASS" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP2985IM5-2.8">
<pin name="VIN" direction="pwr"/>
<pin name="ON/OFF" direction="in"/>
<pin name="BP" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP2985IM5-3.0">
<pin name="VIN" direction="pwr"/>
<pin name="ON/OFF" direction="in"/>
<pin name="BYPASS" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP2985IM5-3.1">
<pin name="VIN" direction="pwr"/>
<pin name="ON/OFF" direction="in"/>
<pin name="BP" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP2985IM5-3.2">
<pin name="VIN" direction="pwr"/>
<pin name="ON/OFF" direction="in"/>
<pin name="BP" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP2985IM5-3.3">
<pin name="VIN" direction="pwr"/>
<pin name="ON/OFF" direction="in"/>
<pin name="BYPASS" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP2985IM5-3.6">
<pin name="VIN" direction="pwr"/>
<pin name="ON/OFF" direction="in"/>
<pin name="BP" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP2985IM5-3.8">
<pin name="VIN" direction="pwr"/>
<pin name="ON/OFF" direction="in"/>
<pin name="BP" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP2985IM5-4.0">
<pin name="VIN" direction="pwr"/>
<pin name="ON/OFF" direction="in"/>
<pin name="BP" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP2985IM5-4.5">
<pin name="VIN" direction="pwr"/>
<pin name="ON/OFF" direction="in"/>
<pin name="BP" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP2985IM5-5.0">
<pin name="VIN" direction="pwr"/>
<pin name="ON/OFF" direction="in"/>
<pin name="BYPASS" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP2985IM5-6.1">
<pin name="VIN" direction="pwr"/>
<pin name="ON/OFF" direction="in"/>
<pin name="BP" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP2986AILD-3.3">
<pin name="IN" direction="pwr"/>
<pin name="FB" direction="in"/>
<pin name="TAP" direction="in"/>
<pin name="SENSE" direction="in"/>
<pin name="~ERROR" direction="in"/>
<pin name="~SD" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="HEAT_PAD" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LP2986AIM-3.0">
<pin name="IN" direction="pwr"/>
<pin name="FB" direction="in"/>
<pin name="TAP" direction="in"/>
<pin name="SENSE" direction="in"/>
<pin name="~ERROR" direction="in"/>
<pin name="~SD" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LP2986AIM-3.3">
<pin name="IN" direction="pwr"/>
<pin name="FB" direction="in"/>
<pin name="TAP" direction="in"/>
<pin name="SENSE" direction="in"/>
<pin name="~ERROR" direction="in"/>
<pin name="~SD" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LP2986AIM-5.0">
<pin name="IN" direction="in"/>
<pin name="FDBK" direction="pas"/>
<pin name="SEN" direction="pas"/>
<pin name="~SD" direction="in"/>
<pin name="TAP" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
<pin name="~ERR" direction="pas"/>
</symbol>
<symbol name="LP2986AIMM-3.0">
<pin name="IN" direction="pwr"/>
<pin name="FB" direction="in"/>
<pin name="TAP" direction="in"/>
<pin name="SENSE" direction="in"/>
<pin name="~ERROR" direction="in"/>
<pin name="~SD" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LP2986AIMM-3.3">
<pin name="IN" direction="in"/>
<pin name="SEN" direction="in"/>
<pin name="TAP" direction="pas"/>
<pin name="~SD" direction="pas"/>
<pin name="FEEDBACK" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
<pin name="~ERR" direction="out"/>
</symbol>
<symbol name="LP2986AIMM-5.0">
<pin name="IN" direction="in"/>
<pin name="SEN" direction="in"/>
<pin name="TAP" direction="pas"/>
<pin name="~SD" direction="pas"/>
<pin name="FEEDBACK" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
<pin name="~ERR" direction="out"/>
</symbol>
<symbol name="LP2986ILD-3.3">
<pin name="IN" direction="pwr"/>
<pin name="FB" direction="in"/>
<pin name="TAP" direction="in"/>
<pin name="SENSE" direction="in"/>
<pin name="~ERROR" direction="in"/>
<pin name="~SD" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="HEAT_PAD" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LP2986IM-3.0">
<pin name="IN" direction="pwr"/>
<pin name="FB" direction="in"/>
<pin name="TAP" direction="in"/>
<pin name="SENSE" direction="in"/>
<pin name="~ERROR" direction="in"/>
<pin name="~SD" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LP2986IM-3.3">
<pin name="IN" direction="pwr"/>
<pin name="FB" direction="in"/>
<pin name="TAP" direction="in"/>
<pin name="SENSE" direction="in"/>
<pin name="~ERROR" direction="in"/>
<pin name="~SD" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LP2986IM-5.0">
<pin name="IN" direction="pwr"/>
<pin name="FB" direction="in"/>
<pin name="TAP" direction="in"/>
<pin name="SENSE" direction="in"/>
<pin name="~ERROR" direction="in"/>
<pin name="~SD" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LP2986IMM-3.0">
<pin name="IN" direction="pwr"/>
<pin name="FB" direction="in"/>
<pin name="TAP" direction="in"/>
<pin name="SENSE" direction="in"/>
<pin name="~ERROR" direction="in"/>
<pin name="~SD" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LP2986IMM-3.3">
<pin name="IN" direction="pwr"/>
<pin name="FB" direction="in"/>
<pin name="TAP" direction="in"/>
<pin name="SENSE" direction="in"/>
<pin name="~ERROR" direction="in"/>
<pin name="~SD" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LP2986IMM-5.0">
<pin name="IN" direction="pwr"/>
<pin name="FB" direction="in"/>
<pin name="TAP" direction="in"/>
<pin name="SENSE" direction="in"/>
<pin name="~ERROR" direction="in"/>
<pin name="~SD" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LP2987AILD-5.0">
<pin name="INPUT" direction="pwr"/>
<pin name="DELAY" direction="in"/>
<pin name="SENSE" direction="in"/>
<pin name="~ERROR" direction="in"/>
<pin name="~SHUTDOWN" direction="in"/>
<pin name="HEATPAD" direction="pas"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="OUTPUT" direction="out"/>
</symbol>
<symbol name="LP2988AIM-5.0">
<pin name="INPUT" direction="pwr"/>
<pin name="DELAY" direction="in"/>
<pin name="SENSE" direction="in"/>
<pin name="~ERROR" direction="in"/>
<pin name="~SHUTDOWN" direction="in"/>
<pin name="BYPASS" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUTPUT" direction="out"/>
</symbol>
<symbol name="LP2988AIMM-3.0">
<pin name="INPUT" direction="pwr"/>
<pin name="BYPASS" direction="in"/>
<pin name="DELAY" direction="in"/>
<pin name="SENSE" direction="in"/>
<pin name="~ERROR" direction="in"/>
<pin name="~SHUTDOWN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUTPUT" direction="out"/>
</symbol>
<symbol name="LP2988AIMM-3.3">
<pin name="INPUT" direction="pwr"/>
<pin name="BYPASS" direction="in"/>
<pin name="DELAY" direction="in"/>
<pin name="SENSE" direction="in"/>
<pin name="~ERROR" direction="in"/>
<pin name="~SHUTDOWN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUTPUT" direction="out"/>
</symbol>
<symbol name="LP2988AIMM-5.0">
<pin name="INPUT" direction="pwr"/>
<pin name="BYPASS" direction="in"/>
<pin name="DELAY" direction="in"/>
<pin name="SENSE" direction="in"/>
<pin name="~ERROR" direction="in"/>
<pin name="~SHUTDOWN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUTPUT" direction="out"/>
</symbol>
<symbol name="LP2988ILD-3.0">
<pin name="INPUT" direction="pwr"/>
<pin name="DELAY" direction="in"/>
<pin name="SENSE" direction="in"/>
<pin name="~ERROR" direction="in"/>
<pin name="~SHUTDOWN" direction="in"/>
<pin name="HEATPAD" direction="pas"/>
<pin name="BYPASS" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUTPUT" direction="out"/>
</symbol>
<symbol name="LP2988ILD-3.3">
<pin name="INPUT" direction="pwr"/>
<pin name="DELAY" direction="in"/>
<pin name="SENSE" direction="in"/>
<pin name="~ERROR" direction="in"/>
<pin name="~SHUTDOWN" direction="in"/>
<pin name="HEATPAD" direction="pas"/>
<pin name="BYPASS" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUTPUT" direction="out"/>
</symbol>
<symbol name="LP2988ILD-5.0">
<pin name="INPUT" direction="pwr"/>
<pin name="DELAY" direction="in"/>
<pin name="SENSE" direction="in"/>
<pin name="~ERROR" direction="in"/>
<pin name="~SHUTDOWN" direction="in"/>
<pin name="HEATPAD" direction="pas"/>
<pin name="BYPASS" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUTPUT" direction="out"/>
</symbol>
<symbol name="LP2988IM-5.0">
<pin name="INPUT" direction="pwr"/>
<pin name="DELAY" direction="in"/>
<pin name="SENSE" direction="in"/>
<pin name="~ERROR" direction="in"/>
<pin name="~SHUTDOWN" direction="in"/>
<pin name="BYPASS" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUTPUT" direction="out"/>
</symbol>
<symbol name="LP2988IMM-3.0">
<pin name="INPUT" direction="pwr"/>
<pin name="BYPASS" direction="in"/>
<pin name="DELAY" direction="in"/>
<pin name="SENSE" direction="in"/>
<pin name="~ERROR" direction="in"/>
<pin name="~SHUTDOWN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUTPUT" direction="out"/>
</symbol>
<symbol name="LP2988IMM-3.3">
<pin name="INPUT" direction="pwr"/>
<pin name="BYPASS" direction="in"/>
<pin name="DELAY" direction="in"/>
<pin name="SENSE" direction="in"/>
<pin name="~ERROR" direction="in"/>
<pin name="~SHUTDOWN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUTPUT" direction="out"/>
</symbol>
<symbol name="LP2988IMM-5.0">
<pin name="INPUT" direction="pwr"/>
<pin name="BYPASS" direction="in"/>
<pin name="DELAY" direction="in"/>
<pin name="SENSE" direction="in"/>
<pin name="~ERROR" direction="in"/>
<pin name="~SHUTDOWN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUTPUT" direction="out"/>
</symbol>
<symbol name="LP2989AILD-3.0">
<pin name="INPUT" direction="pwr"/>
<pin name="SENSE" direction="in"/>
<pin name="~ERROR" direction="in"/>
<pin name="BYPASS" direction="in"/>
<pin name="~SHUTDOWN" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="HEATPAD" direction="pas"/>
<pin name="OUTPUT" direction="out"/>
</symbol>
<symbol name="LP2989AILD-3.3">
<pin name="INPUT" direction="pwr"/>
<pin name="SENSE" direction="in"/>
<pin name="~ERROR" direction="in"/>
<pin name="BYPASS" direction="in"/>
<pin name="~SHUTDOWN" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="HEATPAD" direction="pas"/>
<pin name="OUTPUT" direction="out"/>
</symbol>
<symbol name="LP2989AILD-5.0">
<pin name="INPUT" direction="pwr"/>
<pin name="SENSE" direction="in"/>
<pin name="~ERROR" direction="in"/>
<pin name="BYPASS" direction="in"/>
<pin name="~SHUTDOWN" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="HEATPAD" direction="pas"/>
<pin name="OUTPUT" direction="out"/>
</symbol>
<symbol name="LP2989AIM-1.8">
<pin name="INPUT" direction="pwr"/>
<pin name="BYPASS" direction="in"/>
<pin name="~SHUTDOWN" direction="in"/>
<pin name="SENSE" direction="in"/>
<pin name="~ERROR" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="OUTPUT" direction="out"/>
</symbol>
<symbol name="LP2989AIM-2.5">
<pin name="INPUT" direction="pwr"/>
<pin name="BYPASS" direction="in"/>
<pin name="~SHUTDOWN" direction="in"/>
<pin name="SENSE" direction="in"/>
<pin name="~ERROR" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="OUTPUT" direction="out"/>
</symbol>
<symbol name="LP2989AIM-3.3">
<pin name="INPUT" direction="pwr"/>
<pin name="BYPASS" direction="in"/>
<pin name="~SHUTDOWN" direction="in"/>
<pin name="SENSE" direction="in"/>
<pin name="~ERROR" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="OUTPUT" direction="out"/>
</symbol>
<symbol name="LP2989AIM-5.0">
<pin name="INPUT" direction="pwr"/>
<pin name="SENSE" direction="in"/>
<pin name="~SHUTDOWN" direction="in"/>
<pin name="BYPASS" direction="pas"/>
<pin name="N/C" direction="nc"/>
<pin name="GROUND" direction="pas"/>
<pin name="OUTPUT" direction="out"/>
<pin name="~ERROR" direction="out"/>
</symbol>
<symbol name="LP2989AIMM-3.3">
<pin name="INPUT" direction="pwr"/>
<pin name="BYPASS" direction="in"/>
<pin name="SENSE" direction="in"/>
<pin name="~ERROR" direction="in"/>
<pin name="~SHUTDOWN" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="OUTPUT" direction="out"/>
</symbol>
<symbol name="LP2989AIMM-5.0">
<pin name="INPUT" direction="pwr"/>
<pin name="BYPASS" direction="in"/>
<pin name="SENSE" direction="in"/>
<pin name="~ERROR" direction="in"/>
<pin name="~SHUTDOWN" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="OUTPUT" direction="out"/>
</symbol>
<symbol name="LP2989ILD-3.0">
<pin name="INPUT" direction="pwr"/>
<pin name="SENSE" direction="in"/>
<pin name="~ERROR" direction="in"/>
<pin name="BYPASS" direction="in"/>
<pin name="~SHUTDOWN" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="HEATPAD" direction="pas"/>
<pin name="OUTPUT" direction="out"/>
</symbol>
<symbol name="LP2989ILD-3.3">
<pin name="INPUT" direction="pwr"/>
<pin name="SENSE" direction="in"/>
<pin name="~ERROR" direction="in"/>
<pin name="BYPASS" direction="in"/>
<pin name="~SHUTDOWN" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="HEATPAD" direction="pas"/>
<pin name="OUTPUT" direction="out"/>
</symbol>
<symbol name="LP2989IM-1.8">
<pin name="INPUT" direction="pwr"/>
<pin name="BYPASS" direction="in"/>
<pin name="~SHUTDOWN" direction="in"/>
<pin name="SENSE" direction="in"/>
<pin name="~ERROR" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="OUTPUT" direction="out"/>
</symbol>
<symbol name="LP2989IM-2.5">
<pin name="VIN" direction="pwr"/>
<pin name="BYPASS" direction="in"/>
<pin name="SENSE" direction="in"/>
<pin name="~ERROR" direction="in"/>
<pin name="~SD" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP2989IM-3.3">
<pin name="VIN" direction="pwr"/>
<pin name="BYPASS" direction="in"/>
<pin name="SENSE" direction="in"/>
<pin name="~ERROR" direction="in"/>
<pin name="~SD" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP2989IM-5.0">
<pin name="VIN" direction="pwr"/>
<pin name="BYPASS" direction="in"/>
<pin name="SENSE" direction="in"/>
<pin name="~ERROR" direction="in"/>
<pin name="~SD" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP2989IMM-3.0">
<pin name="INPUT" direction="pwr"/>
<pin name="BYPASS" direction="in"/>
<pin name="SENSE" direction="in"/>
<pin name="~ERROR" direction="in"/>
<pin name="~SHUTDOWN" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="OUTPUT" direction="out"/>
</symbol>
<symbol name="LP2989IMM-3.3">
<pin name="INPUT" direction="pwr"/>
<pin name="BYPASS" direction="in"/>
<pin name="SENSE" direction="in"/>
<pin name="~ERROR" direction="in"/>
<pin name="~SHUTDOWN" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="OUTPUT" direction="out"/>
</symbol>
<symbol name="LP2989IMM-5.0">
<pin name="INPUT" direction="pwr"/>
<pin name="BYPASS" direction="in"/>
<pin name="SENSE" direction="in"/>
<pin name="~ERROR" direction="in"/>
<pin name="~SHUTDOWN" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="OUTPUT" direction="out"/>
</symbol>
<symbol name="LP2992AILD-3.3">
<pin name="VIN" direction="in"/>
<pin name="BYP" direction="in"/>
<pin name="ON/~OFF" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP2992AILD-5.0">
<pin name="VIN" direction="in"/>
<pin name="BYP" direction="in"/>
<pin name="ON/~OFF" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP2992AIM5-1.5">
<pin name="VIN" direction="pwr"/>
<pin name="ON/~OFF" direction="in"/>
<pin name="BYPASS" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP2992AIM5-1.8">
<pin name="VIN" direction="pwr"/>
<pin name="ON/~OFF" direction="in"/>
<pin name="BYPASS" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP2992AIM5-2.5">
<pin name="VIN" direction="pwr"/>
<pin name="ON/~OFF" direction="in"/>
<pin name="BYPASS" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP2992AIM5-3.3">
<pin name="VIN" direction="pwr"/>
<pin name="ON/~OFF" direction="in"/>
<pin name="BYPASS" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP2992AIM5-5.0">
<pin name="VIN" direction="pwr"/>
<pin name="ON/~OFF" direction="in"/>
<pin name="BYPASS" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP2992ILD-3.3">
<pin name="VIN" direction="pwr"/>
<pin name="BYPASS" direction="in"/>
<pin name="ON/~OFF" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="HEATPAD" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP2992ILD-5.0">
<pin name="VIN" direction="pwr"/>
<pin name="BYPASS" direction="in"/>
<pin name="ON/~OFF" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="HEATPAD" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP2992IM5-1.5">
<pin name="VIN" direction="pwr"/>
<pin name="ON/~OFF" direction="in"/>
<pin name="BYPASS" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP2992IM5-1.8">
<pin name="VIN" direction="pwr"/>
<pin name="ON/~OFF" direction="in"/>
<pin name="BYPASS" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP2992IM5-2.5">
<pin name="VIN" direction="pwr"/>
<pin name="ON/~OFF" direction="in"/>
<pin name="BYPASS" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP2992IM5-3.0">
<pin name="VIN" direction="pwr"/>
<pin name="ON/~OFF" direction="in"/>
<pin name="BYPASS" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP2992IM5-3.3">
<pin name="VIN" direction="pwr"/>
<pin name="ON/~OFF" direction="in"/>
<pin name="BYPASS" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP2992IM5-5.0">
<pin name="VIN" direction="pwr"/>
<pin name="ON/~OFF" direction="in"/>
<pin name="BYPASS" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP2995M">
<pin name="VDDQ" direction="in"/>
<pin name="AVIN" direction="in"/>
<pin name="PVIN" direction="in"/>
<pin name="VSENSE" direction="pas"/>
<pin name="VREF" direction="pas"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="VTT" direction="out"/>
</symbol>
<symbol name="LP2995MR">
<pin name="VDDQ" direction="pwr"/>
<pin name="VSENSE" direction="in"/>
<pin name="VREF" direction="in"/>
<pin name="PVIN" direction="in"/>
<pin name="AVIN" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="VTT" direction="out"/>
</symbol>
<symbol name="LP2996LQ">
<pin name="VDDQ" direction="pwr"/>
<pin name="~SD" direction="in"/>
<pin name="VSENSE" direction="in"/>
<pin name="VREF" direction="in"/>
<pin name="AVIN" direction="in"/>
<pin name="PVIN_2" direction="in"/>
<pin name="PVIN" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC_6" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="VTT_2" direction="out"/>
<pin name="VTT" direction="out"/>
</symbol>
<symbol name="LP2996M">
<pin name="VDDQ" direction="pwr"/>
<pin name="AVIN" direction="in"/>
<pin name="PVIN" direction="in"/>
<pin name="~SD" direction="pas"/>
<pin name="VSEN" direction="pas"/>
<pin name="VREF" direction="pwr"/>
<pin name="GND" direction="pas"/>
<pin name="VTT" direction="out"/>
</symbol>
<symbol name="LP2996MR">
<pin name="VDDQ" direction="pwr"/>
<pin name="~SD" direction="in"/>
<pin name="VREF" direction="in"/>
<pin name="VSENSE" direction="in"/>
<pin name="AVIN" direction="in"/>
<pin name="PVIN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="VTT" direction="out"/>
</symbol>
<symbol name="LP2997M">
<pin name="VDDQ" direction="pwr"/>
<pin name="AVIN" direction="in"/>
<pin name="PVIN" direction="in"/>
<pin name="~SD" direction="pas"/>
<pin name="VSEN" direction="pas"/>
<pin name="VREF" direction="pwr"/>
<pin name="GND" direction="pas"/>
<pin name="VTT" direction="out"/>
</symbol>
<symbol name="LP2997MR">
<pin name="VDDQ" direction="pwr"/>
<pin name="AVIN" direction="in"/>
<pin name="PVIN" direction="in"/>
<pin name="~SD" direction="pas"/>
<pin name="VSEN" direction="pas"/>
<pin name="VREF" direction="pwr"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VTT" direction="out"/>
</symbol>
<symbol name="LP2998MA">
<pin name="VDDQ" direction="pwr"/>
<pin name="~SD" direction="in"/>
<pin name="VREF" direction="in"/>
<pin name="VSEN" direction="in"/>
<pin name="PVIN" direction="in"/>
<pin name="AVIN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VTT" direction="out"/>
</symbol>
<symbol name="LP2998MR">
<pin name="VDDQ" direction="pwr"/>
<pin name="~SD" direction="in"/>
<pin name="VREF" direction="in"/>
<pin name="VSEN" direction="in"/>
<pin name="AVIN" direction="in"/>
<pin name="PVIN" direction="in"/>
<pin name="EP" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VTT" direction="out"/>
</symbol>
<symbol name="LP324M">
<pin name="V+" direction="pwr"/>
<pin name="-IN1" direction="in"/>
<pin name="+IN1" direction="in"/>
<pin name="+IN2" direction="in"/>
<pin name="-IN2" direction="in"/>
<pin name="-IN3" direction="in"/>
<pin name="+IN3" direction="in"/>
<pin name="+IN4" direction="in"/>
<pin name="-IN4" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT1" direction="out"/>
<pin name="OUT2" direction="out"/>
<pin name="OUT3" direction="out"/>
<pin name="OUT4" direction="out"/>
</symbol>
<symbol name="LP324MT">
<pin name="V+" direction="pwr"/>
<pin name="-INA" direction="in"/>
<pin name="+INA" direction="in"/>
<pin name="+INB" direction="in"/>
<pin name="-INB" direction="in"/>
<pin name="-INC" direction="in"/>
<pin name="+INC" direction="in"/>
<pin name="+IND" direction="in"/>
<pin name="-IND" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
<pin name="OUTC" direction="out"/>
<pin name="OUTD" direction="out"/>
</symbol>
<symbol name="LP324N">
<pin name="V+" direction="pwr"/>
<pin name="-IN1" direction="in"/>
<pin name="+IN1" direction="in"/>
<pin name="+IN2" direction="in"/>
<pin name="-IN2" direction="in"/>
<pin name="-IN3" direction="in"/>
<pin name="+IN3" direction="in"/>
<pin name="+IN4" direction="in"/>
<pin name="-IN4" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT1" direction="out"/>
<pin name="OUT2" direction="out"/>
<pin name="OUT3" direction="out"/>
<pin name="OUT4" direction="out"/>
</symbol>
<symbol name="LP339M">
<pin name="V+" direction="pwr"/>
<pin name="IN1-" direction="in"/>
<pin name="IN1+" direction="in"/>
<pin name="IN2-" direction="in"/>
<pin name="IN2+" direction="in"/>
<pin name="IN3-" direction="in"/>
<pin name="IN3+" direction="in"/>
<pin name="IN4-" direction="in"/>
<pin name="IN4+" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT1" direction="out"/>
<pin name="OUT2" direction="out"/>
<pin name="OUT3" direction="out"/>
<pin name="OUT4" direction="out"/>
</symbol>
<symbol name="LP339N">
<pin name="V+" direction="pwr"/>
<pin name="-IN1" direction="in"/>
<pin name="+IN1" direction="in"/>
<pin name="-IN2" direction="in"/>
<pin name="+IN2" direction="in"/>
<pin name="-IN3" direction="in"/>
<pin name="+IN3" direction="in"/>
<pin name="-IN4" direction="in"/>
<pin name="+IN4" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT1" direction="out"/>
<pin name="OUT2" direction="out"/>
<pin name="OUT3" direction="out"/>
<pin name="OUT4" direction="out"/>
</symbol>
<symbol name="LP3470M5-2.63">
<pin name="VCC" direction="pwr"/>
<pin name="VCC1" direction="pwr"/>
<pin name="SRT" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="~RESET" direction="out"/>
</symbol>
<symbol name="LP3470M5-2.93">
<pin name="VCC1" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="SRT" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="~RESET" direction="out"/>
</symbol>
<symbol name="LP3470M5-3.08">
<pin name="VCC1" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="SRT" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="~RESET" direction="out"/>
</symbol>
<symbol name="LP3470M5-4.63">
<pin name="VCC1" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="SRT" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="~RESET" direction="out"/>
</symbol>
<symbol name="LP38511MR-ADJ">
<pin name="IN_2" direction="in"/>
<pin name="IN" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="ADJ" direction="pas"/>
<pin name="NC" direction="nc"/>
<pin name="EP" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="OUT_2" direction="out"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LP38511TJ-ADJ">
<pin name="EN" direction="in"/>
<pin name="IN" direction="in"/>
<pin name="ADJ" direction="in"/>
<pin name="DAP" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LP38512MR-ADJ">
<pin name="IN_2" direction="in"/>
<pin name="IN" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="ADJ" direction="pas"/>
<pin name="NC" direction="nc"/>
<pin name="EP" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="OUT_2" direction="out"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LP38512TJ-ADJ">
<pin name="EN" direction="in"/>
<pin name="IN" direction="in"/>
<pin name="ADJ" direction="in"/>
<pin name="DAP" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LP38512TS-1.8">
<pin name="IN" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="~ERR" direction="pas"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LP38513S-1.8">
<pin name="IN" direction="pwr"/>
<pin name="EN" direction="pas"/>
<pin name="~ERROR" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LP38513T-1.8">
<pin name="VIN" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="*ERROR" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP3852EMP-2.5">
<pin name="VIN" direction="pwr"/>
<pin name="~SD" direction="in"/>
<pin name="~ERROR" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP3852EMP-3.3">
<pin name="VIN" direction="pwr"/>
<pin name="~SD" direction="in"/>
<pin name="~ERROR" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP3853ES-1.8">
<pin name="VIN" direction="pwr"/>
<pin name="~SD" direction="in"/>
<pin name="~ERROR~/SENSE" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP3853ES-2.5">
<pin name="VIN" direction="pwr"/>
<pin name="~SD" direction="in"/>
<pin name="~ERROR~/SENSE" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP3853ES-3.3">
<pin name="VIN" direction="pwr"/>
<pin name="~SD" direction="in"/>
<pin name="~ERROR~/SENSE" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP3853ES-5.0">
<pin name="VIN" direction="pwr"/>
<pin name="~SD" direction="in"/>
<pin name="~ERROR~/SENSE" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP3855EMP-2.5">
<pin name="VIN" direction="pwr"/>
<pin name="~SD" direction="in"/>
<pin name="~ERROR" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP3855EMP-3.3">
<pin name="VIN" direction="pwr"/>
<pin name="~SD" direction="in"/>
<pin name="~ERROR" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP3855EMP-ADJ">
<pin name="VIN" direction="pwr"/>
<pin name="~SD" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
<pin name="ADJ" direction="out"/>
</symbol>
<symbol name="LP3855ES-3.3">
<pin name="VIN" direction="pwr"/>
<pin name="~SD" direction="in"/>
<pin name="~ERROR" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP3855ES-ADJ">
<pin name="VIN" direction="pwr"/>
<pin name="~SD" direction="in"/>
<pin name="~ERROR" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP3856ES-1.8">
<pin name="VIN" direction="pwr"/>
<pin name="~SD" direction="pas"/>
<pin name="SENSE" direction="pas"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP3856ES-2.5">
<pin name="VIN" direction="pwr"/>
<pin name="~SD" direction="in"/>
<pin name="~ERROR~/SENSE" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP3856ES-3.3">
<pin name="VIN" direction="pwr"/>
<pin name="~SD" direction="pas"/>
<pin name="SENSE" direction="pas"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP3856ES-ADJ">
<pin name="VIN" direction="pwr"/>
<pin name="~SD" direction="pas"/>
<pin name="ADJ" direction="pas"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP3856ET-ADJ">
<pin name="ADJ" direction="in"/>
<pin name="VIN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
<pin name="*SD" direction="in"/>
</symbol>
<symbol name="LP38690DT-1.8">
<pin name="VIN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP38690DT-2.5">
<pin name="VIN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP38690DT-3.3">
<pin name="VIN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP38690DT-5.0">
<pin name="VIN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP38690SD-2.5">
<pin name="VIN_2" direction="in"/>
<pin name="VIN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="EP" direction="pas"/>
<pin name="NC" direction="nc"/>
<pin name="VOUT" direction="out"/>
<pin name="SNS" direction="pas"/>
</symbol>
<symbol name="LP38690SD-3.3">
<pin name="VIN_2" direction="in"/>
<pin name="VIN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="EP" direction="pas"/>
<pin name="NC" direction="nc"/>
<pin name="VOUT" direction="out"/>
<pin name="SNS" direction="pas"/>
</symbol>
<symbol name="LP38690SD-5.0">
<pin name="VIN_2" direction="in"/>
<pin name="VIN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="EP" direction="pas"/>
<pin name="NC" direction="nc"/>
<pin name="VOUT" direction="out"/>
<pin name="SNS" direction="pas"/>
</symbol>
<symbol name="LP38690SD-ADJ">
<pin name="VIN_2" direction="pwr"/>
<pin name="VIN" direction="pwr"/>
<pin name="ADJ" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP38691DT-1.8">
<pin name="VIN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP38691DT-3.3">
<pin name="VIN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP38691DT-5.0">
<pin name="VIN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP38691SD-1.8">
<pin name="VIN_2" direction="in"/>
<pin name="VIN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="EP" direction="pas"/>
<pin name="NC" direction="nc"/>
<pin name="VOUT" direction="out"/>
<pin name="SNS" direction="pas"/>
</symbol>
<symbol name="LP38691SD-2.5">
<pin name="VIN_2" direction="in"/>
<pin name="VIN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="EP" direction="pas"/>
<pin name="NC" direction="nc"/>
<pin name="VOUT" direction="out"/>
<pin name="SNS" direction="pas"/>
</symbol>
<symbol name="LP38691SD-3.3">
<pin name="VIN_2" direction="in"/>
<pin name="VIN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="EP" direction="pas"/>
<pin name="NC" direction="nc"/>
<pin name="VOUT" direction="out"/>
<pin name="SNS" direction="pas"/>
</symbol>
<symbol name="LP38691SD-5.0">
<pin name="VIN_2" direction="in"/>
<pin name="VIN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="EP" direction="pas"/>
<pin name="NC" direction="nc"/>
<pin name="VOUT" direction="out"/>
<pin name="SNS" direction="pas"/>
</symbol>
<symbol name="LP38691SD-ADJ">
<pin name="VIN_2" direction="in"/>
<pin name="VIN" direction="pwr"/>
<pin name="ADJ" direction="pas"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP38692MP-1.8">
<pin name="VIN" direction="in"/>
<pin name="VEN" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="N/C" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP38692MP-2.5">
<pin name="VIN" direction="in"/>
<pin name="VEN" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="N/C" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP38692MP-3.3">
<pin name="VIN" direction="pwr"/>
<pin name="VEN" direction="in"/>
<pin name="N/C" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP38692MP-5.0">
<pin name="VIN" direction="pwr"/>
<pin name="VEN" direction="in"/>
<pin name="N/C" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP38692MP-ADJ">
<pin name="VIN" direction="pwr"/>
<pin name="ADJ" direction="pas"/>
<pin name="VEN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP38692SD-2.5">
<pin name="VIN_2" direction="in"/>
<pin name="VIN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="EP" direction="pas"/>
<pin name="VEN" direction="nc"/>
<pin name="VOUT" direction="out"/>
<pin name="SNS" direction="pas"/>
</symbol>
<symbol name="LP38692SD-3.3">
<pin name="VIN_2" direction="in"/>
<pin name="VIN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="EP" direction="pas"/>
<pin name="VEN" direction="nc"/>
<pin name="VOUT" direction="out"/>
<pin name="SNS" direction="pas"/>
</symbol>
<symbol name="LP38692SD-5.0">
<pin name="VIN_2" direction="in"/>
<pin name="VIN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="EP" direction="pas"/>
<pin name="VEN" direction="nc"/>
<pin name="VOUT" direction="out"/>
<pin name="SNS" direction="pas"/>
</symbol>
<symbol name="LP38692SD-ADJ">
<pin name="VIN_2" direction="pwr"/>
<pin name="VIN" direction="pwr"/>
<pin name="VEN" direction="in"/>
<pin name="ADJ" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP38693MP-1.8">
<pin name="VIN" direction="in"/>
<pin name="VEN" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="N/C" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP38693MP-2.5">
<pin name="VIN" direction="in"/>
<pin name="VEN" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="N/C" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP38693MP-3.3">
<pin name="VIN" direction="pwr"/>
<pin name="VEN" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP38693MP-5.0">
<pin name="VIN" direction="pwr"/>
<pin name="VEN" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP38693MP-ADJ">
<pin name="VIN" direction="in"/>
<pin name="VEN" direction="pas"/>
<pin name="ADJ" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP38693SD-3.3">
<pin name="VIN_2" direction="in"/>
<pin name="VIN" direction="in"/>
<pin name="VEN" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="EP" direction="pas"/>
<pin name="VOUT" direction="out"/>
<pin name="SNS" direction="pas"/>
</symbol>
<symbol name="LP38693SD-5.0">
<pin name="VIN_2" direction="in"/>
<pin name="VIN" direction="in"/>
<pin name="VEN" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="EP" direction="pas"/>
<pin name="VOUT" direction="out"/>
<pin name="SNS" direction="pas"/>
</symbol>
<symbol name="LP38693SD-ADJ">
<pin name="VIN_2" direction="pwr"/>
<pin name="VIN" direction="pwr"/>
<pin name="VEN" direction="in"/>
<pin name="ADJ" direction="in"/>
<pin name="EP" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP3871EMP-1.8">
<pin name="VIN" direction="pwr"/>
<pin name="~SD" direction="in"/>
<pin name="~ERROR" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP3871EMP-2.5">
<pin name="VIN" direction="pwr"/>
<pin name="~SD" direction="in"/>
<pin name="~ERROR" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP3871EMP-3.3">
<pin name="VIN" direction="in"/>
<pin name="~SD" direction="pas"/>
<pin name="~ERR" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP3871ES-3.3">
<pin name="VIN" direction="pwr"/>
<pin name="~SD" direction="pas"/>
<pin name="~ERROR" direction="pas"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP3872EMP-3.3">
<pin name="VIN" direction="pwr"/>
<pin name="~SD" direction="in"/>
<pin name="~ERROR" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP3872ES-1.8">
<pin name="VIN" direction="pwr"/>
<pin name="~SD" direction="pas"/>
<pin name="~ERROR" direction="pas"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP3872ES-3.3">
<pin name="VIN" direction="pwr"/>
<pin name="~SD" direction="pas"/>
<pin name="~ERROR" direction="pas"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP3872ET-1.8">
<pin name="ERROR-SENSE" direction="in"/>
<pin name="VIN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
<pin name="*SD" direction="in"/>
</symbol>
<symbol name="LP3873ES-1.8">
<pin name="VIN" direction="pwr"/>
<pin name="~SD" direction="pas"/>
<pin name="~ERROR" direction="pas"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP3873ES-2.5">
<pin name="VIN" direction="pwr"/>
<pin name="~SD" direction="pas"/>
<pin name="~ERROR" direction="pas"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP3873ES-3.3">
<pin name="VIN" direction="pwr"/>
<pin name="~SD" direction="pas"/>
<pin name="~ERROR" direction="pas"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP3874EMP-1.8">
<pin name="VIN" direction="pwr"/>
<pin name="~SD" direction="in"/>
<pin name="~ERROR" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP3874EMP-2.5">
<pin name="VIN" direction="pwr"/>
<pin name="~SD" direction="in"/>
<pin name="~ERROR" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP3874EMP-3.3">
<pin name="VIN" direction="in"/>
<pin name="~SD" direction="pas"/>
<pin name="SEN" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP3874EMP-5.0">
<pin name="VIN" direction="in"/>
<pin name="~SD" direction="pas"/>
<pin name="SEN" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP3874EMP-ADJ">
<pin name="VIN" direction="pwr"/>
<pin name="~SD" direction="in"/>
<pin name="ADJ" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP3874ES-3.3">
<pin name="VIN" direction="pwr"/>
<pin name="~SD" direction="pas"/>
<pin name="SENSE" direction="pas"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP3874ES-ADJ">
<pin name="VIN" direction="pwr"/>
<pin name="~SD" direction="pas"/>
<pin name="SENSE" direction="pas"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP3875EMP-1.8">
<pin name="VIN" direction="pwr"/>
<pin name="~SD" direction="in"/>
<pin name="SENSE" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP3875EMP-3.3">
<pin name="VIN" direction="pwr"/>
<pin name="~SD" direction="in"/>
<pin name="SENSE" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP3875EMP-ADJ">
<pin name="VIN" direction="in"/>
<pin name="~SD" direction="pas"/>
<pin name="ADJ" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP3875ES-1.8">
<pin name="VIN" direction="pwr"/>
<pin name="~SD" direction="pas"/>
<pin name="SENSE" direction="pas"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP3875ES-2.5">
<pin name="VIN" direction="pwr"/>
<pin name="~SD" direction="pas"/>
<pin name="SENSE" direction="pas"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP3875ES-3.3">
<pin name="VIN" direction="pwr"/>
<pin name="~SD" direction="pas"/>
<pin name="SENSE" direction="pas"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP3875ES-ADJ">
<pin name="VIN" direction="pwr"/>
<pin name="~SD" direction="pas"/>
<pin name="ADJ" direction="pas"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP3875ET-3.3">
<pin name="ERROR-SENSE" direction="in"/>
<pin name="VIN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
<pin name="*SD" direction="in"/>
</symbol>
<symbol name="LP3876ES-1.8">
<pin name="VIN" direction="pwr"/>
<pin name="~SD" direction="pas"/>
<pin name="SENSE" direction="pas"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP3876ES-2.5">
<pin name="VIN" direction="pwr"/>
<pin name="~SD" direction="pas"/>
<pin name="SENSE" direction="pas"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP3876ES-3.3">
<pin name="VIN" direction="pwr"/>
<pin name="~SD" direction="pas"/>
<pin name="SENSE" direction="pas"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP3876ES-ADJ">
<pin name="VIN" direction="pwr"/>
<pin name="~SD" direction="pas"/>
<pin name="ADJ" direction="pas"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP3878MR-ADJ">
<pin name="IN" direction="in"/>
<pin name="BYPASS" direction="pas"/>
<pin name="ADJ" direction="pas"/>
<pin name="~SD" direction="pas"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LP3879MR-1.0">
<pin name="IN" direction="in"/>
<pin name="SEN" direction="pas"/>
<pin name="BYPASS" direction="pas"/>
<pin name="~SD" direction="pas"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LP3879MR-1.2">
<pin name="IN" direction="in"/>
<pin name="SEN" direction="pas"/>
<pin name="BYPASS" direction="pas"/>
<pin name="~SD" direction="pas"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LP3879SD-1.0">
<pin name="IN" direction="pwr"/>
<pin name="~SHUTDOWN" direction="in"/>
<pin name="SENSE" direction="in"/>
<pin name="BYPASS" direction="in"/>
<pin name="EP" direction="pas"/>
<pin name="N/C_2" direction="nc"/>
<pin name="N/C" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LP3879SD-1.2">
<pin name="IN" direction="pwr"/>
<pin name="~SHUTDOWN" direction="in"/>
<pin name="SENSE" direction="in"/>
<pin name="BYPASS" direction="in"/>
<pin name="EP" direction="pas"/>
<pin name="N/C_2" direction="nc"/>
<pin name="N/C" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LP3881EMR-1.8">
<pin name="VIN" direction="pwr"/>
<pin name="S/D" direction="pas"/>
<pin name="VBIAS" direction="pas"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT_2" direction="out"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP3881ES-1.2">
<pin name="IN" direction="pwr"/>
<pin name="~SD" direction="pas"/>
<pin name="BIAS" direction="pas"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LP3881ES-1.5">
<pin name="IN" direction="pwr"/>
<pin name="~SD" direction="pas"/>
<pin name="BIAS" direction="pas"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LP3881ET-1.5">
<pin name="BIAS" direction="in"/>
<pin name="VIN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
<pin name="*SHUTDOWN" direction="in"/>
</symbol>
<symbol name="LP3882EMR-1.2">
<pin name="VIN" direction="pwr"/>
<pin name="~SD" direction="pas"/>
<pin name="VBIAS" direction="pas"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT_2" direction="out"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP3882ES-1.2">
<pin name="IN" direction="in"/>
<pin name="~SD" direction="pas"/>
<pin name="BIAS" direction="pas"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LP3882ET-1.2">
<pin name="BIAS" direction="in"/>
<pin name="VIN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
<pin name="*SHUTDOWN" direction="in"/>
</symbol>
<symbol name="LP3883ES-1.2">
<pin name="IN" direction="in"/>
<pin name="~SD" direction="pas"/>
<pin name="BIAS" direction="pas"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LP38841MR-ADJ">
<pin name="BIAS" direction="pwr"/>
<pin name="IN" direction="in"/>
<pin name="~SD" direction="in"/>
<pin name="ADJ" direction="pas"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LP38841T-0.8">
<pin name="*SHUTDOWN" direction="in"/>
<pin name="INPUT" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUTPUT" direction="out"/>
<pin name="BIAS" direction="in"/>
</symbol>
<symbol name="LP38841T-1.5">
<pin name="*SHUTDOWN" direction="in"/>
<pin name="INPUT" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUTPUT" direction="out"/>
<pin name="BIAS" direction="in"/>
</symbol>
<symbol name="LP38842MR-ADJ">
<pin name="BIAS" direction="pwr"/>
<pin name="IN" direction="in"/>
<pin name="~SD" direction="in"/>
<pin name="ADJ" direction="pas"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LP38842S-1.2">
<pin name="IN" direction="in"/>
<pin name="~SD" direction="pas"/>
<pin name="BIAS" direction="pas"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LP38843S-1.2">
<pin name="IN" direction="pwr"/>
<pin name="~SHUTDOWN" direction="in"/>
<pin name="BIAS" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LP38843T-1.5">
<pin name="BIAS" direction="in"/>
<pin name="VIN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
<pin name="*SHUTDOWN" direction="in"/>
</symbol>
<symbol name="LP38851MR-ADJ">
<pin name="IN" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="SS" direction="in"/>
<pin name="ADJ" direction="in"/>
<pin name="BIAS" direction="pwr"/>
<pin name="N/C" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LP38851S-ADJ">
<pin name="IN" direction="pwr"/>
<pin name="EN" direction="in"/>
<pin name="ADJ" direction="in"/>
<pin name="SS" direction="in"/>
<pin name="BIAS" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LP38851T-ADJ">
<pin name="SS" direction="pas"/>
<pin name="EN" direction="pas"/>
<pin name="IN" direction="pas"/>
<pin name="BIAS" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="ADJ" direction="out"/>
<pin name="OUT" direction="pas"/>
</symbol>
<symbol name="LP38852S-ADJ">
<pin name="IN" direction="pwr"/>
<pin name="EN" direction="in"/>
<pin name="ADJ" direction="in"/>
<pin name="SS" direction="in"/>
<pin name="BIAS" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LP38853MR-ADJ">
<pin name="BIAS" direction="pwr"/>
<pin name="IN" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="ADJ" direction="pas"/>
<pin name="SS" direction="pas"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LP38853S-ADJ">
<pin name="BIAS" direction="pwr"/>
<pin name="EN" direction="in"/>
<pin name="ADJ" direction="pas"/>
<pin name="SS" direction="in"/>
<pin name="IN" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LP38853T-ADJ">
<pin name="SS" direction="pas"/>
<pin name="EN" direction="pas"/>
<pin name="IN" direction="pas"/>
<pin name="BIAS" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="ADJ" direction="out"/>
<pin name="OUT" direction="pas"/>
</symbol>
<symbol name="LP38855T-0.8">
<pin name="BIAS" direction="in"/>
<pin name="IN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
<pin name="EN" direction="in"/>
</symbol>
<symbol name="LP38855T-1.2">
<pin name="BIAS" direction="in"/>
<pin name="IN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
<pin name="EN" direction="in"/>
</symbol>
<symbol name="LP38856S-0.8">
<pin name="IN" direction="pwr"/>
<pin name="EN" direction="in"/>
<pin name="BIAS" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LP38856S-1.2">
<pin name="BIAS" direction="pwr"/>
<pin name="EN" direction="in"/>
<pin name="IN" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LP38856T-0.8">
<pin name="BIAS" direction="in"/>
<pin name="IN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
<pin name="EN" direction="in"/>
</symbol>
<symbol name="LP38856T-1.2">
<pin name="BIAS" direction="in"/>
<pin name="IN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
<pin name="EN" direction="in"/>
</symbol>
<symbol name="LP38858T-0.8">
<pin name="BIAS" direction="in"/>
<pin name="IN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
<pin name="*SS" direction="in"/>
</symbol>
<symbol name="LP38858T-1.2">
<pin name="BIAS" direction="in"/>
<pin name="IN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
<pin name="*SS" direction="in"/>
</symbol>
<symbol name="LP38859S-1.2">
<pin name="BIAS" direction="pwr"/>
<pin name="IN" direction="in"/>
<pin name="SS" direction="pas"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LP38859T-0.8">
<pin name="BIAS" direction="in"/>
<pin name="IN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
<pin name="*SS" direction="in"/>
</symbol>
<symbol name="LP38859T-1.2">
<pin name="IN" direction="pwr"/>
<pin name="SS" direction="in"/>
<pin name="BIAS" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LP3891EMR-1.2">
<pin name="VIN" direction="pwr"/>
<pin name="BIAS" direction="in"/>
<pin name="S/D" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="VOUT_2" direction="out"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP3891ES-1.2">
<pin name="IN" direction="in"/>
<pin name="~SD" direction="pas"/>
<pin name="BIAS" direction="pas"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LP3891ET-1.5">
<pin name="BIAS" direction="in"/>
<pin name="VIN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
<pin name="*SHUTDOWN" direction="in"/>
</symbol>
<symbol name="LP3892ES-1.2">
<pin name="IN" direction="in"/>
<pin name="~SD" direction="pas"/>
<pin name="BIAS" direction="pas"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LP3892ES-1.5">
<pin name="IN" direction="pwr"/>
<pin name="~SHUTDOWN" direction="in"/>
<pin name="BIAS" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LP3892ET-1.2">
<pin name="BIAS" direction="in"/>
<pin name="VIN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
<pin name="*SHUTDOWN" direction="in"/>
</symbol>
<symbol name="LP3893ES-1.2">
<pin name="IN" direction="pwr"/>
<pin name="~SHUTDOWN" direction="in"/>
<pin name="BIAS" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LP3893ET-1.5">
<pin name="BIAS" direction="in"/>
<pin name="VIN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
<pin name="*SHUTDOWN" direction="in"/>
</symbol>
<symbol name="LP3918TL-A">
<pin name="VIN1" direction="pwr"/>
<pin name="VIN2" direction="pwr"/>
<pin name="PWR_ON" direction="in"/>
<pin name="HF_PWR" direction="in"/>
<pin name="RX_EN" direction="in"/>
<pin name="TX_EN" direction="in"/>
<pin name="PS_HOLD" direction="in"/>
<pin name="SCL" direction="in"/>
<pin name="ACOK_N" direction="in"/>
<pin name="TCXO_EN" direction="in"/>
<pin name="CHGIN" direction="in"/>
<pin name="BATT" direction="in"/>
<pin name="GNDA" direction="pas"/>
<pin name="VSS" direction="pwr"/>
<pin name="LDO1" direction="out"/>
<pin name="LDO2" direction="out"/>
<pin name="LDO3" direction="out"/>
<pin name="LDO4" direction="out"/>
<pin name="LDO5" direction="out"/>
<pin name="LDO6" direction="out"/>
<pin name="LDO7" direction="out"/>
<pin name="RESET_N" direction="out"/>
<pin name="PON_N" direction="out"/>
<pin name="SDA"/>
<pin name="IMON" direction="out"/>
</symbol>
<symbol name="LP3918TL">
<pin name="VIN1" direction="pwr"/>
<pin name="VIN2" direction="pwr"/>
<pin name="PWR_ON" direction="in"/>
<pin name="HF_PWR" direction="in"/>
<pin name="RX_EN" direction="in"/>
<pin name="TX_EN" direction="in"/>
<pin name="PS_HOLD" direction="in"/>
<pin name="SCL" direction="in"/>
<pin name="ACOK_N" direction="in"/>
<pin name="TCXO_EN" direction="in"/>
<pin name="CHGIN" direction="in"/>
<pin name="BATT" direction="in"/>
<pin name="GNDA" direction="pas"/>
<pin name="VSS" direction="pwr"/>
<pin name="LDO1" direction="out"/>
<pin name="LDO2" direction="out"/>
<pin name="LDO3" direction="out"/>
<pin name="LDO4" direction="out"/>
<pin name="LDO5" direction="out"/>
<pin name="LDO6" direction="out"/>
<pin name="LDO7" direction="out"/>
<pin name="RESET_N" direction="out"/>
<pin name="PON_N" direction="out"/>
<pin name="SDA"/>
<pin name="IMON" direction="out"/>
</symbol>
<symbol name="LP3921SQ">
<pin name="VDD" direction="pwr"/>
<pin name="VIN1" direction="pwr"/>
<pin name="VIN2" direction="pwr"/>
<pin name="HF_PWR" direction="in"/>
<pin name="PWR_ON" direction="in"/>
<pin name="CHG_IN" direction="in"/>
<pin name="BATT" direction="in"/>
<pin name="SCL" direction="in"/>
<pin name="BYPASS" direction="in"/>
<pin name="TCXO_EN" direction="in"/>
<pin name="ACOK_N" direction="in"/>
<pin name="PS_HOLD" direction="in"/>
<pin name="RX_EN" direction="in"/>
<pin name="TX_EN" direction="in"/>
<pin name="IN+" direction="in"/>
<pin name="IN-" direction="in"/>
<pin name="GNDA" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VSS" direction="pwr"/>
<pin name="EPAD" direction="pas"/>
<pin name="RESET_N" direction="out"/>
<pin name="OUT+" direction="out"/>
<pin name="OUT-" direction="out"/>
<pin name="SDA"/>
<pin name="IMON" direction="out"/>
<pin name="PON_N" direction="out"/>
<pin name="LDO1" direction="out"/>
<pin name="LDO2" direction="out"/>
<pin name="LDO3" direction="out"/>
<pin name="LDO4" direction="out"/>
<pin name="LDO5" direction="out"/>
<pin name="LDO6" direction="out"/>
<pin name="LDO7" direction="out"/>
</symbol>
<symbol name="LP3943ISQ">
<pin name="VDD" direction="pwr"/>
<pin name="~RST" direction="in"/>
<pin name="SCL" direction="in"/>
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="SDA"/>
<pin name="GND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="LED0" direction="out"/>
<pin name="LED1" direction="out"/>
<pin name="LED2" direction="out"/>
<pin name="LED3" direction="out"/>
<pin name="LED4" direction="out"/>
<pin name="LED5" direction="out"/>
<pin name="LED6" direction="out"/>
<pin name="LED7" direction="out"/>
<pin name="LED8" direction="out"/>
<pin name="LED9" direction="out"/>
<pin name="LED10" direction="out"/>
<pin name="LED11" direction="out"/>
<pin name="LED12" direction="out"/>
<pin name="LED13" direction="out"/>
<pin name="LED14" direction="out"/>
<pin name="LED15" direction="out"/>
</symbol>
<symbol name="LP3947ISD-51">
<pin name="BATT" direction="pwr"/>
<pin name="EN" direction="in"/>
<pin name="SCL" direction="in"/>
<pin name="SDA"/>
<pin name="VBSENSE" direction="in"/>
<pin name="CHG-IN" direction="in"/>
<pin name="MODE" direction="in"/>
<pin name="ISEL" direction="in"/>
<pin name="TS" direction="in"/>
<pin name="EP" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VT" direction="out"/>
<pin name="DIFF-AMP" direction="out"/>
<pin name="EOC" direction="out"/>
<pin name="CHG" direction="out"/>
</symbol>
<symbol name="LP3952RL">
<pin name="VDD1" direction="pwr"/>
<pin name="VDD2" direction="pwr"/>
<pin name="VDDA" direction="pwr"/>
<pin name="VDDIO" direction="pwr"/>
<pin name="ADDR_SEL" direction="in"/>
<pin name="NRST" direction="in"/>
<pin name="IRGB" direction="in"/>
<pin name="SCL" direction="in"/>
<pin name="IRT" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="PWM" direction="in"/>
<pin name="GNDT" direction="pas"/>
<pin name="ASE" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND_11" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDA" direction="pas"/>
<pin name="GND_SW" direction="pas"/>
<pin name="GND_RGB" direction="pas"/>
<pin name="R1" direction="out"/>
<pin name="R2" direction="out"/>
<pin name="G1" direction="out"/>
<pin name="G2" direction="out"/>
<pin name="B1" direction="out"/>
<pin name="B2" direction="out"/>
<pin name="SDA"/>
<pin name="SW" direction="out"/>
<pin name="VREF" direction="out"/>
</symbol>
<symbol name="LP39542RL">
<pin name="VDDA" direction="pwr"/>
<pin name="VDD1" direction="pwr"/>
<pin name="VDD2" direction="pwr"/>
<pin name="VDDIO" direction="pwr"/>
<pin name="SCL" direction="in"/>
<pin name="SDA"/>
<pin name="ADDR_SEL" direction="in"/>
<pin name="IRT" direction="in"/>
<pin name="ASE" direction="in"/>
<pin name="NRST" direction="in"/>
<pin name="IRGB" direction="in"/>
<pin name="IFLASH" direction="in"/>
<pin name="SYNC_PWM" direction="in"/>
<pin name="FLASH_EN" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="GNDA" direction="pas"/>
<pin name="GNDT" direction="pas"/>
<pin name="GND_SW" direction="pas"/>
<pin name="GND_RGB" direction="pas"/>
<pin name="GND_WLED" direction="pas"/>
<pin name="WLED1" direction="out"/>
<pin name="WLED2" direction="out"/>
<pin name="WLED3" direction="out"/>
<pin name="WLED4" direction="out"/>
<pin name="WLED5" direction="out"/>
<pin name="WLED6" direction="out"/>
<pin name="R1" direction="out"/>
<pin name="R2" direction="out"/>
<pin name="B1" direction="out"/>
<pin name="B2" direction="out"/>
<pin name="G1" direction="out"/>
<pin name="G2" direction="out"/>
<pin name="VREF" direction="out"/>
<pin name="FLASH" direction="out"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="LP3961EMP-1.8">
<pin name="VIN" direction="pwr"/>
<pin name="~SD" direction="pas"/>
<pin name="~ERR" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP3961EMP-2.5">
<pin name="VIN" direction="pwr"/>
<pin name="~SD" direction="pas"/>
<pin name="~ERR" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP3961EMP-3.3">
<pin name="VIN" direction="pwr"/>
<pin name="~SD" direction="pas"/>
<pin name="~ERR" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP3961EMP-5.0">
<pin name="VIN" direction="pwr"/>
<pin name="~SD" direction="in"/>
<pin name="~ERROR" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP3961ES-1.8">
<pin name="VIN" direction="pwr"/>
<pin name="~SD" direction="in"/>
<pin name="~ERROR/SENSE/ADJ" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP3961ES-2.5">
<pin name="VIN" direction="pwr"/>
<pin name="~SD" direction="pas"/>
<pin name="~ERROR" direction="pas"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP3961ES-3.3">
<pin name="VIN" direction="pwr"/>
<pin name="~SD" direction="pas"/>
<pin name="~ERROR" direction="pas"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP3962EMP-2.5">
<pin name="VIN" direction="pwr"/>
<pin name="~SD" direction="in"/>
<pin name="~ERROR" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP3962EMP-3.3">
<pin name="VIN" direction="pwr"/>
<pin name="~SD" direction="in"/>
<pin name="~ERROR" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP3962ES-1.8">
<pin name="VIN" direction="pwr"/>
<pin name="~SD" direction="in"/>
<pin name="~ERROR/SENSE/ADJ" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP3962ES-2.5">
<pin name="VIN" direction="pwr"/>
<pin name="~SD" direction="in"/>
<pin name="~ERROR/SENSE/ADJ" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP3962ES-3.3">
<pin name="VIN" direction="pwr"/>
<pin name="~SD" direction="in"/>
<pin name="~ERROR/SENSE/ADJ" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP3963ES-2.5">
<pin name="VIN" direction="pwr"/>
<pin name="~SD" direction="in"/>
<pin name="~ERROR/SENSE/ADJ" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP3963ES-3.3">
<pin name="VIN" direction="pwr"/>
<pin name="~SD" direction="in"/>
<pin name="~ERROR/SENSE/ADJ" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP3964EMP-1.8">
<pin name="VIN" direction="pwr"/>
<pin name="~SD" direction="in"/>
<pin name="SENSE/ADJ" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP3964EMP-2.5">
<pin name="VIN" direction="pwr"/>
<pin name="~SD" direction="pas"/>
<pin name="SEN/ADJ" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP3964EMP-3.3">
<pin name="VIN" direction="pwr"/>
<pin name="~SD" direction="in"/>
<pin name="~ERROR" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP3964EMP-ADJ">
<pin name="VIN" direction="pwr"/>
<pin name="~SD" direction="pas"/>
<pin name="ADJ" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP3964ES-2.5">
<pin name="VIN" direction="pwr"/>
<pin name="~SD" direction="in"/>
<pin name="~ERROR/SENSE/ADJ" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP3964ES-3.3">
<pin name="VIN" direction="pwr"/>
<pin name="~SD" direction="pas"/>
<pin name="SENSE/ADJ" direction="pas"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP3964ES-ADJ">
<pin name="VIN" direction="pwr"/>
<pin name="~SD" direction="in"/>
<pin name="SENSE/ADJ" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP3964ET-ADJ">
<pin name="*ERROR-SENS-ADJ" direction="in"/>
<pin name="VIN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
<pin name="*SHUTDOWN" direction="in"/>
</symbol>
<symbol name="LP3965EMP-1.8">
<pin name="VIN" direction="pwr"/>
<pin name="~SD" direction="in"/>
<pin name="SENSE/ADJ" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP3965EMP-2.5">
<pin name="VIN" direction="pwr"/>
<pin name="~SD" direction="in"/>
<pin name="SENSE/ADJ" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP3965EMP-3.3">
<pin name="VIN" direction="pwr"/>
<pin name="~SD" direction="in"/>
<pin name="SENSE/ADJ" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP3965EMP-ADJ">
<pin name="VIN" direction="pwr"/>
<pin name="~SD" direction="in"/>
<pin name="SENSE/ADJ" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP3965ES-1.8">
<pin name="VIN" direction="pwr"/>
<pin name="~SD" direction="in"/>
<pin name="~ERROR/SENSE/ADJ" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP3965ES-2.5">
<pin name="VIN" direction="pwr"/>
<pin name="~SD" direction="in"/>
<pin name="~ERROR/SENSE/ADJ" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP3965ES-3.3">
<pin name="VIN" direction="pwr"/>
<pin name="~SD" direction="in"/>
<pin name="~ERROR/SENSE/ADJ" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP3965ES-ADJ">
<pin name="VIN" direction="pwr"/>
<pin name="~SD" direction="in"/>
<pin name="~ERROR/SENSE/ADJ" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP3966ES-1.8">
<pin name="VIN" direction="pwr"/>
<pin name="~SD" direction="in"/>
<pin name="~ERROR/SENSE/ADJ" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP3966ES-2.5">
<pin name="VIN" direction="pwr"/>
<pin name="~SD" direction="in"/>
<pin name="~ERROR/SENSE/ADJ" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP3966ES-3.3">
<pin name="VIN" direction="pwr"/>
<pin name="~SD" direction="in"/>
<pin name="~ERROR/SENSE/ADJ" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP3966ES-ADJ">
<pin name="VIN" direction="pwr"/>
<pin name="~SD" direction="in"/>
<pin name="~ERROR/SENSE/ADJ" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP3966ET-ADJ">
<pin name="*ERROR-SENS-ADJ" direction="in"/>
<pin name="VIN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="*SHUTDOWN" direction="in"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP3981ILD-2.5">
<pin name="VIN" direction="in"/>
<pin name="BYPASS" direction="in"/>
<pin name="VEN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="VOUT" direction="out"/>
<pin name="VOUT-SENSE" direction="out"/>
</symbol>
<symbol name="LP3981ILD-3.3">
<pin name="VIN" direction="in"/>
<pin name="BYPASS" direction="in"/>
<pin name="VEN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="VOUT" direction="out"/>
<pin name="VOUT-SENSE" direction="out"/>
</symbol>
<symbol name="LP3981IMM-2.5">
<pin name="VIN" direction="in"/>
<pin name="BYPASS" direction="in"/>
<pin name="VEN" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
<pin name="VOUT-SENSE" direction="out"/>
</symbol>
<symbol name="LP3981IMM-2.8">
<pin name="VIN" direction="in"/>
<pin name="BYPASS" direction="in"/>
<pin name="VEN" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
<pin name="VOUT-SENSE" direction="out"/>
</symbol>
<symbol name="LP3981IMM-3.0">
<pin name="VIN" direction="in"/>
<pin name="BYPASS" direction="in"/>
<pin name="VEN" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
<pin name="VOUT-SENSE" direction="out"/>
</symbol>
<symbol name="LP3981IMM-3.3">
<pin name="VIN" direction="in"/>
<pin name="BYPASS" direction="in"/>
<pin name="VEN" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
<pin name="VOUT-SENSE" direction="out"/>
</symbol>
<symbol name="LP3982ILD-1.8">
<pin name="VIN" direction="pwr"/>
<pin name="SET" direction="in"/>
<pin name="CC" direction="in"/>
<pin name="~SHDN" direction="in"/>
<pin name="~FAULT" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="VOUT_2" direction="out"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP3982ILD-3.3">
<pin name="VIN" direction="pwr"/>
<pin name="SET" direction="in"/>
<pin name="CC" direction="in"/>
<pin name="~SHDN" direction="in"/>
<pin name="~FAULT" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="VOUT_2" direction="out"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP3982ILD-ADJ">
<pin name="VIN" direction="pwr"/>
<pin name="SET" direction="in"/>
<pin name="CC" direction="in"/>
<pin name="~SHDN" direction="in"/>
<pin name="~FAULT" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="VOUT_2" direction="out"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP3982IMM-1.8">
<pin name="IN" direction="in"/>
<pin name="~SET" direction="in"/>
<pin name="CC" direction="pas"/>
<pin name="~SHDN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT_2" direction="out"/>
<pin name="OUT" direction="out"/>
<pin name="~FAULT" direction="pas"/>
</symbol>
<symbol name="LP3982IMM-2.5">
<pin name="IN" direction="in"/>
<pin name="~SET" direction="in"/>
<pin name="CC" direction="in"/>
<pin name="~SD" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT_2" direction="out"/>
<pin name="OUT" direction="out"/>
<pin name="~FAULT" direction="pas"/>
</symbol>
<symbol name="LP3982IMM-3.0">
<pin name="IN" direction="pwr"/>
<pin name="SET" direction="in"/>
<pin name="CC" direction="in"/>
<pin name="~SHDN" direction="in"/>
<pin name="~FAULT" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT_2" direction="out"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LP3982IMM-3.3">
<pin name="IN" direction="pwr"/>
<pin name="SET" direction="in"/>
<pin name="CC" direction="in"/>
<pin name="~SHDN" direction="in"/>
<pin name="~FAULT" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT_2" direction="out"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LP3982IMM-ADJ">
<pin name="IN" direction="pwr"/>
<pin name="SET" direction="in"/>
<pin name="CC" direction="in"/>
<pin name="~SHDN" direction="in"/>
<pin name="~FAULT" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT_2" direction="out"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LP3985IM5-2.5">
<pin name="VIN" direction="pwr"/>
<pin name="VEN" direction="in"/>
<pin name="BYPASS" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP3985IM5-2.8">
<pin name="VIN" direction="pwr"/>
<pin name="VEN" direction="in"/>
<pin name="BYPASS" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP3985IM5-3.0">
<pin name="VIN" direction="pwr"/>
<pin name="VEN" direction="in"/>
<pin name="BYPASS" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP3985IM5-3.3">
<pin name="VIN" direction="pwr"/>
<pin name="VEN" direction="in"/>
<pin name="BYPASS" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP3985IM5-4.7">
<pin name="VIN" direction="pwr"/>
<pin name="VEN" direction="in"/>
<pin name="BYPASS" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP3985IM5-5.0">
<pin name="VIN" direction="pwr"/>
<pin name="VEN" direction="in"/>
<pin name="BYPASS" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP3985ITL-2.7">
<pin name="VIN" direction="pwr"/>
<pin name="VEN" direction="in"/>
<pin name="BYPASS" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP3985ITL-285">
<pin name="VIN" direction="pwr"/>
<pin name="VEN" direction="in"/>
<pin name="BYPASS" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP3985ITL-3.3">
<pin name="VIN" direction="pwr"/>
<pin name="VEN" direction="in"/>
<pin name="BYPASS" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP3985ITL-4.75">
<pin name="VIN" direction="pwr"/>
<pin name="VEN" direction="in"/>
<pin name="BYPASS" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP3985ITL-5.0">
<pin name="VIN" direction="pwr"/>
<pin name="VEN" direction="in"/>
<pin name="BYPASS" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP3990MF-1.5">
<pin name="VIN" direction="pwr"/>
<pin name="VEN" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP3990MF-1.8">
<pin name="VIN" direction="pwr"/>
<pin name="VEN" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP3990TL-1.2">
<pin name="VIN" direction="pwr"/>
<pin name="VEN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP3990TL-1.5">
<pin name="VIN" direction="pwr"/>
<pin name="VEN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP3991TL-1.2">
<pin name="VIN" direction="in"/>
<pin name="VEN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP3991TL-1.3">
<pin name="VIN" direction="pwr"/>
<pin name="VEN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP3991TL-1.5">
<pin name="VIN" direction="pwr"/>
<pin name="VEN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP3991TL-2.8">
<pin name="VIN" direction="pwr"/>
<pin name="VEN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP3992IMF-1.5">
<pin name="VIN" direction="pwr"/>
<pin name="~SD" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
<pin name="COUT" direction="out"/>
</symbol>
<symbol name="LP3995ILD-1.8">
<pin name="VIN" direction="pwr"/>
<pin name="VEN" direction="in"/>
<pin name="C_BYPASS" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP3995ITL-1.8">
<pin name="VIN" direction="pwr"/>
<pin name="VEN" direction="in"/>
<pin name="CYPASS" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP3995ITL-1.9">
<pin name="VIN" direction="pwr"/>
<pin name="VEN" direction="in"/>
<pin name="CYPASS" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP3995ITL-2.1">
<pin name="VIN" direction="pwr"/>
<pin name="VEN" direction="in"/>
<pin name="CYPASS" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP3995ITL-2.5">
<pin name="VIN" direction="pwr"/>
<pin name="VEN" direction="in"/>
<pin name="CYPASS" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP3995ITL-2.85">
<pin name="VIN" direction="pwr"/>
<pin name="VEN" direction="in"/>
<pin name="CYPASS" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP3997MM-3.3">
<pin name="VIN" direction="pwr"/>
<pin name="~SD" direction="in"/>
<pin name="CBYP" direction="in"/>
<pin name="DELAY" direction="in"/>
<pin name="SENSE" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
<pin name="~ERROR" direction="out"/>
</symbol>
<symbol name="LP3999ITL-1.8">
<pin name="VIN" direction="pwr"/>
<pin name="VEN" direction="in"/>
<pin name="CBYPASS" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP3999ITL-2.4">
<pin name="VIN" direction="pwr"/>
<pin name="VEN" direction="in"/>
<pin name="CBYPASS" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP5524TM-5">
<pin name="VIN" direction="pwr"/>
<pin name="ENA" direction="in"/>
<pin name="ENB" direction="in"/>
<pin name="ISET" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="D1A" direction="out"/>
<pin name="D2A" direction="out"/>
<pin name="D1B" direction="out"/>
<pin name="D2B" direction="out"/>
</symbol>
<symbol name="LP55281RL">
<pin name="VDDA" direction="pwr"/>
<pin name="VDDIO" direction="pwr"/>
<pin name="VDD1" direction="pwr"/>
<pin name="VDD2" direction="pwr"/>
<pin name="SCK/SCL" direction="in"/>
<pin name="IF_SEL" direction="in"/>
<pin name="IRGB" direction="in"/>
<pin name="VREF" direction="in"/>
<pin name="IRT" direction="in"/>
<pin name="NRST" direction="in"/>
<pin name="SI/A0" direction="in"/>
<pin name="ASE1" direction="in"/>
<pin name="ASE2" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDA" direction="pas"/>
<pin name="GND_SW" direction="pas"/>
<pin name="GND_RGB1" direction="pas"/>
<pin name="GND_RGB2" direction="pas"/>
<pin name="ALED" direction="out"/>
<pin name="SS/SDA"/>
<pin name="SO" direction="out"/>
<pin name="SW" direction="out"/>
<pin name="FB" direction="in"/>
<pin name="R1" direction="out"/>
<pin name="R2" direction="out"/>
<pin name="R3" direction="out"/>
<pin name="R4" direction="out"/>
<pin name="G1" direction="out"/>
<pin name="G2" direction="out"/>
<pin name="G3" direction="out"/>
<pin name="G4" direction="out"/>
<pin name="B1" direction="out"/>
<pin name="B2" direction="out"/>
<pin name="B3" direction="out"/>
<pin name="B4" direction="out"/>
</symbol>
<symbol name="LP55281TL">
<pin name="VDDA" direction="pwr"/>
<pin name="VDDIO" direction="pwr"/>
<pin name="VDD1" direction="pwr"/>
<pin name="VDD2" direction="pwr"/>
<pin name="SCK/SCL" direction="in"/>
<pin name="IF_SEL" direction="in"/>
<pin name="IRGB" direction="in"/>
<pin name="VREF" direction="in"/>
<pin name="IRT" direction="in"/>
<pin name="NRST" direction="in"/>
<pin name="SI/A0" direction="in"/>
<pin name="ASE1" direction="in"/>
<pin name="ASE2" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GNDA" direction="pas"/>
<pin name="GND_SW" direction="pas"/>
<pin name="GND_RGB1" direction="pas"/>
<pin name="GND_RGB2" direction="pas"/>
<pin name="ALED" direction="out"/>
<pin name="SS/SDA"/>
<pin name="SO" direction="out"/>
<pin name="SW" direction="out"/>
<pin name="FB" direction="in"/>
<pin name="R1" direction="out"/>
<pin name="R2" direction="out"/>
<pin name="R3" direction="out"/>
<pin name="R4" direction="out"/>
<pin name="G1" direction="out"/>
<pin name="G2" direction="out"/>
<pin name="G3" direction="out"/>
<pin name="G4" direction="out"/>
<pin name="B1" direction="out"/>
<pin name="B2" direction="out"/>
<pin name="B3" direction="out"/>
<pin name="B4" direction="out"/>
</symbol>
<symbol name="LP5900SD-1.5">
<pin name="VIN" direction="pwr"/>
<pin name="VEN" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP5900SD-1.8">
<pin name="VIN" direction="pwr"/>
<pin name="VEN" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP5900SD-2.2">
<pin name="VIN" direction="pwr"/>
<pin name="VEN" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP5900SD-2.5">
<pin name="VIN" direction="pwr"/>
<pin name="VEN" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP5900SD-2.7">
<pin name="VIN" direction="pwr"/>
<pin name="VEN" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP5900SD-2.8">
<pin name="VIN" direction="pwr"/>
<pin name="VEN" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP5900SD-3.0">
<pin name="VIN" direction="pwr"/>
<pin name="VEN" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP5900SD-3.3">
<pin name="VIN" direction="pwr"/>
<pin name="VEN" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP5900TL-1.5">
<pin name="VIN" direction="pwr"/>
<pin name="VEN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP5900TL-1.8">
<pin name="VIN" direction="pwr"/>
<pin name="VEN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP5900TL-2.2">
<pin name="VIN" direction="pwr"/>
<pin name="VEN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP5900TL-2.5">
<pin name="VIN" direction="pwr"/>
<pin name="VEN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP5900TL-2.6">
<pin name="VIN" direction="pwr"/>
<pin name="VEN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP5900TL-2.7">
<pin name="VIN" direction="pwr"/>
<pin name="VEN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP5900TL-3.0">
<pin name="VIN" direction="pwr"/>
<pin name="VEN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP5900TL-3.3">
<pin name="VIN" direction="pwr"/>
<pin name="VEN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP5951MF-1.3">
<pin name="VIN" direction="pwr"/>
<pin name="EN" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP5951MF-1.5">
<pin name="VIN" direction="pwr"/>
<pin name="EN" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP5951MF-1.8">
<pin name="VIN" direction="pwr"/>
<pin name="EN" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP5951MF-2.0">
<pin name="VIN" direction="pwr"/>
<pin name="EN" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP5951MF-2.5">
<pin name="VIN" direction="pwr"/>
<pin name="EN" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP5951MF-2.8">
<pin name="VIN" direction="pwr"/>
<pin name="EN" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP5951MF-3.0">
<pin name="VIN" direction="pwr"/>
<pin name="EN" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP5951MF-3.3">
<pin name="VIN" direction="pwr"/>
<pin name="EN" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP5951MG-1.3">
<pin name="VIN" direction="pwr"/>
<pin name="EN" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP5951MG-1.5">
<pin name="VIN" direction="pwr"/>
<pin name="EN" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP5951MG-1.8">
<pin name="VIN" direction="pwr"/>
<pin name="EN" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP5951MG-2.0">
<pin name="VIN" direction="pwr"/>
<pin name="EN" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP5951MG-2.5">
<pin name="VIN" direction="pwr"/>
<pin name="EN" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP5951MG-2.8">
<pin name="VIN" direction="pwr"/>
<pin name="EN" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP5951MG-3.0">
<pin name="VIN" direction="pwr"/>
<pin name="EN" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP5951MG-3.3">
<pin name="VIN" direction="pwr"/>
<pin name="EN" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP5952TL-0.7">
<pin name="VIN" direction="pwr"/>
<pin name="VBATT" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP5952TL-1.2">
<pin name="VIN" direction="pwr"/>
<pin name="VBATT" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP5952TL-1.3">
<pin name="VIN" direction="pwr"/>
<pin name="VBATT" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP5952TL-1.4">
<pin name="VIN" direction="pwr"/>
<pin name="VBATT" direction="pwr"/>
<pin name="EN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP5952TL-1.5">
<pin name="VIN" direction="pwr"/>
<pin name="VBATT" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP5952TL-1.6">
<pin name="VIN" direction="pwr"/>
<pin name="VBATT" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP5952TL-1.8">
<pin name="VIN" direction="pwr"/>
<pin name="VBATT" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP5952TL-2.0">
<pin name="VIN" direction="pwr"/>
<pin name="VBATT" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LP5996SD-3333">
<pin name="VIN" direction="pwr"/>
<pin name="CBYP" direction="in"/>
<pin name="EN1" direction="in"/>
<pin name="EN2" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="VOUT1" direction="out"/>
<pin name="VOUT2" direction="out"/>
</symbol>
<symbol name="LP8358MF-1.2">
<pin name="VIN" direction="pwr"/>
<pin name="EN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="PG" direction="out"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LPC660AIM">
<pin name="V+" direction="pwr"/>
<pin name="-IN1" direction="in"/>
<pin name="+IN1" direction="in"/>
<pin name="+IN2" direction="in"/>
<pin name="-IN2" direction="in"/>
<pin name="-IN3" direction="in"/>
<pin name="+IN3" direction="in"/>
<pin name="+IN4" direction="in"/>
<pin name="-IN4" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT1" direction="out"/>
<pin name="OUT2" direction="out"/>
<pin name="OUT3" direction="out"/>
<pin name="OUT4" direction="out"/>
</symbol>
<symbol name="LPC661IM">
<pin name="V+" direction="pwr"/>
<pin name="NEG" direction="in"/>
<pin name="POS" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LPC662AIM">
<pin name="V+" direction="pwr"/>
<pin name="NEGA" direction="in"/>
<pin name="POSA" direction="in"/>
<pin name="NEGB" direction="in"/>
<pin name="POSB" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="LPC662IM">
<pin name="V+" direction="pwr"/>
<pin name="NEGA" direction="in"/>
<pin name="POSA" direction="in"/>
<pin name="NEGB" direction="in"/>
<pin name="POSB" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="LPV321M5">
<pin name="V+" direction="pwr"/>
<pin name="+IN" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LPV321M7">
<pin name="V-" direction="pwr"/>
<pin name="+IN" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="V+" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LPV324M">
<pin name="V+" direction="pwr"/>
<pin name="-INA" direction="in"/>
<pin name="+INA" direction="in"/>
<pin name="+INB" direction="in"/>
<pin name="-INB" direction="in"/>
<pin name="-INC" direction="in"/>
<pin name="+INC" direction="in"/>
<pin name="+IND" direction="in"/>
<pin name="-IND" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
<pin name="OUTC" direction="out"/>
<pin name="OUTD" direction="out"/>
</symbol>
<symbol name="LPV324MT">
<pin name="V+" direction="pwr"/>
<pin name="-INA" direction="in"/>
<pin name="+INA" direction="in"/>
<pin name="+INB" direction="in"/>
<pin name="-INB" direction="in"/>
<pin name="-INC" direction="in"/>
<pin name="+INC" direction="in"/>
<pin name="+IND" direction="in"/>
<pin name="-IND" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
<pin name="OUTC" direction="out"/>
<pin name="OUTD" direction="out"/>
</symbol>
<symbol name="LPV358MM">
<pin name="V+" direction="pwr"/>
<pin name="-INA" direction="in"/>
<pin name="+INA" direction="in"/>
<pin name="+INB" direction="in"/>
<pin name="-INB" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="LPV511MG">
<pin name="V+" direction="pwr"/>
<pin name="VIN+" direction="in"/>
<pin name="VIN-" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LPV531MK">
<pin name="V+" direction="pwr"/>
<pin name="+IN" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="ISEL" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LPV7215MF">
<pin name="V+" direction="pwr"/>
<pin name="+VIN" direction="in"/>
<pin name="-VIN" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LPV7215MG">
<pin name="V+" direction="pwr"/>
<pin name="VIN+" direction="in"/>
<pin name="VIN-" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="PC16550DN">
<pin name="VDD" direction="pwr"/>
<pin name="RCLK" direction="in"/>
<pin name="CS0" direction="in"/>
<pin name="CS1" direction="in"/>
<pin name="~CS2" direction="in"/>
<pin name="MR" direction="in"/>
<pin name="~RI" direction="in"/>
<pin name="~WR" direction="in"/>
<pin name="~RD" direction="pas"/>
<pin name="SIN" direction="in"/>
<pin name="XIN" direction="in"/>
<pin name="WR" direction="in"/>
<pin name="RD" direction="pas"/>
<pin name="~ADS" direction="in"/>
<pin name="~CTS" direction="in"/>
<pin name="~DSR" direction="in"/>
<pin name="~DCD" direction="in"/>
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="VSS" direction="pwr"/>
<pin name="D0" direction="hiz"/>
<pin name="D1" direction="hiz"/>
<pin name="D2" direction="hiz"/>
<pin name="D3" direction="hiz"/>
<pin name="D4" direction="hiz"/>
<pin name="D5" direction="hiz"/>
<pin name="D6" direction="hiz"/>
<pin name="D7" direction="hiz"/>
<pin name="~BAUDOUT" direction="out"/>
<pin name="SOUT" direction="out"/>
<pin name="XOUT" direction="out"/>
<pin name="~OUT1" direction="out"/>
<pin name="~OUT2" direction="out"/>
<pin name="~RTS" direction="pas"/>
<pin name="DDIS" direction="pas"/>
<pin name="INTR" direction="pas"/>
<pin name="~DTR" direction="pas"/>
<pin name="~TXRDY" direction="pas"/>
<pin name="~RXRDY"/>
</symbol>
<symbol name="SCAN12100TYA">
<pin name="PVDD33_2" direction="pwr"/>
<pin name="PVDD33_3" direction="pwr"/>
<pin name="PVDD33_4" direction="pwr"/>
<pin name="PVDD33" direction="pwr"/>
<pin name="AVDD33_2" direction="pwr"/>
<pin name="AVDD33_3" direction="pwr"/>
<pin name="AVDD33_4" direction="pwr"/>
<pin name="AVDD33" direction="pwr"/>
<pin name="AVDD18_2" direction="pwr"/>
<pin name="AVDD18_3" direction="pwr"/>
<pin name="AVDD18_4" direction="pwr"/>
<pin name="AVDD18_5" direction="pwr"/>
<pin name="AVDD18_6" direction="pwr"/>
<pin name="AVDD18_7" direction="pwr"/>
<pin name="AVDD18" direction="pwr"/>
<pin name="IOVDD_2" direction="pwr"/>
<pin name="IOVDD_3" direction="pwr"/>
<pin name="IOVDD_4" direction="pwr"/>
<pin name="IOVDD" direction="pwr"/>
<pin name="ADD0" direction="in"/>
<pin name="ADD1" direction="in"/>
<pin name="ADD2" direction="in"/>
<pin name="ADD3" direction="in"/>
<pin name="ADD4" direction="in"/>
<pin name="DIN_[0]" direction="in"/>
<pin name="DIN_[1]" direction="in"/>
<pin name="DIN_[2]" direction="in"/>
<pin name="DIN_[3]" direction="in"/>
<pin name="DIN_[4]" direction="in"/>
<pin name="DIN_[5]" direction="in"/>
<pin name="DIN_[6]" direction="in"/>
<pin name="DIN_[7]" direction="in"/>
<pin name="DIN_[8]" direction="in"/>
<pin name="DIN_[9]" direction="in"/>
<pin name="RINN" direction="in"/>
<pin name="RINP" direction="in"/>
<pin name="REFCLKP" direction="in"/>
<pin name="REFCLKN" direction="in"/>
<pin name="SYSCLKP" direction="in"/>
<pin name="SYSCLKN" direction="in"/>
<pin name="TXCLK" direction="in"/>
<pin name="RXCLK" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="MDC" direction="in"/>
<pin name="TMS" direction="in"/>
<pin name="MDIO" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="TRSTB" direction="in"/>
<pin name="VSEL" direction="in"/>
<pin name="TXPWDNB" direction="in"/>
<pin name="RXPWDNB" direction="in"/>
<pin name="CALIGN_EN" direction="in"/>
<pin name="RXCLKMODE" direction="in"/>
<pin name="OPMODE" direction="in"/>
<pin name="TENBMODE" direction="in"/>
<pin name="RESETB" direction="in"/>
<pin name="RES1" direction="in"/>
<pin name="RES2" direction="in"/>
<pin name="PE[1]" direction="in"/>
<pin name="PE[0]" direction="in"/>
<pin name="EQ_[0]" direction="in"/>
<pin name="EQ_[1]" direction="in"/>
<pin name="SPMODE[0]" direction="in"/>
<pin name="SPMODE[1]" direction="in"/>
<pin name="LOOP_[0]" direction="in"/>
<pin name="LOOP_[1]" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND_11" direction="pas"/>
<pin name="GND_12" direction="pas"/>
<pin name="GND_13" direction="pas"/>
<pin name="GND_14" direction="pas"/>
<pin name="GND_15" direction="pas"/>
<pin name="GND_16" direction="pas"/>
<pin name="GND_17" direction="pas"/>
<pin name="GND_18" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="ROUT_[0]" direction="out"/>
<pin name="ROUT_[1]" direction="out"/>
<pin name="ROUT_[2]" direction="out"/>
<pin name="ROUT_[3]" direction="out"/>
<pin name="ROUT_[4]" direction="out"/>
<pin name="ROUT_[5]" direction="out"/>
<pin name="ROUT_[6]" direction="out"/>
<pin name="ROUT_[7]" direction="out"/>
<pin name="ROUT_[8]" direction="out"/>
<pin name="ROUT_[9]" direction="out"/>
<pin name="DOUTN" direction="out"/>
<pin name="DOUTP" direction="out"/>
<pin name="TDO" direction="out"/>
<pin name="LOS" direction="out"/>
<pin name="LOCKB" direction="out"/>
<pin name="CDET" direction="out"/>
</symbol>
<symbol name="SCAN25100TYA">
<pin name="PVDD33_2" direction="pwr"/>
<pin name="PVDD33_3" direction="pwr"/>
<pin name="PVDD33_4" direction="pwr"/>
<pin name="PVDD33" direction="pwr"/>
<pin name="AVDD33_2" direction="pwr"/>
<pin name="AVDD33_3" direction="pwr"/>
<pin name="AVDD33_4" direction="pwr"/>
<pin name="AVDD33" direction="pwr"/>
<pin name="AVDD18_2" direction="pwr"/>
<pin name="AVDD18_3" direction="pwr"/>
<pin name="AVDD18_4" direction="pwr"/>
<pin name="AVDD18_5" direction="pwr"/>
<pin name="AVDD18_6" direction="pwr"/>
<pin name="AVDD18_7" direction="pwr"/>
<pin name="AVDD18" direction="pwr"/>
<pin name="IOVDD_2" direction="pwr"/>
<pin name="IOVDD_3" direction="pwr"/>
<pin name="IOVDD_4" direction="pwr"/>
<pin name="IOVDD" direction="pwr"/>
<pin name="ADD0" direction="in"/>
<pin name="ADD1" direction="in"/>
<pin name="ADD2" direction="in"/>
<pin name="ADD3" direction="in"/>
<pin name="ADD4" direction="in"/>
<pin name="DIN_[0]" direction="in"/>
<pin name="DIN_[1]" direction="in"/>
<pin name="DIN_[2]" direction="in"/>
<pin name="DIN_[3]" direction="in"/>
<pin name="DIN_[4]" direction="in"/>
<pin name="DIN_[5]" direction="in"/>
<pin name="DIN_[6]" direction="in"/>
<pin name="DIN_[7]" direction="in"/>
<pin name="DIN_[8]" direction="in"/>
<pin name="DIN_[9]" direction="in"/>
<pin name="RINN" direction="in"/>
<pin name="RINP" direction="in"/>
<pin name="REFCLKP" direction="in"/>
<pin name="REFCLKN" direction="in"/>
<pin name="SYSCLKP" direction="in"/>
<pin name="SYSCLKN" direction="in"/>
<pin name="TXCLK" direction="in"/>
<pin name="RXCLK" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="MDC" direction="in"/>
<pin name="TMS" direction="in"/>
<pin name="MDIO" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="TRSTB" direction="in"/>
<pin name="VSEL" direction="in"/>
<pin name="TXPWDNB" direction="in"/>
<pin name="RXPWDNB" direction="in"/>
<pin name="CALIGN_EN" direction="in"/>
<pin name="RXCLKMODE" direction="in"/>
<pin name="OPMODE" direction="in"/>
<pin name="TENBMODE" direction="in"/>
<pin name="RESETB" direction="in"/>
<pin name="RES1" direction="in"/>
<pin name="RES2" direction="in"/>
<pin name="PE[1]" direction="in"/>
<pin name="PE[0]" direction="in"/>
<pin name="EQ_[0]" direction="in"/>
<pin name="EQ_[1]" direction="in"/>
<pin name="SPMODE[0]" direction="in"/>
<pin name="SPMODE[1]" direction="in"/>
<pin name="LOOP_[0]" direction="in"/>
<pin name="LOOP_[1]" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND_11" direction="pas"/>
<pin name="GND_12" direction="pas"/>
<pin name="GND_13" direction="pas"/>
<pin name="GND_14" direction="pas"/>
<pin name="GND_15" direction="pas"/>
<pin name="GND_16" direction="pas"/>
<pin name="GND_17" direction="pas"/>
<pin name="GND_18" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="ROUT_[0]" direction="out"/>
<pin name="ROUT_[1]" direction="out"/>
<pin name="ROUT_[2]" direction="out"/>
<pin name="ROUT_[3]" direction="out"/>
<pin name="ROUT_[4]" direction="out"/>
<pin name="ROUT_[5]" direction="out"/>
<pin name="ROUT_[6]" direction="out"/>
<pin name="ROUT_[7]" direction="out"/>
<pin name="ROUT_[8]" direction="out"/>
<pin name="ROUT_[9]" direction="out"/>
<pin name="DOUTN" direction="out"/>
<pin name="DOUTP" direction="out"/>
<pin name="TDO" direction="out"/>
<pin name="LOS" direction="out"/>
<pin name="LOCKB" direction="out"/>
<pin name="CDET" direction="out"/>
</symbol>
<symbol name="SCAN90CP02VY">
<pin name="VDDA_2" direction="pwr"/>
<pin name="VDDA" direction="pwr"/>
<pin name="VDD1" direction="pwr"/>
<pin name="VDD2_2" direction="pwr"/>
<pin name="VDD2" direction="pwr"/>
<pin name="PEM00" direction="in"/>
<pin name="PEM01" direction="in"/>
<pin name="PEM10" direction="in"/>
<pin name="PEM11" direction="in"/>
<pin name="SEL1" direction="in"/>
<pin name="SEL0" direction="in"/>
<pin name="~EN0" direction="in"/>
<pin name="~EN1" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="TMS" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="~TRST" direction="in"/>
<pin name="IN0+" direction="in"/>
<pin name="IN0-" direction="in"/>
<pin name="IN1+" direction="in"/>
<pin name="IN1-" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="TDO" direction="out"/>
<pin name="OUT1-" direction="out"/>
<pin name="OUT1+" direction="out"/>
<pin name="OUT0-" direction="out"/>
<pin name="OUT0+" direction="out"/>
</symbol>
<symbol name="SCAN921025HSM">
<pin name="AVCC_2" direction="pwr"/>
<pin name="AVCC_3" direction="pwr"/>
<pin name="AVCC_4" direction="pwr"/>
<pin name="AVCC_5" direction="pwr"/>
<pin name="AVCC" direction="pwr"/>
<pin name="DVCC_2" direction="pwr"/>
<pin name="DVCC_3" direction="pwr"/>
<pin name="DVCC" direction="pwr"/>
<pin name="SYNC1" direction="in"/>
<pin name="SYNC2" direction="in"/>
<pin name="TMS" direction="in"/>
<pin name="DEN" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="TCLK" direction="in"/>
<pin name="~TRST" direction="in"/>
<pin name="~PWRDN" direction="in"/>
<pin name="TCLKR/~F" direction="in"/>
<pin name="DIN0" direction="in"/>
<pin name="DIN1" direction="in"/>
<pin name="DIN2" direction="in"/>
<pin name="DIN3" direction="in"/>
<pin name="DIN4" direction="in"/>
<pin name="DIN5" direction="in"/>
<pin name="DIN6" direction="in"/>
<pin name="DIN7" direction="in"/>
<pin name="DIN8" direction="in"/>
<pin name="DIN9" direction="in"/>
<pin name="AGND_2" direction="pas"/>
<pin name="AGND_3" direction="pas"/>
<pin name="AGND_4" direction="pas"/>
<pin name="AGND_5" direction="pas"/>
<pin name="AGND" direction="pas"/>
<pin name="DGND_2" direction="pas"/>
<pin name="DGND_3" direction="pas"/>
<pin name="DGND_4" direction="pas"/>
<pin name="DGND_5" direction="pas"/>
<pin name="DGND" direction="pas"/>
<pin name="DO+" direction="out"/>
<pin name="DO-" direction="out"/>
<pin name="TDO" direction="out"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC_6" direction="nc"/>
<pin name="NC_7" direction="nc"/>
<pin name="NC_8" direction="nc"/>
<pin name="NC" direction="nc"/>
</symbol>
<symbol name="SCAN921260UJB_A">
<pin name="AVDD_2" direction="pwr"/>
<pin name="AVDD_3" direction="pwr"/>
<pin name="AVDD_4" direction="pwr"/>
<pin name="AVDD" direction="pwr"/>
<pin name="DVDD_2" direction="pwr"/>
<pin name="DVDD_3" direction="pwr"/>
<pin name="DVDD_4" direction="pwr"/>
<pin name="DVDD_5" direction="pwr"/>
<pin name="DVDD_6" direction="pwr"/>
<pin name="DVDD_7" direction="pwr"/>
<pin name="DVDD_8" direction="pwr"/>
<pin name="DVDD_9" direction="pwr"/>
<pin name="DVDD_10" direction="pwr"/>
<pin name="DVDD_11" direction="pwr"/>
<pin name="DVDD_12" direction="pwr"/>
<pin name="DVDD_13" direction="pwr"/>
<pin name="DVDD_14" direction="pwr"/>
<pin name="DVDD" direction="pwr"/>
<pin name="PVDD_2" direction="pwr"/>
<pin name="PVDD_3" direction="pwr"/>
<pin name="PVDD_4" direction="pwr"/>
<pin name="PVDD" direction="pwr"/>
<pin name="RCLK0" direction="in"/>
<pin name="RCLK5" direction="in"/>
<pin name="BISTMODE_REQ" direction="in"/>
<pin name="CHTST_EN" direction="in"/>
<pin name="RFCLK" direction="in"/>
<pin name="REN" direction="in"/>
<pin name="~PWRDN" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="TDO" direction="in"/>
<pin name="TMS" direction="in"/>
<pin name="~TRST" direction="in"/>
<pin name="BIST_SEL0" direction="in"/>
<pin name="BIST_SEL1" direction="in"/>
<pin name="BIST_SEL2" direction="in"/>
<pin name="SEL0" direction="in"/>
<pin name="SEL1" direction="in"/>
<pin name="SEL2" direction="in"/>
<pin name="RIN0-" direction="in"/>
<pin name="RIN0+" direction="in"/>
<pin name="RIN1-" direction="in"/>
<pin name="RIN1+" direction="in"/>
<pin name="RIN2-" direction="in"/>
<pin name="RIN2+" direction="in"/>
<pin name="RIN3-" direction="in"/>
<pin name="RIN3+" direction="in"/>
<pin name="RIN4-" direction="in"/>
<pin name="RIN4+" direction="in"/>
<pin name="RIN5-" direction="in"/>
<pin name="RIN5+" direction="in"/>
<pin name="RIN6-" direction="in"/>
<pin name="RIN6+" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="AGND_2" direction="pas"/>
<pin name="AGND_3" direction="pas"/>
<pin name="AGND_4" direction="pas"/>
<pin name="AGND_5" direction="pas"/>
<pin name="AGND" direction="pas"/>
<pin name="PGND_2" direction="pas"/>
<pin name="PGND_3" direction="pas"/>
<pin name="DGND_2" direction="pas"/>
<pin name="DGND_3" direction="pas"/>
<pin name="DGND_4" direction="pas"/>
<pin name="DGND_5" direction="pas"/>
<pin name="DGND_6" direction="pas"/>
<pin name="DGND_7" direction="pas"/>
<pin name="DGND_8" direction="pas"/>
<pin name="DGND_9" direction="pas"/>
<pin name="DGND_10" direction="pas"/>
<pin name="DGND_11" direction="pas"/>
<pin name="DGND_12" direction="pas"/>
<pin name="DGND_13" direction="pas"/>
<pin name="DGND_14" direction="pas"/>
<pin name="DGND_15" direction="pas"/>
<pin name="DGND_16" direction="pas"/>
<pin name="DGND" direction="pas"/>
<pin name="PGND_4" direction="pas"/>
<pin name="PGND_5" direction="pas"/>
<pin name="PGND_6" direction="pas"/>
<pin name="PGND_7" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="ROUT05" direction="out"/>
<pin name="ROUT07" direction="out"/>
<pin name="ROUT06" direction="out"/>
<pin name="ROUT08" direction="out"/>
<pin name="ROUT09" direction="out"/>
<pin name="ROUT55" direction="out"/>
<pin name="ROUT56" direction="out"/>
<pin name="ROUT57" direction="out"/>
<pin name="ROUT58" direction="out"/>
<pin name="ROUT59" direction="out"/>
<pin name="~LOCK0" direction="out"/>
<pin name="~LOCK5" direction="out"/>
<pin name="CHTST" direction="out"/>
</symbol>
<symbol name="SCAN921260UJB_B">
<pin name="PVDD_2" direction="pwr"/>
<pin name="PVDD_3" direction="pwr"/>
<pin name="PVDD_4" direction="pwr"/>
<pin name="PVDD_5" direction="pwr"/>
<pin name="PVDD_6" direction="pwr"/>
<pin name="PVDD_7" direction="pwr"/>
<pin name="PVDD_8" direction="pwr"/>
<pin name="PVDD" direction="pwr"/>
<pin name="DVDD_2" direction="pwr"/>
<pin name="DVDD_3" direction="pwr"/>
<pin name="DVDD_4" direction="pwr"/>
<pin name="DVDD_5" direction="pwr"/>
<pin name="DVDD_6" direction="pwr"/>
<pin name="DVDD_7" direction="pwr"/>
<pin name="DVDD_8" direction="pwr"/>
<pin name="DVDD_9" direction="pwr"/>
<pin name="DVDD_10" direction="pwr"/>
<pin name="DVDD_11" direction="pwr"/>
<pin name="DVDD" direction="pwr"/>
<pin name="BIST_ACT" direction="in"/>
<pin name="RCLK1" direction="in"/>
<pin name="RCLK2" direction="in"/>
<pin name="RCLK3" direction="in"/>
<pin name="RCLK4" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="DGND_2" direction="pas"/>
<pin name="DGND_3" direction="pas"/>
<pin name="DGND_4" direction="pas"/>
<pin name="DGND_5" direction="pas"/>
<pin name="DGND_6" direction="pas"/>
<pin name="PGND_2" direction="pas"/>
<pin name="PGND_3" direction="pas"/>
<pin name="PGND_4" direction="pas"/>
<pin name="PGND_5" direction="pas"/>
<pin name="PGND_6" direction="pas"/>
<pin name="PGND_7" direction="pas"/>
<pin name="PGND_8" direction="pas"/>
<pin name="PGND_9" direction="pas"/>
<pin name="PGND" direction="pas"/>
<pin name="DGND_7" direction="pas"/>
<pin name="DGND_8" direction="pas"/>
<pin name="DGND_9" direction="pas"/>
<pin name="DGND" direction="pas"/>
<pin name="ROUT00" direction="out"/>
<pin name="ROUT01" direction="out"/>
<pin name="ROUT02" direction="out"/>
<pin name="ROUT03" direction="out"/>
<pin name="ROUT04" direction="out"/>
<pin name="ROUT10" direction="out"/>
<pin name="ROUT11" direction="out"/>
<pin name="ROUT12" direction="out"/>
<pin name="ROUT13" direction="out"/>
<pin name="ROUT14" direction="out"/>
<pin name="ROUT15" direction="out"/>
<pin name="ROUT16" direction="out"/>
<pin name="ROUT17" direction="out"/>
<pin name="ROUT18" direction="out"/>
<pin name="ROUT19" direction="out"/>
<pin name="ROUT20" direction="out"/>
<pin name="ROUT21" direction="out"/>
<pin name="ROUT22" direction="out"/>
<pin name="ROUT23" direction="out"/>
<pin name="ROUT24" direction="out"/>
<pin name="ROUT25" direction="out"/>
<pin name="ROUT26" direction="out"/>
<pin name="ROUT27" direction="out"/>
<pin name="ROUT28" direction="out"/>
<pin name="ROUT29" direction="out"/>
<pin name="ROUT30" direction="out"/>
<pin name="ROUT31" direction="out"/>
<pin name="ROUT32" direction="out"/>
<pin name="ROUT33" direction="out"/>
<pin name="ROUT34" direction="out"/>
<pin name="ROUT35" direction="out"/>
<pin name="ROUT36" direction="out"/>
<pin name="ROUT37" direction="out"/>
<pin name="ROUT38" direction="out"/>
<pin name="ROUT39" direction="out"/>
<pin name="ROUT40" direction="out"/>
<pin name="ROUT41" direction="out"/>
<pin name="ROUT42" direction="out"/>
<pin name="ROUT43" direction="out"/>
<pin name="ROUT44" direction="out"/>
<pin name="ROUT45" direction="out"/>
<pin name="ROUT46" direction="out"/>
<pin name="ROUT47" direction="out"/>
<pin name="ROUT48" direction="out"/>
<pin name="ROUT49" direction="out"/>
<pin name="ROUT50" direction="out"/>
<pin name="ROUT51" direction="out"/>
<pin name="ROUT52" direction="out"/>
<pin name="ROUT53" direction="out"/>
<pin name="ROUT54" direction="out"/>
<pin name="~LOCK1" direction="out"/>
<pin name="~LOCK2" direction="out"/>
<pin name="~LOCK3" direction="out"/>
<pin name="~LOCK4" direction="out"/>
</symbol>
<symbol name="SCANSTA101SM">
<pin name="VDD_2" direction="pwr"/>
<pin name="VDD_3" direction="pwr"/>
<pin name="VDD_4" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="TCK" direction="in"/>
<pin name="SCK" direction="in"/>
<pin name="~CE" direction="in"/>
<pin name="~OE" direction="in"/>
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="~RST" direction="in"/>
<pin name="~TRST" direction="in"/>
<pin name="~STB" direction="in"/>
<pin name="TMS" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="R/~W" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="TDO" direction="out"/>
<pin name="INT" direction="out"/>
<pin name="~DTACK" direction="out"/>
<pin name="~TRST0_SM" direction="out"/>
<pin name="TRSIT_SM" direction="out"/>
<pin name="TDO_SM" direction="out"/>
<pin name="TCK_SM" direction="out"/>
<pin name="TDI_SM" direction="out"/>
<pin name="TMS_SM" direction="pas"/>
<pin name="D0"/>
<pin name="D1"/>
<pin name="D2"/>
<pin name="D3"/>
<pin name="D4"/>
<pin name="D5"/>
<pin name="D6"/>
<pin name="D7"/>
<pin name="D8"/>
<pin name="D9"/>
<pin name="D10"/>
<pin name="D11"/>
<pin name="D12"/>
<pin name="D13"/>
<pin name="D14"/>
<pin name="D15"/>
</symbol>
<symbol name="SCANSTA111MT">
<pin name="VCC_2" direction="pwr"/>
<pin name="VCC_3" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="TCKB" direction="in"/>
<pin name="~TRST~B" direction="in"/>
<pin name="~OE" direction="in"/>
<pin name="~TEST-~ENABLE" direction="in"/>
<pin name="S0" direction="in"/>
<pin name="S1" direction="in"/>
<pin name="S2" direction="in"/>
<pin name="S3" direction="in"/>
<pin name="S4" direction="in"/>
<pin name="S5" direction="in"/>
<pin name="S6" direction="in"/>
<pin name="TMSB" direction="in"/>
<pin name="TDIB" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="AB" direction="in"/>
<pin name="A0" direction="in"/>
<pin name="TDI0" direction="in"/>
<pin name="TDI1" direction="in"/>
<pin name="TDI2" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="Y1" direction="out"/>
<pin name="Y0" direction="out"/>
<pin name="YB" direction="out"/>
<pin name="TDO0" direction="out"/>
<pin name="TDO1" direction="out"/>
<pin name="TDO2" direction="out"/>
<pin name="TDOB" direction="out"/>
<pin name="TRIST1" direction="out"/>
<pin name="TRIST2" direction="out"/>
<pin name="~TRST1" direction="out"/>
<pin name="~TRST2" direction="out"/>
<pin name="TRIST0" direction="out"/>
<pin name="~TRST0" direction="out"/>
<pin name="TRISTB" direction="out"/>
<pin name="TCK0" direction="out"/>
<pin name="TCK1" direction="out"/>
<pin name="TCK2" direction="out"/>
<pin name="TMS0" direction="out"/>
<pin name="TMS1" direction="out"/>
<pin name="TMS2" direction="out"/>
<pin name="LSP_ACTIVE_0" direction="out"/>
<pin name="LSP_ACTIVE1" direction="out"/>
<pin name="LSP_ACTIVE2" direction="out"/>
</symbol>
<symbol name="SCANSTA112SM">
<pin name="VCC_2" direction="pwr"/>
<pin name="VCC_3" direction="pwr"/>
<pin name="VCC_4" direction="pwr"/>
<pin name="VCC_5" direction="pwr"/>
<pin name="VCC_6" direction="pwr"/>
<pin name="VCC_7" direction="pwr"/>
<pin name="VCC_8" direction="pwr"/>
<pin name="VCC_9" direction="pwr"/>
<pin name="VCC_10" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="~OE" direction="in"/>
<pin name="S0" direction="in"/>
<pin name="S1" direction="in"/>
<pin name="S2" direction="in"/>
<pin name="S3" direction="in"/>
<pin name="S4" direction="in"/>
<pin name="S5" direction="in"/>
<pin name="S6" direction="in"/>
<pin name="S7" direction="in"/>
<pin name="LSPSEL0" direction="in"/>
<pin name="LSPSEL1" direction="in"/>
<pin name="LSPSEL2" direction="in"/>
<pin name="LSPSEL3" direction="in"/>
<pin name="LSPSEL4" direction="in"/>
<pin name="LSPSEL5" direction="in"/>
<pin name="LSPSEL6" direction="in"/>
<pin name="A101" direction="in"/>
<pin name="A1B1" direction="in"/>
<pin name="A1B0" direction="in"/>
<pin name="ADDMASK" direction="in"/>
<pin name="TRANS" direction="in"/>
<pin name="SB/~S" direction="in"/>
<pin name="A0B1" direction="in"/>
<pin name="A001" direction="in"/>
<pin name="A0B0" direction="in"/>
<pin name="~RESET" direction="in"/>
<pin name="TDIB0" direction="in"/>
<pin name="TRISTB0"/>
<pin name="MPSELB1/~B0" direction="in"/>
<pin name="TLRTRST" direction="in"/>
<pin name="TLRTRST6" direction="in"/>
<pin name="TDI04" direction="in"/>
<pin name="TDI01" direction="in"/>
<pin name="TDO03"/>
<pin name="TDI06" direction="in"/>
<pin name="TDIB1" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="TCK01" direction="out"/>
<pin name="TCK02" direction="out"/>
<pin name="TCK03" direction="out"/>
<pin name="TCK04" direction="out"/>
<pin name="TCK05" direction="out"/>
<pin name="TCK06" direction="out"/>
<pin name="TMS01" direction="out"/>
<pin name="TMS02" direction="out"/>
<pin name="TMS03" direction="out"/>
<pin name="TMS04" direction="out"/>
<pin name="TMS05" direction="out"/>
<pin name="TMS06" direction="out"/>
<pin name="~TRSTB1" direction="out"/>
<pin name="TRISTB1" direction="out"/>
<pin name="~TRST04" direction="out"/>
<pin name="~TRST05" direction="out"/>
<pin name="TDO01" direction="out"/>
<pin name="TDO02" direction="out"/>
<pin name="TDO04" direction="out"/>
<pin name="TDO05" direction="out"/>
<pin name="~TRST06" direction="out"/>
<pin name="~TRST03" direction="out"/>
<pin name="TRIST03" direction="out"/>
<pin name="~TRST02" direction="out"/>
<pin name="~TRSTB0"/>
<pin name="TDI02" direction="out"/>
<pin name="TDI03" direction="out"/>
<pin name="TDI05" direction="out"/>
<pin name="TDO06" direction="out"/>
<pin name="TDOB0"/>
<pin name="TDOB1"/>
<pin name="TMSB0"/>
<pin name="TMSB1"/>
<pin name="Y0B0" direction="out"/>
<pin name="Y1B1" direction="out"/>
<pin name="Y001" direction="out"/>
<pin name="Y101" direction="out"/>
<pin name="Y1B0" direction="out"/>
<pin name="Y0B1" direction="out"/>
<pin name="TRIST01" direction="out"/>
<pin name="~TRST01" direction="out"/>
<pin name="TRIST02" direction="out"/>
<pin name="TCKB0"/>
<pin name="TCKB1"/>
</symbol>
<symbol name="SCANSTA112VS">
<pin name="VCC_2" direction="pwr"/>
<pin name="VCC_3" direction="pwr"/>
<pin name="VCC_4" direction="pwr"/>
<pin name="VCC_5" direction="pwr"/>
<pin name="VCC_6" direction="pwr"/>
<pin name="VCC_7" direction="pwr"/>
<pin name="VCC_8" direction="pwr"/>
<pin name="VCC_9" direction="pwr"/>
<pin name="VCC_10" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="TCKB0"/>
<pin name="TCKB1"/>
<pin name="S0" direction="in"/>
<pin name="S1" direction="in"/>
<pin name="S2" direction="in"/>
<pin name="S3" direction="in"/>
<pin name="S4" direction="in"/>
<pin name="S5" direction="in"/>
<pin name="S6" direction="in"/>
<pin name="S7" direction="in"/>
<pin name="~RESET" direction="in"/>
<pin name="ADDMASK" direction="in"/>
<pin name="TRANS" direction="in"/>
<pin name="SB/~S" direction="in"/>
<pin name="~OE" direction="in"/>
<pin name="LSPSEL0" direction="in"/>
<pin name="LSPSEL1" direction="in"/>
<pin name="LSPSEL2" direction="in"/>
<pin name="LSPSEL3" direction="in"/>
<pin name="LSPSEL4" direction="in"/>
<pin name="LSPSEL5" direction="in"/>
<pin name="LSPSEL6" direction="in"/>
<pin name="TDIB0" direction="in"/>
<pin name="TDOB0"/>
<pin name="~TRSTB0"/>
<pin name="~TRSTB1"/>
<pin name="A1B0" direction="in"/>
<pin name="A0B0" direction="in"/>
<pin name="A0B1" direction="in"/>
<pin name="A1B1" direction="in"/>
<pin name="TDIB1" direction="in"/>
<pin name="TDOB1"/>
<pin name="TMSB1"/>
<pin name="TMSB0"/>
<pin name="TLR_TRST" direction="in"/>
<pin name="TLR_TRST6" direction="in"/>
<pin name="MPSELB1/~B0" direction="in"/>
<pin name="A101" direction="in"/>
<pin name="A001" direction="in"/>
<pin name="TDI01" direction="in"/>
<pin name="TDI02" direction="in"/>
<pin name="TDI03" direction="in"/>
<pin name="TDI04" direction="in"/>
<pin name="TDI05" direction="in"/>
<pin name="TDI06" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND_6" direction="pas"/>
<pin name="GND_7" direction="pas"/>
<pin name="GND_8" direction="pas"/>
<pin name="GND_9" direction="pas"/>
<pin name="GND_10" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="TRISTB0" direction="out"/>
<pin name="TRSITB1" direction="out"/>
<pin name="TDO01" direction="out"/>
<pin name="TDO02" direction="out"/>
<pin name="TDO03" direction="out"/>
<pin name="TDO04" direction="out"/>
<pin name="TD005" direction="out"/>
<pin name="TDO06" direction="out"/>
<pin name="TMS01" direction="out"/>
<pin name="TMS02" direction="out"/>
<pin name="TMS03" direction="out"/>
<pin name="TMS04" direction="out"/>
<pin name="TMS05" direction="out"/>
<pin name="TMS06" direction="out"/>
<pin name="~TRST~01" direction="out"/>
<pin name="TRIST01" direction="out"/>
<pin name="~TRST02" direction="out"/>
<pin name="TRIST02" direction="out"/>
<pin name="TCK01" direction="out"/>
<pin name="TCK02" direction="out"/>
<pin name="TCK03" direction="out"/>
<pin name="TCK04" direction="out"/>
<pin name="TCK05" direction="out"/>
<pin name="TCK06" direction="out"/>
<pin name="~TRST03" direction="out"/>
<pin name="TRIST03" direction="out"/>
<pin name="~TRST04" direction="out"/>
<pin name="~TRST05" direction="out"/>
<pin name="~TRST06" direction="out"/>
<pin name="Y101" direction="out"/>
<pin name="Y001" direction="out"/>
<pin name="Y0B1" direction="out"/>
<pin name="Y0B0" direction="out"/>
<pin name="Y1B0" direction="out"/>
<pin name="Y1B1" direction="out"/>
</symbol>
<symbol name="SCANSTA476TSD">
<pin name="VDD_2" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="VREF" direction="in"/>
<pin name="~TRST" direction="pas"/>
<pin name="TDI" direction="in"/>
<pin name="TMS" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="A5" direction="in"/>
<pin name="A6" direction="in"/>
<pin name="A7" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="TDO" direction="out"/>
</symbol>
<symbol name="TL082CM">
<pin name="-INA" direction="in"/>
<pin name="+INA" direction="in"/>
<pin name="-INB" direction="in"/>
<pin name="+INB" direction="in"/>
<pin name="V+" direction="pas"/>
<pin name="V-" direction="pas"/>
<pin name="OUTB" direction="out"/>
<pin name="OUTA" direction="out"/>
</symbol>
<symbol name="TL082CP">
<pin name="-INA" direction="in"/>
<pin name="+INA" direction="in"/>
<pin name="-INB" direction="in"/>
<pin name="+INB" direction="in"/>
<pin name="V+" direction="pas"/>
<pin name="V-" direction="pas"/>
<pin name="OUTB" direction="out"/>
<pin name="OUTA" direction="out"/>
</symbol>
<symbol name="LM1086IS-3.3">
<pin name="IN" direction="in"/>
<pin name="ADJ/GND" direction="pas"/>
<pin name="OUT" direction="out"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LM1086IS-1.8">
<pin name="IN" direction="in"/>
<pin name="ADJ/GND" direction="pas"/>
<pin name="OUT" direction="out"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LM1086CS-ADJ">
<pin name="IN" direction="in"/>
<pin name="ADJ/GND" direction="pas"/>
<pin name="OUT" direction="out"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LM1086IS-5.0">
<pin name="IN" direction="in"/>
<pin name="ADJ/GND" direction="pas"/>
<pin name="OUT" direction="out"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LM1086CS-3.3">
<pin name="IN" direction="in"/>
<pin name="ADJ/GND" direction="pas"/>
<pin name="OUT" direction="out"/>
<pin name="VOUT" direction="out"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="ADC0801LCN" prefix="U">
<description>A/D converters</description>
<gates>
<gate name="A" symbol="ADC0801LCN"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-20">
<connects>
<connect gate="A" pin="AGND" pad="8"/>
<connect gate="A" pin="CLKIN" pad="4"/>
<connect gate="A" pin="CLKR" pad="19"/>
<connect gate="A" pin="DB0" pad="18"/>
<connect gate="A" pin="DB1" pad="17"/>
<connect gate="A" pin="DB2" pad="16"/>
<connect gate="A" pin="DB3" pad="15"/>
<connect gate="A" pin="DB4" pad="14"/>
<connect gate="A" pin="DB5" pad="13"/>
<connect gate="A" pin="DB6" pad="12"/>
<connect gate="A" pin="DB7" pad="11"/>
<connect gate="A" pin="DGND" pad="10"/>
<connect gate="A" pin="VCC" pad="20"/>
<connect gate="A" pin="VIN+" pad="6"/>
<connect gate="A" pin="VIN-" pad="7"/>
<connect gate="A" pin="VREF/2" pad="9"/>
<connect gate="A" pin="~CS" pad="1"/>
<connect gate="A" pin="~INTR" pad="5"/>
<connect gate="A" pin="~RD" pad="2"/>
<connect gate="A" pin="~WR" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DESCRIPTION" value="A/D converters"/>
<attribute name="MPN" value="ADC0801LCN"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K1419"/>
<attribute name="PACKAGE" value="DIP-20"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADC0802LCN" prefix="U">
<description>A/D converters</description>
<gates>
<gate name="A" symbol="ADC0802LCN"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-20">
<connects>
<connect gate="A" pin="AGND" pad="8"/>
<connect gate="A" pin="CLKIN" pad="4"/>
<connect gate="A" pin="CLKR" pad="19"/>
<connect gate="A" pin="DB0" pad="18"/>
<connect gate="A" pin="DB1" pad="17"/>
<connect gate="A" pin="DB2" pad="16"/>
<connect gate="A" pin="DB3" pad="15"/>
<connect gate="A" pin="DB4" pad="14"/>
<connect gate="A" pin="DB5" pad="13"/>
<connect gate="A" pin="DB6" pad="12"/>
<connect gate="A" pin="DB7" pad="11"/>
<connect gate="A" pin="DGND" pad="10"/>
<connect gate="A" pin="VCC" pad="20"/>
<connect gate="A" pin="VIN+" pad="6"/>
<connect gate="A" pin="VIN-" pad="7"/>
<connect gate="A" pin="VREF/2" pad="9"/>
<connect gate="A" pin="~CS" pad="1"/>
<connect gate="A" pin="~INTR" pad="5"/>
<connect gate="A" pin="~RD" pad="2"/>
<connect gate="A" pin="~WR" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DESCRIPTION" value="A/D converters"/>
<attribute name="MPN" value="ADC0802LCN"/>
<attribute name="OC_FARNELL" value="1367571"/>
<attribute name="OC_NEWARK" value="07B4579"/>
<attribute name="PACKAGE" value="DIP-20"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADC0803LCN" prefix="U">
<description>A/D Converter</description>
<gates>
<gate name="A" symbol="ADC0803LCN"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-20">
<connects>
<connect gate="A" pin="AGND" pad="8"/>
<connect gate="A" pin="CLK_IN" pad="4"/>
<connect gate="A" pin="CLK_R" pad="19"/>
<connect gate="A" pin="DB0" pad="18"/>
<connect gate="A" pin="DB1" pad="17"/>
<connect gate="A" pin="DB2" pad="16"/>
<connect gate="A" pin="DB3" pad="15"/>
<connect gate="A" pin="DB4" pad="14"/>
<connect gate="A" pin="DB5" pad="13"/>
<connect gate="A" pin="DB6" pad="12"/>
<connect gate="A" pin="DB7" pad="11"/>
<connect gate="A" pin="DGND" pad="10"/>
<connect gate="A" pin="VCC" pad="20"/>
<connect gate="A" pin="VIN+" pad="6"/>
<connect gate="A" pin="VIN-" pad="7"/>
<connect gate="A" pin="VREF/2" pad="9"/>
<connect gate="A" pin="~CS" pad="1"/>
<connect gate="A" pin="~INTR" pad="5"/>
<connect gate="A" pin="~RD" pad="2"/>
<connect gate="A" pin="~WR" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="ADC0803LCN"/>
<attribute name="OC_FARNELL" value="9486577"/>
<attribute name="OC_NEWARK" value="41K1423"/>
<attribute name="PACKAGE" value="20-DIP"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADC0804LCN" prefix="U">
<description>A/D Converter</description>
<gates>
<gate name="A" symbol="ADC0804LCN"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-20">
<connects>
<connect gate="A" pin="AGND" pad="8"/>
<connect gate="A" pin="CLK_IN" pad="4"/>
<connect gate="A" pin="CLK_R" pad="19"/>
<connect gate="A" pin="DB0" pad="18"/>
<connect gate="A" pin="DB1" pad="17"/>
<connect gate="A" pin="DB2" pad="16"/>
<connect gate="A" pin="DB3" pad="15"/>
<connect gate="A" pin="DB4" pad="14"/>
<connect gate="A" pin="DB5" pad="13"/>
<connect gate="A" pin="DB6" pad="12"/>
<connect gate="A" pin="DB7" pad="11"/>
<connect gate="A" pin="DGND" pad="10"/>
<connect gate="A" pin="VCC" pad="20"/>
<connect gate="A" pin="VIN(+)" pad="6"/>
<connect gate="A" pin="VIN(-)" pad="7"/>
<connect gate="A" pin="VREF/2" pad="9"/>
<connect gate="A" pin="~CS" pad="1"/>
<connect gate="A" pin="~INTR" pad="5"/>
<connect gate="A" pin="~RD" pad="2"/>
<connect gate="A" pin="~WR" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="ADC0804LCN"/>
<attribute name="OC_FARNELL" value="9486593"/>
<attribute name="OC_NEWARK" value="07B4596"/>
<attribute name="PACKAGE" value="20-DIP"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADC0804LCWM" prefix="U">
<description>A/D converters</description>
<gates>
<gate name="A" symbol="ADC0804LCWM"/>
</gates>
<devices>
<device name="" package="SOIC127P1032X264-20N">
<connects>
<connect gate="A" pin="AGND" pad="8"/>
<connect gate="A" pin="CLKIN" pad="4"/>
<connect gate="A" pin="CLKR" pad="19"/>
<connect gate="A" pin="DB0" pad="18"/>
<connect gate="A" pin="DB1" pad="17"/>
<connect gate="A" pin="DB2" pad="16"/>
<connect gate="A" pin="DB3" pad="15"/>
<connect gate="A" pin="DB4" pad="14"/>
<connect gate="A" pin="DB5" pad="13"/>
<connect gate="A" pin="DB6" pad="12"/>
<connect gate="A" pin="DB7" pad="11"/>
<connect gate="A" pin="DGND" pad="10"/>
<connect gate="A" pin="VCC" pad="20"/>
<connect gate="A" pin="VIN+" pad="6"/>
<connect gate="A" pin="VIN-" pad="7"/>
<connect gate="A" pin="VREF/2" pad="9"/>
<connect gate="A" pin="~CS" pad="1"/>
<connect gate="A" pin="~INTR" pad="5"/>
<connect gate="A" pin="~RD" pad="2"/>
<connect gate="A" pin="~WR" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="ADC0804LCWM"/>
<attribute name="OC_FARNELL" value="9486585"/>
<attribute name="OC_NEWARK" value="07B4597"/>
<attribute name="PACKAGE" value="SOIC-20"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADC08060CIMT" prefix="U">
<description>A/D converters</description>
<gates>
<gate name="A" symbol="ADC08060CIMT"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-20N">
<connects>
<connect gate="A" pin="AGND" pad="11"/>
<connect gate="A" pin="AGND_2" pad="2"/>
<connect gate="A" pin="AGND_3" pad="5"/>
<connect gate="A" pin="AGND_4" pad="8"/>
<connect gate="A" pin="CLOCK" pad="24"/>
<connect gate="A" pin="D0" pad="22"/>
<connect gate="A" pin="D1" pad="21"/>
<connect gate="A" pin="D2" pad="20"/>
<connect gate="A" pin="D3" pad="19"/>
<connect gate="A" pin="D4" pad="16"/>
<connect gate="A" pin="D5" pad="15"/>
<connect gate="A" pin="D6" pad="14"/>
<connect gate="A" pin="D7" pad="13"/>
<connect gate="A" pin="DR_GND" pad="17"/>
<connect gate="A" pin="DR_VD" pad="18"/>
<connect gate="A" pin="PD" pad="23"/>
<connect gate="A" pin="VA" pad="4"/>
<connect gate="A" pin="VA_2" pad="1"/>
<connect gate="A" pin="VA_3" pad="12"/>
<connect gate="A" pin="VIN" pad="6"/>
<connect gate="A" pin="VIN_GND" pad="7"/>
<connect gate="A" pin="VRB" pad="10"/>
<connect gate="A" pin="VRM" pad="9"/>
<connect gate="A" pin="VRT" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="ADC08060CIMT"/>
<attribute name="OC_FARNELL" value="1673973"/>
<attribute name="OC_NEWARK" value="41K1432"/>
<attribute name="PACKAGE" value="TSSOP-20"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADC0808CCN" prefix="U">
<description>A/D Converter</description>
<gates>
<gate name="A" symbol="ADC0808CCN"/>
</gates>
<devices>
<device name="" package="DIP254P1524X483-28">
<connects>
<connect gate="A" pin="2_(1)" pad="21"/>
<connect gate="A" pin="2_(2)" pad="20"/>
<connect gate="A" pin="2_(3)" pad="19"/>
<connect gate="A" pin="2_(4)" pad="18"/>
<connect gate="A" pin="2_(5)" pad="8"/>
<connect gate="A" pin="2_(6)" pad="15"/>
<connect gate="A" pin="2_(7)" pad="14"/>
<connect gate="A" pin="2_(8)" pad="17"/>
<connect gate="A" pin="ADDA" pad="25"/>
<connect gate="A" pin="ADDB" pad="24"/>
<connect gate="A" pin="ADDC" pad="23"/>
<connect gate="A" pin="ALE" pad="22"/>
<connect gate="A" pin="CLK" pad="10"/>
<connect gate="A" pin="EOC" pad="7"/>
<connect gate="A" pin="GND" pad="13"/>
<connect gate="A" pin="IN0" pad="26"/>
<connect gate="A" pin="IN1" pad="27"/>
<connect gate="A" pin="IN2" pad="28"/>
<connect gate="A" pin="IN3" pad="1"/>
<connect gate="A" pin="IN4" pad="2"/>
<connect gate="A" pin="IN5" pad="3"/>
<connect gate="A" pin="IN6" pad="4"/>
<connect gate="A" pin="IN7" pad="5"/>
<connect gate="A" pin="OUT_EN" pad="9"/>
<connect gate="A" pin="START" pad="6"/>
<connect gate="A" pin="VCC" pad="11"/>
<connect gate="A" pin="VREF(+)" pad="12"/>
<connect gate="A" pin="VREF(-)" pad="16"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="ADC0808CCN"/>
<attribute name="OC_FARNELL" value="9486674"/>
<attribute name="OC_NEWARK" value="41K1435"/>
<attribute name="PACKAGE" value="28-DIP"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADC0808CCV" prefix="U">
<description>A/D converters</description>
<gates>
<gate name="A" symbol="ADC0808CCV"/>
</gates>
<devices>
<device name="" package="PLCC127P1245X1245X457-28N">
<connects>
<connect gate="A" pin="2_-1" pad="21"/>
<connect gate="A" pin="2_-2" pad="20"/>
<connect gate="A" pin="2_-3" pad="19"/>
<connect gate="A" pin="2_-4" pad="18"/>
<connect gate="A" pin="2_-5" pad="8"/>
<connect gate="A" pin="2_-6" pad="15"/>
<connect gate="A" pin="2_-7" pad="14"/>
<connect gate="A" pin="2_-8" pad="17"/>
<connect gate="A" pin="ADD_A" pad="25"/>
<connect gate="A" pin="ADD_B" pad="24"/>
<connect gate="A" pin="ADD_C" pad="23"/>
<connect gate="A" pin="ALE" pad="22"/>
<connect gate="A" pin="CLOCK" pad="10"/>
<connect gate="A" pin="EOC" pad="7"/>
<connect gate="A" pin="GND" pad="13"/>
<connect gate="A" pin="IN_0" pad="26"/>
<connect gate="A" pin="IN_1" pad="27"/>
<connect gate="A" pin="IN_2" pad="28"/>
<connect gate="A" pin="IN_3" pad="1"/>
<connect gate="A" pin="IN_4" pad="2"/>
<connect gate="A" pin="IN_5" pad="3"/>
<connect gate="A" pin="IN_6" pad="4"/>
<connect gate="A" pin="IN_7" pad="5"/>
<connect gate="A" pin="OUTPUT_ENABLE" pad="9"/>
<connect gate="A" pin="START" pad="6"/>
<connect gate="A" pin="VCC" pad="11"/>
<connect gate="A" pin="VREF(+)" pad="12"/>
<connect gate="A" pin="VREF(-)" pad="16"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="ADC0808CCV"/>
<attribute name="OC_FARNELL" value="1673957"/>
<attribute name="OC_NEWARK" value="41K1436"/>
<attribute name="PACKAGE" value="PLCC-28"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADC0809CCN" prefix="U">
<description>A/D Converter</description>
<gates>
<gate name="A" symbol="ADC0809CCN"/>
</gates>
<devices>
<device name="" package="DIP254P1524X483-28">
<connects>
<connect gate="A" pin="2_(1)" pad="21"/>
<connect gate="A" pin="2_(2)" pad="20"/>
<connect gate="A" pin="2_(3)" pad="19"/>
<connect gate="A" pin="2_(4)" pad="18"/>
<connect gate="A" pin="2_(5)" pad="8"/>
<connect gate="A" pin="2_(6)" pad="15"/>
<connect gate="A" pin="2_(7)" pad="14"/>
<connect gate="A" pin="2_(8)" pad="17"/>
<connect gate="A" pin="ADDA" pad="25"/>
<connect gate="A" pin="ADDB" pad="24"/>
<connect gate="A" pin="ADDC" pad="23"/>
<connect gate="A" pin="ALE" pad="22"/>
<connect gate="A" pin="CLK" pad="10"/>
<connect gate="A" pin="EOC" pad="7"/>
<connect gate="A" pin="GND" pad="13"/>
<connect gate="A" pin="IN0" pad="26"/>
<connect gate="A" pin="IN1" pad="27"/>
<connect gate="A" pin="IN2" pad="28"/>
<connect gate="A" pin="IN3" pad="1"/>
<connect gate="A" pin="IN4" pad="2"/>
<connect gate="A" pin="IN5" pad="3"/>
<connect gate="A" pin="IN6" pad="4"/>
<connect gate="A" pin="IN7" pad="5"/>
<connect gate="A" pin="OUT_EN" pad="9"/>
<connect gate="A" pin="START" pad="6"/>
<connect gate="A" pin="VCC" pad="11"/>
<connect gate="A" pin="VREF(+)" pad="12"/>
<connect gate="A" pin="VREF(-)" pad="16"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="ADC0809CCN"/>
<attribute name="OC_FARNELL" value="9486682"/>
<attribute name="OC_NEWARK" value="07B4614"/>
<attribute name="PACKAGE" value="28-DIP"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADC0809CCV" prefix="U">
<description>A/D converters</description>
<gates>
<gate name="A" symbol="ADC0809CCV"/>
</gates>
<devices>
<device name="" package="PLCC127P1245X1245X457-28N">
<connects>
<connect gate="A" pin="2_-1" pad="21"/>
<connect gate="A" pin="2_-2" pad="20"/>
<connect gate="A" pin="2_-3" pad="19"/>
<connect gate="A" pin="2_-4" pad="18"/>
<connect gate="A" pin="2_-5" pad="8"/>
<connect gate="A" pin="2_-6" pad="15"/>
<connect gate="A" pin="2_-7" pad="14"/>
<connect gate="A" pin="2_-8" pad="17"/>
<connect gate="A" pin="ADD_A" pad="25"/>
<connect gate="A" pin="ADD_B" pad="24"/>
<connect gate="A" pin="ADD_C" pad="23"/>
<connect gate="A" pin="ALE" pad="22"/>
<connect gate="A" pin="CLOCK" pad="10"/>
<connect gate="A" pin="EOC" pad="7"/>
<connect gate="A" pin="GND" pad="13"/>
<connect gate="A" pin="IN_0" pad="26"/>
<connect gate="A" pin="IN_1" pad="27"/>
<connect gate="A" pin="IN_2" pad="28"/>
<connect gate="A" pin="IN_3" pad="1"/>
<connect gate="A" pin="IN_4" pad="2"/>
<connect gate="A" pin="IN_5" pad="3"/>
<connect gate="A" pin="IN_6" pad="4"/>
<connect gate="A" pin="IN_7" pad="5"/>
<connect gate="A" pin="OUTPUT_ENABLE" pad="9"/>
<connect gate="A" pin="START" pad="6"/>
<connect gate="A" pin="VCC" pad="11"/>
<connect gate="A" pin="VREF(+)" pad="12"/>
<connect gate="A" pin="VREF(-)" pad="16"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="ADC0809CCV"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K1439"/>
<attribute name="PACKAGE" value="PLCC-28"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADC08100CIMTC" prefix="U">
<description>A/D Converter</description>
<gates>
<gate name="A" symbol="ADC08100CIMTC"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-24N">
<connects>
<connect gate="A" pin="AGND" pad="11"/>
<connect gate="A" pin="AGND_2" pad="2"/>
<connect gate="A" pin="AGND_3" pad="8"/>
<connect gate="A" pin="AGND_4" pad="5"/>
<connect gate="A" pin="CLK" pad="24"/>
<connect gate="A" pin="D0" pad="22"/>
<connect gate="A" pin="D1" pad="21"/>
<connect gate="A" pin="D2" pad="20"/>
<connect gate="A" pin="D3" pad="19"/>
<connect gate="A" pin="D4" pad="16"/>
<connect gate="A" pin="D5" pad="15"/>
<connect gate="A" pin="D6" pad="14"/>
<connect gate="A" pin="D7" pad="13"/>
<connect gate="A" pin="DRVD" pad="18"/>
<connect gate="A" pin="DR_GND" pad="17"/>
<connect gate="A" pin="PD" pad="23"/>
<connect gate="A" pin="VA" pad="1"/>
<connect gate="A" pin="VA_2" pad="4"/>
<connect gate="A" pin="VA_3" pad="12"/>
<connect gate="A" pin="VIN" pad="6"/>
<connect gate="A" pin="VIN_GND" pad="7"/>
<connect gate="A" pin="VRB" pad="10"/>
<connect gate="A" pin="VRM" pad="9"/>
<connect gate="A" pin="VRT" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="ADC08100CIMTC"/>
<attribute name="OC_FARNELL" value="8180679"/>
<attribute name="OC_NEWARK" value="41K1449"/>
<attribute name="PACKAGE" value="24-TSSOP"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADC081500CIYB" prefix="U">
<description>Low Power, 8-Bit, 1.5 GSPS A/D Converter</description>
<gates>
<gate name="A" symbol="ADC081500CIYB"/>
</gates>
<devices>
<device name="" package="QFP50P2200X2200X160-129N">
<connects>
<connect gate="A" pin="CAL" pad="30"/>
<connect gate="A" pin="CALDLY/~SCS" pad="127"/>
<connect gate="A" pin="CALRUN" pad="126"/>
<connect gate="A" pin="CLK+" pad="18"/>
<connect gate="A" pin="CLK-" pad="19"/>
<connect gate="A" pin="D0+" pad="103"/>
<connect gate="A" pin="D0-" pad="102"/>
<connect gate="A" pin="D1+" pad="101"/>
<connect gate="A" pin="D1-" pad="100"/>
<connect gate="A" pin="D2+" pad="96"/>
<connect gate="A" pin="D2-" pad="95"/>
<connect gate="A" pin="D3+" pad="94"/>
<connect gate="A" pin="D3-" pad="93"/>
<connect gate="A" pin="D4+" pad="92"/>
<connect gate="A" pin="D4-" pad="91"/>
<connect gate="A" pin="D5+" pad="90"/>
<connect gate="A" pin="D5-" pad="89"/>
<connect gate="A" pin="D6+" pad="86"/>
<connect gate="A" pin="D6-" pad="85"/>
<connect gate="A" pin="D7+" pad="84"/>
<connect gate="A" pin="D7-" pad="83"/>
<connect gate="A" pin="DCLK+" pad="82"/>
<connect gate="A" pin="DCLK-" pad="81"/>
<connect gate="A" pin="DCLK_RST" pad="15"/>
<connect gate="A" pin="DD0+" pad="125"/>
<connect gate="A" pin="DD0-" pad="124"/>
<connect gate="A" pin="DD1+" pad="123"/>
<connect gate="A" pin="DD1-" pad="122"/>
<connect gate="A" pin="DD2+" pad="118"/>
<connect gate="A" pin="DD2-" pad="117"/>
<connect gate="A" pin="DD3+" pad="116"/>
<connect gate="A" pin="DD3-" pad="115"/>
<connect gate="A" pin="DD4+" pad="114"/>
<connect gate="A" pin="DD4-" pad="113"/>
<connect gate="A" pin="DD5+" pad="112"/>
<connect gate="A" pin="DD5-" pad="111"/>
<connect gate="A" pin="DD6+" pad="107"/>
<connect gate="A" pin="DD6-" pad="106"/>
<connect gate="A" pin="DD7+" pad="105"/>
<connect gate="A" pin="DD7-" pad="104"/>
<connect gate="A" pin="DR_GND" pad="119"/>
<connect gate="A" pin="DR_GND_2" pad="42"/>
<connect gate="A" pin="DR_GND_3" pad="108"/>
<connect gate="A" pin="DR_GND_4" pad="74"/>
<connect gate="A" pin="DR_GND_5" pad="87"/>
<connect gate="A" pin="DR_GND_6" pad="53"/>
<connect gate="A" pin="DR_GND_7" pad="64"/>
<connect gate="A" pin="DR_GND_8" pad="97"/>
<connect gate="A" pin="EPAD" pad="129"/>
<connect gate="A" pin="FSR/ECE" pad="14"/>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="GND_2" pad="1"/>
<connect gate="A" pin="GND_3" pad="12"/>
<connect gate="A" pin="GND_4" pad="24"/>
<connect gate="A" pin="GND_5" pad="27"/>
<connect gate="A" pin="GND_6" pad="21"/>
<connect gate="A" pin="GND_7" pad="9"/>
<connect gate="A" pin="GND_8" pad="41"/>
<connect gate="A" pin="NC" pad="61"/>
<connect gate="A" pin="NC_10" pad="77"/>
<connect gate="A" pin="NC_11" pad="78"/>
<connect gate="A" pin="NC_12" pad="109"/>
<connect gate="A" pin="NC_13" pad="98"/>
<connect gate="A" pin="NC_14" pad="120"/>
<connect gate="A" pin="NC_15" pad="36"/>
<connect gate="A" pin="NC_16" pad="37"/>
<connect gate="A" pin="NC_17" pad="38"/>
<connect gate="A" pin="NC_18" pad="39"/>
<connect gate="A" pin="NC_19" pad="43"/>
<connect gate="A" pin="NC_2" pad="67"/>
<connect gate="A" pin="NC_20" pad="44"/>
<connect gate="A" pin="NC_21" pad="45"/>
<connect gate="A" pin="NC_22" pad="46"/>
<connect gate="A" pin="NC_23" pad="52"/>
<connect gate="A" pin="NC_24" pad="29"/>
<connect gate="A" pin="NC_25" pad="47"/>
<connect gate="A" pin="NC_26" pad="54"/>
<connect gate="A" pin="NC_27" pad="48"/>
<connect gate="A" pin="NC_28" pad="55"/>
<connect gate="A" pin="NC_29" pad="49"/>
<connect gate="A" pin="NC_3" pad="22"/>
<connect gate="A" pin="NC_30" pad="56"/>
<connect gate="A" pin="NC_31" pad="50"/>
<connect gate="A" pin="NC_32" pad="63"/>
<connect gate="A" pin="NC_33" pad="57"/>
<connect gate="A" pin="NC_34" pad="71"/>
<connect gate="A" pin="NC_35" pad="58"/>
<connect gate="A" pin="NC_36" pad="72"/>
<connect gate="A" pin="NC_37" pad="59"/>
<connect gate="A" pin="NC_38" pad="65"/>
<connect gate="A" pin="NC_39" pad="60"/>
<connect gate="A" pin="NC_4" pad="68"/>
<connect gate="A" pin="NC_40" pad="66"/>
<connect gate="A" pin="NC_5" pad="23"/>
<connect gate="A" pin="NC_6" pad="69"/>
<connect gate="A" pin="NC_7" pad="70"/>
<connect gate="A" pin="NC_8" pad="75"/>
<connect gate="A" pin="NC_9" pad="76"/>
<connect gate="A" pin="OR+" pad="79"/>
<connect gate="A" pin="OR-" pad="80"/>
<connect gate="A" pin="OUTV/SCLK" pad="3"/>
<connect gate="A" pin="OUT_EDGE/DDR/SDATA" pad="4"/>
<connect gate="A" pin="PD" pad="26"/>
<connect gate="A" pin="REXT" pad="32"/>
<connect gate="A" pin="TDIODE_N" pad="35"/>
<connect gate="A" pin="TDIODE_P" pad="34"/>
<connect gate="A" pin="VA" pad="128"/>
<connect gate="A" pin="VA_10" pad="25"/>
<connect gate="A" pin="VA_11" pad="28"/>
<connect gate="A" pin="VA_2" pad="5"/>
<connect gate="A" pin="VA_3" pad="2"/>
<connect gate="A" pin="VA_4" pad="8"/>
<connect gate="A" pin="VA_5" pad="16"/>
<connect gate="A" pin="VA_6" pad="13"/>
<connect gate="A" pin="VA_7" pad="33"/>
<connect gate="A" pin="VA_8" pad="17"/>
<connect gate="A" pin="VA_9" pad="20"/>
<connect gate="A" pin="VBG" pad="31"/>
<connect gate="A" pin="VCMO" pad="7"/>
<connect gate="A" pin="VDR" pad="99"/>
<connect gate="A" pin="VDR_2" pad="51"/>
<connect gate="A" pin="VDR_3" pad="62"/>
<connect gate="A" pin="VDR_4" pad="40"/>
<connect gate="A" pin="VDR_5" pad="121"/>
<connect gate="A" pin="VDR_6" pad="73"/>
<connect gate="A" pin="VDR_7" pad="110"/>
<connect gate="A" pin="VDR_8" pad="88"/>
<connect gate="A" pin="VIN+" pad="11"/>
<connect gate="A" pin="VIN-" pad="10"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="ADC081500CIYB"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="69K1488"/>
<attribute name="PACKAGE" value="QFP-128"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADC0816CCN" prefix="U">
<description>A/D converters</description>
<gates>
<gate name="A" symbol="ADC0816CCN"/>
</gates>
<devices>
<device name="" package="DIP254P1524X533-40">
<connects>
<connect gate="A" pin="2_-1" pad="31"/>
<connect gate="A" pin="2_-2" pad="30"/>
<connect gate="A" pin="2_-3" pad="29"/>
<connect gate="A" pin="2_-4" pad="28"/>
<connect gate="A" pin="2_-5" pad="27"/>
<connect gate="A" pin="2_-6" pad="26"/>
<connect gate="A" pin="2_-7" pad="25"/>
<connect gate="A" pin="2_-8" pad="24"/>
<connect gate="A" pin="ADD_A" pad="36"/>
<connect gate="A" pin="ADD_B" pad="35"/>
<connect gate="A" pin="ADD_C" pad="34"/>
<connect gate="A" pin="ADD_D" pad="33"/>
<connect gate="A" pin="ALE" pad="32"/>
<connect gate="A" pin="CLOCK" pad="22"/>
<connect gate="A" pin="COMPARATOR_IN" pad="18"/>
<connect gate="A" pin="EOC" pad="13"/>
<connect gate="A" pin="EXPANSION_CONTROL" pad="37"/>
<connect gate="A" pin="GND" pad="20"/>
<connect gate="A" pin="IN0" pad="38"/>
<connect gate="A" pin="IN1" pad="39"/>
<connect gate="A" pin="IN10" pad="8"/>
<connect gate="A" pin="IN11" pad="9"/>
<connect gate="A" pin="IN12" pad="10"/>
<connect gate="A" pin="IN13" pad="11"/>
<connect gate="A" pin="IN14" pad="12"/>
<connect gate="A" pin="IN15" pad="14"/>
<connect gate="A" pin="IN2" pad="40"/>
<connect gate="A" pin="IN3" pad="1"/>
<connect gate="A" pin="IN4" pad="2"/>
<connect gate="A" pin="IN5" pad="3"/>
<connect gate="A" pin="IN6" pad="4"/>
<connect gate="A" pin="IN7" pad="5"/>
<connect gate="A" pin="IN8" pad="6"/>
<connect gate="A" pin="IN9" pad="7"/>
<connect gate="A" pin="MULTIPLEXER_OUT" pad="15"/>
<connect gate="A" pin="OUTPUT_ENABLE" pad="21"/>
<connect gate="A" pin="REF(+)" pad="19"/>
<connect gate="A" pin="REF(-)" pad="23"/>
<connect gate="A" pin="START" pad="16"/>
<connect gate="A" pin="VCC" pad="17"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="ADC0816CCN"/>
<attribute name="OC_FARNELL" value="1564674"/>
<attribute name="OC_NEWARK" value="41K1454"/>
<attribute name="PACKAGE" value="DIP-40"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADC0817CCN" prefix="U">
<description>A/D Converter</description>
<gates>
<gate name="A" symbol="ADC0817CCN"/>
</gates>
<devices>
<device name="" package="DIP254P1524X533-40">
<connects>
<connect gate="A" pin="2_1" pad="31"/>
<connect gate="A" pin="2_2" pad="30"/>
<connect gate="A" pin="2_3" pad="29"/>
<connect gate="A" pin="2_4" pad="28"/>
<connect gate="A" pin="2_5" pad="27"/>
<connect gate="A" pin="2_6" pad="26"/>
<connect gate="A" pin="2_7" pad="25"/>
<connect gate="A" pin="2_8" pad="24"/>
<connect gate="A" pin="ADD_A" pad="36"/>
<connect gate="A" pin="ADD_B" pad="35"/>
<connect gate="A" pin="ADD_C" pad="34"/>
<connect gate="A" pin="ADD_D" pad="33"/>
<connect gate="A" pin="ALE" pad="32"/>
<connect gate="A" pin="CLK" pad="22"/>
<connect gate="A" pin="COMPARATOR_IN" pad="18"/>
<connect gate="A" pin="EOC" pad="13"/>
<connect gate="A" pin="EXPANSION_CONTROL" pad="37"/>
<connect gate="A" pin="GND" pad="20"/>
<connect gate="A" pin="IN0" pad="38"/>
<connect gate="A" pin="IN1" pad="39"/>
<connect gate="A" pin="IN10" pad="8"/>
<connect gate="A" pin="IN11" pad="9"/>
<connect gate="A" pin="IN12" pad="10"/>
<connect gate="A" pin="IN13" pad="11"/>
<connect gate="A" pin="IN14" pad="12"/>
<connect gate="A" pin="IN15" pad="14"/>
<connect gate="A" pin="IN2" pad="40"/>
<connect gate="A" pin="IN3" pad="1"/>
<connect gate="A" pin="IN4" pad="2"/>
<connect gate="A" pin="IN5" pad="3"/>
<connect gate="A" pin="IN6" pad="4"/>
<connect gate="A" pin="IN7" pad="5"/>
<connect gate="A" pin="IN8" pad="6"/>
<connect gate="A" pin="IN9" pad="7"/>
<connect gate="A" pin="MULTIPLEXER_OUT" pad="15"/>
<connect gate="A" pin="OUT_EN" pad="21"/>
<connect gate="A" pin="REF(+)" pad="19"/>
<connect gate="A" pin="REF(-)" pad="23"/>
<connect gate="A" pin="START" pad="16"/>
<connect gate="A" pin="VCC" pad="17"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="ADC0817CCN"/>
<attribute name="OC_FARNELL" value="9486690"/>
<attribute name="OC_NEWARK" value="07B4630"/>
<attribute name="PACKAGE" value="40-DIP"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADC081S021CIMF" prefix="U">
<description>8-Bit A/D Converter</description>
<gates>
<gate name="A" symbol="ADC081S021CIMF"/>
</gates>
<devices>
<device name="" package="SOT95P284X122-6N">
<connects>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="SCLK" pad="4"/>
<connect gate="A" pin="SDATA" pad="5"/>
<connect gate="A" pin="VA" pad="1"/>
<connect gate="A" pin="VIN" pad="3"/>
<connect gate="A" pin="~CS" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="ADC081S021CIMF"/>
<attribute name="OC_FARNELL" value="1250030"/>
<attribute name="OC_NEWARK" value="69K1478"/>
<attribute name="PACKAGE" value="SOT23-6"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADC081S101CIMF" prefix="U">
<description>8-Bit A/D Converter</description>
<gates>
<gate name="A" symbol="ADC081S101CIMF"/>
</gates>
<devices>
<device name="" package="SOT95P285X120-6N">
<connects>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="SCLK" pad="4"/>
<connect gate="A" pin="SDATA" pad="5"/>
<connect gate="A" pin="VA" pad="1"/>
<connect gate="A" pin="VIN" pad="3"/>
<connect gate="A" pin="~CS" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="ADC081S101CIMF"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K1445"/>
<attribute name="PACKAGE" value="SOT-6"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADC081S101CISD" prefix="U">
<description>8-Bit A/D Converter</description>
<gates>
<gate name="A" symbol="ADC081S101CISD"/>
</gates>
<devices>
<device name="" package="DFN250X220X80-7N">
<connects>
<connect gate="A" pin="EPAD" pad="7"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="SCLK" pad="4"/>
<connect gate="A" pin="SDATA" pad="5"/>
<connect gate="A" pin="VA" pad="1"/>
<connect gate="A" pin="VIN" pad="3"/>
<connect gate="A" pin="~CS" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="ADC081S101CISD"/>
<attribute name="OC_FARNELL" value="1312527"/>
<attribute name="OC_NEWARK" value="21K6683"/>
<attribute name="PACKAGE" value="DFN-8"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADC08200CIMT" prefix="U">
<description>A/D Converter</description>
<gates>
<gate name="A" symbol="ADC08200CIMT"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-24N">
<connects>
<connect gate="A" pin="AGND" pad="11"/>
<connect gate="A" pin="AGND_2" pad="2"/>
<connect gate="A" pin="AGND_3" pad="5"/>
<connect gate="A" pin="AGND_4" pad="8"/>
<connect gate="A" pin="CLK" pad="24"/>
<connect gate="A" pin="D0" pad="22"/>
<connect gate="A" pin="D1" pad="21"/>
<connect gate="A" pin="D2" pad="20"/>
<connect gate="A" pin="D3" pad="19"/>
<connect gate="A" pin="D4" pad="16"/>
<connect gate="A" pin="D5" pad="15"/>
<connect gate="A" pin="D6" pad="14"/>
<connect gate="A" pin="D7" pad="13"/>
<connect gate="A" pin="DR_GND" pad="17"/>
<connect gate="A" pin="PD" pad="23"/>
<connect gate="A" pin="VA" pad="12"/>
<connect gate="A" pin="VA_2" pad="1"/>
<connect gate="A" pin="VA_3" pad="4"/>
<connect gate="A" pin="VDR" pad="18"/>
<connect gate="A" pin="VIN" pad="6"/>
<connect gate="A" pin="VIN_GND" pad="7"/>
<connect gate="A" pin="VRB" pad="10"/>
<connect gate="A" pin="VRM" pad="9"/>
<connect gate="A" pin="VRT" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="ADC08200CIMT"/>
<attribute name="OC_FARNELL" value="8206805"/>
<attribute name="OC_NEWARK" value="-"/>
<attribute name="PACKAGE" value="24-TSSOP"/>
<attribute name="SUPPLIER" value="NATIONAL SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADC0820CCN" prefix="U">
<description>A/D converters</description>
<gates>
<gate name="A" symbol="ADC0820CCN"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-20">
<connects>
<connect gate="A" pin="DB0" pad="2"/>
<connect gate="A" pin="DB1" pad="3"/>
<connect gate="A" pin="DB2" pad="4"/>
<connect gate="A" pin="DB3" pad="5"/>
<connect gate="A" pin="DB_4" pad="14"/>
<connect gate="A" pin="DB_5" pad="15"/>
<connect gate="A" pin="DB_6" pad="16"/>
<connect gate="A" pin="DB_7" pad="17"/>
<connect gate="A" pin="GND" pad="10"/>
<connect gate="A" pin="MODE" pad="7"/>
<connect gate="A" pin="NC" pad="19"/>
<connect gate="A" pin="VCC" pad="20"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="VREF(+)" pad="12"/>
<connect gate="A" pin="VREF(-)" pad="11"/>
<connect gate="A" pin="~CS" pad="13"/>
<connect gate="A" pin="~INT" pad="9"/>
<connect gate="A" pin="~OFL" pad="18"/>
<connect gate="A" pin="~RD" pad="8"/>
<connect gate="A" pin="~WR~/RDY" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="ADC0820CCN"/>
<attribute name="OC_FARNELL" value="1673948"/>
<attribute name="OC_NEWARK" value="41K1465"/>
<attribute name="PACKAGE" value="DIP-20"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADC0820CCWM" prefix="U">
<description>A/D converters</description>
<gates>
<gate name="A" symbol="ADC0820CCWM"/>
</gates>
<devices>
<device name="" package="SOIC127P1032X264-20N">
<connects>
<connect gate="A" pin="DB0" pad="2"/>
<connect gate="A" pin="DB1" pad="3"/>
<connect gate="A" pin="DB2" pad="4"/>
<connect gate="A" pin="DB3" pad="5"/>
<connect gate="A" pin="DB4" pad="14"/>
<connect gate="A" pin="DB5" pad="15"/>
<connect gate="A" pin="DB6" pad="16"/>
<connect gate="A" pin="DB7" pad="17"/>
<connect gate="A" pin="GND" pad="10"/>
<connect gate="A" pin="MODE" pad="7"/>
<connect gate="A" pin="NC" pad="19"/>
<connect gate="A" pin="VCC" pad="20"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="VREF(+)" pad="12"/>
<connect gate="A" pin="VREF(-)" pad="11"/>
<connect gate="A" pin="~CS" pad="13"/>
<connect gate="A" pin="~INT" pad="9"/>
<connect gate="A" pin="~OFL" pad="18"/>
<connect gate="A" pin="~RD" pad="8"/>
<connect gate="A" pin="~WR/RDY" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="ADC0820CCWM"/>
<attribute name="OC_FARNELL" value="1564768"/>
<attribute name="OC_NEWARK" value="07B4637"/>
<attribute name="PACKAGE" value="SOIC-20"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADC082S021CIMM" prefix="U">
<description>A/D Converter</description>
<gates>
<gate name="A" symbol="ADC082S021CIMM"/>
</gates>
<devices>
<device name="" package="SOP65P490X109-8N">
<connects>
<connect gate="A" pin="DIN" pad="6"/>
<connect gate="A" pin="DOUT" pad="7"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="IN1" pad="5"/>
<connect gate="A" pin="IN2" pad="4"/>
<connect gate="A" pin="SCLK" pad="8"/>
<connect gate="A" pin="VA" pad="2"/>
<connect gate="A" pin="~CS" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="ADC082S021CIMM"/>
<attribute name="OC_FARNELL" value="1007978"/>
<attribute name="OC_NEWARK" value="41K1457"/>
<attribute name="PACKAGE" value="SOP-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADC082S101CIMM" prefix="U">
<description>8-Bit A/D Converter</description>
<gates>
<gate name="A" symbol="ADC082S101CIMM"/>
</gates>
<devices>
<device name="" package="SOP65P490X110-8N">
<connects>
<connect gate="A" pin="DIN" pad="6"/>
<connect gate="A" pin="DOUT" pad="7"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="IN1" pad="5"/>
<connect gate="A" pin="IN2" pad="4"/>
<connect gate="A" pin="SCLK" pad="8"/>
<connect gate="A" pin="VA" pad="2"/>
<connect gate="A" pin="~CS" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="ADC082S101CIMM"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K1461"/>
<attribute name="PACKAGE" value="MSOP-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADC0831CCN" prefix="U">
<description>A/D converters</description>
<gates>
<gate name="A" symbol="ADC0831CCN"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-8">
<connects>
<connect gate="A" pin="CLK" pad="7"/>
<connect gate="A" pin="DO" pad="6"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="VIN+" pad="2"/>
<connect gate="A" pin="VIN-" pad="3"/>
<connect gate="A" pin="VREF" pad="5"/>
<connect gate="A" pin="~CS" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="ADC0831CCN"/>
<attribute name="OC_FARNELL" value="1673947"/>
<attribute name="OC_NEWARK" value="07B4639"/>
<attribute name="PACKAGE" value="DIP-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADC0832CCN" prefix="U">
<description>A/D converters</description>
<gates>
<gate name="A" symbol="ADC0832CCN"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-8">
<connects>
<connect gate="A" pin="CLK" pad="7"/>
<connect gate="A" pin="DO" pad="6"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="VIN+" pad="2"/>
<connect gate="A" pin="VIN-" pad="3"/>
<connect gate="A" pin="VREF" pad="5"/>
<connect gate="A" pin="~CS" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="ADC0832CCN"/>
<attribute name="OC_FARNELL" value="1468862"/>
<attribute name="OC_NEWARK" value="41K1473"/>
<attribute name="PACKAGE" value="DIP-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADC0834CCWM" prefix="U">
<description>A/D converters</description>
<gates>
<gate name="A" symbol="ADC0834CCWM"/>
</gates>
<devices>
<device name="" package="SOIC127P1032X264-14N">
<connects>
<connect gate="A" pin="AGND" pad="8"/>
<connect gate="A" pin="CH0" pad="3"/>
<connect gate="A" pin="CH1" pad="4"/>
<connect gate="A" pin="CH2" pad="5"/>
<connect gate="A" pin="CH3" pad="6"/>
<connect gate="A" pin="CLK" pad="12"/>
<connect gate="A" pin="DGND" pad="7"/>
<connect gate="A" pin="DI" pad="13"/>
<connect gate="A" pin="DO" pad="10"/>
<connect gate="A" pin="SARS" pad="11"/>
<connect gate="A" pin="V+" pad="1"/>
<connect gate="A" pin="VCC" pad="14"/>
<connect gate="A" pin="VREF" pad="9"/>
<connect gate="A" pin="~CS" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="ADC0834CCWM"/>
<attribute name="OC_FARNELL" value="1673949"/>
<attribute name="OC_NEWARK" value="07B4652"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADC0838CCN" prefix="U">
<description>A/D Converter with multiplexer</description>
<gates>
<gate name="A" symbol="ADC0838CCN"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-20">
<connects>
<connect gate="A" pin="AGND" pad="11"/>
<connect gate="A" pin="CH0" pad="1"/>
<connect gate="A" pin="CH1" pad="2"/>
<connect gate="A" pin="CH2" pad="3"/>
<connect gate="A" pin="CH3" pad="4"/>
<connect gate="A" pin="CH4" pad="5"/>
<connect gate="A" pin="CH5" pad="6"/>
<connect gate="A" pin="CH6" pad="7"/>
<connect gate="A" pin="CH7" pad="8"/>
<connect gate="A" pin="CLK" pad="16"/>
<connect gate="A" pin="COM" pad="9"/>
<connect gate="A" pin="D0" pad="14"/>
<connect gate="A" pin="DGND" pad="10"/>
<connect gate="A" pin="DI" pad="17"/>
<connect gate="A" pin="SARS" pad="15"/>
<connect gate="A" pin="V+" pad="19"/>
<connect gate="A" pin="VCC" pad="20"/>
<connect gate="A" pin="VREF" pad="12"/>
<connect gate="A" pin="~CS" pad="18"/>
<connect gate="A" pin="~SE" pad="13"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="ADC0838CCN"/>
<attribute name="OC_FARNELL" value="9486615"/>
<attribute name="OC_NEWARK" value="41K1484"/>
<attribute name="PACKAGE" value="DIP-20"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADC0838CCWM" prefix="U">
<description>A/D converters</description>
<gates>
<gate name="A" symbol="ADC0838CCWM"/>
</gates>
<devices>
<device name="" package="SOIC127P1032X264-20N">
<connects>
<connect gate="A" pin="AGND" pad="11"/>
<connect gate="A" pin="CH0" pad="1"/>
<connect gate="A" pin="CH1" pad="2"/>
<connect gate="A" pin="CH2" pad="3"/>
<connect gate="A" pin="CH3" pad="4"/>
<connect gate="A" pin="CH4" pad="5"/>
<connect gate="A" pin="CH5" pad="6"/>
<connect gate="A" pin="CH6" pad="7"/>
<connect gate="A" pin="CH7" pad="8"/>
<connect gate="A" pin="CLK" pad="16"/>
<connect gate="A" pin="COM" pad="9"/>
<connect gate="A" pin="DGND" pad="10"/>
<connect gate="A" pin="DI" pad="17"/>
<connect gate="A" pin="DO" pad="14"/>
<connect gate="A" pin="SARS" pad="15"/>
<connect gate="A" pin="V+" pad="19"/>
<connect gate="A" pin="VCC" pad="20"/>
<connect gate="A" pin="VREF" pad="12"/>
<connect gate="A" pin="~CS" pad="18"/>
<connect gate="A" pin="~SE" pad="13"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="ADC0838CCWM"/>
<attribute name="OC_FARNELL" value="1673975"/>
<attribute name="OC_NEWARK" value="41K1485"/>
<attribute name="PACKAGE" value="SOIC-20"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADC0844CCN" prefix="U">
<description>A/D Converter with multiplexer</description>
<gates>
<gate name="A" symbol="ADC0844CCN"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-20">
<connects>
<connect gate="A" pin="AGND" pad="7"/>
<connect gate="A" pin="CH1" pad="3"/>
<connect gate="A" pin="CH2" pad="4"/>
<connect gate="A" pin="CH3" pad="5"/>
<connect gate="A" pin="CH4" pad="6"/>
<connect gate="A" pin="DB0/MA0" pad="17"/>
<connect gate="A" pin="DB1/MA1" pad="16"/>
<connect gate="A" pin="DB2/MA2" pad="15"/>
<connect gate="A" pin="DB3/MA3" pad="14"/>
<connect gate="A" pin="DB4" pad="13"/>
<connect gate="A" pin="DB5" pad="12"/>
<connect gate="A" pin="DB6" pad="11"/>
<connect gate="A" pin="DB7" pad="9"/>
<connect gate="A" pin="DGND" pad="10"/>
<connect gate="A" pin="VCC" pad="20"/>
<connect gate="A" pin="VREF" pad="8"/>
<connect gate="A" pin="~CS" pad="2"/>
<connect gate="A" pin="~INTR" pad="18"/>
<connect gate="A" pin="~RD" pad="1"/>
<connect gate="A" pin="~WR" pad="19"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="ADC0844CCN"/>
<attribute name="OC_FARNELL" value="9486623"/>
<attribute name="OC_NEWARK" value="07B4665"/>
<attribute name="PACKAGE" value="DIP-20"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADC0848CCN" prefix="U">
<description>A/D Converter with multiplexer</description>
<gates>
<gate name="A" symbol="ADC0848CCN"/>
</gates>
<devices>
<device name="" package="DIP254P762X457-24">
<connects>
<connect gate="A" pin="AGND" pad="10"/>
<connect gate="A" pin="CH1" pad="2"/>
<connect gate="A" pin="CH2" pad="3"/>
<connect gate="A" pin="CH3" pad="4"/>
<connect gate="A" pin="CH4" pad="5"/>
<connect gate="A" pin="CH5" pad="6"/>
<connect gate="A" pin="CH6" pad="7"/>
<connect gate="A" pin="CH7" pad="8"/>
<connect gate="A" pin="CH8" pad="9"/>
<connect gate="A" pin="DB0/MA0" pad="20"/>
<connect gate="A" pin="DB1/MA1" pad="19"/>
<connect gate="A" pin="DB2/MA2" pad="18"/>
<connect gate="A" pin="DB3/MA3" pad="17"/>
<connect gate="A" pin="DB4/MA4" pad="16"/>
<connect gate="A" pin="DB5" pad="15"/>
<connect gate="A" pin="DB6" pad="14"/>
<connect gate="A" pin="DB7" pad="13"/>
<connect gate="A" pin="DGND" pad="12"/>
<connect gate="A" pin="VCC" pad="24"/>
<connect gate="A" pin="VREF" pad="11"/>
<connect gate="A" pin="~CS" pad="23"/>
<connect gate="A" pin="~INTR" pad="21"/>
<connect gate="A" pin="~RD" pad="1"/>
<connect gate="A" pin="~WR" pad="22"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="ADC0848CCN"/>
<attribute name="OC_FARNELL" value="9486631"/>
<attribute name="OC_NEWARK" value="41K1499"/>
<attribute name="PACKAGE" value="24-DIP"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADC0848CCV" prefix="U">
<description>A/D Converters</description>
<gates>
<gate name="A" symbol="ADC0848CCV"/>
</gates>
<devices>
<device name="" package="PLCC127P1245X1245X457-28N">
<connects>
<connect gate="A" pin="AGND" pad="13"/>
<connect gate="A" pin="CH1" pad="4"/>
<connect gate="A" pin="CH2" pad="5"/>
<connect gate="A" pin="CH3" pad="6"/>
<connect gate="A" pin="CH4" pad="7"/>
<connect gate="A" pin="CH5" pad="9"/>
<connect gate="A" pin="CH6" pad="10"/>
<connect gate="A" pin="CH7" pad="11"/>
<connect gate="A" pin="CH8" pad="12"/>
<connect gate="A" pin="DB0/MA0" pad="25"/>
<connect gate="A" pin="DB1/MA1" pad="24"/>
<connect gate="A" pin="DB2/MA2" pad="23"/>
<connect gate="A" pin="DB3/MA3" pad="21"/>
<connect gate="A" pin="DB4/MA4" pad="20"/>
<connect gate="A" pin="DB5" pad="19"/>
<connect gate="A" pin="DB6" pad="18"/>
<connect gate="A" pin="DB7" pad="17"/>
<connect gate="A" pin="DGND" pad="16"/>
<connect gate="A" pin="NC" pad="22"/>
<connect gate="A" pin="NC_2" pad="8"/>
<connect gate="A" pin="NC_3" pad="15"/>
<connect gate="A" pin="NC_4" pad="1"/>
<connect gate="A" pin="VCC" pad="2"/>
<connect gate="A" pin="VREF" pad="14"/>
<connect gate="A" pin="~CS" pad="28"/>
<connect gate="A" pin="~INTR" pad="26"/>
<connect gate="A" pin="~RD" pad="3"/>
<connect gate="A" pin="~WR" pad="27"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="ADC0848CCV"/>
<attribute name="OC_FARNELL" value="9494308"/>
<attribute name="OC_NEWARK" value="41K1500"/>
<attribute name="PACKAGE" value="PLCC-28"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADC084S021CIMM" prefix="U">
<description>8-Bit A/D Converter</description>
<gates>
<gate name="A" symbol="ADC084S021CIMM"/>
</gates>
<devices>
<device name="" package="SOP50P490X110-10N">
<connects>
<connect gate="A" pin="DIN" pad="8"/>
<connect gate="A" pin="DOUT" pad="9"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="IN1" pad="7"/>
<connect gate="A" pin="IN2" pad="6"/>
<connect gate="A" pin="IN3" pad="5"/>
<connect gate="A" pin="IN4" pad="4"/>
<connect gate="A" pin="SCLK" pad="10"/>
<connect gate="A" pin="VA" pad="2"/>
<connect gate="A" pin="~CS" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="ADC084S021CIMM"/>
<attribute name="OC_FARNELL" value="1673976"/>
<attribute name="OC_NEWARK" value="41K1489"/>
<attribute name="PACKAGE" value="MSOP-10"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADC084S051CIMM" prefix="U">
<description>A/D Converter</description>
<gates>
<gate name="A" symbol="ADC084S051CIMM"/>
</gates>
<devices>
<device name="" package="SOP50P490X109-10N">
<connects>
<connect gate="A" pin="DIN" pad="8"/>
<connect gate="A" pin="DOUT" pad="9"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="IN1" pad="7"/>
<connect gate="A" pin="IN2" pad="6"/>
<connect gate="A" pin="IN3" pad="5"/>
<connect gate="A" pin="IN4" pad="4"/>
<connect gate="A" pin="SCLK" pad="10"/>
<connect gate="A" pin="VA" pad="2"/>
<connect gate="A" pin="~CS" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="ADC084S051CIMM"/>
<attribute name="OC_FARNELL" value="1007983"/>
<attribute name="OC_NEWARK" value="96K6174"/>
<attribute name="PACKAGE" value="SOP-10"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADC084S101CIMM" prefix="U">
<description>8-Bit A/D Converter</description>
<gates>
<gate name="A" symbol="ADC084S101CIMM"/>
</gates>
<devices>
<device name="" package="SOP50P490X110-10N">
<connects>
<connect gate="A" pin="DIN" pad="8"/>
<connect gate="A" pin="DOUT" pad="9"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="IN1" pad="7"/>
<connect gate="A" pin="IN2" pad="6"/>
<connect gate="A" pin="IN3" pad="5"/>
<connect gate="A" pin="IN4" pad="4"/>
<connect gate="A" pin="SCLK" pad="10"/>
<connect gate="A" pin="VA" pad="2"/>
<connect gate="A" pin="~CS" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="ADC084S101CIMM"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K1493"/>
<attribute name="PACKAGE" value="MSOP-10"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADC08500CIYB" prefix="U">
<description>Low Power 8-Bit, 500 MSPS A/D Converter</description>
<gates>
<gate name="A" symbol="ADC08500CIYB"/>
</gates>
<devices>
<device name="" package="QFP50P2200X2200X160-129N">
<connects>
<connect gate="A" pin="CAL" pad="30"/>
<connect gate="A" pin="CALDLY/~SCS" pad="127"/>
<connect gate="A" pin="CALRUN" pad="126"/>
<connect gate="A" pin="CLK+" pad="18"/>
<connect gate="A" pin="CLK-" pad="19"/>
<connect gate="A" pin="D0+" pad="103"/>
<connect gate="A" pin="D0-" pad="102"/>
<connect gate="A" pin="D1+" pad="101"/>
<connect gate="A" pin="D1-" pad="100"/>
<connect gate="A" pin="D2+" pad="96"/>
<connect gate="A" pin="D2-" pad="95"/>
<connect gate="A" pin="D3+" pad="94"/>
<connect gate="A" pin="D3-" pad="93"/>
<connect gate="A" pin="D4+" pad="92"/>
<connect gate="A" pin="D4-" pad="91"/>
<connect gate="A" pin="D5+" pad="90"/>
<connect gate="A" pin="D5-" pad="89"/>
<connect gate="A" pin="D6+" pad="86"/>
<connect gate="A" pin="D6-" pad="85"/>
<connect gate="A" pin="D7+" pad="84"/>
<connect gate="A" pin="D7-" pad="83"/>
<connect gate="A" pin="DCLK+" pad="82"/>
<connect gate="A" pin="DCLK-" pad="81"/>
<connect gate="A" pin="DCLK_RST" pad="15"/>
<connect gate="A" pin="DD0+" pad="125"/>
<connect gate="A" pin="DD0-" pad="124"/>
<connect gate="A" pin="DD1+" pad="123"/>
<connect gate="A" pin="DD1-" pad="122"/>
<connect gate="A" pin="DD2+" pad="118"/>
<connect gate="A" pin="DD2-" pad="117"/>
<connect gate="A" pin="DD3+" pad="116"/>
<connect gate="A" pin="DD3-" pad="115"/>
<connect gate="A" pin="DD4+" pad="114"/>
<connect gate="A" pin="DD4-" pad="113"/>
<connect gate="A" pin="DD5+" pad="112"/>
<connect gate="A" pin="DD5-" pad="111"/>
<connect gate="A" pin="DD6+" pad="107"/>
<connect gate="A" pin="DD6-" pad="106"/>
<connect gate="A" pin="DD7+" pad="105"/>
<connect gate="A" pin="DD7-" pad="104"/>
<connect gate="A" pin="DR_GND" pad="119"/>
<connect gate="A" pin="DR_GND_2" pad="42"/>
<connect gate="A" pin="DR_GND_3" pad="108"/>
<connect gate="A" pin="DR_GND_4" pad="74"/>
<connect gate="A" pin="DR_GND_5" pad="87"/>
<connect gate="A" pin="DR_GND_6" pad="53"/>
<connect gate="A" pin="DR_GND_7" pad="64"/>
<connect gate="A" pin="DR_GND_8" pad="97"/>
<connect gate="A" pin="EPAD" pad="129"/>
<connect gate="A" pin="FSR/ECE" pad="14"/>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="GND_2" pad="1"/>
<connect gate="A" pin="GND_3" pad="12"/>
<connect gate="A" pin="GND_4" pad="24"/>
<connect gate="A" pin="GND_5" pad="27"/>
<connect gate="A" pin="GND_6" pad="21"/>
<connect gate="A" pin="GND_7" pad="9"/>
<connect gate="A" pin="GND_8" pad="41"/>
<connect gate="A" pin="NC" pad="61"/>
<connect gate="A" pin="NC_10" pad="77"/>
<connect gate="A" pin="NC_11" pad="78"/>
<connect gate="A" pin="NC_12" pad="109"/>
<connect gate="A" pin="NC_13" pad="98"/>
<connect gate="A" pin="NC_14" pad="120"/>
<connect gate="A" pin="NC_15" pad="36"/>
<connect gate="A" pin="NC_16" pad="37"/>
<connect gate="A" pin="NC_17" pad="38"/>
<connect gate="A" pin="NC_18" pad="39"/>
<connect gate="A" pin="NC_19" pad="43"/>
<connect gate="A" pin="NC_2" pad="67"/>
<connect gate="A" pin="NC_20" pad="44"/>
<connect gate="A" pin="NC_21" pad="45"/>
<connect gate="A" pin="NC_22" pad="46"/>
<connect gate="A" pin="NC_23" pad="52"/>
<connect gate="A" pin="NC_24" pad="29"/>
<connect gate="A" pin="NC_25" pad="47"/>
<connect gate="A" pin="NC_26" pad="54"/>
<connect gate="A" pin="NC_27" pad="48"/>
<connect gate="A" pin="NC_28" pad="55"/>
<connect gate="A" pin="NC_29" pad="49"/>
<connect gate="A" pin="NC_3" pad="22"/>
<connect gate="A" pin="NC_30" pad="56"/>
<connect gate="A" pin="NC_31" pad="50"/>
<connect gate="A" pin="NC_32" pad="63"/>
<connect gate="A" pin="NC_33" pad="57"/>
<connect gate="A" pin="NC_34" pad="71"/>
<connect gate="A" pin="NC_35" pad="58"/>
<connect gate="A" pin="NC_36" pad="72"/>
<connect gate="A" pin="NC_37" pad="59"/>
<connect gate="A" pin="NC_38" pad="65"/>
<connect gate="A" pin="NC_39" pad="60"/>
<connect gate="A" pin="NC_4" pad="68"/>
<connect gate="A" pin="NC_40" pad="66"/>
<connect gate="A" pin="NC_5" pad="23"/>
<connect gate="A" pin="NC_6" pad="69"/>
<connect gate="A" pin="NC_7" pad="70"/>
<connect gate="A" pin="NC_8" pad="75"/>
<connect gate="A" pin="NC_9" pad="76"/>
<connect gate="A" pin="OR+" pad="79"/>
<connect gate="A" pin="OR-" pad="80"/>
<connect gate="A" pin="OUTV/SCLK" pad="3"/>
<connect gate="A" pin="OUT_EDGE/DDR/SDATA" pad="4"/>
<connect gate="A" pin="PD" pad="26"/>
<connect gate="A" pin="REXT" pad="32"/>
<connect gate="A" pin="TDIODE_N" pad="35"/>
<connect gate="A" pin="TDIODE_P" pad="34"/>
<connect gate="A" pin="VA" pad="128"/>
<connect gate="A" pin="VA_10" pad="25"/>
<connect gate="A" pin="VA_11" pad="28"/>
<connect gate="A" pin="VA_2" pad="5"/>
<connect gate="A" pin="VA_3" pad="2"/>
<connect gate="A" pin="VA_4" pad="8"/>
<connect gate="A" pin="VA_5" pad="16"/>
<connect gate="A" pin="VA_6" pad="13"/>
<connect gate="A" pin="VA_7" pad="33"/>
<connect gate="A" pin="VA_8" pad="17"/>
<connect gate="A" pin="VA_9" pad="20"/>
<connect gate="A" pin="VBG" pad="31"/>
<connect gate="A" pin="VCMO" pad="7"/>
<connect gate="A" pin="VDR" pad="99"/>
<connect gate="A" pin="VDR_2" pad="51"/>
<connect gate="A" pin="VDR_3" pad="62"/>
<connect gate="A" pin="VDR_4" pad="40"/>
<connect gate="A" pin="VDR_5" pad="121"/>
<connect gate="A" pin="VDR_6" pad="73"/>
<connect gate="A" pin="VDR_7" pad="110"/>
<connect gate="A" pin="VDR_8" pad="88"/>
<connect gate="A" pin="VIN+" pad="11"/>
<connect gate="A" pin="VIN-" pad="10"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="ADC08500CIYB"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="54M4434"/>
<attribute name="PACKAGE" value="QFP-128"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADC08831IM" prefix="U">
<description>A/D converters</description>
<gates>
<gate name="A" symbol="ADC08831IM"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="CLK" pad="7"/>
<connect gate="A" pin="DO" pad="6"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="VIN+" pad="2"/>
<connect gate="A" pin="VIN-" pad="3"/>
<connect gate="A" pin="VREF_IN" pad="5"/>
<connect gate="A" pin="~CS" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="ADC08831IM"/>
<attribute name="OC_FARNELL" value="1673977"/>
<attribute name="OC_NEWARK" value="41K1502"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADC08832IM" prefix="U">
<description>8-Bit Serial I/O CMOS A/D Converters</description>
<gates>
<gate name="A" symbol="ADC08832IM"/>
</gates>
<devices>
<device name="" package="SOIC127P620X175-8N">
<connects>
<connect gate="A" pin="CH0" pad="2"/>
<connect gate="A" pin="CH1" pad="3"/>
<connect gate="A" pin="CLK" pad="7"/>
<connect gate="A" pin="DI" pad="5"/>
<connect gate="A" pin="DO" pad="6"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="VCC(VREF)" pad="8"/>
<connect gate="A" pin="~CS" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="ADC08832IM"/>
<attribute name="OC_FARNELL" value="1798305"/>
<attribute name="OC_NEWARK" value="73R9365"/>
<attribute name="PACKAGE" value="8-SOIC"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADC088S022CIMT" prefix="U">
<description>A/D Converter</description>
<gates>
<gate name="A" symbol="ADC088S022CIMT"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-16N">
<connects>
<connect gate="A" pin="AGND" pad="3"/>
<connect gate="A" pin="DGND" pad="12"/>
<connect gate="A" pin="DIN" pad="14"/>
<connect gate="A" pin="DOUT" pad="15"/>
<connect gate="A" pin="IN0" pad="4"/>
<connect gate="A" pin="IN1" pad="5"/>
<connect gate="A" pin="IN2" pad="6"/>
<connect gate="A" pin="IN3" pad="7"/>
<connect gate="A" pin="IN4" pad="8"/>
<connect gate="A" pin="IN5" pad="9"/>
<connect gate="A" pin="IN6" pad="10"/>
<connect gate="A" pin="IN7" pad="11"/>
<connect gate="A" pin="SCLK" pad="16"/>
<connect gate="A" pin="VA" pad="2"/>
<connect gate="A" pin="VD" pad="13"/>
<connect gate="A" pin="~CS" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="ADC088S022CIMT"/>
<attribute name="OC_FARNELL" value="1250037"/>
<attribute name="OC_NEWARK" value="79K5518"/>
<attribute name="PACKAGE" value="TSSOP-16"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADC088S102CIMT" prefix="U">
<description>8-Bit A/D Converter</description>
<gates>
<gate name="A" symbol="ADC088S102CIMT"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-16N">
<connects>
<connect gate="A" pin="AGND" pad="3"/>
<connect gate="A" pin="DGND" pad="12"/>
<connect gate="A" pin="DIN" pad="14"/>
<connect gate="A" pin="DOUT" pad="15"/>
<connect gate="A" pin="IN0" pad="4"/>
<connect gate="A" pin="IN1" pad="5"/>
<connect gate="A" pin="IN2" pad="6"/>
<connect gate="A" pin="IN3" pad="7"/>
<connect gate="A" pin="IN4" pad="8"/>
<connect gate="A" pin="IN5" pad="9"/>
<connect gate="A" pin="IN6" pad="10"/>
<connect gate="A" pin="IN7" pad="11"/>
<connect gate="A" pin="SCLK" pad="16"/>
<connect gate="A" pin="VA" pad="2"/>
<connect gate="A" pin="VD" pad="13"/>
<connect gate="A" pin="~CS" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="ADC088S102CIMT"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="60K8366"/>
<attribute name="PACKAGE" value="TSSOP-16"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADC08D1000CIYB" prefix="U">
<description>Low Power, Dual 8-Bit, 1 GSPS A/D Converter</description>
<gates>
<gate name="A" symbol="ADC08D1000CIYB"/>
</gates>
<devices>
<device name="" package="QFP50P2200X2200X160-129N">
<connects>
<connect gate="A" pin="CAL" pad="30"/>
<connect gate="A" pin="CALDLY/DES/~SCS" pad="127"/>
<connect gate="A" pin="CALRUN" pad="126"/>
<connect gate="A" pin="CLK+" pad="18"/>
<connect gate="A" pin="CLK-" pad="19"/>
<connect gate="A" pin="DCLK+" pad="82"/>
<connect gate="A" pin="DCLK-" pad="81"/>
<connect gate="A" pin="DCLK_RST" pad="15"/>
<connect gate="A" pin="DI0+" pad="103"/>
<connect gate="A" pin="DI0-" pad="102"/>
<connect gate="A" pin="DI1+" pad="101"/>
<connect gate="A" pin="DI1-" pad="100"/>
<connect gate="A" pin="DI2+" pad="96"/>
<connect gate="A" pin="DI2-" pad="95"/>
<connect gate="A" pin="DI3+" pad="94"/>
<connect gate="A" pin="DI3-" pad="93"/>
<connect gate="A" pin="DI4+" pad="92"/>
<connect gate="A" pin="DI4-" pad="91"/>
<connect gate="A" pin="DI5+" pad="90"/>
<connect gate="A" pin="DI5-" pad="89"/>
<connect gate="A" pin="DI6+" pad="86"/>
<connect gate="A" pin="DI6-" pad="85"/>
<connect gate="A" pin="DI7+" pad="84"/>
<connect gate="A" pin="DI7-" pad="83"/>
<connect gate="A" pin="DID0+" pad="125"/>
<connect gate="A" pin="DID0-" pad="124"/>
<connect gate="A" pin="DID1+" pad="123"/>
<connect gate="A" pin="DID1-" pad="122"/>
<connect gate="A" pin="DID2+" pad="118"/>
<connect gate="A" pin="DID2-" pad="117"/>
<connect gate="A" pin="DID3+" pad="116"/>
<connect gate="A" pin="DID3-" pad="115"/>
<connect gate="A" pin="DID4+" pad="114"/>
<connect gate="A" pin="DID4-" pad="113"/>
<connect gate="A" pin="DID5+" pad="112"/>
<connect gate="A" pin="DID5-" pad="111"/>
<connect gate="A" pin="DID6+" pad="107"/>
<connect gate="A" pin="DID6-" pad="106"/>
<connect gate="A" pin="DID7+" pad="105"/>
<connect gate="A" pin="DID7-" pad="104"/>
<connect gate="A" pin="DQ0+" pad="58"/>
<connect gate="A" pin="DQ0-" pad="59"/>
<connect gate="A" pin="DQ1+" pad="60"/>
<connect gate="A" pin="DQ1-" pad="61"/>
<connect gate="A" pin="DQ2+" pad="65"/>
<connect gate="A" pin="DQ2-" pad="66"/>
<connect gate="A" pin="DQ3+" pad="67"/>
<connect gate="A" pin="DQ3-" pad="68"/>
<connect gate="A" pin="DQ4+" pad="69"/>
<connect gate="A" pin="DQ4-" pad="70"/>
<connect gate="A" pin="DQ5+" pad="71"/>
<connect gate="A" pin="DQ5-" pad="72"/>
<connect gate="A" pin="DQ6+" pad="75"/>
<connect gate="A" pin="DQ6-" pad="76"/>
<connect gate="A" pin="DQ7+" pad="77"/>
<connect gate="A" pin="DQ7-" pad="78"/>
<connect gate="A" pin="DQD0+" pad="36"/>
<connect gate="A" pin="DQD0-" pad="37"/>
<connect gate="A" pin="DQD1+" pad="38"/>
<connect gate="A" pin="DQD1-" pad="39"/>
<connect gate="A" pin="DQD2+" pad="43"/>
<connect gate="A" pin="DQD2-" pad="44"/>
<connect gate="A" pin="DQD3+" pad="45"/>
<connect gate="A" pin="DQD3-" pad="46"/>
<connect gate="A" pin="DQD4+" pad="47"/>
<connect gate="A" pin="DQD4-" pad="48"/>
<connect gate="A" pin="DQD5+" pad="49"/>
<connect gate="A" pin="DQD5-" pad="50"/>
<connect gate="A" pin="DQD6+" pad="54"/>
<connect gate="A" pin="DQD6-" pad="55"/>
<connect gate="A" pin="DQD7+" pad="56"/>
<connect gate="A" pin="DQD7-" pad="57"/>
<connect gate="A" pin="DR_GND" pad="119"/>
<connect gate="A" pin="DR_GND_2" pad="42"/>
<connect gate="A" pin="DR_GND_3" pad="108"/>
<connect gate="A" pin="DR_GND_4" pad="74"/>
<connect gate="A" pin="DR_GND_5" pad="87"/>
<connect gate="A" pin="DR_GND_6" pad="53"/>
<connect gate="A" pin="DR_GND_7" pad="64"/>
<connect gate="A" pin="DR_GND_8" pad="97"/>
<connect gate="A" pin="EPAD" pad="129"/>
<connect gate="A" pin="FSR/ECE" pad="14"/>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="GND_2" pad="1"/>
<connect gate="A" pin="GND_3" pad="12"/>
<connect gate="A" pin="GND_4" pad="24"/>
<connect gate="A" pin="GND_5" pad="27"/>
<connect gate="A" pin="GND_6" pad="21"/>
<connect gate="A" pin="GND_7" pad="9"/>
<connect gate="A" pin="GND_8" pad="41"/>
<connect gate="A" pin="NC" pad="120"/>
<connect gate="A" pin="NC_2" pad="109"/>
<connect gate="A" pin="NC_3" pad="52"/>
<connect gate="A" pin="NC_4" pad="63"/>
<connect gate="A" pin="NC_5" pad="98"/>
<connect gate="A" pin="OR+" pad="79"/>
<connect gate="A" pin="OR-" pad="80"/>
<connect gate="A" pin="OUTV/SCLK" pad="3"/>
<connect gate="A" pin="OUT_EDGE/DDR/SDATA" pad="4"/>
<connect gate="A" pin="PD" pad="26"/>
<connect gate="A" pin="PDQ" pad="29"/>
<connect gate="A" pin="REXT" pad="32"/>
<connect gate="A" pin="TDIODE_N" pad="35"/>
<connect gate="A" pin="TDIODE_P" pad="34"/>
<connect gate="A" pin="VA" pad="128"/>
<connect gate="A" pin="VA_10" pad="25"/>
<connect gate="A" pin="VA_11" pad="28"/>
<connect gate="A" pin="VA_2" pad="5"/>
<connect gate="A" pin="VA_3" pad="2"/>
<connect gate="A" pin="VA_4" pad="8"/>
<connect gate="A" pin="VA_5" pad="16"/>
<connect gate="A" pin="VA_6" pad="13"/>
<connect gate="A" pin="VA_7" pad="33"/>
<connect gate="A" pin="VA_8" pad="17"/>
<connect gate="A" pin="VA_9" pad="20"/>
<connect gate="A" pin="VBG" pad="31"/>
<connect gate="A" pin="VCMO" pad="7"/>
<connect gate="A" pin="VDR" pad="99"/>
<connect gate="A" pin="VDR_2" pad="51"/>
<connect gate="A" pin="VDR_3" pad="62"/>
<connect gate="A" pin="VDR_4" pad="40"/>
<connect gate="A" pin="VDR_5" pad="121"/>
<connect gate="A" pin="VDR_6" pad="73"/>
<connect gate="A" pin="VDR_7" pad="110"/>
<connect gate="A" pin="VDR_8" pad="88"/>
<connect gate="A" pin="VIN+" pad="11"/>
<connect gate="A" pin="VIN-" pad="10"/>
<connect gate="A" pin="VINQ+" pad="22"/>
<connect gate="A" pin="VINQ-" pad="23"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="ADC08D1000CIYB"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K1416"/>
<attribute name="PACKAGE" value="QFP-128"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADC08D1500CIYB" prefix="U">
<description>Low Power, Dual 8-Bit, 1 GSPS A/D Converter</description>
<gates>
<gate name="A" symbol="ADC08D1500CIYB"/>
</gates>
<devices>
<device name="" package="QFP50P2200X2200X160-129N">
<connects>
<connect gate="A" pin="CAL" pad="30"/>
<connect gate="A" pin="CALDLY/DES/~SCS" pad="127"/>
<connect gate="A" pin="CALRUN" pad="126"/>
<connect gate="A" pin="CLK+" pad="18"/>
<connect gate="A" pin="CLK-" pad="19"/>
<connect gate="A" pin="DCLK+" pad="82"/>
<connect gate="A" pin="DCLK-" pad="81"/>
<connect gate="A" pin="DCLK_RST" pad="15"/>
<connect gate="A" pin="DI0+" pad="103"/>
<connect gate="A" pin="DI0-" pad="102"/>
<connect gate="A" pin="DI1+" pad="101"/>
<connect gate="A" pin="DI1-" pad="100"/>
<connect gate="A" pin="DI2+" pad="96"/>
<connect gate="A" pin="DI2-" pad="95"/>
<connect gate="A" pin="DI3+" pad="94"/>
<connect gate="A" pin="DI3-" pad="93"/>
<connect gate="A" pin="DI4+" pad="92"/>
<connect gate="A" pin="DI4-" pad="91"/>
<connect gate="A" pin="DI5+" pad="90"/>
<connect gate="A" pin="DI5-" pad="89"/>
<connect gate="A" pin="DI6+" pad="86"/>
<connect gate="A" pin="DI6-" pad="85"/>
<connect gate="A" pin="DI7+" pad="84"/>
<connect gate="A" pin="DI7-" pad="83"/>
<connect gate="A" pin="DID0+" pad="125"/>
<connect gate="A" pin="DID0-" pad="124"/>
<connect gate="A" pin="DID1+" pad="123"/>
<connect gate="A" pin="DID1-" pad="122"/>
<connect gate="A" pin="DID2+" pad="118"/>
<connect gate="A" pin="DID2-" pad="117"/>
<connect gate="A" pin="DID3+" pad="116"/>
<connect gate="A" pin="DID3-" pad="115"/>
<connect gate="A" pin="DID4+" pad="114"/>
<connect gate="A" pin="DID4-" pad="113"/>
<connect gate="A" pin="DID5+" pad="112"/>
<connect gate="A" pin="DID5-" pad="111"/>
<connect gate="A" pin="DID6+" pad="107"/>
<connect gate="A" pin="DID6-" pad="106"/>
<connect gate="A" pin="DID7+" pad="105"/>
<connect gate="A" pin="DID7-" pad="104"/>
<connect gate="A" pin="DQ0+" pad="58"/>
<connect gate="A" pin="DQ0-" pad="59"/>
<connect gate="A" pin="DQ1+" pad="60"/>
<connect gate="A" pin="DQ1-" pad="61"/>
<connect gate="A" pin="DQ2+" pad="65"/>
<connect gate="A" pin="DQ2-" pad="66"/>
<connect gate="A" pin="DQ3+" pad="67"/>
<connect gate="A" pin="DQ3-" pad="68"/>
<connect gate="A" pin="DQ4+" pad="69"/>
<connect gate="A" pin="DQ4-" pad="70"/>
<connect gate="A" pin="DQ5+" pad="71"/>
<connect gate="A" pin="DQ5-" pad="72"/>
<connect gate="A" pin="DQ6+" pad="75"/>
<connect gate="A" pin="DQ6-" pad="76"/>
<connect gate="A" pin="DQ7+" pad="77"/>
<connect gate="A" pin="DQ7-" pad="78"/>
<connect gate="A" pin="DQD0+" pad="36"/>
<connect gate="A" pin="DQD0-" pad="37"/>
<connect gate="A" pin="DQD1+" pad="38"/>
<connect gate="A" pin="DQD1-" pad="39"/>
<connect gate="A" pin="DQD2+" pad="43"/>
<connect gate="A" pin="DQD2-" pad="44"/>
<connect gate="A" pin="DQD3+" pad="45"/>
<connect gate="A" pin="DQD3-" pad="46"/>
<connect gate="A" pin="DQD4+" pad="47"/>
<connect gate="A" pin="DQD4-" pad="48"/>
<connect gate="A" pin="DQD5+" pad="49"/>
<connect gate="A" pin="DQD5-" pad="50"/>
<connect gate="A" pin="DQD6+" pad="54"/>
<connect gate="A" pin="DQD6-" pad="55"/>
<connect gate="A" pin="DQD7+" pad="56"/>
<connect gate="A" pin="DQD7-" pad="57"/>
<connect gate="A" pin="DR_GND" pad="119"/>
<connect gate="A" pin="DR_GND_2" pad="42"/>
<connect gate="A" pin="DR_GND_3" pad="108"/>
<connect gate="A" pin="DR_GND_4" pad="74"/>
<connect gate="A" pin="DR_GND_5" pad="87"/>
<connect gate="A" pin="DR_GND_6" pad="53"/>
<connect gate="A" pin="DR_GND_7" pad="64"/>
<connect gate="A" pin="DR_GND_8" pad="97"/>
<connect gate="A" pin="EPAD" pad="129"/>
<connect gate="A" pin="FSR/ECE" pad="14"/>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="GND_2" pad="1"/>
<connect gate="A" pin="GND_3" pad="12"/>
<connect gate="A" pin="GND_4" pad="24"/>
<connect gate="A" pin="GND_5" pad="27"/>
<connect gate="A" pin="GND_6" pad="21"/>
<connect gate="A" pin="GND_7" pad="9"/>
<connect gate="A" pin="GND_8" pad="41"/>
<connect gate="A" pin="NC" pad="120"/>
<connect gate="A" pin="NC_2" pad="109"/>
<connect gate="A" pin="NC_3" pad="52"/>
<connect gate="A" pin="NC_4" pad="63"/>
<connect gate="A" pin="NC_5" pad="98"/>
<connect gate="A" pin="OR+" pad="79"/>
<connect gate="A" pin="OR-" pad="80"/>
<connect gate="A" pin="OUTV/SCLK" pad="3"/>
<connect gate="A" pin="OUT_EDGE/DDR/SDATA" pad="4"/>
<connect gate="A" pin="PD" pad="26"/>
<connect gate="A" pin="PDQ" pad="29"/>
<connect gate="A" pin="REXT" pad="32"/>
<connect gate="A" pin="TDIODE_N" pad="35"/>
<connect gate="A" pin="TDIODE_P" pad="34"/>
<connect gate="A" pin="VA" pad="128"/>
<connect gate="A" pin="VA_10" pad="25"/>
<connect gate="A" pin="VA_11" pad="28"/>
<connect gate="A" pin="VA_2" pad="5"/>
<connect gate="A" pin="VA_3" pad="2"/>
<connect gate="A" pin="VA_4" pad="8"/>
<connect gate="A" pin="VA_5" pad="16"/>
<connect gate="A" pin="VA_6" pad="13"/>
<connect gate="A" pin="VA_7" pad="33"/>
<connect gate="A" pin="VA_8" pad="17"/>
<connect gate="A" pin="VA_9" pad="20"/>
<connect gate="A" pin="VBG" pad="31"/>
<connect gate="A" pin="VCMO" pad="7"/>
<connect gate="A" pin="VDR" pad="99"/>
<connect gate="A" pin="VDR_2" pad="51"/>
<connect gate="A" pin="VDR_3" pad="62"/>
<connect gate="A" pin="VDR_4" pad="40"/>
<connect gate="A" pin="VDR_5" pad="121"/>
<connect gate="A" pin="VDR_6" pad="73"/>
<connect gate="A" pin="VDR_7" pad="110"/>
<connect gate="A" pin="VDR_8" pad="88"/>
<connect gate="A" pin="VINI+" pad="11"/>
<connect gate="A" pin="VINI-" pad="10"/>
<connect gate="A" pin="VINQ+" pad="22"/>
<connect gate="A" pin="VINQ-" pad="23"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="ADC08D1500CIYB"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="69K1473"/>
<attribute name="PACKAGE" value="QFP-128"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADC08D500CIYB" prefix="U">
<description>Low Power, Dual 8-Bit, 1 MSPS A/D Converter</description>
<gates>
<gate name="A" symbol="ADC08D500CIYB"/>
</gates>
<devices>
<device name="" package="QFP50P2200X2200X160-129N">
<connects>
<connect gate="A" pin="CAL" pad="30"/>
<connect gate="A" pin="CALDLY/DES/~SCS" pad="127"/>
<connect gate="A" pin="CALRUN" pad="126"/>
<connect gate="A" pin="CLK+" pad="18"/>
<connect gate="A" pin="CLK-" pad="19"/>
<connect gate="A" pin="DCLK+" pad="82"/>
<connect gate="A" pin="DCLK-" pad="81"/>
<connect gate="A" pin="DCLK_RST" pad="15"/>
<connect gate="A" pin="DI0+" pad="103"/>
<connect gate="A" pin="DI0-" pad="102"/>
<connect gate="A" pin="DI1+" pad="101"/>
<connect gate="A" pin="DI1-" pad="100"/>
<connect gate="A" pin="DI2+" pad="96"/>
<connect gate="A" pin="DI2-" pad="95"/>
<connect gate="A" pin="DI3+" pad="94"/>
<connect gate="A" pin="DI3-" pad="93"/>
<connect gate="A" pin="DI4+" pad="92"/>
<connect gate="A" pin="DI4-" pad="91"/>
<connect gate="A" pin="DI5+" pad="90"/>
<connect gate="A" pin="DI5-" pad="89"/>
<connect gate="A" pin="DI6+" pad="86"/>
<connect gate="A" pin="DI6-" pad="85"/>
<connect gate="A" pin="DI7+" pad="84"/>
<connect gate="A" pin="DI7-" pad="83"/>
<connect gate="A" pin="DID0+" pad="125"/>
<connect gate="A" pin="DID0-" pad="124"/>
<connect gate="A" pin="DID1+" pad="123"/>
<connect gate="A" pin="DID1-" pad="122"/>
<connect gate="A" pin="DID2+" pad="118"/>
<connect gate="A" pin="DID2-" pad="117"/>
<connect gate="A" pin="DID3+" pad="116"/>
<connect gate="A" pin="DID3-" pad="115"/>
<connect gate="A" pin="DID4+" pad="114"/>
<connect gate="A" pin="DID4-" pad="113"/>
<connect gate="A" pin="DID5+" pad="112"/>
<connect gate="A" pin="DID5-" pad="111"/>
<connect gate="A" pin="DID6+" pad="107"/>
<connect gate="A" pin="DID6-" pad="106"/>
<connect gate="A" pin="DID7+" pad="105"/>
<connect gate="A" pin="DID7-" pad="104"/>
<connect gate="A" pin="DQ0+" pad="58"/>
<connect gate="A" pin="DQ0-" pad="59"/>
<connect gate="A" pin="DQ1+" pad="60"/>
<connect gate="A" pin="DQ1-" pad="61"/>
<connect gate="A" pin="DQ2+" pad="65"/>
<connect gate="A" pin="DQ2-" pad="66"/>
<connect gate="A" pin="DQ3+" pad="67"/>
<connect gate="A" pin="DQ3-" pad="68"/>
<connect gate="A" pin="DQ4+" pad="69"/>
<connect gate="A" pin="DQ4-" pad="70"/>
<connect gate="A" pin="DQ5+" pad="71"/>
<connect gate="A" pin="DQ5-" pad="72"/>
<connect gate="A" pin="DQ6+" pad="75"/>
<connect gate="A" pin="DQ6-" pad="76"/>
<connect gate="A" pin="DQ7+" pad="77"/>
<connect gate="A" pin="DQ7-" pad="78"/>
<connect gate="A" pin="DQD0+" pad="36"/>
<connect gate="A" pin="DQD0-" pad="37"/>
<connect gate="A" pin="DQD1+" pad="38"/>
<connect gate="A" pin="DQD1-" pad="39"/>
<connect gate="A" pin="DQD2+" pad="43"/>
<connect gate="A" pin="DQD2-" pad="44"/>
<connect gate="A" pin="DQD3+" pad="45"/>
<connect gate="A" pin="DQD3-" pad="46"/>
<connect gate="A" pin="DQD4+" pad="47"/>
<connect gate="A" pin="DQD4-" pad="48"/>
<connect gate="A" pin="DQD5+" pad="49"/>
<connect gate="A" pin="DQD5-" pad="50"/>
<connect gate="A" pin="DQD6+" pad="54"/>
<connect gate="A" pin="DQD6-" pad="55"/>
<connect gate="A" pin="DQD7+" pad="56"/>
<connect gate="A" pin="DQD7-" pad="57"/>
<connect gate="A" pin="DR_GND" pad="119"/>
<connect gate="A" pin="DR_GND_2" pad="42"/>
<connect gate="A" pin="DR_GND_3" pad="108"/>
<connect gate="A" pin="DR_GND_4" pad="74"/>
<connect gate="A" pin="DR_GND_5" pad="87"/>
<connect gate="A" pin="DR_GND_6" pad="53"/>
<connect gate="A" pin="DR_GND_7" pad="64"/>
<connect gate="A" pin="DR_GND_8" pad="97"/>
<connect gate="A" pin="EPAD" pad="129"/>
<connect gate="A" pin="FSR/ECE" pad="14"/>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="GND_2" pad="1"/>
<connect gate="A" pin="GND_3" pad="12"/>
<connect gate="A" pin="GND_4" pad="24"/>
<connect gate="A" pin="GND_5" pad="27"/>
<connect gate="A" pin="GND_6" pad="21"/>
<connect gate="A" pin="GND_7" pad="9"/>
<connect gate="A" pin="GND_8" pad="41"/>
<connect gate="A" pin="NC" pad="120"/>
<connect gate="A" pin="NC_2" pad="109"/>
<connect gate="A" pin="NC_3" pad="52"/>
<connect gate="A" pin="NC_4" pad="63"/>
<connect gate="A" pin="NC_5" pad="98"/>
<connect gate="A" pin="OR+" pad="79"/>
<connect gate="A" pin="OR-" pad="80"/>
<connect gate="A" pin="OUTV/SCLK" pad="3"/>
<connect gate="A" pin="OUT_EDGE/DDR/SDATA" pad="4"/>
<connect gate="A" pin="PD" pad="26"/>
<connect gate="A" pin="PDQ" pad="29"/>
<connect gate="A" pin="REXT" pad="32"/>
<connect gate="A" pin="TDIODE_N" pad="35"/>
<connect gate="A" pin="TDIODE_P" pad="34"/>
<connect gate="A" pin="VA" pad="128"/>
<connect gate="A" pin="VA_10" pad="25"/>
<connect gate="A" pin="VA_11" pad="28"/>
<connect gate="A" pin="VA_2" pad="5"/>
<connect gate="A" pin="VA_3" pad="2"/>
<connect gate="A" pin="VA_4" pad="8"/>
<connect gate="A" pin="VA_5" pad="16"/>
<connect gate="A" pin="VA_6" pad="13"/>
<connect gate="A" pin="VA_7" pad="33"/>
<connect gate="A" pin="VA_8" pad="17"/>
<connect gate="A" pin="VA_9" pad="20"/>
<connect gate="A" pin="VBG" pad="31"/>
<connect gate="A" pin="VCMO" pad="7"/>
<connect gate="A" pin="VDR" pad="99"/>
<connect gate="A" pin="VDR_2" pad="51"/>
<connect gate="A" pin="VDR_3" pad="62"/>
<connect gate="A" pin="VDR_4" pad="40"/>
<connect gate="A" pin="VDR_5" pad="121"/>
<connect gate="A" pin="VDR_6" pad="73"/>
<connect gate="A" pin="VDR_7" pad="110"/>
<connect gate="A" pin="VDR_8" pad="88"/>
<connect gate="A" pin="VINI+" pad="11"/>
<connect gate="A" pin="VINI-" pad="10"/>
<connect gate="A" pin="VINQ+" pad="22"/>
<connect gate="A" pin="VINQ-" pad="23"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="ADC08D500CIYB"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="65K5034"/>
<attribute name="PACKAGE" value="QFP-128"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADC08L060CIMT" prefix="U">
<description>A/D converters</description>
<gates>
<gate name="A" symbol="ADC08L060CIMT"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-24N">
<connects>
<connect gate="A" pin="AGND" pad="11"/>
<connect gate="A" pin="AGND_2" pad="5"/>
<connect gate="A" pin="AGND_3" pad="8"/>
<connect gate="A" pin="AGND_4" pad="2"/>
<connect gate="A" pin="CLOCK" pad="24"/>
<connect gate="A" pin="D0" pad="22"/>
<connect gate="A" pin="D1" pad="21"/>
<connect gate="A" pin="D2" pad="20"/>
<connect gate="A" pin="D3" pad="19"/>
<connect gate="A" pin="D4" pad="16"/>
<connect gate="A" pin="D5" pad="15"/>
<connect gate="A" pin="D6" pad="14"/>
<connect gate="A" pin="D7" pad="13"/>
<connect gate="A" pin="DR_GND" pad="17"/>
<connect gate="A" pin="DR_VD" pad="18"/>
<connect gate="A" pin="PD" pad="23"/>
<connect gate="A" pin="VA" pad="12"/>
<connect gate="A" pin="VA_2" pad="1"/>
<connect gate="A" pin="VA_3" pad="4"/>
<connect gate="A" pin="VIN" pad="6"/>
<connect gate="A" pin="VIN_GND" pad="7"/>
<connect gate="A" pin="VRB" pad="10"/>
<connect gate="A" pin="VRM" pad="9"/>
<connect gate="A" pin="VRT" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="ADC08L060CIMT"/>
<attribute name="OC_FARNELL" value="1673972"/>
<attribute name="OC_NEWARK" value="41K1417"/>
<attribute name="PACKAGE" value="SOP-24"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADC10064CIWM" prefix="U">
<description>A/D Converter</description>
<gates>
<gate name="A" symbol="ADC10064CIWM"/>
</gates>
<devices>
<device name="" package="SOIC127P1030X265-28N">
<connects>
<connect gate="A" pin="AGND" pad="15"/>
<connect gate="A" pin="AVCC" pad="8"/>
<connect gate="A" pin="DB0" pad="28"/>
<connect gate="A" pin="DB1" pad="27"/>
<connect gate="A" pin="DB2" pad="26"/>
<connect gate="A" pin="DB3" pad="25"/>
<connect gate="A" pin="DB4" pad="24"/>
<connect gate="A" pin="DB5" pad="23"/>
<connect gate="A" pin="DB6" pad="22"/>
<connect gate="A" pin="DB7" pad="20"/>
<connect gate="A" pin="DB8" pad="19"/>
<connect gate="A" pin="DB9" pad="18"/>
<connect gate="A" pin="DGND" pad="16"/>
<connect gate="A" pin="DVCC" pad="1"/>
<connect gate="A" pin="N.C." pad="21"/>
<connect gate="A" pin="S0" pad="6"/>
<connect gate="A" pin="S1" pad="7"/>
<connect gate="A" pin="SPEED_ADJ" pad="17"/>
<connect gate="A" pin="VIN0" pad="10"/>
<connect gate="A" pin="VIN1" pad="11"/>
<connect gate="A" pin="VIN2" pad="12"/>
<connect gate="A" pin="VIN3" pad="13"/>
<connect gate="A" pin="VREF+" pad="14"/>
<connect gate="A" pin="VREF-" pad="9"/>
<connect gate="A" pin="~CS" pad="5"/>
<connect gate="A" pin="~INT" pad="2"/>
<connect gate="A" pin="~RD" pad="4"/>
<connect gate="A" pin="~S/H" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="ADC10064CIWM"/>
<attribute name="OC_FARNELL" value="1798347"/>
<attribute name="OC_NEWARK" value="73R9366"/>
<attribute name="PACKAGE" value="28-SOIC"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADC10065CIMT" prefix="U">
<description>A/D converters</description>
<gates>
<gate name="A" symbol="ADC10065CIMT"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-28N">
<connects>
<connect gate="A" pin="CLK" pad="1"/>
<connect gate="A" pin="D0" pad="27"/>
<connect gate="A" pin="D1" pad="26"/>
<connect gate="A" pin="D2" pad="25"/>
<connect gate="A" pin="D3" pad="24"/>
<connect gate="A" pin="D4" pad="23"/>
<connect gate="A" pin="D5" pad="20"/>
<connect gate="A" pin="D6" pad="19"/>
<connect gate="A" pin="D7" pad="18"/>
<connect gate="A" pin="D8" pad="17"/>
<connect gate="A" pin="D9" pad="16"/>
<connect gate="A" pin="DF" pad="15"/>
<connect gate="A" pin="IRS" pad="5"/>
<connect gate="A" pin="STDBY" pad="28"/>
<connect gate="A" pin="VCOM" pad="4"/>
<connect gate="A" pin="VDDA" pad="10"/>
<connect gate="A" pin="VDDA_2" pad="9"/>
<connect gate="A" pin="VDDA_3" pad="2"/>
<connect gate="A" pin="VDDIO" pad="22"/>
<connect gate="A" pin="VIN+" pad="13"/>
<connect gate="A" pin="VIN-" pad="12"/>
<connect gate="A" pin="VREF" pad="6"/>
<connect gate="A" pin="VREFB" pad="8"/>
<connect gate="A" pin="VREFT" pad="7"/>
<connect gate="A" pin="VSSA" pad="11"/>
<connect gate="A" pin="VSSA_2" pad="3"/>
<connect gate="A" pin="VSSA_3" pad="14"/>
<connect gate="A" pin="VSSIO" pad="21"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="ADC10065CIMT"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K1524"/>
<attribute name="PACKAGE" value="SOP-28"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADC10080CIMT" prefix="U">
<description>A/D converters</description>
<gates>
<gate name="A" symbol="ADC10080CIMT"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-28N">
<connects>
<connect gate="A" pin="CLK" pad="1"/>
<connect gate="A" pin="D0" pad="27"/>
<connect gate="A" pin="D1" pad="26"/>
<connect gate="A" pin="D2" pad="25"/>
<connect gate="A" pin="D3" pad="24"/>
<connect gate="A" pin="D4" pad="23"/>
<connect gate="A" pin="D5" pad="20"/>
<connect gate="A" pin="D6" pad="19"/>
<connect gate="A" pin="D7" pad="18"/>
<connect gate="A" pin="D8" pad="17"/>
<connect gate="A" pin="D9" pad="16"/>
<connect gate="A" pin="DF" pad="15"/>
<connect gate="A" pin="IRS" pad="5"/>
<connect gate="A" pin="STDBY" pad="28"/>
<connect gate="A" pin="VCOM" pad="4"/>
<connect gate="A" pin="VDDA" pad="10"/>
<connect gate="A" pin="VDDA_2" pad="9"/>
<connect gate="A" pin="VDDA_3" pad="2"/>
<connect gate="A" pin="VDDIO" pad="22"/>
<connect gate="A" pin="VIN+" pad="13"/>
<connect gate="A" pin="VIN-" pad="12"/>
<connect gate="A" pin="VREF" pad="6"/>
<connect gate="A" pin="VREFB" pad="8"/>
<connect gate="A" pin="VREFT" pad="7"/>
<connect gate="A" pin="VSSA" pad="14"/>
<connect gate="A" pin="VSSA_2" pad="3"/>
<connect gate="A" pin="VSSA_3" pad="11"/>
<connect gate="A" pin="VSSIO" pad="21"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="ADC10080CIMT"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K1525"/>
<attribute name="PACKAGE" value="SOP-28"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADC10154CIWM" prefix="U">
<description>A/D converters</description>
<gates>
<gate name="A" symbol="ADC10154CIWM"/>
</gates>
<devices>
<device name="" package="SOIC127P1032X265-24N">
<connects>
<connect gate="A" pin="AV+" pad="1"/>
<connect gate="A" pin="CH0" pad="4"/>
<connect gate="A" pin="CH1" pad="5"/>
<connect gate="A" pin="CH2" pad="6"/>
<connect gate="A" pin="CH3" pad="7"/>
<connect gate="A" pin="CLK" pad="22"/>
<connect gate="A" pin="DB0" pad="20"/>
<connect gate="A" pin="DB1" pad="19"/>
<connect gate="A" pin="DB2" pad="18"/>
<connect gate="A" pin="DB3" pad="17"/>
<connect gate="A" pin="DB4" pad="16"/>
<connect gate="A" pin="DB5" pad="15"/>
<connect gate="A" pin="DB6" pad="14"/>
<connect gate="A" pin="DB7" pad="13"/>
<connect gate="A" pin="DGND" pad="12"/>
<connect gate="A" pin="DV+" pad="24"/>
<connect gate="A" pin="V-" pad="11"/>
<connect gate="A" pin="VREF+" pad="9"/>
<connect gate="A" pin="VREF-" pad="10"/>
<connect gate="A" pin="VREF_OUT" pad="8"/>
<connect gate="A" pin="~CS" pad="2"/>
<connect gate="A" pin="~INT" pad="21"/>
<connect gate="A" pin="~RD" pad="3"/>
<connect gate="A" pin="~WR" pad="23"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="ADC10154CIWM"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K1529"/>
<attribute name="PACKAGE" value="ADCIC"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADC10158CIWM" prefix="U">
<description>ADCs</description>
<gates>
<gate name="A" symbol="ADC10158CIWM"/>
</gates>
<devices>
<device name="" package="SOIC127P1032X265-28N">
<connects>
<connect gate="A" pin="AV+" pad="1"/>
<connect gate="A" pin="CH0" pad="2"/>
<connect gate="A" pin="CH1" pad="3"/>
<connect gate="A" pin="CH2" pad="4"/>
<connect gate="A" pin="CH3" pad="5"/>
<connect gate="A" pin="CH4" pad="6"/>
<connect gate="A" pin="CH5" pad="7"/>
<connect gate="A" pin="CH6" pad="8"/>
<connect gate="A" pin="CH7" pad="9"/>
<connect gate="A" pin="CLK" pad="24"/>
<connect gate="A" pin="DB0(MA0)" pad="22"/>
<connect gate="A" pin="DB1(MA1)" pad="21"/>
<connect gate="A" pin="DB2(MA2)" pad="20"/>
<connect gate="A" pin="DB3(MA3)" pad="19"/>
<connect gate="A" pin="DB4(MA4)" pad="18"/>
<connect gate="A" pin="DB5(U/~S)" pad="17"/>
<connect gate="A" pin="DB6(8/~10)" pad="16"/>
<connect gate="A" pin="DB7(L/~R)" pad="15"/>
<connect gate="A" pin="DGND" pad="14"/>
<connect gate="A" pin="DV+" pad="28"/>
<connect gate="A" pin="V-" pad="13"/>
<connect gate="A" pin="VREF+" pad="11"/>
<connect gate="A" pin="VREF-" pad="12"/>
<connect gate="A" pin="VREFOUT" pad="10"/>
<connect gate="A" pin="~CS" pad="27"/>
<connect gate="A" pin="~INT" pad="23"/>
<connect gate="A" pin="~RD" pad="26"/>
<connect gate="A" pin="~WR" pad="25"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="ADC10158CIWM"/>
<attribute name="OC_FARNELL" value="1798348"/>
<attribute name="OC_NEWARK" value="73R9367"/>
<attribute name="PACKAGE" value="28-SOIC"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADC101S021CIMF" prefix="U">
<description>10-Bit A/D Converter</description>
<gates>
<gate name="A" symbol="ADC101S021CIMF"/>
</gates>
<devices>
<device name="" package="SOT95P285X120-6N">
<connects>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="SCLK" pad="4"/>
<connect gate="A" pin="SDATA" pad="5"/>
<connect gate="A" pin="VA" pad="1"/>
<connect gate="A" pin="VIN" pad="3"/>
<connect gate="A" pin="~CS" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="ADC101S021CIMF"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="69K1507"/>
<attribute name="PACKAGE" value="SOT-6"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADC101S021CISD" prefix="U">
<description>10-Bit A/D Converter</description>
<gates>
<gate name="A" symbol="ADC101S021CISD"/>
</gates>
<devices>
<device name="" package="DFN220X250X80-7N">
<connects>
<connect gate="A" pin="EPAD" pad="7"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="SCLK" pad="4"/>
<connect gate="A" pin="SDATA" pad="5"/>
<connect gate="A" pin="VA" pad="1"/>
<connect gate="A" pin="VIN" pad="3"/>
<connect gate="A" pin="~CS" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="ADC101S021CISD"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="79K5522"/>
<attribute name="PACKAGE" value="DFN-6"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADC101S051CIMF" prefix="U">
<description>A/D Converters</description>
<gates>
<gate name="A" symbol="ADC101S051CIMF"/>
</gates>
<devices>
<device name="" package="SOT95P284X122-6N">
<connects>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="SCLK" pad="4"/>
<connect gate="A" pin="SDATA" pad="5"/>
<connect gate="A" pin="VA" pad="1"/>
<connect gate="A" pin="VIN" pad="3"/>
<connect gate="A" pin="~CS" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="ADC101S051CIMF"/>
<attribute name="OC_FARNELL" value="1250029"/>
<attribute name="OC_NEWARK" value="12M7667"/>
<attribute name="PACKAGE" value="SOT-6"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADC101S051CISD" prefix="U">
<description>10-Bit A/D Converter</description>
<gates>
<gate name="A" symbol="ADC101S051CISD"/>
</gates>
<devices>
<device name="" package="DFN220X250X80-7N">
<connects>
<connect gate="A" pin="EPAD" pad="7"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="SCLK" pad="4"/>
<connect gate="A" pin="SDATA" pad="5"/>
<connect gate="A" pin="VA" pad="1"/>
<connect gate="A" pin="VIN" pad="3"/>
<connect gate="A" pin="~CS" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="ADC101S021CISD"/>
<attribute name="OC_FARNELL" value="1312529"/>
<attribute name="OC_NEWARK" value="-"/>
<attribute name="PACKAGE" value="DFN-6"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADC101S101CIMF" prefix="U">
<description>A/D Converters</description>
<gates>
<gate name="A" symbol="ADC101S101CIMF"/>
</gates>
<devices>
<device name="" package="SOT95P284X122-6N">
<connects>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="SCLK" pad="4"/>
<connect gate="A" pin="SDATA" pad="5"/>
<connect gate="A" pin="VDD" pad="1"/>
<connect gate="A" pin="VIN" pad="3"/>
<connect gate="A" pin="~CS" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="ADC101S101CIMF"/>
<attribute name="OC_FARNELL" value="1007985"/>
<attribute name="OC_NEWARK" value="41K1527"/>
<attribute name="PACKAGE" value="SOT-6"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADC102S021CIMM" prefix="U">
<description>A/D converters</description>
<gates>
<gate name="A" symbol="ADC102S021CIMM"/>
</gates>
<devices>
<device name="" package="SOP65P490X109-8N">
<connects>
<connect gate="A" pin="DIN" pad="6"/>
<connect gate="A" pin="DOUT" pad="7"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="IN1" pad="5"/>
<connect gate="A" pin="IN2" pad="4"/>
<connect gate="A" pin="SCLK" pad="8"/>
<connect gate="A" pin="VA" pad="2"/>
<connect gate="A" pin="~CS" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="ADC102S021CIMM"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K1531"/>
<attribute name="PACKAGE" value="SOP-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADC102S101CIMM" prefix="U">
<description>A/D converters</description>
<gates>
<gate name="A" symbol="ADC102S101CIMM"/>
</gates>
<devices>
<device name="" package="SOP65P490X109-8N">
<connects>
<connect gate="A" pin="DIN" pad="6"/>
<connect gate="A" pin="DOUT" pad="7"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="IN1" pad="5"/>
<connect gate="A" pin="IN2" pad="4"/>
<connect gate="A" pin="SCLK" pad="8"/>
<connect gate="A" pin="VA" pad="2"/>
<connect gate="A" pin="~CS" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="ADC102S101CIMM"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K1535"/>
<attribute name="PACKAGE" value="MSOP-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADC104S021CIMM" prefix="U">
<description>10-Bit A/D Converter</description>
<gates>
<gate name="A" symbol="ADC104S021CIMM"/>
</gates>
<devices>
<device name="" package="SOP50P490X109-10N">
<connects>
<connect gate="A" pin="DIN" pad="8"/>
<connect gate="A" pin="DOUT" pad="9"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="IN1" pad="7"/>
<connect gate="A" pin="IN2" pad="6"/>
<connect gate="A" pin="IN3" pad="5"/>
<connect gate="A" pin="IN4" pad="4"/>
<connect gate="A" pin="SCLK" pad="10"/>
<connect gate="A" pin="VA" pad="2"/>
<connect gate="A" pin="~CS" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="National"/>
<attribute name="OC_FARNELL" value="1007989"/>
<attribute name="OC_NEWARK" value="41K1538"/>
<attribute name="PACKAGE" value="SOP-10"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADC104S051CIMM" prefix="U">
<description>A/D converters</description>
<gates>
<gate name="A" symbol="ADC104S051CIMM"/>
</gates>
<devices>
<device name="" package="SOP50P490X109-10N">
<connects>
<connect gate="A" pin="DIN" pad="8"/>
<connect gate="A" pin="DOUT" pad="9"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="IN1" pad="7"/>
<connect gate="A" pin="IN2" pad="6"/>
<connect gate="A" pin="IN3" pad="5"/>
<connect gate="A" pin="IN4" pad="4"/>
<connect gate="A" pin="SCLK" pad="10"/>
<connect gate="A" pin="VA" pad="2"/>
<connect gate="A" pin="~CS" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="ADC104S051CIMM"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K1540"/>
<attribute name="PACKAGE" value="TSSOP-10"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADC104S101CIMM" prefix="U">
<description>A/D converters</description>
<gates>
<gate name="A" symbol="ADC104S101CIMM"/>
</gates>
<devices>
<device name="" package="SOP50P490X109-10N">
<connects>
<connect gate="A" pin="DIN" pad="8"/>
<connect gate="A" pin="DOUT" pad="9"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="IN1" pad="7"/>
<connect gate="A" pin="IN2" pad="6"/>
<connect gate="A" pin="IN3" pad="5"/>
<connect gate="A" pin="IN4" pad="4"/>
<connect gate="A" pin="SCLK" pad="10"/>
<connect gate="A" pin="VA" pad="2"/>
<connect gate="A" pin="~CS" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="ADC104S101CIMM"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K1542"/>
<attribute name="PACKAGE" value="TSSOP-10"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADC10664CIWM" prefix="U">
<description>A/D converters</description>
<gates>
<gate name="A" symbol="ADC10664CIWM"/>
</gates>
<devices>
<device name="" package="SOIC127P1032X265-28N">
<connects>
<connect gate="A" pin="AGND" pad="15"/>
<connect gate="A" pin="AVCC" pad="8"/>
<connect gate="A" pin="DB0" pad="28"/>
<connect gate="A" pin="DB1" pad="27"/>
<connect gate="A" pin="DB2" pad="26"/>
<connect gate="A" pin="DB3" pad="25"/>
<connect gate="A" pin="DB4" pad="24"/>
<connect gate="A" pin="DB5" pad="23"/>
<connect gate="A" pin="DB6" pad="22"/>
<connect gate="A" pin="DB7" pad="20"/>
<connect gate="A" pin="DB8" pad="19"/>
<connect gate="A" pin="DB9" pad="18"/>
<connect gate="A" pin="DGND" pad="16"/>
<connect gate="A" pin="D_VCC" pad="1"/>
<connect gate="A" pin="NC" pad="21"/>
<connect gate="A" pin="S0" pad="6"/>
<connect gate="A" pin="S1" pad="7"/>
<connect gate="A" pin="SPEED_ADJ" pad="17"/>
<connect gate="A" pin="VIN0" pad="10"/>
<connect gate="A" pin="VIN1" pad="11"/>
<connect gate="A" pin="VIN2" pad="12"/>
<connect gate="A" pin="VIN3" pad="13"/>
<connect gate="A" pin="VREF+" pad="14"/>
<connect gate="A" pin="VREF-" pad="9"/>
<connect gate="A" pin="~CS" pad="5"/>
<connect gate="A" pin="~INT" pad="2"/>
<connect gate="A" pin="~RD" pad="4"/>
<connect gate="A" pin="~S/H" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="ADC10664CIWM"/>
<attribute name="OC_FARNELL" value="1673979"/>
<attribute name="OC_NEWARK" value="41K1550"/>
<attribute name="PACKAGE" value="SOIC-28"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADC10738CIWM" prefix="U">
<description>A/D converters</description>
<gates>
<gate name="A" symbol="ADC10738CIWM"/>
</gates>
<devices>
<device name="" package="SOP127P1032X265-24N">
<connects>
<connect gate="A" pin="AGND" pad="15"/>
<connect gate="A" pin="AV+" pad="1"/>
<connect gate="A" pin="CH0" pad="2"/>
<connect gate="A" pin="CH1" pad="3"/>
<connect gate="A" pin="CH2" pad="4"/>
<connect gate="A" pin="CH3" pad="5"/>
<connect gate="A" pin="CH4" pad="6"/>
<connect gate="A" pin="CH5" pad="7"/>
<connect gate="A" pin="CH6" pad="8"/>
<connect gate="A" pin="CH7" pad="9"/>
<connect gate="A" pin="CLK" pad="20"/>
<connect gate="A" pin="COM" pad="10"/>
<connect gate="A" pin="DGND" pad="12"/>
<connect gate="A" pin="DI" pad="21"/>
<connect gate="A" pin="DO" pad="18"/>
<connect gate="A" pin="DV+" pad="24"/>
<connect gate="A" pin="NC" pad="14"/>
<connect gate="A" pin="NC_2" pad="13"/>
<connect gate="A" pin="PD" pad="11"/>
<connect gate="A" pin="SARS" pad="19"/>
<connect gate="A" pin="VREF+" pad="16"/>
<connect gate="A" pin="VREF-" pad="17"/>
<connect gate="A" pin="VREF_OUT" pad="23"/>
<connect gate="A" pin="~CS" pad="22"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="ADC10738CIWM"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K1552"/>
<attribute name="PACKAGE" value="ADCIC"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADC108S022CIMT" prefix="U">
<description>A/D converters</description>
<gates>
<gate name="A" symbol="ADC108S022CIMT"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-16N">
<connects>
<connect gate="A" pin="AGND" pad="3"/>
<connect gate="A" pin="DGND" pad="12"/>
<connect gate="A" pin="DIN" pad="14"/>
<connect gate="A" pin="DOUT" pad="15"/>
<connect gate="A" pin="IN0" pad="4"/>
<connect gate="A" pin="IN1" pad="5"/>
<connect gate="A" pin="IN2" pad="6"/>
<connect gate="A" pin="IN3" pad="7"/>
<connect gate="A" pin="IN4" pad="8"/>
<connect gate="A" pin="IN5" pad="9"/>
<connect gate="A" pin="IN6" pad="10"/>
<connect gate="A" pin="IN7" pad="11"/>
<connect gate="A" pin="SCLK" pad="16"/>
<connect gate="A" pin="VA" pad="2"/>
<connect gate="A" pin="VD" pad="13"/>
<connect gate="A" pin="~CS" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="ADC108S022CIMT"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="69K1515"/>
<attribute name="PACKAGE" value="SOP-16"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADC108S052CIMT" prefix="U">
<description>A/D Converter</description>
<gates>
<gate name="A" symbol="ADC108S052CIMT"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-16N">
<connects>
<connect gate="A" pin="AGND" pad="3"/>
<connect gate="A" pin="DGND" pad="12"/>
<connect gate="A" pin="DIN" pad="14"/>
<connect gate="A" pin="DOUT" pad="15"/>
<connect gate="A" pin="IN0" pad="4"/>
<connect gate="A" pin="IN1" pad="5"/>
<connect gate="A" pin="IN2" pad="6"/>
<connect gate="A" pin="IN3" pad="7"/>
<connect gate="A" pin="IN4" pad="8"/>
<connect gate="A" pin="IN5" pad="9"/>
<connect gate="A" pin="IN6" pad="10"/>
<connect gate="A" pin="IN7" pad="11"/>
<connect gate="A" pin="SCLK" pad="16"/>
<connect gate="A" pin="VA" pad="2"/>
<connect gate="A" pin="VD" pad="13"/>
<connect gate="A" pin="~CS" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="ADC108S052CIMT"/>
<attribute name="OC_FARNELL" value="1250035"/>
<attribute name="OC_NEWARK" value="12M7670"/>
<attribute name="PACKAGE" value="TSSOP-16"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADC108S102CIMT" prefix="U">
<description>A/D converters</description>
<gates>
<gate name="A" symbol="ADC108S102CIMT"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-16N">
<connects>
<connect gate="A" pin="AGND" pad="3"/>
<connect gate="A" pin="DGND" pad="12"/>
<connect gate="A" pin="DIN" pad="14"/>
<connect gate="A" pin="DOUT" pad="15"/>
<connect gate="A" pin="IN0" pad="4"/>
<connect gate="A" pin="IN1" pad="5"/>
<connect gate="A" pin="IN2" pad="6"/>
<connect gate="A" pin="IN3" pad="7"/>
<connect gate="A" pin="IN4" pad="8"/>
<connect gate="A" pin="IN5" pad="9"/>
<connect gate="A" pin="IN6" pad="10"/>
<connect gate="A" pin="IN7" pad="11"/>
<connect gate="A" pin="SCLK" pad="16"/>
<connect gate="A" pin="VA" pad="2"/>
<connect gate="A" pin="VD" pad="13"/>
<connect gate="A" pin="~CS" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="ADC108S102CIMT"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="60K8367"/>
<attribute name="PACKAGE" value="SOP-16"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADC10D020CIVS" prefix="U">
<description>A/D converters</description>
<gates>
<gate name="A" symbol="ADC10D020CIVS"/>
</gates>
<devices>
<device name="" package="QFP50P700X700X120-48N">
<connects>
<connect gate="A" pin="AGND" pad="42"/>
<connect gate="A" pin="AGND_2" pad="39"/>
<connect gate="A" pin="AGND_3" pad="3"/>
<connect gate="A" pin="AGND_4" pad="46"/>
<connect gate="A" pin="CLK" pad="33"/>
<connect gate="A" pin="DGND" pad="5"/>
<connect gate="A" pin="DR_GND" pad="29"/>
<connect gate="A" pin="DR_GND_2" pad="7"/>
<connect gate="A" pin="GAIN" pad="36"/>
<connect gate="A" pin="I+" pad="48"/>
<connect gate="A" pin="I-" pad="47"/>
<connect gate="A" pin="I/~Q" pad="28"/>
<connect gate="A" pin="I0" pad="17"/>
<connect gate="A" pin="I1" pad="16"/>
<connect gate="A" pin="I2" pad="15"/>
<connect gate="A" pin="I3" pad="14"/>
<connect gate="A" pin="I4" pad="13"/>
<connect gate="A" pin="I5" pad="12"/>
<connect gate="A" pin="I6" pad="11"/>
<connect gate="A" pin="I7" pad="10"/>
<connect gate="A" pin="I8" pad="9"/>
<connect gate="A" pin="I9" pad="8"/>
<connect gate="A" pin="OC" pad="31"/>
<connect gate="A" pin="OF" pad="32"/>
<connect gate="A" pin="OS" pad="2"/>
<connect gate="A" pin="PD" pad="35"/>
<connect gate="A" pin="Q+" pad="37"/>
<connect gate="A" pin="Q-" pad="38"/>
<connect gate="A" pin="Q0" pad="27"/>
<connect gate="A" pin="Q1" pad="26"/>
<connect gate="A" pin="Q2" pad="25"/>
<connect gate="A" pin="Q3" pad="24"/>
<connect gate="A" pin="Q4" pad="23"/>
<connect gate="A" pin="Q5" pad="22"/>
<connect gate="A" pin="Q6" pad="21"/>
<connect gate="A" pin="Q7" pad="20"/>
<connect gate="A" pin="Q8" pad="19"/>
<connect gate="A" pin="Q9" pad="18"/>
<connect gate="A" pin="STDBY" pad="34"/>
<connect gate="A" pin="VA" pad="41"/>
<connect gate="A" pin="VA_2" pad="40"/>
<connect gate="A" pin="VCMO" pad="45"/>
<connect gate="A" pin="VD" pad="4"/>
<connect gate="A" pin="VDR" pad="6"/>
<connect gate="A" pin="VDR_2" pad="30"/>
<connect gate="A" pin="VREF" pad="1"/>
<connect gate="A" pin="VRN" pad="44"/>
<connect gate="A" pin="VRP" pad="43"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="ADC10D020CIVS"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="74C3298"/>
<attribute name="PACKAGE" value="QFP-48"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADC10D040CIVS" prefix="U">
<description>A/D Converter</description>
<gates>
<gate name="A" symbol="ADC10D040CIVS"/>
</gates>
<devices>
<device name="" package="QFP50P900X900X120-48N">
<connects>
<connect gate="A" pin="AGND" pad="42"/>
<connect gate="A" pin="AGND_2" pad="3"/>
<connect gate="A" pin="AGND_3" pad="39"/>
<connect gate="A" pin="AGND_4" pad="46"/>
<connect gate="A" pin="CLK" pad="33"/>
<connect gate="A" pin="DGND" pad="5"/>
<connect gate="A" pin="DR_GND" pad="7"/>
<connect gate="A" pin="DR_GND_2" pad="29"/>
<connect gate="A" pin="GAIN" pad="36"/>
<connect gate="A" pin="I+" pad="48"/>
<connect gate="A" pin="I-" pad="47"/>
<connect gate="A" pin="I/~Q" pad="28"/>
<connect gate="A" pin="I0" pad="17"/>
<connect gate="A" pin="I1" pad="16"/>
<connect gate="A" pin="I2" pad="15"/>
<connect gate="A" pin="I3" pad="14"/>
<connect gate="A" pin="I4" pad="13"/>
<connect gate="A" pin="I5" pad="12"/>
<connect gate="A" pin="I6" pad="11"/>
<connect gate="A" pin="I7" pad="10"/>
<connect gate="A" pin="I8" pad="9"/>
<connect gate="A" pin="I9" pad="8"/>
<connect gate="A" pin="OC" pad="31"/>
<connect gate="A" pin="OF" pad="32"/>
<connect gate="A" pin="OS" pad="2"/>
<connect gate="A" pin="PD" pad="35"/>
<connect gate="A" pin="Q+" pad="37"/>
<connect gate="A" pin="Q-" pad="38"/>
<connect gate="A" pin="Q0" pad="27"/>
<connect gate="A" pin="Q1" pad="26"/>
<connect gate="A" pin="Q2" pad="25"/>
<connect gate="A" pin="Q3" pad="24"/>
<connect gate="A" pin="Q4" pad="23"/>
<connect gate="A" pin="Q5" pad="22"/>
<connect gate="A" pin="Q6" pad="21"/>
<connect gate="A" pin="Q7" pad="20"/>
<connect gate="A" pin="Q8" pad="19"/>
<connect gate="A" pin="Q9" pad="18"/>
<connect gate="A" pin="STBY" pad="34"/>
<connect gate="A" pin="VA" pad="41"/>
<connect gate="A" pin="VA_2" pad="40"/>
<connect gate="A" pin="VCMO" pad="45"/>
<connect gate="A" pin="VD" pad="4"/>
<connect gate="A" pin="VDR" pad="6"/>
<connect gate="A" pin="VDR_2" pad="30"/>
<connect gate="A" pin="VREF" pad="1"/>
<connect gate="A" pin="VRN" pad="44"/>
<connect gate="A" pin="VRP" pad="43"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="ADC10D040CIVS"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K1517"/>
<attribute name="PACKAGE" value="QFP-48"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADC10D1000CCMLS" prefix="U">
<description>A/D Converter</description>
<gates>
<gate name="A" symbol="ADC10D1000CCMLS_1"/>
<gate name="B" symbol="ADC10D1000CCMLS_2"/>
<gate name="C" symbol="ADC10D1000CCMLS_3"/>
<gate name="D" symbol="ADC10D1000CCMLS_4"/>
</gates>
<devices>
<device name="" package="BGA376C20X20127PX127P_279X279X">
<connects>
<connect gate="A" pin="CAL" pad="D6"/>
<connect gate="A" pin="CALRUN" pad="B5"/>
<connect gate="A" pin="DI0+" pad="C19"/>
<connect gate="A" pin="DI0-" pad="C20"/>
<connect gate="A" pin="DI1+" pad="D18"/>
<connect gate="A" pin="DI1-" pad="E18"/>
<connect gate="A" pin="DI2+" pad="D19"/>
<connect gate="A" pin="DI2-" pad="D20"/>
<connect gate="A" pin="DI3+" pad="E19"/>
<connect gate="A" pin="DI3-" pad="E20"/>
<connect gate="A" pin="DI4+" pad="F18"/>
<connect gate="A" pin="DID0+" pad="B11"/>
<connect gate="A" pin="DID0-" pad="C11"/>
<connect gate="A" pin="DID1+" pad="A12"/>
<connect gate="A" pin="DID1-" pad="B12"/>
<connect gate="A" pin="DID2+" pad="C12"/>
<connect gate="A" pin="DID2-" pad="D12"/>
<connect gate="A" pin="DID3+" pad="B13"/>
<connect gate="A" pin="DID3-" pad="C13"/>
<connect gate="A" pin="DID4+" pad="A14"/>
<connect gate="A" pin="DID4-" pad="B14"/>
<connect gate="A" pin="DID5+" pad="C14"/>
<connect gate="A" pin="DID5-" pad="D14"/>
<connect gate="A" pin="DID6+" pad="B15"/>
<connect gate="A" pin="DID6-" pad="C15"/>
<connect gate="A" pin="DID7+" pad="A16"/>
<connect gate="A" pin="DID7-" pad="B16"/>
<connect gate="A" pin="DID8+" pad="B17"/>
<connect gate="A" pin="DID8-" pad="C16"/>
<connect gate="A" pin="DID9+" pad="A18"/>
<connect gate="A" pin="DID9-" pad="A19"/>
<connect gate="A" pin="GND" pad="A7"/>
<connect gate="A" pin="GNDDR" pad="F17"/>
<connect gate="A" pin="GNDDR_10" pad="C10"/>
<connect gate="A" pin="GNDDR_11" pad="C17"/>
<connect gate="A" pin="GNDDR_12" pad="D10"/>
<connect gate="A" pin="GNDDR_13" pad="D13"/>
<connect gate="A" pin="GNDDR_14" pad="D16"/>
<connect gate="A" pin="GNDDR_15" pad="E17"/>
<connect gate="A" pin="GNDDR_2" pad="A10"/>
<connect gate="A" pin="GNDDR_3" pad="A13"/>
<connect gate="A" pin="GNDDR_4" pad="A17"/>
<connect gate="A" pin="GNDDR_5" pad="A20"/>
<connect gate="A" pin="GNDDR_6" pad="B10"/>
<connect gate="A" pin="GNDDR_7" pad="B18"/>
<connect gate="A" pin="GNDDR_8" pad="B19"/>
<connect gate="A" pin="GNDDR_9" pad="B20"/>
<connect gate="A" pin="GNDE" pad="C9"/>
<connect gate="A" pin="GNDE_2" pad="A9"/>
<connect gate="A" pin="GNDE_3" pad="B8"/>
<connect gate="A" pin="GNDTC" pad="F2"/>
<connect gate="A" pin="GND_2" pad="B2"/>
<connect gate="A" pin="GND_3" pad="C6"/>
<connect gate="A" pin="GND_4" pad="D4"/>
<connect gate="A" pin="GND_5" pad="C2"/>
<connect gate="A" pin="GND_6" pad="B7"/>
<connect gate="A" pin="GND_7" pad="A1"/>
<connect gate="A" pin="GND_8" pad="D5"/>
<connect gate="A" pin="GND_9" pad="E4"/>
<connect gate="A" pin="NDM" pad="A5"/>
<connect gate="A" pin="REXT+" pad="C3"/>
<connect gate="A" pin="REXT-" pad="D3"/>
<connect gate="A" pin="RTRIM+" pad="C1"/>
<connect gate="A" pin="RTRIM-" pad="D2"/>
<connect gate="A" pin="SCLK" pad="C5"/>
<connect gate="A" pin="SDI" pad="B4"/>
<connect gate="A" pin="SDO" pad="A3"/>
<connect gate="A" pin="TDIODE+" pad="E2"/>
<connect gate="A" pin="TDIODE-" pad="F3"/>
<connect gate="A" pin="TPM" pad="A4"/>
<connect gate="A" pin="VA" pad="F1"/>
<connect gate="A" pin="VA_2" pad="C7"/>
<connect gate="A" pin="VA_3" pad="B6"/>
<connect gate="A" pin="VA_4" pad="A2"/>
<connect gate="A" pin="VA_5" pad="A6"/>
<connect gate="A" pin="VA_6" pad="D9"/>
<connect gate="A" pin="VA_7" pad="D1"/>
<connect gate="A" pin="VA_8" pad="D8"/>
<connect gate="A" pin="VA_9" pad="E1"/>
<connect gate="A" pin="VBG" pad="B1"/>
<connect gate="A" pin="VBIASI" pad="D7"/>
<connect gate="A" pin="VBIASI_2" pad="E3"/>
<connect gate="A" pin="VBIASQ" pad="F4"/>
<connect gate="A" pin="VDR" pad="D17"/>
<connect gate="A" pin="VDR_2" pad="A11"/>
<connect gate="A" pin="VDR_3" pad="D11"/>
<connect gate="A" pin="VDR_4" pad="C18"/>
<connect gate="A" pin="VDR_5" pad="A15"/>
<connect gate="A" pin="VDR_6" pad="D15"/>
<connect gate="A" pin="VE" pad="B9"/>
<connect gate="A" pin="VE_2" pad="A8"/>
<connect gate="A" pin="VE_3" pad="C8"/>
<connect gate="A" pin="~ECE" pad="B3"/>
<connect gate="A" pin="~SCSB" pad="C4"/>
<connect gate="B" pin="CLK+" pad="U2"/>
<connect gate="B" pin="DCLKI+" pad="K19"/>
<connect gate="B" pin="DCLKI-" pad="K20"/>
<connect gate="B" pin="DCLKQ+" pad="L19"/>
<connect gate="B" pin="DCLKQ-" pad="L20"/>
<connect gate="B" pin="DI4-" pad="F19"/>
<connect gate="B" pin="DI5+" pad="G17"/>
<connect gate="B" pin="DI5-" pad="G18"/>
<connect gate="B" pin="DI6+" pad="G19"/>
<connect gate="B" pin="DI6-" pad="G20"/>
<connect gate="B" pin="DI7+" pad="H17"/>
<connect gate="B" pin="DI7-" pad="H18"/>
<connect gate="B" pin="DI8+" pad="H19"/>
<connect gate="B" pin="DI8-" pad="H20"/>
<connect gate="B" pin="DI9+" pad="J18"/>
<connect gate="B" pin="DI9-" pad="J19"/>
<connect gate="B" pin="DQ1-" pad="T18"/>
<connect gate="B" pin="DQ3+" pad="T19"/>
<connect gate="B" pin="DQ3-" pad="T20"/>
<connect gate="B" pin="DQ4+" pad="R18"/>
<connect gate="B" pin="DQ4-" pad="R19"/>
<connect gate="B" pin="DQ5+" pad="P17"/>
<connect gate="B" pin="DQ5-" pad="P18"/>
<connect gate="B" pin="DQ6+" pad="P19"/>
<connect gate="B" pin="DQ6-" pad="P20"/>
<connect gate="B" pin="DQ7+" pad="N17"/>
<connect gate="B" pin="DQ7-" pad="N18"/>
<connect gate="B" pin="DQ8+" pad="N19"/>
<connect gate="B" pin="DQ8-" pad="N20"/>
<connect gate="B" pin="DQ9+" pad="M18"/>
<connect gate="B" pin="DQ9-" pad="M19"/>
<connect gate="B" pin="DQD2-" pad="U12"/>
<connect gate="B" pin="GND" pad="U5"/>
<connect gate="B" pin="GNDDR" pad="U10"/>
<connect gate="B" pin="GNDDR_2" pad="F20"/>
<connect gate="B" pin="GNDDR_3" pad="M17"/>
<connect gate="B" pin="GNDDR_4" pad="M20"/>
<connect gate="B" pin="GNDTC" pad="U1"/>
<connect gate="B" pin="GNDTC_10" pad="R2"/>
<connect gate="B" pin="GNDTC_11" pad="T2"/>
<connect gate="B" pin="GNDTC_12" pad="T3"/>
<connect gate="B" pin="GNDTC_2" pad="G2"/>
<connect gate="B" pin="GNDTC_3" pad="H3"/>
<connect gate="B" pin="GNDTC_4" pad="J2"/>
<connect gate="B" pin="GNDTC_5" pad="K4"/>
<connect gate="B" pin="GNDTC_6" pad="L4"/>
<connect gate="B" pin="GNDTC_7" pad="M2"/>
<connect gate="B" pin="GNDTC_8" pad="N3"/>
<connect gate="B" pin="GNDTC_9" pad="P2"/>
<connect gate="B" pin="GND_2" pad="T4"/>
<connect gate="B" pin="GND_3" pad="K1"/>
<connect gate="B" pin="GND_4" pad="L1"/>
<connect gate="B" pin="GND_5" pad="U4"/>
<connect gate="B" pin="ORI+" pad="K17"/>
<connect gate="B" pin="ORI-" pad="K18"/>
<connect gate="B" pin="ORQ+" pad="L17"/>
<connect gate="B" pin="ORQ-" pad="L18"/>
<connect gate="B" pin="PDI" pad="U3"/>
<connect gate="B" pin="RCOUT1-" pad="U6"/>
<connect gate="B" pin="VA" pad="R1"/>
<connect gate="B" pin="VA_2" pad="U8"/>
<connect gate="B" pin="VA_3" pad="H4"/>
<connect gate="B" pin="VA_4" pad="U9"/>
<connect gate="B" pin="VA_5" pad="N4"/>
<connect gate="B" pin="VA_6" pad="T1"/>
<connect gate="B" pin="VBIASI" pad="K2"/>
<connect gate="B" pin="VBIASI_2" pad="J4"/>
<connect gate="B" pin="VBIASQ" pad="U7"/>
<connect gate="B" pin="VBIASQ_2" pad="L2"/>
<connect gate="B" pin="VBIASQ_3" pad="M4"/>
<connect gate="B" pin="VDR" pad="T17"/>
<connect gate="B" pin="VDR_2" pad="J17"/>
<connect gate="B" pin="VDR_3" pad="J20"/>
<connect gate="B" pin="VDR_4" pad="R17"/>
<connect gate="B" pin="VDR_5" pad="R20"/>
<connect gate="B" pin="VDR_6" pad="U11"/>
<connect gate="B" pin="VINI+" pad="H1"/>
<connect gate="B" pin="VINI-" pad="J1"/>
<connect gate="B" pin="VINQ+" pad="N1"/>
<connect gate="B" pin="VINQ-" pad="M1"/>
<connect gate="B" pin="VTC" pad="M3"/>
<connect gate="B" pin="VTC_10" pad="P3"/>
<connect gate="B" pin="VTC_11" pad="P1"/>
<connect gate="B" pin="VTC_12" pad="R3"/>
<connect gate="B" pin="VTC_13" pad="P4"/>
<connect gate="B" pin="VTC_14" pad="R4"/>
<connect gate="B" pin="VTC_2" pad="G3"/>
<connect gate="B" pin="VTC_3" pad="G4"/>
<connect gate="B" pin="VTC_4" pad="H2"/>
<connect gate="B" pin="VTC_5" pad="K3"/>
<connect gate="B" pin="VTC_6" pad="J3"/>
<connect gate="B" pin="VTC_7" pad="G1"/>
<connect gate="B" pin="VTC_8" pad="L3"/>
<connect gate="B" pin="VTC_9" pad="N2"/>
<connect gate="C" pin="CLK-" pad="V1"/>
<connect gate="C" pin="DCLK_RST+" pad="V2"/>
<connect gate="C" pin="DCLK_RST-" pad="W1"/>
<connect gate="C" pin="DDRPH" pad="W4"/>
<connect gate="C" pin="DQ0+" pad="V19"/>
<connect gate="C" pin="DQ0-" pad="V20"/>
<connect gate="C" pin="DQ1+" pad="U18"/>
<connect gate="C" pin="DQ2+" pad="U19"/>
<connect gate="C" pin="DQ2-" pad="U20"/>
<connect gate="C" pin="DQD0+" pad="W11"/>
<connect gate="C" pin="DQD0-" pad="V11"/>
<connect gate="C" pin="DQD1+" pad="Y12"/>
<connect gate="C" pin="DQD1-" pad="W12"/>
<connect gate="C" pin="DQD2+" pad="V12"/>
<connect gate="C" pin="DQD3+" pad="W13"/>
<connect gate="C" pin="DQD3-" pad="V13"/>
<connect gate="C" pin="DQD4+" pad="Y14"/>
<connect gate="C" pin="DQD4-" pad="W14"/>
<connect gate="C" pin="DQD5+" pad="V14"/>
<connect gate="C" pin="DQD5-" pad="U14"/>
<connect gate="C" pin="DQD6+" pad="W15"/>
<connect gate="C" pin="DQD6-" pad="V15"/>
<connect gate="C" pin="DQD7+" pad="Y16"/>
<connect gate="C" pin="DQD7-" pad="W16"/>
<connect gate="C" pin="DQD8+" pad="W17"/>
<connect gate="C" pin="DQD8-" pad="V16"/>
<connect gate="C" pin="DQD9+" pad="Y18"/>
<connect gate="C" pin="DQD9-" pad="Y19"/>
<connect gate="C" pin="FSR" pad="Y3"/>
<connect gate="C" pin="GND" pad="AC6"/>
<connect gate="C" pin="GNDDR" pad="Y20"/>
<connect gate="C" pin="GNDDR_10" pad="W20"/>
<connect gate="C" pin="GNDDR_11" pad="Y10"/>
<connect gate="C" pin="GNDDR_12" pad="Y13"/>
<connect gate="C" pin="GNDDR_13" pad="Y17"/>
<connect gate="C" pin="GNDDR_2" pad="U13"/>
<connect gate="C" pin="GNDDR_3" pad="U17"/>
<connect gate="C" pin="GNDDR_4" pad="V10"/>
<connect gate="C" pin="GNDDR_5" pad="V17"/>
<connect gate="C" pin="GNDDR_6" pad="V18"/>
<connect gate="C" pin="GNDDR_7" pad="W10"/>
<connect gate="C" pin="GNDDR_8" pad="W18"/>
<connect gate="C" pin="GNDDR_9" pad="W19"/>
<connect gate="C" pin="GNDE" pad="Y9"/>
<connect gate="C" pin="GNDE_2" pad="V9"/>
<connect gate="C" pin="GNDE_3" pad="W8"/>
<connect gate="C" pin="GND_10" pad="AA4"/>
<connect gate="C" pin="GND_11" pad="AA5"/>
<connect gate="C" pin="GND_12" pad="AA6"/>
<connect gate="C" pin="GND_13" pad="AA7"/>
<connect gate="C" pin="GND_14" pad="AA8"/>
<connect gate="C" pin="GND_15" pad="AA9"/>
<connect gate="C" pin="GND_16" pad="AA10"/>
<connect gate="C" pin="GND_17" pad="AA11"/>
<connect gate="C" pin="GND_18" pad="AB1"/>
<connect gate="C" pin="GND_19" pad="AB2"/>
<connect gate="C" pin="GND_2" pad="AA3"/>
<connect gate="C" pin="GND_20" pad="AB3"/>
<connect gate="C" pin="GND_21" pad="AB4"/>
<connect gate="C" pin="GND_22" pad="AB5"/>
<connect gate="C" pin="GND_23" pad="AB6"/>
<connect gate="C" pin="GND_24" pad="AB7"/>
<connect gate="C" pin="GND_25" pad="AB8"/>
<connect gate="C" pin="GND_26" pad="AB9"/>
<connect gate="C" pin="GND_27" pad="AB10"/>
<connect gate="C" pin="GND_28" pad="AB11"/>
<connect gate="C" pin="GND_29" pad="AC1"/>
<connect gate="C" pin="GND_3" pad="V5"/>
<connect gate="C" pin="GND_30" pad="AC2"/>
<connect gate="C" pin="GND_31" pad="AC3"/>
<connect gate="C" pin="GND_32" pad="AC4"/>
<connect gate="C" pin="GND_33" pad="AC5"/>
<connect gate="C" pin="GND_4" pad="Y1"/>
<connect gate="C" pin="GND_5" pad="V4"/>
<connect gate="C" pin="GND_6" pad="W7"/>
<connect gate="C" pin="GND_7" pad="W2"/>
<connect gate="C" pin="GND_8" pad="AA2"/>
<connect gate="C" pin="GND_9" pad="Y7"/>
<connect gate="C" pin="PDQ" pad="V3"/>
<connect gate="C" pin="RCLK+" pad="Y4"/>
<connect gate="C" pin="RCLK-" pad="W5"/>
<connect gate="C" pin="RCOUT1+" pad="Y5"/>
<connect gate="C" pin="RCOUT2+" pad="V6"/>
<connect gate="C" pin="RCOUT2-" pad="V7"/>
<connect gate="C" pin="RSV" pad="W3"/>
<connect gate="C" pin="VA" pad="Y6"/>
<connect gate="C" pin="VA_2" pad="Y2"/>
<connect gate="C" pin="VA_3" pad="W6"/>
<connect gate="C" pin="VDR" pad="Y15"/>
<connect gate="C" pin="VDR_2" pad="U15"/>
<connect gate="C" pin="VDR_3" pad="Y11"/>
<connect gate="C" pin="VDR_4" pad="U16"/>
<connect gate="C" pin="VE" pad="Y8"/>
<connect gate="C" pin="VE_2" pad="V8"/>
<connect gate="C" pin="VE_3" pad="W9"/>
<connect gate="D" pin="GND" pad="AH2"/>
<connect gate="D" pin="GND_10" pad="AH11"/>
<connect gate="D" pin="GND_11" pad="AJ1"/>
<connect gate="D" pin="GND_12" pad="AJ2"/>
<connect gate="D" pin="GND_13" pad="AJ3"/>
<connect gate="D" pin="GND_14" pad="AJ4"/>
<connect gate="D" pin="GND_15" pad="AJ5"/>
<connect gate="D" pin="GND_16" pad="AJ6"/>
<connect gate="D" pin="GND_17" pad="AJ7"/>
<connect gate="D" pin="GND_18" pad="AJ8"/>
<connect gate="D" pin="GND_19" pad="AJ9"/>
<connect gate="D" pin="GND_2" pad="AH3"/>
<connect gate="D" pin="GND_20" pad="AJ10"/>
<connect gate="D" pin="GND_21" pad="AJ11"/>
<connect gate="D" pin="GND_22" pad="AK1"/>
<connect gate="D" pin="GND_23" pad="AK2"/>
<connect gate="D" pin="GND_24" pad="AK3"/>
<connect gate="D" pin="GND_25" pad="AK4"/>
<connect gate="D" pin="GND_26" pad="AK5"/>
<connect gate="D" pin="GND_27" pad="AK6"/>
<connect gate="D" pin="GND_28" pad="AK7"/>
<connect gate="D" pin="GND_29" pad="AK8"/>
<connect gate="D" pin="GND_3" pad="AH4"/>
<connect gate="D" pin="GND_30" pad="AK9"/>
<connect gate="D" pin="GND_31" pad="AK10"/>
<connect gate="D" pin="GND_32" pad="AK11"/>
<connect gate="D" pin="GND_33" pad="AL1"/>
<connect gate="D" pin="GND_34" pad="AL2"/>
<connect gate="D" pin="GND_35" pad="AL3"/>
<connect gate="D" pin="GND_36" pad="AL4"/>
<connect gate="D" pin="GND_37" pad="AL5"/>
<connect gate="D" pin="GND_38" pad="AL6"/>
<connect gate="D" pin="GND_39" pad="AL7"/>
<connect gate="D" pin="GND_4" pad="AH5"/>
<connect gate="D" pin="GND_40" pad="AL8"/>
<connect gate="D" pin="GND_41" pad="AL9"/>
<connect gate="D" pin="GND_42" pad="AL10"/>
<connect gate="D" pin="GND_43" pad="AL11"/>
<connect gate="D" pin="GND_44" pad="AC7"/>
<connect gate="D" pin="GND_45" pad="AC8"/>
<connect gate="D" pin="GND_46" pad="AC9"/>
<connect gate="D" pin="GND_47" pad="AC10"/>
<connect gate="D" pin="GND_48" pad="AC11"/>
<connect gate="D" pin="GND_49" pad="AD1"/>
<connect gate="D" pin="GND_5" pad="AH6"/>
<connect gate="D" pin="GND_50" pad="AD2"/>
<connect gate="D" pin="GND_51" pad="AD3"/>
<connect gate="D" pin="GND_52" pad="AD4"/>
<connect gate="D" pin="GND_53" pad="AD5"/>
<connect gate="D" pin="GND_54" pad="AD6"/>
<connect gate="D" pin="GND_55" pad="AD7"/>
<connect gate="D" pin="GND_56" pad="AD8"/>
<connect gate="D" pin="GND_57" pad="AD9"/>
<connect gate="D" pin="GND_58" pad="AD10"/>
<connect gate="D" pin="GND_59" pad="AD11"/>
<connect gate="D" pin="GND_6" pad="AH7"/>
<connect gate="D" pin="GND_60" pad="AE1"/>
<connect gate="D" pin="GND_61" pad="AE2"/>
<connect gate="D" pin="GND_62" pad="AE3"/>
<connect gate="D" pin="GND_63" pad="AE4"/>
<connect gate="D" pin="GND_64" pad="AE5"/>
<connect gate="D" pin="GND_65" pad="AE6"/>
<connect gate="D" pin="GND_66" pad="AE7"/>
<connect gate="D" pin="GND_67" pad="AE8"/>
<connect gate="D" pin="GND_68" pad="AE9"/>
<connect gate="D" pin="GND_69" pad="AE10"/>
<connect gate="D" pin="GND_7" pad="AH8"/>
<connect gate="D" pin="GND_70" pad="AE11"/>
<connect gate="D" pin="GND_71" pad="AF1"/>
<connect gate="D" pin="GND_72" pad="AF2"/>
<connect gate="D" pin="GND_73" pad="AF3"/>
<connect gate="D" pin="GND_74" pad="AF5"/>
<connect gate="D" pin="GND_75" pad="AF4"/>
<connect gate="D" pin="GND_76" pad="AF6"/>
<connect gate="D" pin="GND_77" pad="AF7"/>
<connect gate="D" pin="GND_78" pad="AF8"/>
<connect gate="D" pin="GND_79" pad="AF9"/>
<connect gate="D" pin="GND_8" pad="AH9"/>
<connect gate="D" pin="GND_80" pad="AF10"/>
<connect gate="D" pin="GND_81" pad="AF11"/>
<connect gate="D" pin="GND_82" pad="AG1"/>
<connect gate="D" pin="GND_83" pad="AG2"/>
<connect gate="D" pin="GND_84" pad="AG3"/>
<connect gate="D" pin="GND_85" pad="AG4"/>
<connect gate="D" pin="GND_86" pad="AG5"/>
<connect gate="D" pin="GND_87" pad="AG6"/>
<connect gate="D" pin="GND_88" pad="AG7"/>
<connect gate="D" pin="GND_89" pad="AG8"/>
<connect gate="D" pin="GND_9" pad="AH10"/>
<connect gate="D" pin="GND_90" pad="AG9"/>
<connect gate="D" pin="GND_91" pad="AG10"/>
<connect gate="D" pin="GND_92" pad="AG11"/>
<connect gate="D" pin="GND_93" pad="AH1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="ADC10D1000CCMLS"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="31T9240"/>
<attribute name="PACKAGE" value="PGA-376"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADC1173CIMTC" prefix="U">
<description>A/D Converter</description>
<gates>
<gate name="A" symbol="ADC1173CIMTC"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-24N">
<connects>
<connect gate="A" pin="AVDD" pad="18"/>
<connect gate="A" pin="AVDD_2" pad="14"/>
<connect gate="A" pin="AVDD_3" pad="15"/>
<connect gate="A" pin="AVSS" pad="21"/>
<connect gate="A" pin="AVSS_2" pad="20"/>
<connect gate="A" pin="CLK" pad="12"/>
<connect gate="A" pin="D0" pad="3"/>
<connect gate="A" pin="D1" pad="4"/>
<connect gate="A" pin="D2" pad="5"/>
<connect gate="A" pin="D3" pad="6"/>
<connect gate="A" pin="D4" pad="7"/>
<connect gate="A" pin="D5" pad="8"/>
<connect gate="A" pin="D6" pad="9"/>
<connect gate="A" pin="D7" pad="10"/>
<connect gate="A" pin="DVDD" pad="13"/>
<connect gate="A" pin="DVDD_2" pad="11"/>
<connect gate="A" pin="DVSS" pad="24"/>
<connect gate="A" pin="DVSS_2" pad="2"/>
<connect gate="A" pin="VIN" pad="19"/>
<connect gate="A" pin="VRB" pad="23"/>
<connect gate="A" pin="VRBS" pad="22"/>
<connect gate="A" pin="VRT" pad="17"/>
<connect gate="A" pin="VRTS" pad="16"/>
<connect gate="A" pin="~OE" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="ADC1173CIMTC"/>
<attribute name="OC_FARNELL" value="9778179"/>
<attribute name="OC_NEWARK" value="41K1556"/>
<attribute name="PACKAGE" value="SOP-24"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADC12010CIVY" prefix="U">
<description>A/D Converter</description>
<gates>
<gate name="A" symbol="ADC12010CIVY"/>
</gates>
<devices>
<device name="" package="QFP80P900X900X160-32N">
<connects>
<connect gate="A" pin="AGND" pad="28"/>
<connect gate="A" pin="AGND_2" pad="4"/>
<connect gate="A" pin="AGND_3" pad="7"/>
<connect gate="A" pin="CLK" pad="10"/>
<connect gate="A" pin="D0" pad="14"/>
<connect gate="A" pin="D1" pad="15"/>
<connect gate="A" pin="D10" pad="26"/>
<connect gate="A" pin="D11" pad="27"/>
<connect gate="A" pin="D2" pad="16"/>
<connect gate="A" pin="D3" pad="17"/>
<connect gate="A" pin="D4" pad="18"/>
<connect gate="A" pin="D5" pad="19"/>
<connect gate="A" pin="D6" pad="22"/>
<connect gate="A" pin="D7" pad="23"/>
<connect gate="A" pin="D8" pad="24"/>
<connect gate="A" pin="D9" pad="25"/>
<connect gate="A" pin="DGND" pad="9"/>
<connect gate="A" pin="DGND_2" pad="12"/>
<connect gate="A" pin="DR_GND" pad="20"/>
<connect gate="A" pin="PD" pad="8"/>
<connect gate="A" pin="VA" pad="29"/>
<connect gate="A" pin="VA_2" pad="5"/>
<connect gate="A" pin="VA_3" pad="6"/>
<connect gate="A" pin="VD" pad="13"/>
<connect gate="A" pin="VDR" pad="21"/>
<connect gate="A" pin="VIN+" pad="2"/>
<connect gate="A" pin="VIN-" pad="3"/>
<connect gate="A" pin="VREF" pad="1"/>
<connect gate="A" pin="VRM" pad="32"/>
<connect gate="A" pin="VRN" pad="30"/>
<connect gate="A" pin="VRP" pad="31"/>
<connect gate="A" pin="~OE" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="ADC12010CIVY"/>
<attribute name="OC_FARNELL" value="1286728"/>
<attribute name="OC_NEWARK" value="41K1575"/>
<attribute name="PACKAGE" value="QFP-32"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADC12020CIVY" prefix="U">
<description>A/D Converter</description>
<gates>
<gate name="A" symbol="ADC12020CIVY"/>
</gates>
<devices>
<device name="" package="QFP80P900X900X160-32N">
<connects>
<connect gate="A" pin="AGND" pad="28"/>
<connect gate="A" pin="AGND_2" pad="4"/>
<connect gate="A" pin="AGND_3" pad="7"/>
<connect gate="A" pin="CLK" pad="10"/>
<connect gate="A" pin="D0" pad="14"/>
<connect gate="A" pin="D1" pad="15"/>
<connect gate="A" pin="D10" pad="26"/>
<connect gate="A" pin="D11" pad="27"/>
<connect gate="A" pin="D2" pad="16"/>
<connect gate="A" pin="D3" pad="17"/>
<connect gate="A" pin="D4" pad="18"/>
<connect gate="A" pin="D5" pad="19"/>
<connect gate="A" pin="D6" pad="22"/>
<connect gate="A" pin="D7" pad="23"/>
<connect gate="A" pin="D8" pad="24"/>
<connect gate="A" pin="D9" pad="25"/>
<connect gate="A" pin="DGND" pad="9"/>
<connect gate="A" pin="DGND_2" pad="12"/>
<connect gate="A" pin="DR_GND" pad="20"/>
<connect gate="A" pin="PD" pad="8"/>
<connect gate="A" pin="VA" pad="29"/>
<connect gate="A" pin="VA_2" pad="5"/>
<connect gate="A" pin="VA_3" pad="6"/>
<connect gate="A" pin="VD" pad="13"/>
<connect gate="A" pin="VDR" pad="21"/>
<connect gate="A" pin="VIN+" pad="2"/>
<connect gate="A" pin="VIN-" pad="3"/>
<connect gate="A" pin="VREF" pad="1"/>
<connect gate="A" pin="VRM" pad="32"/>
<connect gate="A" pin="VRN" pad="30"/>
<connect gate="A" pin="VRP" pad="31"/>
<connect gate="A" pin="~OE" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="ADC12020CIVY"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K1576"/>
<attribute name="PACKAGE" value="QFP-32"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADC12038CIWM" prefix="U">
<description>A/D Converters</description>
<gates>
<gate name="A" symbol="ADC12038CIWM"/>
</gates>
<devices>
<device name="" package="SOIC127P1032X265-28N">
<connects>
<connect gate="A" pin="A/DIN1" pad="11"/>
<connect gate="A" pin="A/DIN2" pad="13"/>
<connect gate="A" pin="AGND" pad="18"/>
<connect gate="A" pin="CCLK" pad="26"/>
<connect gate="A" pin="CH0" pad="1"/>
<connect gate="A" pin="CH1" pad="2"/>
<connect gate="A" pin="CH2" pad="3"/>
<connect gate="A" pin="CH3" pad="4"/>
<connect gate="A" pin="CH4" pad="5"/>
<connect gate="A" pin="CH5" pad="6"/>
<connect gate="A" pin="CH6" pad="7"/>
<connect gate="A" pin="CH7" pad="8"/>
<connect gate="A" pin="COM" pad="9"/>
<connect gate="A" pin="DGND" pad="14"/>
<connect gate="A" pin="DI" pad="24"/>
<connect gate="A" pin="DO" pad="23"/>
<connect gate="A" pin="EOC" pad="20"/>
<connect gate="A" pin="MUXOUT1" pad="10"/>
<connect gate="A" pin="MUXOUT2" pad="12"/>
<connect gate="A" pin="PD" pad="19"/>
<connect gate="A" pin="SCLK" pad="25"/>
<connect gate="A" pin="VA+" pad="15"/>
<connect gate="A" pin="VD+" pad="28"/>
<connect gate="A" pin="VREF+" pad="17"/>
<connect gate="A" pin="VREF-" pad="16"/>
<connect gate="A" pin="~CONV" pad="21"/>
<connect gate="A" pin="~CS" pad="22"/>
<connect gate="A" pin="~DOR" pad="27"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="ADC12038CIWM"/>
<attribute name="OC_FARNELL" value="1673980"/>
<attribute name="OC_NEWARK" value="41K1582"/>
<attribute name="PACKAGE" value="SOIC-28"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADC12040CIVY" prefix="U">
<description>A/D Converters</description>
<gates>
<gate name="A" symbol="ADC12040CIVY"/>
</gates>
<devices>
<device name="" package="QFP80P900X900X160-32N">
<connects>
<connect gate="A" pin="AGND" pad="4"/>
<connect gate="A" pin="AGND_2" pad="7"/>
<connect gate="A" pin="AGND_3" pad="28"/>
<connect gate="A" pin="CLK" pad="10"/>
<connect gate="A" pin="D0" pad="14"/>
<connect gate="A" pin="D1" pad="15"/>
<connect gate="A" pin="D10" pad="26"/>
<connect gate="A" pin="D11" pad="27"/>
<connect gate="A" pin="D2" pad="16"/>
<connect gate="A" pin="D3" pad="17"/>
<connect gate="A" pin="D4" pad="18"/>
<connect gate="A" pin="D5" pad="19"/>
<connect gate="A" pin="D6" pad="22"/>
<connect gate="A" pin="D7" pad="23"/>
<connect gate="A" pin="D8" pad="24"/>
<connect gate="A" pin="D9" pad="25"/>
<connect gate="A" pin="DGND" pad="12"/>
<connect gate="A" pin="DGND_2" pad="9"/>
<connect gate="A" pin="DR_GND" pad="20"/>
<connect gate="A" pin="PD" pad="8"/>
<connect gate="A" pin="VA" pad="29"/>
<connect gate="A" pin="VA_2" pad="5"/>
<connect gate="A" pin="VA_3" pad="6"/>
<connect gate="A" pin="VD" pad="13"/>
<connect gate="A" pin="VDR" pad="21"/>
<connect gate="A" pin="VIN+" pad="2"/>
<connect gate="A" pin="VIN-" pad="3"/>
<connect gate="A" pin="VREF" pad="1"/>
<connect gate="A" pin="VRM" pad="32"/>
<connect gate="A" pin="VRN" pad="30"/>
<connect gate="A" pin="VRP" pad="31"/>
<connect gate="A" pin="~OE" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="ADC12040CIVY"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="34C6375"/>
<attribute name="PACKAGE" value="QFP-32"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADC12048CIV" prefix="U">
<description>A/D Converters</description>
<gates>
<gate name="A" symbol="ADC12048CIV"/>
</gates>
<devices>
<device name="" package="PLCC127P1753X1753X457-44N">
<connects>
<connect gate="A" pin="ADCIN+" pad="22"/>
<connect gate="A" pin="ADCIN-" pad="20"/>
<connect gate="A" pin="AGND" pad="11"/>
<connect gate="A" pin="CH0" pad="6"/>
<connect gate="A" pin="CH1" pad="7"/>
<connect gate="A" pin="CH2" pad="8"/>
<connect gate="A" pin="CH3" pad="9"/>
<connect gate="A" pin="CH4" pad="15"/>
<connect gate="A" pin="CH5" pad="16"/>
<connect gate="A" pin="CH6" pad="17"/>
<connect gate="A" pin="CH7" pad="18"/>
<connect gate="A" pin="CLK" pad="43"/>
<connect gate="A" pin="COM" pad="14"/>
<connect gate="A" pin="D0" pad="26"/>
<connect gate="A" pin="D1" pad="27"/>
<connect gate="A" pin="D10" pad="38"/>
<connect gate="A" pin="D11" pad="39"/>
<connect gate="A" pin="D12" pad="40"/>
<connect gate="A" pin="D2" pad="28"/>
<connect gate="A" pin="D3" pad="29"/>
<connect gate="A" pin="D4" pad="30"/>
<connect gate="A" pin="D5" pad="31"/>
<connect gate="A" pin="D6" pad="34"/>
<connect gate="A" pin="D7" pad="35"/>
<connect gate="A" pin="D8" pad="36"/>
<connect gate="A" pin="D9" pad="37"/>
<connect gate="A" pin="DGND" pad="42"/>
<connect gate="A" pin="DGND_2" pad="33"/>
<connect gate="A" pin="MUXOUT+" pad="21"/>
<connect gate="A" pin="MUXOUT-" pad="19"/>
<connect gate="A" pin="NC" pad="23"/>
<connect gate="A" pin="NC_2" pad="5"/>
<connect gate="A" pin="SYNC" pad="25"/>
<connect gate="A" pin="VA+" pad="10"/>
<connect gate="A" pin="VD+" pad="32"/>
<connect gate="A" pin="VD+_2" pad="41"/>
<connect gate="A" pin="VREF+" pad="13"/>
<connect gate="A" pin="VREF-" pad="12"/>
<connect gate="A" pin="WMODE" pad="24"/>
<connect gate="A" pin="~CS" pad="2"/>
<connect gate="A" pin="~RD" pad="1"/>
<connect gate="A" pin="~RDY" pad="3"/>
<connect gate="A" pin="~STDBY" pad="4"/>
<connect gate="A" pin="~WR" pad="44"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="ADC12048CIV"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="13B4912"/>
<attribute name="PACKAGE" value="PLCC-44"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADC12048CIVF" prefix="U">
<description>A/D Converters</description>
<gates>
<gate name="A" symbol="ADC12048CIVF"/>
</gates>
<devices>
<device name="" package="QFP80P1320X1320X245-44N">
<connects>
<connect gate="A" pin="ADCIN+" pad="16"/>
<connect gate="A" pin="ADCIN-" pad="14"/>
<connect gate="A" pin="AGND" pad="5"/>
<connect gate="A" pin="CH0" pad="44"/>
<connect gate="A" pin="CH1" pad="1"/>
<connect gate="A" pin="CH2" pad="2"/>
<connect gate="A" pin="CH3" pad="3"/>
<connect gate="A" pin="CH4" pad="9"/>
<connect gate="A" pin="CH5" pad="10"/>
<connect gate="A" pin="CH6" pad="11"/>
<connect gate="A" pin="CH7" pad="12"/>
<connect gate="A" pin="CLK" pad="37"/>
<connect gate="A" pin="COM" pad="8"/>
<connect gate="A" pin="D0" pad="20"/>
<connect gate="A" pin="D1" pad="21"/>
<connect gate="A" pin="D10" pad="32"/>
<connect gate="A" pin="D11" pad="33"/>
<connect gate="A" pin="D12" pad="34"/>
<connect gate="A" pin="D2" pad="22"/>
<connect gate="A" pin="D3" pad="23"/>
<connect gate="A" pin="D4" pad="24"/>
<connect gate="A" pin="D5" pad="25"/>
<connect gate="A" pin="D6" pad="28"/>
<connect gate="A" pin="D7" pad="29"/>
<connect gate="A" pin="D8" pad="30"/>
<connect gate="A" pin="D9" pad="31"/>
<connect gate="A" pin="DGND" pad="27"/>
<connect gate="A" pin="DGND_2" pad="36"/>
<connect gate="A" pin="MUXOUT+" pad="15"/>
<connect gate="A" pin="MUXOUT_-" pad="13"/>
<connect gate="A" pin="NC" pad="43"/>
<connect gate="A" pin="NC_2" pad="17"/>
<connect gate="A" pin="SYNC" pad="19"/>
<connect gate="A" pin="VA+" pad="4"/>
<connect gate="A" pin="VD+" pad="26"/>
<connect gate="A" pin="VD+_2" pad="35"/>
<connect gate="A" pin="VREF+" pad="7"/>
<connect gate="A" pin="VREF-" pad="6"/>
<connect gate="A" pin="WMODE" pad="18"/>
<connect gate="A" pin="~CS" pad="40"/>
<connect gate="A" pin="~RD" pad="39"/>
<connect gate="A" pin="~RDY" pad="41"/>
<connect gate="A" pin="~STDBY" pad="42"/>
<connect gate="A" pin="~WR" pad="38"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="ADC12048CIVF"/>
<attribute name="OC_FARNELL" value="1673951"/>
<attribute name="OC_NEWARK" value="41K1586"/>
<attribute name="PACKAGE" value="QFP-44"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADC12130CIWM" prefix="U">
<description>A/D Converters</description>
<gates>
<gate name="A" symbol="ADC12130CIWM"/>
</gates>
<devices>
<device name="" package="SOIC127P1030X265-16N">
<connects>
<connect gate="A" pin="CCLK" pad="15"/>
<connect gate="A" pin="CH0" pad="1"/>
<connect gate="A" pin="CH1" pad="2"/>
<connect gate="A" pin="COM" pad="3"/>
<connect gate="A" pin="DGND" pad="8"/>
<connect gate="A" pin="DI" pad="13"/>
<connect gate="A" pin="DO" pad="12"/>
<connect gate="A" pin="EOC" pad="5"/>
<connect gate="A" pin="SCLK" pad="14"/>
<connect gate="A" pin="VA+" pad="9"/>
<connect gate="A" pin="VD+" pad="16"/>
<connect gate="A" pin="VREF+" pad="7"/>
<connect gate="A" pin="VREF-" pad="6"/>
<connect gate="A" pin="~CONV" pad="10"/>
<connect gate="A" pin="~CS" pad="11"/>
<connect gate="A" pin="~DOR" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="ADC12130CIWM"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="07B4761"/>
<attribute name="PACKAGE" value="SOIC-16"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADC12138CIMSA" prefix="U">
<description>A/D Converters</description>
<gates>
<gate name="A" symbol="ADC12138CIMSA"/>
</gates>
<devices>
<device name="" package="SOP65P770X200-28N">
<connects>
<connect gate="A" pin="A/DIN1" pad="11"/>
<connect gate="A" pin="A/DIN2" pad="13"/>
<connect gate="A" pin="AGND" pad="18"/>
<connect gate="A" pin="CCLK" pad="26"/>
<connect gate="A" pin="CH0" pad="1"/>
<connect gate="A" pin="CH1" pad="2"/>
<connect gate="A" pin="CH2" pad="3"/>
<connect gate="A" pin="CH3" pad="4"/>
<connect gate="A" pin="CH4" pad="5"/>
<connect gate="A" pin="CH5" pad="6"/>
<connect gate="A" pin="CH6" pad="7"/>
<connect gate="A" pin="CH7" pad="8"/>
<connect gate="A" pin="COM" pad="9"/>
<connect gate="A" pin="DGND" pad="14"/>
<connect gate="A" pin="DI" pad="24"/>
<connect gate="A" pin="DO" pad="23"/>
<connect gate="A" pin="EOC" pad="20"/>
<connect gate="A" pin="MUXOUT1" pad="10"/>
<connect gate="A" pin="MUXOUT2" pad="12"/>
<connect gate="A" pin="PD" pad="19"/>
<connect gate="A" pin="SCLK" pad="25"/>
<connect gate="A" pin="VA+" pad="15"/>
<connect gate="A" pin="VD+" pad="28"/>
<connect gate="A" pin="VREF+" pad="17"/>
<connect gate="A" pin="VREF-" pad="16"/>
<connect gate="A" pin="~CONV" pad="21"/>
<connect gate="A" pin="~CS" pad="22"/>
<connect gate="A" pin="~DOR" pad="27"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="ADC12138CIMSA"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K1593"/>
<attribute name="PACKAGE" value="SOP-28"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADC12138CIWM" prefix="U">
<description>A/D Converters</description>
<gates>
<gate name="A" symbol="ADC12138CIWM"/>
</gates>
<devices>
<device name="" package="SOIC127P1032X265-28N">
<connects>
<connect gate="A" pin="A/DIN1" pad="11"/>
<connect gate="A" pin="A/DIN2" pad="13"/>
<connect gate="A" pin="AGND" pad="18"/>
<connect gate="A" pin="CCLK" pad="26"/>
<connect gate="A" pin="CH0" pad="1"/>
<connect gate="A" pin="CH1" pad="2"/>
<connect gate="A" pin="CH2" pad="3"/>
<connect gate="A" pin="CH3" pad="4"/>
<connect gate="A" pin="CH4" pad="5"/>
<connect gate="A" pin="CH5" pad="6"/>
<connect gate="A" pin="CH6" pad="7"/>
<connect gate="A" pin="CH7" pad="8"/>
<connect gate="A" pin="COM" pad="9"/>
<connect gate="A" pin="DGND" pad="14"/>
<connect gate="A" pin="DI" pad="24"/>
<connect gate="A" pin="DO" pad="23"/>
<connect gate="A" pin="EOC" pad="20"/>
<connect gate="A" pin="MUXOUT1" pad="10"/>
<connect gate="A" pin="MUXOUT2" pad="12"/>
<connect gate="A" pin="PD" pad="19"/>
<connect gate="A" pin="SCLK" pad="25"/>
<connect gate="A" pin="VA+" pad="15"/>
<connect gate="A" pin="VD+" pad="28"/>
<connect gate="A" pin="VREF+" pad="17"/>
<connect gate="A" pin="VREF-" pad="16"/>
<connect gate="A" pin="~CONV" pad="21"/>
<connect gate="A" pin="~CS" pad="22"/>
<connect gate="A" pin="~DOR" pad="27"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="ADC12138CIWM"/>
<attribute name="OC_FARNELL" value="1798306"/>
<attribute name="OC_NEWARK" value="73R9368"/>
<attribute name="PACKAGE" value="28-SOIC"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADC121C021CIMK" prefix="U">
<description>12-Bit Analog-to-Digital Converter</description>
<gates>
<gate name="A" symbol="ADC121C021CIMK"/>
</gates>
<devices>
<device name="" package="SOT95P285X100-6N">
<connects>
<connect gate="A" pin="ALERT" pad="4"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="SCL" pad="5"/>
<connect gate="A" pin="SDA" pad="6"/>
<connect gate="A" pin="VA" pad="1"/>
<connect gate="A" pin="VIN" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="ADC121C021CIMK"/>
<attribute name="OC_FARNELL" value="1552428"/>
<attribute name="OC_NEWARK" value="78M7722"/>
<attribute name="PACKAGE" value="SOT-6"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADC121C027CIMK" prefix="U">
<description>12-Bit Analog-to-Digital Converter</description>
<gates>
<gate name="A" symbol="ADC121C027CIMK"/>
</gates>
<devices>
<device name="" package="SOT95P285X100-6N">
<connects>
<connect gate="A" pin="ADDR" pad="4"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="SCL" pad="5"/>
<connect gate="A" pin="SDA" pad="6"/>
<connect gate="A" pin="VA" pad="1"/>
<connect gate="A" pin="VIN" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="ADC121C027CIMK"/>
<attribute name="OC_FARNELL" value="1552431"/>
<attribute name="OC_NEWARK" value="78M7723"/>
<attribute name="PACKAGE" value="SOT-6"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADC121S021CIMF" prefix="U">
<description>A/D Converters</description>
<gates>
<gate name="A" symbol="ADC121S021CIMF"/>
</gates>
<devices>
<device name="" package="SOT95P284X122-6N">
<connects>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="SCLK" pad="4"/>
<connect gate="A" pin="SDATA" pad="5"/>
<connect gate="A" pin="VA" pad="1"/>
<connect gate="A" pin="VIN" pad="3"/>
<connect gate="A" pin="~CS" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="ADC121S021CIMF"/>
<attribute name="OC_FARNELL" value="1250025"/>
<attribute name="OC_NEWARK" value="69K1526"/>
<attribute name="PACKAGE" value="SOT-6"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADC121S021CISD" prefix="U">
<description>A/D converters</description>
<gates>
<gate name="A" symbol="ADC121S021CISD"/>
</gates>
<devices>
<device name="" package="DFN220X250X80-7N">
<connects>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="SCLK" pad="4"/>
<connect gate="A" pin="SDATA" pad="5"/>
<connect gate="A" pin="VA" pad="1"/>
<connect gate="A" pin="VIN" pad="3"/>
<connect gate="A" pin="~CS" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="ADC121S021CISD"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="79K5534"/>
<attribute name="PACKAGE" value="DFN-6"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADC121S051CIMF" prefix="U">
<description>A/D Converter</description>
<gates>
<gate name="A" symbol="ADC121S051CIMF"/>
</gates>
<devices>
<device name="" package="SOT95P284X122-6N">
<connects>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="SCLK" pad="4"/>
<connect gate="A" pin="SDATA" pad="5"/>
<connect gate="A" pin="VA" pad="1"/>
<connect gate="A" pin="VIN" pad="3"/>
<connect gate="A" pin="~CS" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="ADC121S051CIMF"/>
<attribute name="OC_FARNELL" value="1250027"/>
<attribute name="OC_NEWARK" value="69K1528"/>
<attribute name="PACKAGE" value="SOT23-6"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADC121S101CIMF" prefix="U">
<description>A/D Converters</description>
<gates>
<gate name="A" symbol="ADC121S101CIMF"/>
</gates>
<devices>
<device name="" package="SOT95P284X122-6N">
<connects>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="SCLK" pad="4"/>
<connect gate="A" pin="SDATA" pad="5"/>
<connect gate="A" pin="VDD" pad="1"/>
<connect gate="A" pin="VIN" pad="3"/>
<connect gate="A" pin="~CS" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="ADC121S101CIMF"/>
<attribute name="OC_FARNELL" value="1007992"/>
<attribute name="OC_NEWARK" value="41K1589"/>
<attribute name="PACKAGE" value="SOT-6"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADC121S101CISD" prefix="U">
<description>A/D converters</description>
<gates>
<gate name="A" symbol="ADC121S101CISD"/>
</gates>
<devices>
<device name="" package="DFN220X250X80-7N">
<connects>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="SCLK" pad="4"/>
<connect gate="A" pin="SDATA" pad="5"/>
<connect gate="A" pin="THERMAL_PAD" pad="7"/>
<connect gate="A" pin="VA" pad="1"/>
<connect gate="A" pin="VIN" pad="3"/>
<connect gate="A" pin="~CS" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="ADC121S101CISD"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="79K5542"/>
<attribute name="PACKAGE" value="DFN-6"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADC121S625CIMM" prefix="U">
<description>A/D converters</description>
<gates>
<gate name="A" symbol="ADC121S625CIMM"/>
</gates>
<devices>
<device name="" package="SOP65P490X109-8N">
<connects>
<connect gate="A" pin="+IN" pad="2"/>
<connect gate="A" pin="+VA" pad="8"/>
<connect gate="A" pin="-IN" pad="3"/>
<connect gate="A" pin="DOUT" pad="6"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="SCLK" pad="7"/>
<connect gate="A" pin="VREF" pad="1"/>
<connect gate="A" pin="~CS" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="ADC121S625CIMM"/>
<attribute name="OC_FARNELL" value="1250039"/>
<attribute name="OC_NEWARK" value="65K5036"/>
<attribute name="PACKAGE" value="MSOP-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADC122S021CIMM" prefix="U">
<description>12-Bit A/D Converter</description>
<gates>
<gate name="A" symbol="ADC122S021CIMM"/>
</gates>
<devices>
<device name="" package="SOP65P490X109-8N">
<connects>
<connect gate="A" pin="DIN" pad="6"/>
<connect gate="A" pin="DOUT" pad="7"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="IN1" pad="5"/>
<connect gate="A" pin="IN2" pad="4"/>
<connect gate="A" pin="SCLK" pad="8"/>
<connect gate="A" pin="VA" pad="2"/>
<connect gate="A" pin="~CS" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="ADC122S021CIMM"/>
<attribute name="OC_FARNELL" value="1007994"/>
<attribute name="OC_NEWARK" value="41K1597"/>
<attribute name="PACKAGE" value="MSOP-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADC122S051CIMM" prefix="U">
<description>12-Bit A/D Converter</description>
<gates>
<gate name="A" symbol="ADC122S051CIMM"/>
</gates>
<devices>
<device name="" package="SOP65P490X109-8N">
<connects>
<connect gate="A" pin="DIN" pad="6"/>
<connect gate="A" pin="DOUT" pad="7"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="IN1" pad="5"/>
<connect gate="A" pin="IN2" pad="4"/>
<connect gate="A" pin="SCLK" pad="8"/>
<connect gate="A" pin="VA" pad="2"/>
<connect gate="A" pin="~CS" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="ADC122S051CIMM"/>
<attribute name="OC_FARNELL" value="1007995"/>
<attribute name="OC_NEWARK" value="96K6192"/>
<attribute name="PACKAGE" value="MSOP-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADC122S101CIMM" prefix="U">
<description>A/D converters</description>
<gates>
<gate name="A" symbol="ADC122S101CIMM"/>
</gates>
<devices>
<device name="" package="SOP65P490X109-8N">
<connects>
<connect gate="A" pin="DIN" pad="6"/>
<connect gate="A" pin="DOUT" pad="7"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="IN1" pad="5"/>
<connect gate="A" pin="IN2" pad="4"/>
<connect gate="A" pin="SCLK" pad="8"/>
<connect gate="A" pin="VA" pad="2"/>
<connect gate="A" pin="~CS" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="ADC122S101CIMM"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K1601"/>
<attribute name="PACKAGE" value="MSOP-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADC122S706CIMT" prefix="U">
<description>A/D Converter</description>
<gates>
<gate name="A" symbol="ADC122S706CIMT"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-14N">
<connects>
<connect gate="A" pin="CHA+" pad="2"/>
<connect gate="A" pin="CHA-" pad="3"/>
<connect gate="A" pin="CHB+" pad="6"/>
<connect gate="A" pin="CHB-" pad="5"/>
<connect gate="A" pin="DOUTA" pad="11"/>
<connect gate="A" pin="DOUTB" pad="12"/>
<connect gate="A" pin="DUAL" pad="8"/>
<connect gate="A" pin="GND" pad="9"/>
<connect gate="A" pin="GND_2" pad="4"/>
<connect gate="A" pin="SCLK" pad="13"/>
<connect gate="A" pin="VA" pad="7"/>
<connect gate="A" pin="VD" pad="10"/>
<connect gate="A" pin="VREF" pad="1"/>
<connect gate="A" pin="~CS" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="ADC122S706CIMT"/>
<attribute name="OC_FARNELL" value="1535368"/>
<attribute name="OC_NEWARK" value="73M8821"/>
<attribute name="PACKAGE" value="TSSOP-14"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADC124S021CIMM" prefix="U">
<description>A/D converters</description>
<gates>
<gate name="A" symbol="ADC124S021CIMM"/>
</gates>
<devices>
<device name="" package="SOP50P490X109-10N">
<connects>
<connect gate="A" pin="DIN" pad="8"/>
<connect gate="A" pin="DOUT" pad="9"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="IN1" pad="7"/>
<connect gate="A" pin="IN2" pad="6"/>
<connect gate="A" pin="IN3" pad="5"/>
<connect gate="A" pin="IN4" pad="4"/>
<connect gate="A" pin="SCLK" pad="10"/>
<connect gate="A" pin="VA" pad="2"/>
<connect gate="A" pin="~CS" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="ADC124S021CIMM"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K1604"/>
<attribute name="PACKAGE" value="MSOP-10"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADC124S051CIMM" prefix="U">
<description>A/D converters</description>
<gates>
<gate name="A" symbol="ADC124S051CIMM"/>
</gates>
<devices>
<device name="" package="SOP50P490X109-10N">
<connects>
<connect gate="A" pin="DIN" pad="8"/>
<connect gate="A" pin="DOUT" pad="9"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="IN1" pad="7"/>
<connect gate="A" pin="IN2" pad="6"/>
<connect gate="A" pin="IN3" pad="5"/>
<connect gate="A" pin="IN4" pad="4"/>
<connect gate="A" pin="SCLK" pad="10"/>
<connect gate="A" pin="VA" pad="2"/>
<connect gate="A" pin="~CS" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="ADC124S051CIMM"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K1606"/>
<attribute name="PACKAGE" value="MSOP-10"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADC124S101CIMM" prefix="U">
<description>A/D converters</description>
<gates>
<gate name="A" symbol="ADC124S101CIMM"/>
</gates>
<devices>
<device name="" package="SOP50P490X109-10N">
<connects>
<connect gate="A" pin="DIN" pad="8"/>
<connect gate="A" pin="DOUT" pad="9"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="IN1" pad="7"/>
<connect gate="A" pin="IN2" pad="6"/>
<connect gate="A" pin="IN3" pad="5"/>
<connect gate="A" pin="IN4" pad="4"/>
<connect gate="A" pin="SCLK" pad="10"/>
<connect gate="A" pin="VA" pad="2"/>
<connect gate="A" pin="~CS" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="ADC124S101CIMM"/>
<attribute name="OC_FARNELL" value="1149936"/>
<attribute name="OC_NEWARK" value="41K1608"/>
<attribute name="PACKAGE" value="MSOP-10"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADC128S022CIMT" prefix="U">
<description>12-Bit A/D Converter</description>
<gates>
<gate name="A" symbol="ADC128S022CIMT"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-16N">
<connects>
<connect gate="A" pin="AGND" pad="3"/>
<connect gate="A" pin="DGND" pad="12"/>
<connect gate="A" pin="DIN" pad="14"/>
<connect gate="A" pin="DOUT" pad="15"/>
<connect gate="A" pin="IN0" pad="4"/>
<connect gate="A" pin="IN1" pad="5"/>
<connect gate="A" pin="IN2" pad="6"/>
<connect gate="A" pin="IN3" pad="7"/>
<connect gate="A" pin="IN4" pad="8"/>
<connect gate="A" pin="IN5" pad="9"/>
<connect gate="A" pin="IN6" pad="10"/>
<connect gate="A" pin="IN7" pad="11"/>
<connect gate="A" pin="SCLK" pad="16"/>
<connect gate="A" pin="VA" pad="2"/>
<connect gate="A" pin="VD" pad="13"/>
<connect gate="A" pin="~CS" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="ADC128S022CIMT"/>
<attribute name="OC_FARNELL" value="1250032"/>
<attribute name="OC_NEWARK" value="69K1533"/>
<attribute name="PACKAGE" value="SOP-16"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADC128S052CIMT" prefix="U">
<description>12-Bit A/D Converter</description>
<gates>
<gate name="A" symbol="ADC128S052CIMT"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-16N">
<connects>
<connect gate="A" pin="AGND" pad="3"/>
<connect gate="A" pin="DGND" pad="12"/>
<connect gate="A" pin="DIN" pad="14"/>
<connect gate="A" pin="DOUT" pad="15"/>
<connect gate="A" pin="IN0" pad="4"/>
<connect gate="A" pin="IN1" pad="5"/>
<connect gate="A" pin="IN2" pad="6"/>
<connect gate="A" pin="IN3" pad="7"/>
<connect gate="A" pin="IN4" pad="8"/>
<connect gate="A" pin="IN5" pad="9"/>
<connect gate="A" pin="IN6" pad="10"/>
<connect gate="A" pin="IN7" pad="11"/>
<connect gate="A" pin="SCLK" pad="16"/>
<connect gate="A" pin="VA" pad="2"/>
<connect gate="A" pin="VD" pad="13"/>
<connect gate="A" pin="~CS" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="ADC128S052CIMT"/>
<attribute name="OC_FARNELL" value="1250033"/>
<attribute name="OC_NEWARK" value="12M7683"/>
<attribute name="PACKAGE" value="SOP-16"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADC128S102CIMT" prefix="U">
<description>12-Bit A/D Converter</description>
<gates>
<gate name="A" symbol="ADC128S102CIMT"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-16N">
<connects>
<connect gate="A" pin="AGND" pad="3"/>
<connect gate="A" pin="DGND" pad="12"/>
<connect gate="A" pin="DIN" pad="14"/>
<connect gate="A" pin="DOUT" pad="15"/>
<connect gate="A" pin="IN0" pad="4"/>
<connect gate="A" pin="IN1" pad="5"/>
<connect gate="A" pin="IN2" pad="6"/>
<connect gate="A" pin="IN3" pad="7"/>
<connect gate="A" pin="IN4" pad="8"/>
<connect gate="A" pin="IN5" pad="9"/>
<connect gate="A" pin="IN6" pad="10"/>
<connect gate="A" pin="IN7" pad="11"/>
<connect gate="A" pin="SCLK" pad="16"/>
<connect gate="A" pin="VA" pad="2"/>
<connect gate="A" pin="VD" pad="13"/>
<connect gate="A" pin="~CS" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="ADC128S102CIMT"/>
<attribute name="OC_FARNELL" value="1286732"/>
<attribute name="OC_NEWARK" value="60K8368"/>
<attribute name="PACKAGE" value="SOP-16"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADC12C105CISQ" prefix="U">
<description>A/D Converter</description>
<gates>
<gate name="A" symbol="ADC12C105CISQ"/>
</gates>
<devices>
<device name="" package="QFN50P500X500X80-33N">
<connects>
<connect gate="A" pin="AGND" pad="9"/>
<connect gate="A" pin="AGND_2" pad="4"/>
<connect gate="A" pin="AGND_3" pad="7"/>
<connect gate="A" pin="CLK" pad="11"/>
<connect gate="A" pin="D0" pad="15"/>
<connect gate="A" pin="D1" pad="16"/>
<connect gate="A" pin="D10" pad="28"/>
<connect gate="A" pin="D11(MSB)" pad="29"/>
<connect gate="A" pin="D2" pad="17"/>
<connect gate="A" pin="D3" pad="18"/>
<connect gate="A" pin="D4" pad="19"/>
<connect gate="A" pin="D5" pad="23"/>
<connect gate="A" pin="D6" pad="24"/>
<connect gate="A" pin="D7" pad="25"/>
<connect gate="A" pin="D8" pad="26"/>
<connect gate="A" pin="D9" pad="27"/>
<connect gate="A" pin="DRDY" pad="21"/>
<connect gate="A" pin="DRGND" pad="22"/>
<connect gate="A" pin="EPAD" pad="33"/>
<connect gate="A" pin="NC" pad="14"/>
<connect gate="A" pin="NC_2" pad="13"/>
<connect gate="A" pin="OF/DCS" pad="12"/>
<connect gate="A" pin="PD" pad="30"/>
<connect gate="A" pin="VA" pad="10"/>
<connect gate="A" pin="VA_2" pad="3"/>
<connect gate="A" pin="VA_3" pad="8"/>
<connect gate="A" pin="VCMO" pad="32"/>
<connect gate="A" pin="VDR" pad="20"/>
<connect gate="A" pin="VIN+" pad="5"/>
<connect gate="A" pin="VIN-" pad="6"/>
<connect gate="A" pin="VREF" pad="31"/>
<connect gate="A" pin="VRN" pad="1"/>
<connect gate="A" pin="VRP" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="ADC12C105CISQ"/>
<attribute name="OC_FARNELL" value="1433177"/>
<attribute name="OC_NEWARK" value="-"/>
<attribute name="PACKAGE" value="QFN-32"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADC12D040CIVS" prefix="U">
<description>A/D Converter</description>
<gates>
<gate name="A" symbol="ADC12D040CIVS"/>
</gates>
<devices>
<device name="" package="QFP50P1200DX1200X120-64N">
<connects>
<connect gate="A" pin="AGND" pad="64"/>
<connect gate="A" pin="AGND_2" pad="3"/>
<connect gate="A" pin="AGND_3" pad="8"/>
<connect gate="A" pin="AGND_4" pad="10"/>
<connect gate="A" pin="AGND_5" pad="17"/>
<connect gate="A" pin="AGND_6" pad="20"/>
<connect gate="A" pin="AGND_7" pad="61"/>
<connect gate="A" pin="CLK" pad="60"/>
<connect gate="A" pin="DA0" pad="24"/>
<connect gate="A" pin="DA1" pad="25"/>
<connect gate="A" pin="DA10" pad="38"/>
<connect gate="A" pin="DA11" pad="39"/>
<connect gate="A" pin="DA2" pad="26"/>
<connect gate="A" pin="DA3" pad="27"/>
<connect gate="A" pin="DA4" pad="28"/>
<connect gate="A" pin="DA5" pad="29"/>
<connect gate="A" pin="DA6" pad="34"/>
<connect gate="A" pin="DA7" pad="35"/>
<connect gate="A" pin="DA8" pad="36"/>
<connect gate="A" pin="DA9" pad="37"/>
<connect gate="A" pin="DB0" pad="42"/>
<connect gate="A" pin="DB1" pad="43"/>
<connect gate="A" pin="DB10" pad="56"/>
<connect gate="A" pin="DB11" pad="57"/>
<connect gate="A" pin="DB2" pad="44"/>
<connect gate="A" pin="DB3" pad="45"/>
<connect gate="A" pin="DB4" pad="46"/>
<connect gate="A" pin="DB5" pad="47"/>
<connect gate="A" pin="DB6" pad="52"/>
<connect gate="A" pin="DB7" pad="53"/>
<connect gate="A" pin="DB8" pad="54"/>
<connect gate="A" pin="DB9" pad="55"/>
<connect gate="A" pin="DGND" pad="49"/>
<connect gate="A" pin="DGND_2" pad="32"/>
<connect gate="A" pin="DR_GND" pad="58"/>
<connect gate="A" pin="DR_GND_2" pad="23"/>
<connect gate="A" pin="DR_GND_3" pad="31"/>
<connect gate="A" pin="DR_GND_4" pad="40"/>
<connect gate="A" pin="DR_GND_5" pad="50"/>
<connect gate="A" pin="OF" pad="21"/>
<connect gate="A" pin="PD" pad="59"/>
<connect gate="A" pin="VA" pad="63"/>
<connect gate="A" pin="VA_2" pad="9"/>
<connect gate="A" pin="VA_3" pad="18"/>
<connect gate="A" pin="VA_4" pad="19"/>
<connect gate="A" pin="VA_5" pad="62"/>
<connect gate="A" pin="VD" pad="48"/>
<connect gate="A" pin="VDR" pad="51"/>
<connect gate="A" pin="VDR_2" pad="30"/>
<connect gate="A" pin="VD_2" pad="33"/>
<connect gate="A" pin="VINB+" pad="2"/>
<connect gate="A" pin="VINB-" pad="1"/>
<connect gate="A" pin="VIN_A+" pad="15"/>
<connect gate="A" pin="VIN_A-" pad="16"/>
<connect gate="A" pin="VREF" pad="7"/>
<connect gate="A" pin="VRM_A" pad="14"/>
<connect gate="A" pin="VRM_B" pad="4"/>
<connect gate="A" pin="VRN_A" pad="12"/>
<connect gate="A" pin="VRN_B" pad="6"/>
<connect gate="A" pin="VRP_A" pad="13"/>
<connect gate="A" pin="VRP_B" pad="5"/>
<connect gate="A" pin="~INT~/_EXT_REF" pad="11"/>
<connect gate="A" pin="~OEA" pad="22"/>
<connect gate="A" pin="~OEB" pad="41"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="ADC12D040CIVS"/>
<attribute name="OC_FARNELL" value="8180695"/>
<attribute name="OC_NEWARK" value="37K8916"/>
<attribute name="PACKAGE" value="QFP-64"/>
<attribute name="SUPPLIER" value="National Semionductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADC12DL040CIVS" prefix="U">
<description>Dual 12-Bit, 40 MSPS, 3V, 210mW A/D Converter</description>
<gates>
<gate name="A" symbol="ADC12DL040CIVS"/>
</gates>
<devices>
<device name="" package="QFP50P1200X1200X120-64N">
<connects>
<connect gate="A" pin="AGND" pad="61"/>
<connect gate="A" pin="AGND_2" pad="8"/>
<connect gate="A" pin="AGND_3" pad="3"/>
<connect gate="A" pin="AGND_4" pad="17"/>
<connect gate="A" pin="AGND_5" pad="20"/>
<connect gate="A" pin="AGND_6" pad="10"/>
<connect gate="A" pin="AGND_7" pad="64"/>
<connect gate="A" pin="CLK" pad="60"/>
<connect gate="A" pin="DA0" pad="24"/>
<connect gate="A" pin="DA1" pad="25"/>
<connect gate="A" pin="DA10" pad="38"/>
<connect gate="A" pin="DA11" pad="39"/>
<connect gate="A" pin="DA2" pad="26"/>
<connect gate="A" pin="DA3" pad="27"/>
<connect gate="A" pin="DA4" pad="28"/>
<connect gate="A" pin="DA5" pad="29"/>
<connect gate="A" pin="DA6" pad="34"/>
<connect gate="A" pin="DA7" pad="35"/>
<connect gate="A" pin="DA8" pad="36"/>
<connect gate="A" pin="DA9" pad="37"/>
<connect gate="A" pin="DB0/ABB" pad="42"/>
<connect gate="A" pin="DB1" pad="43"/>
<connect gate="A" pin="DB10" pad="56"/>
<connect gate="A" pin="DB11" pad="57"/>
<connect gate="A" pin="DB2" pad="44"/>
<connect gate="A" pin="DB3" pad="45"/>
<connect gate="A" pin="DB4" pad="46"/>
<connect gate="A" pin="DB5" pad="47"/>
<connect gate="A" pin="DB6" pad="52"/>
<connect gate="A" pin="DB7" pad="53"/>
<connect gate="A" pin="DB8" pad="54"/>
<connect gate="A" pin="DB9" pad="55"/>
<connect gate="A" pin="DF/DCS" pad="21"/>
<connect gate="A" pin="DGND" pad="49"/>
<connect gate="A" pin="DGND_2" pad="32"/>
<connect gate="A" pin="DR_GND" pad="23"/>
<connect gate="A" pin="DR_GND_2" pad="40"/>
<connect gate="A" pin="DR_GND_3" pad="31"/>
<connect gate="A" pin="DR_GND_4" pad="58"/>
<connect gate="A" pin="DR_GND_5" pad="50"/>
<connect gate="A" pin="MULTIPLEX" pad="11"/>
<connect gate="A" pin="PD" pad="59"/>
<connect gate="A" pin="VA" pad="63"/>
<connect gate="A" pin="VA_2" pad="18"/>
<connect gate="A" pin="VA_3" pad="62"/>
<connect gate="A" pin="VA_4" pad="9"/>
<connect gate="A" pin="VA_5" pad="19"/>
<connect gate="A" pin="VD" pad="48"/>
<connect gate="A" pin="VDR" pad="51"/>
<connect gate="A" pin="VDR_2" pad="30"/>
<connect gate="A" pin="VD_2" pad="33"/>
<connect gate="A" pin="VINB+" pad="2"/>
<connect gate="A" pin="VIN_A+" pad="15"/>
<connect gate="A" pin="VIN_A-" pad="16"/>
<connect gate="A" pin="VIN_B-" pad="1"/>
<connect gate="A" pin="VREF" pad="7"/>
<connect gate="A" pin="VRM_A" pad="14"/>
<connect gate="A" pin="VRM_B" pad="4"/>
<connect gate="A" pin="VRN_A" pad="12"/>
<connect gate="A" pin="VRN_B" pad="6"/>
<connect gate="A" pin="VRP_A" pad="13"/>
<connect gate="A" pin="VRP_B" pad="5"/>
<connect gate="A" pin="~OEA" pad="22"/>
<connect gate="A" pin="~OEB" pad="41"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="ADC12DL040CIVS"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K1560"/>
<attribute name="PACKAGE" value="QFP-64"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADC12DL065CIVS" prefix="U">
<description>Dual 12-Bit, 40 MSPS, 3V, 210mW A/D Converter</description>
<gates>
<gate name="A" symbol="ADC12DL065CIVS"/>
</gates>
<devices>
<device name="" package="QFP50P1200X1200X120-64N">
<connects>
<connect gate="A" pin="AGND" pad="61"/>
<connect gate="A" pin="AGND_2" pad="8"/>
<connect gate="A" pin="AGND_3" pad="3"/>
<connect gate="A" pin="AGND_4" pad="17"/>
<connect gate="A" pin="AGND_5" pad="20"/>
<connect gate="A" pin="AGND_6" pad="10"/>
<connect gate="A" pin="AGND_7" pad="64"/>
<connect gate="A" pin="CLK" pad="60"/>
<connect gate="A" pin="DA0" pad="24"/>
<connect gate="A" pin="DA1" pad="25"/>
<connect gate="A" pin="DA10" pad="38"/>
<connect gate="A" pin="DA11" pad="39"/>
<connect gate="A" pin="DA2" pad="26"/>
<connect gate="A" pin="DA3" pad="27"/>
<connect gate="A" pin="DA4" pad="28"/>
<connect gate="A" pin="DA5" pad="29"/>
<connect gate="A" pin="DA6" pad="34"/>
<connect gate="A" pin="DA7" pad="35"/>
<connect gate="A" pin="DA8" pad="36"/>
<connect gate="A" pin="DA9" pad="37"/>
<connect gate="A" pin="DB0/ABB" pad="42"/>
<connect gate="A" pin="DB1" pad="43"/>
<connect gate="A" pin="DB10" pad="56"/>
<connect gate="A" pin="DB11" pad="57"/>
<connect gate="A" pin="DB2" pad="44"/>
<connect gate="A" pin="DB3" pad="45"/>
<connect gate="A" pin="DB4" pad="46"/>
<connect gate="A" pin="DB5" pad="47"/>
<connect gate="A" pin="DB6" pad="52"/>
<connect gate="A" pin="DB7" pad="53"/>
<connect gate="A" pin="DB8" pad="54"/>
<connect gate="A" pin="DB9" pad="55"/>
<connect gate="A" pin="DF/DCS" pad="21"/>
<connect gate="A" pin="DGND" pad="49"/>
<connect gate="A" pin="DGND_2" pad="32"/>
<connect gate="A" pin="DR_GND" pad="23"/>
<connect gate="A" pin="DR_GND_2" pad="40"/>
<connect gate="A" pin="DR_GND_3" pad="31"/>
<connect gate="A" pin="DR_GND_4" pad="58"/>
<connect gate="A" pin="DR_GND_5" pad="50"/>
<connect gate="A" pin="MULTIPLEX" pad="11"/>
<connect gate="A" pin="PD" pad="59"/>
<connect gate="A" pin="VA" pad="63"/>
<connect gate="A" pin="VA_2" pad="18"/>
<connect gate="A" pin="VA_3" pad="62"/>
<connect gate="A" pin="VA_4" pad="9"/>
<connect gate="A" pin="VA_5" pad="19"/>
<connect gate="A" pin="VD" pad="48"/>
<connect gate="A" pin="VDR" pad="51"/>
<connect gate="A" pin="VDR_2" pad="30"/>
<connect gate="A" pin="VD_2" pad="33"/>
<connect gate="A" pin="VINB+" pad="2"/>
<connect gate="A" pin="VIN_A+" pad="15"/>
<connect gate="A" pin="VIN_A-" pad="16"/>
<connect gate="A" pin="VIN_B-" pad="1"/>
<connect gate="A" pin="VREF" pad="7"/>
<connect gate="A" pin="VRM_A" pad="14"/>
<connect gate="A" pin="VRM_B" pad="4"/>
<connect gate="A" pin="VRN_A" pad="12"/>
<connect gate="A" pin="VRN_B" pad="6"/>
<connect gate="A" pin="VRP_A" pad="13"/>
<connect gate="A" pin="VRP_B" pad="5"/>
<connect gate="A" pin="~OEA" pad="22"/>
<connect gate="A" pin="~OEB" pad="41"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="ADC12DL065CIVS"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="65K5035"/>
<attribute name="PACKAGE" value="QFP-64"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADC12DL066CIVS" prefix="U">
<description>Dual 12-Bit, 40 MSPS, 3V, 210mW A/D Converter</description>
<gates>
<gate name="A" symbol="ADC12DL066CIVS"/>
</gates>
<devices>
<device name="" package="QFP50P1200X1200X120-64N">
<connects>
<connect gate="A" pin="AGND" pad="61"/>
<connect gate="A" pin="AGND_2" pad="8"/>
<connect gate="A" pin="AGND_3" pad="3"/>
<connect gate="A" pin="AGND_4" pad="17"/>
<connect gate="A" pin="AGND_5" pad="20"/>
<connect gate="A" pin="AGND_6" pad="10"/>
<connect gate="A" pin="AGND_7" pad="64"/>
<connect gate="A" pin="CLK" pad="60"/>
<connect gate="A" pin="DA0" pad="24"/>
<connect gate="A" pin="DA1" pad="25"/>
<connect gate="A" pin="DA10" pad="38"/>
<connect gate="A" pin="DA11" pad="39"/>
<connect gate="A" pin="DA2" pad="26"/>
<connect gate="A" pin="DA3" pad="27"/>
<connect gate="A" pin="DA4" pad="28"/>
<connect gate="A" pin="DA5" pad="29"/>
<connect gate="A" pin="DA6" pad="34"/>
<connect gate="A" pin="DA7" pad="35"/>
<connect gate="A" pin="DA8" pad="36"/>
<connect gate="A" pin="DA9" pad="37"/>
<connect gate="A" pin="DB0/ABB" pad="42"/>
<connect gate="A" pin="DB1" pad="43"/>
<connect gate="A" pin="DB10" pad="56"/>
<connect gate="A" pin="DB11" pad="57"/>
<connect gate="A" pin="DB2" pad="44"/>
<connect gate="A" pin="DB3" pad="45"/>
<connect gate="A" pin="DB4" pad="46"/>
<connect gate="A" pin="DB5" pad="47"/>
<connect gate="A" pin="DB6" pad="52"/>
<connect gate="A" pin="DB7" pad="53"/>
<connect gate="A" pin="DB8" pad="54"/>
<connect gate="A" pin="DB9" pad="55"/>
<connect gate="A" pin="DGND" pad="49"/>
<connect gate="A" pin="DGND_2" pad="32"/>
<connect gate="A" pin="DR_GND" pad="23"/>
<connect gate="A" pin="DR_GND_2" pad="40"/>
<connect gate="A" pin="DR_GND_3" pad="31"/>
<connect gate="A" pin="DR_GND_4" pad="58"/>
<connect gate="A" pin="DR_GND_5" pad="50"/>
<connect gate="A" pin="OF" pad="21"/>
<connect gate="A" pin="PD" pad="59"/>
<connect gate="A" pin="VA" pad="63"/>
<connect gate="A" pin="VA_2" pad="18"/>
<connect gate="A" pin="VA_3" pad="62"/>
<connect gate="A" pin="VA_4" pad="9"/>
<connect gate="A" pin="VA_5" pad="19"/>
<connect gate="A" pin="VD" pad="48"/>
<connect gate="A" pin="VDR" pad="51"/>
<connect gate="A" pin="VDR_2" pad="30"/>
<connect gate="A" pin="VD_2" pad="33"/>
<connect gate="A" pin="VINB+" pad="2"/>
<connect gate="A" pin="VIN_A+" pad="15"/>
<connect gate="A" pin="VIN_A-" pad="16"/>
<connect gate="A" pin="VIN_B-" pad="1"/>
<connect gate="A" pin="VREF" pad="7"/>
<connect gate="A" pin="VRM_A" pad="14"/>
<connect gate="A" pin="VRM_B" pad="4"/>
<connect gate="A" pin="VRN_A" pad="12"/>
<connect gate="A" pin="VRN_B" pad="6"/>
<connect gate="A" pin="VRP_A" pad="13"/>
<connect gate="A" pin="VRP_B" pad="5"/>
<connect gate="A" pin="~INT/EXT_REF" pad="11"/>
<connect gate="A" pin="~OEA" pad="22"/>
<connect gate="A" pin="~OEB" pad="41"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="ADC12DL066CIVS"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K1561"/>
<attribute name="PACKAGE" value="QFP-64"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADC12DL080CIVS" prefix="U">
<description>A/D Converter</description>
<gates>
<gate name="A" symbol="ADC12DL080CIVS"/>
</gates>
<devices>
<device name="" package="QFP50P1200X1200X120-64N">
<connects>
<connect gate="A" pin="(LSB)DA0" pad="24"/>
<connect gate="A" pin="AGND" pad="8"/>
<connect gate="A" pin="AGND_2" pad="3"/>
<connect gate="A" pin="AGND_3" pad="17"/>
<connect gate="A" pin="AGND_4" pad="20"/>
<connect gate="A" pin="AGND_5" pad="10"/>
<connect gate="A" pin="AGND_6" pad="61"/>
<connect gate="A" pin="AGND_7" pad="64"/>
<connect gate="A" pin="CLK" pad="60"/>
<connect gate="A" pin="DA1" pad="25"/>
<connect gate="A" pin="DA10" pad="38"/>
<connect gate="A" pin="DA11(MSB)" pad="39"/>
<connect gate="A" pin="DA2" pad="26"/>
<connect gate="A" pin="DA3" pad="27"/>
<connect gate="A" pin="DA4" pad="28"/>
<connect gate="A" pin="DA5" pad="29"/>
<connect gate="A" pin="DA6" pad="34"/>
<connect gate="A" pin="DA7" pad="35"/>
<connect gate="A" pin="DA8" pad="36"/>
<connect gate="A" pin="DA9" pad="37"/>
<connect gate="A" pin="DB0(LSB)" pad="42"/>
<connect gate="A" pin="DB1" pad="43"/>
<connect gate="A" pin="DB10" pad="56"/>
<connect gate="A" pin="DB11(MSB)" pad="57"/>
<connect gate="A" pin="DB2" pad="44"/>
<connect gate="A" pin="DB3" pad="45"/>
<connect gate="A" pin="DB4" pad="46"/>
<connect gate="A" pin="DB5" pad="47"/>
<connect gate="A" pin="DB6" pad="52"/>
<connect gate="A" pin="DB7" pad="53"/>
<connect gate="A" pin="DB8" pad="54"/>
<connect gate="A" pin="DB9" pad="55"/>
<connect gate="A" pin="DGND" pad="49"/>
<connect gate="A" pin="DGND_2" pad="32"/>
<connect gate="A" pin="DRGND" pad="40"/>
<connect gate="A" pin="DRGND_2" pad="23"/>
<connect gate="A" pin="DRGND_3" pad="31"/>
<connect gate="A" pin="DRGND_4" pad="58"/>
<connect gate="A" pin="DRGND_5" pad="50"/>
<connect gate="A" pin="OF/DOEN" pad="21"/>
<connect gate="A" pin="PD" pad="59"/>
<connect gate="A" pin="REFSEL/DCS" pad="11"/>
<connect gate="A" pin="VA" pad="63"/>
<connect gate="A" pin="VA_2" pad="9"/>
<connect gate="A" pin="VA_3" pad="18"/>
<connect gate="A" pin="VA_4" pad="19"/>
<connect gate="A" pin="VA_5" pad="62"/>
<connect gate="A" pin="VD" pad="48"/>
<connect gate="A" pin="VDR" pad="30"/>
<connect gate="A" pin="VDR_2" pad="51"/>
<connect gate="A" pin="VD_2" pad="33"/>
<connect gate="A" pin="VINB+" pad="2"/>
<connect gate="A" pin="VIN_A+" pad="15"/>
<connect gate="A" pin="VIN_A-" pad="16"/>
<connect gate="A" pin="VIN_B-" pad="1"/>
<connect gate="A" pin="VREF" pad="7"/>
<connect gate="A" pin="VRM_A" pad="14"/>
<connect gate="A" pin="VRM_B" pad="4"/>
<connect gate="A" pin="VRN_A" pad="12"/>
<connect gate="A" pin="VRN_B" pad="6"/>
<connect gate="A" pin="VRP_A" pad="13"/>
<connect gate="A" pin="VRP_B" pad="5"/>
<connect gate="A" pin="~OEA/OF" pad="22"/>
<connect gate="A" pin="~OEB/DRDY" pad="41"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="ADC12DL080CIVS"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="79K5532"/>
<attribute name="PACKAGE" value="QFP-64"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADC12EU050CIPLQ" prefix="U">
<description>Analog-to-Digital Converter</description>
<gates>
<gate name="A" symbol="ADC12EU050CIPLQ"/>
</gates>
<devices>
<device name="" package="QFN50P1000X1000X100-69N">
<connects>
<connect gate="A" pin="AGND" pad="69"/>
<connect gate="A" pin="BCLK+" pad="36"/>
<connect gate="A" pin="BCLK-" pad="37"/>
<connect gate="A" pin="CLK+_(SE)" pad="47"/>
<connect gate="A" pin="CLK-" pad="48"/>
<connect gate="A" pin="DCAP" pad="6"/>
<connect gate="A" pin="DGND" pad="41"/>
<connect gate="A" pin="DGND_2" pad="13"/>
<connect gate="A" pin="DGND_3" pad="14"/>
<connect gate="A" pin="DGND_4" pad="22"/>
<connect gate="A" pin="DGND_5" pad="30"/>
<connect gate="A" pin="DGND_6" pad="40"/>
<connect gate="A" pin="DO0+" pad="15"/>
<connect gate="A" pin="DO0-" pad="16"/>
<connect gate="A" pin="DO1+" pad="18"/>
<connect gate="A" pin="DO1-" pad="19"/>
<connect gate="A" pin="DO2+" pad="20"/>
<connect gate="A" pin="DO2-" pad="21"/>
<connect gate="A" pin="DO3+" pad="23"/>
<connect gate="A" pin="DO3-" pad="24"/>
<connect gate="A" pin="DO4+" pad="25"/>
<connect gate="A" pin="DO4-" pad="26"/>
<connect gate="A" pin="DO5+" pad="28"/>
<connect gate="A" pin="DO5-" pad="29"/>
<connect gate="A" pin="DO6+" pad="31"/>
<connect gate="A" pin="DO6-" pad="32"/>
<connect gate="A" pin="DO7+" pad="33"/>
<connect gate="A" pin="DO7-" pad="34"/>
<connect gate="A" pin="RREF" pad="7"/>
<connect gate="A" pin="SCLK" pad="45"/>
<connect gate="A" pin="SDATA" pad="44"/>
<connect gate="A" pin="SLEEP" pad="10"/>
<connect gate="A" pin="VA" pad="66"/>
<connect gate="A" pin="VA_2" pad="1"/>
<connect gate="A" pin="VA_3" pad="8"/>
<connect gate="A" pin="VA_4" pad="51"/>
<connect gate="A" pin="VA_5" pad="54"/>
<connect gate="A" pin="VA_6" pad="57"/>
<connect gate="A" pin="VA_7" pad="60"/>
<connect gate="A" pin="VA_8" pad="63"/>
<connect gate="A" pin="VD" pad="43"/>
<connect gate="A" pin="VDR" pad="35"/>
<connect gate="A" pin="VDR_2" pad="17"/>
<connect gate="A" pin="VDR_3" pad="27"/>
<connect gate="A" pin="VD_2" pad="11"/>
<connect gate="A" pin="VD_3" pad="12"/>
<connect gate="A" pin="VD_4" pad="42"/>
<connect gate="A" pin="VIN0+" pad="2"/>
<connect gate="A" pin="VIN0-" pad="3"/>
<connect gate="A" pin="VIN1+" pad="67"/>
<connect gate="A" pin="VIN1-" pad="68"/>
<connect gate="A" pin="VIN2+" pad="64"/>
<connect gate="A" pin="VIN2-" pad="65"/>
<connect gate="A" pin="VIN3+" pad="61"/>
<connect gate="A" pin="VIN3-" pad="62"/>
<connect gate="A" pin="VIN4+" pad="58"/>
<connect gate="A" pin="VIN4-" pad="59"/>
<connect gate="A" pin="VIN5+" pad="55"/>
<connect gate="A" pin="VIN5-" pad="56"/>
<connect gate="A" pin="VIN6+" pad="52"/>
<connect gate="A" pin="VIN6-" pad="53"/>
<connect gate="A" pin="VIN7+" pad="49"/>
<connect gate="A" pin="VIN7-" pad="50"/>
<connect gate="A" pin="VREFB" pad="4"/>
<connect gate="A" pin="VREFT" pad="5"/>
<connect gate="A" pin="WCLK+" pad="38"/>
<connect gate="A" pin="WCLK-" pad="39"/>
<connect gate="A" pin="~RST" pad="9"/>
<connect gate="A" pin="~SSEL" pad="46"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="ADC12EU050CIPLQ"/>
<attribute name="OC_FARNELL" value="1689550"/>
<attribute name="OC_NEWARK" value="34P3006"/>
<attribute name="PACKAGE" value="LLP-68"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADC12L063CIVY" prefix="U">
<description>A/D Converter</description>
<gates>
<gate name="A" symbol="ADC12L063CIVY"/>
</gates>
<devices>
<device name="" package="QFP80P900X900X145-64N">
<connects>
<connect gate="A" pin="AGND" pad="28"/>
<connect gate="A" pin="AGND_2" pad="4"/>
<connect gate="A" pin="AGND_3" pad="7"/>
<connect gate="A" pin="CLK" pad="10"/>
<connect gate="A" pin="D0" pad="14"/>
<connect gate="A" pin="D1" pad="15"/>
<connect gate="A" pin="D10" pad="26"/>
<connect gate="A" pin="D11" pad="27"/>
<connect gate="A" pin="D2" pad="16"/>
<connect gate="A" pin="D3" pad="17"/>
<connect gate="A" pin="D4" pad="18"/>
<connect gate="A" pin="D5" pad="19"/>
<connect gate="A" pin="D6" pad="22"/>
<connect gate="A" pin="D7" pad="23"/>
<connect gate="A" pin="D8" pad="24"/>
<connect gate="A" pin="D9" pad="25"/>
<connect gate="A" pin="DGND" pad="12"/>
<connect gate="A" pin="DGND_2" pad="9"/>
<connect gate="A" pin="DR_GND" pad="20"/>
<connect gate="A" pin="PD" pad="8"/>
<connect gate="A" pin="VA" pad="6"/>
<connect gate="A" pin="VA_2" pad="5"/>
<connect gate="A" pin="VA_3" pad="29"/>
<connect gate="A" pin="VD" pad="13"/>
<connect gate="A" pin="VDR" pad="21"/>
<connect gate="A" pin="VIN+" pad="2"/>
<connect gate="A" pin="VIN-" pad="3"/>
<connect gate="A" pin="VREF" pad="1"/>
<connect gate="A" pin="VRM" pad="32"/>
<connect gate="A" pin="VRN" pad="30"/>
<connect gate="A" pin="VRP" pad="31"/>
<connect gate="A" pin="~OE" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="ADC12L063CIVY"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K1571"/>
<attribute name="PACKAGE" value="QFP-32"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADC12L066CIVY" prefix="U">
<description>12-Bit, 66 MSPS, 450 MHz Bandwidth A/D Converter</description>
<gates>
<gate name="A" symbol="ADC12L066CIVY"/>
</gates>
<devices>
<device name="" package="QFP80P900X900X160-32N">
<connects>
<connect gate="A" pin="AGND" pad="28"/>
<connect gate="A" pin="AGND_2" pad="4"/>
<connect gate="A" pin="AGND_3" pad="7"/>
<connect gate="A" pin="CLK" pad="10"/>
<connect gate="A" pin="D0" pad="14"/>
<connect gate="A" pin="D1" pad="15"/>
<connect gate="A" pin="D10" pad="26"/>
<connect gate="A" pin="D11" pad="27"/>
<connect gate="A" pin="D2" pad="16"/>
<connect gate="A" pin="D3" pad="17"/>
<connect gate="A" pin="D4" pad="18"/>
<connect gate="A" pin="D5" pad="19"/>
<connect gate="A" pin="D6" pad="22"/>
<connect gate="A" pin="D7" pad="23"/>
<connect gate="A" pin="D8" pad="24"/>
<connect gate="A" pin="D9" pad="25"/>
<connect gate="A" pin="DGND" pad="12"/>
<connect gate="A" pin="DGND_2" pad="9"/>
<connect gate="A" pin="DR_GND" pad="20"/>
<connect gate="A" pin="PD" pad="8"/>
<connect gate="A" pin="VA" pad="29"/>
<connect gate="A" pin="VA_2" pad="5"/>
<connect gate="A" pin="VA_3" pad="6"/>
<connect gate="A" pin="VD" pad="13"/>
<connect gate="A" pin="VDR" pad="21"/>
<connect gate="A" pin="VIN+" pad="2"/>
<connect gate="A" pin="VIN-" pad="3"/>
<connect gate="A" pin="VREF" pad="1"/>
<connect gate="A" pin="VRM" pad="32"/>
<connect gate="A" pin="VRN" pad="30"/>
<connect gate="A" pin="VRP" pad="31"/>
<connect gate="A" pin="~OE" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="ADC12L066CIVY"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K1572"/>
<attribute name="PACKAGE" value="QFP-32"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADC12L080CIVY" prefix="U">
<description>12-Bit, 80 MSPS, 450 MHz Bandwidth A/D Converter</description>
<gates>
<gate name="A" symbol="ADC12L080CIVY"/>
</gates>
<devices>
<device name="" package="QFP80P900X900X160-32N">
<connects>
<connect gate="A" pin="AGND" pad="28"/>
<connect gate="A" pin="AGND_2" pad="4"/>
<connect gate="A" pin="AGND_3" pad="7"/>
<connect gate="A" pin="CLK" pad="10"/>
<connect gate="A" pin="D0" pad="14"/>
<connect gate="A" pin="D1" pad="15"/>
<connect gate="A" pin="D10" pad="26"/>
<connect gate="A" pin="D11" pad="27"/>
<connect gate="A" pin="D2" pad="16"/>
<connect gate="A" pin="D3" pad="17"/>
<connect gate="A" pin="D4" pad="18"/>
<connect gate="A" pin="D5" pad="19"/>
<connect gate="A" pin="D6" pad="22"/>
<connect gate="A" pin="D7" pad="23"/>
<connect gate="A" pin="D8" pad="24"/>
<connect gate="A" pin="D9" pad="25"/>
<connect gate="A" pin="DGND" pad="12"/>
<connect gate="A" pin="DGND_2" pad="9"/>
<connect gate="A" pin="DR_GND" pad="20"/>
<connect gate="A" pin="OF" pad="11"/>
<connect gate="A" pin="PD" pad="8"/>
<connect gate="A" pin="VA" pad="6"/>
<connect gate="A" pin="VA_2" pad="5"/>
<connect gate="A" pin="VA_3" pad="29"/>
<connect gate="A" pin="VD" pad="13"/>
<connect gate="A" pin="VDR" pad="21"/>
<connect gate="A" pin="VIN+" pad="2"/>
<connect gate="A" pin="VIN-" pad="3"/>
<connect gate="A" pin="VREF" pad="1"/>
<connect gate="A" pin="VRM" pad="32"/>
<connect gate="A" pin="VRN" pad="30"/>
<connect gate="A" pin="VRP" pad="31"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="ADC12L080CIVY"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K1574"/>
<attribute name="PACKAGE" value="LQFP-32"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADC14155CISQ" prefix="U">
<description>A/D converters</description>
<gates>
<gate name="A" symbol="ADC14155CISQ"/>
</gates>
<devices>
<device name="" package="QFN50P700X700X80-49N">
<connects>
<connect gate="A" pin="(LSB)D0" pad="17"/>
<connect gate="A" pin="AGND" pad="2"/>
<connect gate="A" pin="AGND_2" pad="5"/>
<connect gate="A" pin="AGND_3" pad="38"/>
<connect gate="A" pin="AGND_4" pad="10"/>
<connect gate="A" pin="AGND_5" pad="42"/>
<connect gate="A" pin="AGND_6" pad="39"/>
<connect gate="A" pin="AGND_7" pad="47"/>
<connect gate="A" pin="CLK+" pad="11"/>
<connect gate="A" pin="CLK-" pad="12"/>
<connect gate="A" pin="CLK_SEL/DF" pad="8"/>
<connect gate="A" pin="D1" pad="18"/>
<connect gate="A" pin="D10" pad="29"/>
<connect gate="A" pin="D11" pad="30"/>
<connect gate="A" pin="D12" pad="31"/>
<connect gate="A" pin="D13(MSB)" pad="32"/>
<connect gate="A" pin="D2" pad="19"/>
<connect gate="A" pin="D3" pad="20"/>
<connect gate="A" pin="D4" pad="21"/>
<connect gate="A" pin="D5" pad="22"/>
<connect gate="A" pin="D6" pad="23"/>
<connect gate="A" pin="D7" pad="24"/>
<connect gate="A" pin="D8" pad="27"/>
<connect gate="A" pin="D9" pad="28"/>
<connect gate="A" pin="DGND" pad="14"/>
<connect gate="A" pin="DRDY" pad="34"/>
<connect gate="A" pin="DRGND" pad="35"/>
<connect gate="A" pin="DRGND_2" pad="26"/>
<connect gate="A" pin="DRGND_3" pad="16"/>
<connect gate="A" pin="OVR" pad="33"/>
<connect gate="A" pin="PD" pad="7"/>
<connect gate="A" pin="VA" pad="48"/>
<connect gate="A" pin="VA_2" pad="1"/>
<connect gate="A" pin="VA_3" pad="9"/>
<connect gate="A" pin="VA_4" pad="6"/>
<connect gate="A" pin="VA_5" pad="40"/>
<connect gate="A" pin="VA_6" pad="37"/>
<connect gate="A" pin="VA_7" pad="41"/>
<connect gate="A" pin="VD" pad="13"/>
<connect gate="A" pin="VDR" pad="36"/>
<connect gate="A" pin="VDR_2" pad="15"/>
<connect gate="A" pin="VDR_3" pad="25"/>
<connect gate="A" pin="VIN+" pad="4"/>
<connect gate="A" pin="VIN-" pad="3"/>
<connect gate="A" pin="VREF" pad="46"/>
<connect gate="A" pin="VRM" pad="45"/>
<connect gate="A" pin="VRN" pad="44"/>
<connect gate="A" pin="VRP" pad="43"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="ADC14155CISQ"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="12M7685"/>
<attribute name="PACKAGE" value="LCC-48"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADC14C080CISQ" prefix="U">
<description>14-Bit, 65/80 MSPS A/D Converter</description>
<gates>
<gate name="A" symbol="ADC14C080CISQ"/>
</gates>
<devices>
<device name="" package="QFN50P500X500X80-33N">
<connects>
<connect gate="A" pin="AGND" pad="9"/>
<connect gate="A" pin="AGND_2" pad="4"/>
<connect gate="A" pin="AGND_3" pad="7"/>
<connect gate="A" pin="CLK" pad="11"/>
<connect gate="A" pin="D0" pad="13"/>
<connect gate="A" pin="D1" pad="14"/>
<connect gate="A" pin="D10" pad="26"/>
<connect gate="A" pin="D11" pad="27"/>
<connect gate="A" pin="D12" pad="28"/>
<connect gate="A" pin="D13(MSB)" pad="29"/>
<connect gate="A" pin="D2" pad="15"/>
<connect gate="A" pin="D3" pad="16"/>
<connect gate="A" pin="D4" pad="17"/>
<connect gate="A" pin="D5" pad="18"/>
<connect gate="A" pin="D6" pad="19"/>
<connect gate="A" pin="D7" pad="23"/>
<connect gate="A" pin="D8" pad="24"/>
<connect gate="A" pin="D9" pad="25"/>
<connect gate="A" pin="DRDY" pad="21"/>
<connect gate="A" pin="DRGND" pad="22"/>
<connect gate="A" pin="EPAD" pad="33"/>
<connect gate="A" pin="OF/DCS" pad="12"/>
<connect gate="A" pin="PD" pad="30"/>
<connect gate="A" pin="VA" pad="3"/>
<connect gate="A" pin="VA_2" pad="8"/>
<connect gate="A" pin="VA_3" pad="10"/>
<connect gate="A" pin="VCMO" pad="32"/>
<connect gate="A" pin="VDR" pad="20"/>
<connect gate="A" pin="VIN+" pad="5"/>
<connect gate="A" pin="VIN-" pad="6"/>
<connect gate="A" pin="VREF" pad="31"/>
<connect gate="A" pin="VRN" pad="1"/>
<connect gate="A" pin="VRP" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="ADC14C080CISQ"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="55M4611"/>
<attribute name="PACKAGE" value="QFN-32"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADC14C105CISQ" prefix="U">
<description>14-Bit, 95/105 MSPS A/D Converter</description>
<gates>
<gate name="A" symbol="ADC14C105CISQ"/>
</gates>
<devices>
<device name="" package="QFN50P500X500X80-33N">
<connects>
<connect gate="A" pin="AGND" pad="9"/>
<connect gate="A" pin="AGND_2" pad="4"/>
<connect gate="A" pin="AGND_3" pad="7"/>
<connect gate="A" pin="CLK" pad="11"/>
<connect gate="A" pin="D0" pad="13"/>
<connect gate="A" pin="D1" pad="14"/>
<connect gate="A" pin="D10" pad="26"/>
<connect gate="A" pin="D11" pad="27"/>
<connect gate="A" pin="D12" pad="28"/>
<connect gate="A" pin="D13(MSB)" pad="29"/>
<connect gate="A" pin="D2" pad="15"/>
<connect gate="A" pin="D3" pad="16"/>
<connect gate="A" pin="D4" pad="17"/>
<connect gate="A" pin="D5" pad="18"/>
<connect gate="A" pin="D6" pad="19"/>
<connect gate="A" pin="D7" pad="23"/>
<connect gate="A" pin="D8" pad="24"/>
<connect gate="A" pin="D9" pad="25"/>
<connect gate="A" pin="DRDY" pad="21"/>
<connect gate="A" pin="DRGND" pad="22"/>
<connect gate="A" pin="EPAD" pad="33"/>
<connect gate="A" pin="OF/DCS" pad="12"/>
<connect gate="A" pin="PD" pad="30"/>
<connect gate="A" pin="VA" pad="3"/>
<connect gate="A" pin="VA_2" pad="8"/>
<connect gate="A" pin="VA_3" pad="10"/>
<connect gate="A" pin="VCMO" pad="32"/>
<connect gate="A" pin="VDR" pad="20"/>
<connect gate="A" pin="VIN+" pad="5"/>
<connect gate="A" pin="VIN-" pad="6"/>
<connect gate="A" pin="VREF" pad="31"/>
<connect gate="A" pin="VRN" pad="1"/>
<connect gate="A" pin="VRP" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="ADC14C105CISQ"/>
<attribute name="OC_FARNELL" value="1433178"/>
<attribute name="OC_NEWARK" value="60M5663"/>
<attribute name="PACKAGE" value="QFN-32"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADC14DS080CISQ" prefix="U">
<description>Dual 14-Bit, 80 MSPS A/D Converter</description>
<gates>
<gate name="A" symbol="ADC14DS080CISQ"/>
</gates>
<devices>
<device name="" package="QFN50P900X900X80-61N">
<connects>
<connect gate="A" pin="AGND" pad="12"/>
<connect gate="A" pin="AGND_2" pad="1"/>
<connect gate="A" pin="AGND_3" pad="15"/>
<connect gate="A" pin="AGND_4" pad="4"/>
<connect gate="A" pin="CLK" pad="18"/>
<connect gate="A" pin="DLC" pad="48"/>
<connect gate="A" pin="DLL_LOCK" pad="24"/>
<connect gate="A" pin="DRGND" pad="51"/>
<connect gate="A" pin="DRGND_2" pad="25"/>
<connect gate="A" pin="DRGND_3" pad="39"/>
<connect gate="A" pin="EPAD" pad="61"/>
<connect gate="A" pin="FRAME+" pad="43"/>
<connect gate="A" pin="FRAME-" pad="42"/>
<connect gate="A" pin="LVDS_BIAS" pad="29"/>
<connect gate="A" pin="N/C" pad="23"/>
<connect gate="A" pin="N/C_2" pad="21"/>
<connect gate="A" pin="N/C_3" pad="22"/>
<connect gate="A" pin="N/C_4" pad="41"/>
<connect gate="A" pin="OF/DCS" pad="19"/>
<connect gate="A" pin="ORA" pad="46"/>
<connect gate="A" pin="ORB" pad="30"/>
<connect gate="A" pin="OUTCLK+" pad="45"/>
<connect gate="A" pin="OUTCLK-" pad="44"/>
<connect gate="A" pin="PD_A" pad="57"/>
<connect gate="A" pin="PD_B" pad="20"/>
<connect gate="A" pin="RESET_DLL" pad="28"/>
<connect gate="A" pin="SCLK" pad="52"/>
<connect gate="A" pin="SCSB" pad="55"/>
<connect gate="A" pin="SD0_A+" pad="36"/>
<connect gate="A" pin="SD0_A-" pad="35"/>
<connect gate="A" pin="SD0_B+" pad="32"/>
<connect gate="A" pin="SD0_B-" pad="31"/>
<connect gate="A" pin="SD1_A+" pad="38"/>
<connect gate="A" pin="SD1_A-" pad="37"/>
<connect gate="A" pin="SD1_B+" pad="34"/>
<connect gate="A" pin="SD1_B-" pad="33"/>
<connect gate="A" pin="SDI" pad="54"/>
<connect gate="A" pin="SDO" pad="53"/>
<connect gate="A" pin="SPI_EN" pad="56"/>
<connect gate="A" pin="TEST" pad="27"/>
<connect gate="A" pin="VA" pad="17"/>
<connect gate="A" pin="VA_2" pad="16"/>
<connect gate="A" pin="VA_3" pad="58"/>
<connect gate="A" pin="VA_4" pad="8"/>
<connect gate="A" pin="VA_5" pad="60"/>
<connect gate="A" pin="VCMOA" pad="7"/>
<connect gate="A" pin="VCMOB" pad="9"/>
<connect gate="A" pin="VDR" pad="50"/>
<connect gate="A" pin="VDR_2" pad="26"/>
<connect gate="A" pin="VDR_3" pad="40"/>
<connect gate="A" pin="VDR_4" pad="49"/>
<connect gate="A" pin="VINA+" pad="3"/>
<connect gate="A" pin="VINA-" pad="2"/>
<connect gate="A" pin="VINB+" pad="13"/>
<connect gate="A" pin="VINB-" pad="14"/>
<connect gate="A" pin="VREF" pad="59"/>
<connect gate="A" pin="VRNA" pad="6"/>
<connect gate="A" pin="VRNB" pad="10"/>
<connect gate="A" pin="VRPA" pad="5"/>
<connect gate="A" pin="VRPB" pad="11"/>
<connect gate="A" pin="WAM" pad="47"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="ADC14DS080CISQ"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="75M6025"/>
<attribute name="PACKAGE" value="QFN-64"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADC14DS105CISQ" prefix="U">
<description>Dual 14-Bit, 80 MSPS A/D Converter</description>
<gates>
<gate name="A" symbol="ADC14DS105CISQ"/>
</gates>
<devices>
<device name="" package="QFN50P900X900X80-61N">
<connects>
<connect gate="A" pin="AGND" pad="12"/>
<connect gate="A" pin="AGND_2" pad="1"/>
<connect gate="A" pin="AGND_3" pad="15"/>
<connect gate="A" pin="AGND_4" pad="4"/>
<connect gate="A" pin="CLK" pad="18"/>
<connect gate="A" pin="DLC" pad="48"/>
<connect gate="A" pin="DLL_LOCK" pad="24"/>
<connect gate="A" pin="DRGND" pad="51"/>
<connect gate="A" pin="DRGND_2" pad="25"/>
<connect gate="A" pin="DRGND_3" pad="39"/>
<connect gate="A" pin="EPAD" pad="61"/>
<connect gate="A" pin="FRAME+" pad="43"/>
<connect gate="A" pin="FRAME-" pad="42"/>
<connect gate="A" pin="LVDS_BIAS" pad="29"/>
<connect gate="A" pin="N/C" pad="23"/>
<connect gate="A" pin="N/C_2" pad="21"/>
<connect gate="A" pin="N/C_3" pad="22"/>
<connect gate="A" pin="N/C_4" pad="41"/>
<connect gate="A" pin="OF/DCS" pad="19"/>
<connect gate="A" pin="ORA" pad="46"/>
<connect gate="A" pin="ORB" pad="30"/>
<connect gate="A" pin="OUTCLK+" pad="45"/>
<connect gate="A" pin="OUTCLK-" pad="44"/>
<connect gate="A" pin="PD_A" pad="57"/>
<connect gate="A" pin="PD_B" pad="20"/>
<connect gate="A" pin="RESET_DLL" pad="28"/>
<connect gate="A" pin="SCLK" pad="52"/>
<connect gate="A" pin="SCSB" pad="55"/>
<connect gate="A" pin="SD0_A+" pad="36"/>
<connect gate="A" pin="SD0_A-" pad="35"/>
<connect gate="A" pin="SD0_B+" pad="32"/>
<connect gate="A" pin="SD0_B-" pad="31"/>
<connect gate="A" pin="SD1_A+" pad="38"/>
<connect gate="A" pin="SD1_A-" pad="37"/>
<connect gate="A" pin="SD1_B+" pad="34"/>
<connect gate="A" pin="SD1_B-" pad="33"/>
<connect gate="A" pin="SDI" pad="54"/>
<connect gate="A" pin="SDO" pad="53"/>
<connect gate="A" pin="SPI_EN" pad="56"/>
<connect gate="A" pin="TEST" pad="27"/>
<connect gate="A" pin="VA" pad="17"/>
<connect gate="A" pin="VA_2" pad="16"/>
<connect gate="A" pin="VA_3" pad="58"/>
<connect gate="A" pin="VA_4" pad="8"/>
<connect gate="A" pin="VA_5" pad="60"/>
<connect gate="A" pin="VCMOA" pad="7"/>
<connect gate="A" pin="VCMOB" pad="9"/>
<connect gate="A" pin="VDR" pad="50"/>
<connect gate="A" pin="VDR_2" pad="26"/>
<connect gate="A" pin="VDR_3" pad="40"/>
<connect gate="A" pin="VDR_4" pad="49"/>
<connect gate="A" pin="VINA+" pad="3"/>
<connect gate="A" pin="VINA-" pad="2"/>
<connect gate="A" pin="VINB+" pad="13"/>
<connect gate="A" pin="VINB-" pad="14"/>
<connect gate="A" pin="VREF" pad="59"/>
<connect gate="A" pin="VRNA" pad="6"/>
<connect gate="A" pin="VRNB" pad="10"/>
<connect gate="A" pin="VRPA" pad="5"/>
<connect gate="A" pin="VRPB" pad="11"/>
<connect gate="A" pin="WAM" pad="47"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="ADC14DS105CISQ"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="64M6815"/>
<attribute name="PACKAGE" value="QFN-64"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADC14L020CIVY" prefix="U">
<description>A/D Converter</description>
<gates>
<gate name="A" symbol="ADC14L020CIVY"/>
</gates>
<devices>
<device name="" package="QFP80P900X900X160-32N">
<connects>
<connect gate="A" pin="(LSB)D0" pad="12"/>
<connect gate="A" pin="AGND" pad="28"/>
<connect gate="A" pin="AGND_2" pad="4"/>
<connect gate="A" pin="AGND_3" pad="7"/>
<connect gate="A" pin="CLK" pad="10"/>
<connect gate="A" pin="D1" pad="13"/>
<connect gate="A" pin="D10" pad="24"/>
<connect gate="A" pin="D11" pad="25"/>
<connect gate="A" pin="D12" pad="26"/>
<connect gate="A" pin="D13" pad="27"/>
<connect gate="A" pin="D2" pad="14"/>
<connect gate="A" pin="D3" pad="15"/>
<connect gate="A" pin="D4" pad="16"/>
<connect gate="A" pin="D5" pad="17"/>
<connect gate="A" pin="D6" pad="18"/>
<connect gate="A" pin="D7" pad="19"/>
<connect gate="A" pin="D8" pad="22"/>
<connect gate="A" pin="D9" pad="23"/>
<connect gate="A" pin="DF/DCS" pad="11"/>
<connect gate="A" pin="DGND" pad="9"/>
<connect gate="A" pin="DRGND" pad="20"/>
<connect gate="A" pin="PD" pad="8"/>
<connect gate="A" pin="VA" pad="29"/>
<connect gate="A" pin="VA_2" pad="5"/>
<connect gate="A" pin="VD" pad="6"/>
<connect gate="A" pin="VDR" pad="21"/>
<connect gate="A" pin="VIN+" pad="2"/>
<connect gate="A" pin="VIN-" pad="3"/>
<connect gate="A" pin="VREF" pad="1"/>
<connect gate="A" pin="VRM" pad="32"/>
<connect gate="A" pin="VRN" pad="30"/>
<connect gate="A" pin="VRP" pad="31"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="ADC14L020CIVY"/>
<attribute name="OC_FARNELL" value="1554775"/>
<attribute name="OC_NEWARK" value="94M6085"/>
<attribute name="PACKAGE" value="QFP-32"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADC14L040CIVY" prefix="U">
<description>A/D Converter</description>
<gates>
<gate name="A" symbol="ADC14L040CIVY"/>
</gates>
<devices>
<device name="" package="QFP80P900X900X160-32N">
<connects>
<connect gate="A" pin="(LSB)D0" pad="12"/>
<connect gate="A" pin="AGND" pad="28"/>
<connect gate="A" pin="AGND_2" pad="4"/>
<connect gate="A" pin="AGND_3" pad="7"/>
<connect gate="A" pin="CLK" pad="10"/>
<connect gate="A" pin="D1" pad="13"/>
<connect gate="A" pin="D10" pad="24"/>
<connect gate="A" pin="D11" pad="25"/>
<connect gate="A" pin="D12" pad="26"/>
<connect gate="A" pin="D13" pad="27"/>
<connect gate="A" pin="D2" pad="14"/>
<connect gate="A" pin="D3" pad="15"/>
<connect gate="A" pin="D4" pad="16"/>
<connect gate="A" pin="D5" pad="17"/>
<connect gate="A" pin="D6" pad="18"/>
<connect gate="A" pin="D7" pad="19"/>
<connect gate="A" pin="D8" pad="22"/>
<connect gate="A" pin="D9" pad="23"/>
<connect gate="A" pin="DF/DCS" pad="11"/>
<connect gate="A" pin="DGND" pad="9"/>
<connect gate="A" pin="DRGND" pad="20"/>
<connect gate="A" pin="PD" pad="8"/>
<connect gate="A" pin="VA" pad="29"/>
<connect gate="A" pin="VA_2" pad="5"/>
<connect gate="A" pin="VD" pad="6"/>
<connect gate="A" pin="VDR" pad="21"/>
<connect gate="A" pin="VIN+" pad="2"/>
<connect gate="A" pin="VIN-" pad="3"/>
<connect gate="A" pin="VREF" pad="1"/>
<connect gate="A" pin="VRM" pad="32"/>
<connect gate="A" pin="VRN" pad="30"/>
<connect gate="A" pin="VRP" pad="31"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="ADC14L040CIVY"/>
<attribute name="OC_FARNELL" value="1554776"/>
<attribute name="OC_NEWARK" value="65K5038"/>
<attribute name="PACKAGE" value="QFP-32"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADC16V130CISQ" prefix="U">
<description>A/D Converter</description>
<gates>
<gate name="A" symbol="ADC16V130CISQ"/>
</gates>
<devices>
<device name="" package="QFN50P900X900X80-65N">
<connects>
<connect gate="A" pin="AGND" pad="12"/>
<connect gate="A" pin="AGND_2" pad="3"/>
<connect gate="A" pin="AGND_3" pad="56"/>
<connect gate="A" pin="AGND_4" pad="8"/>
<connect gate="A" pin="AGND_5" pad="63"/>
<connect gate="A" pin="AGND_6" pad="60"/>
<connect gate="A" pin="AGND_7" pad="65"/>
<connect gate="A" pin="CLK+" pad="10"/>
<connect gate="A" pin="CLK-" pad="11"/>
<connect gate="A" pin="CLK_SEL/DF" pad="1"/>
<connect gate="A" pin="D0+" pad="16"/>
<connect gate="A" pin="D0-" pad="15"/>
<connect gate="A" pin="D1+" pad="18"/>
<connect gate="A" pin="D1-" pad="17"/>
<connect gate="A" pin="D10+" pad="40"/>
<connect gate="A" pin="D10-" pad="39"/>
<connect gate="A" pin="D11+" pad="42"/>
<connect gate="A" pin="D11-" pad="41"/>
<connect gate="A" pin="D12+" pad="46"/>
<connect gate="A" pin="D12-" pad="45"/>
<connect gate="A" pin="D13+" pad="48"/>
<connect gate="A" pin="D13-" pad="47"/>
<connect gate="A" pin="D14+" pad="50"/>
<connect gate="A" pin="D14-" pad="49"/>
<connect gate="A" pin="D15+" pad="52"/>
<connect gate="A" pin="D15-" pad="51"/>
<connect gate="A" pin="D2+" pad="20"/>
<connect gate="A" pin="D2-" pad="19"/>
<connect gate="A" pin="D3+" pad="22"/>
<connect gate="A" pin="D3-" pad="21"/>
<connect gate="A" pin="D4+" pad="26"/>
<connect gate="A" pin="D4-" pad="25"/>
<connect gate="A" pin="D5+" pad="28"/>
<connect gate="A" pin="D5-" pad="27"/>
<connect gate="A" pin="D6+" pad="30"/>
<connect gate="A" pin="D6-" pad="29"/>
<connect gate="A" pin="D7+" pad="32"/>
<connect gate="A" pin="D7-" pad="31"/>
<connect gate="A" pin="D8+" pad="36"/>
<connect gate="A" pin="D8-" pad="35"/>
<connect gate="A" pin="D9+" pad="38"/>
<connect gate="A" pin="D9-" pad="37"/>
<connect gate="A" pin="DRGND" pad="43"/>
<connect gate="A" pin="DRGND_2" pad="23"/>
<connect gate="A" pin="OR+" pad="54"/>
<connect gate="A" pin="OR-" pad="53"/>
<connect gate="A" pin="OUTCLK+" pad="34"/>
<connect gate="A" pin="OUTCLK-" pad="33"/>
<connect gate="A" pin="PD" pad="14"/>
<connect gate="A" pin="VA1.8" pad="64"/>
<connect gate="A" pin="VA1.8_2" pad="9"/>
<connect gate="A" pin="VA3.0" pad="59"/>
<connect gate="A" pin="VA3.0_2" pad="2"/>
<connect gate="A" pin="VA3.0_3" pad="55"/>
<connect gate="A" pin="VAD1.8" pad="13"/>
<connect gate="A" pin="VDR" pad="44"/>
<connect gate="A" pin="VDR_2" pad="24"/>
<connect gate="A" pin="VIN+" pad="61"/>
<connect gate="A" pin="VIN-" pad="62"/>
<connect gate="A" pin="VREF" pad="57"/>
<connect gate="A" pin="VRM" pad="58"/>
<connect gate="A" pin="VRN" pad="5"/>
<connect gate="A" pin="VRN_2" pad="4"/>
<connect gate="A" pin="VRP" pad="7"/>
<connect gate="A" pin="VRP_2" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="ADC16V130CISQ"/>
<attribute name="OC_FARNELL" value="1689553"/>
<attribute name="OC_NEWARK" value="45P3256"/>
<attribute name="PACKAGE" value="LLP-64"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADC78H89CIMT" prefix="U">
<description>12-Bit A/D Converter</description>
<gates>
<gate name="A" symbol="ADC78H89CIMT"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-16N">
<connects>
<connect gate="A" pin="AGND" pad="4"/>
<connect gate="A" pin="AIN1" pad="5"/>
<connect gate="A" pin="AIN2" pad="6"/>
<connect gate="A" pin="AIN3" pad="7"/>
<connect gate="A" pin="AIN4" pad="8"/>
<connect gate="A" pin="AIN5" pad="9"/>
<connect gate="A" pin="AIN6" pad="10"/>
<connect gate="A" pin="AIN7" pad="11"/>
<connect gate="A" pin="AIN8" pad="2"/>
<connect gate="A" pin="AVDD" pad="3"/>
<connect gate="A" pin="DGND" pad="12"/>
<connect gate="A" pin="DIN" pad="15"/>
<connect gate="A" pin="DOUT" pad="13"/>
<connect gate="A" pin="DVDD" pad="14"/>
<connect gate="A" pin="SCLK" pad="16"/>
<connect gate="A" pin="~CS" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="ADC78H89CIMT"/>
<attribute name="OC_FARNELL" value="9779752"/>
<attribute name="OC_NEWARK" value="96K6197"/>
<attribute name="PACKAGE" value="SOP-16"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADC78H90CIMT" prefix="U">
<description>12-Bit A/D Converter</description>
<gates>
<gate name="A" symbol="ADC78H90CIMT"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-16N">
<connects>
<connect gate="A" pin="AGND" pad="3"/>
<connect gate="A" pin="AIN1" pad="4"/>
<connect gate="A" pin="AIN2" pad="5"/>
<connect gate="A" pin="AIN3" pad="6"/>
<connect gate="A" pin="AIN4" pad="7"/>
<connect gate="A" pin="AIN5" pad="8"/>
<connect gate="A" pin="AIN6" pad="9"/>
<connect gate="A" pin="AIN7" pad="10"/>
<connect gate="A" pin="AIN8" pad="11"/>
<connect gate="A" pin="AVDD" pad="2"/>
<connect gate="A" pin="DGND" pad="12"/>
<connect gate="A" pin="DIN" pad="14"/>
<connect gate="A" pin="DOUT" pad="15"/>
<connect gate="A" pin="DVDD" pad="13"/>
<connect gate="A" pin="SCLK" pad="16"/>
<connect gate="A" pin="~CS" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="ADC78H90CIMT"/>
<attribute name="OC_FARNELL" value="9779744"/>
<attribute name="OC_NEWARK" value="41K1613"/>
<attribute name="PACKAGE" value="SOP-16"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CLC001AJE-TR13" prefix="U">
<description>Cable Driver</description>
<gates>
<gate name="A" symbol="CLC001AJE-TR13"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="RREF" pad="4"/>
<connect gate="A" pin="SDO" pad="6"/>
<connect gate="A" pin="VBB" pad="1"/>
<connect gate="A" pin="VDD" pad="8"/>
<connect gate="A" pin="VIN+" pad="2"/>
<connect gate="A" pin="VIN-" pad="3"/>
<connect gate="A" pin="VSS" pad="5"/>
<connect gate="A" pin="~SDO" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="CLC001AJE-TR13"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K1615"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CLC001AJE" prefix="U">
<description>Digital Cable Driver</description>
<gates>
<gate name="A" symbol="CLC001AJE"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="RREF" pad="4"/>
<connect gate="A" pin="SDO" pad="6"/>
<connect gate="A" pin="VBB" pad="1"/>
<connect gate="A" pin="VDD" pad="8"/>
<connect gate="A" pin="VIN+" pad="2"/>
<connect gate="A" pin="VIN-" pad="3"/>
<connect gate="A" pin="VSS" pad="5"/>
<connect gate="A" pin="~SDO" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="CLC001AJE"/>
<attribute name="OC_FARNELL" value="1286813"/>
<attribute name="OC_NEWARK" value="34C6383"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CLC020BCQ" prefix="U">
<description>Integrated cable Driver</description>
<gates>
<gate name="A" symbol="CLC020BCQ"/>
</gates>
<devices>
<device name="" package="PLCC127P1245X1245X457-28N">
<connects>
<connect gate="A" pin="D0" pad="3"/>
<connect gate="A" pin="D1" pad="4"/>
<connect gate="A" pin="D2" pad="5"/>
<connect gate="A" pin="D3" pad="6"/>
<connect gate="A" pin="D4" pad="7"/>
<connect gate="A" pin="D5" pad="8"/>
<connect gate="A" pin="D6" pad="9"/>
<connect gate="A" pin="D7" pad="10"/>
<connect gate="A" pin="D8" pad="11"/>
<connect gate="A" pin="D9" pad="12"/>
<connect gate="A" pin="LOCK_DETECT" pad="14"/>
<connect gate="A" pin="PCLK" pad="13"/>
<connect gate="A" pin="RREF" pad="19"/>
<connect gate="A" pin="SDO" pad="22"/>
<connect gate="A" pin="TEST_OUT" pad="26"/>
<connect gate="A" pin="TPG_EN" pad="17"/>
<connect gate="A" pin="VDD" pad="2"/>
<connect gate="A" pin="VDDO" pad="16"/>
<connect gate="A" pin="VDDOD" pad="20"/>
<connect gate="A" pin="VDDSD" pad="24"/>
<connect gate="A" pin="VDD_2" pad="1"/>
<connect gate="A" pin="VSS" pad="28"/>
<connect gate="A" pin="VSSO" pad="15"/>
<connect gate="A" pin="VSSOD" pad="18"/>
<connect gate="A" pin="VSSSD" pad="21"/>
<connect gate="A" pin="VSS_2" pad="27"/>
<connect gate="A" pin="~SDO" pad="23"/>
<connect gate="A" pin="~SYNC_DET_EN" pad="25"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="CLC020BCQ"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K1634"/>
<attribute name="PACKAGE" value="PLCC-28"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CLC021AVGZ-3.3" prefix="U">
<description>Digital Video Serializer</description>
<gates>
<gate name="A" symbol="CLC021AVGZ-3.3"/>
</gates>
<devices>
<device name="" package="QFP80P1320X1320X245-44N">
<connects>
<connect gate="A" pin="ANC" pad="43"/>
<connect gate="A" pin="D0" pad="12"/>
<connect gate="A" pin="D1" pad="13"/>
<connect gate="A" pin="D2" pad="14"/>
<connect gate="A" pin="D3" pad="15"/>
<connect gate="A" pin="D4" pad="16"/>
<connect gate="A" pin="D5" pad="17"/>
<connect gate="A" pin="D6" pad="18"/>
<connect gate="A" pin="D7" pad="19"/>
<connect gate="A" pin="D8" pad="20"/>
<connect gate="A" pin="D9" pad="21"/>
<connect gate="A" pin="EDH_FORCE" pad="8"/>
<connect gate="A" pin="F/LFB2" pad="25"/>
<connect gate="A" pin="H/LFB0" pad="23"/>
<connect gate="A" pin="LOCK_DET" pad="26"/>
<connect gate="A" pin="N/C" pad="34"/>
<connect gate="A" pin="N/C_2" pad="11"/>
<connect gate="A" pin="NRZ/~NRZI" pad="2"/>
<connect gate="A" pin="NSP" pad="42"/>
<connect gate="A" pin="PAL/~NTSC" pad="44"/>
<connect gate="A" pin="PCLK" pad="22"/>
<connect gate="A" pin="RESET" pad="1"/>
<connect gate="A" pin="RREF" pad="35"/>
<connect gate="A" pin="SDO" pad="38"/>
<connect gate="A" pin="TEST_OUT" pad="3"/>
<connect gate="A" pin="TPG_ENB" pad="29"/>
<connect gate="A" pin="V/LFB1" pad="24"/>
<connect gate="A" pin="VDD" pad="7"/>
<connect gate="A" pin="VDDO" pad="28"/>
<connect gate="A" pin="VDDOD" pad="36"/>
<connect gate="A" pin="VDDOD_2" pad="32"/>
<connect gate="A" pin="VDDOD_3" pad="33"/>
<connect gate="A" pin="VDDSD" pad="40"/>
<connect gate="A" pin="VDD_2" pad="6"/>
<connect gate="A" pin="VSS" pad="5"/>
<connect gate="A" pin="VSSO" pad="27"/>
<connect gate="A" pin="VSSOD" pad="31"/>
<connect gate="A" pin="VSSOD_2" pad="30"/>
<connect gate="A" pin="VSSSD" pad="37"/>
<connect gate="A" pin="VSS_2" pad="4"/>
<connect gate="A" pin="~EDH_ENABLE" pad="9"/>
<connect gate="A" pin="~SDO" pad="39"/>
<connect gate="A" pin="~SMPTE_MODE" pad="10"/>
<connect gate="A" pin="~SYNC.~DET.~ENB" pad="41"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="CLC021AVGZ-33"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="29H5407"/>
<attribute name="PACKAGE" value="Digital Video Serializer"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CLC021AVGZ-5.0" prefix="U">
<description>Digital Video Serializer</description>
<gates>
<gate name="A" symbol="CLC021AVGZ-5.0"/>
</gates>
<devices>
<device name="" package="QFP80P1320X1320X245-44N">
<connects>
<connect gate="A" pin="ANC" pad="43"/>
<connect gate="A" pin="D0" pad="12"/>
<connect gate="A" pin="D1" pad="13"/>
<connect gate="A" pin="D2" pad="14"/>
<connect gate="A" pin="D3" pad="15"/>
<connect gate="A" pin="D4" pad="16"/>
<connect gate="A" pin="D5" pad="17"/>
<connect gate="A" pin="D6" pad="18"/>
<connect gate="A" pin="D7" pad="19"/>
<connect gate="A" pin="D8" pad="20"/>
<connect gate="A" pin="D9" pad="21"/>
<connect gate="A" pin="EDH_FORCE" pad="8"/>
<connect gate="A" pin="F/LFB2" pad="25"/>
<connect gate="A" pin="H/LFB0" pad="23"/>
<connect gate="A" pin="LOCK_DET" pad="26"/>
<connect gate="A" pin="N/C" pad="34"/>
<connect gate="A" pin="N/C_2" pad="11"/>
<connect gate="A" pin="NRZ/~NRZI" pad="2"/>
<connect gate="A" pin="NSP" pad="42"/>
<connect gate="A" pin="PAL/~NTSC" pad="44"/>
<connect gate="A" pin="PCLK" pad="22"/>
<connect gate="A" pin="RESET" pad="1"/>
<connect gate="A" pin="RREF" pad="35"/>
<connect gate="A" pin="SDO" pad="38"/>
<connect gate="A" pin="TEST_OUT" pad="3"/>
<connect gate="A" pin="TPG_ENB" pad="29"/>
<connect gate="A" pin="V/LFB1" pad="24"/>
<connect gate="A" pin="VDD" pad="7"/>
<connect gate="A" pin="VDDO" pad="28"/>
<connect gate="A" pin="VDDOD" pad="36"/>
<connect gate="A" pin="VDDOD_2" pad="32"/>
<connect gate="A" pin="VDDOD_3" pad="33"/>
<connect gate="A" pin="VDDSD" pad="40"/>
<connect gate="A" pin="VDD_2" pad="6"/>
<connect gate="A" pin="VSS" pad="5"/>
<connect gate="A" pin="VSSO" pad="27"/>
<connect gate="A" pin="VSSOD" pad="31"/>
<connect gate="A" pin="VSSOD_2" pad="30"/>
<connect gate="A" pin="VSSSD" pad="37"/>
<connect gate="A" pin="VSS_2" pad="4"/>
<connect gate="A" pin="~EDH_ENABLE" pad="9"/>
<connect gate="A" pin="~SDO" pad="39"/>
<connect gate="A" pin="~SMPTE_MODE" pad="10"/>
<connect gate="A" pin="~SYNC.~DET.~ENB" pad="41"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="CLC021AVGZ-5.0"/>
<attribute name="OC_FARNELL" value="1495092"/>
<attribute name="OC_NEWARK" value="41K1636"/>
<attribute name="PACKAGE" value="Digital Video Serializer"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DAC0808LCN" prefix="U">
<description>D/A Converter</description>
<gates>
<gate name="A" symbol="DAC0808LCN"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-16">
<connects>
<connect gate="A" pin="A1" pad="5"/>
<connect gate="A" pin="A2" pad="6"/>
<connect gate="A" pin="A3" pad="7"/>
<connect gate="A" pin="A4" pad="8"/>
<connect gate="A" pin="A5" pad="9"/>
<connect gate="A" pin="A6" pad="10"/>
<connect gate="A" pin="A7" pad="11"/>
<connect gate="A" pin="A8" pad="12"/>
<connect gate="A" pin="COMP" pad="16"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="IO" pad="4"/>
<connect gate="A" pin="NC" pad="1"/>
<connect gate="A" pin="VCC" pad="13"/>
<connect gate="A" pin="VEE" pad="3"/>
<connect gate="A" pin="VREF(+)" pad="14"/>
<connect gate="A" pin="VREF(-)" pad="15"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DAC0808LCN"/>
<attribute name="OC_FARNELL" value="9486658"/>
<attribute name="OC_NEWARK" value="07B5074"/>
<attribute name="PACKAGE" value="16-DIP"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DAC081S101CIMM" prefix="U">
<description>D/A Converter</description>
<gates>
<gate name="A" symbol="DAC081S101CIMM"/>
</gates>
<devices>
<device name="" package="SOP65P490X109-8N">
<connects>
<connect gate="A" pin="DIN" pad="7"/>
<connect gate="A" pin="GND" pad="8"/>
<connect gate="A" pin="NC" pad="2"/>
<connect gate="A" pin="NC_2" pad="3"/>
<connect gate="A" pin="SCLK" pad="6"/>
<connect gate="A" pin="VA" pad="1"/>
<connect gate="A" pin="VOUT" pad="4"/>
<connect gate="A" pin="~SYNC" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DAC081S101CIMM"/>
<attribute name="OC_FARNELL" value="1101194"/>
<attribute name="OC_NEWARK" value="65K5279"/>
<attribute name="PACKAGE" value="8-MSOP"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DAC082S085CIMM" prefix="U">
<description>D/A Converter</description>
<gates>
<gate name="A" symbol="DAC082S085CIMM"/>
</gates>
<devices>
<device name="" package="SOP50P490X109-10N">
<connects>
<connect gate="A" pin="DIN" pad="8"/>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="NC" pad="5"/>
<connect gate="A" pin="NC_2" pad="4"/>
<connect gate="A" pin="SCLK" pad="10"/>
<connect gate="A" pin="VA" pad="1"/>
<connect gate="A" pin="VOUTA" pad="2"/>
<connect gate="A" pin="VOUTB" pad="3"/>
<connect gate="A" pin="VREFIN" pad="7"/>
<connect gate="A" pin="~SYNC" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DAC082S085CIMM"/>
<attribute name="OC_FARNELL" value="1312535"/>
<attribute name="OC_NEWARK" value="12M9632"/>
<attribute name="PACKAGE" value="10-MSOP"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DAC0832LCN" prefix="U">
<description>D/A Converter</description>
<gates>
<gate name="A" symbol="DAC0832LCN"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-20">
<connects>
<connect gate="A" pin="DI0" pad="7"/>
<connect gate="A" pin="DI1" pad="6"/>
<connect gate="A" pin="DI2" pad="5"/>
<connect gate="A" pin="DI3" pad="4"/>
<connect gate="A" pin="DI4" pad="16"/>
<connect gate="A" pin="DI5" pad="15"/>
<connect gate="A" pin="DI6" pad="14"/>
<connect gate="A" pin="DI7" pad="13"/>
<connect gate="A" pin="GND" pad="10"/>
<connect gate="A" pin="GND_2" pad="3"/>
<connect gate="A" pin="ILE(BYTE1/~BYTE2)" pad="19"/>
<connect gate="A" pin="IOUT1" pad="11"/>
<connect gate="A" pin="IOUT2" pad="12"/>
<connect gate="A" pin="RFB" pad="9"/>
<connect gate="A" pin="VCC" pad="20"/>
<connect gate="A" pin="VREF" pad="8"/>
<connect gate="A" pin="~CS" pad="1"/>
<connect gate="A" pin="~WR1" pad="2"/>
<connect gate="A" pin="~WR2" pad="18"/>
<connect gate="A" pin="~XFER" pad="17"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DAC0832LCN"/>
<attribute name="OC_FARNELL" value="9486666"/>
<attribute name="OC_NEWARK" value="41K1771"/>
<attribute name="PACKAGE" value="20-DIP"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DAC084S085CIMM" prefix="U">
<description>D/A Converter</description>
<gates>
<gate name="A" symbol="DAC084S085CIMM"/>
</gates>
<devices>
<device name="" package="SOP50P490X109-10N">
<connects>
<connect gate="A" pin="DIN" pad="8"/>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="SCLK" pad="10"/>
<connect gate="A" pin="VA" pad="1"/>
<connect gate="A" pin="VOUTA" pad="2"/>
<connect gate="A" pin="VOUTB" pad="3"/>
<connect gate="A" pin="VOUTC" pad="4"/>
<connect gate="A" pin="VOUTD" pad="5"/>
<connect gate="A" pin="VREFIN" pad="7"/>
<connect gate="A" pin="~SYNC" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DAC084S085CIMM"/>
<attribute name="OC_FARNELL" value="1312536"/>
<attribute name="OC_NEWARK" value="12M9636"/>
<attribute name="PACKAGE" value="10-MSOP"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DAC101S101CIMM" prefix="U">
<description>A/D CONVERTER</description>
<gates>
<gate name="A" symbol="DAC101S101CIMM"/>
</gates>
<devices>
<device name="" package="SOP65P490X109-8N">
<connects>
<connect gate="A" pin="DIN" pad="7"/>
<connect gate="A" pin="GND" pad="8"/>
<connect gate="A" pin="NC" pad="2"/>
<connect gate="A" pin="NC_2" pad="3"/>
<connect gate="A" pin="SCLK" pad="6"/>
<connect gate="A" pin="VA" pad="1"/>
<connect gate="A" pin="VOUT" pad="4"/>
<connect gate="A" pin="~SYNC" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DAC101S101CIMM"/>
<attribute name="OC_FARNELL" value="1101197"/>
<attribute name="OC_NEWARK" value="96K8408"/>
<attribute name="PACKAGE" value="8-MSOP"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DAC108S085CIMT" prefix="U">
<description>Digital-to-Analog Converter</description>
<gates>
<gate name="A" symbol="DAC108S085CIMT"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-16N">
<connects>
<connect gate="A" pin="DIN" pad="1"/>
<connect gate="A" pin="DOUT" pad="2"/>
<connect gate="A" pin="GND" pad="10"/>
<connect gate="A" pin="SCLK" pad="16"/>
<connect gate="A" pin="VA" pad="7"/>
<connect gate="A" pin="VOUTA" pad="3"/>
<connect gate="A" pin="VOUTB" pad="4"/>
<connect gate="A" pin="VOUTC" pad="5"/>
<connect gate="A" pin="VOUTD" pad="6"/>
<connect gate="A" pin="VOUTE" pad="14"/>
<connect gate="A" pin="VOUTF" pad="13"/>
<connect gate="A" pin="VOUTG" pad="12"/>
<connect gate="A" pin="VOUTH" pad="11"/>
<connect gate="A" pin="VREF1" pad="8"/>
<connect gate="A" pin="VREF2" pad="9"/>
<connect gate="A" pin="~SYNC" pad="15"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DAC108S085CIMT"/>
<attribute name="OC_FARNELL" value="1495063"/>
<attribute name="OC_NEWARK" value="61M5726"/>
<attribute name="PACKAGE" value="16-TSSOP"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DAC121S101CIMK" prefix="U">
<description>Digital-to-Analog Converter</description>
<gates>
<gate name="A" symbol="DAC121S101CIMK"/>
</gates>
<devices>
<device name="" package="SOT95P285X90-6N">
<connects>
<connect gate="A" pin="DIN" pad="4"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="SCLK" pad="5"/>
<connect gate="A" pin="VA" pad="3"/>
<connect gate="A" pin="VOUT" pad="1"/>
<connect gate="A" pin="~SYNC" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DAC121S101CIMK"/>
<attribute name="OC_FARNELL" value="1101198"/>
<attribute name="OC_NEWARK" value="65K5283"/>
<attribute name="PACKAGE" value="TSOT-6"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DAC128S085CIMT" prefix="U">
<description>Digital-to-Analog Converter</description>
<gates>
<gate name="A" symbol="DAC128S085CIMT"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-16N">
<connects>
<connect gate="A" pin="DIN" pad="1"/>
<connect gate="A" pin="DOUT" pad="2"/>
<connect gate="A" pin="GND" pad="10"/>
<connect gate="A" pin="SCLK" pad="16"/>
<connect gate="A" pin="VA" pad="7"/>
<connect gate="A" pin="VOUTA" pad="3"/>
<connect gate="A" pin="VOUTB" pad="4"/>
<connect gate="A" pin="VOUTC" pad="5"/>
<connect gate="A" pin="VOUTD" pad="6"/>
<connect gate="A" pin="VOUTE" pad="14"/>
<connect gate="A" pin="VOUTF" pad="13"/>
<connect gate="A" pin="VOUTG" pad="12"/>
<connect gate="A" pin="VOUTH" pad="11"/>
<connect gate="A" pin="VREF1" pad="8"/>
<connect gate="A" pin="VREF2" pad="9"/>
<connect gate="A" pin="~SYNC" pad="15"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DAC128S085CIMT"/>
<attribute name="OC_FARNELL" value="1495073"/>
<attribute name="OC_NEWARK" value="64M6828"/>
<attribute name="PACKAGE" value="16-TSSOP"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DP83816AVNG" prefix="U">
<description>PCI Ethernet Media Access Controller</description>
<gates>
<gate name="A" symbol="DP83816AVNG_A"/>
<gate name="B" symbol="DP83816AVNG_B"/>
</gates>
<devices>
<device name="" package="QFP50P2200X2200X160-144N">
<connects>
<connect gate="A" pin="AD26" pad="72"/>
<connect gate="A" pin="AD27" pad="71"/>
<connect gate="A" pin="AD28" pad="70"/>
<connect gate="A" pin="AD29" pad="68"/>
<connect gate="A" pin="AD30" pad="67"/>
<connect gate="A" pin="AD31" pad="66"/>
<connect gate="A" pin="AUXVDD" pad="9"/>
<connect gate="A" pin="AUXVDD_2" pad="56"/>
<connect gate="A" pin="AUXVDD_3" pad="21"/>
<connect gate="A" pin="AUXVDD_4" pad="27"/>
<connect gate="A" pin="AUXVDD_5" pad="33"/>
<connect gate="A" pin="AUXVDD_6" pad="58"/>
<connect gate="A" pin="C1" pad="19"/>
<connect gate="A" pin="COL/MA16" pad="28"/>
<connect gate="A" pin="CRS" pad="29"/>
<connect gate="A" pin="GNTN" pad="63"/>
<connect gate="A" pin="IAUXVDD" pad="47"/>
<connect gate="A" pin="IAUXVDD_2" pad="39"/>
<connect gate="A" pin="INTAN" pad="61"/>
<connect gate="A" pin="MA3/EEDI" pad="1"/>
<connect gate="A" pin="MA4/EECLK" pad="2"/>
<connect gate="A" pin="MA5" pad="3"/>
<connect gate="A" pin="MDC" pad="5"/>
<connect gate="A" pin="MDIO" pad="4"/>
<connect gate="A" pin="NC" pad="43"/>
<connect gate="A" pin="NC_2" pad="34"/>
<connect gate="A" pin="NC_3" pad="36"/>
<connect gate="A" pin="NC_4" pad="37"/>
<connect gate="A" pin="NC_5" pad="42"/>
<connect gate="A" pin="PCICLK" pad="60"/>
<connect gate="A" pin="PCIVDD" pad="69"/>
<connect gate="A" pin="PMEN/CLKRUNN" pad="59"/>
<connect gate="A" pin="REGEN" pad="48"/>
<connect gate="A" pin="REQN" pad="64"/>
<connect gate="A" pin="RESERVED" pad="50"/>
<connect gate="A" pin="RESERVED_2" pad="41"/>
<connect gate="A" pin="RSTN" pad="62"/>
<connect gate="A" pin="RXCLK" pad="6"/>
<connect gate="A" pin="RXD0/MA6" pad="7"/>
<connect gate="A" pin="RXD1/MA7" pad="10"/>
<connect gate="A" pin="RXD2/MA8" pad="11"/>
<connect gate="A" pin="RXD3/MA9" pad="12"/>
<connect gate="A" pin="RXDV/MA11" pad="15"/>
<connect gate="A" pin="RXER/MA10" pad="14"/>
<connect gate="A" pin="RXOE" pad="13"/>
<connect gate="A" pin="TPRDM" pad="45"/>
<connect gate="A" pin="TPRDP" pad="46"/>
<connect gate="A" pin="TPTDM" pad="53"/>
<connect gate="A" pin="TPTDP" pad="54"/>
<connect gate="A" pin="TXCLK" pad="31"/>
<connect gate="A" pin="TXD0/MA12" pad="22"/>
<connect gate="A" pin="TXD1/MA13" pad="23"/>
<connect gate="A" pin="TXD2/MA14" pad="24"/>
<connect gate="A" pin="TXD3/MA15" pad="25"/>
<connect gate="A" pin="TXEN" pad="30"/>
<connect gate="A" pin="VREF" pad="40"/>
<connect gate="A" pin="VSS" pad="8"/>
<connect gate="A" pin="VSS_10" pad="65"/>
<connect gate="A" pin="VSS_11" pad="44"/>
<connect gate="A" pin="VSS_12" pad="52"/>
<connect gate="A" pin="VSS_13" pad="35"/>
<connect gate="A" pin="VSS_14" pad="55"/>
<connect gate="A" pin="VSS_2" pad="16"/>
<connect gate="A" pin="VSS_3" pad="38"/>
<connect gate="A" pin="VSS_4" pad="20"/>
<connect gate="A" pin="VSS_5" pad="49"/>
<connect gate="A" pin="VSS_6" pad="32"/>
<connect gate="A" pin="VSS_7" pad="26"/>
<connect gate="A" pin="VSS_8" pad="51"/>
<connect gate="A" pin="VSS_9" pad="57"/>
<connect gate="A" pin="X1" pad="17"/>
<connect gate="A" pin="X2" pad="18"/>
<connect gate="B" pin="3VAUX" pad="122"/>
<connect gate="B" pin="AD0" pad="121"/>
<connect gate="B" pin="AD1" pad="120"/>
<connect gate="B" pin="AD10" pad="108"/>
<connect gate="B" pin="AD11" pad="106"/>
<connect gate="B" pin="AD12" pad="105"/>
<connect gate="B" pin="AD13" pad="104"/>
<connect gate="B" pin="AD14" pad="102"/>
<connect gate="B" pin="AD15" pad="101"/>
<connect gate="B" pin="AD16" pad="88"/>
<connect gate="B" pin="AD17" pad="87"/>
<connect gate="B" pin="AD18" pad="86"/>
<connect gate="B" pin="AD19" pad="83"/>
<connect gate="B" pin="AD2" pad="119"/>
<connect gate="B" pin="AD20" pad="82"/>
<connect gate="B" pin="AD21" pad="81"/>
<connect gate="B" pin="AD22" pad="79"/>
<connect gate="B" pin="AD23" pad="78"/>
<connect gate="B" pin="AD24" pad="74"/>
<connect gate="B" pin="AD25" pad="73"/>
<connect gate="B" pin="AD3" pad="118"/>
<connect gate="B" pin="AD4" pad="116"/>
<connect gate="B" pin="AD5" pad="115"/>
<connect gate="B" pin="AD6" pad="113"/>
<connect gate="B" pin="AD7" pad="112"/>
<connect gate="B" pin="AD8" pad="110"/>
<connect gate="B" pin="AD9" pad="109"/>
<connect gate="B" pin="AUXVDD" pad="137"/>
<connect gate="B" pin="CBEN0" pad="111"/>
<connect gate="B" pin="CBEN1" pad="100"/>
<connect gate="B" pin="CBEN2" pad="89"/>
<connect gate="B" pin="CBEN3" pad="75"/>
<connect gate="B" pin="DEVSELN" pad="95"/>
<connect gate="B" pin="EESEL" pad="128"/>
<connect gate="B" pin="FRAMEN" pad="91"/>
<connect gate="B" pin="IDSEL" pad="76"/>
<connect gate="B" pin="IRDYN" pad="92"/>
<connect gate="B" pin="MA0/LEDACTN" pad="142"/>
<connect gate="B" pin="MA1/LED10N" pad="143"/>
<connect gate="B" pin="MA2/LED100N" pad="144"/>
<connect gate="B" pin="MCSN" pad="129"/>
<connect gate="B" pin="MD0" pad="132"/>
<connect gate="B" pin="MD1/CFGDISN" pad="133"/>
<connect gate="B" pin="MD2" pad="134"/>
<connect gate="B" pin="MD3" pad="135"/>
<connect gate="B" pin="MD4/EEDO" pad="138"/>
<connect gate="B" pin="MD5" pad="139"/>
<connect gate="B" pin="MD6" pad="140"/>
<connect gate="B" pin="MD7" pad="141"/>
<connect gate="B" pin="MRDN" pad="130"/>
<connect gate="B" pin="MWRN" pad="131"/>
<connect gate="B" pin="NC" pad="126"/>
<connect gate="B" pin="NC_2" pad="124"/>
<connect gate="B" pin="NC_3" pad="84"/>
<connect gate="B" pin="NC_4" pad="125"/>
<connect gate="B" pin="NC_5" pad="85"/>
<connect gate="B" pin="PAR" pad="99"/>
<connect gate="B" pin="PCIVDD" pad="94"/>
<connect gate="B" pin="PCIVDD_2" pad="107"/>
<connect gate="B" pin="PCIVDD_3" pad="117"/>
<connect gate="B" pin="PCIVDD_4" pad="80"/>
<connect gate="B" pin="PERRN" pad="97"/>
<connect gate="B" pin="PWRGOOD" pad="123"/>
<connect gate="B" pin="RESERVED" pad="127"/>
<connect gate="B" pin="SERRN" pad="98"/>
<connect gate="B" pin="STOPN" pad="96"/>
<connect gate="B" pin="TRDYN" pad="93"/>
<connect gate="B" pin="VSS" pad="136"/>
<connect gate="B" pin="VSS_2" pad="77"/>
<connect gate="B" pin="VSS_3" pad="90"/>
<connect gate="B" pin="VSS_4" pad="103"/>
<connect gate="B" pin="VSS_5" pad="114"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DP83816AVNG"/>
<attribute name="OC_FARNELL" value="1496006"/>
<attribute name="OC_NEWARK" value="41K1777"/>
<attribute name="PACKAGE" value="LQFP-144"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DP83848CVV" prefix="U">
<description>Single Port 10/100 Mb/s Ethernet Physical Layer Transceiver</description>
<gates>
<gate name="A" symbol="DP83848CVV"/>
</gates>
<devices>
<device name="" package="QFP50P900X900X160-48N">
<connects>
<connect gate="A" pin="25MHZ_OUT" pad="25"/>
<connect gate="A" pin="AGND" pad="19"/>
<connect gate="A" pin="AGND_2" pad="15"/>
<connect gate="A" pin="AVDD33" pad="22"/>
<connect gate="A" pin="COL/PHYAD0" pad="42"/>
<connect gate="A" pin="CRS/CRS_DV/LED_CFG" pad="40"/>
<connect gate="A" pin="DGND" pad="36"/>
<connect gate="A" pin="IOGND" pad="47"/>
<connect gate="A" pin="IOGND_2" pad="35"/>
<connect gate="A" pin="IOVDD3" pad="32"/>
<connect gate="A" pin="IOVDD33" pad="48"/>
<connect gate="A" pin="LED_ACT/COL/AN_" pad="26"/>
<connect gate="A" pin="LED_LINK/AN0" pad="28"/>
<connect gate="A" pin="LED_SPEED/AN1" pad="27"/>
<connect gate="A" pin="MDC" pad="31"/>
<connect gate="A" pin="MDIO" pad="30"/>
<connect gate="A" pin="PFBIN1" pad="18"/>
<connect gate="A" pin="PFBIN2" pad="37"/>
<connect gate="A" pin="PFBOUT" pad="23"/>
<connect gate="A" pin="PWR_DOWN/INT" pad="7"/>
<connect gate="A" pin="RBIAS" pad="24"/>
<connect gate="A" pin="RD+" pad="14"/>
<connect gate="A" pin="RD-" pad="13"/>
<connect gate="A" pin="RESERVED" pad="12"/>
<connect gate="A" pin="RESERVED_2" pad="8"/>
<connect gate="A" pin="RESERVED_3" pad="20"/>
<connect gate="A" pin="RESERVED_4" pad="9"/>
<connect gate="A" pin="RESERVED_5" pad="21"/>
<connect gate="A" pin="RESERVED_6" pad="10"/>
<connect gate="A" pin="RESERVED_7" pad="11"/>
<connect gate="A" pin="RESET_N" pad="29"/>
<connect gate="A" pin="RXD_0/PHYAD1" pad="43"/>
<connect gate="A" pin="RXD_1/PHYAD2" pad="44"/>
<connect gate="A" pin="RXD_2/PHYAD3" pad="45"/>
<connect gate="A" pin="RXD_3/PHYAD4" pad="46"/>
<connect gate="A" pin="RX_CLK" pad="38"/>
<connect gate="A" pin="RX_DV/MII_MODE" pad="39"/>
<connect gate="A" pin="RX_ER/MDIX_EN" pad="41"/>
<connect gate="A" pin="TD+" pad="17"/>
<connect gate="A" pin="TD-" pad="16"/>
<connect gate="A" pin="TXD_0" pad="3"/>
<connect gate="A" pin="TXD_1" pad="4"/>
<connect gate="A" pin="TXD_2" pad="5"/>
<connect gate="A" pin="TXD_3/SNI_MODE" pad="6"/>
<connect gate="A" pin="TX_CLK" pad="1"/>
<connect gate="A" pin="TX_EN" pad="2"/>
<connect gate="A" pin="X1" pad="34"/>
<connect gate="A" pin="X2" pad="33"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DP83848CVV"/>
<attribute name="OC_FARNELL" value="1286816"/>
<attribute name="OC_NEWARK" value="79K6187"/>
<attribute name="PACKAGE" value="QFP-48"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DP83848HSQ" prefix="U">
<description>Single 10/100 Ethernet Transceiver</description>
<gates>
<gate name="A" symbol="DP83848HSQ"/>
</gates>
<devices>
<device name="" package="QFN50P600X600X80-41N">
<connects>
<connect gate="A" pin="25MHZ_OUT" pad="21"/>
<connect gate="A" pin="AGND" pad="17"/>
<connect gate="A" pin="AGND_2" pad="13"/>
<connect gate="A" pin="AVDD33" pad="18"/>
<connect gate="A" pin="COL/PHYAD0" pad="35"/>
<connect gate="A" pin="CRS/CRS_DV/LED_CFG" pad="33"/>
<connect gate="A" pin="DGND" pad="29"/>
<connect gate="A" pin="EPAD" pad="41"/>
<connect gate="A" pin="IOGND" pad="40"/>
<connect gate="A" pin="IOVDD33" pad="26"/>
<connect gate="A" pin="IO_VDD33" pad="1"/>
<connect gate="A" pin="LED_LINK/AN0" pad="22"/>
<connect gate="A" pin="MDC" pad="25"/>
<connect gate="A" pin="MDIO" pad="24"/>
<connect gate="A" pin="PFBIN1" pad="16"/>
<connect gate="A" pin="PFBIN2" pad="30"/>
<connect gate="A" pin="PFBOUT" pad="19"/>
<connect gate="A" pin="RBIAS" pad="20"/>
<connect gate="A" pin="RD+" pad="12"/>
<connect gate="A" pin="RD-" pad="11"/>
<connect gate="A" pin="RESERVED" pad="10"/>
<connect gate="A" pin="RESERVED_2" pad="8"/>
<connect gate="A" pin="RESERVED_3" pad="9"/>
<connect gate="A" pin="RESET_N" pad="23"/>
<connect gate="A" pin="RXD_0/PHYAD1" pad="36"/>
<connect gate="A" pin="RXD_1/PHYAD2" pad="37"/>
<connect gate="A" pin="RXD_2/PHYAD3" pad="38"/>
<connect gate="A" pin="RXD_3/PHYAD4" pad="39"/>
<connect gate="A" pin="RX_CLK" pad="31"/>
<connect gate="A" pin="RX_DV/MII_MODE" pad="32"/>
<connect gate="A" pin="RX_ER/MDIX_EN" pad="34"/>
<connect gate="A" pin="TD_+" pad="15"/>
<connect gate="A" pin="TD_-" pad="14"/>
<connect gate="A" pin="TXD_0" pad="4"/>
<connect gate="A" pin="TXD_1" pad="5"/>
<connect gate="A" pin="TXD_2" pad="6"/>
<connect gate="A" pin="TXD_3" pad="7"/>
<connect gate="A" pin="TX_CLK" pad="2"/>
<connect gate="A" pin="TX_EN" pad="3"/>
<connect gate="A" pin="X1" pad="28"/>
<connect gate="A" pin="X2" pad="27"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DP83848HSQ"/>
<attribute name="OC_FARNELL" value="1602444"/>
<attribute name="OC_NEWARK" value="99K1888"/>
<attribute name="PACKAGE" value="QFN-40"/>
<attribute name="SUPPLIER" value="National Semiconducotors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DP83848MSQ" prefix="U">
<description>Ethernet Transceiver</description>
<gates>
<gate name="A" symbol="DP83848MSQ"/>
</gates>
<devices>
<device name="" package="QFN50P600X600X80-41N">
<connects>
<connect gate="A" pin="25MHZ_OUT" pad="21"/>
<connect gate="A" pin="AGND" pad="17"/>
<connect gate="A" pin="AGND_2" pad="13"/>
<connect gate="A" pin="AVDD33" pad="18"/>
<connect gate="A" pin="COL/PHYAD0" pad="35"/>
<connect gate="A" pin="CRS/CRS_DV/LED_CFG" pad="33"/>
<connect gate="A" pin="DGND" pad="29"/>
<connect gate="A" pin="GND" pad="41"/>
<connect gate="A" pin="IOGND" pad="40"/>
<connect gate="A" pin="IOVDD33" pad="26"/>
<connect gate="A" pin="IO_VDD33" pad="1"/>
<connect gate="A" pin="LED_LINK/AN0" pad="22"/>
<connect gate="A" pin="MDC" pad="25"/>
<connect gate="A" pin="MDIO" pad="24"/>
<connect gate="A" pin="PFBIN1" pad="16"/>
<connect gate="A" pin="PFBIN2" pad="30"/>
<connect gate="A" pin="PFBOUT" pad="19"/>
<connect gate="A" pin="RBIAS" pad="20"/>
<connect gate="A" pin="RD+" pad="12"/>
<connect gate="A" pin="RD-" pad="11"/>
<connect gate="A" pin="RESERVED" pad="10"/>
<connect gate="A" pin="RESERVED_2" pad="8"/>
<connect gate="A" pin="RESERVED_3" pad="9"/>
<connect gate="A" pin="RESET_N" pad="23"/>
<connect gate="A" pin="RXD_0/PHYAD1" pad="36"/>
<connect gate="A" pin="RXD_1/PHYAD2" pad="37"/>
<connect gate="A" pin="RXD_2/PHYAD3" pad="38"/>
<connect gate="A" pin="RXD_3/PHYAD4" pad="39"/>
<connect gate="A" pin="RX_CLK" pad="31"/>
<connect gate="A" pin="RX_DVMI_MODE" pad="32"/>
<connect gate="A" pin="RX_ER/MDIX_EN" pad="34"/>
<connect gate="A" pin="TD_+" pad="15"/>
<connect gate="A" pin="TD_-" pad="14"/>
<connect gate="A" pin="TXD_0" pad="4"/>
<connect gate="A" pin="TXD_1" pad="5"/>
<connect gate="A" pin="TXD_2" pad="6"/>
<connect gate="A" pin="TXD_3" pad="7"/>
<connect gate="A" pin="TX_CLK" pad="2"/>
<connect gate="A" pin="TX_EN" pad="3"/>
<connect gate="A" pin="X1" pad="28"/>
<connect gate="A" pin="X2" pad="27"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DP83848MSQ"/>
<attribute name="OC_FARNELL" value="1602446"/>
<attribute name="OC_NEWARK" value="99K1891"/>
<attribute name="PACKAGE" value="LLP-40"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DP83848TSQ" prefix="U">
<description>Single 10/100 Ethernet Transceiver</description>
<gates>
<gate name="A" symbol="DP83848TSQ"/>
</gates>
<devices>
<device name="" package="QFN50P600X600X80-41N">
<connects>
<connect gate="A" pin="25MHZ_OUT" pad="21"/>
<connect gate="A" pin="AGND" pad="17"/>
<connect gate="A" pin="AGND_2" pad="13"/>
<connect gate="A" pin="AVDD33" pad="18"/>
<connect gate="A" pin="COL/PHYAD0" pad="35"/>
<connect gate="A" pin="CRS/CRS_DV/LED_CFG" pad="33"/>
<connect gate="A" pin="DGND" pad="29"/>
<connect gate="A" pin="EPAD" pad="41"/>
<connect gate="A" pin="IOGND" pad="40"/>
<connect gate="A" pin="IOVDD33" pad="26"/>
<connect gate="A" pin="IO_VDD33" pad="1"/>
<connect gate="A" pin="LED_LINK/AN0" pad="22"/>
<connect gate="A" pin="MDC" pad="25"/>
<connect gate="A" pin="MDIO" pad="24"/>
<connect gate="A" pin="PFBIN1" pad="16"/>
<connect gate="A" pin="PFBIN2" pad="30"/>
<connect gate="A" pin="PFBOUT" pad="19"/>
<connect gate="A" pin="RBIAS" pad="20"/>
<connect gate="A" pin="RD+" pad="12"/>
<connect gate="A" pin="RD-" pad="11"/>
<connect gate="A" pin="RESERVED" pad="10"/>
<connect gate="A" pin="RESERVED_2" pad="8"/>
<connect gate="A" pin="RESERVED_3" pad="9"/>
<connect gate="A" pin="RESET_N" pad="23"/>
<connect gate="A" pin="RXD_0/PHYAD1" pad="36"/>
<connect gate="A" pin="RXD_1/PHYAD2" pad="37"/>
<connect gate="A" pin="RXD_2/PHYAD3" pad="38"/>
<connect gate="A" pin="RXD_3/PHYAD4" pad="39"/>
<connect gate="A" pin="RX_CLK" pad="31"/>
<connect gate="A" pin="RX_DV/MII_MODE" pad="32"/>
<connect gate="A" pin="RX_ER/MDIX_EN" pad="34"/>
<connect gate="A" pin="TD_+" pad="15"/>
<connect gate="A" pin="TD_-" pad="14"/>
<connect gate="A" pin="TXD_0" pad="4"/>
<connect gate="A" pin="TXD_1" pad="5"/>
<connect gate="A" pin="TXD_2" pad="6"/>
<connect gate="A" pin="TXD_3" pad="7"/>
<connect gate="A" pin="TX_CLK" pad="2"/>
<connect gate="A" pin="TX_EN" pad="3"/>
<connect gate="A" pin="X1" pad="28"/>
<connect gate="A" pin="X2" pad="27"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DP83848TSQ"/>
<attribute name="OC_FARNELL" value="1602447"/>
<attribute name="OC_NEWARK" value="99K1892"/>
<attribute name="PACKAGE" value="QFN-40"/>
<attribute name="SUPPLIER" value="National Semiconducotors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DP83848VYB" prefix="U">
<description>10/100 Mb/s Ethernet Physical Layer Transceiver</description>
<gates>
<gate name="A" symbol="DP83848VYB"/>
</gates>
<devices>
<device name="" package="QFP50P900X900X160-49N">
<connects>
<connect gate="A" pin="25MHZ_OUT" pad="25"/>
<connect gate="A" pin="AGND" pad="19"/>
<connect gate="A" pin="AGND_2" pad="15"/>
<connect gate="A" pin="AVDD33" pad="22"/>
<connect gate="A" pin="COL/PHYAD0" pad="42"/>
<connect gate="A" pin="CRS/CRS_DV/LED_CFG" pad="40"/>
<connect gate="A" pin="DGND" pad="36"/>
<connect gate="A" pin="EPAD" pad="49"/>
<connect gate="A" pin="IOGND" pad="47"/>
<connect gate="A" pin="IOGND_2" pad="35"/>
<connect gate="A" pin="IOVDD33" pad="48"/>
<connect gate="A" pin="IOVDD33_2" pad="32"/>
<connect gate="A" pin="LED_ACT/COL/AN_EN" pad="26"/>
<connect gate="A" pin="LED_LINK/AN0" pad="28"/>
<connect gate="A" pin="LED_SPEED/AN1" pad="27"/>
<connect gate="A" pin="MDC" pad="31"/>
<connect gate="A" pin="MDIO" pad="30"/>
<connect gate="A" pin="PFBIN1" pad="18"/>
<connect gate="A" pin="PFBIN2" pad="37"/>
<connect gate="A" pin="PFBOUT" pad="23"/>
<connect gate="A" pin="PWR_DOWN/INT" pad="7"/>
<connect gate="A" pin="RBIAS" pad="24"/>
<connect gate="A" pin="RD+" pad="14"/>
<connect gate="A" pin="RD-" pad="13"/>
<connect gate="A" pin="RESERVED" pad="20"/>
<connect gate="A" pin="RESERVED_2" pad="21"/>
<connect gate="A" pin="RESET" pad="29"/>
<connect gate="A" pin="RXD_0/PHYAD1" pad="43"/>
<connect gate="A" pin="RXD_1/PHYAD2" pad="44"/>
<connect gate="A" pin="RXD_2/PHYAD3" pad="45"/>
<connect gate="A" pin="RXD_3/PHYAD4" pad="46"/>
<connect gate="A" pin="RX_CLK" pad="38"/>
<connect gate="A" pin="RX_DV/MII_MODE" pad="39"/>
<connect gate="A" pin="RX_ER/MDIX_EN" pad="41"/>
<connect gate="A" pin="TCK" pad="8"/>
<connect gate="A" pin="TD+" pad="17"/>
<connect gate="A" pin="TD-" pad="16"/>
<connect gate="A" pin="TDI" pad="12"/>
<connect gate="A" pin="TDO" pad="9"/>
<connect gate="A" pin="TMS" pad="10"/>
<connect gate="A" pin="TRST" pad="11"/>
<connect gate="A" pin="TXD_0" pad="3"/>
<connect gate="A" pin="TXD_1" pad="4"/>
<connect gate="A" pin="TXD_2" pad="5"/>
<connect gate="A" pin="TXD_3/SNI_MODE" pad="6"/>
<connect gate="A" pin="TX_CLK" pad="1"/>
<connect gate="A" pin="TX_EN" pad="2"/>
<connect gate="A" pin="X1" pad="34"/>
<connect gate="A" pin="X2" pad="33"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DP83848VYB"/>
<attribute name="OC_FARNELL" value="1602448"/>
<attribute name="OC_NEWARK" value="11N4484"/>
<attribute name="PACKAGE" value="QFP-48"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DP83848YB" prefix="U">
<description>Transceiver</description>
<gates>
<gate name="A" symbol="DP83848YB"/>
</gates>
<devices>
<device name="" package="QFP50P900X900X160-49N">
<connects>
<connect gate="A" pin="25MHZ_OUT" pad="25"/>
<connect gate="A" pin="AGND" pad="19"/>
<connect gate="A" pin="AGND_2" pad="15"/>
<connect gate="A" pin="AVDD33" pad="22"/>
<connect gate="A" pin="COL/PHYAD0" pad="42"/>
<connect gate="A" pin="CRS/CRS_DV/LED_CFG" pad="40"/>
<connect gate="A" pin="DGND" pad="36"/>
<connect gate="A" pin="EP" pad="49"/>
<connect gate="A" pin="IOGND" pad="47"/>
<connect gate="A" pin="IOGND_2" pad="35"/>
<connect gate="A" pin="IOVDD33" pad="48"/>
<connect gate="A" pin="IOVDD33_2" pad="32"/>
<connect gate="A" pin="LED_ACT/COL/AN_EN" pad="26"/>
<connect gate="A" pin="LED_LINK/AN0" pad="28"/>
<connect gate="A" pin="LED_SPEED/AN1" pad="27"/>
<connect gate="A" pin="MDC" pad="31"/>
<connect gate="A" pin="MDIO" pad="30"/>
<connect gate="A" pin="PFBIN1" pad="18"/>
<connect gate="A" pin="PFBIN2" pad="37"/>
<connect gate="A" pin="PFBOUT" pad="23"/>
<connect gate="A" pin="PWR_DOWN/INT" pad="7"/>
<connect gate="A" pin="RBIAS" pad="24"/>
<connect gate="A" pin="RD+" pad="14"/>
<connect gate="A" pin="RD-" pad="13"/>
<connect gate="A" pin="RESERVED" pad="21"/>
<connect gate="A" pin="RESERVED_2" pad="20"/>
<connect gate="A" pin="RESET_N" pad="29"/>
<connect gate="A" pin="RXD_0/PHYAD1" pad="43"/>
<connect gate="A" pin="RXD_1/PHYAD2" pad="44"/>
<connect gate="A" pin="RXD_2/PHYAD3" pad="45"/>
<connect gate="A" pin="RXD_3/PHYAD4" pad="46"/>
<connect gate="A" pin="RX_CLK" pad="38"/>
<connect gate="A" pin="RX_DV/MII_MODE" pad="39"/>
<connect gate="A" pin="RX_ER/MDIX_EN" pad="41"/>
<connect gate="A" pin="TCK" pad="8"/>
<connect gate="A" pin="TD+" pad="17"/>
<connect gate="A" pin="TD-" pad="16"/>
<connect gate="A" pin="TDI" pad="12"/>
<connect gate="A" pin="TDO" pad="9"/>
<connect gate="A" pin="TMS" pad="10"/>
<connect gate="A" pin="TRST" pad="11"/>
<connect gate="A" pin="TXD_0" pad="3"/>
<connect gate="A" pin="TXD_1" pad="4"/>
<connect gate="A" pin="TXD_2" pad="5"/>
<connect gate="A" pin="TXD_3/SNI_MODE" pad="6"/>
<connect gate="A" pin="TX_CLK" pad="1"/>
<connect gate="A" pin="TX_EN" pad="2"/>
<connect gate="A" pin="X1" pad="34"/>
<connect gate="A" pin="X2" pad="33"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DP83848YB"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="79K6188"/>
<attribute name="PACKAGE" value="QFP-48"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DP83849CVS" prefix="U">
<description>Dual Port 10/100 Mb/s Ethernet Physical Layer Transceiver</description>
<gates>
<gate name="A" symbol="DP83849CVS"/>
</gates>
<devices>
<device name="" package="QFP50P1400X1400X120-80N">
<connects>
<connect gate="A" pin="ANA33VDD" pad="30"/>
<connect gate="A" pin="ANAGND1" pad="22"/>
<connect gate="A" pin="ANAGND2" pad="29"/>
<connect gate="A" pin="ANAGND3" pad="33"/>
<connect gate="A" pin="ANAGND4" pad="40"/>
<connect gate="A" pin="CDGND1" pad="25"/>
<connect gate="A" pin="CDGND2" pad="37"/>
<connect gate="A" pin="CLK2MAC" pad="68"/>
<connect gate="A" pin="COL_A" pad="3"/>
<connect gate="A" pin="COL_B" pad="59"/>
<connect gate="A" pin="COREGND1" pad="6"/>
<connect gate="A" pin="COREGND2" pad="55"/>
<connect gate="A" pin="CRS_A/CRS_DV_A/LED_CFG_A" pad="1"/>
<connect gate="A" pin="CRS_B/CRS_DV_B/LED_CFG_B" pad="61"/>
<connect gate="A" pin="IOGND1" pad="10"/>
<connect gate="A" pin="IOGND2" pad="52"/>
<connect gate="A" pin="IOGND3" pad="64"/>
<connect gate="A" pin="IOGND4" pad="77"/>
<connect gate="A" pin="IOVDD1" pad="11"/>
<connect gate="A" pin="IOVDD2" pad="51"/>
<connect gate="A" pin="IOVDD3" pad="65"/>
<connect gate="A" pin="IOVDD4" pad="78"/>
<connect gate="A" pin="LED_ACT/LED_COL/AN_EN_A" pad="21"/>
<connect gate="A" pin="LED_ACT/LED_COL/AN_EN_B" pad="41"/>
<connect gate="A" pin="LED_LINK_A/AN0_A" pad="19"/>
<connect gate="A" pin="LED_LINK_B/AN0_B" pad="43"/>
<connect gate="A" pin="LED_SPEED_A/AN1_A" pad="20"/>
<connect gate="A" pin="LED_SPEED_B/AN1_B" pad="42"/>
<connect gate="A" pin="MDC" pad="67"/>
<connect gate="A" pin="MDIO" pad="66"/>
<connect gate="A" pin="PFBIN1" pad="7"/>
<connect gate="A" pin="PFBIN2" pad="28"/>
<connect gate="A" pin="PFBIN3" pad="34"/>
<connect gate="A" pin="PFBIN4" pad="54"/>
<connect gate="A" pin="PFBOUT" pad="31"/>
<connect gate="A" pin="PWRDOWN_INT_A" pad="18"/>
<connect gate="A" pin="PWRDOWN_INT_B" pad="44"/>
<connect gate="A" pin="RBIAS" pad="32"/>
<connect gate="A" pin="RESERVED" pad="76"/>
<connect gate="A" pin="RESERVED_2" pad="72"/>
<connect gate="A" pin="RESERVED_3" pad="73"/>
<connect gate="A" pin="RESERVED_4" pad="74"/>
<connect gate="A" pin="RESERVED_5" pad="75"/>
<connect gate="A" pin="RESET_N" pad="71"/>
<connect gate="A" pin="RXD0_A/PHYAD1" pad="4"/>
<connect gate="A" pin="RXD0_B/PHYAD3" pad="58"/>
<connect gate="A" pin="RXD1_A/PHYAD2" pad="5"/>
<connect gate="A" pin="RXD1_B/PHYAD4" pad="57"/>
<connect gate="A" pin="RXD2_A/CLK2MAC_DIS" pad="8"/>
<connect gate="A" pin="RXD2_B" pad="56"/>
<connect gate="A" pin="RXD3_A/ED_EN_A" pad="9"/>
<connect gate="A" pin="RXD3_B/ED_EN_B" pad="53"/>
<connect gate="A" pin="RX_CLK_A" pad="79"/>
<connect gate="A" pin="RX_CLK_B" pad="63"/>
<connect gate="A" pin="RX_DV_A/MII_MODE_A" pad="80"/>
<connect gate="A" pin="RX_DV_B/MII_MODE_B" pad="62"/>
<connect gate="A" pin="RX_ER_A/MDIX_EN_A" pad="2"/>
<connect gate="A" pin="RX_ER_B/MDIX_EN_B" pad="60"/>
<connect gate="A" pin="TPRDM_A" pad="23"/>
<connect gate="A" pin="TPRDM_B" pad="39"/>
<connect gate="A" pin="TPRDP_A" pad="24"/>
<connect gate="A" pin="TPRDP_B" pad="38"/>
<connect gate="A" pin="TPTDM_A" pad="26"/>
<connect gate="A" pin="TPTDM_B" pad="36"/>
<connect gate="A" pin="TPTDP_A" pad="27"/>
<connect gate="A" pin="TPTDP_B" pad="35"/>
<connect gate="A" pin="TXD0_A" pad="14"/>
<connect gate="A" pin="TXD0_B" pad="48"/>
<connect gate="A" pin="TXD1_A" pad="15"/>
<connect gate="A" pin="TXD1_B" pad="47"/>
<connect gate="A" pin="TXD2_A" pad="16"/>
<connect gate="A" pin="TXD2_B" pad="46"/>
<connect gate="A" pin="TXD3_A/SNI_MODE_A" pad="17"/>
<connect gate="A" pin="TXD3_B/SNI_MODE_B" pad="45"/>
<connect gate="A" pin="TX_CLK_A" pad="12"/>
<connect gate="A" pin="TX_CLK_B" pad="50"/>
<connect gate="A" pin="TX_EN_A" pad="13"/>
<connect gate="A" pin="TX_EN_B" pad="49"/>
<connect gate="A" pin="X1" pad="70"/>
<connect gate="A" pin="X2" pad="69"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DP83849CVS"/>
<attribute name="OC_FARNELL" value="1271400"/>
<attribute name="OC_NEWARK" value="12M9707"/>
<attribute name="PACKAGE" value="QFP-80"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DP83865DVH" prefix="U">
<description>Ethernet Physical Layer</description>
<gates>
<gate name="A" symbol="DP83865DVH_A"/>
<gate name="B" symbol="DP83865DVH_B"/>
</gates>
<devices>
<device name="" package="QFP50P1723X2323X315-128N">
<connects>
<connect gate="A" pin="ACTIVITY_LED_/_SPEED0_STRAP" pad="7"/>
<connect gate="A" pin="COL/CLK_MAC_FREQ" pad="39"/>
<connect gate="A" pin="CORE_VDD" pad="63"/>
<connect gate="A" pin="CORE_VDD_2" pad="19"/>
<connect gate="A" pin="CORE_VDD_3" pad="25"/>
<connect gate="A" pin="CORE_VDD_4" pad="48"/>
<connect gate="A" pin="CORE_VDD_5" pad="11"/>
<connect gate="A" pin="CORE_VDD_6" pad="35"/>
<connect gate="A" pin="CRS/RGMII_SEL0" pad="40"/>
<connect gate="A" pin="DUPLEX_LED_/_PHYADDR0_STRAP" pad="13"/>
<connect gate="A" pin="IO_VDD" pad="29"/>
<connect gate="A" pin="IO_VDD_2" pad="21"/>
<connect gate="A" pin="IO_VDD_3" pad="53"/>
<connect gate="A" pin="IO_VDD_4" pad="4"/>
<connect gate="A" pin="IO_VDD_5" pad="37"/>
<connect gate="A" pin="IO_VDD_6" pad="15"/>
<connect gate="A" pin="IO_VDD_7" pad="42"/>
<connect gate="A" pin="IO_VDD_8" pad="58"/>
<connect gate="A" pin="LINK1000_LED_/_AN_EN_STRAP" pad="10"/>
<connect gate="A" pin="LINK100_LED_/_DUPLEX_STRAP" pad="9"/>
<connect gate="A" pin="LINK10_LED_/_RLED/SPEED1_STRAP" pad="8"/>
<connect gate="A" pin="NON_IEEE_STRAP" pad="1"/>
<connect gate="A" pin="PHYADDR1_STRAP" pad="14"/>
<connect gate="A" pin="PHYADDR2_STRAP" pad="17"/>
<connect gate="A" pin="PHYADDR3_STRAP" pad="18"/>
<connect gate="A" pin="RESERVED" pad="23"/>
<connect gate="A" pin="RESERVED_2" pad="2"/>
<connect gate="A" pin="RXD0/RX0" pad="56"/>
<connect gate="A" pin="RXD1/RX1" pad="55"/>
<connect gate="A" pin="RXD2/RX2" pad="52"/>
<connect gate="A" pin="RXD3/RX3" pad="51"/>
<connect gate="A" pin="RXD4" pad="50"/>
<connect gate="A" pin="RXD5" pad="47"/>
<connect gate="A" pin="RXD6" pad="46"/>
<connect gate="A" pin="RXD7" pad="45"/>
<connect gate="A" pin="RX_CLK" pad="57"/>
<connect gate="A" pin="RX_DV/RCK" pad="44"/>
<connect gate="A" pin="RX_ER/RXDV_ER" pad="41"/>
<connect gate="A" pin="TCK" pad="24"/>
<connect gate="A" pin="TDI" pad="31"/>
<connect gate="A" pin="TDO" pad="28"/>
<connect gate="A" pin="TMS" pad="27"/>
<connect gate="A" pin="TX_CLK/RGMII_SEL1" pad="60"/>
<connect gate="A" pin="TX_EN/TXEN_ER" pad="62"/>
<connect gate="A" pin="TX_ER" pad="61"/>
<connect gate="A" pin="TX_TCLK_/_MAN_MDIX_STRAP" pad="6"/>
<connect gate="A" pin="VDD_SEL_STRAP" pad="34"/>
<connect gate="A" pin="VSS" pad="22"/>
<connect gate="A" pin="VSS_10" pad="26"/>
<connect gate="A" pin="VSS_11" pad="20"/>
<connect gate="A" pin="VSS_12" pad="30"/>
<connect gate="A" pin="VSS_13" pad="59"/>
<connect gate="A" pin="VSS_14" pad="36"/>
<connect gate="A" pin="VSS_2" pad="43"/>
<connect gate="A" pin="VSS_3" pad="5"/>
<connect gate="A" pin="VSS_4" pad="54"/>
<connect gate="A" pin="VSS_5" pad="64"/>
<connect gate="A" pin="VSS_6" pad="12"/>
<connect gate="A" pin="VSS_7" pad="38"/>
<connect gate="A" pin="VSS_8" pad="16"/>
<connect gate="A" pin="VSS_9" pad="49"/>
<connect gate="A" pin="~INTERRUPT" pad="3"/>
<connect gate="A" pin="~RESET" pad="33"/>
<connect gate="A" pin="~TRST" pad="32"/>
<connect gate="B" pin="1V8_AVDD1" pad="123"/>
<connect gate="B" pin="1V8_AVDD1_2" pad="111"/>
<connect gate="B" pin="1V8_AVDD1_3" pad="105"/>
<connect gate="B" pin="1V8_AVDD1_4" pad="117"/>
<connect gate="B" pin="1V8_AVDD1_5" pad="103"/>
<connect gate="B" pin="1V8_AVDD2" pad="98"/>
<connect gate="B" pin="1V8_AVDD3" pad="100"/>
<connect gate="B" pin="2V5_AVDD1" pad="101"/>
<connect gate="B" pin="2V5_AVDD2" pad="96"/>
<connect gate="B" pin="BG_REF" pad="102"/>
<connect gate="B" pin="CLK_IN" pad="86"/>
<connect gate="B" pin="CLK_OUT" pad="87"/>
<connect gate="B" pin="CLK_TO_MAC" pad="85"/>
<connect gate="B" pin="CORE_VDD" pad="92"/>
<connect gate="B" pin="CORE_VDD_2" pad="73"/>
<connect gate="B" pin="GTX_CLK/TCK" pad="79"/>
<connect gate="B" pin="IO_VDD" pad="83"/>
<connect gate="B" pin="IO_VDD_2" pad="77"/>
<connect gate="B" pin="IO_VDD_3" pad="90"/>
<connect gate="B" pin="IO_VDD_4" pad="69"/>
<connect gate="B" pin="MAC_CLK_EN_STRAP" pad="88"/>
<connect gate="B" pin="MDC" pad="81"/>
<connect gate="B" pin="MDIA_N" pad="109"/>
<connect gate="B" pin="MDIA_P" pad="108"/>
<connect gate="B" pin="MDIB_N" pad="115"/>
<connect gate="B" pin="MDIB_P" pad="114"/>
<connect gate="B" pin="MDIC_N" pad="121"/>
<connect gate="B" pin="MDIC_P" pad="120"/>
<connect gate="B" pin="MDID_N" pad="127"/>
<connect gate="B" pin="MDID_P" pad="126"/>
<connect gate="B" pin="MDIO" pad="80"/>
<connect gate="B" pin="MDIX_EN_STRAP" pad="89"/>
<connect gate="B" pin="MULTI_EN_STRAP_/_TX_TRIGGER" pad="94"/>
<connect gate="B" pin="PHYADDR4_STRAP" pad="95"/>
<connect gate="B" pin="RESERVED" pad="84"/>
<connect gate="B" pin="TXD0/TX0" pad="76"/>
<connect gate="B" pin="TXD1/TX1" pad="75"/>
<connect gate="B" pin="TXD2/TX2" pad="72"/>
<connect gate="B" pin="TXD3/TX3" pad="71"/>
<connect gate="B" pin="TXD4" pad="68"/>
<connect gate="B" pin="TXD5" pad="67"/>
<connect gate="B" pin="TXD6" pad="66"/>
<connect gate="B" pin="TXD7" pad="65"/>
<connect gate="B" pin="VSS" pad="119"/>
<connect gate="B" pin="VSS_10" pad="116"/>
<connect gate="B" pin="VSS_11" pad="93"/>
<connect gate="B" pin="VSS_12" pad="70"/>
<connect gate="B" pin="VSS_13" pad="125"/>
<connect gate="B" pin="VSS_14" pad="104"/>
<connect gate="B" pin="VSS_15" pad="97"/>
<connect gate="B" pin="VSS_16" pad="124"/>
<connect gate="B" pin="VSS_17" pad="122"/>
<connect gate="B" pin="VSS_18" pad="110"/>
<connect gate="B" pin="VSS_19" pad="113"/>
<connect gate="B" pin="VSS_2" pad="82"/>
<connect gate="B" pin="VSS_20" pad="91"/>
<connect gate="B" pin="VSS_21" pad="118"/>
<connect gate="B" pin="VSS_3" pad="107"/>
<connect gate="B" pin="VSS_4" pad="128"/>
<connect gate="B" pin="VSS_5" pad="106"/>
<connect gate="B" pin="VSS_6" pad="78"/>
<connect gate="B" pin="VSS_7" pad="99"/>
<connect gate="B" pin="VSS_8" pad="112"/>
<connect gate="B" pin="VSS_9" pad="74"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DP83865DVH"/>
<attribute name="OC_FARNELL" value="8238600"/>
<attribute name="OC_NEWARK" value="41J5300"/>
<attribute name="PACKAGE" value="QFP-128"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS08MB200TSQ" prefix="U">
<description>LVDS  MUX/Buffer</description>
<gates>
<gate name="A" symbol="DS08MB200TSQ"/>
</gates>
<devices>
<device name="" package="QFN50P700X700X80-49N">
<connects>
<connect gate="A" pin="DAP" pad="49"/>
<connect gate="A" pin="ENA_0" pad="36"/>
<connect gate="A" pin="ENA_1" pad="13"/>
<connect gate="A" pin="ENB_0" pad="35"/>
<connect gate="A" pin="ENB_1" pad="14"/>
<connect gate="A" pin="ENL_0" pad="45"/>
<connect gate="A" pin="ENL_1" pad="4"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="GND_2" pad="46"/>
<connect gate="A" pin="GND_3" pad="2"/>
<connect gate="A" pin="GND_4" pad="47"/>
<connect gate="A" pin="LI_0+" pad="40"/>
<connect gate="A" pin="LI_0-" pad="39"/>
<connect gate="A" pin="LI_1+" pad="9"/>
<connect gate="A" pin="LI_1-" pad="10"/>
<connect gate="A" pin="LO_0+" pad="42"/>
<connect gate="A" pin="LO_0-" pad="41"/>
<connect gate="A" pin="LO_1+" pad="7"/>
<connect gate="A" pin="LO_1-" pad="8"/>
<connect gate="A" pin="MUX_S0" pad="38"/>
<connect gate="A" pin="MUX_S1" pad="11"/>
<connect gate="A" pin="N/C" pad="26"/>
<connect gate="A" pin="N/C_2" pad="44"/>
<connect gate="A" pin="N/C_3" pad="1"/>
<connect gate="A" pin="N/C_4" pad="5"/>
<connect gate="A" pin="N/C_5" pad="23"/>
<connect gate="A" pin="N/C_6" pad="24"/>
<connect gate="A" pin="N/C_7" pad="25"/>
<connect gate="A" pin="SIA_0+" pad="30"/>
<connect gate="A" pin="SIA_0-" pad="29"/>
<connect gate="A" pin="SIA_1+" pad="19"/>
<connect gate="A" pin="SIA_1-" pad="20"/>
<connect gate="A" pin="SIB_0+" pad="28"/>
<connect gate="A" pin="SIB_0-" pad="27"/>
<connect gate="A" pin="SIB_1+" pad="21"/>
<connect gate="A" pin="SIB_1-" pad="22"/>
<connect gate="A" pin="SOA_0+" pad="34"/>
<connect gate="A" pin="SOA_0-" pad="33"/>
<connect gate="A" pin="SOA_1+" pad="15"/>
<connect gate="A" pin="SOA_1-" pad="16"/>
<connect gate="A" pin="SOB_0+" pad="32"/>
<connect gate="A" pin="SOB_0-" pad="31"/>
<connect gate="A" pin="SOB_1+" pad="17"/>
<connect gate="A" pin="SOB_1-" pad="18"/>
<connect gate="A" pin="VDD" pad="43"/>
<connect gate="A" pin="VDD_2" pad="48"/>
<connect gate="A" pin="VDD_3" pad="12"/>
<connect gate="A" pin="VDD_4" pad="37"/>
<connect gate="A" pin="VDD_5" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS08MB200TSQ"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="12M9717"/>
<attribute name="PACKAGE" value="LLP-48"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS10BR254TSQ" prefix="U">
<description>LVDS Repeater</description>
<gates>
<gate name="A" symbol="DS10BR254TSQ"/>
</gates>
<devices>
<device name="" package="QFN50P600X600X80-41N">
<connects>
<connect gate="A" pin="GND" pad="16"/>
<connect gate="A" pin="GND_2" pad="41"/>
<connect gate="A" pin="IN1+" pad="4"/>
<connect gate="A" pin="IN1-" pad="5"/>
<connect gate="A" pin="IN2+" pad="6"/>
<connect gate="A" pin="IN2-" pad="7"/>
<connect gate="A" pin="NC" pad="2"/>
<connect gate="A" pin="NC_10" pad="13"/>
<connect gate="A" pin="NC_11" pad="12"/>
<connect gate="A" pin="NC_12" pad="11"/>
<connect gate="A" pin="NC_13" pad="10"/>
<connect gate="A" pin="NC_14" pad="9"/>
<connect gate="A" pin="NC_2" pad="1"/>
<connect gate="A" pin="NC_3" pad="40"/>
<connect gate="A" pin="NC_4" pad="39"/>
<connect gate="A" pin="NC_5" pad="31"/>
<connect gate="A" pin="NC_6" pad="20"/>
<connect gate="A" pin="NC_7" pad="19"/>
<connect gate="A" pin="NC_8" pad="18"/>
<connect gate="A" pin="NC_9" pad="17"/>
<connect gate="A" pin="OUT0+" pad="29"/>
<connect gate="A" pin="OUT0-" pad="28"/>
<connect gate="A" pin="OUT1+" pad="27"/>
<connect gate="A" pin="OUT1-" pad="26"/>
<connect gate="A" pin="OUT2+" pad="24"/>
<connect gate="A" pin="OUT2-" pad="23"/>
<connect gate="A" pin="OUT3+" pad="22"/>
<connect gate="A" pin="OUT3-" pad="21"/>
<connect gate="A" pin="SEL_IN" pad="14"/>
<connect gate="A" pin="VDD" pad="30"/>
<connect gate="A" pin="VDD_2" pad="3"/>
<connect gate="A" pin="VDD_3" pad="8"/>
<connect gate="A" pin="VDD_4" pad="25"/>
<connect gate="A" pin="VDD_5" pad="15"/>
<connect gate="A" pin="~LOS1" pad="37"/>
<connect gate="A" pin="~LOS2" pad="36"/>
<connect gate="A" pin="~PWDN" pad="38"/>
<connect gate="A" pin="~PWDN0" pad="35"/>
<connect gate="A" pin="~PWDN1" pad="34"/>
<connect gate="A" pin="~PWDN2" pad="33"/>
<connect gate="A" pin="~PWDN3" pad="32"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS10BR254TSQ"/>
<attribute name="OC_FARNELL" value="1552432"/>
<attribute name="OC_NEWARK" value="78M7724"/>
<attribute name="PACKAGE" value="LLP-40"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS10CP152QMA" prefix="U">
<description>LVDS Crosspoint Switch</description>
<gates>
<gate name="A" symbol="DS10CP152QMA"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-16N">
<connects>
<connect gate="A" pin="EN0" pad="16"/>
<connect gate="A" pin="EN1" pad="15"/>
<connect gate="A" pin="GND" pad="12"/>
<connect gate="A" pin="IN0+" pad="3"/>
<connect gate="A" pin="IN0-" pad="4"/>
<connect gate="A" pin="IN1+" pad="6"/>
<connect gate="A" pin="IN1-" pad="7"/>
<connect gate="A" pin="NC" pad="8"/>
<connect gate="A" pin="NC_2" pad="9"/>
<connect gate="A" pin="OUT0+" pad="14"/>
<connect gate="A" pin="OUT0-" pad="13"/>
<connect gate="A" pin="OUT1+" pad="11"/>
<connect gate="A" pin="OUT1-" pad="10"/>
<connect gate="A" pin="SEL0" pad="2"/>
<connect gate="A" pin="SEL1" pad="1"/>
<connect gate="A" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS10CP152QMA"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="07P4953"/>
<attribute name="PACKAGE" value="SOIC-16"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS10CP152TMA" prefix="U">
<description>LVDS Crosspoint Switch</description>
<gates>
<gate name="A" symbol="DS10CP152TMA"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-16N">
<connects>
<connect gate="A" pin="EN0" pad="16"/>
<connect gate="A" pin="EN1" pad="15"/>
<connect gate="A" pin="GND" pad="12"/>
<connect gate="A" pin="IN0+" pad="3"/>
<connect gate="A" pin="IN0-" pad="4"/>
<connect gate="A" pin="IN1+" pad="6"/>
<connect gate="A" pin="IN1-" pad="7"/>
<connect gate="A" pin="NC" pad="8"/>
<connect gate="A" pin="NC_2" pad="9"/>
<connect gate="A" pin="OUT0+" pad="14"/>
<connect gate="A" pin="OUT0-" pad="13"/>
<connect gate="A" pin="OUT1+" pad="11"/>
<connect gate="A" pin="OUT1-" pad="10"/>
<connect gate="A" pin="SEL0" pad="2"/>
<connect gate="A" pin="SEL1" pad="1"/>
<connect gate="A" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS10CP152TMA"/>
<attribute name="OC_FARNELL" value="1542528"/>
<attribute name="OC_NEWARK" value="94M6886"/>
<attribute name="PACKAGE" value="SOIC-16"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS10CP154ATSQ" prefix="U">
<description>Crosspoint Switch</description>
<gates>
<gate name="A" symbol="DS10CP154ATSQ"/>
</gates>
<devices>
<device name="" package="QFN50P600X600X80-41N">
<connects>
<connect gate="A" pin="EN_SMB" pad="17"/>
<connect gate="A" pin="GND" pad="16"/>
<connect gate="A" pin="GND_2" pad="41"/>
<connect gate="A" pin="IN0+" pad="1"/>
<connect gate="A" pin="IN0-" pad="2"/>
<connect gate="A" pin="IN1+" pad="4"/>
<connect gate="A" pin="IN1-" pad="5"/>
<connect gate="A" pin="IN2+" pad="6"/>
<connect gate="A" pin="IN2-" pad="7"/>
<connect gate="A" pin="IN3+" pad="9"/>
<connect gate="A" pin="IN3-" pad="10"/>
<connect gate="A" pin="NC" pad="18"/>
<connect gate="A" pin="NC_2" pad="12"/>
<connect gate="A" pin="NC_3" pad="11"/>
<connect gate="A" pin="NC_4" pad="40"/>
<connect gate="A" pin="NC_5" pad="39"/>
<connect gate="A" pin="NC_6" pad="31"/>
<connect gate="A" pin="NC_7" pad="20"/>
<connect gate="A" pin="NC_8" pad="19"/>
<connect gate="A" pin="OUT0+" pad="29"/>
<connect gate="A" pin="OUT0-" pad="28"/>
<connect gate="A" pin="OUT1+" pad="27"/>
<connect gate="A" pin="OUT1-" pad="26"/>
<connect gate="A" pin="OUT2+" pad="24"/>
<connect gate="A" pin="OUT2-" pad="23"/>
<connect gate="A" pin="OUT3+" pad="22"/>
<connect gate="A" pin="OUT3-" pad="21"/>
<connect gate="A" pin="S00/SCL" pad="37"/>
<connect gate="A" pin="S01/SDA" pad="36"/>
<connect gate="A" pin="S10/ADDR0" pad="35"/>
<connect gate="A" pin="S11/ADDR1" pad="34"/>
<connect gate="A" pin="S20/ADDR2" pad="33"/>
<connect gate="A" pin="S21/ADDR3" pad="32"/>
<connect gate="A" pin="S30" pad="13"/>
<connect gate="A" pin="S31" pad="14"/>
<connect gate="A" pin="VDD" pad="30"/>
<connect gate="A" pin="VDD_2" pad="3"/>
<connect gate="A" pin="VDD_3" pad="8"/>
<connect gate="A" pin="VDD_4" pad="25"/>
<connect gate="A" pin="VDD_5" pad="15"/>
<connect gate="A" pin="~PWDN" pad="38"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS10CP154ATSQ"/>
<attribute name="OC_FARNELL" value="1667412"/>
<attribute name="OC_NEWARK" value="15P1450"/>
<attribute name="PACKAGE" value="LLP-40"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS14185WM" prefix="U">
<description>3 Driver x 5 Receiver</description>
<gates>
<gate name="A" symbol="DS14185WM"/>
</gates>
<devices>
<device name="" package="SOIC127P1032X264-20N">
<connects>
<connect gate="A" pin="DIN1" pad="16"/>
<connect gate="A" pin="DIN2" pad="15"/>
<connect gate="A" pin="DIN3" pad="13"/>
<connect gate="A" pin="DOUT1" pad="5"/>
<connect gate="A" pin="DOUT2" pad="6"/>
<connect gate="A" pin="DOUT3" pad="8"/>
<connect gate="A" pin="GND" pad="11"/>
<connect gate="A" pin="RIN1" pad="2"/>
<connect gate="A" pin="RIN2" pad="3"/>
<connect gate="A" pin="RIN3" pad="4"/>
<connect gate="A" pin="RIN4" pad="7"/>
<connect gate="A" pin="RIN5" pad="9"/>
<connect gate="A" pin="ROUT1" pad="19"/>
<connect gate="A" pin="ROUT2" pad="18"/>
<connect gate="A" pin="ROUT3" pad="17"/>
<connect gate="A" pin="ROUT4" pad="14"/>
<connect gate="A" pin="ROUT5" pad="12"/>
<connect gate="A" pin="V+" pad="1"/>
<connect gate="A" pin="V-" pad="10"/>
<connect gate="A" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS14185WM"/>
<attribute name="OC_FARNELL" value="9494243"/>
<attribute name="OC_NEWARK" value="41K1814"/>
<attribute name="PACKAGE" value="SOIC-20"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS1487M" prefix="U">
<description>RS-485 1/4 Unit Load Multipoint Transceiver</description>
<gates>
<gate name="A" symbol="DS1487M"/>
</gates>
<devices>
<device name="" package="SOIC127P620X175-8N">
<connects>
<connect gate="A" pin="A" pad="6"/>
<connect gate="A" pin="B" pad="7"/>
<connect gate="A" pin="DE" pad="3"/>
<connect gate="A" pin="DI" pad="4"/>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="RE*" pad="2"/>
<connect gate="A" pin="RO" pad="1"/>
<connect gate="A" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS1487M"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K1816"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS14C232CM" prefix="U">
<description>Driver/Receiver</description>
<gates>
<gate name="A" symbol="DS14C232CM"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-16N">
<connects>
<connect gate="A" pin="C1+" pad="1"/>
<connect gate="A" pin="C1-" pad="3"/>
<connect gate="A" pin="C2+" pad="4"/>
<connect gate="A" pin="C2-" pad="5"/>
<connect gate="A" pin="DIN1" pad="11"/>
<connect gate="A" pin="DIN2" pad="10"/>
<connect gate="A" pin="DOUT1" pad="14"/>
<connect gate="A" pin="DOUT2" pad="7"/>
<connect gate="A" pin="GND" pad="15"/>
<connect gate="A" pin="RIN1" pad="13"/>
<connect gate="A" pin="RIN2" pad="8"/>
<connect gate="A" pin="ROUT1" pad="12"/>
<connect gate="A" pin="ROUT2" pad="9"/>
<connect gate="A" pin="V+" pad="2"/>
<connect gate="A" pin="V-" pad="6"/>
<connect gate="A" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS14C232CM"/>
<attribute name="OC_FARNELL" value="9490124"/>
<attribute name="OC_NEWARK" value="41K1795"/>
<attribute name="PACKAGE" value="SOIC-16"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS14C232CN" prefix="U">
<description>Driver/Receiver</description>
<gates>
<gate name="A" symbol="DS14C232CN"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-16">
<connects>
<connect gate="A" pin="C1+" pad="1"/>
<connect gate="A" pin="C1-" pad="3"/>
<connect gate="A" pin="C2+" pad="4"/>
<connect gate="A" pin="C2-" pad="5"/>
<connect gate="A" pin="DIN1" pad="11"/>
<connect gate="A" pin="DIN2" pad="10"/>
<connect gate="A" pin="DOUT1" pad="14"/>
<connect gate="A" pin="DOUT2" pad="7"/>
<connect gate="A" pin="GND" pad="15"/>
<connect gate="A" pin="RIN1" pad="13"/>
<connect gate="A" pin="RIN2" pad="8"/>
<connect gate="A" pin="ROUT1" pad="12"/>
<connect gate="A" pin="ROUT2" pad="9"/>
<connect gate="A" pin="V+" pad="2"/>
<connect gate="A" pin="V-" pad="6"/>
<connect gate="A" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS14C232CN"/>
<attribute name="OC_FARNELL" value="9490116"/>
<attribute name="OC_NEWARK" value="41K1797"/>
<attribute name="PACKAGE" value="DIP-16"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS14C232TM" prefix="U">
<description>Driver/Receiver</description>
<gates>
<gate name="A" symbol="DS14C232TM"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-16N">
<connects>
<connect gate="A" pin="C1+" pad="1"/>
<connect gate="A" pin="C1-" pad="3"/>
<connect gate="A" pin="C2+" pad="4"/>
<connect gate="A" pin="C2-" pad="5"/>
<connect gate="A" pin="DIN1" pad="11"/>
<connect gate="A" pin="DIN2" pad="10"/>
<connect gate="A" pin="DOUT1" pad="14"/>
<connect gate="A" pin="DOUT2" pad="7"/>
<connect gate="A" pin="GND" pad="15"/>
<connect gate="A" pin="RIN1" pad="13"/>
<connect gate="A" pin="RIN2" pad="8"/>
<connect gate="A" pin="ROUT1" pad="12"/>
<connect gate="A" pin="ROUT2" pad="9"/>
<connect gate="A" pin="V+" pad="2"/>
<connect gate="A" pin="V-" pad="6"/>
<connect gate="A" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS14C232TM"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K1798"/>
<attribute name="PACKAGE" value="SOIC-16"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS14C335MSA" prefix="U">
<description>Driver/Receiver</description>
<gates>
<gate name="A" symbol="DS14C335MSA"/>
</gates>
<devices>
<device name="" package="SOP65P770X200-28N">
<connects>
<connect gate="A" pin="C1+" pad="6"/>
<connect gate="A" pin="C1-" pad="24"/>
<connect gate="A" pin="C2+" pad="2"/>
<connect gate="A" pin="C2-" pad="4"/>
<connect gate="A" pin="C3+" pad="28"/>
<connect gate="A" pin="C3-" pad="26"/>
<connect gate="A" pin="DIN1" pad="7"/>
<connect gate="A" pin="DIN2" pad="8"/>
<connect gate="A" pin="DIN3" pad="9"/>
<connect gate="A" pin="DOUT1" pad="22"/>
<connect gate="A" pin="DOUT2" pad="21"/>
<connect gate="A" pin="DOUT3" pad="20"/>
<connect gate="A" pin="GND" pad="27"/>
<connect gate="A" pin="GND_2" pad="5"/>
<connect gate="A" pin="RIN1" pad="19"/>
<connect gate="A" pin="RIN2" pad="18"/>
<connect gate="A" pin="RIN3" pad="17"/>
<connect gate="A" pin="RIN4" pad="16"/>
<connect gate="A" pin="RIN5" pad="15"/>
<connect gate="A" pin="ROUT1" pad="10"/>
<connect gate="A" pin="ROUT2" pad="11"/>
<connect gate="A" pin="ROUT3" pad="12"/>
<connect gate="A" pin="ROUT4" pad="13"/>
<connect gate="A" pin="ROUT5" pad="14"/>
<connect gate="A" pin="SD" pad="23"/>
<connect gate="A" pin="V+" pad="1"/>
<connect gate="A" pin="V-" pad="25"/>
<connect gate="A" pin="VCC" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS14C335MSA"/>
<attribute name="OC_FARNELL" value="1685313"/>
<attribute name="OC_NEWARK" value="07B5202"/>
<attribute name="PACKAGE" value="SOP-28"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS14C535MSA" prefix="U">
<description>Driver/Receiver</description>
<gates>
<gate name="A" symbol="DS14C535MSA"/>
</gates>
<devices>
<device name="" package="SOP65P770X200-28N">
<connects>
<connect gate="A" pin="C1+" pad="2"/>
<connect gate="A" pin="C1-" pad="4"/>
<connect gate="A" pin="C2+" pad="28"/>
<connect gate="A" pin="C2-" pad="26"/>
<connect gate="A" pin="DIN1" pad="7"/>
<connect gate="A" pin="DIN2" pad="8"/>
<connect gate="A" pin="DIN3" pad="9"/>
<connect gate="A" pin="DOUT1" pad="22"/>
<connect gate="A" pin="DOUT2" pad="21"/>
<connect gate="A" pin="DOUT3" pad="20"/>
<connect gate="A" pin="GND" pad="27"/>
<connect gate="A" pin="GND_2" pad="5"/>
<connect gate="A" pin="N/C" pad="6"/>
<connect gate="A" pin="N/C_2" pad="24"/>
<connect gate="A" pin="RIN1" pad="19"/>
<connect gate="A" pin="RIN2" pad="18"/>
<connect gate="A" pin="RIN3" pad="17"/>
<connect gate="A" pin="RIN4" pad="16"/>
<connect gate="A" pin="RIN5" pad="15"/>
<connect gate="A" pin="ROUT1" pad="10"/>
<connect gate="A" pin="ROUT2" pad="11"/>
<connect gate="A" pin="ROUT3" pad="12"/>
<connect gate="A" pin="ROUT4" pad="13"/>
<connect gate="A" pin="ROUT5" pad="14"/>
<connect gate="A" pin="SD" pad="23"/>
<connect gate="A" pin="V+" pad="1"/>
<connect gate="A" pin="V-" pad="25"/>
<connect gate="A" pin="VCC" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS14C535MSA"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="92F243"/>
<attribute name="PACKAGE" value="SOP-28"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS14C88M" prefix="U">
<description>CMOS Line Driver</description>
<gates>
<gate name="A" symbol="DS14C88M"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="INA" pad="2"/>
<connect gate="A" pin="IN_B1" pad="4"/>
<connect gate="A" pin="IN_B2" pad="5"/>
<connect gate="A" pin="IN_C1" pad="9"/>
<connect gate="A" pin="IN_C2" pad="10"/>
<connect gate="A" pin="IN_D1" pad="12"/>
<connect gate="A" pin="IN_D2" pad="13"/>
<connect gate="A" pin="OUT_A" pad="3"/>
<connect gate="A" pin="OUT_B" pad="6"/>
<connect gate="A" pin="OUT_C" pad="8"/>
<connect gate="A" pin="OUT_D" pad="11"/>
<connect gate="A" pin="V+" pad="14"/>
<connect gate="A" pin="V-" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS14C88M"/>
<attribute name="OC_FARNELL" value="9487824"/>
<attribute name="OC_NEWARK" value="96K8875"/>
<attribute name="PACKAGE" value="14-SOIC"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS14C88N" prefix="U">
<description>Line Driver</description>
<gates>
<gate name="A" symbol="DS14C88N"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-14">
<connects>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="IN_A" pad="2"/>
<connect gate="A" pin="IN_B1" pad="4"/>
<connect gate="A" pin="IN_B2" pad="5"/>
<connect gate="A" pin="IN_C1" pad="9"/>
<connect gate="A" pin="IN_C2" pad="10"/>
<connect gate="A" pin="IN_D1" pad="12"/>
<connect gate="A" pin="IN_D2" pad="13"/>
<connect gate="A" pin="OUT_A" pad="3"/>
<connect gate="A" pin="OUT_B" pad="6"/>
<connect gate="A" pin="OUT_C" pad="8"/>
<connect gate="A" pin="OUT_D" pad="11"/>
<connect gate="A" pin="V+" pad="14"/>
<connect gate="A" pin="V-" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS14C88N"/>
<attribute name="OC_FARNELL" value="9487832"/>
<attribute name="OC_NEWARK" value="41K1810"/>
<attribute name="PACKAGE" value="14-DIP"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS14C89AM" prefix="U">
<description>CMOS Receiver</description>
<gates>
<gate name="A" symbol="DS14C89AM"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="INA" pad="1"/>
<connect gate="A" pin="INB" pad="4"/>
<connect gate="A" pin="INC" pad="10"/>
<connect gate="A" pin="IND" pad="13"/>
<connect gate="A" pin="NC" pad="12"/>
<connect gate="A" pin="NC_2" pad="2"/>
<connect gate="A" pin="NC_3" pad="5"/>
<connect gate="A" pin="NC_4" pad="9"/>
<connect gate="A" pin="OUTA" pad="3"/>
<connect gate="A" pin="OUTB" pad="6"/>
<connect gate="A" pin="OUTC" pad="8"/>
<connect gate="A" pin="OUTD" pad="11"/>
<connect gate="A" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS14C89AM"/>
<attribute name="OC_FARNELL" value="9487921"/>
<attribute name="OC_NEWARK" value="07B5208"/>
<attribute name="PACKAGE" value="14-SOIC"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS14C89AN" prefix="U">
<description>CMOS Receiver</description>
<gates>
<gate name="A" symbol="DS14C89AN"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-14">
<connects>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="INA" pad="1"/>
<connect gate="A" pin="INB" pad="4"/>
<connect gate="A" pin="INC" pad="10"/>
<connect gate="A" pin="IND" pad="13"/>
<connect gate="A" pin="NC" pad="12"/>
<connect gate="A" pin="NC_2" pad="9"/>
<connect gate="A" pin="NC_3" pad="5"/>
<connect gate="A" pin="NC_4" pad="2"/>
<connect gate="A" pin="OUTA" pad="3"/>
<connect gate="A" pin="OUTB" pad="6"/>
<connect gate="A" pin="OUTC" pad="8"/>
<connect gate="A" pin="OUTD" pad="11"/>
<connect gate="A" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS14C89AN"/>
<attribute name="OC_FARNELL" value="9487930"/>
<attribute name="OC_NEWARK" value="07B5210"/>
<attribute name="PACKAGE" value="DIP-14"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS15BR400TVS" prefix="U">
<description>Buffer/Repeater</description>
<gates>
<gate name="A" symbol="DS15BR400TVS"/>
</gates>
<devices>
<device name="" package="QFP50P900X900X120-48N">
<connects>
<connect gate="A" pin="GND" pad="18"/>
<connect gate="A" pin="GND_10" pad="9"/>
<connect gate="A" pin="GND_2" pad="37"/>
<connect gate="A" pin="GND_3" pad="38"/>
<connect gate="A" pin="GND_4" pad="43"/>
<connect gate="A" pin="GND_5" pad="23"/>
<connect gate="A" pin="GND_6" pad="44"/>
<connect gate="A" pin="GND_7" pad="24"/>
<connect gate="A" pin="GND_8" pad="8"/>
<connect gate="A" pin="GND_9" pad="17"/>
<connect gate="A" pin="IN0+" pad="13"/>
<connect gate="A" pin="IN0-" pad="14"/>
<connect gate="A" pin="IN1+" pad="15"/>
<connect gate="A" pin="IN1-" pad="16"/>
<connect gate="A" pin="IN2+" pad="19"/>
<connect gate="A" pin="IN2-" pad="20"/>
<connect gate="A" pin="IN3+" pad="21"/>
<connect gate="A" pin="IN3-" pad="22"/>
<connect gate="A" pin="N/C" pad="27"/>
<connect gate="A" pin="N/C_10" pad="26"/>
<connect gate="A" pin="N/C_2" pad="34"/>
<connect gate="A" pin="N/C_3" pad="35"/>
<connect gate="A" pin="N/C_4" pad="1"/>
<connect gate="A" pin="N/C_5" pad="36"/>
<connect gate="A" pin="N/C_6" pad="6"/>
<connect gate="A" pin="N/C_7" pad="30"/>
<connect gate="A" pin="N/C_8" pad="25"/>
<connect gate="A" pin="N/C_9" pad="31"/>
<connect gate="A" pin="OUT0+" pad="48"/>
<connect gate="A" pin="OUT0-" pad="47"/>
<connect gate="A" pin="OUT1+" pad="46"/>
<connect gate="A" pin="OUT1-" pad="45"/>
<connect gate="A" pin="OUT2+" pad="42"/>
<connect gate="A" pin="OUT2-" pad="41"/>
<connect gate="A" pin="OUT3+" pad="40"/>
<connect gate="A" pin="OUT3-" pad="39"/>
<connect gate="A" pin="PEM" pad="2"/>
<connect gate="A" pin="VDD" pad="33"/>
<connect gate="A" pin="VDD_10" pad="32"/>
<connect gate="A" pin="VDD_2" pad="28"/>
<connect gate="A" pin="VDD_3" pad="10"/>
<connect gate="A" pin="VDD_4" pad="3"/>
<connect gate="A" pin="VDD_5" pad="29"/>
<connect gate="A" pin="VDD_6" pad="4"/>
<connect gate="A" pin="VDD_7" pad="11"/>
<connect gate="A" pin="VDD_8" pad="5"/>
<connect gate="A" pin="VDD_9" pad="7"/>
<connect gate="A" pin="~PWDN" pad="12"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS15BR400TVS"/>
<attribute name="OC_FARNELL" value="1685362"/>
<attribute name="OC_NEWARK" value="32M0908"/>
<attribute name="PACKAGE" value="QFP-48"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS15EA101SQ" prefix="U">
<description>Adaptive Cable Equalizer</description>
<gates>
<gate name="A" symbol="DS15EA101SQ"/>
</gates>
<devices>
<device name="" package="QFN50P400X400X80-17N">
<connects>
<connect gate="A" pin="CAP+" pad="5"/>
<connect gate="A" pin="CAP-" pad="6"/>
<connect gate="A" pin="GND" pad="17"/>
<connect gate="A" pin="GND_2" pad="1"/>
<connect gate="A" pin="GND_3" pad="7"/>
<connect gate="A" pin="GND_4" pad="4"/>
<connect gate="A" pin="GND_5" pad="8"/>
<connect gate="A" pin="GND_6" pad="9"/>
<connect gate="A" pin="GND_7" pad="12"/>
<connect gate="A" pin="IN+" pad="2"/>
<connect gate="A" pin="IN-" pad="3"/>
<connect gate="A" pin="LOS" pad="15"/>
<connect gate="A" pin="OUT+" pad="11"/>
<connect gate="A" pin="OUT-" pad="10"/>
<connect gate="A" pin="VCC" pad="16"/>
<connect gate="A" pin="VCC_2" pad="13"/>
<connect gate="A" pin="~EN" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS15EA101SQ"/>
<attribute name="OC_FARNELL" value="1685579"/>
<attribute name="OC_NEWARK" value="32M0914"/>
<attribute name="PACKAGE" value="LLP-16"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS15MB200TSQ" prefix="U">
<description>LVDS  MUX/Buffer</description>
<gates>
<gate name="A" symbol="DS15MB200TSQ"/>
</gates>
<devices>
<device name="" package="QFN50P700X700X80-49N">
<connects>
<connect gate="A" pin="DAP" pad="49"/>
<connect gate="A" pin="ENA_0" pad="36"/>
<connect gate="A" pin="ENA_1" pad="13"/>
<connect gate="A" pin="ENB_0" pad="35"/>
<connect gate="A" pin="ENB_1" pad="14"/>
<connect gate="A" pin="ENL_0" pad="45"/>
<connect gate="A" pin="ENL_1" pad="4"/>
<connect gate="A" pin="GND" pad="47"/>
<connect gate="A" pin="GND_2" pad="2"/>
<connect gate="A" pin="GND_3" pad="46"/>
<connect gate="A" pin="GND_4" pad="3"/>
<connect gate="A" pin="LI_0+" pad="40"/>
<connect gate="A" pin="LI_0-" pad="39"/>
<connect gate="A" pin="LI_1+" pad="9"/>
<connect gate="A" pin="LI_1-" pad="10"/>
<connect gate="A" pin="LO_0+" pad="42"/>
<connect gate="A" pin="LO_0-" pad="41"/>
<connect gate="A" pin="LO_1+" pad="7"/>
<connect gate="A" pin="LO_1-" pad="8"/>
<connect gate="A" pin="MUX_S0" pad="38"/>
<connect gate="A" pin="MUX_S1" pad="11"/>
<connect gate="A" pin="N/C" pad="1"/>
<connect gate="A" pin="PREA_0" pad="26"/>
<connect gate="A" pin="PREA_1" pad="23"/>
<connect gate="A" pin="PREB_0" pad="25"/>
<connect gate="A" pin="PREB_1" pad="24"/>
<connect gate="A" pin="PREL_0" pad="44"/>
<connect gate="A" pin="PREL_1" pad="5"/>
<connect gate="A" pin="SIA_0+" pad="30"/>
<connect gate="A" pin="SIA_0-" pad="29"/>
<connect gate="A" pin="SIA_1+" pad="19"/>
<connect gate="A" pin="SIA_1-" pad="20"/>
<connect gate="A" pin="SIB_0+" pad="28"/>
<connect gate="A" pin="SIB_0-" pad="27"/>
<connect gate="A" pin="SIB_1+" pad="21"/>
<connect gate="A" pin="SIB_1-" pad="22"/>
<connect gate="A" pin="SOA_0+" pad="34"/>
<connect gate="A" pin="SOA_0-" pad="33"/>
<connect gate="A" pin="SOA_1+" pad="15"/>
<connect gate="A" pin="SOA_1-" pad="16"/>
<connect gate="A" pin="SOB_0+" pad="32"/>
<connect gate="A" pin="SOB_0-" pad="31"/>
<connect gate="A" pin="SOB_1+" pad="17"/>
<connect gate="A" pin="SOB_1-" pad="18"/>
<connect gate="A" pin="VDD" pad="43"/>
<connect gate="A" pin="VDD_2" pad="37"/>
<connect gate="A" pin="VDD_3" pad="48"/>
<connect gate="A" pin="VDD_4" pad="6"/>
<connect gate="A" pin="VDD_5" pad="12"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS15MB200TSQ"/>
<attribute name="OC_FARNELL" value="1694623"/>
<attribute name="OC_NEWARK" value="79K6191"/>
<attribute name="PACKAGE" value="LLP-48"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS16EV5110SQ" prefix="U">
<description>EQUALIZER</description>
<gates>
<gate name="A" symbol="DS16EV5110SQ"/>
</gates>
<devices>
<device name="" package="QFN50P700X700X80-49N">
<connects>
<connect gate="A" pin="BST_0" pad="23"/>
<connect gate="A" pin="BST_1" pad="14"/>
<connect gate="A" pin="BST_2" pad="37"/>
<connect gate="A" pin="CS" pad="16"/>
<connect gate="A" pin="C_IN+" pad="2"/>
<connect gate="A" pin="C_IN-" pad="1"/>
<connect gate="A" pin="C_OUT+" pad="35"/>
<connect gate="A" pin="C_OUT-" pad="36"/>
<connect gate="A" pin="D_IN0+" pad="5"/>
<connect gate="A" pin="D_IN0-" pad="4"/>
<connect gate="A" pin="D_IN1+" pad="9"/>
<connect gate="A" pin="D_IN1-" pad="8"/>
<connect gate="A" pin="D_IN2+" pad="12"/>
<connect gate="A" pin="D_IN2-" pad="11"/>
<connect gate="A" pin="D_OUT0+" pad="32"/>
<connect gate="A" pin="D_OUT0-" pad="33"/>
<connect gate="A" pin="D_OUT1+" pad="28"/>
<connect gate="A" pin="D_OUT1-" pad="29"/>
<connect gate="A" pin="D_OUT2+" pad="25"/>
<connect gate="A" pin="D_OUT2-" pad="26"/>
<connect gate="A" pin="EN" pad="44"/>
<connect gate="A" pin="FEB" pad="21"/>
<connect gate="A" pin="GND" pad="34"/>
<connect gate="A" pin="GND_2" pad="30"/>
<connect gate="A" pin="GND_3" pad="24"/>
<connect gate="A" pin="GND_4" pad="22"/>
<connect gate="A" pin="GND_5" pad="31"/>
<connect gate="A" pin="GND_6" pad="49"/>
<connect gate="A" pin="GND_7" pad="27"/>
<connect gate="A" pin="RESERVE" pad="19"/>
<connect gate="A" pin="RESERVE_10" pad="20"/>
<connect gate="A" pin="RESERVE_2" pad="48"/>
<connect gate="A" pin="RESERVE_3" pad="47"/>
<connect gate="A" pin="RESERVE_4" pad="43"/>
<connect gate="A" pin="RESERVE_5" pad="42"/>
<connect gate="A" pin="RESERVE_6" pad="41"/>
<connect gate="A" pin="RESERVE_7" pad="40"/>
<connect gate="A" pin="RESERVE_8" pad="39"/>
<connect gate="A" pin="RESERVE_9" pad="38"/>
<connect gate="A" pin="SD" pad="45"/>
<connect gate="A" pin="SDA" pad="18"/>
<connect gate="A" pin="SDC" pad="17"/>
<connect gate="A" pin="VDD" pad="7"/>
<connect gate="A" pin="VDD_2" pad="6"/>
<connect gate="A" pin="VDD_3" pad="10"/>
<connect gate="A" pin="VDD_4" pad="13"/>
<connect gate="A" pin="VDD_5" pad="46"/>
<connect gate="A" pin="VDD_6" pad="3"/>
<connect gate="A" pin="VDD_7" pad="15"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS16EV5110SQ"/>
<attribute name="OC_FARNELL" value="1685755"/>
<attribute name="OC_NEWARK" value="54M4546"/>
<attribute name="PACKAGE" value="None"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS16F95AJA">
<description>Transceiver</description>
<gates>
<gate name="A" symbol="DS16F95AJA"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-8">
<connects>
<connect gate="A" pin="A" pad="6"/>
<connect gate="A" pin="B" pad="7"/>
<connect gate="A" pin="DE" pad="3"/>
<connect gate="A" pin="DI" pad="4"/>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="RO" pad="1"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="~RE" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS16F95AJA"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="55R2914"/>
<attribute name="PACKAGE" value="DIP-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS22EV5110SQ" prefix="U">
<description>Equalizer</description>
<gates>
<gate name="A" symbol="DS22EV5110SQ"/>
</gates>
<devices>
<device name="" package="QFN50P700X700X80-49N">
<connects>
<connect gate="A" pin="BYPASS" pad="47"/>
<connect gate="A" pin="C_IN+" pad="2"/>
<connect gate="A" pin="C_IN-" pad="1"/>
<connect gate="A" pin="C_OUT+" pad="35"/>
<connect gate="A" pin="C_OUT-" pad="36"/>
<connect gate="A" pin="DE0" pad="43"/>
<connect gate="A" pin="DE1" pad="42"/>
<connect gate="A" pin="DIN1+" pad="9"/>
<connect gate="A" pin="D_IN0+" pad="5"/>
<connect gate="A" pin="D_IN0-" pad="4"/>
<connect gate="A" pin="D_IN1-" pad="8"/>
<connect gate="A" pin="D_IN2+" pad="12"/>
<connect gate="A" pin="D_IN2-" pad="11"/>
<connect gate="A" pin="D_OUT0+" pad="32"/>
<connect gate="A" pin="D_OUT0-" pad="33"/>
<connect gate="A" pin="D_OUT1+" pad="28"/>
<connect gate="A" pin="D_OUT1-" pad="29"/>
<connect gate="A" pin="D_OUT2+" pad="25"/>
<connect gate="A" pin="D_OUT2-" pad="26"/>
<connect gate="A" pin="EN" pad="44"/>
<connect gate="A" pin="EQ0" pad="39"/>
<connect gate="A" pin="EQ1" pad="38"/>
<connect gate="A" pin="EQ2" pad="37"/>
<connect gate="A" pin="GND" pad="31"/>
<connect gate="A" pin="GND_2" pad="49"/>
<connect gate="A" pin="GND_3" pad="27"/>
<connect gate="A" pin="GND_4" pad="22"/>
<connect gate="A" pin="GND_5" pad="30"/>
<connect gate="A" pin="GND_6" pad="24"/>
<connect gate="A" pin="GND_7" pad="34"/>
<connect gate="A" pin="LFN" pad="41"/>
<connect gate="A" pin="LFP" pad="40"/>
<connect gate="A" pin="LOCK" pad="14"/>
<connect gate="A" pin="RESRV" pad="23"/>
<connect gate="A" pin="RESRV_2" pad="16"/>
<connect gate="A" pin="RESRV_3" pad="18"/>
<connect gate="A" pin="RESRV_4" pad="17"/>
<connect gate="A" pin="RESRV_5" pad="19"/>
<connect gate="A" pin="RESRV_6" pad="21"/>
<connect gate="A" pin="RESRV_7" pad="20"/>
<connect gate="A" pin="SD" pad="45"/>
<connect gate="A" pin="VDD" pad="46"/>
<connect gate="A" pin="VDD_2" pad="7"/>
<connect gate="A" pin="VDD_3" pad="3"/>
<connect gate="A" pin="VDD_4" pad="10"/>
<connect gate="A" pin="VDD_5" pad="13"/>
<connect gate="A" pin="VDD_6" pad="6"/>
<connect gate="A" pin="VDD_7" pad="15"/>
<connect gate="A" pin="VOD_CRL" pad="48"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS22EV5110SQ"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="55R2917"/>
<attribute name="PACKAGE" value="LLP-48"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS25BR101TSD">
<description>LVDS Buffer</description>
<gates>
<gate name="A" symbol="DS25BR101TSD"/>
</gates>
<devices>
<device name="" package="DFN300X300X80-9N">
<connects>
<connect gate="A" pin="EQ" pad="1"/>
<connect gate="A" pin="GND" pad="9"/>
<connect gate="A" pin="IN+" pad="2"/>
<connect gate="A" pin="IN-" pad="3"/>
<connect gate="A" pin="NC" pad="5"/>
<connect gate="A" pin="OUT+" pad="7"/>
<connect gate="A" pin="OUT-" pad="6"/>
<connect gate="A" pin="PE" pad="4"/>
<connect gate="A" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS25BR101TSD"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="77R4470"/>
<attribute name="PACKAGE" value="LLP-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS25BR204TSQ" prefix="U">
<description>LVDS Repeater</description>
<gates>
<gate name="A" symbol="DS25BR204TSQ"/>
</gates>
<devices>
<device name="" package="QFN50P600X600X80-41N">
<connects>
<connect gate="A" pin="EQ1" pad="39"/>
<connect gate="A" pin="EQ2" pad="11"/>
<connect gate="A" pin="GND" pad="41"/>
<connect gate="A" pin="GND_2" pad="16"/>
<connect gate="A" pin="IN1+" pad="4"/>
<connect gate="A" pin="IN1-" pad="5"/>
<connect gate="A" pin="IN2+" pad="6"/>
<connect gate="A" pin="IN2-" pad="7"/>
<connect gate="A" pin="NC" pad="40"/>
<connect gate="A" pin="NC_2" pad="1"/>
<connect gate="A" pin="NC_3" pad="2"/>
<connect gate="A" pin="NC_4" pad="9"/>
<connect gate="A" pin="NC_5" pad="10"/>
<connect gate="A" pin="NC_6" pad="12"/>
<connect gate="A" pin="NC_7" pad="13"/>
<connect gate="A" pin="NC_8" pad="17"/>
<connect gate="A" pin="OUT0+" pad="29"/>
<connect gate="A" pin="OUT0-" pad="28"/>
<connect gate="A" pin="OUT1+" pad="27"/>
<connect gate="A" pin="OUT1-" pad="26"/>
<connect gate="A" pin="OUT2+" pad="24"/>
<connect gate="A" pin="OUT2-" pad="23"/>
<connect gate="A" pin="OUT3+" pad="22"/>
<connect gate="A" pin="OUT3-" pad="21"/>
<connect gate="A" pin="PE0" pad="31"/>
<connect gate="A" pin="PE1" pad="20"/>
<connect gate="A" pin="PE2" pad="19"/>
<connect gate="A" pin="PE3" pad="18"/>
<connect gate="A" pin="SEL_IN" pad="14"/>
<connect gate="A" pin="VDD" pad="30"/>
<connect gate="A" pin="VDD_2" pad="3"/>
<connect gate="A" pin="VDD_3" pad="8"/>
<connect gate="A" pin="VDD_4" pad="15"/>
<connect gate="A" pin="VDD_5" pad="25"/>
<connect gate="A" pin="~LOS1" pad="37"/>
<connect gate="A" pin="~LOS2" pad="36"/>
<connect gate="A" pin="~PWDN" pad="38"/>
<connect gate="A" pin="~PWDN0" pad="35"/>
<connect gate="A" pin="~PWDN1" pad="34"/>
<connect gate="A" pin="~PWDN2" pad="33"/>
<connect gate="A" pin="~PWDN3" pad="32"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS25BR204TSQ"/>
<attribute name="OC_FARNELL" value="1542529"/>
<attribute name="OC_NEWARK" value="94M6890"/>
<attribute name="PACKAGE" value="QFN-40"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS25BR400TSQ" prefix="U">
<description>Transceiver</description>
<gates>
<gate name="A" symbol="DS25BR400TSQ"/>
</gates>
<devices>
<device name="" package="QFN50P900X900X80-61N">
<connects>
<connect gate="A" pin="EP" pad="61"/>
<connect gate="A" pin="GND" pad="38"/>
<connect gate="A" pin="GND_2" pad="53"/>
<connect gate="A" pin="GND_3" pad="2"/>
<connect gate="A" pin="GND_4" pad="8"/>
<connect gate="A" pin="GND_5" pad="14"/>
<connect gate="A" pin="GND_6" pad="17"/>
<connect gate="A" pin="GND_7" pad="47"/>
<connect gate="A" pin="GND_8" pad="23"/>
<connect gate="A" pin="GND_9" pad="29"/>
<connect gate="A" pin="IA_0+" pad="58"/>
<connect gate="A" pin="IA_0-" pad="57"/>
<connect gate="A" pin="IA_1+" pad="6"/>
<connect gate="A" pin="IA_1-" pad="7"/>
<connect gate="A" pin="IA_2+" pad="10"/>
<connect gate="A" pin="IA_2-" pad="9"/>
<connect gate="A" pin="IA_3+" pad="18"/>
<connect gate="A" pin="IA_3-" pad="19"/>
<connect gate="A" pin="IB_0+" pad="51"/>
<connect gate="A" pin="IB_0-" pad="52"/>
<connect gate="A" pin="IB_1+" pad="43"/>
<connect gate="A" pin="IB_1-" pad="42"/>
<connect gate="A" pin="IB_2+" pad="33"/>
<connect gate="A" pin="IB_2-" pad="34"/>
<connect gate="A" pin="IB_3+" pad="25"/>
<connect gate="A" pin="IB_3-" pad="24"/>
<connect gate="A" pin="OA_0+" pad="48"/>
<connect gate="A" pin="OA_0-" pad="49"/>
<connect gate="A" pin="OA_1+" pad="40"/>
<connect gate="A" pin="OA_1-" pad="39"/>
<connect gate="A" pin="OA_2+" pad="36"/>
<connect gate="A" pin="OA_2-" pad="37"/>
<connect gate="A" pin="OA_3+" pad="28"/>
<connect gate="A" pin="OA_3-" pad="27"/>
<connect gate="A" pin="OB_0+" pad="55"/>
<connect gate="A" pin="OB_0-" pad="54"/>
<connect gate="A" pin="OB_1+" pad="3"/>
<connect gate="A" pin="OB_1-" pad="4"/>
<connect gate="A" pin="OB_2+" pad="13"/>
<connect gate="A" pin="OB_2-" pad="12"/>
<connect gate="A" pin="OB_3+" pad="21"/>
<connect gate="A" pin="OB_3-" pad="22"/>
<connect gate="A" pin="PREA_0" pad="15"/>
<connect gate="A" pin="PREA_1" pad="1"/>
<connect gate="A" pin="PREB_0" pad="31"/>
<connect gate="A" pin="PREB_1" pad="45"/>
<connect gate="A" pin="RSV" pad="59"/>
<connect gate="A" pin="VCC" pad="50"/>
<connect gate="A" pin="VCC_2" pad="5"/>
<connect gate="A" pin="VCC_3" pad="26"/>
<connect gate="A" pin="VCC_4" pad="11"/>
<connect gate="A" pin="VCC_5" pad="20"/>
<connect gate="A" pin="VCC_6" pad="56"/>
<connect gate="A" pin="VCC_7" pad="35"/>
<connect gate="A" pin="VCC_8" pad="41"/>
<connect gate="A" pin="~EQA" pad="60"/>
<connect gate="A" pin="~EQB" pad="16"/>
<connect gate="A" pin="~LB0" pad="46"/>
<connect gate="A" pin="~LB1" pad="44"/>
<connect gate="A" pin="~LB2" pad="32"/>
<connect gate="A" pin="~LB3" pad="30"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS25BR400TSQ"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="99K1993"/>
<attribute name="PACKAGE" value="LLP-60"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS25BR440TSQ" prefix="U">
<description>LVDS Buffer</description>
<gates>
<gate name="A" symbol="DS25BR440TSQ"/>
</gates>
<devices>
<device name="" package="QFN50P600X600X80-41N">
<connects>
<connect gate="A" pin="EQ0" pad="40"/>
<connect gate="A" pin="EQ1" pad="39"/>
<connect gate="A" pin="EQ2" pad="11"/>
<connect gate="A" pin="EQ3" pad="12"/>
<connect gate="A" pin="GND" pad="41"/>
<connect gate="A" pin="GND_2" pad="16"/>
<connect gate="A" pin="IN0+" pad="1"/>
<connect gate="A" pin="IN0-" pad="2"/>
<connect gate="A" pin="IN1+" pad="4"/>
<connect gate="A" pin="IN1-" pad="5"/>
<connect gate="A" pin="IN2+" pad="6"/>
<connect gate="A" pin="IN2-" pad="7"/>
<connect gate="A" pin="IN3+" pad="9"/>
<connect gate="A" pin="IN3-" pad="10"/>
<connect gate="A" pin="NC" pad="17"/>
<connect gate="A" pin="OUT0+" pad="29"/>
<connect gate="A" pin="OUT0-" pad="28"/>
<connect gate="A" pin="OUT1+" pad="27"/>
<connect gate="A" pin="OUT1-" pad="26"/>
<connect gate="A" pin="OUT2+" pad="24"/>
<connect gate="A" pin="OUT2-" pad="23"/>
<connect gate="A" pin="OUT3+" pad="22"/>
<connect gate="A" pin="OUT3-" pad="21"/>
<connect gate="A" pin="PE0" pad="31"/>
<connect gate="A" pin="PE1" pad="20"/>
<connect gate="A" pin="PE2" pad="19"/>
<connect gate="A" pin="PE3" pad="18"/>
<connect gate="A" pin="VDD" pad="15"/>
<connect gate="A" pin="VDD_2" pad="25"/>
<connect gate="A" pin="VDD_3" pad="3"/>
<connect gate="A" pin="VDD_4" pad="30"/>
<connect gate="A" pin="VDD_5" pad="8"/>
<connect gate="A" pin="~LOS0" pad="14"/>
<connect gate="A" pin="~LOS1" pad="37"/>
<connect gate="A" pin="~LOS2" pad="36"/>
<connect gate="A" pin="~LOS3" pad="13"/>
<connect gate="A" pin="~PWDN" pad="38"/>
<connect gate="A" pin="~PWDN0" pad="35"/>
<connect gate="A" pin="~PWDN1" pad="34"/>
<connect gate="A" pin="~PWDN2" pad="33"/>
<connect gate="A" pin="~PWDN3" pad="32"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS25BR440TSQ"/>
<attribute name="OC_FARNELL" value="1685403"/>
<attribute name="OC_NEWARK" value="95M8821"/>
<attribute name="PACKAGE" value="LPP-40"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS25CP102QSQ" prefix="U">
<description>Transmit Pre-Emphasis and Receive Equalization</description>
<gates>
<gate name="A" symbol="DS25CP102QSQ"/>
</gates>
<devices>
<device name="" package="DFN400X400X80-17N">
<connects>
<connect gate="A" pin="EN0" pad="14"/>
<connect gate="A" pin="EN1" pad="13"/>
<connect gate="A" pin="EQ" pad="6"/>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="GND_2" pad="17"/>
<connect gate="A" pin="IN0+" pad="1"/>
<connect gate="A" pin="IN0-" pad="2"/>
<connect gate="A" pin="IN1+" pad="3"/>
<connect gate="A" pin="IN1-" pad="4"/>
<connect gate="A" pin="OUT0+" pad="12"/>
<connect gate="A" pin="OUT0-" pad="11"/>
<connect gate="A" pin="OUT1+" pad="10"/>
<connect gate="A" pin="OUT1-" pad="9"/>
<connect gate="A" pin="PE" pad="15"/>
<connect gate="A" pin="SEL0" pad="7"/>
<connect gate="A" pin="SEL1" pad="8"/>
<connect gate="A" pin="VDD" pad="16"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS25CP102QSQ"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="07P4955"/>
<attribute name="PACKAGE" value="LLP-16"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS25CP102TSQ" prefix="U">
<description>Transmit Pre-Emphasis and Receive Equalization</description>
<gates>
<gate name="A" symbol="DS25CP102TSQ"/>
</gates>
<devices>
<device name="" package="QFN50P400X400X80-17N">
<connects>
<connect gate="A" pin="EN0" pad="14"/>
<connect gate="A" pin="EN1" pad="13"/>
<connect gate="A" pin="EQ" pad="6"/>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="GND_2" pad="17"/>
<connect gate="A" pin="IN0+" pad="1"/>
<connect gate="A" pin="IN0-" pad="2"/>
<connect gate="A" pin="IN1+" pad="3"/>
<connect gate="A" pin="IN1-" pad="4"/>
<connect gate="A" pin="OUT0+" pad="12"/>
<connect gate="A" pin="OUT0-" pad="11"/>
<connect gate="A" pin="OUT1+" pad="10"/>
<connect gate="A" pin="OUT1-" pad="9"/>
<connect gate="A" pin="PE" pad="15"/>
<connect gate="A" pin="SEL0" pad="7"/>
<connect gate="A" pin="SEL1" pad="8"/>
<connect gate="A" pin="VDD" pad="16"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS25CP102TSQ"/>
<attribute name="OC_FARNELL" value="1685353"/>
<attribute name="OC_NEWARK" value="64M6835"/>
<attribute name="PACKAGE" value="LLP-16"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS25CP104ATSQ" prefix="U">
<description>Crosspoint Switch with Transmit</description>
<gates>
<gate name="A" symbol="DS25CP104ATSQ"/>
</gates>
<devices>
<device name="" package="QFN50P600X600X80-41N">
<connects>
<connect gate="A" pin="EN_SMB" pad="17"/>
<connect gate="A" pin="EQ0" pad="40"/>
<connect gate="A" pin="EQ1" pad="39"/>
<connect gate="A" pin="EQ2" pad="11"/>
<connect gate="A" pin="EQ3" pad="12"/>
<connect gate="A" pin="GND" pad="41"/>
<connect gate="A" pin="GND_2" pad="16"/>
<connect gate="A" pin="IN0+" pad="1"/>
<connect gate="A" pin="IN0-" pad="2"/>
<connect gate="A" pin="IN1+" pad="4"/>
<connect gate="A" pin="IN1-" pad="5"/>
<connect gate="A" pin="IN2+" pad="6"/>
<connect gate="A" pin="IN2-" pad="7"/>
<connect gate="A" pin="IN3+" pad="9"/>
<connect gate="A" pin="IN3-" pad="10"/>
<connect gate="A" pin="OUT0+" pad="29"/>
<connect gate="A" pin="OUT0-" pad="28"/>
<connect gate="A" pin="OUT1+" pad="27"/>
<connect gate="A" pin="OUT1-" pad="26"/>
<connect gate="A" pin="OUT2+" pad="24"/>
<connect gate="A" pin="OUT2-" pad="23"/>
<connect gate="A" pin="OUT3+" pad="22"/>
<connect gate="A" pin="OUT3-" pad="21"/>
<connect gate="A" pin="PE0" pad="31"/>
<connect gate="A" pin="PE1" pad="20"/>
<connect gate="A" pin="PE2" pad="19"/>
<connect gate="A" pin="PE3" pad="18"/>
<connect gate="A" pin="S00/SCL" pad="37"/>
<connect gate="A" pin="S01/SDA" pad="36"/>
<connect gate="A" pin="S10/ADDR0" pad="35"/>
<connect gate="A" pin="S11/ADDR1" pad="34"/>
<connect gate="A" pin="S20/ADDR2" pad="33"/>
<connect gate="A" pin="S21/ADDR3" pad="32"/>
<connect gate="A" pin="S30" pad="13"/>
<connect gate="A" pin="S31" pad="14"/>
<connect gate="A" pin="VDD" pad="30"/>
<connect gate="A" pin="VDD_2" pad="3"/>
<connect gate="A" pin="VDD_3" pad="8"/>
<connect gate="A" pin="VDD_4" pad="15"/>
<connect gate="A" pin="VDD_5" pad="25"/>
<connect gate="A" pin="~PWDN" pad="38"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS25CP104ATSQ"/>
<attribute name="OC_FARNELL" value="1667413"/>
<attribute name="OC_NEWARK" value="12P9270"/>
<attribute name="PACKAGE" value="LLP-40"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS25CP152QSQ" prefix="U">
<description>LVDS Switch</description>
<gates>
<gate name="A" symbol="DS25CP152QSQ"/>
</gates>
<devices>
<device name="" package="DFN400X400X80-17N">
<connects>
<connect gate="A" pin="EN0" pad="14"/>
<connect gate="A" pin="EN1" pad="13"/>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="GND_2" pad="17"/>
<connect gate="A" pin="IN0+" pad="1"/>
<connect gate="A" pin="IN0-" pad="2"/>
<connect gate="A" pin="IN1+" pad="3"/>
<connect gate="A" pin="IN1-" pad="4"/>
<connect gate="A" pin="NC" pad="15"/>
<connect gate="A" pin="NC_2" pad="6"/>
<connect gate="A" pin="OUT0+" pad="12"/>
<connect gate="A" pin="OUT0-" pad="11"/>
<connect gate="A" pin="OUT1+" pad="10"/>
<connect gate="A" pin="OUT1-" pad="9"/>
<connect gate="A" pin="SEL0" pad="7"/>
<connect gate="A" pin="SEL1" pad="8"/>
<connect gate="A" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS25CP152QSQ"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="07P4957"/>
<attribute name="PACKAGE" value="LLP-16"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS25CP152TSQ" prefix="U">
<description>LVDS Switch</description>
<gates>
<gate name="A" symbol="DS25CP152TSQ"/>
</gates>
<devices>
<device name="" package="QFN50P400X400X80-17N">
<connects>
<connect gate="A" pin="EN0" pad="14"/>
<connect gate="A" pin="EN1" pad="13"/>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="GND_2" pad="17"/>
<connect gate="A" pin="IN0+" pad="1"/>
<connect gate="A" pin="IN0-" pad="2"/>
<connect gate="A" pin="IN1+" pad="3"/>
<connect gate="A" pin="IN1-" pad="4"/>
<connect gate="A" pin="NC" pad="15"/>
<connect gate="A" pin="NC_2" pad="6"/>
<connect gate="A" pin="OUT0+" pad="12"/>
<connect gate="A" pin="OUT0-" pad="11"/>
<connect gate="A" pin="OUT1+" pad="10"/>
<connect gate="A" pin="OUT1-" pad="9"/>
<connect gate="A" pin="SEL0" pad="7"/>
<connect gate="A" pin="SEL1" pad="8"/>
<connect gate="A" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS25CP152TSQ"/>
<attribute name="OC_FARNELL" value="1552433"/>
<attribute name="OC_NEWARK" value="78M7725"/>
<attribute name="PACKAGE" value="LLP-16"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS25MB200TSQ" prefix="U">
<description>MUX/Buffer</description>
<gates>
<gate name="A" symbol="DS25MB200TSQ"/>
</gates>
<devices>
<device name="" package="QFN50P700X700X80-49N">
<connects>
<connect gate="A" pin="EP" pad="49"/>
<connect gate="A" pin="GND" pad="32"/>
<connect gate="A" pin="GND_2" pad="5"/>
<connect gate="A" pin="GND_3" pad="17"/>
<connect gate="A" pin="GND_4" pad="41"/>
<connect gate="A" pin="GND_5" pad="11"/>
<connect gate="A" pin="LB0A" pad="47"/>
<connect gate="A" pin="LB0B" pad="48"/>
<connect gate="A" pin="LIB1A" pad="23"/>
<connect gate="A" pin="LIB1B" pad="24"/>
<connect gate="A" pin="LI_0+" pad="6"/>
<connect gate="A" pin="LI_0-" pad="7"/>
<connect gate="A" pin="LI_1+" pad="30"/>
<connect gate="A" pin="LI_1-" pad="31"/>
<connect gate="A" pin="LO_0+" pad="33"/>
<connect gate="A" pin="LO_0-" pad="34"/>
<connect gate="A" pin="LO_1+" pad="9"/>
<connect gate="A" pin="LO_1-" pad="10"/>
<connect gate="A" pin="MUX_S0" pad="37"/>
<connect gate="A" pin="MUX_S1" pad="13"/>
<connect gate="A" pin="PREL0" pad="12"/>
<connect gate="A" pin="PREL1" pad="1"/>
<connect gate="A" pin="PRES0" pad="36"/>
<connect gate="A" pin="PRES1" pad="25"/>
<connect gate="A" pin="RSV" pad="26"/>
<connect gate="A" pin="SIA_0+" pad="40"/>
<connect gate="A" pin="SIA_0-" pad="39"/>
<connect gate="A" pin="SIA_1+" pad="16"/>
<connect gate="A" pin="SIA_1-" pad="15"/>
<connect gate="A" pin="SIB_0+" pad="43"/>
<connect gate="A" pin="SIB_0-" pad="42"/>
<connect gate="A" pin="SIB_1+" pad="19"/>
<connect gate="A" pin="SIB_1-" pad="18"/>
<connect gate="A" pin="SOA_0+" pad="46"/>
<connect gate="A" pin="SOA_0-" pad="45"/>
<connect gate="A" pin="SOA_1+" pad="22"/>
<connect gate="A" pin="SOA_1-" pad="21"/>
<connect gate="A" pin="SOB_0+" pad="4"/>
<connect gate="A" pin="SOB_0-" pad="3"/>
<connect gate="A" pin="SOB_1+" pad="28"/>
<connect gate="A" pin="SOB_1-" pad="27"/>
<connect gate="A" pin="VCC" pad="38"/>
<connect gate="A" pin="VCC_2" pad="8"/>
<connect gate="A" pin="VCC_3" pad="35"/>
<connect gate="A" pin="VCC_4" pad="20"/>
<connect gate="A" pin="VCC_5" pad="14"/>
<connect gate="A" pin="VCC_6" pad="29"/>
<connect gate="A" pin="VCC_7" pad="44"/>
<connect gate="A" pin="VCC_8" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS25MB200TSQ"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="99K1995"/>
<attribute name="PACKAGE" value="Interface"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS26C31TM" prefix="U">
<description>Line Driver</description>
<gates>
<gate name="A" symbol="DS26C31TM"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-16N">
<connects>
<connect gate="A" pin="5V" pad="16"/>
<connect gate="A" pin="EN" pad="4"/>
<connect gate="A" pin="GND" pad="8"/>
<connect gate="A" pin="IN_A" pad="1"/>
<connect gate="A" pin="IN_B" pad="7"/>
<connect gate="A" pin="IN_C" pad="9"/>
<connect gate="A" pin="IN_D" pad="15"/>
<connect gate="A" pin="OUTA+" pad="2"/>
<connect gate="A" pin="OUTA-" pad="3"/>
<connect gate="A" pin="OUTB+" pad="6"/>
<connect gate="A" pin="OUTB-" pad="5"/>
<connect gate="A" pin="OUTC+" pad="10"/>
<connect gate="A" pin="OUTC-" pad="11"/>
<connect gate="A" pin="OUTD+" pad="14"/>
<connect gate="A" pin="OUTD-" pad="13"/>
<connect gate="A" pin="~EN" pad="12"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS26C31TM"/>
<attribute name="OC_FARNELL" value="9490060"/>
<attribute name="OC_NEWARK" value="07B5231"/>
<attribute name="PACKAGE" value="SOIC-16"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS26C31TN" prefix="U">
<description>Line Driver</description>
<gates>
<gate name="A" symbol="DS26C31TN"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-16">
<connects>
<connect gate="A" pin="5V" pad="16"/>
<connect gate="A" pin="CHANNEL_A_OUT" pad="3"/>
<connect gate="A" pin="CHANNEL_A_OUT_2" pad="2"/>
<connect gate="A" pin="CHANNEL_B_OUT" pad="6"/>
<connect gate="A" pin="CHANNEL_B_OUT_2" pad="5"/>
<connect gate="A" pin="CHANNEL_C_OUT" pad="11"/>
<connect gate="A" pin="CHANNEL_C_OUT_2" pad="10"/>
<connect gate="A" pin="CHANNEL_D_OUT" pad="14"/>
<connect gate="A" pin="CHANNEL_D_OUT_2" pad="13"/>
<connect gate="A" pin="EN" pad="4"/>
<connect gate="A" pin="GND" pad="8"/>
<connect gate="A" pin="IN_A" pad="1"/>
<connect gate="A" pin="IN_B" pad="7"/>
<connect gate="A" pin="IN_C" pad="9"/>
<connect gate="A" pin="IN_D" pad="15"/>
<connect gate="A" pin="~EN" pad="12"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS26C31TN"/>
<attribute name="OC_FARNELL" value="9487840"/>
<attribute name="OC_NEWARK" value="41K1829"/>
<attribute name="PACKAGE" value="16-DIP"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS26C32ATM" prefix="U">
<description>Line Receiver</description>
<gates>
<gate name="A" symbol="DS26C32ATM"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-16N">
<connects>
<connect gate="A" pin="+IN_A" pad="2"/>
<connect gate="A" pin="+IN_B" pad="14"/>
<connect gate="A" pin="+IN_C" pad="6"/>
<connect gate="A" pin="+IN_D" pad="10"/>
<connect gate="A" pin="-IN_A" pad="1"/>
<connect gate="A" pin="-IN_B" pad="15"/>
<connect gate="A" pin="-IN_C" pad="7"/>
<connect gate="A" pin="-IN_D" pad="9"/>
<connect gate="A" pin="EN_A" pad="4"/>
<connect gate="A" pin="GND" pad="8"/>
<connect gate="A" pin="OUT_A" pad="3"/>
<connect gate="A" pin="OUT_B" pad="13"/>
<connect gate="A" pin="OUT_C" pad="5"/>
<connect gate="A" pin="OUT_D" pad="11"/>
<connect gate="A" pin="VCC" pad="16"/>
<connect gate="A" pin="~EN" pad="12"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS26C32ATM"/>
<attribute name="OC_FARNELL" value="9490051"/>
<attribute name="OC_NEWARK" value="07B5234"/>
<attribute name="PACKAGE" value="SOIC-16"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS26LS31CM" prefix="U">
<description>Line Driver</description>
<gates>
<gate name="A" symbol="DS26LS31CM"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-16N">
<connects>
<connect gate="A" pin="5V" pad="16"/>
<connect gate="A" pin="EN" pad="4"/>
<connect gate="A" pin="GND" pad="8"/>
<connect gate="A" pin="IN_A" pad="1"/>
<connect gate="A" pin="IN_B" pad="7"/>
<connect gate="A" pin="IN_C" pad="9"/>
<connect gate="A" pin="IN_D" pad="15"/>
<connect gate="A" pin="OUT_A1" pad="3"/>
<connect gate="A" pin="OUT_A2" pad="2"/>
<connect gate="A" pin="OUT_B1" pad="5"/>
<connect gate="A" pin="OUT_B2" pad="6"/>
<connect gate="A" pin="OUT_C1" pad="11"/>
<connect gate="A" pin="OUT_C2" pad="10"/>
<connect gate="A" pin="OUT_D1" pad="13"/>
<connect gate="A" pin="OUT_D2" pad="14"/>
<connect gate="A" pin="~EN" pad="12"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS26LS31CM"/>
<attribute name="OC_FARNELL" value="9487859"/>
<attribute name="OC_NEWARK" value="07B5236"/>
<attribute name="PACKAGE" value="SOIC-16"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS26LS31CN" prefix="U">
<description>Line Driver</description>
<gates>
<gate name="A" symbol="DS26LS31CN"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-16">
<connects>
<connect gate="A" pin="5V" pad="16"/>
<connect gate="A" pin="CHANNEL_A_OUT" pad="3"/>
<connect gate="A" pin="CHANNEL_A_OUT_2" pad="2"/>
<connect gate="A" pin="CHANNEL_B_OUT" pad="6"/>
<connect gate="A" pin="CHANNEL_B_OUT_2" pad="5"/>
<connect gate="A" pin="CHANNEL_C_OUT" pad="11"/>
<connect gate="A" pin="CHANNEL_C_OUT_2" pad="10"/>
<connect gate="A" pin="CHANNEL_D_OUT" pad="14"/>
<connect gate="A" pin="CHANNEL_D_OUT_2" pad="13"/>
<connect gate="A" pin="EN" pad="4"/>
<connect gate="A" pin="GND" pad="8"/>
<connect gate="A" pin="IN_A" pad="1"/>
<connect gate="A" pin="IN_B" pad="7"/>
<connect gate="A" pin="IN_C" pad="9"/>
<connect gate="A" pin="IN_D" pad="15"/>
<connect gate="A" pin="~EN" pad="12"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS26LS31CN"/>
<attribute name="OC_FARNELL" value="9487867"/>
<attribute name="OC_NEWARK" value="41K1835"/>
<attribute name="PACKAGE" value="16-DIP"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS26LS32ACM" prefix="U">
<description>Line Receiver</description>
<gates>
<gate name="A" symbol="DS26LS32ACM"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-16N">
<connects>
<connect gate="A" pin="+IN_A" pad="2"/>
<connect gate="A" pin="+IN_B" pad="14"/>
<connect gate="A" pin="+IN_C" pad="6"/>
<connect gate="A" pin="+IN_D" pad="10"/>
<connect gate="A" pin="-IN_A" pad="1"/>
<connect gate="A" pin="-IN_B" pad="15"/>
<connect gate="A" pin="-IN_C" pad="7"/>
<connect gate="A" pin="-IN_D" pad="9"/>
<connect gate="A" pin="EN_A" pad="4"/>
<connect gate="A" pin="GND" pad="8"/>
<connect gate="A" pin="OUT_A" pad="3"/>
<connect gate="A" pin="OUT_B" pad="13"/>
<connect gate="A" pin="OUT_C" pad="5"/>
<connect gate="A" pin="OUT_D" pad="11"/>
<connect gate="A" pin="VCC" pad="16"/>
<connect gate="A" pin="~EN" pad="12"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS26LS32ACM"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K1836"/>
<attribute name="PACKAGE" value="SOIC-16"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS26LS32ACN" prefix="U">
<description>Receiver</description>
<gates>
<gate name="A" symbol="DS26LS32ACN"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-16">
<connects>
<connect gate="A" pin="+IN_A" pad="2"/>
<connect gate="A" pin="+IN_B" pad="14"/>
<connect gate="A" pin="+IN_C" pad="6"/>
<connect gate="A" pin="+IN_D" pad="10"/>
<connect gate="A" pin="-IN_A" pad="1"/>
<connect gate="A" pin="-IN_B" pad="15"/>
<connect gate="A" pin="-IN_C" pad="7"/>
<connect gate="A" pin="-IN_D" pad="9"/>
<connect gate="A" pin="EN_A" pad="4"/>
<connect gate="A" pin="GND" pad="8"/>
<connect gate="A" pin="OUT_A" pad="3"/>
<connect gate="A" pin="OUT_B" pad="13"/>
<connect gate="A" pin="OUT_C" pad="5"/>
<connect gate="A" pin="OUT_D" pad="11"/>
<connect gate="A" pin="VCC" pad="16"/>
<connect gate="A" pin="~EN" pad="12"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS26LS32ACN"/>
<attribute name="OC_FARNELL" value="9487956"/>
<attribute name="OC_NEWARK" value="41K1838"/>
<attribute name="PACKAGE" value="DIP-16"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS26LS32CM" prefix="U">
<description>Line Receiver</description>
<gates>
<gate name="A" symbol="DS26LS32CM"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-16N">
<connects>
<connect gate="A" pin="+IN_A" pad="2"/>
<connect gate="A" pin="+IN_B" pad="14"/>
<connect gate="A" pin="+IN_C" pad="6"/>
<connect gate="A" pin="+IN_D" pad="10"/>
<connect gate="A" pin="-IN_A" pad="1"/>
<connect gate="A" pin="-IN_B" pad="15"/>
<connect gate="A" pin="-IN_C" pad="7"/>
<connect gate="A" pin="-IN_D" pad="9"/>
<connect gate="A" pin="EN_A" pad="4"/>
<connect gate="A" pin="GND" pad="8"/>
<connect gate="A" pin="OUT_A" pad="3"/>
<connect gate="A" pin="OUT_B" pad="13"/>
<connect gate="A" pin="OUT_C" pad="5"/>
<connect gate="A" pin="OUT_D" pad="11"/>
<connect gate="A" pin="VCC" pad="16"/>
<connect gate="A" pin="~EN" pad="12"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS26LS32CM"/>
<attribute name="OC_FARNELL" value="9487964"/>
<attribute name="OC_NEWARK" value="-"/>
<attribute name="PACKAGE" value="SOIC-16"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS26LS32CN" prefix="U">
<description>Receiver</description>
<gates>
<gate name="A" symbol="DS26LS32CN"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-16">
<connects>
<connect gate="A" pin="+IN_A" pad="2"/>
<connect gate="A" pin="+IN_B" pad="14"/>
<connect gate="A" pin="+IN_C" pad="6"/>
<connect gate="A" pin="+IN_D" pad="10"/>
<connect gate="A" pin="-IN_A" pad="1"/>
<connect gate="A" pin="-IN_B" pad="15"/>
<connect gate="A" pin="-IN_C" pad="7"/>
<connect gate="A" pin="-IN_D" pad="9"/>
<connect gate="A" pin="EN_A" pad="4"/>
<connect gate="A" pin="GND" pad="8"/>
<connect gate="A" pin="OUT_A" pad="3"/>
<connect gate="A" pin="OUT_B" pad="13"/>
<connect gate="A" pin="OUT_C" pad="5"/>
<connect gate="A" pin="OUT_D" pad="11"/>
<connect gate="A" pin="VCC" pad="16"/>
<connect gate="A" pin="~EN" pad="12"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS26LS32CN"/>
<attribute name="OC_FARNELL" value="9487972"/>
<attribute name="OC_NEWARK" value="41K1841"/>
<attribute name="PACKAGE" value="DIP-16"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS32ELX0124SQ" prefix="U">
<description>Link Deserializer</description>
<gates>
<gate name="A" symbol="DS32ELX0124SQ"/>
</gates>
<devices>
<device name="" package="QFN50P700X700X80-49N">
<connects>
<connect gate="A" pin="GND" pad="49"/>
<connect gate="A" pin="GPIO0" pad="3"/>
<connect gate="A" pin="GPIO1" pad="4"/>
<connect gate="A" pin="GPIO2" pad="11"/>
<connect gate="A" pin="LF_CP" pad="27"/>
<connect gate="A" pin="LF_REF" pad="26"/>
<connect gate="A" pin="LT_EN" pad="2"/>
<connect gate="A" pin="NC" pad="29"/>
<connect gate="A" pin="NC_2" pad="8"/>
<connect gate="A" pin="NC_3" pad="23"/>
<connect gate="A" pin="NC_4" pad="24"/>
<connect gate="A" pin="NC_5" pad="9"/>
<connect gate="A" pin="NC_6" pad="13"/>
<connect gate="A" pin="NC_7" pad="10"/>
<connect gate="A" pin="RXCLKOUT+" pad="37"/>
<connect gate="A" pin="RXCLKOUT-" pad="38"/>
<connect gate="A" pin="RXIN0+" pad="16"/>
<connect gate="A" pin="RXIN0-" pad="17"/>
<connect gate="A" pin="RXIN1+" pad="19"/>
<connect gate="A" pin="RXIN1-" pad="20"/>
<connect gate="A" pin="RXOUT0+" pad="39"/>
<connect gate="A" pin="RXOUT0-" pad="40"/>
<connect gate="A" pin="RXOUT1+" pad="41"/>
<connect gate="A" pin="RXOUT1-" pad="42"/>
<connect gate="A" pin="RXOUT2+" pad="43"/>
<connect gate="A" pin="RXOUT2-" pad="44"/>
<connect gate="A" pin="RXOUT3+" pad="45"/>
<connect gate="A" pin="RXOUT3-" pad="46"/>
<connect gate="A" pin="RXOUT4+" pad="47"/>
<connect gate="A" pin="RXOUT4-" pad="48"/>
<connect gate="A" pin="RX_MUX_SEL" pad="12"/>
<connect gate="A" pin="SCK" pad="33"/>
<connect gate="A" pin="SDA" pad="32"/>
<connect gate="A" pin="SMB_CS" pad="34"/>
<connect gate="A" pin="TXOUT+" pad="21"/>
<connect gate="A" pin="TXOUT-" pad="22"/>
<connect gate="A" pin="VDD25" pad="35"/>
<connect gate="A" pin="VDD25_2" pad="7"/>
<connect gate="A" pin="VDD25_3" pad="25"/>
<connect gate="A" pin="VDD33" pad="15"/>
<connect gate="A" pin="VDD33_2" pad="36"/>
<connect gate="A" pin="VDD33_3" pad="1"/>
<connect gate="A" pin="VDD33_4" pad="18"/>
<connect gate="A" pin="VDDPLL" pad="28"/>
<connect gate="A" pin="VOD_CTRL" pad="14"/>
<connect gate="A" pin="~DC_B" pad="5"/>
<connect gate="A" pin="~LOCK" pad="31"/>
<connect gate="A" pin="~RESET" pad="30"/>
<connect gate="A" pin="~RS" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS32ELX0124SQ"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="07P4959"/>
<attribute name="PACKAGE" value="LLP-48"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS32ELX0421SQ" prefix="U">
<description>Link serializer</description>
<gates>
<gate name="A" symbol="DS32ELX0421SQ"/>
</gates>
<devices>
<device name="" package="QFN50P700X700X80-49N">
<connects>
<connect gate="A" pin="DE-EMP0" pad="9"/>
<connect gate="A" pin="DE-EMP1" pad="10"/>
<connect gate="A" pin="GND" pad="49"/>
<connect gate="A" pin="GPIO0" pad="3"/>
<connect gate="A" pin="GPIO1" pad="4"/>
<connect gate="A" pin="GPIO2" pad="11"/>
<connect gate="A" pin="LF_CP" pad="27"/>
<connect gate="A" pin="LF_REF" pad="26"/>
<connect gate="A" pin="NC" pad="24"/>
<connect gate="A" pin="NC_2" pad="2"/>
<connect gate="A" pin="NC_3" pad="21"/>
<connect gate="A" pin="NC_4" pad="22"/>
<connect gate="A" pin="NC_5" pad="8"/>
<connect gate="A" pin="NC_6" pad="13"/>
<connect gate="A" pin="NC_7" pad="23"/>
<connect gate="A" pin="RSVD" pad="29"/>
<connect gate="A" pin="SCK" pad="33"/>
<connect gate="A" pin="SDA" pad="32"/>
<connect gate="A" pin="SMB_CS" pad="34"/>
<connect gate="A" pin="TXCLKIN+" pad="37"/>
<connect gate="A" pin="TXCLKIN-" pad="38"/>
<connect gate="A" pin="TXIN0+" pad="39"/>
<connect gate="A" pin="TXIN0-" pad="40"/>
<connect gate="A" pin="TXIN1+" pad="41"/>
<connect gate="A" pin="TXIN1-" pad="42"/>
<connect gate="A" pin="TXIN2+" pad="43"/>
<connect gate="A" pin="TXIN2-" pad="44"/>
<connect gate="A" pin="TXIN3+" pad="45"/>
<connect gate="A" pin="TXIN3-" pad="46"/>
<connect gate="A" pin="TXIN4+" pad="47"/>
<connect gate="A" pin="TXIN4-" pad="48"/>
<connect gate="A" pin="TXOUT0+" pad="16"/>
<connect gate="A" pin="TXOUT0-" pad="20"/>
<connect gate="A" pin="TXOUT0-_2" pad="17"/>
<connect gate="A" pin="TXOUT1+" pad="19"/>
<connect gate="A" pin="TXOUT1_EN" pad="12"/>
<connect gate="A" pin="VDD25" pad="18"/>
<connect gate="A" pin="VDD25_2" pad="25"/>
<connect gate="A" pin="VDD25_3" pad="35"/>
<connect gate="A" pin="VDD25_4" pad="7"/>
<connect gate="A" pin="VDD25_5" pad="15"/>
<connect gate="A" pin="VDD33" pad="36"/>
<connect gate="A" pin="VDD33_2" pad="1"/>
<connect gate="A" pin="VDDPLL" pad="28"/>
<connect gate="A" pin="VOD_CTRL" pad="14"/>
<connect gate="A" pin="~DC_B" pad="5"/>
<connect gate="A" pin="~LOCK" pad="31"/>
<connect gate="A" pin="~RESET" pad="30"/>
<connect gate="A" pin="~RS" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS32ELX0421SQ"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="07P4962"/>
<attribute name="PACKAGE" value="LLP-48"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS32EV100SD" prefix="U">
<description>Programmable Single Equalizer</description>
<gates>
<gate name="A" symbol="DS32EV100SD"/>
</gates>
<devices>
<device name="" package="DFN400X300X80-15N">
<connects>
<connect gate="A" pin="BST_0" pad="8"/>
<connect gate="A" pin="BST_1" pad="7"/>
<connect gate="A" pin="BST_2" pad="14"/>
<connect gate="A" pin="GND" pad="15"/>
<connect gate="A" pin="GND_2" pad="10"/>
<connect gate="A" pin="GND_3" pad="2"/>
<connect gate="A" pin="GND_4" pad="13"/>
<connect gate="A" pin="GND_5" pad="6"/>
<connect gate="A" pin="GND_6" pad="9"/>
<connect gate="A" pin="IN+" pad="3"/>
<connect gate="A" pin="IN-" pad="4"/>
<connect gate="A" pin="NC" pad="1"/>
<connect gate="A" pin="OUT+" pad="12"/>
<connect gate="A" pin="OUT-" pad="11"/>
<connect gate="A" pin="VDD" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS32EV100SD"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="84M7964"/>
<attribute name="PACKAGE" value="LLP-14"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS32EV400SQ" prefix="U">
<description>QUAD Equalizer</description>
<gates>
<gate name="A" symbol="DS32EV400SQ"/>
</gates>
<devices>
<device name="" package="QFN50P700X700X80-49N">
<connects>
<connect gate="A" pin="BST_0" pad="23"/>
<connect gate="A" pin="BST_1" pad="14"/>
<connect gate="A" pin="BST_2" pad="37"/>
<connect gate="A" pin="CS" pad="16"/>
<connect gate="A" pin="EN0" pad="44"/>
<connect gate="A" pin="EN1" pad="42"/>
<connect gate="A" pin="EN2" pad="40"/>
<connect gate="A" pin="EN3" pad="38"/>
<connect gate="A" pin="FEB" pad="21"/>
<connect gate="A" pin="GND" pad="49"/>
<connect gate="A" pin="GND_2" pad="22"/>
<connect gate="A" pin="GND_3" pad="24"/>
<connect gate="A" pin="GND_4" pad="27"/>
<connect gate="A" pin="GND_5" pad="30"/>
<connect gate="A" pin="GND_6" pad="31"/>
<connect gate="A" pin="GND_7" pad="34"/>
<connect gate="A" pin="IN_0+" pad="1"/>
<connect gate="A" pin="IN_0-" pad="2"/>
<connect gate="A" pin="IN_1+" pad="4"/>
<connect gate="A" pin="IN_1-" pad="5"/>
<connect gate="A" pin="IN_2+" pad="8"/>
<connect gate="A" pin="IN_2-" pad="9"/>
<connect gate="A" pin="IN_3+" pad="11"/>
<connect gate="A" pin="IN_3-" pad="12"/>
<connect gate="A" pin="OUT_0+" pad="36"/>
<connect gate="A" pin="OUT_0-" pad="35"/>
<connect gate="A" pin="OUT_1+" pad="33"/>
<connect gate="A" pin="OUT_1-" pad="32"/>
<connect gate="A" pin="OUT_2+" pad="29"/>
<connect gate="A" pin="OUT_2-" pad="28"/>
<connect gate="A" pin="OUT_3+" pad="26"/>
<connect gate="A" pin="OUT_3-" pad="25"/>
<connect gate="A" pin="RESERVE" pad="20"/>
<connect gate="A" pin="RESERVE_2" pad="19"/>
<connect gate="A" pin="RESERVE_3" pad="48"/>
<connect gate="A" pin="RESERVE_4" pad="47"/>
<connect gate="A" pin="SD0" pad="45"/>
<connect gate="A" pin="SD1" pad="43"/>
<connect gate="A" pin="SD2" pad="41"/>
<connect gate="A" pin="SD3" pad="39"/>
<connect gate="A" pin="SDA" pad="18"/>
<connect gate="A" pin="SDC" pad="17"/>
<connect gate="A" pin="VDD" pad="15"/>
<connect gate="A" pin="VDD_2" pad="3"/>
<connect gate="A" pin="VDD_3" pad="6"/>
<connect gate="A" pin="VDD_4" pad="7"/>
<connect gate="A" pin="VDD_5" pad="10"/>
<connect gate="A" pin="VDD_6" pad="13"/>
<connect gate="A" pin="VDD_7" pad="46"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS32EV400SQ"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="60M5666"/>
<attribute name="PACKAGE" value="DisplayPort? Quad Equalizer"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS3486M" prefix="U">
<description>Literature</description>
<gates>
<gate name="A" symbol="DS3486M"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-16N">
<connects>
<connect gate="A" pin="GND" pad="8"/>
<connect gate="A" pin="IN_A" pad="1"/>
<connect gate="A" pin="IN_A_2" pad="2"/>
<connect gate="A" pin="IN_B" pad="14"/>
<connect gate="A" pin="IN_B_2" pad="15"/>
<connect gate="A" pin="IN_C" pad="6"/>
<connect gate="A" pin="IN_C_2" pad="7"/>
<connect gate="A" pin="IN_D" pad="9"/>
<connect gate="A" pin="IN_D_2" pad="10"/>
<connect gate="A" pin="OUT_A" pad="3"/>
<connect gate="A" pin="OUT_B" pad="13"/>
<connect gate="A" pin="OUT_C" pad="5"/>
<connect gate="A" pin="OUT_D" pad="11"/>
<connect gate="A" pin="TRI_STATE_CONTROL_A/C" pad="4"/>
<connect gate="A" pin="TRI_STATE_CONTROL_B/D" pad="12"/>
<connect gate="A" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS3486M"/>
<attribute name="OC_FARNELL" value="9490558"/>
<attribute name="OC_NEWARK" value="25M8961"/>
<attribute name="PACKAGE" value="SOIC-16"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS34C86TM" prefix="U">
<description>Line Receiver</description>
<gates>
<gate name="A" symbol="DS34C86TM"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-16N">
<connects>
<connect gate="A" pin="+IN_A" pad="2"/>
<connect gate="A" pin="+IN_B" pad="14"/>
<connect gate="A" pin="+IN_C" pad="6"/>
<connect gate="A" pin="+IN_D" pad="10"/>
<connect gate="A" pin="-IN_A" pad="1"/>
<connect gate="A" pin="-IN_B" pad="15"/>
<connect gate="A" pin="-IN_C" pad="7"/>
<connect gate="A" pin="-IN_D" pad="9"/>
<connect gate="A" pin="EN_A/C" pad="4"/>
<connect gate="A" pin="EN_B/D" pad="12"/>
<connect gate="A" pin="GND" pad="8"/>
<connect gate="A" pin="OUT_A" pad="3"/>
<connect gate="A" pin="OUT_B" pad="13"/>
<connect gate="A" pin="OUT_C" pad="5"/>
<connect gate="A" pin="OUT_D" pad="11"/>
<connect gate="A" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS34C86TM"/>
<attribute name="OC_FARNELL" value="9487980"/>
<attribute name="OC_NEWARK" value="41K1846"/>
<attribute name="PACKAGE" value="SOIC-16"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS34C87TM" prefix="U">
<description>Line Driver</description>
<gates>
<gate name="A" symbol="DS34C87TM"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-16N">
<connects>
<connect gate="A" pin="A/B_CTRL" pad="4"/>
<connect gate="A" pin="C/D_CTRL" pad="12"/>
<connect gate="A" pin="GND" pad="8"/>
<connect gate="A" pin="INA" pad="1"/>
<connect gate="A" pin="INB" pad="7"/>
<connect gate="A" pin="INC" pad="9"/>
<connect gate="A" pin="IND" pad="15"/>
<connect gate="A" pin="OUTA" pad="2"/>
<connect gate="A" pin="OUTB" pad="6"/>
<connect gate="A" pin="OUTC" pad="10"/>
<connect gate="A" pin="OUTD" pad="14"/>
<connect gate="A" pin="VCC" pad="16"/>
<connect gate="A" pin="~OUTA" pad="3"/>
<connect gate="A" pin="~OUTB" pad="5"/>
<connect gate="A" pin="~OUTC" pad="11"/>
<connect gate="A" pin="~OUTD" pad="13"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS34C87TM"/>
<attribute name="OC_FARNELL" value="9487875"/>
<attribute name="OC_NEWARK" value="96K8919"/>
<attribute name="PACKAGE" value="SOIC-16"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS34LV86TM" prefix="U">
<description>Line Receiver</description>
<gates>
<gate name="A" symbol="DS34LV86TM"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-16N">
<connects>
<connect gate="A" pin="EN" pad="12"/>
<connect gate="A" pin="EN_2" pad="4"/>
<connect gate="A" pin="GND" pad="8"/>
<connect gate="A" pin="RI1+" pad="2"/>
<connect gate="A" pin="RI1-" pad="1"/>
<connect gate="A" pin="RI2+" pad="6"/>
<connect gate="A" pin="RI2-" pad="7"/>
<connect gate="A" pin="RI3+" pad="10"/>
<connect gate="A" pin="RI3-" pad="9"/>
<connect gate="A" pin="RI4+" pad="14"/>
<connect gate="A" pin="RI4-" pad="15"/>
<connect gate="A" pin="RO1" pad="3"/>
<connect gate="A" pin="RO2" pad="5"/>
<connect gate="A" pin="RO3" pad="11"/>
<connect gate="A" pin="RO4" pad="13"/>
<connect gate="A" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS34LV86TM"/>
<attribute name="OC_FARNELL" value="1469000"/>
<attribute name="OC_NEWARK" value="41K1852"/>
<attribute name="PACKAGE" value="SOIC-16"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS34LV87TM" prefix="U">
<description>Line Driver</description>
<gates>
<gate name="A" symbol="DS34LV87TM"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-16N">
<connects>
<connect gate="A" pin="DI1" pad="1"/>
<connect gate="A" pin="DI2" pad="7"/>
<connect gate="A" pin="DI3" pad="9"/>
<connect gate="A" pin="DI4" pad="15"/>
<connect gate="A" pin="DO1+" pad="2"/>
<connect gate="A" pin="DO1-" pad="3"/>
<connect gate="A" pin="DO2+" pad="6"/>
<connect gate="A" pin="DO2-" pad="5"/>
<connect gate="A" pin="DO3+" pad="10"/>
<connect gate="A" pin="DO3-" pad="11"/>
<connect gate="A" pin="DO4+" pad="14"/>
<connect gate="A" pin="DO4-" pad="13"/>
<connect gate="A" pin="EN" pad="12"/>
<connect gate="A" pin="EN_2" pad="4"/>
<connect gate="A" pin="GND" pad="8"/>
<connect gate="A" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS34LV87TM"/>
<attribute name="OC_FARNELL" value="1468970"/>
<attribute name="OC_NEWARK" value="41K1854"/>
<attribute name="PACKAGE" value="SOIC-16"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS36276M" prefix="U">
<description>Transceiver</description>
<gates>
<gate name="A" symbol="DS36276M"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="DE" pad="3"/>
<connect gate="A" pin="DI" pad="4"/>
<connect gate="A" pin="DO/RI" pad="6"/>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="RO" pad="1"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="~DO/~RI" pad="7"/>
<connect gate="A" pin="~RE" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS36276M"/>
<attribute name="OC_FARNELL" value="1685503"/>
<attribute name="OC_NEWARK" value="41K1880"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS36277TM" prefix="U">
<description>Transceiver</description>
<gates>
<gate name="A" symbol="DS36277TM"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="DI" pad="4"/>
<connect gate="A" pin="DO/RI" pad="6"/>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="RO" pad="1"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="~DE" pad="3"/>
<connect gate="A" pin="~DO/~RI" pad="7"/>
<connect gate="A" pin="~RE" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS36277TM"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K1883"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS3691M" prefix="U">
<description>Line Drivers</description>
<gates>
<gate name="A" symbol="DS3691M"/>
</gates>
<devices>
<device name="" package="SOIC127P620X175-16N">
<connects>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="IN_A" pad="2"/>
<connect gate="A" pin="IN_B/DISABLE" pad="3"/>
<connect gate="A" pin="IN_C/DISABLE" pad="6"/>
<connect gate="A" pin="IN_D" pad="7"/>
<connect gate="A" pin="MODE_SEL" pad="4"/>
<connect gate="A" pin="OUT_A" pad="15"/>
<connect gate="A" pin="OUT_B" pad="14"/>
<connect gate="A" pin="OUT_C" pad="11"/>
<connect gate="A" pin="OUT_D" pad="10"/>
<connect gate="A" pin="RISE_TIME_CTRL_A" pad="16"/>
<connect gate="A" pin="RISE_TIME_CTRL_B" pad="13"/>
<connect gate="A" pin="RISE_TIME_CTRL_C" pad="12"/>
<connect gate="A" pin="RISE_TIME_CTRL_D" pad="9"/>
<connect gate="A" pin="VCC" pad="1"/>
<connect gate="A" pin="VEE" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS3691M"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="07B5301"/>
<attribute name="PACKAGE" value="SOIC-16"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS36950V" prefix="U">
<description>Transceiver</description>
<gates>
<gate name="A" symbol="DS36950V"/>
</gates>
<devices>
<device name="" package="PLCC127P991X991X457-20N">
<connects>
<connect gate="A" pin="DE1" pad="2"/>
<connect gate="A" pin="DE2" pad="5"/>
<connect gate="A" pin="DE3" pad="6"/>
<connect gate="A" pin="DE4" pad="9"/>
<connect gate="A" pin="DR1" pad="3"/>
<connect gate="A" pin="DR2" pad="4"/>
<connect gate="A" pin="DR3" pad="7"/>
<connect gate="A" pin="DR4" pad="8"/>
<connect gate="A" pin="GND" pad="11"/>
<connect gate="A" pin="OA1" pad="20"/>
<connect gate="A" pin="OA2" pad="18"/>
<connect gate="A" pin="OA3" pad="15"/>
<connect gate="A" pin="OA4" pad="13"/>
<connect gate="A" pin="OB1" pad="19"/>
<connect gate="A" pin="OB2" pad="17"/>
<connect gate="A" pin="OB3" pad="14"/>
<connect gate="A" pin="OB4" pad="12"/>
<connect gate="A" pin="VCC" pad="16"/>
<connect gate="A" pin="~RE4" pad="10"/>
<connect gate="A" pin="~REC" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS36950V"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="07B5311"/>
<attribute name="PACKAGE" value="PLCC-20"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS3695AM" prefix="U">
<description>Multipoint RS485/RS422 Transceivers</description>
<gates>
<gate name="A" symbol="DS3695AM"/>
</gates>
<devices>
<device name="" package="SOIC127P620X175-8N">
<connects>
<connect gate="A" pin="DE" pad="3"/>
<connect gate="A" pin="DI" pad="4"/>
<connect gate="A" pin="DO/RI" pad="6"/>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="RO" pad="1"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="~DO/~RI" pad="7"/>
<connect gate="A" pin="~RE" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS3695AM"/>
<attribute name="OC_FARNELL" value="9493409"/>
<attribute name="OC_NEWARK" value="41K1893"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS3695ATM" prefix="U">
<description>Multipoint RS485/RS422 Transceivers</description>
<gates>
<gate name="A" symbol="DS3695ATM"/>
</gates>
<devices>
<device name="" package="SOIC127P620X175-8N">
<connects>
<connect gate="A" pin="DE" pad="3"/>
<connect gate="A" pin="DI" pad="4"/>
<connect gate="A" pin="DO/RI" pad="6"/>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="RO" pad="1"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="~DO/~RI" pad="7"/>
<connect gate="A" pin="~RE" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS3695ATM"/>
<attribute name="OC_FARNELL" value="1798349"/>
<attribute name="OC_NEWARK" value="07B5307"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS3695N" prefix="U">
<description>Transceivers/Repeaters</description>
<gates>
<gate name="A" symbol="DS3695N"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-8">
<connects>
<connect gate="A" pin="DE" pad="3"/>
<connect gate="A" pin="DI" pad="4"/>
<connect gate="A" pin="DO/RI" pad="6"/>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="RO" pad="1"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="~DO/~RI" pad="7"/>
<connect gate="A" pin="~RE" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS3695N"/>
<attribute name="OC_FARNELL" value="9487166"/>
<attribute name="OC_NEWARK" value="07B5309"/>
<attribute name="PACKAGE" value="DIP-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS3695TN" prefix="U">
<description>Multipoint RS485/RS422 Transceivers/Repeaters</description>
<gates>
<gate name="A" symbol="DS3695TN"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-8">
<connects>
<connect gate="A" pin="DE" pad="3"/>
<connect gate="A" pin="DI" pad="4"/>
<connect gate="A" pin="DO/RI" pad="6"/>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="RO" pad="1"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="~DO/~RI" pad="7"/>
<connect gate="A" pin="~RE" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS3695TN"/>
<attribute name="OC_FARNELL" value="1685515"/>
<attribute name="OC_NEWARK" value="41K1898"/>
<attribute name="PACKAGE" value="DIP-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS36C200M" prefix="U">
<description>Transceiver</description>
<gates>
<gate name="A" symbol="DS36C200M"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="DE" pad="3"/>
<connect gate="A" pin="DI/R01" pad="1"/>
<connect gate="A" pin="DI/R02" pad="7"/>
<connect gate="A" pin="DO/RI1+" pad="13"/>
<connect gate="A" pin="DO/RI1-" pad="12"/>
<connect gate="A" pin="DO/RI2+" pad="10"/>
<connect gate="A" pin="DO/RI2-" pad="11"/>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="NC" pad="14"/>
<connect gate="A" pin="NC_2" pad="8"/>
<connect gate="A" pin="NC_3" pad="6"/>
<connect gate="A" pin="NC_4" pad="9"/>
<connect gate="A" pin="VCC" pad="2"/>
<connect gate="A" pin="~RE" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS36C200M"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K1864"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS36C278M" prefix="U">
<description>Transceiver</description>
<gates>
<gate name="A" symbol="DS36C278M"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="DE" pad="3"/>
<connect gate="A" pin="DI" pad="4"/>
<connect gate="A" pin="DO/RI" pad="6"/>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="RO" pad="1"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="~DO/~RI" pad="7"/>
<connect gate="A" pin="~RE" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS36C278M"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K1866"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS36C278TM" prefix="U">
<description>Transceiver</description>
<gates>
<gate name="A" symbol="DS36C278TM"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="DE" pad="3"/>
<connect gate="A" pin="DI" pad="4"/>
<connect gate="A" pin="DO/RI" pad="6"/>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="RO" pad="1"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="~DO/~RI" pad="7"/>
<connect gate="A" pin="~RE" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS36C278TM"/>
<attribute name="OC_FARNELL" value="9494022"/>
<attribute name="OC_NEWARK" value="41K1868"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS36C279M" prefix="U">
<description>Transceiver</description>
<gates>
<gate name="A" symbol="DS36C279M"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="DE" pad="3"/>
<connect gate="A" pin="DI" pad="4"/>
<connect gate="A" pin="DO/RI" pad="6"/>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="RO" pad="1"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="~DO/~RI" pad="7"/>
<connect gate="A" pin="~RE" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS36C279M"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="92F250"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS36C280TM" prefix="U">
<description>Transceiver</description>
<gates>
<gate name="A" symbol="DS36C280TM"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="DE/~RE" pad="3"/>
<connect gate="A" pin="DI" pad="4"/>
<connect gate="A" pin="DO/RI" pad="6"/>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="RO" pad="1"/>
<connect gate="A" pin="SR" pad="2"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="~DO/~RI" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS36C280TM"/>
<attribute name="OC_FARNELL" value="1215198"/>
<attribute name="OC_NEWARK" value="01M7381"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS38EP100SD" prefix="U">
<description>3.8 GBPS POWER SAVER EQUALIZER</description>
<gates>
<gate name="A" symbol="DS38EP100SD"/>
</gates>
<devices>
<device name="" package="DFN250X220X80-6N">
<connects>
<connect gate="A" pin="EP" pad="7"/>
<connect gate="A" pin="IOA+" pad="1"/>
<connect gate="A" pin="IOA-" pad="3"/>
<connect gate="A" pin="IOB+" pad="6"/>
<connect gate="A" pin="IOB-" pad="4"/>
<connect gate="A" pin="NC" pad="5"/>
<connect gate="A" pin="NC_2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS38EP100SD"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="54M4552"/>
<attribute name="PACKAGE" value="LLP-6"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS42BR400TSQ" prefix="U">
<description>Transceiver</description>
<gates>
<gate name="A" symbol="DS42BR400TSQ"/>
</gates>
<devices>
<device name="" package="QFN50P900X900X80-61N">
<connects>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="GND_10" pad="53"/>
<connect gate="A" pin="GND_2" pad="61"/>
<connect gate="A" pin="GND_3" pad="8"/>
<connect gate="A" pin="GND_4" pad="14"/>
<connect gate="A" pin="GND_5" pad="17"/>
<connect gate="A" pin="GND_6" pad="47"/>
<connect gate="A" pin="GND_7" pad="29"/>
<connect gate="A" pin="GND_8" pad="23"/>
<connect gate="A" pin="GND_9" pad="38"/>
<connect gate="A" pin="IA_0+" pad="58"/>
<connect gate="A" pin="IA_0-" pad="57"/>
<connect gate="A" pin="IA_1+" pad="6"/>
<connect gate="A" pin="IA_1-" pad="7"/>
<connect gate="A" pin="IA_2+" pad="10"/>
<connect gate="A" pin="IA_2-" pad="9"/>
<connect gate="A" pin="IA_3+" pad="18"/>
<connect gate="A" pin="IA_3-" pad="19"/>
<connect gate="A" pin="IB_0+" pad="51"/>
<connect gate="A" pin="IB_0-" pad="52"/>
<connect gate="A" pin="IB_1+" pad="43"/>
<connect gate="A" pin="IB_1-" pad="42"/>
<connect gate="A" pin="IB_2+" pad="33"/>
<connect gate="A" pin="IB_2-" pad="34"/>
<connect gate="A" pin="IB_3+" pad="25"/>
<connect gate="A" pin="IB_3-" pad="24"/>
<connect gate="A" pin="OA_0+" pad="48"/>
<connect gate="A" pin="OA_0-" pad="49"/>
<connect gate="A" pin="OA_1+" pad="40"/>
<connect gate="A" pin="OA_1-" pad="39"/>
<connect gate="A" pin="OA_2+" pad="36"/>
<connect gate="A" pin="OA_2-" pad="37"/>
<connect gate="A" pin="OA_3+" pad="28"/>
<connect gate="A" pin="OA_3-" pad="27"/>
<connect gate="A" pin="OB_0+" pad="55"/>
<connect gate="A" pin="OB_0-" pad="54"/>
<connect gate="A" pin="OB_1+" pad="3"/>
<connect gate="A" pin="OB_1-" pad="4"/>
<connect gate="A" pin="OB_2+" pad="13"/>
<connect gate="A" pin="OB_2-" pad="12"/>
<connect gate="A" pin="OB_3+" pad="21"/>
<connect gate="A" pin="OB_3-" pad="22"/>
<connect gate="A" pin="PREA_0" pad="15"/>
<connect gate="A" pin="PREA_1" pad="1"/>
<connect gate="A" pin="PREB_0" pad="31"/>
<connect gate="A" pin="PREB_1" pad="45"/>
<connect gate="A" pin="RSV" pad="59"/>
<connect gate="A" pin="VCC" pad="56"/>
<connect gate="A" pin="VCC_2" pad="5"/>
<connect gate="A" pin="VCC_3" pad="26"/>
<connect gate="A" pin="VCC_4" pad="11"/>
<connect gate="A" pin="VCC_5" pad="20"/>
<connect gate="A" pin="VCC_6" pad="50"/>
<connect gate="A" pin="VCC_7" pad="35"/>
<connect gate="A" pin="VCC_8" pad="41"/>
<connect gate="A" pin="~EQA" pad="60"/>
<connect gate="A" pin="~EQB" pad="16"/>
<connect gate="A" pin="~LB0" pad="46"/>
<connect gate="A" pin="~LB1" pad="44"/>
<connect gate="A" pin="~LB2" pad="32"/>
<connect gate="A" pin="~LB3" pad="30"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS42BR400TSQ"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="99K2018"/>
<attribute name="PACKAGE" value="LLP-60"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS481TM" prefix="U">
<description>Low Power RS-485/RS-422 Multipoint Transceiver</description>
<gates>
<gate name="A" symbol="DS481TM"/>
</gates>
<devices>
<device name="" package="SOIC127P620X175-8N">
<connects>
<connect gate="A" pin="A" pad="6"/>
<connect gate="A" pin="B" pad="7"/>
<connect gate="A" pin="DE" pad="3"/>
<connect gate="A" pin="DI" pad="4"/>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="RO" pad="1"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="~RE" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS481TM"/>
<attribute name="OC_FARNELL" value="1798307"/>
<attribute name="OC_NEWARK" value="75R1950"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS485M" prefix="U">
<description>RS-485/RS-422 Multipoint Transceiver</description>
<gates>
<gate name="A" symbol="DS485M"/>
</gates>
<devices>
<device name="" package="SOIC127P620X175-8N">
<connects>
<connect gate="A" pin="A" pad="6"/>
<connect gate="A" pin="B" pad="7"/>
<connect gate="A" pin="DE" pad="3"/>
<connect gate="A" pin="DI" pad="4"/>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="RO" pad="1"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="~RE" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS485M"/>
<attribute name="OC_FARNELL" value="1853246"/>
<attribute name="OC_NEWARK" value="41K1910"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS485N" prefix="U">
<description>RS-485/RS-422 Multipoint Transceiver</description>
<gates>
<gate name="A" symbol="DS485N"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-8">
<connects>
<connect gate="A" pin="A" pad="6"/>
<connect gate="A" pin="B" pad="7"/>
<connect gate="A" pin="DE" pad="3"/>
<connect gate="A" pin="DI" pad="4"/>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="RO" pad="1"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="~RE" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS485N"/>
<attribute name="OC_FARNELL" value="9490086"/>
<attribute name="OC_NEWARK" value="-"/>
<attribute name="PACKAGE" value="DIP-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS50EV401SQ" prefix="U">
<description>DS50EV401SQ E PACK</description>
<gates>
<gate name="A" symbol="DS50EV401SQ"/>
</gates>
<devices>
<device name="" package="QFN50P700X700X80-49N">
<connects>
<connect gate="A" pin="EN0" pad="44"/>
<connect gate="A" pin="EN1" pad="42"/>
<connect gate="A" pin="EN2" pad="40"/>
<connect gate="A" pin="EN3" pad="38"/>
<connect gate="A" pin="GND" pad="49"/>
<connect gate="A" pin="GND_2" pad="22"/>
<connect gate="A" pin="GND_3" pad="24"/>
<connect gate="A" pin="GND_4" pad="27"/>
<connect gate="A" pin="GND_5" pad="30"/>
<connect gate="A" pin="GND_6" pad="31"/>
<connect gate="A" pin="GND_7" pad="34"/>
<connect gate="A" pin="IN_0+" pad="1"/>
<connect gate="A" pin="IN_0-" pad="2"/>
<connect gate="A" pin="IN_1+" pad="4"/>
<connect gate="A" pin="IN_1-" pad="5"/>
<connect gate="A" pin="IN_2+" pad="8"/>
<connect gate="A" pin="IN_2-" pad="9"/>
<connect gate="A" pin="IN_3+" pad="11"/>
<connect gate="A" pin="IN_3-" pad="12"/>
<connect gate="A" pin="MODE" pad="14"/>
<connect gate="A" pin="OUT_0+" pad="36"/>
<connect gate="A" pin="OUT_0-" pad="35"/>
<connect gate="A" pin="OUT_1+" pad="33"/>
<connect gate="A" pin="OUT_1-" pad="32"/>
<connect gate="A" pin="OUT_2+" pad="29"/>
<connect gate="A" pin="OUT_2-" pad="28"/>
<connect gate="A" pin="OUT_3+" pad="26"/>
<connect gate="A" pin="OUT_3-" pad="25"/>
<connect gate="A" pin="RESERV" pad="16"/>
<connect gate="A" pin="RESERV_10" pad="17"/>
<connect gate="A" pin="RESERV_2" pad="48"/>
<connect gate="A" pin="RESERV_3" pad="47"/>
<connect gate="A" pin="RESERV_4" pad="37"/>
<connect gate="A" pin="RESERV_5" pad="23"/>
<connect gate="A" pin="RESERV_6" pad="21"/>
<connect gate="A" pin="RESERV_7" pad="20"/>
<connect gate="A" pin="RESERV_8" pad="19"/>
<connect gate="A" pin="RESERV_9" pad="18"/>
<connect gate="A" pin="SD0" pad="45"/>
<connect gate="A" pin="SD1" pad="43"/>
<connect gate="A" pin="SD2" pad="41"/>
<connect gate="A" pin="SD3" pad="39"/>
<connect gate="A" pin="VDD" pad="46"/>
<connect gate="A" pin="VDD_2" pad="3"/>
<connect gate="A" pin="VDD_3" pad="6"/>
<connect gate="A" pin="VDD_4" pad="7"/>
<connect gate="A" pin="VDD_5" pad="10"/>
<connect gate="A" pin="VDD_6" pad="13"/>
<connect gate="A" pin="VDD_7" pad="15"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS50EV401SQ"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="84M7968"/>
<attribute name="PACKAGE" value="LLP-48"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS50PCI401SQ">
<description>Express Repeater</description>
<gates>
<gate name="A" symbol="DS50PCI401SQ"/>
</gates>
<devices>
<device name="" package="QFN50P550X1000X80-55N">
<connects>
<connect gate="A" pin="DEMA0/SDA" pad="49"/>
<connect gate="A" pin="DEMA1/SCL" pad="50"/>
<connect gate="A" pin="DEMB0/AD1" pad="53"/>
<connect gate="A" pin="DEMB1/AD0" pad="54"/>
<connect gate="A" pin="ENRXDET" pad="26"/>
<connect gate="A" pin="ENSMB" pad="48"/>
<connect gate="A" pin="EP" pad="55"/>
<connect gate="A" pin="EQA0" pad="20"/>
<connect gate="A" pin="EQA1" pad="19"/>
<connect gate="A" pin="EQB0/AD3" pad="46"/>
<connect gate="A" pin="EQB1/AD2" pad="47"/>
<connect gate="A" pin="IA_0+" pad="10"/>
<connect gate="A" pin="IA_0-" pad="11"/>
<connect gate="A" pin="IA_1+" pad="12"/>
<connect gate="A" pin="IA_1-" pad="13"/>
<connect gate="A" pin="IA_2+" pad="15"/>
<connect gate="A" pin="IA_2-" pad="16"/>
<connect gate="A" pin="IA_3+" pad="17"/>
<connect gate="A" pin="IA_3-" pad="18"/>
<connect gate="A" pin="IB_0+" pad="45"/>
<connect gate="A" pin="IB_0-" pad="44"/>
<connect gate="A" pin="IB_1+" pad="43"/>
<connect gate="A" pin="IB_1-" pad="42"/>
<connect gate="A" pin="IB_2+" pad="40"/>
<connect gate="A" pin="IB_2-" pad="39"/>
<connect gate="A" pin="IB_3+" pad="38"/>
<connect gate="A" pin="IB_3-" pad="37"/>
<connect gate="A" pin="OA_0+" pad="35"/>
<connect gate="A" pin="OA_0-" pad="34"/>
<connect gate="A" pin="OA_1+" pad="33"/>
<connect gate="A" pin="OA_1-" pad="32"/>
<connect gate="A" pin="OA_2+" pad="31"/>
<connect gate="A" pin="OA_2-" pad="30"/>
<connect gate="A" pin="OA_3+" pad="29"/>
<connect gate="A" pin="OA_3-" pad="28"/>
<connect gate="A" pin="OB_0+" pad="1"/>
<connect gate="A" pin="OB_0-" pad="2"/>
<connect gate="A" pin="OB_1+" pad="3"/>
<connect gate="A" pin="OB_1-" pad="4"/>
<connect gate="A" pin="OB_2+" pad="5"/>
<connect gate="A" pin="OB_2-" pad="6"/>
<connect gate="A" pin="OB_3+" pad="7"/>
<connect gate="A" pin="OB_3-" pad="8"/>
<connect gate="A" pin="RATE" pad="21"/>
<connect gate="A" pin="RXDETA" pad="22"/>
<connect gate="A" pin="RXDETB" pad="23"/>
<connect gate="A" pin="SD_TH" pad="27"/>
<connect gate="A" pin="TXIDLEA" pad="24"/>
<connect gate="A" pin="TXIDLEB" pad="25"/>
<connect gate="A" pin="VDD" pad="51"/>
<connect gate="A" pin="VDD_2" pad="9"/>
<connect gate="A" pin="VDD_3" pad="14"/>
<connect gate="A" pin="VDD_4" pad="36"/>
<connect gate="A" pin="VDD_5" pad="41"/>
<connect gate="A" pin="~PRSNT" pad="52"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS64BR401SQ"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="55R2930"/>
<attribute name="PACKAGE" value="LLP-54"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS64BR401SQE" prefix="U">
<description>Repeater with Equalization</description>
<gates>
<gate name="A" symbol="DS64BR401SQE"/>
</gates>
<devices>
<device name="" package="QFN50P550X1000X80-55N">
<connects>
<connect gate="A" pin="DEMA0/SDA" pad="49"/>
<connect gate="A" pin="DEMA1/SCL" pad="50"/>
<connect gate="A" pin="DEMB0/AD1" pad="53"/>
<connect gate="A" pin="DEMB1/AD0" pad="54"/>
<connect gate="A" pin="ENSMB" pad="48"/>
<connect gate="A" pin="EP" pad="55"/>
<connect gate="A" pin="EQA0" pad="20"/>
<connect gate="A" pin="EQA1" pad="19"/>
<connect gate="A" pin="EQB0/AD3" pad="46"/>
<connect gate="A" pin="EQB1/AD2" pad="47"/>
<connect gate="A" pin="IA_0+" pad="10"/>
<connect gate="A" pin="IA_0-" pad="11"/>
<connect gate="A" pin="IA_1+" pad="12"/>
<connect gate="A" pin="IA_1-" pad="13"/>
<connect gate="A" pin="IA_2+" pad="15"/>
<connect gate="A" pin="IA_2-" pad="16"/>
<connect gate="A" pin="IA_3+" pad="17"/>
<connect gate="A" pin="IA_3-" pad="18"/>
<connect gate="A" pin="IB_0+" pad="45"/>
<connect gate="A" pin="IB_0-" pad="44"/>
<connect gate="A" pin="IB_1+" pad="43"/>
<connect gate="A" pin="IB_1-" pad="42"/>
<connect gate="A" pin="IB_2+" pad="40"/>
<connect gate="A" pin="IB_2-" pad="39"/>
<connect gate="A" pin="IB_3+" pad="38"/>
<connect gate="A" pin="IB_3-" pad="37"/>
<connect gate="A" pin="NC" pad="26"/>
<connect gate="A" pin="OA_0+" pad="35"/>
<connect gate="A" pin="OA_0-" pad="34"/>
<connect gate="A" pin="OA_1+" pad="33"/>
<connect gate="A" pin="OA_1-" pad="32"/>
<connect gate="A" pin="OA_2+" pad="31"/>
<connect gate="A" pin="OA_2-" pad="30"/>
<connect gate="A" pin="OA_3+" pad="29"/>
<connect gate="A" pin="OA_3-" pad="28"/>
<connect gate="A" pin="OB_0+" pad="1"/>
<connect gate="A" pin="OB_0-" pad="2"/>
<connect gate="A" pin="OB_1+" pad="3"/>
<connect gate="A" pin="OB_1-" pad="4"/>
<connect gate="A" pin="OB_2+" pad="5"/>
<connect gate="A" pin="OB_2-" pad="6"/>
<connect gate="A" pin="OB_3+" pad="7"/>
<connect gate="A" pin="OB_3-" pad="8"/>
<connect gate="A" pin="PWDN" pad="52"/>
<connect gate="A" pin="RATE" pad="21"/>
<connect gate="A" pin="SD_TH" pad="27"/>
<connect gate="A" pin="TXIDLEA" pad="24"/>
<connect gate="A" pin="TXIDLEB" pad="25"/>
<connect gate="A" pin="VDD" pad="9"/>
<connect gate="A" pin="VDD_2" pad="14"/>
<connect gate="A" pin="VDD_3" pad="36"/>
<connect gate="A" pin="VDD_4" pad="41"/>
<connect gate="A" pin="VDD_5" pad="51"/>
<connect gate="A" pin="VOD0" pad="22"/>
<connect gate="A" pin="VOD1" pad="23"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS64BR401SQE"/>
<attribute name="OC_FARNELL" value="1858088"/>
<attribute name="OC_NEWARK" value="27R1771"/>
<attribute name="PACKAGE" value="LLP-54"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS64EV100SD" prefix="U">
<description>EQUALIZER</description>
<gates>
<gate name="A" symbol="DS64EV100SD"/>
</gates>
<devices>
<device name="" package="DFN400X300X80-14N">
<connects>
<connect gate="A" pin="BST_0" pad="8"/>
<connect gate="A" pin="BST_1" pad="7"/>
<connect gate="A" pin="BST_2" pad="14"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="GND_2" pad="15"/>
<connect gate="A" pin="GND_3" pad="13"/>
<connect gate="A" pin="GND_4" pad="10"/>
<connect gate="A" pin="GND_5" pad="9"/>
<connect gate="A" pin="GND_6" pad="6"/>
<connect gate="A" pin="IN+" pad="3"/>
<connect gate="A" pin="IN-" pad="4"/>
<connect gate="A" pin="NC" pad="1"/>
<connect gate="A" pin="OUT+" pad="12"/>
<connect gate="A" pin="OUT-" pad="11"/>
<connect gate="A" pin="VDD" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS64EV100SD"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="84M7971"/>
<attribute name="PACKAGE" value="LLP-14"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS64EV400SQ" prefix="U">
<description>IC EQUALIZER QUAD PROGR</description>
<gates>
<gate name="A" symbol="DS64EV400SQ"/>
</gates>
<devices>
<device name="" package="QFN50P700X700X80-49N">
<connects>
<connect gate="A" pin="BST_0" pad="23"/>
<connect gate="A" pin="BST_1" pad="14"/>
<connect gate="A" pin="BST_2" pad="37"/>
<connect gate="A" pin="CS" pad="16"/>
<connect gate="A" pin="EN0" pad="44"/>
<connect gate="A" pin="EN1" pad="42"/>
<connect gate="A" pin="EN2" pad="40"/>
<connect gate="A" pin="EN3" pad="38"/>
<connect gate="A" pin="FEB" pad="21"/>
<connect gate="A" pin="GND" pad="31"/>
<connect gate="A" pin="GND_2" pad="24"/>
<connect gate="A" pin="GND_3" pad="22"/>
<connect gate="A" pin="GND_4" pad="49"/>
<connect gate="A" pin="GND_5" pad="27"/>
<connect gate="A" pin="GND_6" pad="30"/>
<connect gate="A" pin="GND_7" pad="34"/>
<connect gate="A" pin="IN_0+" pad="1"/>
<connect gate="A" pin="IN_0-" pad="2"/>
<connect gate="A" pin="IN_1+" pad="4"/>
<connect gate="A" pin="IN_1-" pad="5"/>
<connect gate="A" pin="IN_2+" pad="8"/>
<connect gate="A" pin="IN_2-" pad="9"/>
<connect gate="A" pin="IN_3+" pad="11"/>
<connect gate="A" pin="IN_3-" pad="12"/>
<connect gate="A" pin="OUT_0+" pad="36"/>
<connect gate="A" pin="OUT_0-" pad="35"/>
<connect gate="A" pin="OUT_1+" pad="33"/>
<connect gate="A" pin="OUT_1-" pad="32"/>
<connect gate="A" pin="OUT_2+" pad="29"/>
<connect gate="A" pin="OUT_2-" pad="28"/>
<connect gate="A" pin="OUT_3+" pad="26"/>
<connect gate="A" pin="OUT_3-" pad="25"/>
<connect gate="A" pin="RESERV" pad="20"/>
<connect gate="A" pin="RESERV_2" pad="47"/>
<connect gate="A" pin="RESERV_3" pad="48"/>
<connect gate="A" pin="RESERV_4" pad="19"/>
<connect gate="A" pin="SD0" pad="45"/>
<connect gate="A" pin="SD1" pad="43"/>
<connect gate="A" pin="SD2" pad="41"/>
<connect gate="A" pin="SD3" pad="39"/>
<connect gate="A" pin="SDA" pad="18"/>
<connect gate="A" pin="SDC" pad="17"/>
<connect gate="A" pin="VDD" pad="46"/>
<connect gate="A" pin="VDD_2" pad="6"/>
<connect gate="A" pin="VDD_3" pad="7"/>
<connect gate="A" pin="VDD_4" pad="10"/>
<connect gate="A" pin="VDD_5" pad="13"/>
<connect gate="A" pin="VDD_6" pad="3"/>
<connect gate="A" pin="VDD_7" pad="15"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS64EV400SQ"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="60M5667"/>
<attribute name="PACKAGE" value="LLP-48"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS75176BM" prefix="U">
<description>Transceiver</description>
<gates>
<gate name="A" symbol="DS75176BM"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="DE" pad="3"/>
<connect gate="A" pin="DI" pad="4"/>
<connect gate="A" pin="DO/RI" pad="6"/>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="RO" pad="1"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="~DO/~RI" pad="7"/>
<connect gate="A" pin="~RE" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS75176BM"/>
<attribute name="OC_FARNELL" value="1469011"/>
<attribute name="OC_NEWARK" value="41K1916"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS75176BN" prefix="U">
<description>Transceivers</description>
<gates>
<gate name="A" symbol="DS75176BN"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-8">
<connects>
<connect gate="A" pin="DE" pad="3"/>
<connect gate="A" pin="DI" pad="4"/>
<connect gate="A" pin="DO/RI" pad="6"/>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="RO" pad="1"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="~DO/~RI" pad="7"/>
<connect gate="A" pin="~RE" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS75176BN"/>
<attribute name="OC_FARNELL" value="9487190"/>
<attribute name="OC_NEWARK" value="41K1918"/>
<attribute name="PACKAGE" value="DIP-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS75176BTM" prefix="U">
<description>Transceiver</description>
<gates>
<gate name="A" symbol="DS75176BTM"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="DE" pad="3"/>
<connect gate="A" pin="DI" pad="4"/>
<connect gate="A" pin="DO/RI" pad="6"/>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="RO" pad="1"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="~DO/~RI" pad="7"/>
<connect gate="A" pin="~RE" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS75176BTM"/>
<attribute name="OC_FARNELL" value="1564748"/>
<attribute name="OC_NEWARK" value="07B5367"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS75176BTN" prefix="U">
<description>Transceivers</description>
<gates>
<gate name="A" symbol="DS75176BTN"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-8">
<connects>
<connect gate="A" pin="DE" pad="3"/>
<connect gate="A" pin="DI" pad="4"/>
<connect gate="A" pin="DO/RI" pad="6"/>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="RO" pad="1"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="~DO/~RI" pad="7"/>
<connect gate="A" pin="~RE" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS75176BTN"/>
<attribute name="OC_FARNELL" value="9487204"/>
<attribute name="OC_NEWARK" value="07B5369"/>
<attribute name="PACKAGE" value="DIP-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS80EP100SD" prefix="U">
<description>Power-Saver Equalizer</description>
<gates>
<gate name="A" symbol="DS80EP100SD"/>
</gates>
<devices>
<device name="" package="DFN220X250X80-7N">
<connects>
<connect gate="A" pin="EP" pad="7"/>
<connect gate="A" pin="IOA+" pad="1"/>
<connect gate="A" pin="IOA-" pad="3"/>
<connect gate="A" pin="IOB+" pad="6"/>
<connect gate="A" pin="IOB-" pad="4"/>
<connect gate="A" pin="NC" pad="5"/>
<connect gate="A" pin="NC_2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS80EP100SD"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="54M4556"/>
<attribute name="PACKAGE" value="LLP-6"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS8921M" prefix="U">
<description>Differential Line Driver</description>
<gates>
<gate name="A" symbol="DS8921M"/>
</gates>
<devices>
<device name="" package="SOIC127O620X175-8N">
<connects>
<connect gate="A" pin="DI" pad="3"/>
<connect gate="A" pin="DO+" pad="6"/>
<connect gate="A" pin="DO-" pad="5"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="RI+" pad="8"/>
<connect gate="A" pin="RI-" pad="7"/>
<connect gate="A" pin="RO" pad="2"/>
<connect gate="A" pin="VCC" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS8921M"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K1928"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS8921N" prefix="U">
<description>Line driver and receiver pair</description>
<gates>
<gate name="A" symbol="DS8921N"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-8">
<connects>
<connect gate="A" pin="DI" pad="3"/>
<connect gate="A" pin="DO+" pad="6"/>
<connect gate="A" pin="DO-" pad="5"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="RI+" pad="8"/>
<connect gate="A" pin="RI-" pad="7"/>
<connect gate="A" pin="RO" pad="2"/>
<connect gate="A" pin="VCC" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS8921N"/>
<attribute name="OC_FARNELL" value="9488014"/>
<attribute name="OC_NEWARK" value="DS8921N"/>
<attribute name="PACKAGE" value="DIP-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS8922AM" prefix="U">
<description>RS-422 Dual Differential Line Driver</description>
<gates>
<gate name="A" symbol="DS8922AM"/>
</gates>
<devices>
<device name="" package="SOIC127P620X175-16N">
<connects>
<connect gate="A" pin="DI1" pad="2"/>
<connect gate="A" pin="DI2" pad="7"/>
<connect gate="A" pin="DO1+" pad="14"/>
<connect gate="A" pin="DO1-" pad="13"/>
<connect gate="A" pin="DO2+" pad="11"/>
<connect gate="A" pin="DO2-" pad="12"/>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="RI1+" pad="16"/>
<connect gate="A" pin="RI1-" pad="15"/>
<connect gate="A" pin="RI2+" pad="9"/>
<connect gate="A" pin="RI2-" pad="10"/>
<connect gate="A" pin="RO1" pad="1"/>
<connect gate="A" pin="RO2" pad="8"/>
<connect gate="A" pin="VCC" pad="3"/>
<connect gate="A" pin="~EN1" pad="4"/>
<connect gate="A" pin="~EN2" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS8922AM"/>
<attribute name="OC_FARNELL" value="1469015"/>
<attribute name="OC_NEWARK" value="41K1931"/>
<attribute name="PACKAGE" value="SOIC-16"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS8923AM" prefix="U">
<description>RS-422 Dual Differential Line Driver</description>
<gates>
<gate name="A" symbol="DS8923AM"/>
</gates>
<devices>
<device name="" package="SOIC127P620X175-16N">
<connects>
<connect gate="A" pin="DI1" pad="2"/>
<connect gate="A" pin="DI2" pad="7"/>
<connect gate="A" pin="DO1+" pad="14"/>
<connect gate="A" pin="DO1-" pad="13"/>
<connect gate="A" pin="DO2+" pad="11"/>
<connect gate="A" pin="DO2-" pad="12"/>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="RI1+" pad="16"/>
<connect gate="A" pin="RI1-" pad="15"/>
<connect gate="A" pin="RI2+" pad="9"/>
<connect gate="A" pin="RI2-" pad="10"/>
<connect gate="A" pin="RO1" pad="1"/>
<connect gate="A" pin="RO2" pad="8"/>
<connect gate="A" pin="VCC" pad="3"/>
<connect gate="A" pin="~DEN" pad="4"/>
<connect gate="A" pin="~REN" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS8923AM"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K1936"/>
<attribute name="PACKAGE" value="SOIC-16"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS8923AN" prefix="U">
<description>Line Driver and Receiver</description>
<gates>
<gate name="A" symbol="DS8923AN"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-16">
<connects>
<connect gate="A" pin="DI1" pad="2"/>
<connect gate="A" pin="DI2" pad="7"/>
<connect gate="A" pin="DO1+" pad="14"/>
<connect gate="A" pin="DO1-" pad="13"/>
<connect gate="A" pin="DO2+" pad="11"/>
<connect gate="A" pin="DO2-" pad="12"/>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="RI1+" pad="16"/>
<connect gate="A" pin="RI1-" pad="15"/>
<connect gate="A" pin="RI2+" pad="9"/>
<connect gate="A" pin="RI2-" pad="10"/>
<connect gate="A" pin="RO1" pad="1"/>
<connect gate="A" pin="RO2" pad="8"/>
<connect gate="A" pin="VCC" pad="3"/>
<connect gate="A" pin="~DEN" pad="4"/>
<connect gate="A" pin="~REN" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS8923AN"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K1938"/>
<attribute name="PACKAGE" value="DIP-16"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS89C387TMEA" prefix="U">
<description>Line Driver</description>
<gates>
<gate name="A" symbol="DS89C387TMEA"/>
</gates>
<devices>
<device name="" package="SOP64P1035X274-48N">
<connects>
<connect gate="A" pin="DI_A" pad="47"/>
<connect gate="A" pin="DI_B" pad="46"/>
<connect gate="A" pin="DI_C" pad="7"/>
<connect gate="A" pin="DI_D" pad="8"/>
<connect gate="A" pin="DI_E" pad="40"/>
<connect gate="A" pin="DI_F" pad="39"/>
<connect gate="A" pin="DI_G" pad="15"/>
<connect gate="A" pin="DI_H" pad="16"/>
<connect gate="A" pin="DI_I" pad="32"/>
<connect gate="A" pin="DI_J" pad="31"/>
<connect gate="A" pin="DI_K" pad="22"/>
<connect gate="A" pin="DI_L" pad="23"/>
<connect gate="A" pin="DO*_A" pad="3"/>
<connect gate="A" pin="DO*_B" pad="44"/>
<connect gate="A" pin="DO*_C" pad="5"/>
<connect gate="A" pin="DO*_D" pad="42"/>
<connect gate="A" pin="DO*_E" pad="10"/>
<connect gate="A" pin="DO*_F" pad="36"/>
<connect gate="A" pin="DO*_G" pad="12"/>
<connect gate="A" pin="DO*_H" pad="34"/>
<connect gate="A" pin="DO*_I" pad="18"/>
<connect gate="A" pin="DO*_J" pad="29"/>
<connect gate="A" pin="DO*_K" pad="20"/>
<connect gate="A" pin="DO*_L" pad="27"/>
<connect gate="A" pin="DO_A" pad="2"/>
<connect gate="A" pin="DO_B" pad="45"/>
<connect gate="A" pin="DO_C" pad="6"/>
<connect gate="A" pin="DO_D" pad="41"/>
<connect gate="A" pin="DO_E" pad="9"/>
<connect gate="A" pin="DO_F" pad="37"/>
<connect gate="A" pin="DO_G" pad="13"/>
<connect gate="A" pin="DO_H" pad="33"/>
<connect gate="A" pin="DO_I" pad="17"/>
<connect gate="A" pin="DO_J" pad="30"/>
<connect gate="A" pin="DO_K" pad="21"/>
<connect gate="A" pin="DO_L" pad="26"/>
<connect gate="A" pin="EN_A,C" pad="4"/>
<connect gate="A" pin="EN_B,D" pad="43"/>
<connect gate="A" pin="EN_E,G" pad="11"/>
<connect gate="A" pin="EN_F,H" pad="35"/>
<connect gate="A" pin="EN_I,K" pad="19"/>
<connect gate="A" pin="EN_J,L" pad="28"/>
<connect gate="A" pin="GND" pad="24"/>
<connect gate="A" pin="GND_2" pad="14"/>
<connect gate="A" pin="NC" pad="48"/>
<connect gate="A" pin="NC_2" pad="1"/>
<connect gate="A" pin="NC_3" pad="25"/>
<connect gate="A" pin="VCC" pad="38"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS89C387TMEA"/>
<attribute name="OC_FARNELL" value="1685327"/>
<attribute name="OC_NEWARK" value="65K5419"/>
<attribute name="PACKAGE" value="SSOP-48"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS90C031BTM" prefix="U">
<description>Line Driver</description>
<gates>
<gate name="A" symbol="DS90C031BTM"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-16N">
<connects>
<connect gate="A" pin="DIN1" pad="1"/>
<connect gate="A" pin="DIN2" pad="7"/>
<connect gate="A" pin="DIN3" pad="9"/>
<connect gate="A" pin="DIN4" pad="15"/>
<connect gate="A" pin="DOUT1+" pad="2"/>
<connect gate="A" pin="DOUT1-" pad="3"/>
<connect gate="A" pin="DOUT2+" pad="6"/>
<connect gate="A" pin="DOUT2-" pad="5"/>
<connect gate="A" pin="DOUT3+" pad="10"/>
<connect gate="A" pin="DOUT3-" pad="11"/>
<connect gate="A" pin="DOUT4+" pad="14"/>
<connect gate="A" pin="DOUT4-" pad="13"/>
<connect gate="A" pin="EN" pad="4"/>
<connect gate="A" pin="GND" pad="8"/>
<connect gate="A" pin="VCC" pad="16"/>
<connect gate="A" pin="~EN" pad="12"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS90C031BTM"/>
<attribute name="OC_FARNELL" value="1468971"/>
<attribute name="OC_NEWARK" value="74C3585"/>
<attribute name="PACKAGE" value="SOIC-16"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS90C031TM" prefix="U">
<description>Line Driver</description>
<gates>
<gate name="A" symbol="DS90C031TM"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-16N">
<connects>
<connect gate="A" pin="DIN1" pad="1"/>
<connect gate="A" pin="DIN2" pad="7"/>
<connect gate="A" pin="DIN3" pad="9"/>
<connect gate="A" pin="DIN4" pad="15"/>
<connect gate="A" pin="DOUT1+" pad="2"/>
<connect gate="A" pin="DOUT1-" pad="3"/>
<connect gate="A" pin="DOUT2+" pad="6"/>
<connect gate="A" pin="DOUT2-" pad="5"/>
<connect gate="A" pin="DOUT3+" pad="10"/>
<connect gate="A" pin="DOUT3-" pad="11"/>
<connect gate="A" pin="DOUT4+" pad="14"/>
<connect gate="A" pin="DOUT4-" pad="13"/>
<connect gate="A" pin="EN" pad="4"/>
<connect gate="A" pin="GND" pad="8"/>
<connect gate="A" pin="VCC" pad="16"/>
<connect gate="A" pin="~EN" pad="12"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS90C031TM"/>
<attribute name="OC_FARNELL" value="9490108"/>
<attribute name="OC_NEWARK" value="92F258"/>
<attribute name="PACKAGE" value="SOIC-16"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS90C032BTM" prefix="U">
<description>Line Receiver</description>
<gates>
<gate name="A" symbol="DS90C032BTM"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-16N">
<connects>
<connect gate="A" pin="EN" pad="4"/>
<connect gate="A" pin="GND" pad="8"/>
<connect gate="A" pin="RIN1+" pad="2"/>
<connect gate="A" pin="RIN1-" pad="1"/>
<connect gate="A" pin="RIN2+" pad="6"/>
<connect gate="A" pin="RIN2-" pad="7"/>
<connect gate="A" pin="RIN3+" pad="10"/>
<connect gate="A" pin="RIN3-" pad="9"/>
<connect gate="A" pin="RIN4+" pad="14"/>
<connect gate="A" pin="RIN4-" pad="15"/>
<connect gate="A" pin="ROUT1" pad="3"/>
<connect gate="A" pin="ROUT2" pad="5"/>
<connect gate="A" pin="ROUT3" pad="11"/>
<connect gate="A" pin="ROUT4" pad="13"/>
<connect gate="A" pin="VCC" pad="16"/>
<connect gate="A" pin="~EN" pad="12"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS90C032BTM"/>
<attribute name="OC_FARNELL" value="1469001"/>
<attribute name="OC_NEWARK" value="41K2029"/>
<attribute name="PACKAGE" value="SOIC-16"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS90C032TM" prefix="U">
<description>Line Receiver</description>
<gates>
<gate name="A" symbol="DS90C032TM"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-16N">
<connects>
<connect gate="A" pin="EN" pad="4"/>
<connect gate="A" pin="GND" pad="8"/>
<connect gate="A" pin="RIN1+" pad="2"/>
<connect gate="A" pin="RIN1-" pad="1"/>
<connect gate="A" pin="RIN2+" pad="6"/>
<connect gate="A" pin="RIN2-" pad="7"/>
<connect gate="A" pin="RIN3+" pad="10"/>
<connect gate="A" pin="RIN3-" pad="9"/>
<connect gate="A" pin="RIN4+" pad="14"/>
<connect gate="A" pin="RIN4-" pad="15"/>
<connect gate="A" pin="ROUT1" pad="3"/>
<connect gate="A" pin="ROUT2" pad="5"/>
<connect gate="A" pin="ROUT3" pad="11"/>
<connect gate="A" pin="ROUT4" pad="13"/>
<connect gate="A" pin="VCC" pad="16"/>
<connect gate="A" pin="~EN" pad="12"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS90C032TM"/>
<attribute name="OC_FARNELL" value="9490094"/>
<attribute name="OC_NEWARK" value="92F259"/>
<attribute name="PACKAGE" value="SOIC-16"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS90C124QVS" prefix="U">
<description>Serializer and Deserializer</description>
<gates>
<gate name="A" symbol="DS90C124QVS"/>
</gates>
<devices>
<device name="" package="QFP50P900X900X120-48N">
<connects>
<connect gate="A" pin="LOCK" pad="17"/>
<connect gate="A" pin="RCLK" pad="18"/>
<connect gate="A" pin="REN" pad="48"/>
<connect gate="A" pin="RESRVD" pad="2"/>
<connect gate="A" pin="RIN+" pad="41"/>
<connect gate="A" pin="RIN-" pad="42"/>
<connect gate="A" pin="ROUT[0]" pad="34"/>
<connect gate="A" pin="ROUT[10]" pad="22"/>
<connect gate="A" pin="ROUT[11]" pad="21"/>
<connect gate="A" pin="ROUT[12]" pad="16"/>
<connect gate="A" pin="ROUT[13]" pad="15"/>
<connect gate="A" pin="ROUT[14]" pad="14"/>
<connect gate="A" pin="ROUT[15]" pad="13"/>
<connect gate="A" pin="ROUT[16]" pad="12"/>
<connect gate="A" pin="ROUT[17]" pad="11"/>
<connect gate="A" pin="ROUT[18]" pad="10"/>
<connect gate="A" pin="ROUT[19]" pad="9"/>
<connect gate="A" pin="ROUT[1]" pad="33"/>
<connect gate="A" pin="ROUT[20]" pad="6"/>
<connect gate="A" pin="ROUT[21]" pad="5"/>
<connect gate="A" pin="ROUT[22]" pad="4"/>
<connect gate="A" pin="ROUT[23]" pad="3"/>
<connect gate="A" pin="ROUT[2]" pad="32"/>
<connect gate="A" pin="ROUT[3]" pad="31"/>
<connect gate="A" pin="ROUT[4]" pad="28"/>
<connect gate="A" pin="ROUT[5]" pad="27"/>
<connect gate="A" pin="ROUT[6]" pad="26"/>
<connect gate="A" pin="ROUT[7]" pad="25"/>
<connect gate="A" pin="ROUT[8]" pad="24"/>
<connect gate="A" pin="ROUT[9]" pad="23"/>
<connect gate="A" pin="RPWDNB" pad="1"/>
<connect gate="A" pin="RRFB" pad="43"/>
<connect gate="A" pin="VDDIR" pad="39"/>
<connect gate="A" pin="VDDOR1" pad="30"/>
<connect gate="A" pin="VDDOR2" pad="20"/>
<connect gate="A" pin="VDDOR3" pad="7"/>
<connect gate="A" pin="VDDPR0" pad="47"/>
<connect gate="A" pin="VDDPR1" pad="45"/>
<connect gate="A" pin="VDDR0" pad="36"/>
<connect gate="A" pin="VDDR1" pad="37"/>
<connect gate="A" pin="VSSIR" pad="40"/>
<connect gate="A" pin="VSSOR1" pad="29"/>
<connect gate="A" pin="VSSOR2" pad="19"/>
<connect gate="A" pin="VSSOR3" pad="8"/>
<connect gate="A" pin="VSSPR0" pad="46"/>
<connect gate="A" pin="VSSPR1" pad="44"/>
<connect gate="A" pin="VSSR0" pad="35"/>
<connect gate="A" pin="VSSR1" pad="38"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS90C124QVS"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="11N9007"/>
<attribute name="PACKAGE" value="QFP-48"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS90C241QVS" prefix="U">
<description>Serializer and Deserializer</description>
<gates>
<gate name="A" symbol="DS90C241QVS"/>
</gates>
<devices>
<device name="" package="QFP50P900X900X120-48N">
<connects>
<connect gate="A" pin="DCAOFF" pad="5"/>
<connect gate="A" pin="DCBOFF" pad="8"/>
<connect gate="A" pin="DEN" pad="18"/>
<connect gate="A" pin="DIN0" pad="25"/>
<connect gate="A" pin="DIN1" pad="26"/>
<connect gate="A" pin="DIN10" pad="37"/>
<connect gate="A" pin="DIN11" pad="38"/>
<connect gate="A" pin="DIN12" pad="39"/>
<connect gate="A" pin="DIN13" pad="40"/>
<connect gate="A" pin="DIN14" pad="41"/>
<connect gate="A" pin="DIN15" pad="44"/>
<connect gate="A" pin="DIN16" pad="45"/>
<connect gate="A" pin="DIN17" pad="46"/>
<connect gate="A" pin="DIN18" pad="47"/>
<connect gate="A" pin="DIN19" pad="48"/>
<connect gate="A" pin="DIN2" pad="27"/>
<connect gate="A" pin="DIN20" pad="1"/>
<connect gate="A" pin="DIN21" pad="2"/>
<connect gate="A" pin="DIN22" pad="3"/>
<connect gate="A" pin="DIN23" pad="4"/>
<connect gate="A" pin="DIN3" pad="28"/>
<connect gate="A" pin="DIN4" pad="29"/>
<connect gate="A" pin="DIN5" pad="32"/>
<connect gate="A" pin="DIN6" pad="33"/>
<connect gate="A" pin="DIN7" pad="34"/>
<connect gate="A" pin="DIN8" pad="35"/>
<connect gate="A" pin="DIN9" pad="36"/>
<connect gate="A" pin="DOUT+" pad="20"/>
<connect gate="A" pin="DOUT-" pad="19"/>
<connect gate="A" pin="PRE" pad="23"/>
<connect gate="A" pin="RESRVD" pad="13"/>
<connect gate="A" pin="TCLK" pad="10"/>
<connect gate="A" pin="TPWDNB" pad="9"/>
<connect gate="A" pin="TRFB" pad="11"/>
<connect gate="A" pin="VDDDR" pad="22"/>
<connect gate="A" pin="VDDIT" pad="42"/>
<connect gate="A" pin="VDDL" pad="7"/>
<connect gate="A" pin="VDDPT0" pad="16"/>
<connect gate="A" pin="VDDPT1" pad="14"/>
<connect gate="A" pin="VDDT" pad="30"/>
<connect gate="A" pin="VODSEL" pad="12"/>
<connect gate="A" pin="VSS" pad="24"/>
<connect gate="A" pin="VSSDR" pad="21"/>
<connect gate="A" pin="VSSIT" pad="43"/>
<connect gate="A" pin="VSSL" pad="6"/>
<connect gate="A" pin="VSSPT0" pad="17"/>
<connect gate="A" pin="VSSPT1" pad="15"/>
<connect gate="A" pin="VSST" pad="31"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS90C241QVS"/>
<attribute name="OC_FARNELL" value="1589515"/>
<attribute name="OC_NEWARK" value="08N3577"/>
<attribute name="PACKAGE" value="QFP-48"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS90C3201VS" prefix="U">
<description>Transmitter</description>
<gates>
<gate name="A" symbol="DS90C3201VS_A"/>
<gate name="B" symbol="DS90C3201VS_B"/>
</gates>
<devices>
<device name="" package="QFP40P1600X1600X120-128N">
<connects>
<connect gate="A" pin="MODE0" pad="34"/>
<connect gate="A" pin="MODE1" pad="63"/>
<connect gate="A" pin="PWDNB" pad="30"/>
<connect gate="A" pin="RESRVD" pad="64"/>
<connect gate="A" pin="RFB" pad="33"/>
<connect gate="A" pin="S2CLK" pad="31"/>
<connect gate="A" pin="S2DAT" pad="32"/>
<connect gate="A" pin="TCLKIN" pad="27"/>
<connect gate="A" pin="TCLKOUT+" pad="47"/>
<connect gate="A" pin="TCLKOUT-" pad="48"/>
<connect gate="A" pin="TXEA+" pad="45"/>
<connect gate="A" pin="TXEA-" pad="46"/>
<connect gate="A" pin="TXEA0" pad="14"/>
<connect gate="A" pin="TXEA1" pad="15"/>
<connect gate="A" pin="TXEA2" pad="16"/>
<connect gate="A" pin="TXEA3" pad="17"/>
<connect gate="A" pin="TXEA4" pad="18"/>
<connect gate="A" pin="TXEA5" pad="19"/>
<connect gate="A" pin="TXEA6" pad="20"/>
<connect gate="A" pin="TXEB+" pad="43"/>
<connect gate="A" pin="TXEB-" pad="44"/>
<connect gate="A" pin="TXEB0" pad="5"/>
<connect gate="A" pin="TXEB1" pad="6"/>
<connect gate="A" pin="TXEB2" pad="7"/>
<connect gate="A" pin="TXEB3" pad="8"/>
<connect gate="A" pin="TXEB4" pad="9"/>
<connect gate="A" pin="TXEB5" pad="10"/>
<connect gate="A" pin="TXEB6" pad="11"/>
<connect gate="A" pin="TXEC+" pad="41"/>
<connect gate="A" pin="TXEC-" pad="42"/>
<connect gate="A" pin="TXEC3" pad="1"/>
<connect gate="A" pin="TXEC4" pad="2"/>
<connect gate="A" pin="TXEC5" pad="3"/>
<connect gate="A" pin="TXEC6" pad="4"/>
<connect gate="A" pin="TXED+" pad="39"/>
<connect gate="A" pin="TXED-" pad="40"/>
<connect gate="A" pin="TXEE+" pad="37"/>
<connect gate="A" pin="TXEE-" pad="38"/>
<connect gate="A" pin="TXOA+" pad="59"/>
<connect gate="A" pin="TXOA-" pad="60"/>
<connect gate="A" pin="TXOB+" pad="57"/>
<connect gate="A" pin="TXOB-" pad="58"/>
<connect gate="A" pin="TXOC+" pad="55"/>
<connect gate="A" pin="TXOC-" pad="56"/>
<connect gate="A" pin="TXOD+" pad="53"/>
<connect gate="A" pin="TXOD-" pad="54"/>
<connect gate="A" pin="TXOE+" pad="51"/>
<connect gate="A" pin="TXOE-" pad="52"/>
<connect gate="A" pin="VDDE1" pad="12"/>
<connect gate="A" pin="VDDI" pad="28"/>
<connect gate="A" pin="VDDL" pad="49"/>
<connect gate="A" pin="VDDL_2" pad="35"/>
<connect gate="A" pin="VDDL_3" pad="61"/>
<connect gate="A" pin="VDDP0" pad="24"/>
<connect gate="A" pin="VDDP1" pad="21"/>
<connect gate="A" pin="VDDT0" pad="25"/>
<connect gate="A" pin="VSSE1" pad="13"/>
<connect gate="A" pin="VSSI" pad="29"/>
<connect gate="A" pin="VSSL" pad="50"/>
<connect gate="A" pin="VSSL_2" pad="36"/>
<connect gate="A" pin="VSSL_3" pad="62"/>
<connect gate="A" pin="VSSP0" pad="23"/>
<connect gate="A" pin="VSSP1" pad="22"/>
<connect gate="A" pin="VSST0" pad="26"/>
<connect gate="B" pin="TXEC0" pad="126"/>
<connect gate="B" pin="TXEC1" pad="127"/>
<connect gate="B" pin="TXEC2" pad="128"/>
<connect gate="B" pin="TXED0" pad="119"/>
<connect gate="B" pin="TXED1" pad="120"/>
<connect gate="B" pin="TXED2" pad="121"/>
<connect gate="B" pin="TXED3" pad="122"/>
<connect gate="B" pin="TXED4" pad="123"/>
<connect gate="B" pin="TXED5" pad="124"/>
<connect gate="B" pin="TXED6" pad="125"/>
<connect gate="B" pin="TXEE0" pad="110"/>
<connect gate="B" pin="TXEE1" pad="111"/>
<connect gate="B" pin="TXEE2" pad="112"/>
<connect gate="B" pin="TXEE3" pad="113"/>
<connect gate="B" pin="TXEE4" pad="114"/>
<connect gate="B" pin="TXEE5" pad="115"/>
<connect gate="B" pin="TXEE6" pad="116"/>
<connect gate="B" pin="TXOA0" pad="99"/>
<connect gate="B" pin="TXOA1" pad="100"/>
<connect gate="B" pin="TXOA2" pad="101"/>
<connect gate="B" pin="TXOA3" pad="102"/>
<connect gate="B" pin="TXOA4" pad="103"/>
<connect gate="B" pin="TXOA5" pad="104"/>
<connect gate="B" pin="TXOA6" pad="105"/>
<connect gate="B" pin="TXOB0" pad="92"/>
<connect gate="B" pin="TXOB1" pad="93"/>
<connect gate="B" pin="TXOB2" pad="94"/>
<connect gate="B" pin="TXOB3" pad="95"/>
<connect gate="B" pin="TXOB4" pad="96"/>
<connect gate="B" pin="TXOB5" pad="97"/>
<connect gate="B" pin="TXOB6" pad="98"/>
<connect gate="B" pin="TXOC0" pad="83"/>
<connect gate="B" pin="TXOC1" pad="84"/>
<connect gate="B" pin="TXOC2" pad="85"/>
<connect gate="B" pin="TXOC3" pad="86"/>
<connect gate="B" pin="TXOC4" pad="87"/>
<connect gate="B" pin="TXOC5" pad="88"/>
<connect gate="B" pin="TXOC6" pad="89"/>
<connect gate="B" pin="TXOD0" pad="74"/>
<connect gate="B" pin="TXOD1" pad="75"/>
<connect gate="B" pin="TXOD2" pad="76"/>
<connect gate="B" pin="TXOD3" pad="77"/>
<connect gate="B" pin="TXOD4" pad="78"/>
<connect gate="B" pin="TXOD5" pad="79"/>
<connect gate="B" pin="TXOD6" pad="80"/>
<connect gate="B" pin="TXOE0" pad="65"/>
<connect gate="B" pin="TXOE1" pad="66"/>
<connect gate="B" pin="TXOE2" pad="67"/>
<connect gate="B" pin="TXOE3" pad="68"/>
<connect gate="B" pin="TXOE4" pad="69"/>
<connect gate="B" pin="TXOE5" pad="70"/>
<connect gate="B" pin="TXOE6" pad="71"/>
<connect gate="B" pin="VDDE0" pad="117"/>
<connect gate="B" pin="VDDO0" pad="72"/>
<connect gate="B" pin="VDDO1" pad="90"/>
<connect gate="B" pin="VDDT1" pad="81"/>
<connect gate="B" pin="VDDT2" pad="106"/>
<connect gate="B" pin="VDDT3" pad="107"/>
<connect gate="B" pin="VSSE0" pad="118"/>
<connect gate="B" pin="VSSO0" pad="73"/>
<connect gate="B" pin="VSSO1" pad="91"/>
<connect gate="B" pin="VSST1" pad="82"/>
<connect gate="B" pin="VSST2" pad="108"/>
<connect gate="B" pin="VSST3" pad="109"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS90C3201VS"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="99K2033"/>
<attribute name="PACKAGE" value="QFP-128"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS90C3202VS" prefix="U">
<description>Transmitter</description>
<gates>
<gate name="A" symbol="DS90C3202VS_A"/>
<gate name="B" symbol="DS90C3202VS_B"/>
</gates>
<devices>
<device name="" package="QFP40P1600X1600X120-128N">
<connects>
<connect gate="A" pin="PWDNB" pad="7"/>
<connect gate="A" pin="RCLKOUT" pad="44"/>
<connect gate="A" pin="RXEA0" pad="47"/>
<connect gate="A" pin="RXEA1" pad="48"/>
<connect gate="A" pin="RXEA2" pad="49"/>
<connect gate="A" pin="RXEA3" pad="50"/>
<connect gate="A" pin="RXEA4" pad="51"/>
<connect gate="A" pin="RXEA5" pad="52"/>
<connect gate="A" pin="RXEA6" pad="53"/>
<connect gate="A" pin="RXEB0" pad="35"/>
<connect gate="A" pin="RXEB1" pad="36"/>
<connect gate="A" pin="RXEB2" pad="37"/>
<connect gate="A" pin="RXEB3" pad="38"/>
<connect gate="A" pin="RXEB4" pad="39"/>
<connect gate="A" pin="RXEB5" pad="40"/>
<connect gate="A" pin="RXEB6" pad="41"/>
<connect gate="A" pin="RXEC0" pad="26"/>
<connect gate="A" pin="RXEC1" pad="27"/>
<connect gate="A" pin="RXEC2" pad="28"/>
<connect gate="A" pin="RXEC3" pad="29"/>
<connect gate="A" pin="RXEC4" pad="30"/>
<connect gate="A" pin="RXEC5" pad="31"/>
<connect gate="A" pin="RXEC6" pad="34"/>
<connect gate="A" pin="RXED0" pad="17"/>
<connect gate="A" pin="RXED1" pad="18"/>
<connect gate="A" pin="RXED2" pad="19"/>
<connect gate="A" pin="RXED3" pad="20"/>
<connect gate="A" pin="RXED4" pad="21"/>
<connect gate="A" pin="RXED5" pad="22"/>
<connect gate="A" pin="RXED6" pad="23"/>
<connect gate="A" pin="RXEE0" pad="8"/>
<connect gate="A" pin="RXEE1" pad="9"/>
<connect gate="A" pin="RXEE2" pad="10"/>
<connect gate="A" pin="RXEE3" pad="11"/>
<connect gate="A" pin="RXEE4" pad="12"/>
<connect gate="A" pin="RXEE5" pad="13"/>
<connect gate="A" pin="RXEE6" pad="14"/>
<connect gate="A" pin="RXOD0" pad="63"/>
<connect gate="A" pin="RXOE0" pad="56"/>
<connect gate="A" pin="RXOE1" pad="57"/>
<connect gate="A" pin="RXOE2" pad="58"/>
<connect gate="A" pin="RXOE3" pad="59"/>
<connect gate="A" pin="RXOE4" pad="60"/>
<connect gate="A" pin="RXOE5" pad="61"/>
<connect gate="A" pin="RXOE6" pad="62"/>
<connect gate="A" pin="S2CLK" pad="2"/>
<connect gate="A" pin="S2DAT" pad="1"/>
<connect gate="A" pin="VDD0" pad="16"/>
<connect gate="A" pin="VDD1" pad="33"/>
<connect gate="A" pin="VDD2" pad="46"/>
<connect gate="A" pin="VDD3" pad="55"/>
<connect gate="A" pin="VDDP0" pad="6"/>
<connect gate="A" pin="VDDP1" pad="3"/>
<connect gate="A" pin="VDDR0" pad="25"/>
<connect gate="A" pin="VDDR1" pad="43"/>
<connect gate="A" pin="VSS0" pad="15"/>
<connect gate="A" pin="VSS1" pad="32"/>
<connect gate="A" pin="VSS2" pad="45"/>
<connect gate="A" pin="VSS3" pad="54"/>
<connect gate="A" pin="VSS4" pad="64"/>
<connect gate="A" pin="VSSP0" pad="5"/>
<connect gate="A" pin="VSSP1" pad="4"/>
<connect gate="A" pin="VSSR0" pad="24"/>
<connect gate="A" pin="VSSR1" pad="42"/>
<connect gate="B" pin="MODE0" pad="127"/>
<connect gate="B" pin="MODE1" pad="98"/>
<connect gate="B" pin="RCLKIN+" pad="116"/>
<connect gate="B" pin="RCLKIN-" pad="115"/>
<connect gate="B" pin="RESRVD" pad="97"/>
<connect gate="B" pin="RFB" pad="128"/>
<connect gate="B" pin="RXEA+" pad="118"/>
<connect gate="B" pin="RXEA-" pad="117"/>
<connect gate="B" pin="RXEB+" pad="120"/>
<connect gate="B" pin="RXEB-" pad="119"/>
<connect gate="B" pin="RXEC+" pad="122"/>
<connect gate="B" pin="RXEC-" pad="121"/>
<connect gate="B" pin="RXED+" pad="124"/>
<connect gate="B" pin="RXED-" pad="123"/>
<connect gate="B" pin="RXEE+" pad="126"/>
<connect gate="B" pin="RXEE-" pad="125"/>
<connect gate="B" pin="RXOA+" pad="102"/>
<connect gate="B" pin="RXOA-" pad="101"/>
<connect gate="B" pin="RXOA0" pad="88"/>
<connect gate="B" pin="RXOA1" pad="89"/>
<connect gate="B" pin="RXOA2" pad="90"/>
<connect gate="B" pin="RXOA3" pad="91"/>
<connect gate="B" pin="RXOA4" pad="92"/>
<connect gate="B" pin="RXOA5" pad="93"/>
<connect gate="B" pin="RXOA6" pad="94"/>
<connect gate="B" pin="RXOB+" pad="104"/>
<connect gate="B" pin="RXOB-" pad="103"/>
<connect gate="B" pin="RXOB0" pad="79"/>
<connect gate="B" pin="RXOB1" pad="80"/>
<connect gate="B" pin="RXOB2" pad="81"/>
<connect gate="B" pin="RXOB3" pad="82"/>
<connect gate="B" pin="RXOB4" pad="83"/>
<connect gate="B" pin="RXOB5" pad="84"/>
<connect gate="B" pin="RXOB6" pad="85"/>
<connect gate="B" pin="RXOC+" pad="106"/>
<connect gate="B" pin="RXOC-" pad="105"/>
<connect gate="B" pin="RXOC0" pad="72"/>
<connect gate="B" pin="RXOC1" pad="73"/>
<connect gate="B" pin="RXOC2" pad="74"/>
<connect gate="B" pin="RXOC3" pad="75"/>
<connect gate="B" pin="RXOC4" pad="76"/>
<connect gate="B" pin="RXOC5" pad="77"/>
<connect gate="B" pin="RXOC6" pad="78"/>
<connect gate="B" pin="RXOD+" pad="108"/>
<connect gate="B" pin="RXOD-" pad="107"/>
<connect gate="B" pin="RXOD1" pad="66"/>
<connect gate="B" pin="RXOD2" pad="67"/>
<connect gate="B" pin="RXOD3" pad="68"/>
<connect gate="B" pin="RXOD4" pad="69"/>
<connect gate="B" pin="RXOD5" pad="70"/>
<connect gate="B" pin="RXOD6" pad="71"/>
<connect gate="B" pin="RXOE+" pad="110"/>
<connect gate="B" pin="RXOE-" pad="109"/>
<connect gate="B" pin="VDD4" pad="65"/>
<connect gate="B" pin="VDD5" pad="95"/>
<connect gate="B" pin="VDDL" pad="114"/>
<connect gate="B" pin="VDDL_2" pad="100"/>
<connect gate="B" pin="VDDL_3" pad="113"/>
<connect gate="B" pin="VDDR2" pad="86"/>
<connect gate="B" pin="VSS5" pad="96"/>
<connect gate="B" pin="VSSL" pad="112"/>
<connect gate="B" pin="VSSL_2" pad="99"/>
<connect gate="B" pin="VSSL_3" pad="111"/>
<connect gate="B" pin="VSSR2" pad="87"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS90C3202VS"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="99K2035"/>
<attribute name="PACKAGE" value="QFP-128"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS90C402M" prefix="U">
<description>Receiver</description>
<gates>
<gate name="A" symbol="DS90C402M"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="RI1+" pad="3"/>
<connect gate="A" pin="RI1-" pad="4"/>
<connect gate="A" pin="RI2+" pad="7"/>
<connect gate="A" pin="RI2-" pad="8"/>
<connect gate="A" pin="RO1" pad="2"/>
<connect gate="A" pin="RO2" pad="6"/>
<connect gate="A" pin="VCC" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS90C402M"/>
<attribute name="OC_FARNELL" value="1468975"/>
<attribute name="OC_NEWARK" value="41K2052"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS90CF364AMTD" prefix="U">
<description>LVDS Transmitter</description>
<gates>
<gate name="A" symbol="DS90CF364AMTD"/>
</gates>
<devices>
<device name="" package="SOP50P800X110-48N">
<connects>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="GND_2" pad="25"/>
<connect gate="A" pin="GND_3" pad="32"/>
<connect gate="A" pin="GND_4" pad="38"/>
<connect gate="A" pin="GND_5" pad="44"/>
<connect gate="A" pin="LVDSGND" pad="7"/>
<connect gate="A" pin="LVDSGND_2" pad="13"/>
<connect gate="A" pin="LVDSGND_3" pad="18"/>
<connect gate="A" pin="LVDSVCC" pad="12"/>
<connect gate="A" pin="NC" pad="6"/>
<connect gate="A" pin="PLLGND" pad="21"/>
<connect gate="A" pin="PLLGND_2" pad="19"/>
<connect gate="A" pin="PLLVCC" pad="20"/>
<connect gate="A" pin="RXCLKIN+" pad="17"/>
<connect gate="A" pin="RXCLKIN-" pad="16"/>
<connect gate="A" pin="RXCLKOUT" pad="23"/>
<connect gate="A" pin="RXIN0+" pad="9"/>
<connect gate="A" pin="RXIN0-" pad="8"/>
<connect gate="A" pin="RXIN1+" pad="11"/>
<connect gate="A" pin="RXIN1-" pad="10"/>
<connect gate="A" pin="RXIN2+" pad="15"/>
<connect gate="A" pin="RXIN2-" pad="14"/>
<connect gate="A" pin="RXOUT0" pad="24"/>
<connect gate="A" pin="RXOUT1" pad="26"/>
<connect gate="A" pin="RXOUT10" pad="39"/>
<connect gate="A" pin="RXOUT11" pad="40"/>
<connect gate="A" pin="RXOUT12" pad="41"/>
<connect gate="A" pin="RXOUT13" pad="43"/>
<connect gate="A" pin="RXOUT14" pad="45"/>
<connect gate="A" pin="RXOUT15" pad="46"/>
<connect gate="A" pin="RXOUT16" pad="47"/>
<connect gate="A" pin="RXOUT17" pad="1"/>
<connect gate="A" pin="RXOUT18" pad="2"/>
<connect gate="A" pin="RXOUT19" pad="4"/>
<connect gate="A" pin="RXOUT2" pad="27"/>
<connect gate="A" pin="RXOUT20" pad="5"/>
<connect gate="A" pin="RXOUT3" pad="29"/>
<connect gate="A" pin="RXOUT4" pad="30"/>
<connect gate="A" pin="RXOUT5" pad="31"/>
<connect gate="A" pin="RXOUT6" pad="33"/>
<connect gate="A" pin="RXOUT7" pad="34"/>
<connect gate="A" pin="RXOUT8" pad="35"/>
<connect gate="A" pin="RXOUT9" pad="37"/>
<connect gate="A" pin="VCC" pad="48"/>
<connect gate="A" pin="VCC_2" pad="28"/>
<connect gate="A" pin="VCC_3" pad="36"/>
<connect gate="A" pin="VCC_4" pad="42"/>
<connect gate="A" pin="~PWRDWN" pad="22"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS90CF364AMTD"/>
<attribute name="OC_FARNELL" value="1468865"/>
<attribute name="OC_NEWARK" value="41K1941"/>
<attribute name="PACKAGE" value="TSSOP-48"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS90CF384AMTD" prefix="U">
<description>Flat Panel Display</description>
<gates>
<gate name="A" symbol="DS90CF384AMTD"/>
</gates>
<devices>
<device name="" package="SOP50P810X110-56N">
<connects>
<connect gate="A" pin="GND" pad="28"/>
<connect gate="A" pin="GND_2" pad="4"/>
<connect gate="A" pin="GND_3" pad="36"/>
<connect gate="A" pin="GND_4" pad="52"/>
<connect gate="A" pin="GND_5" pad="44"/>
<connect gate="A" pin="LVDS_GND" pad="14"/>
<connect gate="A" pin="LVDS_GND_2" pad="21"/>
<connect gate="A" pin="LVDS_GND_3" pad="8"/>
<connect gate="A" pin="LVDS_VCC" pad="13"/>
<connect gate="A" pin="PLL_GND" pad="24"/>
<connect gate="A" pin="PLL_GND_2" pad="22"/>
<connect gate="A" pin="PLL_VCC" pad="23"/>
<connect gate="A" pin="RXCLKIN+" pad="18"/>
<connect gate="A" pin="RXCLKIN-" pad="17"/>
<connect gate="A" pin="RXCLK_OUT" pad="26"/>
<connect gate="A" pin="RXIN0+" pad="10"/>
<connect gate="A" pin="RXIN0-" pad="9"/>
<connect gate="A" pin="RXIN1+" pad="12"/>
<connect gate="A" pin="RXIN1-" pad="11"/>
<connect gate="A" pin="RXIN2+" pad="16"/>
<connect gate="A" pin="RXIN2-" pad="15"/>
<connect gate="A" pin="RXIN3+" pad="20"/>
<connect gate="A" pin="RXIN3-" pad="19"/>
<connect gate="A" pin="RXOUT0" pad="27"/>
<connect gate="A" pin="RXOUT1" pad="29"/>
<connect gate="A" pin="RXOUT10" pad="41"/>
<connect gate="A" pin="RXOUT11" pad="42"/>
<connect gate="A" pin="RXOUT12" pad="43"/>
<connect gate="A" pin="RXOUT13" pad="45"/>
<connect gate="A" pin="RXOUT14" pad="46"/>
<connect gate="A" pin="RXOUT15" pad="47"/>
<connect gate="A" pin="RXOUT16" pad="49"/>
<connect gate="A" pin="RXOUT17" pad="50"/>
<connect gate="A" pin="RXOUT18" pad="51"/>
<connect gate="A" pin="RXOUT19" pad="53"/>
<connect gate="A" pin="RXOUT2" pad="30"/>
<connect gate="A" pin="RXOUT20" pad="54"/>
<connect gate="A" pin="RXOUT21" pad="55"/>
<connect gate="A" pin="RXOUT22" pad="1"/>
<connect gate="A" pin="RXOUT23" pad="2"/>
<connect gate="A" pin="RXOUT24" pad="3"/>
<connect gate="A" pin="RXOUT25" pad="5"/>
<connect gate="A" pin="RXOUT26" pad="6"/>
<connect gate="A" pin="RXOUT27" pad="7"/>
<connect gate="A" pin="RXOUT3" pad="32"/>
<connect gate="A" pin="RXOUT4" pad="33"/>
<connect gate="A" pin="RXOUT5" pad="34"/>
<connect gate="A" pin="RXOUT6" pad="35"/>
<connect gate="A" pin="RXOUT7" pad="37"/>
<connect gate="A" pin="RXOUT8" pad="38"/>
<connect gate="A" pin="RXOUT9" pad="39"/>
<connect gate="A" pin="VCC" pad="56"/>
<connect gate="A" pin="VCC_2" pad="31"/>
<connect gate="A" pin="VCC_3" pad="40"/>
<connect gate="A" pin="VCC_4" pad="48"/>
<connect gate="A" pin="~PWR_DOWN" pad="25"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS90CF384AMTD"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="48F5640"/>
<attribute name="PACKAGE" value="SSOP-56"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS90CP04TLQ" prefix="U">
<description>LVDS Crosspoint Switch</description>
<gates>
<gate name="A" symbol="DS90CP04TLQ"/>
</gates>
<devices>
<device name="" package="DFN600X600X80-33N">
<connects>
<connect gate="A" pin="CSCLK" pad="19"/>
<connect gate="A" pin="CSO" pad="18"/>
<connect gate="A" pin="EP" pad="33"/>
<connect gate="A" pin="GND" pad="21"/>
<connect gate="A" pin="GND_2" pad="4"/>
<connect gate="A" pin="GND_3" pad="20"/>
<connect gate="A" pin="IN1+" pad="16"/>
<connect gate="A" pin="IN1-" pad="15"/>
<connect gate="A" pin="IN2+" pad="14"/>
<connect gate="A" pin="IN2-" pad="13"/>
<connect gate="A" pin="IN3+" pad="12"/>
<connect gate="A" pin="IN3-" pad="11"/>
<connect gate="A" pin="IN4+" pad="10"/>
<connect gate="A" pin="IN4-" pad="9"/>
<connect gate="A" pin="LOAD" pad="22"/>
<connect gate="A" pin="MODE" pad="23"/>
<connect gate="A" pin="OUT1+" pad="25"/>
<connect gate="A" pin="OUT1-" pad="26"/>
<connect gate="A" pin="OUT2+" pad="27"/>
<connect gate="A" pin="OUT2-" pad="28"/>
<connect gate="A" pin="OUT3+" pad="29"/>
<connect gate="A" pin="OUT3-" pad="30"/>
<connect gate="A" pin="OUT4+" pad="31"/>
<connect gate="A" pin="OUT4-" pad="32"/>
<connect gate="A" pin="RSCLK" pad="3"/>
<connect gate="A" pin="RSO" pad="2"/>
<connect gate="A" pin="SCLK" pad="6"/>
<connect gate="A" pin="SEL0" pad="5"/>
<connect gate="A" pin="SI/SEL1" pad="7"/>
<connect gate="A" pin="VDD" pad="1"/>
<connect gate="A" pin="VDD_2" pad="17"/>
<connect gate="A" pin="VDD_3" pad="8"/>
<connect gate="A" pin="VDD_4" pad="24"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS90CP04TLQ"/>
<attribute name="OC_FARNELL" value="1685583"/>
<attribute name="OC_NEWARK" value="41K1977"/>
<attribute name="PACKAGE" value="LLP-32"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS90CP22M-8" prefix="U">
<description>Crosspoint Switch</description>
<gates>
<gate name="A" symbol="DS90CP22M-8"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-16N">
<connects>
<connect gate="A" pin="EN0" pad="16"/>
<connect gate="A" pin="EN1" pad="15"/>
<connect gate="A" pin="GND" pad="12"/>
<connect gate="A" pin="IN0+" pad="3"/>
<connect gate="A" pin="IN0-" pad="4"/>
<connect gate="A" pin="IN1+" pad="6"/>
<connect gate="A" pin="IN1-" pad="7"/>
<connect gate="A" pin="NC" pad="9"/>
<connect gate="A" pin="NC_2" pad="8"/>
<connect gate="A" pin="OUT0+" pad="14"/>
<connect gate="A" pin="OUT0-" pad="13"/>
<connect gate="A" pin="OUT1+" pad="11"/>
<connect gate="A" pin="OUT1-" pad="10"/>
<connect gate="A" pin="SEL0" pad="2"/>
<connect gate="A" pin="SEL1" pad="1"/>
<connect gate="A" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS90CP22M-8"/>
<attribute name="OC_FARNELL" value="1286818"/>
<attribute name="OC_NEWARK" value="41K1979"/>
<attribute name="PACKAGE" value="16-SOIC"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS90CP22MT" prefix="U">
<description>LVDS Crosspoint Switch</description>
<gates>
<gate name="A" symbol="DS90CP22MT"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-16N">
<connects>
<connect gate="A" pin="EN0" pad="16"/>
<connect gate="A" pin="EN1" pad="15"/>
<connect gate="A" pin="GND" pad="12"/>
<connect gate="A" pin="IN0+" pad="3"/>
<connect gate="A" pin="IN0-" pad="4"/>
<connect gate="A" pin="IN1+" pad="6"/>
<connect gate="A" pin="IN1-" pad="7"/>
<connect gate="A" pin="NC" pad="9"/>
<connect gate="A" pin="NC_2" pad="8"/>
<connect gate="A" pin="OUT0+" pad="14"/>
<connect gate="A" pin="OUT0-" pad="13"/>
<connect gate="A" pin="OUT1+" pad="11"/>
<connect gate="A" pin="OUT1-" pad="10"/>
<connect gate="A" pin="SEL0" pad="2"/>
<connect gate="A" pin="SEL1" pad="1"/>
<connect gate="A" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS90CP22MT"/>
<attribute name="OC_FARNELL" value="1286819"/>
<attribute name="OC_NEWARK" value="41K1980"/>
<attribute name="PACKAGE" value="TSSOP-16"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS90CR215MTD" prefix="U">
<description>Rising Edge Data Strobe LVDS</description>
<gates>
<gate name="A" symbol="DS90CR215MTD"/>
</gates>
<devices>
<device name="" package="SOP50P800X110-48N">
<connects>
<connect gate="A" pin="GND" pad="24"/>
<connect gate="A" pin="GND_2" pad="5"/>
<connect gate="A" pin="GND_3" pad="46"/>
<connect gate="A" pin="GND_4" pad="11"/>
<connect gate="A" pin="GND_5" pad="17"/>
<connect gate="A" pin="LVDS_GND" pad="42"/>
<connect gate="A" pin="LVDS_GND_2" pad="31"/>
<connect gate="A" pin="LVDS_GND_3" pad="36"/>
<connect gate="A" pin="LVDS_VCC" pad="37"/>
<connect gate="A" pin="NC" pad="43"/>
<connect gate="A" pin="PLL_GND" pad="29"/>
<connect gate="A" pin="PLL_GND_2" pad="28"/>
<connect gate="A" pin="PLL_VCC" pad="30"/>
<connect gate="A" pin="TXCLK_IN" pad="26"/>
<connect gate="A" pin="TXCLK_OUT+" pad="32"/>
<connect gate="A" pin="TXCLK_OUT-" pad="33"/>
<connect gate="A" pin="TXIN0" pad="44"/>
<connect gate="A" pin="TXIN1" pad="45"/>
<connect gate="A" pin="TXIN10" pad="10"/>
<connect gate="A" pin="TXIN11" pad="12"/>
<connect gate="A" pin="TXIN12" pad="13"/>
<connect gate="A" pin="TXIN13" pad="15"/>
<connect gate="A" pin="TXIN14" pad="16"/>
<connect gate="A" pin="TXIN15" pad="18"/>
<connect gate="A" pin="TXIN16" pad="19"/>
<connect gate="A" pin="TXIN17" pad="20"/>
<connect gate="A" pin="TXIN18" pad="22"/>
<connect gate="A" pin="TXIN19" pad="23"/>
<connect gate="A" pin="TXIN2" pad="47"/>
<connect gate="A" pin="TXIN20" pad="25"/>
<connect gate="A" pin="TXIN3" pad="48"/>
<connect gate="A" pin="TXIN4" pad="1"/>
<connect gate="A" pin="TXIN5" pad="3"/>
<connect gate="A" pin="TXIN6" pad="4"/>
<connect gate="A" pin="TXIN7" pad="6"/>
<connect gate="A" pin="TXIN8" pad="7"/>
<connect gate="A" pin="TXIN9" pad="9"/>
<connect gate="A" pin="TXOUT0+" pad="40"/>
<connect gate="A" pin="TXOUT0-" pad="41"/>
<connect gate="A" pin="TXOUT1+" pad="38"/>
<connect gate="A" pin="TXOUT1-" pad="39"/>
<connect gate="A" pin="TXOUT2+" pad="34"/>
<connect gate="A" pin="TXOUT2-" pad="35"/>
<connect gate="A" pin="VCC" pad="21"/>
<connect gate="A" pin="VCC_2" pad="2"/>
<connect gate="A" pin="VCC_3" pad="14"/>
<connect gate="A" pin="VCC_4" pad="8"/>
<connect gate="A" pin="~PWRDWN" pad="27"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS90CR215MTD"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K1987"/>
<attribute name="PACKAGE" value="TSSOP-48"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS90CR216AMTD" prefix="U">
<description>Rising Edge Data Strobe LVDS</description>
<gates>
<gate name="A" symbol="DS90CR216AMTD"/>
</gates>
<devices>
<device name="" package="SOP50P800X110-48N">
<connects>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="GND_2" pad="25"/>
<connect gate="A" pin="GND_3" pad="32"/>
<connect gate="A" pin="GND_4" pad="38"/>
<connect gate="A" pin="GND_5" pad="44"/>
<connect gate="A" pin="LVDSGND" pad="7"/>
<connect gate="A" pin="LVDSGND_2" pad="13"/>
<connect gate="A" pin="LVDSGND_3" pad="18"/>
<connect gate="A" pin="LVDSVCC" pad="12"/>
<connect gate="A" pin="NC" pad="6"/>
<connect gate="A" pin="PLLGND" pad="21"/>
<connect gate="A" pin="PLLGND_2" pad="19"/>
<connect gate="A" pin="PLLVCC" pad="20"/>
<connect gate="A" pin="RXCLKIN+" pad="17"/>
<connect gate="A" pin="RXCLKIN-" pad="16"/>
<connect gate="A" pin="RXCLKOUT" pad="23"/>
<connect gate="A" pin="RXIN0+" pad="9"/>
<connect gate="A" pin="RXIN0-" pad="8"/>
<connect gate="A" pin="RXIN1+" pad="11"/>
<connect gate="A" pin="RXIN1-" pad="10"/>
<connect gate="A" pin="RXIN2+" pad="15"/>
<connect gate="A" pin="RXIN2-" pad="14"/>
<connect gate="A" pin="RXOUT0" pad="24"/>
<connect gate="A" pin="RXOUT1" pad="26"/>
<connect gate="A" pin="RXOUT10" pad="39"/>
<connect gate="A" pin="RXOUT11" pad="40"/>
<connect gate="A" pin="RXOUT12" pad="41"/>
<connect gate="A" pin="RXOUT13" pad="43"/>
<connect gate="A" pin="RXOUT14" pad="45"/>
<connect gate="A" pin="RXOUT15" pad="46"/>
<connect gate="A" pin="RXOUT16" pad="47"/>
<connect gate="A" pin="RXOUT17" pad="1"/>
<connect gate="A" pin="RXOUT18" pad="2"/>
<connect gate="A" pin="RXOUT19" pad="4"/>
<connect gate="A" pin="RXOUT2" pad="27"/>
<connect gate="A" pin="RXOUT20" pad="5"/>
<connect gate="A" pin="RXOUT3" pad="29"/>
<connect gate="A" pin="RXOUT4" pad="30"/>
<connect gate="A" pin="RXOUT5" pad="31"/>
<connect gate="A" pin="RXOUT6" pad="33"/>
<connect gate="A" pin="RXOUT7" pad="34"/>
<connect gate="A" pin="RXOUT8" pad="35"/>
<connect gate="A" pin="RXOUT9" pad="37"/>
<connect gate="A" pin="VCC" pad="48"/>
<connect gate="A" pin="VCC_2" pad="28"/>
<connect gate="A" pin="VCC_3" pad="36"/>
<connect gate="A" pin="VCC_4" pad="42"/>
<connect gate="A" pin="~PWRDWN" pad="22"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS90CR216AMTD"/>
<attribute name="OC_FARNELL" value="1685584"/>
<attribute name="OC_NEWARK" value="41K1989"/>
<attribute name="PACKAGE" value="TSSOP-48"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS90CR217MTD" prefix="U">
<description>Data Strobe LVDS</description>
<gates>
<gate name="A" symbol="DS90CR217MTD"/>
</gates>
<devices>
<device name="" package="SOP50P800X110-48N">
<connects>
<connect gate="A" pin="GND" pad="46"/>
<connect gate="A" pin="GND_2" pad="5"/>
<connect gate="A" pin="GND_3" pad="11"/>
<connect gate="A" pin="GND_4" pad="17"/>
<connect gate="A" pin="GND_5" pad="24"/>
<connect gate="A" pin="LVDS_GND" pad="42"/>
<connect gate="A" pin="LVDS_GND_2" pad="31"/>
<connect gate="A" pin="LVDS_GND_3" pad="36"/>
<connect gate="A" pin="LVDS_VCC" pad="37"/>
<connect gate="A" pin="NC" pad="43"/>
<connect gate="A" pin="PLL_GND" pad="30"/>
<connect gate="A" pin="PLL_GND_2" pad="28"/>
<connect gate="A" pin="PLL_VCC" pad="29"/>
<connect gate="A" pin="TXCLK_IN" pad="26"/>
<connect gate="A" pin="TXCLK_OUT+" pad="32"/>
<connect gate="A" pin="TXCLK_OUT-" pad="33"/>
<connect gate="A" pin="TXIN0" pad="44"/>
<connect gate="A" pin="TXIN1" pad="45"/>
<connect gate="A" pin="TXIN10" pad="10"/>
<connect gate="A" pin="TXIN11" pad="12"/>
<connect gate="A" pin="TXIN12" pad="13"/>
<connect gate="A" pin="TXIN13" pad="15"/>
<connect gate="A" pin="TXIN14" pad="16"/>
<connect gate="A" pin="TXIN15" pad="18"/>
<connect gate="A" pin="TXIN16" pad="19"/>
<connect gate="A" pin="TXIN17" pad="20"/>
<connect gate="A" pin="TXIN18" pad="22"/>
<connect gate="A" pin="TXIN19" pad="23"/>
<connect gate="A" pin="TXIN2" pad="47"/>
<connect gate="A" pin="TXIN20" pad="25"/>
<connect gate="A" pin="TXIN3" pad="48"/>
<connect gate="A" pin="TXIN4" pad="1"/>
<connect gate="A" pin="TXIN5" pad="3"/>
<connect gate="A" pin="TXIN6" pad="4"/>
<connect gate="A" pin="TXIN7" pad="6"/>
<connect gate="A" pin="TXIN8" pad="7"/>
<connect gate="A" pin="TXIN9" pad="9"/>
<connect gate="A" pin="TXOUT0+" pad="40"/>
<connect gate="A" pin="TXOUT0-" pad="41"/>
<connect gate="A" pin="TXOUT1+" pad="38"/>
<connect gate="A" pin="TXOUT1-" pad="39"/>
<connect gate="A" pin="TXOUT2+" pad="34"/>
<connect gate="A" pin="TXOUT2-" pad="35"/>
<connect gate="A" pin="VCC" pad="21"/>
<connect gate="A" pin="VCC_2" pad="2"/>
<connect gate="A" pin="VCC_3" pad="14"/>
<connect gate="A" pin="VCC_4" pad="8"/>
<connect gate="A" pin="~PWRDWN" pad="27"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS90CR217MTD"/>
<attribute name="OC_FARNELL" value="1693934"/>
<attribute name="OC_NEWARK" value="41K1993"/>
<attribute name="PACKAGE" value="TSSOP-48"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS90CR218AMTD" prefix="U">
<description>Rising Edge Data Strobe</description>
<gates>
<gate name="A" symbol="DS90CR218AMTD"/>
</gates>
<devices>
<device name="" package="SOP50P810X110-48N">
<connects>
<connect gate="A" pin="GND" pad="44"/>
<connect gate="A" pin="GND_2" pad="25"/>
<connect gate="A" pin="GND_3" pad="32"/>
<connect gate="A" pin="GND_4" pad="38"/>
<connect gate="A" pin="GND_5" pad="3"/>
<connect gate="A" pin="LVDSGND" pad="18"/>
<connect gate="A" pin="LVDSGND_2" pad="7"/>
<connect gate="A" pin="LVDSGND_3" pad="13"/>
<connect gate="A" pin="LVDSVCC" pad="12"/>
<connect gate="A" pin="NC" pad="6"/>
<connect gate="A" pin="PLLGND" pad="21"/>
<connect gate="A" pin="PLLGND_2" pad="19"/>
<connect gate="A" pin="PLLVCC" pad="20"/>
<connect gate="A" pin="RXCLKIN+" pad="17"/>
<connect gate="A" pin="RXCLKIN-" pad="16"/>
<connect gate="A" pin="RXCLKOUT" pad="23"/>
<connect gate="A" pin="RXIN0+" pad="9"/>
<connect gate="A" pin="RXIN0-" pad="8"/>
<connect gate="A" pin="RXIN1+" pad="11"/>
<connect gate="A" pin="RXIN1-" pad="10"/>
<connect gate="A" pin="RXIN2+" pad="15"/>
<connect gate="A" pin="RXIN2-" pad="14"/>
<connect gate="A" pin="RXOUT0" pad="24"/>
<connect gate="A" pin="RXOUT1" pad="26"/>
<connect gate="A" pin="RXOUT10" pad="39"/>
<connect gate="A" pin="RXOUT11" pad="40"/>
<connect gate="A" pin="RXOUT12" pad="41"/>
<connect gate="A" pin="RXOUT13" pad="43"/>
<connect gate="A" pin="RXOUT14" pad="45"/>
<connect gate="A" pin="RXOUT15" pad="46"/>
<connect gate="A" pin="RXOUT16" pad="47"/>
<connect gate="A" pin="RXOUT17" pad="1"/>
<connect gate="A" pin="RXOUT18" pad="2"/>
<connect gate="A" pin="RXOUT19" pad="4"/>
<connect gate="A" pin="RXOUT2" pad="27"/>
<connect gate="A" pin="RXOUT20" pad="5"/>
<connect gate="A" pin="RXOUT3" pad="29"/>
<connect gate="A" pin="RXOUT4" pad="30"/>
<connect gate="A" pin="RXOUT5" pad="31"/>
<connect gate="A" pin="RXOUT6" pad="33"/>
<connect gate="A" pin="RXOUT7" pad="34"/>
<connect gate="A" pin="RXOUT8" pad="35"/>
<connect gate="A" pin="RXOUT9" pad="37"/>
<connect gate="A" pin="VCC" pad="42"/>
<connect gate="A" pin="VCC_2" pad="48"/>
<connect gate="A" pin="VCC_3" pad="28"/>
<connect gate="A" pin="VCC_4" pad="36"/>
<connect gate="A" pin="~PWRDWN" pad="22"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS90CR218AMTD"/>
<attribute name="OC_FARNELL" value="1286820"/>
<attribute name="OC_NEWARK" value="74C3562"/>
<attribute name="PACKAGE" value="SOP-48"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS90CR285MTD" prefix="U">
<description>Data Strobe LVDS</description>
<gates>
<gate name="A" symbol="DS90CR285MTD"/>
</gates>
<devices>
<device name="" package="SOP50P810X110-56N">
<connects>
<connect gate="A" pin="GND" pad="13"/>
<connect gate="A" pin="GND_2" pad="53"/>
<connect gate="A" pin="GND_3" pad="5"/>
<connect gate="A" pin="GND_4" pad="21"/>
<connect gate="A" pin="GND_5" pad="29"/>
<connect gate="A" pin="LVDS_GND" pad="49"/>
<connect gate="A" pin="LVDS_GND_2" pad="36"/>
<connect gate="A" pin="LVDS_GND_3" pad="43"/>
<connect gate="A" pin="LVDS_VCC" pad="44"/>
<connect gate="A" pin="PLL_GND" pad="33"/>
<connect gate="A" pin="PLL_GND_2" pad="35"/>
<connect gate="A" pin="PLL_VCC" pad="34"/>
<connect gate="A" pin="TXCLKOUT+" pad="39"/>
<connect gate="A" pin="TXCLKOUT-" pad="40"/>
<connect gate="A" pin="TXCLK_IN" pad="31"/>
<connect gate="A" pin="TXIN0" pad="51"/>
<connect gate="A" pin="TXIN1" pad="52"/>
<connect gate="A" pin="TXIN10" pad="8"/>
<connect gate="A" pin="TXIN11" pad="10"/>
<connect gate="A" pin="TXIN12" pad="11"/>
<connect gate="A" pin="TXIN13" pad="12"/>
<connect gate="A" pin="TXIN14" pad="14"/>
<connect gate="A" pin="TXIN15" pad="15"/>
<connect gate="A" pin="TXIN16" pad="16"/>
<connect gate="A" pin="TXIN17" pad="18"/>
<connect gate="A" pin="TXIN18" pad="19"/>
<connect gate="A" pin="TXIN19" pad="20"/>
<connect gate="A" pin="TXIN2" pad="54"/>
<connect gate="A" pin="TXIN20" pad="22"/>
<connect gate="A" pin="TXIN21" pad="23"/>
<connect gate="A" pin="TXIN22" pad="24"/>
<connect gate="A" pin="TXIN23" pad="25"/>
<connect gate="A" pin="TXIN24" pad="27"/>
<connect gate="A" pin="TXIN25" pad="28"/>
<connect gate="A" pin="TXIN26" pad="30"/>
<connect gate="A" pin="TXIN27" pad="50"/>
<connect gate="A" pin="TXIN3" pad="55"/>
<connect gate="A" pin="TXIN4" pad="56"/>
<connect gate="A" pin="TXIN5" pad="2"/>
<connect gate="A" pin="TXIN6" pad="3"/>
<connect gate="A" pin="TXIN7" pad="4"/>
<connect gate="A" pin="TXIN8" pad="6"/>
<connect gate="A" pin="TXIN9" pad="7"/>
<connect gate="A" pin="TXOUT0+" pad="47"/>
<connect gate="A" pin="TXOUT0-" pad="48"/>
<connect gate="A" pin="TXOUT1+" pad="45"/>
<connect gate="A" pin="TXOUT1-" pad="46"/>
<connect gate="A" pin="TXOUT2+" pad="41"/>
<connect gate="A" pin="TXOUT2-" pad="42"/>
<connect gate="A" pin="TXOUT3+" pad="37"/>
<connect gate="A" pin="TXOUT3-" pad="38"/>
<connect gate="A" pin="VCC" pad="17"/>
<connect gate="A" pin="VCC_2" pad="9"/>
<connect gate="A" pin="VCC_3" pad="26"/>
<connect gate="A" pin="VCC_4" pad="1"/>
<connect gate="A" pin="~PWRDWN" pad="32"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS90CR285MTD"/>
<attribute name="OC_FARNELL" value="1564785"/>
<attribute name="OC_NEWARK" value="41K2003"/>
<attribute name="PACKAGE" value="SOP-56"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS90CR286AQMT" prefix="U">
<description>IC RCVR 28BIT CHAN LINK</description>
<gates>
<gate name="A" symbol="DS90CR286AQMT"/>
</gates>
<devices>
<device name="" package="SOP50P810X110-56N">
<connects>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="GND_2" pad="52"/>
<connect gate="A" pin="GND_3" pad="44"/>
<connect gate="A" pin="GND_4" pad="36"/>
<connect gate="A" pin="GND_5" pad="28"/>
<connect gate="A" pin="LVDS_GND" pad="8"/>
<connect gate="A" pin="LVDS_GND_2" pad="14"/>
<connect gate="A" pin="LVDS_GND_3" pad="21"/>
<connect gate="A" pin="LVDS_VCC" pad="13"/>
<connect gate="A" pin="PLL_GND" pad="22"/>
<connect gate="A" pin="PLL_GND_2" pad="24"/>
<connect gate="A" pin="PLL_VCC" pad="23"/>
<connect gate="A" pin="RXCLKIN+" pad="18"/>
<connect gate="A" pin="RXCLKIN-" pad="17"/>
<connect gate="A" pin="RXCLK_OUT" pad="26"/>
<connect gate="A" pin="RXIN0+" pad="10"/>
<connect gate="A" pin="RXIN0-" pad="9"/>
<connect gate="A" pin="RXIN1+" pad="12"/>
<connect gate="A" pin="RXIN1-" pad="11"/>
<connect gate="A" pin="RXIN2+" pad="16"/>
<connect gate="A" pin="RXIN2-" pad="15"/>
<connect gate="A" pin="RXIN3+" pad="20"/>
<connect gate="A" pin="RXIN3-" pad="19"/>
<connect gate="A" pin="RXOUT0" pad="27"/>
<connect gate="A" pin="RXOUT1" pad="29"/>
<connect gate="A" pin="RXOUT10" pad="41"/>
<connect gate="A" pin="RXOUT11" pad="42"/>
<connect gate="A" pin="RXOUT12" pad="43"/>
<connect gate="A" pin="RXOUT13" pad="45"/>
<connect gate="A" pin="RXOUT14" pad="46"/>
<connect gate="A" pin="RXOUT15" pad="47"/>
<connect gate="A" pin="RXOUT16" pad="49"/>
<connect gate="A" pin="RXOUT17" pad="50"/>
<connect gate="A" pin="RXOUT18" pad="51"/>
<connect gate="A" pin="RXOUT19" pad="53"/>
<connect gate="A" pin="RXOUT2" pad="30"/>
<connect gate="A" pin="RXOUT20" pad="54"/>
<connect gate="A" pin="RXOUT21" pad="55"/>
<connect gate="A" pin="RXOUT22" pad="1"/>
<connect gate="A" pin="RXOUT23" pad="2"/>
<connect gate="A" pin="RXOUT24" pad="3"/>
<connect gate="A" pin="RXOUT25" pad="5"/>
<connect gate="A" pin="RXOUT26" pad="6"/>
<connect gate="A" pin="RXOUT27" pad="7"/>
<connect gate="A" pin="RXOUT3" pad="32"/>
<connect gate="A" pin="RXOUT4" pad="33"/>
<connect gate="A" pin="RXOUT5" pad="34"/>
<connect gate="A" pin="RXOUT6" pad="35"/>
<connect gate="A" pin="RXOUT7" pad="37"/>
<connect gate="A" pin="RXOUT8" pad="38"/>
<connect gate="A" pin="RXOUT9" pad="39"/>
<connect gate="A" pin="VCC" pad="56"/>
<connect gate="A" pin="VCC_2" pad="31"/>
<connect gate="A" pin="VCC_3" pad="40"/>
<connect gate="A" pin="VCC_4" pad="48"/>
<connect gate="A" pin="~PWR_DOWN" pad="25"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS90CR286AQMT"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="55R2934"/>
<attribute name="PACKAGE" value="SOP-56"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS90CR287MTD" prefix="U">
<description>Edge Data Strobe</description>
<gates>
<gate name="A" symbol="DS90CR287MTD"/>
</gates>
<devices>
<device name="" package="SOP50P810X110-56N">
<connects>
<connect gate="A" pin="GND" pad="53"/>
<connect gate="A" pin="GND_2" pad="5"/>
<connect gate="A" pin="GND_3" pad="21"/>
<connect gate="A" pin="GND_4" pad="13"/>
<connect gate="A" pin="GND_5" pad="29"/>
<connect gate="A" pin="LVDS_GND" pad="49"/>
<connect gate="A" pin="LVDS_GND_2" pad="36"/>
<connect gate="A" pin="LVDS_GND_3" pad="43"/>
<connect gate="A" pin="LVDS_VCC" pad="44"/>
<connect gate="A" pin="PLL_GND" pad="35"/>
<connect gate="A" pin="PLL_GND_2" pad="33"/>
<connect gate="A" pin="PLL_VCC" pad="34"/>
<connect gate="A" pin="TXCLKOUT+" pad="39"/>
<connect gate="A" pin="TXCLKOUT-" pad="40"/>
<connect gate="A" pin="TXCLK_IN" pad="31"/>
<connect gate="A" pin="TXIN0" pad="51"/>
<connect gate="A" pin="TXIN1" pad="52"/>
<connect gate="A" pin="TXIN10" pad="8"/>
<connect gate="A" pin="TXIN11" pad="10"/>
<connect gate="A" pin="TXIN12" pad="11"/>
<connect gate="A" pin="TXIN13" pad="12"/>
<connect gate="A" pin="TXIN14" pad="14"/>
<connect gate="A" pin="TXIN15" pad="15"/>
<connect gate="A" pin="TXIN16" pad="16"/>
<connect gate="A" pin="TXIN17" pad="18"/>
<connect gate="A" pin="TXIN18" pad="19"/>
<connect gate="A" pin="TXIN19" pad="20"/>
<connect gate="A" pin="TXIN2" pad="54"/>
<connect gate="A" pin="TXIN20" pad="22"/>
<connect gate="A" pin="TXIN21" pad="23"/>
<connect gate="A" pin="TXIN22" pad="24"/>
<connect gate="A" pin="TXIN23" pad="26"/>
<connect gate="A" pin="TXIN24" pad="27"/>
<connect gate="A" pin="TXIN25" pad="28"/>
<connect gate="A" pin="TXIN26" pad="30"/>
<connect gate="A" pin="TXIN27" pad="50"/>
<connect gate="A" pin="TXIN3" pad="55"/>
<connect gate="A" pin="TXIN4" pad="56"/>
<connect gate="A" pin="TXIN5" pad="2"/>
<connect gate="A" pin="TXIN6" pad="3"/>
<connect gate="A" pin="TXIN7" pad="4"/>
<connect gate="A" pin="TXIN8" pad="6"/>
<connect gate="A" pin="TXIN9" pad="7"/>
<connect gate="A" pin="TXOUT0+" pad="47"/>
<connect gate="A" pin="TXOUT0-" pad="48"/>
<connect gate="A" pin="TXOUT1+" pad="45"/>
<connect gate="A" pin="TXOUT1-" pad="46"/>
<connect gate="A" pin="TXOUT2+" pad="41"/>
<connect gate="A" pin="TXOUT2-" pad="42"/>
<connect gate="A" pin="TXOUT3+" pad="37"/>
<connect gate="A" pin="TXOUT3-" pad="38"/>
<connect gate="A" pin="VCC" pad="9"/>
<connect gate="A" pin="VCC_2" pad="17"/>
<connect gate="A" pin="VCC_3" pad="25"/>
<connect gate="A" pin="VCC_4" pad="1"/>
<connect gate="A" pin="~PWR~_~DWN" pad="32"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS90CR287MTD"/>
<attribute name="OC_FARNELL" value="1215184"/>
<attribute name="OC_NEWARK" value="01M7382"/>
<attribute name="PACKAGE" value="SSOP-56"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS90CR288AMTD" prefix="U">
<description>Edge Data Strobe</description>
<gates>
<gate name="A" symbol="DS90CR288AMTD"/>
</gates>
<devices>
<device name="" package="SOP50P810X110-56N">
<connects>
<connect gate="A" pin="GND" pad="28"/>
<connect gate="A" pin="GND_2" pad="4"/>
<connect gate="A" pin="GND_3" pad="44"/>
<connect gate="A" pin="GND_4" pad="52"/>
<connect gate="A" pin="GND_5" pad="36"/>
<connect gate="A" pin="LVDSGND" pad="21"/>
<connect gate="A" pin="LVDSGND_2" pad="8"/>
<connect gate="A" pin="LVDSGND_3" pad="14"/>
<connect gate="A" pin="LVDSVCC" pad="13"/>
<connect gate="A" pin="PLLGND" pad="24"/>
<connect gate="A" pin="PLLGND_2" pad="22"/>
<connect gate="A" pin="PLLVCC" pad="23"/>
<connect gate="A" pin="RXCLKIN+" pad="18"/>
<connect gate="A" pin="RXCLKIN-" pad="17"/>
<connect gate="A" pin="RXCLK_OUT" pad="26"/>
<connect gate="A" pin="RXIN0+" pad="10"/>
<connect gate="A" pin="RXIN0-" pad="9"/>
<connect gate="A" pin="RXIN1+" pad="12"/>
<connect gate="A" pin="RXIN1-" pad="11"/>
<connect gate="A" pin="RXIN2+" pad="16"/>
<connect gate="A" pin="RXIN2-" pad="15"/>
<connect gate="A" pin="RXIN3+" pad="20"/>
<connect gate="A" pin="RXIN3-" pad="19"/>
<connect gate="A" pin="RXOUT0" pad="27"/>
<connect gate="A" pin="RXOUT1" pad="29"/>
<connect gate="A" pin="RXOUT10" pad="41"/>
<connect gate="A" pin="RXOUT11" pad="42"/>
<connect gate="A" pin="RXOUT12" pad="43"/>
<connect gate="A" pin="RXOUT13" pad="45"/>
<connect gate="A" pin="RXOUT14" pad="46"/>
<connect gate="A" pin="RXOUT15" pad="47"/>
<connect gate="A" pin="RXOUT16" pad="49"/>
<connect gate="A" pin="RXOUT17" pad="50"/>
<connect gate="A" pin="RXOUT18" pad="51"/>
<connect gate="A" pin="RXOUT19" pad="53"/>
<connect gate="A" pin="RXOUT2" pad="30"/>
<connect gate="A" pin="RXOUT20" pad="54"/>
<connect gate="A" pin="RXOUT21" pad="55"/>
<connect gate="A" pin="RXOUT22" pad="1"/>
<connect gate="A" pin="RXOUT23" pad="2"/>
<connect gate="A" pin="RXOUT24" pad="3"/>
<connect gate="A" pin="RXOUT25" pad="5"/>
<connect gate="A" pin="RXOUT26" pad="6"/>
<connect gate="A" pin="RXOUT27" pad="7"/>
<connect gate="A" pin="RXOUT3" pad="32"/>
<connect gate="A" pin="RXOUT4" pad="33"/>
<connect gate="A" pin="RXOUT5" pad="34"/>
<connect gate="A" pin="RXOUT6" pad="35"/>
<connect gate="A" pin="RXOUT7" pad="37"/>
<connect gate="A" pin="RXOUT8" pad="38"/>
<connect gate="A" pin="RXOUT9" pad="39"/>
<connect gate="A" pin="VCC" pad="48"/>
<connect gate="A" pin="VCC_2" pad="31"/>
<connect gate="A" pin="VCC_3" pad="40"/>
<connect gate="A" pin="VCC_4" pad="56"/>
<connect gate="A" pin="~PWRDN" pad="25"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS90CR288AMTD"/>
<attribute name="OC_FARNELL" value="1685539"/>
<attribute name="OC_NEWARK" value="41K2011"/>
<attribute name="PACKAGE" value="SOP-56"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS90CR482VS" prefix="U">
<description>48-Bit LVDS Channel Link SER/DES</description>
<gates>
<gate name="A" symbol="DS90CR482VS"/>
</gates>
<devices>
<device name="" package="QFP50P1600X1600X120-100N">
<connects>
<connect gate="A" pin="DESKEW" pad="4"/>
<connect gate="A" pin="GND" pad="16"/>
<connect gate="A" pin="GND_2" pad="7"/>
<connect gate="A" pin="GND_3" pad="35"/>
<connect gate="A" pin="GND_4" pad="25"/>
<connect gate="A" pin="GND_5" pad="44"/>
<connect gate="A" pin="GND_6" pad="63"/>
<connect gate="A" pin="GND_7" pad="72"/>
<connect gate="A" pin="GND_8" pad="54"/>
<connect gate="A" pin="LVDSGND" pad="100"/>
<connect gate="A" pin="LVDSGND_2" pad="76"/>
<connect gate="A" pin="LVDSGND_3" pad="88"/>
<connect gate="A" pin="LVDSVCC" pad="93"/>
<connect gate="A" pin="LVDSVCC_2" pad="81"/>
<connect gate="A" pin="NC" pad="75"/>
<connect gate="A" pin="NC_2" pad="69"/>
<connect gate="A" pin="NC_3" pad="70"/>
<connect gate="A" pin="NC_4" pad="71"/>
<connect gate="A" pin="NC_5" pad="73"/>
<connect gate="A" pin="NC_6" pad="74"/>
<connect gate="A" pin="PLLGND" pad="3"/>
<connect gate="A" pin="PLLGND_2" pad="1"/>
<connect gate="A" pin="PLLSEL" pad="5"/>
<connect gate="A" pin="PLLVCC" pad="2"/>
<connect gate="A" pin="RXCLKM" pad="92"/>
<connect gate="A" pin="RXCLKOUT" pad="42"/>
<connect gate="A" pin="RXCLKP" pad="91"/>
<connect gate="A" pin="RXIN0M" pad="99"/>
<connect gate="A" pin="RXIN0P" pad="98"/>
<connect gate="A" pin="RXIN1M" pad="97"/>
<connect gate="A" pin="RXIN1P" pad="96"/>
<connect gate="A" pin="RXINM2" pad="95"/>
<connect gate="A" pin="RXINM3" pad="90"/>
<connect gate="A" pin="RXINM4" pad="87"/>
<connect gate="A" pin="RXINM5" pad="85"/>
<connect gate="A" pin="RXINM6" pad="83"/>
<connect gate="A" pin="RXINM7" pad="80"/>
<connect gate="A" pin="RXINP2" pad="94"/>
<connect gate="A" pin="RXINP3" pad="89"/>
<connect gate="A" pin="RXINP4" pad="86"/>
<connect gate="A" pin="RXINP5" pad="84"/>
<connect gate="A" pin="RXINP6" pad="82"/>
<connect gate="A" pin="RXINP7" pad="79"/>
<connect gate="A" pin="RXOUT0" pad="8"/>
<connect gate="A" pin="RXOUT1" pad="9"/>
<connect gate="A" pin="RXOUT10" pad="20"/>
<connect gate="A" pin="RXOUT11" pad="21"/>
<connect gate="A" pin="RXOUT12" pad="22"/>
<connect gate="A" pin="RXOUT13" pad="24"/>
<connect gate="A" pin="RXOUT14" pad="26"/>
<connect gate="A" pin="RXOUT15" pad="27"/>
<connect gate="A" pin="RXOUT16" pad="28"/>
<connect gate="A" pin="RXOUT17" pad="29"/>
<connect gate="A" pin="RXOUT18" pad="30"/>
<connect gate="A" pin="RXOUT19" pad="31"/>
<connect gate="A" pin="RXOUT2" pad="10"/>
<connect gate="A" pin="RXOUT20" pad="32"/>
<connect gate="A" pin="RXOUT21" pad="34"/>
<connect gate="A" pin="RXOUT22" pad="36"/>
<connect gate="A" pin="RXOUT23" pad="37"/>
<connect gate="A" pin="RXOUT24" pad="38"/>
<connect gate="A" pin="RXOUT25" pad="39"/>
<connect gate="A" pin="RXOUT26" pad="40"/>
<connect gate="A" pin="RXOUT27" pad="41"/>
<connect gate="A" pin="RXOUT28" pad="43"/>
<connect gate="A" pin="RXOUT29" pad="46"/>
<connect gate="A" pin="RXOUT3" pad="11"/>
<connect gate="A" pin="RXOUT30" pad="47"/>
<connect gate="A" pin="RXOUT31" pad="48"/>
<connect gate="A" pin="RXOUT32" pad="49"/>
<connect gate="A" pin="RXOUT33" pad="50"/>
<connect gate="A" pin="RXOUT34" pad="51"/>
<connect gate="A" pin="RXOUT35" pad="52"/>
<connect gate="A" pin="RXOUT36" pad="53"/>
<connect gate="A" pin="RXOUT37" pad="55"/>
<connect gate="A" pin="RXOUT38" pad="57"/>
<connect gate="A" pin="RXOUT39" pad="58"/>
<connect gate="A" pin="RXOUT4" pad="12"/>
<connect gate="A" pin="RXOUT40" pad="59"/>
<connect gate="A" pin="RXOUT41" pad="60"/>
<connect gate="A" pin="RXOUT42" pad="61"/>
<connect gate="A" pin="RXOUT43" pad="62"/>
<connect gate="A" pin="RXOUT44" pad="64"/>
<connect gate="A" pin="RXOUT45" pad="65"/>
<connect gate="A" pin="RXOUT46" pad="67"/>
<connect gate="A" pin="RXOUT47" pad="68"/>
<connect gate="A" pin="RXOUT5" pad="14"/>
<connect gate="A" pin="RXOUT6" pad="15"/>
<connect gate="A" pin="RXOUT7" pad="17"/>
<connect gate="A" pin="RXOUT8" pad="18"/>
<connect gate="A" pin="RXOUT9" pad="19"/>
<connect gate="A" pin="VCC" pad="56"/>
<connect gate="A" pin="VCC_2" pad="33"/>
<connect gate="A" pin="VCC_3" pad="23"/>
<connect gate="A" pin="VCC_4" pad="66"/>
<connect gate="A" pin="VCC_5" pad="6"/>
<connect gate="A" pin="VCC_6" pad="45"/>
<connect gate="A" pin="VCC_7" pad="77"/>
<connect gate="A" pin="VCC_8" pad="13"/>
<connect gate="A" pin="~PD" pad="78"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS90CR482VS"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K2015"/>
<attribute name="PACKAGE" value="QFP-100"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS90CR483AVJD" prefix="U">
<description>48-Bit LVDS Channel Link SER/DES</description>
<gates>
<gate name="A" symbol="DS90CR483AVJD"/>
</gates>
<devices>
<device name="" package="QFP50P1600X1600X120-100N">
<connects>
<connect gate="A" pin="BAL" pad="24"/>
<connect gate="A" pin="DS_OPT" pad="56"/>
<connect gate="A" pin="GND" pad="98"/>
<connect gate="A" pin="GND_2" pad="83"/>
<connect gate="A" pin="GND_3" pad="13"/>
<connect gate="A" pin="GND_4" pad="52"/>
<connect gate="A" pin="GND_5" pad="68"/>
<connect gate="A" pin="LVDSGND" pad="51"/>
<connect gate="A" pin="LVDSGND_2" pad="43"/>
<connect gate="A" pin="LVDSGND_3" pad="25"/>
<connect gate="A" pin="LVDSGND_4" pad="35"/>
<connect gate="A" pin="LVDSVCC" pad="30"/>
<connect gate="A" pin="LVDSVCC_2" pad="40"/>
<connect gate="A" pin="LVDSVCC_3" pad="48"/>
<connect gate="A" pin="NC" pad="55"/>
<connect gate="A" pin="NC_2" pad="26"/>
<connect gate="A" pin="NC_3" pad="27"/>
<connect gate="A" pin="NC_4" pad="54"/>
<connect gate="A" pin="PLLGND" pad="16"/>
<connect gate="A" pin="PLLGND_2" pad="17"/>
<connect gate="A" pin="PLLGND_3" pad="19"/>
<connect gate="A" pin="PLLSEL" pad="15"/>
<connect gate="A" pin="PLLVCC" pad="12"/>
<connect gate="A" pin="PLLVCC_2" pad="18"/>
<connect gate="A" pin="PRE" pad="14"/>
<connect gate="A" pin="TXCLKIN" pad="11"/>
<connect gate="A" pin="TXCLKM" pad="42"/>
<connect gate="A" pin="TXCLKP" pad="41"/>
<connect gate="A" pin="TXIN0" pad="10"/>
<connect gate="A" pin="TXIN1" pad="9"/>
<connect gate="A" pin="TXIN10" pad="100"/>
<connect gate="A" pin="TXIN11" pad="99"/>
<connect gate="A" pin="TXIN12" pad="96"/>
<connect gate="A" pin="TXIN13" pad="95"/>
<connect gate="A" pin="TXIN14" pad="94"/>
<connect gate="A" pin="TXIN15" pad="93"/>
<connect gate="A" pin="TXIN16" pad="92"/>
<connect gate="A" pin="TXIN17" pad="91"/>
<connect gate="A" pin="TXIN18" pad="90"/>
<connect gate="A" pin="TXIN19" pad="89"/>
<connect gate="A" pin="TXIN2" pad="8"/>
<connect gate="A" pin="TXIN20" pad="88"/>
<connect gate="A" pin="TXIN21" pad="87"/>
<connect gate="A" pin="TXIN22" pad="86"/>
<connect gate="A" pin="TXIN23" pad="85"/>
<connect gate="A" pin="TXIN24" pad="84"/>
<connect gate="A" pin="TXIN25" pad="81"/>
<connect gate="A" pin="TXIN26" pad="80"/>
<connect gate="A" pin="TXIN27" pad="79"/>
<connect gate="A" pin="TXIN28" pad="78"/>
<connect gate="A" pin="TXIN29" pad="77"/>
<connect gate="A" pin="TXIN3" pad="7"/>
<connect gate="A" pin="TXIN30" pad="76"/>
<connect gate="A" pin="TXIN31" pad="75"/>
<connect gate="A" pin="TXIN32" pad="74"/>
<connect gate="A" pin="TXIN33" pad="73"/>
<connect gate="A" pin="TXIN34" pad="72"/>
<connect gate="A" pin="TXIN35" pad="71"/>
<connect gate="A" pin="TXIN36" pad="70"/>
<connect gate="A" pin="TXIN37" pad="69"/>
<connect gate="A" pin="TXIN38" pad="66"/>
<connect gate="A" pin="TXIN39" pad="65"/>
<connect gate="A" pin="TXIN4" pad="6"/>
<connect gate="A" pin="TXIN40" pad="64"/>
<connect gate="A" pin="TXIN41" pad="63"/>
<connect gate="A" pin="TXIN42" pad="62"/>
<connect gate="A" pin="TXIN43" pad="61"/>
<connect gate="A" pin="TXIN44" pad="60"/>
<connect gate="A" pin="TXIN45" pad="59"/>
<connect gate="A" pin="TXIN46" pad="58"/>
<connect gate="A" pin="TXIN47" pad="57"/>
<connect gate="A" pin="TXIN5" pad="5"/>
<connect gate="A" pin="TXIN6" pad="4"/>
<connect gate="A" pin="TXIN7" pad="3"/>
<connect gate="A" pin="TXIN8" pad="2"/>
<connect gate="A" pin="TXIN9" pad="1"/>
<connect gate="A" pin="TXOUTM0" pad="50"/>
<connect gate="A" pin="TXOUTM1" pad="47"/>
<connect gate="A" pin="TXOUTM2" pad="45"/>
<connect gate="A" pin="TXOUTM3" pad="39"/>
<connect gate="A" pin="TXOUTM4" pad="37"/>
<connect gate="A" pin="TXOUTM5" pad="34"/>
<connect gate="A" pin="TXOUTM6" pad="32"/>
<connect gate="A" pin="TXOUTM7" pad="29"/>
<connect gate="A" pin="TXOUTP0" pad="49"/>
<connect gate="A" pin="TXOUTP1" pad="46"/>
<connect gate="A" pin="TXOUTP2" pad="44"/>
<connect gate="A" pin="TXOUTP3" pad="38"/>
<connect gate="A" pin="TXOUTP4" pad="36"/>
<connect gate="A" pin="TXOUTP5" pad="33"/>
<connect gate="A" pin="TXOUTP6" pad="31"/>
<connect gate="A" pin="TXOUTP7" pad="28"/>
<connect gate="A" pin="VCC" pad="97"/>
<connect gate="A" pin="VCC_2" pad="67"/>
<connect gate="A" pin="VCC_3" pad="23"/>
<connect gate="A" pin="VCC_4" pad="21"/>
<connect gate="A" pin="VCC_5" pad="20"/>
<connect gate="A" pin="VCC_6" pad="53"/>
<connect gate="A" pin="VCC_7" pad="82"/>
<connect gate="A" pin="~PD" pad="22"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS90CR483AVJD"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="11N9003"/>
<attribute name="PACKAGE" value="QFP-100"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS90CR484AVJD" prefix="U">
<description>48-Bit LVDS Channel Link SER/DES</description>
<gates>
<gate name="A" symbol="DS90CR484AVJD"/>
</gates>
<devices>
<device name="" package="QFP50P1600X1600X120-100N">
<connects>
<connect gate="A" pin="DESKEW" pad="4"/>
<connect gate="A" pin="GND" pad="25"/>
<connect gate="A" pin="GND_2" pad="7"/>
<connect gate="A" pin="GND_3" pad="72"/>
<connect gate="A" pin="GND_4" pad="35"/>
<connect gate="A" pin="GND_5" pad="63"/>
<connect gate="A" pin="GND_6" pad="54"/>
<connect gate="A" pin="GND_7" pad="44"/>
<connect gate="A" pin="GND_8" pad="16"/>
<connect gate="A" pin="LVDSGND" pad="100"/>
<connect gate="A" pin="LVDSGND_2" pad="88"/>
<connect gate="A" pin="LVDSGND_3" pad="76"/>
<connect gate="A" pin="LVDSVCC" pad="93"/>
<connect gate="A" pin="LVDSVCC_2" pad="81"/>
<connect gate="A" pin="NC" pad="75"/>
<connect gate="A" pin="NC_2" pad="70"/>
<connect gate="A" pin="NC_3" pad="71"/>
<connect gate="A" pin="NC_4" pad="73"/>
<connect gate="A" pin="NC_5" pad="74"/>
<connect gate="A" pin="NC_6" pad="69"/>
<connect gate="A" pin="PLLGND" pad="1"/>
<connect gate="A" pin="PLLGND_2" pad="3"/>
<connect gate="A" pin="PLLSEL" pad="5"/>
<connect gate="A" pin="PLLVCC" pad="2"/>
<connect gate="A" pin="RXCLKM" pad="92"/>
<connect gate="A" pin="RXCLKOUT" pad="42"/>
<connect gate="A" pin="RXCLKP" pad="91"/>
<connect gate="A" pin="RXINM0" pad="99"/>
<connect gate="A" pin="RXINM1" pad="97"/>
<connect gate="A" pin="RXINM2" pad="95"/>
<connect gate="A" pin="RXINM3" pad="90"/>
<connect gate="A" pin="RXINM4" pad="87"/>
<connect gate="A" pin="RXINM5" pad="85"/>
<connect gate="A" pin="RXINM6" pad="83"/>
<connect gate="A" pin="RXINM7" pad="80"/>
<connect gate="A" pin="RXINP0" pad="98"/>
<connect gate="A" pin="RXINP1" pad="96"/>
<connect gate="A" pin="RXINP2" pad="94"/>
<connect gate="A" pin="RXINP3" pad="89"/>
<connect gate="A" pin="RXINP4" pad="86"/>
<connect gate="A" pin="RXINP5" pad="84"/>
<connect gate="A" pin="RXINP6" pad="82"/>
<connect gate="A" pin="RXINP7" pad="79"/>
<connect gate="A" pin="RXOUT0" pad="8"/>
<connect gate="A" pin="RXOUT1" pad="9"/>
<connect gate="A" pin="RXOUT10" pad="20"/>
<connect gate="A" pin="RXOUT11" pad="21"/>
<connect gate="A" pin="RXOUT12" pad="22"/>
<connect gate="A" pin="RXOUT13" pad="24"/>
<connect gate="A" pin="RXOUT14" pad="26"/>
<connect gate="A" pin="RXOUT15" pad="27"/>
<connect gate="A" pin="RXOUT16" pad="28"/>
<connect gate="A" pin="RXOUT17" pad="29"/>
<connect gate="A" pin="RXOUT18" pad="30"/>
<connect gate="A" pin="RXOUT19" pad="31"/>
<connect gate="A" pin="RXOUT2" pad="10"/>
<connect gate="A" pin="RXOUT20" pad="32"/>
<connect gate="A" pin="RXOUT21" pad="34"/>
<connect gate="A" pin="RXOUT22" pad="36"/>
<connect gate="A" pin="RXOUT23" pad="37"/>
<connect gate="A" pin="RXOUT24" pad="38"/>
<connect gate="A" pin="RXOUT25" pad="39"/>
<connect gate="A" pin="RXOUT26" pad="40"/>
<connect gate="A" pin="RXOUT27" pad="41"/>
<connect gate="A" pin="RXOUT28" pad="43"/>
<connect gate="A" pin="RXOUT29" pad="46"/>
<connect gate="A" pin="RXOUT3" pad="11"/>
<connect gate="A" pin="RXOUT30" pad="47"/>
<connect gate="A" pin="RXOUT31" pad="48"/>
<connect gate="A" pin="RXOUT32" pad="49"/>
<connect gate="A" pin="RXOUT33" pad="50"/>
<connect gate="A" pin="RXOUT34" pad="51"/>
<connect gate="A" pin="RXOUT35" pad="52"/>
<connect gate="A" pin="RXOUT36" pad="53"/>
<connect gate="A" pin="RXOUT37" pad="55"/>
<connect gate="A" pin="RXOUT38" pad="57"/>
<connect gate="A" pin="RXOUT39" pad="58"/>
<connect gate="A" pin="RXOUT4" pad="12"/>
<connect gate="A" pin="RXOUT40" pad="59"/>
<connect gate="A" pin="RXOUT41" pad="60"/>
<connect gate="A" pin="RXOUT42" pad="61"/>
<connect gate="A" pin="RXOUT43" pad="62"/>
<connect gate="A" pin="RXOUT44" pad="64"/>
<connect gate="A" pin="RXOUT45" pad="65"/>
<connect gate="A" pin="RXOUT46" pad="67"/>
<connect gate="A" pin="RXOUT47" pad="68"/>
<connect gate="A" pin="RXOUT5" pad="14"/>
<connect gate="A" pin="RXOUT6" pad="15"/>
<connect gate="A" pin="RXOUT7" pad="17"/>
<connect gate="A" pin="RXOUT8" pad="18"/>
<connect gate="A" pin="RXOUT9" pad="19"/>
<connect gate="A" pin="VCC" pad="13"/>
<connect gate="A" pin="VCC_2" pad="77"/>
<connect gate="A" pin="VCC_3" pad="6"/>
<connect gate="A" pin="VCC_4" pad="23"/>
<connect gate="A" pin="VCC_5" pad="33"/>
<connect gate="A" pin="VCC_6" pad="56"/>
<connect gate="A" pin="VCC_7" pad="45"/>
<connect gate="A" pin="VCC_8" pad="66"/>
<connect gate="A" pin="~PD" pad="78"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS90CR484AVJD"/>
<attribute name="OC_FARNELL" value="1609182"/>
<attribute name="OC_NEWARK" value="11N9005"/>
<attribute name="PACKAGE" value="QFP-100"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS90CR485VS" prefix="U">
<description>48-bit Channel Link Serializer</description>
<gates>
<gate name="A" symbol="DS90CR485VS"/>
</gates>
<devices>
<device name="" package="QFP50P1600X1600X120-100N">
<connects>
<connect gate="A" pin="BAL" pad="24"/>
<connect gate="A" pin="CLK1M" pad="42"/>
<connect gate="A" pin="CLK1P" pad="41"/>
<connect gate="A" pin="CLKIN" pad="87"/>
<connect gate="A" pin="CON1" pad="18"/>
<connect gate="A" pin="CON2" pad="19"/>
<connect gate="A" pin="CON3" pad="20"/>
<connect gate="A" pin="CON4" pad="23"/>
<connect gate="A" pin="CON5" pad="57"/>
<connect gate="A" pin="CON6" pad="58"/>
<connect gate="A" pin="CON7" pad="74"/>
<connect gate="A" pin="CON8" pad="75"/>
<connect gate="A" pin="D0" pad="8"/>
<connect gate="A" pin="D1" pad="7"/>
<connect gate="A" pin="D10" pad="98"/>
<connect gate="A" pin="D11" pad="97"/>
<connect gate="A" pin="D12" pad="94"/>
<connect gate="A" pin="D13" pad="93"/>
<connect gate="A" pin="D14" pad="92"/>
<connect gate="A" pin="D15" pad="91"/>
<connect gate="A" pin="D16" pad="90"/>
<connect gate="A" pin="D17" pad="89"/>
<connect gate="A" pin="D18" pad="86"/>
<connect gate="A" pin="D19" pad="85"/>
<connect gate="A" pin="D2" pad="6"/>
<connect gate="A" pin="D20" pad="84"/>
<connect gate="A" pin="D21" pad="83"/>
<connect gate="A" pin="D22" pad="82"/>
<connect gate="A" pin="D23" pad="81"/>
<connect gate="A" pin="D3" pad="5"/>
<connect gate="A" pin="D4" pad="4"/>
<connect gate="A" pin="D5" pad="3"/>
<connect gate="A" pin="D6" pad="2"/>
<connect gate="A" pin="D7" pad="1"/>
<connect gate="A" pin="D8" pad="100"/>
<connect gate="A" pin="D9" pad="99"/>
<connect gate="A" pin="DS_OPT" pad="76"/>
<connect gate="A" pin="GND" pad="69"/>
<connect gate="A" pin="GND3" pad="80"/>
<connect gate="A" pin="GND_2" pad="9"/>
<connect gate="A" pin="GND_3" pad="11"/>
<connect gate="A" pin="GND_4" pad="96"/>
<connect gate="A" pin="GND_5" pad="71"/>
<connect gate="A" pin="GND_6" pad="77"/>
<connect gate="A" pin="LVDSGND" pad="52"/>
<connect gate="A" pin="LVDSGND_2" pad="25"/>
<connect gate="A" pin="LVDSGND_3" pad="35"/>
<connect gate="A" pin="LVDSGND_4" pad="51"/>
<connect gate="A" pin="LVDSGND_5" pad="43"/>
<connect gate="A" pin="LVDSVCC" pad="48"/>
<connect gate="A" pin="LVDSVCC_2" pad="40"/>
<connect gate="A" pin="LVDSVCC_3" pad="53"/>
<connect gate="A" pin="LVDSVCC_4" pad="30"/>
<connect gate="A" pin="NC" pad="66"/>
<connect gate="A" pin="NC_10" pad="62"/>
<connect gate="A" pin="NC_11" pad="67"/>
<connect gate="A" pin="NC_12" pad="26"/>
<connect gate="A" pin="NC_13" pad="64"/>
<connect gate="A" pin="NC_14" pad="65"/>
<connect gate="A" pin="NC_2" pad="59"/>
<connect gate="A" pin="NC_3" pad="88"/>
<connect gate="A" pin="NC_4" pad="60"/>
<connect gate="A" pin="NC_5" pad="61"/>
<connect gate="A" pin="NC_6" pad="54"/>
<connect gate="A" pin="NC_7" pad="63"/>
<connect gate="A" pin="NC_8" pad="78"/>
<connect gate="A" pin="NC_9" pad="27"/>
<connect gate="A" pin="PAT_SEL" pad="56"/>
<connect gate="A" pin="PLLGND" pad="17"/>
<connect gate="A" pin="PLLGND_2" pad="14"/>
<connect gate="A" pin="PLLGND_3" pad="15"/>
<connect gate="A" pin="PLLSEL" pad="13"/>
<connect gate="A" pin="PLLVCC" pad="16"/>
<connect gate="A" pin="PLLVCC_2" pad="10"/>
<connect gate="A" pin="PRBS_EN" pad="55"/>
<connect gate="A" pin="PRE" pad="12"/>
<connect gate="A" pin="TEST1" pad="72"/>
<connect gate="A" pin="TEST2" pad="73"/>
<connect gate="A" pin="TSEN" pad="21"/>
<connect gate="A" pin="TXOUT0M" pad="50"/>
<connect gate="A" pin="TXOUT0P" pad="49"/>
<connect gate="A" pin="TXOUT1M" pad="47"/>
<connect gate="A" pin="TXOUT1P" pad="46"/>
<connect gate="A" pin="TXOUT2M" pad="45"/>
<connect gate="A" pin="TXOUT2P" pad="44"/>
<connect gate="A" pin="TXOUT3M" pad="39"/>
<connect gate="A" pin="TXOUT3P" pad="38"/>
<connect gate="A" pin="TXOUT4M" pad="37"/>
<connect gate="A" pin="TXOUT4P" pad="36"/>
<connect gate="A" pin="TXOUT5M" pad="34"/>
<connect gate="A" pin="TXOUT5P" pad="33"/>
<connect gate="A" pin="TXOUT6M" pad="32"/>
<connect gate="A" pin="TXOUT6P" pad="31"/>
<connect gate="A" pin="TXOUT7M" pad="29"/>
<connect gate="A" pin="TXOUT7P" pad="28"/>
<connect gate="A" pin="VCC" pad="70"/>
<connect gate="A" pin="VCC3" pad="79"/>
<connect gate="A" pin="VCC_2" pad="95"/>
<connect gate="A" pin="VCC_3" pad="68"/>
<connect gate="A" pin="~PD" pad="22"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS90CR485VS"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K2021"/>
<attribute name="PACKAGE" value="QFP-100"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS90CR486VS" prefix="U">
<description>48-Bit Channel Link Deserializer</description>
<gates>
<gate name="A" symbol="DS90CR486VS"/>
</gates>
<devices>
<device name="" package="QFP50P1600X1600X120-100N">
<connects>
<connect gate="A" pin="CON1" pad="77"/>
<connect gate="A" pin="DESKEW" pad="4"/>
<connect gate="A" pin="GND" pad="44"/>
<connect gate="A" pin="GND_2" pad="16"/>
<connect gate="A" pin="GND_3" pad="7"/>
<connect gate="A" pin="GND_4" pad="54"/>
<connect gate="A" pin="GND_5" pad="25"/>
<connect gate="A" pin="GND_6" pad="35"/>
<connect gate="A" pin="GND_7" pad="72"/>
<connect gate="A" pin="GND_8" pad="63"/>
<connect gate="A" pin="LVDSGND" pad="100"/>
<connect gate="A" pin="LVDSGND_2" pad="76"/>
<connect gate="A" pin="LVDSGND_3" pad="88"/>
<connect gate="A" pin="LVDSVCC" pad="81"/>
<connect gate="A" pin="LVDSVCC_2" pad="93"/>
<connect gate="A" pin="NC" pad="75"/>
<connect gate="A" pin="NC_2" pad="69"/>
<connect gate="A" pin="NC_3" pad="70"/>
<connect gate="A" pin="NC_4" pad="73"/>
<connect gate="A" pin="NC_5" pad="71"/>
<connect gate="A" pin="NC_6" pad="74"/>
<connect gate="A" pin="PLLGND" pad="3"/>
<connect gate="A" pin="PLLGND_2" pad="1"/>
<connect gate="A" pin="PLLSEL" pad="5"/>
<connect gate="A" pin="PLLVCC" pad="2"/>
<connect gate="A" pin="RXCLKM" pad="92"/>
<connect gate="A" pin="RXCLKOUT" pad="42"/>
<connect gate="A" pin="RXCLKP" pad="91"/>
<connect gate="A" pin="RXIN0M" pad="99"/>
<connect gate="A" pin="RXIN0P" pad="98"/>
<connect gate="A" pin="RXIN1M" pad="97"/>
<connect gate="A" pin="RXIN1P" pad="96"/>
<connect gate="A" pin="RXINM2" pad="95"/>
<connect gate="A" pin="RXINM3" pad="90"/>
<connect gate="A" pin="RXINM4" pad="87"/>
<connect gate="A" pin="RXINM5" pad="85"/>
<connect gate="A" pin="RXINM6" pad="83"/>
<connect gate="A" pin="RXINM7" pad="80"/>
<connect gate="A" pin="RXINP2" pad="94"/>
<connect gate="A" pin="RXINP3" pad="89"/>
<connect gate="A" pin="RXINP4" pad="86"/>
<connect gate="A" pin="RXINP5" pad="84"/>
<connect gate="A" pin="RXINP6" pad="82"/>
<connect gate="A" pin="RXINP7" pad="79"/>
<connect gate="A" pin="RXOUT0" pad="8"/>
<connect gate="A" pin="RXOUT1" pad="9"/>
<connect gate="A" pin="RXOUT10" pad="20"/>
<connect gate="A" pin="RXOUT11" pad="21"/>
<connect gate="A" pin="RXOUT12" pad="22"/>
<connect gate="A" pin="RXOUT13" pad="24"/>
<connect gate="A" pin="RXOUT14" pad="26"/>
<connect gate="A" pin="RXOUT15" pad="27"/>
<connect gate="A" pin="RXOUT16" pad="28"/>
<connect gate="A" pin="RXOUT17" pad="29"/>
<connect gate="A" pin="RXOUT18" pad="30"/>
<connect gate="A" pin="RXOUT19" pad="31"/>
<connect gate="A" pin="RXOUT2" pad="10"/>
<connect gate="A" pin="RXOUT20" pad="32"/>
<connect gate="A" pin="RXOUT21" pad="34"/>
<connect gate="A" pin="RXOUT22" pad="36"/>
<connect gate="A" pin="RXOUT23" pad="37"/>
<connect gate="A" pin="RXOUT24" pad="38"/>
<connect gate="A" pin="RXOUT25" pad="39"/>
<connect gate="A" pin="RXOUT26" pad="40"/>
<connect gate="A" pin="RXOUT27" pad="41"/>
<connect gate="A" pin="RXOUT28" pad="43"/>
<connect gate="A" pin="RXOUT29" pad="46"/>
<connect gate="A" pin="RXOUT3" pad="11"/>
<connect gate="A" pin="RXOUT30" pad="47"/>
<connect gate="A" pin="RXOUT31" pad="48"/>
<connect gate="A" pin="RXOUT32" pad="49"/>
<connect gate="A" pin="RXOUT33" pad="50"/>
<connect gate="A" pin="RXOUT34" pad="51"/>
<connect gate="A" pin="RXOUT35" pad="52"/>
<connect gate="A" pin="RXOUT36" pad="53"/>
<connect gate="A" pin="RXOUT37" pad="55"/>
<connect gate="A" pin="RXOUT38" pad="57"/>
<connect gate="A" pin="RXOUT39" pad="58"/>
<connect gate="A" pin="RXOUT4" pad="12"/>
<connect gate="A" pin="RXOUT40" pad="59"/>
<connect gate="A" pin="RXOUT41" pad="60"/>
<connect gate="A" pin="RXOUT42" pad="61"/>
<connect gate="A" pin="RXOUT43" pad="62"/>
<connect gate="A" pin="RXOUT44" pad="64"/>
<connect gate="A" pin="RXOUT45" pad="65"/>
<connect gate="A" pin="RXOUT46" pad="67"/>
<connect gate="A" pin="RXOUT47" pad="68"/>
<connect gate="A" pin="RXOUT5" pad="14"/>
<connect gate="A" pin="RXOUT6" pad="15"/>
<connect gate="A" pin="RXOUT7" pad="17"/>
<connect gate="A" pin="RXOUT8" pad="18"/>
<connect gate="A" pin="RXOUT9" pad="19"/>
<connect gate="A" pin="VCC" pad="33"/>
<connect gate="A" pin="VCC_2" pad="45"/>
<connect gate="A" pin="VCC_3" pad="56"/>
<connect gate="A" pin="VCC_4" pad="66"/>
<connect gate="A" pin="VCC_5" pad="6"/>
<connect gate="A" pin="VCC_6" pad="13"/>
<connect gate="A" pin="VCC_7" pad="23"/>
<connect gate="A" pin="~PD" pad="78"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS90CR486VS"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K2023"/>
<attribute name="PACKAGE" value="QFP-80"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS90LT012AHMF" prefix="U">
<description>Line Receiver</description>
<gates>
<gate name="A" symbol="DS90LT012AHMF"/>
</gates>
<devices>
<device name="" package="SOT95P284X122-5N">
<connects>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="IN+" pad="3"/>
<connect gate="A" pin="IN-" pad="4"/>
<connect gate="A" pin="TTLOUT" pad="5"/>
<connect gate="A" pin="VDD" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS90LT012AHMF"/>
<attribute name="OC_FARNELL" value="1694617"/>
<attribute name="OC_NEWARK" value="69K2107"/>
<attribute name="PACKAGE" value="SOT-23-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS90LT012AQMF" prefix="U">
<description>Line Receiver</description>
<gates>
<gate name="A" symbol="DS90LT012AQMF"/>
</gates>
<devices>
<device name="" package="SOT95P284X119-5N">
<connects>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="IN+" pad="3"/>
<connect gate="A" pin="IN-" pad="4"/>
<connect gate="A" pin="TTLOUT" pad="5"/>
<connect gate="A" pin="VDD" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS90LT012AQMF"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="04R8391"/>
<attribute name="PACKAGE" value="SOT-23-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS90LT012ATMF" prefix="U">
<description>CMOS Differential Line Receiver</description>
<gates>
<gate name="A" symbol="DS90LT012ATMF"/>
</gates>
<devices>
<device name="" package="SOT95P284X122-5N">
<connects>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="IN+" pad="3"/>
<connect gate="A" pin="IN-" pad="4"/>
<connect gate="A" pin="TTL_OUT" pad="5"/>
<connect gate="A" pin="VDD" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS90LT012ATMF"/>
<attribute name="OC_FARNELL" value="1798308"/>
<attribute name="OC_NEWARK" value="73R9502"/>
<attribute name="PACKAGE" value="SOT23-5"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS90LV001TLD" prefix="U">
<description>LVDS Buffer</description>
<gates>
<gate name="A" symbol="DS90LV001TLD"/>
</gates>
<devices>
<device name="" package="DFN300X300X80-9N">
<connects>
<connect gate="A" pin="EN" pad="8"/>
<connect gate="A" pin="EP" pad="9"/>
<connect gate="A" pin="GND" pad="1"/>
<connect gate="A" pin="IN+" pad="3"/>
<connect gate="A" pin="IN-" pad="2"/>
<connect gate="A" pin="NC" pad="4"/>
<connect gate="A" pin="OUT+" pad="6"/>
<connect gate="A" pin="OUT-" pad="7"/>
<connect gate="A" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS90LV001TLD"/>
<attribute name="OC_FARNELL" value="1798309"/>
<attribute name="OC_NEWARK" value="73R9503"/>
<attribute name="PACKAGE" value="LLP-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS90LV001TM" prefix="U">
<description>LVDS Buffer</description>
<gates>
<gate name="A" symbol="DS90LV001TM"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="EN" pad="8"/>
<connect gate="A" pin="GND" pad="1"/>
<connect gate="A" pin="IN+" pad="3"/>
<connect gate="A" pin="IN_-" pad="2"/>
<connect gate="A" pin="NC" pad="4"/>
<connect gate="A" pin="OUT+" pad="6"/>
<connect gate="A" pin="OUT-" pad="7"/>
<connect gate="A" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS90LV001TM"/>
<attribute name="OC_FARNELL" value="1286824"/>
<attribute name="OC_NEWARK" value="41K2059"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS90LV004TVS" prefix="U">
<description>LVDS Buffer/Repeater</description>
<gates>
<gate name="A" symbol="DS90LV004TVS"/>
</gates>
<devices>
<device name="" package="QFP50P900X900X120-48N">
<connects>
<connect gate="A" pin="GND" pad="26"/>
<connect gate="A" pin="GND_10" pad="18"/>
<connect gate="A" pin="GND_11" pad="23"/>
<connect gate="A" pin="GND_12" pad="24"/>
<connect gate="A" pin="GND_2" pad="38"/>
<connect gate="A" pin="GND_3" pad="43"/>
<connect gate="A" pin="GND_4" pad="9"/>
<connect gate="A" pin="GND_5" pad="17"/>
<connect gate="A" pin="GND_6" pad="37"/>
<connect gate="A" pin="GND_7" pad="8"/>
<connect gate="A" pin="GND_8" pad="44"/>
<connect gate="A" pin="GND_9" pad="25"/>
<connect gate="A" pin="IN0+" pad="13"/>
<connect gate="A" pin="IN0-" pad="14"/>
<connect gate="A" pin="IN1+" pad="15"/>
<connect gate="A" pin="IN1-" pad="16"/>
<connect gate="A" pin="IN2+" pad="19"/>
<connect gate="A" pin="IN2-" pad="20"/>
<connect gate="A" pin="IN3+" pad="21"/>
<connect gate="A" pin="IN3-" pad="22"/>
<connect gate="A" pin="N/C" pad="35"/>
<connect gate="A" pin="N/C_2" pad="30"/>
<connect gate="A" pin="N/C_3" pad="31"/>
<connect gate="A" pin="N/C_4" pad="6"/>
<connect gate="A" pin="N/C_5" pad="36"/>
<connect gate="A" pin="OUT0+" pad="48"/>
<connect gate="A" pin="OUT0-" pad="47"/>
<connect gate="A" pin="OUT1+" pad="46"/>
<connect gate="A" pin="OUT1-" pad="45"/>
<connect gate="A" pin="OUT2+" pad="42"/>
<connect gate="A" pin="OUT2-" pad="41"/>
<connect gate="A" pin="OUT3+" pad="40"/>
<connect gate="A" pin="OUT3-" pad="39"/>
<connect gate="A" pin="PEM0" pad="1"/>
<connect gate="A" pin="PEM1" pad="2"/>
<connect gate="A" pin="VDD" pad="33"/>
<connect gate="A" pin="VDD_10" pad="32"/>
<connect gate="A" pin="VDD_11" pad="34"/>
<connect gate="A" pin="VDD_12" pad="3"/>
<connect gate="A" pin="VDD_2" pad="4"/>
<connect gate="A" pin="VDD_3" pad="5"/>
<connect gate="A" pin="VDD_4" pad="27"/>
<connect gate="A" pin="VDD_5" pad="10"/>
<connect gate="A" pin="VDD_6" pad="29"/>
<connect gate="A" pin="VDD_7" pad="7"/>
<connect gate="A" pin="VDD_8" pad="28"/>
<connect gate="A" pin="VDD_9" pad="11"/>
<connect gate="A" pin="~PWDN" pad="12"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS90LV004TVS"/>
<attribute name="OC_FARNELL" value="1528378"/>
<attribute name="OC_NEWARK" value="65K5420"/>
<attribute name="PACKAGE" value="PQFP-48"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS90LV011AHMF" prefix="U">
<description>Differential Driver</description>
<gates>
<gate name="A" symbol="DS90LV011AHMF"/>
</gates>
<devices>
<device name="" package="SOT95P284X119-5N">
<connects>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="OUT+" pad="4"/>
<connect gate="A" pin="OUT-" pad="3"/>
<connect gate="A" pin="TTL_IN" pad="5"/>
<connect gate="A" pin="VDD" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS90LV011AHMF"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="69K2111"/>
<attribute name="PACKAGE" value="SOT-23-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS90LV011AQMF" prefix="U">
<description>DS90LV011AQ.pdf</description>
<gates>
<gate name="A" symbol="DS90LV011AQMF"/>
</gates>
<devices>
<device name="" package="SOT95P284X119-5N">
<connects>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="OUT+" pad="4"/>
<connect gate="A" pin="OUT-" pad="3"/>
<connect gate="A" pin="TTL_IN" pad="5"/>
<connect gate="A" pin="VDD" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS90LV011AQMF"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="34P4069"/>
<attribute name="PACKAGE" value="SOT-23-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS90LV011ATMF" prefix="U">
<description>Differential Driver</description>
<gates>
<gate name="A" symbol="DS90LV011ATMF"/>
</gates>
<devices>
<device name="" package="SOT95P284X119-5N">
<connects>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="OUT+" pad="4"/>
<connect gate="A" pin="OUT-" pad="3"/>
<connect gate="A" pin="TTL_IN" pad="5"/>
<connect gate="A" pin="VDD" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS90LV011ATMF"/>
<attribute name="OC_FARNELL" value="8206821"/>
<attribute name="OC_NEWARK" value="41K2063"/>
<attribute name="PACKAGE" value="SOT23-5"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS90LV012ATMF" prefix="U">
<description>Line Receiver</description>
<gates>
<gate name="A" symbol="DS90LV012ATMF"/>
</gates>
<devices>
<device name="" package="SOT95P284X122-5N">
<connects>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="IN+" pad="3"/>
<connect gate="A" pin="IN-" pad="4"/>
<connect gate="A" pin="TTLOUT" pad="5"/>
<connect gate="A" pin="VDD" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS90LV012ATMF"/>
<attribute name="OC_FARNELL" value="1468993"/>
<attribute name="OC_NEWARK" value="26H3907"/>
<attribute name="PACKAGE" value="SOT-23-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS90LV017ATM" prefix="U">
<description>Driver</description>
<gates>
<gate name="A" symbol="DS90LV017ATM"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="DI1" pad="2"/>
<connect gate="A" pin="DO1+" pad="7"/>
<connect gate="A" pin="DO1-" pad="8"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="NC" pad="3"/>
<connect gate="A" pin="NC_2" pad="5"/>
<connect gate="A" pin="NC_3" pad="6"/>
<connect gate="A" pin="VCC" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS90LV017ATM"/>
<attribute name="OC_FARNELL" value="1286825"/>
<attribute name="OC_NEWARK" value="41K2069"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS90LV018ATM" prefix="U">
<description>Line Receiver</description>
<gates>
<gate name="A" symbol="DS90LV018ATM"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="NC" pad="4"/>
<connect gate="A" pin="NC_2" pad="6"/>
<connect gate="A" pin="NC_3" pad="3"/>
<connect gate="A" pin="RIN1+" pad="2"/>
<connect gate="A" pin="RIN1-" pad="1"/>
<connect gate="A" pin="ROUT1" pad="7"/>
<connect gate="A" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS90LV018ATM"/>
<attribute name="OC_FARNELL" value="9485821"/>
<attribute name="OC_NEWARK" value="83F4647"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS90LV019TM" prefix="U">
<description>LVDS Driver/Receiver</description>
<gates>
<gate name="A" symbol="DS90LV019TM"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-14N">
<connects>
<connect gate="A" pin="DE" pad="1"/>
<connect gate="A" pin="DIN" pad="2"/>
<connect gate="A" pin="DO+" pad="12"/>
<connect gate="A" pin="DO-" pad="11"/>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="NC" pad="6"/>
<connect gate="A" pin="NC_2" pad="3"/>
<connect gate="A" pin="NC_3" pad="5"/>
<connect gate="A" pin="NC_4" pad="13"/>
<connect gate="A" pin="RI+" pad="10"/>
<connect gate="A" pin="RI-" pad="9"/>
<connect gate="A" pin="ROUT" pad="4"/>
<connect gate="A" pin="VCC" pad="14"/>
<connect gate="A" pin="~RE" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS90LV019TM"/>
<attribute name="OC_FARNELL" value="1286826"/>
<attribute name="OC_NEWARK" value="83F4629"/>
<attribute name="PACKAGE" value="SOP-14"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS90LV019TMTC" prefix="U">
<description>LVDS Driver/Receiver</description>
<gates>
<gate name="A" symbol="DS90LV019TMTC"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-14N">
<connects>
<connect gate="A" pin="DE" pad="1"/>
<connect gate="A" pin="DIN" pad="2"/>
<connect gate="A" pin="DO+" pad="12"/>
<connect gate="A" pin="DO-" pad="11"/>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="NC" pad="6"/>
<connect gate="A" pin="NC_2" pad="3"/>
<connect gate="A" pin="NC_3" pad="5"/>
<connect gate="A" pin="NC_4" pad="13"/>
<connect gate="A" pin="RI+" pad="10"/>
<connect gate="A" pin="RI-" pad="9"/>
<connect gate="A" pin="ROUT" pad="4"/>
<connect gate="A" pin="VCC" pad="14"/>
<connect gate="A" pin="~RE" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS90LV019TMTC"/>
<attribute name="OC_FARNELL" value="1286826"/>
<attribute name="OC_NEWARK" value="38K1016"/>
<attribute name="PACKAGE" value="SOP-14"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS90LV027AQMA" prefix="U">
<description>Differential Driver</description>
<gates>
<gate name="A" symbol="DS90LV027AQMA"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="DI1" pad="2"/>
<connect gate="A" pin="DI2" pad="3"/>
<connect gate="A" pin="DO+1" pad="7"/>
<connect gate="A" pin="DO+2" pad="6"/>
<connect gate="A" pin="DO-1" pad="8"/>
<connect gate="A" pin="DO-2" pad="5"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="VCC" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS90LV027AQMA"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="07P4971"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS90LV027ATM" prefix="U">
<description>Differential Driver</description>
<gates>
<gate name="A" symbol="DS90LV027ATM"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8">
<connects>
<connect gate="A" pin="DI1" pad="2"/>
<connect gate="A" pin="DI2" pad="3"/>
<connect gate="A" pin="DO+1" pad="7"/>
<connect gate="A" pin="DO+2" pad="6"/>
<connect gate="A" pin="DO-1" pad="8"/>
<connect gate="A" pin="DO-2" pad="5"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="VCC" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS90LV027ATM"/>
<attribute name="OC_FARNELL" value="1468976"/>
<attribute name="OC_NEWARK" value="41K2078"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS90LV028AHM" prefix="U">
<description>Line Receiver</description>
<gates>
<gate name="A" symbol="DS90LV028AHM"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="RIN1+" pad="2"/>
<connect gate="A" pin="RIN1-" pad="1"/>
<connect gate="A" pin="RIN2+" pad="3"/>
<connect gate="A" pin="RIN2-" pad="4"/>
<connect gate="A" pin="ROUT1" pad="7"/>
<connect gate="A" pin="ROUT2" pad="6"/>
<connect gate="A" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS90LV028AHM"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="69K2119"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS90LV028AQMA" prefix="U">
<description>LVDS DUAL RECEIVER AEC-Q</description>
<gates>
<gate name="A" symbol="DS90LV028AQMA"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="RIN1+" pad="2"/>
<connect gate="A" pin="RIN1-" pad="1"/>
<connect gate="A" pin="RIN2+" pad="3"/>
<connect gate="A" pin="RIN2-" pad="4"/>
<connect gate="A" pin="ROUT1" pad="7"/>
<connect gate="A" pin="ROUT2" pad="6"/>
<connect gate="A" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS90LV028AQMA"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="07P4973"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS90LV028ATM" prefix="U">
<description>Line Receiver</description>
<gates>
<gate name="A" symbol="DS90LV028ATM"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="RIN1+" pad="2"/>
<connect gate="A" pin="RIN1-" pad="1"/>
<connect gate="A" pin="RIN2+" pad="3"/>
<connect gate="A" pin="RIN2-" pad="4"/>
<connect gate="A" pin="ROUT1" pad="7"/>
<connect gate="A" pin="ROUT2" pad="6"/>
<connect gate="A" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS90LV028ATM"/>
<attribute name="OC_FARNELL" value="9485830"/>
<attribute name="OC_NEWARK" value="09K7532"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS90LV031ATM" prefix="U">
<description>Line Driver</description>
<gates>
<gate name="A" symbol="DS90LV031ATM"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-16N">
<connects>
<connect gate="A" pin="DIN1" pad="1"/>
<connect gate="A" pin="DIN2" pad="7"/>
<connect gate="A" pin="DIN3" pad="9"/>
<connect gate="A" pin="DIN4" pad="15"/>
<connect gate="A" pin="DOUT1+" pad="2"/>
<connect gate="A" pin="DOUT1-" pad="3"/>
<connect gate="A" pin="DOUT2+" pad="6"/>
<connect gate="A" pin="DOUT2-" pad="5"/>
<connect gate="A" pin="DOUT3+" pad="10"/>
<connect gate="A" pin="DOUT3-" pad="11"/>
<connect gate="A" pin="DOUT4+" pad="14"/>
<connect gate="A" pin="DOUT4-" pad="13"/>
<connect gate="A" pin="EN" pad="4"/>
<connect gate="A" pin="GND" pad="8"/>
<connect gate="A" pin="VCC" pad="16"/>
<connect gate="A" pin="~EN" pad="12"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS90LV031ATM"/>
<attribute name="OC_FARNELL" value="1468994"/>
<attribute name="OC_NEWARK" value="41K2084"/>
<attribute name="PACKAGE" value="SOIC-16"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS90LV031ATMTC" prefix="U">
<description>Line Driver</description>
<gates>
<gate name="A" symbol="DS90LV031ATMTC"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-16N">
<connects>
<connect gate="A" pin="DIN1" pad="1"/>
<connect gate="A" pin="DIN2" pad="7"/>
<connect gate="A" pin="DIN3" pad="9"/>
<connect gate="A" pin="DIN4" pad="15"/>
<connect gate="A" pin="DOUT1+" pad="2"/>
<connect gate="A" pin="DOUT1-" pad="3"/>
<connect gate="A" pin="DOUT2+" pad="6"/>
<connect gate="A" pin="DOUT2-" pad="5"/>
<connect gate="A" pin="DOUT3+" pad="10"/>
<connect gate="A" pin="DOUT3-" pad="11"/>
<connect gate="A" pin="DOUT4+" pad="14"/>
<connect gate="A" pin="DOUT4-" pad="13"/>
<connect gate="A" pin="EN" pad="4"/>
<connect gate="A" pin="GND" pad="8"/>
<connect gate="A" pin="VCC" pad="16"/>
<connect gate="A" pin="~EN" pad="12"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS90LV031ATMTC"/>
<attribute name="OC_FARNELL" value="1468995"/>
<attribute name="OC_NEWARK" value="41K2085"/>
<attribute name="PACKAGE" value="TSSOP-16"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS90LV032ATM" prefix="U">
<description>Line Receiver</description>
<gates>
<gate name="A" symbol="DS90LV032ATM"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-16N">
<connects>
<connect gate="A" pin="EN" pad="4"/>
<connect gate="A" pin="GND" pad="8"/>
<connect gate="A" pin="RIN1+" pad="2"/>
<connect gate="A" pin="RIN1-" pad="1"/>
<connect gate="A" pin="RIN2+" pad="6"/>
<connect gate="A" pin="RIN2-" pad="7"/>
<connect gate="A" pin="RIN3+" pad="10"/>
<connect gate="A" pin="RIN3-" pad="9"/>
<connect gate="A" pin="RIN4+" pad="14"/>
<connect gate="A" pin="RIN4-" pad="15"/>
<connect gate="A" pin="ROUT1" pad="3"/>
<connect gate="A" pin="ROUT2" pad="5"/>
<connect gate="A" pin="ROUT3" pad="11"/>
<connect gate="A" pin="ROUT4" pad="13"/>
<connect gate="A" pin="VCC" pad="16"/>
<connect gate="A" pin="~EN" pad="12"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS90LV032ATM"/>
<attribute name="OC_FARNELL" value="1469003"/>
<attribute name="OC_NEWARK" value="41K2089"/>
<attribute name="PACKAGE" value="SOIC-16"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS90LV032ATMTC" prefix="U">
<description>Line Receiver</description>
<gates>
<gate name="A" symbol="DS90LV032ATMTC"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-16N">
<connects>
<connect gate="A" pin="EN" pad="4"/>
<connect gate="A" pin="GND" pad="8"/>
<connect gate="A" pin="RIN1+" pad="2"/>
<connect gate="A" pin="RIN1-" pad="1"/>
<connect gate="A" pin="RIN2+" pad="6"/>
<connect gate="A" pin="RIN2-" pad="7"/>
<connect gate="A" pin="RIN3+" pad="10"/>
<connect gate="A" pin="RIN3-" pad="9"/>
<connect gate="A" pin="RIN4+" pad="14"/>
<connect gate="A" pin="RIN4-" pad="15"/>
<connect gate="A" pin="ROUT1" pad="3"/>
<connect gate="A" pin="ROUT2" pad="5"/>
<connect gate="A" pin="ROUT3" pad="11"/>
<connect gate="A" pin="ROUT4" pad="13"/>
<connect gate="A" pin="VCC" pad="16"/>
<connect gate="A" pin="~EN" pad="12"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS90LV032ATMTC"/>
<attribute name="OC_FARNELL" value="1211795"/>
<attribute name="OC_NEWARK" value="41K2090"/>
<attribute name="PACKAGE" value="TSSOP-16"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS90LV047ATM" prefix="U">
<description>CMOS Differential Line Driver</description>
<gates>
<gate name="A" symbol="DS90LV047ATM"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-16N">
<connects>
<connect gate="A" pin="DIN1" pad="2"/>
<connect gate="A" pin="DIN2" pad="3"/>
<connect gate="A" pin="DIN3" pad="6"/>
<connect gate="A" pin="DIN4" pad="7"/>
<connect gate="A" pin="DOUT1+" pad="15"/>
<connect gate="A" pin="DOUT1-" pad="16"/>
<connect gate="A" pin="DOUT2+" pad="14"/>
<connect gate="A" pin="DOUT2-" pad="13"/>
<connect gate="A" pin="DOUT3+" pad="11"/>
<connect gate="A" pin="DOUT3-" pad="12"/>
<connect gate="A" pin="DOUT4+" pad="10"/>
<connect gate="A" pin="DOUT4-" pad="9"/>
<connect gate="A" pin="EN" pad="1"/>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="VCC" pad="4"/>
<connect gate="A" pin="~EN" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS90LV047ATM"/>
<attribute name="OC_FARNELL" value="9485848"/>
<attribute name="OC_NEWARK" value="41K2093"/>
<attribute name="PACKAGE" value="16-SOIC"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS90LV047ATMTC" prefix="U">
<description>CMOS Differential Line Driver</description>
<gates>
<gate name="A" symbol="DS90LV047ATMTC"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-16N">
<connects>
<connect gate="A" pin="*EN" pad="8"/>
<connect gate="A" pin="DIN1" pad="2"/>
<connect gate="A" pin="DIN2" pad="3"/>
<connect gate="A" pin="DIN3" pad="6"/>
<connect gate="A" pin="DIN4" pad="7"/>
<connect gate="A" pin="DOUT1+" pad="15"/>
<connect gate="A" pin="DOUT1-" pad="16"/>
<connect gate="A" pin="DOUT2+" pad="14"/>
<connect gate="A" pin="DOUT2-" pad="13"/>
<connect gate="A" pin="DOUT3+" pad="11"/>
<connect gate="A" pin="DOUT3-" pad="12"/>
<connect gate="A" pin="DOUT4+" pad="10"/>
<connect gate="A" pin="DOUT4-" pad="9"/>
<connect gate="A" pin="EN" pad="1"/>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="VCC" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS90LV047ATMTC"/>
<attribute name="OC_FARNELL" value="9778659"/>
<attribute name="OC_NEWARK" value="41K2094"/>
<attribute name="PACKAGE" value="16-TSSOP"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS90LV048ATM" prefix="U">
<description>Line Receiver</description>
<gates>
<gate name="A" symbol="DS90LV048ATM"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-16N">
<connects>
<connect gate="A" pin="EN" pad="16"/>
<connect gate="A" pin="GND" pad="12"/>
<connect gate="A" pin="RIN1+" pad="2"/>
<connect gate="A" pin="RIN1-" pad="1"/>
<connect gate="A" pin="RIN2+" pad="3"/>
<connect gate="A" pin="RIN2-" pad="4"/>
<connect gate="A" pin="RIN3+" pad="6"/>
<connect gate="A" pin="RIN3-" pad="5"/>
<connect gate="A" pin="RIN4+" pad="7"/>
<connect gate="A" pin="RIN4-" pad="8"/>
<connect gate="A" pin="ROUT1" pad="15"/>
<connect gate="A" pin="ROUT2" pad="14"/>
<connect gate="A" pin="ROUT3" pad="11"/>
<connect gate="A" pin="ROUT4" pad="10"/>
<connect gate="A" pin="VCC" pad="13"/>
<connect gate="A" pin="~EN" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS90LV048ATM"/>
<attribute name="OC_FARNELL" value="9485856"/>
<attribute name="OC_NEWARK" value="48F5644"/>
<attribute name="PACKAGE" value="Interface"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS90LV048ATMTC" prefix="U">
<description>LVDS Quad CMOS Differential Line Receiver</description>
<gates>
<gate name="A" symbol="DS90LV048ATMTC"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-16N">
<connects>
<connect gate="A" pin="EN" pad="16"/>
<connect gate="A" pin="GND" pad="12"/>
<connect gate="A" pin="RIN1+" pad="2"/>
<connect gate="A" pin="RIN1-" pad="1"/>
<connect gate="A" pin="RIN2+" pad="3"/>
<connect gate="A" pin="RIN2-" pad="4"/>
<connect gate="A" pin="RIN3+" pad="6"/>
<connect gate="A" pin="RIN3-" pad="5"/>
<connect gate="A" pin="RIN4+" pad="7"/>
<connect gate="A" pin="RIN4-" pad="8"/>
<connect gate="A" pin="ROUT1" pad="15"/>
<connect gate="A" pin="ROUT2" pad="14"/>
<connect gate="A" pin="ROUT3" pad="11"/>
<connect gate="A" pin="ROUT4" pad="10"/>
<connect gate="A" pin="VCC" pad="13"/>
<connect gate="A" pin="~EN" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS90LV048ATMTC"/>
<attribute name="OC_FARNELL" value="9778667"/>
<attribute name="OC_NEWARK" value="74C3618"/>
<attribute name="PACKAGE" value="TSSOP-16"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS90LV049HMT" prefix="U">
<description>IC LDRVR/RCVR PAIR LVDS</description>
<gates>
<gate name="A" symbol="DS90LV049HMT"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-16N">
<connects>
<connect gate="A" pin="DIN1" pad="10"/>
<connect gate="A" pin="DIN2" pad="11"/>
<connect gate="A" pin="DOUT1+" pad="7"/>
<connect gate="A" pin="DOUT1-" pad="8"/>
<connect gate="A" pin="DOUT2+" pad="6"/>
<connect gate="A" pin="DOUT2-" pad="5"/>
<connect gate="A" pin="EN" pad="16"/>
<connect gate="A" pin="GND" pad="13"/>
<connect gate="A" pin="RIN1+" pad="2"/>
<connect gate="A" pin="RIN1-" pad="1"/>
<connect gate="A" pin="RIN2+" pad="3"/>
<connect gate="A" pin="RIN2-" pad="4"/>
<connect gate="A" pin="ROUT1" pad="15"/>
<connect gate="A" pin="ROUT2" pad="14"/>
<connect gate="A" pin="VDD" pad="12"/>
<connect gate="A" pin="~EN" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS90LV049HMT"/>
<attribute name="OC_FARNELL" value="1685759"/>
<attribute name="OC_NEWARK" value="69K2123"/>
<attribute name="PACKAGE" value="16-TSSOP"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS90LV049QMT" prefix="U">
<description>IC LDRVR/RCVR PAIR LVDS</description>
<gates>
<gate name="A" symbol="DS90LV049QMT"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-16N">
<connects>
<connect gate="A" pin="DIN1" pad="10"/>
<connect gate="A" pin="DIN2" pad="11"/>
<connect gate="A" pin="DOUT1+" pad="7"/>
<connect gate="A" pin="DOUT1-" pad="8"/>
<connect gate="A" pin="DOUT2+" pad="6"/>
<connect gate="A" pin="DOUT2-" pad="5"/>
<connect gate="A" pin="EN" pad="16"/>
<connect gate="A" pin="GND" pad="13"/>
<connect gate="A" pin="RIN1+" pad="2"/>
<connect gate="A" pin="RIN1-" pad="1"/>
<connect gate="A" pin="RIN2+" pad="3"/>
<connect gate="A" pin="RIN2-" pad="4"/>
<connect gate="A" pin="ROUT1" pad="15"/>
<connect gate="A" pin="ROUT2" pad="14"/>
<connect gate="A" pin="VDD" pad="12"/>
<connect gate="A" pin="~EN" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS90LV049QMT"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="07P4975"/>
<attribute name="PACKAGE" value="16-TSSOP"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS90LV049TMT" prefix="U">
<description>Driver with Dual Line Receiver</description>
<gates>
<gate name="A" symbol="DS90LV049TMT"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-16N">
<connects>
<connect gate="A" pin="DIN1" pad="10"/>
<connect gate="A" pin="DIN2" pad="11"/>
<connect gate="A" pin="DOUT1+" pad="7"/>
<connect gate="A" pin="DOUT1-" pad="8"/>
<connect gate="A" pin="DOUT2+" pad="6"/>
<connect gate="A" pin="DOUT2-" pad="5"/>
<connect gate="A" pin="EN" pad="16"/>
<connect gate="A" pin="GND" pad="13"/>
<connect gate="A" pin="RIN1+" pad="2"/>
<connect gate="A" pin="RIN1-" pad="1"/>
<connect gate="A" pin="RIN2+" pad="3"/>
<connect gate="A" pin="RIN2-" pad="4"/>
<connect gate="A" pin="ROUT1" pad="15"/>
<connect gate="A" pin="ROUT2" pad="14"/>
<connect gate="A" pin="VDD" pad="12"/>
<connect gate="A" pin="~EN" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS90LV049TMT"/>
<attribute name="OC_FARNELL" value="1798310"/>
<attribute name="OC_NEWARK" value="73R9504"/>
<attribute name="PACKAGE" value="16-TSSOP"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS90LV110ATMT" prefix="U">
<description>LVDS Data/Clock</description>
<gates>
<gate name="A" symbol="DS90LV110ATMT"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-28N">
<connects>
<connect gate="A" pin="EN" pad="5"/>
<connect gate="A" pin="IN+" pad="7"/>
<connect gate="A" pin="IN-" pad="8"/>
<connect gate="A" pin="OUT1+" pad="3"/>
<connect gate="A" pin="OUT1-" pad="4"/>
<connect gate="A" pin="OUT10+" pad="11"/>
<connect gate="A" pin="OUT10-" pad="12"/>
<connect gate="A" pin="OUT2+" pad="1"/>
<connect gate="A" pin="OUT2-" pad="2"/>
<connect gate="A" pin="OUT3+" pad="28"/>
<connect gate="A" pin="OUT3-" pad="27"/>
<connect gate="A" pin="OUT4+" pad="26"/>
<connect gate="A" pin="OUT4-" pad="25"/>
<connect gate="A" pin="OUT5+" pad="24"/>
<connect gate="A" pin="OUT5-" pad="23"/>
<connect gate="A" pin="OUT6+" pad="20"/>
<connect gate="A" pin="OUT6-" pad="19"/>
<connect gate="A" pin="OUT7+" pad="18"/>
<connect gate="A" pin="OUT7-" pad="17"/>
<connect gate="A" pin="OUT8+" pad="16"/>
<connect gate="A" pin="OUT8-" pad="15"/>
<connect gate="A" pin="OUT9+" pad="13"/>
<connect gate="A" pin="OUT9-" pad="14"/>
<connect gate="A" pin="VDD" pad="22"/>
<connect gate="A" pin="VDD_2" pad="10"/>
<connect gate="A" pin="VSS" pad="21"/>
<connect gate="A" pin="VSS_2" pad="9"/>
<connect gate="A" pin="VSS_3" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS90LV110ATMT"/>
<attribute name="OC_FARNELL" value="1008241"/>
<attribute name="OC_NEWARK" value="41K2102"/>
<attribute name="PACKAGE" value="SOP-28"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS90LV110TMTC" prefix="U">
<description>1 to 10 LVDS Data/Clock Distributor</description>
<gates>
<gate name="A" symbol="DS90LV110TMTC"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-28N">
<connects>
<connect gate="A" pin="EN" pad="5"/>
<connect gate="A" pin="IN+" pad="7"/>
<connect gate="A" pin="IN-" pad="8"/>
<connect gate="A" pin="OUT1+" pad="3"/>
<connect gate="A" pin="OUT1-" pad="4"/>
<connect gate="A" pin="OUT10+" pad="11"/>
<connect gate="A" pin="OUT10-" pad="12"/>
<connect gate="A" pin="OUT2+" pad="1"/>
<connect gate="A" pin="OUT2-" pad="2"/>
<connect gate="A" pin="OUT3+" pad="28"/>
<connect gate="A" pin="OUT3-" pad="27"/>
<connect gate="A" pin="OUT4+" pad="26"/>
<connect gate="A" pin="OUT4-" pad="25"/>
<connect gate="A" pin="OUT5+" pad="24"/>
<connect gate="A" pin="OUT5-" pad="23"/>
<connect gate="A" pin="OUT6+" pad="20"/>
<connect gate="A" pin="OUT6-" pad="19"/>
<connect gate="A" pin="OUT7+" pad="18"/>
<connect gate="A" pin="OUT7-" pad="17"/>
<connect gate="A" pin="OUT8+" pad="16"/>
<connect gate="A" pin="OUT8-" pad="15"/>
<connect gate="A" pin="OUT9+" pad="13"/>
<connect gate="A" pin="OUT9-" pad="14"/>
<connect gate="A" pin="VDD" pad="22"/>
<connect gate="A" pin="VDD_2" pad="10"/>
<connect gate="A" pin="VSS" pad="21"/>
<connect gate="A" pin="VSS_2" pad="9"/>
<connect gate="A" pin="VSS_3" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS90LV110TMTC"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="34C6419"/>
<attribute name="PACKAGE" value="TSSOP-28"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS90LV804TSQ" prefix="U">
<description>4-Channel 800 Mbps LVDS Buffer/Repeater</description>
<gates>
<gate name="A" symbol="DS90LV804TSQ"/>
</gates>
<devices>
<device name="" package="QFP50P500X500X80-33N">
<connects>
<connect gate="A" pin="EN" pad="8"/>
<connect gate="A" pin="EPAD" pad="33"/>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="GND_2" pad="17"/>
<connect gate="A" pin="GND_3" pad="1"/>
<connect gate="A" pin="GND_4" pad="18"/>
<connect gate="A" pin="GND_5" pad="2"/>
<connect gate="A" pin="IN0+" pad="9"/>
<connect gate="A" pin="IN0-" pad="10"/>
<connect gate="A" pin="IN1+" pad="11"/>
<connect gate="A" pin="IN1-" pad="12"/>
<connect gate="A" pin="IN2+" pad="13"/>
<connect gate="A" pin="IN2-" pad="14"/>
<connect gate="A" pin="IN3+" pad="15"/>
<connect gate="A" pin="IN3-" pad="16"/>
<connect gate="A" pin="NC" pad="24"/>
<connect gate="A" pin="NC_2" pad="23"/>
<connect gate="A" pin="OUT0+" pad="32"/>
<connect gate="A" pin="OUT0-" pad="31"/>
<connect gate="A" pin="OUT1+" pad="30"/>
<connect gate="A" pin="OUT1-" pad="29"/>
<connect gate="A" pin="OUT2+" pad="28"/>
<connect gate="A" pin="OUT2-" pad="27"/>
<connect gate="A" pin="OUT3+" pad="26"/>
<connect gate="A" pin="OUT3-" pad="25"/>
<connect gate="A" pin="VDD" pad="22"/>
<connect gate="A" pin="VDD_2" pad="3"/>
<connect gate="A" pin="VDD_3" pad="19"/>
<connect gate="A" pin="VDD_4" pad="4"/>
<connect gate="A" pin="VDD_5" pad="20"/>
<connect gate="A" pin="VDD_6" pad="6"/>
<connect gate="A" pin="VDD_7" pad="21"/>
<connect gate="A" pin="VDD_8" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS90LV804TSQ"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="69K2127"/>
<attribute name="PACKAGE" value="QFN-32"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS90UR124QVS" prefix="U">
<description>DC-Balanced 24-Bit FPD-Link II Serializer</description>
<gates>
<gate name="A" symbol="DS90UR124QVS"/>
</gates>
<devices>
<device name="" package="QFP50P1200X1200X120-64N">
<connects>
<connect gate="A" pin="BISTEN" pad="61"/>
<connect gate="A" pin="BISTM" pad="62"/>
<connect gate="A" pin="LOCK" pad="23"/>
<connect gate="A" pin="PASS" pad="45"/>
<connect gate="A" pin="PTOSEL" pad="49"/>
<connect gate="A" pin="RAOFF" pad="63"/>
<connect gate="A" pin="RCLK" pad="24"/>
<connect gate="A" pin="REN" pad="60"/>
<connect gate="A" pin="RES0" pad="50"/>
<connect gate="A" pin="RES0_10" pad="33"/>
<connect gate="A" pin="RES0_11" pad="34"/>
<connect gate="A" pin="RES0_2" pad="1"/>
<connect gate="A" pin="RES0_3" pad="2"/>
<connect gate="A" pin="RES0_4" pad="3"/>
<connect gate="A" pin="RES0_5" pad="4"/>
<connect gate="A" pin="RES0_6" pad="5"/>
<connect gate="A" pin="RES0_7" pad="6"/>
<connect gate="A" pin="RES0_8" pad="17"/>
<connect gate="A" pin="RES0_9" pad="18"/>
<connect gate="A" pin="RIN+" pad="53"/>
<connect gate="A" pin="RIN-" pad="54"/>
<connect gate="A" pin="ROUT0" pad="44"/>
<connect gate="A" pin="ROUT1" pad="43"/>
<connect gate="A" pin="ROUT10" pad="28"/>
<connect gate="A" pin="ROUT11" pad="27"/>
<connect gate="A" pin="ROUT12" pad="22"/>
<connect gate="A" pin="ROUT13" pad="21"/>
<connect gate="A" pin="ROUT14" pad="20"/>
<connect gate="A" pin="ROUT15" pad="19"/>
<connect gate="A" pin="ROUT16" pad="16"/>
<connect gate="A" pin="ROUT17" pad="15"/>
<connect gate="A" pin="ROUT18" pad="14"/>
<connect gate="A" pin="ROUT19" pad="13"/>
<connect gate="A" pin="ROUT2" pad="42"/>
<connect gate="A" pin="ROUT20" pad="10"/>
<connect gate="A" pin="ROUT21" pad="9"/>
<connect gate="A" pin="ROUT22" pad="8"/>
<connect gate="A" pin="ROUT23" pad="7"/>
<connect gate="A" pin="ROUT3" pad="41"/>
<connect gate="A" pin="ROUT4" pad="38"/>
<connect gate="A" pin="ROUT5" pad="37"/>
<connect gate="A" pin="ROUT6" pad="36"/>
<connect gate="A" pin="ROUT7" pad="35"/>
<connect gate="A" pin="ROUT8" pad="30"/>
<connect gate="A" pin="ROUT9" pad="29"/>
<connect gate="A" pin="RPWDNB" pad="48"/>
<connect gate="A" pin="RRFB" pad="55"/>
<connect gate="A" pin="SLEW" pad="64"/>
<connect gate="A" pin="VDD" pad="59"/>
<connect gate="A" pin="VDD_2" pad="46"/>
<connect gate="A" pin="VDD_3" pad="40"/>
<connect gate="A" pin="VDD_4" pad="26"/>
<connect gate="A" pin="VDD_5" pad="51"/>
<connect gate="A" pin="VDD_6" pad="11"/>
<connect gate="A" pin="VDD_7" pad="32"/>
<connect gate="A" pin="VDD_8" pad="57"/>
<connect gate="A" pin="VSS" pad="25"/>
<connect gate="A" pin="VSS_2" pad="52"/>
<connect gate="A" pin="VSS_3" pad="58"/>
<connect gate="A" pin="VSS_4" pad="12"/>
<connect gate="A" pin="VSS_5" pad="56"/>
<connect gate="A" pin="VSS_6" pad="31"/>
<connect gate="A" pin="VSS_7" pad="47"/>
<connect gate="A" pin="VSS_8" pad="39"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS90UR124QVS"/>
<attribute name="OC_FARNELL" value="1589516"/>
<attribute name="OC_NEWARK" value="11N9010"/>
<attribute name="PACKAGE" value="QFP-64"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS90UR241QVS" prefix="U">
<description>DC-Balanced 24-Bit FPD-Link II Serializer</description>
<gates>
<gate name="A" symbol="DS90UR241QVS"/>
</gates>
<devices>
<device name="" package="QFP50P900X900X120-48N">
<connects>
<connect gate="A" pin="DEN" pad="18"/>
<connect gate="A" pin="DIN0" pad="25"/>
<connect gate="A" pin="DIN1" pad="26"/>
<connect gate="A" pin="DIN10" pad="37"/>
<connect gate="A" pin="DIN11" pad="38"/>
<connect gate="A" pin="DIN12" pad="39"/>
<connect gate="A" pin="DIN13" pad="40"/>
<connect gate="A" pin="DIN14" pad="41"/>
<connect gate="A" pin="DIN15" pad="44"/>
<connect gate="A" pin="DIN16" pad="45"/>
<connect gate="A" pin="DIN17" pad="46"/>
<connect gate="A" pin="DIN18" pad="47"/>
<connect gate="A" pin="DIN19" pad="48"/>
<connect gate="A" pin="DIN2" pad="27"/>
<connect gate="A" pin="DIN20" pad="1"/>
<connect gate="A" pin="DIN21" pad="2"/>
<connect gate="A" pin="DIN22" pad="3"/>
<connect gate="A" pin="DIN23" pad="4"/>
<connect gate="A" pin="DIN3" pad="28"/>
<connect gate="A" pin="DIN4" pad="29"/>
<connect gate="A" pin="DIN5" pad="32"/>
<connect gate="A" pin="DIN6" pad="33"/>
<connect gate="A" pin="DIN7" pad="34"/>
<connect gate="A" pin="DIN8" pad="35"/>
<connect gate="A" pin="DIN9" pad="36"/>
<connect gate="A" pin="DOUT+" pad="20"/>
<connect gate="A" pin="DOUT-" pad="19"/>
<connect gate="A" pin="PRE" pad="23"/>
<connect gate="A" pin="RAOFF" pad="12"/>
<connect gate="A" pin="RES0" pad="8"/>
<connect gate="A" pin="RES0_2" pad="5"/>
<connect gate="A" pin="RES0_3" pad="13"/>
<connect gate="A" pin="TCLK" pad="10"/>
<connect gate="A" pin="TPWDNB" pad="9"/>
<connect gate="A" pin="TRFB" pad="11"/>
<connect gate="A" pin="VDD" pad="16"/>
<connect gate="A" pin="VDD_2" pad="14"/>
<connect gate="A" pin="VDD_3" pad="30"/>
<connect gate="A" pin="VDD_4" pad="7"/>
<connect gate="A" pin="VDD_5" pad="22"/>
<connect gate="A" pin="VDD_6" pad="42"/>
<connect gate="A" pin="VODSEL" pad="24"/>
<connect gate="A" pin="VSS" pad="43"/>
<connect gate="A" pin="VSS_2" pad="21"/>
<connect gate="A" pin="VSS_3" pad="15"/>
<connect gate="A" pin="VSS_4" pad="17"/>
<connect gate="A" pin="VSS_5" pad="31"/>
<connect gate="A" pin="VSS_6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS90UR241QVS"/>
<attribute name="OC_FARNELL" value="1589514"/>
<attribute name="OC_NEWARK" value="11N9012"/>
<attribute name="PACKAGE" value="QFP-48"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS91C176TMA" prefix="U">
<description>IC, M-LVDS TRANSCEIVER</description>
<gates>
<gate name="A" symbol="DS91C176TMA"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="A" pad="6"/>
<connect gate="A" pin="B" pad="7"/>
<connect gate="A" pin="D" pad="4"/>
<connect gate="A" pin="DE" pad="3"/>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="R" pad="1"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="~RE" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS91C176TMA"/>
<attribute name="OC_FARNELL" value="1685786"/>
<attribute name="OC_NEWARK" value="99K2043"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS91C180TMA" prefix="U">
<description>Driver/Receiver</description>
<gates>
<gate name="A" symbol="DS91C180TMA"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="A" pad="12"/>
<connect gate="A" pin="B" pad="11"/>
<connect gate="A" pin="D" pad="5"/>
<connect gate="A" pin="DE" pad="4"/>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="GND_2" pad="6"/>
<connect gate="A" pin="NC" pad="8"/>
<connect gate="A" pin="NC_2" pad="1"/>
<connect gate="A" pin="R" pad="2"/>
<connect gate="A" pin="VCC" pad="14"/>
<connect gate="A" pin="VCC_2" pad="13"/>
<connect gate="A" pin="Y" pad="9"/>
<connect gate="A" pin="Z" pad="10"/>
<connect gate="A" pin="~RE" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS91C180TMA"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="99K2045"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS91D176TMA" prefix="U">
<description>IC, M-LVDS TRANSCEIVER</description>
<gates>
<gate name="A" symbol="DS91D176TMA"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="A" pad="6"/>
<connect gate="A" pin="B" pad="7"/>
<connect gate="A" pin="D" pad="4"/>
<connect gate="A" pin="DE" pad="3"/>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="R" pad="1"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="~RE" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS91D176TMA"/>
<attribute name="OC_FARNELL" value="1654919"/>
<attribute name="OC_NEWARK" value="99K2048"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS91D180TMA" prefix="U">
<description>Driver/Receiver Pair</description>
<gates>
<gate name="A" symbol="DS91D180TMA"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="A" pad="12"/>
<connect gate="A" pin="B" pad="11"/>
<connect gate="A" pin="D" pad="5"/>
<connect gate="A" pin="DE" pad="4"/>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="GND_2" pad="6"/>
<connect gate="A" pin="NC" pad="8"/>
<connect gate="A" pin="NC_2" pad="1"/>
<connect gate="A" pin="R" pad="2"/>
<connect gate="A" pin="VCC" pad="14"/>
<connect gate="A" pin="VCC_2" pad="13"/>
<connect gate="A" pin="Y" pad="9"/>
<connect gate="A" pin="Z" pad="10"/>
<connect gate="A" pin="~RE" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS91D180TMA"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="99K2049"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS91M040TSQ" prefix="U">
<description>125 MHz Quad M-LVDS Transceiver</description>
<gates>
<gate name="A" symbol="DS91M040TSQ"/>
</gates>
<devices>
<device name="" package="QFP50P500X500X80-33N">
<connects>
<connect gate="A" pin="A0" pad="23"/>
<connect gate="A" pin="A1" pad="21"/>
<connect gate="A" pin="A2" pad="19"/>
<connect gate="A" pin="A3" pad="17"/>
<connect gate="A" pin="B0" pad="24"/>
<connect gate="A" pin="B1" pad="22"/>
<connect gate="A" pin="B2" pad="20"/>
<connect gate="A" pin="B3" pad="18"/>
<connect gate="A" pin="DE0" pad="25"/>
<connect gate="A" pin="DE1" pad="27"/>
<connect gate="A" pin="DE2" pad="14"/>
<connect gate="A" pin="DE3" pad="16"/>
<connect gate="A" pin="DI0" pad="2"/>
<connect gate="A" pin="DI1" pad="4"/>
<connect gate="A" pin="DI2" pad="6"/>
<connect gate="A" pin="DI3" pad="8"/>
<connect gate="A" pin="EPAD" pad="33"/>
<connect gate="A" pin="FSEN1" pad="32"/>
<connect gate="A" pin="FSEN2" pad="9"/>
<connect gate="A" pin="GND" pad="31"/>
<connect gate="A" pin="MDE" pad="10"/>
<connect gate="A" pin="RO0" pad="1"/>
<connect gate="A" pin="RO1" pad="3"/>
<connect gate="A" pin="RO2" pad="5"/>
<connect gate="A" pin="RO3" pad="7"/>
<connect gate="A" pin="VDD" pad="29"/>
<connect gate="A" pin="VDD_2" pad="12"/>
<connect gate="A" pin="VDD_3" pad="30"/>
<connect gate="A" pin="VDD_4" pad="11"/>
<connect gate="A" pin="~RE0" pad="26"/>
<connect gate="A" pin="~RE1" pad="28"/>
<connect gate="A" pin="~RE2" pad="13"/>
<connect gate="A" pin="~RE3" pad="15"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS91M040TSQ"/>
<attribute name="OC_FARNELL" value="1852992"/>
<attribute name="OC_NEWARK" value="11N9016"/>
<attribute name="PACKAGE" value="QFN-32"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS91M047TMA" prefix="U">
<description>Quad M-LVDS Line Driver</description>
<gates>
<gate name="A" symbol="DS91M047TMA"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-16N">
<connects>
<connect gate="A" pin="A0" pad="15"/>
<connect gate="A" pin="A1" pad="14"/>
<connect gate="A" pin="A2" pad="11"/>
<connect gate="A" pin="A3" pad="10"/>
<connect gate="A" pin="B0" pad="16"/>
<connect gate="A" pin="B1" pad="13"/>
<connect gate="A" pin="B2" pad="12"/>
<connect gate="A" pin="B3" pad="9"/>
<connect gate="A" pin="DE" pad="1"/>
<connect gate="A" pin="DI0" pad="2"/>
<connect gate="A" pin="DI1" pad="3"/>
<connect gate="A" pin="DI2" pad="6"/>
<connect gate="A" pin="DI3" pad="7"/>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="VDD" pad="4"/>
<connect gate="A" pin="~DE" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS91M047TMA"/>
<attribute name="OC_FARNELL" value="1689552"/>
<attribute name="OC_NEWARK" value="07P4979"/>
<attribute name="PACKAGE" value="SOIC-16"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS91M124TMA" prefix="U">
<description>M-LVDS Repeater</description>
<gates>
<gate name="A" symbol="DS91M124TMA"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-16N">
<connects>
<connect gate="A" pin="A0" pad="15"/>
<connect gate="A" pin="A1" pad="14"/>
<connect gate="A" pin="A2" pad="11"/>
<connect gate="A" pin="A3" pad="10"/>
<connect gate="A" pin="B0" pad="16"/>
<connect gate="A" pin="B1" pad="13"/>
<connect gate="A" pin="B2" pad="12"/>
<connect gate="A" pin="B3" pad="9"/>
<connect gate="A" pin="DE1" pad="2"/>
<connect gate="A" pin="DE2" pad="3"/>
<connect gate="A" pin="DE3" pad="8"/>
<connect gate="A" pin="DEO" pad="1"/>
<connect gate="A" pin="DI" pad="6"/>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="NC" pad="7"/>
<connect gate="A" pin="VDD" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS91M124TMA"/>
<attribute name="OC_FARNELL" value="1689548"/>
<attribute name="OC_NEWARK" value="40P2711"/>
<attribute name="PACKAGE" value="SOIC-16"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS91M125TMA" prefix="U">
<description>M-LVDS Repeater</description>
<gates>
<gate name="A" symbol="DS91M125TMA"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-16N">
<connects>
<connect gate="A" pin="A0" pad="15"/>
<connect gate="A" pin="A1" pad="14"/>
<connect gate="A" pin="A2" pad="11"/>
<connect gate="A" pin="A3" pad="10"/>
<connect gate="A" pin="B0" pad="16"/>
<connect gate="A" pin="B1" pad="13"/>
<connect gate="A" pin="B2" pad="12"/>
<connect gate="A" pin="B3" pad="9"/>
<connect gate="A" pin="DE1" pad="2"/>
<connect gate="A" pin="DE2" pad="3"/>
<connect gate="A" pin="DE3" pad="8"/>
<connect gate="A" pin="DEO" pad="1"/>
<connect gate="A" pin="DI+" pad="6"/>
<connect gate="A" pin="DI-" pad="7"/>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="VDD" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS91M125TMA"/>
<attribute name="OC_FARNELL" value="1689549"/>
<attribute name="OC_NEWARK" value="40P2712"/>
<attribute name="PACKAGE" value="SOIC-16"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS92001TMA" prefix="U">
<description>LVDS-BLVDS Buffer</description>
<gates>
<gate name="A" symbol="DS92001TMA"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="EN" pad="8"/>
<connect gate="A" pin="GND" pad="1"/>
<connect gate="A" pin="IN+" pad="3"/>
<connect gate="A" pin="IN_" pad="2"/>
<connect gate="A" pin="NC" pad="4"/>
<connect gate="A" pin="OUT+" pad="6"/>
<connect gate="A" pin="OUT-" pad="7"/>
<connect gate="A" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS92001TMA"/>
<attribute name="OC_FARNELL" value="1685783"/>
<attribute name="OC_NEWARK" value="41K2134"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS92CK16TMTC" prefix="U">
<description>BLVDS 1 to 6 Clock Buffer/Bus Transceiver</description>
<gates>
<gate name="A" symbol="DS92CK16TMTC"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-24N">
<connects>
<connect gate="A" pin="CLKI/O+" pad="6"/>
<connect gate="A" pin="CLKI/O-" pad="7"/>
<connect gate="A" pin="CLKOUT0" pad="23"/>
<connect gate="A" pin="CLKOUT1" pad="21"/>
<connect gate="A" pin="CLKOUT2" pad="19"/>
<connect gate="A" pin="CLKOUT3" pad="17"/>
<connect gate="A" pin="CLKOUT4" pad="15"/>
<connect gate="A" pin="CLKOUT5" pad="13"/>
<connect gate="A" pin="CRDCLKIN" pad="9"/>
<connect gate="A" pin="GND" pad="18"/>
<connect gate="A" pin="GNDA" pad="8"/>
<connect gate="A" pin="GNDA_2" pad="5"/>
<connect gate="A" pin="GND_2" pad="12"/>
<connect gate="A" pin="GND_3" pad="1"/>
<connect gate="A" pin="GND_4" pad="14"/>
<connect gate="A" pin="GND_5" pad="22"/>
<connect gate="A" pin="NC" pad="10"/>
<connect gate="A" pin="NC_2" pad="3"/>
<connect gate="A" pin="VCC" pad="20"/>
<connect gate="A" pin="VCCA" pad="4"/>
<connect gate="A" pin="VCC_2" pad="16"/>
<connect gate="A" pin="VCC_3" pad="24"/>
<connect gate="A" pin="~DE" pad="11"/>
<connect gate="A" pin="~OE" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS92CK16TMTC"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="74C3620"/>
<attribute name="PACKAGE" value="TSSOP-24"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS92LV010ATM" prefix="U">
<description>Bus LVDS 3.3/5.0V Single Transceiver</description>
<gates>
<gate name="A" symbol="DS92LV010ATM"/>
</gates>
<devices>
<device name="" package="SOIC127P620X175-8N">
<connects>
<connect gate="A" pin="DE" pad="1"/>
<connect gate="A" pin="DIN" pad="2"/>
<connect gate="A" pin="DO+/RI+" pad="7"/>
<connect gate="A" pin="DO-/RI-" pad="6"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="ROUT" pad="3"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="~RE" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS92LV010ATM"/>
<attribute name="OC_FARNELL" value="9485791"/>
<attribute name="OC_NEWARK" value="41K2108"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS92LV040ATLQA" prefix="U">
<description>LVDS Transceiver</description>
<gates>
<gate name="A" symbol="DS92LV040ATLQA"/>
</gates>
<devices>
<device name="" package="QFN50P700X700X80-45N">
<connects>
<connect gate="A" pin="AGND" pad="25"/>
<connect gate="A" pin="AGND_2" pad="9"/>
<connect gate="A" pin="AGND_3" pad="17"/>
<connect gate="A" pin="AVCC" pad="27"/>
<connect gate="A" pin="AVCC_2" pad="7"/>
<connect gate="A" pin="AVCC_3" pad="10"/>
<connect gate="A" pin="AVCC_4" pad="22"/>
<connect gate="A" pin="DE12" pad="26"/>
<connect gate="A" pin="DE34" pad="8"/>
<connect gate="A" pin="DIN1" pad="35"/>
<connect gate="A" pin="DIN2" pad="37"/>
<connect gate="A" pin="DIN3" pad="40"/>
<connect gate="A" pin="DIN4" pad="42"/>
<connect gate="A" pin="DO1+/RIN1+" pad="21"/>
<connect gate="A" pin="DO1-/RIN1-" pad="20"/>
<connect gate="A" pin="DO2+/RIN2+" pad="19"/>
<connect gate="A" pin="DO2-/RIN2-" pad="18"/>
<connect gate="A" pin="DO3+/RIN3+" pad="16"/>
<connect gate="A" pin="DO3-/RIN3-" pad="15"/>
<connect gate="A" pin="DO4+/RIN4+" pad="14"/>
<connect gate="A" pin="DO4-/RIN4-" pad="13"/>
<connect gate="A" pin="EP" pad="45"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="GND_2" pad="28"/>
<connect gate="A" pin="GND_3" pad="31"/>
<connect gate="A" pin="GND_4" pad="39"/>
<connect gate="A" pin="NC" pad="34"/>
<connect gate="A" pin="NC_10" pad="33"/>
<connect gate="A" pin="NC_2" pad="11"/>
<connect gate="A" pin="NC_3" pad="1"/>
<connect gate="A" pin="NC_4" pad="12"/>
<connect gate="A" pin="NC_5" pad="23"/>
<connect gate="A" pin="NC_6" pad="24"/>
<connect gate="A" pin="NC_7" pad="32"/>
<connect gate="A" pin="NC_8" pad="2"/>
<connect gate="A" pin="NC_9" pad="44"/>
<connect gate="A" pin="RO1" pad="36"/>
<connect gate="A" pin="RO2" pad="38"/>
<connect gate="A" pin="RO3" pad="41"/>
<connect gate="A" pin="RO4" pad="43"/>
<connect gate="A" pin="VCC" pad="30"/>
<connect gate="A" pin="VCC_2" pad="3"/>
<connect gate="A" pin="VCC_3" pad="6"/>
<connect gate="A" pin="~RE12" pad="29"/>
<connect gate="A" pin="~RE34" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS92LV040ATLQA"/>
<attribute name="OC_FARNELL" value="1495091"/>
<attribute name="OC_NEWARK" value="41K2110"/>
<attribute name="PACKAGE" value="LLP-44"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS92LV090ATVEH" prefix="U">
<description>9 Channel Bus LVDS Transceiver</description>
<gates>
<gate name="A" symbol="DS92LV090ATVEH"/>
</gates>
<devices>
<device name="" package="QFP50P1200X1200X145-64N">
<connects>
<connect gate="A" pin="AGND" pad="53"/>
<connect gate="A" pin="AGND_2" pad="33"/>
<connect gate="A" pin="AGND_3" pad="49"/>
<connect gate="A" pin="AGND_4" pad="28"/>
<connect gate="A" pin="AGND_5" pad="43"/>
<connect gate="A" pin="AVCC" pad="48"/>
<connect gate="A" pin="AVCC_2" pad="29"/>
<connect gate="A" pin="AVCC_3" pad="32"/>
<connect gate="A" pin="AVCC_4" pad="42"/>
<connect gate="A" pin="AVCC_5" pad="52"/>
<connect gate="A" pin="DE" pad="16"/>
<connect gate="A" pin="DIN0" pad="58"/>
<connect gate="A" pin="DIN1" pad="60"/>
<connect gate="A" pin="DIN2" pad="62"/>
<connect gate="A" pin="DIN3" pad="2"/>
<connect gate="A" pin="DIN4" pad="6"/>
<connect gate="A" pin="DIN5" pad="12"/>
<connect gate="A" pin="DIN6" pad="18"/>
<connect gate="A" pin="DIN7" pad="20"/>
<connect gate="A" pin="DIN8" pad="22"/>
<connect gate="A" pin="DO0+/RO0+" pad="55"/>
<connect gate="A" pin="DO0-/RO0-" pad="54"/>
<connect gate="A" pin="DO1+/RIN1+" pad="51"/>
<connect gate="A" pin="DO1-/RIN1-" pad="50"/>
<connect gate="A" pin="DO2+/RIN2+" pad="47"/>
<connect gate="A" pin="DO2-/RIN2-" pad="46"/>
<connect gate="A" pin="DO3+/RIN3+" pad="45"/>
<connect gate="A" pin="DO3-/RIN3-" pad="44"/>
<connect gate="A" pin="DO4+/RIN4+" pad="41"/>
<connect gate="A" pin="DO4-/RIN4-" pad="40"/>
<connect gate="A" pin="DO5+/RIN5+" pad="37"/>
<connect gate="A" pin="DO5-/RIN5-" pad="36"/>
<connect gate="A" pin="DO6+/RIN6+" pad="35"/>
<connect gate="A" pin="DO6-/RIN6-" pad="34"/>
<connect gate="A" pin="DO7+/RIN7+" pad="31"/>
<connect gate="A" pin="DO7-/RIN7-" pad="30"/>
<connect gate="A" pin="DO8+/RO8+" pad="27"/>
<connect gate="A" pin="DO8-/RIN8-" pad="26"/>
<connect gate="A" pin="GND" pad="25"/>
<connect gate="A" pin="GND_2" pad="4"/>
<connect gate="A" pin="GND_3" pad="14"/>
<connect gate="A" pin="GND_4" pad="9"/>
<connect gate="A" pin="GND_5" pad="56"/>
<connect gate="A" pin="GND_6" pad="5"/>
<connect gate="A" pin="NC" pad="11"/>
<connect gate="A" pin="NC_2" pad="38"/>
<connect gate="A" pin="NC_3" pad="39"/>
<connect gate="A" pin="NC_4" pad="1"/>
<connect gate="A" pin="NC_5" pad="8"/>
<connect gate="A" pin="RO0" pad="59"/>
<connect gate="A" pin="RO1" pad="61"/>
<connect gate="A" pin="RO2" pad="63"/>
<connect gate="A" pin="RO3" pad="3"/>
<connect gate="A" pin="RO4" pad="7"/>
<connect gate="A" pin="RO5" pad="13"/>
<connect gate="A" pin="RO6" pad="19"/>
<connect gate="A" pin="RO7" pad="21"/>
<connect gate="A" pin="RO8" pad="23"/>
<connect gate="A" pin="VCC" pad="24"/>
<connect gate="A" pin="VCC_2" pad="10"/>
<connect gate="A" pin="VCC_3" pad="57"/>
<connect gate="A" pin="VCC_4" pad="15"/>
<connect gate="A" pin="VCC_5" pad="64"/>
<connect gate="A" pin="~RE" pad="17"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS92LV090ATVEH"/>
<attribute name="OC_FARNELL" value="41K2112"/>
<attribute name="OC_NEWARK" value="1286835"/>
<attribute name="PACKAGE" value="QFP-64"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS92LV1021AMSA" prefix="U">
<description>10 Bit Bus LVDS Serializer</description>
<gates>
<gate name="A" symbol="DS92LV1021AMSA"/>
</gates>
<devices>
<device name="" package="SOP65P790X200-28N">
<connects>
<connect gate="A" pin="AGND" pad="20"/>
<connect gate="A" pin="AGND_2" pad="18"/>
<connect gate="A" pin="AGND_3" pad="23"/>
<connect gate="A" pin="AGND_4" pad="25"/>
<connect gate="A" pin="AVCC" pad="26"/>
<connect gate="A" pin="AVCC_2" pad="17"/>
<connect gate="A" pin="D0-" pad="21"/>
<connect gate="A" pin="DEN" pad="19"/>
<connect gate="A" pin="DGND" pad="16"/>
<connect gate="A" pin="DGND_2" pad="15"/>
<connect gate="A" pin="DIN0" pad="3"/>
<connect gate="A" pin="DIN1" pad="4"/>
<connect gate="A" pin="DIN2" pad="5"/>
<connect gate="A" pin="DIN3" pad="6"/>
<connect gate="A" pin="DIN4" pad="7"/>
<connect gate="A" pin="DIN5" pad="8"/>
<connect gate="A" pin="DIN6" pad="9"/>
<connect gate="A" pin="DIN7" pad="10"/>
<connect gate="A" pin="DIN8" pad="11"/>
<connect gate="A" pin="DIN9" pad="12"/>
<connect gate="A" pin="DO+" pad="22"/>
<connect gate="A" pin="DVCC" pad="28"/>
<connect gate="A" pin="DVCC_2" pad="27"/>
<connect gate="A" pin="SYNC1" pad="1"/>
<connect gate="A" pin="SYNC2" pad="2"/>
<connect gate="A" pin="TCLK" pad="14"/>
<connect gate="A" pin="TCLK_R~/~F" pad="13"/>
<connect gate="A" pin="~PWRDN" pad="24"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS92LV1021AMSA"/>
<attribute name="OC_FARNELL" value="8206830"/>
<attribute name="OC_NEWARK" value="41K2114"/>
<attribute name="PACKAGE" value="8206830"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS92LV1023EMQ" prefix="U">
<description>Bit Bus LVDS Serializer</description>
<gates>
<gate name="A" symbol="DS92LV1023EMQ"/>
</gates>
<devices>
<device name="" package="SOP65P790X200-28N">
<connects>
<connect gate="A" pin="AGND" pad="25"/>
<connect gate="A" pin="AGND_2" pad="18"/>
<connect gate="A" pin="AGND_3" pad="20"/>
<connect gate="A" pin="AGND_4" pad="23"/>
<connect gate="A" pin="AVCC" pad="26"/>
<connect gate="A" pin="AVCC_2" pad="17"/>
<connect gate="A" pin="D0-" pad="21"/>
<connect gate="A" pin="DEN" pad="19"/>
<connect gate="A" pin="DGND" pad="16"/>
<connect gate="A" pin="DGND_2" pad="15"/>
<connect gate="A" pin="DIN0" pad="3"/>
<connect gate="A" pin="DIN1" pad="4"/>
<connect gate="A" pin="DIN2" pad="5"/>
<connect gate="A" pin="DIN3" pad="6"/>
<connect gate="A" pin="DIN4" pad="7"/>
<connect gate="A" pin="DIN5" pad="8"/>
<connect gate="A" pin="DIN6" pad="9"/>
<connect gate="A" pin="DIN7" pad="10"/>
<connect gate="A" pin="DIN8" pad="11"/>
<connect gate="A" pin="DIN9" pad="12"/>
<connect gate="A" pin="DO+" pad="22"/>
<connect gate="A" pin="DVCC" pad="28"/>
<connect gate="A" pin="DVCC_2" pad="27"/>
<connect gate="A" pin="SYNC1" pad="1"/>
<connect gate="A" pin="SYNC2" pad="2"/>
<connect gate="A" pin="TCLK" pad="14"/>
<connect gate="A" pin="TCLK_R~/~F" pad="13"/>
<connect gate="A" pin="~PWRDN" pad="24"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS92LV1023EMQ"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="99K2052"/>
<attribute name="PACKAGE" value="SSOP-28"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS92LV1212AMSA" prefix="U">
<description>10-Bit Bus LVDS Random Lock Deserializer</description>
<gates>
<gate name="A" symbol="DS92LV1212AMSA"/>
</gates>
<devices>
<device name="" package="SOP65P790X200-28N">
<connects>
<connect gate="A" pin="AGND" pad="13"/>
<connect gate="A" pin="AGND_2" pad="12"/>
<connect gate="A" pin="AGND_3" pad="1"/>
<connect gate="A" pin="AVCC" pad="11"/>
<connect gate="A" pin="AVCC_2" pad="4"/>
<connect gate="A" pin="DGND" pad="22"/>
<connect gate="A" pin="DGND_2" pad="14"/>
<connect gate="A" pin="DGND_3" pad="20"/>
<connect gate="A" pin="DVCC" pad="21"/>
<connect gate="A" pin="DVCC_2" pad="23"/>
<connect gate="A" pin="RCLK" pad="9"/>
<connect gate="A" pin="RCLK_R~/~F" pad="2"/>
<connect gate="A" pin="REFCLK" pad="3"/>
<connect gate="A" pin="REN" pad="8"/>
<connect gate="A" pin="RI+" pad="5"/>
<connect gate="A" pin="RI-" pad="6"/>
<connect gate="A" pin="ROUT0" pad="28"/>
<connect gate="A" pin="ROUT1" pad="27"/>
<connect gate="A" pin="ROUT2" pad="26"/>
<connect gate="A" pin="ROUT3" pad="25"/>
<connect gate="A" pin="ROUT4" pad="24"/>
<connect gate="A" pin="ROUT5" pad="19"/>
<connect gate="A" pin="ROUT6" pad="18"/>
<connect gate="A" pin="ROUT7" pad="17"/>
<connect gate="A" pin="ROUT8" pad="16"/>
<connect gate="A" pin="ROUT9" pad="15"/>
<connect gate="A" pin="~LOCK" pad="10"/>
<connect gate="A" pin="~PWRDN" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS92LV1212AMSA"/>
<attribute name="OC_FARNELL" value="1850235"/>
<attribute name="OC_NEWARK" value="41K2121"/>
<attribute name="PACKAGE" value="SSOP-28"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS92LV1224TMSA" prefix="U">
<description>LVDS Deserializer</description>
<gates>
<gate name="A" symbol="DS92LV1224TMSA"/>
</gates>
<devices>
<device name="" package="SOP65P770X200-28N">
<connects>
<connect gate="A" pin="AGND" pad="13"/>
<connect gate="A" pin="AGND_2" pad="1"/>
<connect gate="A" pin="AGND_3" pad="12"/>
<connect gate="A" pin="AVCC" pad="11"/>
<connect gate="A" pin="AVCC_2" pad="4"/>
<connect gate="A" pin="DGND" pad="20"/>
<connect gate="A" pin="DGND_2" pad="14"/>
<connect gate="A" pin="DGND_3" pad="22"/>
<connect gate="A" pin="DVCC" pad="23"/>
<connect gate="A" pin="DVCC_2" pad="21"/>
<connect gate="A" pin="RCLK" pad="9"/>
<connect gate="A" pin="RCLK_R/~F" pad="2"/>
<connect gate="A" pin="REFCLK" pad="3"/>
<connect gate="A" pin="REN" pad="8"/>
<connect gate="A" pin="RI+" pad="5"/>
<connect gate="A" pin="RI-" pad="6"/>
<connect gate="A" pin="ROUT0" pad="28"/>
<connect gate="A" pin="ROUT1" pad="27"/>
<connect gate="A" pin="ROUT2" pad="26"/>
<connect gate="A" pin="ROUT3" pad="25"/>
<connect gate="A" pin="ROUT4" pad="24"/>
<connect gate="A" pin="ROUT5" pad="19"/>
<connect gate="A" pin="ROUT6" pad="18"/>
<connect gate="A" pin="ROUT7" pad="17"/>
<connect gate="A" pin="ROUT8" pad="16"/>
<connect gate="A" pin="ROUT9" pad="15"/>
<connect gate="A" pin="~LOCK" pad="10"/>
<connect gate="A" pin="~PWRDN" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS92LV1224TMSA"/>
<attribute name="OC_FARNELL" value="1798311"/>
<attribute name="OC_NEWARK" value="73R9505"/>
<attribute name="PACKAGE" value="28-SSOP"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS92LV16TVHG" prefix="U">
<description>LVDS Serializer/Deserializer</description>
<gates>
<gate name="A" symbol="DS92LV16TVHG"/>
</gates>
<devices>
<device name="" package="QFP50P1400X1400X140-80N">
<connects>
<connect gate="A" pin="AGND" pad="12"/>
<connect gate="A" pin="AGND_2" pad="16"/>
<connect gate="A" pin="AGND_3" pad="6"/>
<connect gate="A" pin="AGND_4" pad="9"/>
<connect gate="A" pin="AVDD" pad="10"/>
<connect gate="A" pin="AVDD_2" pad="5"/>
<connect gate="A" pin="AVDD_3" pad="11"/>
<connect gate="A" pin="AVDD_4" pad="15"/>
<connect gate="A" pin="CONFIG1" pad="3"/>
<connect gate="A" pin="CONFIG2" pad="18"/>
<connect gate="A" pin="DEN" pad="19"/>
<connect gate="A" pin="DGND" pad="44"/>
<connect gate="A" pin="DGND_2" pad="41"/>
<connect gate="A" pin="DGND_3" pad="51"/>
<connect gate="A" pin="DGND_4" pad="52"/>
<connect gate="A" pin="DGND_5" pad="59"/>
<connect gate="A" pin="DGND_6" pad="60"/>
<connect gate="A" pin="DGND_7" pad="61"/>
<connect gate="A" pin="DGND_8" pad="68"/>
<connect gate="A" pin="DGND_9" pad="80"/>
<connect gate="A" pin="DIN0" pad="21"/>
<connect gate="A" pin="DIN1" pad="22"/>
<connect gate="A" pin="DIN10" pad="35"/>
<connect gate="A" pin="DIN11" pad="36"/>
<connect gate="A" pin="DIN12" pad="37"/>
<connect gate="A" pin="DIN13" pad="38"/>
<connect gate="A" pin="DIN14" pad="39"/>
<connect gate="A" pin="DIN15" pad="40"/>
<connect gate="A" pin="DIN2" pad="23"/>
<connect gate="A" pin="DIN3" pad="24"/>
<connect gate="A" pin="DIN4" pad="25"/>
<connect gate="A" pin="DIN5" pad="26"/>
<connect gate="A" pin="DIN6" pad="27"/>
<connect gate="A" pin="DIN7" pad="28"/>
<connect gate="A" pin="DIN8" pad="33"/>
<connect gate="A" pin="DIN9" pad="34"/>
<connect gate="A" pin="DO+" pad="13"/>
<connect gate="A" pin="DO-" pad="14"/>
<connect gate="A" pin="DVDD" pad="62"/>
<connect gate="A" pin="DVDD_2" pad="58"/>
<connect gate="A" pin="DVDD_3" pad="50"/>
<connect gate="A" pin="DVDD_4" pad="53"/>
<connect gate="A" pin="DVDD_5" pad="69"/>
<connect gate="A" pin="DVDD_6" pad="43"/>
<connect gate="A" pin="LINE_LE" pad="78"/>
<connect gate="A" pin="LOCAL_LE" pad="79"/>
<connect gate="A" pin="PGND" pad="74"/>
<connect gate="A" pin="PGND_2" pad="29"/>
<connect gate="A" pin="PGND_3" pad="32"/>
<connect gate="A" pin="PGND_4" pad="76"/>
<connect gate="A" pin="PVDD" pad="77"/>
<connect gate="A" pin="PVDD_2" pad="30"/>
<connect gate="A" pin="PVDD_3" pad="31"/>
<connect gate="A" pin="PVDD_4" pad="75"/>
<connect gate="A" pin="RCLK" pad="49"/>
<connect gate="A" pin="REFCLK" pad="4"/>
<connect gate="A" pin="REN" pad="2"/>
<connect gate="A" pin="RIN+" pad="7"/>
<connect gate="A" pin="RIN-" pad="8"/>
<connect gate="A" pin="ROUT0" pad="45"/>
<connect gate="A" pin="ROUT1" pad="46"/>
<connect gate="A" pin="ROUT10" pad="66"/>
<connect gate="A" pin="ROUT11" pad="67"/>
<connect gate="A" pin="ROUT12" pad="70"/>
<connect gate="A" pin="ROUT13" pad="71"/>
<connect gate="A" pin="ROUT14" pad="72"/>
<connect gate="A" pin="ROUT15" pad="73"/>
<connect gate="A" pin="ROUT2" pad="47"/>
<connect gate="A" pin="ROUT3" pad="48"/>
<connect gate="A" pin="ROUT4" pad="54"/>
<connect gate="A" pin="ROUT5" pad="55"/>
<connect gate="A" pin="ROUT6" pad="56"/>
<connect gate="A" pin="ROUT7" pad="57"/>
<connect gate="A" pin="ROUT8" pad="64"/>
<connect gate="A" pin="ROUT9" pad="65"/>
<connect gate="A" pin="SYNC" pad="20"/>
<connect gate="A" pin="TCLK" pad="17"/>
<connect gate="A" pin="~LOCK" pad="63"/>
<connect gate="A" pin="~RPWDN" pad="1"/>
<connect gate="A" pin="~TPWDN" pad="42"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS92LV16TVHG"/>
<attribute name="OC_FARNELL" value="8206848"/>
<attribute name="OC_NEWARK" value="38K1020"/>
<attribute name="PACKAGE" value="QFP-80"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS92LV18TVV" prefix="U">
<description>18-Bit Bus LVDS Serializer/Deserializer</description>
<gates>
<gate name="A" symbol="DS92LV18TVV"/>
</gates>
<devices>
<device name="" package="QFP50P1400X1400X160-80N">
<connects>
<connect gate="A" pin="AGND" pad="16"/>
<connect gate="A" pin="AGND_2" pad="9"/>
<connect gate="A" pin="AGND_3" pad="6"/>
<connect gate="A" pin="AGND_4" pad="12"/>
<connect gate="A" pin="AVDD" pad="11"/>
<connect gate="A" pin="AVDD_2" pad="5"/>
<connect gate="A" pin="AVDD_3" pad="15"/>
<connect gate="A" pin="AVDD_4" pad="10"/>
<connect gate="A" pin="DEN" pad="19"/>
<connect gate="A" pin="DGND" pad="68"/>
<connect gate="A" pin="DGND_2" pad="51"/>
<connect gate="A" pin="DGND_3" pad="59"/>
<connect gate="A" pin="DGND_4" pad="44"/>
<connect gate="A" pin="DGND_5" pad="60"/>
<connect gate="A" pin="DGND_6" pad="52"/>
<connect gate="A" pin="DGND_7" pad="61"/>
<connect gate="A" pin="DGND_8" pad="41"/>
<connect gate="A" pin="DIN0" pad="21"/>
<connect gate="A" pin="DIN1" pad="22"/>
<connect gate="A" pin="DIN10" pad="35"/>
<connect gate="A" pin="DIN11" pad="36"/>
<connect gate="A" pin="DIN12" pad="37"/>
<connect gate="A" pin="DIN13" pad="38"/>
<connect gate="A" pin="DIN14" pad="39"/>
<connect gate="A" pin="DIN15" pad="40"/>
<connect gate="A" pin="DIN16" pad="18"/>
<connect gate="A" pin="DIN17" pad="3"/>
<connect gate="A" pin="DIN2" pad="23"/>
<connect gate="A" pin="DIN3" pad="24"/>
<connect gate="A" pin="DIN4" pad="25"/>
<connect gate="A" pin="DIN5" pad="26"/>
<connect gate="A" pin="DIN6" pad="27"/>
<connect gate="A" pin="DIN7" pad="28"/>
<connect gate="A" pin="DIN8" pad="33"/>
<connect gate="A" pin="DIN9" pad="34"/>
<connect gate="A" pin="DO+" pad="13"/>
<connect gate="A" pin="DO-" pad="14"/>
<connect gate="A" pin="DVDD" pad="53"/>
<connect gate="A" pin="DVDD_2" pad="43"/>
<connect gate="A" pin="DVDD_3" pad="58"/>
<connect gate="A" pin="DVDD_4" pad="50"/>
<connect gate="A" pin="DVDD_5" pad="69"/>
<connect gate="A" pin="LINE_LE" pad="78"/>
<connect gate="A" pin="LOCAL_LE" pad="79"/>
<connect gate="A" pin="PGND" pad="76"/>
<connect gate="A" pin="PGND_2" pad="74"/>
<connect gate="A" pin="PGND_3" pad="29"/>
<connect gate="A" pin="PGND_4" pad="32"/>
<connect gate="A" pin="PVDD" pad="77"/>
<connect gate="A" pin="PVDD_2" pad="30"/>
<connect gate="A" pin="PVDD_3" pad="31"/>
<connect gate="A" pin="PVDD_4" pad="75"/>
<connect gate="A" pin="RCLK" pad="49"/>
<connect gate="A" pin="REFCLKK" pad="4"/>
<connect gate="A" pin="REN" pad="2"/>
<connect gate="A" pin="RIN+" pad="7"/>
<connect gate="A" pin="RIN-" pad="8"/>
<connect gate="A" pin="ROUT0" pad="45"/>
<connect gate="A" pin="ROUT1" pad="46"/>
<connect gate="A" pin="ROUT10" pad="66"/>
<connect gate="A" pin="ROUT11" pad="67"/>
<connect gate="A" pin="ROUT12" pad="70"/>
<connect gate="A" pin="ROUT13" pad="71"/>
<connect gate="A" pin="ROUT14" pad="72"/>
<connect gate="A" pin="ROUT15" pad="73"/>
<connect gate="A" pin="ROUT16" pad="62"/>
<connect gate="A" pin="ROUT17" pad="80"/>
<connect gate="A" pin="ROUT2" pad="47"/>
<connect gate="A" pin="ROUT3" pad="48"/>
<connect gate="A" pin="ROUT4" pad="54"/>
<connect gate="A" pin="ROUT5" pad="55"/>
<connect gate="A" pin="ROUT6" pad="56"/>
<connect gate="A" pin="ROUT7" pad="57"/>
<connect gate="A" pin="ROUT8" pad="64"/>
<connect gate="A" pin="ROUT9" pad="65"/>
<connect gate="A" pin="SYNC" pad="20"/>
<connect gate="A" pin="TCLK" pad="17"/>
<connect gate="A" pin="~LOCK" pad="63"/>
<connect gate="A" pin="~RPWDN" pad="1"/>
<connect gate="A" pin="~TPWDN" pad="42"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS92LV18TVV"/>
<attribute name="OC_FARNELL" value="1693938"/>
<attribute name="OC_NEWARK" value="41K2129"/>
<attribute name="PACKAGE" value="QFP-80"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS92LV3222TVS">
<description>32-Bit Channel Link II Serializer / Deserializer</description>
<gates>
<gate name="A" symbol="DS92LV3222TVS"/>
</gates>
<devices>
<device name="" package="QFP50P1200X1200X120-64">
<connects>
<connect gate="A" pin="LOCK" pad="3"/>
<connect gate="A" pin="NC" pad="60"/>
<connect gate="A" pin="NC_2" pad="57"/>
<connect gate="A" pin="NC_3" pad="58"/>
<connect gate="A" pin="NC_4" pad="59"/>
<connect gate="A" pin="PDB" pad="49"/>
<connect gate="A" pin="REN" pad="50"/>
<connect gate="A" pin="RSVD" pad="47"/>
<connect gate="A" pin="RXCLKOUT" pad="4"/>
<connect gate="A" pin="RXIN0+" pad="51"/>
<connect gate="A" pin="RXIN0-" pad="52"/>
<connect gate="A" pin="RXIN1+" pad="53"/>
<connect gate="A" pin="RXIN1-" pad="54"/>
<connect gate="A" pin="RXOUT0" pad="46"/>
<connect gate="A" pin="RXOUT1" pad="45"/>
<connect gate="A" pin="RXOUT10" pad="34"/>
<connect gate="A" pin="RXOUT11" pad="33"/>
<connect gate="A" pin="RXOUT12" pad="32"/>
<connect gate="A" pin="RXOUT13" pad="31"/>
<connect gate="A" pin="RXOUT14" pad="30"/>
<connect gate="A" pin="RXOUT15" pad="29"/>
<connect gate="A" pin="RXOUT16" pad="28"/>
<connect gate="A" pin="RXOUT17" pad="25"/>
<connect gate="A" pin="RXOUT18" pad="24"/>
<connect gate="A" pin="RXOUT19" pad="23"/>
<connect gate="A" pin="RXOUT2" pad="44"/>
<connect gate="A" pin="RXOUT20" pad="22"/>
<connect gate="A" pin="RXOUT21" pad="21"/>
<connect gate="A" pin="RXOUT22" pad="20"/>
<connect gate="A" pin="RXOUT23" pad="19"/>
<connect gate="A" pin="RXOUT24" pad="14"/>
<connect gate="A" pin="RXOUT25" pad="13"/>
<connect gate="A" pin="RXOUT26" pad="12"/>
<connect gate="A" pin="RXOUT27" pad="11"/>
<connect gate="A" pin="RXOUT28" pad="10"/>
<connect gate="A" pin="RXOUT29" pad="7"/>
<connect gate="A" pin="RXOUT3" pad="43"/>
<connect gate="A" pin="RXOUT30" pad="6"/>
<connect gate="A" pin="RXOUT31" pad="5"/>
<connect gate="A" pin="RXOUT4" pad="42"/>
<connect gate="A" pin="RXOUT5" pad="39"/>
<connect gate="A" pin="RXOUT6" pad="38"/>
<connect gate="A" pin="RXOUT7" pad="37"/>
<connect gate="A" pin="RXOUT8" pad="36"/>
<connect gate="A" pin="RXOUT9" pad="35"/>
<connect gate="A" pin="R_FB" pad="48"/>
<connect gate="A" pin="VDD" pad="61"/>
<connect gate="A" pin="VDDA" pad="55"/>
<connect gate="A" pin="VDDPLL" pad="40"/>
<connect gate="A" pin="VDDPLL_2" pad="1"/>
<connect gate="A" pin="VDDPLL_3" pad="64"/>
<connect gate="A" pin="VDD_2" pad="9"/>
<connect gate="A" pin="VDD_3" pad="16"/>
<connect gate="A" pin="VDD_4" pad="17"/>
<connect gate="A" pin="VDD_5" pad="26"/>
<connect gate="A" pin="VSS" pad="62"/>
<connect gate="A" pin="VSSA" pad="56"/>
<connect gate="A" pin="VSSPLL" pad="63"/>
<connect gate="A" pin="VSSPLL_2" pad="2"/>
<connect gate="A" pin="VSSPLL_3" pad="41"/>
<connect gate="A" pin="VSS_2" pad="15"/>
<connect gate="A" pin="VSS_3" pad="8"/>
<connect gate="A" pin="VSS_4" pad="18"/>
<connect gate="A" pin="VSS_5" pad="27"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS92LV3222TVS"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="55R2938"/>
<attribute name="PACKAGE" value="QFP-64"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS92LV3241TVS">
<description>32-Bit Channel Link II Serializer / Deserializer</description>
<gates>
<gate name="A" symbol="DS92LV3241TVS"/>
</gates>
<devices>
<device name="" package="QFP50P1200X1200X120-64">
<connects>
<connect gate="A" pin="BISTEN" pad="13"/>
<connect gate="A" pin="IOVDD" pad="49"/>
<connect gate="A" pin="IOVSS" pad="50"/>
<connect gate="A" pin="MODE" pad="15"/>
<connect gate="A" pin="PDB" pad="12"/>
<connect gate="A" pin="PRE" pad="19"/>
<connect gate="A" pin="RSVD" pad="16"/>
<connect gate="A" pin="R_FB" pad="14"/>
<connect gate="A" pin="TXCLKIN" pad="11"/>
<connect gate="A" pin="TXIN0" pad="33"/>
<connect gate="A" pin="TXIN1" pad="34"/>
<connect gate="A" pin="TXIN10" pad="45"/>
<connect gate="A" pin="TXIN11" pad="46"/>
<connect gate="A" pin="TXIN12" pad="47"/>
<connect gate="A" pin="TXIN13" pad="48"/>
<connect gate="A" pin="TXIN14" pad="51"/>
<connect gate="A" pin="TXIN15" pad="52"/>
<connect gate="A" pin="TXIN16" pad="57"/>
<connect gate="A" pin="TXIN17" pad="58"/>
<connect gate="A" pin="TXIN18" pad="59"/>
<connect gate="A" pin="TXIN19" pad="60"/>
<connect gate="A" pin="TXIN2" pad="35"/>
<connect gate="A" pin="TXIN20" pad="61"/>
<connect gate="A" pin="TXIN21" pad="62"/>
<connect gate="A" pin="TXIN22" pad="63"/>
<connect gate="A" pin="TXIN23" pad="64"/>
<connect gate="A" pin="TXIN24" pad="1"/>
<connect gate="A" pin="TXIN25" pad="2"/>
<connect gate="A" pin="TXIN26" pad="3"/>
<connect gate="A" pin="TXIN27" pad="4"/>
<connect gate="A" pin="TXIN28" pad="5"/>
<connect gate="A" pin="TXIN29" pad="8"/>
<connect gate="A" pin="TXIN3" pad="36"/>
<connect gate="A" pin="TXIN30" pad="9"/>
<connect gate="A" pin="TXIN31" pad="10"/>
<connect gate="A" pin="TXIN4" pad="37"/>
<connect gate="A" pin="TXIN5" pad="38"/>
<connect gate="A" pin="TXIN6" pad="39"/>
<connect gate="A" pin="TXIN7" pad="40"/>
<connect gate="A" pin="TXIN8" pad="41"/>
<connect gate="A" pin="TXIN9" pad="44"/>
<connect gate="A" pin="TXOUT0+" pad="30"/>
<connect gate="A" pin="TXOUT0-" pad="29"/>
<connect gate="A" pin="TXOUT1+" pad="28"/>
<connect gate="A" pin="TXOUT1-" pad="27"/>
<connect gate="A" pin="TXOUT2+" pad="24"/>
<connect gate="A" pin="TXOUT2-" pad="23"/>
<connect gate="A" pin="TXOUT3+" pad="22"/>
<connect gate="A" pin="TXOUT3-" pad="21"/>
<connect gate="A" pin="VDD" pad="42"/>
<connect gate="A" pin="VDDA" pad="26"/>
<connect gate="A" pin="VDDPLL" pad="56"/>
<connect gate="A" pin="VDDPLL_2" pad="53"/>
<connect gate="A" pin="VDD_2" pad="7"/>
<connect gate="A" pin="VDD_3" pad="18"/>
<connect gate="A" pin="VDD_4" pad="32"/>
<connect gate="A" pin="VSEL" pad="20"/>
<connect gate="A" pin="VSS" pad="43"/>
<connect gate="A" pin="VSSA" pad="25"/>
<connect gate="A" pin="VSSPLL" pad="55"/>
<connect gate="A" pin="VSSPLL_2" pad="54"/>
<connect gate="A" pin="VSS_2" pad="17"/>
<connect gate="A" pin="VSS_3" pad="6"/>
<connect gate="A" pin="VSS_4" pad="31"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS92LV3241TVS"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="55R2940"/>
<attribute name="PACKAGE" value="QFP-64"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS92LV3242TVS">
<description>32-Bit Channel Link II Serializer / Deserializer</description>
<gates>
<gate name="A" symbol="DS92LV3242TVS"/>
</gates>
<devices>
<device name="" package="QFP50P1200X1200X120-64">
<connects>
<connect gate="A" pin="LOCK" pad="3"/>
<connect gate="A" pin="PDB" pad="49"/>
<connect gate="A" pin="REN" pad="50"/>
<connect gate="A" pin="RSVD" pad="47"/>
<connect gate="A" pin="RXCLKOUT" pad="4"/>
<connect gate="A" pin="RXIN0+" pad="51"/>
<connect gate="A" pin="RXIN0-" pad="52"/>
<connect gate="A" pin="RXIN1+" pad="53"/>
<connect gate="A" pin="RXIN1-" pad="54"/>
<connect gate="A" pin="RXIN2+" pad="57"/>
<connect gate="A" pin="RXIN2-" pad="58"/>
<connect gate="A" pin="RXIN3+" pad="59"/>
<connect gate="A" pin="RXIN3-" pad="60"/>
<connect gate="A" pin="RXOUT0" pad="46"/>
<connect gate="A" pin="RXOUT1" pad="45"/>
<connect gate="A" pin="RXOUT10" pad="34"/>
<connect gate="A" pin="RXOUT11" pad="33"/>
<connect gate="A" pin="RXOUT12" pad="32"/>
<connect gate="A" pin="RXOUT13" pad="31"/>
<connect gate="A" pin="RXOUT14" pad="30"/>
<connect gate="A" pin="RXOUT15" pad="29"/>
<connect gate="A" pin="RXOUT16" pad="28"/>
<connect gate="A" pin="RXOUT17" pad="25"/>
<connect gate="A" pin="RXOUT18" pad="24"/>
<connect gate="A" pin="RXOUT19" pad="23"/>
<connect gate="A" pin="RXOUT2" pad="44"/>
<connect gate="A" pin="RXOUT20" pad="22"/>
<connect gate="A" pin="RXOUT21" pad="21"/>
<connect gate="A" pin="RXOUT22" pad="20"/>
<connect gate="A" pin="RXOUT23" pad="19"/>
<connect gate="A" pin="RXOUT24" pad="14"/>
<connect gate="A" pin="RXOUT25" pad="13"/>
<connect gate="A" pin="RXOUT26" pad="12"/>
<connect gate="A" pin="RXOUT27" pad="11"/>
<connect gate="A" pin="RXOUT28" pad="10"/>
<connect gate="A" pin="RXOUT29" pad="7"/>
<connect gate="A" pin="RXOUT3" pad="43"/>
<connect gate="A" pin="RXOUT30" pad="6"/>
<connect gate="A" pin="RXOUT31" pad="5"/>
<connect gate="A" pin="RXOUT4" pad="42"/>
<connect gate="A" pin="RXOUT5" pad="39"/>
<connect gate="A" pin="RXOUT6" pad="38"/>
<connect gate="A" pin="RXOUT7" pad="37"/>
<connect gate="A" pin="RXOUT8" pad="36"/>
<connect gate="A" pin="RXOUT9" pad="35"/>
<connect gate="A" pin="R_FB" pad="48"/>
<connect gate="A" pin="VDD" pad="61"/>
<connect gate="A" pin="VDDA" pad="55"/>
<connect gate="A" pin="VDDPLL" pad="64"/>
<connect gate="A" pin="VDDPLL_2" pad="1"/>
<connect gate="A" pin="VDDPLL_3" pad="40"/>
<connect gate="A" pin="VDD_2" pad="9"/>
<connect gate="A" pin="VDD_3" pad="16"/>
<connect gate="A" pin="VDD_4" pad="17"/>
<connect gate="A" pin="VDD_5" pad="26"/>
<connect gate="A" pin="VSS" pad="62"/>
<connect gate="A" pin="VSSA" pad="56"/>
<connect gate="A" pin="VSSPLL" pad="63"/>
<connect gate="A" pin="VSSPLL_2" pad="2"/>
<connect gate="A" pin="VSSPLL_3" pad="41"/>
<connect gate="A" pin="VSS_2" pad="8"/>
<connect gate="A" pin="VSS_3" pad="15"/>
<connect gate="A" pin="VSS_4" pad="18"/>
<connect gate="A" pin="VSS_5" pad="27"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS92LV3241TVS"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="55R2942"/>
<attribute name="PACKAGE" value="QFP-64"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS92LV8028TUF" prefix="U">
<description>8 Channel 10:1 Serializer</description>
<gates>
<gate name="A" symbol="DS92LV8028TUF_A"/>
<gate name="B" symbol="DS92LV8028TUF_B"/>
</gates>
<devices>
<device name="" package="BGA196C14X14X100C_1500X1500X14">
<connects>
<connect gate="A" pin="AGND" pad="E7"/>
<connect gate="A" pin="AGND_2" pad="D6"/>
<connect gate="A" pin="AGND_3" pad="C7"/>
<connect gate="A" pin="AGND_4" pad="G7"/>
<connect gate="A" pin="AGND_5" pad="D7"/>
<connect gate="A" pin="AGND_6" pad="C9"/>
<connect gate="A" pin="AGND_7" pad="D9"/>
<connect gate="A" pin="AGND_8" pad="E5"/>
<connect gate="A" pin="AGND_9" pad="C10"/>
<connect gate="A" pin="AVDD" pad="C8"/>
<connect gate="A" pin="AVDD_2" pad="C11"/>
<connect gate="A" pin="AVDD_3" pad="C6"/>
<connect gate="A" pin="AVDD_4" pad="D8"/>
<connect gate="A" pin="AVDD_5" pad="F7"/>
<connect gate="A" pin="AVDD_6" pad="E6"/>
<connect gate="A" pin="AVDD_7" pad="D10"/>
<connect gate="A" pin="AVDD_8" pad="E8"/>
<connect gate="A" pin="AVDD_9" pad="D5"/>
<connect gate="A" pin="BIST_ACT" pad="B12"/>
<connect gate="A" pin="BIST_SEL" pad="B13"/>
<connect gate="A" pin="BIST_SEL_2" pad="D11"/>
<connect gate="A" pin="BIST_SEL_3" pad="A13"/>
<connect gate="A" pin="BIST_SEL_4" pad="E11"/>
<connect gate="A" pin="DGND" pad="E10"/>
<connect gate="A" pin="DGND_10" pad="C4"/>
<connect gate="A" pin="DGND_11" pad="E9"/>
<connect gate="A" pin="DGND_12" pad="E14"/>
<connect gate="A" pin="DGND_13" pad="E12"/>
<connect gate="A" pin="DGND_14" pad="F6"/>
<connect gate="A" pin="DGND_15" pad="E2"/>
<connect gate="A" pin="DGND_16" pad="E13"/>
<connect gate="A" pin="DGND_17" pad="F10"/>
<connect gate="A" pin="DGND_2" pad="A2"/>
<connect gate="A" pin="DGND_3" pad="A12"/>
<connect gate="A" pin="DGND_4" pad="B2"/>
<connect gate="A" pin="DGND_5" pad="A3"/>
<connect gate="A" pin="DGND_6" pad="B3"/>
<connect gate="A" pin="DGND_7" pad="C2"/>
<connect gate="A" pin="DGND_8" pad="D12"/>
<connect gate="A" pin="DGND_9" pad="E1"/>
<connect gate="A" pin="DIN0&lt;0&gt;" pad="F11"/>
<connect gate="A" pin="DIN0&lt;1&gt;" pad="G14"/>
<connect gate="A" pin="DIN0&lt;2&gt;" pad="F12"/>
<connect gate="A" pin="DIN0&lt;3&gt;" pad="G12"/>
<connect gate="A" pin="DIN0&lt;4&gt;" pad="G11"/>
<connect gate="A" pin="DIN6&lt;7&gt;" pad="G4"/>
<connect gate="A" pin="DIN7&lt;1&gt;" pad="F4"/>
<connect gate="A" pin="DIN7&lt;2&gt;" pad="G1"/>
<connect gate="A" pin="DIN7&lt;3&gt;" pad="G3"/>
<connect gate="A" pin="DIN7&lt;4&gt;" pad="E4"/>
<connect gate="A" pin="DIN7&lt;5&gt;" pad="G2"/>
<connect gate="A" pin="DIN7&lt;6&gt;" pad="E3"/>
<connect gate="A" pin="DIN7&lt;7&gt;" pad="F1"/>
<connect gate="A" pin="DIN7&lt;8&gt;" pad="F3"/>
<connect gate="A" pin="DIN7&lt;9&gt;" pad="F2"/>
<connect gate="A" pin="DOUT0+" pad="B11"/>
<connect gate="A" pin="DOUT0-" pad="A11"/>
<connect gate="A" pin="DOUT1+" pad="B10"/>
<connect gate="A" pin="DOUT1-" pad="A10"/>
<connect gate="A" pin="DOUT2+" pad="B9"/>
<connect gate="A" pin="DOUT2-" pad="A9"/>
<connect gate="A" pin="DOUT3+" pad="B8"/>
<connect gate="A" pin="DOUT3-" pad="A8"/>
<connect gate="A" pin="DOUT4+" pad="B7"/>
<connect gate="A" pin="DOUT4-" pad="A7"/>
<connect gate="A" pin="DOUT5+" pad="A6"/>
<connect gate="A" pin="DOUT5-" pad="B6"/>
<connect gate="A" pin="DOUT6+" pad="A5"/>
<connect gate="A" pin="DOUT6-" pad="B5"/>
<connect gate="A" pin="DOUT7+" pad="A4"/>
<connect gate="A" pin="DOUT7-" pad="B4"/>
<connect gate="A" pin="DVDD" pad="F5"/>
<connect gate="A" pin="DVDD_10" pad="G13"/>
<connect gate="A" pin="DVDD_11" pad="D14"/>
<connect gate="A" pin="DVDD_12" pad="G10"/>
<connect gate="A" pin="DVDD_13" pad="G6"/>
<connect gate="A" pin="DVDD_14" pad="C5"/>
<connect gate="A" pin="DVDD_2" pad="C3"/>
<connect gate="A" pin="DVDD_3" pad="B1"/>
<connect gate="A" pin="DVDD_4" pad="D4"/>
<connect gate="A" pin="DVDD_5" pad="F8"/>
<connect gate="A" pin="DVDD_6" pad="F13"/>
<connect gate="A" pin="DVDD_7" pad="D13"/>
<connect gate="A" pin="DVDD_8" pad="F9"/>
<connect gate="A" pin="DVDD_9" pad="A1"/>
<connect gate="A" pin="NC1" pad="G5"/>
<connect gate="A" pin="NC11" pad="G8"/>
<connect gate="A" pin="NC12" pad="G9"/>
<connect gate="A" pin="PGND" pad="D1"/>
<connect gate="A" pin="PGND_2" pad="C1"/>
<connect gate="A" pin="PVDD" pad="D3"/>
<connect gate="A" pin="PVDD_2" pad="D2"/>
<connect gate="A" pin="TCK" pad="C13"/>
<connect gate="A" pin="TCLK" pad="F14"/>
<connect gate="A" pin="TDI" pad="B14"/>
<connect gate="A" pin="TDO" pad="C14"/>
<connect gate="A" pin="TMS" pad="A14"/>
<connect gate="A" pin="TRSTN" pad="C12"/>
<connect gate="B" pin="DEN" pad="M14"/>
<connect gate="B" pin="DGND" pad="P1"/>
<connect gate="B" pin="DGND_2" pad="K6"/>
<connect gate="B" pin="DGND_3" pad="K10"/>
<connect gate="B" pin="DGND_4" pad="M13"/>
<connect gate="B" pin="DGND_5" pad="H10"/>
<connect gate="B" pin="DIN0&lt;5&gt;" pad="H11"/>
<connect gate="B" pin="DIN0&lt;6&gt;" pad="H14"/>
<connect gate="B" pin="DIN0&lt;7&gt;" pad="H12"/>
<connect gate="B" pin="DIN0&lt;8&gt;" pad="J12"/>
<connect gate="B" pin="DIN0&lt;9&gt;" pad="H13"/>
<connect gate="B" pin="DIN1&lt;0&gt;" pad="J14"/>
<connect gate="B" pin="DIN1&lt;1&gt;" pad="J11"/>
<connect gate="B" pin="DIN1&lt;2&gt;" pad="J13"/>
<connect gate="B" pin="DIN1&lt;3&gt;" pad="K12"/>
<connect gate="B" pin="DIN1&lt;4&gt;" pad="K14"/>
<connect gate="B" pin="DIN1&lt;5&gt;" pad="K13"/>
<connect gate="B" pin="DIN1&lt;6&gt;" pad="L12"/>
<connect gate="B" pin="DIN1&lt;7&gt;" pad="L14"/>
<connect gate="B" pin="DIN1&lt;8&gt;" pad="K11"/>
<connect gate="B" pin="DIN1&lt;9&gt;" pad="L13"/>
<connect gate="B" pin="DIN2&lt;0&gt;" pad="P12"/>
<connect gate="B" pin="DIN2&lt;1&gt;" pad="N11"/>
<connect gate="B" pin="DIN2&lt;2&gt;" pad="P11"/>
<connect gate="B" pin="DIN2&lt;3&gt;" pad="N10"/>
<connect gate="B" pin="DIN2&lt;4&gt;" pad="P10"/>
<connect gate="B" pin="DIN2&lt;5&gt;" pad="M11"/>
<connect gate="B" pin="DIN2&lt;6&gt;" pad="N9"/>
<connect gate="B" pin="DIN2&lt;7&gt;" pad="M10"/>
<connect gate="B" pin="DIN2&lt;8&gt;" pad="P9"/>
<connect gate="B" pin="DIN2&lt;9&gt;" pad="L11"/>
<connect gate="B" pin="DIN3&lt;0&gt;" pad="N8"/>
<connect gate="B" pin="DIN3&lt;1&gt;" pad="L10"/>
<connect gate="B" pin="DIN3&lt;2&gt;" pad="M9"/>
<connect gate="B" pin="DIN3&lt;3&gt;" pad="P8"/>
<connect gate="B" pin="DIN3&lt;4&gt;" pad="L9"/>
<connect gate="B" pin="DIN3&lt;5&gt;" pad="M8"/>
<connect gate="B" pin="DIN3&lt;6&gt;" pad="M7"/>
<connect gate="B" pin="DIN3&lt;7&gt;" pad="L8"/>
<connect gate="B" pin="DIN3&lt;8&gt;" pad="P7"/>
<connect gate="B" pin="DIN3&lt;9&gt;" pad="L7"/>
<connect gate="B" pin="DIN4&lt;0&gt;" pad="L6"/>
<connect gate="B" pin="DIN4&lt;1&gt;" pad="N7"/>
<connect gate="B" pin="DIN4&lt;2&gt;" pad="M6"/>
<connect gate="B" pin="DIN4&lt;3&gt;" pad="P6"/>
<connect gate="B" pin="DIN4&lt;4&gt;" pad="L5"/>
<connect gate="B" pin="DIN4&lt;5&gt;" pad="M5"/>
<connect gate="B" pin="DIN4&lt;6&gt;" pad="N6"/>
<connect gate="B" pin="DIN4&lt;7&gt;" pad="K4"/>
<connect gate="B" pin="DIN4&lt;8&gt;" pad="P5"/>
<connect gate="B" pin="DIN4&lt;9&gt;" pad="L4"/>
<connect gate="B" pin="DIN5&lt;0&gt;" pad="N5"/>
<connect gate="B" pin="DIN5&lt;1&gt;" pad="M4"/>
<connect gate="B" pin="DIN5&lt;2&gt;" pad="P4"/>
<connect gate="B" pin="DIN5&lt;3&gt;" pad="K3"/>
<connect gate="B" pin="DIN5&lt;4&gt;" pad="N4"/>
<connect gate="B" pin="DIN5&lt;5&gt;" pad="L3"/>
<connect gate="B" pin="DIN5&lt;6&gt;" pad="P3"/>
<connect gate="B" pin="DIN5&lt;7&gt;" pad="M3"/>
<connect gate="B" pin="DIN5&lt;8&gt;" pad="N3"/>
<connect gate="B" pin="DIN5&lt;9&gt;" pad="P2"/>
<connect gate="B" pin="DIN6&lt;0&gt;" pad="K2"/>
<connect gate="B" pin="DIN6&lt;1&gt;" pad="K1"/>
<connect gate="B" pin="DIN6&lt;2&gt;" pad="J4"/>
<connect gate="B" pin="DIN6&lt;3&gt;" pad="J2"/>
<connect gate="B" pin="DIN6&lt;4&gt;" pad="J3"/>
<connect gate="B" pin="DIN6&lt;5&gt;" pad="J1"/>
<connect gate="B" pin="DIN6&lt;6&gt;" pad="H4"/>
<connect gate="B" pin="DIN6&lt;8&gt;" pad="H2"/>
<connect gate="B" pin="DIN6&lt;9&gt;" pad="H1"/>
<connect gate="B" pin="DIN7&lt;0&gt;" pad="H3"/>
<connect gate="B" pin="DVDD" pad="H7"/>
<connect gate="B" pin="NC10" pad="H9"/>
<connect gate="B" pin="NC2" pad="H6"/>
<connect gate="B" pin="NC3" pad="H5"/>
<connect gate="B" pin="NC4" pad="J5"/>
<connect gate="B" pin="NC5" pad="J6"/>
<connect gate="B" pin="NC6" pad="J7"/>
<connect gate="B" pin="NC7" pad="H8"/>
<connect gate="B" pin="NC8" pad="J9"/>
<connect gate="B" pin="NC9" pad="J10"/>
<connect gate="B" pin="SYNC&lt;0&gt;" pad="J8"/>
<connect gate="B" pin="SYNC&lt;1&gt;" pad="N12"/>
<connect gate="B" pin="SYNC&lt;2&gt;" pad="K8"/>
<connect gate="B" pin="SYNC&lt;3&gt;" pad="K9"/>
<connect gate="B" pin="SYNC&lt;4&gt;" pad="K5"/>
<connect gate="B" pin="SYNC&lt;5&gt;" pad="L2"/>
<connect gate="B" pin="SYNC&lt;6&gt;" pad="K7"/>
<connect gate="B" pin="SYNC&lt;7&gt;" pad="L1"/>
<connect gate="B" pin="~MS_PWDN" pad="N14"/>
<connect gate="B" pin="~PWDN&lt;0&gt;" pad="N13"/>
<connect gate="B" pin="~PWDN&lt;1&gt;" pad="M12"/>
<connect gate="B" pin="~PWDN&lt;2&gt;" pad="P14"/>
<connect gate="B" pin="~PWDN&lt;3&gt;" pad="P13"/>
<connect gate="B" pin="~PWDN&lt;4&gt;" pad="N2"/>
<connect gate="B" pin="~PWDN&lt;5&gt;" pad="N1"/>
<connect gate="B" pin="~PWDN&lt;6&gt;" pad="M2"/>
<connect gate="B" pin="~PWDN&lt;7&gt;" pad="M1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS92LV8028TUF"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="65K5422"/>
<attribute name="PACKAGE" value="BGA-196"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS96174CN" prefix="U">
<description>Differential Line Driver</description>
<gates>
<gate name="A" symbol="DS96174CN"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-16">
<connects>
<connect gate="A" pin="1A" pad="1"/>
<connect gate="A" pin="1Y" pad="2"/>
<connect gate="A" pin="1Z" pad="3"/>
<connect gate="A" pin="2A" pad="7"/>
<connect gate="A" pin="2Y" pad="6"/>
<connect gate="A" pin="2Z" pad="5"/>
<connect gate="A" pin="3A" pad="9"/>
<connect gate="A" pin="3Y" pad="10"/>
<connect gate="A" pin="3Z" pad="11"/>
<connect gate="A" pin="4A" pad="15"/>
<connect gate="A" pin="4Y" pad="14"/>
<connect gate="A" pin="4Z" pad="13"/>
<connect gate="A" pin="E1,2" pad="4"/>
<connect gate="A" pin="E3,4" pad="12"/>
<connect gate="A" pin="GND" pad="8"/>
<connect gate="A" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS96174CN"/>
<attribute name="OC_FARNELL" value="9493905"/>
<attribute name="OC_NEWARK" value="07B5487"/>
<attribute name="PACKAGE" value="16-DIP"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS96175CN" prefix="U">
<description>Line Receiver</description>
<gates>
<gate name="A" symbol="DS96175CN"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-16">
<connects>
<connect gate="A" pin="1A" pad="2"/>
<connect gate="A" pin="1B" pad="1"/>
<connect gate="A" pin="1Y" pad="3"/>
<connect gate="A" pin="2A" pad="6"/>
<connect gate="A" pin="2B" pad="7"/>
<connect gate="A" pin="2Y" pad="5"/>
<connect gate="A" pin="3A" pad="10"/>
<connect gate="A" pin="3B" pad="9"/>
<connect gate="A" pin="3Y" pad="11"/>
<connect gate="A" pin="4A" pad="14"/>
<connect gate="A" pin="4B" pad="15"/>
<connect gate="A" pin="4Y" pad="13"/>
<connect gate="A" pin="E1,2" pad="4"/>
<connect gate="A" pin="E3,4" pad="12"/>
<connect gate="A" pin="GND" pad="8"/>
<connect gate="A" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS96175CN"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K2138"/>
<attribute name="PACKAGE" value="DIP-16"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS96176CN" prefix="U">
<description>Transceivers</description>
<gates>
<gate name="A" symbol="DS96176CN"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-8">
<connects>
<connect gate="A" pin="A" pad="6"/>
<connect gate="A" pin="B" pad="7"/>
<connect gate="A" pin="DE" pad="3"/>
<connect gate="A" pin="DI" pad="4"/>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="RO" pad="1"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="~RE" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS96176CN"/>
<attribute name="OC_FARNELL" value="1685483"/>
<attribute name="OC_NEWARK" value="41K2139"/>
<attribute name="PACKAGE" value="DIP-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS9637ACM" prefix="U">
<description>Dual Differential Line Receiver</description>
<gates>
<gate name="A" symbol="DS9637ACM"/>
</gates>
<devices>
<device name="" package="SOIC127P62X175-8N">
<connects>
<connect gate="A" pin="+INA" pad="8"/>
<connect gate="A" pin="+INB" pad="6"/>
<connect gate="A" pin="-INA" pad="7"/>
<connect gate="A" pin="-INB" pad="5"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="OUTA" pad="2"/>
<connect gate="A" pin="OUTB" pad="3"/>
<connect gate="A" pin="VCC" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS9637ACM"/>
<attribute name="OC_FARNELL" value="41K2140"/>
<attribute name="OC_NEWARK" value="-"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS9638CM" prefix="U">
<description>RS-422 Dual High Speed Differential Line Driver</description>
<gates>
<gate name="A" symbol="DS9638CM"/>
</gates>
<devices>
<device name="" package="SOIC127P62X175-8N">
<connects>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="INA" pad="2"/>
<connect gate="A" pin="INB" pad="3"/>
<connect gate="A" pin="OUTA" pad="8"/>
<connect gate="A" pin="OUTB" pad="6"/>
<connect gate="A" pin="OUT~A" pad="7"/>
<connect gate="A" pin="OUT~B" pad="5"/>
<connect gate="A" pin="VCC" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS9638CM"/>
<attribute name="OC_FARNELL" value="41K2142"/>
<attribute name="OC_NEWARK" value="-"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS99R421QSQ" prefix="U">
<description>LVDS Converter</description>
<gates>
<gate name="A" symbol="DS99R421QSQ"/>
</gates>
<devices>
<device name="" package="QFN50P600X600X80-33N">
<connects>
<connect gate="A" pin="BISTEN" pad="27"/>
<connect gate="A" pin="DEN" pad="15"/>
<connect gate="A" pin="DOUT+" pad="14"/>
<connect gate="A" pin="DOUT-" pad="13"/>
<connect gate="A" pin="OS0" pad="1"/>
<connect gate="A" pin="OS1" pad="2"/>
<connect gate="A" pin="OS2" pad="3"/>
<connect gate="A" pin="PRE" pad="10"/>
<connect gate="A" pin="PWDNB" pad="4"/>
<connect gate="A" pin="RESRVD" pad="21"/>
<connect gate="A" pin="RESRVD_2" pad="9"/>
<connect gate="A" pin="RESRVD_3" pad="36"/>
<connect gate="A" pin="RESRVD_4" pad="24"/>
<connect gate="A" pin="RXCLKIN+" pad="35"/>
<connect gate="A" pin="RXCLKIN-" pad="34"/>
<connect gate="A" pin="RXIN0+" pad="29"/>
<connect gate="A" pin="RXIN0-" pad="28"/>
<connect gate="A" pin="RXIN1+" pad="31"/>
<connect gate="A" pin="RXIN1-" pad="30"/>
<connect gate="A" pin="RXIN2+" pad="33"/>
<connect gate="A" pin="RXIN2-" pad="32"/>
<connect gate="A" pin="VDDD" pad="19"/>
<connect gate="A" pin="VDDDES" pad="22"/>
<connect gate="A" pin="VDDDR" pad="11"/>
<connect gate="A" pin="VDDIN" pad="25"/>
<connect gate="A" pin="VDDP0" pad="7"/>
<connect gate="A" pin="VDDP1" pad="5"/>
<connect gate="A" pin="VDDSER" pad="17"/>
<connect gate="A" pin="VODSEL" pad="18"/>
<connect gate="A" pin="VSSD" pad="20"/>
<connect gate="A" pin="VSSDES" pad="23"/>
<connect gate="A" pin="VSSDR" pad="12"/>
<connect gate="A" pin="VSSIN" pad="26"/>
<connect gate="A" pin="VSSP0" pad="8"/>
<connect gate="A" pin="VSSP1" pad="6"/>
<connect gate="A" pin="VSSSER" pad="16"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="DS99R421QSQ"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="08N3578"/>
<attribute name="PACKAGE" value="QFN-32"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LF147J" prefix="U">
<description>Operational Amplifiers</description>
<gates>
<gate name="A" symbol="LF147J"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-14">
<connects>
<connect gate="A" pin="+IN1" pad="3"/>
<connect gate="A" pin="+IN2" pad="5"/>
<connect gate="A" pin="+IN3" pad="10"/>
<connect gate="A" pin="+IN4" pad="12"/>
<connect gate="A" pin="-IN1-" pad="2"/>
<connect gate="A" pin="-IN2" pad="6"/>
<connect gate="A" pin="-IN3" pad="9"/>
<connect gate="A" pin="-IN4" pad="13"/>
<connect gate="A" pin="OUT1" pad="1"/>
<connect gate="A" pin="OUT2" pad="7"/>
<connect gate="A" pin="OUT3" pad="8"/>
<connect gate="A" pin="OUT4" pad="14"/>
<connect gate="A" pin="V+" pad="4"/>
<connect gate="A" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LF147J"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="13B5239"/>
<attribute name="PACKAGE" value="DIP-14"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LF156H" prefix="U">
<description>IC OP AMP MONO JFET IN</description>
<gates>
<gate name="A" symbol="LF156H"/>
</gates>
<devices>
<device name="" package="TO254P914X530-8P">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="BALANCE" pad="5"/>
<connect gate="A" pin="BALANCE_2" pad="1"/>
<connect gate="A" pin="NC" pad="8"/>
<connect gate="A" pin="OUTPUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LF156H"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="31T9670"/>
<attribute name="PACKAGE" value="TO99-8"/>
<attribute name="SUPPLIER" value="National Semicondutors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LF347BN" prefix="U">
<description>Operational Amplifiers</description>
<gates>
<gate name="A" symbol="LF347BN"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-14">
<connects>
<connect gate="A" pin="+IN1" pad="3"/>
<connect gate="A" pin="+IN2" pad="5"/>
<connect gate="A" pin="+IN3" pad="10"/>
<connect gate="A" pin="+IN4" pad="12"/>
<connect gate="A" pin="-IN1" pad="2"/>
<connect gate="A" pin="-IN2" pad="6"/>
<connect gate="A" pin="-IN3" pad="9"/>
<connect gate="A" pin="-IN4" pad="13"/>
<connect gate="A" pin="OUT1" pad="1"/>
<connect gate="A" pin="OUT2" pad="7"/>
<connect gate="A" pin="OUT3" pad="8"/>
<connect gate="A" pin="OUT4" pad="14"/>
<connect gate="A" pin="V+" pad="4"/>
<connect gate="A" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LF347BN"/>
<attribute name="OC_FARNELL" value="9487069"/>
<attribute name="OC_NEWARK" value="07B5533"/>
<attribute name="PACKAGE" value="DIP-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LF347M" prefix="U">
<description>Operational Amplifiers</description>
<gates>
<gate name="A" symbol="LF347M"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="+IN1" pad="3"/>
<connect gate="A" pin="+IN2" pad="5"/>
<connect gate="A" pin="+IN3" pad="10"/>
<connect gate="A" pin="+IN4" pad="12"/>
<connect gate="A" pin="-IN1" pad="2"/>
<connect gate="A" pin="-IN2" pad="6"/>
<connect gate="A" pin="-IN3" pad="9"/>
<connect gate="A" pin="-IN4" pad="13"/>
<connect gate="A" pin="OUT1" pad="1"/>
<connect gate="A" pin="OUT2" pad="7"/>
<connect gate="A" pin="OUT3" pad="8"/>
<connect gate="A" pin="OUT4" pad="14"/>
<connect gate="A" pin="V+" pad="4"/>
<connect gate="A" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LF347M"/>
<attribute name="OC_FARNELL" value="1468875"/>
<attribute name="OC_NEWARK" value="07B5534"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LF347N" prefix="U">
<description>OpAmpIC</description>
<gates>
<gate name="A" symbol="LF347N"/>
</gates>
<devices>
<device name="" package="DIP254P760X508-14">
<connects>
<connect gate="A" pin="IN1+" pad="3"/>
<connect gate="A" pin="IN1-" pad="2"/>
<connect gate="A" pin="IN2+" pad="5"/>
<connect gate="A" pin="IN2-" pad="6"/>
<connect gate="A" pin="IN3+" pad="10"/>
<connect gate="A" pin="IN3-" pad="9"/>
<connect gate="A" pin="IN4+" pad="12"/>
<connect gate="A" pin="IN4-" pad="13"/>
<connect gate="A" pin="OUT1" pad="1"/>
<connect gate="A" pin="OUT2" pad="7"/>
<connect gate="A" pin="OUT3" pad="8"/>
<connect gate="A" pin="OUT4" pad="14"/>
<connect gate="A" pin="V+" pad="4"/>
<connect gate="A" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LF347N"/>
<attribute name="OC_FARNELL" value="9487077"/>
<attribute name="OC_NEWARK" value="41K2541"/>
<attribute name="PACKAGE" value="DIP-14"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LF353M" prefix="U">
<description>OpAmpIC</description>
<gates>
<gate name="A" symbol="LF353M"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="NEGA" pad="2"/>
<connect gate="A" pin="NEGB" pad="6"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="POSA" pad="3"/>
<connect gate="A" pin="POSB" pad="5"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LF353M"/>
<attribute name="OC_FARNELL" value="1149977"/>
<attribute name="OC_NEWARK" value="07B5537"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LF353N" prefix="U">
<description>OpAmpIC</description>
<gates>
<gate name="A" symbol="LF353N"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-8">
<connects>
<connect gate="A" pin="NEGA" pad="2"/>
<connect gate="A" pin="NEGB" pad="6"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="POSA" pad="3"/>
<connect gate="A" pin="POSB" pad="5"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LF353N"/>
<attribute name="OC_FARNELL" value="9487034"/>
<attribute name="OC_NEWARK" value="41K2544"/>
<attribute name="PACKAGE" value="DIP-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LF356H" prefix="U">
<description>IC, OP AMP, JFET</description>
<gates>
<gate name="A" symbol="LF356H"/>
</gates>
<devices>
<device name="" package="TO254P914X470-8P">
<connects>
<connect gate="A" pin="+INA" pad="3"/>
<connect gate="A" pin="-INA" pad="2"/>
<connect gate="A" pin="BALANCE" pad="5"/>
<connect gate="A" pin="BALANCE_2" pad="1"/>
<connect gate="A" pin="NC" pad="8"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LF356H"/>
<attribute name="OC_FARNELL" value="1216160"/>
<attribute name="OC_NEWARK" value="01M8115"/>
<attribute name="PACKAGE" value="TO-99-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LF356M" prefix="U">
<description>Operational Amplifiers</description>
<gates>
<gate name="A" symbol="LF356M"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="BAL" pad="5"/>
<connect gate="A" pin="BAL_2" pad="1"/>
<connect gate="A" pin="NC" pad="8"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LF356M"/>
<attribute name="OC_FARNELL" value="9486992"/>
<attribute name="OC_NEWARK" value="07B5540"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LF356N" prefix="U">
<description>OP Amps</description>
<gates>
<gate name="A" symbol="LF356N"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-8">
<connects>
<connect gate="A" pin="IN" pad="3"/>
<connect gate="A" pin="IN_2" pad="2"/>
<connect gate="A" pin="NC" pad="8"/>
<connect gate="A" pin="OFS" pad="5"/>
<connect gate="A" pin="OFS_2" pad="1"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LF356N"/>
<attribute name="OC_FARNELL" value="9487000"/>
<attribute name="OC_NEWARK" value="41K2547"/>
<attribute name="PACKAGE" value="8-DIP"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LF411ACN" prefix="U">
<description>OP AMP</description>
<gates>
<gate name="A" symbol="LF411ACN"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-8">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="BALANCE" pad="5"/>
<connect gate="A" pin="BALANCE_2" pad="1"/>
<connect gate="A" pin="N/C" pad="8"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LF411ACN"/>
<attribute name="OC_FARNELL" value="9487018"/>
<attribute name="OC_NEWARK" value="07B5549"/>
<attribute name="PACKAGE" value="8-DIP"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LF411CN" prefix="U">
<description>OP AMP</description>
<gates>
<gate name="A" symbol="LF411CN"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-8">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="BALANCE" pad="5"/>
<connect gate="A" pin="BALANCE_2" pad="1"/>
<connect gate="A" pin="N/C" pad="8"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LF411CN"/>
<attribute name="OC_FARNELL" value="9487026"/>
<attribute name="OC_NEWARK" value="07B5550"/>
<attribute name="PACKAGE" value="8-DIP"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LF412ACN" prefix="U">
<description>Operational Amplifiers</description>
<gates>
<gate name="A" symbol="LF412ACN"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-8">
<connects>
<connect gate="A" pin="NEGA" pad="2"/>
<connect gate="A" pin="NEGB" pad="6"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="POSA" pad="3"/>
<connect gate="A" pin="POSB" pad="5"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LF412ACN"/>
<attribute name="OC_FARNELL" value="1468876"/>
<attribute name="OC_NEWARK" value="07B5551"/>
<attribute name="PACKAGE" value="DIP-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LF412CN" prefix="U">
<description>OP AMP</description>
<gates>
<gate name="A" symbol="LF412CN"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-8">
<connects>
<connect gate="A" pin="NEG_A" pad="2"/>
<connect gate="A" pin="NEG_B" pad="6"/>
<connect gate="A" pin="OUT_A" pad="1"/>
<connect gate="A" pin="OUT_B" pad="7"/>
<connect gate="A" pin="POS_A" pad="3"/>
<connect gate="A" pin="POS_B" pad="5"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LF412CN"/>
<attribute name="OC_FARNELL" value="9487042"/>
<attribute name="OC_NEWARK" value="07B5552"/>
<attribute name="PACKAGE" value="8-DIP"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LF412MH" prefix="U">
<description>IC OP AMP DUAL LOW JFET IN</description>
<gates>
<gate name="A" symbol="LF412MH"/>
</gates>
<devices>
<device name="" package="TO292P914X470-8P">
<connects>
<connect gate="A" pin="+INA" pad="3"/>
<connect gate="A" pin="+INB" pad="5"/>
<connect gate="A" pin="-INA" pad="2"/>
<connect gate="A" pin="-INB" pad="6"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LF412MH"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="31T9700"/>
<attribute name="PACKAGE" value="TO-5-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LF442ACN" prefix="U">
<description>Operational Amplifiers</description>
<gates>
<gate name="A" symbol="LF442ACN"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-8">
<connects>
<connect gate="A" pin="NEGA" pad="2"/>
<connect gate="A" pin="NEGB" pad="6"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="POSA" pad="3"/>
<connect gate="A" pin="POSB" pad="5"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LF442ACN"/>
<attribute name="OC_FARNELL" value="1685311"/>
<attribute name="OC_NEWARK" value="41K2556"/>
<attribute name="PACKAGE" value="DIP-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LF442AMH" prefix="U">
<description>IC OP AMP DUAL LP JFET</description>
<gates>
<gate name="A" symbol="LF442AMH"/>
</gates>
<devices>
<device name="" package="TO292P914X470-8P">
<connects>
<connect gate="A" pin="+INA" pad="3"/>
<connect gate="A" pin="+INB" pad="5"/>
<connect gate="A" pin="-INA" pad="2"/>
<connect gate="A" pin="-INB" pad="6"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LF442AMH"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="31T9701"/>
<attribute name="PACKAGE" value="TO-5-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LF442CN" prefix="U">
<description>OP AMP</description>
<gates>
<gate name="A" symbol="LF442CN"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-8">
<connects>
<connect gate="A" pin="NEG_A" pad="2"/>
<connect gate="A" pin="NEG_B" pad="6"/>
<connect gate="A" pin="OUT_A" pad="1"/>
<connect gate="A" pin="OUT_B" pad="7"/>
<connect gate="A" pin="POS_A" pad="3"/>
<connect gate="A" pin="POS_B" pad="5"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LF442CN"/>
<attribute name="OC_FARNELL" value="9487050"/>
<attribute name="OC_NEWARK" value="07B5554"/>
<attribute name="PACKAGE" value="8-DIP"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LF444ACN" prefix="U">
<description>OpAmpIC</description>
<gates>
<gate name="A" symbol="LF444ACN"/>
</gates>
<devices>
<device name="" package="DIP245762X508-14">
<connects>
<connect gate="A" pin="IN1+" pad="3"/>
<connect gate="A" pin="IN1-" pad="2"/>
<connect gate="A" pin="IN2+" pad="5"/>
<connect gate="A" pin="IN2-" pad="6"/>
<connect gate="A" pin="IN3+" pad="10"/>
<connect gate="A" pin="IN3-" pad="9"/>
<connect gate="A" pin="IN4+" pad="12"/>
<connect gate="A" pin="IN4-" pad="13"/>
<connect gate="A" pin="OUT1" pad="1"/>
<connect gate="A" pin="OUT2" pad="7"/>
<connect gate="A" pin="OUT3" pad="8"/>
<connect gate="A" pin="OUT4" pad="14"/>
<connect gate="A" pin="V+" pad="4"/>
<connect gate="A" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LF444ACN"/>
<attribute name="OC_FARNELL" value="1468878"/>
<attribute name="OC_NEWARK" value="41K2558"/>
<attribute name="PACKAGE" value="DIP-14"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LF444CM" prefix="U">
<description>OpAmpIC</description>
<gates>
<gate name="A" symbol="LF444CM"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="IN1+" pad="3"/>
<connect gate="A" pin="IN1-" pad="2"/>
<connect gate="A" pin="IN2+" pad="5"/>
<connect gate="A" pin="IN2-" pad="6"/>
<connect gate="A" pin="IN3+" pad="10"/>
<connect gate="A" pin="IN3-" pad="9"/>
<connect gate="A" pin="IN4+" pad="12"/>
<connect gate="A" pin="IN4-" pad="13"/>
<connect gate="A" pin="OUT1" pad="1"/>
<connect gate="A" pin="OUT2" pad="7"/>
<connect gate="A" pin="OUT3" pad="8"/>
<connect gate="A" pin="OUT4" pad="14"/>
<connect gate="A" pin="V+" pad="4"/>
<connect gate="A" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LF444CM"/>
<attribute name="OC_FARNELL" value="1564711"/>
<attribute name="OC_NEWARK" value="07B5556"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LF444CN" prefix="U">
<description>OP AMP</description>
<gates>
<gate name="A" symbol="LF444CN"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-14">
<connects>
<connect gate="A" pin="IN1+" pad="3"/>
<connect gate="A" pin="IN1-" pad="2"/>
<connect gate="A" pin="IN2+" pad="5"/>
<connect gate="A" pin="IN2-" pad="6"/>
<connect gate="A" pin="IN3+" pad="10"/>
<connect gate="A" pin="IN3-" pad="9"/>
<connect gate="A" pin="IN4+" pad="12"/>
<connect gate="A" pin="IN4-" pad="13"/>
<connect gate="A" pin="OUT_1" pad="1"/>
<connect gate="A" pin="OUT_2" pad="7"/>
<connect gate="A" pin="OUT_3" pad="8"/>
<connect gate="A" pin="OUT_4" pad="14"/>
<connect gate="A" pin="V+" pad="4"/>
<connect gate="A" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LF444CN"/>
<attribute name="OC_FARNELL" value="9487085"/>
<attribute name="OC_NEWARK" value="07B5558"/>
<attribute name="PACKAGE" value="14-DIP"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM101AH" prefix="U">
<description>IC, OP-AMP</description>
<gates>
<gate name="A" symbol="LM101AH"/>
</gates>
<devices>
<device name="" package="TO254P914X470-8P">
<connects>
<connect gate="A" pin="+INA" pad="3"/>
<connect gate="A" pin="-INA" pad="2"/>
<connect gate="A" pin="BALANCE" pad="5"/>
<connect gate="A" pin="BALANCE_2" pad="1"/>
<connect gate="A" pin="COMP" pad="8"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM101AH"/>
<attribute name="OC_FARNELL" value="1216149"/>
<attribute name="OC_NEWARK" value="31T9751"/>
<attribute name="PACKAGE" value="TO-99-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM101AHLQMLV" prefix="U">
<description>Operational Amplifier</description>
<gates>
<gate name="A" symbol="LM101AHLQMLV"/>
</gates>
<devices>
<device name="" package="TO254P914X530-8P">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="BALANCE" pad="5"/>
<connect gate="A" pin="BALANCE_2" pad="1"/>
<connect gate="A" pin="COMPENSATION" pad="8"/>
<connect gate="A" pin="OUTPUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM101AHLQMLV"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="31T9752"/>
<attribute name="PACKAGE" value="TO99-8"/>
<attribute name="SUPPLIER" value="National Semicondutors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM101AJLQMLV" prefix="U">
<description>OpAmpIC</description>
<gates>
<gate name="A" symbol="LM101AJLQMLV"/>
</gates>
<devices>
<device name="" package="DIP254762X508-8">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="BAL" pad="5"/>
<connect gate="A" pin="BAL/COMP" pad="1"/>
<connect gate="A" pin="COMP" pad="8"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM101AJLQMLV"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="31T9753"/>
<attribute name="PACKAGE" value="DIP-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM1084IS-12" prefix="U">
<description>Low Dropout Positive Regulators</description>
<gates>
<gate name="A" symbol="LM1084IS-12"/>
</gates>
<devices>
<device name="" package="TO254P1435X457-3N">
<connects>
<connect gate="A" pin="ADJ/GND" pad="1"/>
<connect gate="A" pin="IN" pad="3"/>
<connect gate="A" pin="OUT" pad="2"/>
<connect gate="A" pin="VOUT" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM1084IS-12"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K3359"/>
<attribute name="PACKAGE" value="TO-263-3"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM1084IS-3.3" prefix="U">
<description>Low Dropout Positive Regulators</description>
<gates>
<gate name="A" symbol="LM1084IS-3.3"/>
</gates>
<devices>
<device name="" package="TO254P1435X457-3N">
<connects>
<connect gate="A" pin="ADJ/GND" pad="1"/>
<connect gate="A" pin="IN" pad="3"/>
<connect gate="A" pin="OUT" pad="2"/>
<connect gate="A" pin="VOUT" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM1084IS-3.3"/>
<attribute name="OC_FARNELL" value="1564625"/>
<attribute name="OC_NEWARK" value="41K3361"/>
<attribute name="PACKAGE" value="TO-263-3"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM1084IS-5.0" prefix="U">
<description>Low Dropout Positive Regulators</description>
<gates>
<gate name="A" symbol="LM1084IS-5.0"/>
</gates>
<devices>
<device name="" package="TO254P1435X457-3N">
<connects>
<connect gate="A" pin="ADJ/GND" pad="1"/>
<connect gate="A" pin="IN" pad="3"/>
<connect gate="A" pin="OUT" pad="2"/>
<connect gate="A" pin="VOUT" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM1084IS-5.0"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K3362"/>
<attribute name="PACKAGE" value="TO-263-3"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM1084IT-3.3" prefix="U">
<description>IC, V REG, LINEAR, 3.3V</description>
<gates>
<gate name="A" symbol="LM1084IT-3.3"/>
</gates>
<devices>
<device name="" package="TO254P470X1016X2222-3P">
<connects>
<connect gate="A" pin="ADJ/GND" pad="1"/>
<connect gate="A" pin="VIN" pad="3"/>
<connect gate="A" pin="VOUT" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM1084IT-3.3"/>
<attribute name="OC_FARNELL" value="1469037"/>
<attribute name="OC_NEWARK" value="41K3369"/>
<attribute name="PACKAGE" value="TO-220"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM1084IT-5.0" prefix="U">
<description>IC, LDO VOLT REG, 5V, 5A</description>
<gates>
<gate name="A" symbol="LM1084IT-5.0"/>
</gates>
<devices>
<device name="" package="TO254P470X1016X2222-3P">
<connects>
<connect gate="A" pin="ADJ/GND" pad="1"/>
<connect gate="A" pin="IN" pad="3"/>
<connect gate="A" pin="OUT" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM1084IT-5.0"/>
<attribute name="OC_FARNELL" value="8207291"/>
<attribute name="OC_NEWARK" value="41K3370"/>
<attribute name="PACKAGE" value="TO-220"/>
<attribute name="SUPPLIER" value="NATIONAL SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM1085IS-12" prefix="U">
<description>Low Dropout Positive Regulators</description>
<gates>
<gate name="A" symbol="LM1085IS-12"/>
</gates>
<devices>
<device name="" package="TO254P1435X457-3N">
<connects>
<connect gate="A" pin="ADJ/GND" pad="1"/>
<connect gate="A" pin="IN" pad="3"/>
<connect gate="A" pin="OUT" pad="2"/>
<connect gate="A" pin="VOUT" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM1085IS-12"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K3372"/>
<attribute name="PACKAGE" value="TO-263-3"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM1085IS-3.3" prefix="U">
<description>Low Dropout Positive Regulators</description>
<gates>
<gate name="A" symbol="LM1085IS-3.3"/>
</gates>
<devices>
<device name="" package="TO254P1435X457-3N">
<connects>
<connect gate="A" pin="ADJ/GND" pad="1"/>
<connect gate="A" pin="IN" pad="3"/>
<connect gate="A" pin="OUT" pad="2"/>
<connect gate="A" pin="VOUT" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM1085IS-3.3"/>
<attribute name="OC_FARNELL" value="1469039"/>
<attribute name="OC_NEWARK" value="41K3373"/>
<attribute name="PACKAGE" value="TO-263-3"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM1085IS-5.0" prefix="U">
<description>Low Dropout Positive Regulators</description>
<gates>
<gate name="A" symbol="LM1085IS-5.0"/>
</gates>
<devices>
<device name="" package="TO254P1435X457-3N">
<connects>
<connect gate="A" pin="ADJ/GND" pad="1"/>
<connect gate="A" pin="IN" pad="3"/>
<connect gate="A" pin="OUT" pad="2"/>
<connect gate="A" pin="VOUT" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM1085IS-5.0"/>
<attribute name="OC_FARNELL" value="1469040"/>
<attribute name="OC_NEWARK" value="41K3374"/>
<attribute name="PACKAGE" value="TO-263-3"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM1085IT-3.3" prefix="U">
<description>IC REG POSITIVE 3A LDO</description>
<gates>
<gate name="A" symbol="LM1085IT-3.3"/>
</gates>
<devices>
<device name="" package="TO254P470X1016X2222-3P">
<connects>
<connect gate="A" pin="ADJ/GND" pad="1"/>
<connect gate="A" pin="VIN" pad="3"/>
<connect gate="A" pin="VOUT" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM1085IT-3.3"/>
<attribute name="OC_FARNELL" value="1469041"/>
<attribute name="OC_NEWARK" value="41K3381"/>
<attribute name="PACKAGE" value="TO-220"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM1085IT-5.0" prefix="U">
<description>IC, LDO VOLT REG, 5V, 1.5A</description>
<gates>
<gate name="A" symbol="LM1085IT-5.0"/>
</gates>
<devices>
<device name="" package="TO254P470X1016X2222-3P">
<connects>
<connect gate="A" pin="ADJ/GND" pad="1"/>
<connect gate="A" pin="VIN" pad="3"/>
<connect gate="A" pin="VOUT" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM1085IT-5.0"/>
<attribute name="OC_FARNELL" value="1469042"/>
<attribute name="OC_NEWARK" value="41K3382"/>
<attribute name="PACKAGE" value="TO-220"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM1085IT-ADJ" prefix="U">
<description>IC, ADJ LDO REG, 1.2V TO 15V, 3A</description>
<gates>
<gate name="A" symbol="LM1085IT-ADJ"/>
</gates>
<devices>
<device name="" package="TO254P470X1016X2222-3P">
<connects>
<connect gate="A" pin="ADJ/GND" pad="1"/>
<connect gate="A" pin="IN" pad="3"/>
<connect gate="A" pin="OUT" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM1085IT-ADJ"/>
<attribute name="OC_FARNELL" value="8207364"/>
<attribute name="OC_NEWARK" value="41K3379"/>
<attribute name="PACKAGE" value="TO-220"/>
<attribute name="SUPPLIER" value="NATIONAL SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM1086CS-2.5" prefix="U">
<description>Low Dropout Positive Regulators</description>
<gates>
<gate name="A" symbol="LM1086CS-2.5"/>
</gates>
<devices>
<device name="" package="TO254P1435X457-3N">
<connects>
<connect gate="A" pin="ADJ/GND" pad="1"/>
<connect gate="A" pin="IN" pad="3"/>
<connect gate="A" pin="OUT" pad="2"/>
<connect gate="A" pin="VOUT" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM1086CS-2.5"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K3384"/>
<attribute name="PACKAGE" value="TO-263-3"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM1086CT-3.3" prefix="U">
<description>IC, LDO VOLT REG, 3.3V, 1.5A</description>
<gates>
<gate name="A" symbol="LM1086CT-3.3"/>
</gates>
<devices>
<device name="" package="TO254P470X1016X2222-3P">
<connects>
<connect gate="A" pin="ADJ/GND" pad="1"/>
<connect gate="A" pin="IN" pad="3"/>
<connect gate="A" pin="OUT" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM1086CT-3.3"/>
<attribute name="OC_FARNELL" value="9489983"/>
<attribute name="OC_NEWARK" value="41K3395"/>
<attribute name="PACKAGE" value="TO-220"/>
<attribute name="SUPPLIER" value="NATIONAL SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM1086CT-5.0" prefix="U">
<description>IC, LDO VOLT REG, 5V, 1.5A</description>
<gates>
<gate name="A" symbol="LM1086CT-5.0"/>
</gates>
<devices>
<device name="" package="TO254P470X1016X2222-3P">
<connects>
<connect gate="A" pin="ADJ/GND" pad="1"/>
<connect gate="A" pin="VIN" pad="3"/>
<connect gate="A" pin="VOUT" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM1086CT-5.0"/>
<attribute name="OC_FARNELL" value="1685486"/>
<attribute name="OC_NEWARK" value="41K3396"/>
<attribute name="PACKAGE" value="TO-220"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM1086CT-ADJ" prefix="U">
<description>IC, ADJ LDO REG, 1.2V TO 15V, 1.5A</description>
<gates>
<gate name="A" symbol="LM1086CT-ADJ"/>
</gates>
<devices>
<device name="" package="TO254P470X1016X2222-3P">
<connects>
<connect gate="A" pin="ADJ/GND" pad="1"/>
<connect gate="A" pin="IN" pad="3"/>
<connect gate="A" pin="OUT" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM1086CT-ADJ"/>
<attribute name="OC_FARNELL" value="9489967"/>
<attribute name="OC_NEWARK" value="41K3393"/>
<attribute name="PACKAGE" value="TO-220"/>
<attribute name="SUPPLIER" value="NATIONAL SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM1086IT-3.3" prefix="U">
<description>IC, LDO VOLT REG, 3.3V, 1.5A</description>
<gates>
<gate name="A" symbol="LM1086IT-3.3"/>
</gates>
<devices>
<device name="" package="TO254P470X1016X2222-3P">
<connects>
<connect gate="A" pin="ADJ/GND" pad="1"/>
<connect gate="A" pin="VIN" pad="3"/>
<connect gate="A" pin="VOUT" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM1086IT-3.3"/>
<attribute name="OC_FARNELL" value="1685601"/>
<attribute name="OC_NEWARK" value="41K3424"/>
<attribute name="PACKAGE" value="TO-220"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM1086IT-5.0" prefix="U">
<description>IC, LDO VOLT REG, 5.0V, 1.5A</description>
<gates>
<gate name="A" symbol="LM1086IT-5.0"/>
</gates>
<devices>
<device name="" package="TO254P470X1016X2222-3P">
<connects>
<connect gate="A" pin="ADJ/GND" pad="1"/>
<connect gate="A" pin="VIN" pad="3"/>
<connect gate="A" pin="VOUT" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM1086IT-5.0"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K3425"/>
<attribute name="PACKAGE" value="TO-220"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM10CLN" prefix="U">
<description>OP AMP</description>
<gates>
<gate name="A" symbol="LM10CLN"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-8">
<connects>
<connect gate="A" pin="BALANCE" pad="5"/>
<connect gate="A" pin="OP_AMP_IN+" pad="3"/>
<connect gate="A" pin="OP_AMP_IN-" pad="2"/>
<connect gate="A" pin="OP_AMP_OUT" pad="6"/>
<connect gate="A" pin="REFERENCE_FEED_BACK" pad="8"/>
<connect gate="A" pin="REFERENCE_OUT" pad="1"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM10CLN"/>
<attribute name="OC_FARNELL" value="9486704"/>
<attribute name="OC_NEWARK" value="97K3184"/>
<attribute name="PACKAGE" value="8-DIP"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM10CN" prefix="U">
<description>OP AMP</description>
<gates>
<gate name="A" symbol="LM10CN"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-8">
<connects>
<connect gate="A" pin="BALANCE" pad="5"/>
<connect gate="A" pin="OP_AMP_IN+" pad="3"/>
<connect gate="A" pin="OP_AMP_IN-" pad="2"/>
<connect gate="A" pin="OP_AMP_OUT" pad="6"/>
<connect gate="A" pin="REFERENCE_FEED_BACK" pad="8"/>
<connect gate="A" pin="REFERENCE_OUT" pad="1"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM10CN"/>
<attribute name="OC_FARNELL" value="9486712"/>
<attribute name="OC_NEWARK" value="07B5852"/>
<attribute name="PACKAGE" value="8-DIP"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM10CWM" prefix="U">
<description>OpAmpIC</description>
<gates>
<gate name="A" symbol="LM10CWM"/>
</gates>
<devices>
<device name="" package="SOIC127P1032X264-14N">
<connects>
<connect gate="A" pin="BAL" pad="9"/>
<connect gate="A" pin="NC" pad="14"/>
<connect gate="A" pin="NC_2" pad="1"/>
<connect gate="A" pin="NC_3" pad="7"/>
<connect gate="A" pin="NC_4" pad="2"/>
<connect gate="A" pin="NC_5" pad="8"/>
<connect gate="A" pin="NC_6" pad="13"/>
<connect gate="A" pin="OP_AMP_IN+" pad="5"/>
<connect gate="A" pin="OP_AMP_IN-" pad="4"/>
<connect gate="A" pin="OP_AMP_OUT" pad="10"/>
<connect gate="A" pin="REF_FEEDBACK" pad="12"/>
<connect gate="A" pin="REF_OUT" pad="3"/>
<connect gate="A" pin="V+" pad="11"/>
<connect gate="A" pin="V-" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM10CWM"/>
<attribute name="OC_FARNELL" value="1468909"/>
<attribute name="OC_NEWARK" value="41K3354"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM1117DT-1.8" prefix="U">
<description>IC, LDO, 800MA, 1.8V, 3TO252</description>
<gates>
<gate name="A" symbol="LM1117DT-1.8"/>
</gates>
<devices>
<device name="" package="TO228P970X238-3N">
<connects>
<connect gate="A" pin="ADJ_/_GND" pad="1"/>
<connect gate="A" pin="VIN" pad="3"/>
<connect gate="A" pin="VOUT" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM1117DT-1.8"/>
<attribute name="OC_FARNELL" value="1798351"/>
<attribute name="OC_NEWARK" value="73R9726"/>
<attribute name="PACKAGE" value="TO-252-3"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM1117DT-2.5" prefix="U">
<description>IC REG LDO 800MA 2.5V</description>
<gates>
<gate name="A" symbol="LM1117DT-2.5"/>
</gates>
<devices>
<device name="" package="TO228P970X238-3N">
<connects>
<connect gate="A" pin="ADJ_/_GND" pad="1"/>
<connect gate="A" pin="VIN" pad="3"/>
<connect gate="A" pin="VOUT" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM1117DT-25"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K3428"/>
<attribute name="PACKAGE" value="TO-252-3"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM1117DT-3.3" prefix="U">
<description>IC, LDO VOLT REG, 3.3V, 0.8A</description>
<gates>
<gate name="A" symbol="LM1117DT-3.3"/>
</gates>
<devices>
<device name="" package="TO228P970X238-3N">
<connects>
<connect gate="A" pin="ADJ_/_GND" pad="1"/>
<connect gate="A" pin="VIN" pad="3"/>
<connect gate="A" pin="VOUT" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM1117DT-3.3"/>
<attribute name="OC_FARNELL" value="9486275"/>
<attribute name="OC_NEWARK" value="41K3430"/>
<attribute name="PACKAGE" value="TO-252-3"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM1117DT-5.0" prefix="U">
<description>IC, LDO VOLT REG, 5V, 0.8A</description>
<gates>
<gate name="A" symbol="LM1117DT-5.0"/>
</gates>
<devices>
<device name="" package="TO228P970X238-3N">
<connects>
<connect gate="A" pin="ADJ_/_GND" pad="1"/>
<connect gate="A" pin="VIN" pad="3"/>
<connect gate="A" pin="VOUT" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM1117DT-5.0"/>
<attribute name="OC_FARNELL" value="9486283"/>
<attribute name="OC_NEWARK" value="41K3431"/>
<attribute name="PACKAGE" value="TO-252-3"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM1117DT-ADJ" prefix="U">
<description>IC, ADJ LDO REG, 1.25V TO 13.8V</description>
<gates>
<gate name="A" symbol="LM1117DT-ADJ"/>
</gates>
<devices>
<device name="" package="TO228P970X238-3N">
<connects>
<connect gate="A" pin="ADJ_/_GND" pad="1"/>
<connect gate="A" pin="VIN" pad="3"/>
<connect gate="A" pin="VOUT" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM1117DT-ADJ"/>
<attribute name="OC_FARNELL" value="1364485"/>
<attribute name="OC_NEWARK" value="41K3426"/>
<attribute name="PACKAGE" value="TO-252-3"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM1117IDT-3.3" prefix="U">
<description>IC REG LDO 800MA 3.3V</description>
<gates>
<gate name="A" symbol="LM1117IDT-3.3"/>
</gates>
<devices>
<device name="" package="TO228P970X238-3N">
<connects>
<connect gate="A" pin="ADJ_/_GND" pad="1"/>
<connect gate="A" pin="VIN" pad="3"/>
<connect gate="A" pin="VOUT" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM1117IDT-3.3"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K3438"/>
<attribute name="PACKAGE" value="TO-252-3"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM1117IDT-5.0" prefix="U">
<description>IC REG LDO 800MA 5.0V</description>
<gates>
<gate name="A" symbol="LM1117IDT-5.0"/>
</gates>
<devices>
<device name="" package="TO228P970X238-3N">
<connects>
<connect gate="A" pin="ADJ_/_GND" pad="1"/>
<connect gate="A" pin="VIN" pad="3"/>
<connect gate="A" pin="VOUT" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM1117IDT-5.0"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K3439"/>
<attribute name="PACKAGE" value="TO-252-3"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM1117IMP-3.3" prefix="U">
<description>IC REG LDO 800MA 3.3V</description>
<gates>
<gate name="A" symbol="LM1117IMP-3.3"/>
</gates>
<devices>
<device name="" package="SOT230P696X180-4N">
<connects>
<connect gate="A" pin="ADJ/GND" pad="1"/>
<connect gate="A" pin="VIN" pad="3"/>
<connect gate="A" pin="VOUT" pad="2"/>
<connect gate="A" pin="VOUT_2" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM1117IMP-3.3"/>
<attribute name="OC_FARNELL" value="1469051"/>
<attribute name="OC_NEWARK" value="41K3450"/>
<attribute name="PACKAGE" value="SOT-223"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM1117IMP-5.0" prefix="U">
<description>IC REG LDO 800MA 5.0V</description>
<gates>
<gate name="A" symbol="LM1117IMP-5.0"/>
</gates>
<devices>
<device name="" package="SOT230P696X180-4N">
<connects>
<connect gate="A" pin="ADJ/GND" pad="1"/>
<connect gate="A" pin="VIN" pad="3"/>
<connect gate="A" pin="VOUT" pad="2"/>
<connect gate="A" pin="VOUT_2" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM1117IMP-5.0"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K3451"/>
<attribute name="PACKAGE" value="SOT-223"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM1117LD-1.8" prefix="U">
<description>Linear regulators</description>
<gates>
<gate name="A" symbol="LM1117LD-1.8"/>
</gates>
<devices>
<device name="" package="DFN400X400X80-9N">
<connects>
<connect gate="A" pin="ADJ/GND" pad="1"/>
<connect gate="A" pin="NC" pad="8"/>
<connect gate="A" pin="VIN" pad="4"/>
<connect gate="A" pin="VIN_2" pad="2"/>
<connect gate="A" pin="VIN_3" pad="3"/>
<connect gate="A" pin="VOUT" pad="9"/>
<connect gate="A" pin="VOUT_2" pad="5"/>
<connect gate="A" pin="VOUT_3" pad="6"/>
<connect gate="A" pin="VOUT_4" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM1117LD-1.8"/>
<attribute name="OC_FARNELL" value="1798353"/>
<attribute name="OC_NEWARK" value="75R2089"/>
<attribute name="PACKAGE" value="LLP-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM1117LD-3.3" prefix="U">
<description>Linear regulators</description>
<gates>
<gate name="A" symbol="LM1117LD-3.3"/>
</gates>
<devices>
<device name="" package="DFN400X400X80-9N">
<connects>
<connect gate="A" pin="ADJ/GND" pad="1"/>
<connect gate="A" pin="NC" pad="8"/>
<connect gate="A" pin="VIN" pad="4"/>
<connect gate="A" pin="VIN_2" pad="2"/>
<connect gate="A" pin="VIN_3" pad="3"/>
<connect gate="A" pin="VOUT" pad="9"/>
<connect gate="A" pin="VOUT_2" pad="5"/>
<connect gate="A" pin="VOUT_3" pad="6"/>
<connect gate="A" pin="VOUT_4" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM1117LD-3.3"/>
<attribute name="OC_FARNELL" value="8221901"/>
<attribute name="OC_NEWARK" value="38K3616"/>
<attribute name="PACKAGE" value="LLP-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM1117MP-1.8" prefix="U">
<description>IC REG LDO 800MA 1.8V</description>
<gates>
<gate name="A" symbol="LM1117MP-1.8"/>
</gates>
<devices>
<device name="" package="SOT230P696X180-4N">
<connects>
<connect gate="A" pin="ADJ/GND" pad="1"/>
<connect gate="A" pin="VIN" pad="3"/>
<connect gate="A" pin="VOUT" pad="2"/>
<connect gate="A" pin="VOUT_2" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM1117MP-1.8"/>
<attribute name="OC_FARNELL" value="1469053"/>
<attribute name="OC_NEWARK" value="41K3467"/>
<attribute name="PACKAGE" value="SOT-223"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM1117MP-2.5" prefix="U">
<description>Linear regulators</description>
<gates>
<gate name="A" symbol="LM1117MP-2.5"/>
</gates>
<devices>
<device name="" package="SOT230P696X180-4N">
<connects>
<connect gate="A" pin="ADJ/GND" pad="1"/>
<connect gate="A" pin="IN" pad="3"/>
<connect gate="A" pin="OUT" pad="2"/>
<connect gate="A" pin="VOUT" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM1117MP-2.5"/>
<attribute name="OC_FARNELL" value="9779205"/>
<attribute name="OC_NEWARK" value="41K3468"/>
<attribute name="PACKAGE" value="SOT223-3"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM1117MP-3.3" prefix="U">
<description>Linear regulators</description>
<gates>
<gate name="A" symbol="LM1117MP-3.3"/>
</gates>
<devices>
<device name="" package="SOT230P696X180-4N">
<connects>
<connect gate="A" pin="ADJ/GND" pad="1"/>
<connect gate="A" pin="IN" pad="3"/>
<connect gate="A" pin="OUT" pad="2"/>
<connect gate="A" pin="VOUT" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM1117MP-3.3"/>
<attribute name="OC_FARNELL" value="9778195"/>
<attribute name="OC_NEWARK" value="41K3470"/>
<attribute name="PACKAGE" value="SOT223-3"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM1117MP-5.0" prefix="U">
<description>Linear regulators</description>
<gates>
<gate name="A" symbol="LM1117MP-5.0"/>
</gates>
<devices>
<device name="" package="SOT230P696X180-4N">
<connects>
<connect gate="A" pin="ADJ/GND" pad="1"/>
<connect gate="A" pin="IN" pad="3"/>
<connect gate="A" pin="OUT" pad="2"/>
<connect gate="A" pin="VOUT" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM1117MP-5.0"/>
<attribute name="OC_FARNELL" value="9778209"/>
<attribute name="OC_NEWARK" value="41K3471"/>
<attribute name="PACKAGE" value="SOT223-3"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM1117MP-ADJ" prefix="U">
<description>Linear regulators</description>
<gates>
<gate name="A" symbol="LM1117MP-ADJ"/>
</gates>
<devices>
<device name="" package="SOT230P696X180-4N">
<connects>
<connect gate="A" pin="ADJ/GND" pad="1"/>
<connect gate="A" pin="IN" pad="3"/>
<connect gate="A" pin="OUT" pad="2"/>
<connect gate="A" pin="VOUT" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM1117MP-ADJ"/>
<attribute name="OC_FARNELL" value="9778187"/>
<attribute name="OC_NEWARK" value="13B5337"/>
<attribute name="PACKAGE" value="SOT223-3"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM1117S-ADJ" prefix="U">
<description>Low-Dropout Linear Regulator</description>
<gates>
<gate name="A" symbol="LM1117S-ADJ"/>
</gates>
<devices>
<device name="" package="TO254P1435X457-4N">
<connects>
<connect gate="A" pin="ADJ/GND" pad="1"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="IN" pad="3"/>
<connect gate="A" pin="OUT" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM1117S-ADJ"/>
<attribute name="OC_FARNELL" value="8221910"/>
<attribute name="OC_NEWARK" value="41K3478"/>
<attribute name="PACKAGE" value="TO-263-3"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM1117T-2.5" prefix="U">
<description>IC, LDO, 800MA, 2.5V</description>
<gates>
<gate name="A" symbol="LM1117T-2.5"/>
</gates>
<devices>
<device name="" package="TO254P470X1016X2222-3P">
<connects>
<connect gate="A" pin="ADJ/GND" pad="1"/>
<connect gate="A" pin="IN" pad="3"/>
<connect gate="A" pin="OUT" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM1117T-2.5"/>
<attribute name="OC_FARNELL" value="1798354"/>
<attribute name="OC_NEWARK" value="75R2090"/>
<attribute name="PACKAGE" value="TO-220"/>
<attribute name="SUPPLIER" value="NATIONAL SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM1117T-3.3" prefix="U">
<description>IC, LDO VOLT REG, 3.3V, 0.8A</description>
<gates>
<gate name="A" symbol="LM1117T-3.3"/>
</gates>
<devices>
<device name="" package="TO254P470X1016X2222-3P">
<connects>
<connect gate="A" pin="ADJ/GND" pad="1"/>
<connect gate="A" pin="IN" pad="3"/>
<connect gate="A" pin="OUT" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM1117T-3.3"/>
<attribute name="OC_FARNELL" value="9485813"/>
<attribute name="OC_NEWARK" value="41K3490"/>
<attribute name="PACKAGE" value="TO-220"/>
<attribute name="SUPPLIER" value="NATIONAL SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM1117T-5.0" prefix="U">
<description>IC, LDO VOLT REG, 5V, 0.8A</description>
<gates>
<gate name="A" symbol="LM1117T-5.0"/>
</gates>
<devices>
<device name="" package="TO254P470X1016X2222-3P">
<connects>
<connect gate="A" pin="ADJ/GND" pad="1"/>
<connect gate="A" pin="IN" pad="3"/>
<connect gate="A" pin="OUT" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM1117T-5.0"/>
<attribute name="OC_FARNELL" value="1215183"/>
<attribute name="OC_NEWARK" value="41K3491"/>
<attribute name="PACKAGE" value="TO-220"/>
<attribute name="SUPPLIER" value="NATIONAL SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM1117T-ADJ" prefix="U">
<description>IC, ADJ LDO REG, 1.25V TO 13.8V</description>
<gates>
<gate name="A" symbol="LM1117T-ADJ"/>
</gates>
<devices>
<device name="" package="TO254P470X1016X2222-3P">
<connects>
<connect gate="A" pin="ADJ/GND" pad="1"/>
<connect gate="A" pin="IN" pad="3"/>
<connect gate="A" pin="OUT" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM1117T-ADJ"/>
<attribute name="OC_FARNELL" value="9485805"/>
<attribute name="OC_NEWARK" value="41K3486"/>
<attribute name="PACKAGE" value="TO-220"/>
<attribute name="SUPPLIER" value="NATIONAL SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM111H" prefix="U">
<description>"COMPARATOR MIL SPEC, TO-5-8, 111</description>
<gates>
<gate name="A" symbol="LM111H"/>
</gates>
<devices>
<device name="" package="TO254P914X470-8P">
<connects>
<connect gate="A" pin="+IN" pad="2"/>
<connect gate="A" pin="-IN" pad="3"/>
<connect gate="A" pin="BALANCE" pad="5"/>
<connect gate="A" pin="BALANCE/STROBE" pad="6"/>
<connect gate="A" pin="GND" pad="1"/>
<connect gate="A" pin="OUT" pad="7"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM111H"/>
<attribute name="OC_FARNELL" value="1216162"/>
<attribute name="OC_NEWARK" value="01M8125"/>
<attribute name="PACKAGE" value="TO-99-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM111HLQMLV" prefix="U">
<description>3-TERMINAL ADJUSTABLE REGULATOR</description>
<gates>
<gate name="A" symbol="LM111HLQMLV"/>
</gates>
<devices>
<device name="" package="TO254P914X530-8P">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="+V" pad="8"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="BALANCE" pad="5"/>
<connect gate="A" pin="BALANCE/STROBE" pad="6"/>
<connect gate="A" pin="GND" pad="1"/>
<connect gate="A" pin="OUTPUT" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM111HLQMLV"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="31T9760"/>
<attribute name="PACKAGE" value="TO99-8"/>
<attribute name="SUPPLIER" value="National Semicondutors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM111J-8" prefix="U">
<description>DIFFERENTIAL COMPARATORS WITH STROBES</description>
<gates>
<gate name="A" symbol="LM111J-8"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-8">
<connects>
<connect gate="A" pin="BAL/STRB" pad="6"/>
<connect gate="A" pin="BALANCE" pad="5"/>
<connect gate="A" pin="COL_OUT" pad="7"/>
<connect gate="A" pin="EMIT_OUT" pad="1"/>
<connect gate="A" pin="IN+" pad="2"/>
<connect gate="A" pin="IN-" pad="3"/>
<connect gate="A" pin="VCC+" pad="8"/>
<connect gate="A" pin="VCC-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM111J-8"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="13B5332"/>
<attribute name="PACKAGE" value="DIP-8"/>
<attribute name="SUPPLIER" value="NATIONAL SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM111J-8LQMLV" prefix="U">
<description>OpAmpIC</description>
<gates>
<gate name="A" symbol="LM111J-8LQMLV"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-8">
<connects>
<connect gate="A" pin="+IN" pad="2"/>
<connect gate="A" pin="-IN" pad="3"/>
<connect gate="A" pin="BAL" pad="5"/>
<connect gate="A" pin="BAL/STROBE" pad="6"/>
<connect gate="A" pin="GND" pad="1"/>
<connect gate="A" pin="OUT" pad="7"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM111J-8LQMLV"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="31T9762"/>
<attribute name="PACKAGE" value="DIP-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM111WGLQMLV" prefix="U">
<description>OpAmpIC</description>
<gates>
<gate name="A" symbol="LM111WGLQMLV"/>
</gates>
<devices>
<device name="" package="SOIC127P1041X200-10N">
<connects>
<connect gate="A" pin="+IN" pad="2"/>
<connect gate="A" pin="-IN" pad="3"/>
<connect gate="A" pin="BAL" pad="6"/>
<connect gate="A" pin="BAL/STROBE" pad="7"/>
<connect gate="A" pin="GND" pad="1"/>
<connect gate="A" pin="NC" pad="4"/>
<connect gate="A" pin="NC_2" pad="8"/>
<connect gate="A" pin="OUT" pad="9"/>
<connect gate="A" pin="V+" pad="10"/>
<connect gate="A" pin="V-" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM111WGLQMLV"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="31T9764"/>
<attribute name="PACKAGE" value="SOIC-10"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM119H" prefix="U">
<description>IC COMPARATOR DUAL</description>
<gates>
<gate name="A" symbol="LM119H"/>
</gates>
<devices>
<device name="" package="TO292P939X470-10P">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="+IN_2" pad="8"/>
<connect gate="A" pin="-IN" pad="4"/>
<connect gate="A" pin="-IN_2" pad="9"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="GND2" pad="7"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="A" pin="OUT_2" pad="6"/>
<connect gate="A" pin="V+" pad="10"/>
<connect gate="A" pin="V-" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM119H"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="31T9781"/>
<attribute name="PACKAGE" value="TO-100"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM124AJRLQMLV" prefix="U">
<description>OpAmpIC</description>
<gates>
<gate name="A" symbol="LM124AJRLQMLV"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-14">
<connects>
<connect gate="A" pin="+IN1" pad="3"/>
<connect gate="A" pin="+IN2" pad="5"/>
<connect gate="A" pin="+IN3" pad="10"/>
<connect gate="A" pin="+IN4" pad="12"/>
<connect gate="A" pin="-IN1" pad="2"/>
<connect gate="A" pin="-IN2" pad="6"/>
<connect gate="A" pin="-IN3" pad="9"/>
<connect gate="A" pin="-IN4" pad="13"/>
<connect gate="A" pin="GND" pad="11"/>
<connect gate="A" pin="OUT1" pad="1"/>
<connect gate="A" pin="OUT2" pad="7"/>
<connect gate="A" pin="OUT3" pad="8"/>
<connect gate="A" pin="OUT4" pad="14"/>
<connect gate="A" pin="V+" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM124AJRLQMLV"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="31T9792"/>
<attribute name="PACKAGE" value="DIP-14"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM124AJRQMLV" prefix="U">
<description>OpAmpIC</description>
<gates>
<gate name="A" symbol="LM124AJRQMLV"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-14">
<connects>
<connect gate="A" pin="+IN1" pad="3"/>
<connect gate="A" pin="+IN2" pad="5"/>
<connect gate="A" pin="+IN3" pad="10"/>
<connect gate="A" pin="+IN4" pad="12"/>
<connect gate="A" pin="-IN1" pad="2"/>
<connect gate="A" pin="-IN2" pad="6"/>
<connect gate="A" pin="-IN3" pad="9"/>
<connect gate="A" pin="-IN4" pad="13"/>
<connect gate="A" pin="GND" pad="11"/>
<connect gate="A" pin="OUT1" pad="1"/>
<connect gate="A" pin="OUT2" pad="7"/>
<connect gate="A" pin="OUT3" pad="8"/>
<connect gate="A" pin="OUT4" pad="14"/>
<connect gate="A" pin="V+" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM124AJRQMLV"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="31T9793"/>
<attribute name="PACKAGE" value="DIP-14"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM124AWGRLQMLV" prefix="U">
<description>OpAmpIC</description>
<gates>
<gate name="A" symbol="LM124AWGRLQMLV"/>
</gates>
<devices>
<device name="" package="SOIC127P1041X233-14N">
<connects>
<connect gate="A" pin="+IN1" pad="3"/>
<connect gate="A" pin="+IN2" pad="5"/>
<connect gate="A" pin="+IN3" pad="10"/>
<connect gate="A" pin="+IN4" pad="12"/>
<connect gate="A" pin="-IN1" pad="2"/>
<connect gate="A" pin="-IN2" pad="6"/>
<connect gate="A" pin="-IN3" pad="9"/>
<connect gate="A" pin="-IN4" pad="13"/>
<connect gate="A" pin="OUT1" pad="1"/>
<connect gate="A" pin="OUT2" pad="7"/>
<connect gate="A" pin="OUT3" pad="8"/>
<connect gate="A" pin="OUT4" pad="14"/>
<connect gate="A" pin="V+" pad="4"/>
<connect gate="A" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM124AWGRLQMLV"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="31T9794"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM124AWGRQMLV" prefix="U">
<description>OpAmpIC</description>
<gates>
<gate name="A" symbol="LM124AWGRQMLV"/>
</gates>
<devices>
<device name="" package="SOIC127P1041X233-14N">
<connects>
<connect gate="A" pin="+IN1" pad="3"/>
<connect gate="A" pin="+IN2" pad="5"/>
<connect gate="A" pin="+IN3" pad="10"/>
<connect gate="A" pin="+IN4" pad="12"/>
<connect gate="A" pin="-IN1" pad="2"/>
<connect gate="A" pin="-IN2" pad="6"/>
<connect gate="A" pin="-IN3" pad="9"/>
<connect gate="A" pin="-IN4" pad="13"/>
<connect gate="A" pin="OUT1" pad="1"/>
<connect gate="A" pin="OUT2" pad="7"/>
<connect gate="A" pin="OUT3" pad="8"/>
<connect gate="A" pin="OUT4" pad="14"/>
<connect gate="A" pin="V+" pad="4"/>
<connect gate="A" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM124AWGRQMLV"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="31T9795"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM124J" prefix="U">
<description>Low Power Quad Operational Amplifiers</description>
<gates>
<gate name="A" symbol="LM124J"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-14">
<connects>
<connect gate="A" pin="GND" pad="11"/>
<connect gate="A" pin="IN1+" pad="3"/>
<connect gate="A" pin="IN1-" pad="2"/>
<connect gate="A" pin="IN2+" pad="5"/>
<connect gate="A" pin="IN2-" pad="6"/>
<connect gate="A" pin="IN3+" pad="10"/>
<connect gate="A" pin="IN3-" pad="9"/>
<connect gate="A" pin="IN4+" pad="12"/>
<connect gate="A" pin="IN4-" pad="13"/>
<connect gate="A" pin="OUT1" pad="1"/>
<connect gate="A" pin="OUT2" pad="7"/>
<connect gate="A" pin="OUT3" pad="8"/>
<connect gate="A" pin="OUT4" pad="14"/>
<connect gate="A" pin="V+" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM124J"/>
<attribute name="OC_FARNELL" value="399978"/>
<attribute name="OC_NEWARK" value="10WX6988"/>
<attribute name="PACKAGE" value="CDIP-14"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM12H458CIV" prefix="U">
<description>Sign Data Acquisition</description>
<gates>
<gate name="A" symbol="LM12H458CIV"/>
</gates>
<devices>
<device name="" package="PLCC127P1753X1753X457-44N">
<connects>
<connect gate="A" pin="A0" pad="24"/>
<connect gate="A" pin="A1" pad="25"/>
<connect gate="A" pin="A2" pad="26"/>
<connect gate="A" pin="A3" pad="27"/>
<connect gate="A" pin="A4" pad="28"/>
<connect gate="A" pin="ALE" pad="22"/>
<connect gate="A" pin="BW" pad="30"/>
<connect gate="A" pin="CLK" pad="23"/>
<connect gate="A" pin="D0" pad="2"/>
<connect gate="A" pin="D1" pad="3"/>
<connect gate="A" pin="D10" pad="13"/>
<connect gate="A" pin="D11" pad="14"/>
<connect gate="A" pin="D12" pad="15"/>
<connect gate="A" pin="D13" pad="16"/>
<connect gate="A" pin="D14" pad="17"/>
<connect gate="A" pin="D15" pad="18"/>
<connect gate="A" pin="D2" pad="4"/>
<connect gate="A" pin="D3" pad="5"/>
<connect gate="A" pin="D4" pad="6"/>
<connect gate="A" pin="D5" pad="7"/>
<connect gate="A" pin="D6" pad="8"/>
<connect gate="A" pin="D7" pad="9"/>
<connect gate="A" pin="D8" pad="10"/>
<connect gate="A" pin="D9" pad="11"/>
<connect gate="A" pin="DMARQ" pad="32"/>
<connect gate="A" pin="GND" pad="33"/>
<connect gate="A" pin="IN0" pad="34"/>
<connect gate="A" pin="IN1" pad="35"/>
<connect gate="A" pin="IN2" pad="36"/>
<connect gate="A" pin="IN3" pad="37"/>
<connect gate="A" pin="IN4(MUXOUT-)" pad="38"/>
<connect gate="A" pin="IN5(MUXOUT+)" pad="39"/>
<connect gate="A" pin="IN6(S/H_IN-)" pad="40"/>
<connect gate="A" pin="IN7(S/H_IN+)" pad="41"/>
<connect gate="A" pin="SYNC" pad="29"/>
<connect gate="A" pin="VA+" pad="1"/>
<connect gate="A" pin="VD+" pad="12"/>
<connect gate="A" pin="VREF+" pad="43"/>
<connect gate="A" pin="VREF-" pad="42"/>
<connect gate="A" pin="VREFOUT" pad="44"/>
<connect gate="A" pin="~CS" pad="21"/>
<connect gate="A" pin="~INT" pad="31"/>
<connect gate="A" pin="~RD" pad="19"/>
<connect gate="A" pin="~WR" pad="20"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM12H458CIV"/>
<attribute name="OC_FARNELL" value="1673953"/>
<attribute name="OC_NEWARK" value="41K3492"/>
<attribute name="PACKAGE" value="PLCC-44"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM135H" prefix="U">
<description>IC, TEMP SENSOR, ± 0.5°C</description>
<gates>
<gate name="A" symbol="LM135H"/>
</gates>
<devices>
<device name="" package="TO127P543X266-3P">
<connects>
<connect gate="A" pin="+VE" pad="2"/>
<connect gate="A" pin="-VE" pad="3"/>
<connect gate="A" pin="ADJ" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM135H"/>
<attribute name="OC_FARNELL" value="1216167"/>
<attribute name="OC_NEWARK" value="13B5413"/>
<attribute name="PACKAGE" value="TO-46-3"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM13700M" prefix="U">
<description>Dual Operational Transconductance Amplifiers</description>
<gates>
<gate name="A" symbol="LM13700M"/>
</gates>
<devices>
<device name="" package="SOIC127P620X175-16N">
<connects>
<connect gate="A" pin="+IN" pad="14"/>
<connect gate="A" pin="+IN_2" pad="3"/>
<connect gate="A" pin="-IN" pad="13"/>
<connect gate="A" pin="-IN_2" pad="4"/>
<connect gate="A" pin="AMP_BIAS_IN" pad="16"/>
<connect gate="A" pin="AMP_BIAS_IN_2" pad="1"/>
<connect gate="A" pin="BUFFER_IN" pad="10"/>
<connect gate="A" pin="BUFFER_IN_2" pad="7"/>
<connect gate="A" pin="BUFFER_OUT" pad="9"/>
<connect gate="A" pin="BUFFER_OUT_2" pad="8"/>
<connect gate="A" pin="DIODE_BIAS" pad="15"/>
<connect gate="A" pin="DIODE_BIAS_2" pad="2"/>
<connect gate="A" pin="OUT" pad="5"/>
<connect gate="A" pin="OUT_2" pad="12"/>
<connect gate="A" pin="V+" pad="11"/>
<connect gate="A" pin="V-" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM13700M"/>
<attribute name="OC_FARNELL" value="1468910"/>
<attribute name="OC_NEWARK" value="41K3505"/>
<attribute name="PACKAGE" value="SOIC-16"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM13700N" prefix="U">
<description>Dual Operational Transconductance Amplifiers</description>
<gates>
<gate name="A" symbol="LM13700N"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-16">
<connects>
<connect gate="A" pin="+IN" pad="14"/>
<connect gate="A" pin="+IN_2" pad="3"/>
<connect gate="A" pin="-IN" pad="13"/>
<connect gate="A" pin="-IN_2" pad="4"/>
<connect gate="A" pin="AMP_BIAS_IN" pad="16"/>
<connect gate="A" pin="AMP_BIAS_IN_2" pad="1"/>
<connect gate="A" pin="BUFFER_IN" pad="10"/>
<connect gate="A" pin="BUFFER_IN_2" pad="7"/>
<connect gate="A" pin="BUFFER_OUT" pad="9"/>
<connect gate="A" pin="BUFFER_OUT_2" pad="8"/>
<connect gate="A" pin="DIODE_BIAS" pad="15"/>
<connect gate="A" pin="DIODE_BIAS_2" pad="2"/>
<connect gate="A" pin="OUT" pad="5"/>
<connect gate="A" pin="OUT_2" pad="12"/>
<connect gate="A" pin="V+" pad="11"/>
<connect gate="A" pin="V-" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM13700N"/>
<attribute name="OC_FARNELL" value="1651866"/>
<attribute name="OC_NEWARK" value="41K3507"/>
<attribute name="PACKAGE" value="SOIC-16"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM139AJRLQMLV" prefix="U">
<description>OpAmpIC</description>
<gates>
<gate name="A" symbol="LM139AJRLQMLV"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-14">
<connects>
<connect gate="A" pin="+IN1" pad="5"/>
<connect gate="A" pin="+IN2" pad="7"/>
<connect gate="A" pin="+IN3" pad="9"/>
<connect gate="A" pin="+IN4" pad="11"/>
<connect gate="A" pin="-IN1" pad="4"/>
<connect gate="A" pin="-IN2" pad="6"/>
<connect gate="A" pin="-IN3" pad="8"/>
<connect gate="A" pin="-IN4" pad="10"/>
<connect gate="A" pin="GND" pad="12"/>
<connect gate="A" pin="OUT1" pad="2"/>
<connect gate="A" pin="OUT2" pad="1"/>
<connect gate="A" pin="OUT3" pad="14"/>
<connect gate="A" pin="OUT4" pad="13"/>
<connect gate="A" pin="V+" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM139AJRLQMLV"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="31T9806"/>
<attribute name="PACKAGE" value="DIP-14"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM139AJRQMLV" prefix="U">
<description>OpAmpIC</description>
<gates>
<gate name="A" symbol="LM139AJRQMLV"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-14">
<connects>
<connect gate="A" pin="+IN1" pad="5"/>
<connect gate="A" pin="+IN2" pad="7"/>
<connect gate="A" pin="+IN3" pad="9"/>
<connect gate="A" pin="+IN4" pad="11"/>
<connect gate="A" pin="-IN1" pad="4"/>
<connect gate="A" pin="-IN2" pad="6"/>
<connect gate="A" pin="-IN3" pad="8"/>
<connect gate="A" pin="-IN4" pad="10"/>
<connect gate="A" pin="GND" pad="12"/>
<connect gate="A" pin="OUT1" pad="2"/>
<connect gate="A" pin="OUT2" pad="1"/>
<connect gate="A" pin="OUT3" pad="14"/>
<connect gate="A" pin="OUT4" pad="13"/>
<connect gate="A" pin="V+" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM139AJRQMLV"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="31T9807"/>
<attribute name="PACKAGE" value="DIP-14"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM139AWGRQMLV" prefix="U">
<description>OpAmpIC</description>
<gates>
<gate name="A" symbol="LM139AWGRQMLV"/>
</gates>
<devices>
<device name="" package="SOIC127P1041X233-14N">
<connects>
<connect gate="A" pin="+IN1" pad="5"/>
<connect gate="A" pin="+IN2" pad="7"/>
<connect gate="A" pin="+IN3" pad="9"/>
<connect gate="A" pin="+IN4" pad="11"/>
<connect gate="A" pin="-IN1" pad="4"/>
<connect gate="A" pin="-IN2" pad="6"/>
<connect gate="A" pin="-IN3" pad="8"/>
<connect gate="A" pin="-IN4" pad="10"/>
<connect gate="A" pin="GND" pad="12"/>
<connect gate="A" pin="OUT1" pad="2"/>
<connect gate="A" pin="OUT2" pad="1"/>
<connect gate="A" pin="OUT3" pad="14"/>
<connect gate="A" pin="OUT4" pad="13"/>
<connect gate="A" pin="V+" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM139AWGRQMLV"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="31T9810"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM139J" prefix="U">
<description>Quad Comparators</description>
<gates>
<gate name="A" symbol="LM139J"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-14">
<connects>
<connect gate="A" pin="+IN1" pad="5"/>
<connect gate="A" pin="+IN2" pad="7"/>
<connect gate="A" pin="+IN3" pad="9"/>
<connect gate="A" pin="+IN4" pad="11"/>
<connect gate="A" pin="-IN1" pad="4"/>
<connect gate="A" pin="-IN2" pad="6"/>
<connect gate="A" pin="-IN3" pad="8"/>
<connect gate="A" pin="-IN4" pad="10"/>
<connect gate="A" pin="GND" pad="12"/>
<connect gate="A" pin="OUT1" pad="2"/>
<connect gate="A" pin="OUT2" pad="1"/>
<connect gate="A" pin="OUT3" pad="14"/>
<connect gate="A" pin="OUT4" pad="13"/>
<connect gate="A" pin="V+" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM139J"/>
<attribute name="OC_FARNELL" value="404445"/>
<attribute name="OC_NEWARK" value="74P0224"/>
<attribute name="PACKAGE" value="14-CDIP"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM1458M" prefix="U">
<description>Dual Operational Amplifier</description>
<gates>
<gate name="A" symbol="LM1458M"/>
</gates>
<devices>
<device name="" package="SOIC127P620X175-8N">
<connects>
<connect gate="A" pin="NEG_INA" pad="2"/>
<connect gate="A" pin="NEG_INB" pad="6"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="POS_INA" pad="3"/>
<connect gate="A" pin="POS_INB" pad="5"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM1458M"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K3508"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM1458N" prefix="U">
<description>OP AMP</description>
<gates>
<gate name="A" symbol="LM1458N"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-8">
<connects>
<connect gate="A" pin="NEG_A" pad="2"/>
<connect gate="A" pin="NEG_B" pad="6"/>
<connect gate="A" pin="OUT_A" pad="1"/>
<connect gate="A" pin="OUT_B" pad="7"/>
<connect gate="A" pin="POS_A" pad="3"/>
<connect gate="A" pin="POS_B" pad="5"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM1458N"/>
<attribute name="OC_FARNELL" value="9486852"/>
<attribute name="OC_NEWARK" value="07B5894"/>
<attribute name="PACKAGE" value="8-DIP"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM148J" prefix="U">
<description>OpAmpIC</description>
<gates>
<gate name="A" symbol="LM148J"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-14">
<connects>
<connect gate="A" pin="+IN1" pad="3"/>
<connect gate="A" pin="+IN2" pad="5"/>
<connect gate="A" pin="+IN3" pad="10"/>
<connect gate="A" pin="+IN4" pad="12"/>
<connect gate="A" pin="-IN1" pad="2"/>
<connect gate="A" pin="-IN2" pad="6"/>
<connect gate="A" pin="-IN3" pad="9"/>
<connect gate="A" pin="-IN4" pad="13"/>
<connect gate="A" pin="OUT1" pad="1"/>
<connect gate="A" pin="OUT2" pad="7"/>
<connect gate="A" pin="OUT3" pad="8"/>
<connect gate="A" pin="OUT4" pad="14"/>
<connect gate="A" pin="V+" pad="4"/>
<connect gate="A" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM148J"/>
<attribute name="OC_FARNELL" value="1416365"/>
<attribute name="OC_NEWARK" value="13B5466"/>
<attribute name="PACKAGE" value="DIP-14"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM1558H" prefix="U">
<description>OP AMP, DUAL COMPENSATED, 1558</description>
<gates>
<gate name="A" symbol="LM1558H"/>
</gates>
<devices>
<device name="" package="TO254P914X470-8P">
<connects>
<connect gate="A" pin="+INA" pad="3"/>
<connect gate="A" pin="+INB" pad="5"/>
<connect gate="A" pin="-INA" pad="2"/>
<connect gate="A" pin="-INB" pad="6"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM1558H"/>
<attribute name="OC_FARNELL" value="1216159"/>
<attribute name="OC_NEWARK" value="31T9818"/>
<attribute name="PACKAGE" value="TO-99-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM158AH" prefix="U">
<description>IC OP AMP DUAL LOW PWR</description>
<gates>
<gate name="A" symbol="LM158AH"/>
</gates>
<devices>
<device name="" package="TO254P914X470-8P">
<connects>
<connect gate="A" pin="+INA" pad="3"/>
<connect gate="A" pin="+INB" pad="5"/>
<connect gate="A" pin="-INA" pad="2"/>
<connect gate="A" pin="-INB" pad="6"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM158AH"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="31T9819"/>
<attribute name="PACKAGE" value="TO-99-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM158H" prefix="U">
<description>IC, OP-AMP, 1MHZ, 0.5V/µS</description>
<gates>
<gate name="A" symbol="LM158H"/>
</gates>
<devices>
<device name="" package="TO254P914X470-8P">
<connects>
<connect gate="A" pin="+INA" pad="3"/>
<connect gate="A" pin="+INB" pad="5"/>
<connect gate="A" pin="-INA" pad="2"/>
<connect gate="A" pin="-INB" pad="6"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM158H"/>
<attribute name="OC_FARNELL" value="1216157"/>
<attribute name="OC_NEWARK" value="01M8133"/>
<attribute name="PACKAGE" value="TO-99-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM158J" prefix="U">
<description>OpAmpIC</description>
<gates>
<gate name="A" symbol="LM158J"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-8">
<connects>
<connect gate="A" pin="NEGA" pad="2"/>
<connect gate="A" pin="NEGB" pad="6"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="POSA" pad="3"/>
<connect gate="A" pin="POSB" pad="5"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM158J"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="14R8491"/>
<attribute name="PACKAGE" value="DIP-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM1770SMF" prefix="U">
<description>Synchronous Buck Controller</description>
<gates>
<gate name="A" symbol="LM1770SMF"/>
</gates>
<devices>
<device name="" package="SOT95P285X120-5N">
<connects>
<connect gate="A" pin="FB" pad="5"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="HG" pad="4"/>
<connect gate="A" pin="LG" pad="3"/>
<connect gate="A" pin="VIN" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM1770SMF"/>
<attribute name="OC_FARNELL" value="1312542"/>
<attribute name="OC_NEWARK" value="-"/>
<attribute name="PACKAGE" value="SOT-5"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM1770TMF" prefix="U">
<description>Synchronous Buck Controller</description>
<gates>
<gate name="A" symbol="LM1770TMF"/>
</gates>
<devices>
<device name="" package="SOT95P285X120-5N">
<connects>
<connect gate="A" pin="FB" pad="5"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="HG" pad="4"/>
<connect gate="A" pin="LG" pad="3"/>
<connect gate="A" pin="VIN" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM1770TMF"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="69K2377"/>
<attribute name="PACKAGE" value="SOT-5"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM1770UMF" prefix="U">
<description>SOT23 Synchronous Buck Controller</description>
<gates>
<gate name="A" symbol="LM1770UMF"/>
</gates>
<devices>
<device name="" package="SOT95P285X120-5N">
<connects>
<connect gate="A" pin="FB" pad="5"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="HG" pad="4"/>
<connect gate="A" pin="LG" pad="3"/>
<connect gate="A" pin="VIN" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM1770UMF"/>
<attribute name="OC_FARNELL" value="1312544"/>
<attribute name="OC_NEWARK" value="31M5338"/>
<attribute name="PACKAGE" value="SOT-23-5"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM1771SMM" prefix="U">
<description>Synchronous Buck Controller</description>
<gates>
<gate name="A" symbol="LM1771SMM"/>
</gates>
<devices>
<device name="" package="SOP65P490X110-8N">
<connects>
<connect gate="A" pin="EN" pad="8"/>
<connect gate="A" pin="FB" pad="1"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="GND_2" pad="2"/>
<connect gate="A" pin="HG" pad="4"/>
<connect gate="A" pin="LG" pad="5"/>
<connect gate="A" pin="VIN" pad="7"/>
<connect gate="A" pin="VIN_2" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM1771SMM"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="32M0971"/>
<attribute name="PACKAGE" value="MSOP-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM1771SSD" prefix="U">
<description>Synchronous Buck Controller</description>
<gates>
<gate name="A" symbol="LM1771SSD"/>
</gates>
<devices>
<device name="" package="DFN300X300X80-7N">
<connects>
<connect gate="A" pin="EN" pad="6"/>
<connect gate="A" pin="EPAD" pad="7"/>
<connect gate="A" pin="FB" pad="1"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="HG" pad="3"/>
<connect gate="A" pin="LG" pad="4"/>
<connect gate="A" pin="VIN" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM1771SSD"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="13M1691"/>
<attribute name="PACKAGE" value="DFN-6"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM1771TMM" prefix="U">
<description>Synchronous Buck Controller</description>
<gates>
<gate name="A" symbol="LM1771TMM"/>
</gates>
<devices>
<device name="" package="SOP65P490X109-8N">
<connects>
<connect gate="A" pin="EN" pad="8"/>
<connect gate="A" pin="FB" pad="1"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="GND_2" pad="2"/>
<connect gate="A" pin="HG" pad="4"/>
<connect gate="A" pin="LG" pad="5"/>
<connect gate="A" pin="VIN" pad="7"/>
<connect gate="A" pin="VIN_2" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM1771TMM"/>
<attribute name="OC_FARNELL" value="1313867"/>
<attribute name="OC_NEWARK" value="31M5341"/>
<attribute name="PACKAGE" value="SOP-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM1771UMM" prefix="U">
<description>Synchronous Buck Controller</description>
<gates>
<gate name="A" symbol="LM1771UMM"/>
</gates>
<devices>
<device name="" package="SOP65P490X110X8N">
<connects>
<connect gate="A" pin="EN" pad="8"/>
<connect gate="A" pin="FB" pad="1"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="GND_2" pad="2"/>
<connect gate="A" pin="HG" pad="4"/>
<connect gate="A" pin="LG" pad="5"/>
<connect gate="A" pin="VIN" pad="7"/>
<connect gate="A" pin="VIN_2" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM1771UMM"/>
<attribute name="OC_FARNELL" value="1313868"/>
<attribute name="OC_NEWARK" value="32M0975"/>
<attribute name="PACKAGE" value="MSOP-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM193AH" prefix="U">
<description>IC COMP DUAL LOW PWR OFF</description>
<gates>
<gate name="A" symbol="LM193AH"/>
</gates>
<devices>
<device name="" package="TO254P914X470-8P">
<connects>
<connect gate="A" pin="+INA" pad="3"/>
<connect gate="A" pin="+INB" pad="5"/>
<connect gate="A" pin="-INA" pad="2"/>
<connect gate="A" pin="-INB" pad="6"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM193AH"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="31T9839"/>
<attribute name="PACKAGE" value="TO-99-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM193AJ-QMLV" prefix="U">
<description>OpAmpIC</description>
<gates>
<gate name="A" symbol="LM193AJ-QMLV"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-8">
<connects>
<connect gate="A" pin="NEGA" pad="2"/>
<connect gate="A" pin="NEGB" pad="6"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="POSA" pad="3"/>
<connect gate="A" pin="POSB" pad="5"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM193AJ-QMLV"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="31T9842"/>
<attribute name="PACKAGE" value="DIP-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM193H" prefix="U">
<description>IC COMP DUAL LOW PWR OFF</description>
<gates>
<gate name="A" symbol="LM193H"/>
</gates>
<devices>
<device name="" package="TO254P914X470-8P">
<connects>
<connect gate="A" pin="+INA" pad="3"/>
<connect gate="A" pin="+INB" pad="5"/>
<connect gate="A" pin="-INA" pad="2"/>
<connect gate="A" pin="-INB" pad="6"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM193H"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="31T9845"/>
<attribute name="PACKAGE" value="TO-99-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM19CIZ" prefix="U">
<description>IC, TEMPERATURE SENSOR, ± 2.5°C</description>
<gates>
<gate name="A" symbol="LM19CIZ"/>
</gates>
<devices>
<device name="" package="TO127P254X495-3P">
<connects>
<connect gate="A" pin="+VS" pad="1"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="VOUT" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM19CIZ"/>
<attribute name="OC_FARNELL" value="9489649"/>
<attribute name="OC_NEWARK" value="41K3539"/>
<attribute name="PACKAGE" value="TO-92"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM20123MH" prefix="U">
<description>Synchronous Buck Regulator</description>
<gates>
<gate name="A" symbol="LM20123MH"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-17N">
<connects>
<connect gate="A" pin="AGND" pad="15"/>
<connect gate="A" pin="AVIN" pad="14"/>
<connect gate="A" pin="COMP" pad="4"/>
<connect gate="A" pin="EN" pad="12"/>
<connect gate="A" pin="EPAD" pad="17"/>
<connect gate="A" pin="FB" pad="2"/>
<connect gate="A" pin="NC" pad="16"/>
<connect gate="A" pin="NC_2" pad="5"/>
<connect gate="A" pin="PGND" pad="11"/>
<connect gate="A" pin="PGND_2" pad="10"/>
<connect gate="A" pin="PGOOD" pad="3"/>
<connect gate="A" pin="PVIN" pad="7"/>
<connect gate="A" pin="PVIN_2" pad="6"/>
<connect gate="A" pin="SS/TRK" pad="1"/>
<connect gate="A" pin="SW" pad="9"/>
<connect gate="A" pin="SW_2" pad="8"/>
<connect gate="A" pin="VCC" pad="13"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM20123MH"/>
<attribute name="OC_FARNELL" value="1506824"/>
<attribute name="OC_NEWARK" value="60M3434"/>
<attribute name="PACKAGE" value="TSSOP-14"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM20124MH" prefix="U">
<description>Synchronous Buck Regulator</description>
<gates>
<gate name="A" symbol="LM20124MH"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-17N">
<connects>
<connect gate="A" pin="AGND" pad="15"/>
<connect gate="A" pin="AVIN" pad="14"/>
<connect gate="A" pin="COMP" pad="4"/>
<connect gate="A" pin="EN" pad="12"/>
<connect gate="A" pin="EPAD" pad="17"/>
<connect gate="A" pin="FB" pad="2"/>
<connect gate="A" pin="NC" pad="16"/>
<connect gate="A" pin="NC_2" pad="5"/>
<connect gate="A" pin="PGND" pad="11"/>
<connect gate="A" pin="PGND_2" pad="10"/>
<connect gate="A" pin="PGOOD" pad="3"/>
<connect gate="A" pin="PVIN" pad="7"/>
<connect gate="A" pin="PVIN_2" pad="6"/>
<connect gate="A" pin="SS/TRK" pad="1"/>
<connect gate="A" pin="SW" pad="9"/>
<connect gate="A" pin="SW_2" pad="8"/>
<connect gate="A" pin="VCC" pad="13"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM20124MH"/>
<attribute name="OC_FARNELL" value="1506826"/>
<attribute name="OC_NEWARK" value="54M4639"/>
<attribute name="PACKAGE" value="TSSOP-14"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM20125MH" prefix="U">
<description>Synchronous Buck Regulator</description>
<gates>
<gate name="A" symbol="LM20125MH"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-17N">
<connects>
<connect gate="A" pin="AGND" pad="15"/>
<connect gate="A" pin="AVIN" pad="14"/>
<connect gate="A" pin="COMP" pad="4"/>
<connect gate="A" pin="EN" pad="12"/>
<connect gate="A" pin="EPAD" pad="17"/>
<connect gate="A" pin="FB" pad="2"/>
<connect gate="A" pin="NC" pad="16"/>
<connect gate="A" pin="NC_2" pad="5"/>
<connect gate="A" pin="PGND" pad="11"/>
<connect gate="A" pin="PGND_2" pad="10"/>
<connect gate="A" pin="PGOOD" pad="3"/>
<connect gate="A" pin="PVIN" pad="7"/>
<connect gate="A" pin="PVIN_2" pad="6"/>
<connect gate="A" pin="SS/TRK" pad="1"/>
<connect gate="A" pin="SW" pad="9"/>
<connect gate="A" pin="SW_2" pad="8"/>
<connect gate="A" pin="VCC" pad="13"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM20125MH"/>
<attribute name="OC_FARNELL" value="1506829"/>
<attribute name="OC_NEWARK" value="54M4641"/>
<attribute name="PACKAGE" value="TSSOP-14"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM20133MH" prefix="U">
<description>Synchronous Buck Regulator</description>
<gates>
<gate name="A" symbol="LM20133MH"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-17N">
<connects>
<connect gate="A" pin="AGND" pad="15"/>
<connect gate="A" pin="AVIN" pad="14"/>
<connect gate="A" pin="COMP" pad="4"/>
<connect gate="A" pin="EN" pad="12"/>
<connect gate="A" pin="EPAD" pad="17"/>
<connect gate="A" pin="FB" pad="2"/>
<connect gate="A" pin="NC" pad="16"/>
<connect gate="A" pin="NC_2" pad="5"/>
<connect gate="A" pin="PGND" pad="11"/>
<connect gate="A" pin="PGND_2" pad="10"/>
<connect gate="A" pin="PGOOD" pad="3"/>
<connect gate="A" pin="PVIN" pad="7"/>
<connect gate="A" pin="PVIN_2" pad="6"/>
<connect gate="A" pin="SS/TRK" pad="1"/>
<connect gate="A" pin="SW" pad="9"/>
<connect gate="A" pin="SW_2" pad="8"/>
<connect gate="A" pin="VCC" pad="13"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM20133MH"/>
<attribute name="OC_FARNELL" value="1495075"/>
<attribute name="OC_NEWARK" value="60M3435"/>
<attribute name="PACKAGE" value="TSSOP-14"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM20134MH" prefix="U">
<description>Synchronous Buck Regulator</description>
<gates>
<gate name="A" symbol="LM20134MH"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-17N">
<connects>
<connect gate="A" pin="AGND" pad="15"/>
<connect gate="A" pin="AVIN" pad="14"/>
<connect gate="A" pin="COMP" pad="4"/>
<connect gate="A" pin="EN" pad="12"/>
<connect gate="A" pin="EPAD" pad="17"/>
<connect gate="A" pin="FB" pad="2"/>
<connect gate="A" pin="NC" pad="16"/>
<connect gate="A" pin="NC_2" pad="5"/>
<connect gate="A" pin="PGND" pad="11"/>
<connect gate="A" pin="PGND_2" pad="10"/>
<connect gate="A" pin="PGOOD" pad="3"/>
<connect gate="A" pin="PVIN" pad="7"/>
<connect gate="A" pin="PVIN_2" pad="6"/>
<connect gate="A" pin="SS/TRK" pad="1"/>
<connect gate="A" pin="SW" pad="9"/>
<connect gate="A" pin="SW_2" pad="8"/>
<connect gate="A" pin="VCC" pad="13"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM20134MH"/>
<attribute name="OC_FARNELL" value="1506827"/>
<attribute name="OC_NEWARK" value="60M3436"/>
<attribute name="PACKAGE" value="TSSOP-14"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM20136MH" prefix="U">
<description>Synchronous Buck Regulator</description>
<gates>
<gate name="A" symbol="LM20136MH"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-17N">
<connects>
<connect gate="A" pin="AGND" pad="15"/>
<connect gate="A" pin="AVIN" pad="14"/>
<connect gate="A" pin="COMP" pad="4"/>
<connect gate="A" pin="EN" pad="12"/>
<connect gate="A" pin="EP" pad="17"/>
<connect gate="A" pin="FB" pad="2"/>
<connect gate="A" pin="NC" pad="5"/>
<connect gate="A" pin="PGND" pad="11"/>
<connect gate="A" pin="PGND_2" pad="10"/>
<connect gate="A" pin="PGOOD" pad="3"/>
<connect gate="A" pin="PVIN" pad="7"/>
<connect gate="A" pin="PVIN_2" pad="6"/>
<connect gate="A" pin="SS/TRK" pad="1"/>
<connect gate="A" pin="SW" pad="9"/>
<connect gate="A" pin="SW_2" pad="8"/>
<connect gate="A" pin="SYNC" pad="16"/>
<connect gate="A" pin="VCC" pad="13"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM20136MH"/>
<attribute name="OC_FARNELL" value="1699375"/>
<attribute name="OC_NEWARK" value="80P4531"/>
<attribute name="PACKAGE" value="SOP-16"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM20143MH" prefix="U">
<description>Synchronous Buck Regulator</description>
<gates>
<gate name="A" symbol="LM20143MH"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-17N">
<connects>
<connect gate="A" pin="AGND" pad="15"/>
<connect gate="A" pin="AVIN" pad="14"/>
<connect gate="A" pin="COMP" pad="4"/>
<connect gate="A" pin="EN" pad="12"/>
<connect gate="A" pin="EPAD" pad="17"/>
<connect gate="A" pin="FB" pad="2"/>
<connect gate="A" pin="NC" pad="5"/>
<connect gate="A" pin="PGND" pad="11"/>
<connect gate="A" pin="PGND_2" pad="10"/>
<connect gate="A" pin="PGOOD" pad="3"/>
<connect gate="A" pin="PVIN" pad="7"/>
<connect gate="A" pin="PVIN_2" pad="6"/>
<connect gate="A" pin="RT" pad="16"/>
<connect gate="A" pin="SS/TRK" pad="1"/>
<connect gate="A" pin="SW" pad="8"/>
<connect gate="A" pin="SW_2" pad="9"/>
<connect gate="A" pin="VCC" pad="13"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM20143MH"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="60M3437"/>
<attribute name="PACKAGE" value="TSSOP-16"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM20144MH" prefix="U">
<description>Synchronous Buck Regulator</description>
<gates>
<gate name="A" symbol="LM20144MH"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-17N">
<connects>
<connect gate="A" pin="AGND" pad="15"/>
<connect gate="A" pin="AVIN" pad="14"/>
<connect gate="A" pin="COMP" pad="4"/>
<connect gate="A" pin="EN" pad="12"/>
<connect gate="A" pin="EPAD" pad="17"/>
<connect gate="A" pin="FB" pad="2"/>
<connect gate="A" pin="NC" pad="5"/>
<connect gate="A" pin="PGND" pad="11"/>
<connect gate="A" pin="PGND_2" pad="10"/>
<connect gate="A" pin="PGOOD" pad="3"/>
<connect gate="A" pin="PVIN" pad="7"/>
<connect gate="A" pin="PVIN_2" pad="6"/>
<connect gate="A" pin="RT" pad="16"/>
<connect gate="A" pin="SS/TRK" pad="1"/>
<connect gate="A" pin="SW" pad="8"/>
<connect gate="A" pin="SW_2" pad="9"/>
<connect gate="A" pin="VCC" pad="13"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM20144MH"/>
<attribute name="OC_FARNELL" value="1495076"/>
<attribute name="OC_NEWARK" value="60M3438"/>
<attribute name="PACKAGE" value="TSSOP-16"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM20145MH" prefix="U">
<description>Synchronous Buck Regulator</description>
<gates>
<gate name="A" symbol="LM20145MH"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-17N">
<connects>
<connect gate="A" pin="AGND" pad="15"/>
<connect gate="A" pin="AVIN" pad="14"/>
<connect gate="A" pin="COMP" pad="4"/>
<connect gate="A" pin="EN" pad="12"/>
<connect gate="A" pin="EPAD" pad="17"/>
<connect gate="A" pin="FB" pad="2"/>
<connect gate="A" pin="NC" pad="5"/>
<connect gate="A" pin="PGND" pad="11"/>
<connect gate="A" pin="PGND_2" pad="10"/>
<connect gate="A" pin="PGOOD" pad="3"/>
<connect gate="A" pin="PVIN" pad="7"/>
<connect gate="A" pin="PVIN_2" pad="6"/>
<connect gate="A" pin="RT" pad="16"/>
<connect gate="A" pin="SS/TRK" pad="1"/>
<connect gate="A" pin="SW" pad="8"/>
<connect gate="A" pin="SW_2" pad="9"/>
<connect gate="A" pin="VCC" pad="13"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM20145MH"/>
<attribute name="OC_FARNELL" value="1495077"/>
<attribute name="OC_NEWARK" value="60M3439"/>
<attribute name="PACKAGE" value="TSSOP-16"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM20146MH" prefix="U">
<description>Synchronous Buck Regulator</description>
<gates>
<gate name="A" symbol="LM20146MH"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-17N">
<connects>
<connect gate="A" pin="AGND" pad="15"/>
<connect gate="A" pin="AVIN" pad="14"/>
<connect gate="A" pin="COMP" pad="4"/>
<connect gate="A" pin="EN" pad="12"/>
<connect gate="A" pin="EP" pad="17"/>
<connect gate="A" pin="FB" pad="2"/>
<connect gate="A" pin="NC" pad="5"/>
<connect gate="A" pin="PGND" pad="11"/>
<connect gate="A" pin="PGND_2" pad="10"/>
<connect gate="A" pin="PGOOD" pad="3"/>
<connect gate="A" pin="PVIN" pad="7"/>
<connect gate="A" pin="PVIN_2" pad="6"/>
<connect gate="A" pin="RT" pad="16"/>
<connect gate="A" pin="SS/TRK" pad="1"/>
<connect gate="A" pin="SW" pad="9"/>
<connect gate="A" pin="SW_2" pad="8"/>
<connect gate="A" pin="VCC" pad="13"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM20146MH"/>
<attribute name="OC_FARNELL" value="1699376"/>
<attribute name="OC_NEWARK" value="80P4532"/>
<attribute name="PACKAGE" value="SOP-16"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM20154MH" prefix="U">
<description>Synchronous Buck Controller</description>
<gates>
<gate name="A" symbol="LM20154MH"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-17N">
<connects>
<connect gate="A" pin="AGND" pad="15"/>
<connect gate="A" pin="AVIN" pad="14"/>
<connect gate="A" pin="COMP" pad="4"/>
<connect gate="A" pin="EN" pad="12"/>
<connect gate="A" pin="EPAD" pad="17"/>
<connect gate="A" pin="FB" pad="2"/>
<connect gate="A" pin="NC" pad="5"/>
<connect gate="A" pin="PGND" pad="11"/>
<connect gate="A" pin="PGND_2" pad="10"/>
<connect gate="A" pin="PGOOD" pad="3"/>
<connect gate="A" pin="PVIN" pad="7"/>
<connect gate="A" pin="PVIN_2" pad="6"/>
<connect gate="A" pin="SS/TRK" pad="1"/>
<connect gate="A" pin="SW" pad="8"/>
<connect gate="A" pin="SW_2" pad="9"/>
<connect gate="A" pin="SYNCOUT" pad="16"/>
<connect gate="A" pin="VCC" pad="13"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM20154MH"/>
<attribute name="OC_FARNELL" value="1506828"/>
<attribute name="OC_NEWARK" value="60M3440"/>
<attribute name="PACKAGE" value="TSSOP-16"/>
<attribute name="SUPPLIER" value="National semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM20242MH" prefix="U">
<description>Adjustable Frequency Synchronous Buck Regulator</description>
<gates>
<gate name="A" symbol="LM20242MH"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-21N">
<connects>
<connect gate="A" pin="AGND" pad="12"/>
<connect gate="A" pin="BOOT" pad="17"/>
<connect gate="A" pin="COMP" pad="4"/>
<connect gate="A" pin="EN" pad="19"/>
<connect gate="A" pin="EPAD" pad="21"/>
<connect gate="A" pin="FB" pad="2"/>
<connect gate="A" pin="GND" pad="11"/>
<connect gate="A" pin="GND_2" pad="9"/>
<connect gate="A" pin="GND_3" pad="10"/>
<connect gate="A" pin="PGOOD" pad="3"/>
<connect gate="A" pin="RT" pad="20"/>
<connect gate="A" pin="SS/TRK" pad="1"/>
<connect gate="A" pin="SW" pad="14"/>
<connect gate="A" pin="SW_2" pad="7"/>
<connect gate="A" pin="SW_3" pad="8"/>
<connect gate="A" pin="SW_4" pad="13"/>
<connect gate="A" pin="VCC" pad="18"/>
<connect gate="A" pin="VIN" pad="16"/>
<connect gate="A" pin="VIN_2" pad="5"/>
<connect gate="A" pin="VIN_3" pad="6"/>
<connect gate="A" pin="VIN_4" pad="15"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM20242MH"/>
<attribute name="OC_FARNELL" value="1495078"/>
<attribute name="OC_NEWARK" value="54M4643"/>
<attribute name="PACKAGE" value="TSSOP-20"/>
<attribute name="SUPPLIER" value="National semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM20323MH" prefix="U">
<description>Synchronous Buck Controller</description>
<gates>
<gate name="A" symbol="LM20323MH"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-21N">
<connects>
<connect gate="A" pin="AGND" pad="12"/>
<connect gate="A" pin="BOOT" pad="17"/>
<connect gate="A" pin="COMP" pad="4"/>
<connect gate="A" pin="EN" pad="19"/>
<connect gate="A" pin="EPAD" pad="21"/>
<connect gate="A" pin="FB" pad="2"/>
<connect gate="A" pin="GND" pad="11"/>
<connect gate="A" pin="GND_2" pad="9"/>
<connect gate="A" pin="GND_3" pad="10"/>
<connect gate="A" pin="NC" pad="20"/>
<connect gate="A" pin="PGOOD" pad="3"/>
<connect gate="A" pin="SS/TRK" pad="1"/>
<connect gate="A" pin="SW" pad="14"/>
<connect gate="A" pin="SW_2" pad="7"/>
<connect gate="A" pin="SW_3" pad="8"/>
<connect gate="A" pin="SW_4" pad="13"/>
<connect gate="A" pin="VCC" pad="18"/>
<connect gate="A" pin="VIN" pad="16"/>
<connect gate="A" pin="VIN_2" pad="5"/>
<connect gate="A" pin="VIN_3" pad="6"/>
<connect gate="A" pin="VIN_4" pad="15"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM20323MH"/>
<attribute name="OC_FARNELL" value="1663035"/>
<attribute name="OC_NEWARK" value="15P1962"/>
<attribute name="PACKAGE" value="TSSOP-20"/>
<attribute name="SUPPLIER" value="National semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM20333MH" prefix="U">
<description>Synchronous Buck Controller</description>
<gates>
<gate name="A" symbol="LM20333MH"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-21N">
<connects>
<connect gate="A" pin="AGND" pad="12"/>
<connect gate="A" pin="BOOT" pad="17"/>
<connect gate="A" pin="COMP" pad="4"/>
<connect gate="A" pin="EN" pad="19"/>
<connect gate="A" pin="EPAD" pad="21"/>
<connect gate="A" pin="FB" pad="2"/>
<connect gate="A" pin="GND" pad="11"/>
<connect gate="A" pin="GND_2" pad="9"/>
<connect gate="A" pin="GND_3" pad="10"/>
<connect gate="A" pin="PGOOD" pad="3"/>
<connect gate="A" pin="SS/TRK" pad="1"/>
<connect gate="A" pin="SW" pad="14"/>
<connect gate="A" pin="SW_2" pad="7"/>
<connect gate="A" pin="SW_3" pad="8"/>
<connect gate="A" pin="SW_4" pad="13"/>
<connect gate="A" pin="SYNC" pad="20"/>
<connect gate="A" pin="VCC" pad="18"/>
<connect gate="A" pin="VIN" pad="16"/>
<connect gate="A" pin="VIN_2" pad="5"/>
<connect gate="A" pin="VIN_3" pad="6"/>
<connect gate="A" pin="VIN_4" pad="15"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM20333MH"/>
<attribute name="OC_FARNELL" value="1663037"/>
<attribute name="OC_NEWARK" value="11N9183"/>
<attribute name="PACKAGE" value="TSSOP-20"/>
<attribute name="SUPPLIER" value="National semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM20343MH" prefix="U">
<description>Adjustable Frequency Synchronous Buck Regulator</description>
<gates>
<gate name="A" symbol="LM20343MH"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-21N">
<connects>
<connect gate="A" pin="AGND" pad="12"/>
<connect gate="A" pin="BOOT" pad="17"/>
<connect gate="A" pin="COMP" pad="4"/>
<connect gate="A" pin="EN" pad="19"/>
<connect gate="A" pin="EPAD" pad="21"/>
<connect gate="A" pin="FB" pad="2"/>
<connect gate="A" pin="GND" pad="11"/>
<connect gate="A" pin="GND_2" pad="9"/>
<connect gate="A" pin="GND_3" pad="10"/>
<connect gate="A" pin="PGOOD" pad="3"/>
<connect gate="A" pin="RT" pad="20"/>
<connect gate="A" pin="SS/TRK" pad="1"/>
<connect gate="A" pin="SW" pad="14"/>
<connect gate="A" pin="SW_2" pad="7"/>
<connect gate="A" pin="SW_3" pad="8"/>
<connect gate="A" pin="SW_4" pad="13"/>
<connect gate="A" pin="VCC" pad="18"/>
<connect gate="A" pin="VIN" pad="16"/>
<connect gate="A" pin="VIN_2" pad="5"/>
<connect gate="A" pin="VIN_3" pad="6"/>
<connect gate="A" pin="VIN_4" pad="15"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM20343MH"/>
<attribute name="OC_FARNELL" value="1663009"/>
<attribute name="OC_NEWARK" value="11N9187"/>
<attribute name="PACKAGE" value="TSSOP-20"/>
<attribute name="SUPPLIER" value="National semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM20BIM7" prefix="U">
<description>micro SMD Temperature Sensor</description>
<gates>
<gate name="A" symbol="LM20BIM7"/>
</gates>
<devices>
<device name="" package="SOT65P240X110-5N">
<connects>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="GND_2" pad="5"/>
<connect gate="A" pin="NC" pad="1"/>
<connect gate="A" pin="V+" pad="4"/>
<connect gate="A" pin="VO" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM20BIM7"/>
<attribute name="OC_FARNELL" value="9779264"/>
<attribute name="OC_NEWARK" value="25C3870"/>
<attribute name="PACKAGE" value="SC-70-5"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM20CIM7" prefix="U">
<description>TempSensors</description>
<gates>
<gate name="A" symbol="LM20CIM7"/>
</gates>
<devices>
<device name="" package="SOT65P210X110-5N">
<connects>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="GND_2" pad="2"/>
<connect gate="A" pin="NC" pad="1"/>
<connect gate="A" pin="V+" pad="4"/>
<connect gate="A" pin="VO" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM20CIM7"/>
<attribute name="OC_FARNELL" value="1472349"/>
<attribute name="OC_NEWARK" value="41K3552"/>
<attribute name="PACKAGE" value="SC70-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM224J" prefix="U">
<description>Low Power Quad Operational Amplifiers</description>
<gates>
<gate name="A" symbol="LM224J"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-14">
<connects>
<connect gate="A" pin="+IN1" pad="3"/>
<connect gate="A" pin="+IN2" pad="5"/>
<connect gate="A" pin="+IN3" pad="10"/>
<connect gate="A" pin="+IN4" pad="13"/>
<connect gate="A" pin="+IN4_2" pad="12"/>
<connect gate="A" pin="-IN1" pad="2"/>
<connect gate="A" pin="-IN2" pad="6"/>
<connect gate="A" pin="-IN3" pad="9"/>
<connect gate="A" pin="GND" pad="11"/>
<connect gate="A" pin="OUT1" pad="1"/>
<connect gate="A" pin="OUT2" pad="7"/>
<connect gate="A" pin="OUT3" pad="8"/>
<connect gate="A" pin="OUT4" pad="14"/>
<connect gate="A" pin="V+" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM224J"/>
<attribute name="OC_FARNELL" value="400105"/>
<attribute name="OC_NEWARK" value="13B5528"/>
<attribute name="PACKAGE" value="14-CDIP"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM22670MR-5.0" prefix="U">
<description>SIMPLE SWITCHER</description>
<gates>
<gate name="A" symbol="LM22670MR-5.0"/>
</gates>
<devices>
<device name="" package="SOIC127P620X168-9N">
<connects>
<connect gate="A" pin="BOOT" pad="1"/>
<connect gate="A" pin="EN" pad="5"/>
<connect gate="A" pin="EPAD" pad="9"/>
<connect gate="A" pin="FB" pad="4"/>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="NC" pad="2"/>
<connect gate="A" pin="RT/SYNC" pad="3"/>
<connect gate="A" pin="SW" pad="8"/>
<connect gate="A" pin="VIN" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM22670MR-5.0"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="34P4759"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="National semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM22670MR-ADJ" prefix="U">
<description>Step-Down Voltage Regulator</description>
<gates>
<gate name="A" symbol="LM22670MR-ADJ"/>
</gates>
<devices>
<device name="" package="SOIC127P600X168-9N">
<connects>
<connect gate="A" pin="BOOT" pad="1"/>
<connect gate="A" pin="EN" pad="5"/>
<connect gate="A" pin="EPAD" pad="9"/>
<connect gate="A" pin="FB" pad="4"/>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="NC" pad="2"/>
<connect gate="A" pin="RT/SYNC" pad="3"/>
<connect gate="A" pin="SW" pad="8"/>
<connect gate="A" pin="VIN" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM22670MR-ADJ"/>
<attribute name="OC_FARNELL" value="1657735"/>
<attribute name="OC_NEWARK" value="34P4758"/>
<attribute name="PACKAGE" value="SOIC-9"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM22670TJ-5.0" prefix="U">
<description>SIMPLE SWITCHER</description>
<gates>
<gate name="A" symbol="LM22670TJ-5.0"/>
</gates>
<devices>
<device name="" package="TO127P1435X210-7N">
<connects>
<connect gate="A" pin="BOOT" pad="3"/>
<connect gate="A" pin="EN" pad="7"/>
<connect gate="A" pin="EPAD" pad="8"/>
<connect gate="A" pin="FB" pad="6"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="RT/SYNC" pad="5"/>
<connect gate="A" pin="SW" pad="1"/>
<connect gate="A" pin="VIN" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM22670TJ-5.0"/>
<attribute name="OC_FARNELL" value=""/>
<attribute name="OC_NEWARK" value="34P4763"/>
<attribute name="PACKAGE" value="TO-263-7"/>
<attribute name="SUPPLIER" value="National semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM22670TJ-ADJ" prefix="U">
<description>SIMPLE SWITCHER</description>
<gates>
<gate name="A" symbol="LM22670TJ-ADJ"/>
</gates>
<devices>
<device name="" package="TO127P1435X210-7N">
<connects>
<connect gate="A" pin="BOOT" pad="3"/>
<connect gate="A" pin="EN" pad="7"/>
<connect gate="A" pin="EPAD" pad="8"/>
<connect gate="A" pin="FB" pad="6"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="RT/SYNC" pad="5"/>
<connect gate="A" pin="SW" pad="1"/>
<connect gate="A" pin="VIN" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM22670TJ-ADJ"/>
<attribute name="OC_FARNELL" value=""/>
<attribute name="OC_NEWARK" value="34P4762"/>
<attribute name="PACKAGE" value="TO-263-7"/>
<attribute name="SUPPLIER" value="National semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM22671MR-ADJ" prefix="U">
<description>SIMPLE SWITCHER</description>
<gates>
<gate name="A" symbol="LM22671MR-ADJ"/>
</gates>
<devices>
<device name="" package="SOIC127P620X168-9N">
<connects>
<connect gate="A" pin="BOOT" pad="1"/>
<connect gate="A" pin="EN" pad="5"/>
<connect gate="A" pin="EPAD" pad="9"/>
<connect gate="A" pin="FB" pad="4"/>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="RT/SYNC" pad="3"/>
<connect gate="A" pin="SS" pad="2"/>
<connect gate="A" pin="SW" pad="8"/>
<connect gate="A" pin="VIN" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM22671MR-ADJ"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="34P4764"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="National semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM22672MR-ADJ" prefix="U">
<description>SIMPLE SWITCHER</description>
<gates>
<gate name="A" symbol="LM22672MR-ADJ"/>
</gates>
<devices>
<device name="" package="SOIC127P620X168-9N">
<connects>
<connect gate="A" pin="BOOT" pad="1"/>
<connect gate="A" pin="EN" pad="5"/>
<connect gate="A" pin="EPAD" pad="9"/>
<connect gate="A" pin="FB" pad="4"/>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="RT/SYNC" pad="3"/>
<connect gate="A" pin="SS" pad="2"/>
<connect gate="A" pin="SW" pad="8"/>
<connect gate="A" pin="VIN" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM22672MR-ADJ"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="34P4768"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="National semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM22673MR-ADJ" prefix="U">
<description>Step-Down Voltage Regulator</description>
<gates>
<gate name="A" symbol="LM22673MR-ADJ"/>
</gates>
<devices>
<device name="" package="SOIC127P600X168-9N">
<connects>
<connect gate="A" pin="BOOT" pad="1"/>
<connect gate="A" pin="EPAD" pad="9"/>
<connect gate="A" pin="FB" pad="4"/>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="IADJ" pad="3"/>
<connect gate="A" pin="NC" pad="2"/>
<connect gate="A" pin="SS" pad="5"/>
<connect gate="A" pin="SW" pad="8"/>
<connect gate="A" pin="VIN" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM22673MR-ADJ"/>
<attribute name="OC_FARNELL" value="1657736"/>
<attribute name="OC_NEWARK" value="12P7511"/>
<attribute name="PACKAGE" value="SOIC-9"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM22673TJ-ADJ" prefix="U">
<description>SIMPLE SWITCHER</description>
<gates>
<gate name="A" symbol="LM22673TJ-ADJ"/>
</gates>
<devices>
<device name="" package="TO127P1435X210-7N">
<connects>
<connect gate="A" pin="BOOT" pad="3"/>
<connect gate="A" pin="EPAD" pad="8"/>
<connect gate="A" pin="FB" pad="6"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="IADJ" pad="5"/>
<connect gate="A" pin="SS" pad="7"/>
<connect gate="A" pin="SW" pad="1"/>
<connect gate="A" pin="VIN" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM22673TJ-ADJ"/>
<attribute name="OC_FARNELL" value=""/>
<attribute name="OC_NEWARK" value="34P4776"/>
<attribute name="PACKAGE" value="TO-263-7"/>
<attribute name="SUPPLIER" value="National semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM22674MR-ADJ" prefix="U">
<description>Step-Down Voltage Regulator</description>
<gates>
<gate name="A" symbol="LM22674MR-ADJ"/>
</gates>
<devices>
<device name="" package="SOIC127P600X168-9N">
<connects>
<connect gate="A" pin="BOOT" pad="1"/>
<connect gate="A" pin="EN" pad="5"/>
<connect gate="A" pin="EPAD" pad="9"/>
<connect gate="A" pin="FB" pad="4"/>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="NC" pad="3"/>
<connect gate="A" pin="NC_2" pad="2"/>
<connect gate="A" pin="SW" pad="8"/>
<connect gate="A" pin="VIN" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM22674MR-ADJ"/>
<attribute name="OC_FARNELL" value="1657737"/>
<attribute name="OC_NEWARK" value="12P7512"/>
<attribute name="PACKAGE" value="SOIC-9"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM22675MR-ADJ" prefix="U">
<description>Step-Down Voltage Regulator</description>
<gates>
<gate name="A" symbol="LM22675MR-ADJ"/>
</gates>
<devices>
<device name="" package="SOIC127P600X168-9N">
<connects>
<connect gate="A" pin="BOOT" pad="1"/>
<connect gate="A" pin="EN" pad="5"/>
<connect gate="A" pin="EPAD" pad="9"/>
<connect gate="A" pin="FB" pad="4"/>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="NC" pad="3"/>
<connect gate="A" pin="NC_2" pad="2"/>
<connect gate="A" pin="SW" pad="8"/>
<connect gate="A" pin="VIN" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM22675MR-ADJ"/>
<attribute name="OC_FARNELL" value="1657738"/>
<attribute name="OC_NEWARK" value="12P7513"/>
<attribute name="PACKAGE" value="SOIC-9"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM22676MR-ADJ" prefix="U">
<description>Step-Down Voltage Regulator</description>
<gates>
<gate name="A" symbol="LM22676MR-ADJ"/>
</gates>
<devices>
<device name="" package="SOIC127P600X168-9N">
<connects>
<connect gate="A" pin="BOOT" pad="1"/>
<connect gate="A" pin="EN" pad="5"/>
<connect gate="A" pin="EPAD" pad="9"/>
<connect gate="A" pin="FB" pad="4"/>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="NC" pad="3"/>
<connect gate="A" pin="NC_2" pad="2"/>
<connect gate="A" pin="SW" pad="8"/>
<connect gate="A" pin="VIN" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM22676MR-ADJ"/>
<attribute name="OC_FARNELL" value="1657734"/>
<attribute name="OC_NEWARK" value="12P7514"/>
<attribute name="PACKAGE" value="SOIC-9"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM22676TJ-ADJ" prefix="U">
<description>3A SIMPLE SWITCHER®, Step-Down Voltage Regulator</description>
<gates>
<gate name="A" symbol="LM22676TJ-ADJ"/>
</gates>
<devices>
<device name="" package="TO127P1435X210-8N">
<connects>
<connect gate="A" pin="BOOT" pad="3"/>
<connect gate="A" pin="EN" pad="7"/>
<connect gate="A" pin="EPAD" pad="8"/>
<connect gate="A" pin="FB" pad="6"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="NC" pad="5"/>
<connect gate="A" pin="SW" pad="1"/>
<connect gate="A" pin="VIN" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM22676TJ-ADJ"/>
<attribute name="OC_FARNELL" value="1657733"/>
<attribute name="OC_NEWARK" value="34P4790"/>
<attribute name="PACKAGE" value="TO-263-7"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM22677TJ-ADJ" prefix="U">
<description>3A SIMPLE SWITCHER®, Step-Down Voltage Regulator</description>
<gates>
<gate name="A" symbol="LM22677TJ-ADJ"/>
</gates>
<devices>
<device name="" package="TO127P1435X210-8N">
<connects>
<connect gate="A" pin="BOOT" pad="3"/>
<connect gate="A" pin="EN" pad="7"/>
<connect gate="A" pin="EPAD" pad="8"/>
<connect gate="A" pin="FB" pad="6"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="RT/SYNC" pad="5"/>
<connect gate="A" pin="SW" pad="1"/>
<connect gate="A" pin="VIN" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM22677TJ-ADJ"/>
<attribute name="OC_FARNELL" value="1657730"/>
<attribute name="OC_NEWARK" value="12P7516"/>
<attribute name="PACKAGE" value="TO-263-7"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM22678TJ-ADJ" prefix="U">
<description>3A SIMPLE SWITCHER®, Step-Down Voltage Regulator</description>
<gates>
<gate name="A" symbol="LM22678TJ-ADJ"/>
</gates>
<devices>
<device name="" package="TO127P1435X210-8N">
<connects>
<connect gate="A" pin="BOOT" pad="3"/>
<connect gate="A" pin="EN" pad="7"/>
<connect gate="A" pin="FB" pad="6"/>
<connect gate="A" pin="GND" pad="8"/>
<connect gate="A" pin="GND_2" pad="4"/>
<connect gate="A" pin="NC" pad="5"/>
<connect gate="A" pin="SW" pad="1"/>
<connect gate="A" pin="VIN" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM22678TJ-ADJ"/>
<attribute name="OC_FARNELL" value="1657729"/>
<attribute name="OC_NEWARK" value="34P4794"/>
<attribute name="PACKAGE" value="TO-263-7"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM22679TJ-ADJ" prefix="U">
<description>3A SIMPLE SWITCHER®, Step-Down Voltage Regulator</description>
<gates>
<gate name="A" symbol="LM22679TJ-ADJ"/>
</gates>
<devices>
<device name="" package="TO127P1435X210-8N">
<connects>
<connect gate="A" pin="BOOT" pad="3"/>
<connect gate="A" pin="FB" pad="6"/>
<connect gate="A" pin="GND" pad="8"/>
<connect gate="A" pin="GND_2" pad="4"/>
<connect gate="A" pin="IADJ" pad="5"/>
<connect gate="A" pin="SS" pad="7"/>
<connect gate="A" pin="SW" pad="1"/>
<connect gate="A" pin="VIN" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM22679TJ-ADJ"/>
<attribute name="OC_FARNELL" value="1657731"/>
<attribute name="OC_NEWARK" value="12P7518"/>
<attribute name="PACKAGE" value="TO-263-7"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM22680MR-ADJ">
<description>Step-Down Voltage Regulator</description>
<gates>
<gate name="A" symbol="LM22680MR-ADJ"/>
</gates>
<devices>
<device name="" package="SOIC127P620X168-9N">
<connects>
<connect gate="A" pin="BOOT" pad="1"/>
<connect gate="A" pin="EN" pad="5"/>
<connect gate="A" pin="EP" pad="9"/>
<connect gate="A" pin="FB" pad="4"/>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="SS" pad="2"/>
<connect gate="A" pin="SW" pad="8"/>
<connect gate="A" pin="VIN" pad="7"/>
<connect gate="A" pin="~RT/SYNC" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM22680MR-ADJ"/>
<attribute name="OC_FARNELL" value="1697054"/>
<attribute name="OC_NEWARK" value="80P4533"/>
<attribute name="PACKAGE" value="PSOP-8"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM239J" prefix="U">
<description>Quad Comparators</description>
<gates>
<gate name="A" symbol="LM239J"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-14">
<connects>
<connect gate="A" pin="+IN1" pad="5"/>
<connect gate="A" pin="+IN2" pad="7"/>
<connect gate="A" pin="+IN3" pad="9"/>
<connect gate="A" pin="+IN4" pad="11"/>
<connect gate="A" pin="-IN1" pad="4"/>
<connect gate="A" pin="-IN2" pad="6"/>
<connect gate="A" pin="-IN3" pad="8"/>
<connect gate="A" pin="-IN4" pad="10"/>
<connect gate="A" pin="GND" pad="12"/>
<connect gate="A" pin="OUT1" pad="2"/>
<connect gate="A" pin="OUT2" pad="1"/>
<connect gate="A" pin="OUT3" pad="14"/>
<connect gate="A" pin="OUT4" pad="13"/>
<connect gate="A" pin="V+" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM239J"/>
<attribute name="OC_FARNELL" value="404457"/>
<attribute name="OC_NEWARK" value="72K7155"/>
<attribute name="PACKAGE" value="14-CDIP"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM25005MH" prefix="U">
<description>Step-Down Switching Regulator</description>
<gates>
<gate name="A" symbol="LM25005MH"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-21N">
<connects>
<connect gate="A" pin="AGND" pad="10"/>
<connect gate="A" pin="BST" pad="20"/>
<connect gate="A" pin="COMP" pad="6"/>
<connect gate="A" pin="EPAD" pad="21"/>
<connect gate="A" pin="FB" pad="7"/>
<connect gate="A" pin="IS" pad="16"/>
<connect gate="A" pin="IS_2" pad="15"/>
<connect gate="A" pin="OUT" pad="12"/>
<connect gate="A" pin="PGND" pad="14"/>
<connect gate="A" pin="PGND_2" pad="13"/>
<connect gate="A" pin="PRE" pad="19"/>
<connect gate="A" pin="RAMP" pad="9"/>
<connect gate="A" pin="RT" pad="8"/>
<connect gate="A" pin="SD" pad="2"/>
<connect gate="A" pin="SS" pad="11"/>
<connect gate="A" pin="SW" pad="18"/>
<connect gate="A" pin="SW_2" pad="17"/>
<connect gate="A" pin="SYNC" pad="5"/>
<connect gate="A" pin="VCC" pad="1"/>
<connect gate="A" pin="VIN" pad="4"/>
<connect gate="A" pin="VIN_2" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM25005MH"/>
<attribute name="OC_FARNELL" value="1286737"/>
<attribute name="OC_NEWARK" value="79K7769"/>
<attribute name="PACKAGE" value="TSSOP-20"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM25007MM" prefix="U">
<description>Step-Down Switching Regulator</description>
<gates>
<gate name="A" symbol="LM25007MM"/>
</gates>
<devices>
<device name="" package="SOP65P490X109-8N">
<connects>
<connect gate="A" pin="BST" pad="2"/>
<connect gate="A" pin="FEEDBACK" pad="5"/>
<connect gate="A" pin="RCL" pad="3"/>
<connect gate="A" pin="RON" pad="6"/>
<connect gate="A" pin="RTN" pad="4"/>
<connect gate="A" pin="SWITCH" pad="1"/>
<connect gate="A" pin="VCC" pad="7"/>
<connect gate="A" pin="VIN" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM25007MM"/>
<attribute name="OC_FARNELL" value="1312549"/>
<attribute name="OC_NEWARK" value="31M5346"/>
<attribute name="PACKAGE" value="SOP-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM25007SD" prefix="U">
<description>Step-Down Switching Regulator</description>
<gates>
<gate name="A" symbol="LM25007SD"/>
</gates>
<devices>
<device name="" package="DFN400X400X80-9N">
<connects>
<connect gate="A" pin="BST" pad="2"/>
<connect gate="A" pin="EPAD" pad="9"/>
<connect gate="A" pin="FB" pad="5"/>
<connect gate="A" pin="RCL" pad="3"/>
<connect gate="A" pin="RON" pad="6"/>
<connect gate="A" pin="RTN" pad="4"/>
<connect gate="A" pin="SW" pad="1"/>
<connect gate="A" pin="VCC" pad="7"/>
<connect gate="A" pin="VIN" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM25007SD"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="79K7777"/>
<attribute name="PACKAGE" value="DFN-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM25010MH" prefix="U">
<description>Step-Down Switching Regulator</description>
<gates>
<gate name="A" symbol="LM25010MH"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-15N">
<connects>
<connect gate="A" pin="BST" pad="3"/>
<connect gate="A" pin="EPAD" pad="15"/>
<connect gate="A" pin="FB" pad="9"/>
<connect gate="A" pin="ISEN" pad="4"/>
<connect gate="A" pin="NC" pad="8"/>
<connect gate="A" pin="NC_2" pad="14"/>
<connect gate="A" pin="NC_3" pad="1"/>
<connect gate="A" pin="NC_4" pad="7"/>
<connect gate="A" pin="RON/SD" pad="11"/>
<connect gate="A" pin="RTN" pad="6"/>
<connect gate="A" pin="SGND" pad="5"/>
<connect gate="A" pin="SS" pad="10"/>
<connect gate="A" pin="SW" pad="2"/>
<connect gate="A" pin="VCC" pad="12"/>
<connect gate="A" pin="VIN" pad="13"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM25010MH"/>
<attribute name="OC_FARNELL" value="1286738"/>
<attribute name="OC_NEWARK" value="79K7781"/>
<attribute name="PACKAGE" value="TSSOP-14"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM25010SD" prefix="U">
<description>Step Down Switching Regulator</description>
<gates>
<gate name="A" symbol="LM25010SD"/>
</gates>
<devices>
<device name="" package="DFN400X400X80-11N">
<connects>
<connect gate="A" pin="BST" pad="2"/>
<connect gate="A" pin="EPAD" pad="11"/>
<connect gate="A" pin="FB" pad="6"/>
<connect gate="A" pin="ISEN" pad="3"/>
<connect gate="A" pin="RON/SD" pad="8"/>
<connect gate="A" pin="RTN" pad="5"/>
<connect gate="A" pin="SGND" pad="4"/>
<connect gate="A" pin="SS" pad="7"/>
<connect gate="A" pin="SW" pad="1"/>
<connect gate="A" pin="VCC" pad="9"/>
<connect gate="A" pin="VIN" pad="10"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM25010SD"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="79K7785"/>
<attribute name="PACKAGE" value="DFN-10"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM25011MY" prefix="U">
<description>On-Time Switching Regulator</description>
<gates>
<gate name="A" symbol="LM25011MY"/>
</gates>
<devices>
<device name="" package="SOP50P490X110-11N">
<connects>
<connect gate="A" pin="BST" pad="10"/>
<connect gate="A" pin="CS" pad="8"/>
<connect gate="A" pin="CSG" pad="7"/>
<connect gate="A" pin="EPAD" pad="11"/>
<connect gate="A" pin="FB" pad="6"/>
<connect gate="A" pin="PGD" pad="3"/>
<connect gate="A" pin="RT" pad="2"/>
<connect gate="A" pin="SGND" pad="5"/>
<connect gate="A" pin="SS" pad="4"/>
<connect gate="A" pin="SW" pad="9"/>
<connect gate="A" pin="VIN" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM25011MY"/>
<attribute name="OC_FARNELL" value="1735793"/>
<attribute name="OC_NEWARK" value="14R4582"/>
<attribute name="PACKAGE" value="MSOP-10"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM25037MT" prefix="U">
<description>Dual-Mode PWM Controller</description>
<gates>
<gate name="A" symbol="LM25037MT"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-16N">
<connects>
<connect gate="A" pin="AGND" pad="6"/>
<connect gate="A" pin="COMP" pad="3"/>
<connect gate="A" pin="CS" pad="8"/>
<connect gate="A" pin="FB" pad="4"/>
<connect gate="A" pin="OUTA" pad="13"/>
<connect gate="A" pin="OUTB" pad="12"/>
<connect gate="A" pin="PGND" pad="11"/>
<connect gate="A" pin="RAMP" pad="1"/>
<connect gate="A" pin="REF" pad="15"/>
<connect gate="A" pin="RES" pad="9"/>
<connect gate="A" pin="RT1" pad="7"/>
<connect gate="A" pin="RT2" pad="5"/>
<connect gate="A" pin="SS" pad="10"/>
<connect gate="A" pin="UVLO" pad="2"/>
<connect gate="A" pin="VCC" pad="14"/>
<connect gate="A" pin="VIN" pad="16"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM25037MT"/>
<attribute name="OC_FARNELL" value="1663007"/>
<attribute name="OC_NEWARK" value="02P9788"/>
<attribute name="PACKAGE" value="TSSOP-16"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM25037QMT" prefix="U">
<description>Dual-Mode PWM Controller</description>
<gates>
<gate name="A" symbol="LM25037QMT"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-16N">
<connects>
<connect gate="A" pin="AGND" pad="6"/>
<connect gate="A" pin="COMP" pad="3"/>
<connect gate="A" pin="CS" pad="8"/>
<connect gate="A" pin="FB" pad="4"/>
<connect gate="A" pin="OUTA" pad="13"/>
<connect gate="A" pin="OUTB" pad="12"/>
<connect gate="A" pin="PGND" pad="11"/>
<connect gate="A" pin="RAMP" pad="1"/>
<connect gate="A" pin="REF" pad="15"/>
<connect gate="A" pin="RES" pad="9"/>
<connect gate="A" pin="RT1" pad="7"/>
<connect gate="A" pin="RT2" pad="5"/>
<connect gate="A" pin="SS" pad="10"/>
<connect gate="A" pin="UVLO" pad="2"/>
<connect gate="A" pin="VCC" pad="14"/>
<connect gate="A" pin="VIN" pad="16"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM25037QMT"/>
<attribute name="OC_FARNELL" value="1736510"/>
<attribute name="OC_NEWARK" value="16R1309"/>
<attribute name="PACKAGE" value="TSSOP-16"/>
<attribute name="SUPPLIER" value="National semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM25061PMM-1" prefix="U">
<description>Positive Low Voltage Power Limiting Hot Swap Controller</description>
<gates>
<gate name="A" symbol="LM25061PMM-1"/>
</gates>
<devices>
<device name="" package="SOP50P490X110-10N">
<connects>
<connect gate="A" pin="FB" pad="4"/>
<connect gate="A" pin="GATE" pad="10"/>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="OUT" pad="9"/>
<connect gate="A" pin="PGD" pad="8"/>
<connect gate="A" pin="PWR" pad="7"/>
<connect gate="A" pin="SENSE" pad="1"/>
<connect gate="A" pin="TIMER" pad="6"/>
<connect gate="A" pin="UVLO/EN" pad="3"/>
<connect gate="A" pin="VIN" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM25061PMM-1"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="55R3809"/>
<attribute name="PACKAGE" value="MSOP-10"/>
<attribute name="SUPPLIER" value="National semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM25061PMM-2" prefix="U">
<description>Positive Low Voltage Power Limiting Hot Swap Controller</description>
<gates>
<gate name="A" symbol="LM25061PMM-2"/>
</gates>
<devices>
<device name="" package="SOP50P490X110-10N">
<connects>
<connect gate="A" pin="FB" pad="4"/>
<connect gate="A" pin="GATE" pad="10"/>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="OUT" pad="9"/>
<connect gate="A" pin="PGD" pad="8"/>
<connect gate="A" pin="PWR" pad="7"/>
<connect gate="A" pin="SENSE" pad="1"/>
<connect gate="A" pin="TIMER" pad="6"/>
<connect gate="A" pin="UVLO/EN" pad="3"/>
<connect gate="A" pin="VIN" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM25061PMM-2"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="55R3810"/>
<attribute name="PACKAGE" value="MSOP-10"/>
<attribute name="SUPPLIER" value="National semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM25069PMM-1" prefix="U">
<description>Positive Low Voltage Power Limiting Hot Swap Controller</description>
<gates>
<gate name="A" symbol="LM25069PMM-1"/>
</gates>
<devices>
<device name="" package="SOP50P490X110-10N">
<connects>
<connect gate="A" pin="GATE" pad="10"/>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="OUT" pad="9"/>
<connect gate="A" pin="OVLO" pad="4"/>
<connect gate="A" pin="PGD" pad="8"/>
<connect gate="A" pin="PWR" pad="7"/>
<connect gate="A" pin="SENSE" pad="1"/>
<connect gate="A" pin="TIMER" pad="6"/>
<connect gate="A" pin="UVLO/EN" pad="3"/>
<connect gate="A" pin="VIN" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM25069PMM-1"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="55R3813"/>
<attribute name="PACKAGE" value="MSOP-10"/>
<attribute name="SUPPLIER" value="National semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM25069PMM-2" prefix="U">
<description>Positive Low Voltage Power Limiting Hot Swap Controller</description>
<gates>
<gate name="A" symbol="LM25069PMM-2"/>
</gates>
<devices>
<device name="" package="SOP50P490X110-10N">
<connects>
<connect gate="A" pin="GATE" pad="10"/>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="OUT" pad="9"/>
<connect gate="A" pin="OVLO" pad="4"/>
<connect gate="A" pin="PGD" pad="8"/>
<connect gate="A" pin="PWR" pad="7"/>
<connect gate="A" pin="SENSE" pad="1"/>
<connect gate="A" pin="TIMER" pad="6"/>
<connect gate="A" pin="UVLO/EN" pad="3"/>
<connect gate="A" pin="VIN" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM25069PMM-2"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="55R3814"/>
<attribute name="PACKAGE" value="MSOP-10"/>
<attribute name="SUPPLIER" value="National semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM25085AMM" prefix="U">
<description>Switching Controller</description>
<gates>
<gate name="A" symbol="LM25085AMM"/>
</gates>
<devices>
<device name="" package="SOP65P490X109-8N">
<connects>
<connect gate="A" pin="ADJ" pad="1"/>
<connect gate="A" pin="FB" pad="3"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="ISEN" pad="5"/>
<connect gate="A" pin="PGATE" pad="6"/>
<connect gate="A" pin="RT" pad="2"/>
<connect gate="A" pin="VCC" pad="7"/>
<connect gate="A" pin="VIN" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM25085AMM"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="55R3817"/>
<attribute name="PACKAGE" value="MSOP-8"/>
<attribute name="SUPPLIER" value="National semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM25085AMY" prefix="U">
<description>On-Time PFET Buck Switching Controller</description>
<gates>
<gate name="A" symbol="LM25085AMY"/>
</gates>
<devices>
<device name="" package="SOP65P490X110-9N">
<connects>
<connect gate="A" pin="ADJ" pad="1"/>
<connect gate="A" pin="EPAD" pad="9"/>
<connect gate="A" pin="FB" pad="3"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="ISEN" pad="5"/>
<connect gate="A" pin="PGATE" pad="6"/>
<connect gate="A" pin="RT" pad="2"/>
<connect gate="A" pin="VCC" pad="7"/>
<connect gate="A" pin="VIN" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM25085AMY"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="55R3820"/>
<attribute name="PACKAGE" value="MSOP-8"/>
<attribute name="SUPPLIER" value="National semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM25085ASD" prefix="U">
<description>On-Time PFET Buck Switching Controller</description>
<gates>
<gate name="A" symbol="LM25085ASD"/>
</gates>
<devices>
<device name="" package="DFN300X300X80-9N">
<connects>
<connect gate="A" pin="ADJ" pad="1"/>
<connect gate="A" pin="EPAD" pad="9"/>
<connect gate="A" pin="FB" pad="3"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="ISEN" pad="5"/>
<connect gate="A" pin="PGATE" pad="6"/>
<connect gate="A" pin="RT" pad="2"/>
<connect gate="A" pin="VCC" pad="7"/>
<connect gate="A" pin="VIN" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM25085ASD"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="55R3823"/>
<attribute name="PACKAGE" value="DFN-8"/>
<attribute name="SUPPLIER" value="National semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM25085QMY">
<description>On-Time PFET Buck Switching Controller</description>
<gates>
<gate name="A" symbol="LM25085QMY"/>
</gates>
<devices>
<device name="" package="SOP65P490X110-9N">
<connects>
<connect gate="A" pin="ADJ" pad="1"/>
<connect gate="A" pin="EPAD" pad="9"/>
<connect gate="A" pin="FB" pad="3"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="ISEN" pad="5"/>
<connect gate="A" pin="PGATE" pad="6"/>
<connect gate="A" pin="RT" pad="2"/>
<connect gate="A" pin="VCC" pad="7"/>
<connect gate="A" pin="VIN" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM25085QMY"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="77R5195"/>
<attribute name="PACKAGE" value="MSOP-8"/>
<attribute name="SUPPLIER" value="National semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM25085SD" prefix="U">
<description>On-Time PFET Buck Switching Controller</description>
<gates>
<gate name="A" symbol="LM25085SD"/>
</gates>
<devices>
<device name="" package="DFN300X300X80-9N">
<connects>
<connect gate="A" pin="ADJ" pad="1"/>
<connect gate="A" pin="EPAD" pad="9"/>
<connect gate="A" pin="FB" pad="3"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="ISEN" pad="5"/>
<connect gate="A" pin="PGATE" pad="6"/>
<connect gate="A" pin="RT" pad="2"/>
<connect gate="A" pin="VCC" pad="7"/>
<connect gate="A" pin="VIN" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM25085SD"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="55R3826"/>
<attribute name="PACKAGE" value="DFN-8"/>
<attribute name="SUPPLIER" value="National semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM25088MH-1">
<description>Wide Input Range Non-Synchronous Buck Controller</description>
<gates>
<gate name="A" symbol="LM25088MH-1"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-17N">
<connects>
<connect gate="A" pin="BOOT" pad="15"/>
<connect gate="A" pin="COMP" pad="7"/>
<connect gate="A" pin="CS" pad="12"/>
<connect gate="A" pin="CSG" pad="11"/>
<connect gate="A" pin="DITH" pad="10"/>
<connect gate="A" pin="EN" pad="2"/>
<connect gate="A" pin="EPAD" pad="17"/>
<connect gate="A" pin="FB" pad="8"/>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="HG" pad="14"/>
<connect gate="A" pin="OUT" pad="9"/>
<connect gate="A" pin="RAMP" pad="4"/>
<connect gate="A" pin="RT/SYNC" pad="5"/>
<connect gate="A" pin="SS" pad="3"/>
<connect gate="A" pin="SW" pad="13"/>
<connect gate="A" pin="VCC" pad="16"/>
<connect gate="A" pin="VIN" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM25088MH-1"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="46P3250"/>
<attribute name="PACKAGE" value="TSSOP-16"/>
<attribute name="SUPPLIER" value="National semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM25088MH-2">
<description>Wide Input Range Non-Synchronous Buck Controller</description>
<gates>
<gate name="A" symbol="LM25088MH-2"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-17N">
<connects>
<connect gate="A" pin="BOOT" pad="15"/>
<connect gate="A" pin="COMP" pad="7"/>
<connect gate="A" pin="CS" pad="12"/>
<connect gate="A" pin="CSG" pad="11"/>
<connect gate="A" pin="DITH" pad="10"/>
<connect gate="A" pin="EN" pad="2"/>
<connect gate="A" pin="EPAD" pad="17"/>
<connect gate="A" pin="FB" pad="8"/>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="HG" pad="14"/>
<connect gate="A" pin="OUT" pad="9"/>
<connect gate="A" pin="RAMP" pad="4"/>
<connect gate="A" pin="RT/SYNC" pad="5"/>
<connect gate="A" pin="SS" pad="3"/>
<connect gate="A" pin="SW" pad="13"/>
<connect gate="A" pin="VCC" pad="16"/>
<connect gate="A" pin="VIN" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM25088MH-2"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="46P3251"/>
<attribute name="PACKAGE" value="TSSOP-16"/>
<attribute name="SUPPLIER" value="National semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM25115AMT" prefix="U">
<description>Secondary Side Post Regulator/DC-DC Converter</description>
<gates>
<gate name="A" symbol="LM25115AMT"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-16N">
<connects>
<connect gate="A" pin="AGND" pad="3"/>
<connect gate="A" pin="CO" pad="4"/>
<connect gate="A" pin="COMP" pad="5"/>
<connect gate="A" pin="CS" pad="1"/>
<connect gate="A" pin="FB" pad="6"/>
<connect gate="A" pin="HB" pad="15"/>
<connect gate="A" pin="HO" pad="14"/>
<connect gate="A" pin="HS" pad="13"/>
<connect gate="A" pin="LO" pad="11"/>
<connect gate="A" pin="PGND" pad="10"/>
<connect gate="A" pin="RAMP" pad="8"/>
<connect gate="A" pin="SYNC" pad="9"/>
<connect gate="A" pin="TRK/SS" pad="7"/>
<connect gate="A" pin="VBIAS" pad="16"/>
<connect gate="A" pin="VCC" pad="12"/>
<connect gate="A" pin="VOUT" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM25115AMT"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="32M0982"/>
<attribute name="PACKAGE" value="TSSOP-16"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM25115MT" prefix="U">
<description>Secondary Side Post Regulator Controller</description>
<gates>
<gate name="A" symbol="LM25115MT"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-16N">
<connects>
<connect gate="A" pin="AGND" pad="3"/>
<connect gate="A" pin="CO" pad="4"/>
<connect gate="A" pin="COMP" pad="5"/>
<connect gate="A" pin="CS" pad="1"/>
<connect gate="A" pin="FB" pad="6"/>
<connect gate="A" pin="HB" pad="15"/>
<connect gate="A" pin="HO" pad="14"/>
<connect gate="A" pin="HS" pad="13"/>
<connect gate="A" pin="LO" pad="11"/>
<connect gate="A" pin="PGND" pad="10"/>
<connect gate="A" pin="RAMP" pad="8"/>
<connect gate="A" pin="SS" pad="7"/>
<connect gate="A" pin="SYNC" pad="9"/>
<connect gate="A" pin="VBIAS" pad="16"/>
<connect gate="A" pin="VCC" pad="12"/>
<connect gate="A" pin="VOUT" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM25115MT"/>
<attribute name="OC_FARNELL" value="1286739"/>
<attribute name="OC_NEWARK" value="79K7788"/>
<attribute name="PACKAGE" value="TSSOP-16"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM25115SD" prefix="U">
<description>Secondary Side Post Regulator Controller</description>
<gates>
<gate name="A" symbol="LM25115SD"/>
</gates>
<devices>
<device name="" package="DFN500X500X80-16N">
<connects>
<connect gate="A" pin="AGND" pad="3"/>
<connect gate="A" pin="CO" pad="4"/>
<connect gate="A" pin="COMP" pad="5"/>
<connect gate="A" pin="CS" pad="1"/>
<connect gate="A" pin="FB" pad="6"/>
<connect gate="A" pin="HB" pad="15"/>
<connect gate="A" pin="HO" pad="14"/>
<connect gate="A" pin="HS" pad="13"/>
<connect gate="A" pin="LO" pad="11"/>
<connect gate="A" pin="PGND" pad="10"/>
<connect gate="A" pin="RAMP" pad="8"/>
<connect gate="A" pin="SS" pad="7"/>
<connect gate="A" pin="SYNC" pad="9"/>
<connect gate="A" pin="THER_PAD" pad="17"/>
<connect gate="A" pin="VBIAS" pad="16"/>
<connect gate="A" pin="VCC" pad="12"/>
<connect gate="A" pin="VOUT" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM25115SD"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="99K2331"/>
<attribute name="PACKAGE" value="DFN-16"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM25574MT" prefix="U">
<description>Step-Down Switching Regulator</description>
<gates>
<gate name="A" symbol="LM25574MT"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-16N">
<connects>
<connect gate="A" pin="AGND" pad="9"/>
<connect gate="A" pin="BST" pad="16"/>
<connect gate="A" pin="COMP" pad="5"/>
<connect gate="A" pin="FB" pad="6"/>
<connect gate="A" pin="IS" pad="13"/>
<connect gate="A" pin="OUT" pad="11"/>
<connect gate="A" pin="PGND" pad="12"/>
<connect gate="A" pin="PRE" pad="15"/>
<connect gate="A" pin="RAMP" pad="8"/>
<connect gate="A" pin="RT" pad="7"/>
<connect gate="A" pin="SD" pad="2"/>
<connect gate="A" pin="SS" pad="10"/>
<connect gate="A" pin="SW" pad="14"/>
<connect gate="A" pin="SYNC" pad="4"/>
<connect gate="A" pin="VCC" pad="1"/>
<connect gate="A" pin="VIN" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM25574MT"/>
<attribute name="OC_FARNELL" value="1325415"/>
<attribute name="OC_NEWARK" value="32M0988"/>
<attribute name="PACKAGE" value="SOP-16"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM25574QMT" prefix="U">
<description>Step-Down Switching Regulator</description>
<gates>
<gate name="A" symbol="LM25574QMT"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-16N">
<connects>
<connect gate="A" pin="AGND" pad="9"/>
<connect gate="A" pin="BST" pad="16"/>
<connect gate="A" pin="COMP" pad="5"/>
<connect gate="A" pin="FB" pad="6"/>
<connect gate="A" pin="IS" pad="13"/>
<connect gate="A" pin="OUT" pad="11"/>
<connect gate="A" pin="PGND" pad="12"/>
<connect gate="A" pin="PRE" pad="15"/>
<connect gate="A" pin="RAMP" pad="8"/>
<connect gate="A" pin="RT" pad="7"/>
<connect gate="A" pin="SD" pad="2"/>
<connect gate="A" pin="SS" pad="10"/>
<connect gate="A" pin="SW" pad="14"/>
<connect gate="A" pin="SYNC" pad="4"/>
<connect gate="A" pin="VCC" pad="1"/>
<connect gate="A" pin="VIN" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM25574QMT"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="55R3830"/>
<attribute name="PACKAGE" value="TSSOP-16"/>
<attribute name="SUPPLIER" value="National semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM25575MH" prefix="U">
<description>Step-Down Switching Regulator</description>
<gates>
<gate name="A" symbol="LM25575MH"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-17N">
<connects>
<connect gate="A" pin="AGND" pad="9"/>
<connect gate="A" pin="BST" pad="16"/>
<connect gate="A" pin="COMP" pad="5"/>
<connect gate="A" pin="EP" pad="17"/>
<connect gate="A" pin="FB" pad="6"/>
<connect gate="A" pin="IS" pad="13"/>
<connect gate="A" pin="OUT" pad="11"/>
<connect gate="A" pin="PGND" pad="12"/>
<connect gate="A" pin="PRE" pad="15"/>
<connect gate="A" pin="RAMP" pad="8"/>
<connect gate="A" pin="RT" pad="7"/>
<connect gate="A" pin="SD" pad="2"/>
<connect gate="A" pin="SS" pad="10"/>
<connect gate="A" pin="SW" pad="14"/>
<connect gate="A" pin="SYNC" pad="4"/>
<connect gate="A" pin="VCC" pad="1"/>
<connect gate="A" pin="VIN" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM25575MH"/>
<attribute name="OC_FARNELL" value="1325416"/>
<attribute name="OC_NEWARK" value="32M0992"/>
<attribute name="PACKAGE" value="TSSOP-16"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM25575QMH" prefix="U">
<description>Step-Down Switching Regulator</description>
<gates>
<gate name="A" symbol="LM25575QMH"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-17N">
<connects>
<connect gate="A" pin="AGND" pad="9"/>
<connect gate="A" pin="BST" pad="16"/>
<connect gate="A" pin="COMP" pad="5"/>
<connect gate="A" pin="EPAD" pad="17"/>
<connect gate="A" pin="FB" pad="6"/>
<connect gate="A" pin="IS" pad="13"/>
<connect gate="A" pin="OUT" pad="11"/>
<connect gate="A" pin="PGND" pad="12"/>
<connect gate="A" pin="PRE" pad="15"/>
<connect gate="A" pin="RAMP" pad="8"/>
<connect gate="A" pin="RT" pad="7"/>
<connect gate="A" pin="SD" pad="2"/>
<connect gate="A" pin="SS" pad="10"/>
<connect gate="A" pin="SW" pad="14"/>
<connect gate="A" pin="SYNC" pad="4"/>
<connect gate="A" pin="VCC" pad="1"/>
<connect gate="A" pin="VIN" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM25575QMH"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="55R3833"/>
<attribute name="PACKAGE" value="TSSOP-16"/>
<attribute name="SUPPLIER" value="National semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM25576MH" prefix="U">
<description>Switching Regulator</description>
<gates>
<gate name="A" symbol="LM25576MH"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-21N">
<connects>
<connect gate="A" pin="AGND" pad="10"/>
<connect gate="A" pin="BST" pad="20"/>
<connect gate="A" pin="COMP" pad="6"/>
<connect gate="A" pin="EP" pad="21"/>
<connect gate="A" pin="FB" pad="7"/>
<connect gate="A" pin="IS" pad="16"/>
<connect gate="A" pin="IS_2" pad="15"/>
<connect gate="A" pin="OUT" pad="12"/>
<connect gate="A" pin="PGND" pad="14"/>
<connect gate="A" pin="PGND_2" pad="13"/>
<connect gate="A" pin="PRE" pad="19"/>
<connect gate="A" pin="RAMP" pad="9"/>
<connect gate="A" pin="RT" pad="8"/>
<connect gate="A" pin="SD" pad="2"/>
<connect gate="A" pin="SS" pad="11"/>
<connect gate="A" pin="SW" pad="18"/>
<connect gate="A" pin="SW_2" pad="17"/>
<connect gate="A" pin="SYNC" pad="5"/>
<connect gate="A" pin="VCC" pad="1"/>
<connect gate="A" pin="VIN" pad="4"/>
<connect gate="A" pin="VIN_2" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM25576MH"/>
<attribute name="OC_FARNELL" value="1325421"/>
<attribute name="OC_NEWARK" value="32M0997"/>
<attribute name="PACKAGE" value="TSSOP-20"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM25576QMH" prefix="U">
<description>Step-Down Switching Regulator</description>
<gates>
<gate name="A" symbol="LM25576QMH"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-21N">
<connects>
<connect gate="A" pin="AGND" pad="10"/>
<connect gate="A" pin="BST" pad="20"/>
<connect gate="A" pin="COMP" pad="6"/>
<connect gate="A" pin="EPAD" pad="21"/>
<connect gate="A" pin="FB" pad="7"/>
<connect gate="A" pin="IS" pad="16"/>
<connect gate="A" pin="IS_2" pad="15"/>
<connect gate="A" pin="OUT" pad="12"/>
<connect gate="A" pin="PGND" pad="14"/>
<connect gate="A" pin="PGND_2" pad="13"/>
<connect gate="A" pin="PRE" pad="19"/>
<connect gate="A" pin="RAMP" pad="9"/>
<connect gate="A" pin="RT" pad="8"/>
<connect gate="A" pin="SD" pad="2"/>
<connect gate="A" pin="SS" pad="11"/>
<connect gate="A" pin="SW" pad="18"/>
<connect gate="A" pin="SW_2" pad="17"/>
<connect gate="A" pin="SYNC" pad="5"/>
<connect gate="A" pin="VCC" pad="1"/>
<connect gate="A" pin="VIN" pad="4"/>
<connect gate="A" pin="VIN_2" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM25576QMH"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="55R3835"/>
<attribute name="PACKAGE" value="TSSOP-20"/>
<attribute name="SUPPLIER" value="National semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2575M-5.0" prefix="U">
<description>Step-Down Voltage Regulator</description>
<gates>
<gate name="A" symbol="LM2575M-5.0"/>
</gates>
<devices>
<device name="" package="SOIC127P640X265-24N">
<connects>
<connect gate="A" pin="FB" pad="7"/>
<connect gate="A" pin="NC" pad="6"/>
<connect gate="A" pin="NC_10" pad="23"/>
<connect gate="A" pin="NC_11" pad="2"/>
<connect gate="A" pin="NC_12" pad="24"/>
<connect gate="A" pin="NC_13" pad="3"/>
<connect gate="A" pin="NC_14" pad="4"/>
<connect gate="A" pin="NC_15" pad="5"/>
<connect gate="A" pin="NC_2" pad="16"/>
<connect gate="A" pin="NC_3" pad="19"/>
<connect gate="A" pin="NC_4" pad="20"/>
<connect gate="A" pin="NC_5" pad="21"/>
<connect gate="A" pin="NC_6" pad="13"/>
<connect gate="A" pin="NC_7" pad="22"/>
<connect gate="A" pin="NC_8" pad="9"/>
<connect gate="A" pin="NC_9" pad="11"/>
<connect gate="A" pin="ON/OFF" pad="10"/>
<connect gate="A" pin="OUT" pad="18"/>
<connect gate="A" pin="OUT_2" pad="17"/>
<connect gate="A" pin="PWR_GND" pad="12"/>
<connect gate="A" pin="PWR_GND_2" pad="1"/>
<connect gate="A" pin="SIG_GND" pad="8"/>
<connect gate="A" pin="VIN" pad="15"/>
<connect gate="A" pin="VIN_2" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2575M-5.0"/>
<attribute name="OC_FARNELL" value="9493441"/>
<attribute name="OC_NEWARK" value="41K3646"/>
<attribute name="PACKAGE" value="24-SOIC"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2575N-5.0" prefix="U">
<description>SIMPLE SWITCHER</description>
<gates>
<gate name="A" symbol="LM2575N-5.0"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-16">
<connects>
<connect gate="A" pin="FB" pad="7"/>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="GND_2" pad="11"/>
<connect gate="A" pin="GND_3" pad="12"/>
<connect gate="A" pin="GND_4" pad="13"/>
<connect gate="A" pin="GND_5" pad="14"/>
<connect gate="A" pin="NC" pad="10"/>
<connect gate="A" pin="NC_2" pad="1"/>
<connect gate="A" pin="NC_3" pad="2"/>
<connect gate="A" pin="NC_4" pad="6"/>
<connect gate="A" pin="NC_5" pad="8"/>
<connect gate="A" pin="NC_6" pad="15"/>
<connect gate="A" pin="NC_7" pad="4"/>
<connect gate="A" pin="ON/OFF" pad="9"/>
<connect gate="A" pin="OUT" pad="3"/>
<connect gate="A" pin="VIN" pad="16"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2575N-50"/>
<attribute name="OC_FARNELL" value="9486054"/>
<attribute name="OC_NEWARK" value="41K3655"/>
<attribute name="PACKAGE" value="DIP-16"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2575S-12" prefix="U">
<description>Step-Down Voltage Regulator</description>
<gates>
<gate name="A" symbol="LM2575S-12"/>
</gates>
<devices>
<device name="" package="TO170X1435X457-6N">
<connects>
<connect gate="A" pin="FB" pad="4"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="GND_2" pad="6"/>
<connect gate="A" pin="OUT" pad="2"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="~ON/OFF" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2575S-12"/>
<attribute name="OC_FARNELL" value="1798355"/>
<attribute name="OC_NEWARK" value="73R9727"/>
<attribute name="PACKAGE" value="TO-263-5"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2575S-15" prefix="U">
<description>Voltage Regulator</description>
<gates>
<gate name="A" symbol="LM2575S-15"/>
</gates>
<devices>
<device name="" package="TO170P1435X465-6N">
<connects>
<connect gate="A" pin="FB" pad="4"/>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="GND_2" pad="3"/>
<connect gate="A" pin="OUT" pad="2"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="~ON~/OFF" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2575S-15"/>
<attribute name="OC_FARNELL" value="1798356"/>
<attribute name="OC_NEWARK" value="75R2093"/>
<attribute name="PACKAGE" value="TO-263-5"/>
<attribute name="SUPPLIER" value="National"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2575S-3.3" prefix="U">
<description>Step-Down Voltage Regulator</description>
<gates>
<gate name="A" symbol="LM2575S-3.3"/>
</gates>
<devices>
<device name="" package="TO170P1435X457-6N">
<connects>
<connect gate="A" pin="COMP" pad="1"/>
<connect gate="A" pin="FB" pad="2"/>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="GND_2" pad="3"/>
<connect gate="A" pin="SW" pad="4"/>
<connect gate="A" pin="VIN" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2575S-3.3"/>
<attribute name="OC_FARNELL" value="8221944"/>
<attribute name="OC_NEWARK" value="41K3659"/>
<attribute name="PACKAGE" value="TO-263-5"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2575S-5.0" prefix="U">
<description>Step-Down Voltage Regulator</description>
<gates>
<gate name="A" symbol="LM2575S-5.0"/>
</gates>
<devices>
<device name="" package="TO170P1435X457-6N">
<connects>
<connect gate="A" pin="COMP" pad="1"/>
<connect gate="A" pin="FB" pad="2"/>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="GND_2" pad="3"/>
<connect gate="A" pin="SW" pad="4"/>
<connect gate="A" pin="VIN" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2575S-5.0"/>
<attribute name="OC_FARNELL" value="1523849"/>
<attribute name="OC_NEWARK" value="41K3660"/>
<attribute name="PACKAGE" value="TO-263-5"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2575S-ADJ" prefix="U">
<description>Step-Down Voltage Regulator</description>
<gates>
<gate name="A" symbol="LM2575S-ADJ"/>
</gates>
<devices>
<device name="" package="TO170P1435X457-6N">
<connects>
<connect gate="A" pin="COMP" pad="1"/>
<connect gate="A" pin="FB" pad="2"/>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="GND_2" pad="3"/>
<connect gate="A" pin="SW" pad="4"/>
<connect gate="A" pin="VIN" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2575S-ADJ"/>
<attribute name="OC_FARNELL" value="9489878"/>
<attribute name="OC_NEWARK" value="41K3656"/>
<attribute name="PACKAGE" value="TO-263-5"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2575T-12" prefix="U">
<description>IC, STEP-DOWN REGULATOR</description>
<gates>
<gate name="A" symbol="LM2575T-12"/>
</gates>
<devices>
<device name="" package="TO170P470X1016X2092-5P">
<connects>
<connect gate="A" pin="FB" pad="4"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="ON/OFF" pad="5"/>
<connect gate="A" pin="OUTPUT" pad="2"/>
<connect gate="A" pin="VIN" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2575T-12"/>
<attribute name="OC_FARNELL" value="9488073"/>
<attribute name="OC_NEWARK" value="41K3667"/>
<attribute name="PACKAGE" value="TO220-5"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2575T-15" prefix="U">
<description>IC, STEP-DOWN REGULATOR</description>
<gates>
<gate name="A" symbol="LM2575T-15"/>
</gates>
<devices>
<device name="" package="TO170P470X1016X2092-5P">
<connects>
<connect gate="A" pin="FB" pad="4"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="ON/OFF" pad="5"/>
<connect gate="A" pin="OUTPUT" pad="2"/>
<connect gate="A" pin="VIN" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2575T-15"/>
<attribute name="OC_FARNELL" value="9488081"/>
<attribute name="OC_NEWARK" value="41K3668"/>
<attribute name="PACKAGE" value="TO220-5"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2575T-3.3" prefix="U">
<description>DC/DC Converter IC</description>
<gates>
<gate name="A" symbol="LM2575T-3.3"/>
</gates>
<devices>
<device name="" package="TO170P470X1016X2092-5P">
<connects>
<connect gate="A" pin="FB" pad="4"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="ON/OFF" pad="5"/>
<connect gate="A" pin="OUTPUT" pad="2"/>
<connect gate="A" pin="VIN" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2575T-3.3"/>
<attribute name="OC_FARNELL" value="9493549"/>
<attribute name="OC_NEWARK" value="41K3669"/>
<attribute name="PACKAGE" value="TO220-5"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2575T-5.0" prefix="U">
<description>IC, STEP-DOWN REGULATOR</description>
<gates>
<gate name="A" symbol="LM2575T-5.0"/>
</gates>
<devices>
<device name="" package="TO170P470X1016X2092-5P">
<connects>
<connect gate="A" pin="FB" pad="4"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="ON/OFF" pad="5"/>
<connect gate="A" pin="OUTPUT" pad="2"/>
<connect gate="A" pin="VIN" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2575T-5.0"/>
<attribute name="OC_FARNELL" value="9488090"/>
<attribute name="OC_NEWARK" value="41K3670"/>
<attribute name="PACKAGE" value="TO220-5"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2575T-ADJ" prefix="U">
<description>IC, STEP-DOWN REGULATOR</description>
<gates>
<gate name="A" symbol="LM2575T-ADJ"/>
</gates>
<devices>
<device name="" package="TO170P470X1016X2092-5P">
<connects>
<connect gate="A" pin="FB" pad="4"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="ON/OFF" pad="5"/>
<connect gate="A" pin="OUTPUT" pad="2"/>
<connect gate="A" pin="VIN" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2575T-ADJ"/>
<attribute name="OC_FARNELL" value="9488103"/>
<attribute name="OC_NEWARK" value="41K3666"/>
<attribute name="PACKAGE" value="TO220-5"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2585S-12" prefix="U">
<description>FLYBACK REGULATOR</description>
<gates>
<gate name="A" symbol="LM2585S-12"/>
</gates>
<devices>
<device name="" package="TO170P1435X457-5N">
<connects>
<connect gate="A" pin="COMP" pad="1"/>
<connect gate="A" pin="FB" pad="2"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="GND_2" pad="6"/>
<connect gate="A" pin="SW" pad="4"/>
<connect gate="A" pin="VIN" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2585S-12"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K3723"/>
<attribute name="PACKAGE" value="TO-263-5"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2585S-3.3" prefix="U">
<description>FLYBACK REGULATOR</description>
<gates>
<gate name="A" symbol="LM2585S-3.3"/>
</gates>
<devices>
<device name="" package="TO170P1435X457-5N">
<connects>
<connect gate="A" pin="COMP" pad="1"/>
<connect gate="A" pin="FB" pad="2"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="GND_2" pad="6"/>
<connect gate="A" pin="SW" pad="4"/>
<connect gate="A" pin="VIN" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2585S-3.3"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K3724"/>
<attribute name="PACKAGE" value="TO-263-5"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2585S-5.0" prefix="U">
<description>FLYBACK REGULATOR</description>
<gates>
<gate name="A" symbol="LM2585S-5.0"/>
</gates>
<devices>
<device name="" package="TO170P1435X457-5N">
<connects>
<connect gate="A" pin="COMP" pad="1"/>
<connect gate="A" pin="FB" pad="2"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="GND_2" pad="6"/>
<connect gate="A" pin="SW" pad="4"/>
<connect gate="A" pin="VIN" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2585S-5.0"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="07B6060"/>
<attribute name="PACKAGE" value="TO-263-5"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2585S-ADJ" prefix="U">
<description>FLYBACK REGULATOR</description>
<gates>
<gate name="A" symbol="LM2585S-ADJ"/>
</gates>
<devices>
<device name="" package="TO170P1435X457-5N">
<connects>
<connect gate="A" pin="COMP" pad="1"/>
<connect gate="A" pin="FB" pad="2"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="GND_2" pad="6"/>
<connect gate="A" pin="SW" pad="4"/>
<connect gate="A" pin="VIN" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2585S-ADJ"/>
<attribute name="OC_FARNELL" value="1469182"/>
<attribute name="OC_NEWARK" value="41K3722"/>
<attribute name="PACKAGE" value="TO-263-5"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2585T-3.3" prefix="U">
<description>C, FLYBACK REGULATOR</description>
<gates>
<gate name="A" symbol="LM2585T-3.3"/>
</gates>
<devices>
<device name="" package="TO170P470X1016X2092-5P">
<connects>
<connect gate="A" pin="COMP" pad="1"/>
<connect gate="A" pin="FEEDBACK" pad="2"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="SWITCH" pad="4"/>
<connect gate="A" pin="VIN" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2585T-3.3"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K3732"/>
<attribute name="PACKAGE" value="TO220-5"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2585T-5.0" prefix="U">
<description>IC, FLYBACK REGULATOR</description>
<gates>
<gate name="A" symbol="LM2585T-5.0"/>
</gates>
<devices>
<device name="" package="TO170P470X1016X2092-5P">
<connects>
<connect gate="A" pin="COMP" pad="1"/>
<connect gate="A" pin="FEEDBACK" pad="2"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="SWITCH" pad="4"/>
<connect gate="A" pin="VIN" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2585T-5.0"/>
<attribute name="OC_FARNELL" value="1564633"/>
<attribute name="OC_NEWARK" value="41K3733"/>
<attribute name="PACKAGE" value="TO220-5"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2585T-ADJ" prefix="U">
<description>IC, FLYBACK REGULATOR</description>
<gates>
<gate name="A" symbol="LM2585T-ADJ"/>
</gates>
<devices>
<device name="" package="TO170P470X1016X2092-5P">
<connects>
<connect gate="A" pin="COMP" pad="1"/>
<connect gate="A" pin="FEEDBACK" pad="2"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="SWITCH" pad="4"/>
<connect gate="A" pin="VIN" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2585T-ADJ"/>
<attribute name="OC_FARNELL" value="9494324"/>
<attribute name="OC_NEWARK" value="41K3730"/>
<attribute name="PACKAGE" value="TO220-5"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2586S-5.0" prefix="U">
<description>SIMPLE SWITCHER</description>
<gates>
<gate name="A" symbol="LM2586S-5.0"/>
</gates>
<devices>
<device name="" package="TO127P1435X457-7N">
<connects>
<connect gate="A" pin="COMP" pad="2"/>
<connect gate="A" pin="FB" pad="3"/>
<connect gate="A" pin="FREQ.ADJ._ON/~OFF" pad="1"/>
<connect gate="A" pin="FREQ_SYNC" pad="6"/>
<connect gate="A" pin="GND" pad="8"/>
<connect gate="A" pin="GND_2" pad="4"/>
<connect gate="A" pin="SWITCH" pad="5"/>
<connect gate="A" pin="VIN" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2586S-50"/>
<attribute name="OC_FARNELL" value="1685568"/>
<attribute name="OC_NEWARK" value="41K3737"/>
<attribute name="PACKAGE" value="TO-263-7"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2586S-ADJ" prefix="U">
<description>Flyback Regulator</description>
<gates>
<gate name="A" symbol="LM2586S-ADJ"/>
</gates>
<devices>
<device name="" package="TO127P1435X457-8N">
<connects>
<connect gate="A" pin="COMP" pad="2"/>
<connect gate="A" pin="FB" pad="3"/>
<connect gate="A" pin="FREQ_ADJ_OR_ON/~OFF" pad="1"/>
<connect gate="A" pin="FREQ_SYNC" pad="6"/>
<connect gate="A" pin="GND" pad="8"/>
<connect gate="A" pin="GND_2" pad="4"/>
<connect gate="A" pin="SW" pad="5"/>
<connect gate="A" pin="VIN" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2586S-ADJ"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="07B6069"/>
<attribute name="PACKAGE" value="TO-263-7"/>
<attribute name="SUPPLIER" value="NATIONAL SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2586T-3.3" prefix="U">
<description>IC MULTI CONFIG 3.3V 3A</description>
<gates>
<gate name="A" symbol="LM2586T-3.3"/>
</gates>
<devices>
<device name="" package="TO127P469X1016X2102-7P">
<connects>
<connect gate="A" pin="COMP" pad="2"/>
<connect gate="A" pin="FEEDBACK" pad="3"/>
<connect gate="A" pin="FREQ_ADJ_OR_ON/~OFF" pad="1"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="SWITCH" pad="5"/>
<connect gate="A" pin="SYNC" pad="6"/>
<connect gate="A" pin="VIN" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2586T-33"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K3744"/>
<attribute name="PACKAGE" value="TO220-7"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2586T-5.0" prefix="U">
<description>IC MULTI CONFIG 5V 3A</description>
<gates>
<gate name="A" symbol="LM2586T-5.0"/>
</gates>
<devices>
<device name="" package="TO127P469X1016X2102-7P">
<connects>
<connect gate="A" pin="COMP" pad="2"/>
<connect gate="A" pin="FEEDBACK" pad="3"/>
<connect gate="A" pin="FREQ_ADJ_OR_ON/~OFF" pad="1"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="SWITCH" pad="5"/>
<connect gate="A" pin="SYNC" pad="6"/>
<connect gate="A" pin="VIN" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2586T-5.0"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K3745"/>
<attribute name="PACKAGE" value="TO220-7"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2586T-ADJ" prefix="U">
<description>IC MULTI CONFIG ADJ 3A</description>
<gates>
<gate name="A" symbol="LM2586T-ADJ"/>
</gates>
<devices>
<device name="" package="TO127P469X1016X2102-7P">
<connects>
<connect gate="A" pin="COMP" pad="2"/>
<connect gate="A" pin="FEEDBACK" pad="3"/>
<connect gate="A" pin="FREQ_ADJ_OR_ON/~OFF" pad="1"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="SWITCH" pad="5"/>
<connect gate="A" pin="SYNC" pad="6"/>
<connect gate="A" pin="VIN" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2586T-ADJ"/>
<attribute name="OC_FARNELL" value="1564732"/>
<attribute name="OC_NEWARK" value="41K3742"/>
<attribute name="PACKAGE" value="TO220-7"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2587S-3.3" prefix="U">
<description>SIMPLE SWITCHER</description>
<gates>
<gate name="A" symbol="LM2587S-3.3"/>
</gates>
<devices>
<device name="" package="TO170P1435X457-5N">
<connects>
<connect gate="A" pin="FB" pad="4"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="GND_2" pad="6"/>
<connect gate="A" pin="OUT" pad="2"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="~ON/OFF" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2591HVS-3.3"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K3781"/>
<attribute name="PACKAGE" value="TO-263-5"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2587S-5.0" prefix="U">
<description>Flyback Regulator</description>
<gates>
<gate name="A" symbol="LM2587S-5.0"/>
</gates>
<devices>
<device name="" package="TO170P1435X457-6N">
<connects>
<connect gate="A" pin="COMP" pad="1"/>
<connect gate="A" pin="FB" pad="2"/>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="GND_2" pad="3"/>
<connect gate="A" pin="SW" pad="4"/>
<connect gate="A" pin="VIN" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2587S-5.0"/>
<attribute name="OC_FARNELL" value="9493689"/>
<attribute name="OC_NEWARK" value="38K3638"/>
<attribute name="PACKAGE" value="TO-263-5"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2587S-ADJ" prefix="U">
<description>Flyback Regulator</description>
<gates>
<gate name="A" symbol="LM2587S-ADJ"/>
</gates>
<devices>
<device name="" package="TO170P1435X457-6N">
<connects>
<connect gate="A" pin="COMP" pad="1"/>
<connect gate="A" pin="FB" pad="2"/>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="GND_2" pad="3"/>
<connect gate="A" pin="SW" pad="4"/>
<connect gate="A" pin="VIN" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2587S-ADJ"/>
<attribute name="OC_FARNELL" value="9493697"/>
<attribute name="OC_NEWARK" value="07B6081"/>
<attribute name="PACKAGE" value="TO-263-5"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2587T-12" prefix="U">
<description>IC MULTI CONFIG 12V 5A</description>
<gates>
<gate name="A" symbol="LM2587T-12"/>
</gates>
<devices>
<device name="" package="TO170P470X1016X2092-5P">
<connects>
<connect gate="A" pin="COMP" pad="1"/>
<connect gate="A" pin="FB" pad="2"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="SW" pad="4"/>
<connect gate="A" pin="VIN" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2587T-12"/>
<attribute name="OC_FARNELL" value="1685487"/>
<attribute name="OC_NEWARK" value="41K3755"/>
<attribute name="PACKAGE" value="TO220-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2587T-3.3" prefix="U">
<description>IC MULTI CONFIG 3.3V 5A</description>
<gates>
<gate name="A" symbol="LM2587T-3.3"/>
</gates>
<devices>
<device name="" package="TO170P470X1016X2092-5P">
<connects>
<connect gate="A" pin="COMP" pad="1"/>
<connect gate="A" pin="FB" pad="2"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="SW" pad="4"/>
<connect gate="A" pin="VIN" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2587T-3.3"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K3756"/>
<attribute name="PACKAGE" value="TO220-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2587T-5.0" prefix="U">
<description>SWITCHING REG 5A 5.0V, 2587</description>
<gates>
<gate name="A" symbol="LM2587T-5.0"/>
</gates>
<devices>
<device name="" package="TO170P470X1016X2092-5P">
<connects>
<connect gate="A" pin="COMP" pad="1"/>
<connect gate="A" pin="FB" pad="2"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="SW" pad="4"/>
<connect gate="A" pin="VIN" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2587T-5.0"/>
<attribute name="OC_FARNELL" value="9493573"/>
<attribute name="OC_NEWARK" value="38K3639"/>
<attribute name="PACKAGE" value="TO220-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2587T-ADJ" prefix="U">
<description>IC, FLYBACK REGULATOR</description>
<gates>
<gate name="A" symbol="LM2587T-ADJ"/>
</gates>
<devices>
<device name="" package="TO170P470X1016X2092-5P">
<connects>
<connect gate="A" pin="COMP" pad="1"/>
<connect gate="A" pin="FB" pad="2"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="SW" pad="4"/>
<connect gate="A" pin="VIN" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2587T-ADJ"/>
<attribute name="OC_FARNELL" value="1564716"/>
<attribute name="OC_NEWARK" value="41K3754"/>
<attribute name="PACKAGE" value="TO220-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2588S-12" prefix="U">
<description>SIMPLE SWITCHER</description>
<gates>
<gate name="A" symbol="LM2588S-12"/>
</gates>
<devices>
<device name="" package="TO127P1435X457-7N">
<connects>
<connect gate="A" pin="COMP" pad="2"/>
<connect gate="A" pin="FB" pad="3"/>
<connect gate="A" pin="FREQ.ADJ._ON/~OFF" pad="1"/>
<connect gate="A" pin="FREQ_SYNC" pad="6"/>
<connect gate="A" pin="GND" pad="8"/>
<connect gate="A" pin="GND_2" pad="4"/>
<connect gate="A" pin="SWITCH" pad="5"/>
<connect gate="A" pin="VIN" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2588S-12"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="07B6094"/>
<attribute name="PACKAGE" value="TO-263-7"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2588S-5.0" prefix="U">
<description>SIMPLE SWITCHER</description>
<gates>
<gate name="A" symbol="LM2588S-5.0"/>
</gates>
<devices>
<device name="" package="TO127P1435X457-7N">
<connects>
<connect gate="A" pin="COMP" pad="2"/>
<connect gate="A" pin="FB" pad="3"/>
<connect gate="A" pin="FREQ.ADJ._ON/~OFF" pad="1"/>
<connect gate="A" pin="FREQ_SYNC" pad="6"/>
<connect gate="A" pin="GND" pad="8"/>
<connect gate="A" pin="GND_2" pad="4"/>
<connect gate="A" pin="SWITCH" pad="5"/>
<connect gate="A" pin="VIN" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2588S-5.0"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K3761"/>
<attribute name="PACKAGE" value="TO-263-7"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2588S-ADJ" prefix="U">
<description>SIMPLE SWITCHER</description>
<gates>
<gate name="A" symbol="LM2588S-ADJ"/>
</gates>
<devices>
<device name="" package="TO127P1435X457-7N">
<connects>
<connect gate="A" pin="COMP" pad="2"/>
<connect gate="A" pin="FB" pad="3"/>
<connect gate="A" pin="FREQ.ADJ._ON/~OFF" pad="1"/>
<connect gate="A" pin="FREQ_SYNC" pad="6"/>
<connect gate="A" pin="GND" pad="8"/>
<connect gate="A" pin="GND_2" pad="4"/>
<connect gate="A" pin="SWITCH" pad="5"/>
<connect gate="A" pin="VIN" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2588S-ADJ"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="07B6093"/>
<attribute name="PACKAGE" value="TO-263-7"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2588T-5.0" prefix="U">
<description>IC, FLYBACK REGULATOR</description>
<gates>
<gate name="A" symbol="LM2588T-5.0"/>
</gates>
<devices>
<device name="" package="TO127P457X1016X2052-7P">
<connects>
<connect gate="A" pin="COMPENSATION" pad="2"/>
<connect gate="A" pin="FB" pad="3"/>
<connect gate="A" pin="FRQ-ADJ-ON/OFF" pad="1"/>
<connect gate="A" pin="FRQ-SYNC" pad="6"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="SWITCH" pad="5"/>
<connect gate="A" pin="VIN" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2588T-5.0"/>
<attribute name="OC_FARNELL" value="9493778"/>
<attribute name="OC_NEWARK" value="07B6104"/>
<attribute name="PACKAGE" value="TO-220-7"/>
<attribute name="SUPPLIER" value="NATIONAL SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2588T-ADJ" prefix="U">
<description>IC, FLYBACK REGULATOR</description>
<gates>
<gate name="A" symbol="LM2588T-ADJ"/>
</gates>
<devices>
<device name="" package="TO127P457X1016X2052-7P">
<connects>
<connect gate="A" pin="COMPENSATION" pad="2"/>
<connect gate="A" pin="FB" pad="3"/>
<connect gate="A" pin="FRQ-ADJ-ON/OFF" pad="1"/>
<connect gate="A" pin="FRQ-SYNC" pad="6"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="SWITCH" pad="5"/>
<connect gate="A" pin="VIN" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2588T-ADJ"/>
<attribute name="OC_FARNELL" value="9493719"/>
<attribute name="OC_NEWARK" value="41K3766"/>
<attribute name="PACKAGE" value="TO-220-7"/>
<attribute name="SUPPLIER" value="NATIONAL SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM258H" prefix="U">
<description>IC OP AMP DUAL</description>
<gates>
<gate name="A" symbol="LM258H"/>
</gates>
<devices>
<device name="" package="TO254P914X470-8P">
<connects>
<connect gate="A" pin="+INA" pad="3"/>
<connect gate="A" pin="+INB" pad="5"/>
<connect gate="A" pin="-INA" pad="2"/>
<connect gate="A" pin="-INB" pad="6"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM258H"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="31T9908"/>
<attribute name="PACKAGE" value="TO-99-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2590HVS-3.3" prefix="U">
<description>SIMPLE SWITCHER</description>
<gates>
<gate name="A" symbol="LM2590HVS-3.3"/>
</gates>
<devices>
<device name="" package="TO127P1435X457-7N">
<connects>
<connect gate="A" pin="DELAY" pad="5"/>
<connect gate="A" pin="FB" pad="6"/>
<connect gate="A" pin="FLAG" pad="3"/>
<connect gate="A" pin="GND" pad="8"/>
<connect gate="A" pin="GND_2" pad="4"/>
<connect gate="A" pin="OUT" pad="2"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="~SD/SS" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2590HVS-3.3"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K3771"/>
<attribute name="PACKAGE" value="TO-263-7"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2590HVS-5.0" prefix="U">
<description>SIMPLE SWITCHER</description>
<gates>
<gate name="A" symbol="LM2590HVS-5.0"/>
</gates>
<devices>
<device name="" package="TO127P1435X457-7N">
<connects>
<connect gate="A" pin="DELAY" pad="5"/>
<connect gate="A" pin="FB" pad="6"/>
<connect gate="A" pin="FLAG" pad="3"/>
<connect gate="A" pin="GND" pad="8"/>
<connect gate="A" pin="GND_2" pad="4"/>
<connect gate="A" pin="OUT" pad="2"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="~SD/SS" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2590HVS-3.3"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K3772"/>
<attribute name="PACKAGE" value="TO-263-7"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2590HVS-ADJ" prefix="U">
<description>SIMPLE SWITCHER</description>
<gates>
<gate name="A" symbol="LM2590HVS-ADJ"/>
</gates>
<devices>
<device name="" package="TO127P1435X457-7N">
<connects>
<connect gate="A" pin="DELAY" pad="5"/>
<connect gate="A" pin="FB" pad="6"/>
<connect gate="A" pin="FLAG" pad="3"/>
<connect gate="A" pin="GND" pad="8"/>
<connect gate="A" pin="GND_2" pad="4"/>
<connect gate="A" pin="OUT" pad="2"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="~SD/SS" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2590HVS-ADJ"/>
<attribute name="OC_FARNELL" value="1286837"/>
<attribute name="OC_NEWARK" value="26M0322"/>
<attribute name="PACKAGE" value="TO-263-7"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2590HVT-3.3" prefix="U">
<description>IC BUCK 3.3V 1A</description>
<gates>
<gate name="A" symbol="LM2590HVT-3.3"/>
</gates>
<devices>
<device name="" package="TO127P470X1016X1740-7P">
<connects>
<connect gate="A" pin="*SD-SS" pad="7"/>
<connect gate="A" pin="DELAY" pad="5"/>
<connect gate="A" pin="FEEDBACK" pad="6"/>
<connect gate="A" pin="FLAG" pad="3"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="OUTPUT" pad="2"/>
<connect gate="A" pin="VIN" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2590HVT-3.3"/>
<attribute name="OC_FARNELL" value="9489495"/>
<attribute name="OC_NEWARK" value="34C6478"/>
<attribute name="PACKAGE" value="TO220-7"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2590HVT-5.0" prefix="U">
<description>IC BUCK 5V 1A</description>
<gates>
<gate name="A" symbol="LM2590HVT-5.0"/>
</gates>
<devices>
<device name="" package="TO127P470X1016X1740-7P">
<connects>
<connect gate="A" pin="*SD-SS" pad="7"/>
<connect gate="A" pin="DELAY" pad="5"/>
<connect gate="A" pin="FEEDBACK" pad="6"/>
<connect gate="A" pin="FLAG" pad="3"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="OUTPUT" pad="2"/>
<connect gate="A" pin="VIN" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2590HVT-5.0"/>
<attribute name="OC_FARNELL" value="9489509"/>
<attribute name="OC_NEWARK" value="34C6479"/>
<attribute name="PACKAGE" value="TO220-7"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2590HVT-ADJ" prefix="U">
<description>IC BUCK ADJ 1A</description>
<gates>
<gate name="A" symbol="LM2590HVT-ADJ"/>
</gates>
<devices>
<device name="" package="TO127P470X1016X1740-7P">
<connects>
<connect gate="A" pin="*SD-SS" pad="7"/>
<connect gate="A" pin="DELAY" pad="5"/>
<connect gate="A" pin="FEEDBACK" pad="6"/>
<connect gate="A" pin="FLAG" pad="3"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="OUTPUT" pad="2"/>
<connect gate="A" pin="VIN" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2590HVT-ADJ"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="34C6477"/>
<attribute name="PACKAGE" value="TO220-7"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2591HVS-3.3" prefix="U">
<description>SIMPLE SWITCHER</description>
<gates>
<gate name="A" symbol="LM2591HVS-3.3"/>
</gates>
<devices>
<device name="" package="TO170P1435X457-5N">
<connects>
<connect gate="A" pin="FB" pad="4"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="GND_2" pad="6"/>
<connect gate="A" pin="OUT" pad="2"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="~ON/OFF" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2591HVS-3.3"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K3781"/>
<attribute name="PACKAGE" value="TO-263-5"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2591HVS-5.0" prefix="U">
<description>SIMPLE SWITCHER</description>
<gates>
<gate name="A" symbol="LM2591HVS-5.0"/>
</gates>
<devices>
<device name="" package="TO170P1435X457-5N">
<connects>
<connect gate="A" pin="FB" pad="4"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="GND_2" pad="6"/>
<connect gate="A" pin="OUT" pad="2"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="~ON/OFF" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2591HVS-5.0"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K3782"/>
<attribute name="PACKAGE" value="TO-263-5"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2591HVS-ADJ" prefix="U">
<description>SIMPLE SWITCHER</description>
<gates>
<gate name="A" symbol="LM2591HVS-ADJ"/>
</gates>
<devices>
<device name="" package="TO170P1435X457-5N">
<connects>
<connect gate="A" pin="FB" pad="4"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="GND_2" pad="6"/>
<connect gate="A" pin="OUT" pad="2"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="~ON/OFF" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2591HVS-ADJ"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K3780"/>
<attribute name="PACKAGE" value="TO-263-5"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2591HVT-3.3" prefix="U">
<description>IC BUCK 3.3V 1AO</description>
<gates>
<gate name="A" symbol="LM2591HVT-3.3"/>
</gates>
<devices>
<device name="" package="TO170P470X1016X2092-5P">
<connects>
<connect gate="A" pin="*ON-OFF" pad="5"/>
<connect gate="A" pin="FEEDBACK" pad="4"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="OUTPUT" pad="2"/>
<connect gate="A" pin="VIN" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2591HVT-3.3"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K3787"/>
<attribute name="PACKAGE" value="TO220-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2591HVT-5.0" prefix="U">
<description>SWITCHING REG 1A 5.0V, 2591</description>
<gates>
<gate name="A" symbol="LM2591HVT-5.0"/>
</gates>
<devices>
<device name="" package="TO170P470X1016X2092-5P">
<connects>
<connect gate="A" pin="FB" pad="4"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="OUTPUT" pad="2"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="~ON~/OFF" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2591HVT-5.0"/>
<attribute name="OC_FARNELL" value="9489533"/>
<attribute name="OC_NEWARK" value="97K3243"/>
<attribute name="PACKAGE" value="TO-220-5"/>
<attribute name="SUPPLIER" value="NATIONAL SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2591HVT-ADJ" prefix="U">
<description>IC, STEP-DOWN REGULATOR</description>
<gates>
<gate name="A" symbol="LM2591HVT-ADJ"/>
</gates>
<devices>
<device name="" package="TO170P470X1016X2092-5P">
<connects>
<connect gate="A" pin="FB" pad="4"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="OUTPUT" pad="2"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="~ON~/OFF" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2591HVT-ADJ"/>
<attribute name="OC_FARNELL" value="9489541"/>
<attribute name="OC_NEWARK" value="41K3786"/>
<attribute name="PACKAGE" value="TO-220-5"/>
<attribute name="SUPPLIER" value="NATIONAL SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2592HVS-3.3" prefix="U">
<description>SIMPLE SWITCHER</description>
<gates>
<gate name="A" symbol="LM2592HVS-3.3"/>
</gates>
<devices>
<device name="" package="TO170P1435X457-5N">
<connects>
<connect gate="A" pin="FB" pad="4"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="GND_2" pad="6"/>
<connect gate="A" pin="OUT" pad="2"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="~ON/OFF" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2592HVS-3.3"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K3790"/>
<attribute name="PACKAGE" value="TO-263-5"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2592HVS-5.0" prefix="U">
<description>SIMPLE SWITCHER</description>
<gates>
<gate name="A" symbol="LM2592HVS-5.0"/>
</gates>
<devices>
<device name="" package="TO170P1435X457-5N">
<connects>
<connect gate="A" pin="FB" pad="4"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="GND_2" pad="6"/>
<connect gate="A" pin="OUT" pad="2"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="~ON/OFF" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2592HVS-5.0"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K3791"/>
<attribute name="PACKAGE" value="TO-263-5"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2592HVS-ADJ" prefix="U">
<description>SIMPLE SWITCHER®Power Converter</description>
<gates>
<gate name="A" symbol="LM2592HVS-ADJ"/>
</gates>
<devices>
<device name="" package="TO170P1435X457-6N">
<connects>
<connect gate="A" pin="FB" pad="4"/>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="GND_2" pad="3"/>
<connect gate="A" pin="OUT" pad="2"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="~ON/OFF" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MANUFACTURER_PART_NUMBER" value="LM2592HVS-ADJ"/>
<attribute name="OC_FARNELL" value="4102459"/>
<attribute name="OC_NEWARK" value="41K3789"/>
<attribute name="PACKAGE" value="TO-263-5"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2592HVT-3.3" prefix="U">
<description>IC, STEP-DOWN REGULATOR</description>
<gates>
<gate name="A" symbol="LM2592HVT-3.3"/>
</gates>
<devices>
<device name="" package="TO170P470X1016X2092-5P">
<connects>
<connect gate="A" pin="FB" pad="4"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="OUTPUT" pad="2"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="~ON~/OFF" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2592HVT-3.3"/>
<attribute name="OC_FARNELL" value="9489550"/>
<attribute name="OC_NEWARK" value="41K3796"/>
<attribute name="PACKAGE" value="TO-220-5"/>
<attribute name="SUPPLIER" value="NATIONAL SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2592HVT-5.0" prefix="U">
<description>IC, STEP-DOWN REGULATOR</description>
<gates>
<gate name="A" symbol="LM2592HVT-5.0"/>
</gates>
<devices>
<device name="" package="TO170P470X1016X2092-5P">
<connects>
<connect gate="A" pin="FB" pad="4"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="OUTPUT" pad="2"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="~ON~/OFF" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2592HVT-5.0"/>
<attribute name="OC_FARNELL" value="9489576"/>
<attribute name="OC_NEWARK" value="41K3797"/>
<attribute name="PACKAGE" value="TO-220-5"/>
<attribute name="SUPPLIER" value="NATIONAL SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2592HVT-ADJ" prefix="U">
<description>IC, STEP-DOWN REGULATOR</description>
<gates>
<gate name="A" symbol="LM2592HVT-ADJ"/>
</gates>
<devices>
<device name="" package="TO170P470X1016X2092-5P">
<connects>
<connect gate="A" pin="FB" pad="4"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="OUTPUT" pad="2"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="~ON~/OFF" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2592HVT-ADJ"/>
<attribute name="OC_FARNELL" value="9489584"/>
<attribute name="OC_NEWARK" value="41K3795"/>
<attribute name="PACKAGE" value="TO-220-5"/>
<attribute name="SUPPLIER" value="NATIONAL SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2593HVS-3.3" prefix="U">
<description>SIMPLE SWITCHER</description>
<gates>
<gate name="A" symbol="LM2593HVS-3.3"/>
</gates>
<devices>
<device name="" package="TO127O1435X465-7N">
<connects>
<connect gate="A" pin="DELAY" pad="5"/>
<connect gate="A" pin="FB" pad="6"/>
<connect gate="A" pin="FLAG" pad="3"/>
<connect gate="A" pin="GND" pad="8"/>
<connect gate="A" pin="GND_2" pad="4"/>
<connect gate="A" pin="OUT" pad="2"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="~SD/SS" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2593HVS-3.3"/>
<attribute name="OC_FARNELL" value="1564634"/>
<attribute name="OC_NEWARK" value="34C6499"/>
<attribute name="PACKAGE" value="TO-263-7"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2593HVS-5.0" prefix="U">
<description>SIMPLE SWITCHER</description>
<gates>
<gate name="A" symbol="LM2593HVS-5.0"/>
</gates>
<devices>
<device name="" package="TO127O1435X465-7N">
<connects>
<connect gate="A" pin="DELAY" pad="5"/>
<connect gate="A" pin="FB" pad="6"/>
<connect gate="A" pin="FLAG" pad="3"/>
<connect gate="A" pin="GND" pad="8"/>
<connect gate="A" pin="GND_2" pad="4"/>
<connect gate="A" pin="OUT" pad="2"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="~SD/SS" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2593HVS-5.0"/>
<attribute name="OC_FARNELL" value="1469188"/>
<attribute name="OC_NEWARK" value="41K3800"/>
<attribute name="PACKAGE" value="TO-263-7"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2593HVS-ADJ" prefix="U">
<description>SIMPLE SWITCHER</description>
<gates>
<gate name="A" symbol="LM2593HVS-ADJ"/>
</gates>
<devices>
<device name="" package="TO127O1435X465-7N">
<connects>
<connect gate="A" pin="DELAY" pad="5"/>
<connect gate="A" pin="FB" pad="6"/>
<connect gate="A" pin="FLAG" pad="3"/>
<connect gate="A" pin="GND" pad="8"/>
<connect gate="A" pin="GND_2" pad="4"/>
<connect gate="A" pin="OUT" pad="2"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="~SD/SS" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2593HVS-ADJ"/>
<attribute name="OC_FARNELL" value="1469188"/>
<attribute name="OC_NEWARK" value="41K3800"/>
<attribute name="PACKAGE" value="TO-263-7"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2593HVT-3.3" prefix="U">
<description>IC BUCK 3.3V 2A</description>
<gates>
<gate name="A" symbol="LM2593HVT-3.3"/>
</gates>
<devices>
<device name="" package="TO127P470X1016X1740-7P">
<connects>
<connect gate="A" pin="*SD-SS" pad="7"/>
<connect gate="A" pin="DELAY" pad="5"/>
<connect gate="A" pin="FEEDBACK" pad="6"/>
<connect gate="A" pin="FLAG" pad="3"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="OUTPUT" pad="2"/>
<connect gate="A" pin="VIN" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2593HVT-3.3"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K3805"/>
<attribute name="PACKAGE" value="TO220-7"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2593HVT-5.0" prefix="U">
<description>IC BUCK 5V 2A</description>
<gates>
<gate name="A" symbol="LM2593HVT-5.0"/>
</gates>
<devices>
<device name="" package="TO127P470X1016X1740-7P">
<connects>
<connect gate="A" pin="*SD-SS" pad="7"/>
<connect gate="A" pin="DELAY" pad="5"/>
<connect gate="A" pin="FEEDBACK" pad="6"/>
<connect gate="A" pin="FLAG" pad="3"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="OUTPUT" pad="2"/>
<connect gate="A" pin="VIN" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2593HVT-5.0"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="34C6506"/>
<attribute name="PACKAGE" value="TO220-7"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2593HVT-ADJ" prefix="U">
<description>IC BUCK ADJ 2A</description>
<gates>
<gate name="A" symbol="LM2593HVT-ADJ"/>
</gates>
<devices>
<device name="" package="TO127P470X1016X1740-7P">
<connects>
<connect gate="A" pin="*SD-SS" pad="7"/>
<connect gate="A" pin="DELAY" pad="5"/>
<connect gate="A" pin="FEEDBACK" pad="6"/>
<connect gate="A" pin="FLAG" pad="3"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="OUTPUT" pad="2"/>
<connect gate="A" pin="VIN" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2593HVT-ADJ"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="34C6504"/>
<attribute name="PACKAGE" value="TO220-7"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2594HVM-12" prefix="U">
<description>SIMPLE SWITCHER® Power Converter</description>
<gates>
<gate name="A" symbol="LM2594HVM-12"/>
</gates>
<devices>
<device name="" package="SOIC127P620X175-8N">
<connects>
<connect gate="A" pin="FB" pad="4"/>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="NC" pad="3"/>
<connect gate="A" pin="NC_2" pad="1"/>
<connect gate="A" pin="NC_3" pad="2"/>
<connect gate="A" pin="OUTPUT" pad="8"/>
<connect gate="A" pin="VIN" pad="7"/>
<connect gate="A" pin="~ON/OFF" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2594HVM-12"/>
<attribute name="OC_FARNELL" value="1495089"/>
<attribute name="OC_NEWARK" value="41K3808"/>
<attribute name="PACKAGE" value="8-SOIC"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2594HVM-3.3" prefix="U">
<description>SIMPLE SWITCHER</description>
<gates>
<gate name="A" symbol="LM2594HVM-3.3"/>
</gates>
<devices>
<device name="" package="SOIC127P620X175-8N">
<connects>
<connect gate="A" pin="FB" pad="4"/>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="NC" pad="3"/>
<connect gate="A" pin="NC_2" pad="1"/>
<connect gate="A" pin="NC_3" pad="2"/>
<connect gate="A" pin="OUT" pad="8"/>
<connect gate="A" pin="VIN" pad="7"/>
<connect gate="A" pin="~ON~/OFF" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2594HVM-33"/>
<attribute name="OC_FARNELL" value="1564635"/>
<attribute name="OC_NEWARK" value="41K3809"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2594HVM-5.0" prefix="U">
<description>SIMPLE SWITCHER</description>
<gates>
<gate name="A" symbol="LM2594HVM-5.0"/>
</gates>
<devices>
<device name="" package="SOIC127P620X175-8N">
<connects>
<connect gate="A" pin="FB" pad="4"/>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="NC" pad="3"/>
<connect gate="A" pin="NC_2" pad="1"/>
<connect gate="A" pin="NC_3" pad="2"/>
<connect gate="A" pin="OUT" pad="8"/>
<connect gate="A" pin="VIN" pad="7"/>
<connect gate="A" pin="~ON~/OFF" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2594HVM-5.0"/>
<attribute name="OC_FARNELL" value="1469190"/>
<attribute name="OC_NEWARK" value="41K3810"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2594HVM-ADJ" prefix="U">
<description>Voltage Regulator</description>
<gates>
<gate name="A" symbol="LM2594HVM-ADJ"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="FB" pad="4"/>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="NC" pad="3"/>
<connect gate="A" pin="NC_2" pad="1"/>
<connect gate="A" pin="NC_3" pad="2"/>
<connect gate="A" pin="OUT" pad="8"/>
<connect gate="A" pin="VIN" pad="7"/>
<connect gate="A" pin="~ON/OFF" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2594HVM-ADJ"/>
<attribute name="OC_FARNELL" value="4210049"/>
<attribute name="OC_NEWARK" value="41K3807"/>
<attribute name="PACKAGE" value="8-SOIC"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2594HVN-12" prefix="U">
<description>SIMPLE SWITCHER</description>
<gates>
<gate name="A" symbol="LM2594HVN-12"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-8">
<connects>
<connect gate="A" pin="FB" pad="4"/>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="NC" pad="3"/>
<connect gate="A" pin="NC_2" pad="1"/>
<connect gate="A" pin="NC_3" pad="2"/>
<connect gate="A" pin="OUT" pad="8"/>
<connect gate="A" pin="VIN" pad="7"/>
<connect gate="A" pin="~ON~/OFF" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2594HVN-12"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="13B5550"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2594HVN-3.3" prefix="U">
<description>SIMPLE SWITCHER</description>
<gates>
<gate name="A" symbol="LM2594HVN-3.3"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-8">
<connects>
<connect gate="A" pin="FB" pad="4"/>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="NC" pad="3"/>
<connect gate="A" pin="NC_2" pad="1"/>
<connect gate="A" pin="NC_3" pad="2"/>
<connect gate="A" pin="OUT" pad="8"/>
<connect gate="A" pin="VIN" pad="7"/>
<connect gate="A" pin="~ON~/OFF" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2594HVN-3.3"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="13B5551"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2594HVN-5.0" prefix="U">
<description>SIMPLE SWITCHER</description>
<gates>
<gate name="A" symbol="LM2594HVN-5.0"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-8">
<connects>
<connect gate="A" pin="FB" pad="4"/>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="NC" pad="3"/>
<connect gate="A" pin="NC_2" pad="1"/>
<connect gate="A" pin="NC_3" pad="2"/>
<connect gate="A" pin="OUT" pad="8"/>
<connect gate="A" pin="VIN" pad="7"/>
<connect gate="A" pin="~ON~/OFF" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2594HVN-5.0"/>
<attribute name="OC_FARNELL" value="1469191"/>
<attribute name="OC_NEWARK" value="41K3818"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2594HVN-ADJ" prefix="U">
<description>SIMPLE SWITCHER</description>
<gates>
<gate name="A" symbol="LM2594HVN-ADJ"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-8">
<connects>
<connect gate="A" pin="FB" pad="4"/>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="NC" pad="3"/>
<connect gate="A" pin="NC_2" pad="1"/>
<connect gate="A" pin="NC_3" pad="2"/>
<connect gate="A" pin="OUT" pad="8"/>
<connect gate="A" pin="VIN" pad="7"/>
<connect gate="A" pin="~ON~/OFF" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2594HVN-ADJ"/>
<attribute name="OC_FARNELL" value="1211794"/>
<attribute name="OC_NEWARK" value="41K3815"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2594M-12" prefix="U">
<description>SIMPLE SWITCHER</description>
<gates>
<gate name="A" symbol="LM2594M-12"/>
</gates>
<devices>
<device name="" package="SOIC127P620X175-8N">
<connects>
<connect gate="A" pin="FB" pad="4"/>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="NC" pad="3"/>
<connect gate="A" pin="NC_2" pad="1"/>
<connect gate="A" pin="NC_3" pad="2"/>
<connect gate="A" pin="OUT" pad="8"/>
<connect gate="A" pin="VIN" pad="7"/>
<connect gate="A" pin="~ON~/OFF" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2594M-12"/>
<attribute name="OC_FARNELL" value="1850240"/>
<attribute name="OC_NEWARK" value="41K3820"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2594M-3.3" prefix="U">
<description>SIMPLE SWITCHER® Power Converter</description>
<gates>
<gate name="A" symbol="LM2594M-3.3"/>
</gates>
<devices>
<device name="" package="SOIC127P620X175-8N">
<connects>
<connect gate="A" pin="FB" pad="4"/>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="NC" pad="3"/>
<connect gate="A" pin="NC_2" pad="1"/>
<connect gate="A" pin="NC_3" pad="2"/>
<connect gate="A" pin="ON/OFF" pad="5"/>
<connect gate="A" pin="OUT" pad="8"/>
<connect gate="A" pin="VIN" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2594M-3.3"/>
<attribute name="OC_FARNELL" value="1215200"/>
<attribute name="OC_NEWARK" value="41K3821"/>
<attribute name="PACKAGE" value="8-SOIC"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2594M-5.0" prefix="U">
<description>SIMPLE SWITCHER® Power Converter</description>
<gates>
<gate name="A" symbol="LM2594M-5.0"/>
</gates>
<devices>
<device name="" package="SOIC127P620X175-8N">
<connects>
<connect gate="A" pin="FB" pad="4"/>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="NC" pad="3"/>
<connect gate="A" pin="NC_2" pad="1"/>
<connect gate="A" pin="NC_3" pad="2"/>
<connect gate="A" pin="ON/OFF" pad="5"/>
<connect gate="A" pin="OUT" pad="8"/>
<connect gate="A" pin="VIN" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2594M-5.0"/>
<attribute name="OC_FARNELL" value="9779841"/>
<attribute name="OC_NEWARK" value="07B6108"/>
<attribute name="PACKAGE" value="8-SOIC"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2594M-ADJ" prefix="U">
<description>SIMPLE SWITCHER® Power Converter</description>
<gates>
<gate name="A" symbol="LM2594M-ADJ"/>
</gates>
<devices>
<device name="" package="SOIC127P620X175-8N">
<connects>
<connect gate="A" pin="FB" pad="4"/>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="NC" pad="3"/>
<connect gate="A" pin="NC_2" pad="1"/>
<connect gate="A" pin="NC_3" pad="2"/>
<connect gate="A" pin="ON/OFF" pad="5"/>
<connect gate="A" pin="OUT" pad="8"/>
<connect gate="A" pin="VIN" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2594M-ADJ"/>
<attribute name="OC_FARNELL" value="9494332"/>
<attribute name="OC_NEWARK" value="41K3819"/>
<attribute name="PACKAGE" value="8-SOIC"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2594N-12" prefix="U">
<description>SIMPLE SWITCHER</description>
<gates>
<gate name="A" symbol="LM2594N-12"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-8">
<connects>
<connect gate="A" pin="FB" pad="4"/>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="NC" pad="3"/>
<connect gate="A" pin="NC_2" pad="1"/>
<connect gate="A" pin="NC_3" pad="2"/>
<connect gate="A" pin="OUT" pad="8"/>
<connect gate="A" pin="VIN" pad="7"/>
<connect gate="A" pin="~ON~/OFF" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2594N-12"/>
<attribute name="OC_FARNELL" value="9493751"/>
<attribute name="OC_NEWARK" value="38K3643"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2594N-3.3" prefix="U">
<description>SIMPLE SWITCHER</description>
<gates>
<gate name="A" symbol="LM2594N-3.3"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-8">
<connects>
<connect gate="A" pin="FB" pad="4"/>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="NC" pad="3"/>
<connect gate="A" pin="NC_2" pad="1"/>
<connect gate="A" pin="NC_3" pad="2"/>
<connect gate="A" pin="OUT" pad="8"/>
<connect gate="A" pin="VIN" pad="7"/>
<connect gate="A" pin="~ON~/OFF" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2594N-3.3"/>
<attribute name="OC_FARNELL" value="9493832"/>
<attribute name="OC_NEWARK" value="38K3644"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2594N-5.0" prefix="U">
<description>SIMPLE SWITCHER</description>
<gates>
<gate name="A" symbol="LM2594N-5.0"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-8">
<connects>
<connect gate="A" pin="FB" pad="4"/>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="NC" pad="3"/>
<connect gate="A" pin="NC_2" pad="1"/>
<connect gate="A" pin="NC_3" pad="2"/>
<connect gate="A" pin="OUT" pad="8"/>
<connect gate="A" pin="VIN" pad="7"/>
<connect gate="A" pin="~ON~/OFF" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2594N-5.0"/>
<attribute name="OC_FARNELL" value="9493646"/>
<attribute name="OC_NEWARK" value="41K3829"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2594N-ADJ" prefix="U">
<description>SIMPLE SWITCHER</description>
<gates>
<gate name="A" symbol="LM2594N-ADJ"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-8">
<connects>
<connect gate="A" pin="FB" pad="4"/>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="NC" pad="3"/>
<connect gate="A" pin="NC_2" pad="1"/>
<connect gate="A" pin="NC_3" pad="2"/>
<connect gate="A" pin="OUT" pad="8"/>
<connect gate="A" pin="VIN" pad="7"/>
<connect gate="A" pin="~ON~/OFF" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2594N-ADJ"/>
<attribute name="OC_FARNELL" value="9493654"/>
<attribute name="OC_NEWARK" value="41K3826"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2595S-12" prefix="U">
<description>SIMPLE SWITCHER</description>
<gates>
<gate name="A" symbol="LM2595S-12"/>
</gates>
<devices>
<device name="" package="TO170P1435X465-5N">
<connects>
<connect gate="A" pin="FB" pad="4"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="GND_2" pad="6"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="A" pin="VIN" pad="2"/>
<connect gate="A" pin="~ON/OFF" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2595S-12"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="07B6118"/>
<attribute name="PACKAGE" value="TO-263-5"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2595S-3.3" prefix="U">
<description>SIMPLE SWITCHER Power Converter</description>
<gates>
<gate name="A" symbol="LM2595S-3.3"/>
</gates>
<devices>
<device name="" package="TO170P1435X457-6N">
<connects>
<connect gate="A" pin="FB" pad="4"/>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="GND_2" pad="3"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="A" pin="VIN" pad="2"/>
<connect gate="A" pin="~ON/OFF" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2595S-3.3"/>
<attribute name="OC_FARNELL" value="1693990"/>
<attribute name="OC_NEWARK" value="07B6119"/>
<attribute name="PACKAGE" value="TO-263-5"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2595S-5.0" prefix="U">
<description>SIMPLE SWITCHER Power Converter</description>
<gates>
<gate name="A" symbol="LM2595S-5.0"/>
</gates>
<devices>
<device name="" package="TO170P1435X457-6N">
<connects>
<connect gate="A" pin="FB" pad="4"/>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="GND_2" pad="3"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="A" pin="VIN" pad="2"/>
<connect gate="A" pin="~ON/OFF" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2595S-5.0"/>
<attribute name="OC_FARNELL" value="1215203"/>
<attribute name="OC_NEWARK" value="41K3833"/>
<attribute name="PACKAGE" value="TO-263-5"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2595S-ADJ" prefix="U">
<description>Step-Down Voltage Regulator</description>
<gates>
<gate name="A" symbol="LM2595S-ADJ"/>
</gates>
<devices>
<device name="" package="TO170P1435X465-6N">
<connects>
<connect gate="A" pin="FB" pad="4"/>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="GND_2" pad="3"/>
<connect gate="A" pin="OUT" pad="2"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="~ON~/OFF" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2595S-ADJ"/>
<attribute name="OC_FARNELL" value="1215204"/>
<attribute name="OC_NEWARK" value="41K3830"/>
<attribute name="PACKAGE" value="TO-263-5"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2595T-12" prefix="U">
<description>IC, STEP-DOWN REGULATOR</description>
<gates>
<gate name="A" symbol="LM2595T-12"/>
</gates>
<devices>
<device name="" package="TO170P470X1016X2092-5P">
<connects>
<connect gate="A" pin="FB" pad="4"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="OUTOUT" pad="1"/>
<connect gate="A" pin="VIN" pad="2"/>
<connect gate="A" pin="~ON~/OFF" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2595T-12"/>
<attribute name="OC_FARNELL" value="9494057"/>
<attribute name="OC_NEWARK" value="41K3839"/>
<attribute name="PACKAGE" value="TO-220-5"/>
<attribute name="SUPPLIER" value="NATIONAL SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2595T-3.3" prefix="U">
<description>SWITCHING REG 1A 3.3V, 2595</description>
<gates>
<gate name="A" symbol="LM2595T-3.3"/>
</gates>
<devices>
<device name="" package="TO170P470X1016X2092-5P">
<connects>
<connect gate="A" pin="FB" pad="4"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="OUTOUT" pad="1"/>
<connect gate="A" pin="VIN" pad="2"/>
<connect gate="A" pin="~ON~/OFF" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2595T-3.3"/>
<attribute name="OC_FARNELL" value="9494340"/>
<attribute name="OC_NEWARK" value="38K3647"/>
<attribute name="PACKAGE" value="TO-220-5"/>
<attribute name="SUPPLIER" value="NATIONAL SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2595T-5.0" prefix="U">
<description>IC, STEP-DOWN REGULATOR</description>
<gates>
<gate name="A" symbol="LM2595T-5.0"/>
</gates>
<devices>
<device name="" package="TO170P470X1016X2092-5P">
<connects>
<connect gate="A" pin="FB" pad="4"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="OUTOUT" pad="1"/>
<connect gate="A" pin="VIN" pad="2"/>
<connect gate="A" pin="~ON~/OFF" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2595T-5.0"/>
<attribute name="OC_FARNELL" value="9494065"/>
<attribute name="OC_NEWARK" value="41K3841"/>
<attribute name="PACKAGE" value="TO-220-5"/>
<attribute name="SUPPLIER" value="NATIONAL SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2595T-ADJ" prefix="U">
<description>IC, STEP-DOWN REGULATOR</description>
<gates>
<gate name="A" symbol="LM2595T-ADJ"/>
</gates>
<devices>
<device name="" package="TO170P470X1016X2092-5P">
<connects>
<connect gate="A" pin="FB" pad="4"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="OUTOUT" pad="1"/>
<connect gate="A" pin="VIN" pad="2"/>
<connect gate="A" pin="~ON~/OFF" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2595T-ADJ"/>
<attribute name="OC_FARNELL" value="9494049"/>
<attribute name="OC_NEWARK" value="41K3838"/>
<attribute name="PACKAGE" value="TO-220-5"/>
<attribute name="SUPPLIER" value="NATIONAL SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2596S-12" prefix="U">
<description>Voltage Regulator</description>
<gates>
<gate name="A" symbol="LM2596S-12"/>
</gates>
<devices>
<device name="" package="TO170P1435X465-6N">
<connects>
<connect gate="A" pin="FB" pad="4"/>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="GND_2" pad="3"/>
<connect gate="A" pin="OUT" pad="2"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="~ON~/OFF" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2596S-12"/>
<attribute name="OC_FARNELL" value="9494359"/>
<attribute name="OC_NEWARK" value="41K3843"/>
<attribute name="PACKAGE" value="TO-263-5"/>
<attribute name="SUPPLIER" value="National"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2596S-3.3" prefix="U">
<description>Step-Down Voltage Regulator</description>
<gates>
<gate name="A" symbol="LM2596S-3.3"/>
</gates>
<devices>
<device name="" package="TO170P1435X465-6N">
<connects>
<connect gate="A" pin="FB" pad="4"/>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="GND_2" pad="3"/>
<connect gate="A" pin="OUT" pad="2"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="~ON~/OFF" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2596S-3.3"/>
<attribute name="OC_FARNELL" value="1214545"/>
<attribute name="OC_NEWARK" value="23K0827"/>
<attribute name="PACKAGE" value="TO-263-5"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2596S-5.0" prefix="U">
<description>Step-Down Voltage Regulator</description>
<gates>
<gate name="A" symbol="LM2596S-5.0"/>
</gates>
<devices>
<device name="" package="TO170P1435X465-6N">
<connects>
<connect gate="A" pin="FB" pad="4"/>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="GND_2" pad="3"/>
<connect gate="A" pin="OUT" pad="2"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="~ON~/OFF" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2596S-50"/>
<attribute name="OC_FARNELL" value="1214546"/>
<attribute name="OC_NEWARK" value="41K3844"/>
<attribute name="PACKAGE" value="TO-263-5"/>
<attribute name="SUPPLIER" value="National"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2596T-12" prefix="U">
<description>IC, STEP-DOWN VOLTAGE REGULATOR</description>
<gates>
<gate name="A" symbol="LM2596T-12"/>
</gates>
<devices>
<device name="" package="TO170P470X1016X2092-5P">
<connects>
<connect gate="A" pin="*ON-OFF" pad="5"/>
<connect gate="A" pin="FEEDBACK" pad="4"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="OUTPUT" pad="2"/>
<connect gate="A" pin="VIN" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2596T-12"/>
<attribute name="OC_FARNELL" value="9494375"/>
<attribute name="OC_NEWARK" value="41K3849"/>
<attribute name="PACKAGE" value="TO220-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2596T-3.3" prefix="U">
<description>SWITCHING REG, 3A 3.3V</description>
<gates>
<gate name="A" symbol="LM2596T-3.3"/>
</gates>
<devices>
<device name="" package="TO170P470X1016X2092-5P">
<connects>
<connect gate="A" pin="*ON-OFF" pad="5"/>
<connect gate="A" pin="FEEDBACK" pad="4"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="OUTPUT" pad="2"/>
<connect gate="A" pin="VIN" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2596T-3.3"/>
<attribute name="OC_FARNELL" value="1215205"/>
<attribute name="OC_NEWARK" value="07B6139"/>
<attribute name="PACKAGE" value="TO220-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2596T-5.0" prefix="U">
<description>IC, STEP-DOWN VOLTAGE REGULATOR</description>
<gates>
<gate name="A" symbol="LM2596T-5.0"/>
</gates>
<devices>
<device name="" package="TO170P470X1016X2092-5P">
<connects>
<connect gate="A" pin="*ON-OFF" pad="5"/>
<connect gate="A" pin="FEEDBACK" pad="4"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="OUTPUT" pad="2"/>
<connect gate="A" pin="VIN" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2596T-5.0"/>
<attribute name="OC_FARNELL" value="1206529"/>
<attribute name="OC_NEWARK" value="41K3851"/>
<attribute name="PACKAGE" value="TO220-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2597HVM-12" prefix="U">
<description>SIMPLE SWITCHER</description>
<gates>
<gate name="A" symbol="LM2597HVM-12"/>
</gates>
<devices>
<device name="" package="SOIC127P620X175-8N">
<connects>
<connect gate="A" pin="B/S" pad="3"/>
<connect gate="A" pin="DELAY" pad="2"/>
<connect gate="A" pin="ERROR_FLAG" pad="1"/>
<connect gate="A" pin="FB" pad="4"/>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="OUT" pad="8"/>
<connect gate="A" pin="VIN" pad="7"/>
<connect gate="A" pin="~SD/SS" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2597HVM-12"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K3853"/>
<attribute name="PACKAGE" value="Switcher"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2597HVM-3.3" prefix="U">
<description>Voltage Regulator</description>
<gates>
<gate name="A" symbol="LM2597HVM-3.3"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="B/S" pad="3"/>
<connect gate="A" pin="DELAY" pad="2"/>
<connect gate="A" pin="ERR_FLOG" pad="1"/>
<connect gate="A" pin="FB" pad="4"/>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="OUT" pad="8"/>
<connect gate="A" pin="VIN" pad="7"/>
<connect gate="A" pin="~SD/SS" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2597HVM-3.3"/>
<attribute name="OC_FARNELL" value="1495090"/>
<attribute name="OC_NEWARK" value="61M7301"/>
<attribute name="PACKAGE" value="8-SOIC"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2597HVM-5.0" prefix="U">
<description>SIMPLE SWITCHER</description>
<gates>
<gate name="A" symbol="LM2597HVM-5.0"/>
</gates>
<devices>
<device name="" package="SOIC127P620X175-8N">
<connects>
<connect gate="A" pin="B/S" pad="3"/>
<connect gate="A" pin="DELAY" pad="2"/>
<connect gate="A" pin="ERROR_FLAG" pad="1"/>
<connect gate="A" pin="FB" pad="4"/>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="OUT" pad="8"/>
<connect gate="A" pin="VIN" pad="7"/>
<connect gate="A" pin="~SD/SS" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2597HVM-5.0"/>
<attribute name="OC_FARNELL" value="1564636"/>
<attribute name="OC_NEWARK" value="41K3855"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2597HVM-ADJ" prefix="U">
<description>SIMPLE SWITCHER</description>
<gates>
<gate name="A" symbol="LM2597HVM-ADJ"/>
</gates>
<devices>
<device name="" package="SOIC127P620X175-8N">
<connects>
<connect gate="A" pin="B/S" pad="3"/>
<connect gate="A" pin="DELAY" pad="2"/>
<connect gate="A" pin="ERROR_FLAG" pad="1"/>
<connect gate="A" pin="FB" pad="4"/>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="OUT" pad="8"/>
<connect gate="A" pin="VIN" pad="7"/>
<connect gate="A" pin="~SD/SS" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2597HVM-ADJ"/>
<attribute name="OC_FARNELL" value="1286838"/>
<attribute name="OC_NEWARK" value="26M0323"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2597HVN-ADJ" prefix="U">
<description>SIMPLE SWITCHER</description>
<gates>
<gate name="A" symbol="LM2597HVN-ADJ"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-8">
<connects>
<connect gate="A" pin="B/S" pad="3"/>
<connect gate="A" pin="DELAY" pad="2"/>
<connect gate="A" pin="ERROR_FLAG" pad="1"/>
<connect gate="A" pin="FB" pad="4"/>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="OUT" pad="8"/>
<connect gate="A" pin="VIN" pad="7"/>
<connect gate="A" pin="~SD/SS" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2597HVN-ADJ"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K3860"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2597M-12" prefix="U">
<description>SIMPLE SWITCHER</description>
<gates>
<gate name="A" symbol="LM2597M-12"/>
</gates>
<devices>
<device name="" package="SOIC127P620X175-8N">
<connects>
<connect gate="A" pin="B/S" pad="3"/>
<connect gate="A" pin="DELAY" pad="2"/>
<connect gate="A" pin="ERROR_FLAG" pad="1"/>
<connect gate="A" pin="FB" pad="4"/>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="OUT" pad="8"/>
<connect gate="A" pin="VIN" pad="7"/>
<connect gate="A" pin="~SD/SS" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2597M-12"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K3865"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2597M-3.3" prefix="U">
<description>Power converter</description>
<gates>
<gate name="A" symbol="LM2597M-3.3"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="B/S" pad="3"/>
<connect gate="A" pin="DELAY" pad="2"/>
<connect gate="A" pin="ERROR_FLAG" pad="1"/>
<connect gate="A" pin="FB" pad="4"/>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="OUTPUT" pad="8"/>
<connect gate="A" pin="VIN" pad="7"/>
<connect gate="A" pin="~SD/SS" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2597M-3.3"/>
<attribute name="OC_FARNELL" value="9494383"/>
<attribute name="OC_NEWARK" value="07B6143"/>
<attribute name="PACKAGE" value="8-SOIC"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2597M-5.0" prefix="U">
<description>Power converter</description>
<gates>
<gate name="A" symbol="LM2597M-5.0"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="B/S" pad="3"/>
<connect gate="A" pin="DELAY" pad="2"/>
<connect gate="A" pin="ERROR_FLAG" pad="1"/>
<connect gate="A" pin="FB" pad="4"/>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="OUTPUT" pad="8"/>
<connect gate="A" pin="VIN" pad="7"/>
<connect gate="A" pin="~SD/SS" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2597M-5.0"/>
<attribute name="OC_FARNELL" value="9494391"/>
<attribute name="OC_NEWARK" value="38K3652"/>
<attribute name="PACKAGE" value="8-SOIC"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2597M-ADJ" prefix="U">
<description>Power converter</description>
<gates>
<gate name="A" symbol="LM2597M-ADJ"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="B/S" pad="3"/>
<connect gate="A" pin="DELAY" pad="2"/>
<connect gate="A" pin="ERROR_FLAG" pad="1"/>
<connect gate="A" pin="FB" pad="4"/>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="OUTPUT" pad="8"/>
<connect gate="A" pin="VIN" pad="7"/>
<connect gate="A" pin="~SD/SS" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2597M-ADJ"/>
<attribute name="OC_FARNELL" value="9494405"/>
<attribute name="OC_NEWARK" value="97K3257"/>
<attribute name="PACKAGE" value="8-SOIC"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2597N-12" prefix="U">
<description>SIMPLE SWITCHER</description>
<gates>
<gate name="A" symbol="LM2597N-12"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-8">
<connects>
<connect gate="A" pin="B/S" pad="3"/>
<connect gate="A" pin="DELAY" pad="2"/>
<connect gate="A" pin="ERROR_FLAG" pad="1"/>
<connect gate="A" pin="FB" pad="4"/>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="OUT" pad="8"/>
<connect gate="A" pin="VIN" pad="7"/>
<connect gate="A" pin="~SD/SS" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2597N-12"/>
<attribute name="OC_FARNELL" value="9493662"/>
<attribute name="OC_NEWARK" value="-"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2597N-3.3" prefix="U">
<description>SIMPLE SWITCHER</description>
<gates>
<gate name="A" symbol="LM2597N-3.3"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-8">
<connects>
<connect gate="A" pin="B/S" pad="3"/>
<connect gate="A" pin="DELAY" pad="2"/>
<connect gate="A" pin="ERROR_FLAG" pad="1"/>
<connect gate="A" pin="FB" pad="4"/>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="OUT" pad="8"/>
<connect gate="A" pin="VIN" pad="7"/>
<connect gate="A" pin="~SD/SS" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2597N-3.3"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="07B6151"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2597N-5.0" prefix="U">
<description>SIMPLE SWITCHER</description>
<gates>
<gate name="A" symbol="LM2597N-5.0"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-8">
<connects>
<connect gate="A" pin="B/S" pad="3"/>
<connect gate="A" pin="DELAY" pad="2"/>
<connect gate="A" pin="ERROR_FLAG" pad="1"/>
<connect gate="A" pin="FB" pad="4"/>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="OUT" pad="8"/>
<connect gate="A" pin="VIN" pad="7"/>
<connect gate="A" pin="~SD/SS" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2597N-5.0"/>
<attribute name="OC_FARNELL" value="9493760"/>
<attribute name="OC_NEWARK" value="38K3655"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2597N-ADJ" prefix="U">
<description>SIMPLE SWITCHER</description>
<gates>
<gate name="A" symbol="LM2597N-ADJ"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-8">
<connects>
<connect gate="A" pin="B/S" pad="3"/>
<connect gate="A" pin="DELAY" pad="2"/>
<connect gate="A" pin="ERROR_FLAG" pad="1"/>
<connect gate="A" pin="FB" pad="4"/>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="OUT" pad="8"/>
<connect gate="A" pin="VIN" pad="7"/>
<connect gate="A" pin="~SD/SS" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2597N-ADJ"/>
<attribute name="OC_FARNELL" value="9493670"/>
<attribute name="OC_NEWARK" value="07B6149"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2598S-3.3" prefix="U">
<description>SIMPLE SWITCHER</description>
<gates>
<gate name="A" symbol="LM2598S-3.3"/>
</gates>
<devices>
<device name="" package="TO127O1435X465-7N">
<connects>
<connect gate="A" pin="DELAY" pad="5"/>
<connect gate="A" pin="FB" pad="6"/>
<connect gate="A" pin="FLAG" pad="3"/>
<connect gate="A" pin="GND" pad="8"/>
<connect gate="A" pin="GND_2" pad="4"/>
<connect gate="A" pin="OUT" pad="2"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="~SD/SS" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2598S-3.3"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="07B6155"/>
<attribute name="PACKAGE" value="TO-263-7"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2598S-5.0" prefix="U">
<description>SIMPLE SWITCHER</description>
<gates>
<gate name="A" symbol="LM2598S-5.0"/>
</gates>
<devices>
<device name="" package="TO127O1435X465-7N">
<connects>
<connect gate="A" pin="DELAY" pad="5"/>
<connect gate="A" pin="FB" pad="6"/>
<connect gate="A" pin="FLAG" pad="3"/>
<connect gate="A" pin="GND" pad="8"/>
<connect gate="A" pin="GND_2" pad="4"/>
<connect gate="A" pin="OUT" pad="2"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="~SD/SS" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2598S-5.0"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="07B6156"/>
<attribute name="PACKAGE" value="TO-263-7"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2598S-ADJ" prefix="U">
<description>SIMPLE SWITCHER</description>
<gates>
<gate name="A" symbol="LM2598S-ADJ"/>
</gates>
<devices>
<device name="" package="TO127O1435X465-7N">
<connects>
<connect gate="A" pin="DELAY" pad="5"/>
<connect gate="A" pin="FB" pad="6"/>
<connect gate="A" pin="FLAG" pad="3"/>
<connect gate="A" pin="GND" pad="8"/>
<connect gate="A" pin="GND_2" pad="4"/>
<connect gate="A" pin="OUT" pad="2"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="~SD/SS" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2598S-ADJ"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K3876"/>
<attribute name="PACKAGE" value="TO-263-7"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2598T-3.3" prefix="U">
<description>IC BUCK 3.3V 1A</description>
<gates>
<gate name="A" symbol="LM2598T-3.3"/>
</gates>
<devices>
<device name="" package="TO127P470X1016X1740-7P">
<connects>
<connect gate="A" pin="*SD-SS" pad="7"/>
<connect gate="A" pin="DELAY" pad="5"/>
<connect gate="A" pin="FEEDBACK" pad="6"/>
<connect gate="A" pin="FLAG" pad="3"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="OUTPUT" pad="2"/>
<connect gate="A" pin="VIN" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2598T-3.3"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K3886"/>
<attribute name="PACKAGE" value="TO220-7"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2598T-5.0" prefix="U">
<description>IC BUCK 5V 1A</description>
<gates>
<gate name="A" symbol="LM2598T-5.0"/>
</gates>
<devices>
<device name="" package="TO127P470X1016X1740-7P">
<connects>
<connect gate="A" pin="*SD-SS" pad="7"/>
<connect gate="A" pin="DELAY" pad="5"/>
<connect gate="A" pin="FEEDBACK" pad="6"/>
<connect gate="A" pin="FLAG" pad="3"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="OUTPUT" pad="2"/>
<connect gate="A" pin="VIN" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2598T-5.0"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K3887"/>
<attribute name="PACKAGE" value="TO220-7"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2598T-ADJ" prefix="U">
<description>IC BUCK ADJ 1A</description>
<gates>
<gate name="A" symbol="LM2598T-ADJ"/>
</gates>
<devices>
<device name="" package="TO127P470X1016X1740-7P">
<connects>
<connect gate="A" pin="*SD-SS" pad="7"/>
<connect gate="A" pin="DELAY" pad="5"/>
<connect gate="A" pin="FEEDBACK" pad="6"/>
<connect gate="A" pin="FLAG" pad="3"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="OUTPUT" pad="2"/>
<connect gate="A" pin="VIN" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2598T-ADJ"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="07B6161"/>
<attribute name="PACKAGE" value="TO220-7"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2599S-12" prefix="U">
<description>SIMPLE SWITCHER</description>
<gates>
<gate name="A" symbol="LM2599S-12"/>
</gates>
<devices>
<device name="" package="TO127O1435X465-7N">
<connects>
<connect gate="A" pin="DELAY" pad="5"/>
<connect gate="A" pin="FB" pad="6"/>
<connect gate="A" pin="FLAG" pad="3"/>
<connect gate="A" pin="GND" pad="8"/>
<connect gate="A" pin="GND_2" pad="4"/>
<connect gate="A" pin="OUT" pad="2"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="~SD/SS" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2599S-12"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K3889"/>
<attribute name="PACKAGE" value="TO-263-7"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2599S-3.3" prefix="U">
<description>SIMPLE SWITCHER</description>
<gates>
<gate name="A" symbol="LM2599S-3.3"/>
</gates>
<devices>
<device name="" package="TO127O1435X465-7N">
<connects>
<connect gate="A" pin="DELAY" pad="5"/>
<connect gate="A" pin="FB" pad="6"/>
<connect gate="A" pin="FLAG" pad="3"/>
<connect gate="A" pin="GND" pad="8"/>
<connect gate="A" pin="GND_2" pad="4"/>
<connect gate="A" pin="OUT" pad="2"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="~SD/SS" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2599S-3.3"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K3890"/>
<attribute name="PACKAGE" value="TO-263-7"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2599S-5.0" prefix="U">
<description>SIMPLE SWITCHER</description>
<gates>
<gate name="A" symbol="LM2599S-5.0"/>
</gates>
<devices>
<device name="" package="TO127O1435X465-7N">
<connects>
<connect gate="A" pin="DELAY" pad="5"/>
<connect gate="A" pin="FB" pad="6"/>
<connect gate="A" pin="FLAG" pad="3"/>
<connect gate="A" pin="GND" pad="8"/>
<connect gate="A" pin="GND_2" pad="4"/>
<connect gate="A" pin="OUT" pad="2"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="~SD/SS" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2599S-3.3"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K3891"/>
<attribute name="PACKAGE" value="TO-263-7"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2599S-ADJ" prefix="U">
<description>SIMPLE SWITCHER</description>
<gates>
<gate name="A" symbol="LM2599S-ADJ"/>
</gates>
<devices>
<device name="" package="TO127O1435X465-7N">
<connects>
<connect gate="A" pin="DELAY" pad="5"/>
<connect gate="A" pin="FB" pad="6"/>
<connect gate="A" pin="FLAG" pad="3"/>
<connect gate="A" pin="GND" pad="8"/>
<connect gate="A" pin="GND_2" pad="4"/>
<connect gate="A" pin="OUT" pad="2"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="~SD/SS" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2599S-ADJ"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K3888"/>
<attribute name="PACKAGE" value="TO-263-7"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2599T-12" prefix="U">
<description>SWITCHING REG 3A 12V, 2599, TO2207</description>
<gates>
<gate name="A" symbol="LM2599T-12"/>
</gates>
<devices>
<device name="" package="TO127P470X1016X1740-7P">
<connects>
<connect gate="A" pin="*SD-SS" pad="7"/>
<connect gate="A" pin="DELAY" pad="5"/>
<connect gate="A" pin="FEEDBACK" pad="6"/>
<connect gate="A" pin="FLAG" pad="3"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="OUTPUT" pad="2"/>
<connect gate="A" pin="VIN" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2599T-12"/>
<attribute name="OC_FARNELL" value="9494090"/>
<attribute name="OC_NEWARK" value="38K3656"/>
<attribute name="PACKAGE" value="TO220-7"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2599T-3.3" prefix="U">
<description>IC BUCK 3.3V 3A</description>
<gates>
<gate name="A" symbol="LM2599T-3.3"/>
</gates>
<devices>
<device name="" package="TO127P470X1016X1740-7P">
<connects>
<connect gate="A" pin="*SD-SS" pad="7"/>
<connect gate="A" pin="DELAY" pad="5"/>
<connect gate="A" pin="FEEDBACK" pad="6"/>
<connect gate="A" pin="FLAG" pad="3"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="OUTPUT" pad="2"/>
<connect gate="A" pin="VIN" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2599T-3.3"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K3898"/>
<attribute name="PACKAGE" value="TO220-7"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2599T-5.0" prefix="U">
<description>SWITCHING REG 3A 5.0V, 2599</description>
<gates>
<gate name="A" symbol="LM2599T-5.0"/>
</gates>
<devices>
<device name="" package="TO127P470X1016X1740-7P">
<connects>
<connect gate="A" pin="*SD-SS" pad="7"/>
<connect gate="A" pin="DELAY" pad="5"/>
<connect gate="A" pin="FEEDBACK" pad="6"/>
<connect gate="A" pin="FLAG" pad="3"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="OUTPUT" pad="2"/>
<connect gate="A" pin="VIN" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2599T-5.0"/>
<attribute name="OC_FARNELL" value="9494103"/>
<attribute name="OC_NEWARK" value="38K3657"/>
<attribute name="PACKAGE" value="TO220-7"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2599T-ADJ" prefix="U">
<description>IC, DC-DC CONV</description>
<gates>
<gate name="A" symbol="LM2599T-ADJ"/>
</gates>
<devices>
<device name="" package="TO127P470X1016X1740-7P">
<connects>
<connect gate="A" pin="*SD-SS" pad="7"/>
<connect gate="A" pin="DELAY" pad="5"/>
<connect gate="A" pin="FEEDBACK" pad="6"/>
<connect gate="A" pin="FLAG" pad="3"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="OUTPUT" pad="2"/>
<connect gate="A" pin="VIN" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2599T-ADJ"/>
<attribute name="OC_FARNELL" value="9494081"/>
<attribute name="OC_NEWARK" value="97K3259"/>
<attribute name="PACKAGE" value="TO220-7"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM26001MXA" prefix="U">
<description>Switching Regulator</description>
<gates>
<gate name="A" symbol="LM26001MXA"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-17N">
<connects>
<connect gate="A" pin="BOOT" pad="14"/>
<connect gate="A" pin="COMP" pad="6"/>
<connect gate="A" pin="EN" pad="4"/>
<connect gate="A" pin="EPAD" pad="17"/>
<connect gate="A" pin="FB" pad="7"/>
<connect gate="A" pin="FPWM" pad="10"/>
<connect gate="A" pin="FREQ" pad="9"/>
<connect gate="A" pin="GND" pad="8"/>
<connect gate="A" pin="PGOOD" pad="3"/>
<connect gate="A" pin="SS" pad="5"/>
<connect gate="A" pin="SW" pad="16"/>
<connect gate="A" pin="SW_2" pad="15"/>
<connect gate="A" pin="SYNC" pad="11"/>
<connect gate="A" pin="VBIAS" pad="12"/>
<connect gate="A" pin="VDD" pad="13"/>
<connect gate="A" pin="VIN" pad="2"/>
<connect gate="A" pin="VIN_2" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM26001MXA"/>
<attribute name="OC_FARNELL" value="1559872"/>
<attribute name="OC_NEWARK" value="99K2336"/>
<attribute name="PACKAGE" value="TSSOP-16"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM26001QMXA" prefix="U">
<description>1.5A Switching Regulator</description>
<gates>
<gate name="A" symbol="LM26001QMXA"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-17N">
<connects>
<connect gate="A" pin="BOOT" pad="14"/>
<connect gate="A" pin="COMP" pad="6"/>
<connect gate="A" pin="EN" pad="4"/>
<connect gate="A" pin="EP" pad="17"/>
<connect gate="A" pin="FB" pad="7"/>
<connect gate="A" pin="FPWM" pad="10"/>
<connect gate="A" pin="FREQ" pad="9"/>
<connect gate="A" pin="GND" pad="8"/>
<connect gate="A" pin="PGOOD" pad="3"/>
<connect gate="A" pin="SS" pad="5"/>
<connect gate="A" pin="SW" pad="16"/>
<connect gate="A" pin="SW_2" pad="15"/>
<connect gate="A" pin="SYNC" pad="11"/>
<connect gate="A" pin="VBIAS" pad="12"/>
<connect gate="A" pin="VDD" pad="13"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="VIN_2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM26001QMXA"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="55R3838"/>
<attribute name="PACKAGE" value="TSSOP-16"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM26003MH" prefix="U">
<description>Switching Regulator</description>
<gates>
<gate name="A" symbol="LM26003MH"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-21N">
<connects>
<connect gate="A" pin="AGND" pad="10"/>
<connect gate="A" pin="AVIN" pad="4"/>
<connect gate="A" pin="BOOT" pad="17"/>
<connect gate="A" pin="COMP" pad="8"/>
<connect gate="A" pin="EN" pad="6"/>
<connect gate="A" pin="EPAD" pad="21"/>
<connect gate="A" pin="FB" pad="9"/>
<connect gate="A" pin="FPWM" pad="13"/>
<connect gate="A" pin="FREQ" pad="12"/>
<connect gate="A" pin="PGND" pad="11"/>
<connect gate="A" pin="PGOOD" pad="5"/>
<connect gate="A" pin="SS" pad="7"/>
<connect gate="A" pin="SW" pad="20"/>
<connect gate="A" pin="SW_2" pad="18"/>
<connect gate="A" pin="SW_3" pad="19"/>
<connect gate="A" pin="SYNC" pad="14"/>
<connect gate="A" pin="VBIAS" pad="15"/>
<connect gate="A" pin="VDD" pad="16"/>
<connect gate="A" pin="VIN" pad="3"/>
<connect gate="A" pin="VIN_2" pad="1"/>
<connect gate="A" pin="VIN_3" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM26003MH"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="34P4806"/>
<attribute name="PACKAGE" value="TSSOP-20"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM26003QMH" prefix="U">
<description>Switching Regulator</description>
<gates>
<gate name="A" symbol="LM26003QMH"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-21N">
<connects>
<connect gate="A" pin="AGND" pad="10"/>
<connect gate="A" pin="AVIN" pad="4"/>
<connect gate="A" pin="BOOT" pad="17"/>
<connect gate="A" pin="COMP" pad="8"/>
<connect gate="A" pin="EN" pad="6"/>
<connect gate="A" pin="EPAD" pad="21"/>
<connect gate="A" pin="FB" pad="9"/>
<connect gate="A" pin="FPWM" pad="13"/>
<connect gate="A" pin="FREQ" pad="12"/>
<connect gate="A" pin="PGND" pad="11"/>
<connect gate="A" pin="PGOOD" pad="5"/>
<connect gate="A" pin="SS" pad="7"/>
<connect gate="A" pin="SW" pad="20"/>
<connect gate="A" pin="SW_2" pad="18"/>
<connect gate="A" pin="SW_3" pad="19"/>
<connect gate="A" pin="SYNC" pad="14"/>
<connect gate="A" pin="VBIAS" pad="15"/>
<connect gate="A" pin="VDD" pad="16"/>
<connect gate="A" pin="VIN" pad="3"/>
<connect gate="A" pin="VIN_2" pad="1"/>
<connect gate="A" pin="VIN_3" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM26003QMH"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="55R3840"/>
<attribute name="PACKAGE" value="TSSOP-20"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2611AMF" prefix="U">
<description>Cuk Converter</description>
<gates>
<gate name="A" symbol="LM2611AMF"/>
</gates>
<devices>
<device name="" package="SOT95P285X120-5N">
<connects>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="NFB" pad="3"/>
<connect gate="A" pin="SW" pad="1"/>
<connect gate="A" pin="VIN" pad="5"/>
<connect gate="A" pin="~SHDN" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2611AMF"/>
<attribute name="OC_FARNELL" value="9779094"/>
<attribute name="OC_NEWARK" value="34C6513"/>
<attribute name="PACKAGE" value="SOT23-5"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2611BMF" prefix="U">
<description>Cuk Converter</description>
<gates>
<gate name="A" symbol="LM2611BMF"/>
</gates>
<devices>
<device name="" package="SOT95P285X120-5N">
<connects>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="NFB" pad="3"/>
<connect gate="A" pin="SW" pad="1"/>
<connect gate="A" pin="VIN" pad="5"/>
<connect gate="A" pin="~SHDN" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2611BMF"/>
<attribute name="OC_FARNELL" value="1853249"/>
<attribute name="OC_NEWARK" value="41K3930"/>
<attribute name="PACKAGE" value="SOT-5"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2621MM" prefix="U">
<description>DC/DC Boost Converter</description>
<gates>
<gate name="A" symbol="LM2621MM"/>
</gates>
<devices>
<device name="" package="SOP65P490X110-8N">
<connects>
<connect gate="A" pin="BOOT" pad="7"/>
<connect gate="A" pin="EN" pad="2"/>
<connect gate="A" pin="FB" pad="4"/>
<connect gate="A" pin="FREQ" pad="3"/>
<connect gate="A" pin="PGND" pad="1"/>
<connect gate="A" pin="SGND" pad="5"/>
<connect gate="A" pin="SW" pad="8"/>
<connect gate="A" pin="VDD" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2621MM"/>
<attribute name="OC_FARNELL" value="9779248"/>
<attribute name="OC_NEWARK" value="48F3506"/>
<attribute name="PACKAGE" value="8-MSOP"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2622MM-ADJ" prefix="U">
<description>PWM DC/DC Converter</description>
<gates>
<gate name="A" symbol="LM2622MM-ADJ"/>
</gates>
<devices>
<device name="" package="SOP65P490X110-8N">
<connects>
<connect gate="A" pin="FB" pad="2"/>
<connect gate="A" pin="FSLCT" pad="7"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="NC" pad="8"/>
<connect gate="A" pin="SW" pad="5"/>
<connect gate="A" pin="VC" pad="1"/>
<connect gate="A" pin="VIN" pad="6"/>
<connect gate="A" pin="~SHDN" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2622MM-ADJ"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K3954"/>
<attribute name="PACKAGE" value="MSOP-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2623AMM" prefix="U">
<description>DC/DC Converter</description>
<gates>
<gate name="A" symbol="LM2623AMM"/>
</gates>
<devices>
<device name="" package="SOP65P490X110-8N">
<connects>
<connect gate="A" pin="BOOT" pad="7"/>
<connect gate="A" pin="EN" pad="2"/>
<connect gate="A" pin="FB" pad="4"/>
<connect gate="A" pin="FREQ" pad="3"/>
<connect gate="A" pin="PGND" pad="1"/>
<connect gate="A" pin="SGND" pad="5"/>
<connect gate="A" pin="SW" pad="8"/>
<connect gate="A" pin="VDD" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2623AMM"/>
<attribute name="OC_FARNELL" value="8207445"/>
<attribute name="OC_NEWARK" value="41K3958"/>
<attribute name="PACKAGE" value="8-MSOP"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2623LD" prefix="U">
<description>DC/DC Boost Converter</description>
<gates>
<gate name="A" symbol="LM2623LD"/>
</gates>
<devices>
<device name="" package="DFN400X400X80-15N">
<connects>
<connect gate="A" pin="BOOT" pad="11"/>
<connect gate="A" pin="EN" pad="4"/>
<connect gate="A" pin="EPAD" pad="15"/>
<connect gate="A" pin="FB" pad="6"/>
<connect gate="A" pin="FREQ" pad="5"/>
<connect gate="A" pin="NC" pad="8"/>
<connect gate="A" pin="NC_2" pad="7"/>
<connect gate="A" pin="NC_3" pad="1"/>
<connect gate="A" pin="NC_4" pad="14"/>
<connect gate="A" pin="PGND" pad="3"/>
<connect gate="A" pin="PGND_2" pad="2"/>
<connect gate="A" pin="SGND" pad="9"/>
<connect gate="A" pin="SW" pad="13"/>
<connect gate="A" pin="SW_2" pad="12"/>
<connect gate="A" pin="VDD" pad="10"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2623LD"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="26H4011"/>
<attribute name="PACKAGE" value="DFN-14"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2623MM" prefix="U">
<description>DC/DC Boost Converter</description>
<gates>
<gate name="A" symbol="LM2623MM"/>
</gates>
<devices>
<device name="" package="SOP65P490X110-8N">
<connects>
<connect gate="A" pin="BOOT" pad="7"/>
<connect gate="A" pin="EN" pad="2"/>
<connect gate="A" pin="FB" pad="4"/>
<connect gate="A" pin="FREQ" pad="3"/>
<connect gate="A" pin="PGND" pad="1"/>
<connect gate="A" pin="SGND" pad="5"/>
<connect gate="A" pin="SW" pad="8"/>
<connect gate="A" pin="VDD" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2623MM"/>
<attribute name="OC_FARNELL" value="8207453"/>
<attribute name="OC_NEWARK" value="41K3962"/>
<attribute name="PACKAGE" value="8-MSOP"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM26400YMH" prefix="U">
<description>Wide Input Range Buck Regulator</description>
<gates>
<gate name="A" symbol="LM26400YMH"/>
</gates>
<devices>
<device name="" package="DFN500X500X80-17N">
<connects>
<connect gate="A" pin="AVIN" pad="4"/>
<connect gate="A" pin="BST1" pad="16"/>
<connect gate="A" pin="BST2" pad="9"/>
<connect gate="A" pin="EN1" pad="3"/>
<connect gate="A" pin="EN2" pad="6"/>
<connect gate="A" pin="EPAD" pad="17"/>
<connect gate="A" pin="FB1" pad="1"/>
<connect gate="A" pin="FB2" pad="8"/>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="PVIN" pad="14"/>
<connect gate="A" pin="PVIN_2" pad="11"/>
<connect gate="A" pin="PVIN_3" pad="12"/>
<connect gate="A" pin="PVIN_4" pad="13"/>
<connect gate="A" pin="SS1" pad="2"/>
<connect gate="A" pin="SS2" pad="7"/>
<connect gate="A" pin="SW1" pad="15"/>
<connect gate="A" pin="SW2" pad="10"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM26400YSD"/>
<attribute name="OC_FARNELL" value="1333957"/>
<attribute name="OC_NEWARK" value="34M6729"/>
<attribute name="PACKAGE" value="DFN-16"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM26400YSD" prefix="U">
<description>Wide Input Range Buck Regulator</description>
<gates>
<gate name="A" symbol="LM26400YSD"/>
</gates>
<devices>
<device name="" package="DFN500X500X80-17N">
<connects>
<connect gate="A" pin="AVIN" pad="4"/>
<connect gate="A" pin="BST1" pad="16"/>
<connect gate="A" pin="BST2" pad="9"/>
<connect gate="A" pin="EN1" pad="3"/>
<connect gate="A" pin="EN2" pad="6"/>
<connect gate="A" pin="EPAD" pad="17"/>
<connect gate="A" pin="FB1" pad="1"/>
<connect gate="A" pin="FB2" pad="8"/>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="PVIN" pad="14"/>
<connect gate="A" pin="PVIN_2" pad="11"/>
<connect gate="A" pin="PVIN_3" pad="12"/>
<connect gate="A" pin="PVIN_4" pad="13"/>
<connect gate="A" pin="SS1" pad="2"/>
<connect gate="A" pin="SS2" pad="7"/>
<connect gate="A" pin="SW1" pad="15"/>
<connect gate="A" pin="SW2" pad="10"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM26400YSD"/>
<attribute name="OC_FARNELL" value="1333957"/>
<attribute name="OC_NEWARK" value="34M6729"/>
<attribute name="PACKAGE" value="DFN-16"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2640MTC-ADJ" prefix="U">
<description>Step-Down Switching Power Supply Controller</description>
<gates>
<gate name="A" symbol="LM2640MTC-ADJ"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-28N">
<connects>
<connect gate="A" pin="2NDFB/~FPWM" pad="10"/>
<connect gate="A" pin="CBOOT1" pad="18"/>
<connect gate="A" pin="CBOOT2" pad="25"/>
<connect gate="A" pin="COMP1" pad="13"/>
<connect gate="A" pin="COMP2" pad="3"/>
<connect gate="A" pin="CSH1" pad="15"/>
<connect gate="A" pin="CSH2" pad="1"/>
<connect gate="A" pin="CSL1" pad="21"/>
<connect gate="A" pin="CSL2" pad="28"/>
<connect gate="A" pin="FB1" pad="14"/>
<connect gate="A" pin="FB2" pad="2"/>
<connect gate="A" pin="GND" pad="8"/>
<connect gate="A" pin="HDRV1" pad="16"/>
<connect gate="A" pin="HDRV2" pad="27"/>
<connect gate="A" pin="IN" pad="23"/>
<connect gate="A" pin="LDRV1" pad="19"/>
<connect gate="A" pin="LDRV2" pad="24"/>
<connect gate="A" pin="LIN" pad="22"/>
<connect gate="A" pin="ON/~OFF1" pad="11"/>
<connect gate="A" pin="ON/~OFF2" pad="5"/>
<connect gate="A" pin="PGND" pad="20"/>
<connect gate="A" pin="REF" pad="9"/>
<connect gate="A" pin="SS1" pad="12"/>
<connect gate="A" pin="SS2" pad="4"/>
<connect gate="A" pin="SW1" pad="17"/>
<connect gate="A" pin="SW2" pad="26"/>
<connect gate="A" pin="SYNC" pad="7"/>
<connect gate="A" pin="~SD" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2640MTC-ADJ"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K3982"/>
<attribute name="PACKAGE" value="TSSOP-28"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM26420XMH" prefix="U">
<description>Frequency Synchronous Step-Down DCDC Regulator</description>
<gates>
<gate name="A" symbol="LM26420XMH"/>
</gates>
<devices>
<device name="" package="SOP65P640X175-21N">
<connects>
<connect gate="A" pin="AGND" pad="20"/>
<connect gate="A" pin="EN1" pad="2"/>
<connect gate="A" pin="EN2" pad="19"/>
<connect gate="A" pin="EPAD" pad="21"/>
<connect gate="A" pin="FB1" pad="8"/>
<connect gate="A" pin="FB2" pad="13"/>
<connect gate="A" pin="GND" pad="11"/>
<connect gate="A" pin="GND_2" pad="10"/>
<connect gate="A" pin="PGND" pad="15"/>
<connect gate="A" pin="PGND1" pad="7"/>
<connect gate="A" pin="PGND1_2" pad="6"/>
<connect gate="A" pin="PGND_2" pad="12"/>
<connect gate="A" pin="PGND_3" pad="14"/>
<connect gate="A" pin="PGND_4" pad="9"/>
<connect gate="A" pin="SW1" pad="5"/>
<connect gate="A" pin="SW2" pad="16"/>
<connect gate="A" pin="VINC" pad="1"/>
<connect gate="A" pin="VIND1" pad="3"/>
<connect gate="A" pin="VIND1_2" pad="4"/>
<connect gate="A" pin="VIND2" pad="18"/>
<connect gate="A" pin="VIND2_2" pad="17"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM26420XMH"/>
<attribute name="OC_FARNELL" value="1735794"/>
<attribute name="OC_NEWARK" value="14R4583"/>
<attribute name="PACKAGE" value="TSSOP-20"/>
<attribute name="SUPPLIER" value="National semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM26420XSQ" prefix="U">
<description>Frequency Synchronous Step-Down DCDC Regulator</description>
<gates>
<gate name="A" symbol="LM26420XSQ"/>
</gates>
<devices>
<device name="" package="QFN65P400X400X80-17N">
<connects>
<connect gate="A" pin="AGND" pad="14"/>
<connect gate="A" pin="EN1" pad="16"/>
<connect gate="A" pin="EN2" pad="13"/>
<connect gate="A" pin="EPAD" pad="17"/>
<connect gate="A" pin="FB1" pad="5"/>
<connect gate="A" pin="FB2" pad="8"/>
<connect gate="A" pin="FG1" pad="6"/>
<connect gate="A" pin="FG2" pad="7"/>
<connect gate="A" pin="PGND1" pad="4"/>
<connect gate="A" pin="PGND2" pad="9"/>
<connect gate="A" pin="SW1" pad="3"/>
<connect gate="A" pin="SW2" pad="10"/>
<connect gate="A" pin="VIND1" pad="2"/>
<connect gate="A" pin="VIND1_2" pad="1"/>
<connect gate="A" pin="VIND2" pad="12"/>
<connect gate="A" pin="VIND2_2" pad="11"/>
<connect gate="A" pin="VINDC" pad="15"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM26420XSQ"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="55R3844"/>
<attribute name="PACKAGE" value="QFN-16"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM26420YMH" prefix="U">
<description>Frequency Synchronous Step-Down DCDC Regulator</description>
<gates>
<gate name="A" symbol="LM26420YMH"/>
</gates>
<devices>
<device name="" package="SOP65P640X175-21N">
<connects>
<connect gate="A" pin="AGND" pad="20"/>
<connect gate="A" pin="EN1" pad="2"/>
<connect gate="A" pin="EN2" pad="19"/>
<connect gate="A" pin="EPAD" pad="21"/>
<connect gate="A" pin="FB1" pad="8"/>
<connect gate="A" pin="FB2" pad="13"/>
<connect gate="A" pin="GND" pad="11"/>
<connect gate="A" pin="GND_2" pad="10"/>
<connect gate="A" pin="PGND" pad="15"/>
<connect gate="A" pin="PGND1" pad="7"/>
<connect gate="A" pin="PGND1_2" pad="6"/>
<connect gate="A" pin="PGND_2" pad="12"/>
<connect gate="A" pin="PGND_3" pad="14"/>
<connect gate="A" pin="PGND_4" pad="9"/>
<connect gate="A" pin="SW1" pad="5"/>
<connect gate="A" pin="SW2" pad="16"/>
<connect gate="A" pin="VINC" pad="1"/>
<connect gate="A" pin="VIND1" pad="3"/>
<connect gate="A" pin="VIND1_2" pad="4"/>
<connect gate="A" pin="VIND2" pad="18"/>
<connect gate="A" pin="VIND2_2" pad="17"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM26420YMH"/>
<attribute name="OC_FARNELL" value="1735795"/>
<attribute name="OC_NEWARK" value="14R4584"/>
<attribute name="PACKAGE" value="TSSOP-20"/>
<attribute name="SUPPLIER" value="National semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM26420YSQ" prefix="U">
<description>Frequency Synchronous Step-Down DCDC Regulator</description>
<gates>
<gate name="A" symbol="LM26420YSQ"/>
</gates>
<devices>
<device name="" package="QFN65P400X400X80-17N">
<connects>
<connect gate="A" pin="AGND" pad="14"/>
<connect gate="A" pin="EN1" pad="16"/>
<connect gate="A" pin="EN2" pad="13"/>
<connect gate="A" pin="EPAD" pad="17"/>
<connect gate="A" pin="FB1" pad="5"/>
<connect gate="A" pin="FB2" pad="8"/>
<connect gate="A" pin="FG1" pad="6"/>
<connect gate="A" pin="FG2" pad="7"/>
<connect gate="A" pin="PGND1" pad="4"/>
<connect gate="A" pin="PGND2" pad="9"/>
<connect gate="A" pin="SW1" pad="3"/>
<connect gate="A" pin="SW2" pad="10"/>
<connect gate="A" pin="VINC" pad="15"/>
<connect gate="A" pin="VIND1" pad="2"/>
<connect gate="A" pin="VIND1_2" pad="1"/>
<connect gate="A" pin="VIND2" pad="12"/>
<connect gate="A" pin="VIND2_2" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM26420YSQ"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="55R3849"/>
<attribute name="PACKAGE" value="QFN-16"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2642MTC" prefix="U">
<description>Two-Phase Synchronous Step-Down Switching Controller</description>
<gates>
<gate name="A" symbol="LM2642MTC"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-28N">
<connects>
<connect gate="A" pin="CBOOT1" pad="25"/>
<connect gate="A" pin="CBOOT2" pad="18"/>
<connect gate="A" pin="COMP1" pad="3"/>
<connect gate="A" pin="COMP2" pad="12"/>
<connect gate="A" pin="FB1" pad="4"/>
<connect gate="A" pin="FB2" pad="11"/>
<connect gate="A" pin="HDRV1" pad="26"/>
<connect gate="A" pin="HDRV2" pad="17"/>
<connect gate="A" pin="ILIM1" pad="2"/>
<connect gate="A" pin="ILIM2" pad="13"/>
<connect gate="A" pin="KS1" pad="1"/>
<connect gate="A" pin="KS2" pad="14"/>
<connect gate="A" pin="LDRV1" pad="23"/>
<connect gate="A" pin="LDRV2" pad="20"/>
<connect gate="A" pin="ON/SS1" pad="9"/>
<connect gate="A" pin="ON/SS2" pad="10"/>
<connect gate="A" pin="PGND" pad="21"/>
<connect gate="A" pin="PGOOD1" pad="5"/>
<connect gate="A" pin="RSENS2" pad="15"/>
<connect gate="A" pin="RSNS1" pad="28"/>
<connect gate="A" pin="SGND" pad="8"/>
<connect gate="A" pin="SW1" pad="27"/>
<connect gate="A" pin="SW2" pad="16"/>
<connect gate="A" pin="UVDELAY" pad="6"/>
<connect gate="A" pin="VDD1" pad="24"/>
<connect gate="A" pin="VDD2" pad="19"/>
<connect gate="A" pin="VIN" pad="22"/>
<connect gate="A" pin="VLIN5" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="National"/>
<attribute name="OC_FARNELL" value="8221952"/>
<attribute name="OC_NEWARK" value="41K3986"/>
<attribute name="PACKAGE" value="SOP-28"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2647MTC" prefix="U">
<description>Dual Synchronous Buck Regulator Controller</description>
<gates>
<gate name="A" symbol="LM2647MTC"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-28N">
<connects>
<connect gate="A" pin="BOOT1" pad="25"/>
<connect gate="A" pin="BOOT2" pad="18"/>
<connect gate="A" pin="COMP1" pad="3"/>
<connect gate="A" pin="COMP2" pad="12"/>
<connect gate="A" pin="EN" pad="8"/>
<connect gate="A" pin="FB1" pad="2"/>
<connect gate="A" pin="FB2" pad="13"/>
<connect gate="A" pin="FPWM" pad="10"/>
<connect gate="A" pin="FREQ" pad="6"/>
<connect gate="A" pin="HDRV1" pad="26"/>
<connect gate="A" pin="HDRV2" pad="17"/>
<connect gate="A" pin="ILIM1" pad="28"/>
<connect gate="A" pin="ILIM2" pad="15"/>
<connect gate="A" pin="LDRV1" pad="23"/>
<connect gate="A" pin="LDRV2" pad="20"/>
<connect gate="A" pin="PGND1" pad="24"/>
<connect gate="A" pin="PGND2" pad="19"/>
<connect gate="A" pin="PGOOD" pad="9"/>
<connect gate="A" pin="SENSE1" pad="1"/>
<connect gate="A" pin="SENSE2" pad="14"/>
<connect gate="A" pin="SGND" pad="7"/>
<connect gate="A" pin="SS1" pad="4"/>
<connect gate="A" pin="SS2" pad="11"/>
<connect gate="A" pin="SW1" pad="27"/>
<connect gate="A" pin="SW2" pad="16"/>
<connect gate="A" pin="V5" pad="21"/>
<connect gate="A" pin="VDD" pad="5"/>
<connect gate="A" pin="VIN" pad="22"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2647MTC"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K3992"/>
<attribute name="PACKAGE" value="TSSOP-28"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM26480SQ-AA" prefix="U">
<description>Dual High-Current Step-Down DC/DC and Dual Linear Regulators</description>
<gates>
<gate name="A" symbol="LM26480SQ-AA"/>
</gates>
<devices>
<device name="" package="QFN400X400X80-25N">
<connects>
<connect gate="A" pin="AVDD" pad="10"/>
<connect gate="A" pin="ENLDO1" pad="17"/>
<connect gate="A" pin="ENLDO2" pad="16"/>
<connect gate="A" pin="ENSW1" pad="7"/>
<connect gate="A" pin="ENSW2" pad="12"/>
<connect gate="A" pin="EPAD" pad="25"/>
<connect gate="A" pin="FB1" pad="8"/>
<connect gate="A" pin="FB2" pad="11"/>
<connect gate="A" pin="FBL1" pad="21"/>
<connect gate="A" pin="FBL2" pad="22"/>
<connect gate="A" pin="GND_C" pad="9"/>
<connect gate="A" pin="GND_L" pad="18"/>
<connect gate="A" pin="GND_SW1" pad="4"/>
<connect gate="A" pin="GND_SW2" pad="15"/>
<connect gate="A" pin="LDO1" pad="20"/>
<connect gate="A" pin="LDO2" pad="23"/>
<connect gate="A" pin="NPOR" pad="3"/>
<connect gate="A" pin="SW1" pad="5"/>
<connect gate="A" pin="SW2" pad="14"/>
<connect gate="A" pin="SYNC" pad="2"/>
<connect gate="A" pin="VIN1" pad="6"/>
<connect gate="A" pin="VIN2" pad="13"/>
<connect gate="A" pin="VINLDO1" pad="19"/>
<connect gate="A" pin="VINLDO12" pad="1"/>
<connect gate="A" pin="VINLDO2" pad="24"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM26480SQ-AA"/>
<attribute name="OC_FARNELL" value="1552434"/>
<attribute name="OC_NEWARK" value="78M7734"/>
<attribute name="PACKAGE" value="QFN-24"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2650M-ADJ" prefix="U">
<description>DC/DC CONVERTER</description>
<gates>
<gate name="A" symbol="LM2650M-ADJ"/>
</gates>
<devices>
<device name="" package="SOIC127P1032X265-24N">
<connects>
<connect gate="A" pin="BOOT" pad="11"/>
<connect gate="A" pin="COMP" pad="15"/>
<connect gate="A" pin="EA_OUT" pad="16"/>
<connect gate="A" pin="FB" pad="13"/>
<connect gate="A" pin="FREQ_ADJ" pad="20"/>
<connect gate="A" pin="GND" pad="18"/>
<connect gate="A" pin="PGND" pad="9"/>
<connect gate="A" pin="PGND_2" pad="3"/>
<connect gate="A" pin="PGND_3" pad="10"/>
<connect gate="A" pin="PGND_4" pad="4"/>
<connect gate="A" pin="PVIN" pad="7"/>
<connect gate="A" pin="PVIN_2" pad="6"/>
<connect gate="A" pin="SD" pad="22"/>
<connect gate="A" pin="SLEEP_IN_ADJ" pad="24"/>
<connect gate="A" pin="SLEEP_LOGIC" pad="2"/>
<connect gate="A" pin="SLEEP_OUT_ADJ" pad="23"/>
<connect gate="A" pin="SS" pad="17"/>
<connect gate="A" pin="SUB" pad="12"/>
<connect gate="A" pin="SUB_2" pad="1"/>
<connect gate="A" pin="SW" pad="8"/>
<connect gate="A" pin="SW_2" pad="5"/>
<connect gate="A" pin="SYNC" pad="21"/>
<connect gate="A" pin="VDD" pad="14"/>
<connect gate="A" pin="VIN" pad="19"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2650M-ADJ"/>
<attribute name="OC_FARNELL" value="9494200"/>
<attribute name="OC_NEWARK" value="97K3263"/>
<attribute name="PACKAGE" value="24-SOIC"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2651MTC-1.8" prefix="U">
<description>Switching Regulator</description>
<gates>
<gate name="A" symbol="LM2651MTC-1.8"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-16N">
<connects>
<connect gate="A" pin="AGND" pad="13"/>
<connect gate="A" pin="AGND_2" pad="12"/>
<connect gate="A" pin="AVIN" pad="7"/>
<connect gate="A" pin="COMP" pad="10"/>
<connect gate="A" pin="FB" pad="9"/>
<connect gate="A" pin="NC" pad="11"/>
<connect gate="A" pin="PGND" pad="16"/>
<connect gate="A" pin="PGND_2" pad="14"/>
<connect gate="A" pin="PGND_3" pad="15"/>
<connect gate="A" pin="SW" pad="2"/>
<connect gate="A" pin="SW_2" pad="1"/>
<connect gate="A" pin="VCB" pad="6"/>
<connect gate="A" pin="VIN" pad="5"/>
<connect gate="A" pin="VIN_2" pad="3"/>
<connect gate="A" pin="VIN_3" pad="4"/>
<connect gate="A" pin="~SD(SS)" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2651MTC-18"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="74C4011"/>
<attribute name="PACKAGE" value="TSSOP-16"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2651MTC-3.3" prefix="U">
<description>Switching Regulator</description>
<gates>
<gate name="A" symbol="LM2651MTC-3.3"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-16N">
<connects>
<connect gate="A" pin="AGND" pad="13"/>
<connect gate="A" pin="AGND_2" pad="12"/>
<connect gate="A" pin="AVIN" pad="7"/>
<connect gate="A" pin="COMP" pad="10"/>
<connect gate="A" pin="FB" pad="9"/>
<connect gate="A" pin="NC" pad="11"/>
<connect gate="A" pin="PGND" pad="16"/>
<connect gate="A" pin="PGND_2" pad="14"/>
<connect gate="A" pin="PGND_3" pad="15"/>
<connect gate="A" pin="SW" pad="2"/>
<connect gate="A" pin="SW_2" pad="1"/>
<connect gate="A" pin="VCB" pad="6"/>
<connect gate="A" pin="VIN" pad="5"/>
<connect gate="A" pin="VIN_2" pad="3"/>
<connect gate="A" pin="VIN_3" pad="4"/>
<connect gate="A" pin="~SD(SS)" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2651MTC-3.3"/>
<attribute name="OC_FARNELL" value="1469197"/>
<attribute name="OC_NEWARK" value="41K4001"/>
<attribute name="PACKAGE" value="TSSOP-16"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2651MTC-ADJ" prefix="U">
<description>Switching Regulator</description>
<gates>
<gate name="A" symbol="LM2651MTC-ADJ"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-16N">
<connects>
<connect gate="A" pin="AGND" pad="13"/>
<connect gate="A" pin="AGND_2" pad="12"/>
<connect gate="A" pin="AVIN" pad="7"/>
<connect gate="A" pin="COMP" pad="10"/>
<connect gate="A" pin="FB" pad="9"/>
<connect gate="A" pin="NC" pad="11"/>
<connect gate="A" pin="PGND" pad="16"/>
<connect gate="A" pin="PGND_2" pad="14"/>
<connect gate="A" pin="PGND_3" pad="15"/>
<connect gate="A" pin="SW" pad="2"/>
<connect gate="A" pin="SW_2" pad="1"/>
<connect gate="A" pin="VCB" pad="6"/>
<connect gate="A" pin="VIN" pad="5"/>
<connect gate="A" pin="VIN_2" pad="3"/>
<connect gate="A" pin="VIN_3" pad="4"/>
<connect gate="A" pin="~SD/SS" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2651MTC-ADJ"/>
<attribute name="OC_FARNELL" value="41K3998"/>
<attribute name="OC_NEWARK" value="9778900"/>
<attribute name="PACKAGE" value="16-TSSOP"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2653MTC-ADJ" prefix="U">
<description>Switching Regulator</description>
<gates>
<gate name="A" symbol="LM2653MTC-ADJ"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-16N">
<connects>
<connect gate="A" pin="AGND" pad="13"/>
<connect gate="A" pin="AVIN" pad="7"/>
<connect gate="A" pin="COMP" pad="10"/>
<connect gate="A" pin="FB" pad="9"/>
<connect gate="A" pin="LDELAY" pad="12"/>
<connect gate="A" pin="PGND" pad="16"/>
<connect gate="A" pin="PGND_2" pad="14"/>
<connect gate="A" pin="PGND_3" pad="15"/>
<connect gate="A" pin="PGOOD" pad="11"/>
<connect gate="A" pin="SW" pad="2"/>
<connect gate="A" pin="SW_2" pad="1"/>
<connect gate="A" pin="VCB" pad="6"/>
<connect gate="A" pin="VIN" pad="5"/>
<connect gate="A" pin="VIN_2" pad="3"/>
<connect gate="A" pin="VIN_3" pad="4"/>
<connect gate="A" pin="~SD(SS)" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2653MTC-ADJ"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K4006"/>
<attribute name="PACKAGE" value="TSSOP-16"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2655MTC-3.3" prefix="U">
<description>Switching Regulator</description>
<gates>
<gate name="A" symbol="LM2655MTC-3.3"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-16N">
<connects>
<connect gate="A" pin="AVIN" pad="7"/>
<connect gate="A" pin="COMP" pad="10"/>
<connect gate="A" pin="FB" pad="9"/>
<connect gate="A" pin="GND" pad="13"/>
<connect gate="A" pin="LDELAY" pad="11"/>
<connect gate="A" pin="LDR" pad="12"/>
<connect gate="A" pin="PVIN" pad="16"/>
<connect gate="A" pin="PVIN_2" pad="4"/>
<connect gate="A" pin="PVIN_3" pad="3"/>
<connect gate="A" pin="PVIN_4" pad="5"/>
<connect gate="A" pin="PVIN_5" pad="14"/>
<connect gate="A" pin="PVIN_6" pad="15"/>
<connect gate="A" pin="SW" pad="2"/>
<connect gate="A" pin="SW_2" pad="1"/>
<connect gate="A" pin="VCB" pad="6"/>
<connect gate="A" pin="~SD(SS)" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2655MTC-3.3"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K4009"/>
<attribute name="PACKAGE" value="TSSOP-16"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2655MTC-ADJ" prefix="U">
<description>Switching Regulator</description>
<gates>
<gate name="A" symbol="LM2655MTC-ADJ"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-16N">
<connects>
<connect gate="A" pin="AVIN" pad="7"/>
<connect gate="A" pin="COMP" pad="10"/>
<connect gate="A" pin="FB" pad="9"/>
<connect gate="A" pin="GND" pad="13"/>
<connect gate="A" pin="LDELAY" pad="11"/>
<connect gate="A" pin="LDR" pad="12"/>
<connect gate="A" pin="PVIN" pad="16"/>
<connect gate="A" pin="PVIN_2" pad="4"/>
<connect gate="A" pin="PVIN_3" pad="3"/>
<connect gate="A" pin="PVIN_4" pad="5"/>
<connect gate="A" pin="PVIN_5" pad="14"/>
<connect gate="A" pin="PVIN_6" pad="15"/>
<connect gate="A" pin="SW" pad="2"/>
<connect gate="A" pin="SW_2" pad="1"/>
<connect gate="A" pin="VCB" pad="6"/>
<connect gate="A" pin="~SD(SS)" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2655MTC-ADJ"/>
<attribute name="OC_FARNELL" value="1685619"/>
<attribute name="OC_NEWARK" value="41K4008"/>
<attribute name="PACKAGE" value="TSSOP-16"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2660M" prefix="U">
<description>Switched Capacitor Voltage Converter</description>
<gates>
<gate name="A" symbol="LM2660M"/>
</gates>
<devices>
<device name="" package="SOIC127P620X175-8N">
<connects>
<connect gate="A" pin="CAP+" pad="2"/>
<connect gate="A" pin="CAP-" pad="4"/>
<connect gate="A" pin="FC" pad="1"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="LV" pad="6"/>
<connect gate="A" pin="OSC" pad="7"/>
<connect gate="A" pin="OUT" pad="5"/>
<connect gate="A" pin="V+" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2660M"/>
<attribute name="OC_FARNELL" value="9493816"/>
<attribute name="OC_NEWARK" value="41K4014"/>
<attribute name="PACKAGE" value="8-SOIC"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2660MM" prefix="U">
<description>Voltage Converter</description>
<gates>
<gate name="A" symbol="LM2660MM"/>
</gates>
<devices>
<device name="" package="SOP65P490X110-8N">
<connects>
<connect gate="A" pin="CAP+" pad="2"/>
<connect gate="A" pin="CAP-" pad="4"/>
<connect gate="A" pin="FC" pad="1"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="LV" pad="6"/>
<connect gate="A" pin="OSC" pad="7"/>
<connect gate="A" pin="OUT" pad="5"/>
<connect gate="A" pin="V+" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2660MM"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K4015"/>
<attribute name="PACKAGE" value="MSOP-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2662M" prefix="U">
<description>Switched Capacitor Voltage Converter</description>
<gates>
<gate name="A" symbol="LM2662M"/>
</gates>
<devices>
<device name="" package="SOIC127P620X175-8N">
<connects>
<connect gate="A" pin="CAP+" pad="2"/>
<connect gate="A" pin="CAP-" pad="4"/>
<connect gate="A" pin="FC" pad="1"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="LV" pad="6"/>
<connect gate="A" pin="OSC" pad="7"/>
<connect gate="A" pin="OUT" pad="5"/>
<connect gate="A" pin="V+" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2662M"/>
<attribute name="OC_FARNELL" value="9306803"/>
<attribute name="OC_NEWARK" value="07B6186"/>
<attribute name="PACKAGE" value="8-SOIC"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2663M" prefix="U">
<description>Voltage Converter</description>
<gates>
<gate name="A" symbol="LM2663M"/>
</gates>
<devices>
<device name="" package="SOIC127P620X175-8N">
<connects>
<connect gate="A" pin="CAP+" pad="2"/>
<connect gate="A" pin="CAP-" pad="4"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="LV" pad="6"/>
<connect gate="A" pin="OSC" pad="7"/>
<connect gate="A" pin="OUT" pad="5"/>
<connect gate="A" pin="SD" pad="1"/>
<connect gate="A" pin="V+" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2663M"/>
<attribute name="OC_FARNELL" value="1469160"/>
<attribute name="OC_NEWARK" value="41K4024"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2664M6" prefix="U">
<description>Switched Capacitor Voltage Converter</description>
<gates>
<gate name="A" symbol="LM2664M6"/>
</gates>
<devices>
<device name="" package="SOT95P300X120-6N">
<connects>
<connect gate="A" pin="CAP+" pad="6"/>
<connect gate="A" pin="CAP-" pad="3"/>
<connect gate="A" pin="GND" pad="1"/>
<connect gate="A" pin="OUT" pad="2"/>
<connect gate="A" pin="V+" pad="5"/>
<connect gate="A" pin="~SD" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2664M6"/>
<attribute name="OC_FARNELL" value="9779671"/>
<attribute name="OC_NEWARK" value="-"/>
<attribute name="PACKAGE" value="SOT-23-6"/>
<attribute name="SUPPLIER" value="NATIONAL SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2665M6" prefix="U">
<description>Voltage Converter</description>
<gates>
<gate name="A" symbol="LM2665M6"/>
</gates>
<devices>
<device name="" package="SOT95P285X120-6N">
<connects>
<connect gate="A" pin="CAP+" pad="6"/>
<connect gate="A" pin="CAP-" pad="3"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="OUT" pad="5"/>
<connect gate="A" pin="SD" pad="4"/>
<connect gate="A" pin="V+" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2665M6"/>
<attribute name="OC_FARNELL" value="1469163"/>
<attribute name="OC_NEWARK" value="41K4028"/>
<attribute name="PACKAGE" value="SOT-6"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2670S-12" prefix="U">
<description>SIMPLE SWITCHER</description>
<gates>
<gate name="A" symbol="LM2670S-12"/>
</gates>
<devices>
<device name="" package="TO127P1435X457-7N">
<connects>
<connect gate="A" pin="C_BOOST" pad="3"/>
<connect gate="A" pin="FB" pad="6"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="GND_2" pad="8"/>
<connect gate="A" pin="IN" pad="2"/>
<connect gate="A" pin="ON/~OFF" pad="7"/>
<connect gate="A" pin="SW_OUT" pad="1"/>
<connect gate="A" pin="SYNC" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2670S-12"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K4031"/>
<attribute name="PACKAGE" value="TO-263-7"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2670S-3.3" prefix="U">
<description>SIMPLE SWITCHER</description>
<gates>
<gate name="A" symbol="LM2670S-3.3"/>
</gates>
<devices>
<device name="" package="TO127P1435X457-7N">
<connects>
<connect gate="A" pin="C_BOOST" pad="3"/>
<connect gate="A" pin="FB" pad="6"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="GND_2" pad="8"/>
<connect gate="A" pin="IN" pad="2"/>
<connect gate="A" pin="ON/~OFF" pad="7"/>
<connect gate="A" pin="SW_OUT" pad="1"/>
<connect gate="A" pin="SYNC" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2670S-3.3"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K4032"/>
<attribute name="PACKAGE" value="TO-263-7"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2670S-5.0" prefix="U">
<description>SIMPLE SWITCHER</description>
<gates>
<gate name="A" symbol="LM2670S-5.0"/>
</gates>
<devices>
<device name="" package="TO127P1435X457-7N">
<connects>
<connect gate="A" pin="C_BOOST" pad="3"/>
<connect gate="A" pin="FB" pad="6"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="GND_2" pad="8"/>
<connect gate="A" pin="IN" pad="2"/>
<connect gate="A" pin="ON/~OFF" pad="7"/>
<connect gate="A" pin="SW_OUT" pad="1"/>
<connect gate="A" pin="SYNC" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2670S-5.0"/>
<attribute name="OC_FARNELL" value="1564795"/>
<attribute name="OC_NEWARK" value="41K4033"/>
<attribute name="PACKAGE" value="TO-263-7"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2670S-ADJ" prefix="U">
<description>SIMPLE SWITCHER</description>
<gates>
<gate name="A" symbol="LM2670S-ADJ"/>
</gates>
<devices>
<device name="" package="TO127P1435X457-7N">
<connects>
<connect gate="A" pin="C_BOOST" pad="3"/>
<connect gate="A" pin="FB" pad="6"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="GND_2" pad="8"/>
<connect gate="A" pin="IN" pad="2"/>
<connect gate="A" pin="ON/~OFF" pad="7"/>
<connect gate="A" pin="SW_OUT" pad="1"/>
<connect gate="A" pin="SYNC" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2670S-ADJ"/>
<attribute name="OC_FARNELL" value="1286849"/>
<attribute name="OC_NEWARK" value="41K4030"/>
<attribute name="PACKAGE" value="TO-263-7"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2670SD-12" prefix="U">
<description>SIMPLE SWITCHER</description>
<gates>
<gate name="A" symbol="LM2670SD-12"/>
</gates>
<devices>
<device name="" package="DFN600X500X100-15N">
<connects>
<connect gate="A" pin="CB" pad="4"/>
<connect gate="A" pin="EPAD" pad="15"/>
<connect gate="A" pin="FB" pad="7"/>
<connect gate="A" pin="GND" pad="9"/>
<connect gate="A" pin="NC" pad="10"/>
<connect gate="A" pin="NC_2" pad="5"/>
<connect gate="A" pin="NC_3" pad="1"/>
<connect gate="A" pin="NC_4" pad="11"/>
<connect gate="A" pin="ON/OFF" pad="8"/>
<connect gate="A" pin="SYNC" pad="6"/>
<connect gate="A" pin="VIN" pad="3"/>
<connect gate="A" pin="VIN_2" pad="2"/>
<connect gate="A" pin="VSW" pad="14"/>
<connect gate="A" pin="VSW_2" pad="12"/>
<connect gate="A" pin="VSW_3" pad="13"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2670SD-12"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="09J8497"/>
<attribute name="PACKAGE" value="DFN-15"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2670SD-ADJ" prefix="U">
<description>Step-Down Voltage Regulator</description>
<gates>
<gate name="A" symbol="LM2670SD-ADJ"/>
</gates>
<devices>
<device name="" package="DFN500X400X100-15N">
<connects>
<connect gate="A" pin="CB" pad="4"/>
<connect gate="A" pin="EPAD" pad="15"/>
<connect gate="A" pin="FB" pad="7"/>
<connect gate="A" pin="GND" pad="9"/>
<connect gate="A" pin="NC" pad="11"/>
<connect gate="A" pin="NC_2" pad="5"/>
<connect gate="A" pin="NC_3" pad="1"/>
<connect gate="A" pin="NC_4" pad="10"/>
<connect gate="A" pin="ON/~OFF" pad="8"/>
<connect gate="A" pin="SYNC" pad="6"/>
<connect gate="A" pin="VIN" pad="3"/>
<connect gate="A" pin="VIN_2" pad="2"/>
<connect gate="A" pin="VSW" pad="14"/>
<connect gate="A" pin="VSW_2" pad="12"/>
<connect gate="A" pin="VSW_3" pad="13"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2670SD-ADJ"/>
<attribute name="OC_FARNELL" value="1495087"/>
<attribute name="OC_NEWARK" value="41K4034"/>
<attribute name="PACKAGE" value="DFN-14"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2670T-ADJ" prefix="U">
<description>IC BUCK ADJ 3A</description>
<gates>
<gate name="A" symbol="LM2670T-ADJ"/>
</gates>
<devices>
<device name="" package="TO127P470X1016X1740-7P">
<connects>
<connect gate="A" pin="*ON-OFF" pad="7"/>
<connect gate="A" pin="C_BOOST" pad="3"/>
<connect gate="A" pin="FEEDBACK" pad="6"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="INPUT" pad="2"/>
<connect gate="A" pin="SW_OUTPUT" pad="1"/>
<connect gate="A" pin="SYNC" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2670T-ADJ"/>
<attribute name="OC_FARNELL" value="1685622"/>
<attribute name="OC_NEWARK" value="41K4046"/>
<attribute name="PACKAGE" value="TO220-7"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2671M-12" prefix="U">
<description>SIMPLE SWITCHER</description>
<gates>
<gate name="A" symbol="LM2671M-12"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="CB" pad="1"/>
<connect gate="A" pin="FB" pad="4"/>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="ON/~OFF" pad="5"/>
<connect gate="A" pin="SS" pad="2"/>
<connect gate="A" pin="SW" pad="8"/>
<connect gate="A" pin="SYNC" pad="3"/>
<connect gate="A" pin="VIN" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2671M-12"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="07B6193"/>
<attribute name="PACKAGE" value="SO-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2671M-3.3" prefix="U">
<description>SIMPLE SWITCHER</description>
<gates>
<gate name="A" symbol="LM2671M-3.3"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="CB" pad="1"/>
<connect gate="A" pin="FB" pad="4"/>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="ON/~OFF" pad="5"/>
<connect gate="A" pin="SS" pad="2"/>
<connect gate="A" pin="SW" pad="8"/>
<connect gate="A" pin="SYNC" pad="3"/>
<connect gate="A" pin="VIN" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2671M-3.3"/>
<attribute name="OC_FARNELL" value="1685779"/>
<attribute name="OC_NEWARK" value="41K4060"/>
<attribute name="PACKAGE" value="SO-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2671M-5.0" prefix="U">
<description>SIMPLE SWITCHER</description>
<gates>
<gate name="A" symbol="LM2671M-5.0"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="CB" pad="1"/>
<connect gate="A" pin="FB" pad="4"/>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="ON/~OFF" pad="5"/>
<connect gate="A" pin="SS" pad="2"/>
<connect gate="A" pin="SW" pad="8"/>
<connect gate="A" pin="SYNC" pad="3"/>
<connect gate="A" pin="VIN" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2671M-5.0"/>
<attribute name="OC_FARNELL" value="1469200"/>
<attribute name="OC_NEWARK" value="41K4061"/>
<attribute name="PACKAGE" value="SO-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2671M-ADJ" prefix="U">
<description>SIMPLE SWITCHER</description>
<gates>
<gate name="A" symbol="LM2671M-ADJ"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="CB" pad="1"/>
<connect gate="A" pin="FB" pad="4"/>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="ON/~OFF" pad="5"/>
<connect gate="A" pin="SS" pad="2"/>
<connect gate="A" pin="SW" pad="8"/>
<connect gate="A" pin="SYNC" pad="3"/>
<connect gate="A" pin="VIN" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2671M-ADJ"/>
<attribute name="OC_FARNELL" value="1850242"/>
<attribute name="OC_NEWARK" value="41K4058"/>
<attribute name="PACKAGE" value="SO-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2671N-3.3" prefix="U">
<description>SIMPLE SWITCHER</description>
<gates>
<gate name="A" symbol="LM2671N-3.3"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-8">
<connects>
<connect gate="A" pin="CB" pad="1"/>
<connect gate="A" pin="FB" pad="4"/>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="ON/~OFF" pad="5"/>
<connect gate="A" pin="SS" pad="2"/>
<connect gate="A" pin="SW" pad="8"/>
<connect gate="A" pin="SYNC" pad="3"/>
<connect gate="A" pin="VIN" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2671N-3.3"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="07B6200"/>
<attribute name="PACKAGE" value="DIP-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2671N-5.0" prefix="U">
<description>SIMPLE SWITCHER</description>
<gates>
<gate name="A" symbol="LM2671N-5.0"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-8">
<connects>
<connect gate="A" pin="CB" pad="1"/>
<connect gate="A" pin="FB" pad="4"/>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="ON/~OFF" pad="5"/>
<connect gate="A" pin="SS" pad="2"/>
<connect gate="A" pin="SW" pad="8"/>
<connect gate="A" pin="SYNC" pad="3"/>
<connect gate="A" pin="VIN" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2671N-5.0"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K4069"/>
<attribute name="PACKAGE" value="DIP-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2671N-ADJ" prefix="U">
<description>SIMPLE SWITCHER</description>
<gates>
<gate name="A" symbol="LM2671N-ADJ"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-8">
<connects>
<connect gate="A" pin="CB" pad="1"/>
<connect gate="A" pin="FB" pad="4"/>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="ON/~OFF" pad="5"/>
<connect gate="A" pin="SS" pad="2"/>
<connect gate="A" pin="SW" pad="8"/>
<connect gate="A" pin="SYNC" pad="3"/>
<connect gate="A" pin="VIN" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2671N-ADJ"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K4066"/>
<attribute name="PACKAGE" value="DIP-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2672M-12" prefix="U">
<description>SIMPLE SWITCHER</description>
<gates>
<gate name="A" symbol="LM2672M-12"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="CB" pad="1"/>
<connect gate="A" pin="FB" pad="4"/>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="ON/~OFF" pad="5"/>
<connect gate="A" pin="SS" pad="2"/>
<connect gate="A" pin="SYNC" pad="3"/>
<connect gate="A" pin="VIN" pad="7"/>
<connect gate="A" pin="VSW" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2672M-12"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K4079"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2672M-3.3" prefix="U">
<description>Power converter</description>
<gates>
<gate name="A" symbol="LM2672M-3.3"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="CB" pad="1"/>
<connect gate="A" pin="FB" pad="4"/>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="ON/~OFF" pad="5"/>
<connect gate="A" pin="SS" pad="2"/>
<connect gate="A" pin="SYNC" pad="3"/>
<connect gate="A" pin="VIN" pad="7"/>
<connect gate="A" pin="VSW" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2672M-3.3"/>
<attribute name="OC_FARNELL" value="4466550"/>
<attribute name="OC_NEWARK" value="41K4080"/>
<attribute name="PACKAGE" value="8-SOIC"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2672M-5.0" prefix="U">
<description>Power converter</description>
<gates>
<gate name="A" symbol="LM2672M-5.0"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="CB" pad="1"/>
<connect gate="A" pin="FB" pad="4"/>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="ON/~OFF" pad="5"/>
<connect gate="A" pin="SS" pad="2"/>
<connect gate="A" pin="SYNC" pad="3"/>
<connect gate="A" pin="VIN" pad="7"/>
<connect gate="A" pin="VSW" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2672M-5.0"/>
<attribute name="OC_FARNELL" value="9489797"/>
<attribute name="OC_NEWARK" value="41K4081"/>
<attribute name="PACKAGE" value="8-SOIC"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2672M-ADJ" prefix="U">
<description>Step-Down Voltage Regulator</description>
<gates>
<gate name="A" symbol="LM2672M-ADJ"/>
</gates>
<devices>
<device name="" package="SOIC127P620X175-8N">
<connects>
<connect gate="A" pin="CB" pad="1"/>
<connect gate="A" pin="FB" pad="4"/>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="ON/~OFF" pad="5"/>
<connect gate="A" pin="SS" pad="2"/>
<connect gate="A" pin="SYNC" pad="3"/>
<connect gate="A" pin="VIN" pad="7"/>
<connect gate="A" pin="VSW" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2672M-ADJ"/>
<attribute name="OC_FARNELL" value="9489789"/>
<attribute name="OC_NEWARK" value="41K4078"/>
<attribute name="PACKAGE" value="8-SOIC"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2672N-3.3" prefix="U">
<description>SIMPLE SWITCHER</description>
<gates>
<gate name="A" symbol="LM2672N-3.3"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-8">
<connects>
<connect gate="A" pin="CB" pad="1"/>
<connect gate="A" pin="FB" pad="4"/>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="ON/~OFF" pad="5"/>
<connect gate="A" pin="SS" pad="2"/>
<connect gate="A" pin="SYNC" pad="3"/>
<connect gate="A" pin="VIN" pad="7"/>
<connect gate="A" pin="VSW" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2672N-3.3"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="07B6210"/>
<attribute name="PACKAGE" value="DIP-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2672N-5.0" prefix="U">
<description>SIMPLE SWITCHER</description>
<gates>
<gate name="A" symbol="LM2672N-5.0"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-8">
<connects>
<connect gate="A" pin="CB" pad="1"/>
<connect gate="A" pin="FB" pad="4"/>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="ON/~OFF" pad="5"/>
<connect gate="A" pin="SS" pad="2"/>
<connect gate="A" pin="SYNC" pad="3"/>
<connect gate="A" pin="VIN" pad="7"/>
<connect gate="A" pin="VSW" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2672N-5.0"/>
<attribute name="OC_FARNELL" value="9489827"/>
<attribute name="OC_NEWARK" value="97K3271"/>
<attribute name="PACKAGE" value="DIP-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2672N-ADJ" prefix="U">
<description>SIMPLE SWITCHER</description>
<gates>
<gate name="A" symbol="LM2672N-ADJ"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-8">
<connects>
<connect gate="A" pin="CB" pad="1"/>
<connect gate="A" pin="FB" pad="4"/>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="ON/~OFF" pad="5"/>
<connect gate="A" pin="SS" pad="2"/>
<connect gate="A" pin="SYNC" pad="3"/>
<connect gate="A" pin="VIN" pad="7"/>
<connect gate="A" pin="VSW" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2672N-ADJ"/>
<attribute name="OC_FARNELL" value="9489835"/>
<attribute name="OC_NEWARK" value="41K4086"/>
<attribute name="PACKAGE" value="DIP-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2673S-12" prefix="U">
<description>Step-Down Voltage Regulator</description>
<gates>
<gate name="A" symbol="LM2673S-12"/>
</gates>
<devices>
<device name="" package="TO263127P1435X457-8N">
<connects>
<connect gate="A" pin="BOOST" pad="3"/>
<connect gate="A" pin="CL_ADJ" pad="5"/>
<connect gate="A" pin="FB" pad="6"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="SS" pad="7"/>
<connect gate="A" pin="SW" pad="1"/>
<connect gate="A" pin="TAB" pad="8"/>
<connect gate="A" pin="VIN" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2673S-12"/>
<attribute name="OC_FARNELL" value="9486151"/>
<attribute name="OC_NEWARK" value="41K4091"/>
<attribute name="PACKAGE" value="TO263-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2673S-3.3" prefix="U">
<description>Step-Down Voltage Regulator</description>
<gates>
<gate name="A" symbol="LM2673S-3.3"/>
</gates>
<devices>
<device name="" package="TO127P1435X457-8N">
<connects>
<connect gate="A" pin="CURRENT_ADJ" pad="5"/>
<connect gate="A" pin="C_BOOST" pad="3"/>
<connect gate="A" pin="FB" pad="6"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="GND_2" pad="8"/>
<connect gate="A" pin="IN" pad="2"/>
<connect gate="A" pin="SS" pad="7"/>
<connect gate="A" pin="SW_OUT" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2673S-3.3"/>
<attribute name="OC_FARNELL" value="1798316"/>
<attribute name="OC_NEWARK" value="41K4092"/>
<attribute name="PACKAGE" value="TO-236-7"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2673S-5.0" prefix="U">
<description>Step-Down Voltage Regulator</description>
<gates>
<gate name="A" symbol="LM2673S-5.0"/>
</gates>
<devices>
<device name="" package="TO127P1435X457-8N">
<connects>
<connect gate="A" pin="CURRENT_ADJ" pad="5"/>
<connect gate="A" pin="C_BOOST" pad="3"/>
<connect gate="A" pin="FB" pad="6"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="GND_2" pad="8"/>
<connect gate="A" pin="IN" pad="2"/>
<connect gate="A" pin="SS" pad="7"/>
<connect gate="A" pin="SW_OUT" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2673S-5.0"/>
<attribute name="OC_FARNELL" value="9486178"/>
<attribute name="OC_NEWARK" value="41K4093"/>
<attribute name="PACKAGE" value="TO-236-7"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2673S-ADJ" prefix="U">
<description>Step-Down Voltage Regulator</description>
<gates>
<gate name="A" symbol="LM2673S-ADJ"/>
</gates>
<devices>
<device name="" package="TO127P1435X457-8N">
<connects>
<connect gate="A" pin="CURRENT_ADJ" pad="5"/>
<connect gate="A" pin="C_BOOST" pad="3"/>
<connect gate="A" pin="FB" pad="6"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="GND_2" pad="8"/>
<connect gate="A" pin="IN" pad="2"/>
<connect gate="A" pin="SS" pad="7"/>
<connect gate="A" pin="SW_OUT" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2673S-ADJ"/>
<attribute name="OC_FARNELL" value="9486160"/>
<attribute name="OC_NEWARK" value="41K4090"/>
<attribute name="PACKAGE" value="TO-236-7"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2673SD-3.3" prefix="U">
<description>Step-Down Voltage Regulator</description>
<gates>
<gate name="A" symbol="LM2673SD-3.3"/>
</gates>
<devices>
<device name="" package="DFN600X500X100-15N">
<connects>
<connect gate="A" pin="BOOST" pad="4"/>
<connect gate="A" pin="CL_ADJ" pad="6"/>
<connect gate="A" pin="FB" pad="7"/>
<connect gate="A" pin="GND" pad="9"/>
<connect gate="A" pin="NC" pad="11"/>
<connect gate="A" pin="NC_2" pad="5"/>
<connect gate="A" pin="NC_3" pad="1"/>
<connect gate="A" pin="NC_4" pad="10"/>
<connect gate="A" pin="SS" pad="8"/>
<connect gate="A" pin="SW" pad="14"/>
<connect gate="A" pin="SW_2" pad="12"/>
<connect gate="A" pin="SW_3" pad="13"/>
<connect gate="A" pin="THER.PAD" pad="15"/>
<connect gate="A" pin="VIN" pad="3"/>
<connect gate="A" pin="VIN_2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2673SD-3.3"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K4096"/>
<attribute name="PACKAGE" value="DFN-15"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2673SD-5.0" prefix="U">
<description>Step-Down Voltage Regulator</description>
<gates>
<gate name="A" symbol="LM2673SD-5.0"/>
</gates>
<devices>
<device name="" package="DFN600X500X100-15N">
<connects>
<connect gate="A" pin="BOOST" pad="4"/>
<connect gate="A" pin="CL_ADJ" pad="6"/>
<connect gate="A" pin="FB" pad="7"/>
<connect gate="A" pin="GND" pad="9"/>
<connect gate="A" pin="NC" pad="1"/>
<connect gate="A" pin="NC_2" pad="5"/>
<connect gate="A" pin="NC_3" pad="10"/>
<connect gate="A" pin="NC_4" pad="11"/>
<connect gate="A" pin="SS" pad="8"/>
<connect gate="A" pin="SW" pad="14"/>
<connect gate="A" pin="SW_2" pad="12"/>
<connect gate="A" pin="SW_3" pad="13"/>
<connect gate="A" pin="THER_PAD" pad="15"/>
<connect gate="A" pin="VIN" pad="3"/>
<connect gate="A" pin="VIN_2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2673SD-5.0"/>
<attribute name="OC_FARNELL" value="1685623"/>
<attribute name="OC_NEWARK" value="41K4097"/>
<attribute name="PACKAGE" value="DFN-15"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2673SD-ADJ" prefix="U">
<description>Step-Down Voltage Regulator</description>
<gates>
<gate name="A" symbol="LM2673SD-ADJ"/>
</gates>
<devices>
<device name="" package="DFN600X500X100-15N">
<connects>
<connect gate="A" pin="BOOST" pad="4"/>
<connect gate="A" pin="CL_ADJ" pad="6"/>
<connect gate="A" pin="FB" pad="7"/>
<connect gate="A" pin="GND" pad="9"/>
<connect gate="A" pin="NC" pad="11"/>
<connect gate="A" pin="NC_2" pad="1"/>
<connect gate="A" pin="NC_3" pad="5"/>
<connect gate="A" pin="NC_4" pad="10"/>
<connect gate="A" pin="SS" pad="8"/>
<connect gate="A" pin="SW" pad="14"/>
<connect gate="A" pin="SW_2" pad="12"/>
<connect gate="A" pin="SW_3" pad="13"/>
<connect gate="A" pin="THER_PAD" pad="15"/>
<connect gate="A" pin="VIN" pad="3"/>
<connect gate="A" pin="VIN_2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2673SD-ADJ"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K4094"/>
<attribute name="PACKAGE" value="DFN-15"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2673T-12" prefix="U">
<description>SWITCHING REG 3A 12V, 2673, TO2207</description>
<gates>
<gate name="A" symbol="LM2673T-12"/>
</gates>
<devices>
<device name="" package="TO127P457X1016X2052-7P">
<connects>
<connect gate="A" pin="BOOST" pad="3"/>
<connect gate="A" pin="CL_ADJ" pad="5"/>
<connect gate="A" pin="FB" pad="6"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="SS" pad="7"/>
<connect gate="A" pin="SW" pad="1"/>
<connect gate="A" pin="VIN" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2673T-12"/>
<attribute name="OC_FARNELL" value="9485732"/>
<attribute name="OC_NEWARK" value="38K3665"/>
<attribute name="PACKAGE" value="TO-220-7"/>
<attribute name="SUPPLIER" value="NATIONAL SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2673T-3.3" prefix="U">
<description>IC BUCK 3.3V 3A</description>
<gates>
<gate name="A" symbol="LM2673T-3.3"/>
</gates>
<devices>
<device name="" package="TO127P470X1016X1740-7P">
<connects>
<connect gate="A" pin="CURRENT_ADJ" pad="5"/>
<connect gate="A" pin="C_BOOST" pad="3"/>
<connect gate="A" pin="FEEDBACK" pad="6"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="INPUT" pad="2"/>
<connect gate="A" pin="SOFTSTART" pad="7"/>
<connect gate="A" pin="SW_OUTPUT" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2673T-3.3"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K4108"/>
<attribute name="PACKAGE" value="TO220-7"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2673T-5.0" prefix="U">
<description>IC, STEP-DOWN REGULATOR</description>
<gates>
<gate name="A" symbol="LM2673T-5.0"/>
</gates>
<devices>
<device name="" package="TO127P457X1016X2052-7P">
<connects>
<connect gate="A" pin="BOOST" pad="3"/>
<connect gate="A" pin="CL_ADJ" pad="5"/>
<connect gate="A" pin="FB" pad="6"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="SS" pad="7"/>
<connect gate="A" pin="SW" pad="1"/>
<connect gate="A" pin="VIN" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2673T-5.0"/>
<attribute name="OC_FARNELL" value="9485740"/>
<attribute name="OC_NEWARK" value="13B5585"/>
<attribute name="PACKAGE" value="TO-220-7"/>
<attribute name="SUPPLIER" value="NATIONAL SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2673T-ADJ" prefix="U">
<description>SWITCHING REG 3A ADJ, 2673</description>
<gates>
<gate name="A" symbol="LM2673T-ADJ"/>
</gates>
<devices>
<device name="" package="TO127P457X1016X2052-7P">
<connects>
<connect gate="A" pin="BOOST" pad="3"/>
<connect gate="A" pin="CL_ADJ" pad="5"/>
<connect gate="A" pin="FB" pad="6"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="SS" pad="7"/>
<connect gate="A" pin="SW" pad="1"/>
<connect gate="A" pin="VIN" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2673T-ADJ"/>
<attribute name="OC_FARNELL" value="9485724"/>
<attribute name="OC_NEWARK" value="97K3273"/>
<attribute name="PACKAGE" value="TO-220-7"/>
<attribute name="SUPPLIER" value="NATIONAL SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2674LD-3.3" prefix="U">
<description>SIMPLE SWITCHER</description>
<gates>
<gate name="A" symbol="LM2674LD-3.3"/>
</gates>
<devices>
<device name="" package="DFN500X500X80-17N">
<connects>
<connect gate="A" pin="CB" pad="1"/>
<connect gate="A" pin="EPAD" pad="17"/>
<connect gate="A" pin="FB" pad="8"/>
<connect gate="A" pin="GND" pad="12"/>
<connect gate="A" pin="GND_2" pad="11"/>
<connect gate="A" pin="NC" pad="7"/>
<connect gate="A" pin="NC_2" pad="2"/>
<connect gate="A" pin="NC_3" pad="3"/>
<connect gate="A" pin="NC_4" pad="4"/>
<connect gate="A" pin="NC_5" pad="10"/>
<connect gate="A" pin="NC_6" pad="5"/>
<connect gate="A" pin="NC_7" pad="13"/>
<connect gate="A" pin="NC_8" pad="6"/>
<connect gate="A" pin="ON/OFF" pad="9"/>
<connect gate="A" pin="VIN" pad="14"/>
<connect gate="A" pin="VSW" pad="16"/>
<connect gate="A" pin="VSW_2" pad="15"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2674LD-33"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K4112"/>
<attribute name="PACKAGE" value="DFN-16"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2674LD-ADJ" prefix="U">
<description>SIMPLE SWITCHER</description>
<gates>
<gate name="A" symbol="LM2674LD-ADJ"/>
</gates>
<devices>
<device name="" package="DFN500X500X80-17N">
<connects>
<connect gate="A" pin="CB" pad="1"/>
<connect gate="A" pin="EPAD" pad="17"/>
<connect gate="A" pin="FB" pad="8"/>
<connect gate="A" pin="GND" pad="12"/>
<connect gate="A" pin="GND_2" pad="11"/>
<connect gate="A" pin="NC" pad="7"/>
<connect gate="A" pin="NC_2" pad="2"/>
<connect gate="A" pin="NC_3" pad="3"/>
<connect gate="A" pin="NC_4" pad="4"/>
<connect gate="A" pin="NC_5" pad="10"/>
<connect gate="A" pin="NC_6" pad="5"/>
<connect gate="A" pin="NC_7" pad="13"/>
<connect gate="A" pin="NC_8" pad="6"/>
<connect gate="A" pin="ON/OFF" pad="9"/>
<connect gate="A" pin="VIN" pad="14"/>
<connect gate="A" pin="VSW" pad="16"/>
<connect gate="A" pin="VSW_2" pad="15"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2674LD-ADJ"/>
<attribute name="OC_FARNELL" value="1312682"/>
<attribute name="OC_NEWARK" value="41K4110"/>
<attribute name="PACKAGE" value="DFN-16"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2674M-12" prefix="U">
<description>Step-Down Voltage Regulator</description>
<gates>
<gate name="A" symbol="LM2674M-12"/>
</gates>
<devices>
<device name="" package="SOIC127P620X175-8N">
<connects>
<connect gate="A" pin="CB" pad="1"/>
<connect gate="A" pin="FB" pad="4"/>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="NC" pad="3"/>
<connect gate="A" pin="NC_2" pad="2"/>
<connect gate="A" pin="ON/~OFF" pad="5"/>
<connect gate="A" pin="VIN" pad="7"/>
<connect gate="A" pin="VSW" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2674M-12"/>
<attribute name="OC_FARNELL" value="41K4119"/>
<attribute name="OC_NEWARK" value="1495086"/>
<attribute name="PACKAGE" value="8-SOIC"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2674M-3.3" prefix="U">
<description>SIMPLE SWITCHER</description>
<gates>
<gate name="A" symbol="LM2674M-3.3"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="CB" pad="1"/>
<connect gate="A" pin="FB" pad="4"/>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="NC" pad="3"/>
<connect gate="A" pin="NC_2" pad="2"/>
<connect gate="A" pin="ON/~OFF" pad="5"/>
<connect gate="A" pin="VIN" pad="7"/>
<connect gate="A" pin="VSW" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2674M-3.3"/>
<attribute name="OC_FARNELL" value="1469206"/>
<attribute name="OC_NEWARK" value="41K4120"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2674M-5.0" prefix="U">
<description>Step-Down Voltage Regulator</description>
<gates>
<gate name="A" symbol="LM2674M-5.0"/>
</gates>
<devices>
<device name="" package="SOIC127P620X175-8N">
<connects>
<connect gate="A" pin="CB" pad="1"/>
<connect gate="A" pin="FB" pad="4"/>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="NC" pad="3"/>
<connect gate="A" pin="NC_2" pad="2"/>
<connect gate="A" pin="ON/~OFF" pad="5"/>
<connect gate="A" pin="VIN" pad="7"/>
<connect gate="A" pin="VSW" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2674M-5.0"/>
<attribute name="OC_FARNELL" value="9489754"/>
<attribute name="OC_NEWARK" value="41K4121"/>
<attribute name="PACKAGE" value="8-SOIC"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2674M-ADJ" prefix="U">
<description>Step-Down Voltage Regulator</description>
<gates>
<gate name="A" symbol="LM2674M-ADJ"/>
</gates>
<devices>
<device name="" package="SOIC127P620X175-8N">
<connects>
<connect gate="A" pin="CB" pad="1"/>
<connect gate="A" pin="FB" pad="4"/>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="NC" pad="3"/>
<connect gate="A" pin="NC_2" pad="2"/>
<connect gate="A" pin="ON/~OFF" pad="5"/>
<connect gate="A" pin="VIN" pad="7"/>
<connect gate="A" pin="VSW" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2674M-ADJ"/>
<attribute name="OC_FARNELL" value="9489940"/>
<attribute name="OC_NEWARK" value="41K4118"/>
<attribute name="PACKAGE" value="8-SOIC"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2674N-3.3" prefix="U">
<description>SIMPLE SWITCHER</description>
<gates>
<gate name="A" symbol="LM2674N-3.3"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-8">
<connects>
<connect gate="A" pin="CB" pad="1"/>
<connect gate="A" pin="FB" pad="4"/>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="NC" pad="3"/>
<connect gate="A" pin="NC_2" pad="2"/>
<connect gate="A" pin="ON/~OFF" pad="5"/>
<connect gate="A" pin="VIN" pad="7"/>
<connect gate="A" pin="VSW" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2674N-3.3"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K4128"/>
<attribute name="PACKAGE" value="DIP-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2674N-5.0" prefix="U">
<description>SIMPLE SWITCHER</description>
<gates>
<gate name="A" symbol="LM2674N-5.0"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-8">
<connects>
<connect gate="A" pin="CB" pad="1"/>
<connect gate="A" pin="FB" pad="4"/>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="NC" pad="3"/>
<connect gate="A" pin="NC_2" pad="2"/>
<connect gate="A" pin="ON/~OFF" pad="5"/>
<connect gate="A" pin="VIN" pad="7"/>
<connect gate="A" pin="VSW" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2674N-5.0"/>
<attribute name="OC_FARNELL" value="1685517"/>
<attribute name="OC_NEWARK" value="41K4129"/>
<attribute name="PACKAGE" value="DIP-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2674N-ADJ" prefix="U">
<description>SIMPLE SWITCHER</description>
<gates>
<gate name="A" symbol="LM2674N-ADJ"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-8">
<connects>
<connect gate="A" pin="CB" pad="1"/>
<connect gate="A" pin="FB" pad="4"/>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="NC" pad="3"/>
<connect gate="A" pin="NC_2" pad="2"/>
<connect gate="A" pin="ON/~OFF" pad="5"/>
<connect gate="A" pin="VIN" pad="7"/>
<connect gate="A" pin="VSW" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2674N-ADJ"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="07B6217"/>
<attribute name="PACKAGE" value="DIP-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2675LD-5.0" prefix="U">
<description>SIMPLE SWITCHER</description>
<gates>
<gate name="A" symbol="LM2675LD-5.0"/>
</gates>
<devices>
<device name="" package="DFN500X500X80-17N">
<connects>
<connect gate="A" pin="CB" pad="1"/>
<connect gate="A" pin="EPAD" pad="17"/>
<connect gate="A" pin="FB" pad="8"/>
<connect gate="A" pin="GND" pad="12"/>
<connect gate="A" pin="GND_2" pad="11"/>
<connect gate="A" pin="NC" pad="7"/>
<connect gate="A" pin="NC_2" pad="2"/>
<connect gate="A" pin="NC_3" pad="3"/>
<connect gate="A" pin="NC_4" pad="4"/>
<connect gate="A" pin="NC_5" pad="10"/>
<connect gate="A" pin="NC_6" pad="5"/>
<connect gate="A" pin="NC_7" pad="13"/>
<connect gate="A" pin="NC_8" pad="6"/>
<connect gate="A" pin="ON/OFF" pad="9"/>
<connect gate="A" pin="VIN" pad="14"/>
<connect gate="A" pin="VSW" pad="16"/>
<connect gate="A" pin="VSW_2" pad="15"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2675LD-5.0"/>
<attribute name="OC_FARNELL" value="1312682"/>
<attribute name="OC_NEWARK" value="41K4133"/>
<attribute name="PACKAGE" value="DFN-16"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2675LD-ADJ" prefix="U">
<description>IC REG SW ADJ 1A STEP-DOWN</description>
<gates>
<gate name="A" symbol="LM2675LD-ADJ"/>
</gates>
<devices>
<device name="" package="DFN500X500X80-17N">
<connects>
<connect gate="A" pin="BOOST" pad="1"/>
<connect gate="A" pin="EP" pad="17"/>
<connect gate="A" pin="FB" pad="8"/>
<connect gate="A" pin="GND" pad="12"/>
<connect gate="A" pin="GND_2" pad="11"/>
<connect gate="A" pin="NC" pad="7"/>
<connect gate="A" pin="NC_2" pad="10"/>
<connect gate="A" pin="NC_3" pad="2"/>
<connect gate="A" pin="NC_4" pad="13"/>
<connect gate="A" pin="NC_5" pad="3"/>
<connect gate="A" pin="NC_6" pad="4"/>
<connect gate="A" pin="NC_7" pad="5"/>
<connect gate="A" pin="NC_8" pad="6"/>
<connect gate="A" pin="ON/~OFF" pad="9"/>
<connect gate="A" pin="SW" pad="16"/>
<connect gate="A" pin="SW_2" pad="15"/>
<connect gate="A" pin="VIN" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2675LD-ADJ"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="34C6545"/>
<attribute name="PACKAGE" value="16-WFDFN Exposed Pad"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2675M-12" prefix="U">
<description>IC REG SIMPLE SWITCHER</description>
<gates>
<gate name="A" symbol="LM2675M-12"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="BOOST" pad="1"/>
<connect gate="A" pin="FB" pad="4"/>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="NC" pad="3"/>
<connect gate="A" pin="NC_2" pad="2"/>
<connect gate="A" pin="ON/~OFF" pad="5"/>
<connect gate="A" pin="SW" pad="8"/>
<connect gate="A" pin="VIN" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2675M-12"/>
<attribute name="OC_FARNELL" value="1469208"/>
<attribute name="OC_NEWARK" value="41K4139"/>
<attribute name="PACKAGE" value="8-SOIC"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2675M-3.3" prefix="U">
<description>Step-Down Voltage Regulator</description>
<gates>
<gate name="A" symbol="LM2675M-3.3"/>
</gates>
<devices>
<device name="" package="SOIC127P620X175-8N">
<connects>
<connect gate="A" pin="CB" pad="1"/>
<connect gate="A" pin="FB" pad="4"/>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="NC" pad="3"/>
<connect gate="A" pin="NC_2" pad="2"/>
<connect gate="A" pin="ON/~OFF" pad="5"/>
<connect gate="A" pin="VIN" pad="7"/>
<connect gate="A" pin="VSW" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2675M-3.3"/>
<attribute name="OC_FARNELL" value="9489800"/>
<attribute name="OC_NEWARK" value="41K4140"/>
<attribute name="PACKAGE" value="8-SOIC"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2675M-5.0" prefix="U">
<description>Step-Down Voltage Regulator</description>
<gates>
<gate name="A" symbol="LM2675M-5.0"/>
</gates>
<devices>
<device name="" package="SOIC127P620X175-8N">
<connects>
<connect gate="A" pin="CB" pad="1"/>
<connect gate="A" pin="FB" pad="4"/>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="NC" pad="3"/>
<connect gate="A" pin="NC_2" pad="2"/>
<connect gate="A" pin="ON/~OFF" pad="5"/>
<connect gate="A" pin="VIN" pad="7"/>
<connect gate="A" pin="VSW" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2675M-5.0"/>
<attribute name="OC_FARNELL" value="9489746"/>
<attribute name="OC_NEWARK" value="41K4141"/>
<attribute name="PACKAGE" value="8-SOIC"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2675M-ADJ" prefix="U">
<description>Step-Down Voltage Regulator</description>
<gates>
<gate name="A" symbol="LM2675M-ADJ"/>
</gates>
<devices>
<device name="" package="SOIC127P620X175-8N">
<connects>
<connect gate="A" pin="CB" pad="1"/>
<connect gate="A" pin="FB" pad="4"/>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="NC" pad="3"/>
<connect gate="A" pin="NC_2" pad="2"/>
<connect gate="A" pin="ON/~OFF" pad="5"/>
<connect gate="A" pin="VIN" pad="7"/>
<connect gate="A" pin="VSW" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2675M-ADJ"/>
<attribute name="OC_FARNELL" value="9489770"/>
<attribute name="OC_NEWARK" value="41K4138"/>
<attribute name="PACKAGE" value="8-SOIC"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2675N-12" prefix="U">
<description>IC REG SIMPLE SWITCHER</description>
<gates>
<gate name="A" symbol="LM2675N-12"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-8">
<connects>
<connect gate="A" pin="BOOST" pad="1"/>
<connect gate="A" pin="FB" pad="4"/>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="NC" pad="3"/>
<connect gate="A" pin="NC_2" pad="2"/>
<connect gate="A" pin="ON/~OFF" pad="5"/>
<connect gate="A" pin="SW" pad="8"/>
<connect gate="A" pin="VIN" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2675N-12"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="07B6228"/>
<attribute name="PACKAGE" value="8-DIP"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2675N-3.3" prefix="U">
<description>IC, STEP-DOWN REGULATOR</description>
<gates>
<gate name="A" symbol="LM2675N-3.3"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-8">
<connects>
<connect gate="A" pin="BOOST" pad="1"/>
<connect gate="A" pin="FB" pad="4"/>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="NC" pad="3"/>
<connect gate="A" pin="NC_2" pad="2"/>
<connect gate="A" pin="ON/~OFF" pad="5"/>
<connect gate="A" pin="SW" pad="8"/>
<connect gate="A" pin="VIN" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2675N-3.3"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="07B6229"/>
<attribute name="PACKAGE" value="8-DIP"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2675N-5.0" prefix="U">
<description>IC, STEP-DOWN REGULATOR</description>
<gates>
<gate name="A" symbol="LM2675N-5.0"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-8">
<connects>
<connect gate="A" pin="BOOST" pad="1"/>
<connect gate="A" pin="FB" pad="4"/>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="NC" pad="3"/>
<connect gate="A" pin="NC_2" pad="2"/>
<connect gate="A" pin="ON/~OFF" pad="5"/>
<connect gate="A" pin="SW" pad="8"/>
<connect gate="A" pin="VIN" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2675N-5.0"/>
<attribute name="OC_FARNELL" value="9489819"/>
<attribute name="OC_NEWARK" value="41K4149"/>
<attribute name="PACKAGE" value="8-DIP"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2675N-ADJ" prefix="U">
<description>IC, STEP-DOWN REGULATOR</description>
<gates>
<gate name="A" symbol="LM2675N-ADJ"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-8">
<connects>
<connect gate="A" pin="BOOST" pad="1"/>
<connect gate="A" pin="FB" pad="4"/>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="NC" pad="3"/>
<connect gate="A" pin="NC_2" pad="2"/>
<connect gate="A" pin="ON/~OFF" pad="5"/>
<connect gate="A" pin="SW" pad="8"/>
<connect gate="A" pin="VIN" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2675N-ADJ"/>
<attribute name="OC_FARNELL" value="1495085"/>
<attribute name="OC_NEWARK" value="41K4146"/>
<attribute name="PACKAGE" value="8-DIP"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2676S-12" prefix="U">
<description>IC, STEP-DOWN REGULATOR</description>
<gates>
<gate name="A" symbol="LM2676S-12"/>
</gates>
<devices>
<device name="" package="TO127P1435X457-8N">
<connects>
<connect gate="A" pin="BOOST" pad="3"/>
<connect gate="A" pin="FB" pad="6"/>
<connect gate="A" pin="GND" pad="8"/>
<connect gate="A" pin="GND_2" pad="4"/>
<connect gate="A" pin="N.C." pad="5"/>
<connect gate="A" pin="ON/~OFF" pad="7"/>
<connect gate="A" pin="SW" pad="1"/>
<connect gate="A" pin="VIN" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2676S-12"/>
<attribute name="OC_FARNELL" value="1469212"/>
<attribute name="OC_NEWARK" value="41K4151"/>
<attribute name="PACKAGE" value="TO-263-7"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2676S-3.3" prefix="U">
<description>IC BUCK 3.3V 3A</description>
<gates>
<gate name="A" symbol="LM2676S-3.3"/>
</gates>
<devices>
<device name="" package="TO127P1435X457-8N">
<connects>
<connect gate="A" pin="BOOST" pad="3"/>
<connect gate="A" pin="FB" pad="6"/>
<connect gate="A" pin="GND" pad="8"/>
<connect gate="A" pin="GND_2" pad="4"/>
<connect gate="A" pin="N.C." pad="5"/>
<connect gate="A" pin="ON/~OFF" pad="7"/>
<connect gate="A" pin="SW" pad="1"/>
<connect gate="A" pin="VIN" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2676S-3.3"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K4152"/>
<attribute name="PACKAGE" value="TO-263-7"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2676S-5.0" prefix="U">
<description>IC BUCK 5V 3A</description>
<gates>
<gate name="A" symbol="LM2676S-5.0"/>
</gates>
<devices>
<device name="" package="TO127P1435X457-8N">
<connects>
<connect gate="A" pin="BOOST" pad="3"/>
<connect gate="A" pin="FB" pad="6"/>
<connect gate="A" pin="GND" pad="8"/>
<connect gate="A" pin="GND_2" pad="4"/>
<connect gate="A" pin="N.C." pad="5"/>
<connect gate="A" pin="ON/~OFF" pad="7"/>
<connect gate="A" pin="SW" pad="1"/>
<connect gate="A" pin="VIN" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2676S-5.0"/>
<attribute name="OC_FARNELL" value="1564684"/>
<attribute name="OC_NEWARK" value="41K4153"/>
<attribute name="PACKAGE" value="TO-263-7"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2676S-ADJ" prefix="U">
<description>IC BUCK ADJ 3A</description>
<gates>
<gate name="A" symbol="LM2676S-ADJ"/>
</gates>
<devices>
<device name="" package="TO127P1435X457-8N">
<connects>
<connect gate="A" pin="BOOST" pad="3"/>
<connect gate="A" pin="FB" pad="6"/>
<connect gate="A" pin="GND" pad="8"/>
<connect gate="A" pin="GND_2" pad="4"/>
<connect gate="A" pin="N.C." pad="5"/>
<connect gate="A" pin="ON/~OFF" pad="7"/>
<connect gate="A" pin="SW" pad="1"/>
<connect gate="A" pin="VIN" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2676S-ADJ"/>
<attribute name="OC_FARNELL" value="1469211"/>
<attribute name="OC_NEWARK" value="41K4150"/>
<attribute name="PACKAGE" value="TO-263-7"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2676SD-12" prefix="U">
<description>IC REG SIMPLE SWITCHER</description>
<gates>
<gate name="A" symbol="LM2676SD-12"/>
</gates>
<devices>
<device name="" package="DFN500X600X100-15N">
<connects>
<connect gate="A" pin="BOOST" pad="4"/>
<connect gate="A" pin="EP" pad="15"/>
<connect gate="A" pin="FB" pad="7"/>
<connect gate="A" pin="GND" pad="9"/>
<connect gate="A" pin="NC" pad="1"/>
<connect gate="A" pin="NC_2" pad="10"/>
<connect gate="A" pin="NC_3" pad="11"/>
<connect gate="A" pin="NC_4" pad="5"/>
<connect gate="A" pin="NC_5" pad="6"/>
<connect gate="A" pin="ON/~OFF" pad="8"/>
<connect gate="A" pin="SW" pad="14"/>
<connect gate="A" pin="SW_2" pad="12"/>
<connect gate="A" pin="SW_3" pad="13"/>
<connect gate="A" pin="VIN" pad="3"/>
<connect gate="A" pin="VIN_2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2676SD-12"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="09J8513"/>
<attribute name="PACKAGE" value="14-VDFN Exposed Pad"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2676SD-3.3" prefix="U">
<description>IC REG SIMPLE SWITCHER</description>
<gates>
<gate name="A" symbol="LM2676SD-3.3"/>
</gates>
<devices>
<device name="" package="DFN500X600X100-15N">
<connects>
<connect gate="A" pin="BOOST" pad="4"/>
<connect gate="A" pin="EP" pad="15"/>
<connect gate="A" pin="FB" pad="7"/>
<connect gate="A" pin="GND" pad="9"/>
<connect gate="A" pin="NC" pad="1"/>
<connect gate="A" pin="NC_2" pad="10"/>
<connect gate="A" pin="NC_3" pad="11"/>
<connect gate="A" pin="NC_4" pad="5"/>
<connect gate="A" pin="NC_5" pad="6"/>
<connect gate="A" pin="ON/~OFF" pad="8"/>
<connect gate="A" pin="SW" pad="14"/>
<connect gate="A" pin="SW_2" pad="12"/>
<connect gate="A" pin="SW_3" pad="13"/>
<connect gate="A" pin="VIN" pad="3"/>
<connect gate="A" pin="VIN_2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2676SD-3.3"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K4156"/>
<attribute name="PACKAGE" value="14-VDFN Exposed Pad"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2676SD-5.0" prefix="U">
<description>SIMPLE SWITCHER</description>
<gates>
<gate name="A" symbol="LM2676SD-5.0"/>
</gates>
<devices>
<device name="" package="DFN500X400X100-15N">
<connects>
<connect gate="A" pin="CD" pad="4"/>
<connect gate="A" pin="EPAD" pad="15"/>
<connect gate="A" pin="FB" pad="7"/>
<connect gate="A" pin="GND" pad="9"/>
<connect gate="A" pin="NC" pad="11"/>
<connect gate="A" pin="NC_2" pad="5"/>
<connect gate="A" pin="NC_3" pad="1"/>
<connect gate="A" pin="NC_4" pad="6"/>
<connect gate="A" pin="NC_5" pad="10"/>
<connect gate="A" pin="ON/~OFF" pad="8"/>
<connect gate="A" pin="VIN" pad="3"/>
<connect gate="A" pin="VIN_2" pad="2"/>
<connect gate="A" pin="VSW" pad="14"/>
<connect gate="A" pin="VSW_2" pad="12"/>
<connect gate="A" pin="VSW_3" pad="13"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2676SD-5.0"/>
<attribute name="OC_FARNELL" value="1495084"/>
<attribute name="OC_NEWARK" value="41K4157"/>
<attribute name="PACKAGE" value="DFN-14"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2676SD-ADJ" prefix="U">
<description>IC REG SIMPLE SWITCHER</description>
<gates>
<gate name="A" symbol="LM2676SD-ADJ"/>
</gates>
<devices>
<device name="" package="DFN500X600X100-15N">
<connects>
<connect gate="A" pin="BOOST" pad="4"/>
<connect gate="A" pin="EP" pad="15"/>
<connect gate="A" pin="FB" pad="7"/>
<connect gate="A" pin="GND" pad="9"/>
<connect gate="A" pin="NC" pad="1"/>
<connect gate="A" pin="NC_2" pad="10"/>
<connect gate="A" pin="NC_3" pad="11"/>
<connect gate="A" pin="NC_4" pad="5"/>
<connect gate="A" pin="NC_5" pad="6"/>
<connect gate="A" pin="ON/~OFF" pad="8"/>
<connect gate="A" pin="SW" pad="14"/>
<connect gate="A" pin="SW_2" pad="12"/>
<connect gate="A" pin="SW_3" pad="13"/>
<connect gate="A" pin="VIN" pad="3"/>
<connect gate="A" pin="VIN_2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2676SD-ADJ"/>
<attribute name="OC_FARNELL" value="1685541"/>
<attribute name="OC_NEWARK" value="41K4154"/>
<attribute name="PACKAGE" value="14-VDFN Exposed Pad"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2676T-12" prefix="U">
<description>IC, STEP-DOWN REGULATOR, TO-220-7</description>
<gates>
<gate name="A" symbol="LM2676T-12"/>
</gates>
<devices>
<device name="" package="TO127P457X1016X2052-7P">
<connects>
<connect gate="A" pin="BOOST" pad="3"/>
<connect gate="A" pin="FB" pad="6"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="NC" pad="5"/>
<connect gate="A" pin="ON/OFF" pad="7"/>
<connect gate="A" pin="SW" pad="1"/>
<connect gate="A" pin="VIN" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2676T-12"/>
<attribute name="OC_FARNELL" value="9485767"/>
<attribute name="OC_NEWARK" value="41K4167"/>
<attribute name="PACKAGE" value="TO-220-7"/>
<attribute name="SUPPLIER" value="NATIONAL SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2676T-3.3" prefix="U">
<description>IC BUCK 3.3V 3A</description>
<gates>
<gate name="A" symbol="LM2676T-3.3"/>
</gates>
<devices>
<device name="" package="TO127P457X1016X2052-7P">
<connects>
<connect gate="A" pin="BOOST" pad="3"/>
<connect gate="A" pin="FB" pad="6"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="N.C." pad="5"/>
<connect gate="A" pin="ON/~OFF" pad="7"/>
<connect gate="A" pin="SW" pad="1"/>
<connect gate="A" pin="VIN" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2676T-33"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="48F3513"/>
<attribute name="PACKAGE" value="TO220-7"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2676T-5.0" prefix="U">
<description>IC, STEP-DOWN REGULATOR</description>
<gates>
<gate name="A" symbol="LM2676T-5.0"/>
</gates>
<devices>
<device name="" package="TO127P457X1016X2052-7P">
<connects>
<connect gate="A" pin="BOOST" pad="3"/>
<connect gate="A" pin="FB" pad="6"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="NC" pad="5"/>
<connect gate="A" pin="ON/OFF" pad="7"/>
<connect gate="A" pin="SW" pad="1"/>
<connect gate="A" pin="VIN" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2676T-5.0"/>
<attribute name="OC_FARNELL" value="9485775"/>
<attribute name="OC_NEWARK" value="41K4169"/>
<attribute name="PACKAGE" value="TO-220-7"/>
<attribute name="SUPPLIER" value="NATIONAL SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2676T-ADJ" prefix="U">
<description>IC, STEP-DOWN REGULATOR</description>
<gates>
<gate name="A" symbol="LM2676T-ADJ"/>
</gates>
<devices>
<device name="" package="TO127P457X1016X2052-7P">
<connects>
<connect gate="A" pin="BOOST" pad="3"/>
<connect gate="A" pin="FB" pad="6"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="NC" pad="5"/>
<connect gate="A" pin="ON/OFF" pad="7"/>
<connect gate="A" pin="SW" pad="1"/>
<connect gate="A" pin="VIN" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2676T-ADJ"/>
<attribute name="OC_FARNELL" value="9485759"/>
<attribute name="OC_NEWARK" value="41K4166"/>
<attribute name="PACKAGE" value="TO-220-7"/>
<attribute name="SUPPLIER" value="NATIONAL SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2677S-12" prefix="U">
<description>IC BUCK 12V 5A</description>
<gates>
<gate name="A" symbol="LM2677S-12"/>
</gates>
<devices>
<device name="" package="TO127P1435X457-8N">
<connects>
<connect gate="A" pin="BOOST" pad="3"/>
<connect gate="A" pin="FB" pad="6"/>
<connect gate="A" pin="GND" pad="8"/>
<connect gate="A" pin="GND_2" pad="4"/>
<connect gate="A" pin="ON/~OFF" pad="7"/>
<connect gate="A" pin="SW" pad="1"/>
<connect gate="A" pin="SYNC" pad="5"/>
<connect gate="A" pin="VIN" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2677S-12"/>
<attribute name="OC_FARNELL" value="1685625"/>
<attribute name="OC_NEWARK" value="41K4171"/>
<attribute name="PACKAGE" value="TO-263-7"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2677S-3.3" prefix="U">
<description>IC BUCK 3.3V 5A</description>
<gates>
<gate name="A" symbol="LM2677S-3.3"/>
</gates>
<devices>
<device name="" package="TO127P1435X457-8N">
<connects>
<connect gate="A" pin="BOOST" pad="3"/>
<connect gate="A" pin="FB" pad="6"/>
<connect gate="A" pin="GND" pad="8"/>
<connect gate="A" pin="GND_2" pad="4"/>
<connect gate="A" pin="ON/~OFF" pad="7"/>
<connect gate="A" pin="SW" pad="1"/>
<connect gate="A" pin="SYNC" pad="5"/>
<connect gate="A" pin="VIN" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2677S-3.3"/>
<attribute name="OC_FARNELL" value="1685626"/>
<attribute name="OC_NEWARK" value="41K4172"/>
<attribute name="PACKAGE" value="TO-263-7"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2677S-5.0" prefix="U">
<description>IC BUCK 5V 5A</description>
<gates>
<gate name="A" symbol="LM2677S-5.0"/>
</gates>
<devices>
<device name="" package="TO127P1435X457-8N">
<connects>
<connect gate="A" pin="BOOST" pad="3"/>
<connect gate="A" pin="FB" pad="6"/>
<connect gate="A" pin="GND" pad="8"/>
<connect gate="A" pin="GND_2" pad="4"/>
<connect gate="A" pin="ON/~OFF" pad="7"/>
<connect gate="A" pin="SW" pad="1"/>
<connect gate="A" pin="SYNC" pad="5"/>
<connect gate="A" pin="VIN" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2677S-5.0"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K4173"/>
<attribute name="PACKAGE" value="TO-263-7"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2677S-ADJ" prefix="U">
<description>IC BUCK ADJ 5A</description>
<gates>
<gate name="A" symbol="LM2677S-ADJ"/>
</gates>
<devices>
<device name="" package="TO127P1435X457-8N">
<connects>
<connect gate="A" pin="BOOST" pad="3"/>
<connect gate="A" pin="FB" pad="6"/>
<connect gate="A" pin="GND" pad="8"/>
<connect gate="A" pin="GND_2" pad="4"/>
<connect gate="A" pin="ON/~OFF" pad="7"/>
<connect gate="A" pin="SW" pad="1"/>
<connect gate="A" pin="SYNC" pad="5"/>
<connect gate="A" pin="VIN" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2677S-ADJ"/>
<attribute name="OC_FARNELL" value="1564714"/>
<attribute name="OC_NEWARK" value="41K4170"/>
<attribute name="PACKAGE" value="TO-263-7"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2677SD-3.3" prefix="U">
<description>IC REG SIMPLE SWITCHER</description>
<gates>
<gate name="A" symbol="LM2677SD-3.3"/>
</gates>
<devices>
<device name="" package="DFN500X600X100-15N">
<connects>
<connect gate="A" pin="BOOST" pad="4"/>
<connect gate="A" pin="EP" pad="15"/>
<connect gate="A" pin="FB" pad="7"/>
<connect gate="A" pin="GND" pad="9"/>
<connect gate="A" pin="NC" pad="1"/>
<connect gate="A" pin="NC_2" pad="10"/>
<connect gate="A" pin="NC_3" pad="11"/>
<connect gate="A" pin="NC_4" pad="5"/>
<connect gate="A" pin="ON/~OFF" pad="8"/>
<connect gate="A" pin="SW" pad="14"/>
<connect gate="A" pin="SW_2" pad="12"/>
<connect gate="A" pin="SW_3" pad="13"/>
<connect gate="A" pin="SYNC" pad="6"/>
<connect gate="A" pin="VIN" pad="3"/>
<connect gate="A" pin="VIN_2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2677SD-3.3"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K4176"/>
<attribute name="PACKAGE" value="14-VDFN Exposed Pad"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2677SD-ADJ" prefix="U">
<description>IC REG SIMPLE SWITCHER</description>
<gates>
<gate name="A" symbol="LM2677SD-ADJ"/>
</gates>
<devices>
<device name="" package="DFN500X600X100-15N">
<connects>
<connect gate="A" pin="BOOST" pad="4"/>
<connect gate="A" pin="EP" pad="15"/>
<connect gate="A" pin="FB" pad="7"/>
<connect gate="A" pin="GND" pad="9"/>
<connect gate="A" pin="NC" pad="1"/>
<connect gate="A" pin="NC_2" pad="10"/>
<connect gate="A" pin="NC_3" pad="11"/>
<connect gate="A" pin="NC_4" pad="5"/>
<connect gate="A" pin="ON/~OFF" pad="8"/>
<connect gate="A" pin="SW" pad="14"/>
<connect gate="A" pin="SW_2" pad="12"/>
<connect gate="A" pin="SW_3" pad="13"/>
<connect gate="A" pin="SYNC" pad="6"/>
<connect gate="A" pin="VIN" pad="3"/>
<connect gate="A" pin="VIN_2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2677SD-ADJ"/>
<attribute name="OC_FARNELL" value="1685627"/>
<attribute name="OC_NEWARK" value="41K4174"/>
<attribute name="PACKAGE" value="14-VDFN Exposed Pad"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2677T-3.3" prefix="U">
<description>IC BUCK 3.3V 5A</description>
<gates>
<gate name="A" symbol="LM2677T-3.3"/>
</gates>
<devices>
<device name="" package="TO127P457X1016X2052-7P">
<connects>
<connect gate="A" pin="BOOST" pad="3"/>
<connect gate="A" pin="FB" pad="6"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="ON/~OFF" pad="7"/>
<connect gate="A" pin="SW" pad="1"/>
<connect gate="A" pin="SYNC" pad="5"/>
<connect gate="A" pin="VIN" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2677T-3.3"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="74C4040"/>
<attribute name="PACKAGE" value="TO220-7"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2677T-5.0" prefix="U">
<description>IC BUCK 5V 5A</description>
<gates>
<gate name="A" symbol="LM2677T-5.0"/>
</gates>
<devices>
<device name="" package="TO127P457X1016X2052-7P">
<connects>
<connect gate="A" pin="BOOST" pad="3"/>
<connect gate="A" pin="FB" pad="6"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="ON/~OFF" pad="7"/>
<connect gate="A" pin="SW" pad="1"/>
<connect gate="A" pin="SYNC" pad="5"/>
<connect gate="A" pin="VIN" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2677T-5.0"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K4189"/>
<attribute name="PACKAGE" value="TO220-7"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2677T-ADJ" prefix="U">
<description>IC, STEP-DOWN REGULATOR</description>
<gates>
<gate name="A" symbol="LM2677T-ADJ"/>
</gates>
<devices>
<device name="" package="TO127P457X1016X2052-7P">
<connects>
<connect gate="A" pin="BOOST" pad="3"/>
<connect gate="A" pin="FB" pad="6"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="SS" pad="7"/>
<connect gate="A" pin="SW" pad="1"/>
<connect gate="A" pin="SYNC" pad="5"/>
<connect gate="A" pin="VIN" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2677T-ADJ"/>
<attribute name="OC_FARNELL" value="8221960"/>
<attribute name="OC_NEWARK" value="41K4186"/>
<attribute name="PACKAGE" value="TO-220-7"/>
<attribute name="SUPPLIER" value="NATIONAL SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2678S-12" prefix="U">
<description>IC BUCK 12V 5A</description>
<gates>
<gate name="A" symbol="LM2678S-12"/>
</gates>
<devices>
<device name="" package="TO127P1435X457-8N">
<connects>
<connect gate="A" pin="BOOST" pad="3"/>
<connect gate="A" pin="FB" pad="6"/>
<connect gate="A" pin="GND" pad="8"/>
<connect gate="A" pin="GND_2" pad="4"/>
<connect gate="A" pin="N.C." pad="5"/>
<connect gate="A" pin="ON/~OFF" pad="7"/>
<connect gate="A" pin="SW" pad="1"/>
<connect gate="A" pin="VIN" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2678S-12"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="83F4652"/>
<attribute name="PACKAGE" value="TO-263-7"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2678S-3.3" prefix="U">
<description>IC BUCK 3.3V 5A</description>
<gates>
<gate name="A" symbol="LM2678S-3.3"/>
</gates>
<devices>
<device name="" package="TO127P1435X457-8N">
<connects>
<connect gate="A" pin="BOOST" pad="3"/>
<connect gate="A" pin="FB" pad="6"/>
<connect gate="A" pin="GND" pad="8"/>
<connect gate="A" pin="GND_2" pad="4"/>
<connect gate="A" pin="N.C." pad="5"/>
<connect gate="A" pin="ON/~OFF" pad="7"/>
<connect gate="A" pin="SW" pad="1"/>
<connect gate="A" pin="VIN" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2678S-3.3"/>
<attribute name="OC_FARNELL" value="1469214"/>
<attribute name="OC_NEWARK" value="41K4191"/>
<attribute name="PACKAGE" value="TO-263-7"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2678S-5.0" prefix="U">
<description>IC BUCK 5V 5A</description>
<gates>
<gate name="A" symbol="LM2678S-5.0"/>
</gates>
<devices>
<device name="" package="TO127P1435X457-8N">
<connects>
<connect gate="A" pin="BOOST" pad="3"/>
<connect gate="A" pin="FB" pad="6"/>
<connect gate="A" pin="GND" pad="8"/>
<connect gate="A" pin="GND_2" pad="4"/>
<connect gate="A" pin="N.C." pad="5"/>
<connect gate="A" pin="ON/~OFF" pad="7"/>
<connect gate="A" pin="SW" pad="1"/>
<connect gate="A" pin="VIN" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2678S-5.0"/>
<attribute name="OC_FARNELL" value="1469215"/>
<attribute name="OC_NEWARK" value="41K4192"/>
<attribute name="PACKAGE" value="TO-263-7"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2678S-ADJ" prefix="U">
<description>SIMPLE SWITCHER</description>
<gates>
<gate name="A" symbol="LM2678S-ADJ"/>
</gates>
<devices>
<device name="" package="TO127P1435X457-8N">
<connects>
<connect gate="A" pin="C_BOOST" pad="3"/>
<connect gate="A" pin="FB" pad="6"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="GND_2" pad="8"/>
<connect gate="A" pin="NC" pad="5"/>
<connect gate="A" pin="ON/~OFF" pad="7"/>
<connect gate="A" pin="SW_IN" pad="1"/>
<connect gate="A" pin="VIN" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2678S-ADJ"/>
<attribute name="OC_FARNELL" value="8207399"/>
<attribute name="OC_NEWARK" value="28K1912"/>
<attribute name="PACKAGE" value="TO-236-7"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2678SD-5.0" prefix="U">
<description>IC REG SIMPLE SWITCHER</description>
<gates>
<gate name="A" symbol="LM2678SD-5.0"/>
</gates>
<devices>
<device name="" package="DFN500X600X100-15N">
<connects>
<connect gate="A" pin="BOOST" pad="4"/>
<connect gate="A" pin="EP" pad="15"/>
<connect gate="A" pin="FB" pad="7"/>
<connect gate="A" pin="GND" pad="9"/>
<connect gate="A" pin="NC" pad="1"/>
<connect gate="A" pin="NC_2" pad="10"/>
<connect gate="A" pin="NC_3" pad="11"/>
<connect gate="A" pin="NC_4" pad="5"/>
<connect gate="A" pin="NC_5" pad="6"/>
<connect gate="A" pin="ON/~OFF" pad="8"/>
<connect gate="A" pin="SW" pad="14"/>
<connect gate="A" pin="SW_2" pad="12"/>
<connect gate="A" pin="SW_3" pad="13"/>
<connect gate="A" pin="VIN" pad="3"/>
<connect gate="A" pin="VIN_2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2678SD-5.0"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K4196"/>
<attribute name="PACKAGE" value="14-VDFN Exposed Pad"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2678SD-ADJ" prefix="U">
<description>IC REG SIMPLE SWITCHER</description>
<gates>
<gate name="A" symbol="LM2678SD-ADJ"/>
</gates>
<devices>
<device name="" package="DFN500X600X100-15N">
<connects>
<connect gate="A" pin="BOOST" pad="4"/>
<connect gate="A" pin="EP" pad="15"/>
<connect gate="A" pin="FB" pad="7"/>
<connect gate="A" pin="GND" pad="9"/>
<connect gate="A" pin="NC" pad="1"/>
<connect gate="A" pin="NC_2" pad="10"/>
<connect gate="A" pin="NC_3" pad="11"/>
<connect gate="A" pin="NC_4" pad="5"/>
<connect gate="A" pin="NC_5" pad="6"/>
<connect gate="A" pin="ON/~OFF" pad="8"/>
<connect gate="A" pin="SW" pad="14"/>
<connect gate="A" pin="SW_2" pad="12"/>
<connect gate="A" pin="SW_3" pad="13"/>
<connect gate="A" pin="VIN" pad="3"/>
<connect gate="A" pin="VIN_2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2678SD-ADJ"/>
<attribute name="OC_FARNELL" value="1685628"/>
<attribute name="OC_NEWARK" value="41K4193"/>
<attribute name="PACKAGE" value="14-VDFN Exposed Pad"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2678T-12" prefix="U">
<description>IC, STEP-DOWN REGULATOR, TO-220-7</description>
<gates>
<gate name="A" symbol="LM2678T-12"/>
</gates>
<devices>
<device name="" package="TO127P457X1016X2052-7P">
<connects>
<connect gate="A" pin="BOOST" pad="3"/>
<connect gate="A" pin="FB" pad="6"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="NC" pad="5"/>
<connect gate="A" pin="SS" pad="7"/>
<connect gate="A" pin="SW" pad="1"/>
<connect gate="A" pin="VIN" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2678T-12"/>
<attribute name="OC_FARNELL" value="9778357"/>
<attribute name="OC_NEWARK" value="41K4206"/>
<attribute name="PACKAGE" value="TO-220-7"/>
<attribute name="SUPPLIER" value="NATIONAL SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2678T-3.3" prefix="U">
<description>IC BUCK 3.3V 5A</description>
<gates>
<gate name="A" symbol="LM2678T-3.3"/>
</gates>
<devices>
<device name="" package="TO127P457X1016X2052-7P">
<connects>
<connect gate="A" pin="BOOST" pad="3"/>
<connect gate="A" pin="FB" pad="6"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="N.C." pad="5"/>
<connect gate="A" pin="ON/~OFF" pad="7"/>
<connect gate="A" pin="SW" pad="1"/>
<connect gate="A" pin="VIN" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2678T-3.3"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K4207"/>
<attribute name="PACKAGE" value="TO220-7"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2678T-5.0" prefix="U">
<description>IC, STEP-DOWN REGULATOR</description>
<gates>
<gate name="A" symbol="LM2678T-5.0"/>
</gates>
<devices>
<device name="" package="TO127P457X1016X2052-7P">
<connects>
<connect gate="A" pin="BOOST" pad="3"/>
<connect gate="A" pin="FB" pad="6"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="NC" pad="5"/>
<connect gate="A" pin="SS" pad="7"/>
<connect gate="A" pin="SW" pad="1"/>
<connect gate="A" pin="VIN" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LLM2678T-5.0"/>
<attribute name="OC_FARNELL" value="9778365"/>
<attribute name="OC_NEWARK" value="41K4208"/>
<attribute name="PACKAGE" value="TO-220-7"/>
<attribute name="SUPPLIER" value="NATIONAL SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2678T-ADJ" prefix="U">
<description>IC, STEP-DOWN REGULATOR</description>
<gates>
<gate name="A" symbol="LM2678T-ADJ"/>
</gates>
<devices>
<device name="" package="TO127P457X1016X2052-7P">
<connects>
<connect gate="A" pin="BOOST" pad="3"/>
<connect gate="A" pin="FB" pad="6"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="NC" pad="5"/>
<connect gate="A" pin="SS" pad="7"/>
<connect gate="A" pin="SW" pad="1"/>
<connect gate="A" pin="VIN" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2678T-ADJ"/>
<attribute name="OC_FARNELL" value="9486186"/>
<attribute name="OC_NEWARK" value="41K4205"/>
<attribute name="PACKAGE" value="TO-220-7"/>
<attribute name="SUPPLIER" value="NATIONAL SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2679S-12" prefix="U">
<description>IC BUCK 12V 5A</description>
<gates>
<gate name="A" symbol="LM2679S-12"/>
</gates>
<devices>
<device name="" package="TO127P1435X457-8N">
<connects>
<connect gate="A" pin="BOOST" pad="3"/>
<connect gate="A" pin="CURRENT_ADJ" pad="5"/>
<connect gate="A" pin="FB" pad="6"/>
<connect gate="A" pin="GND" pad="8"/>
<connect gate="A" pin="GND_2" pad="4"/>
<connect gate="A" pin="SOFTSTART" pad="7"/>
<connect gate="A" pin="SW" pad="1"/>
<connect gate="A" pin="VIN" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2679S-12"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K4210"/>
<attribute name="PACKAGE" value="TO-263-7"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2679S-3.3" prefix="U">
<description>IC BUCK 3.3V 5A</description>
<gates>
<gate name="A" symbol="LM2679S-3.3"/>
</gates>
<devices>
<device name="" package="TO127P1435X457-8N">
<connects>
<connect gate="A" pin="BOOST" pad="3"/>
<connect gate="A" pin="CURRENT_ADJ" pad="5"/>
<connect gate="A" pin="FB" pad="6"/>
<connect gate="A" pin="GND" pad="8"/>
<connect gate="A" pin="GND_2" pad="4"/>
<connect gate="A" pin="SOFTSTART" pad="7"/>
<connect gate="A" pin="SW" pad="1"/>
<connect gate="A" pin="VIN" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2679S-3.3"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K4211"/>
<attribute name="PACKAGE" value="TO-263-7"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2679S-5.0" prefix="U">
<description>SIMPLE SWITCHER® 5A Step-Down Voltage Regulator</description>
<gates>
<gate name="A" symbol="LM2679S-5.0"/>
</gates>
<devices>
<device name="" package="TO127P1435X457-8N">
<connects>
<connect gate="A" pin="CURRENT_ADJ" pad="5"/>
<connect gate="A" pin="C__BOOST" pad="3"/>
<connect gate="A" pin="FB" pad="6"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="GND_2" pad="8"/>
<connect gate="A" pin="SS" pad="7"/>
<connect gate="A" pin="SW_OUT" pad="1"/>
<connect gate="A" pin="VIN" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2679S-5.0"/>
<attribute name="OC_FARNELL" value="9486208"/>
<attribute name="OC_NEWARK" value="41K4212"/>
<attribute name="PACKAGE" value="TO-236-7"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2679S-ADJ" prefix="U">
<description>SIMPLE SWITCHER® 5A Step-Down Voltage Regulator</description>
<gates>
<gate name="A" symbol="LM2679S-ADJ"/>
</gates>
<devices>
<device name="" package="TO127P1435X457-8N">
<connects>
<connect gate="A" pin="CURRENT_ADJ" pad="5"/>
<connect gate="A" pin="C__BOOST" pad="3"/>
<connect gate="A" pin="FB" pad="6"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="GND_2" pad="8"/>
<connect gate="A" pin="SS" pad="7"/>
<connect gate="A" pin="SW_OUT" pad="1"/>
<connect gate="A" pin="VIN" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2679S-ADJ"/>
<attribute name="OC_FARNELL" value="9486194"/>
<attribute name="OC_NEWARK" value="41K4209"/>
<attribute name="PACKAGE" value="TO-236-7"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2679SD-5.0" prefix="U">
<description>IC REG SIMPLE SWITCHER</description>
<gates>
<gate name="A" symbol="LM2679SD-5.0"/>
</gates>
<devices>
<device name="" package="DFN500X600X100-15N">
<connects>
<connect gate="A" pin="BOOST" pad="4"/>
<connect gate="A" pin="CURRENT_ADJ" pad="6"/>
<connect gate="A" pin="EP" pad="15"/>
<connect gate="A" pin="FB" pad="7"/>
<connect gate="A" pin="GND" pad="9"/>
<connect gate="A" pin="NC" pad="1"/>
<connect gate="A" pin="NC_2" pad="10"/>
<connect gate="A" pin="NC_3" pad="11"/>
<connect gate="A" pin="NC_4" pad="5"/>
<connect gate="A" pin="SOFTSTART" pad="8"/>
<connect gate="A" pin="SW" pad="14"/>
<connect gate="A" pin="SW_2" pad="12"/>
<connect gate="A" pin="SW_3" pad="13"/>
<connect gate="A" pin="VIN" pad="3"/>
<connect gate="A" pin="VIN_2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2679SD-5.0"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K4216"/>
<attribute name="PACKAGE" value="14-VDFN Exposed Pad"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2679SD-ADJ" prefix="U">
<description>IC REG SIMPLE SWITCHER</description>
<gates>
<gate name="A" symbol="LM2679SD-ADJ"/>
</gates>
<devices>
<device name="" package="DFN500X600X100-15N">
<connects>
<connect gate="A" pin="BOOST" pad="4"/>
<connect gate="A" pin="CURRENT_ADJ" pad="6"/>
<connect gate="A" pin="EP" pad="15"/>
<connect gate="A" pin="FB" pad="7"/>
<connect gate="A" pin="GND" pad="9"/>
<connect gate="A" pin="NC" pad="1"/>
<connect gate="A" pin="NC_2" pad="10"/>
<connect gate="A" pin="NC_3" pad="11"/>
<connect gate="A" pin="NC_4" pad="5"/>
<connect gate="A" pin="SOFTSTART" pad="8"/>
<connect gate="A" pin="SW" pad="14"/>
<connect gate="A" pin="SW_2" pad="12"/>
<connect gate="A" pin="SW_3" pad="13"/>
<connect gate="A" pin="VIN" pad="3"/>
<connect gate="A" pin="VIN_2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2679SD-ADJ"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K4213"/>
<attribute name="PACKAGE" value="14-VDFN Exposed Pad"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2679T-12" prefix="U">
<description>IC BUCK 12V 5A</description>
<gates>
<gate name="A" symbol="LM2679T-12"/>
</gates>
<devices>
<device name="" package="TO127P457X1016X2052-7P">
<connects>
<connect gate="A" pin="BOOST" pad="3"/>
<connect gate="A" pin="CURRENT_ADJ" pad="5"/>
<connect gate="A" pin="FB" pad="6"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="SOFTSTART" pad="7"/>
<connect gate="A" pin="SW" pad="1"/>
<connect gate="A" pin="VIN" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2679T-12"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="83F4664"/>
<attribute name="PACKAGE" value="TO220-7"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2679T-3.3" prefix="U">
<description>IC BUCK 3.3V 5A</description>
<gates>
<gate name="A" symbol="LM2679T-3.3"/>
</gates>
<devices>
<device name="" package="TO127P457X1016X2052-7P">
<connects>
<connect gate="A" pin="BOOST" pad="3"/>
<connect gate="A" pin="CURRENT_ADJ" pad="5"/>
<connect gate="A" pin="FB" pad="6"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="SOFTSTART" pad="7"/>
<connect gate="A" pin="SW" pad="1"/>
<connect gate="A" pin="VIN" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2679T-3.3"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K4227"/>
<attribute name="PACKAGE" value="TO220-7"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2679T-5.0" prefix="U">
<description>IC BUCK 5V 5A</description>
<gates>
<gate name="A" symbol="LM2679T-5.0"/>
</gates>
<devices>
<device name="" package="TO127P457X1016X2052-7P">
<connects>
<connect gate="A" pin="BOOST" pad="3"/>
<connect gate="A" pin="CURRENT_ADJ" pad="5"/>
<connect gate="A" pin="FB" pad="6"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="SOFTSTART" pad="7"/>
<connect gate="A" pin="SW" pad="1"/>
<connect gate="A" pin="VIN" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2679T-5.0"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K4228"/>
<attribute name="PACKAGE" value="TO220-7"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2679T-ADJ" prefix="U">
<description>IC, STEP-DOWN REGULATOR</description>
<gates>
<gate name="A" symbol="LM2679T-ADJ"/>
</gates>
<devices>
<device name="" package="TO127P457X1016X2052-7P">
<connects>
<connect gate="A" pin="BOOST" pad="3"/>
<connect gate="A" pin="CL_ADJ" pad="5"/>
<connect gate="A" pin="FB" pad="6"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="SS" pad="7"/>
<connect gate="A" pin="SW" pad="1"/>
<connect gate="A" pin="VIN" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2679T-ADJ"/>
<attribute name="OC_FARNELL" value="9489762"/>
<attribute name="OC_NEWARK" value="41K4225"/>
<attribute name="PACKAGE" value="TO-220-7"/>
<attribute name="SUPPLIER" value="NATIONAL SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2682MM" prefix="U">
<description>IC, VOLTAGE DOUBLING INVERTER</description>
<gates>
<gate name="A" symbol="LM2682MM"/>
</gates>
<devices>
<device name="" package="SOP65P490X109-8N">
<connects>
<connect gate="A" pin="C1+" pad="7"/>
<connect gate="A" pin="C1-_" pad="1"/>
<connect gate="A" pin="C2+" pad="2"/>
<connect gate="A" pin="C2-_" pad="3"/>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="NC" pad="8"/>
<connect gate="A" pin="VIN" pad="6"/>
<connect gate="A" pin="VOUT" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2682MM"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K4232"/>
<attribute name="PACKAGE" value="SwitchCap"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2687MM" prefix="U">
<description>Voltage Inverter</description>
<gates>
<gate name="A" symbol="LM2687MM"/>
</gates>
<devices>
<device name="" package="SOP65P490X109-8N">
<connects>
<connect gate="A" pin="CAP+" pad="1"/>
<connect gate="A" pin="CAP-" pad="3"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="VFB" pad="6"/>
<connect gate="A" pin="VIN" pad="8"/>
<connect gate="A" pin="VNEG" pad="5"/>
<connect gate="A" pin="VOUT" pad="7"/>
<connect gate="A" pin="~SD" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2687MM"/>
<attribute name="OC_FARNELL" value="9778624"/>
<attribute name="OC_NEWARK" value="41K4241"/>
<attribute name="PACKAGE" value="8-MSOP"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2694MT" prefix="U">
<description>Step Down Switching Regulator</description>
<gates>
<gate name="A" symbol="LM2694MT"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-14N">
<connects>
<connect gate="A" pin="BOOST" pad="3"/>
<connect gate="A" pin="FB" pad="9"/>
<connect gate="A" pin="ISEN" pad="4"/>
<connect gate="A" pin="NC" pad="14"/>
<connect gate="A" pin="NC_2" pad="1"/>
<connect gate="A" pin="NC_3" pad="7"/>
<connect gate="A" pin="NC_4" pad="8"/>
<connect gate="A" pin="RON/SD" pad="11"/>
<connect gate="A" pin="RTN" pad="6"/>
<connect gate="A" pin="SGND" pad="5"/>
<connect gate="A" pin="SS" pad="10"/>
<connect gate="A" pin="SW" pad="2"/>
<connect gate="A" pin="VCC" pad="12"/>
<connect gate="A" pin="VIN" pad="13"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2694MT"/>
<attribute name="OC_FARNELL" value="1286850"/>
<attribute name="OC_NEWARK" value="13M1708"/>
<attribute name="PACKAGE" value="SOP-14"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2694SD" prefix="U">
<description>IC BUCK ADJ .6A</description>
<gates>
<gate name="A" symbol="LM2694SD"/>
</gates>
<devices>
<device name="" package="DFN300X300X80-11N">
<connects>
<connect gate="A" pin="BOOST" pad="2"/>
<connect gate="A" pin="EP" pad="11"/>
<connect gate="A" pin="FB" pad="6"/>
<connect gate="A" pin="ISEN" pad="3"/>
<connect gate="A" pin="RON/SD" pad="8"/>
<connect gate="A" pin="RTN" pad="5"/>
<connect gate="A" pin="SGND" pad="4"/>
<connect gate="A" pin="SS" pad="7"/>
<connect gate="A" pin="SW" pad="1"/>
<connect gate="A" pin="VCC" pad="9"/>
<connect gate="A" pin="VIN" pad="10"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2694SD"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="99K2341"/>
<attribute name="PACKAGE" value="10-WFDFN Exposed Pad"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2695MH" prefix="U">
<description>IC BUCK ADJ 1.25A</description>
<gates>
<gate name="A" symbol="LM2695MH"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-15N">
<connects>
<connect gate="A" pin="BST" pad="3"/>
<connect gate="A" pin="EP" pad="15"/>
<connect gate="A" pin="FB" pad="9"/>
<connect gate="A" pin="ISEN" pad="4"/>
<connect gate="A" pin="NC" pad="1"/>
<connect gate="A" pin="NC_2" pad="14"/>
<connect gate="A" pin="NC_3" pad="7"/>
<connect gate="A" pin="NC_4" pad="8"/>
<connect gate="A" pin="RON/SD" pad="11"/>
<connect gate="A" pin="RTN" pad="6"/>
<connect gate="A" pin="SGND" pad="5"/>
<connect gate="A" pin="SS" pad="10"/>
<connect gate="A" pin="SW" pad="2"/>
<connect gate="A" pin="VCC" pad="12"/>
<connect gate="A" pin="VIN" pad="13"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2695MH"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="79K7791"/>
<attribute name="PACKAGE" value="14-TSSOP - Exposed Pad"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2696MXA" prefix="U">
<description>Constant On Time Buck Regulator</description>
<gates>
<gate name="A" symbol="LM2696MXA"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-17N">
<connects>
<connect gate="A" pin="AVIN" pad="5"/>
<connect gate="A" pin="BOOT" pad="4"/>
<connect gate="A" pin="EPAD" pad="17"/>
<connect gate="A" pin="EXTVCC" pad="6"/>
<connect gate="A" pin="FB" pad="7"/>
<connect gate="A" pin="GND" pad="9"/>
<connect gate="A" pin="NC" pad="8"/>
<connect gate="A" pin="PGOOD" pad="11"/>
<connect gate="A" pin="PVIN" pad="16"/>
<connect gate="A" pin="PVIN_2" pad="14"/>
<connect gate="A" pin="PVIN_3" pad="15"/>
<connect gate="A" pin="RON" pad="12"/>
<connect gate="A" pin="SD" pad="13"/>
<connect gate="A" pin="SS" pad="10"/>
<connect gate="A" pin="SW" pad="3"/>
<connect gate="A" pin="SW_2" pad="1"/>
<connect gate="A" pin="SW_3" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2696MXA"/>
<attribute name="OC_FARNELL" value="1798317"/>
<attribute name="OC_NEWARK" value="73R9730"/>
<attribute name="PACKAGE" value="TSSOP-16"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2698MM-ADJ" prefix="U">
<description>IC MULTI CONFIG ADJ 1.9A</description>
<gates>
<gate name="A" symbol="LM2698MM-ADJ"/>
</gates>
<devices>
<device name="" package="SOP65P490X109-8N">
<connects>
<connect gate="A" pin="FB" pad="2"/>
<connect gate="A" pin="FSLCT" pad="7"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="NC" pad="8"/>
<connect gate="A" pin="SW" pad="5"/>
<connect gate="A" pin="VC" pad="1"/>
<connect gate="A" pin="VIN" pad="6"/>
<connect gate="A" pin="~SD" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2698MM-ADJ"/>
<attribute name="OC_FARNELL" value="1564736"/>
<attribute name="OC_NEWARK" value="41K4243"/>
<attribute name="PACKAGE" value="8 - MSOP"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM26CIM5-PHA" prefix="U">
<description>Preset Thermostat</description>
<gates>
<gate name="A" symbol="LM26CIM5-PHA"/>
</gates>
<devices>
<device name="" package="SOT95P284X122-5N">
<connects>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="HYST" pad="1"/>
<connect gate="A" pin="V+" pad="4"/>
<connect gate="A" pin="VTEMP" pad="3"/>
<connect gate="A" pin="~OS" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM26CIM5-PHA"/>
<attribute name="OC_FARNELL" value="1312672"/>
<attribute name="OC_NEWARK" value="65K5923"/>
<attribute name="PACKAGE" value="SOT-23-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM26CIM5-RPA" prefix="U">
<description>Thermostat</description>
<gates>
<gate name="A" symbol="LM26CIM5-RPA"/>
</gates>
<devices>
<device name="" package="SOT95P284X122-5N">
<connects>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="HYST" pad="1"/>
<connect gate="A" pin="V+" pad="4"/>
<connect gate="A" pin="VTEMP" pad="3"/>
<connect gate="A" pin="~OS" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM26CIM5-RPA"/>
<attribute name="OC_FARNELL" value="1312673"/>
<attribute name="OC_NEWARK" value="41K3901"/>
<attribute name="PACKAGE" value="SOT23-5"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM26CIM5-SHA" prefix="U">
<description>Preset Thermostat</description>
<gates>
<gate name="A" symbol="LM26CIM5-SHA"/>
</gates>
<devices>
<device name="" package="SOT95P284X122-5N">
<connects>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="HYST" pad="1"/>
<connect gate="A" pin="V+" pad="4"/>
<connect gate="A" pin="VTEMP" pad="3"/>
<connect gate="A" pin="~OS" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM26CIM5-SHA"/>
<attribute name="OC_FARNELL" value="1312675"/>
<attribute name="OC_NEWARK" value="41K3902"/>
<attribute name="PACKAGE" value="SOT-23-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM26CIM5-SPA" prefix="U">
<description>Preset Thermostat</description>
<gates>
<gate name="A" symbol="LM26CIM5-SPA"/>
</gates>
<devices>
<device name="" package="SOT95P284X122-5N">
<connects>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="HYST" pad="1"/>
<connect gate="A" pin="V+" pad="4"/>
<connect gate="A" pin="VTEMP" pad="3"/>
<connect gate="A" pin="~OS" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM26CIM5-SPA"/>
<attribute name="OC_FARNELL" value="1312676"/>
<attribute name="OC_NEWARK" value="31M5352"/>
<attribute name="PACKAGE" value="SOT-23-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM26CIM5-TPA" prefix="U">
<description>Thermostat</description>
<gates>
<gate name="A" symbol="LM26CIM5-TPA"/>
</gates>
<devices>
<device name="" package="SOT95P284X122-5N">
<connects>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="HYST" pad="1"/>
<connect gate="A" pin="V+" pad="4"/>
<connect gate="A" pin="VTEMP" pad="3"/>
<connect gate="A" pin="~OS" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM26CIM5-TPA"/>
<attribute name="OC_FARNELL" value="9779124"/>
<attribute name="OC_NEWARK" value="34C6507"/>
<attribute name="PACKAGE" value="SOT23-5"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM26CIM5-VHA" prefix="U">
<description>Factory Preset Thermostat</description>
<gates>
<gate name="A" symbol="LM26CIM5-VHA"/>
</gates>
<devices>
<device name="" package="SOT95P300X120-5N">
<connects>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="HYST" pad="1"/>
<connect gate="A" pin="OS/~OS" pad="5"/>
<connect gate="A" pin="V+" pad="4"/>
<connect gate="A" pin="VTEMP" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM26CIM5-VHA"/>
<attribute name="OC_FARNELL" value="1312677"/>
<attribute name="OC_NEWARK" value="31M5353"/>
<attribute name="PACKAGE" value="SOT-5"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM26CIM5-VPA" prefix="U">
<description>Factory Preset Thermostat</description>
<gates>
<gate name="A" symbol="LM26CIM5-VPA"/>
</gates>
<devices>
<device name="" package="SOT95P300X120-5N">
<connects>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="HYST" pad="1"/>
<connect gate="A" pin="OS/~OS" pad="5"/>
<connect gate="A" pin="V+" pad="4"/>
<connect gate="A" pin="VTEMP" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM26CIM5-VPA"/>
<attribute name="OC_FARNELL" value="1312678"/>
<attribute name="OC_NEWARK" value="41K3906"/>
<attribute name="PACKAGE" value="SOT-5"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM26CIM5-XPA" prefix="U">
<description>Thermostat</description>
<gates>
<gate name="A" symbol="LM26CIM5-XPA"/>
</gates>
<devices>
<device name="" package="SOT95P284X122-5N">
<connects>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="HYST" pad="1"/>
<connect gate="A" pin="V+" pad="4"/>
<connect gate="A" pin="VTEMP" pad="3"/>
<connect gate="A" pin="~OS" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM26CIM5-XPA"/>
<attribute name="OC_FARNELL" value="1197403"/>
<attribute name="OC_NEWARK" value="41K3908"/>
<attribute name="PACKAGE" value="SOT23-5"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM26CIM5-YHA" prefix="U">
<description>Factory Preset Thermostat</description>
<gates>
<gate name="A" symbol="LM26CIM5-YHA"/>
</gates>
<devices>
<device name="" package="SOT95P300X120-5N">
<connects>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="HYST" pad="1"/>
<connect gate="A" pin="OS/~OS" pad="5"/>
<connect gate="A" pin="V+" pad="4"/>
<connect gate="A" pin="VTEMP" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM26CIM5-YHA"/>
<attribute name="OC_FARNELL" value="1312679"/>
<attribute name="OC_NEWARK" value="31M5355"/>
<attribute name="PACKAGE" value="SOT-5"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2700LD-ADJ" prefix="U">
<description>Step-up PWM DC/DC Converter</description>
<gates>
<gate name="A" symbol="LM2700LD-ADJ"/>
</gates>
<devices>
<device name="" package="DFN400X400X80-15N">
<connects>
<connect gate="A" pin="AGND" pad="4"/>
<connect gate="A" pin="FB" pad="2"/>
<connect gate="A" pin="FSLCT" pad="13"/>
<connect gate="A" pin="GND" pad="15"/>
<connect gate="A" pin="NC" pad="14"/>
<connect gate="A" pin="NC_2" pad="11"/>
<connect gate="A" pin="PGND" pad="7"/>
<connect gate="A" pin="PGND_2" pad="5"/>
<connect gate="A" pin="PGND_3" pad="6"/>
<connect gate="A" pin="SW" pad="10"/>
<connect gate="A" pin="SW_2" pad="8"/>
<connect gate="A" pin="SW_3" pad="9"/>
<connect gate="A" pin="VC" pad="1"/>
<connect gate="A" pin="VIN" pad="12"/>
<connect gate="A" pin="~SHDN" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2700LD-ADJ"/>
<attribute name="OC_FARNELL" value="1312688"/>
<attribute name="OC_NEWARK" value="41K4247"/>
<attribute name="PACKAGE" value="DFN-14"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2700MT-ADJ" prefix="U">
<description>Step-up PWM DC/DC Converter</description>
<gates>
<gate name="A" symbol="LM2700MT-ADJ"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-14N">
<connects>
<connect gate="A" pin="AGND" pad="4"/>
<connect gate="A" pin="FB" pad="2"/>
<connect gate="A" pin="FSLCT" pad="13"/>
<connect gate="A" pin="NC" pad="14"/>
<connect gate="A" pin="NC_2" pad="11"/>
<connect gate="A" pin="PGND" pad="7"/>
<connect gate="A" pin="PGND_2" pad="5"/>
<connect gate="A" pin="PGND_3" pad="6"/>
<connect gate="A" pin="SW" pad="10"/>
<connect gate="A" pin="SW_2" pad="8"/>
<connect gate="A" pin="SW_3" pad="9"/>
<connect gate="A" pin="VC" pad="1"/>
<connect gate="A" pin="VIN" pad="12"/>
<connect gate="A" pin="~SHDN" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2700MT-ADJ"/>
<attribute name="OC_FARNELL" value="9778993"/>
<attribute name="OC_NEWARK" value="41K4249"/>
<attribute name="PACKAGE" value="TSSOP-14"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2703MF-ADJ" prefix="U">
<description>DC/DC Converter</description>
<gates>
<gate name="A" symbol="LM2703MF-ADJ"/>
</gates>
<devices>
<device name="" package="SOT95P284X122-5N">
<connects>
<connect gate="A" pin="FB" pad="3"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="SW" pad="1"/>
<connect gate="A" pin="VIN" pad="5"/>
<connect gate="A" pin="~SHDN" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2703MF-ADJ"/>
<attribute name="OC_FARNELL" value="9779442"/>
<attribute name="OC_NEWARK" value="41K4253"/>
<attribute name="PACKAGE" value="SOT23-5"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2704MF-ADJ" prefix="U">
<description>Step-up DC/DC Converter</description>
<gates>
<gate name="A" symbol="LM2704MF-ADJ"/>
</gates>
<devices>
<device name="" package="SOT95P285X120-5N">
<connects>
<connect gate="A" pin="FB" pad="3"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="SW" pad="1"/>
<connect gate="A" pin="VIN" pad="5"/>
<connect gate="A" pin="~SHDN" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2704MF-ADJ"/>
<attribute name="OC_FARNELL" value="8207461"/>
<attribute name="OC_NEWARK" value="41K4255"/>
<attribute name="PACKAGE" value="SOT-23-5"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2705MF-ADJ" prefix="U">
<description>Step-up DC/DC Converter</description>
<gates>
<gate name="A" symbol="LM2705MF-ADJ"/>
</gates>
<devices>
<device name="" package="SOT95P285X120-5N">
<connects>
<connect gate="A" pin="FB" pad="3"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="SW" pad="1"/>
<connect gate="A" pin="VIN" pad="5"/>
<connect gate="A" pin="~SHDN" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2705MF-ADJ"/>
<attribute name="OC_FARNELL" value="9779434"/>
<attribute name="OC_NEWARK" value="41K4257"/>
<attribute name="PACKAGE" value="SOT-23-5"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM27213SQ" prefix="U">
<description>Single Phase Hysteretic Buck Controller</description>
<gates>
<gate name="A" symbol="LM27213SQ"/>
</gates>
<devices>
<device name="" package="QFN50P700X700X80-49N">
<connects>
<connect gate="A" pin="CBOOT" pad="1"/>
<connect gate="A" pin="CLK_EN" pad="12"/>
<connect gate="A" pin="CMP" pad="9"/>
<connect gate="A" pin="CMPREF" pad="10"/>
<connect gate="A" pin="DE_EN" pad="35"/>
<connect gate="A" pin="DGND" pad="13"/>
<connect gate="A" pin="EPAD" pad="49"/>
<connect gate="A" pin="HG" pad="2"/>
<connect gate="A" pin="ILIM" pad="7"/>
<connect gate="A" pin="ILIMREF" pad="8"/>
<connect gate="A" pin="LG" pad="47"/>
<connect gate="A" pin="NC" pad="6"/>
<connect gate="A" pin="NC_2" pad="29"/>
<connect gate="A" pin="NC_3" pad="20"/>
<connect gate="A" pin="NC_4" pad="30"/>
<connect gate="A" pin="NC_5" pad="21"/>
<connect gate="A" pin="NC_6" pad="43"/>
<connect gate="A" pin="NC_7" pad="4"/>
<connect gate="A" pin="NC_8" pad="44"/>
<connect gate="A" pin="NC_9" pad="46"/>
<connect gate="A" pin="PGND" pad="45"/>
<connect gate="A" pin="PGOOD" pad="14"/>
<connect gate="A" pin="PVDD" pad="48"/>
<connect gate="A" pin="P_Z0" pad="22"/>
<connect gate="A" pin="P_Z1" pad="19"/>
<connect gate="A" pin="P_Z2" pad="18"/>
<connect gate="A" pin="SENSE" pad="16"/>
<connect gate="A" pin="SGND" pad="23"/>
<connect gate="A" pin="SLP" pad="33"/>
<connect gate="A" pin="SRCK" pad="5"/>
<connect gate="A" pin="SS" pad="25"/>
<connect gate="A" pin="STP_CPU" pad="34"/>
<connect gate="A" pin="SW" pad="3"/>
<connect gate="A" pin="V1R7" pad="26"/>
<connect gate="A" pin="VBOOT" pad="27"/>
<connect gate="A" pin="VDAC" pad="31"/>
<connect gate="A" pin="VDD" pad="24"/>
<connect gate="A" pin="VID0" pad="41"/>
<connect gate="A" pin="VID1" pad="40"/>
<connect gate="A" pin="VID2" pad="39"/>
<connect gate="A" pin="VID3" pad="38"/>
<connect gate="A" pin="VID4" pad="37"/>
<connect gate="A" pin="VID5" pad="36"/>
<connect gate="A" pin="VOVP" pad="17"/>
<connect gate="A" pin="VREF" pad="11"/>
<connect gate="A" pin="VRON" pad="42"/>
<connect gate="A" pin="VSLP" pad="28"/>
<connect gate="A" pin="VSTP" pad="32"/>
<connect gate="A" pin="XPOK" pad="15"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM27213SQ"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="99K2360"/>
<attribute name="PACKAGE" value="QFN-48"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM27222M" prefix="U">
<description>Synchronous MOSFET Driver</description>
<gates>
<gate name="A" symbol="LM27222M"/>
</gates>
<devices>
<device name="" package="SOIC127P620X175-8N">
<connects>
<connect gate="A" pin="CB" pad="3"/>
<connect gate="A" pin="GND" pad="8"/>
<connect gate="A" pin="HG" pad="2"/>
<connect gate="A" pin="IN" pad="4"/>
<connect gate="A" pin="LEN" pad="5"/>
<connect gate="A" pin="LG" pad="7"/>
<connect gate="A" pin="SW" pad="1"/>
<connect gate="A" pin="VCC" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM27222M"/>
<attribute name="OC_FARNELL" value="1008002"/>
<attribute name="OC_NEWARK" value="97K3291"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2727MTC" prefix="U">
<description>Low Voltage N-Channel MOSFET Synchronous Buck Regulator Controller</description>
<gates>
<gate name="A" symbol="LM2727MTC"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-14N">
<connects>
<connect gate="A" pin="BOOT" pad="1"/>
<connect gate="A" pin="EAO" pad="8"/>
<connect gate="A" pin="FB" pad="10"/>
<connect gate="A" pin="FREQ" pad="11"/>
<connect gate="A" pin="HG" pad="14"/>
<connect gate="A" pin="ISEN" pad="7"/>
<connect gate="A" pin="LG" pad="2"/>
<connect gate="A" pin="PGND" pad="13"/>
<connect gate="A" pin="PGND_2" pad="3"/>
<connect gate="A" pin="PWGD" pad="6"/>
<connect gate="A" pin="SGND" pad="4"/>
<connect gate="A" pin="SS" pad="9"/>
<connect gate="A" pin="VCC" pad="5"/>
<connect gate="A" pin="~SD" pad="12"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2727MTC"/>
<attribute name="OC_FARNELL" value="8181632"/>
<attribute name="OC_NEWARK" value="41K4295"/>
<attribute name="PACKAGE" value="SOP-14"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM27313XMF" prefix="U">
<description>BOOST CONVERTER</description>
<gates>
<gate name="A" symbol="LM27313XMF"/>
</gates>
<devices>
<device name="" package="SOT95P285X120-5N">
<connects>
<connect gate="A" pin="FB" pad="3"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="SW" pad="1"/>
<connect gate="A" pin="VIN" pad="5"/>
<connect gate="A" pin="~SHDN" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM27313XMF"/>
<attribute name="OC_FARNELL" value="1564771"/>
<attribute name="OC_NEWARK" value="32M1010"/>
<attribute name="PACKAGE" value="SOT-23-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2731XMF" prefix="U">
<description>Boost Converters</description>
<gates>
<gate name="A" symbol="LM2731XMF"/>
</gates>
<devices>
<device name="" package="SOT95P284X119-5N">
<connects>
<connect gate="A" pin="FB" pad="3"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="SW" pad="1"/>
<connect gate="A" pin="VIN" pad="5"/>
<connect gate="A" pin="~SD" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2731XMF"/>
<attribute name="OC_FARNELL" value="8181640"/>
<attribute name="OC_NEWARK" value="29H6289"/>
<attribute name="PACKAGE" value="SOT-23-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2731YMF" prefix="U">
<description>Boost Converters</description>
<gates>
<gate name="A" symbol="LM2731YMF"/>
</gates>
<devices>
<device name="" package="SOT95P284X119-5N">
<connects>
<connect gate="A" pin="FB" pad="3"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="SW" pad="1"/>
<connect gate="A" pin="VIN" pad="5"/>
<connect gate="A" pin="~SD" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2731YMF"/>
<attribute name="OC_FARNELL" value="8181659"/>
<attribute name="OC_NEWARK" value="82H4026"/>
<attribute name="PACKAGE" value="SOT-23-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2733XMF" prefix="U">
<description>Boost Converters</description>
<gates>
<gate name="A" symbol="LM2733XMF"/>
</gates>
<devices>
<device name="" package="SOT95P284X119-5N">
<connects>
<connect gate="A" pin="FB" pad="3"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="SW" pad="1"/>
<connect gate="A" pin="VIN" pad="5"/>
<connect gate="A" pin="~SD" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2733XMF"/>
<attribute name="OC_FARNELL" value="8181667"/>
<attribute name="OC_NEWARK" value="26H4073"/>
<attribute name="PACKAGE" value="SOT-23-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2733YMF" prefix="U">
<description>Boost Converters</description>
<gates>
<gate name="A" symbol="LM2733YMF"/>
</gates>
<devices>
<device name="" package="SOT95P284X119-5N">
<connects>
<connect gate="A" pin="FB" pad="3"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="SW" pad="1"/>
<connect gate="A" pin="VIN" pad="5"/>
<connect gate="A" pin="~SD" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2733YMF"/>
<attribute name="OC_FARNELL" value="8181675"/>
<attribute name="OC_NEWARK" value="26H4075"/>
<attribute name="PACKAGE" value="SOT-23-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM27341MY">
<description>Step-Down DC-DC Regulator</description>
<gates>
<gate name="A" symbol="LM27341MY"/>
</gates>
<devices>
<device name="" package="SOP50P490X110-11N">
<connects>
<connect gate="A" pin="AVIN" pad="8"/>
<connect gate="A" pin="BOOST" pad="3"/>
<connect gate="A" pin="EN" pad="4"/>
<connect gate="A" pin="EP" pad="11"/>
<connect gate="A" pin="FB" pad="6"/>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="PVIN" pad="10"/>
<connect gate="A" pin="PVIN_2" pad="9"/>
<connect gate="A" pin="SW" pad="2"/>
<connect gate="A" pin="SW_2" pad="1"/>
<connect gate="A" pin="SYNC" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM27341MY"/>
<attribute name="OC_FARNELL" value="1694593"/>
<attribute name="OC_NEWARK" value="46P3252"/>
<attribute name="PACKAGE" value="MSOP-10"/>
<attribute name="SUPPLIER" value="National semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM27341QMY">
<description>Step-Down DC-DC Regulator</description>
<gates>
<gate name="A" symbol="LM27341QMY"/>
</gates>
<devices>
<device name="" package="SOP50P490X110-11N">
<connects>
<connect gate="A" pin="AVIN" pad="8"/>
<connect gate="A" pin="BOOST" pad="3"/>
<connect gate="A" pin="EN" pad="4"/>
<connect gate="A" pin="EP" pad="11"/>
<connect gate="A" pin="FB" pad="6"/>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="PVIN" pad="10"/>
<connect gate="A" pin="PVIN_2" pad="9"/>
<connect gate="A" pin="SW" pad="2"/>
<connect gate="A" pin="SW_2" pad="1"/>
<connect gate="A" pin="SYNC" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM27341QMY"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="55R3855"/>
<attribute name="PACKAGE" value="MSOP-10"/>
<attribute name="SUPPLIER" value="National semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM27341SD">
<description>STEP-DOWN DC/DC REGULATOR</description>
<gates>
<gate name="A" symbol="LM27341SD"/>
</gates>
<devices>
<device name="" package="DFN300X300X80-11N">
<connects>
<connect gate="A" pin="AVIN" pad="8"/>
<connect gate="A" pin="BOOST" pad="3"/>
<connect gate="A" pin="EN" pad="4"/>
<connect gate="A" pin="EP" pad="11"/>
<connect gate="A" pin="FB" pad="6"/>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="PVIN" pad="10"/>
<connect gate="A" pin="PVIN_2" pad="9"/>
<connect gate="A" pin="SW" pad="2"/>
<connect gate="A" pin="SW_2" pad="1"/>
<connect gate="A" pin="SYNC" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM27341SD"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="46P3253"/>
<attribute name="PACKAGE" value="DFN-10"/>
<attribute name="SUPPLIER" value="National semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM27342MY">
<description>STEP-DOWN DC/DC REGULATOR</description>
<gates>
<gate name="A" symbol="LM27342MY"/>
</gates>
<devices>
<device name="" package="SOP50P490X110-11N">
<connects>
<connect gate="A" pin="AVIN" pad="8"/>
<connect gate="A" pin="BOOST" pad="3"/>
<connect gate="A" pin="EN" pad="4"/>
<connect gate="A" pin="EP" pad="11"/>
<connect gate="A" pin="FB" pad="6"/>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="PVIN" pad="10"/>
<connect gate="A" pin="PVIN_2" pad="9"/>
<connect gate="A" pin="SW" pad="2"/>
<connect gate="A" pin="SW_2" pad="1"/>
<connect gate="A" pin="SYNC" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM27342MY"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="46P3254"/>
<attribute name="PACKAGE" value="MSOP-10"/>
<attribute name="SUPPLIER" value="National semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM27342QMY">
<description>Step-Down DC-DC Regulator</description>
<gates>
<gate name="A" symbol="LM27342QMY"/>
</gates>
<devices>
<device name="" package="SOP50P490X110-11N">
<connects>
<connect gate="A" pin="AVIN" pad="8"/>
<connect gate="A" pin="BOOST" pad="3"/>
<connect gate="A" pin="EN" pad="4"/>
<connect gate="A" pin="EP" pad="11"/>
<connect gate="A" pin="FB" pad="6"/>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="PVIN" pad="10"/>
<connect gate="A" pin="PVIN_2" pad="9"/>
<connect gate="A" pin="SW" pad="2"/>
<connect gate="A" pin="SW_2" pad="1"/>
<connect gate="A" pin="SYNC" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM27342QMY"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="55R3857"/>
<attribute name="PACKAGE" value="MSOP-10"/>
<attribute name="SUPPLIER" value="National semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM27342SD">
<description>STEP-DOWN DC/DC REGULATOR</description>
<gates>
<gate name="A" symbol="LM27342SD"/>
</gates>
<devices>
<device name="" package="DFN300X300X80-11N">
<connects>
<connect gate="A" pin="AVIN" pad="8"/>
<connect gate="A" pin="BOOST" pad="3"/>
<connect gate="A" pin="EN" pad="4"/>
<connect gate="A" pin="EP" pad="11"/>
<connect gate="A" pin="FB" pad="6"/>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="PVIN" pad="10"/>
<connect gate="A" pin="PVIN_2" pad="9"/>
<connect gate="A" pin="SW" pad="2"/>
<connect gate="A" pin="SW_2" pad="1"/>
<connect gate="A" pin="SYNC" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM27342SD"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="46P3255"/>
<attribute name="PACKAGE" value="DFN-10"/>
<attribute name="SUPPLIER" value="National semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2734XMK" prefix="U">
<description>IC BUCK ADJ 1A</description>
<gates>
<gate name="A" symbol="LM2734XMK"/>
</gates>
<devices>
<device name="" package="SOT95P285X100-6N">
<connects>
<connect gate="A" pin="BOOST" pad="1"/>
<connect gate="A" pin="EN" pad="4"/>
<connect gate="A" pin="FB" pad="3"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="SW" pad="6"/>
<connect gate="A" pin="VIN" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2734XMK"/>
<attribute name="OC_FARNELL" value="1652388"/>
<attribute name="OC_NEWARK" value="41K4307"/>
<attribute name="PACKAGE" value="TSOT23-6"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2734XQMK" prefix="U">
<description>Step-Down DC-DC Regulator</description>
<gates>
<gate name="A" symbol="LM2734XQMK"/>
</gates>
<devices>
<device name="" package="SOT95P285X100-6N">
<connects>
<connect gate="A" pin="BST" pad="1"/>
<connect gate="A" pin="EN" pad="4"/>
<connect gate="A" pin="FB" pad="3"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="SW" pad="6"/>
<connect gate="A" pin="VIN" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2734XQMK"/>
<attribute name="OC_FARNELL" value="1663027"/>
<attribute name="OC_NEWARK" value="15P1971"/>
<attribute name="PACKAGE" value="SOT-6"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2734YMK" prefix="U">
<description>Step-Down DC-DC Regulator</description>
<gates>
<gate name="A" symbol="LM2734YMK"/>
</gates>
<devices>
<device name="" package="SOT95P285X100-6N">
<connects>
<connect gate="A" pin="BOOST" pad="1"/>
<connect gate="A" pin="EN" pad="4"/>
<connect gate="A" pin="FB" pad="3"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="SW" pad="6"/>
<connect gate="A" pin="VIN" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2734YMK"/>
<attribute name="OC_FARNELL" value="1312553"/>
<attribute name="OC_NEWARK" value="41K4309"/>
<attribute name="PACKAGE" value="SOT-6"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2734YQMK" prefix="U">
<description>Step-Down DC-DC Regulator</description>
<gates>
<gate name="A" symbol="LM2734YQMK"/>
</gates>
<devices>
<device name="" package="SOT95P285X100-6N">
<connects>
<connect gate="A" pin="BST" pad="1"/>
<connect gate="A" pin="EN" pad="4"/>
<connect gate="A" pin="FB" pad="3"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="SW" pad="6"/>
<connect gate="A" pin="VIN" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2734YQMK"/>
<attribute name="OC_FARNELL" value="1663029"/>
<attribute name="OC_NEWARK" value="15P1973"/>
<attribute name="PACKAGE" value="SOT-6"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2734ZQSD" prefix="U">
<description>IC REG DC-DC 1A STEP DOWN</description>
<gates>
<gate name="A" symbol="LM2734ZQSD"/>
</gates>
<devices>
<device name="" package="DFN300X300X80-7N">
<connects>
<connect gate="A" pin="BOOST" pad="3"/>
<connect gate="A" pin="DAP" pad="7"/>
<connect gate="A" pin="EN" pad="6"/>
<connect gate="A" pin="FB" pad="1"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="SW" pad="4"/>
<connect gate="A" pin="VIN" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2734ZQSD"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="34P4812"/>
<attribute name="PACKAGE" value="6-WDFN Exposed Pad"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2735XMF" prefix="U">
<description>IC BOOST/SEPIC ADJ 2.1A</description>
<gates>
<gate name="A" symbol="LM2735XMF"/>
</gates>
<devices>
<device name="" package="SOT95P285X110-5N">
<connects>
<connect gate="A" pin="EN" pad="4"/>
<connect gate="A" pin="FB" pad="3"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="SW" pad="1"/>
<connect gate="A" pin="VIN" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2735XMF"/>
<attribute name="OC_FARNELL" value="1685534"/>
<attribute name="OC_NEWARK" value="50M8798"/>
<attribute name="PACKAGE" value="SOT23-5"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2735XMY" prefix="U">
<description>Space-Efficient Boost and SEPIC DC-DC Regulator</description>
<gates>
<gate name="A" symbol="LM2735XMY"/>
</gates>
<devices>
<device name="" package="SOP65P490X110-9N">
<connects>
<connect gate="A" pin="AGND" pad="6"/>
<connect gate="A" pin="EN" pad="4"/>
<connect gate="A" pin="EPAD" pad="9"/>
<connect gate="A" pin="FB" pad="5"/>
<connect gate="A" pin="NC" pad="1"/>
<connect gate="A" pin="NC_2" pad="8"/>
<connect gate="A" pin="PGND" pad="2"/>
<connect gate="A" pin="SW" pad="7"/>
<connect gate="A" pin="VIN" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2735XMY"/>
<attribute name="OC_FARNELL" value="1433149"/>
<attribute name="OC_NEWARK" value="50M8799"/>
<attribute name="PACKAGE" value="MSOP-8"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2735XQMF" prefix="U">
<description>SEPIC DC-DC Regulatoe</description>
<gates>
<gate name="A" symbol="LM2735XQMF"/>
</gates>
<devices>
<device name="" package="SOT65P285X120-5N">
<connects>
<connect gate="A" pin="EN" pad="4"/>
<connect gate="A" pin="FB" pad="3"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="SW" pad="1"/>
<connect gate="A" pin="VIN" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2735XQMF"/>
<attribute name="OC_FARNELL" value="1667425"/>
<attribute name="OC_NEWARK" value="15P1977"/>
<attribute name="PACKAGE" value="SOT-23-5"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2735XSD" prefix="U">
<description>IC REG BOOST/SEPIC DC-DC</description>
<gates>
<gate name="A" symbol="LM2735XSD"/>
</gates>
<devices>
<device name="" package="DFN300X300X80-7N">
<connects>
<connect gate="A" pin="AGND" pad="5"/>
<connect gate="A" pin="DAP" pad="7"/>
<connect gate="A" pin="EN" pad="3"/>
<connect gate="A" pin="FB" pad="4"/>
<connect gate="A" pin="PGND" pad="1"/>
<connect gate="A" pin="SW" pad="6"/>
<connect gate="A" pin="VIN" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2735XSD"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="50M8800"/>
<attribute name="PACKAGE" value="6-WDFN Exposed Pad"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2735YMF" prefix="U">
<description>IC BOOST SEPIC ADJ 2.1A</description>
<gates>
<gate name="A" symbol="LM2735YMF"/>
</gates>
<devices>
<device name="" package="SOT95P285X110-5N">
<connects>
<connect gate="A" pin="EN" pad="4"/>
<connect gate="A" pin="FB" pad="3"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="SW" pad="1"/>
<connect gate="A" pin="VIN" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2735YMF"/>
<attribute name="OC_FARNELL" value="1426509"/>
<attribute name="OC_NEWARK" value="50M8801"/>
<attribute name="PACKAGE" value="SOT23-5"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2735YMY" prefix="U">
<description>IC REG BOOST/SEPIC DC-DC</description>
<gates>
<gate name="A" symbol="LM2735YMY"/>
</gates>
<devices>
<device name="" package="SOP65P490X109-9N">
<connects>
<connect gate="A" pin="AGND" pad="6"/>
<connect gate="A" pin="DAP" pad="9"/>
<connect gate="A" pin="EN" pad="4"/>
<connect gate="A" pin="FB" pad="5"/>
<connect gate="A" pin="NC" pad="8"/>
<connect gate="A" pin="NC_2" pad="1"/>
<connect gate="A" pin="PGND" pad="2"/>
<connect gate="A" pin="SW" pad="7"/>
<connect gate="A" pin="VIN" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2735YMY"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="50M8802"/>
<attribute name="PACKAGE" value="8-EMSOP"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2735YQMF" prefix="U">
<description>SEPIC DC-DC Regulatoe</description>
<gates>
<gate name="A" symbol="LM2735YQMF"/>
</gates>
<devices>
<device name="" package="SOT65P285X120-5N">
<connects>
<connect gate="A" pin="EN" pad="4"/>
<connect gate="A" pin="FB" pad="3"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="SW" pad="1"/>
<connect gate="A" pin="VIN" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2735YQMF"/>
<attribute name="OC_FARNELL" value="1699381"/>
<attribute name="OC_NEWARK" value="80P4537"/>
<attribute name="PACKAGE" value="SOT-23-5"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2735YSD" prefix="U">
<description>IC REG BOOST/SEPIC DC-DC</description>
<gates>
<gate name="A" symbol="LM2735YSD"/>
</gates>
<devices>
<device name="" package="DFN300X300X80-7N">
<connects>
<connect gate="A" pin="AGND" pad="5"/>
<connect gate="A" pin="DAP" pad="7"/>
<connect gate="A" pin="EN" pad="3"/>
<connect gate="A" pin="FB" pad="4"/>
<connect gate="A" pin="PGND" pad="1"/>
<connect gate="A" pin="SW" pad="6"/>
<connect gate="A" pin="VIN" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2735YSD"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="50M8803"/>
<attribute name="PACKAGE" value="6-WDFN Exposed Pad"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2736XMK" prefix="U">
<description>IC BUCK ADJ 750MA</description>
<gates>
<gate name="A" symbol="LM2736XMK"/>
</gates>
<devices>
<device name="" package="SOT95P285X100-6N">
<connects>
<connect gate="A" pin="BOOST" pad="1"/>
<connect gate="A" pin="EN" pad="4"/>
<connect gate="A" pin="FB" pad="3"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="SW" pad="6"/>
<connect gate="A" pin="VIN" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2736XMK"/>
<attribute name="OC_FARNELL" value="1685631"/>
<attribute name="OC_NEWARK" value="41K4315"/>
<attribute name="PACKAGE" value="TSOT23-6"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2736YMK" prefix="U">
<description>Step-Down DC-DC Regulator</description>
<gates>
<gate name="A" symbol="LM2736YMK"/>
</gates>
<devices>
<device name="" package="SOT95P285X100-6N">
<connects>
<connect gate="A" pin="BOOST" pad="1"/>
<connect gate="A" pin="EN" pad="4"/>
<connect gate="A" pin="FB" pad="3"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="SW" pad="6"/>
<connect gate="A" pin="VIN" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2736YMK"/>
<attribute name="OC_FARNELL" value="1312554"/>
<attribute name="OC_NEWARK" value="65J5296"/>
<attribute name="PACKAGE" value="SOT-6"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2737MTC" prefix="U">
<description>IC REG CTRLR BUCK N-CH</description>
<gates>
<gate name="A" symbol="LM2737MTC"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-14N">
<connects>
<connect gate="A" pin="BOOT" pad="1"/>
<connect gate="A" pin="EAO" pad="8"/>
<connect gate="A" pin="EN" pad="12"/>
<connect gate="A" pin="FB" pad="10"/>
<connect gate="A" pin="FREQ" pad="11"/>
<connect gate="A" pin="HG" pad="14"/>
<connect gate="A" pin="ISEN" pad="7"/>
<connect gate="A" pin="LG" pad="2"/>
<connect gate="A" pin="PGND" pad="13"/>
<connect gate="A" pin="PGND_2" pad="3"/>
<connect gate="A" pin="PWGD" pad="6"/>
<connect gate="A" pin="SGND" pad="4"/>
<connect gate="A" pin="SS" pad="9"/>
<connect gate="A" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2737MTC"/>
<attribute name="OC_FARNELL" value="1286744"/>
<attribute name="OC_NEWARK" value="41K4319"/>
<attribute name="PACKAGE" value="Switcher"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2738XMY" prefix="U">
<description>Step-Down DC-DC Switching Regulator</description>
<gates>
<gate name="A" symbol="LM2738XMY"/>
</gates>
<devices>
<device name="" package="SOP65P490X110-9N">
<connects>
<connect gate="A" pin="BST" pad="1"/>
<connect gate="A" pin="EN" pad="4"/>
<connect gate="A" pin="EPAD" pad="9"/>
<connect gate="A" pin="FB" pad="6"/>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="GND_2" pad="7"/>
<connect gate="A" pin="IN" pad="2"/>
<connect gate="A" pin="SW" pad="8"/>
<connect gate="A" pin="VCC" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2738XMY"/>
<attribute name="OC_FARNELL" value="1589524"/>
<attribute name="OC_NEWARK" value="08N3583"/>
<attribute name="PACKAGE" value="MSOP-8"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2738XSD" prefix="U">
<description>IC REG SW 1.6MHZ 1.5A</description>
<gates>
<gate name="A" symbol="LM2738XSD"/>
</gates>
<devices>
<device name="" package="DFN300X300X80-9N">
<connects>
<connect gate="A" pin="BST" pad="1"/>
<connect gate="A" pin="EN" pad="4"/>
<connect gate="A" pin="EP" pad="9"/>
<connect gate="A" pin="FB" pad="6"/>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="GND_2" pad="7"/>
<connect gate="A" pin="IN" pad="2"/>
<connect gate="A" pin="SW" pad="8"/>
<connect gate="A" pin="VCC" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2738XSD"/>
<attribute name="OC_FARNELL" value="1685775"/>
<attribute name="OC_NEWARK" value="08N3584"/>
<attribute name="PACKAGE" value="8-WFDFN Exposed Pad"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2738YMY" prefix="U">
<description>Step-Down DC-DC Switching Regulator</description>
<gates>
<gate name="A" symbol="LM2738YMY"/>
</gates>
<devices>
<device name="" package="SOP65P490X110-9N">
<connects>
<connect gate="A" pin="BST" pad="1"/>
<connect gate="A" pin="EN" pad="4"/>
<connect gate="A" pin="EPAD" pad="9"/>
<connect gate="A" pin="FB" pad="6"/>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="GND_2" pad="7"/>
<connect gate="A" pin="IN" pad="2"/>
<connect gate="A" pin="SW" pad="8"/>
<connect gate="A" pin="VCC" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2738YMY"/>
<attribute name="OC_FARNELL" value="1589525"/>
<attribute name="OC_NEWARK" value="08N3585"/>
<attribute name="PACKAGE" value="MSOP-8"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2738YSD" prefix="U">
<description>IC REG SW 550KHZ 1.5A</description>
<gates>
<gate name="A" symbol="LM2738YSD"/>
</gates>
<devices>
<device name="" package="DFN300X300X80-9N">
<connects>
<connect gate="A" pin="BST" pad="1"/>
<connect gate="A" pin="EN" pad="4"/>
<connect gate="A" pin="EP" pad="9"/>
<connect gate="A" pin="FB" pad="6"/>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="GND_2" pad="7"/>
<connect gate="A" pin="IN" pad="2"/>
<connect gate="A" pin="SW" pad="8"/>
<connect gate="A" pin="VCC" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2738YSD"/>
<attribute name="OC_FARNELL" value="1685777"/>
<attribute name="OC_NEWARK" value="08N3586"/>
<attribute name="PACKAGE" value="8-WFDFN Exposed Pad"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2742MTC" prefix="U">
<description>IC CTRL/REG SYNC BUCK</description>
<gates>
<gate name="A" symbol="LM2742MTC"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-14N">
<connects>
<connect gate="A" pin="BOOT" pad="1"/>
<connect gate="A" pin="EAO" pad="8"/>
<connect gate="A" pin="FB" pad="10"/>
<connect gate="A" pin="FREQ" pad="11"/>
<connect gate="A" pin="HG" pad="14"/>
<connect gate="A" pin="ISEN" pad="7"/>
<connect gate="A" pin="LG" pad="2"/>
<connect gate="A" pin="PGND" pad="3"/>
<connect gate="A" pin="PGND_2" pad="13"/>
<connect gate="A" pin="PWGD" pad="6"/>
<connect gate="A" pin="SGND" pad="4"/>
<connect gate="A" pin="SS" pad="9"/>
<connect gate="A" pin="VCC" pad="5"/>
<connect gate="A" pin="~SD" pad="12"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2742MTC"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K4321"/>
<attribute name="PACKAGE" value="14-TSSOP"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2743MTC" prefix="U">
<description>Low Voltage N-Channel MOSFET Synchronous Buck Regulator Controller</description>
<gates>
<gate name="A" symbol="LM2743MTC"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-14N">
<connects>
<connect gate="A" pin="BOOT" pad="1"/>
<connect gate="A" pin="EAO" pad="8"/>
<connect gate="A" pin="FB" pad="10"/>
<connect gate="A" pin="FREQ" pad="11"/>
<connect gate="A" pin="HG" pad="14"/>
<connect gate="A" pin="ISEN" pad="7"/>
<connect gate="A" pin="LG" pad="2"/>
<connect gate="A" pin="PGND" pad="13"/>
<connect gate="A" pin="PGND_2" pad="3"/>
<connect gate="A" pin="PWGD" pad="6"/>
<connect gate="A" pin="SGND" pad="4"/>
<connect gate="A" pin="SS/TRACK" pad="9"/>
<connect gate="A" pin="VCC" pad="5"/>
<connect gate="A" pin="~SD" pad="12"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2743MTC"/>
<attribute name="OC_FARNELL" value="8181705"/>
<attribute name="OC_NEWARK" value="38K3686"/>
<attribute name="PACKAGE" value="SOP-14"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2745MTC" prefix="U">
<description>Synchronous Buck Controller</description>
<gates>
<gate name="A" symbol="LM2745MTC"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-14N">
<connects>
<connect gate="A" pin="BOOT" pad="1"/>
<connect gate="A" pin="EAO" pad="8"/>
<connect gate="A" pin="FB" pad="10"/>
<connect gate="A" pin="FREQ/SYNC" pad="11"/>
<connect gate="A" pin="HG" pad="14"/>
<connect gate="A" pin="ISEN" pad="7"/>
<connect gate="A" pin="LG" pad="2"/>
<connect gate="A" pin="PGND" pad="13"/>
<connect gate="A" pin="PGND_2" pad="3"/>
<connect gate="A" pin="PGOOD" pad="6"/>
<connect gate="A" pin="SGND" pad="4"/>
<connect gate="A" pin="SS/TRACK" pad="9"/>
<connect gate="A" pin="VCC" pad="5"/>
<connect gate="A" pin="~SD" pad="12"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2745MTC"/>
<attribute name="OC_FARNELL" value="1286745"/>
<attribute name="OC_NEWARK" value="41K4327"/>
<attribute name="PACKAGE" value="SOP-14"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2747MTC" prefix="U">
<description>IC CTRLR SYNC BUCK</description>
<gates>
<gate name="A" symbol="LM2747MTC"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-14N">
<connects>
<connect gate="A" pin="BOOT" pad="1"/>
<connect gate="A" pin="EAO" pad="8"/>
<connect gate="A" pin="FB" pad="10"/>
<connect gate="A" pin="FREQ/SYNC" pad="11"/>
<connect gate="A" pin="HG" pad="14"/>
<connect gate="A" pin="ISEN" pad="7"/>
<connect gate="A" pin="LG" pad="2"/>
<connect gate="A" pin="PGND" pad="3"/>
<connect gate="A" pin="PGND_2" pad="13"/>
<connect gate="A" pin="PWGD" pad="6"/>
<connect gate="A" pin="SGND" pad="4"/>
<connect gate="A" pin="SS/TRACK" pad="9"/>
<connect gate="A" pin="VCC" pad="5"/>
<connect gate="A" pin="~SD" pad="12"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2747MTC"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="99K2366"/>
<attribute name="PACKAGE" value="14-TSSOP"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2750LD-5.0" prefix="U">
<description>IC CONV REG SW CAP 5V</description>
<gates>
<gate name="A" symbol="LM2750LD-5.0"/>
</gates>
<devices>
<device name="" package="DFN300X300X80-11N">
<connects>
<connect gate="A" pin="C+" pad="10"/>
<connect gate="A" pin="C-" pad="7"/>
<connect gate="A" pin="FB" pad="3"/>
<connect gate="A" pin="GND" pad="11"/>
<connect gate="A" pin="GND_2" pad="5"/>
<connect gate="A" pin="GND_3" pad="6"/>
<connect gate="A" pin="SD" pad="4"/>
<connect gate="A" pin="VIN" pad="9"/>
<connect gate="A" pin="VIN_2" pad="8"/>
<connect gate="A" pin="VOUT" pad="1"/>
<connect gate="A" pin="VOUT_2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2750LD-50"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K4334"/>
<attribute name="PACKAGE" value="10-WFDFN Exposed Pad"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2750LD-ADJ" prefix="U">
<description>IC CONV REG SW CAP ADJ</description>
<gates>
<gate name="A" symbol="LM2750LD-ADJ"/>
</gates>
<devices>
<device name="" package="DFN300X300X80-11N">
<connects>
<connect gate="A" pin="C+" pad="10"/>
<connect gate="A" pin="C-" pad="7"/>
<connect gate="A" pin="FB" pad="3"/>
<connect gate="A" pin="GND" pad="11"/>
<connect gate="A" pin="GND_2" pad="5"/>
<connect gate="A" pin="GND_3" pad="6"/>
<connect gate="A" pin="SD" pad="4"/>
<connect gate="A" pin="VIN" pad="9"/>
<connect gate="A" pin="VIN_2" pad="8"/>
<connect gate="A" pin="VOUT" pad="1"/>
<connect gate="A" pin="VOUT_2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2750LD-ADJ"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K4333"/>
<attribute name="PACKAGE" value="10-WFDFN Exposed Pad"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2750SD-5.0" prefix="U">
<description>IC CONV REG SW CAP 5V</description>
<gates>
<gate name="A" symbol="LM2750SD-5.0"/>
</gates>
<devices>
<device name="" package="DFN300X300X80-11N">
<connects>
<connect gate="A" pin="C+" pad="10"/>
<connect gate="A" pin="C-" pad="7"/>
<connect gate="A" pin="FB" pad="3"/>
<connect gate="A" pin="GND" pad="11"/>
<connect gate="A" pin="GND_2" pad="5"/>
<connect gate="A" pin="GND_3" pad="6"/>
<connect gate="A" pin="SD" pad="4"/>
<connect gate="A" pin="VIN" pad="9"/>
<connect gate="A" pin="VIN_2" pad="8"/>
<connect gate="A" pin="VOUT" pad="2"/>
<connect gate="A" pin="VOUT_2" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2750SD-5.0"/>
<attribute name="OC_FARNELL" value="1685760"/>
<attribute name="OC_NEWARK" value="69K2411"/>
<attribute name="PACKAGE" value="10-WFDFN Exposed Pad"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2750SD-ADJ" prefix="U">
<description>IC CONV REG SW CAP ADJ</description>
<gates>
<gate name="A" symbol="LM2750SD-ADJ"/>
</gates>
<devices>
<device name="" package="DFN300X300X80-11N">
<connects>
<connect gate="A" pin="C+" pad="10"/>
<connect gate="A" pin="C-" pad="7"/>
<connect gate="A" pin="FB" pad="3"/>
<connect gate="A" pin="GND" pad="11"/>
<connect gate="A" pin="GND_2" pad="5"/>
<connect gate="A" pin="GND_3" pad="6"/>
<connect gate="A" pin="SD" pad="4"/>
<connect gate="A" pin="VIN" pad="9"/>
<connect gate="A" pin="VIN_2" pad="8"/>
<connect gate="A" pin="VOUT" pad="2"/>
<connect gate="A" pin="VOUT_2" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2750SD-ADJ"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="99K2371"/>
<attribute name="PACKAGE" value="10-WFDFN Exposed Pad"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2751SD-A" prefix="U">
<description>LED DRIVR WHITE BCKLGT</description>
<gates>
<gate name="A" symbol="LM2751SD-A"/>
</gates>
<devices>
<device name="" package="DFN300X300X80-11N">
<connects>
<connect gate="A" pin="C1+" pad="2"/>
<connect gate="A" pin="C1-" pad="9"/>
<connect gate="A" pin="C2+" pad="10"/>
<connect gate="A" pin="C2-" pad="7"/>
<connect gate="A" pin="CS0" pad="4"/>
<connect gate="A" pin="CS1" pad="5"/>
<connect gate="A" pin="EN" pad="6"/>
<connect gate="A" pin="GND" pad="8"/>
<connect gate="A" pin="GND_2" pad="11"/>
<connect gate="A" pin="VIN" pad="3"/>
<connect gate="A" pin="VOUT" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2751SD-A"/>
<attribute name="OC_FARNELL" value="1675271"/>
<attribute name="OC_NEWARK" value="41K4337"/>
<attribute name="PACKAGE" value="10-WFDFN Exposed Pad"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2751SD-B" prefix="U">
<description>LED DRIVR WHITE BCKLGT</description>
<gates>
<gate name="A" symbol="LM2751SD-B"/>
</gates>
<devices>
<device name="" package="DFN300X300X80-11N">
<connects>
<connect gate="A" pin="C1+" pad="2"/>
<connect gate="A" pin="C1-" pad="9"/>
<connect gate="A" pin="C2+" pad="10"/>
<connect gate="A" pin="C2-" pad="7"/>
<connect gate="A" pin="CS0" pad="4"/>
<connect gate="A" pin="CS1" pad="5"/>
<connect gate="A" pin="EN" pad="6"/>
<connect gate="A" pin="GND" pad="8"/>
<connect gate="A" pin="GND_2" pad="11"/>
<connect gate="A" pin="VIN" pad="3"/>
<connect gate="A" pin="VOUT" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2751SD-B"/>
<attribute name="OC_FARNELL" value="1312557"/>
<attribute name="OC_NEWARK" value="41K4338"/>
<attribute name="PACKAGE" value="10-WFDFN Exposed Pad"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2753SD" prefix="U">
<description>IC LED DRIVER PHOTO FLASH</description>
<gates>
<gate name="A" symbol="LM2753SD"/>
</gates>
<devices>
<device name="" package="DFN300X300X80-11N">
<connects>
<connect gate="A" pin="C1+" pad="1"/>
<connect gate="A" pin="C1-" pad="3"/>
<connect gate="A" pin="EN" pad="6"/>
<connect gate="A" pin="EP" pad="11"/>
<connect gate="A" pin="FLASH" pad="4"/>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="GND_2" pad="10"/>
<connect gate="A" pin="GND_3" pad="7"/>
<connect gate="A" pin="IOUT" pad="8"/>
<connect gate="A" pin="VIN" pad="2"/>
<connect gate="A" pin="VOUT" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2753SD"/>
<attribute name="OC_FARNELL" value="1871520"/>
<attribute name="OC_NEWARK" value="41K4339"/>
<attribute name="PACKAGE" value="10-WFDFN Exposed Pad"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2754SQ" prefix="U">
<description>IC LED DRIVER PHOTO FLASH</description>
<gates>
<gate name="A" symbol="LM2754SQ"/>
</gates>
<devices>
<device name="" package="QFN50P400X400X80-25N">
<connects>
<connect gate="A" pin="C1+" pad="1"/>
<connect gate="A" pin="C1-" pad="2"/>
<connect gate="A" pin="C2+" pad="7"/>
<connect gate="A" pin="C2-" pad="5"/>
<connect gate="A" pin="D1" pad="12"/>
<connect gate="A" pin="D2" pad="13"/>
<connect gate="A" pin="D3" pad="14"/>
<connect gate="A" pin="D4" pad="15"/>
<connect gate="A" pin="EN" pad="21"/>
<connect gate="A" pin="EP" pad="25"/>
<connect gate="A" pin="GND" pad="17"/>
<connect gate="A" pin="GNDSW" pad="3"/>
<connect gate="A" pin="GND_2" pad="9"/>
<connect gate="A" pin="GND_3" pad="16"/>
<connect gate="A" pin="ISET1" pad="10"/>
<connect gate="A" pin="ISET2" pad="11"/>
<connect gate="A" pin="NC" pad="6"/>
<connect gate="A" pin="NC_2" pad="4"/>
<connect gate="A" pin="SEL" pad="18"/>
<connect gate="A" pin="T/F" pad="20"/>
<connect gate="A" pin="TX" pad="19"/>
<connect gate="A" pin="VIN" pad="22"/>
<connect gate="A" pin="VINSW" pad="24"/>
<connect gate="A" pin="VINSW_2" pad="23"/>
<connect gate="A" pin="VOUT" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2754SQ"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="13M1713"/>
<attribute name="PACKAGE" value="24-WFQFN Exposed Pad"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2755TM" prefix="U">
<description>Charge Pump LED Controller</description>
<gates>
<gate name="A" symbol="LM2755TM"/>
</gates>
<devices>
<device name="" package="BGA18C20PX364P5X7_161X180X60">
<connects>
<connect gate="A" pin="ADDR" pad="E7"/>
<connect gate="A" pin="C1+" pad="E1"/>
<connect gate="A" pin="C1-" pad="E5"/>
<connect gate="A" pin="C2+" pad="E3"/>
<connect gate="A" pin="C2-" pad="D4"/>
<connect gate="A" pin="GND" pad="D6"/>
<connect gate="A" pin="GND_2" pad="C3"/>
<connect gate="A" pin="HWEN" pad="B4"/>
<connect gate="A" pin="ID1" pad="A1"/>
<connect gate="A" pin="ID2" pad="A3"/>
<connect gate="A" pin="ID3" pad="A5"/>
<connect gate="A" pin="ISET" pad="B2"/>
<connect gate="A" pin="POUT" pad="D2"/>
<connect gate="A" pin="SCL" pad="C7"/>
<connect gate="A" pin="SDIO" pad="B6"/>
<connect gate="A" pin="SYNC" pad="A7"/>
<connect gate="A" pin="VIN" pad="C1"/>
<connect gate="A" pin="VIO" pad="C5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2755TM"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="64M6971"/>
<attribute name="PACKAGE" value="BGA-18"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2756TM" prefix="U">
<description>IC LED DRVR WHT BCKLT</description>
<gates>
<gate name="A" symbol="LM2756TM"/>
</gates>
<devices>
<device name="" package="BGA20N40P4X5_161X201X60">
<connects>
<connect gate="A" pin="C1+" pad="A1"/>
<connect gate="A" pin="C1-" pad="C1"/>
<connect gate="A" pin="C2+" pad="B1"/>
<connect gate="A" pin="C2-" pad="B2"/>
<connect gate="A" pin="D1A" pad="D3"/>
<connect gate="A" pin="D1B" pad="B3"/>
<connect gate="A" pin="D1C" pad="C3"/>
<connect gate="A" pin="D2A" pad="E3"/>
<connect gate="A" pin="D3A" pad="E4"/>
<connect gate="A" pin="D4A" pad="D4"/>
<connect gate="A" pin="D53" pad="C4"/>
<connect gate="A" pin="D62" pad="B4"/>
<connect gate="A" pin="GND" pad="A4"/>
<connect gate="A" pin="GND_2" pad="D1"/>
<connect gate="A" pin="HWEN" pad="E1"/>
<connect gate="A" pin="ISET" pad="D2"/>
<connect gate="A" pin="SCL" pad="E2"/>
<connect gate="A" pin="SDIO" pad="C2"/>
<connect gate="A" pin="VIN" pad="A3"/>
<connect gate="A" pin="VOUT" pad="A2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2756TM"/>
<attribute name="OC_FARNELL" value="1495074"/>
<attribute name="OC_NEWARK" value="54M4666"/>
<attribute name="PACKAGE" value="20-WFBGA"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2757TM" prefix="U">
<description>Switched Capacitor Boost Regulator</description>
<gates>
<gate name="A" symbol="LM2757TM"/>
</gates>
<devices>
<device name="" package="BGA12C3X4X40P_161X121X67">
<connects>
<connect gate="A" pin="C1+" pad="A3"/>
<connect gate="A" pin="C1-" pad="B1"/>
<connect gate="A" pin="C2+" pad="A1"/>
<connect gate="A" pin="C2-" pad="C3"/>
<connect gate="A" pin="GND" pad="C2"/>
<connect gate="A" pin="GND_2" pad="C1"/>
<connect gate="A" pin="M0" pad="D3"/>
<connect gate="A" pin="M1" pad="D2"/>
<connect gate="A" pin="NC" pad="D1"/>
<connect gate="A" pin="VIN" pad="B2"/>
<connect gate="A" pin="VIN_2" pad="B3"/>
<connect gate="A" pin="VOUT" pad="A2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2757TM"/>
<attribute name="OC_FARNELL" value="1535363"/>
<attribute name="OC_NEWARK" value="64M6973"/>
<attribute name="PACKAGE" value="BGA-12"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2758TL" prefix="U">
<description>IC LED DRIVER PHOTO FLASH</description>
<gates>
<gate name="A" symbol="LM2758TL"/>
</gates>
<devices>
<device name="" package="BGA12N50P3X4_151X199X60">
<connects>
<connect gate="A" pin="C1+" pad="B1"/>
<connect gate="A" pin="C1-" pad="D2"/>
<connect gate="A" pin="C2+" pad="C2"/>
<connect gate="A" pin="C2-" pad="D1"/>
<connect gate="A" pin="CPOUT" pad="B2"/>
<connect gate="A" pin="EN1" pad="A1"/>
<connect gate="A" pin="EN2" pad="B3"/>
<connect gate="A" pin="ISET" pad="A3"/>
<connect gate="A" pin="LED-" pad="C3"/>
<connect gate="A" pin="PGND" pad="D3"/>
<connect gate="A" pin="SGND" pad="A2"/>
<connect gate="A" pin="VIN" pad="C1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2758TL"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="84M8090"/>
<attribute name="PACKAGE" value="12-WFBGA"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2765M6" prefix="U">
<description>IC SW CAP/DBLR ADJ 20MA</description>
<gates>
<gate name="A" symbol="LM2765M6"/>
</gates>
<devices>
<device name="" package="SOT95P285X122-6N">
<connects>
<connect gate="A" pin="CAP+" pad="6"/>
<connect gate="A" pin="CAP-_" pad="3"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="SD" pad="4"/>
<connect gate="A" pin="V+" pad="1"/>
<connect gate="A" pin="VOUT" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2765M6"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="93R4899"/>
<attribute name="PACKAGE" value="SOT-23-6"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2766M6" prefix="U">
<description>IC SW CAP/DBLR ADJ 20MA</description>
<gates>
<gate name="A" symbol="LM2766M6"/>
</gates>
<devices>
<device name="" package="SOT95P285X122-6N">
<connects>
<connect gate="A" pin="CAP+" pad="6"/>
<connect gate="A" pin="CAP-_" pad="3"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="SD" pad="4"/>
<connect gate="A" pin="V+" pad="1"/>
<connect gate="A" pin="VOUT" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2766M6"/>
<attribute name="OC_FARNELL" value="1685633"/>
<attribute name="OC_NEWARK" value="41K4345"/>
<attribute name="PACKAGE" value="SOT-23-6"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2767M5" prefix="U">
<description>Switched Capacitor Voltage Converter</description>
<gates>
<gate name="A" symbol="LM2767M5"/>
</gates>
<devices>
<device name="" package="SOT95P300X120-5N">
<connects>
<connect gate="A" pin="CAP+" pad="5"/>
<connect gate="A" pin="CAP-" pad="3"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="V+" pad="4"/>
<connect gate="A" pin="VOUT" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2767M5"/>
<attribute name="OC_FARNELL" value="1197392"/>
<attribute name="OC_NEWARK" value="41K4347"/>
<attribute name="PACKAGE" value="SOT-23-5"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2771SD" prefix="U">
<description>IC CONV DC/DC SW 250MA</description>
<gates>
<gate name="A" symbol="LM2771SD"/>
</gates>
<devices>
<device name="" package="DFN300X300X80-11N">
<connects>
<connect gate="A" pin="C1+" pad="7"/>
<connect gate="A" pin="C1-" pad="6"/>
<connect gate="A" pin="EN" pad="10"/>
<connect gate="A" pin="GND" pad="11"/>
<connect gate="A" pin="GND_2" pad="2"/>
<connect gate="A" pin="GND_3" pad="9"/>
<connect gate="A" pin="NC" pad="4"/>
<connect gate="A" pin="NC_2" pad="8"/>
<connect gate="A" pin="NC_3" pad="5"/>
<connect gate="A" pin="VOUT" pad="1"/>
<connect gate="A" pin="VOUT_2" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2771SD"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="99K2374"/>
<attribute name="PACKAGE" value="10-WFDFN Exposed Pad"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2794TL" prefix="U">
<description>IC LED DRVR WHT BCKLT</description>
<gates>
<gate name="A" symbol="LM2794TL"/>
</gates>
<devices>
<device name="" package="BGA14C43PX50P5X4_209X240X60">
<connects>
<connect gate="A" pin="BRGT" pad="B6"/>
<connect gate="A" pin="C1+" pad="A1"/>
<connect gate="A" pin="C1-_" pad="B2"/>
<connect gate="A" pin="C2+" pad="A5"/>
<connect gate="A" pin="C2-_" pad="E1"/>
<connect gate="A" pin="D1" pad="E3"/>
<connect gate="A" pin="D2" pad="E5"/>
<connect gate="A" pin="D3" pad="E7"/>
<connect gate="A" pin="D4" pad="D6"/>
<connect gate="A" pin="GND" pad="D2"/>
<connect gate="A" pin="ISET" pad="C7"/>
<connect gate="A" pin="POUT" pad="A3"/>
<connect gate="A" pin="VIN" pad="C1"/>
<connect gate="A" pin="~SD" pad="A7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2794TL"/>
<attribute name="OC_FARNELL" value="1871521"/>
<attribute name="OC_NEWARK" value="41K4375"/>
<attribute name="PACKAGE" value="14-WFBGA"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM27951SD" prefix="U">
<description>LED DRIVER, SW CAP, POWERWISE</description>
<gates>
<gate name="A" symbol="LM27951SD"/>
</gates>
<devices>
<device name="" package="DFN300X400X80-15N">
<connects>
<connect gate="A" pin="C1+" pad="3"/>
<connect gate="A" pin="C1-" pad="14"/>
<connect gate="A" pin="C2+" pad="1"/>
<connect gate="A" pin="C2-" pad="12"/>
<connect gate="A" pin="D1" pad="7"/>
<connect gate="A" pin="D2" pad="6"/>
<connect gate="A" pin="D3" pad="5"/>
<connect gate="A" pin="D4" pad="4"/>
<connect gate="A" pin="EN" pad="9"/>
<connect gate="A" pin="EP" pad="15"/>
<connect gate="A" pin="GND" pad="13"/>
<connect gate="A" pin="ISET" pad="8"/>
<connect gate="A" pin="PWM" pad="10"/>
<connect gate="A" pin="VIN" pad="11"/>
<connect gate="A" pin="VOUT" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM27951SD"/>
<attribute name="OC_FARNELL" value="1312559"/>
<attribute name="OC_NEWARK" value="69K2419"/>
<attribute name="PACKAGE" value="SwitchCap"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM27952SD" prefix="U">
<description>IC, LED DRIVER, CHARGE PUMP</description>
<gates>
<gate name="A" symbol="LM27952SD"/>
</gates>
<devices>
<device name="" package="DFN300X400X80-15N">
<connects>
<connect gate="A" pin="C1+" pad="3"/>
<connect gate="A" pin="C1-" pad="14"/>
<connect gate="A" pin="C2+" pad="1"/>
<connect gate="A" pin="C2-" pad="12"/>
<connect gate="A" pin="D1" pad="7"/>
<connect gate="A" pin="D2" pad="6"/>
<connect gate="A" pin="D3" pad="5"/>
<connect gate="A" pin="D4" pad="4"/>
<connect gate="A" pin="EN" pad="9"/>
<connect gate="A" pin="EP" pad="15"/>
<connect gate="A" pin="GND" pad="13"/>
<connect gate="A" pin="ISET" pad="8"/>
<connect gate="A" pin="PWM" pad="10"/>
<connect gate="A" pin="VIN" pad="11"/>
<connect gate="A" pin="VOUT" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM27952SD"/>
<attribute name="OC_FARNELL" value="1226781"/>
<attribute name="OC_NEWARK" value="41K4379"/>
<attribute name="PACKAGE" value="SwitchCap"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM27964SQ-C" prefix="U">
<description>IC LED DRIVR WHITE BCKLGT</description>
<gates>
<gate name="A" symbol="LM27964SQ-C"/>
</gates>
<devices>
<device name="" package="QFN50P400X400X80-25N">
<connects>
<connect gate="A" pin="C1" pad="22"/>
<connect gate="A" pin="C1_2" pad="19"/>
<connect gate="A" pin="C2" pad="21"/>
<connect gate="A" pin="C2_2" pad="20"/>
<connect gate="A" pin="D1A" pad="16"/>
<connect gate="A" pin="D1B" pad="4"/>
<connect gate="A" pin="D2A" pad="15"/>
<connect gate="A" pin="D2B" pad="5"/>
<connect gate="A" pin="D3A" pad="14"/>
<connect gate="A" pin="D4A" pad="13"/>
<connect gate="A" pin="DKEY" pad="6"/>
<connect gate="A" pin="EP" pad="25"/>
<connect gate="A" pin="GND" pad="10"/>
<connect gate="A" pin="GND_2" pad="18"/>
<connect gate="A" pin="GND_3" pad="9"/>
<connect gate="A" pin="ISETA" pad="17"/>
<connect gate="A" pin="ISETB" pad="3"/>
<connect gate="A" pin="ISETK" pad="12"/>
<connect gate="A" pin="NC" pad="8"/>
<connect gate="A" pin="NC_2" pad="11"/>
<connect gate="A" pin="POUT" pad="23"/>
<connect gate="A" pin="SCL" pad="1"/>
<connect gate="A" pin="SDIO" pad="2"/>
<connect gate="A" pin="VIN" pad="24"/>
<connect gate="A" pin="VIO" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM27964SQ-C"/>
<attribute name="OC_FARNELL" value="1865926"/>
<attribute name="OC_NEWARK" value="04R9160"/>
<attribute name="PACKAGE" value="24-WFQFN Exposed Pad"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM27964SQ-I" prefix="U">
<description>IC LED DRIVR WHITE BCKLGT</description>
<gates>
<gate name="A" symbol="LM27964SQ-I"/>
</gates>
<devices>
<device name="" package="QFN50P400X400X80-25N">
<connects>
<connect gate="A" pin="C1" pad="22"/>
<connect gate="A" pin="C1_2" pad="19"/>
<connect gate="A" pin="C2" pad="21"/>
<connect gate="A" pin="C2_2" pad="20"/>
<connect gate="A" pin="D1A" pad="16"/>
<connect gate="A" pin="D1B" pad="4"/>
<connect gate="A" pin="D2A" pad="15"/>
<connect gate="A" pin="D2B" pad="5"/>
<connect gate="A" pin="D3A" pad="14"/>
<connect gate="A" pin="D4A" pad="13"/>
<connect gate="A" pin="DKEY" pad="6"/>
<connect gate="A" pin="EP" pad="25"/>
<connect gate="A" pin="GND" pad="10"/>
<connect gate="A" pin="GND_2" pad="18"/>
<connect gate="A" pin="GND_3" pad="9"/>
<connect gate="A" pin="ISETA" pad="17"/>
<connect gate="A" pin="ISETB" pad="3"/>
<connect gate="A" pin="ISETK" pad="12"/>
<connect gate="A" pin="NC" pad="8"/>
<connect gate="A" pin="NC_2" pad="11"/>
<connect gate="A" pin="POUT" pad="23"/>
<connect gate="A" pin="SCL" pad="1"/>
<connect gate="A" pin="SDIO" pad="2"/>
<connect gate="A" pin="VIN" pad="24"/>
<connect gate="A" pin="VIO" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM27964SQ-I"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="65K5926"/>
<attribute name="PACKAGE" value="24-WFQFN Exposed Pad"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM27965SQ" prefix="U">
<description>IC, LED DRIVER, CHARGE PUMP</description>
<gates>
<gate name="A" symbol="LM27965SQ"/>
</gates>
<devices>
<device name="" package="QFN50P400X400X80-25N">
<connects>
<connect gate="A" pin="*RESET" pad="10"/>
<connect gate="A" pin="C1" pad="22"/>
<connect gate="A" pin="C1_2" pad="19"/>
<connect gate="A" pin="C2" pad="21"/>
<connect gate="A" pin="C2_2" pad="20"/>
<connect gate="A" pin="D1A" pad="16"/>
<connect gate="A" pin="D1B" pad="4"/>
<connect gate="A" pin="D1C" pad="3"/>
<connect gate="A" pin="D2A" pad="15"/>
<connect gate="A" pin="D2B" pad="5"/>
<connect gate="A" pin="D3A" pad="14"/>
<connect gate="A" pin="D3B" pad="6"/>
<connect gate="A" pin="D4A" pad="13"/>
<connect gate="A" pin="D5A" pad="12"/>
<connect gate="A" pin="EP" pad="25"/>
<connect gate="A" pin="GND" pad="9"/>
<connect gate="A" pin="GND_2" pad="18"/>
<connect gate="A" pin="ISET" pad="17"/>
<connect gate="A" pin="NC" pad="8"/>
<connect gate="A" pin="NC_2" pad="11"/>
<connect gate="A" pin="POUT" pad="23"/>
<connect gate="A" pin="SCL" pad="1"/>
<connect gate="A" pin="SDIO" pad="2"/>
<connect gate="A" pin="VIN" pad="24"/>
<connect gate="A" pin="VIO" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM27965SQ"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="99K2379"/>
<attribute name="PACKAGE" value="24-WFQFN Exposed Pad"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM27966SQ" prefix="U">
<description>IC, LED DRIVER, CHARGE PUMP</description>
<gates>
<gate name="A" symbol="LM27966SQ"/>
</gates>
<devices>
<device name="" package="QFN50P400X400X80-25N">
<connects>
<connect gate="A" pin="*RESET" pad="10"/>
<connect gate="A" pin="C1" pad="22"/>
<connect gate="A" pin="C1_2" pad="19"/>
<connect gate="A" pin="C2" pad="21"/>
<connect gate="A" pin="C2_2" pad="20"/>
<connect gate="A" pin="D1" pad="16"/>
<connect gate="A" pin="D2" pad="15"/>
<connect gate="A" pin="D3" pad="14"/>
<connect gate="A" pin="D4" pad="13"/>
<connect gate="A" pin="D5" pad="12"/>
<connect gate="A" pin="DAUX" pad="3"/>
<connect gate="A" pin="EP" pad="25"/>
<connect gate="A" pin="GND" pad="9"/>
<connect gate="A" pin="GND_2" pad="18"/>
<connect gate="A" pin="ISET" pad="17"/>
<connect gate="A" pin="NC" pad="6"/>
<connect gate="A" pin="NC_2" pad="11"/>
<connect gate="A" pin="NC_3" pad="8"/>
<connect gate="A" pin="NC_4" pad="4"/>
<connect gate="A" pin="NC_5" pad="5"/>
<connect gate="A" pin="POUT" pad="23"/>
<connect gate="A" pin="SCL" pad="1"/>
<connect gate="A" pin="SDIO" pad="2"/>
<connect gate="A" pin="VIN" pad="24"/>
<connect gate="A" pin="VIO" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM27966SQ"/>
<attribute name="OC_FARNELL" value="1675260"/>
<attribute name="OC_NEWARK" value="13M1717"/>
<attribute name="PACKAGE" value="24-WFQFN Exposed Pad"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2825HN-ADJ" prefix="U">
<description>IC CONVERTER DC/DC 1A</description>
<gates>
<gate name="A" symbol="LM2825HN-ADJ"/>
</gates>
<devices>
<device name="" package="DIP254P1524X724-24">
<connects>
<connect gate="A" pin="ADJ" pad="10"/>
<connect gate="A" pin="GND" pad="12"/>
<connect gate="A" pin="GND_2" pad="23"/>
<connect gate="A" pin="GND_3" pad="1"/>
<connect gate="A" pin="GND_4" pad="2"/>
<connect gate="A" pin="GND_5" pad="11"/>
<connect gate="A" pin="NC" pad="9"/>
<connect gate="A" pin="NC_2" pad="15"/>
<connect gate="A" pin="NC_3" pad="22"/>
<connect gate="A" pin="NC_4" pad="24"/>
<connect gate="A" pin="NC_5" pad="3"/>
<connect gate="A" pin="SS/~SD" pad="14"/>
<connect gate="A" pin="SS/~SD_2" pad="13"/>
<connect gate="A" pin="VIN" pad="21"/>
<connect gate="A" pin="VIN_2" pad="16"/>
<connect gate="A" pin="VIN_3" pad="17"/>
<connect gate="A" pin="VIN_4" pad="18"/>
<connect gate="A" pin="VIN_5" pad="19"/>
<connect gate="A" pin="VIN_6" pad="20"/>
<connect gate="A" pin="VOUT" pad="8"/>
<connect gate="A" pin="VOUT_2" pad="4"/>
<connect gate="A" pin="VOUT_3" pad="5"/>
<connect gate="A" pin="VOUT_4" pad="6"/>
<connect gate="A" pin="VOUT_5" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2825HN-ADJ"/>
<attribute name="OC_FARNELL" value="8221987"/>
<attribute name="OC_NEWARK" value="41K4394"/>
<attribute name="PACKAGE" value="24-DIP"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2825N-12" prefix="U">
<description>DC/DC CONVERTER</description>
<gates>
<gate name="A" symbol="LM2825N-12"/>
</gates>
<devices>
<device name="" package="DIP254P1524X724-24">
<connects>
<connect gate="A" pin="ADJ" pad="10"/>
<connect gate="A" pin="GND" pad="23"/>
<connect gate="A" pin="GND_2" pad="1"/>
<connect gate="A" pin="GND_3" pad="2"/>
<connect gate="A" pin="GND_4" pad="11"/>
<connect gate="A" pin="GND_5" pad="12"/>
<connect gate="A" pin="IN" pad="21"/>
<connect gate="A" pin="IN_2" pad="16"/>
<connect gate="A" pin="IN_3" pad="17"/>
<connect gate="A" pin="IN_4" pad="18"/>
<connect gate="A" pin="IN_5" pad="19"/>
<connect gate="A" pin="IN_6" pad="20"/>
<connect gate="A" pin="NC" pad="24"/>
<connect gate="A" pin="NC_2" pad="3"/>
<connect gate="A" pin="NC_3" pad="15"/>
<connect gate="A" pin="NC_4" pad="9"/>
<connect gate="A" pin="NC_5" pad="22"/>
<connect gate="A" pin="OUT" pad="8"/>
<connect gate="A" pin="OUT_2" pad="4"/>
<connect gate="A" pin="OUT_3" pad="5"/>
<connect gate="A" pin="OUT_4" pad="6"/>
<connect gate="A" pin="OUT_5" pad="7"/>
<connect gate="A" pin="~SD/SOFT_START" pad="13"/>
<connect gate="A" pin="~SD/SOFT_START_2" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2825N-12/NOPB"/>
<attribute name="OC_FARNELL" value="9486305"/>
<attribute name="OC_NEWARK" value="97K3296"/>
<attribute name="PACKAGE" value="24-DIP"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2825N-3.3" prefix="U">
<description>DC-DC converter</description>
<gates>
<gate name="A" symbol="LM2825N-3.3"/>
</gates>
<devices>
<device name="" package="DIP254P1524X724-24">
<connects>
<connect gate="A" pin="ADJ" pad="10"/>
<connect gate="A" pin="GND" pad="23"/>
<connect gate="A" pin="GND_2" pad="1"/>
<connect gate="A" pin="GND_3" pad="2"/>
<connect gate="A" pin="GND_4" pad="11"/>
<connect gate="A" pin="GND_5" pad="12"/>
<connect gate="A" pin="IN" pad="21"/>
<connect gate="A" pin="IN_2" pad="16"/>
<connect gate="A" pin="IN_3" pad="17"/>
<connect gate="A" pin="IN_4" pad="18"/>
<connect gate="A" pin="IN_5" pad="19"/>
<connect gate="A" pin="IN_6" pad="20"/>
<connect gate="A" pin="NC" pad="24"/>
<connect gate="A" pin="NC_2" pad="3"/>
<connect gate="A" pin="NC_3" pad="9"/>
<connect gate="A" pin="NC_4" pad="22"/>
<connect gate="A" pin="NC_5" pad="15"/>
<connect gate="A" pin="OUT" pad="8"/>
<connect gate="A" pin="OUT_2" pad="4"/>
<connect gate="A" pin="OUT_3" pad="5"/>
<connect gate="A" pin="OUT_4" pad="6"/>
<connect gate="A" pin="OUT_5" pad="7"/>
<connect gate="A" pin="~SD/SOFT" pad="14"/>
<connect gate="A" pin="~SD/SOFT_2" pad="13"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2825N-3.3"/>
<attribute name="OC_FARNELL" value="9493891"/>
<attribute name="OC_NEWARK" value="38K3690"/>
<attribute name="PACKAGE" value="24-DIP"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2825N-5.0" prefix="U">
<description>DC-DC converter</description>
<gates>
<gate name="A" symbol="LM2825N-5.0"/>
</gates>
<devices>
<device name="" package="DIP254P1524X724-24">
<connects>
<connect gate="A" pin="ADJ" pad="10"/>
<connect gate="A" pin="GND" pad="23"/>
<connect gate="A" pin="GND_2" pad="1"/>
<connect gate="A" pin="GND_3" pad="2"/>
<connect gate="A" pin="GND_4" pad="11"/>
<connect gate="A" pin="GND_5" pad="12"/>
<connect gate="A" pin="IN" pad="21"/>
<connect gate="A" pin="IN_2" pad="16"/>
<connect gate="A" pin="IN_3" pad="17"/>
<connect gate="A" pin="IN_4" pad="18"/>
<connect gate="A" pin="IN_5" pad="19"/>
<connect gate="A" pin="IN_6" pad="20"/>
<connect gate="A" pin="NC" pad="24"/>
<connect gate="A" pin="NC_2" pad="3"/>
<connect gate="A" pin="NC_3" pad="9"/>
<connect gate="A" pin="NC_4" pad="22"/>
<connect gate="A" pin="NC_5" pad="15"/>
<connect gate="A" pin="OUT" pad="8"/>
<connect gate="A" pin="OUT_2" pad="4"/>
<connect gate="A" pin="OUT_3" pad="5"/>
<connect gate="A" pin="OUT_4" pad="6"/>
<connect gate="A" pin="OUT_5" pad="7"/>
<connect gate="A" pin="~SD/SOFT" pad="14"/>
<connect gate="A" pin="~SD/SOFT_2" pad="13"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2825N-5.0"/>
<attribute name="OC_FARNELL" value="9493883"/>
<attribute name="OC_NEWARK" value="41K4398"/>
<attribute name="PACKAGE" value="24-DIP"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2825N-ADJ" prefix="U">
<description>DC-DC converter</description>
<gates>
<gate name="A" symbol="LM2825N-ADJ"/>
</gates>
<devices>
<device name="" package="DIP254P1524X724-24">
<connects>
<connect gate="A" pin="ADJ" pad="10"/>
<connect gate="A" pin="GND" pad="23"/>
<connect gate="A" pin="GND_2" pad="1"/>
<connect gate="A" pin="GND_3" pad="2"/>
<connect gate="A" pin="GND_4" pad="11"/>
<connect gate="A" pin="GND_5" pad="12"/>
<connect gate="A" pin="IN" pad="21"/>
<connect gate="A" pin="IN_2" pad="16"/>
<connect gate="A" pin="IN_3" pad="17"/>
<connect gate="A" pin="IN_4" pad="18"/>
<connect gate="A" pin="IN_5" pad="19"/>
<connect gate="A" pin="IN_6" pad="20"/>
<connect gate="A" pin="NC" pad="24"/>
<connect gate="A" pin="NC_2" pad="3"/>
<connect gate="A" pin="NC_3" pad="9"/>
<connect gate="A" pin="NC_4" pad="22"/>
<connect gate="A" pin="NC_5" pad="15"/>
<connect gate="A" pin="OUT" pad="8"/>
<connect gate="A" pin="OUT_2" pad="4"/>
<connect gate="A" pin="OUT_3" pad="5"/>
<connect gate="A" pin="OUT_4" pad="6"/>
<connect gate="A" pin="OUT_5" pad="7"/>
<connect gate="A" pin="~SD/SOFT" pad="14"/>
<connect gate="A" pin="~SD/SOFT_2" pad="13"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2825N-ADJ"/>
<attribute name="OC_FARNELL" value="9486313"/>
<attribute name="OC_NEWARK" value="97K3295"/>
<attribute name="PACKAGE" value="24-DIP"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2830XMF" prefix="U">
<description>Load - Step-Down DC-DC Regulator</description>
<gates>
<gate name="A" symbol="LM2830XMF"/>
</gates>
<devices>
<device name="" package="SOT95P285X120-5N">
<connects>
<connect gate="A" pin="EN" pad="4"/>
<connect gate="A" pin="FB" pad="3"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="SW" pad="1"/>
<connect gate="A" pin="VIN" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2830XMF"/>
<attribute name="OC_FARNELL" value="1286715"/>
<attribute name="OC_NEWARK" value="13M1721"/>
<attribute name="PACKAGE" value="SOT-23-5"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2831XMF" prefix="U">
<description>IC BUCK ADJ 1.5A</description>
<gates>
<gate name="A" symbol="LM2831XMF"/>
</gates>
<devices>
<device name="" package="SOT95P285X122-5N">
<connects>
<connect gate="A" pin="EN" pad="4"/>
<connect gate="A" pin="FB" pad="3"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="SW" pad="1"/>
<connect gate="A" pin="VIN" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2831XMF"/>
<attribute name="OC_FARNELL" value="1654260"/>
<attribute name="OC_NEWARK" value="13M1734"/>
<attribute name="PACKAGE" value="SOT23-5"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2831XSD" prefix="U">
<description>IC REGULATOR BUCK 1.5A</description>
<gates>
<gate name="A" symbol="LM2831XSD"/>
</gates>
<devices>
<device name="" package="DFN300X300X80-7N">
<connects>
<connect gate="A" pin="EN" pad="6"/>
<connect gate="A" pin="EP" pad="7"/>
<connect gate="A" pin="FB" pad="1"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="SW" pad="3"/>
<connect gate="A" pin="VINA" pad="5"/>
<connect gate="A" pin="VIND" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2831XSD"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="13M1738"/>
<attribute name="PACKAGE" value="6-WDFN Exposed Pad"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2831YMF" prefix="U">
<description>IC BUCK ADJ 1.5A</description>
<gates>
<gate name="A" symbol="LM2831YMF"/>
</gates>
<devices>
<device name="" package="SOT95P285X122-5N">
<connects>
<connect gate="A" pin="EN" pad="4"/>
<connect gate="A" pin="FB" pad="3"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="SW" pad="1"/>
<connect gate="A" pin="VIN" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2831YMF"/>
<attribute name="OC_FARNELL" value="1286714"/>
<attribute name="OC_NEWARK" value="13M1742"/>
<attribute name="PACKAGE" value="SOT23-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2831YSD" prefix="U">
<description>IC REGULATOR BUCK 1.5A</description>
<gates>
<gate name="A" symbol="LM2831YSD"/>
</gates>
<devices>
<device name="" package="DFN300X300X80-7N">
<connects>
<connect gate="A" pin="EN" pad="6"/>
<connect gate="A" pin="EP" pad="7"/>
<connect gate="A" pin="FB" pad="1"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="SW" pad="3"/>
<connect gate="A" pin="VINA" pad="5"/>
<connect gate="A" pin="VIND" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2831YSD"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="13M1746"/>
<attribute name="PACKAGE" value="6-WDFN Exposed Pad"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2831ZMF" prefix="U">
<description>Load - Step-Down DC-DC Regulator</description>
<gates>
<gate name="A" symbol="LM2831ZMF"/>
</gates>
<devices>
<device name="" package="SOT95P285X120-5N">
<connects>
<connect gate="A" pin="EN" pad="4"/>
<connect gate="A" pin="FB" pad="3"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="SW" pad="1"/>
<connect gate="A" pin="VIN" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2831ZMF"/>
<attribute name="OC_FARNELL" value="1271413"/>
<attribute name="OC_NEWARK" value="13M1750"/>
<attribute name="PACKAGE" value="SOT-23-5"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2831ZSD" prefix="U">
<description>IC REGULATOR BUCK 1.5A</description>
<gates>
<gate name="A" symbol="LM2831ZSD"/>
</gates>
<devices>
<device name="" package="DFN300X300X80-7N">
<connects>
<connect gate="A" pin="EN" pad="6"/>
<connect gate="A" pin="EP" pad="7"/>
<connect gate="A" pin="FB" pad="1"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="SW" pad="3"/>
<connect gate="A" pin="VINA" pad="5"/>
<connect gate="A" pin="VIND" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2831ZSD"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="13M1754"/>
<attribute name="PACKAGE" value="6-WDFN Exposed Pad"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2832XMY" prefix="U">
<description>Step-Down DC-DC Regulator</description>
<gates>
<gate name="A" symbol="LM2832XMY"/>
</gates>
<devices>
<device name="" package="SOP65P490X110-9N">
<connects>
<connect gate="A" pin="EN" pad="4"/>
<connect gate="A" pin="EPAD" pad="9"/>
<connect gate="A" pin="FB" pad="6"/>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="GND_2" pad="7"/>
<connect gate="A" pin="GND_3" pad="3"/>
<connect gate="A" pin="SW" pad="8"/>
<connect gate="A" pin="VINA" pad="2"/>
<connect gate="A" pin="VIND" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2832XMY"/>
<attribute name="OC_FARNELL" value="1271414"/>
<attribute name="OC_NEWARK" value="13M1758"/>
<attribute name="PACKAGE" value="MSOP-8"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2832XSD" prefix="U">
<description>IC REGULATOR BUCK 2A</description>
<gates>
<gate name="A" symbol="LM2832XSD"/>
</gates>
<devices>
<device name="" package="DFN300X300X80-7N">
<connects>
<connect gate="A" pin="EN" pad="6"/>
<connect gate="A" pin="EP" pad="7"/>
<connect gate="A" pin="FB" pad="1"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="SW" pad="3"/>
<connect gate="A" pin="VINA" pad="5"/>
<connect gate="A" pin="VIND" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2832XSD"/>
<attribute name="OC_FARNELL" value="1685577"/>
<attribute name="OC_NEWARK" value="13M1763"/>
<attribute name="PACKAGE" value="6-WDFN Exposed Pad"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2832YMY" prefix="U">
<description>IC REGULATOR BUCK 2A</description>
<gates>
<gate name="A" symbol="LM2832YMY"/>
</gates>
<devices>
<device name="" package="SOP65P490X109-9N">
<connects>
<connect gate="A" pin="EN" pad="4"/>
<connect gate="A" pin="EP" pad="9"/>
<connect gate="A" pin="FB" pad="6"/>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="GND_2" pad="3"/>
<connect gate="A" pin="GND_3" pad="5"/>
<connect gate="A" pin="SW" pad="8"/>
<connect gate="A" pin="VINA" pad="2"/>
<connect gate="A" pin="VIND" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2832YMY"/>
<attribute name="OC_FARNELL" value="1654262"/>
<attribute name="OC_NEWARK" value="13M1767"/>
<attribute name="PACKAGE" value="8-MSOP-EP"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2832YSD" prefix="U">
<description>IC REGULATOR BUCK 2A</description>
<gates>
<gate name="A" symbol="LM2832YSD"/>
</gates>
<devices>
<device name="" package="DFN300X300X80-7N">
<connects>
<connect gate="A" pin="EN" pad="6"/>
<connect gate="A" pin="EP" pad="7"/>
<connect gate="A" pin="FB" pad="1"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="SW" pad="3"/>
<connect gate="A" pin="VINA" pad="5"/>
<connect gate="A" pin="VIND" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2832YSD"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="13M1771"/>
<attribute name="PACKAGE" value="6-WDFN Exposed Pad"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2832ZMY" prefix="U">
<description>IC REGULATOR BUCK 2A</description>
<gates>
<gate name="A" symbol="LM2832ZMY"/>
</gates>
<devices>
<device name="" package="SOP65P490X109-9N">
<connects>
<connect gate="A" pin="EN" pad="4"/>
<connect gate="A" pin="EP" pad="9"/>
<connect gate="A" pin="FB" pad="6"/>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="GND_2" pad="3"/>
<connect gate="A" pin="GND_3" pad="5"/>
<connect gate="A" pin="SW" pad="8"/>
<connect gate="A" pin="VINA" pad="2"/>
<connect gate="A" pin="VIND" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2832ZMY"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="32M1017"/>
<attribute name="PACKAGE" value="8-MSOP-EP"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2833XMY">
<description>IC REG SW DC-DC 1.5MHZ</description>
<gates>
<gate name="A" symbol="LM2833XMY"/>
</gates>
<devices>
<device name="" package="SOP50P490X109-11N">
<connects>
<connect gate="A" pin="EN" pad="2"/>
<connect gate="A" pin="EP" pad="11"/>
<connect gate="A" pin="FB" pad="5"/>
<connect gate="A" pin="NC" pad="4"/>
<connect gate="A" pin="PGND" pad="6"/>
<connect gate="A" pin="SGND" pad="3"/>
<connect gate="A" pin="SW" pad="8"/>
<connect gate="A" pin="SW_2" pad="7"/>
<connect gate="A" pin="VINC" pad="1"/>
<connect gate="A" pin="VIND" pad="10"/>
<connect gate="A" pin="VIND_2" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2833XMY"/>
<attribute name="OC_FARNELL" value="1699382"/>
<attribute name="OC_NEWARK" value="04R9162"/>
<attribute name="PACKAGE" value="MSOP-10"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2833XSD">
<description>Step-Down DC-DC Switching Regulator</description>
<gates>
<gate name="A" symbol="LM2833XSD"/>
</gates>
<devices>
<device name="" package="DFN300X300X80-11N">
<connects>
<connect gate="A" pin="EN" pad="2"/>
<connect gate="A" pin="EP" pad="11"/>
<connect gate="A" pin="FB" pad="5"/>
<connect gate="A" pin="NC" pad="4"/>
<connect gate="A" pin="PGND" pad="6"/>
<connect gate="A" pin="SGND" pad="3"/>
<connect gate="A" pin="SW" pad="8"/>
<connect gate="A" pin="SW_2" pad="7"/>
<connect gate="A" pin="VINC" pad="1"/>
<connect gate="A" pin="VIND" pad="10"/>
<connect gate="A" pin="VIND_2" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2833XSD"/>
<attribute name="OC_FARNELL" value="1699383"/>
<attribute name="OC_NEWARK" value="07P5416"/>
<attribute name="PACKAGE" value="DFN-10"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2833ZMY">
<description>Step-Down DC-DC Switching Regulator</description>
<gates>
<gate name="A" symbol="LM2833ZMY"/>
</gates>
<devices>
<device name="" package="SOP50P490X110-11N">
<connects>
<connect gate="A" pin="EN" pad="2"/>
<connect gate="A" pin="EP" pad="11"/>
<connect gate="A" pin="FB" pad="5"/>
<connect gate="A" pin="NC" pad="4"/>
<connect gate="A" pin="PGND" pad="6"/>
<connect gate="A" pin="SGND" pad="3"/>
<connect gate="A" pin="SW" pad="8"/>
<connect gate="A" pin="SW_2" pad="7"/>
<connect gate="A" pin="VINC" pad="1"/>
<connect gate="A" pin="VIND" pad="10"/>
<connect gate="A" pin="VIND_2" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2833ZMY"/>
<attribute name="OC_FARNELL" value="1699384"/>
<attribute name="OC_NEWARK" value="56P4150"/>
<attribute name="PACKAGE" value="DFN-10"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2833ZSD">
<description>Step-Down DC-DC Switching Regulator</description>
<gates>
<gate name="A" symbol="LM2833ZSD"/>
</gates>
<devices>
<device name="" package="DFN300X300X80-11N">
<connects>
<connect gate="A" pin="EN" pad="2"/>
<connect gate="A" pin="EP" pad="11"/>
<connect gate="A" pin="FB" pad="5"/>
<connect gate="A" pin="NC" pad="4"/>
<connect gate="A" pin="PGND" pad="6"/>
<connect gate="A" pin="SGND" pad="3"/>
<connect gate="A" pin="SW" pad="8"/>
<connect gate="A" pin="SW_2" pad="7"/>
<connect gate="A" pin="VINC" pad="1"/>
<connect gate="A" pin="VIND" pad="10"/>
<connect gate="A" pin="VIND_2" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2833ZSD"/>
<attribute name="OC_FARNELL" value="1699385"/>
<attribute name="OC_NEWARK" value="56P4151"/>
<attribute name="PACKAGE" value="DFN-10"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2841XMK-ADJL" prefix="U">
<description>IC BUCK ADJ 0.3A</description>
<gates>
<gate name="A" symbol="LM2841XMK-ADJL"/>
</gates>
<devices>
<device name="" package="SOT95P285X100-6N">
<connects>
<connect gate="A" pin="*SHDN" pad="4"/>
<connect gate="A" pin="CB" pad="1"/>
<connect gate="A" pin="FB" pad="3"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="SW" pad="6"/>
<connect gate="A" pin="VIN" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2841XMK-ADJL"/>
<attribute name="OC_FARNELL" value="1714819"/>
<attribute name="OC_NEWARK" value="10R2189"/>
<attribute name="PACKAGE" value="TSOT23-6"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2841YMK-ADJL" prefix="U">
<description>IC BUCK ADJ 0.3A</description>
<gates>
<gate name="A" symbol="LM2841YMK-ADJL"/>
</gates>
<devices>
<device name="" package="SOT95P285X100-6N">
<connects>
<connect gate="A" pin="*SHDN" pad="4"/>
<connect gate="A" pin="CB" pad="1"/>
<connect gate="A" pin="FB" pad="3"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="SW" pad="6"/>
<connect gate="A" pin="VIN" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2841YMK-ADJL"/>
<attribute name="OC_FARNELL" value="1714821"/>
<attribute name="OC_NEWARK" value="10R2190"/>
<attribute name="PACKAGE" value="TSOT23-6"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2842XMK-ADJL" prefix="U">
<description>IC BUCK ADJ 0.6A</description>
<gates>
<gate name="A" symbol="LM2842XMK-ADJL"/>
</gates>
<devices>
<device name="" package="SOT95P285X100-6N">
<connects>
<connect gate="A" pin="*SHDN" pad="4"/>
<connect gate="A" pin="CB" pad="1"/>
<connect gate="A" pin="FB" pad="3"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="SW" pad="6"/>
<connect gate="A" pin="VIN" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2842XMK-ADJL"/>
<attribute name="OC_FARNELL" value="1714822"/>
<attribute name="OC_NEWARK" value="10R2191"/>
<attribute name="PACKAGE" value="TSOT23-6"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2842YMK-ADJL" prefix="U">
<description>IC BUCK ADJ 0.6A</description>
<gates>
<gate name="A" symbol="LM2842YMK-ADJL"/>
</gates>
<devices>
<device name="" package="SOT95P285X100-6N">
<connects>
<connect gate="A" pin="*SHDN" pad="4"/>
<connect gate="A" pin="CB" pad="1"/>
<connect gate="A" pin="FB" pad="3"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="SW" pad="6"/>
<connect gate="A" pin="VIN" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2842YMK-ADJL"/>
<attribute name="OC_FARNELL" value="1714823"/>
<attribute name="OC_NEWARK" value="10R2192"/>
<attribute name="PACKAGE" value="TSOT23-6"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2852XMXA-0.8" prefix="U">
<description>IC REG SYNC BUCK 2A</description>
<gates>
<gate name="A" symbol="LM2852XMXA-0.8"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-15N">
<connects>
<connect gate="A" pin="AVIN" pad="1"/>
<connect gate="A" pin="EN" pad="2"/>
<connect gate="A" pin="EP" pad="15"/>
<connect gate="A" pin="NC" pad="13"/>
<connect gate="A" pin="NC_2" pad="5"/>
<connect gate="A" pin="NC_3" pad="12"/>
<connect gate="A" pin="PGND" pad="11"/>
<connect gate="A" pin="PGND_2" pad="10"/>
<connect gate="A" pin="PVIN" pad="7"/>
<connect gate="A" pin="PVIN_2" pad="6"/>
<connect gate="A" pin="SGND" pad="3"/>
<connect gate="A" pin="SNS" pad="14"/>
<connect gate="A" pin="SS" pad="4"/>
<connect gate="A" pin="SW" pad="9"/>
<connect gate="A" pin="SW_2" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2852XMXA-0.8"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="57K7392"/>
<attribute name="PACKAGE" value="14-TSSOP"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2852XMXA-1.0" prefix="U">
<description>IC REG SYNC BUCK 2A</description>
<gates>
<gate name="A" symbol="LM2852XMXA-1.0"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-15N">
<connects>
<connect gate="A" pin="AVIN" pad="1"/>
<connect gate="A" pin="EN" pad="2"/>
<connect gate="A" pin="EP" pad="15"/>
<connect gate="A" pin="NC" pad="13"/>
<connect gate="A" pin="NC_2" pad="5"/>
<connect gate="A" pin="NC_3" pad="12"/>
<connect gate="A" pin="PGND" pad="11"/>
<connect gate="A" pin="PGND_2" pad="10"/>
<connect gate="A" pin="PVIN" pad="7"/>
<connect gate="A" pin="PVIN_2" pad="6"/>
<connect gate="A" pin="SGND" pad="3"/>
<connect gate="A" pin="SNS" pad="14"/>
<connect gate="A" pin="SS" pad="4"/>
<connect gate="A" pin="SW" pad="9"/>
<connect gate="A" pin="SW_2" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2852XMXA-1.0"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="65K5967"/>
<attribute name="PACKAGE" value="14-TSSOP"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2852XMXA-1.2" prefix="U">
<description>IC REG SYNC BUCK 2A</description>
<gates>
<gate name="A" symbol="LM2852XMXA-1.2"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-15N">
<connects>
<connect gate="A" pin="AVIN" pad="1"/>
<connect gate="A" pin="EN" pad="2"/>
<connect gate="A" pin="EP" pad="15"/>
<connect gate="A" pin="NC" pad="13"/>
<connect gate="A" pin="NC_2" pad="5"/>
<connect gate="A" pin="NC_3" pad="12"/>
<connect gate="A" pin="PGND" pad="11"/>
<connect gate="A" pin="PGND_2" pad="10"/>
<connect gate="A" pin="PVIN" pad="7"/>
<connect gate="A" pin="PVIN_2" pad="6"/>
<connect gate="A" pin="SGND" pad="3"/>
<connect gate="A" pin="SNS" pad="14"/>
<connect gate="A" pin="SS" pad="4"/>
<connect gate="A" pin="SW" pad="9"/>
<connect gate="A" pin="SW_2" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2852XMXA-1.2"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="57K7394"/>
<attribute name="PACKAGE" value="14-TSSOP"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2852XMXA-1.5" prefix="U">
<description>IC REG SYNC BUCK 2A</description>
<gates>
<gate name="A" symbol="LM2852XMXA-1.5"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-15N">
<connects>
<connect gate="A" pin="AVIN" pad="1"/>
<connect gate="A" pin="EN" pad="2"/>
<connect gate="A" pin="EP" pad="15"/>
<connect gate="A" pin="NC" pad="13"/>
<connect gate="A" pin="NC_2" pad="5"/>
<connect gate="A" pin="NC_3" pad="12"/>
<connect gate="A" pin="PGND" pad="11"/>
<connect gate="A" pin="PGND_2" pad="10"/>
<connect gate="A" pin="PVIN" pad="7"/>
<connect gate="A" pin="PVIN_2" pad="6"/>
<connect gate="A" pin="SGND" pad="3"/>
<connect gate="A" pin="SNS" pad="14"/>
<connect gate="A" pin="SS" pad="4"/>
<connect gate="A" pin="SW" pad="9"/>
<connect gate="A" pin="SW_2" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2852XMXA-1.5"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="65K5969"/>
<attribute name="PACKAGE" value="14-TSSOP"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2852XMXA-1.8" prefix="U">
<description>IC REG SYNC BUCK 2A</description>
<gates>
<gate name="A" symbol="LM2852XMXA-1.8"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-15N">
<connects>
<connect gate="A" pin="AVIN" pad="1"/>
<connect gate="A" pin="EN" pad="2"/>
<connect gate="A" pin="EP" pad="15"/>
<connect gate="A" pin="NC" pad="13"/>
<connect gate="A" pin="NC_2" pad="5"/>
<connect gate="A" pin="NC_3" pad="12"/>
<connect gate="A" pin="PGND" pad="11"/>
<connect gate="A" pin="PGND_2" pad="10"/>
<connect gate="A" pin="PVIN" pad="7"/>
<connect gate="A" pin="PVIN_2" pad="6"/>
<connect gate="A" pin="SGND" pad="3"/>
<connect gate="A" pin="SNS" pad="14"/>
<connect gate="A" pin="SS" pad="4"/>
<connect gate="A" pin="SW" pad="9"/>
<connect gate="A" pin="SW_2" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2852XMXA-1.8"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="65K5970"/>
<attribute name="PACKAGE" value="14-TSSOP"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2852XMXA-2.5" prefix="U">
<description>IC REG SYNC BUCK 2A</description>
<gates>
<gate name="A" symbol="LM2852XMXA-2.5"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-15N">
<connects>
<connect gate="A" pin="AVIN" pad="1"/>
<connect gate="A" pin="EN" pad="2"/>
<connect gate="A" pin="EP" pad="15"/>
<connect gate="A" pin="NC" pad="13"/>
<connect gate="A" pin="NC_2" pad="5"/>
<connect gate="A" pin="NC_3" pad="12"/>
<connect gate="A" pin="PGND" pad="11"/>
<connect gate="A" pin="PGND_2" pad="10"/>
<connect gate="A" pin="PVIN" pad="7"/>
<connect gate="A" pin="PVIN_2" pad="6"/>
<connect gate="A" pin="SGND" pad="3"/>
<connect gate="A" pin="SNS" pad="14"/>
<connect gate="A" pin="SS" pad="4"/>
<connect gate="A" pin="SW" pad="9"/>
<connect gate="A" pin="SW_2" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2852XMXA-2.5"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="65K5971"/>
<attribute name="PACKAGE" value="14-TSSOP"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2852XMXA-3.0" prefix="U">
<description>IC REG SYNC BUCK 2A</description>
<gates>
<gate name="A" symbol="LM2852XMXA-3.0"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-15N">
<connects>
<connect gate="A" pin="AVIN" pad="1"/>
<connect gate="A" pin="EN" pad="2"/>
<connect gate="A" pin="EP" pad="15"/>
<connect gate="A" pin="NC" pad="13"/>
<connect gate="A" pin="NC_2" pad="5"/>
<connect gate="A" pin="NC_3" pad="12"/>
<connect gate="A" pin="PGND" pad="11"/>
<connect gate="A" pin="PGND_2" pad="10"/>
<connect gate="A" pin="PVIN" pad="7"/>
<connect gate="A" pin="PVIN_2" pad="6"/>
<connect gate="A" pin="SGND" pad="3"/>
<connect gate="A" pin="SNS" pad="14"/>
<connect gate="A" pin="SS" pad="4"/>
<connect gate="A" pin="SW" pad="9"/>
<connect gate="A" pin="SW_2" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2852XMXA-3.0"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="57K7398"/>
<attribute name="PACKAGE" value="14-TSSOP"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2852XMXA-3.3" prefix="U">
<description>IC REG SYNC BUCK 2A</description>
<gates>
<gate name="A" symbol="LM2852XMXA-3.3"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-15N">
<connects>
<connect gate="A" pin="AVIN" pad="1"/>
<connect gate="A" pin="EN" pad="2"/>
<connect gate="A" pin="EP" pad="15"/>
<connect gate="A" pin="NC" pad="13"/>
<connect gate="A" pin="NC_2" pad="5"/>
<connect gate="A" pin="NC_3" pad="12"/>
<connect gate="A" pin="PGND" pad="11"/>
<connect gate="A" pin="PGND_2" pad="10"/>
<connect gate="A" pin="PVIN" pad="7"/>
<connect gate="A" pin="PVIN_2" pad="6"/>
<connect gate="A" pin="SGND" pad="3"/>
<connect gate="A" pin="SNS" pad="14"/>
<connect gate="A" pin="SS" pad="4"/>
<connect gate="A" pin="SW" pad="9"/>
<connect gate="A" pin="SW_2" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2852XMXA-3.3"/>
<attribute name="OC_FARNELL" value="1559753"/>
<attribute name="OC_NEWARK" value="65K5973"/>
<attribute name="PACKAGE" value="14-TSSOP"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2852YMXA-1.0" prefix="U">
<description>IC REG SYNC BUCK 2A 1.0V</description>
<gates>
<gate name="A" symbol="LM2852YMXA-1.0"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-15N">
<connects>
<connect gate="A" pin="AVIN" pad="1"/>
<connect gate="A" pin="EN" pad="2"/>
<connect gate="A" pin="EP" pad="15"/>
<connect gate="A" pin="NC" pad="13"/>
<connect gate="A" pin="NC_2" pad="5"/>
<connect gate="A" pin="NC_3" pad="12"/>
<connect gate="A" pin="PGND" pad="11"/>
<connect gate="A" pin="PGND_2" pad="10"/>
<connect gate="A" pin="PVIN" pad="7"/>
<connect gate="A" pin="PVIN_2" pad="6"/>
<connect gate="A" pin="SGND" pad="3"/>
<connect gate="A" pin="SNS" pad="14"/>
<connect gate="A" pin="SS" pad="4"/>
<connect gate="A" pin="SW" pad="9"/>
<connect gate="A" pin="SW_2" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2852YMXA-1.0"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K4425"/>
<attribute name="PACKAGE" value="14-TSSOP"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2852YMXA-1.2" prefix="U">
<description>IC REG SYNC BUCK 2A 1.2V</description>
<gates>
<gate name="A" symbol="LM2852YMXA-1.2"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-15N">
<connects>
<connect gate="A" pin="AVIN" pad="1"/>
<connect gate="A" pin="EN" pad="2"/>
<connect gate="A" pin="EP" pad="15"/>
<connect gate="A" pin="NC" pad="13"/>
<connect gate="A" pin="NC_2" pad="5"/>
<connect gate="A" pin="NC_3" pad="12"/>
<connect gate="A" pin="PGND" pad="11"/>
<connect gate="A" pin="PGND_2" pad="10"/>
<connect gate="A" pin="PVIN" pad="7"/>
<connect gate="A" pin="PVIN_2" pad="6"/>
<connect gate="A" pin="SGND" pad="3"/>
<connect gate="A" pin="SNS" pad="14"/>
<connect gate="A" pin="SS" pad="4"/>
<connect gate="A" pin="SW" pad="9"/>
<connect gate="A" pin="SW_2" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2852YMXA-1.2"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K4426"/>
<attribute name="PACKAGE" value="14-TSSOP"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2852YMXA-1.3" prefix="U">
<description>IC REG SYNC BUCK 2A 1.3V</description>
<gates>
<gate name="A" symbol="LM2852YMXA-1.3"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-15N">
<connects>
<connect gate="A" pin="AVIN" pad="1"/>
<connect gate="A" pin="EN" pad="2"/>
<connect gate="A" pin="EP" pad="15"/>
<connect gate="A" pin="NC" pad="13"/>
<connect gate="A" pin="NC_2" pad="5"/>
<connect gate="A" pin="NC_3" pad="12"/>
<connect gate="A" pin="PGND" pad="11"/>
<connect gate="A" pin="PGND_2" pad="10"/>
<connect gate="A" pin="PVIN" pad="7"/>
<connect gate="A" pin="PVIN_2" pad="6"/>
<connect gate="A" pin="SGND" pad="3"/>
<connect gate="A" pin="SNS" pad="14"/>
<connect gate="A" pin="SS" pad="4"/>
<connect gate="A" pin="SW" pad="9"/>
<connect gate="A" pin="SW_2" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2852YMXA-1.3"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="79K7812"/>
<attribute name="PACKAGE" value="14-TSSOP"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2852YMXA-1.8" prefix="U">
<description>IC REG SYNC BUCK 2A 1.8V</description>
<gates>
<gate name="A" symbol="LM2852YMXA-1.8"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-15N">
<connects>
<connect gate="A" pin="AVIN" pad="1"/>
<connect gate="A" pin="EN" pad="2"/>
<connect gate="A" pin="EP" pad="15"/>
<connect gate="A" pin="NC" pad="13"/>
<connect gate="A" pin="NC_2" pad="5"/>
<connect gate="A" pin="NC_3" pad="12"/>
<connect gate="A" pin="PGND" pad="11"/>
<connect gate="A" pin="PGND_2" pad="10"/>
<connect gate="A" pin="PVIN" pad="7"/>
<connect gate="A" pin="PVIN_2" pad="6"/>
<connect gate="A" pin="SGND" pad="3"/>
<connect gate="A" pin="SNS" pad="14"/>
<connect gate="A" pin="SS" pad="4"/>
<connect gate="A" pin="SW" pad="9"/>
<connect gate="A" pin="SW_2" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2852YMXA-1.8"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K4428"/>
<attribute name="PACKAGE" value="14-TSSOP"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2852YMXA-2.5" prefix="U">
<description>IC REG SYNC BUCK 2A 2.5V</description>
<gates>
<gate name="A" symbol="LM2852YMXA-2.5"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-15N">
<connects>
<connect gate="A" pin="AVIN" pad="1"/>
<connect gate="A" pin="EN" pad="2"/>
<connect gate="A" pin="EP" pad="15"/>
<connect gate="A" pin="NC" pad="13"/>
<connect gate="A" pin="NC_2" pad="5"/>
<connect gate="A" pin="NC_3" pad="12"/>
<connect gate="A" pin="PGND" pad="11"/>
<connect gate="A" pin="PGND_2" pad="10"/>
<connect gate="A" pin="PVIN" pad="7"/>
<connect gate="A" pin="PVIN_2" pad="6"/>
<connect gate="A" pin="SGND" pad="3"/>
<connect gate="A" pin="SNS" pad="14"/>
<connect gate="A" pin="SS" pad="4"/>
<connect gate="A" pin="SW" pad="9"/>
<connect gate="A" pin="SW_2" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2852YMXA-2.5"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K4429"/>
<attribute name="PACKAGE" value="14-TSSOP"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2852YMXA-3.0" prefix="U">
<description>IC REG SYNC BUCK 2A 3.0V</description>
<gates>
<gate name="A" symbol="LM2852YMXA-3.0"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-15N">
<connects>
<connect gate="A" pin="AVIN" pad="1"/>
<connect gate="A" pin="EN" pad="2"/>
<connect gate="A" pin="EP" pad="15"/>
<connect gate="A" pin="NC" pad="13"/>
<connect gate="A" pin="NC_2" pad="5"/>
<connect gate="A" pin="NC_3" pad="12"/>
<connect gate="A" pin="PGND" pad="11"/>
<connect gate="A" pin="PGND_2" pad="10"/>
<connect gate="A" pin="PVIN" pad="7"/>
<connect gate="A" pin="PVIN_2" pad="6"/>
<connect gate="A" pin="SGND" pad="3"/>
<connect gate="A" pin="SNS" pad="14"/>
<connect gate="A" pin="SS" pad="4"/>
<connect gate="A" pin="SW" pad="9"/>
<connect gate="A" pin="SW_2" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2852YMXA-3.0"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="32M1018"/>
<attribute name="PACKAGE" value="14-TSSOP"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2852YMXA-3.3" prefix="U">
<description>IC REG SYNC BUCK 2A 3.3V</description>
<gates>
<gate name="A" symbol="LM2852YMXA-3.3"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-15N">
<connects>
<connect gate="A" pin="AVIN" pad="1"/>
<connect gate="A" pin="EN" pad="2"/>
<connect gate="A" pin="EP" pad="15"/>
<connect gate="A" pin="NC" pad="13"/>
<connect gate="A" pin="NC_2" pad="5"/>
<connect gate="A" pin="NC_3" pad="12"/>
<connect gate="A" pin="PGND" pad="11"/>
<connect gate="A" pin="PGND_2" pad="10"/>
<connect gate="A" pin="PVIN" pad="7"/>
<connect gate="A" pin="PVIN_2" pad="6"/>
<connect gate="A" pin="SGND" pad="3"/>
<connect gate="A" pin="SNS" pad="14"/>
<connect gate="A" pin="SS" pad="4"/>
<connect gate="A" pin="SW" pad="9"/>
<connect gate="A" pin="SW_2" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2852YMXA-3.3"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K4430"/>
<attribute name="PACKAGE" value="14-TSSOP"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2853MH-0.8" prefix="U">
<description>IC REG SYNC BUCK 3A 0.8V</description>
<gates>
<gate name="A" symbol="LM2853MH-0.8"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-15N">
<connects>
<connect gate="A" pin="AVIN" pad="1"/>
<connect gate="A" pin="EN" pad="2"/>
<connect gate="A" pin="EP" pad="15"/>
<connect gate="A" pin="NC" pad="13"/>
<connect gate="A" pin="NC_2" pad="5"/>
<connect gate="A" pin="NC_3" pad="12"/>
<connect gate="A" pin="PGND" pad="11"/>
<connect gate="A" pin="PGND_2" pad="10"/>
<connect gate="A" pin="PVIN" pad="7"/>
<connect gate="A" pin="PVIN_2" pad="6"/>
<connect gate="A" pin="SGND" pad="3"/>
<connect gate="A" pin="SNS" pad="14"/>
<connect gate="A" pin="SS" pad="4"/>
<connect gate="A" pin="SW" pad="9"/>
<connect gate="A" pin="SW_2" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2853MH-0.8"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="32M1022"/>
<attribute name="PACKAGE" value="14-TSSOP"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2853MH-1.0" prefix="U">
<description>IC REG SYNC BUCK 3A 1.0V</description>
<gates>
<gate name="A" symbol="LM2853MH-1.0"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-15N">
<connects>
<connect gate="A" pin="AVIN" pad="1"/>
<connect gate="A" pin="EN" pad="2"/>
<connect gate="A" pin="EP" pad="15"/>
<connect gate="A" pin="NC" pad="13"/>
<connect gate="A" pin="NC_2" pad="5"/>
<connect gate="A" pin="NC_3" pad="12"/>
<connect gate="A" pin="PGND" pad="11"/>
<connect gate="A" pin="PGND_2" pad="10"/>
<connect gate="A" pin="PVIN" pad="7"/>
<connect gate="A" pin="PVIN_2" pad="6"/>
<connect gate="A" pin="SGND" pad="3"/>
<connect gate="A" pin="SNS" pad="14"/>
<connect gate="A" pin="SS" pad="4"/>
<connect gate="A" pin="SW" pad="9"/>
<connect gate="A" pin="SW_2" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2853MH-1.0"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="32M1023"/>
<attribute name="PACKAGE" value="14-TSSOP"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2853MH-1.2" prefix="U">
<description>IC REG SYNC BUCK 3A 1.2V</description>
<gates>
<gate name="A" symbol="LM2853MH-1.2"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-15N">
<connects>
<connect gate="A" pin="AVIN" pad="1"/>
<connect gate="A" pin="EN" pad="2"/>
<connect gate="A" pin="EP" pad="15"/>
<connect gate="A" pin="NC" pad="13"/>
<connect gate="A" pin="NC_2" pad="5"/>
<connect gate="A" pin="NC_3" pad="12"/>
<connect gate="A" pin="PGND" pad="11"/>
<connect gate="A" pin="PGND_2" pad="10"/>
<connect gate="A" pin="PVIN" pad="7"/>
<connect gate="A" pin="PVIN_2" pad="6"/>
<connect gate="A" pin="SGND" pad="3"/>
<connect gate="A" pin="SNS" pad="14"/>
<connect gate="A" pin="SS" pad="4"/>
<connect gate="A" pin="SW" pad="9"/>
<connect gate="A" pin="SW_2" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2853MH-1.2"/>
<attribute name="OC_FARNELL" value="1564776"/>
<attribute name="OC_NEWARK" value="32M1024"/>
<attribute name="PACKAGE" value="14-TSSOP"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2853MH-1.5" prefix="U">
<description>IC REG SYNC BUCK 3A 1.5V</description>
<gates>
<gate name="A" symbol="LM2853MH-1.5"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-15N">
<connects>
<connect gate="A" pin="AVIN" pad="1"/>
<connect gate="A" pin="EN" pad="2"/>
<connect gate="A" pin="EP" pad="15"/>
<connect gate="A" pin="NC" pad="13"/>
<connect gate="A" pin="NC_2" pad="5"/>
<connect gate="A" pin="NC_3" pad="12"/>
<connect gate="A" pin="PGND" pad="11"/>
<connect gate="A" pin="PGND_2" pad="10"/>
<connect gate="A" pin="PVIN" pad="7"/>
<connect gate="A" pin="PVIN_2" pad="6"/>
<connect gate="A" pin="SGND" pad="3"/>
<connect gate="A" pin="SNS" pad="14"/>
<connect gate="A" pin="SS" pad="4"/>
<connect gate="A" pin="SW" pad="9"/>
<connect gate="A" pin="SW_2" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2853MH-1.5"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="32M1025"/>
<attribute name="PACKAGE" value="14-TSSOP"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2853MH-1.8" prefix="U">
<description>IC REG SYNC BUCK 3A 1.8V</description>
<gates>
<gate name="A" symbol="LM2853MH-1.8"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-15N">
<connects>
<connect gate="A" pin="AVIN" pad="1"/>
<connect gate="A" pin="EN" pad="2"/>
<connect gate="A" pin="EP" pad="15"/>
<connect gate="A" pin="NC" pad="13"/>
<connect gate="A" pin="NC_2" pad="5"/>
<connect gate="A" pin="NC_3" pad="12"/>
<connect gate="A" pin="PGND" pad="11"/>
<connect gate="A" pin="PGND_2" pad="10"/>
<connect gate="A" pin="PVIN" pad="7"/>
<connect gate="A" pin="PVIN_2" pad="6"/>
<connect gate="A" pin="SGND" pad="3"/>
<connect gate="A" pin="SNS" pad="14"/>
<connect gate="A" pin="SS" pad="4"/>
<connect gate="A" pin="SW" pad="9"/>
<connect gate="A" pin="SW_2" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2853MH-1.8"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="32M1026"/>
<attribute name="PACKAGE" value="14-TSSOP"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2853MH-2.5" prefix="U">
<description>IC REG SYNC BUCK 3A 2.5V</description>
<gates>
<gate name="A" symbol="LM2853MH-2.5"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-15N">
<connects>
<connect gate="A" pin="AVIN" pad="1"/>
<connect gate="A" pin="EN" pad="2"/>
<connect gate="A" pin="EP" pad="15"/>
<connect gate="A" pin="NC" pad="13"/>
<connect gate="A" pin="NC_2" pad="5"/>
<connect gate="A" pin="NC_3" pad="12"/>
<connect gate="A" pin="PGND" pad="11"/>
<connect gate="A" pin="PGND_2" pad="10"/>
<connect gate="A" pin="PVIN" pad="7"/>
<connect gate="A" pin="PVIN_2" pad="6"/>
<connect gate="A" pin="SGND" pad="3"/>
<connect gate="A" pin="SNS" pad="14"/>
<connect gate="A" pin="SS" pad="4"/>
<connect gate="A" pin="SW" pad="9"/>
<connect gate="A" pin="SW_2" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2853MH-2.5"/>
<attribute name="OC_FARNELL" value="1652389"/>
<attribute name="OC_NEWARK" value="32M1027"/>
<attribute name="PACKAGE" value="14-TSSOP"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2853MH-3.0" prefix="U">
<description>IC REG SYNC BUCK 3A 3.0V</description>
<gates>
<gate name="A" symbol="LM2853MH-3.0"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-15N">
<connects>
<connect gate="A" pin="AVIN" pad="1"/>
<connect gate="A" pin="EN" pad="2"/>
<connect gate="A" pin="EP" pad="15"/>
<connect gate="A" pin="NC" pad="13"/>
<connect gate="A" pin="NC_2" pad="5"/>
<connect gate="A" pin="NC_3" pad="12"/>
<connect gate="A" pin="PGND" pad="11"/>
<connect gate="A" pin="PGND_2" pad="10"/>
<connect gate="A" pin="PVIN" pad="7"/>
<connect gate="A" pin="PVIN_2" pad="6"/>
<connect gate="A" pin="SGND" pad="3"/>
<connect gate="A" pin="SNS" pad="14"/>
<connect gate="A" pin="SS" pad="4"/>
<connect gate="A" pin="SW" pad="9"/>
<connect gate="A" pin="SW_2" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2853MH-3.0"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="32M1028"/>
<attribute name="PACKAGE" value="14-TSSOP"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2853MH-3.3" prefix="U">
<description>IC REG SYNC BUCK 3A 3.3V</description>
<gates>
<gate name="A" symbol="LM2853MH-3.3"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-15N">
<connects>
<connect gate="A" pin="AVIN" pad="1"/>
<connect gate="A" pin="EN" pad="2"/>
<connect gate="A" pin="EP" pad="15"/>
<connect gate="A" pin="NC" pad="13"/>
<connect gate="A" pin="NC_2" pad="5"/>
<connect gate="A" pin="NC_3" pad="12"/>
<connect gate="A" pin="PGND" pad="11"/>
<connect gate="A" pin="PGND_2" pad="10"/>
<connect gate="A" pin="PVIN" pad="7"/>
<connect gate="A" pin="PVIN_2" pad="6"/>
<connect gate="A" pin="SGND" pad="3"/>
<connect gate="A" pin="SNS" pad="14"/>
<connect gate="A" pin="SS" pad="4"/>
<connect gate="A" pin="SW" pad="9"/>
<connect gate="A" pin="SW_2" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2853MH-3.3"/>
<attribute name="OC_FARNELL" value="1564772"/>
<attribute name="OC_NEWARK" value="32M1029"/>
<attribute name="PACKAGE" value="14-TSSOP"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2854MH-1000" prefix="U">
<description>IC REG 4A SYNC SMPL SW</description>
<gates>
<gate name="A" symbol="LM2854MH-1000"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-17N">
<connects>
<connect gate="A" pin="AGND" pad="15"/>
<connect gate="A" pin="AVIN" pad="10"/>
<connect gate="A" pin="EN" pad="11"/>
<connect gate="A" pin="EP" pad="17"/>
<connect gate="A" pin="FB" pad="16"/>
<connect gate="A" pin="NC" pad="1"/>
<connect gate="A" pin="NC_2" pad="9"/>
<connect gate="A" pin="NC_3" pad="8"/>
<connect gate="A" pin="PGND" pad="2"/>
<connect gate="A" pin="PGND_2" pad="4"/>
<connect gate="A" pin="PGND_3" pad="3"/>
<connect gate="A" pin="PVIN" pad="7"/>
<connect gate="A" pin="PVIN_2" pad="5"/>
<connect gate="A" pin="PVIN_3" pad="6"/>
<connect gate="A" pin="SS" pad="14"/>
<connect gate="A" pin="SW" pad="13"/>
<connect gate="A" pin="SW_2" pad="12"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2854MH-1000"/>
<attribute name="OC_FARNELL" value="1685774"/>
<attribute name="OC_NEWARK" value="95M8826"/>
<attribute name="PACKAGE" value="16 ETSSOP"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2854MH-500" prefix="U">
<description>Buck Regulator</description>
<gates>
<gate name="A" symbol="LM2854MH-500"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-17N">
<connects>
<connect gate="A" pin="AGND" pad="15"/>
<connect gate="A" pin="AVIN" pad="10"/>
<connect gate="A" pin="EN" pad="11"/>
<connect gate="A" pin="EPAD" pad="17"/>
<connect gate="A" pin="FB" pad="16"/>
<connect gate="A" pin="NC" pad="1"/>
<connect gate="A" pin="NC_2" pad="9"/>
<connect gate="A" pin="NC_3" pad="8"/>
<connect gate="A" pin="PGND" pad="2"/>
<connect gate="A" pin="PGND_2" pad="3"/>
<connect gate="A" pin="PGND_3" pad="4"/>
<connect gate="A" pin="PVIN" pad="7"/>
<connect gate="A" pin="PVIN_2" pad="5"/>
<connect gate="A" pin="PVIN_3" pad="6"/>
<connect gate="A" pin="SS" pad="14"/>
<connect gate="A" pin="SW" pad="13"/>
<connect gate="A" pin="SW_2" pad="12"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2854MH-500"/>
<attribute name="OC_FARNELL" value="1589528"/>
<attribute name="OC_NEWARK" value="95M8827"/>
<attribute name="PACKAGE" value="TSSOP-16"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2901M" prefix="U">
<description>IC COMPARATOR QUAD VOLT</description>
<gates>
<gate name="A" symbol="LM2901M"/>
</gates>
<devices>
<device name="" package="SOP127P600X180-14N">
<connects>
<connect gate="A" pin="+INA_" pad="5"/>
<connect gate="A" pin="+INB" pad="7"/>
<connect gate="A" pin="+INC" pad="9"/>
<connect gate="A" pin="+IND" pad="11"/>
<connect gate="A" pin="-INA" pad="4"/>
<connect gate="A" pin="-INB" pad="6"/>
<connect gate="A" pin="-INC" pad="8"/>
<connect gate="A" pin="-IND" pad="10"/>
<connect gate="A" pin="GND" pad="12"/>
<connect gate="A" pin="OUTA" pad="2"/>
<connect gate="A" pin="OUTB" pad="1"/>
<connect gate="A" pin="OUTC" pad="14"/>
<connect gate="A" pin="OUTD" pad="13"/>
<connect gate="A" pin="VCC" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2901M"/>
<attribute name="OC_FARNELL" value="9487689"/>
<attribute name="OC_NEWARK" value="82C8132"/>
<attribute name="PACKAGE" value="14-SOP"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2901N" prefix="U">
<description>IC COMPARATOR LP</description>
<gates>
<gate name="A" symbol="LM2901N"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-14">
<connects>
<connect gate="A" pin="+INA_" pad="5"/>
<connect gate="A" pin="+INB" pad="7"/>
<connect gate="A" pin="+INC" pad="9"/>
<connect gate="A" pin="+IND" pad="11"/>
<connect gate="A" pin="-INA" pad="4"/>
<connect gate="A" pin="-INB" pad="6"/>
<connect gate="A" pin="-INC" pad="8"/>
<connect gate="A" pin="-IND" pad="10"/>
<connect gate="A" pin="GND" pad="12"/>
<connect gate="A" pin="OUTA" pad="2"/>
<connect gate="A" pin="OUTB" pad="1"/>
<connect gate="A" pin="OUTC" pad="14"/>
<connect gate="A" pin="OUTD" pad="13"/>
<connect gate="A" pin="VCC" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2901N"/>
<attribute name="OC_FARNELL" value="9487697"/>
<attribute name="OC_NEWARK" value="89K0664"/>
<attribute name="PACKAGE" value="14-DIP"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2902M" prefix="U">
<description>Low Power Quad Operational Amplifiers</description>
<gates>
<gate name="A" symbol="LM2902M"/>
</gates>
<devices>
<device name="" package="SOIC127P620X175-14N">
<connects>
<connect gate="A" pin="GND" pad="11"/>
<connect gate="A" pin="IN1+" pad="3"/>
<connect gate="A" pin="IN1-" pad="2"/>
<connect gate="A" pin="IN2+" pad="5"/>
<connect gate="A" pin="IN2-" pad="6"/>
<connect gate="A" pin="IN3+" pad="10"/>
<connect gate="A" pin="IN3-" pad="9"/>
<connect gate="A" pin="IN4+" pad="13"/>
<connect gate="A" pin="IN4-" pad="12"/>
<connect gate="A" pin="OUT1" pad="1"/>
<connect gate="A" pin="OUT2" pad="7"/>
<connect gate="A" pin="OUT3" pad="8"/>
<connect gate="A" pin="OUT4" pad="14"/>
<connect gate="A" pin="V+" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2902M"/>
<attribute name="OC_FARNELL" value="9486887"/>
<attribute name="OC_NEWARK" value="41K4443"/>
<attribute name="PACKAGE" value="14-SOIC"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2902N" prefix="U">
<description>IC OP AMP QUAD LOW POWER</description>
<gates>
<gate name="A" symbol="LM2902N"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-14">
<connects>
<connect gate="A" pin="+INA_" pad="3"/>
<connect gate="A" pin="+INB" pad="5"/>
<connect gate="A" pin="+INC" pad="10"/>
<connect gate="A" pin="+IND" pad="12"/>
<connect gate="A" pin="-INA" pad="2"/>
<connect gate="A" pin="-INB" pad="6"/>
<connect gate="A" pin="-INC" pad="9"/>
<connect gate="A" pin="-IND" pad="13"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="OUTC" pad="8"/>
<connect gate="A" pin="OUTD" pad="14"/>
<connect gate="A" pin="V+" pad="4"/>
<connect gate="A" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2902N"/>
<attribute name="OC_FARNELL" value="9486895"/>
<attribute name="OC_NEWARK" value="07B6274"/>
<attribute name="PACKAGE" value="14-DIP"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2903M" prefix="U">
<description>IC COMPARATOR DUAL DIFF</description>
<gates>
<gate name="A" symbol="LM2903M"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="+INA" pad="3"/>
<connect gate="A" pin="+INB" pad="5"/>
<connect gate="A" pin="-INA" pad="2"/>
<connect gate="A" pin="-INB" pad="6"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2903M"/>
<attribute name="OC_FARNELL" value="9487620"/>
<attribute name="OC_NEWARK" value="97K3305"/>
<attribute name="PACKAGE" value="SOIC 8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2903N" prefix="U">
<description>IC COMPARATOR DUAL VOLT</description>
<gates>
<gate name="A" symbol="LM2903N"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-8">
<connects>
<connect gate="A" pin="+INA" pad="3"/>
<connect gate="A" pin="+INB" pad="5"/>
<connect gate="A" pin="-INA" pad="2"/>
<connect gate="A" pin="-INB" pad="6"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2903N"/>
<attribute name="OC_FARNELL" value="9487638"/>
<attribute name="OC_NEWARK" value="07B6277"/>
<attribute name="PACKAGE" value="8-DIP"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2904M" prefix="U">
<description>IC, OP-AMP, 1MHZ, 0.1V/µs</description>
<gates>
<gate name="A" symbol="LM2904M"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="+INA" pad="3"/>
<connect gate="A" pin="+INB" pad="5"/>
<connect gate="A" pin="-INA" pad="2"/>
<connect gate="A" pin="-INB" pad="6"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2904M"/>
<attribute name="OC_FARNELL" value="9486860"/>
<attribute name="OC_NEWARK" value="07B6278"/>
<attribute name="PACKAGE" value="SOIC 8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2904N" prefix="U">
<description>IC OP AMP DUAL LOW PWR</description>
<gates>
<gate name="A" symbol="LM2904N"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-8">
<connects>
<connect gate="A" pin="+INA" pad="3"/>
<connect gate="A" pin="+INB" pad="5"/>
<connect gate="A" pin="-INA" pad="2"/>
<connect gate="A" pin="-INB" pad="6"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2904N"/>
<attribute name="OC_FARNELL" value="9486879"/>
<attribute name="OC_NEWARK" value="07B6280"/>
<attribute name="PACKAGE" value="8-DIP"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2931AT-5.0" prefix="U">
<description>IC, LDO VOLT REG, 5V, 0.1A</description>
<gates>
<gate name="A" symbol="LM2931AT-5.0"/>
</gates>
<devices>
<device name="" package="TO254P470X1016X2222-3P">
<connects>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="IN" pad="1"/>
<connect gate="A" pin="OUT" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2931AT-5.0"/>
<attribute name="OC_FARNELL" value="1798361"/>
<attribute name="OC_NEWARK" value="41K4480"/>
<attribute name="PACKAGE" value="TO-220"/>
<attribute name="SUPPLIER" value="NATIONAL SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2931AZ-5.0" prefix="U">
<description>IC, LDO VOLT REG, 5V, 0.1A</description>
<gates>
<gate name="A" symbol="LM2931AZ-5.0"/>
</gates>
<devices>
<device name="" package="TO127P254X495-3P">
<connects>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="IN" pad="3"/>
<connect gate="A" pin="OUT" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2931AZ-5.0"/>
<attribute name="OC_FARNELL" value="9489487"/>
<attribute name="OC_NEWARK" value="41K4481"/>
<attribute name="PACKAGE" value="TO-92"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2931CT" prefix="U">
<description>Series Low Dropout Regulators</description>
<gates>
<gate name="A" symbol="LM2931CT"/>
</gates>
<devices>
<device name="" package="TO170P1435X457-6N">
<connects>
<connect gate="A" pin="ADJ" pad="1"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="GND_2" pad="6"/>
<connect gate="A" pin="IN" pad="4"/>
<connect gate="A" pin="ON/OFF" pad="2"/>
<connect gate="A" pin="OUT" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2931CT"/>
<attribute name="OC_FARNELL" value="9489363"/>
<attribute name="OC_NEWARK" value="41K4486"/>
<attribute name="PACKAGE" value="TO220-5"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2931T-5.0" prefix="U">
<description>IC, LDO VOLT REG, 5V, 0.1A</description>
<gates>
<gate name="A" symbol="LM2931T-5.0"/>
</gates>
<devices>
<device name="" package="TO254P470X1016X2222-3P">
<connects>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="IN" pad="1"/>
<connect gate="A" pin="OUT" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2931T-5.0"/>
<attribute name="OC_FARNELL" value="9489614"/>
<attribute name="OC_NEWARK" value="41K4491"/>
<attribute name="PACKAGE" value="TO-220"/>
<attribute name="SUPPLIER" value="NATIONAL SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2931Z-5.0" prefix="U">
<description>IC, V REG LDO +5.0V, 2931, TO-92-3</description>
<gates>
<gate name="A" symbol="LM2931Z-5.0"/>
</gates>
<devices>
<device name="" package="TO127P254X495-3P">
<connects>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="IN" pad="3"/>
<connect gate="A" pin="OUT" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2931Z-5.0"/>
<attribute name="OC_FARNELL" value="9489568"/>
<attribute name="OC_NEWARK" value="97K3327"/>
<attribute name="PACKAGE" value="TO-92"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2937ES-10" prefix="U">
<description>Linear Voltage Regulator IC</description>
<gates>
<gate name="A" symbol="LM2937ES-10"/>
</gates>
<devices>
<device name="" package="TO254P1435X464-4N">
<connects>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="TAB" pad="4"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="VOUT" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2937ES-10"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K4534"/>
<attribute name="PACKAGE" value="TO-263"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2937ES-12" prefix="U">
<description>IC, LDO VOLT REG, 12V, 0.5A</description>
<gates>
<gate name="A" symbol="LM2937ES-12"/>
</gates>
<devices>
<device name="" package="TO254P1435X464-4N">
<connects>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="TAB" pad="4"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="VOUT" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2937ES-12"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="07B6318"/>
<attribute name="PACKAGE" value="TO-263"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2937ES-15" prefix="U">
<description>IC,VOLT REGULATOR,FIXED,+15V,BIPOLAR</description>
<gates>
<gate name="A" symbol="LM2937ES-15"/>
</gates>
<devices>
<device name="" package="TO254P1435X464-4N">
<connects>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="TAB" pad="4"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="VOUT" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2937ES-15"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="07B6319"/>
<attribute name="PACKAGE" value="TO-263"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2937ES-5.0" prefix="U">
<description>IC, LDO VOLT REG, 5V, 0.5A</description>
<gates>
<gate name="A" symbol="LM2937ES-5.0"/>
</gates>
<devices>
<device name="" package="TO254P1435X464-4N">
<connects>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="TAB" pad="4"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="VOUT" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2937ES-5.0"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K4539"/>
<attribute name="PACKAGE" value="TO-263"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2937ES-8.0" prefix="U">
<description>IC, LDO VOLT REG, 8V, 0.5A</description>
<gates>
<gate name="A" symbol="LM2937ES-8.0"/>
</gates>
<devices>
<device name="" package="TO254P1435X464-4N">
<connects>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="TAB" pad="4"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="VOUT" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2937ES-8.0"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K4540"/>
<attribute name="PACKAGE" value="TO-263"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2937ET-10" prefix="U">
<description>IC, LDO VOLT REG, 10V, 0.5A</description>
<gates>
<gate name="A" symbol="LM2937ET-10"/>
</gates>
<devices>
<device name="" package="TO254P482X1024X3124-3P">
<connects>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="VOUT" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2937ET-10"/>
<attribute name="OC_FARNELL" value="1564642"/>
<attribute name="OC_NEWARK" value="07B6331"/>
<attribute name="PACKAGE" value="LDO"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2937ET-12" prefix="U">
<description>IC, LDO VOLT REG, 12V, 0.5A</description>
<gates>
<gate name="A" symbol="LM2937ET-12"/>
</gates>
<devices>
<device name="" package="TO254P470X1016X2222-3P">
<connects>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="IN" pad="1"/>
<connect gate="A" pin="OUT" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2937ET-12"/>
<attribute name="OC_FARNELL" value="9493492"/>
<attribute name="OC_NEWARK" value="41K4549"/>
<attribute name="PACKAGE" value="TO-220"/>
<attribute name="SUPPLIER" value="NATIONAL SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2937ET-15" prefix="U">
<description>IC, LDO VOLT REG, 15V, 0.5A</description>
<gates>
<gate name="A" symbol="LM2937ET-15"/>
</gates>
<devices>
<device name="" package="TO254P470X1016X2222-3P">
<connects>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="IN" pad="1"/>
<connect gate="A" pin="OUT" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2937ET-15"/>
<attribute name="OC_FARNELL" value="9493506"/>
<attribute name="OC_NEWARK" value="41K4550"/>
<attribute name="PACKAGE" value="TO-220"/>
<attribute name="SUPPLIER" value="NATIONAL SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2937ET-5.0" prefix="U">
<description>IC, LDO VOLT REG, 5V, 0.5A</description>
<gates>
<gate name="A" symbol="LM2937ET-5.0"/>
</gates>
<devices>
<device name="" package="TO254P470X1016X2222-3P">
<connects>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="IN" pad="1"/>
<connect gate="A" pin="OUT" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2937ET-5.0"/>
<attribute name="OC_FARNELL" value="9486038"/>
<attribute name="OC_NEWARK" value="41K4553"/>
<attribute name="PACKAGE" value="TO-220"/>
<attribute name="SUPPLIER" value="NATIONAL SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2937ET-8.0" prefix="U">
<description>IC, LDO VOLT REG, 8V, 0.5A</description>
<gates>
<gate name="A" symbol="LM2937ET-8.0"/>
</gates>
<devices>
<device name="" package="TO254P470X1016X2222-3P">
<connects>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="IN" pad="1"/>
<connect gate="A" pin="OUT" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2937ET-8.0"/>
<attribute name="OC_FARNELL" value="1694530"/>
<attribute name="OC_NEWARK" value="41K4554"/>
<attribute name="PACKAGE" value="TO-220"/>
<attribute name="SUPPLIER" value="NATIONAL SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2937IMP-10" prefix="U">
<description>IC, LDO VOLT REG, 10V, 0.5A</description>
<gates>
<gate name="A" symbol="LM2937IMP-10"/>
</gates>
<devices>
<device name="" package="SOT230P700X180-4N">
<connects>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="GND_(TAB)" pad="4"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="VOUT" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2937IMP-10"/>
<attribute name="OC_FARNELL" value="1469068"/>
<attribute name="OC_NEWARK" value="41K4555"/>
<attribute name="PACKAGE" value="SOT-223-3"/>
<attribute name="SUPPLIER" value="Microchip"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2937IMP-12" prefix="U">
<description>IC, LDO VOLT REG, 12V, 0.5A</description>
<gates>
<gate name="A" symbol="LM2937IMP-12"/>
</gates>
<devices>
<device name="" package="SOT230P700X180-4N">
<connects>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="GND_(TAB)" pad="4"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="VOUT" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2937IMP-12"/>
<attribute name="OC_FARNELL" value="1469069"/>
<attribute name="OC_NEWARK" value="41K4556"/>
<attribute name="PACKAGE" value="SOT-223-3"/>
<attribute name="SUPPLIER" value="Microchip"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2937IMP-15" prefix="U">
<description>Voltage Regulator IC</description>
<gates>
<gate name="A" symbol="LM2937IMP-15"/>
</gates>
<devices>
<device name="" package="SOT230P700X180-4N">
<connects>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="GND_(TAB)" pad="4"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="VOUT" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2937IMP-15"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K4557"/>
<attribute name="PACKAGE" value="SOT-223-3"/>
<attribute name="SUPPLIER" value="Microchip"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2937IMP-5.0" prefix="U">
<description>IC, LDO VOLT REG, 5V, 0.5A</description>
<gates>
<gate name="A" symbol="LM2937IMP-5.0"/>
</gates>
<devices>
<device name="" package="SOT230P700X180-4N">
<connects>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="GND_(TAB)" pad="4"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="VOUT" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2937IMP-5.0"/>
<attribute name="OC_FARNELL" value="1798318"/>
<attribute name="OC_NEWARK" value="83F3856"/>
<attribute name="PACKAGE" value="SOT-223-3"/>
<attribute name="SUPPLIER" value="Microchip"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2937IMP-8.0" prefix="U">
<description>IC, LDO VOLT REG, 8V, 0.5A</description>
<gates>
<gate name="A" symbol="LM2937IMP-8.0"/>
</gates>
<devices>
<device name="" package="SOT230P700X180-4N">
<connects>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="GND_(TAB)" pad="4"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="VOUT" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2937IMP-8.0"/>
<attribute name="OC_FARNELL" value="1685532"/>
<attribute name="OC_NEWARK" value="07B6342"/>
<attribute name="PACKAGE" value="SOT-223-3"/>
<attribute name="SUPPLIER" value="Microchip"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM293H" prefix="U">
<description>IC COMPARATOR LP DUAL</description>
<gates>
<gate name="A" symbol="LM293H"/>
</gates>
<devices>
<device name="" package="TO254P914X470-8P">
<connects>
<connect gate="A" pin="+INA" pad="3"/>
<connect gate="A" pin="+INB" pad="5"/>
<connect gate="A" pin="-INA" pad="2"/>
<connect gate="A" pin="-INB" pad="6"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM293H"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="31T9917"/>
<attribute name="PACKAGE" value="TO-99-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2940CS-5.0" prefix="U">
<description>Dropout Regulator</description>
<gates>
<gate name="A" symbol="LM2940CS-5.0"/>
</gates>
<devices>
<device name="" package="TO254P1435X464-4N">
<connects>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="GND_2" pad="2"/>
<connect gate="A" pin="IN" pad="1"/>
<connect gate="A" pin="OUT" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2940CS-5.0"/>
<attribute name="OC_FARNELL" value="9779850"/>
<attribute name="OC_NEWARK" value="07B6352"/>
<attribute name="PACKAGE" value="TO-263-3"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2940CS-9.0" prefix="U">
<description>Dropout Regulator</description>
<gates>
<gate name="A" symbol="LM2940CS-9.0"/>
</gates>
<devices>
<device name="" package="TO254P1435X464-4N">
<connects>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="GND_2" pad="2"/>
<connect gate="A" pin="IN" pad="1"/>
<connect gate="A" pin="OUT" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2940CS-9.0"/>
<attribute name="OC_FARNELL" value="9494430"/>
<attribute name="OC_NEWARK" value="41K4570"/>
<attribute name="PACKAGE" value="TO-263-3"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2940CT-12" prefix="U">
<description>IC, LDO VOLT REG, 12V, 1A</description>
<gates>
<gate name="A" symbol="LM2940CT-12"/>
</gates>
<devices>
<device name="" package="TO254P470X1016X2222-3P">
<connects>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="IN" pad="1"/>
<connect gate="A" pin="OUT" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2940CT-12"/>
<attribute name="OC_FARNELL" value="9490299"/>
<attribute name="OC_NEWARK" value="41K4575"/>
<attribute name="PACKAGE" value="TO-220"/>
<attribute name="SUPPLIER" value="NATIONAL SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2940CT-15" prefix="U">
<description>IC, LDO VOLT REG, 15V, 1A</description>
<gates>
<gate name="A" symbol="LM2940CT-15"/>
</gates>
<devices>
<device name="" package="TO254P470X1016X2222-3P">
<connects>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="IN" pad="1"/>
<connect gate="A" pin="OUT" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2940CT-15"/>
<attribute name="OC_FARNELL" value="9490337"/>
<attribute name="OC_NEWARK" value="41K4576"/>
<attribute name="PACKAGE" value="TO-220"/>
<attribute name="SUPPLIER" value="NATIONAL SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2940CT-5.0" prefix="U">
<description>IC, LDO VOLT REG, 5V, 1A</description>
<gates>
<gate name="A" symbol="LM2940CT-5.0"/>
</gates>
<devices>
<device name="" package="TO254P470X1016X2222-3P">
<connects>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="IN" pad="1"/>
<connect gate="A" pin="OUT" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2940CT-5.0"/>
<attribute name="OC_FARNELL" value="9490191"/>
<attribute name="OC_NEWARK" value="41K4577"/>
<attribute name="PACKAGE" value="TO-220"/>
<attribute name="SUPPLIER" value="NATIONAL SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2940IMP-5.0" prefix="U">
<description>Low Dropout Regulator</description>
<gates>
<gate name="A" symbol="LM2940IMP-5.0"/>
</gates>
<devices>
<device name="" package="SOT230P696X180-4N">
<connects>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="GND_2" pad="2"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="VOUT" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2940IMP-50"/>
<attribute name="OC_FARNELL" value="9778845"/>
<attribute name="OC_NEWARK" value="41K4582"/>
<attribute name="PACKAGE" value="SOT-223-4"/>
<attribute name="SUPPLIER" value="National"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2940S-5.0" prefix="U">
<description>Dropout Regulator</description>
<gates>
<gate name="A" symbol="LM2940S-5.0"/>
</gates>
<devices>
<device name="" package="TO254P1435X464-4N">
<connects>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="GND_2" pad="2"/>
<connect gate="A" pin="IN" pad="1"/>
<connect gate="A" pin="OUT" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2940S-5.0"/>
<attribute name="OC_FARNELL" value="1523865"/>
<attribute name="OC_NEWARK" value="41K4605"/>
<attribute name="PACKAGE" value="TO-263-3"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2940T-10.0" prefix="U">
<description>IC, LDO VOLT REG, 10V, 1A</description>
<gates>
<gate name="A" symbol="LM2940T-10.0"/>
</gates>
<devices>
<device name="" package="TO254P470X1016X2222-3P">
<connects>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="IN" pad="1"/>
<connect gate="A" pin="OUT" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2940T-10.0"/>
<attribute name="OC_FARNELL" value="9493522"/>
<attribute name="OC_NEWARK" value="41K4613"/>
<attribute name="PACKAGE" value="TO-220"/>
<attribute name="SUPPLIER" value="NATIONAL SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2940T-12.0" prefix="U">
<description>IC, LDO VOLT REG, 12V, 1A</description>
<gates>
<gate name="A" symbol="LM2940T-12.0"/>
</gates>
<devices>
<device name="" package="TO254P470X1016X2222-3P">
<connects>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="IN" pad="1"/>
<connect gate="A" pin="OUT" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2940T-12.0"/>
<attribute name="OC_FARNELL" value="9485872"/>
<attribute name="OC_NEWARK" value="41K4614"/>
<attribute name="PACKAGE" value="TO-220"/>
<attribute name="SUPPLIER" value="NATIONAL SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2940T-5.0" prefix="U">
<description>IC, LDO VOLT REG, 5V, 1A</description>
<gates>
<gate name="A" symbol="LM2940T-5.0"/>
</gates>
<devices>
<device name="" package="TO254P470X1016X2222-3P">
<connects>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="IN" pad="1"/>
<connect gate="A" pin="OUT" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2940T-5.0"/>
<attribute name="OC_FARNELL" value="9490205"/>
<attribute name="OC_NEWARK" value="41K4615"/>
<attribute name="PACKAGE" value="TO-220"/>
<attribute name="SUPPLIER" value="NATIONAL SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2940T-8.0" prefix="U">
<description>IC, LDO VOLT REG, 8V, 1A</description>
<gates>
<gate name="A" symbol="LM2940T-8.0"/>
</gates>
<devices>
<device name="" package="TO254P470X1016X2222-3P">
<connects>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="IN" pad="1"/>
<connect gate="A" pin="OUT" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2940T-8.0"/>
<attribute name="OC_FARNELL" value="9490230"/>
<attribute name="OC_NEWARK" value="41K4616"/>
<attribute name="PACKAGE" value="TO-220"/>
<attribute name="SUPPLIER" value="NATIONAL SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2940T-9.0" prefix="U">
<description>IC, LDO VOLT REG, 9V, 1A</description>
<gates>
<gate name="A" symbol="LM2940T-9.0"/>
</gates>
<devices>
<device name="" package="TO254P470X1016X2222-3P">
<connects>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="IN" pad="1"/>
<connect gate="A" pin="OUT" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2940T-9.0"/>
<attribute name="OC_FARNELL" value="9493514"/>
<attribute name="OC_NEWARK" value="41K4617"/>
<attribute name="PACKAGE" value="TO-220"/>
<attribute name="SUPPLIER" value="NATIONAL SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2941CT" prefix="U">
<description>IC, ADJ LDO REG, 5V TO 20V, 1A</description>
<gates>
<gate name="A" symbol="LM2941CT"/>
</gates>
<devices>
<device name="" package="TO170P470X1016X2092-5P">
<connects>
<connect gate="A" pin="ADJ" pad="1"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="IN" pad="4"/>
<connect gate="A" pin="ON/OFF" pad="2"/>
<connect gate="A" pin="OUT" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2941CT"/>
<attribute name="OC_FARNELL" value="9489371"/>
<attribute name="OC_NEWARK" value="41K4620"/>
<attribute name="PACKAGE" value="TO220-5"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2941LD" prefix="U">
<description>REG LDO</description>
<gates>
<gate name="A" symbol="LM2941LD"/>
</gates>
<devices>
<device name="" package="DFN400X400X80-9N">
<connects>
<connect gate="A" pin="ADJ" pad="8"/>
<connect gate="A" pin="GND" pad="9"/>
<connect gate="A" pin="GND_2" pad="2"/>
<connect gate="A" pin="GND_3" pad="7"/>
<connect gate="A" pin="IN" pad="3"/>
<connect gate="A" pin="NC" pad="6"/>
<connect gate="A" pin="NC_2" pad="4"/>
<connect gate="A" pin="ON/OFF" pad="1"/>
<connect gate="A" pin="OUT" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2941LD"/>
<attribute name="OC_FARNELL" value="1798362"/>
<attribute name="OC_NEWARK" value="73R9732"/>
<attribute name="PACKAGE" value="LLP-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2941S" prefix="U">
<description>Adjustable Regulator</description>
<gates>
<gate name="A" symbol="LM2941S"/>
</gates>
<devices>
<device name="" package="TO170P1435X465-6N">
<connects>
<connect gate="A" pin="ADJ" pad="1"/>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="GND_2" pad="3"/>
<connect gate="A" pin="IN" pad="4"/>
<connect gate="A" pin="ON/OFF" pad="2"/>
<connect gate="A" pin="OUT" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2941S"/>
<attribute name="OC_FARNELL" value="9494456"/>
<attribute name="OC_NEWARK" value="07B6391"/>
<attribute name="PACKAGE" value="TO-263-5"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2990S-12" prefix="U">
<description>Negative Low Dropout Regulator</description>
<gates>
<gate name="A" symbol="LM2990S-12"/>
</gates>
<devices>
<device name="" package="TO254P1435X457-4N">
<connects>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="GND_2" pad="1"/>
<connect gate="A" pin="IN" pad="2"/>
<connect gate="A" pin="OUT" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2990S-12"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K4628"/>
<attribute name="PACKAGE" value="TO-263-3"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2990T-12" prefix="U">
<description>IC, LDO VOLT REG, -12V, 1.5A</description>
<gates>
<gate name="A" symbol="LM2990T-12"/>
</gates>
<devices>
<device name="" package="TO254P470X1016X2222-3P">
<connects>
<connect gate="A" pin="GND" pad="1"/>
<connect gate="A" pin="IN" pad="2"/>
<connect gate="A" pin="OUT" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2990T-12"/>
<attribute name="OC_FARNELL" value="9485899"/>
<attribute name="OC_NEWARK" value="41K4634"/>
<attribute name="PACKAGE" value="TO-220"/>
<attribute name="SUPPLIER" value="NATIONAL SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2990T-15" prefix="U">
<description>IC, LDO VOLT REG, -15V, 1.5A</description>
<gates>
<gate name="A" symbol="LM2990T-15"/>
</gates>
<devices>
<device name="" package="TO254P470X1016X2222-3P">
<connects>
<connect gate="A" pin="GND" pad="1"/>
<connect gate="A" pin="IN" pad="2"/>
<connect gate="A" pin="OUT" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2990T-15"/>
<attribute name="OC_FARNELL" value="9485902"/>
<attribute name="OC_NEWARK" value="41K4635"/>
<attribute name="PACKAGE" value="TO-220"/>
<attribute name="SUPPLIER" value="NATIONAL SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2990T-5.0" prefix="U">
<description>IC, LDO VOLT REG, -5V, 1A</description>
<gates>
<gate name="A" symbol="LM2990T-5.0"/>
</gates>
<devices>
<device name="" package="TO254P470X1016X2222-3P">
<connects>
<connect gate="A" pin="GND" pad="1"/>
<connect gate="A" pin="IN" pad="2"/>
<connect gate="A" pin="OUT" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM2990T-5.0"/>
<attribute name="OC_FARNELL" value="9485880"/>
<attribute name="OC_NEWARK" value="41K4636"/>
<attribute name="PACKAGE" value="TO-220"/>
<attribute name="SUPPLIER" value="NATIONAL SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3000SQ" prefix="U">
<description>Dual Synchronous Emulated Current-Mode Controller</description>
<gates>
<gate name="A" symbol="LM3000SQ"/>
</gates>
<devices>
<device name="" package="QFN50P500X500X80-33N">
<connects>
<connect gate="A" pin="CLKOUT" pad="28"/>
<connect gate="A" pin="COMP1" pad="15"/>
<connect gate="A" pin="COMP2" pad="25"/>
<connect gate="A" pin="EA1_GND" pad="13"/>
<connect gate="A" pin="EA2_GND" pad="27"/>
<connect gate="A" pin="EN1" pad="18"/>
<connect gate="A" pin="EN2" pad="23"/>
<connect gate="A" pin="EPAD" pad="33"/>
<connect gate="A" pin="FB1" pad="14"/>
<connect gate="A" pin="FB2" pad="26"/>
<connect gate="A" pin="FREQ/SYNC" pad="17"/>
<connect gate="A" pin="HG1" pad="10"/>
<connect gate="A" pin="HG2" pad="31"/>
<connect gate="A" pin="ILIM1" pad="9"/>
<connect gate="A" pin="ILIM2" pad="32"/>
<connect gate="A" pin="LG1" pad="6"/>
<connect gate="A" pin="LG2" pad="3"/>
<connect gate="A" pin="PGND1" pad="7"/>
<connect gate="A" pin="PGND2" pad="2"/>
<connect gate="A" pin="PGOOD1" pad="16"/>
<connect gate="A" pin="PGOOD2" pad="24"/>
<connect gate="A" pin="SGND" pad="29"/>
<connect gate="A" pin="SS1" pad="20"/>
<connect gate="A" pin="SS2" pad="22"/>
<connect gate="A" pin="TRK1" pad="19"/>
<connect gate="A" pin="TRK2" pad="21"/>
<connect gate="A" pin="VCB1" pad="11"/>
<connect gate="A" pin="VCB2" pad="30"/>
<connect gate="A" pin="VDD" pad="12"/>
<connect gate="A" pin="VDR" pad="5"/>
<connect gate="A" pin="VIN" pad="4"/>
<connect gate="A" pin="VSW1" pad="8"/>
<connect gate="A" pin="VSW2" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM3000SQ"/>
<attribute name="OC_FARNELL" value="16R1311"/>
<attribute name="OC_NEWARK" value="736512"/>
<attribute name="PACKAGE" value="QFN-33"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM301AH" prefix="U">
<description>OP AMP, GENERAL PURPOSE</description>
<gates>
<gate name="A" symbol="LM301AH"/>
</gates>
<devices>
<device name="" package="TO254P914X470-8P">
<connects>
<connect gate="A" pin="+INA" pad="3"/>
<connect gate="A" pin="-INA" pad="2"/>
<connect gate="A" pin="BALANCE" pad="5"/>
<connect gate="A" pin="BALANCE_2" pad="1"/>
<connect gate="A" pin="COMP" pad="8"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM301AH"/>
<attribute name="OC_FARNELL" value="1216151"/>
<attribute name="OC_NEWARK" value="01M8144"/>
<attribute name="PACKAGE" value="TO-99-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM301AN" prefix="U">
<description>OpAmpIC</description>
<gates>
<gate name="A" symbol="LM301AN"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-8">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="BAL" pad="5"/>
<connect gate="A" pin="BAL/COMP" pad="1"/>
<connect gate="A" pin="COMP" pad="8"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM301AN"/>
<attribute name="OC_FARNELL" value="9486720"/>
<attribute name="OC_NEWARK" value="41K4643"/>
<attribute name="PACKAGE" value="DIP-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3100MH" prefix="U">
<description>Step-Down Voltage Regulator</description>
<gates>
<gate name="A" symbol="LM3100MH"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-21N">
<connects>
<connect gate="A" pin="BST" pad="6"/>
<connect gate="A" pin="EN" pad="14"/>
<connect gate="A" pin="EPAD" pad="21"/>
<connect gate="A" pin="FB" pad="13"/>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="NC" pad="20"/>
<connect gate="A" pin="NC_2" pad="9"/>
<connect gate="A" pin="NC_3" pad="12"/>
<connect gate="A" pin="NC_4" pad="19"/>
<connect gate="A" pin="NC_5" pad="10"/>
<connect gate="A" pin="NC_6" pad="1"/>
<connect gate="A" pin="PGND" pad="18"/>
<connect gate="A" pin="PGND_2" pad="17"/>
<connect gate="A" pin="RON" pad="15"/>
<connect gate="A" pin="SS" pad="8"/>
<connect gate="A" pin="SW" pad="3"/>
<connect gate="A" pin="SW_2" pad="2"/>
<connect gate="A" pin="TST" pad="11"/>
<connect gate="A" pin="VCC" pad="16"/>
<connect gate="A" pin="VIN" pad="5"/>
<connect gate="A" pin="VIN_2" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM3100MH"/>
<attribute name="OC_FARNELL" value="1286748"/>
<attribute name="OC_NEWARK" value="79K7816"/>
<attribute name="PACKAGE" value="TSSOP-20"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3102MH" prefix="U">
<description>Step-Down Voltage Regulator</description>
<gates>
<gate name="A" symbol="LM3102MH"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-21N">
<connects>
<connect gate="A" pin="AGND" pad="7"/>
<connect gate="A" pin="BST" pad="6"/>
<connect gate="A" pin="EN" pad="14"/>
<connect gate="A" pin="EPAD" pad="21"/>
<connect gate="A" pin="FB" pad="13"/>
<connect gate="A" pin="GND" pad="11"/>
<connect gate="A" pin="NC" pad="20"/>
<connect gate="A" pin="NC_2" pad="1"/>
<connect gate="A" pin="NC_3" pad="9"/>
<connect gate="A" pin="NC_4" pad="10"/>
<connect gate="A" pin="NC_5" pad="12"/>
<connect gate="A" pin="NC_6" pad="19"/>
<connect gate="A" pin="PGND" pad="18"/>
<connect gate="A" pin="PGND_2" pad="17"/>
<connect gate="A" pin="RON" pad="15"/>
<connect gate="A" pin="SS" pad="8"/>
<connect gate="A" pin="SW" pad="2"/>
<connect gate="A" pin="SW_2" pad="3"/>
<connect gate="A" pin="VCC" pad="16"/>
<connect gate="A" pin="VIN" pad="5"/>
<connect gate="A" pin="VIN_2" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM3102MH"/>
<attribute name="OC_FARNELL" value="1506819"/>
<attribute name="OC_NEWARK" value="54M4671"/>
<attribute name="PACKAGE" value="TSSOP-20"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3103MH" prefix="U">
<description>Step-Down Voltage Regulator</description>
<gates>
<gate name="A" symbol="LM3103MH"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-17N">
<connects>
<connect gate="A" pin="AGND" pad="6"/>
<connect gate="A" pin="BST" pad="5"/>
<connect gate="A" pin="EN" pad="12"/>
<connect gate="A" pin="EPAD" pad="17"/>
<connect gate="A" pin="FB" pad="11"/>
<connect gate="A" pin="GND" pad="9"/>
<connect gate="A" pin="GND_2" pad="10"/>
<connect gate="A" pin="NC" pad="8"/>
<connect gate="A" pin="PGND" pad="16"/>
<connect gate="A" pin="PGND_2" pad="15"/>
<connect gate="A" pin="RON" pad="13"/>
<connect gate="A" pin="SS" pad="7"/>
<connect gate="A" pin="SW" pad="3"/>
<connect gate="A" pin="SW_2" pad="4"/>
<connect gate="A" pin="VCC" pad="14"/>
<connect gate="A" pin="VIN" pad="2"/>
<connect gate="A" pin="VIN_2" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM3103MH"/>
<attribute name="OC_FARNELL" value="1506820"/>
<attribute name="OC_NEWARK" value="64M6981"/>
<attribute name="PACKAGE" value="TSSOP-16"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM311H" prefix="U">
<description>IC VOLTAGE COMPARATOR</description>
<gates>
<gate name="A" symbol="LM311H"/>
</gates>
<devices>
<device name="" package="TO254P914X470-8P">
<connects>
<connect gate="A" pin="+INA" pad="3"/>
<connect gate="A" pin="+INB" pad="5"/>
<connect gate="A" pin="-INA" pad="2"/>
<connect gate="A" pin="-INB" pad="6"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM311H"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="31T9923"/>
<attribute name="PACKAGE" value="TO-99-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM311M" prefix="U">
<description>Voltage Comparator</description>
<gates>
<gate name="A" symbol="LM311M"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="BAL" pad="5"/>
<connect gate="A" pin="BAL/STROBE" pad="6"/>
<connect gate="A" pin="GND1" pad="1"/>
<connect gate="A" pin="IN2" pad="2"/>
<connect gate="A" pin="IN3" pad="3"/>
<connect gate="A" pin="OUT" pad="7"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM311M"/>
<attribute name="OC_FARNELL" value="9487212"/>
<attribute name="OC_NEWARK" value="41K4646"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM311N" prefix="U">
<description>Voltage Comparator</description>
<gates>
<gate name="A" symbol="LM311N"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-8">
<connects>
<connect gate="A" pin="BAL" pad="5"/>
<connect gate="A" pin="BAL/STROBE" pad="6"/>
<connect gate="A" pin="GND" pad="1"/>
<connect gate="A" pin="IN2" pad="2"/>
<connect gate="A" pin="IN3" pad="3"/>
<connect gate="A" pin="OUT" pad="7"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM311N"/>
<attribute name="OC_FARNELL" value="9487220"/>
<attribute name="OC_NEWARK" value="07B6414"/>
<attribute name="PACKAGE" value="DIP-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3150MH" prefix="U">
<description>SIMPLE SWITCHER® CONTROLLER</description>
<gates>
<gate name="A" symbol="LM3150MH"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-15N">
<connects>
<connect gate="A" pin="BST" pad="12"/>
<connect gate="A" pin="EN" pad="3"/>
<connect gate="A" pin="EPAD" pad="15"/>
<connect gate="A" pin="FB" pad="4"/>
<connect gate="A" pin="HG" pad="11"/>
<connect gate="A" pin="ILIM" pad="8"/>
<connect gate="A" pin="LG" pad="13"/>
<connect gate="A" pin="PGND" pad="14"/>
<connect gate="A" pin="RON" pad="7"/>
<connect gate="A" pin="SGND" pad="9"/>
<connect gate="A" pin="SGND_2" pad="5"/>
<connect gate="A" pin="SS" pad="6"/>
<connect gate="A" pin="SW" pad="10"/>
<connect gate="A" pin="VCC" pad="1"/>
<connect gate="A" pin="VIN" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM3150MH"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="34P4821"/>
<attribute name="PACKAGE" value="TSSOP-14"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM318M" prefix="U">
<description>Operational Amplifiers</description>
<gates>
<gate name="A" symbol="LM318M"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="BAL/COMP1" pad="1"/>
<connect gate="A" pin="BAL/COMP3" pad="5"/>
<connect gate="A" pin="COMP2" pad="8"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM318M"/>
<attribute name="OC_FARNELL" value="9486739"/>
<attribute name="OC_NEWARK" value="41K4664"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM318N" prefix="U">
<description>Operational Amplifiers</description>
<gates>
<gate name="A" symbol="LM318N"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-8">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="BAL/COMP1" pad="1"/>
<connect gate="A" pin="BAL/COMP3" pad="5"/>
<connect gate="A" pin="COMP2" pad="8"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM318N"/>
<attribute name="OC_FARNELL" value="1468915"/>
<attribute name="OC_NEWARK" value="07B6426"/>
<attribute name="PACKAGE" value="DIP-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM319AM" prefix="U">
<description>High Speed Dual Comparator</description>
<gates>
<gate name="A" symbol="LM319AM"/>
</gates>
<devices>
<device name="" package="SOIC127P620X175-14N">
<connects>
<connect gate="A" pin="+IN" pad="4"/>
<connect gate="A" pin="+IN2" pad="9"/>
<connect gate="A" pin="-IN" pad="5"/>
<connect gate="A" pin="-IN2" pad="10"/>
<connect gate="A" pin="GND1" pad="3"/>
<connect gate="A" pin="GND2" pad="8"/>
<connect gate="A" pin="NC" pad="2"/>
<connect gate="A" pin="NC_2" pad="13"/>
<connect gate="A" pin="NC_3" pad="14"/>
<connect gate="A" pin="NC_4" pad="1"/>
<connect gate="A" pin="OUT1" pad="12"/>
<connect gate="A" pin="OUT2" pad="7"/>
<connect gate="A" pin="V+" pad="11"/>
<connect gate="A" pin="V-" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM319AM"/>
<attribute name="OC_FARNELL" value="1564707"/>
<attribute name="OC_NEWARK" value="41K4667"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM319M" prefix="U">
<description>High Speed Dual Comparator</description>
<gates>
<gate name="A" symbol="LM319M"/>
</gates>
<devices>
<device name="" package="SOIC127P620X175-14N">
<connects>
<connect gate="A" pin="+IN" pad="4"/>
<connect gate="A" pin="+IN2" pad="9"/>
<connect gate="A" pin="-IN" pad="5"/>
<connect gate="A" pin="-IN2" pad="10"/>
<connect gate="A" pin="GND1" pad="3"/>
<connect gate="A" pin="GND2" pad="8"/>
<connect gate="A" pin="NC" pad="2"/>
<connect gate="A" pin="NC_2" pad="13"/>
<connect gate="A" pin="NC_3" pad="14"/>
<connect gate="A" pin="NC_4" pad="1"/>
<connect gate="A" pin="OUT1" pad="12"/>
<connect gate="A" pin="OUT2" pad="7"/>
<connect gate="A" pin="V+" pad="11"/>
<connect gate="A" pin="V-" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM319M"/>
<attribute name="OC_FARNELL" value="9490469"/>
<attribute name="OC_NEWARK" value="-"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM319N" prefix="U">
<description>High Speed Dual Comparator</description>
<gates>
<gate name="A" symbol="LM319N"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-14">
<connects>
<connect gate="A" pin="+IN" pad="4"/>
<connect gate="A" pin="+IN2" pad="9"/>
<connect gate="A" pin="-IN" pad="5"/>
<connect gate="A" pin="-IN2" pad="10"/>
<connect gate="A" pin="GND1" pad="3"/>
<connect gate="A" pin="GND2" pad="8"/>
<connect gate="A" pin="NC" pad="2"/>
<connect gate="A" pin="NC_2" pad="13"/>
<connect gate="A" pin="NC_3" pad="14"/>
<connect gate="A" pin="NC_4" pad="1"/>
<connect gate="A" pin="OUT1" pad="12"/>
<connect gate="A" pin="OUT2" pad="7"/>
<connect gate="A" pin="V+" pad="11"/>
<connect gate="A" pin="V-" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM319N"/>
<attribute name="OC_FARNELL" value="1094247"/>
<attribute name="OC_NEWARK" value="-"/>
<attribute name="PACKAGE" value="DIP-14"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3200TL" prefix="U">
<description>IC,DC/DC CONVERTER,CMOS</description>
<gates>
<gate name="A" symbol="LM3200TL"/>
</gates>
<devices>
<device name="" package="BGA10C50PX50P3X4_181X217X60">
<connects>
<connect gate="A" pin="BYP" pad="D1"/>
<connect gate="A" pin="BYPOUT" pad="A3"/>
<connect gate="A" pin="EN" pad="D2"/>
<connect gate="A" pin="FB" pad="C1"/>
<connect gate="A" pin="PGND" pad="D3"/>
<connect gate="A" pin="PVIN" pad="B3"/>
<connect gate="A" pin="SGND" pad="A2"/>
<connect gate="A" pin="SW" pad="C3"/>
<connect gate="A" pin="VCON" pad="B1"/>
<connect gate="A" pin="VDD" pad="A1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM3200TL"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K4677"/>
<attribute name="PACKAGE" value="10-WFBGA"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3203TL" prefix="U">
<description>IC,SMPS CONTROLLER,CURRENT-MODE,BGA</description>
<gates>
<gate name="A" symbol="LM3203TL"/>
</gates>
<devices>
<device name="" package="BGA10C50PX50P3X4_181X217X60">
<connects>
<connect gate="A" pin="BYP" pad="D1"/>
<connect gate="A" pin="BYPOUT" pad="A3"/>
<connect gate="A" pin="EN" pad="D2"/>
<connect gate="A" pin="FB" pad="C1"/>
<connect gate="A" pin="PGND" pad="D3"/>
<connect gate="A" pin="PVIN" pad="B3"/>
<connect gate="A" pin="SGND" pad="A2"/>
<connect gate="A" pin="SW" pad="C3"/>
<connect gate="A" pin="VCON" pad="B1"/>
<connect gate="A" pin="VDD" pad="A1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM3203TL"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="69K2445"/>
<attribute name="PACKAGE" value="10-WFBGA"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3205SD-2" prefix="U">
<description>Step-Down DC-DC Converter</description>
<gates>
<gate name="A" symbol="LM3205SD-2"/>
</gates>
<devices>
<device name="" package="DFN300X300X80-11N">
<connects>
<connect gate="A" pin="EN" pad="6"/>
<connect gate="A" pin="EPAD" pad="11"/>
<connect gate="A" pin="FB" pad="5"/>
<connect gate="A" pin="PGND" pad="2"/>
<connect gate="A" pin="PGND_2" pad="1"/>
<connect gate="A" pin="PVIN" pad="9"/>
<connect gate="A" pin="PVIN_2" pad="8"/>
<connect gate="A" pin="SGND" pad="3"/>
<connect gate="A" pin="SW" pad="10"/>
<connect gate="A" pin="VCON" pad="4"/>
<connect gate="A" pin="VDD" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM3205SD-2"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="32M1038"/>
<attribute name="PACKAGE" value="DFN-10"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3205TL" prefix="U">
<description>BUCK CONVERTER, RF POWER AMP</description>
<gates>
<gate name="A" symbol="LM3205TL"/>
</gates>
<devices>
<device name="" package="BGA08C50PX50P3X3_166X181X60">
<connects>
<connect gate="A" pin="EN" pad="C1"/>
<connect gate="A" pin="FB" pad="C3"/>
<connect gate="A" pin="PGND" pad="A3"/>
<connect gate="A" pin="PVIN" pad="A1"/>
<connect gate="A" pin="SGND" pad="B3"/>
<connect gate="A" pin="SW" pad="A2"/>
<connect gate="A" pin="VCON" pad="C2"/>
<connect gate="A" pin="VDD" pad="B1"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPTYPE" value="8-WFBGA"/>
<attribute name="MPN" value="LM3205TL"/>
<attribute name="OC_FARNELL" value="1286807"/>
<attribute name="OC_NEWARK" value="-"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3207TL" prefix="U">
<description>IC CONV DC/DC 650MA ADJ</description>
<gates>
<gate name="A" symbol="LM3207TL"/>
</gates>
<devices>
<device name="" package="BGA09N50P3X3_195X195X60">
<connects>
<connect gate="A" pin="EN" pad="B2"/>
<connect gate="A" pin="ENLDO" pad="B1"/>
<connect gate="A" pin="FB" pad="C1"/>
<connect gate="A" pin="LDO" pad="C3"/>
<connect gate="A" pin="PGND" pad="A3"/>
<connect gate="A" pin="PVIN" pad="A1"/>
<connect gate="A" pin="SGND" pad="B3"/>
<connect gate="A" pin="SW" pad="A2"/>
<connect gate="A" pin="VCON" pad="C2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM3207TL"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="32M1042"/>
<attribute name="PACKAGE" value="Switcher"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3208TL" prefix="U">
<description>Step-Down DC-DC Converter</description>
<gates>
<gate name="A" symbol="LM3208TL"/>
</gates>
<devices>
<device name="" package="BGA8C3X3X50P_181X166X67">
<connects>
<connect gate="A" pin="EN" pad="C1"/>
<connect gate="A" pin="FB" pad="C3"/>
<connect gate="A" pin="PGND" pad="A3"/>
<connect gate="A" pin="PVIN" pad="A1"/>
<connect gate="A" pin="SGND" pad="B3"/>
<connect gate="A" pin="SW" pad="A2"/>
<connect gate="A" pin="VCON" pad="C2"/>
<connect gate="A" pin="VDD" pad="B1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM3208TL"/>
<attribute name="OC_FARNELL" value="1798319"/>
<attribute name="OC_NEWARK" value="73R9733"/>
<attribute name="PACKAGE" value="BGA-8"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3211MT-ADJ" prefix="U">
<description>CONVERTER, DC-DC BOOST, SMD</description>
<gates>
<gate name="A" symbol="LM3211MT-ADJ"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-20N">
<connects>
<connect gate="A" pin="AGND" pad="19"/>
<connect gate="A" pin="FB" pad="18"/>
<connect gate="A" pin="FSLCT" pad="4"/>
<connect gate="A" pin="GMA1-IN" pad="6"/>
<connect gate="A" pin="GMA1-OUT" pad="15"/>
<connect gate="A" pin="GMA2-IN" pad="7"/>
<connect gate="A" pin="GMA2-OUT" pad="14"/>
<connect gate="A" pin="GMA3-IN" pad="8"/>
<connect gate="A" pin="GMA3-OUT" pad="13"/>
<connect gate="A" pin="GMA4-IN" pad="9"/>
<connect gate="A" pin="GMA4-OUT" pad="12"/>
<connect gate="A" pin="GND" pad="20"/>
<connect gate="A" pin="NC" pad="10"/>
<connect gate="A" pin="NC_2" pad="11"/>
<connect gate="A" pin="SS" pad="16"/>
<connect gate="A" pin="VC" pad="17"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="VS+" pad="5"/>
<connect gate="A" pin="VSW" pad="2"/>
<connect gate="A" pin="~SHDN" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM3211MT-ADJ"/>
<attribute name="OC_FARNELL" value="1286875"/>
<attribute name="OC_NEWARK" value="-"/>
<attribute name="PACKAGE" value="20-TSSOP"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM321MF" prefix="U">
<description>Low Power Single Op Amp</description>
<gates>
<gate name="A" symbol="LM321MF"/>
</gates>
<devices>
<device name="" package="SOT95P285X120-5N">
<connects>
<connect gate="A" pin="+IN" pad="1"/>
<connect gate="A" pin="-IN" pad="3"/>
<connect gate="A" pin="OUT" pad="4"/>
<connect gate="A" pin="V+" pad="5"/>
<connect gate="A" pin="V-" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM321MF"/>
<attribute name="OC_FARNELL" value="9779116"/>
<attribute name="OC_NEWARK" value="37K8530"/>
<attribute name="PACKAGE" value="SOT-23-5"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3224MM-ADJ" prefix="U">
<description>Step-up PWM DC/DC Converter</description>
<gates>
<gate name="A" symbol="LM3224MM-ADJ"/>
</gates>
<devices>
<device name="" package="SOP65P490X110-8N">
<connects>
<connect gate="A" pin="FB" pad="2"/>
<connect gate="A" pin="FSLCT" pad="7"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="SS" pad="8"/>
<connect gate="A" pin="SW" pad="5"/>
<connect gate="A" pin="VC" pad="1"/>
<connect gate="A" pin="VIN" pad="6"/>
<connect gate="A" pin="~SHDN" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM3224MM-ADJ"/>
<attribute name="OC_FARNELL" value="1008010"/>
<attribute name="OC_NEWARK" value="41K4682"/>
<attribute name="PACKAGE" value="MSOP-8"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM324AM" prefix="U">
<description>Low Power Quad Operational Amplifiers</description>
<gates>
<gate name="A" symbol="LM324AM"/>
</gates>
<devices>
<device name="" package="SOIC127P620X175-14N">
<connects>
<connect gate="A" pin="+IN1" pad="3"/>
<connect gate="A" pin="+IN2" pad="5"/>
<connect gate="A" pin="+IN3" pad="10"/>
<connect gate="A" pin="+IN4" pad="12"/>
<connect gate="A" pin="-IN1" pad="2"/>
<connect gate="A" pin="-IN2" pad="6"/>
<connect gate="A" pin="-IN3" pad="9"/>
<connect gate="A" pin="-IN4" pad="13"/>
<connect gate="A" pin="GND" pad="11"/>
<connect gate="A" pin="OUT1" pad="1"/>
<connect gate="A" pin="OUT2" pad="7"/>
<connect gate="A" pin="OUT3" pad="8"/>
<connect gate="A" pin="OUT4" pad="14"/>
<connect gate="A" pin="V+" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM324AM"/>
<attribute name="OC_FARNELL" value="9486909"/>
<attribute name="OC_NEWARK" value="-"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM324AN" prefix="U">
<description>Low Power Quad Operational Amplifiers</description>
<gates>
<gate name="A" symbol="LM324AN"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-14">
<connects>
<connect gate="A" pin="+INA_" pad="3"/>
<connect gate="A" pin="+INB" pad="5"/>
<connect gate="A" pin="+INC" pad="10"/>
<connect gate="A" pin="+IND" pad="12"/>
<connect gate="A" pin="-INA" pad="2"/>
<connect gate="A" pin="-INB" pad="6"/>
<connect gate="A" pin="-INC" pad="9"/>
<connect gate="A" pin="-IND" pad="13"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="OUTC" pad="8"/>
<connect gate="A" pin="OUTD" pad="14"/>
<connect gate="A" pin="V+" pad="4"/>
<connect gate="A" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM324AN"/>
<attribute name="OC_FARNELL" value="1523835"/>
<attribute name="OC_NEWARK" value="-"/>
<attribute name="PACKAGE" value="DIP-14"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM324M" prefix="U">
<description>Low Power Quad Operational Amplifiers</description>
<gates>
<gate name="A" symbol="LM324M"/>
</gates>
<devices>
<device name="" package="SOIC127P620X175-14N">
<connects>
<connect gate="A" pin="+IN1" pad="3"/>
<connect gate="A" pin="+IN2" pad="5"/>
<connect gate="A" pin="+IN3" pad="10"/>
<connect gate="A" pin="+IN4" pad="12"/>
<connect gate="A" pin="-IN1" pad="2"/>
<connect gate="A" pin="-IN2" pad="6"/>
<connect gate="A" pin="-IN3" pad="9"/>
<connect gate="A" pin="-IN4" pad="13"/>
<connect gate="A" pin="GND" pad="11"/>
<connect gate="A" pin="OUT1" pad="1"/>
<connect gate="A" pin="OUT2" pad="7"/>
<connect gate="A" pin="OUT3" pad="8"/>
<connect gate="A" pin="OUT4" pad="14"/>
<connect gate="A" pin="V+" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM324M"/>
<attribute name="OC_FARNELL" value="9486925"/>
<attribute name="OC_NEWARK" value="-"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM324MT" prefix="U">
<description>Low Power Quad Operational Amplifiers</description>
<gates>
<gate name="A" symbol="LM324MT"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-14N">
<connects>
<connect gate="A" pin="+IN1" pad="3"/>
<connect gate="A" pin="+IN2" pad="5"/>
<connect gate="A" pin="+IN3" pad="10"/>
<connect gate="A" pin="+IN4" pad="12"/>
<connect gate="A" pin="-IN1" pad="2"/>
<connect gate="A" pin="-IN2" pad="6"/>
<connect gate="A" pin="-IN3" pad="9"/>
<connect gate="A" pin="-IN4" pad="13"/>
<connect gate="A" pin="GND" pad="11"/>
<connect gate="A" pin="OUT1" pad="1"/>
<connect gate="A" pin="OUT2" pad="7"/>
<connect gate="A" pin="OUT3" pad="8"/>
<connect gate="A" pin="OUT4" pad="14"/>
<connect gate="A" pin="V+" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM324MT"/>
<attribute name="OC_FARNELL" value="1468917"/>
<attribute name="OC_NEWARK" value="41K4688"/>
<attribute name="PACKAGE" value="TSSOP-14"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM324N" prefix="U">
<description>Low Power Quad Operational Amplifiers</description>
<gates>
<gate name="A" symbol="LM324N"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-14">
<connects>
<connect gate="A" pin="+INA_" pad="3"/>
<connect gate="A" pin="+INB" pad="5"/>
<connect gate="A" pin="+INC" pad="10"/>
<connect gate="A" pin="+IND" pad="12"/>
<connect gate="A" pin="-INA" pad="2"/>
<connect gate="A" pin="-INB" pad="6"/>
<connect gate="A" pin="-INC" pad="9"/>
<connect gate="A" pin="-IND" pad="13"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="OUTC" pad="8"/>
<connect gate="A" pin="OUTD" pad="14"/>
<connect gate="A" pin="V+" pad="4"/>
<connect gate="A" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM324N"/>
<attribute name="OC_FARNELL" value="1523836"/>
<attribute name="OC_NEWARK" value="-"/>
<attribute name="PACKAGE" value="DIP-14"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3310SQ" prefix="U">
<description>Step-Up PWM DC/DC Converter</description>
<gates>
<gate name="A" symbol="LM3310SQ"/>
</gates>
<devices>
<device name="" package="QFN50P400X400X80-25N">
<connects>
<connect gate="A" pin="AGND" pad="10"/>
<connect gate="A" pin="AVIN" pad="6"/>
<connect gate="A" pin="CE" pad="22"/>
<connect gate="A" pin="EPAD" pad="25"/>
<connect gate="A" pin="FB" pad="20"/>
<connect gate="A" pin="FREQ" pad="16"/>
<connect gate="A" pin="NC" pad="13"/>
<connect gate="A" pin="NC_2" pad="11"/>
<connect gate="A" pin="NC_3" pad="1"/>
<connect gate="A" pin="NC_4" pad="12"/>
<connect gate="A" pin="NEG" pad="8"/>
<connect gate="A" pin="OUT" pad="7"/>
<connect gate="A" pin="PGND" pad="21"/>
<connect gate="A" pin="POS" pad="9"/>
<connect gate="A" pin="RE" pad="23"/>
<connect gate="A" pin="SS" pad="14"/>
<connect gate="A" pin="SW" pad="18"/>
<connect gate="A" pin="VC" pad="15"/>
<connect gate="A" pin="VDD" pad="5"/>
<connect gate="A" pin="VDPM" pad="4"/>
<connect gate="A" pin="VFLK" pad="3"/>
<connect gate="A" pin="VGH" pad="24"/>
<connect gate="A" pin="VGHM" pad="2"/>
<connect gate="A" pin="VIN" pad="17"/>
<connect gate="A" pin="~SHDN" pad="19"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM3310SQ"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="65K6087"/>
<attribute name="PACKAGE" value="QFN-24"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM334Z" prefix="U">
<description>IC, CURRENT SOURCE, ADJ, 40V</description>
<gates>
<gate name="A" symbol="LM334Z"/>
</gates>
<devices>
<device name="" package="TO127P254X495-3P">
<connects>
<connect gate="A" pin="R" pad="2"/>
<connect gate="A" pin="V+" pad="1"/>
<connect gate="A" pin="V-" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM334Z"/>
<attribute name="OC_FARNELL" value="1564650"/>
<attribute name="OC_NEWARK" value="41K4701"/>
<attribute name="PACKAGE" value="TO-92"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM339AM" prefix="U">
<description>Quad Comparators</description>
<gates>
<gate name="A" symbol="LM339AM"/>
</gates>
<devices>
<device name="" package="SOIC127P620X175-14N">
<connects>
<connect gate="A" pin="+IN1" pad="5"/>
<connect gate="A" pin="+IN2" pad="7"/>
<connect gate="A" pin="+IN3" pad="9"/>
<connect gate="A" pin="+IN4" pad="11"/>
<connect gate="A" pin="-IN1" pad="4"/>
<connect gate="A" pin="-IN2" pad="6"/>
<connect gate="A" pin="-IN3" pad="8"/>
<connect gate="A" pin="-IN4" pad="10"/>
<connect gate="A" pin="GND" pad="12"/>
<connect gate="A" pin="OUT1" pad="2"/>
<connect gate="A" pin="OUT2" pad="1"/>
<connect gate="A" pin="OUT3" pad="14"/>
<connect gate="A" pin="OUT4" pad="13"/>
<connect gate="A" pin="V+" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM339AM"/>
<attribute name="OC_FARNELL" value="9490485"/>
<attribute name="OC_NEWARK" value="-"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM339M" prefix="U">
<description>Quad Comparators</description>
<gates>
<gate name="A" symbol="LM339M"/>
</gates>
<devices>
<device name="" package="SOIC127P620X175-14N">
<connects>
<connect gate="A" pin="+IN1" pad="5"/>
<connect gate="A" pin="+IN2" pad="7"/>
<connect gate="A" pin="+IN3" pad="9"/>
<connect gate="A" pin="+IN4" pad="11"/>
<connect gate="A" pin="-IN1" pad="4"/>
<connect gate="A" pin="-IN2" pad="6"/>
<connect gate="A" pin="-IN3" pad="8"/>
<connect gate="A" pin="-IN4" pad="10"/>
<connect gate="A" pin="GND" pad="12"/>
<connect gate="A" pin="OUT1" pad="2"/>
<connect gate="A" pin="OUT2" pad="1"/>
<connect gate="A" pin="OUT3" pad="14"/>
<connect gate="A" pin="OUT4" pad="13"/>
<connect gate="A" pin="V+" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM339M"/>
<attribute name="OC_FARNELL" value="9487654"/>
<attribute name="OC_NEWARK" value="-"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM339N" prefix="U">
<description>Quad Comparators</description>
<gates>
<gate name="A" symbol="LM339N"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-14">
<connects>
<connect gate="A" pin="+IN1" pad="5"/>
<connect gate="A" pin="+IN2" pad="7"/>
<connect gate="A" pin="+IN3" pad="9"/>
<connect gate="A" pin="+IN4" pad="11"/>
<connect gate="A" pin="-IN1" pad="4"/>
<connect gate="A" pin="-IN2" pad="6"/>
<connect gate="A" pin="-IN3" pad="8"/>
<connect gate="A" pin="-IN4" pad="10"/>
<connect gate="A" pin="GND" pad="12"/>
<connect gate="A" pin="OUT1" pad="2"/>
<connect gate="A" pin="OUT2" pad="1"/>
<connect gate="A" pin="OUT3" pad="14"/>
<connect gate="A" pin="OUT4" pad="13"/>
<connect gate="A" pin="V+" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM339N"/>
<attribute name="OC_FARNELL" value="9487670"/>
<attribute name="OC_NEWARK" value="-"/>
<attribute name="PACKAGE" value="DIP-14"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3401MM" prefix="U">
<description>Hysteretic PFET Controller</description>
<gates>
<gate name="A" symbol="LM3401MM"/>
</gates>
<devices>
<device name="" package="SOP65P490X110-8N">
<connects>
<connect gate="A" pin="CS" pad="1"/>
<connect gate="A" pin="DIM" pad="2"/>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="HG" pad="6"/>
<connect gate="A" pin="HYS" pad="4"/>
<connect gate="A" pin="ILIM" pad="8"/>
<connect gate="A" pin="SNS" pad="3"/>
<connect gate="A" pin="VIN" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM3401MM"/>
<attribute name="OC_FARNELL" value="1495068"/>
<attribute name="OC_NEWARK" value="54M4678"/>
<attribute name="PACKAGE" value="MSOP-8"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3402HVMM" prefix="U">
<description>Constant Current Buck Regulator</description>
<gates>
<gate name="A" symbol="LM3402HVMM"/>
</gates>
<devices>
<device name="" package="SOP65P490X109-8N">
<connects>
<connect gate="A" pin="BOOT" pad="2"/>
<connect gate="A" pin="CS" pad="5"/>
<connect gate="A" pin="DIM" pad="3"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="RON" pad="6"/>
<connect gate="A" pin="SWITCH" pad="1"/>
<connect gate="A" pin="VCC" pad="7"/>
<connect gate="A" pin="VIN" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM3402HVMM"/>
<attribute name="OC_FARNELL" value="1290934"/>
<attribute name="OC_NEWARK" value="32M1047"/>
<attribute name="PACKAGE" value="SOP-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3402HVMR" prefix="U">
<description>Constant Current Buck Regulator</description>
<gates>
<gate name="A" symbol="LM3402HVMR"/>
</gates>
<devices>
<device name="" package="SOIC127P620X168-9N">
<connects>
<connect gate="A" pin="BOOT" pad="2"/>
<connect gate="A" pin="CS" pad="5"/>
<connect gate="A" pin="DIM" pad="3"/>
<connect gate="A" pin="EPAD" pad="9"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="RON" pad="6"/>
<connect gate="A" pin="SW" pad="1"/>
<connect gate="A" pin="VCC" pad="7"/>
<connect gate="A" pin="VIN" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM3402HVMR"/>
<attribute name="OC_FARNELL" value="1652390"/>
<attribute name="OC_NEWARK" value="50M8804"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3402MM" prefix="U">
<description>Constant Current Buck Regulator</description>
<gates>
<gate name="A" symbol="LM3402MM"/>
</gates>
<devices>
<device name="" package="SOP65P490X109-8N">
<connects>
<connect gate="A" pin="BOOT" pad="2"/>
<connect gate="A" pin="CS" pad="5"/>
<connect gate="A" pin="DIM" pad="3"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="RON" pad="6"/>
<connect gate="A" pin="SWITCH" pad="1"/>
<connect gate="A" pin="VCC" pad="7"/>
<connect gate="A" pin="VIN" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM3402MM"/>
<attribute name="OC_FARNELL" value="1290935"/>
<attribute name="OC_NEWARK" value="32M1049"/>
<attribute name="PACKAGE" value="SOP-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3402MR" prefix="U">
<description>Constant Current Buck Regulator</description>
<gates>
<gate name="A" symbol="LM3402MR"/>
</gates>
<devices>
<device name="" package="SOIC127P620X168-9N">
<connects>
<connect gate="A" pin="BOOT" pad="2"/>
<connect gate="A" pin="CS" pad="5"/>
<connect gate="A" pin="DIM" pad="3"/>
<connect gate="A" pin="EPAD" pad="9"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="RON" pad="6"/>
<connect gate="A" pin="SW" pad="1"/>
<connect gate="A" pin="VCC" pad="7"/>
<connect gate="A" pin="VIN" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM3402MR"/>
<attribute name="OC_FARNELL" value="1564796"/>
<attribute name="OC_NEWARK" value="50M8805"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3404HVMA" prefix="U">
<description>Constant Current Buck Regulator</description>
<gates>
<gate name="A" symbol="LM3404HVMA"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="BOOT" pad="2"/>
<connect gate="A" pin="CS" pad="5"/>
<connect gate="A" pin="DIM" pad="3"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="RON" pad="6"/>
<connect gate="A" pin="SW" pad="1"/>
<connect gate="A" pin="VCC" pad="7"/>
<connect gate="A" pin="VIN" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM3404HVMA"/>
<attribute name="OC_FARNELL" value="1469165"/>
<attribute name="OC_NEWARK" value="32M1054"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3404MA" prefix="U">
<description>Constant Current Buck Regulator</description>
<gates>
<gate name="A" symbol="LM3404MA"/>
</gates>
<devices>
<device name="" package="SOIC127P620X175-8N">
<connects>
<connect gate="A" pin="BOOT" pad="2"/>
<connect gate="A" pin="CS" pad="5"/>
<connect gate="A" pin="DIM" pad="3"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="RON" pad="6"/>
<connect gate="A" pin="SW" pad="1"/>
<connect gate="A" pin="VCC" pad="7"/>
<connect gate="A" pin="VIN" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM3404MA"/>
<attribute name="OC_FARNELL" value="1320973"/>
<attribute name="OC_NEWARK" value="31M5395"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3405AXMK" prefix="U">
<description>Constant Current Buck LED Regulator</description>
<gates>
<gate name="A" symbol="LM3405AXMK"/>
</gates>
<devices>
<device name="" package="SOT95P285X100-6N">
<connects>
<connect gate="A" pin="BST" pad="1"/>
<connect gate="A" pin="EN/DIM" pad="4"/>
<connect gate="A" pin="FB" pad="3"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="SW" pad="6"/>
<connect gate="A" pin="VIN" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM3405AXMK"/>
<attribute name="OC_FARNELL" value="1675313"/>
<attribute name="OC_NEWARK" value="64M6991"/>
<attribute name="PACKAGE" value="SOT-6"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3405AXMY" prefix="U">
<description>Constant Current Buck LED Driver</description>
<gates>
<gate name="A" symbol="LM3405AXMY"/>
</gates>
<devices>
<device name="" package="SOP65P490X110-9N">
<connects>
<connect gate="A" pin="BOOST" pad="4"/>
<connect gate="A" pin="EN/DIM" pad="8"/>
<connect gate="A" pin="EPAD" pad="9"/>
<connect gate="A" pin="FB" pad="1"/>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="GND_2" pad="2"/>
<connect gate="A" pin="NC" pad="3"/>
<connect gate="A" pin="SW" pad="5"/>
<connect gate="A" pin="VIN" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM3405AXMY"/>
<attribute name="OC_FARNELL" value="1679649"/>
<attribute name="OC_NEWARK" value="19P7831"/>
<attribute name="PACKAGE" value="MSOP-8"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3405XMK" prefix="U">
<description>Constant Current Buck Regulator</description>
<gates>
<gate name="A" symbol="LM3405XMK"/>
</gates>
<devices>
<device name="" package="SOT95P285X100-6N">
<connects>
<connect gate="A" pin="BST" pad="1"/>
<connect gate="A" pin="EN/DIM" pad="4"/>
<connect gate="A" pin="FB" pad="3"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="SW" pad="6"/>
<connect gate="A" pin="VIN" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM3405XMK"/>
<attribute name="OC_FARNELL" value="1359697"/>
<attribute name="OC_NEWARK" value="32M1070"/>
<attribute name="PACKAGE" value="SOT-6"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3406HVMH" prefix="U">
<description>Constant Current Buck Regulator</description>
<gates>
<gate name="A" symbol="LM3406HVMH"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-15N">
<connects>
<connect gate="A" pin="BOOT" pad="3"/>
<connect gate="A" pin="COMP" pad="9"/>
<connect gate="A" pin="CS" pad="6"/>
<connect gate="A" pin="DIM" pad="8"/>
<connect gate="A" pin="EPAD" pad="15"/>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="NC" pad="4"/>
<connect gate="A" pin="RON" pad="10"/>
<connect gate="A" pin="SW" pad="2"/>
<connect gate="A" pin="SW_2" pad="1"/>
<connect gate="A" pin="VCC" pad="11"/>
<connect gate="A" pin="VIN" pad="13"/>
<connect gate="A" pin="VINS" pad="12"/>
<connect gate="A" pin="VIN_2" pad="14"/>
<connect gate="A" pin="VOUT" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM3406HVMH"/>
<attribute name="OC_FARNELL" value="1685410"/>
<attribute name="OC_NEWARK" value="08P3934"/>
<attribute name="PACKAGE" value="TSSOP-14"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3406MH" prefix="U">
<description>Constant Current Buck Regulator</description>
<gates>
<gate name="A" symbol="LM3406MH"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-15N">
<connects>
<connect gate="A" pin="BOOT" pad="3"/>
<connect gate="A" pin="COMP" pad="9"/>
<connect gate="A" pin="CS" pad="6"/>
<connect gate="A" pin="DIM" pad="8"/>
<connect gate="A" pin="EPAD" pad="15"/>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="NC" pad="4"/>
<connect gate="A" pin="RON" pad="10"/>
<connect gate="A" pin="SW" pad="2"/>
<connect gate="A" pin="SW_2" pad="1"/>
<connect gate="A" pin="VCC" pad="11"/>
<connect gate="A" pin="VIN" pad="13"/>
<connect gate="A" pin="VINS" pad="12"/>
<connect gate="A" pin="VIN_2" pad="14"/>
<connect gate="A" pin="VOUT" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM3406MH"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="08P3935"/>
<attribute name="PACKAGE" value="TSSOP-14"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3407MY" prefix="U">
<description>Buck Regulator</description>
<gates>
<gate name="A" symbol="LM3407MY"/>
</gates>
<devices>
<device name="" package="SOP65P490X110-9N">
<connects>
<connect gate="A" pin="DIM" pad="2"/>
<connect gate="A" pin="EN" pad="3"/>
<connect gate="A" pin="EPAD" pad="9"/>
<connect gate="A" pin="FS" pad="4"/>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="ISNS" pad="1"/>
<connect gate="A" pin="LX" pad="8"/>
<connect gate="A" pin="VCC" pad="6"/>
<connect gate="A" pin="VIN" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM3407MY"/>
<attribute name="OC_FARNELL" value="1555100"/>
<attribute name="OC_NEWARK" value="78M7735"/>
<attribute name="PACKAGE" value="MSOP-8"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3409HVMY" prefix="U">
<description>Buck Controller</description>
<gates>
<gate name="A" symbol="LM3409HVMY"/>
</gates>
<devices>
<device name="" package="SOP50P490X109-11N">
<connects>
<connect gate="A" pin="COFF" pad="4"/>
<connect gate="A" pin="CSN" pad="7"/>
<connect gate="A" pin="CSP" pad="8"/>
<connect gate="A" pin="EN" pad="3"/>
<connect gate="A" pin="EP" pad="11"/>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="IADJ" pad="2"/>
<connect gate="A" pin="PGATE" pad="6"/>
<connect gate="A" pin="UVLO" pad="1"/>
<connect gate="A" pin="VCC" pad="9"/>
<connect gate="A" pin="VIN" pad="10"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM3409HVMY"/>
<attribute name="OC_FARNELL" value="1778581"/>
<attribute name="OC_NEWARK" value="14R4585"/>
<attribute name="PACKAGE" value="SOP-10"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3409MY" prefix="U">
<description>Buck Controller</description>
<gates>
<gate name="A" symbol="LM3409MY"/>
</gates>
<devices>
<device name="" package="SOP50P490X109-11N">
<connects>
<connect gate="A" pin="COFF" pad="4"/>
<connect gate="A" pin="CSN" pad="7"/>
<connect gate="A" pin="CSP" pad="8"/>
<connect gate="A" pin="EN" pad="3"/>
<connect gate="A" pin="EP" pad="11"/>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="IADJ" pad="2"/>
<connect gate="A" pin="PGATE" pad="6"/>
<connect gate="A" pin="UVLO" pad="1"/>
<connect gate="A" pin="VCC" pad="9"/>
<connect gate="A" pin="VIN" pad="10"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM3409MY"/>
<attribute name="OC_FARNELL" value="1778582"/>
<attribute name="OC_NEWARK" value="14R4586"/>
<attribute name="PACKAGE" value="SOP-10"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3410XMF" prefix="U">
<description>Constant Current Boost and SEPIC LED Driver</description>
<gates>
<gate name="A" symbol="LM3410XMF"/>
</gates>
<devices>
<device name="" package="SOT95P285X120-5N">
<connects>
<connect gate="A" pin="DIM" pad="4"/>
<connect gate="A" pin="FB" pad="3"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="SW" pad="1"/>
<connect gate="A" pin="VIN" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM3410XMF"/>
<attribute name="OC_FARNELL" value="1685357"/>
<attribute name="OC_NEWARK" value="75M6032"/>
<attribute name="PACKAGE" value="SOT-5"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3410XMY" prefix="U">
<description>Constant Current Boost and SEPIC LED Driver</description>
<gates>
<gate name="A" symbol="LM3410XMY"/>
</gates>
<devices>
<device name="" package="SOP65P490X110-9N">
<connects>
<connect gate="A" pin="AGND" pad="6"/>
<connect gate="A" pin="DIM" pad="4"/>
<connect gate="A" pin="EPAD" pad="9"/>
<connect gate="A" pin="FB" pad="5"/>
<connect gate="A" pin="NC" pad="1"/>
<connect gate="A" pin="NC_2" pad="8"/>
<connect gate="A" pin="PGND" pad="2"/>
<connect gate="A" pin="SW" pad="7"/>
<connect gate="A" pin="VIN" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM3410XMY"/>
<attribute name="OC_FARNELL" value="1685358"/>
<attribute name="OC_NEWARK" value="75M6033"/>
<attribute name="PACKAGE" value="MSOP-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3410XSD" prefix="U">
<description>SEPIC LED Driver</description>
<gates>
<gate name="A" symbol="LM3410XSD"/>
</gates>
<devices>
<device name="" package="DFN300X300X80-7N">
<connects>
<connect gate="A" pin="AGND" pad="5"/>
<connect gate="A" pin="DIM" pad="3"/>
<connect gate="A" pin="EPAD" pad="7"/>
<connect gate="A" pin="FB" pad="4"/>
<connect gate="A" pin="PGND" pad="1"/>
<connect gate="A" pin="SW" pad="6"/>
<connect gate="A" pin="VIN" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM3410XSD"/>
<attribute name="OC_FARNELL" value="1552436"/>
<attribute name="OC_NEWARK" value="94M8003"/>
<attribute name="PACKAGE" value="DFN-6"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3410YMF" prefix="U">
<description>Constant Current Boost and SEPIC LED Driver</description>
<gates>
<gate name="A" symbol="LM3410YMF"/>
</gates>
<devices>
<device name="" package="SOT95P285X120-5N">
<connects>
<connect gate="A" pin="DIM" pad="4"/>
<connect gate="A" pin="FB" pad="3"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="SW" pad="1"/>
<connect gate="A" pin="VIN" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM3410YMF"/>
<attribute name="OC_FARNELL" value="1685359"/>
<attribute name="OC_NEWARK" value="75M6034"/>
<attribute name="PACKAGE" value="SOT-5"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3410YMY" prefix="U">
<description>Constant Current Boost and SEPIC LED Driver</description>
<gates>
<gate name="A" symbol="LM3410YMY"/>
</gates>
<devices>
<device name="" package="SOP65P490X110-9N">
<connects>
<connect gate="A" pin="AGND" pad="6"/>
<connect gate="A" pin="DIM" pad="4"/>
<connect gate="A" pin="EPAD" pad="9"/>
<connect gate="A" pin="FB" pad="5"/>
<connect gate="A" pin="NC" pad="1"/>
<connect gate="A" pin="NC_2" pad="8"/>
<connect gate="A" pin="PGND" pad="2"/>
<connect gate="A" pin="SW" pad="7"/>
<connect gate="A" pin="VIN" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM3410YMY"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="75M6035"/>
<attribute name="PACKAGE" value="MSOP-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3410YSD" prefix="U">
<description>Constant Current Boost and SEPIC LED Driver</description>
<gates>
<gate name="A" symbol="LM3410YSD"/>
</gates>
<devices>
<device name="" package="DFN300X300X80-7N">
<connects>
<connect gate="A" pin="AGND" pad="5"/>
<connect gate="A" pin="DIM" pad="3"/>
<connect gate="A" pin="EPAD" pad="7"/>
<connect gate="A" pin="FB" pad="4"/>
<connect gate="A" pin="PGND" pad="1"/>
<connect gate="A" pin="SW" pad="6"/>
<connect gate="A" pin="VIN" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM3410YSD"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="78M7737"/>
<attribute name="PACKAGE" value="DFN-6"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3421MH" prefix="U">
<description>N-Channel Controllers for Constant Current LED Drivers</description>
<gates>
<gate name="A" symbol="LM3421MH"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-17N">
<connects>
<connect gate="A" pin="AGND" pad="6"/>
<connect gate="A" pin="COMP" pad="3"/>
<connect gate="A" pin="CSH" pad="4"/>
<connect gate="A" pin="DDRV" pad="9"/>
<connect gate="A" pin="EN" pad="2"/>
<connect gate="A" pin="EPAD" pad="17"/>
<connect gate="A" pin="GATE" pad="11"/>
<connect gate="A" pin="HSN" pad="16"/>
<connect gate="A" pin="HSP" pad="15"/>
<connect gate="A" pin="IS" pad="13"/>
<connect gate="A" pin="NDIM" pad="8"/>
<connect gate="A" pin="OVP" pad="7"/>
<connect gate="A" pin="PGND" pad="10"/>
<connect gate="A" pin="RCT" pad="5"/>
<connect gate="A" pin="RPD" pad="14"/>
<connect gate="A" pin="VCC" pad="12"/>
<connect gate="A" pin="VIN" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM3421MH"/>
<attribute name="OC_FARNELL" value="1643506"/>
<attribute name="OC_NEWARK" value="01P0823"/>
<attribute name="PACKAGE" value="TSSOP-16"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3423MH" prefix="U">
<description>N-Channel Controllers for Constant Current LED Drivers</description>
<gates>
<gate name="A" symbol="LM3423MH"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-17N">
<connects>
<connect gate="A" pin="AGND" pad="6"/>
<connect gate="A" pin="COMP" pad="3"/>
<connect gate="A" pin="CSH" pad="4"/>
<connect gate="A" pin="DDRV" pad="9"/>
<connect gate="A" pin="EN" pad="2"/>
<connect gate="A" pin="EPAD" pad="17"/>
<connect gate="A" pin="GATE" pad="11"/>
<connect gate="A" pin="HSN" pad="16"/>
<connect gate="A" pin="HSP" pad="15"/>
<connect gate="A" pin="IS" pad="13"/>
<connect gate="A" pin="NDIM" pad="8"/>
<connect gate="A" pin="OVP" pad="7"/>
<connect gate="A" pin="PGND" pad="10"/>
<connect gate="A" pin="RCT" pad="5"/>
<connect gate="A" pin="RPD" pad="14"/>
<connect gate="A" pin="VCC" pad="12"/>
<connect gate="A" pin="VIN" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM3423MH"/>
<attribute name="OC_FARNELL" value="1643507"/>
<attribute name="OC_NEWARK" value="01P0824"/>
<attribute name="PACKAGE" value="TSSOP-16"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3424MH" prefix="U">
<description>Constant Current N-Channel Controller</description>
<gates>
<gate name="A" symbol="LM3424MH"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-21N">
<connects>
<connect gate="A" pin="COMP" pad="3"/>
<connect gate="A" pin="CSH" pad="4"/>
<connect gate="A" pin="DAP" pad="21"/>
<connect gate="A" pin="DDRV" pad="13"/>
<connect gate="A" pin="EN" pad="2"/>
<connect gate="A" pin="GATE" pad="15"/>
<connect gate="A" pin="GND" pad="14"/>
<connect gate="A" pin="HSN" pad="19"/>
<connect gate="A" pin="HSP" pad="20"/>
<connect gate="A" pin="IS" pad="17"/>
<connect gate="A" pin="NDIM" pad="6"/>
<connect gate="A" pin="OVP" pad="12"/>
<connect gate="A" pin="RT" pad="5"/>
<connect gate="A" pin="SLOPE" pad="18"/>
<connect gate="A" pin="SS" pad="7"/>
<connect gate="A" pin="TGAIN" pad="8"/>
<connect gate="A" pin="TREF" pad="10"/>
<connect gate="A" pin="TSENSE" pad="9"/>
<connect gate="A" pin="VCC" pad="16"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="VS" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM3424MH"/>
<attribute name="OC_FARNELL" value="1778583"/>
<attribute name="OC_NEWARK" value="27R1775"/>
<attribute name="PACKAGE" value="SOP-20"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3424QMH">
<description>Constant Current N-Channel Controller</description>
<gates>
<gate name="A" symbol="LM3424QMH"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-21N">
<connects>
<connect gate="A" pin="COMP" pad="3"/>
<connect gate="A" pin="CSH" pad="4"/>
<connect gate="A" pin="DDRV" pad="13"/>
<connect gate="A" pin="EN" pad="2"/>
<connect gate="A" pin="EPAD" pad="21"/>
<connect gate="A" pin="GATE" pad="15"/>
<connect gate="A" pin="GND" pad="14"/>
<connect gate="A" pin="HSN" pad="19"/>
<connect gate="A" pin="HSP" pad="20"/>
<connect gate="A" pin="IS" pad="17"/>
<connect gate="A" pin="NDIM" pad="6"/>
<connect gate="A" pin="OVP" pad="12"/>
<connect gate="A" pin="RT" pad="5"/>
<connect gate="A" pin="SLOPE" pad="18"/>
<connect gate="A" pin="SS" pad="7"/>
<connect gate="A" pin="TGAIN" pad="8"/>
<connect gate="A" pin="TREF" pad="10"/>
<connect gate="A" pin="TSENSE" pad="9"/>
<connect gate="A" pin="VCC" pad="16"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="VS" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM3424QMH"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="55R3987"/>
<attribute name="PACKAGE" value="TSSOP-20"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3429MH" prefix="U">
<description>N-Channel Controller for Constant Current LED Drivers</description>
<gates>
<gate name="A" symbol="LM3429MH"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-15N">
<connects>
<connect gate="A" pin="AGND" pad="5"/>
<connect gate="A" pin="COMP" pad="2"/>
<connect gate="A" pin="CSH" pad="3"/>
<connect gate="A" pin="DAP" pad="15"/>
<connect gate="A" pin="GATE" pad="10"/>
<connect gate="A" pin="HSN" pad="14"/>
<connect gate="A" pin="HSP" pad="13"/>
<connect gate="A" pin="IS" pad="12"/>
<connect gate="A" pin="NC" pad="8"/>
<connect gate="A" pin="NDIM" pad="7"/>
<connect gate="A" pin="OVP" pad="6"/>
<connect gate="A" pin="PGND" pad="9"/>
<connect gate="A" pin="RCT" pad="4"/>
<connect gate="A" pin="VCC" pad="11"/>
<connect gate="A" pin="VIN" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM3429MH"/>
<attribute name="OC_FARNELL" value="1778585"/>
<attribute name="OC_NEWARK" value="55R1716"/>
<attribute name="PACKAGE" value="SOP-14"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3430SD" prefix="U">
<description>Boost Controller for LED Backlighting</description>
<gates>
<gate name="A" symbol="LM3430SD"/>
</gates>
<devices>
<device name="" package="DFN300X300X80-13N">
<connects>
<connect gate="A" pin="COMP" pad="4"/>
<connect gate="A" pin="CS" pad="9"/>
<connect gate="A" pin="EPAD" pad="13"/>
<connect gate="A" pin="FB" pad="3"/>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="NC" pad="12"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="RT/SYNC" pad="10"/>
<connect gate="A" pin="SS" pad="11"/>
<connect gate="A" pin="UVLO" pad="8"/>
<connect gate="A" pin="VCC" pad="5"/>
<connect gate="A" pin="VDHC" pad="1"/>
<connect gate="A" pin="VIN" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM3430SD"/>
<attribute name="OC_FARNELL" value="1325424"/>
<attribute name="OC_NEWARK" value="32M1075"/>
<attribute name="PACKAGE" value="DFN-12"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3431AMH" prefix="U">
<description>3-Channel Constant Current LED Driver</description>
<gates>
<gate name="A" symbol="LM3431AMH"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-29N">
<connects>
<connect gate="A" pin="AFB" pad="14"/>
<connect gate="A" pin="CFB" pad="17"/>
<connect gate="A" pin="COMP" pad="11"/>
<connect gate="A" pin="CS" pad="5"/>
<connect gate="A" pin="DIM" pad="27"/>
<connect gate="A" pin="DLY" pad="16"/>
<connect gate="A" pin="EN" pad="28"/>
<connect gate="A" pin="EPAD" pad="29"/>
<connect gate="A" pin="FF" pad="8"/>
<connect gate="A" pin="ILIM" pad="6"/>
<connect gate="A" pin="LEDOFF" pad="19"/>
<connect gate="A" pin="LG" pad="4"/>
<connect gate="A" pin="MODE/F" pad="7"/>
<connect gate="A" pin="NDRV1" pad="25"/>
<connect gate="A" pin="NDRV2" pad="23"/>
<connect gate="A" pin="NDRV3" pad="21"/>
<connect gate="A" pin="PGND" pad="2"/>
<connect gate="A" pin="REF" pad="10"/>
<connect gate="A" pin="REFIN" pad="12"/>
<connect gate="A" pin="RT" pad="9"/>
<connect gate="A" pin="SC" pad="18"/>
<connect gate="A" pin="SGND" pad="13"/>
<connect gate="A" pin="SNS1" pad="24"/>
<connect gate="A" pin="SNS2" pad="22"/>
<connect gate="A" pin="SNS3" pad="20"/>
<connect gate="A" pin="SS/SH" pad="15"/>
<connect gate="A" pin="THM" pad="26"/>
<connect gate="A" pin="VCC" pad="3"/>
<connect gate="A" pin="VIN" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM3431AMH"/>
<attribute name="OC_FARNELL" value="1535364"/>
<attribute name="OC_NEWARK" value="71M0341"/>
<attribute name="PACKAGE" value="TSSOP-28"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3431AQMH" prefix="U">
<description>3-Channel Constant Current LED Driver</description>
<gates>
<gate name="A" symbol="LM3431AQMH"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-29N">
<connects>
<connect gate="A" pin="AFB" pad="14"/>
<connect gate="A" pin="CFB" pad="17"/>
<connect gate="A" pin="COMP" pad="12"/>
<connect gate="A" pin="CS" pad="5"/>
<connect gate="A" pin="DIM" pad="27"/>
<connect gate="A" pin="DLY" pad="16"/>
<connect gate="A" pin="EN" pad="28"/>
<connect gate="A" pin="EPAD" pad="29"/>
<connect gate="A" pin="FF" pad="8"/>
<connect gate="A" pin="ILIM" pad="6"/>
<connect gate="A" pin="LEDOFF" pad="19"/>
<connect gate="A" pin="LG" pad="4"/>
<connect gate="A" pin="MODE/F" pad="7"/>
<connect gate="A" pin="NDRV1" pad="25"/>
<connect gate="A" pin="NDRV2" pad="23"/>
<connect gate="A" pin="NDRV3" pad="21"/>
<connect gate="A" pin="PGND" pad="2"/>
<connect gate="A" pin="REF" pad="10"/>
<connect gate="A" pin="REFIN" pad="11"/>
<connect gate="A" pin="RT" pad="9"/>
<connect gate="A" pin="SC" pad="18"/>
<connect gate="A" pin="SGND" pad="13"/>
<connect gate="A" pin="SNS1" pad="24"/>
<connect gate="A" pin="SNS2" pad="22"/>
<connect gate="A" pin="SNS3" pad="20"/>
<connect gate="A" pin="SS/SH" pad="15"/>
<connect gate="A" pin="THM" pad="26"/>
<connect gate="A" pin="VCC" pad="3"/>
<connect gate="A" pin="VIN" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM3431AQMH"/>
<attribute name="OC_FARNELL" value="1865998"/>
<attribute name="OC_NEWARK" value="55R3994"/>
<attribute name="PACKAGE" value="TSSOP-28"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3431MH" prefix="U">
<description>3-Channel Constant Current LED Driver</description>
<gates>
<gate name="A" symbol="LM3431MH"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-29N">
<connects>
<connect gate="A" pin="AFB" pad="14"/>
<connect gate="A" pin="CFB" pad="17"/>
<connect gate="A" pin="COMP" pad="12"/>
<connect gate="A" pin="CS" pad="5"/>
<connect gate="A" pin="DIM" pad="27"/>
<connect gate="A" pin="DLY" pad="16"/>
<connect gate="A" pin="EN" pad="28"/>
<connect gate="A" pin="EPAD" pad="29"/>
<connect gate="A" pin="FF" pad="8"/>
<connect gate="A" pin="ILIM" pad="6"/>
<connect gate="A" pin="LEDOFF" pad="19"/>
<connect gate="A" pin="LG" pad="4"/>
<connect gate="A" pin="MODE/F" pad="7"/>
<connect gate="A" pin="NDRV1" pad="25"/>
<connect gate="A" pin="NDRV2" pad="23"/>
<connect gate="A" pin="NDRV3" pad="21"/>
<connect gate="A" pin="PGND" pad="2"/>
<connect gate="A" pin="REF" pad="10"/>
<connect gate="A" pin="REFIN" pad="11"/>
<connect gate="A" pin="RT" pad="9"/>
<connect gate="A" pin="SC" pad="18"/>
<connect gate="A" pin="SGND" pad="13"/>
<connect gate="A" pin="SNS1" pad="24"/>
<connect gate="A" pin="SNS2" pad="22"/>
<connect gate="A" pin="SNS3" pad="20"/>
<connect gate="A" pin="SS/SH" pad="15"/>
<connect gate="A" pin="THM" pad="26"/>
<connect gate="A" pin="VCC" pad="3"/>
<connect gate="A" pin="VIN" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM3431MH"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="71M0342"/>
<attribute name="PACKAGE" value="TSSOP-28"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3431QMH" prefix="U">
<description>3-Channel Constant Current LED Driver</description>
<gates>
<gate name="A" symbol="LM3431QMH"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-29N">
<connects>
<connect gate="A" pin="AFB" pad="14"/>
<connect gate="A" pin="CFB" pad="17"/>
<connect gate="A" pin="COMP" pad="12"/>
<connect gate="A" pin="CS" pad="5"/>
<connect gate="A" pin="DIM" pad="27"/>
<connect gate="A" pin="DLY" pad="16"/>
<connect gate="A" pin="EN" pad="28"/>
<connect gate="A" pin="EPAD" pad="29"/>
<connect gate="A" pin="FF" pad="8"/>
<connect gate="A" pin="ILIM" pad="6"/>
<connect gate="A" pin="LEDOFF" pad="19"/>
<connect gate="A" pin="LG" pad="4"/>
<connect gate="A" pin="MODE/F" pad="7"/>
<connect gate="A" pin="NDRV1" pad="25"/>
<connect gate="A" pin="NDRV2" pad="23"/>
<connect gate="A" pin="NDRV3" pad="21"/>
<connect gate="A" pin="PGND" pad="2"/>
<connect gate="A" pin="REF" pad="10"/>
<connect gate="A" pin="REFIN" pad="11"/>
<connect gate="A" pin="RT" pad="9"/>
<connect gate="A" pin="SC" pad="18"/>
<connect gate="A" pin="SGND" pad="13"/>
<connect gate="A" pin="SNS1" pad="24"/>
<connect gate="A" pin="SNS2" pad="22"/>
<connect gate="A" pin="SNS3" pad="20"/>
<connect gate="A" pin="SS/SH" pad="15"/>
<connect gate="A" pin="THM" pad="26"/>
<connect gate="A" pin="VCC" pad="3"/>
<connect gate="A" pin="VIN" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM3431QMH"/>
<attribute name="OC_FARNELL" value="1865999"/>
<attribute name="OC_NEWARK" value="55R3996"/>
<attribute name="PACKAGE" value="TSSOP-28"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3432MH" prefix="U">
<description>6-Channel Current Regulator</description>
<gates>
<gate name="A" symbol="LM3432MH"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-29N">
<connects>
<connect gate="A" pin="AGND" pad="7"/>
<connect gate="A" pin="CDHC" pad="8"/>
<connect gate="A" pin="DIM" pad="12"/>
<connect gate="A" pin="EN" pad="10"/>
<connect gate="A" pin="EPAD" pad="29"/>
<connect gate="A" pin="FAULTB" pad="13"/>
<connect gate="A" pin="IOUT1" pad="25"/>
<connect gate="A" pin="IOUT2" pad="23"/>
<connect gate="A" pin="IOUT3" pad="21"/>
<connect gate="A" pin="IOUT4" pad="19"/>
<connect gate="A" pin="IOUT5" pad="17"/>
<connect gate="A" pin="IOUT6" pad="15"/>
<connect gate="A" pin="IREF" pad="6"/>
<connect gate="A" pin="MODE" pad="11"/>
<connect gate="A" pin="NC" pad="2"/>
<connect gate="A" pin="NC_2" pad="24"/>
<connect gate="A" pin="NC_3" pad="22"/>
<connect gate="A" pin="NC_4" pad="26"/>
<connect gate="A" pin="NC_5" pad="20"/>
<connect gate="A" pin="NC_6" pad="18"/>
<connect gate="A" pin="NC_7" pad="16"/>
<connect gate="A" pin="NC_8" pad="4"/>
<connect gate="A" pin="NC_9" pad="3"/>
<connect gate="A" pin="OTMB" pad="14"/>
<connect gate="A" pin="PGND" pad="28"/>
<connect gate="A" pin="PGND_2" pad="27"/>
<connect gate="A" pin="VCC" pad="5"/>
<connect gate="A" pin="VDHC" pad="9"/>
<connect gate="A" pin="VIN" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM3432MH"/>
<attribute name="OC_FARNELL" value="1778586"/>
<attribute name="OC_NEWARK" value="64M6994"/>
<attribute name="PACKAGE" value="TSSOP-28"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3433SQ" prefix="U">
<description>High Brightness LED Driver</description>
<gates>
<gate name="A" symbol="LM3433SQ"/>
</gates>
<devices>
<device name="" package="QFN50P400X400X80-25N">
<connects>
<connect gate="A" pin="ADJ" pad="2"/>
<connect gate="A" pin="BST" pad="16"/>
<connect gate="A" pin="BST2" pad="21"/>
<connect gate="A" pin="CGND" pad="6"/>
<connect gate="A" pin="COMP" pad="8"/>
<connect gate="A" pin="CSN" pad="23"/>
<connect gate="A" pin="CSP" pad="24"/>
<connect gate="A" pin="DIM" pad="4"/>
<connect gate="A" pin="DIMO" pad="20"/>
<connect gate="A" pin="DIMR" pad="19"/>
<connect gate="A" pin="EN" pad="3"/>
<connect gate="A" pin="EPAD" pad="25"/>
<connect gate="A" pin="HO" pad="17"/>
<connect gate="A" pin="HS" pad="18"/>
<connect gate="A" pin="LO" pad="14"/>
<connect gate="A" pin="LS" pad="13"/>
<connect gate="A" pin="NC" pad="22"/>
<connect gate="A" pin="NC_2" pad="9"/>
<connect gate="A" pin="NC_3" pad="11"/>
<connect gate="A" pin="NC_4" pad="12"/>
<connect gate="A" pin="SS" pad="10"/>
<connect gate="A" pin="TON" pad="1"/>
<connect gate="A" pin="VCC" pad="15"/>
<connect gate="A" pin="VEE" pad="7"/>
<connect gate="A" pin="VIN" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM3433SQ"/>
<attribute name="OC_FARNELL" value="1643508"/>
<attribute name="OC_NEWARK" value="64M6996"/>
<attribute name="PACKAGE" value="QFN-24"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3445MM" prefix="U">
<description>Triac Dimmable Offline LED Driver</description>
<gates>
<gate name="A" symbol="LM3445MM"/>
</gates>
<devices>
<device name="" package="SOP50P490X109-10N">
<connects>
<connect gate="A" pin="ASNS" pad="1"/>
<connect gate="A" pin="BLDR" pad="10"/>
<connect gate="A" pin="COFF" pad="4"/>
<connect gate="A" pin="DIM" pad="3"/>
<connect gate="A" pin="FLTR1" pad="2"/>
<connect gate="A" pin="FLTR2" pad="5"/>
<connect gate="A" pin="GATE" pad="8"/>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="ISNS" pad="7"/>
<connect gate="A" pin="VCC" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM3445MM"/>
<attribute name="OC_FARNELL" value="1699377"/>
<attribute name="OC_NEWARK" value="56P4152"/>
<attribute name="PACKAGE" value="SOP-10"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM346M" prefix="U">
<description>Programmable Quad Operational Amplifiers</description>
<gates>
<gate name="A" symbol="LM346M"/>
</gates>
<devices>
<device name="" package="SOIC127P620X175-16N">
<connects>
<connect gate="A" pin="+INA" pad="3"/>
<connect gate="A" pin="+INB" pad="5"/>
<connect gate="A" pin="+INC" pad="12"/>
<connect gate="A" pin="+IND" pad="14"/>
<connect gate="A" pin="-INA" pad="2"/>
<connect gate="A" pin="-INB" pad="6"/>
<connect gate="A" pin="-INC" pad="11"/>
<connect gate="A" pin="-IND" pad="15"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="OUTC" pad="10"/>
<connect gate="A" pin="OUTD" pad="16"/>
<connect gate="A" pin="SET_A,B,D" pad="8"/>
<connect gate="A" pin="SET_C" pad="9"/>
<connect gate="A" pin="V+" pad="4"/>
<connect gate="A" pin="V-" pad="13"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM346M"/>
<attribute name="OC_FARNELL" value="1798363"/>
<attribute name="OC_NEWARK" value="75R2098"/>
<attribute name="PACKAGE" value="SOIC-16"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3475MF" prefix="U">
<description>Hysteretic PFET Buck Controller</description>
<gates>
<gate name="A" symbol="LM3475MF"/>
</gates>
<devices>
<device name="" package="SOT95P285X120-5N">
<connects>
<connect gate="A" pin="EN" pad="3"/>
<connect gate="A" pin="FB" pad="1"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="PGATE" pad="5"/>
<connect gate="A" pin="VIN" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM3475MF"/>
<attribute name="OC_FARNELL" value="1609188"/>
<attribute name="OC_NEWARK" value="12N2277"/>
<attribute name="PACKAGE" value="SOT-23-5"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3477MM" prefix="U">
<description>Switching Regulator</description>
<gates>
<gate name="A" symbol="LM3477MM"/>
</gates>
<devices>
<device name="" package="SOP65P490X110-8N">
<connects>
<connect gate="A" pin="CB" pad="7"/>
<connect gate="A" pin="COMP/~SD" pad="2"/>
<connect gate="A" pin="DR" pad="6"/>
<connect gate="A" pin="FB" pad="3"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="ISEN" pad="1"/>
<connect gate="A" pin="SW" pad="5"/>
<connect gate="A" pin="VIN" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM3477MM"/>
<attribute name="OC_FARNELL" value="9779191"/>
<attribute name="OC_NEWARK" value="41K4816"/>
<attribute name="PACKAGE" value="8-MSOP"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3478MM" prefix="U">
<description>N-Channel Controller for Switching Regulator</description>
<gates>
<gate name="A" symbol="LM3478MM"/>
</gates>
<devices>
<device name="" package="SOP65P490X110-8N">
<connects>
<connect gate="A" pin="AGND" pad="4"/>
<connect gate="A" pin="COMP" pad="2"/>
<connect gate="A" pin="DR" pad="6"/>
<connect gate="A" pin="FA/SD" pad="7"/>
<connect gate="A" pin="FB" pad="3"/>
<connect gate="A" pin="ISEN" pad="1"/>
<connect gate="A" pin="PGND" pad="5"/>
<connect gate="A" pin="VIN" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM3478MM"/>
<attribute name="OC_FARNELL" value="1312568"/>
<attribute name="OC_NEWARK" value="41K4818"/>
<attribute name="PACKAGE" value="8-MSOP"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3478QMM" prefix="U">
<description>Switching Regulator</description>
<gates>
<gate name="A" symbol="LM3478QMM"/>
</gates>
<devices>
<device name="" package="SOP65P490X109-8N">
<connects>
<connect gate="A" pin="AGND" pad="4"/>
<connect gate="A" pin="COMP" pad="2"/>
<connect gate="A" pin="DR" pad="6"/>
<connect gate="A" pin="FA/SD" pad="7"/>
<connect gate="A" pin="FB" pad="3"/>
<connect gate="A" pin="ISENS" pad="1"/>
<connect gate="A" pin="PGND" pad="5"/>
<connect gate="A" pin="VIN" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM3478QMM"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="07P5421"/>
<attribute name="PACKAGE" value="SOP-8"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3480IM3-12" prefix="U">
<description>Low-Dropout Linear Voltage</description>
<gates>
<gate name="A" symbol="LM3480IM3-12"/>
</gates>
<devices>
<device name="" package="SOT95P251X112-3N">
<connects>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM3480IM3-12"/>
<attribute name="OC_FARNELL" value="1469099"/>
<attribute name="OC_NEWARK" value="-"/>
<attribute name="PACKAGE" value="SOT-3"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3480IM3-15" prefix="U">
<description>Low-Dropout Linear Voltage</description>
<gates>
<gate name="A" symbol="LM3480IM3-15"/>
</gates>
<devices>
<device name="" package="SOT95P251X112-3N">
<connects>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM3480IM3-15"/>
<attribute name="OC_FARNELL" value="1469100"/>
<attribute name="OC_NEWARK" value="41K4824"/>
<attribute name="PACKAGE" value="SOT-3"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3480IM3-3.3" prefix="U">
<description>Low-Dropout Linear Voltage</description>
<gates>
<gate name="A" symbol="LM3480IM3-3.3"/>
</gates>
<devices>
<device name="" package="SOT95P251X112-3N">
<connects>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM3480IM3-3.3"/>
<attribute name="OC_FARNELL" value="1469102"/>
<attribute name="OC_NEWARK" value="41K4825"/>
<attribute name="PACKAGE" value="SOT-3"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3480IM3-5.0" prefix="U">
<description>Linear Voltage Regulator</description>
<gates>
<gate name="A" symbol="LM3480IM3-5.0"/>
</gates>
<devices>
<device name="" package="SOT95P263X110-3N">
<connects>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM3480IM3-50"/>
<attribute name="OC_FARNELL" value="3160634"/>
<attribute name="OC_NEWARK" value="83F3816"/>
<attribute name="PACKAGE" value="SOT-23-3"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3481MM" prefix="U">
<description>Switching Regulators</description>
<gates>
<gate name="A" symbol="LM3481MM"/>
</gates>
<devices>
<device name="" package="SOP50P490X110-10N">
<connects>
<connect gate="A" pin="AGND" pad="5"/>
<connect gate="A" pin="COMP" pad="3"/>
<connect gate="A" pin="DR" pad="8"/>
<connect gate="A" pin="FA/SYNC/SD" pad="6"/>
<connect gate="A" pin="FB" pad="4"/>
<connect gate="A" pin="ISEN" pad="1"/>
<connect gate="A" pin="PGND" pad="7"/>
<connect gate="A" pin="UVLO" pad="2"/>
<connect gate="A" pin="VCC" pad="9"/>
<connect gate="A" pin="VIN" pad="10"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM3481MM"/>
<attribute name="OC_FARNELL" value="1798320"/>
<attribute name="OC_NEWARK" value="73R9734"/>
<attribute name="PACKAGE" value="MSOP-10"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3485MM" prefix="U">
<description>Hysteretic PFET Buck Controller</description>
<gates>
<gate name="A" symbol="LM3485MM"/>
</gates>
<devices>
<device name="" package="SOP65P490X110-8N">
<connects>
<connect gate="A" pin="ADJ" pad="5"/>
<connect gate="A" pin="FB" pad="4"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="ISENSE" pad="1"/>
<connect gate="A" pin="NC" pad="3"/>
<connect gate="A" pin="PGATE" pad="7"/>
<connect gate="A" pin="PWRGND" pad="6"/>
<connect gate="A" pin="VIN" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM3485MM"/>
<attribute name="OC_FARNELL" value="1312569"/>
<attribute name="OC_NEWARK" value="41K4830"/>
<attribute name="PACKAGE" value="8-MSOP"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3488MM" prefix="U">
<description>Switching Regulators</description>
<gates>
<gate name="A" symbol="LM3488MM"/>
</gates>
<devices>
<device name="" package="SOP65P490X110-8N">
<connects>
<connect gate="A" pin="AGND" pad="4"/>
<connect gate="A" pin="COMP" pad="2"/>
<connect gate="A" pin="DR" pad="6"/>
<connect gate="A" pin="FA/SYNC/SD" pad="7"/>
<connect gate="A" pin="FB" pad="3"/>
<connect gate="A" pin="ISEN" pad="1"/>
<connect gate="A" pin="PGND" pad="5"/>
<connect gate="A" pin="VIN" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM3488MM"/>
<attribute name="OC_FARNELL" value="9778888"/>
<attribute name="OC_NEWARK" value="74C4157"/>
<attribute name="PACKAGE" value="8-MSOP"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3488QMM" prefix="U">
<description>Switching Regulator</description>
<gates>
<gate name="A" symbol="LM3488QMM"/>
</gates>
<devices>
<device name="" package="SOP65P490X109-8N">
<connects>
<connect gate="A" pin="AGND" pad="4"/>
<connect gate="A" pin="COMP" pad="2"/>
<connect gate="A" pin="DR" pad="6"/>
<connect gate="A" pin="FA/SYNC/SD" pad="7"/>
<connect gate="A" pin="FB" pad="3"/>
<connect gate="A" pin="ISENS" pad="1"/>
<connect gate="A" pin="PGND" pad="5"/>
<connect gate="A" pin="VIN" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM3488QMM"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="55R4006"/>
<attribute name="PACKAGE" value="SOP-8"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3489MM" prefix="U">
<description>Hysteretic PFET Buck Controller</description>
<gates>
<gate name="A" symbol="LM3489MM"/>
</gates>
<devices>
<device name="" package="SOP65P490X109-8N">
<connects>
<connect gate="A" pin="ADJ" pad="5"/>
<connect gate="A" pin="EN" pad="3"/>
<connect gate="A" pin="FB" pad="4"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="ISENSE" pad="1"/>
<connect gate="A" pin="PGATE" pad="7"/>
<connect gate="A" pin="PGND" pad="6"/>
<connect gate="A" pin="VIN" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM3489MM"/>
<attribute name="OC_FARNELL" value="1312570"/>
<attribute name="OC_NEWARK" value="99K2420"/>
<attribute name="PACKAGE" value="SOP-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3489QMM" prefix="U">
<description>Hysteretic PFET Buck Controller</description>
<gates>
<gate name="A" symbol="LM3489QMM"/>
</gates>
<devices>
<device name="" package="SOP65P490X109-8N">
<connects>
<connect gate="A" pin="ADJ" pad="5"/>
<connect gate="A" pin="EN" pad="3"/>
<connect gate="A" pin="FB" pad="4"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="ISENSE" pad="1"/>
<connect gate="A" pin="PGATE" pad="7"/>
<connect gate="A" pin="PGND" pad="6"/>
<connect gate="A" pin="VIN" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM3489QMM"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="55R4009"/>
<attribute name="PACKAGE" value="SOP-8"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM348M" prefix="U">
<description>Quad 741 Op Amps</description>
<gates>
<gate name="A" symbol="LM348M"/>
</gates>
<devices>
<device name="" package="SOIC127P620X175-14N">
<connects>
<connect gate="A" pin="+IN1" pad="3"/>
<connect gate="A" pin="+IN2" pad="5"/>
<connect gate="A" pin="+IN3" pad="10"/>
<connect gate="A" pin="+IN4" pad="12"/>
<connect gate="A" pin="-IN1" pad="2"/>
<connect gate="A" pin="-IN2" pad="6"/>
<connect gate="A" pin="-IN3" pad="9"/>
<connect gate="A" pin="-IN4" pad="13"/>
<connect gate="A" pin="OUT1" pad="1"/>
<connect gate="A" pin="OUT2" pad="7"/>
<connect gate="A" pin="OUT3" pad="8"/>
<connect gate="A" pin="OUT4" pad="14"/>
<connect gate="A" pin="V+" pad="4"/>
<connect gate="A" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM348M"/>
<attribute name="OC_FARNELL" value="9486976"/>
<attribute name="OC_NEWARK" value="-"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM34910SD" prefix="U">
<description>Step Down Switching Regulator</description>
<gates>
<gate name="A" symbol="LM34910SD"/>
</gates>
<devices>
<device name="" package="DFN400X400X80-11N">
<connects>
<connect gate="A" pin="BST" pad="2"/>
<connect gate="A" pin="EPAD" pad="11"/>
<connect gate="A" pin="FB" pad="6"/>
<connect gate="A" pin="ISEN" pad="3"/>
<connect gate="A" pin="RTN" pad="5"/>
<connect gate="A" pin="SD/RON" pad="8"/>
<connect gate="A" pin="SGND" pad="4"/>
<connect gate="A" pin="SS" pad="7"/>
<connect gate="A" pin="SW" pad="1"/>
<connect gate="A" pin="VCC" pad="9"/>
<connect gate="A" pin="VIN" pad="10"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM34910SD"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="65J5309"/>
<attribute name="PACKAGE" value="10-DFN"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM34917ATL" prefix="U">
<description>4V-75V VIN 2 SWITCH BUCK/BOOST</description>
<gates>
<gate name="A" symbol="LM34917ATL"/>
</gates>
<devices>
<device name="" package="BGA12N50P3X4_197X230X60">
<connects>
<connect gate="A" pin="BST" pad="D3"/>
<connect gate="A" pin="FB" pad="A3"/>
<connect gate="A" pin="ISEN" pad="B1"/>
<connect gate="A" pin="RON/SD" pad="B2"/>
<connect gate="A" pin="RTN" pad="A2"/>
<connect gate="A" pin="SGND" pad="A1"/>
<connect gate="A" pin="SS" pad="B3"/>
<connect gate="A" pin="SW" pad="D2"/>
<connect gate="A" pin="SW_2" pad="D1"/>
<connect gate="A" pin="VCC" pad="C3"/>
<connect gate="A" pin="VIN" pad="C2"/>
<connect gate="A" pin="VIN_2" pad="C1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM34917ATL"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="11N9225"/>
<attribute name="PACKAGE" value="12-WFBGA"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM34930TL" prefix="U">
<description>Switching Regulator</description>
<gates>
<gate name="A" symbol="LM34930TL"/>
</gates>
<devices>
<device name="" package="BGA12C50P3X4_207X176X67">
<connects>
<connect gate="A" pin="BST" pad="D3"/>
<connect gate="A" pin="FB" pad="A3"/>
<connect gate="A" pin="GND" pad="A1"/>
<connect gate="A" pin="ISEN" pad="B1"/>
<connect gate="A" pin="NOV" pad="A2"/>
<connect gate="A" pin="RT" pad="B2"/>
<connect gate="A" pin="SS" pad="B3"/>
<connect gate="A" pin="SW" pad="D2"/>
<connect gate="A" pin="SW_2" pad="D1"/>
<connect gate="A" pin="VCC" pad="C3"/>
<connect gate="A" pin="VIN" pad="C2"/>
<connect gate="A" pin="VIN_2" pad="C1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM34930TL"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="11N9227"/>
<attribute name="PACKAGE" value="BGA-12"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3495MTC" prefix="U">
<description>Emulated Peak Current Mode Buck Controller</description>
<gates>
<gate name="A" symbol="LM3495MTC"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-16N">
<connects>
<connect gate="A" pin="BOOST" pad="1"/>
<connect gate="A" pin="COMP/~SD" pad="11"/>
<connect gate="A" pin="CSL" pad="4"/>
<connect gate="A" pin="FB" pad="10"/>
<connect gate="A" pin="FREQ/SYNC" pad="8"/>
<connect gate="A" pin="HG" pad="2"/>
<connect gate="A" pin="ILIM" pad="5"/>
<connect gate="A" pin="LG" pad="15"/>
<connect gate="A" pin="PGND" pad="16"/>
<connect gate="A" pin="SGND" pad="12"/>
<connect gate="A" pin="SNS" pad="7"/>
<connect gate="A" pin="SW/CSH" pad="3"/>
<connect gate="A" pin="TRACK" pad="9"/>
<connect gate="A" pin="VIN" pad="13"/>
<connect gate="A" pin="VLIN5" pad="14"/>
<connect gate="A" pin="~FPWM" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM3495MTC"/>
<attribute name="OC_FARNELL" value="1286749"/>
<attribute name="OC_NEWARK" value="24M3503"/>
<attribute name="PACKAGE" value="TSSOP-16"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3500TL-16" prefix="U">
<description>IC LED DRVR WHT BCKLT 8-MICROSMD</description>
<gates>
<gate name="A" symbol="LM3500TL-16"/>
</gates>
<devices>
<device name="" package="BGA8C50PX50P3X3_192X192X60">
<connects>
<connect gate="A" pin="AGND" pad="A1"/>
<connect gate="A" pin="FB" pad="B3"/>
<connect gate="A" pin="GND" pad="C3"/>
<connect gate="A" pin="NC" pad="A3"/>
<connect gate="A" pin="SHDN" pad="A2"/>
<connect gate="A" pin="VIN" pad="B1"/>
<connect gate="A" pin="VOUT" pad="C1"/>
<connect gate="A" pin="VSW" pad="C2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM3500TL-16"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K4852"/>
<attribute name="PACKAGE" value="8-WFBGA"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3500TL-21" prefix="U">
<description>IC LED DRVR WHT BCKLT 8-MICROSMD</description>
<gates>
<gate name="A" symbol="LM3500TL-21"/>
</gates>
<devices>
<device name="" package="BGA8C50PX50P3X3_192X192X60">
<connects>
<connect gate="A" pin="AGND" pad="A1"/>
<connect gate="A" pin="FB" pad="B3"/>
<connect gate="A" pin="GND" pad="C3"/>
<connect gate="A" pin="NC" pad="A3"/>
<connect gate="A" pin="SHDN" pad="A2"/>
<connect gate="A" pin="VIN" pad="B1"/>
<connect gate="A" pin="VOUT" pad="C1"/>
<connect gate="A" pin="VSW" pad="C2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM3500TL-21"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K4853"/>
<attribute name="PACKAGE" value="8-WFBGA"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3501TL-16" prefix="U">
<description>IC LED DRVR WHT BCKLT 8-MICROSMD</description>
<gates>
<gate name="A" symbol="LM3501TL-16"/>
</gates>
<devices>
<device name="" package="BGA8C50PX50P3X3_192X192X60">
<connects>
<connect gate="A" pin="AGND" pad="A1"/>
<connect gate="A" pin="CNTRL" pad="A3"/>
<connect gate="A" pin="FB" pad="B3"/>
<connect gate="A" pin="GND" pad="C3"/>
<connect gate="A" pin="SHDN" pad="A2"/>
<connect gate="A" pin="VIN" pad="B1"/>
<connect gate="A" pin="VOUT" pad="C1"/>
<connect gate="A" pin="VSW" pad="C2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM3501TL-16"/>
<attribute name="OC_FARNELL" value="8238855"/>
<attribute name="OC_NEWARK" value="41K4856"/>
<attribute name="PACKAGE" value="8-WFBGA"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3501TL-21" prefix="U">
<description>IC LED DRVR WHT BCKLT 8-MICROSMD</description>
<gates>
<gate name="A" symbol="LM3501TL-21"/>
</gates>
<devices>
<device name="" package="BGA8C50PX50P3X3_192X192X60">
<connects>
<connect gate="A" pin="AGND" pad="A1"/>
<connect gate="A" pin="CNTRL" pad="A3"/>
<connect gate="A" pin="FB" pad="B3"/>
<connect gate="A" pin="GND" pad="C3"/>
<connect gate="A" pin="SHDN" pad="A2"/>
<connect gate="A" pin="VIN" pad="B1"/>
<connect gate="A" pin="VOUT" pad="C1"/>
<connect gate="A" pin="VSW" pad="C2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM3501TL-21"/>
<attribute name="OC_FARNELL" value="1675269"/>
<attribute name="OC_NEWARK" value="32M1083"/>
<attribute name="PACKAGE" value="8-WFBGA"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3502ITL-16" prefix="U">
<description>IC LED DRVR WHT BCKLT 10MICROSMD</description>
<gates>
<gate name="A" symbol="LM3502ITL-16"/>
</gates>
<devices>
<device name="" package="BGA10C50PX50P4X3_195X213X60">
<connects>
<connect gate="A" pin="AGND" pad="C3"/>
<connect gate="A" pin="CNTRL" pad="A1"/>
<connect gate="A" pin="EN1" pad="A2"/>
<connect gate="A" pin="EN2" pad="A3"/>
<connect gate="A" pin="FB" pad="B1"/>
<connect gate="A" pin="PGND" pad="D3"/>
<connect gate="A" pin="SW" pad="D2"/>
<connect gate="A" pin="VIN" pad="B3"/>
<connect gate="A" pin="VOUT1" pad="D1"/>
<connect gate="A" pin="VOUT2" pad="C1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM3502ITL-16"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="69K2456"/>
<attribute name="PACKAGE" value="10-WFBGA"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3502ITL-25" prefix="U">
<description>IC LED DRVR WHT BCKLT 10MICROSMD</description>
<gates>
<gate name="A" symbol="LM3502ITL-25"/>
</gates>
<devices>
<device name="" package="BGA10C50PX50P4X3_195X213X60">
<connects>
<connect gate="A" pin="AGND" pad="C3"/>
<connect gate="A" pin="CNTRL" pad="A1"/>
<connect gate="A" pin="EN1" pad="A2"/>
<connect gate="A" pin="EN2" pad="A3"/>
<connect gate="A" pin="FB" pad="B1"/>
<connect gate="A" pin="PGND" pad="D3"/>
<connect gate="A" pin="SW" pad="D2"/>
<connect gate="A" pin="VIN" pad="B3"/>
<connect gate="A" pin="VOUT1" pad="D1"/>
<connect gate="A" pin="VOUT2" pad="C1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM3502ITL-25"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="69K2458"/>
<attribute name="PACKAGE" value="10-WFBGA"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3502ITL-35" prefix="U">
<description>IC LED DRVR WHT BCKLT 10USMD</description>
<gates>
<gate name="A" symbol="LM3502ITL-35"/>
</gates>
<devices>
<device name="" package="BGA10C50PX50P4X3_195X213X60">
<connects>
<connect gate="A" pin="AGND" pad="C3"/>
<connect gate="A" pin="CNTRL" pad="A1"/>
<connect gate="A" pin="EN1" pad="A2"/>
<connect gate="A" pin="EN2" pad="A3"/>
<connect gate="A" pin="FB" pad="B1"/>
<connect gate="A" pin="PGND" pad="D3"/>
<connect gate="A" pin="SW" pad="D2"/>
<connect gate="A" pin="VIN" pad="B3"/>
<connect gate="A" pin="VOUT1" pad="D1"/>
<connect gate="A" pin="VOUT2" pad="C1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM3502ITL-35"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="69K2460"/>
<attribute name="PACKAGE" value="10-WFBGA"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3502ITL-44" prefix="U">
<description>IC LED DRVR WHT BCKLT 10MICROSMD</description>
<gates>
<gate name="A" symbol="LM3502ITL-44"/>
</gates>
<devices>
<device name="" package="BGA10C50PX50P4X3_195X213X60">
<connects>
<connect gate="A" pin="AGND" pad="C3"/>
<connect gate="A" pin="CNTRL" pad="A1"/>
<connect gate="A" pin="EN1" pad="A2"/>
<connect gate="A" pin="EN2" pad="A3"/>
<connect gate="A" pin="FB" pad="B1"/>
<connect gate="A" pin="PGND" pad="D3"/>
<connect gate="A" pin="SW" pad="D2"/>
<connect gate="A" pin="VIN" pad="B3"/>
<connect gate="A" pin="VOUT1" pad="D1"/>
<connect gate="A" pin="VOUT2" pad="C1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM3502ITL-44"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="69K2462"/>
<attribute name="PACKAGE" value="10-WFBGA"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3502SQ-16" prefix="U">
<description>IC, WHITE LED DRIVER, BOOST, LLP-10</description>
<gates>
<gate name="A" symbol="LM3502SQ-16"/>
</gates>
<devices>
<device name="" package="QFN50P400X400X80-17N">
<connects>
<connect gate="A" pin="AGND" pad="14"/>
<connect gate="A" pin="CNTRL" pad="9"/>
<connect gate="A" pin="EN1" pad="10"/>
<connect gate="A" pin="EN2" pad="12"/>
<connect gate="A" pin="EP" pad="17"/>
<connect gate="A" pin="FB" pad="7"/>
<connect gate="A" pin="NC" pad="11"/>
<connect gate="A" pin="NC_2" pad="1"/>
<connect gate="A" pin="NC_3" pad="8"/>
<connect gate="A" pin="NC_4" pad="5"/>
<connect gate="A" pin="PGND" pad="16"/>
<connect gate="A" pin="PGND_2" pad="15"/>
<connect gate="A" pin="SW" pad="3"/>
<connect gate="A" pin="SW_2" pad="2"/>
<connect gate="A" pin="VIN" pad="13"/>
<connect gate="A" pin="VOUT1" pad="4"/>
<connect gate="A" pin="VOUT2" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM3502SQ-16"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="69K2472"/>
<attribute name="PACKAGE" value="16-WFQFN"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3502SQ-25" prefix="U">
<description>IC,SMPS CONTROLLER,CURRENT-MODE,LLCC</description>
<gates>
<gate name="A" symbol="LM3502SQ-25"/>
</gates>
<devices>
<device name="" package="QFN50P400X400X80-17N">
<connects>
<connect gate="A" pin="AGND" pad="14"/>
<connect gate="A" pin="CNTRL" pad="9"/>
<connect gate="A" pin="EN1" pad="10"/>
<connect gate="A" pin="EN2" pad="12"/>
<connect gate="A" pin="EP" pad="17"/>
<connect gate="A" pin="FB" pad="7"/>
<connect gate="A" pin="NC" pad="11"/>
<connect gate="A" pin="NC_2" pad="1"/>
<connect gate="A" pin="NC_3" pad="8"/>
<connect gate="A" pin="NC_4" pad="5"/>
<connect gate="A" pin="PGND" pad="16"/>
<connect gate="A" pin="PGND_2" pad="15"/>
<connect gate="A" pin="SW" pad="3"/>
<connect gate="A" pin="SW_2" pad="2"/>
<connect gate="A" pin="VIN" pad="13"/>
<connect gate="A" pin="VOUT1" pad="4"/>
<connect gate="A" pin="VOUT2" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM3502SQ-25"/>
<attribute name="OC_FARNELL" value="1312573"/>
<attribute name="OC_NEWARK" value="69K2473"/>
<attribute name="PACKAGE" value="16-WFQFN"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3502SQ-35" prefix="U">
<description>IC, WHITE LED DRIVER, BOOST, LLP-10</description>
<gates>
<gate name="A" symbol="LM3502SQ-35"/>
</gates>
<devices>
<device name="" package="QFN50P400X400X80-17N">
<connects>
<connect gate="A" pin="AGND" pad="14"/>
<connect gate="A" pin="CNTRL" pad="9"/>
<connect gate="A" pin="EN1" pad="10"/>
<connect gate="A" pin="EN2" pad="12"/>
<connect gate="A" pin="EP" pad="17"/>
<connect gate="A" pin="FB" pad="7"/>
<connect gate="A" pin="NC" pad="11"/>
<connect gate="A" pin="NC_2" pad="1"/>
<connect gate="A" pin="NC_3" pad="8"/>
<connect gate="A" pin="NC_4" pad="5"/>
<connect gate="A" pin="PGND" pad="16"/>
<connect gate="A" pin="PGND_2" pad="15"/>
<connect gate="A" pin="SW" pad="3"/>
<connect gate="A" pin="SW_2" pad="2"/>
<connect gate="A" pin="VIN" pad="13"/>
<connect gate="A" pin="VOUT1" pad="4"/>
<connect gate="A" pin="VOUT2" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM3502SQ-35"/>
<attribute name="OC_FARNELL" value="1312574"/>
<attribute name="OC_NEWARK" value="69K2476"/>
<attribute name="PACKAGE" value="16-WFQFN"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3502SQ-44" prefix="U">
<description>IC, WHITE LED DRIVER, BOOST, LLP-10</description>
<gates>
<gate name="A" symbol="LM3502SQ-44"/>
</gates>
<devices>
<device name="" package="QFN50P400X400X80-17N">
<connects>
<connect gate="A" pin="AGND" pad="14"/>
<connect gate="A" pin="CNTRL" pad="9"/>
<connect gate="A" pin="EN1" pad="10"/>
<connect gate="A" pin="EN2" pad="12"/>
<connect gate="A" pin="EP" pad="17"/>
<connect gate="A" pin="FB" pad="7"/>
<connect gate="A" pin="NC" pad="11"/>
<connect gate="A" pin="NC_2" pad="1"/>
<connect gate="A" pin="NC_3" pad="8"/>
<connect gate="A" pin="NC_4" pad="5"/>
<connect gate="A" pin="PGND" pad="16"/>
<connect gate="A" pin="PGND_2" pad="15"/>
<connect gate="A" pin="SW" pad="3"/>
<connect gate="A" pin="SW_2" pad="2"/>
<connect gate="A" pin="VIN" pad="13"/>
<connect gate="A" pin="VOUT1" pad="4"/>
<connect gate="A" pin="VOUT2" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM3502SQ-44"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="69K2478"/>
<attribute name="PACKAGE" value="16-WFQFN"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3503ITL-16" prefix="U">
<description>IC, LED DRIVER, CONSTANT CURRENT, µSMD16</description>
<gates>
<gate name="A" symbol="LM3503ITL-16"/>
</gates>
<devices>
<device name="" package="BGA10C50PX50P4X3_195X213X60">
<connects>
<connect gate="A" pin="AGND" pad="C3"/>
<connect gate="A" pin="CNTRL" pad="A1"/>
<connect gate="A" pin="EN1" pad="A2"/>
<connect gate="A" pin="EN2" pad="A3"/>
<connect gate="A" pin="FB" pad="B1"/>
<connect gate="A" pin="PGND" pad="D3"/>
<connect gate="A" pin="SW" pad="D2"/>
<connect gate="A" pin="VIN" pad="B3"/>
<connect gate="A" pin="VOUT1" pad="D1"/>
<connect gate="A" pin="VOUT2" pad="C1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM3503ITL-16"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="69K2488"/>
<attribute name="PACKAGE" value="10-TuSMD"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3503ITL-25" prefix="U">
<description>C, LED DRIVER, CONSTANT CURRENT</description>
<gates>
<gate name="A" symbol="LM3503ITL-25"/>
</gates>
<devices>
<device name="" package="BGA10C50PX50P4X3_195X213X60">
<connects>
<connect gate="A" pin="AGND" pad="C3"/>
<connect gate="A" pin="CNTRL" pad="A1"/>
<connect gate="A" pin="EN1" pad="A2"/>
<connect gate="A" pin="EN2" pad="A3"/>
<connect gate="A" pin="FB" pad="B1"/>
<connect gate="A" pin="PGND" pad="D3"/>
<connect gate="A" pin="SW" pad="D2"/>
<connect gate="A" pin="VIN" pad="B3"/>
<connect gate="A" pin="VOUT1" pad="D1"/>
<connect gate="A" pin="VOUT2" pad="C1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM3503ITL-25"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="69K2490"/>
<attribute name="PACKAGE" value="10-WFBGA"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3503ITL-35" prefix="U">
<description>IC, LED DRIVER, CONSTANT CURRENT</description>
<gates>
<gate name="A" symbol="LM3503ITL-35"/>
</gates>
<devices>
<device name="" package="BGA10C50PX50P4X3_195X213X60">
<connects>
<connect gate="A" pin="AGND" pad="C3"/>
<connect gate="A" pin="CNTRL" pad="A1"/>
<connect gate="A" pin="EN1" pad="A2"/>
<connect gate="A" pin="EN2" pad="A3"/>
<connect gate="A" pin="FB" pad="B1"/>
<connect gate="A" pin="PGND" pad="D3"/>
<connect gate="A" pin="SW" pad="D2"/>
<connect gate="A" pin="VIN" pad="B3"/>
<connect gate="A" pin="VOUT1" pad="D1"/>
<connect gate="A" pin="VOUT2" pad="C1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM3503ITL-35"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="69K2492"/>
<attribute name="PACKAGE" value="10-WFBGA"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3503ITL-44" prefix="U">
<description>IC, LED DRIVER, CONSTANT CURRENT</description>
<gates>
<gate name="A" symbol="LM3503ITL-44"/>
</gates>
<devices>
<device name="" package="BGA10C50PX50P4X3_195X213X60">
<connects>
<connect gate="A" pin="AGND" pad="C3"/>
<connect gate="A" pin="CNTRL" pad="A1"/>
<connect gate="A" pin="EN1" pad="A2"/>
<connect gate="A" pin="EN2" pad="A3"/>
<connect gate="A" pin="FB" pad="B1"/>
<connect gate="A" pin="PGND" pad="D3"/>
<connect gate="A" pin="SW" pad="D2"/>
<connect gate="A" pin="VIN" pad="B3"/>
<connect gate="A" pin="VOUT1" pad="D1"/>
<connect gate="A" pin="VOUT2" pad="C1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM3503ITL-44"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="69K2494"/>
<attribute name="PACKAGE" value="10-WFBGA"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3503SQ-16" prefix="U">
<description>Dual-Display Constant Current LED Driver</description>
<gates>
<gate name="A" symbol="LM3503SQ-16"/>
</gates>
<devices>
<device name="" package="QFN50P400X400X80-13N">
<connects>
<connect gate="A" pin="AGND" pad="14"/>
<connect gate="A" pin="CNTRL" pad="9"/>
<connect gate="A" pin="EN1" pad="10"/>
<connect gate="A" pin="EN2" pad="12"/>
<connect gate="A" pin="FB" pad="7"/>
<connect gate="A" pin="HEAT_PAD" pad="17"/>
<connect gate="A" pin="NC" pad="11"/>
<connect gate="A" pin="NC_2" pad="1"/>
<connect gate="A" pin="NC_3" pad="8"/>
<connect gate="A" pin="NC_4" pad="5"/>
<connect gate="A" pin="PGND" pad="16"/>
<connect gate="A" pin="PGND_2" pad="15"/>
<connect gate="A" pin="SW" pad="3"/>
<connect gate="A" pin="SW_2" pad="2"/>
<connect gate="A" pin="VIN" pad="13"/>
<connect gate="A" pin="VOUT1" pad="4"/>
<connect gate="A" pin="VOUT2" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM3503SQ-16"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="69K2504"/>
<attribute name="PACKAGE" value="QFN-12"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3503SQ-25" prefix="U">
<description>Dual-Display Constant Current LED Driver</description>
<gates>
<gate name="A" symbol="LM3503SQ-25"/>
</gates>
<devices>
<device name="" package="QFN50P400X400X80-13N">
<connects>
<connect gate="A" pin="AGND" pad="14"/>
<connect gate="A" pin="CNTRL" pad="9"/>
<connect gate="A" pin="EN1" pad="10"/>
<connect gate="A" pin="EN2" pad="12"/>
<connect gate="A" pin="FB" pad="7"/>
<connect gate="A" pin="HEAT_PAD" pad="17"/>
<connect gate="A" pin="NC" pad="11"/>
<connect gate="A" pin="NC_2" pad="1"/>
<connect gate="A" pin="NC_3" pad="8"/>
<connect gate="A" pin="NC_4" pad="5"/>
<connect gate="A" pin="PGND" pad="16"/>
<connect gate="A" pin="PGND_2" pad="15"/>
<connect gate="A" pin="SW" pad="3"/>
<connect gate="A" pin="SW_2" pad="2"/>
<connect gate="A" pin="VIN" pad="13"/>
<connect gate="A" pin="VOUT1" pad="4"/>
<connect gate="A" pin="VOUT2" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM3503SQ-25"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="69K2506"/>
<attribute name="PACKAGE" value="QFN-12"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3503SQ-35" prefix="U">
<description>Dual-Display Constant Current LED Driver</description>
<gates>
<gate name="A" symbol="LM3503SQ-35"/>
</gates>
<devices>
<device name="" package="QFN50P400X400X80-13N">
<connects>
<connect gate="A" pin="AGND" pad="14"/>
<connect gate="A" pin="CNTRL" pad="9"/>
<connect gate="A" pin="EN1" pad="10"/>
<connect gate="A" pin="EN2" pad="12"/>
<connect gate="A" pin="FB" pad="7"/>
<connect gate="A" pin="HEAT_PAD" pad="17"/>
<connect gate="A" pin="NC" pad="11"/>
<connect gate="A" pin="NC_2" pad="1"/>
<connect gate="A" pin="NC_3" pad="8"/>
<connect gate="A" pin="NC_4" pad="5"/>
<connect gate="A" pin="PGND" pad="16"/>
<connect gate="A" pin="PGND_2" pad="15"/>
<connect gate="A" pin="SW" pad="3"/>
<connect gate="A" pin="SW_2" pad="2"/>
<connect gate="A" pin="VIN" pad="13"/>
<connect gate="A" pin="VOUT1" pad="4"/>
<connect gate="A" pin="VOUT2" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM3503SQ-35"/>
<attribute name="OC_FARNELL" value="1675301"/>
<attribute name="OC_NEWARK" value="55K6778"/>
<attribute name="PACKAGE" value="QFN-12"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3503SQ-44" prefix="U">
<description>Dual-Display Constant Current LED Driver</description>
<gates>
<gate name="A" symbol="LM3503SQ-44"/>
</gates>
<devices>
<device name="" package="QFN50P400X400X80-13N">
<connects>
<connect gate="A" pin="AGND" pad="14"/>
<connect gate="A" pin="CNTRL" pad="9"/>
<connect gate="A" pin="EN1" pad="10"/>
<connect gate="A" pin="EN2" pad="12"/>
<connect gate="A" pin="FB" pad="7"/>
<connect gate="A" pin="HEAT_PAD" pad="17"/>
<connect gate="A" pin="NC" pad="11"/>
<connect gate="A" pin="NC_2" pad="1"/>
<connect gate="A" pin="NC_3" pad="8"/>
<connect gate="A" pin="NC_4" pad="5"/>
<connect gate="A" pin="PGND" pad="16"/>
<connect gate="A" pin="PGND_2" pad="15"/>
<connect gate="A" pin="SW" pad="3"/>
<connect gate="A" pin="SW_2" pad="2"/>
<connect gate="A" pin="VIN" pad="13"/>
<connect gate="A" pin="VOUT1" pad="4"/>
<connect gate="A" pin="VOUT2" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM3503SQ-44"/>
<attribute name="OC_FARNELL" value="1312579"/>
<attribute name="OC_NEWARK" value="-"/>
<attribute name="PACKAGE" value="QFN-12"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3519MK-20" prefix="U">
<description>High Frequency Boost White LED Driver</description>
<gates>
<gate name="A" symbol="LM3519MK-20"/>
</gates>
<devices>
<device name="" package="SOT95P285X100-6N">
<connects>
<connect gate="A" pin="EN" pad="1"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="LED_RTN" pad="4"/>
<connect gate="A" pin="SW" pad="5"/>
<connect gate="A" pin="VIN" pad="6"/>
<connect gate="A" pin="VOUT" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM3519MK-20"/>
<attribute name="OC_FARNELL" value="1312717"/>
<attribute name="OC_NEWARK" value="79K7826"/>
<attribute name="PACKAGE" value="SOT23-6"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3525M-H" prefix="U">
<description>Single Port USB Power Switch</description>
<gates>
<gate name="A" symbol="LM3525M-H"/>
</gates>
<devices>
<device name="" package="SOIC127P620X175-8N">
<connects>
<connect gate="A" pin="EN" pad="1"/>
<connect gate="A" pin="FLAG" pad="2"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="IN" pad="7"/>
<connect gate="A" pin="NC" pad="4"/>
<connect gate="A" pin="NC_2" pad="5"/>
<connect gate="A" pin="OUT" pad="8"/>
<connect gate="A" pin="OUT_2" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM3525M-H"/>
<attribute name="OC_FARNELL" value="9486330"/>
<attribute name="OC_NEWARK" value="41K4863"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3525M-L" prefix="U">
<description>Single Port USB Power Switch</description>
<gates>
<gate name="A" symbol="LM3525M-L"/>
</gates>
<devices>
<device name="" package="SOIC127P620X175-8N">
<connects>
<connect gate="A" pin="FLAG" pad="2"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="IN" pad="7"/>
<connect gate="A" pin="NC" pad="4"/>
<connect gate="A" pin="NC_2" pad="5"/>
<connect gate="A" pin="OUT" pad="8"/>
<connect gate="A" pin="OUT_2" pad="6"/>
<connect gate="A" pin="~EN" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM3525M-L"/>
<attribute name="OC_FARNELL" value="9486348"/>
<attribute name="OC_NEWARK" value="41K4864"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3526M-H" prefix="U">
<description>Dual Port USB Power Switch</description>
<gates>
<gate name="A" symbol="LM3526M-H"/>
</gates>
<devices>
<device name="" package="SOIC127P640X175-8N">
<connects>
<connect gate="A" pin="ENA" pad="1"/>
<connect gate="A" pin="ENB" pad="4"/>
<connect gate="A" pin="FLAGA" pad="2"/>
<connect gate="A" pin="FLAGB" pad="3"/>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="IN" pad="7"/>
<connect gate="A" pin="OUTA" pad="8"/>
<connect gate="A" pin="OUTB" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM3526M-H"/>
<attribute name="OC_FARNELL" value="1469237"/>
<attribute name="OC_NEWARK" value="41K4867"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3526M-L" prefix="U">
<description>Dual Port USB Power Switch</description>
<gates>
<gate name="A" symbol="LM3526M-L"/>
</gates>
<devices>
<device name="" package="SOIC127P640X175-8N">
<connects>
<connect gate="A" pin="FLAGA" pad="2"/>
<connect gate="A" pin="FLAGB" pad="3"/>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="IN" pad="7"/>
<connect gate="A" pin="OUTA" pad="8"/>
<connect gate="A" pin="OUTB" pad="5"/>
<connect gate="A" pin="~ENA" pad="1"/>
<connect gate="A" pin="~ENB" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM3526M-L"/>
<attribute name="OC_FARNELL" value="1469238"/>
<attribute name="OC_NEWARK" value="41K4868"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3528TME" prefix="U">
<description>High Efficiency, Multi Display LED Driver</description>
<gates>
<gate name="A" symbol="LM3528TME"/>
</gates>
<devices>
<device name="" package="BGA12C3X4X40P_161X121X60">
<connects>
<connect gate="A" pin="GND" pad="D3"/>
<connect gate="A" pin="GPIO1" pad="B1"/>
<connect gate="A" pin="HWEN/PGEN/GPIO" pad="C1"/>
<connect gate="A" pin="IN" pad="C3"/>
<connect gate="A" pin="MAIN" pad="A2"/>
<connect gate="A" pin="OVP" pad="A1"/>
<connect gate="A" pin="SCL" pad="B2"/>
<connect gate="A" pin="SDA" pad="C2"/>
<connect gate="A" pin="SET" pad="B3"/>
<connect gate="A" pin="SUB/FB" pad="A3"/>
<connect gate="A" pin="SW" pad="D2"/>
<connect gate="A" pin="VIO" pad="D1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM3528TME"/>
<attribute name="OC_FARNELL" value="1871518"/>
<attribute name="OC_NEWARK" value="34P4844"/>
<attribute name="PACKAGE" value="BGA-12"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3544M-L" prefix="U">
<description>Quad Port USB Power Distribution Switch</description>
<gates>
<gate name="A" symbol="LM3544M-L"/>
</gates>
<devices>
<device name="" package="SOIC127P620X175-16N">
<connects>
<connect gate="A" pin="FLAG1" pad="16"/>
<connect gate="A" pin="FLAG2" pad="13"/>
<connect gate="A" pin="FLAG3" pad="12"/>
<connect gate="A" pin="FLAG4" pad="9"/>
<connect gate="A" pin="GND1" pad="1"/>
<connect gate="A" pin="GND2" pad="5"/>
<connect gate="A" pin="IN1" pad="2"/>
<connect gate="A" pin="IN2" pad="6"/>
<connect gate="A" pin="OUT1" pad="15"/>
<connect gate="A" pin="OUT2" pad="14"/>
<connect gate="A" pin="OUT3" pad="11"/>
<connect gate="A" pin="OUT4" pad="10"/>
<connect gate="A" pin="~EN1" pad="3"/>
<connect gate="A" pin="~EN2" pad="4"/>
<connect gate="A" pin="~EN3" pad="7"/>
<connect gate="A" pin="~EN4" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM3544M-L"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="74C4172"/>
<attribute name="PACKAGE" value="SOIC-16"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3551SD" prefix="U">
<description>1A White LED Driver</description>
<gates>
<gate name="A" symbol="LM3551SD"/>
</gates>
<devices>
<device name="" package="DFN400X400X80-15N">
<connects>
<connect gate="A" pin="AGND" pad="6"/>
<connect gate="A" pin="EPAD" pad="15"/>
<connect gate="A" pin="FB" pad="4"/>
<connect gate="A" pin="FET-F" pad="2"/>
<connect gate="A" pin="FET-T" pad="14"/>
<connect gate="A" pin="FTO" pad="12"/>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="GND_2" pad="1"/>
<connect gate="A" pin="OVP" pad="10"/>
<connect gate="A" pin="SD" pad="5"/>
<connect gate="A" pin="SS" pad="11"/>
<connect gate="A" pin="SW" pad="8"/>
<connect gate="A" pin="T/F" pad="13"/>
<connect gate="A" pin="VC" pad="3"/>
<connect gate="A" pin="VIN" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM3551SD"/>
<attribute name="OC_FARNELL" value="1312580"/>
<attribute name="OC_NEWARK" value="57K7414"/>
<attribute name="PACKAGE" value="DFN-14"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3552SD" prefix="U">
<description>1A White LED Driver</description>
<gates>
<gate name="A" symbol="LM3552SD"/>
</gates>
<devices>
<device name="" package="DFN400X400X80-15N">
<connects>
<connect gate="A" pin="AGND" pad="6"/>
<connect gate="A" pin="EN" pad="5"/>
<connect gate="A" pin="EPAD" pad="15"/>
<connect gate="A" pin="FB" pad="4"/>
<connect gate="A" pin="FET-F" pad="2"/>
<connect gate="A" pin="FET-T" pad="14"/>
<connect gate="A" pin="FTO" pad="12"/>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="GND_2" pad="1"/>
<connect gate="A" pin="OVP" pad="10"/>
<connect gate="A" pin="SS" pad="11"/>
<connect gate="A" pin="SW" pad="8"/>
<connect gate="A" pin="T/F" pad="13"/>
<connect gate="A" pin="VC" pad="3"/>
<connect gate="A" pin="VIN" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM3552SD"/>
<attribute name="OC_FARNELL" value="1312719"/>
<attribute name="OC_NEWARK" value="65K6206"/>
<attribute name="PACKAGE" value="DFN-14"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3553SD" prefix="U">
<description>Dual Flash LED Driver System</description>
<gates>
<gate name="A" symbol="LM3553SD"/>
</gates>
<devices>
<device name="" package="DFN300X300X80-13N">
<connects>
<connect gate="A" pin="D1" pad="2"/>
<connect gate="A" pin="D2" pad="11"/>
<connect gate="A" pin="EPAD" pad="13"/>
<connect gate="A" pin="FEN" pad="3"/>
<connect gate="A" pin="ISET" pad="1"/>
<connect gate="A" pin="M/F" pad="12"/>
<connect gate="A" pin="OVP" pad="6"/>
<connect gate="A" pin="SCL" pad="8"/>
<connect gate="A" pin="SDA" pad="10"/>
<connect gate="A" pin="SW" pad="5"/>
<connect gate="A" pin="TX" pad="7"/>
<connect gate="A" pin="VIN" pad="4"/>
<connect gate="A" pin="VIO" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM3553SD"/>
<attribute name="OC_FARNELL" value="1675343"/>
<attribute name="OC_NEWARK" value="84M8124"/>
<attribute name="PACKAGE" value="DFN-12"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3557SD-2" prefix="U">
<description>Step-Up Converter</description>
<gates>
<gate name="A" symbol="LM3557SD-2"/>
</gates>
<devices>
<device name="" package="DFN300X300X80-9N">
<connects>
<connect gate="A" pin="EN" pad="4"/>
<connect gate="A" pin="EPAD" pad="9"/>
<connect gate="A" pin="FB" pad="6"/>
<connect gate="A" pin="GND" pad="8"/>
<connect gate="A" pin="NC" pad="3"/>
<connect gate="A" pin="OVP" pad="5"/>
<connect gate="A" pin="SW1" pad="1"/>
<connect gate="A" pin="SW2" pad="7"/>
<connect gate="A" pin="VIN" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM3557SD-2"/>
<attribute name="OC_FARNELL" value="1312582"/>
<attribute name="OC_NEWARK" value="41K4879"/>
<attribute name="PACKAGE" value="DFN-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM358AM" prefix="U">
<description>Low Power Dual Operational Amplifiers</description>
<gates>
<gate name="A" symbol="LM358AM"/>
</gates>
<devices>
<device name="" package="SOIC127P620X175-8N">
<connects>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="NEGA" pad="2"/>
<connect gate="A" pin="NEGB" pad="6"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="POSA" pad="3"/>
<connect gate="A" pin="POSB" pad="5"/>
<connect gate="A" pin="V+" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM358AM"/>
<attribute name="OC_FARNELL" value="9486801"/>
<attribute name="OC_NEWARK" value="-"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM358AN" prefix="U">
<description>Low Power Dual Operational Amplifiers</description>
<gates>
<gate name="A" symbol="LM358AN"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-8">
<connects>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="NEG_A" pad="2"/>
<connect gate="A" pin="NEG_B" pad="6"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="POS_A" pad="3"/>
<connect gate="A" pin="POS_B" pad="5"/>
<connect gate="A" pin="V+" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM358AN"/>
<attribute name="OC_FARNELL" value="9486810"/>
<attribute name="OC_NEWARK" value="-"/>
<attribute name="PACKAGE" value="DIP-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM358M" prefix="U">
<description>Low Power Dual Operational Amplifiers</description>
<gates>
<gate name="A" symbol="LM358M"/>
</gates>
<devices>
<device name="" package="SOIC127P620X175-8N">
<connects>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="NEGA" pad="2"/>
<connect gate="A" pin="NEGB" pad="6"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="POSA" pad="3"/>
<connect gate="A" pin="POSB" pad="5"/>
<connect gate="A" pin="V+" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM358M"/>
<attribute name="OC_FARNELL" value="9486828"/>
<attribute name="OC_NEWARK" value="-"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM358N" prefix="U">
<description>Low Power Dual Operational Amplifiers</description>
<gates>
<gate name="A" symbol="LM358N"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-8">
<connects>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="NEG_A" pad="2"/>
<connect gate="A" pin="NEG_B" pad="6"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="POS_A" pad="3"/>
<connect gate="A" pin="POS_B" pad="5"/>
<connect gate="A" pin="V+" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM358N"/>
<attribute name="OC_FARNELL" value="1523834"/>
<attribute name="OC_NEWARK" value="07B6569"/>
<attribute name="PACKAGE" value="DIP-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM359M" prefix="U">
<description>Programmable, Current Mode Amplifiers</description>
<gates>
<gate name="A" symbol="LM359M"/>
</gates>
<devices>
<device name="" package="SOIC127P620X175-14N">
<connects>
<connect gate="A" pin="+INA" pad="7"/>
<connect gate="A" pin="+INB" pad="9"/>
<connect gate="A" pin="-INA" pad="6"/>
<connect gate="A" pin="-INB" pad="10"/>
<connect gate="A" pin="COMP_A" pad="3"/>
<connect gate="A" pin="COMP_B" pad="13"/>
<connect gate="A" pin="GND_A" pad="4"/>
<connect gate="A" pin="GND_B" pad="11"/>
<connect gate="A" pin="ISET_(IN)" pad="8"/>
<connect gate="A" pin="ISET_(OUT)" pad="1"/>
<connect gate="A" pin="NC" pad="5"/>
<connect gate="A" pin="V+" pad="12"/>
<connect gate="A" pin="VOUTA" pad="2"/>
<connect gate="A" pin="VOUTB" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM359M"/>
<attribute name="OC_FARNELL" value="1694014"/>
<attribute name="OC_NEWARK" value="41K4894"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="NationalS emiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM35AH" prefix="U">
<description>IC, TEMPERATURE SENSOR, ± 0.2°C</description>
<gates>
<gate name="A" symbol="LM35AH"/>
</gates>
<devices>
<device name="" package="TO127P543X266-3P">
<connects>
<connect gate="A" pin="+VS" pad="1"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="VOUT" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM35AH"/>
<attribute name="OC_FARNELL" value="1652472"/>
<attribute name="OC_NEWARK" value="83F3871"/>
<attribute name="PACKAGE" value="TO-46-3"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM35CAH" prefix="U">
<description>IC, PRECISION TEMP SENSOR</description>
<gates>
<gate name="A" symbol="LM35CAH"/>
</gates>
<devices>
<device name="" package="TO127P543X266-3P">
<connects>
<connect gate="A" pin="+VS" pad="1"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="VOUT" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM35CAH"/>
<attribute name="OC_FARNELL" value="1215189"/>
<attribute name="OC_NEWARK" value="01M8158"/>
<attribute name="PACKAGE" value="TO-46-3"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM35CAZ" prefix="U">
<description>IC, TEMPERATURE SENSOR, ± 0.2°C</description>
<gates>
<gate name="A" symbol="LM35CAZ"/>
</gates>
<devices>
<device name="" package="TO127P254X495-3P">
<connects>
<connect gate="A" pin="+VS" pad="1"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="VOUT" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM35CAZ"/>
<attribute name="OC_FARNELL" value="9494529"/>
<attribute name="OC_NEWARK" value="41K4844"/>
<attribute name="PACKAGE" value="TO-92"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM35CZ" prefix="U">
<description>IC, TEMPERATURE SENSOR, ± 0.4°C</description>
<gates>
<gate name="A" symbol="LM35CZ"/>
</gates>
<devices>
<device name="" package="TO127P254X495-3P">
<connects>
<connect gate="A" pin="+VS" pad="1"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="VOUT" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM35CZ"/>
<attribute name="OC_FARNELL" value="9488197"/>
<attribute name="OC_NEWARK" value="41K4845"/>
<attribute name="PACKAGE" value="TO-92"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM35DM" prefix="U">
<description>Precision Centigrade Temperature Sensors</description>
<gates>
<gate name="A" symbol="LM35DM"/>
</gates>
<devices>
<device name="" package="SOIC127P620X175-8N">
<connects>
<connect gate="A" pin="+VS" pad="8"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="NC" pad="2"/>
<connect gate="A" pin="NC_2" pad="6"/>
<connect gate="A" pin="NC_3" pad="7"/>
<connect gate="A" pin="NC_4" pad="3"/>
<connect gate="A" pin="NC_5" pad="5"/>
<connect gate="A" pin="VOUT" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM35DM"/>
<attribute name="OC_FARNELL" value="9493930"/>
<attribute name="OC_NEWARK" value="07B6552"/>
<attribute name="PACKAGE" value="8-SOIC"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM35DZ" prefix="U">
<description>IC, TEMPERATURE SENSOR, ± 0.4°C</description>
<gates>
<gate name="A" symbol="LM35DZ"/>
</gates>
<devices>
<device name="" package="TO127P254X495-3P">
<connects>
<connect gate="A" pin="+VS" pad="1"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="VOUT" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM35DZ"/>
<attribute name="OC_FARNELL" value="9488200"/>
<attribute name="OC_NEWARK" value="41K4849"/>
<attribute name="PACKAGE" value="TO-92"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM360M" prefix="U">
<description>High Speed Differential Comparator</description>
<gates>
<gate name="A" symbol="LM360M"/>
</gates>
<devices>
<device name="" package="SOIC127P620X175-8N">
<connects>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="IN1" pad="3"/>
<connect gate="A" pin="IN2" pad="2"/>
<connect gate="A" pin="NC" pad="1"/>
<connect gate="A" pin="OUT1" pad="7"/>
<connect gate="A" pin="OUT2" pad="6"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM360M"/>
<attribute name="OC_FARNELL" value="1685339"/>
<attribute name="OC_NEWARK" value="41K4901"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM361M" prefix="U">
<description>IC, DIFF COMP, SINGLE, 14NS</description>
<gates>
<gate name="A" symbol="LM361M"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="4"/>
<connect gate="A" pin="GND" pad="10"/>
<connect gate="A" pin="NC" pad="2"/>
<connect gate="A" pin="NC_2" pad="7"/>
<connect gate="A" pin="NC_3" pad="12"/>
<connect gate="A" pin="NC_4" pad="5"/>
<connect gate="A" pin="OUT+" pad="11"/>
<connect gate="A" pin="OUT-" pad="9"/>
<connect gate="A" pin="STROBE1" pad="13"/>
<connect gate="A" pin="STROBE2" pad="8"/>
<connect gate="A" pin="V+" pad="1"/>
<connect gate="A" pin="V-" pad="6"/>
<connect gate="A" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM361M"/>
<attribute name="OC_FARNELL" value="1468957"/>
<attribute name="OC_NEWARK" value="41K4904"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM361N" prefix="U">
<description>Differential comparator</description>
<gates>
<gate name="A" symbol="LM361N"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-14">
<connects>
<connect gate="A" pin="GND" pad="10"/>
<connect gate="A" pin="IN1" pad="3"/>
<connect gate="A" pin="IN2" pad="4"/>
<connect gate="A" pin="NC" pad="12"/>
<connect gate="A" pin="NC_2" pad="2"/>
<connect gate="A" pin="NC_3" pad="5"/>
<connect gate="A" pin="NC_4" pad="7"/>
<connect gate="A" pin="OUT1" pad="11"/>
<connect gate="A" pin="OUT2" pad="9"/>
<connect gate="A" pin="STRB1" pad="13"/>
<connect gate="A" pin="STRB2" pad="8"/>
<connect gate="A" pin="V+" pad="1"/>
<connect gate="A" pin="V-" pad="6"/>
<connect gate="A" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM361N"/>
<attribute name="OC_FARNELL" value="9487573"/>
<attribute name="OC_NEWARK" value="07B6578"/>
<attribute name="PACKAGE" value="14-DIP"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3668SD-2833" prefix="U">
<description>DC/DC Converter</description>
<gates>
<gate name="A" symbol="LM3668SD-2833"/>
</gates>
<devices>
<device name="" package="DFN300X300X80-13N">
<connects>
<connect gate="A" pin="EN" pad="6"/>
<connect gate="A" pin="EPAD" pad="13"/>
<connect gate="A" pin="FB" pad="12"/>
<connect gate="A" pin="MODE/SYNC" pad="10"/>
<connect gate="A" pin="NC" pad="8"/>
<connect gate="A" pin="PGND" pad="3"/>
<connect gate="A" pin="PVIN" pad="5"/>
<connect gate="A" pin="SGND" pad="9"/>
<connect gate="A" pin="SW1" pad="4"/>
<connect gate="A" pin="SW2" pad="2"/>
<connect gate="A" pin="VDD" pad="7"/>
<connect gate="A" pin="VOUT" pad="1"/>
<connect gate="A" pin="VSEL" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM3668SD-2833"/>
<attribute name="OC_FARNELL" value="1852919"/>
<attribute name="OC_NEWARK" value="07P5425"/>
<attribute name="PACKAGE" value="DFN-12"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3670MF-1.2" prefix="U">
<description>IC, STEP-DOWN DC/DC CONVERTER</description>
<gates>
<gate name="A" symbol="LM3670MF-1.2"/>
</gates>
<devices>
<device name="" package="SOT95P284X122-5N">
<connects>
<connect gate="A" pin="EN" pad="3"/>
<connect gate="A" pin="FB" pad="4"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="SW" pad="5"/>
<connect gate="A" pin="VIN" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM3670MF-12"/>
<attribute name="OC_FARNELL" value="1685766"/>
<attribute name="OC_NEWARK" value="79K7829"/>
<attribute name="PACKAGE" value="5-SOT-23"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3670MF-1.8" prefix="U">
<description>IC, STEP-DOWN DC/DC CONVERTER</description>
<gates>
<gate name="A" symbol="LM3670MF-1.8"/>
</gates>
<devices>
<device name="" package="SOT95P284X122-5N">
<connects>
<connect gate="A" pin="EN" pad="3"/>
<connect gate="A" pin="FB" pad="4"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="SW" pad="5"/>
<connect gate="A" pin="VIN" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM3670MF-1.8"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K4933"/>
<attribute name="PACKAGE" value="5-SOT-23"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3670MF-3.3" prefix="U">
<description>IC BUCK 3.3V 350MA</description>
<gates>
<gate name="A" symbol="LM3670MF-3.3"/>
</gates>
<devices>
<device name="" package="SOT95P284X122-5N">
<connects>
<connect gate="A" pin="EN" pad="3"/>
<connect gate="A" pin="FB" pad="4"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="SW" pad="5"/>
<connect gate="A" pin="VIN" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM3670MF-3.3"/>
<attribute name="OC_FARNELL" value="1685757"/>
<attribute name="OC_NEWARK" value="65K6211"/>
<attribute name="PACKAGE" value="5-SOT-23"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3670MF-ADJ" prefix="U">
<description>Step-Down DC-DC Converter</description>
<gates>
<gate name="A" symbol="LM3670MF-ADJ"/>
</gates>
<devices>
<device name="" package="SOT95P285X120-5N">
<connects>
<connect gate="A" pin="EN" pad="3"/>
<connect gate="A" pin="FB" pad="4"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="SW" pad="5"/>
<connect gate="A" pin="VIN" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM3670MF-ADJ"/>
<attribute name="OC_FARNELL" value="1008247"/>
<attribute name="OC_NEWARK" value="41K4932"/>
<attribute name="PACKAGE" value="SOT-23-5"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3671MF-1.2" prefix="U">
<description>IC BUCK SYNC 1.2V 0.6A</description>
<gates>
<gate name="A" symbol="LM3671MF-1.2"/>
</gates>
<devices>
<device name="" package="SOT95P284X122-5N">
<connects>
<connect gate="A" pin="EN" pad="3"/>
<connect gate="A" pin="FB" pad="4"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="SW" pad="5"/>
<connect gate="A" pin="VIN" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM3671MF-1.2"/>
<attribute name="OC_FARNELL" value="1685653"/>
<attribute name="OC_NEWARK" value="41K4937"/>
<attribute name="PACKAGE" value="5-SOT-23"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3671MF-1.25" prefix="U">
<description>DC/DC CONVERTER</description>
<gates>
<gate name="A" symbol="LM3671MF-1.25"/>
</gates>
<devices>
<device name="" package="SOT95P284X119-5N">
<connects>
<connect gate="A" pin="EN" pad="3"/>
<connect gate="A" pin="FB" pad="4"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="SW" pad="5"/>
<connect gate="A" pin="VIN" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM3671MF-1.25"/>
<attribute name="OC_FARNELL" value="1008251"/>
<attribute name="OC_NEWARK" value="41K4938"/>
<attribute name="PACKAGE" value="SOT23-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3671MF-1.5" prefix="U">
<description>Step-Down DC-DC Converter</description>
<gates>
<gate name="A" symbol="LM3671MF-1.5"/>
</gates>
<devices>
<device name="" package="SOT95P285X120-5N">
<connects>
<connect gate="A" pin="EN" pad="3"/>
<connect gate="A" pin="FB" pad="4"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="SW" pad="5"/>
<connect gate="A" pin="VIN" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM3671MF-1.5"/>
<attribute name="OC_FARNELL" value="1008253"/>
<attribute name="OC_NEWARK" value="41K4940"/>
<attribute name="PACKAGE" value="SOT-23-5"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3671MF-1.8" prefix="U">
<description>IC BUCK SYNC 1.8V 0.6A</description>
<gates>
<gate name="A" symbol="LM3671MF-1.8"/>
</gates>
<devices>
<device name="" package="SOT95P284X122-5N">
<connects>
<connect gate="A" pin="EN" pad="3"/>
<connect gate="A" pin="FB" pad="4"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="SW" pad="5"/>
<connect gate="A" pin="VIN" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM3671MF-1.8"/>
<attribute name="OC_FARNELL" value="1685654"/>
<attribute name="OC_NEWARK" value="41K4942"/>
<attribute name="PACKAGE" value="5-SOT-23"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3671MF-1.875" prefix="U">
<description>IC BUCK SYNC 1.88V 0.6A</description>
<gates>
<gate name="A" symbol="LM3671MF-1.875"/>
</gates>
<devices>
<device name="" package="SOT95P284X122-5N">
<connects>
<connect gate="A" pin="EN" pad="3"/>
<connect gate="A" pin="FB" pad="4"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="SW" pad="5"/>
<connect gate="A" pin="VIN" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM3671MF-1.875"/>
<attribute name="OC_FARNELL" value="1008255"/>
<attribute name="OC_NEWARK" value="-"/>
<attribute name="PACKAGE" value="5-SOT-23"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3671MF-2.5" prefix="U">
<description>IC BUCK SYNC 2.5V 0.6A</description>
<gates>
<gate name="A" symbol="LM3671MF-2.5"/>
</gates>
<devices>
<device name="" package="SOT95P284X122-5N">
<connects>
<connect gate="A" pin="EN" pad="3"/>
<connect gate="A" pin="FB" pad="4"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="SW" pad="5"/>
<connect gate="A" pin="VIN" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM3671MF-2.5"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="79K7835"/>
<attribute name="PACKAGE" value="5-SOT-23"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3671MF-3.3" prefix="U">
<description>IC BUCK SYNC 3.3V 0.6A</description>
<gates>
<gate name="A" symbol="LM3671MF-3.3"/>
</gates>
<devices>
<device name="" package="SOT95P284X122-5N">
<connects>
<connect gate="A" pin="EN" pad="3"/>
<connect gate="A" pin="FB" pad="4"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="SW" pad="5"/>
<connect gate="A" pin="VIN" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM3671MF-3.3"/>
<attribute name="OC_FARNELL" value="1685767"/>
<attribute name="OC_NEWARK" value="79K7838"/>
<attribute name="PACKAGE" value="5-SOT-23"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3671MF-ADJ" prefix="U">
<description>Step-Down DC-DC Converter</description>
<gates>
<gate name="A" symbol="LM3671MF-ADJ"/>
</gates>
<devices>
<device name="" package="SOT95P285X120-5N">
<connects>
<connect gate="A" pin="EN" pad="3"/>
<connect gate="A" pin="FB" pad="4"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="SW" pad="5"/>
<connect gate="A" pin="VIN" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM3671MF-ADJ"/>
<attribute name="OC_FARNELL" value="1008256"/>
<attribute name="OC_NEWARK" value="41K4936"/>
<attribute name="PACKAGE" value="SOT-23-5"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3671TL-1.2" prefix="U">
<description>IC CONV DC-DC STEPDOWN 5MICROSMD</description>
<gates>
<gate name="A" symbol="LM3671TL-1.2"/>
</gates>
<devices>
<device name="" package="BGA5C43PX50P3X2_105X138X60">
<connects>
<connect gate="A" pin="EN" pad="C1"/>
<connect gate="A" pin="FB" pad="C3"/>
<connect gate="A" pin="GND" pad="A3"/>
<connect gate="A" pin="SW" pad="B2"/>
<connect gate="A" pin="VIN" pad="A1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM3671TL-1.2"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="69K2518"/>
<attribute name="PACKAGE" value="5-WFBGA"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3671TL-1.8" prefix="U">
<description>IC CONV DC-DC STEPDOWN 5MICROSMD</description>
<gates>
<gate name="A" symbol="LM3671TL-1.8"/>
</gates>
<devices>
<device name="" package="BGA5C43PX50P3X2_105X138X60">
<connects>
<connect gate="A" pin="EN" pad="C1"/>
<connect gate="A" pin="FB" pad="C3"/>
<connect gate="A" pin="GND" pad="A3"/>
<connect gate="A" pin="SW" pad="B2"/>
<connect gate="A" pin="VIN" pad="A1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM3671TL-1.8"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="69K2522"/>
<attribute name="PACKAGE" value="5-WFBGA"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3671TL-3.3" prefix="U">
<description>IC CONV DC-DC STPDN 3.3V</description>
<gates>
<gate name="A" symbol="LM3671TL-3.3"/>
</gates>
<devices>
<device name="" package="BGA5C43PX50P3X2_105X138X60">
<connects>
<connect gate="A" pin="EN" pad="C1"/>
<connect gate="A" pin="FB" pad="C3"/>
<connect gate="A" pin="GND" pad="A3"/>
<connect gate="A" pin="SW" pad="B2"/>
<connect gate="A" pin="VIN" pad="A1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM3671TL-3.3"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="79K7853"/>
<attribute name="PACKAGE" value="5-WFBGA"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3673TL-1.2" prefix="U">
<description>IC CONV DC/DC 350MA 1.2V</description>
<gates>
<gate name="A" symbol="LM3673TL-1.2"/>
</gates>
<devices>
<device name="" package="BGA5C43PX50P3X2_105X138X60">
<connects>
<connect gate="A" pin="EN" pad="C1"/>
<connect gate="A" pin="FB" pad="C3"/>
<connect gate="A" pin="GND" pad="A3"/>
<connect gate="A" pin="SW" pad="B2"/>
<connect gate="A" pin="VIN" pad="A1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM3673TL-1.2"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="13M1803"/>
<attribute name="PACKAGE" value="5-WFBGA"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3673TL-1.5" prefix="U">
<description>IC CONV DC/DC 350MA 1.5V</description>
<gates>
<gate name="A" symbol="LM3673TL-1.5"/>
</gates>
<devices>
<device name="" package="BGA5C43PX50P3X2_105X138X60">
<connects>
<connect gate="A" pin="EN" pad="C1"/>
<connect gate="A" pin="FB" pad="C3"/>
<connect gate="A" pin="GND" pad="A3"/>
<connect gate="A" pin="SW" pad="B2"/>
<connect gate="A" pin="VIN" pad="A1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM3673TL-1.5"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="32M2974"/>
<attribute name="PACKAGE" value="5-WFBGA"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3673TL-ADJ" prefix="U">
<description>IC CONV DC/DC 350MA ADJ</description>
<gates>
<gate name="A" symbol="LM3673TL-ADJ"/>
</gates>
<devices>
<device name="" package="BGA5C43PX50P3X2_105X138X60">
<connects>
<connect gate="A" pin="EN" pad="C1"/>
<connect gate="A" pin="FB" pad="C3"/>
<connect gate="A" pin="GND" pad="A3"/>
<connect gate="A" pin="SW" pad="B2"/>
<connect gate="A" pin="VIN" pad="A1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM3673TL-ADJ"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="13M1802"/>
<attribute name="PACKAGE" value="5-WFBGA"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3674MF-1.2" prefix="U">
<description>IC BUCK SYNC 1.2V 0.6A</description>
<gates>
<gate name="A" symbol="LM3674MF-1.2"/>
</gates>
<devices>
<device name="" package="SOT95P284X122-5N">
<connects>
<connect gate="A" pin="EN" pad="3"/>
<connect gate="A" pin="FB" pad="4"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="SW" pad="5"/>
<connect gate="A" pin="VIN" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM3674MF-1.2"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="79K7865"/>
<attribute name="PACKAGE" value="5-SOT-23"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3674MF-1.5" prefix="U">
<description>IC BUCK SYNC 1.5V 0.6A</description>
<gates>
<gate name="A" symbol="LM3674MF-1.5"/>
</gates>
<devices>
<device name="" package="SOT95P284X122-5N">
<connects>
<connect gate="A" pin="EN" pad="3"/>
<connect gate="A" pin="FB" pad="4"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="SW" pad="5"/>
<connect gate="A" pin="VIN" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM3674MF-1.5"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="79K7867"/>
<attribute name="PACKAGE" value="5-SOT-23"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3674MF-1.8" prefix="U">
<description>IC BUCK SYNC 1.8V 0.6A</description>
<gates>
<gate name="A" symbol="LM3674MF-1.8"/>
</gates>
<devices>
<device name="" package="SOT95P284X122-5N">
<connects>
<connect gate="A" pin="EN" pad="3"/>
<connect gate="A" pin="FB" pad="4"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="SW" pad="5"/>
<connect gate="A" pin="VIN" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM3674MF-1.8"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="79K7869"/>
<attribute name="PACKAGE" value="5-SOT-23"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3674MF-1.875" prefix="U">
<description>IC BUCK SYNC 1.88V 0.6A</description>
<gates>
<gate name="A" symbol="LM3674MF-1.875"/>
</gates>
<devices>
<device name="" package="SOT95P284X122-5N">
<connects>
<connect gate="A" pin="EN" pad="3"/>
<connect gate="A" pin="FB" pad="4"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="SW" pad="5"/>
<connect gate="A" pin="VIN" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM3674MF-1.875"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="99K2433"/>
<attribute name="PACKAGE" value="5-SOT-23"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3674MF-2.8" prefix="U">
<description>IC BUCK SYNC 2.8V 0.6A</description>
<gates>
<gate name="A" symbol="LM3674MF-2.8"/>
</gates>
<devices>
<device name="" package="SOT95P284X122-5N">
<connects>
<connect gate="A" pin="EN" pad="3"/>
<connect gate="A" pin="FB" pad="4"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="SW" pad="5"/>
<connect gate="A" pin="VIN" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM3674MF-2.8"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="99K2435"/>
<attribute name="PACKAGE" value="5-SOT-23"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3674MF-ADJ" prefix="U">
<description>Step-Down DC-DC Converter</description>
<gates>
<gate name="A" symbol="LM3674MF-ADJ"/>
</gates>
<devices>
<device name="" package="SOT95P285X120-5N">
<connects>
<connect gate="A" pin="EN" pad="3"/>
<connect gate="A" pin="FB" pad="4"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="SW" pad="5"/>
<connect gate="A" pin="VIN" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM3674MF-ADJ"/>
<attribute name="OC_FARNELL" value="1312587"/>
<attribute name="OC_NEWARK" value="79K7863"/>
<attribute name="PACKAGE" value="SOT-23-5"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3676SD-1.5" prefix="U">
<description>IC CONV DC-DC 600MA 1.5V</description>
<gates>
<gate name="A" symbol="LM3676SD-1.5"/>
</gates>
<devices>
<device name="" package="DFN50P300X300X80-9N">
<connects>
<connect gate="A" pin="ANY" pad="9"/>
<connect gate="A" pin="EN" pad="5"/>
<connect gate="A" pin="FB" pad="4"/>
<connect gate="A" pin="MODE" pad="3"/>
<connect gate="A" pin="NC" pad="6"/>
<connect gate="A" pin="PGND" pad="1"/>
<connect gate="A" pin="SGND" pad="7"/>
<connect gate="A" pin="SW" pad="2"/>
<connect gate="A" pin="VIN" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM3676SD-15"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="46M5505"/>
<attribute name="PACKAGE" value="8-WFDFN Exposed Pad"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3676SD-1.8" prefix="U">
<description>IC CONV DC-DC 600MA 1.8V</description>
<gates>
<gate name="A" symbol="LM3676SD-1.8"/>
</gates>
<devices>
<device name="" package="DFN50P300X300X80-9N">
<connects>
<connect gate="A" pin="ANY" pad="9"/>
<connect gate="A" pin="EN" pad="5"/>
<connect gate="A" pin="FB" pad="4"/>
<connect gate="A" pin="MODE" pad="3"/>
<connect gate="A" pin="NC" pad="6"/>
<connect gate="A" pin="PGND" pad="1"/>
<connect gate="A" pin="SGND" pad="7"/>
<connect gate="A" pin="SW" pad="2"/>
<connect gate="A" pin="VIN" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM3676SD-1.8"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="46M5507"/>
<attribute name="PACKAGE" value="8-WFDFN Exposed Pad"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3676SD-3.3" prefix="U">
<description>IC CONV DC-DC 600MA 3.3V</description>
<gates>
<gate name="A" symbol="LM3676SD-3.3"/>
</gates>
<devices>
<device name="" package="DFN50P300X300X80-9N">
<connects>
<connect gate="A" pin="ANY" pad="9"/>
<connect gate="A" pin="EN" pad="5"/>
<connect gate="A" pin="FB" pad="4"/>
<connect gate="A" pin="MODE" pad="3"/>
<connect gate="A" pin="NC" pad="6"/>
<connect gate="A" pin="PGND" pad="1"/>
<connect gate="A" pin="SGND" pad="7"/>
<connect gate="A" pin="SW" pad="2"/>
<connect gate="A" pin="VIN" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM3676SD-3.3"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="46M5509"/>
<attribute name="PACKAGE" value="8-WFDFN Exposed Pad"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3676SD-ADJ" prefix="U">
<description>IC CONV DC-DC 600MA ADJ</description>
<gates>
<gate name="A" symbol="LM3676SD-ADJ"/>
</gates>
<devices>
<device name="" package="DFN50P300X300X80-9N">
<connects>
<connect gate="A" pin="ANY" pad="9"/>
<connect gate="A" pin="EN" pad="5"/>
<connect gate="A" pin="FB" pad="4"/>
<connect gate="A" pin="MODE" pad="3"/>
<connect gate="A" pin="NC" pad="6"/>
<connect gate="A" pin="PGND" pad="1"/>
<connect gate="A" pin="SGND" pad="7"/>
<connect gate="A" pin="SW" pad="2"/>
<connect gate="A" pin="VIN" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM3676SD-ADJ"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="46M5502"/>
<attribute name="PACKAGE" value="8-WFDFN Exposed Pad"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3677TL-ADJ" prefix="U">
<description>Step-Down DC-DC Converter</description>
<gates>
<gate name="A" symbol="LM3677TL-ADJ"/>
</gates>
<devices>
<device name="" package="BGA50PX43P3X3_148X110X67">
<connects>
<connect gate="A" pin="EN" pad="C1"/>
<connect gate="A" pin="FB" pad="C3"/>
<connect gate="A" pin="GND" pad="A3"/>
<connect gate="A" pin="SW" pad="B2"/>
<connect gate="A" pin="VIN" pad="A1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM3677TL-ADJ"/>
<attribute name="OC_FARNELL" value="1798322"/>
<attribute name="OC_NEWARK" value="73R9736"/>
<attribute name="PACKAGE" value="BGA-5"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3686TLE-AAEF" prefix="U">
<description>Step-Down DC-DC Converter</description>
<gates>
<gate name="A" symbol="LM3686TLE-AAEF"/>
</gates>
<devices>
<device name="" package="BGA12C3X550P_242X169X60">
<connects>
<connect gate="A" pin="EN_DCDC" pad="B3"/>
<connect gate="A" pin="EN_LDO" pad="C2"/>
<connect gate="A" pin="EN_LILO" pad="B2"/>
<connect gate="A" pin="FB_DCDC" pad="A3"/>
<connect gate="A" pin="PGND" pad="A1"/>
<connect gate="A" pin="QGND" pad="C3"/>
<connect gate="A" pin="SW" pad="A2"/>
<connect gate="A" pin="VBATT" pad="B1"/>
<connect gate="A" pin="VIN_LDO" pad="C1"/>
<connect gate="A" pin="VIN_LILO" pad="D3"/>
<connect gate="A" pin="VOUT_LDO" pad="D1"/>
<connect gate="A" pin="VOUT_LILO" pad="D2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM3686TLE-AAEF"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="55R4027"/>
<attribute name="PACKAGE" value="BGA-12"/>
<attribute name="SUPPLIER" value="National semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3704YCMM-308" prefix="U">
<description>Microprocessor Supervisory Circuits</description>
<gates>
<gate name="A" symbol="LM3704YCMM-308"/>
</gates>
<devices>
<device name="" package="SOP50P490X109-10N">
<connects>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="NC" pad="9"/>
<connect gate="A" pin="NC_2" pad="6"/>
<connect gate="A" pin="NC_3" pad="4"/>
<connect gate="A" pin="PFI" pad="3"/>
<connect gate="A" pin="VCC" pad="1"/>
<connect gate="A" pin="~LLO" pad="7"/>
<connect gate="A" pin="~MR" pad="2"/>
<connect gate="A" pin="~PFO" pad="8"/>
<connect gate="A" pin="~RESET" pad="10"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM3704YCMM-308"/>
<attribute name="OC_FARNELL" value="1312724"/>
<attribute name="OC_NEWARK" value="31M5421"/>
<attribute name="PACKAGE" value="10-MSOP"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3710XQMM-308" prefix="U">
<description>Microprocessor Supervisory</description>
<gates>
<gate name="A" symbol="LM3710XQMM-308"/>
</gates>
<devices>
<device name="" package="SOP50P490X110-10N">
<connects>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="NC" pad="9"/>
<connect gate="A" pin="NC_2" pad="6"/>
<connect gate="A" pin="PFI" pad="3"/>
<connect gate="A" pin="VCC" pad="1"/>
<connect gate="A" pin="WDI" pad="4"/>
<connect gate="A" pin="~LLO" pad="7"/>
<connect gate="A" pin="~MR" pad="2"/>
<connect gate="A" pin="~PFO" pad="8"/>
<connect gate="A" pin="~RESET" pad="10"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM3710XQMM-308"/>
<attribute name="OC_FARNELL" value="1798323"/>
<attribute name="OC_NEWARK" value="73R9737"/>
<attribute name="PACKAGE" value="10-MSOP"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3724EM5-3.08" prefix="U">
<description>MPU</description>
<gates>
<gate name="A" symbol="LM3724EM5-3.08"/>
</gates>
<devices>
<device name="" package="SOT95P284X122-5N">
<connects>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="GND_2" pad="1"/>
<connect gate="A" pin="VCC" pad="5"/>
<connect gate="A" pin="~MR" pad="4"/>
<connect gate="A" pin="~RESET" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM3724EM5-3.08"/>
<attribute name="OC_FARNELL" value="1312735"/>
<attribute name="OC_NEWARK" value="34C6590"/>
<attribute name="PACKAGE" value="SOT23-5"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3724EM5-4.63" prefix="U">
<description>MPU</description>
<gates>
<gate name="A" symbol="LM3724EM5-4.63"/>
</gates>
<devices>
<device name="" package="SOT95P284X122-5N">
<connects>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="GND_2" pad="1"/>
<connect gate="A" pin="VCC" pad="5"/>
<connect gate="A" pin="~MR" pad="4"/>
<connect gate="A" pin="~RESET" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM3724EM5-4.63"/>
<attribute name="OC_FARNELL" value="1312736"/>
<attribute name="OC_NEWARK" value="31M5426"/>
<attribute name="PACKAGE" value="SOT23-5"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3724IM5-2.32" prefix="U">
<description>Microprocessor Reset Circuits</description>
<gates>
<gate name="A" symbol="LM3724IM5-2.32"/>
</gates>
<devices>
<device name="" package="SOT95P285X120-5N">
<connects>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="GND_2" pad="1"/>
<connect gate="A" pin="VCC" pad="5"/>
<connect gate="A" pin="~MR" pad="4"/>
<connect gate="A" pin="~RESET" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM3724IM5-232"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K5030"/>
<attribute name="PACKAGE" value="SOT-23-5"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3724IM5-3.08" prefix="U">
<description>MPU</description>
<gates>
<gate name="A" symbol="LM3724IM5-3.08"/>
</gates>
<devices>
<device name="" package="SOT95P284X122-5N">
<connects>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="GND_2" pad="1"/>
<connect gate="A" pin="VCC" pad="5"/>
<connect gate="A" pin="~MR" pad="4"/>
<connect gate="A" pin="~RESET" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM3724IM5-3.08"/>
<attribute name="OC_FARNELL" value="9779078"/>
<attribute name="OC_NEWARK" value="41K5031"/>
<attribute name="PACKAGE" value="SOT23-5"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3724IM5-4.63" prefix="U">
<description>Microprocessor Reset Circuits</description>
<gates>
<gate name="A" symbol="LM3724IM5-4.63"/>
</gates>
<devices>
<device name="" package="SOT95P284X122-5N">
<connects>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="GND_2" pad="1"/>
<connect gate="A" pin="VCC" pad="5"/>
<connect gate="A" pin="~MR" pad="4"/>
<connect gate="A" pin="~RESET" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM3724IM5-4.63"/>
<attribute name="OC_FARNELL" value="9779086"/>
<attribute name="OC_NEWARK" value="34C6597"/>
<attribute name="PACKAGE" value="SOT23-5"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3743MM-1000" prefix="U">
<description>Synchronous Buck Controller</description>
<gates>
<gate name="A" symbol="LM3743MM-1000"/>
</gates>
<devices>
<device name="" package="SOP50P490X109-10N">
<connects>
<connect gate="A" pin="BOOT" pad="10"/>
<connect gate="A" pin="COMP/EN" pad="6"/>
<connect gate="A" pin="FB" pad="5"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="HGATE" pad="9"/>
<connect gate="A" pin="ILIM" pad="4"/>
<connect gate="A" pin="LGATE" pad="2"/>
<connect gate="A" pin="SS/TRACK" pad="7"/>
<connect gate="A" pin="SW" pad="8"/>
<connect gate="A" pin="VCC" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM3743MM-1000"/>
<attribute name="OC_FARNELL" value="1290936"/>
<attribute name="OC_NEWARK" value="22M0969"/>
<attribute name="PACKAGE" value="SOP-10"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3753SQ">
<description>Scalable 2-Phase Synchronous Buck Controllers</description>
<gates>
<gate name="A" symbol="LM3753SQ"/>
</gates>
<devices>
<device name="" package="QFN50P500X500X80-33N">
<connects>
<connect gate="A" pin="BOOT1" pad="9"/>
<connect gate="A" pin="BOOT2" pad="32"/>
<connect gate="A" pin="COMP" pad="18"/>
<connect gate="A" pin="CS1" pad="30"/>
<connect gate="A" pin="CS2" pad="27"/>
<connect gate="A" pin="CSM" pad="29"/>
<connect gate="A" pin="EN" pad="26"/>
<connect gate="A" pin="EPAD" pad="33"/>
<connect gate="A" pin="FB" pad="19"/>
<connect gate="A" pin="FREQ" pad="24"/>
<connect gate="A" pin="HG1" pad="8"/>
<connect gate="A" pin="HG2" pad="1"/>
<connect gate="A" pin="IAVE" pad="25"/>
<connect gate="A" pin="ILIM" pad="28"/>
<connect gate="A" pin="LG1" pad="6"/>
<connect gate="A" pin="LG2" pad="3"/>
<connect gate="A" pin="NBASE" pad="14"/>
<connect gate="A" pin="PGND" pad="5"/>
<connect gate="A" pin="PGOOD" pad="10"/>
<connect gate="A" pin="PH" pad="31"/>
<connect gate="A" pin="SGND" pad="17"/>
<connect gate="A" pin="SNSM" pad="21"/>
<connect gate="A" pin="SNSP" pad="22"/>
<connect gate="A" pin="SS" pad="23"/>
<connect gate="A" pin="SW1" pad="7"/>
<connect gate="A" pin="SW2" pad="2"/>
<connect gate="A" pin="SYNC" pad="12"/>
<connect gate="A" pin="SYNCOUT" pad="11"/>
<connect gate="A" pin="VCC" pad="16"/>
<connect gate="A" pin="VDD" pad="4"/>
<connect gate="A" pin="VDIF" pad="20"/>
<connect gate="A" pin="VIN" pad="15"/>
<connect gate="A" pin="~FAULT" pad="13"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM3753SQ"/>
<attribute name="OC_FARNELL" value="1798341"/>
<attribute name="OC_NEWARK" value="73R9738"/>
<attribute name="PACKAGE" value="QFN-32"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3754SQ">
<description>Scalable 2-Phase Synchronous Buck Controllers</description>
<gates>
<gate name="A" symbol="LM3754SQ"/>
</gates>
<devices>
<device name="" package="QFN50P500X500X80-33N">
<connects>
<connect gate="A" pin="BOOT1" pad="9"/>
<connect gate="A" pin="BOOT2" pad="32"/>
<connect gate="A" pin="COMP" pad="18"/>
<connect gate="A" pin="CS1" pad="30"/>
<connect gate="A" pin="CS2" pad="27"/>
<connect gate="A" pin="CSM" pad="29"/>
<connect gate="A" pin="EN" pad="26"/>
<connect gate="A" pin="EPAD" pad="33"/>
<connect gate="A" pin="FB" pad="19"/>
<connect gate="A" pin="FREQ" pad="24"/>
<connect gate="A" pin="HG1" pad="8"/>
<connect gate="A" pin="HG2" pad="1"/>
<connect gate="A" pin="IAVE" pad="25"/>
<connect gate="A" pin="ILIM" pad="28"/>
<connect gate="A" pin="LG1" pad="6"/>
<connect gate="A" pin="LG2" pad="3"/>
<connect gate="A" pin="NBASE" pad="14"/>
<connect gate="A" pin="PGND" pad="5"/>
<connect gate="A" pin="PGOOD" pad="10"/>
<connect gate="A" pin="PH" pad="31"/>
<connect gate="A" pin="SGND" pad="17"/>
<connect gate="A" pin="SNSM" pad="21"/>
<connect gate="A" pin="SNSP" pad="22"/>
<connect gate="A" pin="SS" pad="23"/>
<connect gate="A" pin="SW1" pad="7"/>
<connect gate="A" pin="SW2" pad="2"/>
<connect gate="A" pin="SYNC" pad="12"/>
<connect gate="A" pin="SYNCOUT" pad="11"/>
<connect gate="A" pin="VCC" pad="16"/>
<connect gate="A" pin="VDD" pad="4"/>
<connect gate="A" pin="VDIF" pad="20"/>
<connect gate="A" pin="VIN" pad="15"/>
<connect gate="A" pin="~FAULT" pad="13"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM3754SQ"/>
<attribute name="OC_FARNELL" value="1798342"/>
<attribute name="OC_NEWARK" value="73R9739"/>
<attribute name="PACKAGE" value="QFN-32"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3880MF-1AB" prefix="U">
<description>Power Sequencer</description>
<gates>
<gate name="A" symbol="LM3880MF-1AB"/>
</gates>
<devices>
<device name="" package="SOT95P285X120-6N">
<connects>
<connect gate="A" pin="EN" pad="3"/>
<connect gate="A" pin="FLAG1" pad="6"/>
<connect gate="A" pin="FLAG2" pad="5"/>
<connect gate="A" pin="FLAG3" pad="4"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="VCC" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM3880MF-1AB"/>
<attribute name="OC_FARNELL" value="1271399"/>
<attribute name="OC_NEWARK" value="13M1814"/>
<attribute name="PACKAGE" value="SOT-23-6"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3881MM" prefix="U">
<description>Power Sequencer</description>
<gates>
<gate name="A" symbol="LM3881MM"/>
</gates>
<devices>
<device name="" package="SOP65P490X110-8N">
<connects>
<connect gate="A" pin="EN" pad="2"/>
<connect gate="A" pin="FLAG1" pad="8"/>
<connect gate="A" pin="FLAG2" pad="7"/>
<connect gate="A" pin="FLAG3" pad="6"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="INV" pad="4"/>
<connect gate="A" pin="TADJ" pad="5"/>
<connect gate="A" pin="VCC" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM3881MM"/>
<attribute name="OC_FARNELL" value="1552439"/>
<attribute name="OC_NEWARK" value="94M8006"/>
<attribute name="PACKAGE" value="MSOP-8"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3886T" prefix="U">
<description>IC AMP AUDIO PWR 68W AB</description>
<gates>
<gate name="A" symbol="LM3886T"/>
</gates>
<devices>
<device name="" package="AMP_LM3886T">
<connects>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="MUTE" pad="8"/>
<connect gate="A" pin="NC" pad="6"/>
<connect gate="A" pin="NC_2" pad="2"/>
<connect gate="A" pin="NC_3" pad="11"/>
<connect gate="A" pin="OUT" pad="3"/>
<connect gate="A" pin="V+" pad="1"/>
<connect gate="A" pin="V+_2" pad="5"/>
<connect gate="A" pin="V-" pad="4"/>
<connect gate="A" pin="VIN+" pad="10"/>
<connect gate="A" pin="VIN-" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM3886T"/>
<attribute name="OC_FARNELL" value="9493603"/>
<attribute name="OC_NEWARK" value="92F298"/>
<attribute name="PACKAGE" value="TO220-11"/>
<attribute name="SUPPLIER" value="National semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3886TF" prefix="U">
<description>IC AMP AUDIO PWR 68W</description>
<gates>
<gate name="A" symbol="LM3886TF"/>
</gates>
<devices>
<device name="" package="AMP_LM3886T">
<connects>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="MUTE" pad="8"/>
<connect gate="A" pin="NC" pad="6"/>
<connect gate="A" pin="NC_2" pad="2"/>
<connect gate="A" pin="NC_3" pad="11"/>
<connect gate="A" pin="OUT" pad="3"/>
<connect gate="A" pin="V+" pad="1"/>
<connect gate="A" pin="V+_2" pad="5"/>
<connect gate="A" pin="V-" pad="4"/>
<connect gate="A" pin="VIN+" pad="10"/>
<connect gate="A" pin="VIN-" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM3886TF"/>
<attribute name="OC_FARNELL" value="9489681"/>
<attribute name="OC_NEWARK" value="92F299"/>
<attribute name="PACKAGE" value="TO220-11"/>
<attribute name="SUPPLIER" value="National semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM392M" prefix="U">
<description>Low Power Operational Amplifier</description>
<gates>
<gate name="A" symbol="LM392M"/>
</gates>
<devices>
<device name="" package="SOIC127P620X175-8N">
<connects>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="NEG_A" pad="2"/>
<connect gate="A" pin="NEG_B" pad="6"/>
<connect gate="A" pin="OUT_A" pad="1"/>
<connect gate="A" pin="OUT_B" pad="7"/>
<connect gate="A" pin="POS_A" pad="3"/>
<connect gate="A" pin="POS_B" pad="5"/>
<connect gate="A" pin="V+" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM392M"/>
<attribute name="OC_FARNELL" value="9486755"/>
<attribute name="OC_NEWARK" value="41K5114"/>
<attribute name="PACKAGE" value="8-SOIC"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM392N" prefix="U">
<description>OP AMP</description>
<gates>
<gate name="A" symbol="LM392N"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-8">
<connects>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="NEG_A" pad="2"/>
<connect gate="A" pin="NEG_B" pad="6"/>
<connect gate="A" pin="OUT_A" pad="1"/>
<connect gate="A" pin="OUT_B" pad="7"/>
<connect gate="A" pin="POA_A" pad="3"/>
<connect gate="A" pin="POS_B" pad="5"/>
<connect gate="A" pin="V+" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM392N"/>
<attribute name="OC_FARNELL" value="9486763"/>
<attribute name="OC_NEWARK" value="41K5116"/>
<attribute name="PACKAGE" value="8-DIP"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM393M" prefix="U">
<description>Low Power Low Offset Voltage Dual Comparators</description>
<gates>
<gate name="A" symbol="LM393M"/>
</gates>
<devices>
<device name="" package="SOIC127P620X175-8N">
<connects>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="NEGA" pad="2"/>
<connect gate="A" pin="NEGB" pad="6"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="POSA" pad="3"/>
<connect gate="A" pin="POSB" pad="5"/>
<connect gate="A" pin="V+" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM393M"/>
<attribute name="OC_FARNELL" value="9487590"/>
<attribute name="OC_NEWARK" value="-"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM393N" prefix="U">
<description>COMP DUAL LO PWR</description>
<gates>
<gate name="A" symbol="LM393N"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-8">
<connects>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="NEG_A" pad="2"/>
<connect gate="A" pin="NEG_B" pad="6"/>
<connect gate="A" pin="OUT_A" pad="1"/>
<connect gate="A" pin="OUT_B" pad="7"/>
<connect gate="A" pin="POA_A" pad="3"/>
<connect gate="A" pin="POS_B" pad="5"/>
<connect gate="A" pin="V+" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM393N"/>
<attribute name="OC_FARNELL" value="9487611"/>
<attribute name="OC_NEWARK" value="07B6636"/>
<attribute name="PACKAGE" value="8-DIP"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3940IMP-3.3" prefix="U">
<description>Low Dropout Regulator</description>
<gates>
<gate name="A" symbol="LM3940IMP-3.3"/>
</gates>
<devices>
<device name="" package="SOT230P696X180-4N">
<connects>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="GND_2" pad="2"/>
<connect gate="A" pin="IN" pad="1"/>
<connect gate="A" pin="OUT" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MANUFACTURER_PART_NUMBER" value="LM3940IMP-33"/>
<attribute name="OC_FARNELL" value="9779280"/>
<attribute name="OC_NEWARK" value="41K5122"/>
<attribute name="PACKAGE" value="SOT-223-4"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3940IS-3.3" prefix="U">
<description>Low Dropout Regulator</description>
<gates>
<gate name="A" symbol="LM3940IS-3.3"/>
</gates>
<devices>
<device name="" package="TO254P1435X457-4N">
<connects>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="GND_2" pad="2"/>
<connect gate="A" pin="IN" pad="1"/>
<connect gate="A" pin="OUT" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM3940IS-3.3"/>
<attribute name="OC_FARNELL" value="9494545"/>
<attribute name="OC_NEWARK" value="41K5124"/>
<attribute name="PACKAGE" value="TO-263-3"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3940IT-3.3" prefix="U">
<description>IC, LDO VOLT REG, 3.3V, 1A</description>
<gates>
<gate name="A" symbol="LM3940IT-3.3"/>
</gates>
<devices>
<device name="" package="TO254P470X1016X2222-3P">
<connects>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="IN" pad="1"/>
<connect gate="A" pin="OUT" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM3940IT-3.3"/>
<attribute name="OC_FARNELL" value="9494553"/>
<attribute name="OC_NEWARK" value="41K5126"/>
<attribute name="PACKAGE" value="TO-220"/>
<attribute name="SUPPLIER" value="NATIONAL SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM397MF" prefix="U">
<description>Single General Purpose Voltage Comparator</description>
<gates>
<gate name="A" symbol="LM397MF"/>
</gates>
<devices>
<device name="" package="SOT95P285X120-5N">
<connects>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="OUT" pad="4"/>
<connect gate="A" pin="VIN+" pad="3"/>
<connect gate="A" pin="VIN-" pad="1"/>
<connect gate="A" pin="VS" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM397MF"/>
<attribute name="OC_FARNELL" value="9779108"/>
<attribute name="OC_NEWARK" value="74C4319"/>
<attribute name="PACKAGE" value="SOT-23-5"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM4120AIM5-1.8" prefix="U">
<description>Dropout voltage reference</description>
<gates>
<gate name="A" symbol="LM4120AIM5-1.8"/>
</gates>
<devices>
<device name="" package="SOT95P284X122-5N">
<connects>
<connect gate="A" pin="EN" pad="3"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="REF" pad="1"/>
<connect gate="A" pin="VIN" pad="4"/>
<connect gate="A" pin="VOUT" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM4120AIM5-1.8"/>
<attribute name="OC_FARNELL" value="9778772"/>
<attribute name="OC_NEWARK" value="41K5424"/>
<attribute name="PACKAGE" value="SOT-23-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM4120AIM5-2.0" prefix="U">
<description>Precision Micropower Low Dropout Voltage Reference</description>
<gates>
<gate name="A" symbol="LM4120AIM5-2.0"/>
</gates>
<devices>
<device name="" package="SOT95P285X120-5N">
<connects>
<connect gate="A" pin="EN" pad="3"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="REF" pad="1"/>
<connect gate="A" pin="VIN" pad="4"/>
<connect gate="A" pin="VOUT" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM4120AIM5-2.0"/>
<attribute name="OC_FARNELL" value="9778780"/>
<attribute name="OC_NEWARK" value="41K5425"/>
<attribute name="PACKAGE" value="SOT-23-5"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM4120AIM5-2.5" prefix="U">
<description>Dropout voltage reference</description>
<gates>
<gate name="A" symbol="LM4120AIM5-2.5"/>
</gates>
<devices>
<device name="" package="SOT95P284X122-5N">
<connects>
<connect gate="A" pin="EN" pad="3"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="REF" pad="1"/>
<connect gate="A" pin="VIN" pad="4"/>
<connect gate="A" pin="VOUT" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM4120AIM5-2.5"/>
<attribute name="OC_FARNELL" value="9778799"/>
<attribute name="OC_NEWARK" value="41K5426"/>
<attribute name="PACKAGE" value="SOT-23-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM4120AIM5-3.0" prefix="U">
<description>Dropout voltage reference</description>
<gates>
<gate name="A" symbol="LM4120AIM5-3.0"/>
</gates>
<devices>
<device name="" package="SOT95P284X122-5N">
<connects>
<connect gate="A" pin="EN" pad="3"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="REF" pad="1"/>
<connect gate="A" pin="VIN" pad="4"/>
<connect gate="A" pin="VOUT" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM4120AIM5-3.0"/>
<attribute name="OC_FARNELL" value="9778802"/>
<attribute name="OC_NEWARK" value="74C4418"/>
<attribute name="PACKAGE" value="SOT-23-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM4120AIM5-3.3" prefix="U">
<description>Precision Micropower Low Dropout Voltage Reference</description>
<gates>
<gate name="A" symbol="LM4120AIM5-3.3"/>
</gates>
<devices>
<device name="" package="SOT95P285X120-5N">
<connects>
<connect gate="A" pin="EN" pad="3"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="REF" pad="1"/>
<connect gate="A" pin="VIN" pad="4"/>
<connect gate="A" pin="VOUT" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM4120AIM5-3.3"/>
<attribute name="OC_FARNELL" value="9778810"/>
<attribute name="OC_NEWARK" value="41K5428"/>
<attribute name="PACKAGE" value="SOT-23-5"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM4120AIM5-4.1" prefix="U">
<description>Literature Number</description>
<gates>
<gate name="A" symbol="LM4120AIM5-4.1"/>
</gates>
<devices>
<device name="" package="SOT95P284X122-5N">
<connects>
<connect gate="A" pin="EN" pad="3"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="REF" pad="1"/>
<connect gate="A" pin="VIN" pad="4"/>
<connect gate="A" pin="VOUT" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM4120AIM5-4.1"/>
<attribute name="OC_FARNELL" value="9778829"/>
<attribute name="OC_NEWARK" value="74C4420"/>
<attribute name="PACKAGE" value="SOT-23-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM4120AIM5-5.0" prefix="U">
<description>Precision Micropower Low Dropout Voltage Reference</description>
<gates>
<gate name="A" symbol="LM4120AIM5-5.0"/>
</gates>
<devices>
<device name="" package="SOT95P285X120-5N">
<connects>
<connect gate="A" pin="EN" pad="3"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="REF" pad="1"/>
<connect gate="A" pin="VIN" pad="4"/>
<connect gate="A" pin="VOUT" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM4120AIM5-5.0"/>
<attribute name="OC_FARNELL" value="9778837"/>
<attribute name="OC_NEWARK" value="41K5430"/>
<attribute name="PACKAGE" value="SOT-23-5"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM4120IM5-1.8" prefix="U">
<description>Precision Micropower Low Dropout Voltage Reference</description>
<gates>
<gate name="A" symbol="LM4120IM5-1.8"/>
</gates>
<devices>
<device name="" package="SOT95P285X120-5N">
<connects>
<connect gate="A" pin="EN" pad="3"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="REF" pad="1"/>
<connect gate="A" pin="VIN" pad="4"/>
<connect gate="A" pin="VOUT" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM4120IM5-1.8"/>
<attribute name="OC_FARNELL" value="1312740"/>
<attribute name="OC_NEWARK" value="31M5429"/>
<attribute name="PACKAGE" value="SOT-23-5"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM4120IM5-2.0" prefix="U">
<description>Precision Micropower Low Dropout Voltage Reference</description>
<gates>
<gate name="A" symbol="LM4120IM5-2.0"/>
</gates>
<devices>
<device name="" package="SOT95P285X120-5N">
<connects>
<connect gate="A" pin="EN" pad="3"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="REF" pad="1"/>
<connect gate="A" pin="VIN" pad="4"/>
<connect gate="A" pin="VOUT" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM4120IM5-2.0"/>
<attribute name="OC_FARNELL" value="1312743"/>
<attribute name="OC_NEWARK" value="41K5439"/>
<attribute name="PACKAGE" value="SOT-23-5"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM4120IM5-3.0" prefix="U">
<description>Precision Micropower Low Dropout Voltage Reference</description>
<gates>
<gate name="A" symbol="LM4120IM5-3.0"/>
</gates>
<devices>
<device name="" package="SOT95P285X120-5N">
<connects>
<connect gate="A" pin="EN" pad="3"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="REF" pad="1"/>
<connect gate="A" pin="VIN" pad="4"/>
<connect gate="A" pin="VOUT" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM4120IM5-3.0"/>
<attribute name="OC_FARNELL" value="1312745"/>
<attribute name="OC_NEWARK" value="41K5441"/>
<attribute name="PACKAGE" value="SOT-23-5"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM4120IM5-3.3" prefix="U">
<description>Precision Micropower Low Dropout Voltage Reference</description>
<gates>
<gate name="A" symbol="LM4120IM5-3.3"/>
</gates>
<devices>
<device name="" package="SOT95P285X120-5N">
<connects>
<connect gate="A" pin="EN" pad="3"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="REF" pad="1"/>
<connect gate="A" pin="VIN" pad="4"/>
<connect gate="A" pin="VOUT" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM4120IM5-3.3"/>
<attribute name="OC_FARNELL" value="1312746"/>
<attribute name="OC_NEWARK" value="20J4454"/>
<attribute name="PACKAGE" value="SOT-23-5"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM4120IM5-4.1" prefix="U">
<description>Precision Micropower Low Dropout Voltage Reference</description>
<gates>
<gate name="A" symbol="LM4120IM5-4.1"/>
</gates>
<devices>
<device name="" package="SOT95P285X120-5N">
<connects>
<connect gate="A" pin="EN" pad="3"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="REF" pad="1"/>
<connect gate="A" pin="VIN" pad="4"/>
<connect gate="A" pin="VOUT" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM4120IM5-4.1"/>
<attribute name="OC_FARNELL" value="1312747"/>
<attribute name="OC_NEWARK" value="74C4433"/>
<attribute name="PACKAGE" value="SOT-23-5"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM4120IM5-5.0" prefix="U">
<description>Precision Micropower Low Dropout Voltage Reference</description>
<gates>
<gate name="A" symbol="LM4120IM5-5.0"/>
</gates>
<devices>
<device name="" package="SOT95P285X120-5N">
<connects>
<connect gate="A" pin="EN" pad="3"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="REF" pad="1"/>
<connect gate="A" pin="VIN" pad="4"/>
<connect gate="A" pin="VOUT" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM4120IM5-5.0"/>
<attribute name="OC_FARNELL" value="1312748"/>
<attribute name="OC_NEWARK" value="41K5443"/>
<attribute name="PACKAGE" value="SOT-23-5"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM4132AMF-2.5" prefix="U">
<description>Precision Low Dropout Voltage Reference</description>
<gates>
<gate name="A" symbol="LM4132AMF-2.5"/>
</gates>
<devices>
<device name="" package="SOT95P284X122-5N">
<connects>
<connect gate="A" pin="EN" pad="3"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="NC" pad="1"/>
<connect gate="A" pin="VIN" pad="4"/>
<connect gate="A" pin="VREF" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM4132AMF-2.5"/>
<attribute name="OC_FARNELL" value="1312750"/>
<attribute name="OC_NEWARK" value="99K2466"/>
<attribute name="PACKAGE" value="SOT23-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM4132BMF-4.1" prefix="U">
<description>Precision Low Dropout Voltage Reference</description>
<gates>
<gate name="A" symbol="LM4132BMF-4.1"/>
</gates>
<devices>
<device name="" package="SOT95P284X122-5N">
<connects>
<connect gate="A" pin="EN" pad="3"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="NC" pad="1"/>
<connect gate="A" pin="VIN" pad="4"/>
<connect gate="A" pin="VREF" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM4132BMF-4.1"/>
<attribute name="OC_FARNELL" value="1312755"/>
<attribute name="OC_NEWARK" value="32M1158"/>
<attribute name="PACKAGE" value="SOT23-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM4132CMF-2.5" prefix="U">
<description>Precision Low Dropout Voltage Reference</description>
<gates>
<gate name="A" symbol="LM4132CMF-2.5"/>
</gates>
<devices>
<device name="" package="SOT95P284X122-5N">
<connects>
<connect gate="A" pin="EN" pad="3"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="NC" pad="1"/>
<connect gate="A" pin="VIN" pad="4"/>
<connect gate="A" pin="VREF" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM4132CMF-2.5"/>
<attribute name="OC_FARNELL" value="1312757"/>
<attribute name="OC_NEWARK" value="31M5439"/>
<attribute name="PACKAGE" value="SOT23-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM4132DMF-4.1" prefix="U">
<description>Precision Low Dropout Voltage Reference</description>
<gates>
<gate name="A" symbol="LM4132DMF-4.1"/>
</gates>
<devices>
<device name="" package="SOT95P284X122-5N">
<connects>
<connect gate="A" pin="EN" pad="3"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="N/C" pad="1"/>
<connect gate="A" pin="VIN" pad="4"/>
<connect gate="A" pin="VREF" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM4132DMF-4.1"/>
<attribute name="OC_FARNELL" value="1312761"/>
<attribute name="OC_NEWARK" value="-"/>
<attribute name="PACKAGE" value="SOT23-5"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM4132EMF-2.5" prefix="U">
<description>Dropout Voltage Reference</description>
<gates>
<gate name="A" symbol="LM4132EMF-2.5"/>
</gates>
<devices>
<device name="" package="SOT95P284X122-5N">
<connects>
<connect gate="A" pin="EN" pad="3"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="NC" pad="1"/>
<connect gate="A" pin="VIN" pad="4"/>
<connect gate="A" pin="VREF" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM4132EMF-2.5"/>
<attribute name="OC_FARNELL" value="1312763"/>
<attribute name="OC_NEWARK" value="65K6336"/>
<attribute name="PACKAGE" value="SOT-23-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM4132EMF-3.0" prefix="U">
<description>Dropout Voltage Reference</description>
<gates>
<gate name="A" symbol="LM4132EMF-3.0"/>
</gates>
<devices>
<device name="" package="SOT95P284X122-5N">
<connects>
<connect gate="A" pin="EN" pad="3"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="NC" pad="1"/>
<connect gate="A" pin="VIN" pad="4"/>
<connect gate="A" pin="VREF" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM4132EMF-30"/>
<attribute name="OC_FARNELL" value="1798324"/>
<attribute name="OC_NEWARK" value="73R9741"/>
<attribute name="PACKAGE" value="SOT-23-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM4140ACM-1.0" prefix="U">
<description>High Precision Low Noise Low Dropout Voltage</description>
<gates>
<gate name="A" symbol="LM4140ACM-1.0"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="EN" pad="3"/>
<connect gate="A" pin="GND" pad="1"/>
<connect gate="A" pin="GND_2" pad="7"/>
<connect gate="A" pin="GND_3" pad="8"/>
<connect gate="A" pin="GND_4" pad="4"/>
<connect gate="A" pin="NC" pad="5"/>
<connect gate="A" pin="VIN" pad="2"/>
<connect gate="A" pin="VREF" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM4140ACM-1.0"/>
<attribute name="OC_FARNELL" value="1286879"/>
<attribute name="OC_NEWARK" value="41K5471"/>
<attribute name="PACKAGE" value="8-SOIC"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM4140ACM-1.2" prefix="U">
<description>Voltage Refrence</description>
<gates>
<gate name="A" symbol="LM4140ACM-1.2"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="EN" pad="3"/>
<connect gate="A" pin="GND" pad="8"/>
<connect gate="A" pin="GND_2" pad="7"/>
<connect gate="A" pin="GND_3" pad="1"/>
<connect gate="A" pin="GND_4" pad="4"/>
<connect gate="A" pin="NC" pad="5"/>
<connect gate="A" pin="VIN" pad="2"/>
<connect gate="A" pin="VREF" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM4140ACM-1.2"/>
<attribute name="OC_FARNELL" value="1286880"/>
<attribute name="OC_NEWARK" value="41K5472"/>
<attribute name="PACKAGE" value="8-SOIC"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM4140ACM-2.0" prefix="U">
<description>Dropout voltage reference</description>
<gates>
<gate name="A" symbol="LM4140ACM-2.0"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="EN" pad="3"/>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="GND_2" pad="8"/>
<connect gate="A" pin="GND_3" pad="4"/>
<connect gate="A" pin="GND_4" pad="1"/>
<connect gate="A" pin="NC" pad="5"/>
<connect gate="A" pin="VIN" pad="2"/>
<connect gate="A" pin="VREF" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM4140ACM-2.0"/>
<attribute name="OC_FARNELL" value="1286881"/>
<attribute name="OC_NEWARK" value="24M3517"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM4140ACM-2.5" prefix="U">
<description>High Precision Low Noise Low Dropout Voltage</description>
<gates>
<gate name="A" symbol="LM4140ACM-2.5"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="EN" pad="3"/>
<connect gate="A" pin="GND" pad="1"/>
<connect gate="A" pin="GND_2" pad="7"/>
<connect gate="A" pin="GND_3" pad="8"/>
<connect gate="A" pin="GND_4" pad="4"/>
<connect gate="A" pin="NC" pad="5"/>
<connect gate="A" pin="VIN" pad="2"/>
<connect gate="A" pin="VREF" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM4140ACM-2.5"/>
<attribute name="OC_FARNELL" value="1286883"/>
<attribute name="OC_NEWARK" value="41K5474"/>
<attribute name="PACKAGE" value="8-SOIC"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM4140ACM-4.1" prefix="U">
<description>Dropout voltage reference</description>
<gates>
<gate name="A" symbol="LM4140ACM-4.1"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="EN" pad="3"/>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="GND_2" pad="8"/>
<connect gate="A" pin="GND_3" pad="4"/>
<connect gate="A" pin="GND_4" pad="1"/>
<connect gate="A" pin="NC" pad="5"/>
<connect gate="A" pin="VIN" pad="2"/>
<connect gate="A" pin="VREF" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM4140ACM-4.1"/>
<attribute name="OC_FARNELL" value="1286884"/>
<attribute name="OC_NEWARK" value="24M3519"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM4140BCM-1.0" prefix="U">
<description>Dropout voltage reference</description>
<gates>
<gate name="A" symbol="LM4140BCM-1.0"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="EN" pad="3"/>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="GND_2" pad="8"/>
<connect gate="A" pin="GND_3" pad="4"/>
<connect gate="A" pin="GND_4" pad="1"/>
<connect gate="A" pin="NC" pad="5"/>
<connect gate="A" pin="VIN" pad="2"/>
<connect gate="A" pin="VREF" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM4140BCM-1.0"/>
<attribute name="OC_FARNELL" value="1286885"/>
<attribute name="OC_NEWARK" value="41K5481"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM4140BCM-2.5" prefix="U">
<description>Dropout voltage reference</description>
<gates>
<gate name="A" symbol="LM4140BCM-2.5"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="EN" pad="3"/>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="GND_2" pad="8"/>
<connect gate="A" pin="GND_3" pad="4"/>
<connect gate="A" pin="GND_4" pad="1"/>
<connect gate="A" pin="NC" pad="5"/>
<connect gate="A" pin="VIN" pad="2"/>
<connect gate="A" pin="VREF" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM4140BCM-2.5"/>
<attribute name="OC_FARNELL" value="1286888"/>
<attribute name="OC_NEWARK" value="41K5484"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM4140BCM-4.1" prefix="U">
<description>Dropout voltage reference</description>
<gates>
<gate name="A" symbol="LM4140BCM-4.1"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="EN" pad="3"/>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="GND_2" pad="8"/>
<connect gate="A" pin="GND_3" pad="4"/>
<connect gate="A" pin="GND_4" pad="1"/>
<connect gate="A" pin="NC" pad="5"/>
<connect gate="A" pin="VIN" pad="2"/>
<connect gate="A" pin="VREF" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM4140BCM-4.1"/>
<attribute name="OC_FARNELL" value="1286889"/>
<attribute name="OC_NEWARK" value="41K5485"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM4140CCM-1.0" prefix="U">
<description>Dropout voltage reference</description>
<gates>
<gate name="A" symbol="LM4140CCM-1.0"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="EN" pad="3"/>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="GND_2" pad="8"/>
<connect gate="A" pin="GND_3" pad="4"/>
<connect gate="A" pin="GND_4" pad="1"/>
<connect gate="A" pin="NC" pad="5"/>
<connect gate="A" pin="VIN" pad="2"/>
<connect gate="A" pin="VREF" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM4140CCM-1.0"/>
<attribute name="OC_FARNELL" value="1286890"/>
<attribute name="OC_NEWARK" value="41K5491"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM4140CCM-1.2" prefix="U">
<description>Dropout voltage reference</description>
<gates>
<gate name="A" symbol="LM4140CCM-1.2"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="EN" pad="3"/>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="GND_2" pad="8"/>
<connect gate="A" pin="GND_3" pad="4"/>
<connect gate="A" pin="GND_4" pad="1"/>
<connect gate="A" pin="NC" pad="5"/>
<connect gate="A" pin="VIN" pad="2"/>
<connect gate="A" pin="VREF" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM4140CCM-1.2"/>
<attribute name="OC_FARNELL" value="1286891"/>
<attribute name="OC_NEWARK" value="41K5492"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM4140CCM-2.0" prefix="U">
<description>Voltage Refrence</description>
<gates>
<gate name="A" symbol="LM4140CCM-2.0"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="EN" pad="3"/>
<connect gate="A" pin="GND" pad="8"/>
<connect gate="A" pin="GND_2" pad="7"/>
<connect gate="A" pin="GND_3" pad="1"/>
<connect gate="A" pin="GND_4" pad="4"/>
<connect gate="A" pin="NC" pad="5"/>
<connect gate="A" pin="VIN" pad="2"/>
<connect gate="A" pin="VREF" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM4140CCM-2.0"/>
<attribute name="OC_FARNELL" value="1286892"/>
<attribute name="OC_NEWARK" value="41K5493"/>
<attribute name="PACKAGE" value="8-SOIC"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM4140CCM-2.5" prefix="U">
<description>Voltage Refrence</description>
<gates>
<gate name="A" symbol="LM4140CCM-2.5"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="EN" pad="3"/>
<connect gate="A" pin="GND" pad="8"/>
<connect gate="A" pin="GND_2" pad="7"/>
<connect gate="A" pin="GND_3" pad="1"/>
<connect gate="A" pin="GND_4" pad="4"/>
<connect gate="A" pin="NC" pad="5"/>
<connect gate="A" pin="VIN" pad="2"/>
<connect gate="A" pin="VREF" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM4140CCM-2.5"/>
<attribute name="OC_FARNELL" value="1286893"/>
<attribute name="OC_NEWARK" value="41K5494"/>
<attribute name="PACKAGE" value="8-SOIC"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM4140CCM-4.1" prefix="U">
<description>Dropout voltage reference</description>
<gates>
<gate name="A" symbol="LM4140CCM-4.1"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="EN" pad="3"/>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="GND_2" pad="8"/>
<connect gate="A" pin="GND_3" pad="4"/>
<connect gate="A" pin="GND_4" pad="1"/>
<connect gate="A" pin="NC" pad="5"/>
<connect gate="A" pin="VIN" pad="2"/>
<connect gate="A" pin="VREF" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM4140CCM-4.1"/>
<attribute name="OC_FARNELL" value="1286895"/>
<attribute name="OC_NEWARK" value="41K5495"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM4250CM" prefix="U">
<description>Programmable Operational Amplifier</description>
<gates>
<gate name="A" symbol="LM4250CM"/>
</gates>
<devices>
<device name="" package="SOIC127P620X175-8N">
<connects>
<connect gate="A" pin="NEG" pad="2"/>
<connect gate="A" pin="OFFSETNULL" pad="1"/>
<connect gate="A" pin="OFFSETNULL_2" pad="5"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="POS" pad="3"/>
<connect gate="A" pin="QUISCENT_ISET" pad="8"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM4250CM"/>
<attribute name="OC_FARNELL" value="1798366"/>
<attribute name="OC_NEWARK" value="73R9742"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM4250CN" prefix="U">
<description>OP AMP</description>
<gates>
<gate name="A" symbol="LM4250CN"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-8">
<connects>
<connect gate="A" pin="NEG" pad="2"/>
<connect gate="A" pin="OFFSET_NULL" pad="5"/>
<connect gate="A" pin="OFFSET_NULL_2" pad="1"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="POS" pad="3"/>
<connect gate="A" pin="QUIESCENT_CURRENT_SET" pad="8"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM4250CN"/>
<attribute name="OC_FARNELL" value="9486798"/>
<attribute name="OC_NEWARK" value="97K3524"/>
<attribute name="PACKAGE" value="8-DIP"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM4308GR" prefix="U">
<description>18-bit CPU Display</description>
<gates>
<gate name="A" symbol="LM4308GR"/>
</gates>
<devices>
<device name="" package="BGA49C7X7X50P_400X400X110">
<connects>
<connect gate="A" pin="AD" pad="A1"/>
<connect gate="A" pin="CS1" pad="A2"/>
<connect gate="A" pin="CS2" pad="C2"/>
<connect gate="A" pin="D0" pad="E1"/>
<connect gate="A" pin="D1" pad="E2"/>
<connect gate="A" pin="D10" pad="G6"/>
<connect gate="A" pin="D11" pad="F6"/>
<connect gate="A" pin="D12" pad="G7"/>
<connect gate="A" pin="D13" pad="F7"/>
<connect gate="A" pin="D14" pad="E6"/>
<connect gate="A" pin="D15" pad="E7"/>
<connect gate="A" pin="D16" pad="D6"/>
<connect gate="A" pin="D17" pad="C7"/>
<connect gate="A" pin="D2" pad="F1"/>
<connect gate="A" pin="D3" pad="F2"/>
<connect gate="A" pin="D4" pad="G1"/>
<connect gate="A" pin="D5" pad="G2"/>
<connect gate="A" pin="D6" pad="F3"/>
<connect gate="A" pin="D7" pad="G3"/>
<connect gate="A" pin="D8" pad="G5"/>
<connect gate="A" pin="D9" pad="F5"/>
<connect gate="A" pin="DCN_S/DDN_M" pad="A6"/>
<connect gate="A" pin="DCP_S/DDP_M" pad="A7"/>
<connect gate="A" pin="DDN_S/DCN_M" pad="A5"/>
<connect gate="A" pin="DDP_S/DCP_M" pad="A4"/>
<connect gate="A" pin="ERR" pad="C6"/>
<connect gate="A" pin="M/S" pad="B3"/>
<connect gate="A" pin="PD" pad="A3"/>
<connect gate="A" pin="RD" pad="D2"/>
<connect gate="A" pin="RDS0/PLLCON0" pad="B6"/>
<connect gate="A" pin="RDS1/PLLCON1" pad="B7"/>
<connect gate="A" pin="TM" pad="B2"/>
<connect gate="A" pin="VDD" pad="G4"/>
<connect gate="A" pin="VDDA" pad="B5"/>
<connect gate="A" pin="VDDIO" pad="D7"/>
<connect gate="A" pin="VDDIO_2" pad="D1"/>
<connect gate="A" pin="VSS" pad="F4"/>
<connect gate="A" pin="VSSA" pad="B4"/>
<connect gate="A" pin="VSSIO" pad="C5"/>
<connect gate="A" pin="VSSIO_2" pad="D4"/>
<connect gate="A" pin="VSSIO_3" pad="D5"/>
<connect gate="A" pin="VSSIO_4" pad="C4"/>
<connect gate="A" pin="VSSIO_5" pad="D3"/>
<connect gate="A" pin="VSSIO_6" pad="E3"/>
<connect gate="A" pin="VSSIO_7" pad="E5"/>
<connect gate="A" pin="VSSIO_8" pad="C3"/>
<connect gate="A" pin="VSSIO_9" pad="E4"/>
<connect gate="A" pin="WO" pad="B1"/>
<connect gate="A" pin="WR" pad="C1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM4308GR"/>
<attribute name="OC_FARNELL" value="1609188"/>
<attribute name="OC_NEWARK" value="12N2277"/>
<attribute name="PACKAGE" value="BGA-49"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM4308SQ" prefix="U">
<description>18-bit CPU Display</description>
<gates>
<gate name="A" symbol="LM4308SQ"/>
</gates>
<devices>
<device name="" package="QFN40P500X500X80-41N">
<connects>
<connect gate="A" pin="AD" pad="1"/>
<connect gate="A" pin="CLK/WO" pad="2"/>
<connect gate="A" pin="D0" pad="7"/>
<connect gate="A" pin="D1" pad="8"/>
<connect gate="A" pin="D10" pad="19"/>
<connect gate="A" pin="D11" pad="20"/>
<connect gate="A" pin="D12" pad="21"/>
<connect gate="A" pin="D13" pad="22"/>
<connect gate="A" pin="D14" pad="23"/>
<connect gate="A" pin="D15" pad="24"/>
<connect gate="A" pin="D16" pad="25"/>
<connect gate="A" pin="D17" pad="27"/>
<connect gate="A" pin="D2" pad="9"/>
<connect gate="A" pin="D3" pad="10"/>
<connect gate="A" pin="D4" pad="11"/>
<connect gate="A" pin="D5" pad="12"/>
<connect gate="A" pin="D6" pad="13"/>
<connect gate="A" pin="D7" pad="14"/>
<connect gate="A" pin="D8" pad="17"/>
<connect gate="A" pin="D9" pad="18"/>
<connect gate="A" pin="DCN/DDN" pad="34"/>
<connect gate="A" pin="DCP/DDP" pad="36"/>
<connect gate="A" pin="DDN/DCN" pad="32"/>
<connect gate="A" pin="DDP/DCP" pad="31"/>
<connect gate="A" pin="EPAD" pad="41"/>
<connect gate="A" pin="ERR" pad="28"/>
<connect gate="A" pin="M/~S" pad="38"/>
<connect gate="A" pin="NC" pad="15"/>
<connect gate="A" pin="PLLCON0/RDS0" pad="30"/>
<connect gate="A" pin="PLLCON1/RDS1" pad="29"/>
<connect gate="A" pin="TM" pad="40"/>
<connect gate="A" pin="VDD" pad="16"/>
<connect gate="A" pin="VDDA" pad="33"/>
<connect gate="A" pin="VDDIO" pad="26"/>
<connect gate="A" pin="VDDIO_2" pad="6"/>
<connect gate="A" pin="VSSA" pad="35"/>
<connect gate="A" pin="~CS~1" pad="39"/>
<connect gate="A" pin="~CS~2" pad="3"/>
<connect gate="A" pin="~PD" pad="37"/>
<connect gate="A" pin="~RD" pad="5"/>
<connect gate="A" pin="~WR" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM4308SQ"/>
<attribute name="OC_FARNELL" value="1609189"/>
<attribute name="OC_NEWARK" value="12N2278"/>
<attribute name="PACKAGE" value="QFN-40"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM432MA" prefix="U">
<description>OpAmpIC</description>
<gates>
<gate name="A" symbol="LM432MA"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="AIN+" pad="3"/>
<connect gate="A" pin="AIN-" pad="2"/>
<connect gate="A" pin="AOUT" pad="1"/>
<connect gate="A" pin="BIN+" pad="5"/>
<connect gate="A" pin="BIN-" pad="6"/>
<connect gate="A" pin="BOUT" pad="7"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="VS" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM432MA"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K5534"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM4510SD" prefix="U">
<description>Synchronous Step-Up DC/DC Converter</description>
<gates>
<gate name="A" symbol="LM4510SD"/>
</gates>
<devices>
<device name="" package="DFN300X300X80-11N">
<connects>
<connect gate="A" pin="AGND" pad="6"/>
<connect gate="A" pin="COMP" pad="7"/>
<connect gate="A" pin="EN" pad="4"/>
<connect gate="A" pin="EPAD" pad="11"/>
<connect gate="A" pin="FB" pad="8"/>
<connect gate="A" pin="NC" pad="9"/>
<connect gate="A" pin="PGND" pad="2"/>
<connect gate="A" pin="SS" pad="5"/>
<connect gate="A" pin="SW" pad="1"/>
<connect gate="A" pin="VIN" pad="3"/>
<connect gate="A" pin="VOUT" pad="10"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM4510SD"/>
<attribute name="OC_FARNELL" value="1675316"/>
<attribute name="OC_NEWARK" value="64M7022"/>
<attribute name="PACKAGE" value="DFN-10"/>
<attribute name="SUPPLIER" value="National semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM4562HA" prefix="U">
<description>IC OPAMP AUDIO STER AB</description>
<gates>
<gate name="A" symbol="LM4562HA"/>
</gates>
<devices>
<device name="" package="TO254P914X470-8P">
<connects>
<connect gate="A" pin="+INA" pad="3"/>
<connect gate="A" pin="+INB" pad="5"/>
<connect gate="A" pin="-INA" pad="2"/>
<connect gate="A" pin="-INB" pad="6"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM4562HA"/>
<attribute name="OC_FARNELL" value="1685364"/>
<attribute name="OC_NEWARK" value="32M1173"/>
<attribute name="PACKAGE" value="TO-99-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM4562MA" prefix="U">
<description>Operational Amplifier</description>
<gates>
<gate name="A" symbol="LM4562MA"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="NEG_A" pad="2"/>
<connect gate="A" pin="NEG_B" pad="6"/>
<connect gate="A" pin="OUT_A" pad="1"/>
<connect gate="A" pin="OUT_B" pad="7"/>
<connect gate="A" pin="POS_A" pad="3"/>
<connect gate="A" pin="POS_B" pad="5"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM4562MA"/>
<attribute name="OC_FARNELL" value="1685365"/>
<attribute name="OC_NEWARK" value="32M1175"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM4562NA" prefix="U">
<description>Operational Amplifier</description>
<gates>
<gate name="A" symbol="LM4562NA"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-8">
<connects>
<connect gate="A" pin="NEG_A" pad="3"/>
<connect gate="A" pin="NEG_B" pad="6"/>
<connect gate="A" pin="OUT_A" pad="1"/>
<connect gate="A" pin="OUT_B" pad="7"/>
<connect gate="A" pin="POS_A" pad="2"/>
<connect gate="A" pin="POS_B" pad="5"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM4562NA"/>
<attribute name="OC_FARNELL" value="1685366"/>
<attribute name="OC_NEWARK" value="32M1177"/>
<attribute name="PACKAGE" value="DIP-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM4570LQ" prefix="U">
<description>IC MOTOR DRIVER</description>
<gates>
<gate name="A" symbol="LM4570LQ"/>
</gates>
<devices>
<device name="" package="QFN65P200X200X80-9N">
<connects>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="HEAT_PAD" pad="9"/>
<connect gate="A" pin="IN" pad="3"/>
<connect gate="A" pin="REF1" pad="1"/>
<connect gate="A" pin="REF2" pad="2"/>
<connect gate="A" pin="SHDN" pad="8"/>
<connect gate="A" pin="VDD" pad="5"/>
<connect gate="A" pin="VO1" pad="4"/>
<connect gate="A" pin="VO2" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM4570LQ"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="99K2473"/>
<attribute name="PACKAGE" value="QFN-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM45BIM3" prefix="U">
<description>Temperature Sensor</description>
<gates>
<gate name="A" symbol="LM45BIM3"/>
</gates>
<devices>
<device name="" package="SOT95P251X112-3N">
<connects>
<connect gate="A" pin="+VS" pad="1"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="VO" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM45BIM3"/>
<attribute name="OC_FARNELL" value="9779876"/>
<attribute name="OC_NEWARK" value="33K4200"/>
<attribute name="PACKAGE" value="SOT-23-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM45CIM3" prefix="U">
<description>Temperature Sensor</description>
<gates>
<gate name="A" symbol="LM45CIM3"/>
</gates>
<devices>
<device name="" package="SOT95P251X112-3N">
<connects>
<connect gate="A" pin="+VS" pad="1"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="VO" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM45CIM3"/>
<attribute name="OC_FARNELL" value="9779310"/>
<attribute name="OC_NEWARK" value="41K5539"/>
<attribute name="PACKAGE" value="SOT-23-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM4667MM" prefix="U">
<description>Audio Amplifier</description>
<gates>
<gate name="A" symbol="LM4667MM"/>
</gates>
<devices>
<device name="" package="SOP50P490X109-10N">
<connects>
<connect gate="A" pin="GAINSELECT" pad="5"/>
<connect gate="A" pin="GND" pad="8"/>
<connect gate="A" pin="GND_2" pad="7"/>
<connect gate="A" pin="IN+" pad="4"/>
<connect gate="A" pin="IN-" pad="2"/>
<connect gate="A" pin="NC" pad="3"/>
<connect gate="A" pin="VDD" pad="9"/>
<connect gate="A" pin="VO1" pad="6"/>
<connect gate="A" pin="VO2" pad="10"/>
<connect gate="A" pin="~SD" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM4667MM"/>
<attribute name="OC_FARNELL" value="8181080"/>
<attribute name="OC_NEWARK" value="38K3737"/>
<attribute name="PACKAGE" value="MSOP-10"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM4670ITL" prefix="U">
<description>Switching Audio Amplifier</description>
<gates>
<gate name="A" symbol="LM4670ITL"/>
</gates>
<devices>
<device name="" package="BGA9C3X3X50P_146X146X60">
<connects>
<connect gate="A" pin="GND" pad="B3"/>
<connect gate="A" pin="GND_2" pad="A2"/>
<connect gate="A" pin="IN+" pad="A1"/>
<connect gate="A" pin="IN-" pad="C1"/>
<connect gate="A" pin="PVDD" pad="B2"/>
<connect gate="A" pin="VDD" pad="B1"/>
<connect gate="A" pin="VO1" pad="A3"/>
<connect gate="A" pin="VO2" pad="C3"/>
<connect gate="A" pin="~SHDN" pad="C2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM4670ITL"/>
<attribute name="OC_FARNELL" value="1286809"/>
<attribute name="OC_NEWARK" value="26M0394"/>
<attribute name="PACKAGE" value="BGA-9"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM4670SD" prefix="U">
<description>Switching Audio Amplifier</description>
<gates>
<gate name="A" symbol="LM4670SD"/>
</gates>
<devices>
<device name="" package="DFN300X300X80-9N">
<connects>
<connect gate="A" pin="EP" pad="9"/>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="GND_2" pad="4"/>
<connect gate="A" pin="IN+" pad="3"/>
<connect gate="A" pin="IN-" pad="2"/>
<connect gate="A" pin="VDD" pad="7"/>
<connect gate="A" pin="VO1" pad="5"/>
<connect gate="A" pin="VO2" pad="8"/>
<connect gate="A" pin="~SHDN" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM4670SD"/>
<attribute name="OC_FARNELL" value="1312668"/>
<attribute name="OC_NEWARK" value="31M5444"/>
<attribute name="PACKAGE" value="LLP-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM4673SD" prefix="U">
<description>Audio Power Amplifier</description>
<gates>
<gate name="A" symbol="LM4673SD"/>
</gates>
<devices>
<device name="" package="DFN300X300X80-9N">
<connects>
<connect gate="A" pin="EP" pad="9"/>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="IN+" pad="2"/>
<connect gate="A" pin="IN-" pad="1"/>
<connect gate="A" pin="PVDD" pad="7"/>
<connect gate="A" pin="VDD" pad="3"/>
<connect gate="A" pin="VO1" pad="5"/>
<connect gate="A" pin="VO2" pad="8"/>
<connect gate="A" pin="~SD" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM4673SD"/>
<attribute name="OC_FARNELL" value="1312767"/>
<attribute name="OC_NEWARK" value="99K2476"/>
<attribute name="PACKAGE" value="LLP-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM4673TM" prefix="U">
<description>Power Amplifier</description>
<gates>
<gate name="A" symbol="LM4673TM"/>
</gates>
<devices>
<device name="" package="BGA9C40P3X3_140X140X60">
<connects>
<connect gate="A" pin="GND" pad="A2"/>
<connect gate="A" pin="IN+" pad="A1"/>
<connect gate="A" pin="IN-" pad="C1"/>
<connect gate="A" pin="PGND" pad="B3"/>
<connect gate="A" pin="PVDD" pad="C3"/>
<connect gate="A" pin="PVDD_2" pad="B2"/>
<connect gate="A" pin="VDD" pad="B1"/>
<connect gate="A" pin="VO1" pad="A3"/>
<connect gate="A" pin="~SD" pad="C2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM4673TM"/>
<attribute name="OC_FARNELL" value="1286897"/>
<attribute name="OC_NEWARK" value="26M0395"/>
<attribute name="PACKAGE" value="BGA-9"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM4675SD" prefix="U">
<description>Power Amplifier</description>
<gates>
<gate name="A" symbol="LM4675SD"/>
</gates>
<devices>
<device name="" package="DFN300X300X80-9N">
<connects>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="HEAT_PAD" pad="9"/>
<connect gate="A" pin="IN+" pad="1"/>
<connect gate="A" pin="IN-" pad="2"/>
<connect gate="A" pin="PVDD" pad="7"/>
<connect gate="A" pin="VDD" pad="3"/>
<connect gate="A" pin="VO1" pad="5"/>
<connect gate="A" pin="VO2" pad="8"/>
<connect gate="A" pin="~SHDN" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM4675SD"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="32M1181"/>
<attribute name="PACKAGE" value="DFN-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM4702BTA" prefix="U">
<description>IC AMP AUDIO PWR 300W</description>
<gates>
<gate name="A" symbol="LM4702BTA"/>
</gates>
<devices>
<device name="" package="AMP_LM4702BTA">
<connects>
<connect gate="A" pin="COMP1" pad="4"/>
<connect gate="A" pin="COMP2" pad="10"/>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="IN1+" pad="6"/>
<connect gate="A" pin="IN1-" pad="5"/>
<connect gate="A" pin="IN2+" pad="8"/>
<connect gate="A" pin="IN2-" pad="9"/>
<connect gate="A" pin="MUTE" pad="1"/>
<connect gate="A" pin="SINK1" pad="3"/>
<connect gate="A" pin="SINK2" pad="11"/>
<connect gate="A" pin="SOURCE1" pad="2"/>
<connect gate="A" pin="SOURCE2" pad="12"/>
<connect gate="A" pin="VCC+" pad="14"/>
<connect gate="A" pin="VCC+_2" pad="13"/>
<connect gate="A" pin="VEE-" pad="15"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM4702BTA"/>
<attribute name="OC_FARNELL" value="1685367"/>
<attribute name="OC_NEWARK" value="32M1186"/>
<attribute name="PACKAGE" value="TO220-15"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM4702CTA" prefix="U">
<description>IC, AUDIO POWER AMP, AB, 300W</description>
<gates>
<gate name="A" symbol="LM4702CTA"/>
</gates>
<devices>
<device name="" package="AMP_LM4702CTA">
<connects>
<connect gate="A" pin="COMP1" pad="4"/>
<connect gate="A" pin="COMP2" pad="10"/>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="IN1+" pad="6"/>
<connect gate="A" pin="IN1-" pad="5"/>
<connect gate="A" pin="IN2+" pad="8"/>
<connect gate="A" pin="IN2-" pad="9"/>
<connect gate="A" pin="MUTE" pad="1"/>
<connect gate="A" pin="SINK1" pad="3"/>
<connect gate="A" pin="SINK2" pad="11"/>
<connect gate="A" pin="SOURCE1" pad="2"/>
<connect gate="A" pin="SOURCE2" pad="12"/>
<connect gate="A" pin="VCC+" pad="14"/>
<connect gate="A" pin="VCC+_2" pad="13"/>
<connect gate="A" pin="VEE-" pad="15"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM4702CTA"/>
<attribute name="OC_FARNELL" value="1286760"/>
<attribute name="OC_NEWARK" value="69K2549"/>
<attribute name="PACKAGE" value="TO220-15"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM4752TS" prefix="U">
<description>Power Amplifier</description>
<gates>
<gate name="A" symbol="LM4752TS"/>
</gates>
<devices>
<device name="" package="TO127P1435X464-8N">
<connects>
<connect gate="A" pin="BIAS" pad="5"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="INA" pad="6"/>
<connect gate="A" pin="INB" pad="2"/>
<connect gate="A" pin="OUTA" pad="7"/>
<connect gate="A" pin="OUTB" pad="1"/>
<connect gate="A" pin="TAB" pad="8"/>
<connect gate="A" pin="VCC" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM4752TS"/>
<attribute name="OC_FARNELL" value="1798325"/>
<attribute name="OC_NEWARK" value="73R9744"/>
<attribute name="PACKAGE" value="TO-263-7"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM4755TS" prefix="U">
<description>IC AMP AUDIO PWR 11W AB</description>
<gates>
<gate name="A" symbol="LM4755TS"/>
</gates>
<devices>
<device name="" package="TO97P1435X457-10N">
<connects>
<connect gate="A" pin="BIAS" pad="6"/>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="INA" pad="7"/>
<connect gate="A" pin="INB" pad="3"/>
<connect gate="A" pin="MUTE" pad="2"/>
<connect gate="A" pin="NC" pad="9"/>
<connect gate="A" pin="OUTA" pad="8"/>
<connect gate="A" pin="OUTB" pad="1"/>
<connect gate="A" pin="TAB" pad="10"/>
<connect gate="A" pin="VCC" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM4755TS"/>
<attribute name="OC_FARNELL" value="1685378"/>
<attribute name="OC_NEWARK" value="41K5585"/>
<attribute name="PACKAGE" value="TO263-9"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM4765T" prefix="U">
<description>IC AMP AUDIO PWR 30W AB</description>
<gates>
<gate name="A" symbol="LM4765T"/>
</gates>
<devices>
<device name="" package="AMP_LM4765T">
<connects>
<connect gate="A" pin="+IN_A" pad="8"/>
<connect gate="A" pin="+IN_B" pad="13"/>
<connect gate="A" pin="-IN_A" pad="7"/>
<connect gate="A" pin="-IN_B" pad="12"/>
<connect gate="A" pin="GND_A" pad="5"/>
<connect gate="A" pin="GND_B" pad="10"/>
<connect gate="A" pin="MUTE_A" pad="6"/>
<connect gate="A" pin="MUTE_B" pad="11"/>
<connect gate="A" pin="OUTA" pad="3"/>
<connect gate="A" pin="OUTB" pad="1"/>
<connect gate="A" pin="STANDBY_A" pad="9"/>
<connect gate="A" pin="STANDBY_B" pad="14"/>
<connect gate="A" pin="VCCA" pad="2"/>
<connect gate="A" pin="VCC_B" pad="15"/>
<connect gate="A" pin="VEE" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM4765T"/>
<attribute name="OC_FARNELL" value="1685341"/>
<attribute name="OC_NEWARK" value="41K5588"/>
<attribute name="PACKAGE" value="TO220-15"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM4766T" prefix="U">
<description>IC, AUDIO PWR AMP CLASS AB 40W</description>
<gates>
<gate name="A" symbol="LM4766T"/>
</gates>
<devices>
<device name="" package="AMP_LM4766T">
<connects>
<connect gate="A" pin="+IN_A" pad="8"/>
<connect gate="A" pin="+IN_B" pad="13"/>
<connect gate="A" pin="-IN_A" pad="7"/>
<connect gate="A" pin="-IN_B" pad="12"/>
<connect gate="A" pin="GND_A" pad="5"/>
<connect gate="A" pin="GND_B" pad="10"/>
<connect gate="A" pin="MUTE_A" pad="6"/>
<connect gate="A" pin="MUTE_B" pad="11"/>
<connect gate="A" pin="NC" pad="14"/>
<connect gate="A" pin="NC_2" pad="9"/>
<connect gate="A" pin="OUTA" pad="3"/>
<connect gate="A" pin="OUTB" pad="1"/>
<connect gate="A" pin="VCC_A" pad="2"/>
<connect gate="A" pin="VCC_B" pad="15"/>
<connect gate="A" pin="VEE" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM4766T"/>
<attribute name="OC_FARNELL" value="9485864"/>
<attribute name="OC_NEWARK" value="41K5589"/>
<attribute name="PACKAGE" value="TO-220-15"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM4766TF" prefix="U">
<description>IC AMP AUDIO PWR 40W AB</description>
<gates>
<gate name="A" symbol="LM4766TF"/>
</gates>
<devices>
<device name="" package="AMP_LM4766TF">
<connects>
<connect gate="A" pin="+IN_A" pad="8"/>
<connect gate="A" pin="+IN_B" pad="13"/>
<connect gate="A" pin="-IN_A" pad="7"/>
<connect gate="A" pin="-IN_B" pad="12"/>
<connect gate="A" pin="GND_A" pad="5"/>
<connect gate="A" pin="GND_B" pad="10"/>
<connect gate="A" pin="MUTE_A" pad="6"/>
<connect gate="A" pin="MUTE_B" pad="11"/>
<connect gate="A" pin="NC" pad="14"/>
<connect gate="A" pin="NC_2" pad="9"/>
<connect gate="A" pin="OUTA" pad="3"/>
<connect gate="A" pin="OUTB" pad="1"/>
<connect gate="A" pin="VCC_A" pad="2"/>
<connect gate="A" pin="VCC_B" pad="15"/>
<connect gate="A" pin="VEE" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM4766TF"/>
<attribute name="OC_FARNELL" value="1685379"/>
<attribute name="OC_NEWARK" value="41K5590"/>
<attribute name="PACKAGE" value="TO220-15"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM4780TA" prefix="U">
<description>IC, AUDIO PWR AMP CLASS AB 60W</description>
<gates>
<gate name="A" symbol="LM4780TA"/>
</gates>
<devices>
<device name="" package="AMP_LM4780TA">
<connects>
<connect gate="A" pin="+IN_A" pad="16"/>
<connect gate="A" pin="+IN_B" pad="22"/>
<connect gate="A" pin="-IN_A" pad="15"/>
<connect gate="A" pin="-IN_B" pad="21"/>
<connect gate="A" pin="GND" pad="12"/>
<connect gate="A" pin="GND_2" pad="19"/>
<connect gate="A" pin="MUTE_A" pad="14"/>
<connect gate="A" pin="MUTE_B" pad="20"/>
<connect gate="A" pin="NC" pad="26"/>
<connect gate="A" pin="NC_2" pad="13"/>
<connect gate="A" pin="NC_3" pad="1"/>
<connect gate="A" pin="NC_4" pad="3"/>
<connect gate="A" pin="NC_5" pad="6"/>
<connect gate="A" pin="NC_6" pad="23"/>
<connect gate="A" pin="NC_7" pad="24"/>
<connect gate="A" pin="OUT_A" pad="7"/>
<connect gate="A" pin="OUT_B" pad="25"/>
<connect gate="A" pin="V+" pad="17"/>
<connect gate="A" pin="V+_2" pad="5"/>
<connect gate="A" pin="V+_3" pad="8"/>
<connect gate="A" pin="V+_4" pad="9"/>
<connect gate="A" pin="V+_5" pad="27"/>
<connect gate="A" pin="V-" pad="11"/>
<connect gate="A" pin="V-_2" pad="18"/>
<connect gate="A" pin="V-_3" pad="2"/>
<connect gate="A" pin="V-_4" pad="4"/>
<connect gate="A" pin="V-_5" pad="10"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM4780TA"/>
<attribute name="OC_FARNELL" value="9490620"/>
<attribute name="OC_NEWARK" value="55K6809"/>
<attribute name="PACKAGE" value="TO-220-27"/>
<attribute name="SUPPLIER" value="NATIONAL SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM4781TA" prefix="U">
<description>IC AMP AUDIO PWR 35W</description>
<gates>
<gate name="A" symbol="LM4781TA"/>
</gates>
<devices>
<device name="" package="AMP_LM4781TA">
<connects>
<connect gate="A" pin="GND" pad="24"/>
<connect gate="A" pin="GND_2" pad="10"/>
<connect gate="A" pin="GND_3" pad="19"/>
<connect gate="A" pin="IN1+" pad="13"/>
<connect gate="A" pin="IN1-" pad="12"/>
<connect gate="A" pin="IN2+" pad="16"/>
<connect gate="A" pin="IN2-" pad="21"/>
<connect gate="A" pin="IN3+" pad="27"/>
<connect gate="A" pin="IN3-" pad="26"/>
<connect gate="A" pin="MUTE1" pad="11"/>
<connect gate="A" pin="MUTE2" pad="20"/>
<connect gate="A" pin="MUTE3" pad="25"/>
<connect gate="A" pin="NC" pad="22"/>
<connect gate="A" pin="NC_2" pad="9"/>
<connect gate="A" pin="NC_3" pad="6"/>
<connect gate="A" pin="NC_4" pad="18"/>
<connect gate="A" pin="NC_5" pad="3"/>
<connect gate="A" pin="NC_6" pad="4"/>
<connect gate="A" pin="OUT1" pad="7"/>
<connect gate="A" pin="OUT2" pad="15"/>
<connect gate="A" pin="OUT3" pad="23"/>
<connect gate="A" pin="V+" pad="14"/>
<connect gate="A" pin="V+_2" pad="1"/>
<connect gate="A" pin="V+_3" pad="5"/>
<connect gate="A" pin="V-" pad="17"/>
<connect gate="A" pin="V-_2" pad="2"/>
<connect gate="A" pin="V-_3" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM4781TA"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="88H0509"/>
<attribute name="PACKAGE" value="27-TO-220"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM4808M" prefix="U">
<description>Headphone Amplifier</description>
<gates>
<gate name="A" symbol="LM4808M"/>
</gates>
<devices>
<device name="" package="SOIC127P620X175-8N">
<connects>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="IN_A+" pad="3"/>
<connect gate="A" pin="IN_A-" pad="2"/>
<connect gate="A" pin="IN_B+" pad="5"/>
<connect gate="A" pin="IN_B-" pad="6"/>
<connect gate="A" pin="OUT_A" pad="1"/>
<connect gate="A" pin="OUT_B" pad="7"/>
<connect gate="A" pin="VDD" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM4808M"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K5597"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM4808MM" prefix="U">
<description>Headphone Amplifier</description>
<gates>
<gate name="A" symbol="LM4808MM"/>
</gates>
<devices>
<device name="" package="SOP65P490X109-8N">
<connects>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="IN_A_+" pad="3"/>
<connect gate="A" pin="IN_A_-" pad="2"/>
<connect gate="A" pin="IN_B+" pad="5"/>
<connect gate="A" pin="IN_B-" pad="6"/>
<connect gate="A" pin="OUT_A" pad="1"/>
<connect gate="A" pin="OUT_B" pad="7"/>
<connect gate="A" pin="VDD" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM4808MM"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K5598"/>
<attribute name="PACKAGE" value="SOP-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM4809MM" prefix="U">
<description>Dual 105mW Headphone Amplifier</description>
<gates>
<gate name="A" symbol="LM4809MM"/>
</gates>
<devices>
<device name="" package="SOP65P490X110-8N">
<connects>
<connect gate="A" pin="BYPASS" pad="3"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="VDD" pad="8"/>
<connect gate="A" pin="VIN2" pad="6"/>
<connect gate="A" pin="VIN_1" pad="2"/>
<connect gate="A" pin="VOUT1" pad="1"/>
<connect gate="A" pin="VOUT2" pad="7"/>
<connect gate="A" pin="~SHDN" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM4809MM"/>
<attribute name="OC_FARNELL" value="1798326"/>
<attribute name="OC_NEWARK" value="73R9745"/>
<attribute name="PACKAGE" value="MSOP-8"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM48100QMH" prefix="U">
<description>Audio Power Amplifier</description>
<gates>
<gate name="A" symbol="LM48100QMH"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-15N">
<connects>
<connect gate="A" pin="ADR" pad="6"/>
<connect gate="A" pin="BIAS" pad="13"/>
<connect gate="A" pin="EPAD" pad="15"/>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="I2CVDD" pad="4"/>
<connect gate="A" pin="IN1" pad="12"/>
<connect gate="A" pin="IN2" pad="11"/>
<connect gate="A" pin="OUTA" pad="7"/>
<connect gate="A" pin="OUTB" pad="9"/>
<connect gate="A" pin="PGND" pad="8"/>
<connect gate="A" pin="PVDD" pad="10"/>
<connect gate="A" pin="SCL" pad="2"/>
<connect gate="A" pin="SDA" pad="3"/>
<connect gate="A" pin="VDD" pad="14"/>
<connect gate="A" pin="~FAULT" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM48100QMH"/>
<attribute name="OC_FARNELL" value="1697056"/>
<attribute name="OC_NEWARK" value="34P4860"/>
<attribute name="PACKAGE" value="TSSOP-14"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM4811LD" prefix="U">
<description>Headphone Amplifier</description>
<gates>
<gate name="A" symbol="LM4811LD"/>
</gates>
<devices>
<device name="" package="DFN300X300X80-11N">
<connects>
<connect gate="A" pin="BYPASS" pad="3"/>
<connect gate="A" pin="CLK" pad="4"/>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="GND_2" pad="11"/>
<connect gate="A" pin="SHDN" pad="7"/>
<connect gate="A" pin="UP/DN" pad="6"/>
<connect gate="A" pin="VDD" pad="10"/>
<connect gate="A" pin="VIN1" pad="2"/>
<connect gate="A" pin="VIN2" pad="8"/>
<connect gate="A" pin="VOUT1" pad="1"/>
<connect gate="A" pin="VOUT2" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM4811LD"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="74C4536"/>
<attribute name="PACKAGE" value="DFN-10"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM4811MM" prefix="U">
<description>Dual 105mW Headphone Amplifier</description>
<gates>
<gate name="A" symbol="LM4811MM"/>
</gates>
<devices>
<device name="" package="SOP50P490X110-8N">
<connects>
<connect gate="A" pin="BYPASS" pad="3"/>
<connect gate="A" pin="CLK" pad="4"/>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="SHDN" pad="7"/>
<connect gate="A" pin="UP/DN" pad="6"/>
<connect gate="A" pin="VDD" pad="10"/>
<connect gate="A" pin="VIN1" pad="2"/>
<connect gate="A" pin="VIN2" pad="8"/>
<connect gate="A" pin="VOUT1" pad="1"/>
<connect gate="A" pin="VOUT2" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM4811MM"/>
<attribute name="OC_FARNELL" value="9779221"/>
<attribute name="OC_NEWARK" value="41K5617"/>
<attribute name="PACKAGE" value="10-MSOP"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM4838MT" prefix="U">
<description>Stereo 2W Audio Power Amplifiers</description>
<gates>
<gate name="A" symbol="LM4838MT"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-28N">
<connects>
<connect gate="A" pin="BEEP_IN" pad="11"/>
<connect gate="A" pin="BYPASS" pad="22"/>
<connect gate="A" pin="DC_VOL" pad="7"/>
<connect gate="A" pin="GAIN_SELECT" pad="3"/>
<connect gate="A" pin="GND" pad="23"/>
<connect gate="A" pin="GND_2" pad="1"/>
<connect gate="A" pin="GND_3" pad="14"/>
<connect gate="A" pin="GND_4" pad="8"/>
<connect gate="A" pin="GND_5" pad="20"/>
<connect gate="A" pin="HP_SENSE" pad="21"/>
<connect gate="A" pin="LEFT_DOCK_" pad="13"/>
<connect gate="A" pin="LEFT_GAIN_1" pad="19"/>
<connect gate="A" pin="LEFT_GAIN_2" pad="18"/>
<connect gate="A" pin="LEFT_IN" pad="12"/>
<connect gate="A" pin="LEFT_OUT_+" pad="15"/>
<connect gate="A" pin="LEFT_OUT_-" pad="17"/>
<connect gate="A" pin="MODE" pad="4"/>
<connect gate="A" pin="MUTE" pad="5"/>
<connect gate="A" pin="RIGHT_DOCK" pad="9"/>
<connect gate="A" pin="RIGHT_GAIN_1" pad="24"/>
<connect gate="A" pin="RIGHT_GAIN_2" pad="25"/>
<connect gate="A" pin="RIGHT_IN" pad="10"/>
<connect gate="A" pin="RIGHT_OUT_+" pad="28"/>
<connect gate="A" pin="RIGHT_OUT_-" pad="26"/>
<connect gate="A" pin="SHDN" pad="2"/>
<connect gate="A" pin="VDD" pad="27"/>
<connect gate="A" pin="VDD_2" pad="6"/>
<connect gate="A" pin="VDD_3" pad="16"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM4838MT"/>
<attribute name="OC_FARNELL" value="1286898"/>
<attribute name="OC_NEWARK" value="-"/>
<attribute name="PACKAGE" value="TSSOP-28"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM48413TL">
<description>Stereo Class D Audio Power Amp</description>
<gates>
<gate name="A" symbol="LM48413TL"/>
</gates>
<devices>
<device name="" package="BGA14C25PX43P7X5_225X204X67">
<connects>
<connect gate="A" pin="3DEN" pad="A3"/>
<connect gate="A" pin="3DL+" pad="C1"/>
<connect gate="A" pin="3DL-" pad="B4"/>
<connect gate="A" pin="3DR+" pad="C3"/>
<connect gate="A" pin="3DR-" pad="D4"/>
<connect gate="A" pin="GND" pad="B6"/>
<connect gate="A" pin="INL+" pad="B2"/>
<connect gate="A" pin="INL-" pad="A1"/>
<connect gate="A" pin="INR+" pad="D2"/>
<connect gate="A" pin="INR-" pad="E1"/>
<connect gate="A" pin="OUTLA" pad="A5"/>
<connect gate="A" pin="OUTLB" pad="A7"/>
<connect gate="A" pin="OUTRA" pad="E5"/>
<connect gate="A" pin="OUTRB" pad="E7"/>
<connect gate="A" pin="PGND" pad="C7"/>
<connect gate="A" pin="PVDD" pad="D6"/>
<connect gate="A" pin="VDD" pad="C5"/>
<connect gate="A" pin="~SD" pad="E3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM48413TL"/>
<attribute name="OC_FARNELL" value="1697057"/>
<attribute name="OC_NEWARK" value="40P2716"/>
<attribute name="PACKAGE" value="BGA-14"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM4846TL" prefix="U">
<description>Output Capacitor-less Audio Subsystem</description>
<gates>
<gate name="A" symbol="LM4846TL"/>
</gates>
<devices>
<device name="" package="BGA25C5X5X50P_254X251X67">
<connects>
<connect gate="A" pin="CBYPASS" pad="E2"/>
<connect gate="A" pin="GND" pad="C5"/>
<connect gate="A" pin="GND_2" pad="C1"/>
<connect gate="A" pin="I2CSPI_SEL" pad="E1"/>
<connect gate="A" pin="I2CSPI_VDD" pad="A2"/>
<connect gate="A" pin="ID_ENB" pad="B3"/>
<connect gate="A" pin="LHP3D1" pad="D3"/>
<connect gate="A" pin="LHP3D2" pad="E3"/>
<connect gate="A" pin="LIN" pad="E4"/>
<connect gate="A" pin="LOUT" pad="E5"/>
<connect gate="A" pin="MONO+" pad="D1"/>
<connect gate="A" pin="MONO-" pad="B1"/>
<connect gate="A" pin="NC" pad="D2"/>
<connect gate="A" pin="NC_2" pad="B5"/>
<connect gate="A" pin="PHONE_IN" pad="B4"/>
<connect gate="A" pin="RHP3D1" pad="A4"/>
<connect gate="A" pin="RHP3D2" pad="A3"/>
<connect gate="A" pin="RIN" pad="D4"/>
<connect gate="A" pin="ROUT" pad="D5"/>
<connect gate="A" pin="SCL" pad="B2"/>
<connect gate="A" pin="SDA" pad="A1"/>
<connect gate="A" pin="VDD" pad="C4"/>
<connect gate="A" pin="VDD_2" pad="C2"/>
<connect gate="A" pin="VDD_3" pad="C3"/>
<connect gate="A" pin="VOC" pad="A5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM4846TL"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="69K2556"/>
<attribute name="PACKAGE" value="BGA-25"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM48556TL">
<description>CHG PUMP CERAMIC SPEAKER DRIVE</description>
<gates>
<gate name="A" symbol="LM48556TL"/>
</gates>
<devices>
<device name="" package="BGA12C50P3X4_199X148X60">
<connects>
<connect gate="A" pin="C1N" pad="D1"/>
<connect gate="A" pin="C1P" pad="C2"/>
<connect gate="A" pin="CPVSS" pad="C1"/>
<connect gate="A" pin="IN+" pad="A3"/>
<connect gate="A" pin="IN-" pad="B3"/>
<connect gate="A" pin="OUT+" pad="B2"/>
<connect gate="A" pin="OUT-" pad="A1"/>
<connect gate="A" pin="PGND" pad="D2"/>
<connect gate="A" pin="PVDD" pad="D3"/>
<connect gate="A" pin="SVDD" pad="A2"/>
<connect gate="A" pin="SVSS" pad="B1"/>
<connect gate="A" pin="~SD" pad="C3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM48556TL"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="07P5456"/>
<attribute name="PACKAGE" value="BGA-12"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM48557TL" prefix="U">
<description>Speaker Driver</description>
<gates>
<gate name="A" symbol="LM48557TL"/>
</gates>
<devices>
<device name="" package="BGA16C50P4X4_196X196X67">
<connects>
<connect gate="A" pin="C1N" pad="D1"/>
<connect gate="A" pin="C1P" pad="D3"/>
<connect gate="A" pin="CPVSS" pad="C1"/>
<connect gate="A" pin="I2CVDD" pad="C4"/>
<connect gate="A" pin="IN+" pad="B4"/>
<connect gate="A" pin="IN-" pad="A4"/>
<connect gate="A" pin="OUT+" pad="B2"/>
<connect gate="A" pin="OUT-" pad="B1"/>
<connect gate="A" pin="PGND" pad="D2"/>
<connect gate="A" pin="PVDD" pad="D4"/>
<connect gate="A" pin="SCL" pad="C2"/>
<connect gate="A" pin="SDA" pad="C3"/>
<connect gate="A" pin="SGND" pad="A2"/>
<connect gate="A" pin="VCM" pad="A3"/>
<connect gate="A" pin="VDD" pad="A1"/>
<connect gate="A" pin="~RESET" pad="B3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM48557TL"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="55R4066"/>
<attribute name="PACKAGE" value="BGA-16"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM4855ITL" prefix="U">
<description>IC AMP AUDIO PWR 1.5W</description>
<gates>
<gate name="A" symbol="LM4855ITL"/>
</gates>
<devices>
<device name="" package="BGA18C25P43P7X5_199X222X95">
<connects>
<connect gate="A" pin="BYPASS" pad="A1"/>
<connect gate="A" pin="CLOCK" pad="E1"/>
<connect gate="A" pin="DATA" pad="E5"/>
<connect gate="A" pin="ENB" pad="E3"/>
<connect gate="A" pin="GND" pad="C7"/>
<connect gate="A" pin="GND_2" pad="C1"/>
<connect gate="A" pin="LIN" pad="B4"/>
<connect gate="A" pin="LOUT+" pad="D6"/>
<connect gate="A" pin="LOUT-" pad="E7"/>
<connect gate="A" pin="PHONE_IN_IHF" pad="D4"/>
<connect gate="A" pin="PHONE_IN_IHS" pad="A3"/>
<connect gate="A" pin="RIN" pad="A5"/>
<connect gate="A" pin="ROUT+" pad="B6"/>
<connect gate="A" pin="ROUT-" pad="A7"/>
<connect gate="A" pin="SPKR_OUT+" pad="D2"/>
<connect gate="A" pin="SPKR_OUT-" pad="B2"/>
<connect gate="A" pin="VDD" pad="C5"/>
<connect gate="A" pin="VDD_2" pad="C3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM4855ITL"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K5712"/>
<attribute name="PACKAGE" value="18-WFBGA"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM4865M" prefix="U">
<description>Power Amplifier</description>
<gates>
<gate name="A" symbol="LM4865M"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="-VIN" pad="2"/>
<connect gate="A" pin="BYPASS" pad="7"/>
<connect gate="A" pin="DC_VOL/~SD" pad="4"/>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="HPSENSE" pad="3"/>
<connect gate="A" pin="VDD" pad="1"/>
<connect gate="A" pin="VO1" pad="5"/>
<connect gate="A" pin="VO2" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM4865M"/>
<attribute name="OC_FARNELL" value="9486356"/>
<attribute name="OC_NEWARK" value="97K3538"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM4871M" prefix="U">
<description>Power Amplifier</description>
<gates>
<gate name="A" symbol="LM4871M"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="4"/>
<connect gate="A" pin="BYPASS" pad="2"/>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="SHUTDOWN" pad="1"/>
<connect gate="A" pin="V01" pad="5"/>
<connect gate="A" pin="V02" pad="8"/>
<connect gate="A" pin="VDD" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM4871M"/>
<attribute name="OC_FARNELL" value="1468873"/>
<attribute name="OC_NEWARK" value="41K5780"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM4875M" prefix="U">
<description>Power Amplifier</description>
<gates>
<gate name="A" symbol="LM4875M"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="-VIN" pad="2"/>
<connect gate="A" pin="BYPASS" pad="7"/>
<connect gate="A" pin="DC_VOL/~SD" pad="4"/>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="HPSENSE" pad="3"/>
<connect gate="A" pin="VDD" pad="1"/>
<connect gate="A" pin="VO1" pad="5"/>
<connect gate="A" pin="VO2" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM4875M"/>
<attribute name="OC_FARNELL" value="1008023"/>
<attribute name="OC_NEWARK" value="92K6206"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM4875MM" prefix="U">
<description>750 mW Audio Power Amplifier</description>
<gates>
<gate name="A" symbol="LM4875MM"/>
</gates>
<devices>
<device name="" package="SOP65P490X110-8N">
<connects>
<connect gate="A" pin="-VIN" pad="2"/>
<connect gate="A" pin="BYPASS" pad="7"/>
<connect gate="A" pin="DC_VOL/~SD" pad="4"/>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="HPSENSE" pad="3"/>
<connect gate="A" pin="VDD" pad="1"/>
<connect gate="A" pin="VO1" pad="5"/>
<connect gate="A" pin="VO2" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM4875MM"/>
<attribute name="OC_FARNELL" value="1798328"/>
<attribute name="OC_NEWARK" value="75R2099"/>
<attribute name="PACKAGE" value="MSOP-8"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM4876M" prefix="U">
<description>Power Amplifier</description>
<gates>
<gate name="A" symbol="LM4876M"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="4"/>
<connect gate="A" pin="BYPASS" pad="2"/>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="V01" pad="5"/>
<connect gate="A" pin="V02" pad="8"/>
<connect gate="A" pin="VDD" pad="6"/>
<connect gate="A" pin="~SHUTDOWN" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM4876M"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K5802"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM4881MM" prefix="U">
<description>Headphone Amplifier</description>
<gates>
<gate name="A" symbol="LM4881MM"/>
</gates>
<devices>
<device name="" package="SOP65P490X109-8N">
<connects>
<connect gate="A" pin="BYPASS" pad="1"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="OUT_A" pad="7"/>
<connect gate="A" pin="OUT_A_2" pad="5"/>
<connect gate="A" pin="SHUTDOWN" pad="3"/>
<connect gate="A" pin="VDD" pad="6"/>
<connect gate="A" pin="VIN_A" pad="8"/>
<connect gate="A" pin="VIN_B" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM4881MM"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K5819"/>
<attribute name="PACKAGE" value="SOP-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM48821TL" prefix="U">
<description>Headphone Amplifier</description>
<gates>
<gate name="A" symbol="LM48821TL"/>
</gates>
<devices>
<device name="" package="BGA16C50P4X4_197X197X67">
<connects>
<connect gate="A" pin="CCP+" pad="D3"/>
<connect gate="A" pin="CCP-" pad="D1"/>
<connect gate="A" pin="I2CVDD" pad="C4"/>
<connect gate="A" pin="IN_A+" pad="A3"/>
<connect gate="A" pin="IN_A-" pad="A4"/>
<connect gate="A" pin="IN_B+" pad="B3"/>
<connect gate="A" pin="IN_B-" pad="B4"/>
<connect gate="A" pin="PGND" pad="D2"/>
<connect gate="A" pin="PVDD" pad="D4"/>
<connect gate="A" pin="SCL" pad="C2"/>
<connect gate="A" pin="SDA" pad="C3"/>
<connect gate="A" pin="SGND" pad="A2"/>
<connect gate="A" pin="SVDD" pad="A1"/>
<connect gate="A" pin="VOA" pad="B1"/>
<connect gate="A" pin="VOB" pad="B2"/>
<connect gate="A" pin="VSS" pad="C1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM48821TL"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="54M4694"/>
<attribute name="PACKAGE" value="BGA-16"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM48823TL" prefix="U">
<description>Speaker Driver</description>
<gates>
<gate name="A" symbol="LM48823TL"/>
</gates>
<devices>
<device name="" package="BGA16C50P4X4_197X197X67">
<connects>
<connect gate="A" pin="BYPASS" pad="A3"/>
<connect gate="A" pin="C1N" pad="D1"/>
<connect gate="A" pin="C1P" pad="D3"/>
<connect gate="A" pin="I2CVDD" pad="C4"/>
<connect gate="A" pin="INA" pad="A4"/>
<connect gate="A" pin="INB" pad="B4"/>
<connect gate="A" pin="OUTA" pad="B1"/>
<connect gate="A" pin="OUTB" pad="B2"/>
<connect gate="A" pin="PGND" pad="D2"/>
<connect gate="A" pin="PVDD" pad="D4"/>
<connect gate="A" pin="SCL" pad="C2"/>
<connect gate="A" pin="SDA" pad="C3"/>
<connect gate="A" pin="SGND" pad="A2"/>
<connect gate="A" pin="SVDD" pad="A1"/>
<connect gate="A" pin="VSS" pad="C1"/>
<connect gate="A" pin="~RESET" pad="B3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM48823TL"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="07P5459"/>
<attribute name="PACKAGE" value="BGA-16"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM48824TM">
<description>Amplifier</description>
<gates>
<gate name="A" symbol="LM48824TM"/>
</gates>
<devices>
<device name="" package="BGA16C40P4X4_169X169X60">
<connects>
<connect gate="A" pin="C1N" pad="C1"/>
<connect gate="A" pin="C1P" pad="B2"/>
<connect gate="A" pin="COM" pad="C3"/>
<connect gate="A" pin="GND" pad="B1"/>
<connect gate="A" pin="HPVDD" pad="B3"/>
<connect gate="A" pin="HPVSS" pad="C2"/>
<connect gate="A" pin="INL+" pad="B4"/>
<connect gate="A" pin="INL-" pad="A4"/>
<connect gate="A" pin="INR+" pad="C4"/>
<connect gate="A" pin="INR-" pad="D4"/>
<connect gate="A" pin="OUTL" pad="A3"/>
<connect gate="A" pin="OUTR" pad="D3"/>
<connect gate="A" pin="SCL" pad="D2"/>
<connect gate="A" pin="SDA" pad="D1"/>
<connect gate="A" pin="SW" pad="A1"/>
<connect gate="A" pin="VDD" pad="A2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM48824TM"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="55R4068"/>
<attribute name="PACKAGE" value="BGA-25"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM48860TL" prefix="U">
<description>Fixed Gain Stereo Headphone Amplifier</description>
<gates>
<gate name="A" symbol="LM48860TL"/>
</gates>
<devices>
<device name="" package="BGA12C3X4X50P_200X150X67">
<connects>
<connect gate="A" pin="CCP+" pad="D3"/>
<connect gate="A" pin="CCP-" pad="D1"/>
<connect gate="A" pin="LIN" pad="A3"/>
<connect gate="A" pin="LOUT" pad="B3"/>
<connect gate="A" pin="PGND" pad="D2"/>
<connect gate="A" pin="RIN" pad="A1"/>
<connect gate="A" pin="ROUT" pad="B1"/>
<connect gate="A" pin="SGND" pad="A2"/>
<connect gate="A" pin="VDD" pad="C3"/>
<connect gate="A" pin="VSS(CP)" pad="C1"/>
<connect gate="A" pin="~SD_LC" pad="B2"/>
<connect gate="A" pin="~SD_RC" pad="C2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM48860TL"/>
<attribute name="OC_FARNELL" value="1609168"/>
<attribute name="OC_NEWARK" value="11N9273"/>
<attribute name="PACKAGE" value="BGA-12"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM4889MA" prefix="U">
<description>1 Watt Audio Power Amplifier</description>
<gates>
<gate name="A" symbol="LM4889MA"/>
</gates>
<devices>
<device name="" package="SOIC127P620X175-8N">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="4"/>
<connect gate="A" pin="BYPASS" pad="2"/>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="VDD" pad="6"/>
<connect gate="A" pin="VO1" pad="5"/>
<connect gate="A" pin="VO2" pad="8"/>
<connect gate="A" pin="~SHDN" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM4889MA"/>
<attribute name="OC_FARNELL" value="1286916"/>
<attribute name="OC_NEWARK" value="26M0411"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="National"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM4889MM" prefix="U">
<description>Audio Power Amplifier</description>
<gates>
<gate name="A" symbol="LM4889MM"/>
</gates>
<devices>
<device name="" package="SOP65P490X110-8N">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="4"/>
<connect gate="A" pin="BYPASS" pad="2"/>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="VDD" pad="6"/>
<connect gate="A" pin="VO1" pad="5"/>
<connect gate="A" pin="VO2" pad="8"/>
<connect gate="A" pin="~SHDN" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM4889MM"/>
<attribute name="OC_FARNELL" value="1312775"/>
<attribute name="OC_NEWARK" value="41K5839"/>
<attribute name="PACKAGE" value="MSOP-8"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM49100GR" prefix="U">
<description>Headphone Amplifier</description>
<gates>
<gate name="A" symbol="LM49100GR"/>
</gates>
<devices>
<device name="" package="BGA25C50P5X5_300X300X110">
<connects>
<connect gate="A" pin="ADDR" pad="C4"/>
<connect gate="A" pin="AGND" pad="E3"/>
<connect gate="A" pin="BYPASS" pad="A4"/>
<connect gate="A" pin="C1N" pad="B1"/>
<connect gate="A" pin="C1P" pad="B2"/>
<connect gate="A" pin="GND" pad="E4"/>
<connect gate="A" pin="GNDCP" pad="A2"/>
<connect gate="A" pin="GND_2" pad="C3"/>
<connect gate="A" pin="HPL" pad="D1"/>
<connect gate="A" pin="HPR" pad="E1"/>
<connect gate="A" pin="LIN" pad="B4"/>
<connect gate="A" pin="LS+" pad="D5"/>
<connect gate="A" pin="LS-" pad="B5"/>
<connect gate="A" pin="MIN+" pad="A3"/>
<connect gate="A" pin="MIN-" pad="B3"/>
<connect gate="A" pin="RIN" pad="A5"/>
<connect gate="A" pin="SCL" pad="E5"/>
<connect gate="A" pin="SDA" pad="D4"/>
<connect gate="A" pin="VDD12C" pad="D3"/>
<connect gate="A" pin="VDDCP" pad="A1"/>
<connect gate="A" pin="VDDHP" pad="D2"/>
<connect gate="A" pin="VDDLS" pad="E2"/>
<connect gate="A" pin="VDDLS_2" pad="C5"/>
<connect gate="A" pin="VSSCP" pad="C1"/>
<connect gate="A" pin="VSSHP" pad="C2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM49100GR"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="54M4697"/>
<attribute name="PACKAGE" value="BGA-25"/>
<attribute name="SUPPLIER" value="National semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM49101TM">
<description>Amplifier</description>
<gates>
<gate name="A" symbol="LM49101TM"/>
</gates>
<devices>
<device name="" package="BGA25C40P5X5_200X200X67">
<connects>
<connect gate="A" pin="BIAS" pad="E5"/>
<connect gate="A" pin="BYPASS_IN+" pad="D5"/>
<connect gate="A" pin="BYPASS_IN-" pad="D1"/>
<connect gate="A" pin="C1N" pad="B1"/>
<connect gate="A" pin="C1P" pad="B2"/>
<connect gate="A" pin="CPGND" pad="A1"/>
<connect gate="A" pin="GND" pad="C3"/>
<connect gate="A" pin="GND_2" pad="E3"/>
<connect gate="A" pin="HPGND" pad="B4"/>
<connect gate="A" pin="HPL" pad="B3"/>
<connect gate="A" pin="HPR" pad="A3"/>
<connect gate="A" pin="HW_RESET" pad="D4"/>
<connect gate="A" pin="I2CVDD" pad="D2"/>
<connect gate="A" pin="LIN" pad="C5"/>
<connect gate="A" pin="MIN+" pad="A5"/>
<connect gate="A" pin="MIN-" pad="B5"/>
<connect gate="A" pin="MONO+" pad="E1"/>
<connect gate="A" pin="MONO-" pad="E4"/>
<connect gate="A" pin="RIN" pad="C4"/>
<connect gate="A" pin="SCL" pad="D3"/>
<connect gate="A" pin="SDA" pad="C2"/>
<connect gate="A" pin="VDDCP" pad="C1"/>
<connect gate="A" pin="VDDHP" pad="A4"/>
<connect gate="A" pin="VDDLS" pad="E2"/>
<connect gate="A" pin="VSSCP" pad="A2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM49101TM"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="55R4070"/>
<attribute name="PACKAGE" value="BGA-25"/>
<attribute name="SUPPLIER" value="National semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM4910MM" prefix="U">
<description>Headphone Amplifier</description>
<gates>
<gate name="A" symbol="LM4910MM"/>
</gates>
<devices>
<device name="" package="SOP65P490X109-8N">
<connects>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="IN_1" pad="1"/>
<connect gate="A" pin="IN_2" pad="2"/>
<connect gate="A" pin="VDD" pad="5"/>
<connect gate="A" pin="VO1" pad="8"/>
<connect gate="A" pin="VO2" pad="7"/>
<connect gate="A" pin="VO3" pad="6"/>
<connect gate="A" pin="~SD" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM4910MM"/>
<attribute name="OC_FARNELL" value=""/>
<attribute name="OC_NEWARK" value="41K5937"/>
<attribute name="PACKAGE" value="SOP-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM49120TL" prefix="U">
<description>Amplifier</description>
<gates>
<gate name="A" symbol="LM49120TL"/>
</gates>
<devices>
<device name="" package="BGA16C50P4X4_200X200X60">
<connects>
<connect gate="A" pin="BYPASS" pad="B2"/>
<connect gate="A" pin="GND" pad="D2"/>
<connect gate="A" pin="I2CVDD" pad="C2"/>
<connect gate="A" pin="LIN" pad="B3"/>
<connect gate="A" pin="LOUT" pad="A4"/>
<connect gate="A" pin="MONO+" pad="D4"/>
<connect gate="A" pin="MONO-" pad="D1"/>
<connect gate="A" pin="MONO_IN+" pad="B1"/>
<connect gate="A" pin="MONO_IN-" pad="C1"/>
<connect gate="A" pin="RIN" pad="B4"/>
<connect gate="A" pin="ROUT" pad="A3"/>
<connect gate="A" pin="SCL" pad="C3"/>
<connect gate="A" pin="SDA" pad="C4"/>
<connect gate="A" pin="VDD" pad="A2"/>
<connect gate="A" pin="VDD_2" pad="D3"/>
<connect gate="A" pin="VOC" pad="A1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM49120TL"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="34P4865"/>
<attribute name="PACKAGE" value="BGA-16"/>
<attribute name="SUPPLIER" value="National semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM49151TL">
<description>Amplifiers</description>
<gates>
<gate name="A" symbol="LM49151TL"/>
</gates>
<devices>
<device name="" package="BGA20C50P4X5_251X199X675">
<connects>
<connect gate="A" pin="BYPASS" pad="C3"/>
<connect gate="A" pin="CPGND" pad="E4"/>
<connect gate="A" pin="CPN" pad="D3"/>
<connect gate="A" pin="CPP" pad="D4"/>
<connect gate="A" pin="CPVSS" pad="C4"/>
<connect gate="A" pin="GND" pad="A2"/>
<connect gate="A" pin="HPL" pad="E3"/>
<connect gate="A" pin="HPR" pad="E2"/>
<connect gate="A" pin="I2CVDD" pad="A1"/>
<connect gate="A" pin="INL" pad="C1"/>
<connect gate="A" pin="INM+" pad="E1"/>
<connect gate="A" pin="INM-" pad="D1"/>
<connect gate="A" pin="INR" pad="C2"/>
<connect gate="A" pin="LSOUT+" pad="A4"/>
<connect gate="A" pin="LSOUT-" pad="A3"/>
<connect gate="A" pin="LSVDD" pad="B4"/>
<connect gate="A" pin="SCL" pad="B3"/>
<connect gate="A" pin="SDA" pad="B2"/>
<connect gate="A" pin="SET" pad="D2"/>
<connect gate="A" pin="VDD" pad="B1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM49151TL"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="55R4072"/>
<attribute name="PACKAGE" value="BGA-20"/>
<attribute name="SUPPLIER" value="National semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM4916MM" prefix="U">
<description>Stereo Headphone Audio Amplifier</description>
<gates>
<gate name="A" symbol="LM4916MM"/>
</gates>
<devices>
<device name="" package="SOP50P490X109-10N">
<connects>
<connect gate="A" pin="BYPASS" pad="4"/>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="IN_A" pad="1"/>
<connect gate="A" pin="IN_B" pad="5"/>
<connect gate="A" pin="MUTE" pad="3"/>
<connect gate="A" pin="SD" pad="2"/>
<connect gate="A" pin="VDD" pad="10"/>
<connect gate="A" pin="VOA" pad="9"/>
<connect gate="A" pin="VOB" pad="7"/>
<connect gate="A" pin="~SE/BTL" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM4916MM"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K5953"/>
<attribute name="PACKAGE" value="SOP-10"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM49200TL">
<description>Amplifier</description>
<gates>
<gate name="A" symbol="LM49200TL"/>
</gates>
<devices>
<device name="" package="BGA20C50P4X5_251X202X67">
<connects>
<connect gate="A" pin="BIAS" pad="C3"/>
<connect gate="A" pin="C1N" pad="D3"/>
<connect gate="A" pin="C1P" pad="D4"/>
<connect gate="A" pin="CPGND" pad="E4"/>
<connect gate="A" pin="GND" pad="C1"/>
<connect gate="A" pin="HPL" pad="E3"/>
<connect gate="A" pin="HPR" pad="E2"/>
<connect gate="A" pin="I2CVDD" pad="B2"/>
<connect gate="A" pin="LIN" pad="B3"/>
<connect gate="A" pin="LOUT+" pad="D1"/>
<connect gate="A" pin="LOUT-" pad="E1"/>
<connect gate="A" pin="MIN+" pad="A3"/>
<connect gate="A" pin="MIN-" pad="A4"/>
<connect gate="A" pin="RIN" pad="B4"/>
<connect gate="A" pin="ROUT+" pad="B1"/>
<connect gate="A" pin="ROUT-" pad="A1"/>
<connect gate="A" pin="SCL" pad="C2"/>
<connect gate="A" pin="SDA" pad="D2"/>
<connect gate="A" pin="VDD" pad="A2"/>
<connect gate="A" pin="VSSCP" pad="C4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM49200TL"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="55R4074"/>
<attribute name="PACKAGE" value="BGA-20"/>
<attribute name="SUPPLIER" value="National semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM4920TL" prefix="U">
<description>Amplifier</description>
<gates>
<gate name="A" symbol="LM4920TL"/>
</gates>
<devices>
<device name="" package="BGA14C50P4X4_197X197X67">
<connects>
<connect gate="A" pin="+AVDD" pad="D1"/>
<connect gate="A" pin="-AVDD" pad="D3"/>
<connect gate="A" pin="CCP+" pad="A4"/>
<connect gate="A" pin="CCP-" pad="C4"/>
<connect gate="A" pin="CPVDD" pad="A3"/>
<connect gate="A" pin="L_IN" pad="C1"/>
<connect gate="A" pin="L_OUT" pad="D2"/>
<connect gate="A" pin="PGND" pad="B4"/>
<connect gate="A" pin="R_IN" pad="A1"/>
<connect gate="A" pin="R_OUT" pad="C2"/>
<connect gate="A" pin="SD_LC" pad="B2"/>
<connect gate="A" pin="SD_RC" pad="B1"/>
<connect gate="A" pin="SGND" pad="A2"/>
<connect gate="A" pin="VCP_OUT" pad="D4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM4920TL"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="99K2483"/>
<attribute name="PACKAGE" value="BGA-14"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM4921ITL" prefix="U">
<description>DAC</description>
<gates>
<gate name="A" symbol="LM4921ITL"/>
</gates>
<devices>
<device name="" package="BGA20C50P4X5_272X220X67">
<connects>
<connect gate="A" pin="AGND" pad="A3"/>
<connect gate="A" pin="AVDD" pad="B4"/>
<connect gate="A" pin="BYPASS" pad="C4"/>
<connect gate="A" pin="DVDD" pad="C1"/>
<connect gate="A" pin="GNDD" pad="A1"/>
<connect gate="A" pin="GNDX" pad="E1"/>
<connect gate="A" pin="HP-L" pad="B3"/>
<connect gate="A" pin="HP_R" pad="A4"/>
<connect gate="A" pin="I2S-CLK" pad="B1"/>
<connect gate="A" pin="I2S-LRCLK" pad="B2"/>
<connect gate="A" pin="I2S_DATA" pad="C2"/>
<connect gate="A" pin="MCLK/XTAL_IN" pad="E2"/>
<connect gate="A" pin="NC" pad="C3"/>
<connect gate="A" pin="NC_2" pad="D4"/>
<connect gate="A" pin="NC_OPEN" pad="A2"/>
<connect gate="A" pin="SPI_CLK" pad="E3"/>
<connect gate="A" pin="SPI_DATA" pad="E4"/>
<connect gate="A" pin="SPI_EN" pad="D3"/>
<connect gate="A" pin="VDDX" pad="D1"/>
<connect gate="A" pin="XTAL_OUT" pad="D2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM4921ITL"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K5963"/>
<attribute name="PACKAGE" value="BGA-20"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM4923LQ" prefix="U">
<description>1.1 Watt Fully Differential Audio Power Amplifier</description>
<gates>
<gate name="A" symbol="LM4923LQ"/>
</gates>
<devices>
<device name="" package="QFN65P200X200X80-9N">
<connects>
<connect gate="A" pin="BYPASS" pad="6"/>
<connect gate="A" pin="EPAD" pad="9"/>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="IN+" pad="2"/>
<connect gate="A" pin="IN-" pad="1"/>
<connect gate="A" pin="SD" pad="5"/>
<connect gate="A" pin="VDD" pad="3"/>
<connect gate="A" pin="VO+" pad="4"/>
<connect gate="A" pin="VO-" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM4923LQ"/>
<attribute name="OC_FARNELL" value="1798329"/>
<attribute name="OC_NEWARK" value="73R9746"/>
<attribute name="PACKAGE" value="QFN-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM49250RL" prefix="U">
<description>Amplifier</description>
<gates>
<gate name="A" symbol="LM49250RL"/>
</gates>
<devices>
<device name="" package="BGA36C50P6X6_305X305X65">
<connects>
<connect gate="A" pin="ADR" pad="B2"/>
<connect gate="A" pin="BYPASS" pad="F6"/>
<connect gate="A" pin="CCP+" pad="A5"/>
<connect gate="A" pin="CCP-" pad="B5"/>
<connect gate="A" pin="EP+" pad="F4"/>
<connect gate="A" pin="EP-" pad="E4"/>
<connect gate="A" pin="GND" pad="F2"/>
<connect gate="A" pin="GND(CP)" pad="A6"/>
<connect gate="A" pin="GND(HP)" pad="D3"/>
<connect gate="A" pin="GND(LS)" pad="C1"/>
<connect gate="A" pin="GND_2" pad="A2"/>
<connect gate="A" pin="HPL" pad="C6"/>
<connect gate="A" pin="HPR" pad="B6"/>
<connect gate="A" pin="I2CVDD" pad="C2"/>
<connect gate="A" pin="L3D1" pad="B4"/>
<connect gate="A" pin="L3D2" pad="B3"/>
<connect gate="A" pin="LIN+" pad="E6"/>
<connect gate="A" pin="LIN-" pad="D6"/>
<connect gate="A" pin="LLS+" pad="B1"/>
<connect gate="A" pin="LLS-" pad="A1"/>
<connect gate="A" pin="MIN+" pad="D5"/>
<connect gate="A" pin="MIN-" pad="D4"/>
<connect gate="A" pin="R3D1" pad="C4"/>
<connect gate="A" pin="R3D2" pad="C3"/>
<connect gate="A" pin="RIN+" pad="E5"/>
<connect gate="A" pin="RIN-" pad="F5"/>
<connect gate="A" pin="RLS+" pad="E1"/>
<connect gate="A" pin="RLS-" pad="F1"/>
<connect gate="A" pin="SCL" pad="D2"/>
<connect gate="A" pin="SDA" pad="E2"/>
<connect gate="A" pin="VDD" pad="F3"/>
<connect gate="A" pin="VDD(CP)" pad="A3"/>
<connect gate="A" pin="VDD(LS)" pad="D1"/>
<connect gate="A" pin="VO(LDO)" pad="C5"/>
<connect gate="A" pin="VSS(CP)" pad="A4"/>
<connect gate="A" pin="~RESET" pad="E3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM49250RL"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="84M8140"/>
<attribute name="PACKAGE" value="BGA-36"/>
<attribute name="SUPPLIER" value="National semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM49321RL" prefix="U">
<description>Amplifier</description>
<gates>
<gate name="A" symbol="LM49321RL"/>
</gates>
<devices>
<device name="" package="BGA36C50P6X6_351X325X72">
<connects>
<connect gate="A" pin="ADDR/ENB" pad="C4"/>
<connect gate="A" pin="AGND" pad="D2"/>
<connect gate="A" pin="AGND_2" pad="E6"/>
<connect gate="A" pin="AGND_3" pad="D1"/>
<connect gate="A" pin="AVDD" pad="F5"/>
<connect gate="A" pin="AVDD_2" pad="C6"/>
<connect gate="A" pin="BYPASS" pad="C5"/>
<connect gate="A" pin="CHP" pad="D6"/>
<connect gate="A" pin="DGND" pad="A1"/>
<connect gate="A" pin="DIFF+" pad="F1"/>
<connect gate="A" pin="DIFF-" pad="E1"/>
<connect gate="A" pin="DVDD" pad="A5"/>
<connect gate="A" pin="EP+" pad="F3"/>
<connect gate="A" pin="EP-" pad="F2"/>
<connect gate="A" pin="GPIO" pad="B4"/>
<connect gate="A" pin="I/O_VDD" pad="A6"/>
<connect gate="A" pin="I2C_VDD" pad="B5"/>
<connect gate="A" pin="I2S_CLK" pad="B3"/>
<connect gate="A" pin="I2S_SDATA" pad="B2"/>
<connect gate="A" pin="I2S_WS" pad="A3"/>
<connect gate="A" pin="LHP" pad="E5"/>
<connect gate="A" pin="LIN" pad="E2"/>
<connect gate="A" pin="LS+" pad="F6"/>
<connect gate="A" pin="LS-" pad="F4"/>
<connect gate="A" pin="MCLK" pad="A2"/>
<connect gate="A" pin="MODE" pad="D4"/>
<connect gate="A" pin="NC" pad="D3"/>
<connect gate="A" pin="NC_2" pad="E4"/>
<connect gate="A" pin="PLL_GND" pad="C1"/>
<connect gate="A" pin="PLL_IN" pad="C3"/>
<connect gate="A" pin="PLL_OUT" pad="C2"/>
<connect gate="A" pin="PLL_VDD" pad="B1"/>
<connect gate="A" pin="RHP" pad="D5"/>
<connect gate="A" pin="RIN" pad="E3"/>
<connect gate="A" pin="SCL/SCK" pad="B6"/>
<connect gate="A" pin="SDA/SDI" pad="A4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM49321RL"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="34P4869"/>
<attribute name="PACKAGE" value=""/>
<attribute name="SUPPLIER" value="National semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM49350RL" prefix="U">
<description>High Performance Audio Codec Sub-System</description>
<gates>
<gate name="A" symbol="LM49350RL"/>
</gates>
<devices>
<device name="" package="BGA36C6X650P_345X345X725">
<connects>
<connect gate="A" pin="AGND" pad="A3"/>
<connect gate="A" pin="AUX_L" pad="B3"/>
<connect gate="A" pin="AUX_OUT+" pad="C2"/>
<connect gate="A" pin="AUX_OUT-" pad="C3"/>
<connect gate="A" pin="AUX_R" pad="B2"/>
<connect gate="A" pin="A_VDD" pad="A2"/>
<connect gate="A" pin="CP+" pad="D2"/>
<connect gate="A" pin="CP-" pad="D1"/>
<connect gate="A" pin="DGND" pad="D6"/>
<connect gate="A" pin="D_VDD" pad="E6"/>
<connect gate="A" pin="GPIO" pad="A5"/>
<connect gate="A" pin="HPL" pad="B1"/>
<connect gate="A" pin="HPR" pad="A1"/>
<connect gate="A" pin="HP_VSS" pad="C1"/>
<connect gate="A" pin="I/O_VDD" pad="F6"/>
<connect gate="A" pin="LEFT_MIC+" pad="F4"/>
<connect gate="A" pin="LEFT_MIC-" pad="E4"/>
<connect gate="A" pin="LS+" pad="F1"/>
<connect gate="A" pin="LS-" pad="F2"/>
<connect gate="A" pin="LSGND" pad="E1"/>
<connect gate="A" pin="LS_VDD" pad="E2"/>
<connect gate="A" pin="MCLK" pad="C6"/>
<connect gate="A" pin="MIC_BIAS" pad="D3"/>
<connect gate="A" pin="PORT1_CLK" pad="F5"/>
<connect gate="A" pin="PORT1_SDI" pad="E5"/>
<connect gate="A" pin="PORT1_SDO" pad="D5"/>
<connect gate="A" pin="PORT1_SYNC" pad="D4"/>
<connect gate="A" pin="PORT2_CLK" pad="C5"/>
<connect gate="A" pin="PORT2_SDI" pad="B5"/>
<connect gate="A" pin="PORT2_SDO" pad="C4"/>
<connect gate="A" pin="PORT2_SYNC" pad="B4"/>
<connect gate="A" pin="RIGHT_MIC+" pad="F3"/>
<connect gate="A" pin="RIGHT_MIC-" pad="E3"/>
<connect gate="A" pin="SCL" pad="B6"/>
<connect gate="A" pin="SDA" pad="A6"/>
<connect gate="A" pin="VREF_FLT" pad="A4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM49350RL"/>
<attribute name="OC_FARNELL" value="1667423"/>
<attribute name="OC_NEWARK" value="07P5465"/>
<attribute name="PACKAGE" value="BGA-36"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM49352RL">
<description>Amplifier</description>
<gates>
<gate name="A" symbol="LM49352RL"/>
</gates>
<devices>
<device name="" package="BGA36C50P6X6_328X328X72">
<connects>
<connect gate="A" pin="ADC/REF" pad="A5"/>
<connect gate="A" pin="AGND" pad="A3"/>
<connect gate="A" pin="AUXL" pad="B3"/>
<connect gate="A" pin="AUXR" pad="B2"/>
<connect gate="A" pin="AVDD" pad="A2"/>
<connect gate="A" pin="CP+" pad="D2"/>
<connect gate="A" pin="CP-" pad="D1"/>
<connect gate="A" pin="DAC/REF" pad="A4"/>
<connect gate="A" pin="DGND" pad="D6"/>
<connect gate="A" pin="DVDD" pad="E6"/>
<connect gate="A" pin="EP+" pad="D3"/>
<connect gate="A" pin="EP-" pad="C3"/>
<connect gate="A" pin="HPL" pad="B1"/>
<connect gate="A" pin="HPR" pad="A1"/>
<connect gate="A" pin="HPVDD" pad="C2"/>
<connect gate="A" pin="HPVSS" pad="C1"/>
<connect gate="A" pin="IOVDD" pad="F6"/>
<connect gate="A" pin="LS+" pad="F1"/>
<connect gate="A" pin="LS-" pad="F2"/>
<connect gate="A" pin="LSGND" pad="E1"/>
<connect gate="A" pin="LSVDD" pad="E2"/>
<connect gate="A" pin="MCLK" pad="C6"/>
<connect gate="A" pin="MIC+" pad="F4"/>
<connect gate="A" pin="MIC-" pad="E4"/>
<connect gate="A" pin="MONO+" pad="F3"/>
<connect gate="A" pin="MONO-" pad="E3"/>
<connect gate="A" pin="PORT1/CLK" pad="F5"/>
<connect gate="A" pin="PORT1/SDI" pad="E5"/>
<connect gate="A" pin="PORT1/SDO" pad="D5"/>
<connect gate="A" pin="PORT1/SYNC" pad="D4"/>
<connect gate="A" pin="PORT2/CLK" pad="C5"/>
<connect gate="A" pin="PORT2/SDI" pad="B5"/>
<connect gate="A" pin="PORT2/SDO" pad="C4"/>
<connect gate="A" pin="PORT2/SYNC" pad="B4"/>
<connect gate="A" pin="SCL" pad="B6"/>
<connect gate="A" pin="SDA" pad="A6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM49352RL"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="55R4076"/>
<attribute name="PACKAGE" value="BGA-36"/>
<attribute name="SUPPLIER" value="National semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM4935RL" prefix="U">
<description>ADC</description>
<gates>
<gate name="A" symbol="LM4935RL"/>
</gates>
<devices>
<device name="" package="BGA49C50P7X7_392X392X65">
<connects>
<connect gate="A" pin="AUX_L" pad="D3"/>
<connect gate="A" pin="AUX_OUT_NEG" pad="F5"/>
<connect gate="A" pin="AUX_OUT_POS" pad="G5"/>
<connect gate="A" pin="AUX_R" pad="C4"/>
<connect gate="A" pin="A_VDD" pad="A2"/>
<connect gate="A" pin="A_VSS" pad="B1"/>
<connect gate="A" pin="BB_VDD" pad="D6"/>
<connect gate="A" pin="BYPASS" pad="B4"/>
<connect gate="A" pin="CPI_NEG" pad="E4"/>
<connect gate="A" pin="CPI_POS" pad="F3"/>
<connect gate="A" pin="CPO_NEG" pad="F4"/>
<connect gate="A" pin="CPO_POS" pad="G4"/>
<connect gate="A" pin="D_VDD" pad="D7"/>
<connect gate="A" pin="D_VSS" pad="G6"/>
<connect gate="A" pin="EP_NEG" pad="A1"/>
<connect gate="A" pin="EP_POS" pad="B2"/>
<connect gate="A" pin="EXT_BIAS" pad="C2"/>
<connect gate="A" pin="EXT_MIC" pad="A4"/>
<connect gate="A" pin="GPIO_1" pad="D5"/>
<connect gate="A" pin="GPIO_2" pad="C5"/>
<connect gate="A" pin="HP_L" pad="D1"/>
<connect gate="A" pin="HP_R" pad="C1"/>
<connect gate="A" pin="HP_VMID" pad="E1"/>
<connect gate="A" pin="HP_VMID_FB" pad="E2"/>
<connect gate="A" pin="I2S_CLK" pad="F7"/>
<connect gate="A" pin="I2S_SDI" pad="E7"/>
<connect gate="A" pin="I2S_SDO" pad="E6"/>
<connect gate="A" pin="I2S_WS" pad="F6"/>
<connect gate="A" pin="INT_BIAS" pad="C3"/>
<connect gate="A" pin="INT_MIC_NEG" pad="B3"/>
<connect gate="A" pin="INT_MIC_POS" pad="A3"/>
<connect gate="A" pin="IRQ" pad="E5"/>
<connect gate="A" pin="LS_NEG" pad="G3"/>
<connect gate="A" pin="LS_POS" pad="G1"/>
<connect gate="A" pin="LS_VDD" pad="F2"/>
<connect gate="A" pin="LS_VDD_2" pad="F1"/>
<connect gate="A" pin="LS_VSS" pad="G2"/>
<connect gate="A" pin="MCLK" pad="G7"/>
<connect gate="A" pin="MIC_DET" pad="E3"/>
<connect gate="A" pin="PLL_FILT" pad="B6"/>
<connect gate="A" pin="PLL_VDD" pad="B7"/>
<connect gate="A" pin="PLL_VSS" pad="A7"/>
<connect gate="A" pin="SCL" pad="C7"/>
<connect gate="A" pin="SDA" pad="C6"/>
<connect gate="A" pin="SPI_MODE" pad="D4"/>
<connect gate="A" pin="TEST_MODE/~CS" pad="B5"/>
<connect gate="A" pin="VREF_FLT" pad="D2"/>
<connect gate="A" pin="VSAR1" pad="A6"/>
<connect gate="A" pin="VSAR2" pad="A5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM4935RL"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="99K2488"/>
<attribute name="PACKAGE" value="BGA-49"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM4936MH" prefix="U">
<description>Audio Power Amplifiers</description>
<gates>
<gate name="A" symbol="LM4936MH"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-29N">
<connects>
<connect gate="A" pin="BEEP_IN" pad="11"/>
<connect gate="A" pin="BYPASS" pad="22"/>
<connect gate="A" pin="EP" pad="29"/>
<connect gate="A" pin="GND" pad="20"/>
<connect gate="A" pin="GND_2" pad="1"/>
<connect gate="A" pin="GND_3" pad="8"/>
<connect gate="A" pin="GND_4" pad="14"/>
<connect gate="A" pin="GND_5" pad="23"/>
<connect gate="A" pin="HP_SENSES" pad="21"/>
<connect gate="A" pin="I2C/SPI_SELECT" pad="2"/>
<connect gate="A" pin="I2C/SPI_VDD" pad="6"/>
<connect gate="A" pin="ID/CE" pad="3"/>
<connect gate="A" pin="LEFT_DOCK" pad="13"/>
<connect gate="A" pin="LEFT_GAIN1" pad="19"/>
<connect gate="A" pin="LEFT_GAIN2" pad="18"/>
<connect gate="A" pin="LEFT_IN" pad="12"/>
<connect gate="A" pin="LEFT_OUT+" pad="15"/>
<connect gate="A" pin="LEFT_OUT-" pad="17"/>
<connect gate="A" pin="RIGHT_DOCK" pad="9"/>
<connect gate="A" pin="RIGHT_GAIN1" pad="24"/>
<connect gate="A" pin="RIGHT_GAIN2" pad="25"/>
<connect gate="A" pin="RIGHT_IN" pad="10"/>
<connect gate="A" pin="RIGHT_OUT+" pad="28"/>
<connect gate="A" pin="RIGHT_OUT-" pad="26"/>
<connect gate="A" pin="SCL/CLK" pad="4"/>
<connect gate="A" pin="SPA/DATA" pad="5"/>
<connect gate="A" pin="VDD" pad="27"/>
<connect gate="A" pin="VDD_2" pad="16"/>
<connect gate="A" pin="VDD_3" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM4936MH"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="37K0393"/>
<attribute name="PACKAGE" value="SSOP-28"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM4937RL" prefix="U">
<description>Audio Amplifier</description>
<gates>
<gate name="A" symbol="LM4937RL"/>
</gates>
<devices>
<device name="" package="BGA36C50P6X6_351X325X67">
<connects>
<connect gate="A" pin="ADDR/ENB" pad="C4"/>
<connect gate="A" pin="AGND" pad="E6"/>
<connect gate="A" pin="AGND_2" pad="D1"/>
<connect gate="A" pin="AGND_3" pad="D2"/>
<connect gate="A" pin="AVDD" pad="F5"/>
<connect gate="A" pin="AVDD_2" pad="C6"/>
<connect gate="A" pin="BYPASS" pad="C5"/>
<connect gate="A" pin="CHP" pad="D6"/>
<connect gate="A" pin="DGND" pad="A1"/>
<connect gate="A" pin="DIFF+" pad="F1"/>
<connect gate="A" pin="DIFF-" pad="E1"/>
<connect gate="A" pin="DVDD" pad="A5"/>
<connect gate="A" pin="EP+" pad="F3"/>
<connect gate="A" pin="EP-" pad="F2"/>
<connect gate="A" pin="GPIO" pad="B4"/>
<connect gate="A" pin="I2C_VDD" pad="B5"/>
<connect gate="A" pin="I2S_CLK" pad="B3"/>
<connect gate="A" pin="I2S_SDATA" pad="B2"/>
<connect gate="A" pin="I2S_WS" pad="A3"/>
<connect gate="A" pin="LHP" pad="E5"/>
<connect gate="A" pin="LIN" pad="E2"/>
<connect gate="A" pin="LS+" pad="F6"/>
<connect gate="A" pin="LS-" pad="F4"/>
<connect gate="A" pin="MCLK" pad="A2"/>
<connect gate="A" pin="MODE" pad="D4"/>
<connect gate="A" pin="NC" pad="E4"/>
<connect gate="A" pin="NC_2" pad="D3"/>
<connect gate="A" pin="PLLGND" pad="C1"/>
<connect gate="A" pin="PLLVDD" pad="B1"/>
<connect gate="A" pin="PLL_IN" pad="C3"/>
<connect gate="A" pin="PLL_OUT" pad="C2"/>
<connect gate="A" pin="RHP" pad="D5"/>
<connect gate="A" pin="RIN" pad="E3"/>
<connect gate="A" pin="SCL/SCK" pad="B6"/>
<connect gate="A" pin="SDA/SDI" pad="A4"/>
<connect gate="A" pin="VDDIO" pad="A6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM4937RL"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="04R9249"/>
<attribute name="PACKAGE" value="BGA-36"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM4937TL" prefix="U">
<description>Audio Amplifier</description>
<gates>
<gate name="A" symbol="LM4937TL"/>
</gates>
<devices>
<device name="" package="BGA36C50P6X6_351X325X67">
<connects>
<connect gate="A" pin="ADDR/ENB" pad="C4"/>
<connect gate="A" pin="AGND" pad="E6"/>
<connect gate="A" pin="AGND_2" pad="D1"/>
<connect gate="A" pin="AGND_3" pad="D2"/>
<connect gate="A" pin="AVDD" pad="F5"/>
<connect gate="A" pin="AVDD_2" pad="C6"/>
<connect gate="A" pin="BYPASS" pad="C5"/>
<connect gate="A" pin="CHP" pad="D6"/>
<connect gate="A" pin="DGND" pad="A1"/>
<connect gate="A" pin="DIFF+" pad="F1"/>
<connect gate="A" pin="DIFF-" pad="E1"/>
<connect gate="A" pin="DVDD" pad="A5"/>
<connect gate="A" pin="EP+" pad="F3"/>
<connect gate="A" pin="EP-" pad="F2"/>
<connect gate="A" pin="GPIO" pad="B4"/>
<connect gate="A" pin="I2C_VDD" pad="B5"/>
<connect gate="A" pin="I2S_CLK" pad="B3"/>
<connect gate="A" pin="I2S_SDATA" pad="B2"/>
<connect gate="A" pin="I2S_WS" pad="A3"/>
<connect gate="A" pin="LHP" pad="E5"/>
<connect gate="A" pin="LIN" pad="E2"/>
<connect gate="A" pin="LS+" pad="F6"/>
<connect gate="A" pin="LS-" pad="F4"/>
<connect gate="A" pin="MCLK" pad="A2"/>
<connect gate="A" pin="MODE" pad="D4"/>
<connect gate="A" pin="NC" pad="E4"/>
<connect gate="A" pin="NC_2" pad="D3"/>
<connect gate="A" pin="PLLGND" pad="C1"/>
<connect gate="A" pin="PLLVDD" pad="B1"/>
<connect gate="A" pin="PLL_IN" pad="C3"/>
<connect gate="A" pin="PLL_OUT" pad="C2"/>
<connect gate="A" pin="RHP" pad="D5"/>
<connect gate="A" pin="RIN" pad="E3"/>
<connect gate="A" pin="SCL/SCK" pad="B6"/>
<connect gate="A" pin="SDA/SDI" pad="A4"/>
<connect gate="A" pin="VDDIO" pad="A6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM4937TL"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="32M1200"/>
<attribute name="PACKAGE" value="BGA-36"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM4938MH" prefix="U">
<description>Stereo 2W Audio Power Amplifiers</description>
<gates>
<gate name="A" symbol="LM4938MH"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-29N">
<connects>
<connect gate="A" pin="BEEP_IN" pad="11"/>
<connect gate="A" pin="BYPASS" pad="22"/>
<connect gate="A" pin="DC_VOL" pad="7"/>
<connect gate="A" pin="EPAD" pad="29"/>
<connect gate="A" pin="GAINSELECT" pad="3"/>
<connect gate="A" pin="GND" pad="8"/>
<connect gate="A" pin="GND_2" pad="14"/>
<connect gate="A" pin="GND_3" pad="1"/>
<connect gate="A" pin="GND_4" pad="23"/>
<connect gate="A" pin="GND_5" pad="20"/>
<connect gate="A" pin="HP_SENSES" pad="21"/>
<connect gate="A" pin="LEFT_DOCK" pad="13"/>
<connect gate="A" pin="LEFT_GAIN1" pad="19"/>
<connect gate="A" pin="LEFT_GAIN2" pad="18"/>
<connect gate="A" pin="LEFT_IN" pad="12"/>
<connect gate="A" pin="LEFT_OUT+" pad="15"/>
<connect gate="A" pin="LEFT_OUT-" pad="17"/>
<connect gate="A" pin="MODE" pad="4"/>
<connect gate="A" pin="MUTE" pad="5"/>
<connect gate="A" pin="RIGHT_DOCK" pad="9"/>
<connect gate="A" pin="RIGHT_GAIN1" pad="24"/>
<connect gate="A" pin="RIGHT_GAIN2" pad="25"/>
<connect gate="A" pin="RIGHT_IN" pad="10"/>
<connect gate="A" pin="RIGHT_OUT+" pad="28"/>
<connect gate="A" pin="RIGHT_OUT-" pad="26"/>
<connect gate="A" pin="SHDN" pad="2"/>
<connect gate="A" pin="VDD" pad="27"/>
<connect gate="A" pin="VDD_2" pad="6"/>
<connect gate="A" pin="VDD_3" pad="16"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM4938MH"/>
<attribute name="OC_FARNELL" value="1008027"/>
<attribute name="OC_NEWARK" value="92K6210"/>
<attribute name="PACKAGE" value="TSSOP-28"/>
<attribute name="SUPPLIER" value="National"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM49450SQ" prefix="U">
<description>AUDIO AMPLIFIER</description>
<gates>
<gate name="A" symbol="LM49450SQ"/>
</gates>
<devices>
<device name="" package="QFN50P500X500X80-33N">
<connects>
<connect gate="A" pin="BYPASS" pad="17"/>
<connect gate="A" pin="C1N" pad="31"/>
<connect gate="A" pin="C1P" pad="1"/>
<connect gate="A" pin="CPGND" pad="2"/>
<connect gate="A" pin="CPVDD" pad="32"/>
<connect gate="A" pin="DGND" pad="4"/>
<connect gate="A" pin="DVDD" pad="10"/>
<connect gate="A" pin="GND" pad="33"/>
<connect gate="A" pin="GND_2" pad="12"/>
<connect gate="A" pin="HPGND" pad="25"/>
<connect gate="A" pin="HPL" pad="29"/>
<connect gate="A" pin="HPR" pad="27"/>
<connect gate="A" pin="HPS" pad="26"/>
<connect gate="A" pin="HPVDD" pad="28"/>
<connect gate="A" pin="HPVSS" pad="30"/>
<connect gate="A" pin="I2S_CLK" pad="7"/>
<connect gate="A" pin="I2S_SDI" pad="6"/>
<connect gate="A" pin="I2S_WS" pad="5"/>
<connect gate="A" pin="INL" pad="15"/>
<connect gate="A" pin="INR" pad="14"/>
<connect gate="A" pin="IOVDD" pad="11"/>
<connect gate="A" pin="LLS+" pad="19"/>
<connect gate="A" pin="LLS-" pad="20"/>
<connect gate="A" pin="LSGND" pad="21"/>
<connect gate="A" pin="LSVDD" pad="18"/>
<connect gate="A" pin="LSVDD_2" pad="24"/>
<connect gate="A" pin="MCLK" pad="8"/>
<connect gate="A" pin="REF" pad="13"/>
<connect gate="A" pin="RLS+" pad="23"/>
<connect gate="A" pin="RLS-" pad="22"/>
<connect gate="A" pin="SCL" pad="9"/>
<connect gate="A" pin="SDA" pad="3"/>
<connect gate="A" pin="VDD" pad="16"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM49450SQ"/>
<attribute name="OC_FARNELL" value="1685401"/>
<attribute name="OC_NEWARK" value="84M8142"/>
<attribute name="PACKAGE" value="LLP-32"/>
<attribute name="SUPPLIER" value="National semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM4947TL" prefix="U">
<description>Amplifier</description>
<gates>
<gate name="A" symbol="LM4947TL"/>
</gates>
<devices>
<device name="" package="BGA25C50P5X5_251X251X61">
<connects>
<connect gate="A" pin="ADDR" pad="C1"/>
<connect gate="A" pin="AVDD" pad="D4"/>
<connect gate="A" pin="AVDD_2" pad="D1"/>
<connect gate="A" pin="CBYPASS" pad="C4"/>
<connect gate="A" pin="GND" pad="E4"/>
<connect gate="A" pin="GND_2" pad="E2"/>
<connect gate="A" pin="I2CVDD" pad="D3"/>
<connect gate="A" pin="LHP" pad="E5"/>
<connect gate="A" pin="LHP3D1" pad="B4"/>
<connect gate="A" pin="LHP3D2" pad="B5"/>
<connect gate="A" pin="LIN1" pad="A2"/>
<connect gate="A" pin="LIN2" pad="B2"/>
<connect gate="A" pin="LS+" pad="E3"/>
<connect gate="A" pin="LS-" pad="E1"/>
<connect gate="A" pin="LSVDD" pad="D2"/>
<connect gate="A" pin="MIN+" pad="A3"/>
<connect gate="A" pin="MIN-" pad="B3"/>
<connect gate="A" pin="RHP" pad="D5"/>
<connect gate="A" pin="RHP3D1" pad="A4"/>
<connect gate="A" pin="RHP3D2" pad="A5"/>
<connect gate="A" pin="RIN1" pad="B1"/>
<connect gate="A" pin="RIN2" pad="A1"/>
<connect gate="A" pin="SCL" pad="C3"/>
<connect gate="A" pin="SDA" pad="C2"/>
<connect gate="A" pin="VOC" pad="C5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM4947TL"/>
<attribute name="OC_FARNELL" value="1286921"/>
<attribute name="OC_NEWARK" value="13M1886"/>
<attribute name="PACKAGE" value="BGA-25"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM4949TL" prefix="U">
<description>Stereo Class D Audio Subsystem</description>
<gates>
<gate name="A" symbol="LM4949TL"/>
</gates>
<devices>
<device name="" package="BGA25C5X5X50P_272X272X60">
<connects>
<connect gate="A" pin="ADR" pad="B2"/>
<connect gate="A" pin="BYPASS" pad="E5"/>
<connect gate="A" pin="GND" pad="E3"/>
<connect gate="A" pin="GNDLS" pad="C1"/>
<connect gate="A" pin="HPGND" pad="A4"/>
<connect gate="A" pin="HPL" pad="B4"/>
<connect gate="A" pin="HPR" pad="A5"/>
<connect gate="A" pin="I2CVDD" pad="D2"/>
<connect gate="A" pin="LIN+" pad="C4"/>
<connect gate="A" pin="LIN-" pad="D5"/>
<connect gate="A" pin="LLS+" pad="A2"/>
<connect gate="A" pin="LLS-" pad="A1"/>
<connect gate="A" pin="MIN+" pad="D4"/>
<connect gate="A" pin="MIN-" pad="E4"/>
<connect gate="A" pin="RIN+" pad="C3"/>
<connect gate="A" pin="RIN-" pad="B3"/>
<connect gate="A" pin="RLS+" pad="E2"/>
<connect gate="A" pin="RLS-" pad="E1"/>
<connect gate="A" pin="SCL" pad="D3"/>
<connect gate="A" pin="SDA" pad="A3"/>
<connect gate="A" pin="VDD" pad="C2"/>
<connect gate="A" pin="VDDHP" pad="C5"/>
<connect gate="A" pin="VDDLS" pad="D1"/>
<connect gate="A" pin="VDDLS_2" pad="B1"/>
<connect gate="A" pin="VOC" pad="B5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM4949TL"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="32M1206"/>
<attribute name="PACKAGE" value="BGA-25"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM4950TS" prefix="U">
<description>3.1W Stereo Audio Power Amplifier</description>
<gates>
<gate name="A" symbol="LM4950TS"/>
</gates>
<devices>
<device name="" package="TO97P1435X457-10N">
<connects>
<connect gate="A" pin="BYPASS" pad="8"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="GND(TAB)" pad="5"/>
<connect gate="A" pin="GND_2" pad="10"/>
<connect gate="A" pin="VDD" pad="6"/>
<connect gate="A" pin="VINA" pad="1"/>
<connect gate="A" pin="VINB" pad="9"/>
<connect gate="A" pin="VOUTA" pad="3"/>
<connect gate="A" pin="VOUTB" pad="7"/>
<connect gate="A" pin="~SHDN" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM4950TS"/>
<attribute name="OC_FARNELL" value="8181225"/>
<attribute name="OC_NEWARK" value="41K5990"/>
<attribute name="PACKAGE" value="TO-263-9"/>
<attribute name="SUPPLIER" value="National"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM4951SD" prefix="U">
<description>Wide Voltage Range 1.8 Watt Audio Amplifier</description>
<gates>
<gate name="A" symbol="LM4951SD"/>
</gates>
<devices>
<device name="" package="DFN80P400X400X80-11N">
<connects>
<connect gate="A" pin="BYPASS" pad="1"/>
<connect gate="A" pin="CCHG" pad="3"/>
<connect gate="A" pin="EPAD" pad="11"/>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="NC" pad="4"/>
<connect gate="A" pin="NC_2" pad="8"/>
<connect gate="A" pin="VDD" pad="9"/>
<connect gate="A" pin="VIN" pad="5"/>
<connect gate="A" pin="VO+" pad="10"/>
<connect gate="A" pin="VO-" pad="6"/>
<connect gate="A" pin="~SHDN" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM4951SD"/>
<attribute name="OC_FARNELL" value="1312786"/>
<attribute name="OC_NEWARK" value="31M5465"/>
<attribute name="PACKAGE" value="10-DFN"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM4952TS" prefix="U">
<description>3.1W Stereo-SE Audio Power Amplifier</description>
<gates>
<gate name="A" symbol="LM4952TS"/>
</gates>
<devices>
<device name="" package="TO97P1435X475-10N">
<connects>
<connect gate="A" pin="-VINA" pad="2"/>
<connect gate="A" pin="-VINB" pad="8"/>
<connect gate="A" pin="BYPASS" pad="9"/>
<connect gate="A" pin="DC_VOL" pad="1"/>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="GND_2" pad="10"/>
<connect gate="A" pin="VDD" pad="6"/>
<connect gate="A" pin="VOUTA" pad="4"/>
<connect gate="A" pin="VOUTB" pad="7"/>
<connect gate="A" pin="~SHDN" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM4952TS"/>
<attribute name="OC_FARNELL" value="1008028"/>
<attribute name="OC_NEWARK" value="41K5994"/>
<attribute name="PACKAGE" value="TO-263-9"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM4953SD" prefix="U">
<description>Ceramic Speaker Driver</description>
<gates>
<gate name="A" symbol="LM4953SD"/>
</gates>
<devices>
<device name="" package="DFN400X300X80-15N">
<connects>
<connect gate="A" pin="AVDD" pad="10"/>
<connect gate="A" pin="AVSS" pad="8"/>
<connect gate="A" pin="CCP+" pad="3"/>
<connect gate="A" pin="CCP-" pad="5"/>
<connect gate="A" pin="CPVDD" pad="2"/>
<connect gate="A" pin="EPAD" pad="15"/>
<connect gate="A" pin="NC" pad="12"/>
<connect gate="A" pin="NC_2" pad="7"/>
<connect gate="A" pin="OUTA" pad="11"/>
<connect gate="A" pin="OUTB" pad="9"/>
<connect gate="A" pin="PGND" pad="4"/>
<connect gate="A" pin="SD" pad="1"/>
<connect gate="A" pin="SGND" pad="14"/>
<connect gate="A" pin="VCP_OUT" pad="6"/>
<connect gate="A" pin="VIN" pad="13"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM4953SD"/>
<attribute name="OC_FARNELL" value="1798330"/>
<attribute name="OC_NEWARK" value="75R2100"/>
<attribute name="PACKAGE" value="DFN-14"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM4960SQ" prefix="U">
<description>Piezoelectric Speaker Driver</description>
<gates>
<gate name="A" symbol="LM4960SQ"/>
</gates>
<devices>
<device name="" package="QFN50P500X500X80-29N">
<connects>
<connect gate="A" pin="AMP_SHDN" pad="21"/>
<connect gate="A" pin="BYPASS" pad="1"/>
<connect gate="A" pin="EPAD" pad="29"/>
<connect gate="A" pin="FB" pad="8"/>
<connect gate="A" pin="GND" pad="25"/>
<connect gate="A" pin="GND_2" pad="7"/>
<connect gate="A" pin="GND_3" pad="12"/>
<connect gate="A" pin="GND_4" pad="24"/>
<connect gate="A" pin="NC" pad="19"/>
<connect gate="A" pin="NC_10" pad="18"/>
<connect gate="A" pin="NC_11" pad="5"/>
<connect gate="A" pin="NC_12" pad="22"/>
<connect gate="A" pin="NC_13" pad="26"/>
<connect gate="A" pin="NC_2" pad="9"/>
<connect gate="A" pin="NC_3" pad="10"/>
<connect gate="A" pin="NC_4" pad="13"/>
<connect gate="A" pin="NC_5" pad="14"/>
<connect gate="A" pin="NC_6" pad="15"/>
<connect gate="A" pin="NC_7" pad="16"/>
<connect gate="A" pin="NC_8" pad="17"/>
<connect gate="A" pin="NC_9" pad="3"/>
<connect gate="A" pin="REG_SHDN" pad="6"/>
<connect gate="A" pin="SW" pad="11"/>
<connect gate="A" pin="VAMP" pad="27"/>
<connect gate="A" pin="VDD" pad="4"/>
<connect gate="A" pin="VIN_A" pad="20"/>
<connect gate="A" pin="VIN_B" pad="2"/>
<connect gate="A" pin="VOUT_A" pad="23"/>
<connect gate="A" pin="VOUT_B" pad="28"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM4960SQ"/>
<attribute name="OC_FARNELL" value="1312787"/>
<attribute name="OC_NEWARK" value="31M5466"/>
<attribute name="PACKAGE" value="28-QFN"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM4961LQ" prefix="U">
<description>Ceramic Speaker Driver</description>
<gates>
<gate name="A" symbol="LM4961LQ"/>
</gates>
<devices>
<device name="" package="QFN50P500X500X80-29N">
<connects>
<connect gate="A" pin="BAND-SW" pad="19"/>
<connect gate="A" pin="BW1" pad="20"/>
<connect gate="A" pin="BW2" pad="21"/>
<connect gate="A" pin="BYPASS" pad="2"/>
<connect gate="A" pin="CCHG" pad="17"/>
<connect gate="A" pin="EPAD" pad="29"/>
<connect gate="A" pin="FB" pad="8"/>
<connect gate="A" pin="GND" pad="28"/>
<connect gate="A" pin="GND_2" pad="7"/>
<connect gate="A" pin="GND_3" pad="12"/>
<connect gate="A" pin="GND_4" pad="24"/>
<connect gate="A" pin="NC" pad="16"/>
<connect gate="A" pin="NC_2" pad="9"/>
<connect gate="A" pin="NC_3" pad="5"/>
<connect gate="A" pin="NC_4" pad="10"/>
<connect gate="A" pin="NC_5" pad="13"/>
<connect gate="A" pin="NC_6" pad="14"/>
<connect gate="A" pin="NC_7" pad="15"/>
<connect gate="A" pin="NC_8" pad="22"/>
<connect gate="A" pin="NC_9" pad="25"/>
<connect gate="A" pin="SHDN1" pad="6"/>
<connect gate="A" pin="SHDN2" pad="3"/>
<connect gate="A" pin="SW" pad="11"/>
<connect gate="A" pin="SW-OUT" pad="1"/>
<connect gate="A" pin="VAMP" pad="26"/>
<connect gate="A" pin="VDD" pad="4"/>
<connect gate="A" pin="VIN" pad="18"/>
<connect gate="A" pin="VOUT+" pad="27"/>
<connect gate="A" pin="VOUT-" pad="23"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM4961LQ"/>
<attribute name="OC_FARNELL" value="1312788"/>
<attribute name="OC_NEWARK" value="31M5467"/>
<attribute name="PACKAGE" value="QFN-28"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM4970SD" prefix="U">
<description>Audio Synchronized Color LED Driver</description>
<gates>
<gate name="A" symbol="LM4970SD"/>
</gates>
<devices>
<device name="" package="DFN400X300X80-15N">
<connects>
<connect gate="A" pin="ADR" pad="10"/>
<connect gate="A" pin="EPAD" pad="15"/>
<connect gate="A" pin="FILT" pad="1"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="I2CVDD" pad="7"/>
<connect gate="A" pin="LED1" pad="14"/>
<connect gate="A" pin="LED2" pad="13"/>
<connect gate="A" pin="LED3" pad="11"/>
<connect gate="A" pin="LGND" pad="12"/>
<connect gate="A" pin="LIN" pad="5"/>
<connect gate="A" pin="MIN" pad="3"/>
<connect gate="A" pin="RIN" pad="6"/>
<connect gate="A" pin="SCL" pad="9"/>
<connect gate="A" pin="SDA" pad="8"/>
<connect gate="A" pin="VDD" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM4970SD"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K6000"/>
<attribute name="PACKAGE" value="DFN-14"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM5000SD-3" prefix="U">
<description>High Voltage Switch Mode Regulator</description>
<gates>
<gate name="A" symbol="LM5000SD-3"/>
</gates>
<devices>
<device name="" package="DFN500X500X80-17N">
<connects>
<connect gate="A" pin="AGND" pad="4"/>
<connect gate="A" pin="BYP" pad="12"/>
<connect gate="A" pin="COMP" pad="1"/>
<connect gate="A" pin="EPAD" pad="17"/>
<connect gate="A" pin="FB" pad="2"/>
<connect gate="A" pin="FS" pad="15"/>
<connect gate="A" pin="PGND" pad="8"/>
<connect gate="A" pin="PGND_2" pad="5"/>
<connect gate="A" pin="PGND_3" pad="6"/>
<connect gate="A" pin="PGND_4" pad="7"/>
<connect gate="A" pin="SS" pad="14"/>
<connect gate="A" pin="SW" pad="11"/>
<connect gate="A" pin="SW_2" pad="9"/>
<connect gate="A" pin="SW_3" pad="10"/>
<connect gate="A" pin="TEST" pad="16"/>
<connect gate="A" pin="VIN" pad="13"/>
<connect gate="A" pin="~SHDN" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM5000SD-3"/>
<attribute name="OC_FARNELL" value="1685657"/>
<attribute name="OC_NEWARK" value="41K6020"/>
<attribute name="PACKAGE" value="DFN-16"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM5000SD-6" prefix="U">
<description>High Voltage Switch Mode Regulator</description>
<gates>
<gate name="A" symbol="LM5000SD-6"/>
</gates>
<devices>
<device name="" package="DFN500X500X80-17N">
<connects>
<connect gate="A" pin="AGND" pad="4"/>
<connect gate="A" pin="BYP" pad="12"/>
<connect gate="A" pin="COMP" pad="1"/>
<connect gate="A" pin="EPAD" pad="17"/>
<connect gate="A" pin="FB" pad="2"/>
<connect gate="A" pin="FS" pad="15"/>
<connect gate="A" pin="PGND" pad="8"/>
<connect gate="A" pin="PGND_2" pad="5"/>
<connect gate="A" pin="PGND_3" pad="6"/>
<connect gate="A" pin="PGND_4" pad="7"/>
<connect gate="A" pin="SS" pad="14"/>
<connect gate="A" pin="SW" pad="11"/>
<connect gate="A" pin="SW_2" pad="9"/>
<connect gate="A" pin="SW_3" pad="10"/>
<connect gate="A" pin="TEST" pad="16"/>
<connect gate="A" pin="VIN" pad="13"/>
<connect gate="A" pin="~SHDN" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM5000SD-6"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K6021"/>
<attribute name="PACKAGE" value="DFN-16"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM5001MA" prefix="U">
<description>REG SWITCH</description>
<gates>
<gate name="A" symbol="LM5001MA"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="COMP" pad="7"/>
<connect gate="A" pin="EN" pad="8"/>
<connect gate="A" pin="FB" pad="6"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="RT" pad="5"/>
<connect gate="A" pin="SW" pad="1"/>
<connect gate="A" pin="VCC" pad="3"/>
<connect gate="A" pin="VIN" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM5001MA"/>
<attribute name="OC_FARNELL" value="1325417"/>
<attribute name="OC_NEWARK" value="32M1216"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM5002MA" prefix="U">
<description>Switch Mode Regulator</description>
<gates>
<gate name="A" symbol="LM5002MA"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="COMP" pad="7"/>
<connect gate="A" pin="EN" pad="8"/>
<connect gate="A" pin="FB" pad="6"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="RT" pad="5"/>
<connect gate="A" pin="SW" pad="1"/>
<connect gate="A" pin="VCC" pad="3"/>
<connect gate="A" pin="VIN" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM5002MA"/>
<attribute name="OC_FARNELL" value="1325418"/>
<attribute name="OC_NEWARK" value="32M1220"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM5005MH" prefix="U">
<description>High Voltage 2.5 Amp Buck Regulator</description>
<gates>
<gate name="A" symbol="LM5005MH"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-21N">
<connects>
<connect gate="A" pin="AGND" pad="10"/>
<connect gate="A" pin="BST" pad="20"/>
<connect gate="A" pin="COMP" pad="6"/>
<connect gate="A" pin="EPAD" pad="21"/>
<connect gate="A" pin="FB" pad="7"/>
<connect gate="A" pin="IS" pad="16"/>
<connect gate="A" pin="IS_2" pad="15"/>
<connect gate="A" pin="OUT" pad="12"/>
<connect gate="A" pin="PGND" pad="14"/>
<connect gate="A" pin="PGND_2" pad="13"/>
<connect gate="A" pin="PRE" pad="19"/>
<connect gate="A" pin="RAMP" pad="9"/>
<connect gate="A" pin="RT" pad="8"/>
<connect gate="A" pin="SD" pad="2"/>
<connect gate="A" pin="SS" pad="11"/>
<connect gate="A" pin="SW" pad="18"/>
<connect gate="A" pin="SW_2" pad="17"/>
<connect gate="A" pin="SYNC" pad="5"/>
<connect gate="A" pin="VCC" pad="1"/>
<connect gate="A" pin="VIN" pad="4"/>
<connect gate="A" pin="VIN_2" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM5005MH"/>
<attribute name="OC_FARNELL" value="1286761"/>
<attribute name="OC_NEWARK" value="24M3532"/>
<attribute name="PACKAGE" value="TSSOP-20"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM5007MM" prefix="U">
<description>Step-Down Switching Regulator</description>
<gates>
<gate name="A" symbol="LM5007MM"/>
</gates>
<devices>
<device name="" package="SOP65P490X109-8N">
<connects>
<connect gate="A" pin="BST" pad="2"/>
<connect gate="A" pin="FEEDBACK" pad="5"/>
<connect gate="A" pin="RCL" pad="3"/>
<connect gate="A" pin="RON" pad="6"/>
<connect gate="A" pin="RTN" pad="4"/>
<connect gate="A" pin="SW" pad="1"/>
<connect gate="A" pin="VCC" pad="7"/>
<connect gate="A" pin="VIN" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM5007MM"/>
<attribute name="OC_FARNELL" value="9779345"/>
<attribute name="OC_NEWARK" value="97K3542"/>
<attribute name="PACKAGE" value="SOP-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM5007SD" prefix="U">
<description>Step Down Switching Regulator</description>
<gates>
<gate name="A" symbol="LM5007SD"/>
</gates>
<devices>
<device name="" package="DFN400X400X80-9N">
<connects>
<connect gate="A" pin="BST" pad="2"/>
<connect gate="A" pin="EPAD" pad="9"/>
<connect gate="A" pin="FB" pad="5"/>
<connect gate="A" pin="RCL" pad="3"/>
<connect gate="A" pin="RON" pad="6"/>
<connect gate="A" pin="RTN" pad="4"/>
<connect gate="A" pin="SW" pad="1"/>
<connect gate="A" pin="VCC" pad="7"/>
<connect gate="A" pin="VIN" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM5007SD"/>
<attribute name="OC_FARNELL" value="1685543"/>
<attribute name="OC_NEWARK" value="41K6026"/>
<attribute name="PACKAGE" value="DFN-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM5008AMM" prefix="U">
<description>Switching Regulator</description>
<gates>
<gate name="A" symbol="LM5008AMM"/>
</gates>
<devices>
<device name="" package="SOP65P490X110-8N">
<connects>
<connect gate="A" pin="BST" pad="2"/>
<connect gate="A" pin="FB" pad="5"/>
<connect gate="A" pin="RCL" pad="3"/>
<connect gate="A" pin="RT/SD" pad="6"/>
<connect gate="A" pin="RTN" pad="4"/>
<connect gate="A" pin="SW" pad="1"/>
<connect gate="A" pin="VCC" pad="7"/>
<connect gate="A" pin="VIN" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM5008AMM"/>
<attribute name="OC_FARNELL" value="1735798"/>
<attribute name="OC_NEWARK" value="14R4587"/>
<attribute name="PACKAGE" value="MSOP-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM5008ASD" prefix="U">
<description>Constant On-Time Buck Switching Regulator</description>
<gates>
<gate name="A" symbol="LM5008ASD"/>
</gates>
<devices>
<device name="" package="DFN400X400X80-9N">
<connects>
<connect gate="A" pin="BST" pad="2"/>
<connect gate="A" pin="EPAD" pad="9"/>
<connect gate="A" pin="FB" pad="5"/>
<connect gate="A" pin="RCL" pad="3"/>
<connect gate="A" pin="RT/SD" pad="6"/>
<connect gate="A" pin="RTN" pad="4"/>
<connect gate="A" pin="SW" pad="1"/>
<connect gate="A" pin="VCC" pad="7"/>
<connect gate="A" pin="VIN" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM5008ASD"/>
<attribute name="OC_FARNELL" value="1735799"/>
<attribute name="OC_NEWARK" value="14R4588"/>
<attribute name="PACKAGE" value="DFN-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM5008MM" prefix="U">
<description>Step-Down Switching Regulator</description>
<gates>
<gate name="A" symbol="LM5008MM"/>
</gates>
<devices>
<device name="" package="SOP65P490X109-8N">
<connects>
<connect gate="A" pin="BST" pad="2"/>
<connect gate="A" pin="FEEDBACK" pad="5"/>
<connect gate="A" pin="RCL" pad="3"/>
<connect gate="A" pin="RON" pad="6"/>
<connect gate="A" pin="RTN" pad="4"/>
<connect gate="A" pin="SW" pad="1"/>
<connect gate="A" pin="VCC" pad="7"/>
<connect gate="A" pin="VIN" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM5008MM"/>
<attribute name="OC_FARNELL" value="8181721"/>
<attribute name="OC_NEWARK" value="38K3760"/>
<attribute name="PACKAGE" value="SOP-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM5008SDC" prefix="U">
<description>Step Down Switching Regulator</description>
<gates>
<gate name="A" symbol="LM5008SDC"/>
</gates>
<devices>
<device name="" package="DFN400X400X80-9N">
<connects>
<connect gate="A" pin="BST" pad="2"/>
<connect gate="A" pin="EPAD" pad="9"/>
<connect gate="A" pin="FB" pad="5"/>
<connect gate="A" pin="RCL" pad="3"/>
<connect gate="A" pin="RON/SD" pad="6"/>
<connect gate="A" pin="RTN" pad="4"/>
<connect gate="A" pin="SW" pad="1"/>
<connect gate="A" pin="VCC" pad="7"/>
<connect gate="A" pin="VIN" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM5008SDC"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="13M1890"/>
<attribute name="PACKAGE" value="DFN-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM5009AMM" prefix="U">
<description>Switching Regulator</description>
<gates>
<gate name="A" symbol="LM5009AMM"/>
</gates>
<devices>
<device name="" package="SOP65P490X110-8N">
<connects>
<connect gate="A" pin="BST" pad="2"/>
<connect gate="A" pin="FB" pad="5"/>
<connect gate="A" pin="RCL" pad="3"/>
<connect gate="A" pin="RT/SD" pad="6"/>
<connect gate="A" pin="RTN" pad="4"/>
<connect gate="A" pin="SW" pad="1"/>
<connect gate="A" pin="VCC" pad="7"/>
<connect gate="A" pin="VIN" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM5009AMM"/>
<attribute name="OC_FARNELL" value="1735800"/>
<attribute name="OC_NEWARK" value="14R4589"/>
<attribute name="PACKAGE" value="MSOP-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM5009ASD" prefix="U">
<description>Constant On-Time Buck Switching Regulator</description>
<gates>
<gate name="A" symbol="LM5009ASD"/>
</gates>
<devices>
<device name="" package="DFN400X400X80-9N">
<connects>
<connect gate="A" pin="BST" pad="2"/>
<connect gate="A" pin="EPAD" pad="9"/>
<connect gate="A" pin="FB" pad="5"/>
<connect gate="A" pin="RCL" pad="3"/>
<connect gate="A" pin="RT/SD" pad="6"/>
<connect gate="A" pin="RTN" pad="4"/>
<connect gate="A" pin="SW" pad="1"/>
<connect gate="A" pin="VCC" pad="7"/>
<connect gate="A" pin="VIN" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM5009ASD"/>
<attribute name="OC_FARNELL" value="2064690"/>
<attribute name="OC_NEWARK" value="14R4590"/>
<attribute name="PACKAGE" value="DFN-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM5009MM" prefix="U">
<description>Step-Down Switching Regulator</description>
<gates>
<gate name="A" symbol="LM5009MM"/>
</gates>
<devices>
<device name="" package="SOP65P490X109-8N">
<connects>
<connect gate="A" pin="BST" pad="2"/>
<connect gate="A" pin="FEEDBACK" pad="5"/>
<connect gate="A" pin="RCL" pad="3"/>
<connect gate="A" pin="RTN" pad="4"/>
<connect gate="A" pin="SD/RON" pad="6"/>
<connect gate="A" pin="SW" pad="1"/>
<connect gate="A" pin="VCC" pad="7"/>
<connect gate="A" pin="VIN" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM5009MM"/>
<attribute name="OC_FARNELL" value="1312791"/>
<attribute name="OC_NEWARK" value="79K7931"/>
<attribute name="PACKAGE" value="SOP-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM5009SDC" prefix="U">
<description>Step Down Switching Regulator</description>
<gates>
<gate name="A" symbol="LM5009SDC"/>
</gates>
<devices>
<device name="" package="DFN400X400X80-9N">
<connects>
<connect gate="A" pin="BST" pad="2"/>
<connect gate="A" pin="EPAD" pad="9"/>
<connect gate="A" pin="FB" pad="5"/>
<connect gate="A" pin="RCL" pad="3"/>
<connect gate="A" pin="RON/SD" pad="6"/>
<connect gate="A" pin="RTN" pad="4"/>
<connect gate="A" pin="SW" pad="1"/>
<connect gate="A" pin="VCC" pad="7"/>
<connect gate="A" pin="VIN" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM5009SDC"/>
<attribute name="OC_FARNELL" value="1685578"/>
<attribute name="OC_NEWARK" value="13M1893"/>
<attribute name="PACKAGE" value="DFN-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM5010AMH" prefix="U">
<description>Step Down Switching Regulator</description>
<gates>
<gate name="A" symbol="LM5010AMH"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-15N">
<connects>
<connect gate="A" pin="BST" pad="3"/>
<connect gate="A" pin="EPAD" pad="15"/>
<connect gate="A" pin="FB" pad="9"/>
<connect gate="A" pin="ISEN" pad="4"/>
<connect gate="A" pin="NC" pad="8"/>
<connect gate="A" pin="NC_2" pad="1"/>
<connect gate="A" pin="NC_3" pad="7"/>
<connect gate="A" pin="NC_4" pad="14"/>
<connect gate="A" pin="RON/SD" pad="11"/>
<connect gate="A" pin="RTN" pad="6"/>
<connect gate="A" pin="SGND" pad="5"/>
<connect gate="A" pin="SS" pad="10"/>
<connect gate="A" pin="SW" pad="2"/>
<connect gate="A" pin="VCC" pad="12"/>
<connect gate="A" pin="VIN" pad="13"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM5010AMH"/>
<attribute name="OC_FARNELL" value="1286762"/>
<attribute name="OC_NEWARK" value="69K2586"/>
<attribute name="PACKAGE" value="TSSOP-14"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM5010AQ0MH" prefix="U">
<description>Switching Regulator</description>
<gates>
<gate name="A" symbol="LM5010AQ0MH"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-15N">
<connects>
<connect gate="A" pin="BST" pad="3"/>
<connect gate="A" pin="EPAD" pad="15"/>
<connect gate="A" pin="FB" pad="9"/>
<connect gate="A" pin="ISEN" pad="4"/>
<connect gate="A" pin="NC" pad="8"/>
<connect gate="A" pin="NC_2" pad="1"/>
<connect gate="A" pin="NC_3" pad="7"/>
<connect gate="A" pin="NC_4" pad="14"/>
<connect gate="A" pin="RON/SD" pad="11"/>
<connect gate="A" pin="RTN" pad="6"/>
<connect gate="A" pin="SGND" pad="5"/>
<connect gate="A" pin="SS" pad="10"/>
<connect gate="A" pin="SW" pad="2"/>
<connect gate="A" pin="VCC" pad="12"/>
<connect gate="A" pin="VIN" pad="13"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM5010AQ0MH"/>
<attribute name="OC_FARNELL" value="1689546"/>
<attribute name="OC_NEWARK" value="45P3730"/>
<attribute name="PACKAGE" value="TSSOP-14"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM5010AQ1MH">
<description>Step Down Switching Regulator</description>
<gates>
<gate name="A" symbol="LM5010AQ1MH"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-15N">
<connects>
<connect gate="A" pin="BST" pad="3"/>
<connect gate="A" pin="EPAD" pad="15"/>
<connect gate="A" pin="FB" pad="9"/>
<connect gate="A" pin="ISEN" pad="4"/>
<connect gate="A" pin="NC" pad="14"/>
<connect gate="A" pin="NC_2" pad="1"/>
<connect gate="A" pin="NC_3" pad="7"/>
<connect gate="A" pin="NC_4" pad="8"/>
<connect gate="A" pin="RON/SD" pad="11"/>
<connect gate="A" pin="RTN" pad="6"/>
<connect gate="A" pin="SGND" pad="5"/>
<connect gate="A" pin="SS" pad="10"/>
<connect gate="A" pin="SW" pad="2"/>
<connect gate="A" pin="VCC" pad="12"/>
<connect gate="A" pin="VIN" pad="13"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM5010AQ1MH"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="34P4873"/>
<attribute name="PACKAGE" value="TSSOP-14"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM5010ASD" prefix="U">
<description>Step Down Switching Regulator</description>
<gates>
<gate name="A" symbol="LM5010ASD"/>
</gates>
<devices>
<device name="" package="DFN400X400X80-11N">
<connects>
<connect gate="A" pin="BST" pad="2"/>
<connect gate="A" pin="EPAD" pad="11"/>
<connect gate="A" pin="FB" pad="6"/>
<connect gate="A" pin="ISEN" pad="3"/>
<connect gate="A" pin="RTN" pad="5"/>
<connect gate="A" pin="SD/RON" pad="8"/>
<connect gate="A" pin="SGND" pad="4"/>
<connect gate="A" pin="SS" pad="7"/>
<connect gate="A" pin="SW" pad="1"/>
<connect gate="A" pin="VCC" pad="9"/>
<connect gate="A" pin="VIN" pad="10"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM5010ASD"/>
<attribute name="OC_FARNELL" value="1685556"/>
<attribute name="OC_NEWARK" value="69K2590"/>
<attribute name="PACKAGE" value="DFN-10"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM5010MH" prefix="U">
<description>Step Down Switching Regulator</description>
<gates>
<gate name="A" symbol="LM5010MH"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-15N">
<connects>
<connect gate="A" pin="BST" pad="3"/>
<connect gate="A" pin="EPAD" pad="15"/>
<connect gate="A" pin="FB" pad="9"/>
<connect gate="A" pin="ISEN" pad="4"/>
<connect gate="A" pin="NC" pad="14"/>
<connect gate="A" pin="NC_2" pad="1"/>
<connect gate="A" pin="NC_3" pad="7"/>
<connect gate="A" pin="NC_4" pad="8"/>
<connect gate="A" pin="RTN" pad="6"/>
<connect gate="A" pin="SD/RON" pad="11"/>
<connect gate="A" pin="SGND" pad="5"/>
<connect gate="A" pin="SS" pad="10"/>
<connect gate="A" pin="SW" pad="2"/>
<connect gate="A" pin="VCC" pad="12"/>
<connect gate="A" pin="VIN" pad="13"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM5010MH"/>
<attribute name="OC_FARNELL" value="1685658"/>
<attribute name="OC_NEWARK" value="41K6032"/>
<attribute name="PACKAGE" value="TSSOP-14"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM5010SD" prefix="U">
<description>Step Down Switching Regulator</description>
<gates>
<gate name="A" symbol="LM5010SD"/>
</gates>
<devices>
<device name="" package="DFN400X400X80-11N">
<connects>
<connect gate="A" pin="BST" pad="2"/>
<connect gate="A" pin="EPAD" pad="11"/>
<connect gate="A" pin="FB" pad="6"/>
<connect gate="A" pin="ISEN" pad="3"/>
<connect gate="A" pin="RTN" pad="5"/>
<connect gate="A" pin="SD/RON" pad="8"/>
<connect gate="A" pin="SGND" pad="4"/>
<connect gate="A" pin="SS" pad="7"/>
<connect gate="A" pin="SW" pad="1"/>
<connect gate="A" pin="VCC" pad="9"/>
<connect gate="A" pin="VIN" pad="10"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM5010SD"/>
<attribute name="OC_FARNELL" value="1008257"/>
<attribute name="OC_NEWARK" value="41K6034"/>
<attribute name="PACKAGE" value="DFN-10"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM5020MM-1" prefix="U">
<description>Current Mode PWM Controller</description>
<gates>
<gate name="A" symbol="LM5020MM-1"/>
</gates>
<devices>
<device name="" package="SOP50P490X109-10N">
<connects>
<connect gate="A" pin="COMP" pad="3"/>
<connect gate="A" pin="CS" pad="8"/>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="OUT" pad="5"/>
<connect gate="A" pin="RT/SYNC" pad="9"/>
<connect gate="A" pin="SS" pad="10"/>
<connect gate="A" pin="UVLO" pad="7"/>
<connect gate="A" pin="VCC" pad="4"/>
<connect gate="A" pin="VFB" pad="2"/>
<connect gate="A" pin="VIN" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM5020MM-1"/>
<attribute name="OC_FARNELL" value="8181730"/>
<attribute name="OC_NEWARK" value="41K6036"/>
<attribute name="PACKAGE" value="SOP-10"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM5020MM-2" prefix="U">
<description>Current Mode PWM Controller</description>
<gates>
<gate name="A" symbol="LM5020MM-2"/>
</gates>
<devices>
<device name="" package="SOP50P490X109-10N">
<connects>
<connect gate="A" pin="COMP" pad="3"/>
<connect gate="A" pin="CS" pad="8"/>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="OUT" pad="5"/>
<connect gate="A" pin="RT/SYNC" pad="9"/>
<connect gate="A" pin="SS" pad="10"/>
<connect gate="A" pin="UVLO" pad="7"/>
<connect gate="A" pin="VCC" pad="4"/>
<connect gate="A" pin="VFB" pad="2"/>
<connect gate="A" pin="VIN" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM5020MM-2"/>
<attribute name="OC_FARNELL" value="8181748"/>
<attribute name="OC_NEWARK" value="41K6037"/>
<attribute name="PACKAGE" value="SOP-10"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM5020SD-1" prefix="U">
<description>Current Mode PWM Controller</description>
<gates>
<gate name="A" symbol="LM5020SD-1"/>
</gates>
<devices>
<device name="" package="DFN400X400X80-11N">
<connects>
<connect gate="A" pin="COMP" pad="3"/>
<connect gate="A" pin="CS" pad="8"/>
<connect gate="A" pin="EPAD" pad="11"/>
<connect gate="A" pin="FB" pad="2"/>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="OUT" pad="5"/>
<connect gate="A" pin="RT/SYNC" pad="9"/>
<connect gate="A" pin="SS" pad="10"/>
<connect gate="A" pin="UVLO" pad="7"/>
<connect gate="A" pin="VCC" pad="4"/>
<connect gate="A" pin="VIN" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM5020SD-1"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K6040"/>
<attribute name="PACKAGE" value="DFN-10"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM5021MM-1" prefix="U">
<description>PWM CONTROLLER</description>
<gates>
<gate name="A" symbol="LM5021MM-1"/>
</gates>
<devices>
<device name="" package="SOP65P490X110-8N">
<connects>
<connect gate="A" pin="COMP" pad="1"/>
<connect gate="A" pin="CS" pad="6"/>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="OUT" pad="4"/>
<connect gate="A" pin="RT" pad="7"/>
<connect gate="A" pin="SS" pad="8"/>
<connect gate="A" pin="VCC" pad="3"/>
<connect gate="A" pin="VIN" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM5021MM-1"/>
<attribute name="OC_FARNELL" value="1312589"/>
<attribute name="OC_NEWARK" value="65K6375"/>
<attribute name="PACKAGE" value="MSOP-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM5021MM-2" prefix="U">
<description>PWM CONTROLLER</description>
<gates>
<gate name="A" symbol="LM5021MM-2"/>
</gates>
<devices>
<device name="" package="SOP65P490X110-8N">
<connects>
<connect gate="A" pin="COMP" pad="1"/>
<connect gate="A" pin="CS" pad="6"/>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="OUT" pad="4"/>
<connect gate="A" pin="RT" pad="7"/>
<connect gate="A" pin="SS" pad="8"/>
<connect gate="A" pin="VCC" pad="3"/>
<connect gate="A" pin="VIN" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM5021MM-2"/>
<attribute name="OC_FARNELL" value="1312590"/>
<attribute name="OC_NEWARK" value="31M5471"/>
<attribute name="PACKAGE" value="MSOP-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM5022MM" prefix="U">
<description>Low Side Controller for Boost and SEPIC</description>
<gates>
<gate name="A" symbol="LM5022MM"/>
</gates>
<devices>
<device name="" package="SOP50P490X110-10N">
<connects>
<connect gate="A" pin="COMP" pad="3"/>
<connect gate="A" pin="CS" pad="8"/>
<connect gate="A" pin="FB" pad="2"/>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="OUT" pad="5"/>
<connect gate="A" pin="RT/SYNC" pad="9"/>
<connect gate="A" pin="SS" pad="10"/>
<connect gate="A" pin="UVLO" pad="7"/>
<connect gate="A" pin="VCC" pad="4"/>
<connect gate="A" pin="VIN" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM5022MM"/>
<attribute name="OC_FARNELL" value="1325423"/>
<attribute name="OC_NEWARK" value="32M1225"/>
<attribute name="PACKAGE" value="MSOP-10"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM5025AMTC" prefix="U">
<description>Active Clamp Voltage Mode PWM Controller</description>
<gates>
<gate name="A" symbol="LM5025AMTC"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-16N">
<connects>
<connect gate="A" pin="AGND" pad="11"/>
<connect gate="A" pin="COMP" pad="13"/>
<connect gate="A" pin="CS1" pad="3"/>
<connect gate="A" pin="CS2" pad="4"/>
<connect gate="A" pin="OUTA" pad="8"/>
<connect gate="A" pin="OUTB" pad="9"/>
<connect gate="A" pin="PGND" pad="10"/>
<connect gate="A" pin="RAMP" pad="2"/>
<connect gate="A" pin="REF" pad="6"/>
<connect gate="A" pin="RT" pad="14"/>
<connect gate="A" pin="SS" pad="12"/>
<connect gate="A" pin="SYNC" pad="15"/>
<connect gate="A" pin="TIME" pad="5"/>
<connect gate="A" pin="UVLO" pad="16"/>
<connect gate="A" pin="VCC" pad="7"/>
<connect gate="A" pin="VIN" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM5025AMTC"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K6044"/>
<attribute name="PACKAGE" value="TSSOP-16"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM5025ASD" prefix="U">
<description>Active Clamp Voltage Mode PWM Controller</description>
<gates>
<gate name="A" symbol="LM5025ASD"/>
</gates>
<devices>
<device name="" package="DFN500X500X80-17N">
<connects>
<connect gate="A" pin="AGND" pad="11"/>
<connect gate="A" pin="COMP" pad="13"/>
<connect gate="A" pin="CS1" pad="3"/>
<connect gate="A" pin="CS2" pad="4"/>
<connect gate="A" pin="EPAD" pad="17"/>
<connect gate="A" pin="OUTA" pad="8"/>
<connect gate="A" pin="OUTB" pad="9"/>
<connect gate="A" pin="PGND" pad="10"/>
<connect gate="A" pin="RAMP" pad="2"/>
<connect gate="A" pin="REF" pad="6"/>
<connect gate="A" pin="RT" pad="14"/>
<connect gate="A" pin="SS" pad="12"/>
<connect gate="A" pin="SYNC" pad="15"/>
<connect gate="A" pin="TIME" pad="5"/>
<connect gate="A" pin="UVLO" pad="16"/>
<connect gate="A" pin="VCC" pad="7"/>
<connect gate="A" pin="VIN" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM5025ASD"/>
<attribute name="OC_FARNELL" value="1798331"/>
<attribute name="OC_NEWARK" value="73R9747"/>
<attribute name="PACKAGE" value="DFN-16"/>
<attribute name="SUPPLIER" value="National"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM5025BSD" prefix="U">
<description>Active Clamp Voltage Mode PWM Controller</description>
<gates>
<gate name="A" symbol="LM5025BSD"/>
</gates>
<devices>
<device name="" package="DFN500X500X80-17N">
<connects>
<connect gate="A" pin="AGND" pad="11"/>
<connect gate="A" pin="COMP" pad="13"/>
<connect gate="A" pin="CS1" pad="3"/>
<connect gate="A" pin="CS2" pad="4"/>
<connect gate="A" pin="EPAD" pad="17"/>
<connect gate="A" pin="OUT_A" pad="8"/>
<connect gate="A" pin="OUT_B" pad="9"/>
<connect gate="A" pin="PGND" pad="10"/>
<connect gate="A" pin="RAMP" pad="2"/>
<connect gate="A" pin="REF" pad="6"/>
<connect gate="A" pin="RT" pad="14"/>
<connect gate="A" pin="SS" pad="12"/>
<connect gate="A" pin="SYNC" pad="15"/>
<connect gate="A" pin="TIME" pad="5"/>
<connect gate="A" pin="UVLO" pad="16"/>
<connect gate="A" pin="VCC" pad="7"/>
<connect gate="A" pin="VIN" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM5025BSD"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="99K2507"/>
<attribute name="PACKAGE" value="DFN-16"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM5025MTC" prefix="U">
<description>Active Clamp Voltage Mode PWM Controller</description>
<gates>
<gate name="A" symbol="LM5025MTC"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-16N">
<connects>
<connect gate="A" pin="AGND" pad="11"/>
<connect gate="A" pin="COMP" pad="13"/>
<connect gate="A" pin="CS1" pad="3"/>
<connect gate="A" pin="CS2" pad="4"/>
<connect gate="A" pin="OUT_A" pad="8"/>
<connect gate="A" pin="OUT_B" pad="9"/>
<connect gate="A" pin="PGND" pad="10"/>
<connect gate="A" pin="RAMP" pad="2"/>
<connect gate="A" pin="REF" pad="6"/>
<connect gate="A" pin="RT" pad="14"/>
<connect gate="A" pin="SS" pad="12"/>
<connect gate="A" pin="SYNC" pad="15"/>
<connect gate="A" pin="TIME" pad="5"/>
<connect gate="A" pin="UVLO" pad="16"/>
<connect gate="A" pin="VCC" pad="7"/>
<connect gate="A" pin="VIN" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM5025MTC"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K6048"/>
<attribute name="PACKAGE" value="TSSOP-16"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM5025SD" prefix="U">
<description>Active Clamp Voltage Mode PWM Controller</description>
<gates>
<gate name="A" symbol="LM5025SD"/>
</gates>
<devices>
<device name="" package="DFN500X500X80-17N">
<connects>
<connect gate="A" pin="AGND" pad="11"/>
<connect gate="A" pin="COMP" pad="13"/>
<connect gate="A" pin="CS1" pad="3"/>
<connect gate="A" pin="CS2" pad="4"/>
<connect gate="A" pin="EPAD" pad="17"/>
<connect gate="A" pin="OUT_A" pad="8"/>
<connect gate="A" pin="OUT_B" pad="9"/>
<connect gate="A" pin="PGND" pad="10"/>
<connect gate="A" pin="RAMP" pad="2"/>
<connect gate="A" pin="REF" pad="6"/>
<connect gate="A" pin="RT" pad="14"/>
<connect gate="A" pin="SS" pad="12"/>
<connect gate="A" pin="SYNC" pad="15"/>
<connect gate="A" pin="TIME" pad="5"/>
<connect gate="A" pin="UVLO" pad="16"/>
<connect gate="A" pin="VCC" pad="7"/>
<connect gate="A" pin="VIN" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM5025SD"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K6050"/>
<attribute name="PACKAGE" value="Switcher"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM5026MT" prefix="U">
<description>Active Clamp Current Mode PWM Controller</description>
<gates>
<gate name="A" symbol="LM5026MT"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-16N">
<connects>
<connect gate="A" pin="AGND" pad="11"/>
<connect gate="A" pin="COMP" pad="13"/>
<connect gate="A" pin="CS" pad="3"/>
<connect gate="A" pin="DCL" pad="16"/>
<connect gate="A" pin="OUTA" pad="8"/>
<connect gate="A" pin="OUTB" pad="9"/>
<connect gate="A" pin="PGND" pad="10"/>
<connect gate="A" pin="REF" pad="6"/>
<connect gate="A" pin="RES" pad="4"/>
<connect gate="A" pin="RT" pad="14"/>
<connect gate="A" pin="SS" pad="12"/>
<connect gate="A" pin="SYNC" pad="15"/>
<connect gate="A" pin="TIME" pad="5"/>
<connect gate="A" pin="UVLO" pad="2"/>
<connect gate="A" pin="VCC" pad="7"/>
<connect gate="A" pin="VIN" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM5026MT"/>
<attribute name="OC_FARNELL" value="1286765"/>
<attribute name="OC_NEWARK" value="26M0419"/>
<attribute name="PACKAGE" value="TSSOP-16"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM5026SD" prefix="U">
<description>Active Clamp Current Mode PWM Controller</description>
<gates>
<gate name="A" symbol="LM5026SD"/>
</gates>
<devices>
<device name="" package="DFN500X500X80-17N">
<connects>
<connect gate="A" pin="AGND" pad="11"/>
<connect gate="A" pin="COMP" pad="13"/>
<connect gate="A" pin="CS" pad="3"/>
<connect gate="A" pin="DCL" pad="16"/>
<connect gate="A" pin="EPAD" pad="17"/>
<connect gate="A" pin="OUTA" pad="8"/>
<connect gate="A" pin="OUTB" pad="9"/>
<connect gate="A" pin="PGND" pad="10"/>
<connect gate="A" pin="REF" pad="6"/>
<connect gate="A" pin="RES" pad="4"/>
<connect gate="A" pin="RT" pad="14"/>
<connect gate="A" pin="SS" pad="12"/>
<connect gate="A" pin="SYNC" pad="15"/>
<connect gate="A" pin="TIME" pad="5"/>
<connect gate="A" pin="UVLO" pad="2"/>
<connect gate="A" pin="VCC" pad="7"/>
<connect gate="A" pin="VIN" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM5026SD"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="46M5554"/>
<attribute name="PACKAGE" value="DFN-16"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM5027MH" prefix="U">
<description>Voltage Mode Active Clamp Controller</description>
<gates>
<gate name="A" symbol="LM5027MH"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-21N">
<connects>
<connect gate="A" pin="AGND" pad="6"/>
<connect gate="A" pin="COMP" pad="8"/>
<connect gate="A" pin="CS" pad="15"/>
<connect gate="A" pin="EPAD" pad="21"/>
<connect gate="A" pin="OTP" pad="19"/>
<connect gate="A" pin="OUTA" pad="11"/>
<connect gate="A" pin="OUTB" pad="10"/>
<connect gate="A" pin="OUTSR" pad="12"/>
<connect gate="A" pin="PGND" pad="13"/>
<connect gate="A" pin="RAMP" pad="2"/>
<connect gate="A" pin="REF" pad="9"/>
<connect gate="A" pin="RES" pad="17"/>
<connect gate="A" pin="RT" pad="7"/>
<connect gate="A" pin="SS" pad="16"/>
<connect gate="A" pin="SSSR" pad="18"/>
<connect gate="A" pin="TIME1" pad="5"/>
<connect gate="A" pin="TIME2" pad="4"/>
<connect gate="A" pin="TIME3" pad="3"/>
<connect gate="A" pin="UVLO" pad="20"/>
<connect gate="A" pin="VCC" pad="14"/>
<connect gate="A" pin="VIN" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM5027MH"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="55R4090"/>
<attribute name="PACKAGE" value="TSSOP-20"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM5030MM" prefix="U">
<description>Switcher</description>
<gates>
<gate name="A" symbol="LM5030MM"/>
</gates>
<devices>
<device name="" package="SOP50P490X109-10N">
<connects>
<connect gate="A" pin="COMP" pad="3"/>
<connect gate="A" pin="CS" pad="8"/>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="OUT1" pad="5"/>
<connect gate="A" pin="OUT2" pad="6"/>
<connect gate="A" pin="RT" pad="9"/>
<connect gate="A" pin="SS" pad="10"/>
<connect gate="A" pin="VCC" pad="4"/>
<connect gate="A" pin="VFB" pad="2"/>
<connect gate="A" pin="VIN" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM5030MM"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K6052"/>
<attribute name="PACKAGE" value="MSOP-10"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM5030SD" prefix="U">
<description>Push-Pull Current Mode PWM Controller</description>
<gates>
<gate name="A" symbol="LM5030SD"/>
</gates>
<devices>
<device name="" package="DFN400X400X80-11N">
<connects>
<connect gate="A" pin="COMP" pad="3"/>
<connect gate="A" pin="CS" pad="8"/>
<connect gate="A" pin="EPAD" pad="11"/>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="OUT1" pad="5"/>
<connect gate="A" pin="OUT2" pad="6"/>
<connect gate="A" pin="RT" pad="9"/>
<connect gate="A" pin="SS" pad="10"/>
<connect gate="A" pin="VCC" pad="4"/>
<connect gate="A" pin="VFB" pad="2"/>
<connect gate="A" pin="VIN" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM5030SD"/>
<attribute name="OC_FARNELL" value="1798332"/>
<attribute name="OC_NEWARK" value="73R9748"/>
<attribute name="PACKAGE" value="10-DFN"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM5032MTC" prefix="U">
<description>High Voltage Dual Interleaved Current Mode Controller</description>
<gates>
<gate name="A" symbol="LM5032MTC"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-16N">
<connects>
<connect gate="A" pin="COMP1" pad="2"/>
<connect gate="A" pin="COMP2" pad="14"/>
<connect gate="A" pin="CS1" pad="3"/>
<connect gate="A" pin="CS2" pad="13"/>
<connect gate="A" pin="DCL" pad="15"/>
<connect gate="A" pin="GND1" pad="8"/>
<connect gate="A" pin="GND2" pad="9"/>
<connect gate="A" pin="OUT1" pad="7"/>
<connect gate="A" pin="OUT2" pad="10"/>
<connect gate="A" pin="RES" pad="11"/>
<connect gate="A" pin="RT/SYNC" pad="16"/>
<connect gate="A" pin="SS1" pad="4"/>
<connect gate="A" pin="SS2" pad="12"/>
<connect gate="A" pin="UVLO" pad="5"/>
<connect gate="A" pin="VCC" pad="6"/>
<connect gate="A" pin="VIN" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM5032MTC"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K6058"/>
<attribute name="PACKAGE" value="TSSOP-16"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM5033MM" prefix="U">
<description>Push-Pull Voltage Mode PWM Controller</description>
<gates>
<gate name="A" symbol="LM5033MM"/>
</gates>
<devices>
<device name="" package="MSOP50P490X110-10N">
<connects>
<connect gate="A" pin="COMP" pad="3"/>
<connect gate="A" pin="CS" pad="8"/>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="OUT1" pad="5"/>
<connect gate="A" pin="OUT2" pad="6"/>
<connect gate="A" pin="REF" pad="2"/>
<connect gate="A" pin="RT/SYNC" pad="9"/>
<connect gate="A" pin="SS" pad="10"/>
<connect gate="A" pin="VCC" pad="4"/>
<connect gate="A" pin="VIN" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM5033MM"/>
<attribute name="OC_FARNELL" value="1312591"/>
<attribute name="OC_NEWARK" value="65K6383"/>
<attribute name="PACKAGE" value="MSOP-10"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM5033SD" prefix="U">
<description>Push-Pull Voltage Mode PWM Controller</description>
<gates>
<gate name="A" symbol="LM5033SD"/>
</gates>
<devices>
<device name="" package="DFN400X400X80-11N">
<connects>
<connect gate="A" pin="COMP" pad="3"/>
<connect gate="A" pin="CS" pad="8"/>
<connect gate="A" pin="EPAD" pad="11"/>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="OUT1" pad="5"/>
<connect gate="A" pin="OUT2" pad="6"/>
<connect gate="A" pin="REF" pad="2"/>
<connect gate="A" pin="RT/SYNC" pad="9"/>
<connect gate="A" pin="SS" pad="10"/>
<connect gate="A" pin="VCC" pad="4"/>
<connect gate="A" pin="VIN" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM5033SD"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K6060"/>
<attribute name="PACKAGE" value="DFN-10"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM5034MTC" prefix="U">
<description>High Voltage Dual Interleaved Current Mode Controller</description>
<gates>
<gate name="A" symbol="LM5034MTC"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-20N">
<connects>
<connect gate="A" pin="AC1" pad="9"/>
<connect gate="A" pin="AC2" pad="12"/>
<connect gate="A" pin="COMP1" pad="3"/>
<connect gate="A" pin="COMP2" pad="18"/>
<connect gate="A" pin="CS1" pad="4"/>
<connect gate="A" pin="CS2" pad="17"/>
<connect gate="A" pin="DCL" pad="19"/>
<connect gate="A" pin="GND1" pad="10"/>
<connect gate="A" pin="GND2" pad="11"/>
<connect gate="A" pin="OUT1" pad="8"/>
<connect gate="A" pin="OUT2" pad="13"/>
<connect gate="A" pin="OVLP" pad="1"/>
<connect gate="A" pin="RES" pad="15"/>
<connect gate="A" pin="RT/SYNC" pad="20"/>
<connect gate="A" pin="SS1" pad="5"/>
<connect gate="A" pin="SS2" pad="16"/>
<connect gate="A" pin="UVLO" pad="6"/>
<connect gate="A" pin="VCC1" pad="7"/>
<connect gate="A" pin="VCC2" pad="14"/>
<connect gate="A" pin="VIN" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM5034MTC"/>
<attribute name="OC_FARNELL" value="1694027"/>
<attribute name="OC_NEWARK" value="41K6062"/>
<attribute name="PACKAGE" value="TSSOP-20"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM5035AMH" prefix="U">
<description>PWM Controller</description>
<gates>
<gate name="A" symbol="LM5035AMH"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-21N">
<connects>
<connect gate="A" pin="AGND" pad="6"/>
<connect gate="A" pin="COMP" pad="4"/>
<connect gate="A" pin="CS" pad="7"/>
<connect gate="A" pin="DLY" pad="9"/>
<connect gate="A" pin="EPAD" pad="21"/>
<connect gate="A" pin="HB" pad="11"/>
<connect gate="A" pin="HO" pad="13"/>
<connect gate="A" pin="HS" pad="12"/>
<connect gate="A" pin="LO" pad="14"/>
<connect gate="A" pin="OVP" pad="3"/>
<connect gate="A" pin="PGND" pad="15"/>
<connect gate="A" pin="RAMP" pad="1"/>
<connect gate="A" pin="REF" pad="19"/>
<connect gate="A" pin="RES" pad="10"/>
<connect gate="A" pin="RT" pad="5"/>
<connect gate="A" pin="SR1" pad="18"/>
<connect gate="A" pin="SR2" pad="17"/>
<connect gate="A" pin="SS" pad="8"/>
<connect gate="A" pin="UVLO" pad="2"/>
<connect gate="A" pin="VCC" pad="16"/>
<connect gate="A" pin="VIN" pad="20"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM5035AMH"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="84M8148"/>
<attribute name="PACKAGE" value="TSSOP-16"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM5035ASQ" prefix="U">
<description>PWM Controller</description>
<gates>
<gate name="A" symbol="LM5035ASQ"/>
</gates>
<devices>
<device name="" package="QFN50P400X500X80-25N">
<connects>
<connect gate="A" pin="AGND" pad="5"/>
<connect gate="A" pin="COMP" pad="3"/>
<connect gate="A" pin="CS" pad="6"/>
<connect gate="A" pin="DLY" pad="8"/>
<connect gate="A" pin="EPAD" pad="25"/>
<connect gate="A" pin="HB" pad="11"/>
<connect gate="A" pin="HO" pad="13"/>
<connect gate="A" pin="HS" pad="12"/>
<connect gate="A" pin="LO" pad="14"/>
<connect gate="A" pin="NC" pad="22"/>
<connect gate="A" pin="NC_2" pad="1"/>
<connect gate="A" pin="NC_3" pad="10"/>
<connect gate="A" pin="NC_4" pad="20"/>
<connect gate="A" pin="OVP" pad="2"/>
<connect gate="A" pin="PGND" pad="15"/>
<connect gate="A" pin="RAMP" pad="23"/>
<connect gate="A" pin="REF" pad="19"/>
<connect gate="A" pin="RES" pad="9"/>
<connect gate="A" pin="RT" pad="4"/>
<connect gate="A" pin="SR1" pad="18"/>
<connect gate="A" pin="SR2" pad="17"/>
<connect gate="A" pin="SS" pad="7"/>
<connect gate="A" pin="UVLO" pad="24"/>
<connect gate="A" pin="VCC" pad="16"/>
<connect gate="A" pin="VIN" pad="21"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM5035ASQ"/>
<attribute name="OC_FARNELL" value="1685773"/>
<attribute name="OC_NEWARK" value="84M8150"/>
<attribute name="PACKAGE" value="QFN-24"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM5035BMH" prefix="U">
<description>PWM Controller</description>
<gates>
<gate name="A" symbol="LM5035BMH"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-21N">
<connects>
<connect gate="A" pin="AGND" pad="6"/>
<connect gate="A" pin="COMP" pad="4"/>
<connect gate="A" pin="CS" pad="7"/>
<connect gate="A" pin="DLY" pad="9"/>
<connect gate="A" pin="EPAD" pad="21"/>
<connect gate="A" pin="HB" pad="11"/>
<connect gate="A" pin="HO" pad="13"/>
<connect gate="A" pin="HS" pad="12"/>
<connect gate="A" pin="LO" pad="14"/>
<connect gate="A" pin="OVP" pad="3"/>
<connect gate="A" pin="PGND" pad="15"/>
<connect gate="A" pin="RAMP" pad="1"/>
<connect gate="A" pin="REF" pad="19"/>
<connect gate="A" pin="RES" pad="10"/>
<connect gate="A" pin="RT" pad="5"/>
<connect gate="A" pin="SR1" pad="18"/>
<connect gate="A" pin="SR2" pad="17"/>
<connect gate="A" pin="SS" pad="8"/>
<connect gate="A" pin="UVLO" pad="2"/>
<connect gate="A" pin="VCC" pad="16"/>
<connect gate="A" pin="VIN" pad="20"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM5035BMH"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="55R4092"/>
<attribute name="PACKAGE" value="TSSOP-20"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM5035BSQ" prefix="U">
<description>PWM Controller</description>
<gates>
<gate name="A" symbol="LM5035BSQ"/>
</gates>
<devices>
<device name="" package="QFN50P400X500X80-25N">
<connects>
<connect gate="A" pin="AGND" pad="5"/>
<connect gate="A" pin="COMP" pad="3"/>
<connect gate="A" pin="CS" pad="6"/>
<connect gate="A" pin="DLY" pad="8"/>
<connect gate="A" pin="EPAD" pad="25"/>
<connect gate="A" pin="HB" pad="11"/>
<connect gate="A" pin="HO" pad="13"/>
<connect gate="A" pin="HS" pad="12"/>
<connect gate="A" pin="LO" pad="14"/>
<connect gate="A" pin="NC" pad="22"/>
<connect gate="A" pin="NC_2" pad="1"/>
<connect gate="A" pin="NC_3" pad="10"/>
<connect gate="A" pin="NC_4" pad="20"/>
<connect gate="A" pin="OVP" pad="2"/>
<connect gate="A" pin="PGND" pad="15"/>
<connect gate="A" pin="RAMP" pad="23"/>
<connect gate="A" pin="REF" pad="19"/>
<connect gate="A" pin="RES" pad="9"/>
<connect gate="A" pin="RT" pad="4"/>
<connect gate="A" pin="SR1" pad="18"/>
<connect gate="A" pin="SR2" pad="17"/>
<connect gate="A" pin="SS" pad="7"/>
<connect gate="A" pin="UVLO" pad="24"/>
<connect gate="A" pin="VCC" pad="16"/>
<connect gate="A" pin="VIN" pad="21"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM5035BSQ"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="55R4094"/>
<attribute name="PACKAGE" value="QFN-24"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM5035CMH" prefix="U">
<description>PWM Controller</description>
<gates>
<gate name="A" symbol="LM5035CMH"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-21N">
<connects>
<connect gate="A" pin="AGND" pad="6"/>
<connect gate="A" pin="COMP" pad="4"/>
<connect gate="A" pin="CS" pad="7"/>
<connect gate="A" pin="DLY" pad="9"/>
<connect gate="A" pin="EPAD" pad="21"/>
<connect gate="A" pin="HB" pad="11"/>
<connect gate="A" pin="HO" pad="13"/>
<connect gate="A" pin="HS" pad="12"/>
<connect gate="A" pin="LO" pad="14"/>
<connect gate="A" pin="OVP" pad="3"/>
<connect gate="A" pin="PGND" pad="15"/>
<connect gate="A" pin="RAMP" pad="1"/>
<connect gate="A" pin="REF" pad="19"/>
<connect gate="A" pin="RES" pad="10"/>
<connect gate="A" pin="RT" pad="5"/>
<connect gate="A" pin="SR1" pad="18"/>
<connect gate="A" pin="SR2" pad="17"/>
<connect gate="A" pin="SS" pad="8"/>
<connect gate="A" pin="UVLO" pad="2"/>
<connect gate="A" pin="VCC" pad="16"/>
<connect gate="A" pin="VIN" pad="20"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM5035CMH"/>
<attribute name="OC_FARNELL" value="1822988"/>
<attribute name="OC_NEWARK" value="76R6960"/>
<attribute name="PACKAGE" value="TSSOP-20"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM5035CSQ" prefix="U">
<description>PWM Controller</description>
<gates>
<gate name="A" symbol="LM5035CSQ"/>
</gates>
<devices>
<device name="" package="QFN50P400X500X80-25N">
<connects>
<connect gate="A" pin="AGND" pad="5"/>
<connect gate="A" pin="COMP" pad="3"/>
<connect gate="A" pin="CS" pad="6"/>
<connect gate="A" pin="DLY" pad="8"/>
<connect gate="A" pin="EPAD" pad="25"/>
<connect gate="A" pin="HB" pad="11"/>
<connect gate="A" pin="HO" pad="13"/>
<connect gate="A" pin="HS" pad="12"/>
<connect gate="A" pin="LO" pad="14"/>
<connect gate="A" pin="NC" pad="22"/>
<connect gate="A" pin="NC_2" pad="1"/>
<connect gate="A" pin="NC_3" pad="10"/>
<connect gate="A" pin="NC_4" pad="20"/>
<connect gate="A" pin="OVP" pad="2"/>
<connect gate="A" pin="PGND" pad="15"/>
<connect gate="A" pin="RAMP" pad="23"/>
<connect gate="A" pin="REF" pad="19"/>
<connect gate="A" pin="RES" pad="9"/>
<connect gate="A" pin="RT" pad="4"/>
<connect gate="A" pin="SR1" pad="18"/>
<connect gate="A" pin="SR2" pad="17"/>
<connect gate="A" pin="SS" pad="7"/>
<connect gate="A" pin="UVLO" pad="24"/>
<connect gate="A" pin="VCC" pad="16"/>
<connect gate="A" pin="VIN" pad="21"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM5035CSQ"/>
<attribute name="OC_FARNELL" value="1822989"/>
<attribute name="OC_NEWARK" value="76R6961"/>
<attribute name="PACKAGE" value="QFN-24"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM5035MH" prefix="U">
<description>PWM Controller</description>
<gates>
<gate name="A" symbol="LM5035MH"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-21N">
<connects>
<connect gate="A" pin="AGND" pad="6"/>
<connect gate="A" pin="COMP" pad="4"/>
<connect gate="A" pin="CS" pad="7"/>
<connect gate="A" pin="DLY" pad="9"/>
<connect gate="A" pin="EPAD" pad="21"/>
<connect gate="A" pin="HB" pad="11"/>
<connect gate="A" pin="HO" pad="13"/>
<connect gate="A" pin="HS" pad="12"/>
<connect gate="A" pin="LO" pad="14"/>
<connect gate="A" pin="OVP" pad="3"/>
<connect gate="A" pin="PGND" pad="15"/>
<connect gate="A" pin="RAMP" pad="1"/>
<connect gate="A" pin="REF" pad="19"/>
<connect gate="A" pin="RES" pad="10"/>
<connect gate="A" pin="RT" pad="5"/>
<connect gate="A" pin="SR1" pad="18"/>
<connect gate="A" pin="SR2" pad="17"/>
<connect gate="A" pin="SS" pad="8"/>
<connect gate="A" pin="UVLO" pad="2"/>
<connect gate="A" pin="VCC" pad="16"/>
<connect gate="A" pin="VIN" pad="20"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM5035MH"/>
<attribute name="OC_FARNELL" value="1685785"/>
<attribute name="OC_NEWARK" value="79K7937"/>
<attribute name="PACKAGE" value="TSSOP-20"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM5035SQ" prefix="U">
<description>PWM Controller</description>
<gates>
<gate name="A" symbol="LM5035SQ"/>
</gates>
<devices>
<device name="" package="QFN50P400X500X80-25N">
<connects>
<connect gate="A" pin="AGND" pad="5"/>
<connect gate="A" pin="COMP" pad="3"/>
<connect gate="A" pin="CS" pad="6"/>
<connect gate="A" pin="DLY" pad="8"/>
<connect gate="A" pin="EPAD" pad="25"/>
<connect gate="A" pin="HB" pad="11"/>
<connect gate="A" pin="HO" pad="13"/>
<connect gate="A" pin="HS" pad="12"/>
<connect gate="A" pin="LO" pad="14"/>
<connect gate="A" pin="NC" pad="22"/>
<connect gate="A" pin="NC_2" pad="1"/>
<connect gate="A" pin="NC_3" pad="10"/>
<connect gate="A" pin="NC_4" pad="20"/>
<connect gate="A" pin="OVP" pad="2"/>
<connect gate="A" pin="PGND" pad="15"/>
<connect gate="A" pin="RAMP" pad="23"/>
<connect gate="A" pin="REF" pad="19"/>
<connect gate="A" pin="RES" pad="9"/>
<connect gate="A" pin="RT" pad="4"/>
<connect gate="A" pin="SR1" pad="18"/>
<connect gate="A" pin="SR2" pad="17"/>
<connect gate="A" pin="SS" pad="7"/>
<connect gate="A" pin="UVLO" pad="24"/>
<connect gate="A" pin="VCC" pad="16"/>
<connect gate="A" pin="VIN" pad="21"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LLM5035SQ"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="99K2510"/>
<attribute name="PACKAGE" value="QFN-24"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM5041AMTC" prefix="U">
<description>PWM CONTROLLER</description>
<gates>
<gate name="A" symbol="LM5041AMTC"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-16N">
<connects>
<connect gate="A" pin="AGND" pad="11"/>
<connect gate="A" pin="COMP" pad="3"/>
<connect gate="A" pin="CS" pad="12"/>
<connect gate="A" pin="FB" pad="2"/>
<connect gate="A" pin="HD" pad="5"/>
<connect gate="A" pin="LD" pad="6"/>
<connect gate="A" pin="PGND" pad="10"/>
<connect gate="A" pin="PULL" pad="9"/>
<connect gate="A" pin="PUSH" pad="8"/>
<connect gate="A" pin="REF" pad="4"/>
<connect gate="A" pin="RT" pad="15"/>
<connect gate="A" pin="SS" pad="13"/>
<connect gate="A" pin="TIME" pad="14"/>
<connect gate="A" pin="UVLO" pad="16"/>
<connect gate="A" pin="VCC" pad="7"/>
<connect gate="A" pin="VIN" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM5041AMTC"/>
<attribute name="OC_FARNELL" value="1008259"/>
<attribute name="OC_NEWARK" value="97K3548"/>
<attribute name="PACKAGE" value="SOP-16"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM5041BMTC" prefix="U">
<description>Cascaded PWM Controller</description>
<gates>
<gate name="A" symbol="LM5041BMTC"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-16N">
<connects>
<connect gate="A" pin="AGND" pad="11"/>
<connect gate="A" pin="COMP" pad="3"/>
<connect gate="A" pin="CS" pad="12"/>
<connect gate="A" pin="FB" pad="2"/>
<connect gate="A" pin="HD" pad="5"/>
<connect gate="A" pin="LD" pad="6"/>
<connect gate="A" pin="PGND" pad="10"/>
<connect gate="A" pin="PULL" pad="9"/>
<connect gate="A" pin="PUSH" pad="8"/>
<connect gate="A" pin="REF" pad="4"/>
<connect gate="A" pin="RT" pad="15"/>
<connect gate="A" pin="SS" pad="13"/>
<connect gate="A" pin="TIME" pad="14"/>
<connect gate="A" pin="UVLO" pad="16"/>
<connect gate="A" pin="VCC" pad="7"/>
<connect gate="A" pin="VIN" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM5041BMTC"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="55R4096"/>
<attribute name="PACKAGE" value="TSSOP-16"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM5041MTC" prefix="U">
<description>Cascaded PWM Controller</description>
<gates>
<gate name="A" symbol="LM5041MTC"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-16N">
<connects>
<connect gate="A" pin="AGND" pad="11"/>
<connect gate="A" pin="COMP" pad="3"/>
<connect gate="A" pin="CS" pad="12"/>
<connect gate="A" pin="FB" pad="2"/>
<connect gate="A" pin="HD" pad="5"/>
<connect gate="A" pin="LD" pad="6"/>
<connect gate="A" pin="PGND" pad="10"/>
<connect gate="A" pin="PULL" pad="9"/>
<connect gate="A" pin="PUSH" pad="8"/>
<connect gate="A" pin="REF" pad="4"/>
<connect gate="A" pin="RT" pad="15"/>
<connect gate="A" pin="SS" pad="13"/>
<connect gate="A" pin="TIME" pad="14"/>
<connect gate="A" pin="UVLO" pad="16"/>
<connect gate="A" pin="VCC" pad="7"/>
<connect gate="A" pin="VIN" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM5041MTC"/>
<attribute name="OC_FARNELL" value="9779361"/>
<attribute name="OC_NEWARK" value="41K6068"/>
<attribute name="PACKAGE" value="SOP-16"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM5041SD" prefix="U">
<description>Cascaded PWM Controller</description>
<gates>
<gate name="A" symbol="LM5041SD"/>
</gates>
<devices>
<device name="" package="DFN500X500X80-17N">
<connects>
<connect gate="A" pin="AGND" pad="11"/>
<connect gate="A" pin="COMP" pad="3"/>
<connect gate="A" pin="CS" pad="12"/>
<connect gate="A" pin="FB" pad="2"/>
<connect gate="A" pin="HD" pad="5"/>
<connect gate="A" pin="LD" pad="6"/>
<connect gate="A" pin="PGND" pad="10"/>
<connect gate="A" pin="PULL" pad="9"/>
<connect gate="A" pin="PUSH" pad="8"/>
<connect gate="A" pin="REF" pad="4"/>
<connect gate="A" pin="RT" pad="15"/>
<connect gate="A" pin="SS" pad="13"/>
<connect gate="A" pin="THER_PAD" pad="17"/>
<connect gate="A" pin="TIME" pad="14"/>
<connect gate="A" pin="UVLO" pad="16"/>
<connect gate="A" pin="VCC" pad="7"/>
<connect gate="A" pin="VIN" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM5041SD"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K6070"/>
<attribute name="PACKAGE" value="DFN-16"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM5060Q1MM">
<description>High-Side Protection Controller</description>
<gates>
<gate name="A" symbol="LM5060Q1MM"/>
</gates>
<devices>
<device name="" package="SOP50P490X109-10N">
<connects>
<connect gate="A" pin="EN" pad="5"/>
<connect gate="A" pin="GATE" pad="10"/>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="NPGD" pad="8"/>
<connect gate="A" pin="OUT" pad="9"/>
<connect gate="A" pin="OVP" pad="3"/>
<connect gate="A" pin="SENSE" pad="1"/>
<connect gate="A" pin="TIMER" pad="7"/>
<connect gate="A" pin="UVLO" pad="4"/>
<connect gate="A" pin="VIN" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM5060Q1MM"/>
<attribute name="OC_FARNELL" value="1791110"/>
<attribute name="OC_NEWARK" value="55R4099"/>
<attribute name="PACKAGE" value="MSOP-10"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM5067MM-1" prefix="U">
<description>Negative Hot Swap / Inrush Current Controller</description>
<gates>
<gate name="A" symbol="LM5067MM-1"/>
</gates>
<devices>
<device name="" package="SOP50P490X110-10N">
<connects>
<connect gate="A" pin="GATE" pad="8"/>
<connect gate="A" pin="OUT" pad="9"/>
<connect gate="A" pin="OVLO" pad="3"/>
<connect gate="A" pin="PGD" pad="10"/>
<connect gate="A" pin="PWR" pad="4"/>
<connect gate="A" pin="SEN" pad="7"/>
<connect gate="A" pin="TIMER" pad="6"/>
<connect gate="A" pin="UVLO/EN" pad="2"/>
<connect gate="A" pin="VCC" pad="1"/>
<connect gate="A" pin="VEE" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM5067MM-1"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="64M7038"/>
<attribute name="PACKAGE" value="MSOP-10"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM5067MM-2" prefix="U">
<description>Negative Hot Swap / Inrush Current Controller</description>
<gates>
<gate name="A" symbol="LM5067MM-2"/>
</gates>
<devices>
<device name="" package="SOP50P490X110-10N">
<connects>
<connect gate="A" pin="GATE" pad="8"/>
<connect gate="A" pin="OUT" pad="9"/>
<connect gate="A" pin="OVLO" pad="3"/>
<connect gate="A" pin="PGD" pad="10"/>
<connect gate="A" pin="PWR" pad="4"/>
<connect gate="A" pin="SEN" pad="7"/>
<connect gate="A" pin="TIMER" pad="6"/>
<connect gate="A" pin="UVLO/EN" pad="2"/>
<connect gate="A" pin="VCC" pad="1"/>
<connect gate="A" pin="VEE" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM5067MM-2"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="64M7039"/>
<attribute name="PACKAGE" value="MSOP-10"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM5067MW-1" prefix="U">
<description>Negative Hot Swap / Inrush Current Controller</description>
<gates>
<gate name="A" symbol="LM5067MW-1"/>
</gates>
<devices>
<device name="" package="SOIC127P1032X265-14N">
<connects>
<connect gate="A" pin="GATE" pad="10"/>
<connect gate="A" pin="NC" pad="7"/>
<connect gate="A" pin="NC_2" pad="13"/>
<connect gate="A" pin="NC_3" pad="2"/>
<connect gate="A" pin="NC_4" pad="11"/>
<connect gate="A" pin="OUT" pad="12"/>
<connect gate="A" pin="OVLO" pad="4"/>
<connect gate="A" pin="PGD" pad="14"/>
<connect gate="A" pin="PWR" pad="5"/>
<connect gate="A" pin="SENSE" pad="9"/>
<connect gate="A" pin="TIMER" pad="8"/>
<connect gate="A" pin="UVLO/EN" pad="3"/>
<connect gate="A" pin="VCC" pad="1"/>
<connect gate="A" pin="VEE" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM5067MW-1"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="55R4101"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM5068MM-1" prefix="U">
<description>Negative Voltage Hot Swap Controller</description>
<gates>
<gate name="A" symbol="LM5068MM-1"/>
</gates>
<devices>
<device name="" package="SOP65P490X110-8N">
<connects>
<connect gate="A" pin="GATE" pad="6"/>
<connect gate="A" pin="OV" pad="2"/>
<connect gate="A" pin="PWRGD" pad="1"/>
<connect gate="A" pin="SENSE" pad="5"/>
<connect gate="A" pin="TIMER" pad="7"/>
<connect gate="A" pin="UV" pad="3"/>
<connect gate="A" pin="VDD" pad="8"/>
<connect gate="A" pin="VEE" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM5068MM-1"/>
<attribute name="OC_FARNELL" value="1008260"/>
<attribute name="OC_NEWARK" value="97K355097K3550"/>
<attribute name="PACKAGE" value="8-MSOP"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM5068MM-2" prefix="U">
<description>Negative Voltage Hot Swap Controller</description>
<gates>
<gate name="A" symbol="LM5068MM-2"/>
</gates>
<devices>
<device name="" package="SOP65P490X110-8N">
<connects>
<connect gate="A" pin="GATE" pad="6"/>
<connect gate="A" pin="OV" pad="2"/>
<connect gate="A" pin="POWERGOOD" pad="1"/>
<connect gate="A" pin="SENSE" pad="5"/>
<connect gate="A" pin="TIMER" pad="7"/>
<connect gate="A" pin="UV" pad="3"/>
<connect gate="A" pin="VDD" pad="8"/>
<connect gate="A" pin="VEE" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM5068MM-2"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K6073"/>
<attribute name="PACKAGE" value="MSOP-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM5068MM-3" prefix="U">
<description>Negative Voltage Hot Swap Controller</description>
<gates>
<gate name="A" symbol="LM5068MM-3"/>
</gates>
<devices>
<device name="" package="SOP65P490X110-8N">
<connects>
<connect gate="A" pin="GATE" pad="6"/>
<connect gate="A" pin="OV" pad="2"/>
<connect gate="A" pin="POWERGOOD" pad="1"/>
<connect gate="A" pin="SENSE" pad="5"/>
<connect gate="A" pin="TIMER" pad="7"/>
<connect gate="A" pin="UV" pad="3"/>
<connect gate="A" pin="VDD" pad="8"/>
<connect gate="A" pin="VEE" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM5068MM-3"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K6074"/>
<attribute name="PACKAGE" value="MSOP-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM5068MM-4" prefix="U">
<description>Negative Voltage Hot Swap Controller</description>
<gates>
<gate name="A" symbol="LM5068MM-4"/>
</gates>
<devices>
<device name="" package="SOP65P490X110-8N">
<connects>
<connect gate="A" pin="GATE" pad="6"/>
<connect gate="A" pin="OV" pad="2"/>
<connect gate="A" pin="POWERGOOD" pad="1"/>
<connect gate="A" pin="SENSE" pad="5"/>
<connect gate="A" pin="TIMER" pad="7"/>
<connect gate="A" pin="UV" pad="3"/>
<connect gate="A" pin="VDD" pad="8"/>
<connect gate="A" pin="VEE" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM5068MM-4"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K6075"/>
<attribute name="PACKAGE" value="MSOP-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM5069MM-1" prefix="U">
<description>Positive High Voltage Hot Swap / Inrush Current Controller</description>
<gates>
<gate name="A" symbol="LM5069MM-1"/>
</gates>
<devices>
<device name="" package="SOP50P490X110-10N">
<connects>
<connect gate="A" pin="GATE" pad="10"/>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="OUT" pad="9"/>
<connect gate="A" pin="OVLO" pad="4"/>
<connect gate="A" pin="PGD" pad="8"/>
<connect gate="A" pin="PWR" pad="7"/>
<connect gate="A" pin="SENSE" pad="1"/>
<connect gate="A" pin="TMR" pad="6"/>
<connect gate="A" pin="UVLO" pad="3"/>
<connect gate="A" pin="VIN" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM5069MM-1"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="13M1900"/>
<attribute name="PACKAGE" value="MSOP-10"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM5069MM-2" prefix="U">
<description>Current controller</description>
<gates>
<gate name="A" symbol="LM5069MM-2"/>
</gates>
<devices>
<device name="" package="SOP50P490X110-10N">
<connects>
<connect gate="A" pin="GATE" pad="10"/>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="OUT" pad="9"/>
<connect gate="A" pin="OVLO" pad="4"/>
<connect gate="A" pin="PGND" pad="8"/>
<connect gate="A" pin="PWR" pad="7"/>
<connect gate="A" pin="SENSE" pad="1"/>
<connect gate="A" pin="TIMER" pad="6"/>
<connect gate="A" pin="UVLO" pad="3"/>
<connect gate="A" pin="VIN" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM5069MM-2"/>
<attribute name="OC_FARNELL" value="1290933"/>
<attribute name="OC_NEWARK" value="13M1902"/>
<attribute name="PACKAGE" value="MSOP-10"/>
<attribute name="SUPPLIER" value="National"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM5070MTC-50" prefix="U">
<description>PWM Controller</description>
<gates>
<gate name="A" symbol="LM5070MTC-50"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-16N">
<connects>
<connect gate="A" pin="ARTN" pad="16"/>
<connect gate="A" pin="COMP" pad="12"/>
<connect gate="A" pin="CS" pad="13"/>
<connect gate="A" pin="FB" pad="11"/>
<connect gate="A" pin="OUT" pad="9"/>
<connect gate="A" pin="RCLASS" pad="3"/>
<connect gate="A" pin="RCLP" pad="6"/>
<connect gate="A" pin="RSIG" pad="2"/>
<connect gate="A" pin="RT" pad="14"/>
<connect gate="A" pin="RTN" pad="8"/>
<connect gate="A" pin="SS" pad="15"/>
<connect gate="A" pin="UVLO" pad="4"/>
<connect gate="A" pin="UVLORTN" pad="5"/>
<connect gate="A" pin="VCC" pad="10"/>
<connect gate="A" pin="VEE" pad="7"/>
<connect gate="A" pin="VIN" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM5070MTC-50"/>
<attribute name="OC_FARNELL" value="9123520"/>
<attribute name="OC_NEWARK" value="41K6080"/>
<attribute name="PACKAGE" value="TSSOP-16"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM5070MTC-80" prefix="U">
<description>Integrated Power Over Ethernet PD Interface</description>
<gates>
<gate name="A" symbol="LM5070MTC-80"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-16N">
<connects>
<connect gate="A" pin="ARTN" pad="16"/>
<connect gate="A" pin="COMP" pad="12"/>
<connect gate="A" pin="CS" pad="13"/>
<connect gate="A" pin="FB" pad="11"/>
<connect gate="A" pin="OUT" pad="9"/>
<connect gate="A" pin="RCLASS" pad="3"/>
<connect gate="A" pin="RCLP" pad="6"/>
<connect gate="A" pin="RSIG" pad="2"/>
<connect gate="A" pin="RT" pad="14"/>
<connect gate="A" pin="RTN" pad="8"/>
<connect gate="A" pin="SS" pad="15"/>
<connect gate="A" pin="UVLO" pad="4"/>
<connect gate="A" pin="UVLORTN" pad="5"/>
<connect gate="A" pin="VCC" pad="10"/>
<connect gate="A" pin="VEE" pad="7"/>
<connect gate="A" pin="VIN" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM5070MTC-80"/>
<attribute name="OC_FARNELL" value="1685659"/>
<attribute name="OC_NEWARK" value="41K6081"/>
<attribute name="PACKAGE" value="TSSOP-16"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM5070SD-80" prefix="U">
<description>Integrated Power Over Ethernet PD Interface</description>
<gates>
<gate name="A" symbol="LM5070SD-80"/>
</gates>
<devices>
<device name="" package="DFN500X500X80-17N">
<connects>
<connect gate="A" pin="ARTN" pad="16"/>
<connect gate="A" pin="COMP" pad="12"/>
<connect gate="A" pin="CS" pad="13"/>
<connect gate="A" pin="EPAD" pad="17"/>
<connect gate="A" pin="FB" pad="11"/>
<connect gate="A" pin="OUT" pad="9"/>
<connect gate="A" pin="RCLASS" pad="3"/>
<connect gate="A" pin="RCLP" pad="6"/>
<connect gate="A" pin="RSIG" pad="2"/>
<connect gate="A" pin="RT" pad="14"/>
<connect gate="A" pin="RTN" pad="8"/>
<connect gate="A" pin="SS" pad="15"/>
<connect gate="A" pin="UVLO" pad="4"/>
<connect gate="A" pin="UVLORTN" pad="5"/>
<connect gate="A" pin="VCC" pad="10"/>
<connect gate="A" pin="VEE" pad="7"/>
<connect gate="A" pin="VIN" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM5070SD-80"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K6085"/>
<attribute name="PACKAGE" value="DFN-16"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM5071MT-50" prefix="U">
<description>Power Over Ethernet PD Controller</description>
<gates>
<gate name="A" symbol="LM5071MT-50"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-16N">
<connects>
<connect gate="A" pin="ARTN" pad="16"/>
<connect gate="A" pin="AUX" pad="4"/>
<connect gate="A" pin="COMP" pad="12"/>
<connect gate="A" pin="CS" pad="13"/>
<connect gate="A" pin="FB" pad="11"/>
<connect gate="A" pin="OUT" pad="9"/>
<connect gate="A" pin="RCLASS" pad="3"/>
<connect gate="A" pin="RSIG" pad="2"/>
<connect gate="A" pin="RT" pad="14"/>
<connect gate="A" pin="RTN" pad="8"/>
<connect gate="A" pin="SS" pad="15"/>
<connect gate="A" pin="UVLO" pad="5"/>
<connect gate="A" pin="UVLO_RTN" pad="6"/>
<connect gate="A" pin="VCC" pad="10"/>
<connect gate="A" pin="VEE" pad="7"/>
<connect gate="A" pin="VIN" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM5071MT-50"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="79K7941"/>
<attribute name="PACKAGE" value="TSSOP-16"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM5071MT-80" prefix="U">
<description>Power Over Ethernet PD Controller</description>
<gates>
<gate name="A" symbol="LM5071MT-80"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-16N">
<connects>
<connect gate="A" pin="ARTN" pad="16"/>
<connect gate="A" pin="AUX" pad="4"/>
<connect gate="A" pin="COMP" pad="12"/>
<connect gate="A" pin="CS" pad="13"/>
<connect gate="A" pin="FB" pad="11"/>
<connect gate="A" pin="OUT" pad="9"/>
<connect gate="A" pin="RCLASS" pad="3"/>
<connect gate="A" pin="RSIG" pad="2"/>
<connect gate="A" pin="RT" pad="14"/>
<connect gate="A" pin="RTN" pad="8"/>
<connect gate="A" pin="SS" pad="15"/>
<connect gate="A" pin="UVLO" pad="5"/>
<connect gate="A" pin="UVLO_RTN" pad="6"/>
<connect gate="A" pin="VCC" pad="10"/>
<connect gate="A" pin="VEE" pad="7"/>
<connect gate="A" pin="VIN" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM5071MT-80"/>
<attribute name="OC_FARNELL" value="1685768"/>
<attribute name="OC_NEWARK" value="79K7942"/>
<attribute name="PACKAGE" value="TSSOP-16"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM5072MH-50" prefix="U">
<description>PWM Controller</description>
<gates>
<gate name="A" symbol="LM5072MH-50"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-17N">
<connects>
<connect gate="A" pin="ARTN" pad="16"/>
<connect gate="A" pin="COMP" pad="15"/>
<connect gate="A" pin="CS" pad="12"/>
<connect gate="A" pin="DCCL" pad="6"/>
<connect gate="A" pin="EP" pad="17"/>
<connect gate="A" pin="FB" pad="14"/>
<connect gate="A" pin="ICL_FAUX" pad="5"/>
<connect gate="A" pin="NPGOOD" pad="11"/>
<connect gate="A" pin="OUT" pad="9"/>
<connect gate="A" pin="RAUX" pad="13"/>
<connect gate="A" pin="RCLASS" pad="4"/>
<connect gate="A" pin="RT" pad="1"/>
<connect gate="A" pin="RTN" pad="8"/>
<connect gate="A" pin="SS" pad="2"/>
<connect gate="A" pin="VCC" pad="10"/>
<connect gate="A" pin="VEE" pad="7"/>
<connect gate="A" pin="VIN" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM5072MH-50"/>
<attribute name="OC_FARNELL" value="1286768"/>
<attribute name="OC_NEWARK" value="99K2518"/>
<attribute name="PACKAGE" value="TSSOP-16"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM5072MH-80" prefix="U">
<description>PWM Controller</description>
<gates>
<gate name="A" symbol="LM5072MH-80"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-17N">
<connects>
<connect gate="A" pin="ARTN" pad="16"/>
<connect gate="A" pin="COMP" pad="15"/>
<connect gate="A" pin="CS" pad="12"/>
<connect gate="A" pin="DCCL" pad="6"/>
<connect gate="A" pin="EP" pad="17"/>
<connect gate="A" pin="FB" pad="14"/>
<connect gate="A" pin="ICL_FAUX" pad="5"/>
<connect gate="A" pin="NPGOOD" pad="11"/>
<connect gate="A" pin="OUT" pad="9"/>
<connect gate="A" pin="RAUX" pad="13"/>
<connect gate="A" pin="RCLASS" pad="4"/>
<connect gate="A" pin="RT" pad="1"/>
<connect gate="A" pin="RTN" pad="8"/>
<connect gate="A" pin="SS" pad="2"/>
<connect gate="A" pin="VCC" pad="10"/>
<connect gate="A" pin="VEE" pad="7"/>
<connect gate="A" pin="VIN" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM5072MH-80"/>
<attribute name="OC_FARNELL" value="1286769"/>
<attribute name="OC_NEWARK" value="13M1907"/>
<attribute name="PACKAGE" value="TSSOP-16"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM5085MY" prefix="U">
<description>On-Time PFET Buck Switching Controller</description>
<gates>
<gate name="A" symbol="LM5085MY"/>
</gates>
<devices>
<device name="" package="SOP65P490X110-9N">
<connects>
<connect gate="A" pin="ADJ" pad="1"/>
<connect gate="A" pin="EPAD" pad="9"/>
<connect gate="A" pin="FB" pad="3"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="ISEN" pad="5"/>
<connect gate="A" pin="PGATE" pad="6"/>
<connect gate="A" pin="RT" pad="2"/>
<connect gate="A" pin="VCC" pad="7"/>
<connect gate="A" pin="VIN" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM5085MY"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="34P4878"/>
<attribute name="PACKAGE" value="MSOP-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM5085QMY" prefix="U">
<description>On-Time PFET Buck Switching Controller</description>
<gates>
<gate name="A" symbol="LM5085QMY"/>
</gates>
<devices>
<device name="" package="SOP65P490X110-9N">
<connects>
<connect gate="A" pin="ADJ" pad="1"/>
<connect gate="A" pin="EPAD" pad="9"/>
<connect gate="A" pin="FB" pad="3"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="ISEN" pad="5"/>
<connect gate="A" pin="PGATE" pad="6"/>
<connect gate="A" pin="RT" pad="2"/>
<connect gate="A" pin="VCC" pad="7"/>
<connect gate="A" pin="VIN" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM5085QMY"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="55R4104"/>
<attribute name="PACKAGE" value="MSOP-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM5085SD">
<description>On-Time PFET Buck Switching Controller</description>
<gates>
<gate name="A" symbol="LM5085SD"/>
</gates>
<devices>
<device name="" package="DFN300X300X80-9N">
<connects>
<connect gate="A" pin="ADJ" pad="1"/>
<connect gate="A" pin="EP" pad="9"/>
<connect gate="A" pin="FB" pad="3"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="ISEN" pad="5"/>
<connect gate="A" pin="PGATE" pad="6"/>
<connect gate="A" pin="RT" pad="2"/>
<connect gate="A" pin="VCC" pad="7"/>
<connect gate="A" pin="VIN" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM5085SD"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="04R9278"/>
<attribute name="PACKAGE" value="DFN-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM5088MH-1">
<description>Wide Input Range Non-Synchronous Buck Controller</description>
<gates>
<gate name="A" symbol="LM5088MH-1"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-17N">
<connects>
<connect gate="A" pin="BOOT" pad="15"/>
<connect gate="A" pin="COMP" pad="7"/>
<connect gate="A" pin="CS" pad="12"/>
<connect gate="A" pin="CSG" pad="11"/>
<connect gate="A" pin="DITH" pad="10"/>
<connect gate="A" pin="EN" pad="2"/>
<connect gate="A" pin="EPAD" pad="17"/>
<connect gate="A" pin="FB" pad="8"/>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="HG" pad="14"/>
<connect gate="A" pin="OUT" pad="9"/>
<connect gate="A" pin="RAMP" pad="4"/>
<connect gate="A" pin="RT" pad="5"/>
<connect gate="A" pin="SS" pad="3"/>
<connect gate="A" pin="SW" pad="13"/>
<connect gate="A" pin="VCC" pad="16"/>
<connect gate="A" pin="VIN" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM5088MH-1"/>
<attribute name="OC_FARNELL" value="1696599"/>
<attribute name="OC_NEWARK" value="56P4155"/>
<attribute name="PACKAGE" value="TSSOP-16"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM5088MH-2">
<description>Wide Input Range Non-Synchronous Buck Controller</description>
<gates>
<gate name="A" symbol="LM5088MH-2"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-17N">
<connects>
<connect gate="A" pin="BOOT" pad="15"/>
<connect gate="A" pin="COMP" pad="7"/>
<connect gate="A" pin="CS" pad="12"/>
<connect gate="A" pin="CSG" pad="11"/>
<connect gate="A" pin="DITH" pad="10"/>
<connect gate="A" pin="EN" pad="2"/>
<connect gate="A" pin="EPAD" pad="17"/>
<connect gate="A" pin="FB" pad="8"/>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="HG" pad="14"/>
<connect gate="A" pin="OUT" pad="9"/>
<connect gate="A" pin="RAMP" pad="4"/>
<connect gate="A" pin="RT" pad="5"/>
<connect gate="A" pin="SS" pad="3"/>
<connect gate="A" pin="SW" pad="13"/>
<connect gate="A" pin="VCC" pad="16"/>
<connect gate="A" pin="VIN" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM5088MH-2"/>
<attribute name="OC_FARNELL" value="1696599"/>
<attribute name="OC_NEWARK" value="56P4156"/>
<attribute name="PACKAGE" value="TSSOP-16"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM50BIM3" prefix="U">
<description>Single-Supply Centigrade Temperature Sensor</description>
<gates>
<gate name="A" symbol="LM50BIM3"/>
</gates>
<devices>
<device name="" package="SOT95P260X110-3N">
<connects>
<connect gate="A" pin="+VS" pad="1"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="VO" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM50BIM3"/>
<attribute name="OC_FARNELL" value="9779884"/>
<attribute name="OC_NEWARK" value="92F314"/>
<attribute name="PACKAGE" value="SOT23-3"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM50CIM3" prefix="U">
<description>Single-Supply Centigrade Temperature Sensor</description>
<gates>
<gate name="A" symbol="LM50CIM3"/>
</gates>
<devices>
<device name="" package="SOT95P260X110-3N">
<connects>
<connect gate="A" pin="+VS" pad="1"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="VO" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM50CIM3"/>
<attribute name="OC_FARNELL" value="9779620"/>
<attribute name="OC_NEWARK" value="92F315"/>
<attribute name="PACKAGE" value="SOT23-3"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM5100AM" prefix="U">
<description>Gate Driver</description>
<gates>
<gate name="A" symbol="LM5100AM"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="HB" pad="2"/>
<connect gate="A" pin="HI" pad="5"/>
<connect gate="A" pin="HO" pad="3"/>
<connect gate="A" pin="HS" pad="4"/>
<connect gate="A" pin="LI" pad="6"/>
<connect gate="A" pin="LO" pad="8"/>
<connect gate="A" pin="VDD" pad="1"/>
<connect gate="A" pin="VSS" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM5100AM"/>
<attribute name="OC_FARNELL" value="1008264"/>
<attribute name="OC_NEWARK" value="41K6088"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM5101AM" prefix="U">
<description>Gate Driver</description>
<gates>
<gate name="A" symbol="LM5101AM"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="HB" pad="2"/>
<connect gate="A" pin="HI" pad="5"/>
<connect gate="A" pin="HO" pad="3"/>
<connect gate="A" pin="HS" pad="4"/>
<connect gate="A" pin="LI" pad="6"/>
<connect gate="A" pin="LO" pad="8"/>
<connect gate="A" pin="VDD" pad="1"/>
<connect gate="A" pin="VSS" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM5101AM"/>
<attribute name="OC_FARNELL" value="1008266"/>
<attribute name="OC_NEWARK" value="41K6096"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM5101ASD" prefix="U">
<description>High Voltage High-Side and Low-Side Gate Drivers</description>
<gates>
<gate name="A" symbol="LM5101ASD"/>
</gates>
<devices>
<device name="" package="DFN400X400X80-11N">
<connects>
<connect gate="A" pin="EPAD" pad="11"/>
<connect gate="A" pin="HB" pad="2"/>
<connect gate="A" pin="HI" pad="7"/>
<connect gate="A" pin="HO" pad="3"/>
<connect gate="A" pin="HS" pad="4"/>
<connect gate="A" pin="LI" pad="8"/>
<connect gate="A" pin="LO" pad="10"/>
<connect gate="A" pin="NC" pad="6"/>
<connect gate="A" pin="NC_2" pad="5"/>
<connect gate="A" pin="VDD" pad="1"/>
<connect gate="A" pin="VSS" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM5101ASD"/>
<attribute name="OC_FARNELL" value="1008267"/>
<attribute name="OC_NEWARK" value="41K6098"/>
<attribute name="PACKAGE" value="DFN-10"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM5101BMA" prefix="U">
<description>Gate Drivers</description>
<gates>
<gate name="A" symbol="LM5101BMA"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="HB" pad="2"/>
<connect gate="A" pin="HI" pad="5"/>
<connect gate="A" pin="HO" pad="3"/>
<connect gate="A" pin="HS" pad="4"/>
<connect gate="A" pin="LI" pad="6"/>
<connect gate="A" pin="LO" pad="8"/>
<connect gate="A" pin="VDD" pad="1"/>
<connect gate="A" pin="VSS" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM5101BMA"/>
<attribute name="OC_FARNELL" value="1290945"/>
<attribute name="OC_NEWARK" value="32M1238"/>
<attribute name="PACKAGE" value="8-SOIC"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM5101CMA" prefix="U">
<description>Gate Drivers</description>
<gates>
<gate name="A" symbol="LM5101CMA"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="HB" pad="2"/>
<connect gate="A" pin="HI" pad="5"/>
<connect gate="A" pin="HO" pad="3"/>
<connect gate="A" pin="HS" pad="4"/>
<connect gate="A" pin="LI" pad="6"/>
<connect gate="A" pin="LO" pad="8"/>
<connect gate="A" pin="VDD" pad="1"/>
<connect gate="A" pin="VSS" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM5101CMA"/>
<attribute name="OC_FARNELL" value="1290946"/>
<attribute name="OC_NEWARK" value="24M3539"/>
<attribute name="PACKAGE" value="8-SOIC"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM5102SD" prefix="U">
<description>Half Bridge gate driver</description>
<gates>
<gate name="A" symbol="LM5102SD"/>
</gates>
<devices>
<device name="" package="DFN400X400X80-11N">
<connects>
<connect gate="A" pin="EP" pad="11"/>
<connect gate="A" pin="HB" pad="2"/>
<connect gate="A" pin="HI" pad="7"/>
<connect gate="A" pin="HO" pad="3"/>
<connect gate="A" pin="HS" pad="4"/>
<connect gate="A" pin="LI" pad="8"/>
<connect gate="A" pin="LO" pad="10"/>
<connect gate="A" pin="RT1" pad="5"/>
<connect gate="A" pin="RT2" pad="6"/>
<connect gate="A" pin="VDD" pad="1"/>
<connect gate="A" pin="VSS" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM5102SD"/>
<attribute name="OC_FARNELL" value="1798333"/>
<attribute name="OC_NEWARK" value="73R9749"/>
<attribute name="PACKAGE" value="LLP-10"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM5104M" prefix="U">
<description>Half Bridge gate driver</description>
<gates>
<gate name="A" symbol="LM5104M"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="HB" pad="2"/>
<connect gate="A" pin="HO" pad="3"/>
<connect gate="A" pin="HS" pad="4"/>
<connect gate="A" pin="LI" pad="6"/>
<connect gate="A" pin="LO" pad="8"/>
<connect gate="A" pin="RT" pad="5"/>
<connect gate="A" pin="VDD" pad="1"/>
<connect gate="A" pin="VSS" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM5104M"/>
<attribute name="OC_FARNELL" value="8181390"/>
<attribute name="OC_NEWARK" value="41K6108"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM5105SD" prefix="U">
<description>Half Bridge gate driver</description>
<gates>
<gate name="A" symbol="LM5105SD"/>
</gates>
<devices>
<device name="" package="DFN400X400X80-11N">
<connects>
<connect gate="A" pin="EN" pad="7"/>
<connect gate="A" pin="EP" pad="11"/>
<connect gate="A" pin="HB" pad="2"/>
<connect gate="A" pin="HO" pad="3"/>
<connect gate="A" pin="HS" pad="4"/>
<connect gate="A" pin="IN" pad="8"/>
<connect gate="A" pin="LO" pad="10"/>
<connect gate="A" pin="NC" pad="5"/>
<connect gate="A" pin="RDT" pad="6"/>
<connect gate="A" pin="VDD" pad="1"/>
<connect gate="A" pin="VSS" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM5105SD"/>
<attribute name="OC_FARNELL" value="1008268"/>
<attribute name="OC_NEWARK" value="41K6112"/>
<attribute name="PACKAGE" value="LLP-10"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM5106MM" prefix="U">
<description>Half Bridge Gate Driver</description>
<gates>
<gate name="A" symbol="LM5106MM"/>
</gates>
<devices>
<device name="" package="SOP50P490X110-10N">
<connects>
<connect gate="A" pin="EN" pad="7"/>
<connect gate="A" pin="HB" pad="2"/>
<connect gate="A" pin="HO" pad="3"/>
<connect gate="A" pin="HS" pad="4"/>
<connect gate="A" pin="IN" pad="8"/>
<connect gate="A" pin="LO" pad="10"/>
<connect gate="A" pin="NC" pad="5"/>
<connect gate="A" pin="RDT" pad="6"/>
<connect gate="A" pin="VDD" pad="1"/>
<connect gate="A" pin="VSS" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM5106MM"/>
<attribute name="OC_FARNELL" value="1312793"/>
<attribute name="OC_NEWARK" value="31M5478"/>
<attribute name="PACKAGE" value="MSOP-10"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM5107MA" prefix="U">
<description>Peak Half Bridge Gate Driver</description>
<gates>
<gate name="A" symbol="LM5107MA"/>
</gates>
<devices>
<device name="" package="SOIC127P620X175-8N">
<connects>
<connect gate="A" pin="HB" pad="8"/>
<connect gate="A" pin="HI" pad="2"/>
<connect gate="A" pin="HO" pad="7"/>
<connect gate="A" pin="HS" pad="6"/>
<connect gate="A" pin="LI" pad="3"/>
<connect gate="A" pin="LO" pad="5"/>
<connect gate="A" pin="VDD" pad="1"/>
<connect gate="A" pin="VSS" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM5107MA"/>
<attribute name="OC_FARNELL" value="1008269"/>
<attribute name="OC_NEWARK" value="41K6114"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM5109BMA" prefix="U">
<description>High Voltage 1A Peak Half Bridge Gate Driver</description>
<gates>
<gate name="A" symbol="LM5109BMA"/>
</gates>
<devices>
<device name="" package="SOIC127P620X175-8N">
<connects>
<connect gate="A" pin="HB" pad="8"/>
<connect gate="A" pin="HI" pad="2"/>
<connect gate="A" pin="HO" pad="7"/>
<connect gate="A" pin="HS" pad="6"/>
<connect gate="A" pin="LI" pad="3"/>
<connect gate="A" pin="LO" pad="5"/>
<connect gate="A" pin="VDD" pad="1"/>
<connect gate="A" pin="VSS" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM5109BMA"/>
<attribute name="OC_FARNELL" value="1333960"/>
<attribute name="OC_NEWARK" value="32M1247"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM5110-1M" prefix="U">
<description>Compound Gate Driver</description>
<gates>
<gate name="A" symbol="LM5110-1M"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="IN_A" pad="2"/>
<connect gate="A" pin="IN_B" pad="4"/>
<connect gate="A" pin="IN_REF" pad="1"/>
<connect gate="A" pin="OUT_A" pad="7"/>
<connect gate="A" pin="OUT_B" pad="5"/>
<connect gate="A" pin="VCC" pad="6"/>
<connect gate="A" pin="VEE" pad="3"/>
<connect gate="A" pin="~SHDN" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM5110-1M"/>
<attribute name="OC_FARNELL" value="8181403"/>
<attribute name="OC_NEWARK" value="41K6122"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM5110-2M" prefix="U">
<description>Compound Gate Driver</description>
<gates>
<gate name="A" symbol="LM5110-2M"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="IN_A" pad="2"/>
<connect gate="A" pin="IN_B" pad="4"/>
<connect gate="A" pin="IN_REF" pad="1"/>
<connect gate="A" pin="OUT_A" pad="7"/>
<connect gate="A" pin="OUT_B" pad="5"/>
<connect gate="A" pin="VCC" pad="6"/>
<connect gate="A" pin="VEE" pad="3"/>
<connect gate="A" pin="~SHDN" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM5110-2M"/>
<attribute name="OC_FARNELL" value="8181411"/>
<attribute name="OC_NEWARK" value="41K6126"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM5111-1M" prefix="U">
<description>Dual 5A Compound Gate Driver</description>
<gates>
<gate name="A" symbol="LM5111-1M"/>
</gates>
<devices>
<device name="" package="SOIC127P620X175-8N">
<connects>
<connect gate="A" pin="IN_A" pad="2"/>
<connect gate="A" pin="IN_B" pad="4"/>
<connect gate="A" pin="NC" pad="8"/>
<connect gate="A" pin="NC_2" pad="1"/>
<connect gate="A" pin="OUT_A" pad="7"/>
<connect gate="A" pin="OUT_B" pad="5"/>
<connect gate="A" pin="VCC" pad="6"/>
<connect gate="A" pin="VEE" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM5111-1M"/>
<attribute name="OC_FARNELL" value="8238693"/>
<attribute name="OC_NEWARK" value="41K6134"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM5111-1MY" prefix="U">
<description>MOSFET DRIVER</description>
<gates>
<gate name="A" symbol="LM5111-1MY"/>
</gates>
<devices>
<device name="" package="SOP65P490X110-9N">
<connects>
<connect gate="A" pin="EP" pad="9"/>
<connect gate="A" pin="IN_A" pad="2"/>
<connect gate="A" pin="IN_B" pad="4"/>
<connect gate="A" pin="NC" pad="8"/>
<connect gate="A" pin="NC_2" pad="1"/>
<connect gate="A" pin="OUT_A" pad="7"/>
<connect gate="A" pin="OUT_B" pad="5"/>
<connect gate="A" pin="VCC" pad="6"/>
<connect gate="A" pin="VEE" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM5111-1MY"/>
<attribute name="OC_FARNELL" value="1312593"/>
<attribute name="OC_NEWARK" value="32M1250"/>
<attribute name="PACKAGE" value="MSOP-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM5111-2MY" prefix="U">
<description>MOSFET DRIVER</description>
<gates>
<gate name="A" symbol="LM5111-2MY"/>
</gates>
<devices>
<device name="" package="SOP65P490X110-9N">
<connects>
<connect gate="A" pin="EP" pad="9"/>
<connect gate="A" pin="IN_A" pad="2"/>
<connect gate="A" pin="IN_B" pad="4"/>
<connect gate="A" pin="NC" pad="8"/>
<connect gate="A" pin="NC_2" pad="1"/>
<connect gate="A" pin="OUT_A" pad="7"/>
<connect gate="A" pin="OUT_B" pad="5"/>
<connect gate="A" pin="VCC" pad="6"/>
<connect gate="A" pin="VEE" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM5111-2MY"/>
<attribute name="OC_FARNELL" value="1312594"/>
<attribute name="OC_NEWARK" value="99K2528"/>
<attribute name="PACKAGE" value="MSOP-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM5111-4M" prefix="U">
<description>Gate Driver</description>
<gates>
<gate name="A" symbol="LM5111-4M"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="INA" pad="2"/>
<connect gate="A" pin="INB" pad="4"/>
<connect gate="A" pin="NC" pad="8"/>
<connect gate="A" pin="NC_2" pad="1"/>
<connect gate="A" pin="OUTA" pad="7"/>
<connect gate="A" pin="OUTB" pad="5"/>
<connect gate="A" pin="VCC" pad="6"/>
<connect gate="A" pin="VEE" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM5111-4M"/>
<attribute name="OC_FARNELL" value="1535358"/>
<attribute name="OC_NEWARK" value="64M7042"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM5112MY" prefix="U">
<description>Tiny 7A MOSFET Gate Driver</description>
<gates>
<gate name="A" symbol="LM5112MY"/>
</gates>
<devices>
<device name="" package="MUC10A">
<connects>
<connect gate="A" pin="EPAD" pad="9"/>
<connect gate="A" pin="IN" pad="4"/>
<connect gate="A" pin="IN_B" pad="2"/>
<connect gate="A" pin="IN_REF" pad="1"/>
<connect gate="A" pin="NC" pad="8"/>
<connect gate="A" pin="NC_2" pad="5"/>
<connect gate="A" pin="OUT" pad="7"/>
<connect gate="A" pin="VCC" pad="6"/>
<connect gate="A" pin="VEE" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM5112MY"/>
<attribute name="OC_FARNELL" value="1312597"/>
<attribute name="OC_NEWARK" value="32M1256"/>
<attribute name="PACKAGE" value="MSOP-8"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM5115MTC" prefix="U">
<description>Synchronous Buck Controller</description>
<gates>
<gate name="A" symbol="LM5115MTC"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-16N">
<connects>
<connect gate="A" pin="AGND" pad="3"/>
<connect gate="A" pin="CO" pad="4"/>
<connect gate="A" pin="COMP" pad="5"/>
<connect gate="A" pin="CS" pad="1"/>
<connect gate="A" pin="FB" pad="6"/>
<connect gate="A" pin="HB" pad="15"/>
<connect gate="A" pin="HO" pad="14"/>
<connect gate="A" pin="HS" pad="13"/>
<connect gate="A" pin="LO" pad="11"/>
<connect gate="A" pin="PGND" pad="10"/>
<connect gate="A" pin="RAMP" pad="8"/>
<connect gate="A" pin="SS" pad="7"/>
<connect gate="A" pin="SYNC" pad="9"/>
<connect gate="A" pin="VBIAS" pad="16"/>
<connect gate="A" pin="VCC" pad="12"/>
<connect gate="A" pin="VOUT" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM5115MTC"/>
<attribute name="OC_FARNELL" value="1008034"/>
<attribute name="OC_NEWARK" value="41K6142"/>
<attribute name="PACKAGE" value="SOP-16"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM5115SD" prefix="U">
<description>Secondary Side Post Regulator</description>
<gates>
<gate name="A" symbol="LM5115SD"/>
</gates>
<devices>
<device name="" package="DFN500X500X80-17N">
<connects>
<connect gate="A" pin="AGND" pad="3"/>
<connect gate="A" pin="CO" pad="4"/>
<connect gate="A" pin="COMP" pad="5"/>
<connect gate="A" pin="CS" pad="1"/>
<connect gate="A" pin="EPAD" pad="17"/>
<connect gate="A" pin="FB" pad="6"/>
<connect gate="A" pin="HB" pad="15"/>
<connect gate="A" pin="HO" pad="14"/>
<connect gate="A" pin="HS" pad="13"/>
<connect gate="A" pin="LO" pad="11"/>
<connect gate="A" pin="PGND" pad="10"/>
<connect gate="A" pin="RAMP" pad="8"/>
<connect gate="A" pin="SS" pad="7"/>
<connect gate="A" pin="SYNC" pad="9"/>
<connect gate="A" pin="VBIAS" pad="16"/>
<connect gate="A" pin="VCC" pad="12"/>
<connect gate="A" pin="VOUT" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM5115SD"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="99K2534"/>
<attribute name="PACKAGE" value="DFN-16"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM5118MH" prefix="U">
<description>Buck-Boost Controller</description>
<gates>
<gate name="A" symbol="LM5118MH"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-21N">
<connects>
<connect gate="A" pin="AGND" pad="6"/>
<connect gate="A" pin="COMP" pad="9"/>
<connect gate="A" pin="CS" pad="12"/>
<connect gate="A" pin="CSG" pad="13"/>
<connect gate="A" pin="EN" pad="4"/>
<connect gate="A" pin="FB" pad="8"/>
<connect gate="A" pin="HB" pad="18"/>
<connect gate="A" pin="HO" pad="19"/>
<connect gate="A" pin="HS" pad="20"/>
<connect gate="A" pin="LO" pad="15"/>
<connect gate="A" pin="PGND" pad="14"/>
<connect gate="A" pin="RAMP" pad="5"/>
<connect gate="A" pin="RT" pad="3"/>
<connect gate="A" pin="SS" pad="7"/>
<connect gate="A" pin="SYNC" pad="11"/>
<connect gate="A" pin="UVLO" pad="2"/>
<connect gate="A" pin="VCC" pad="16"/>
<connect gate="A" pin="VCCX" pad="17"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="VOUT" pad="10"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM5118MH"/>
<attribute name="OC_FARNELL" value="1609187"/>
<attribute name="OC_NEWARK" value="08N3587"/>
<attribute name="PACKAGE" value="TSSOP-20"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM5118Q1MH" prefix="U">
<description>Wide Voltage Range Buck-Boost Controller</description>
<gates>
<gate name="A" symbol="LM5118Q1MH"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-21N">
<connects>
<connect gate="A" pin="AGND" pad="6"/>
<connect gate="A" pin="COMP" pad="9"/>
<connect gate="A" pin="CS" pad="12"/>
<connect gate="A" pin="CSG" pad="13"/>
<connect gate="A" pin="EN" pad="4"/>
<connect gate="A" pin="EPAD" pad="21"/>
<connect gate="A" pin="FB" pad="8"/>
<connect gate="A" pin="HB" pad="18"/>
<connect gate="A" pin="HO" pad="19"/>
<connect gate="A" pin="HS" pad="20"/>
<connect gate="A" pin="LO" pad="15"/>
<connect gate="A" pin="PGND" pad="14"/>
<connect gate="A" pin="RAMP" pad="5"/>
<connect gate="A" pin="RT" pad="3"/>
<connect gate="A" pin="SS" pad="7"/>
<connect gate="A" pin="SYNC" pad="11"/>
<connect gate="A" pin="UVLO" pad="2"/>
<connect gate="A" pin="VCC" pad="16"/>
<connect gate="A" pin="VCCX" pad="17"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="VOUT" pad="10"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM5118Q1MH"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="55R4118"/>
<attribute name="PACKAGE" value="TSSOP-20"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM5574MT" prefix="U">
<description>Step-Down Switching Regulator</description>
<gates>
<gate name="A" symbol="LM5574MT"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-16N">
<connects>
<connect gate="A" pin="AGND" pad="9"/>
<connect gate="A" pin="BST" pad="16"/>
<connect gate="A" pin="COMP" pad="5"/>
<connect gate="A" pin="FB" pad="6"/>
<connect gate="A" pin="IS" pad="13"/>
<connect gate="A" pin="OUT" pad="11"/>
<connect gate="A" pin="PGND" pad="12"/>
<connect gate="A" pin="PRE" pad="15"/>
<connect gate="A" pin="RAMP" pad="8"/>
<connect gate="A" pin="RT" pad="7"/>
<connect gate="A" pin="SD" pad="2"/>
<connect gate="A" pin="SS" pad="10"/>
<connect gate="A" pin="SW" pad="14"/>
<connect gate="A" pin="SYNC" pad="4"/>
<connect gate="A" pin="VCC" pad="1"/>
<connect gate="A" pin="VIN" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM5574MT"/>
<attribute name="OC_FARNELL" value="1325419"/>
<attribute name="OC_NEWARK" value="32M1267"/>
<attribute name="PACKAGE" value="TSSOP-16"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM5574QMT" prefix="U">
<description>SIMPLE SWITCHER</description>
<gates>
<gate name="A" symbol="LM5574QMT"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-16N">
<connects>
<connect gate="A" pin="AGND" pad="9"/>
<connect gate="A" pin="BST" pad="16"/>
<connect gate="A" pin="COMP" pad="5"/>
<connect gate="A" pin="FB" pad="6"/>
<connect gate="A" pin="IS" pad="13"/>
<connect gate="A" pin="OUT" pad="11"/>
<connect gate="A" pin="PGND" pad="12"/>
<connect gate="A" pin="PRE" pad="15"/>
<connect gate="A" pin="RAMP" pad="8"/>
<connect gate="A" pin="RT" pad="7"/>
<connect gate="A" pin="SD" pad="2"/>
<connect gate="A" pin="SS" pad="10"/>
<connect gate="A" pin="SW" pad="14"/>
<connect gate="A" pin="SYNC" pad="4"/>
<connect gate="A" pin="VCC" pad="1"/>
<connect gate="A" pin="VIN" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM5574QMT"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="55R4120"/>
<attribute name="PACKAGE" value="TSSOP-16"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM5575MH" prefix="U">
<description>Step-Down Switching Regulator</description>
<gates>
<gate name="A" symbol="LM5575MH"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-17N">
<connects>
<connect gate="A" pin="AGND" pad="9"/>
<connect gate="A" pin="BST" pad="16"/>
<connect gate="A" pin="COMP" pad="5"/>
<connect gate="A" pin="EPAD" pad="17"/>
<connect gate="A" pin="FB" pad="6"/>
<connect gate="A" pin="IS" pad="13"/>
<connect gate="A" pin="OUT" pad="11"/>
<connect gate="A" pin="PGND" pad="12"/>
<connect gate="A" pin="PRE" pad="15"/>
<connect gate="A" pin="RAMP" pad="8"/>
<connect gate="A" pin="RT" pad="7"/>
<connect gate="A" pin="SD" pad="2"/>
<connect gate="A" pin="SS" pad="10"/>
<connect gate="A" pin="SW" pad="14"/>
<connect gate="A" pin="SYNC" pad="4"/>
<connect gate="A" pin="VCC" pad="1"/>
<connect gate="A" pin="VIN" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM5575MH"/>
<attribute name="OC_FARNELL" value="1325420"/>
<attribute name="OC_NEWARK" value="32M1271"/>
<attribute name="PACKAGE" value="TSSOP-16"/>
<attribute name="SUPPLIER" value="National"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM5575QMH" prefix="U">
<description>SIMPLE SWITCHER</description>
<gates>
<gate name="A" symbol="LM5575QMH"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-17N">
<connects>
<connect gate="A" pin="AGND" pad="9"/>
<connect gate="A" pin="BST" pad="16"/>
<connect gate="A" pin="COMP" pad="5"/>
<connect gate="A" pin="EP" pad="17"/>
<connect gate="A" pin="FB" pad="6"/>
<connect gate="A" pin="IS" pad="13"/>
<connect gate="A" pin="OUT" pad="11"/>
<connect gate="A" pin="PGND" pad="12"/>
<connect gate="A" pin="PRE" pad="15"/>
<connect gate="A" pin="RAMP" pad="8"/>
<connect gate="A" pin="RT" pad="7"/>
<connect gate="A" pin="SD" pad="2"/>
<connect gate="A" pin="SS" pad="10"/>
<connect gate="A" pin="SW" pad="14"/>
<connect gate="A" pin="SYNC" pad="4"/>
<connect gate="A" pin="VCC" pad="1"/>
<connect gate="A" pin="VIN" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM5575QMH"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="55R4123"/>
<attribute name="PACKAGE" value="TSSOP-16"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM5576MH" prefix="U">
<description>Step-Down Switching Regulator</description>
<gates>
<gate name="A" symbol="LM5576MH"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-21N">
<connects>
<connect gate="A" pin="AGND" pad="10"/>
<connect gate="A" pin="BST" pad="20"/>
<connect gate="A" pin="COMP" pad="6"/>
<connect gate="A" pin="EP" pad="21"/>
<connect gate="A" pin="FB" pad="7"/>
<connect gate="A" pin="IS" pad="16"/>
<connect gate="A" pin="IS_2" pad="15"/>
<connect gate="A" pin="OUT" pad="12"/>
<connect gate="A" pin="PGND" pad="14"/>
<connect gate="A" pin="PGND_2" pad="13"/>
<connect gate="A" pin="PRE" pad="19"/>
<connect gate="A" pin="RAMP" pad="9"/>
<connect gate="A" pin="RT" pad="8"/>
<connect gate="A" pin="SD" pad="2"/>
<connect gate="A" pin="SS" pad="11"/>
<connect gate="A" pin="SW" pad="18"/>
<connect gate="A" pin="SW_2" pad="17"/>
<connect gate="A" pin="SYNC" pad="5"/>
<connect gate="A" pin="VCC" pad="1"/>
<connect gate="A" pin="VIN" pad="4"/>
<connect gate="A" pin="VIN_2" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM5576MH"/>
<attribute name="OC_FARNELL" value="1325422"/>
<attribute name="OC_NEWARK" value="32M1276"/>
<attribute name="PACKAGE" value="TSSOP-20"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM5576QMH" prefix="U">
<description>SIMPLE SWITCHER</description>
<gates>
<gate name="A" symbol="LM5576QMH"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-21N">
<connects>
<connect gate="A" pin="AGND" pad="10"/>
<connect gate="A" pin="BST" pad="20"/>
<connect gate="A" pin="COMP" pad="6"/>
<connect gate="A" pin="EPAD" pad="21"/>
<connect gate="A" pin="FB" pad="7"/>
<connect gate="A" pin="IS" pad="16"/>
<connect gate="A" pin="IS_2" pad="15"/>
<connect gate="A" pin="OUT" pad="12"/>
<connect gate="A" pin="PGND" pad="13"/>
<connect gate="A" pin="PGND_2" pad="14"/>
<connect gate="A" pin="PRE" pad="19"/>
<connect gate="A" pin="RAMP" pad="9"/>
<connect gate="A" pin="RT" pad="8"/>
<connect gate="A" pin="SD" pad="2"/>
<connect gate="A" pin="SS" pad="11"/>
<connect gate="A" pin="SW" pad="18"/>
<connect gate="A" pin="SW_2" pad="17"/>
<connect gate="A" pin="SYNC" pad="5"/>
<connect gate="A" pin="VCC" pad="1"/>
<connect gate="A" pin="VIN" pad="4"/>
<connect gate="A" pin="VIN_2" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM5576QMH"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="55R4125"/>
<attribute name="PACKAGE" value="TSSOP-21"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM5642MH" prefix="U">
<description>Dual Synchronous Buck Converter</description>
<gates>
<gate name="A" symbol="LM5642MH"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-29N">
<connects>
<connect gate="A" pin="CBOOT1" pad="25"/>
<connect gate="A" pin="CBOOT2" pad="18"/>
<connect gate="A" pin="COMP1" pad="3"/>
<connect gate="A" pin="COMP2" pad="12"/>
<connect gate="A" pin="EPAD" pad="29"/>
<connect gate="A" pin="FB1" pad="4"/>
<connect gate="A" pin="FB2" pad="11"/>
<connect gate="A" pin="HDRV1" pad="26"/>
<connect gate="A" pin="HDRV2" pad="17"/>
<connect gate="A" pin="ILIM1" pad="2"/>
<connect gate="A" pin="ILIM2" pad="13"/>
<connect gate="A" pin="KS1" pad="1"/>
<connect gate="A" pin="KS2" pad="14"/>
<connect gate="A" pin="LDRV1" pad="23"/>
<connect gate="A" pin="LDRV2" pad="20"/>
<connect gate="A" pin="ON/SS1" pad="9"/>
<connect gate="A" pin="ON/SS2" pad="10"/>
<connect gate="A" pin="PGND" pad="21"/>
<connect gate="A" pin="RSNS1" pad="28"/>
<connect gate="A" pin="RSNS2" pad="15"/>
<connect gate="A" pin="SGND" pad="8"/>
<connect gate="A" pin="SW1" pad="27"/>
<connect gate="A" pin="SW2" pad="16"/>
<connect gate="A" pin="SYNC" pad="5"/>
<connect gate="A" pin="UVDELAY" pad="6"/>
<connect gate="A" pin="VDD1" pad="24"/>
<connect gate="A" pin="VDD2" pad="19"/>
<connect gate="A" pin="VIN" pad="22"/>
<connect gate="A" pin="VLIN5" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM5642MH"/>
<attribute name="OC_FARNELL" value="1685535"/>
<attribute name="OC_NEWARK" value="50M8806"/>
<attribute name="PACKAGE" value="TSSOP-28"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM5642MTC" prefix="U">
<description>Dual Synchronous Buck Converter</description>
<gates>
<gate name="A" symbol="LM5642MTC"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-28N">
<connects>
<connect gate="A" pin="CBOOT1" pad="25"/>
<connect gate="A" pin="CBOOT2" pad="18"/>
<connect gate="A" pin="COMP1" pad="3"/>
<connect gate="A" pin="COMP2" pad="12"/>
<connect gate="A" pin="FB1" pad="4"/>
<connect gate="A" pin="FB2" pad="11"/>
<connect gate="A" pin="HDRV1" pad="26"/>
<connect gate="A" pin="HDRV2" pad="17"/>
<connect gate="A" pin="ILIM1" pad="2"/>
<connect gate="A" pin="ILIM2" pad="13"/>
<connect gate="A" pin="KS1" pad="1"/>
<connect gate="A" pin="KS2" pad="14"/>
<connect gate="A" pin="LDRV1" pad="23"/>
<connect gate="A" pin="LDRV2" pad="20"/>
<connect gate="A" pin="ON/SS1" pad="9"/>
<connect gate="A" pin="ON/SS2" pad="10"/>
<connect gate="A" pin="PGND" pad="21"/>
<connect gate="A" pin="RSENS2" pad="15"/>
<connect gate="A" pin="RSNS1" pad="28"/>
<connect gate="A" pin="SGND" pad="8"/>
<connect gate="A" pin="SW1" pad="27"/>
<connect gate="A" pin="SW2" pad="16"/>
<connect gate="A" pin="SYNC" pad="5"/>
<connect gate="A" pin="UVDELAY" pad="6"/>
<connect gate="A" pin="VDD1" pad="24"/>
<connect gate="A" pin="VDD2" pad="19"/>
<connect gate="A" pin="VIN" pad="22"/>
<connect gate="A" pin="VLIN5" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM5642MTC"/>
<attribute name="OC_FARNELL" value="8181772"/>
<attribute name="OC_NEWARK" value="82H4139"/>
<attribute name="PACKAGE" value="SOP-28"/>
<attribute name="SUPPLIER" value="NSC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM5642XMH" prefix="U">
<description>High Voltage, Dual Synchronous Buck Converter</description>
<gates>
<gate name="A" symbol="LM5642XMH"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-29N">
<connects>
<connect gate="A" pin="CBOOT1" pad="25"/>
<connect gate="A" pin="CBOOT2" pad="18"/>
<connect gate="A" pin="COMP1" pad="3"/>
<connect gate="A" pin="COMP2" pad="12"/>
<connect gate="A" pin="EPAD" pad="29"/>
<connect gate="A" pin="FB1" pad="4"/>
<connect gate="A" pin="FB2" pad="11"/>
<connect gate="A" pin="HDRV1" pad="26"/>
<connect gate="A" pin="HDRV2" pad="17"/>
<connect gate="A" pin="ILIM1" pad="2"/>
<connect gate="A" pin="ILIM2" pad="13"/>
<connect gate="A" pin="KS1" pad="1"/>
<connect gate="A" pin="KS2" pad="14"/>
<connect gate="A" pin="LDRV1" pad="23"/>
<connect gate="A" pin="LDRV2" pad="20"/>
<connect gate="A" pin="ON/SS1" pad="9"/>
<connect gate="A" pin="ON/SS2" pad="10"/>
<connect gate="A" pin="PGND" pad="21"/>
<connect gate="A" pin="RSNS1" pad="28"/>
<connect gate="A" pin="RSNS2" pad="15"/>
<connect gate="A" pin="SGND" pad="8"/>
<connect gate="A" pin="SW1" pad="27"/>
<connect gate="A" pin="SW2" pad="16"/>
<connect gate="A" pin="SYNC" pad="5"/>
<connect gate="A" pin="UVDELAY" pad="6"/>
<connect gate="A" pin="VDD1" pad="24"/>
<connect gate="A" pin="VDD2" pad="19"/>
<connect gate="A" pin="VIN" pad="22"/>
<connect gate="A" pin="VLIN5" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM5642XMH"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="33M8357"/>
<attribute name="PACKAGE" value="TSSOP-28"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM5642XMT" prefix="U">
<description>Dual Synchronous Buck Converter</description>
<gates>
<gate name="A" symbol="LM5642XMT"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-28N">
<connects>
<connect gate="A" pin="CBOOT1" pad="25"/>
<connect gate="A" pin="CBOOT2" pad="18"/>
<connect gate="A" pin="COMP1" pad="3"/>
<connect gate="A" pin="COMP2" pad="12"/>
<connect gate="A" pin="FB1" pad="4"/>
<connect gate="A" pin="FB2" pad="11"/>
<connect gate="A" pin="HDRV1" pad="26"/>
<connect gate="A" pin="HDRV2" pad="17"/>
<connect gate="A" pin="ILIM1" pad="2"/>
<connect gate="A" pin="ILIM2" pad="13"/>
<connect gate="A" pin="KS1" pad="1"/>
<connect gate="A" pin="KS2" pad="14"/>
<connect gate="A" pin="LDRV1" pad="23"/>
<connect gate="A" pin="LDRV2" pad="20"/>
<connect gate="A" pin="ON/SS1" pad="9"/>
<connect gate="A" pin="ON/SS2" pad="10"/>
<connect gate="A" pin="PGND" pad="21"/>
<connect gate="A" pin="RSNS1" pad="28"/>
<connect gate="A" pin="RSNS2" pad="15"/>
<connect gate="A" pin="SGND" pad="8"/>
<connect gate="A" pin="SW1" pad="27"/>
<connect gate="A" pin="SW2" pad="16"/>
<connect gate="A" pin="SYNC" pad="5"/>
<connect gate="A" pin="UVDELAY" pad="6"/>
<connect gate="A" pin="VDD1" pad="24"/>
<connect gate="A" pin="VDD2" pad="19"/>
<connect gate="A" pin="VIN" pad="22"/>
<connect gate="A" pin="VLIN5" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM5642XMT"/>
<attribute name="OC_FARNELL" value="1495083"/>
<attribute name="OC_NEWARK" value="79K7955"/>
<attribute name="PACKAGE" value="TSSOP-28"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM56BIM" prefix="U">
<description>Low Power thermostat</description>
<gates>
<gate name="A" symbol="LM56BIM"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="OUT1" pad="7"/>
<connect gate="A" pin="OUT2" pad="6"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="VREF" pad="1"/>
<connect gate="A" pin="VT1" pad="3"/>
<connect gate="A" pin="VT2" pad="2"/>
<connect gate="A" pin="VTEMP" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM56BIM"/>
<attribute name="OC_FARNELL" value="9494227"/>
<attribute name="OC_NEWARK" value="07B6801"/>
<attribute name="PACKAGE" value="8-SOP"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM56BIMM" prefix="U">
<description>Low Power thermostat</description>
<gates>
<gate name="A" symbol="LM56BIMM"/>
</gates>
<devices>
<device name="" package="SOP65P490X109-8N">
<connects>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="OUT1" pad="7"/>
<connect gate="A" pin="OUT2" pad="6"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="VREF" pad="1"/>
<connect gate="A" pin="VT1" pad="3"/>
<connect gate="A" pin="VT2" pad="2"/>
<connect gate="A" pin="VTEMP" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM56BIMM"/>
<attribute name="OC_FARNELL" value="9778489"/>
<attribute name="OC_NEWARK" value="83F4669"/>
<attribute name="PACKAGE" value="8-MSOP"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM56CIM" prefix="U">
<description>Low Power thermostat</description>
<gates>
<gate name="A" symbol="LM56CIM"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="OUT1" pad="7"/>
<connect gate="A" pin="OUT2" pad="6"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="VREF" pad="1"/>
<connect gate="A" pin="VT1" pad="3"/>
<connect gate="A" pin="VT2" pad="2"/>
<connect gate="A" pin="VTEMP" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM56CIM"/>
<attribute name="OC_FARNELL" value="9494197"/>
<attribute name="OC_NEWARK" value="41K6156"/>
<attribute name="PACKAGE" value="8-SOP"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM56CIMM" prefix="U">
<description>Low Power thermostat</description>
<gates>
<gate name="A" symbol="LM56CIMM"/>
</gates>
<devices>
<device name="" package="SOP65P490X109-8N">
<connects>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="OUT1" pad="7"/>
<connect gate="A" pin="OUT2" pad="6"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="VREF" pad="1"/>
<connect gate="A" pin="VT1" pad="3"/>
<connect gate="A" pin="VT2" pad="2"/>
<connect gate="A" pin="VTEMP" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM56CIMM"/>
<attribute name="OC_FARNELL" value="1798334"/>
<attribute name="OC_NEWARK" value="73R9750"/>
<attribute name="PACKAGE" value="8-MSOP"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM60BIM3" prefix="U">
<description>Temperature Sensor</description>
<gates>
<gate name="A" symbol="LM60BIM3"/>
</gates>
<devices>
<device name="" package="SOT95P251X112-3N">
<connects>
<connect gate="A" pin="+VS" pad="1"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="VO" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM60BIM3"/>
<attribute name="OC_FARNELL" value="9779132"/>
<attribute name="OC_NEWARK" value="41K6166"/>
<attribute name="PACKAGE" value="SOT-23-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM60BIZ" prefix="U">
<description>IC, TEMPERATURE SENSOR, ± 2°C</description>
<gates>
<gate name="A" symbol="LM60BIZ"/>
</gates>
<devices>
<device name="" package="TO127P254X495-3P">
<connects>
<connect gate="A" pin="+VS" pad="1"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="VOUT" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM60BIZ"/>
<attribute name="OC_FARNELL" value="9489657"/>
<attribute name="OC_NEWARK" value="41K6168"/>
<attribute name="PACKAGE" value="TO-92"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM60CIM3" prefix="U">
<description>Temperature Sensor</description>
<gates>
<gate name="A" symbol="LM60CIM3"/>
</gates>
<devices>
<device name="" package="SOT95P251X112-3N">
<connects>
<connect gate="A" pin="+VS" pad="1"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="VO" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM60CIM3"/>
<attribute name="OC_FARNELL" value="9779698"/>
<attribute name="OC_NEWARK" value="92F317"/>
<attribute name="PACKAGE" value="SOT-23-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM60CIZ" prefix="U">
<description>IC, TEMPERATURE SENSOR, ± 3°C</description>
<gates>
<gate name="A" symbol="LM60CIZ"/>
</gates>
<devices>
<device name="" package="TO127P254X495-3P">
<connects>
<connect gate="A" pin="+VS" pad="1"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="VOUT" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM60CIZ"/>
<attribute name="OC_FARNELL" value="9489665"/>
<attribute name="OC_NEWARK" value="41K6171"/>
<attribute name="PACKAGE" value="TO-92"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM611CM" prefix="U">
<description>OpAmpIC</description>
<gates>
<gate name="A" symbol="LM611CM"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="+IN" pad="9"/>
<connect gate="A" pin="-IN" pad="10"/>
<connect gate="A" pin="ANODE" pad="3"/>
<connect gate="A" pin="CATHODE" pad="5"/>
<connect gate="A" pin="FB" pad="4"/>
<connect gate="A" pin="NC" pad="2"/>
<connect gate="A" pin="NC_2" pad="12"/>
<connect gate="A" pin="NC_3" pad="13"/>
<connect gate="A" pin="NC_4" pad="1"/>
<connect gate="A" pin="NC_5" pad="6"/>
<connect gate="A" pin="NC_6" pad="8"/>
<connect gate="A" pin="OUT" pad="11"/>
<connect gate="A" pin="V+" pad="14"/>
<connect gate="A" pin="V-" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM611CM"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="07B6815"/>
<attribute name="PACKAGE" value="OpAmpIC"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM6132AIM" prefix="U">
<description>OpAmpIC</description>
<gates>
<gate name="A" symbol="LM6132AIM"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="+INA" pad="3"/>
<connect gate="A" pin="+INB" pad="5"/>
<connect gate="A" pin="-INA" pad="2"/>
<connect gate="A" pin="-INB" pad="6"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM6132AIM"/>
<attribute name="OC_FARNELL" value="9490043"/>
<attribute name="OC_NEWARK" value="07B6821"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM6132BIM" prefix="U">
<description>OpAmpIC</description>
<gates>
<gate name="A" symbol="LM6132BIM"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="+INA" pad="3"/>
<connect gate="A" pin="+INB" pad="5"/>
<connect gate="A" pin="-INA" pad="2"/>
<connect gate="A" pin="-INB" pad="6"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM6132BIM"/>
<attribute name="OC_FARNELL" value="9490019"/>
<attribute name="OC_NEWARK" value="41K6186"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM6132BIN" prefix="U">
<description>OP AMP</description>
<gates>
<gate name="A" symbol="LM6132BIN"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-8">
<connects>
<connect gate="A" pin="+INA" pad="3"/>
<connect gate="A" pin="+INB" pad="5"/>
<connect gate="A" pin="+V" pad="8"/>
<connect gate="A" pin="-INA" pad="2"/>
<connect gate="A" pin="-INB" pad="6"/>
<connect gate="A" pin="-V" pad="4"/>
<connect gate="A" pin="OUT_A" pad="1"/>
<connect gate="A" pin="OUT_B" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM6132BIN"/>
<attribute name="OC_FARNELL" value="9493980"/>
<attribute name="OC_NEWARK" value="26M0424"/>
<attribute name="PACKAGE" value="8-DIP"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM6134AIM" prefix="U">
<description>OpAmpIC</description>
<gates>
<gate name="A" symbol="LM6134AIM"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="+INA" pad="3"/>
<connect gate="A" pin="+INB" pad="5"/>
<connect gate="A" pin="+INC" pad="10"/>
<connect gate="A" pin="+IND" pad="12"/>
<connect gate="A" pin="-INA" pad="2"/>
<connect gate="A" pin="-INB" pad="6"/>
<connect gate="A" pin="-INC" pad="9"/>
<connect gate="A" pin="-IND" pad="13"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="OUTC" pad="8"/>
<connect gate="A" pin="OUTD" pad="14"/>
<connect gate="A" pin="V+" pad="4"/>
<connect gate="A" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM6134AIM"/>
<attribute name="OC_FARNELL" value="9490035"/>
<attribute name="OC_NEWARK" value="41K6189"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM6134BIM" prefix="U">
<description>OpAmpIC</description>
<gates>
<gate name="A" symbol="LM6134BIM"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="+INA" pad="3"/>
<connect gate="A" pin="+INB" pad="5"/>
<connect gate="A" pin="+INC" pad="10"/>
<connect gate="A" pin="+IND" pad="12"/>
<connect gate="A" pin="-INA" pad="2"/>
<connect gate="A" pin="-INB" pad="6"/>
<connect gate="A" pin="-INC" pad="9"/>
<connect gate="A" pin="-IND" pad="13"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="OUTC" pad="8"/>
<connect gate="A" pin="OUTD" pad="14"/>
<connect gate="A" pin="V+" pad="4"/>
<connect gate="A" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM6134BIM"/>
<attribute name="OC_FARNELL" value="9490027"/>
<attribute name="OC_NEWARK" value="41K6191"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM6134BIN" prefix="U">
<description>OP AMP</description>
<gates>
<gate name="A" symbol="LM6134BIN"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-14">
<connects>
<connect gate="A" pin="+INA" pad="3"/>
<connect gate="A" pin="+INB" pad="5"/>
<connect gate="A" pin="+INC" pad="10"/>
<connect gate="A" pin="+IND" pad="12"/>
<connect gate="A" pin="-INA" pad="2"/>
<connect gate="A" pin="-INB" pad="6"/>
<connect gate="A" pin="-INC" pad="9"/>
<connect gate="A" pin="-IND" pad="13"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="OUTC" pad="8"/>
<connect gate="A" pin="OUTD" pad="14"/>
<connect gate="A" pin="V+" pad="4"/>
<connect gate="A" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM6134BIN"/>
<attribute name="OC_FARNELL" value="9493999"/>
<attribute name="OC_NEWARK" value="41K6193"/>
<attribute name="PACKAGE" value="14-DIP"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM613IWM" prefix="U">
<description>OpAmpIC</description>
<gates>
<gate name="A" symbol="LM613IWM"/>
</gates>
<devices>
<device name="" package="SOIC127P1032X265-16N">
<connects>
<connect gate="A" pin="+COMP1" pad="3"/>
<connect gate="A" pin="+COMP4" pad="14"/>
<connect gate="A" pin="+OPAMP2" pad="5"/>
<connect gate="A" pin="+OPAMP3" pad="12"/>
<connect gate="A" pin="-COMP1" pad="2"/>
<connect gate="A" pin="-COMP4" pad="15"/>
<connect gate="A" pin="-OPAMP2" pad="6"/>
<connect gate="A" pin="-OPAMP3" pad="11"/>
<connect gate="A" pin="CATHODE" pad="9"/>
<connect gate="A" pin="FB" pad="8"/>
<connect gate="A" pin="OUT1" pad="1"/>
<connect gate="A" pin="OUT2" pad="7"/>
<connect gate="A" pin="OUT3" pad="10"/>
<connect gate="A" pin="OUT4" pad="16"/>
<connect gate="A" pin="V+" pad="4"/>
<connect gate="A" pin="V-" pad="13"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM613IWM"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="07B6819"/>
<attribute name="PACKAGE" value="SOIC-16"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM6142AIM" prefix="U">
<description>OpAmpIC</description>
<gates>
<gate name="A" symbol="LM6142AIM"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="+INA" pad="3"/>
<connect gate="A" pin="+INB" pad="5"/>
<connect gate="A" pin="-INA" pad="2"/>
<connect gate="A" pin="-INB" pad="6"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM6142AIM"/>
<attribute name="OC_FARNELL" value="9494561"/>
<attribute name="OC_NEWARK" value="41K6198"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM6142BIM" prefix="U">
<description>OpAmpIC</description>
<gates>
<gate name="A" symbol="LM6142BIM"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="+INA" pad="3"/>
<connect gate="A" pin="+INB" pad="5"/>
<connect gate="A" pin="-INA" pad="2"/>
<connect gate="A" pin="-INB" pad="6"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM6142BIM"/>
<attribute name="OC_FARNELL" value="9494570"/>
<attribute name="OC_NEWARK" value="41K6201"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM6142BIN" prefix="U">
<description>OP Amps</description>
<gates>
<gate name="A" symbol="LM6142BIN"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-8">
<connects>
<connect gate="A" pin="+INA" pad="3"/>
<connect gate="A" pin="+INB" pad="5"/>
<connect gate="A" pin="-INA" pad="2"/>
<connect gate="A" pin="-INB" pad="6"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM6142BIN"/>
<attribute name="OC_FARNELL" value="1523858"/>
<attribute name="OC_NEWARK" value="97K3573"/>
<attribute name="PACKAGE" value="8-DIP"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM6144AIM" prefix="U">
<description>OpAmpIC</description>
<gates>
<gate name="A" symbol="LM6144AIM"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="+INA" pad="3"/>
<connect gate="A" pin="+INB" pad="5"/>
<connect gate="A" pin="+INC" pad="10"/>
<connect gate="A" pin="+IND" pad="12"/>
<connect gate="A" pin="-INA" pad="2"/>
<connect gate="A" pin="-INB" pad="6"/>
<connect gate="A" pin="-INC" pad="9"/>
<connect gate="A" pin="-IND" pad="13"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="OUTC" pad="8"/>
<connect gate="A" pin="OUTD" pad="14"/>
<connect gate="A" pin="V+" pad="4"/>
<connect gate="A" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM6144AIM"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="07B6840"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM6144BIM" prefix="U">
<description>OpAmpIC</description>
<gates>
<gate name="A" symbol="LM6144BIM"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="+INA" pad="3"/>
<connect gate="A" pin="+INB" pad="5"/>
<connect gate="A" pin="+INC" pad="10"/>
<connect gate="A" pin="+IND" pad="12"/>
<connect gate="A" pin="-INA" pad="2"/>
<connect gate="A" pin="-INB" pad="6"/>
<connect gate="A" pin="-INC" pad="9"/>
<connect gate="A" pin="-IND" pad="13"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="OUTC" pad="8"/>
<connect gate="A" pin="OUTD" pad="14"/>
<connect gate="A" pin="V+" pad="4"/>
<connect gate="A" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM6144BIM"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="07B6842"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM6144BIN" prefix="U">
<description>OP AMP</description>
<gates>
<gate name="A" symbol="LM6144BIN"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-14">
<connects>
<connect gate="A" pin="+INA" pad="3"/>
<connect gate="A" pin="+INB" pad="5"/>
<connect gate="A" pin="+INC" pad="10"/>
<connect gate="A" pin="+IND" pad="12"/>
<connect gate="A" pin="-INA" pad="2"/>
<connect gate="A" pin="-INB" pad="6"/>
<connect gate="A" pin="-INC" pad="9"/>
<connect gate="A" pin="-IND" pad="13"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="OUTC" pad="8"/>
<connect gate="A" pin="OUTD" pad="14"/>
<connect gate="A" pin="V+" pad="4"/>
<connect gate="A" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM6144BIN"/>
<attribute name="OC_FARNELL" value="9493581"/>
<attribute name="OC_NEWARK" value="97K3574"/>
<attribute name="PACKAGE" value="14-DIP"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM614CWM" prefix="U">
<description>OpAmpIC</description>
<gates>
<gate name="A" symbol="LM614CWM"/>
</gates>
<devices>
<device name="" package="SOIC127P1032X265-16N">
<connects>
<connect gate="A" pin="+INA" pad="3"/>
<connect gate="A" pin="+INB" pad="5"/>
<connect gate="A" pin="+INC" pad="12"/>
<connect gate="A" pin="+IND" pad="14"/>
<connect gate="A" pin="-INA" pad="2"/>
<connect gate="A" pin="-INB" pad="6"/>
<connect gate="A" pin="-INC" pad="11"/>
<connect gate="A" pin="-IND" pad="15"/>
<connect gate="A" pin="CATHODE" pad="9"/>
<connect gate="A" pin="FB" pad="8"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="OUTC" pad="10"/>
<connect gate="A" pin="OUTD" pad="16"/>
<connect gate="A" pin="V+" pad="4"/>
<connect gate="A" pin="V-" pad="13"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM614CWM"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K6194"/>
<attribute name="PACKAGE" value="SOIC-16"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM614IWM" prefix="U">
<description>OpAmpIC</description>
<gates>
<gate name="A" symbol="LM614IWM"/>
</gates>
<devices>
<device name="" package="SOIC127P1032X265-16N">
<connects>
<connect gate="A" pin="+INA" pad="3"/>
<connect gate="A" pin="+INB" pad="5"/>
<connect gate="A" pin="+INC" pad="12"/>
<connect gate="A" pin="+IND" pad="14"/>
<connect gate="A" pin="-INA" pad="2"/>
<connect gate="A" pin="-INB" pad="6"/>
<connect gate="A" pin="-INC" pad="11"/>
<connect gate="A" pin="-IND" pad="15"/>
<connect gate="A" pin="CATHODE" pad="9"/>
<connect gate="A" pin="FB" pad="8"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="OUTC" pad="10"/>
<connect gate="A" pin="OUTD" pad="16"/>
<connect gate="A" pin="V+" pad="4"/>
<connect gate="A" pin="V-" pad="13"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM614IWM"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K6196"/>
<attribute name="PACKAGE" value="SOIC-16"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM6152ACM" prefix="U">
<description>OpAmpIC</description>
<gates>
<gate name="A" symbol="LM6152ACM"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="+INA" pad="3"/>
<connect gate="A" pin="+INB" pad="5"/>
<connect gate="A" pin="-INA" pad="2"/>
<connect gate="A" pin="-INB" pad="6"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM6152ACM"/>
<attribute name="OC_FARNELL" value="1564752"/>
<attribute name="OC_NEWARK" value="41K6209"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM6152BCM" prefix="U">
<description>OpAmpIC</description>
<gates>
<gate name="A" symbol="LM6152BCM"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="+INA" pad="3"/>
<connect gate="A" pin="+INB" pad="5"/>
<connect gate="A" pin="-INA" pad="2"/>
<connect gate="A" pin="-INB" pad="6"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM6152BCM"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="07B6847"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM6154BCM" prefix="U">
<description>OpAmpIC</description>
<gates>
<gate name="A" symbol="LM6154BCM"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="+INA" pad="3"/>
<connect gate="A" pin="+INB" pad="5"/>
<connect gate="A" pin="+INC" pad="10"/>
<connect gate="A" pin="+IND" pad="12"/>
<connect gate="A" pin="-INA" pad="2"/>
<connect gate="A" pin="-INB" pad="6"/>
<connect gate="A" pin="-INC" pad="9"/>
<connect gate="A" pin="-IND" pad="13"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="OUTC" pad="8"/>
<connect gate="A" pin="OUTD" pad="14"/>
<connect gate="A" pin="V+" pad="4"/>
<connect gate="A" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM6154BCM"/>
<attribute name="OC_FARNELL" value="1286923"/>
<attribute name="OC_NEWARK" value="41K6213"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM6171AIM" prefix="U">
<description>OpAmpIC</description>
<gates>
<gate name="A" symbol="LM6171AIM"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="NC" pad="8"/>
<connect gate="A" pin="NC_2" pad="1"/>
<connect gate="A" pin="NC_3" pad="5"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM6171AIM"/>
<attribute name="OC_FARNELL" value="1685343"/>
<attribute name="OC_NEWARK" value="07B6856"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM6171BIM" prefix="U">
<description>Voltage Feedback Amp</description>
<gates>
<gate name="A" symbol="LM6171BIM"/>
</gates>
<devices>
<device name="" package="SOIC127P620X175-8N">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="N/C" pad="1"/>
<connect gate="A" pin="N/C_2" pad="5"/>
<connect gate="A" pin="N/C_3" pad="8"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM6171BIM"/>
<attribute name="OC_FARNELL" value="9493620"/>
<attribute name="OC_NEWARK" value="97K3575"/>
<attribute name="PACKAGE" value="8-SOIC"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM6171BIN" prefix="U">
<description>Amplifier</description>
<gates>
<gate name="A" symbol="LM6171BIN"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-8">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="N/C" pad="8"/>
<connect gate="A" pin="N/C_2" pad="1"/>
<connect gate="A" pin="N/C_3" pad="5"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM6171BIN"/>
<attribute name="OC_FARNELL" value="9493611"/>
<attribute name="OC_NEWARK" value="41K6219"/>
<attribute name="PACKAGE" value="8-DIP"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM6172AMJFQMLV" prefix="U">
<description>Feedback Amplifiers</description>
<gates>
<gate name="A" symbol="LM6172AMJFQMLV"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-8">
<connects>
<connect gate="A" pin="+POSA" pad="3"/>
<connect gate="A" pin="+POSB" pad="5"/>
<connect gate="A" pin="-NEGA" pad="2"/>
<connect gate="A" pin="-NEGB" pad="6"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM6172AMJFQMLV"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="31T9973"/>
<attribute name="PACKAGE" value="DIP-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM6172IM" prefix="U">
<description>OpAmpIC</description>
<gates>
<gate name="A" symbol="LM6172IM"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="INVERTING_INPUT_A" pad="2"/>
<connect gate="A" pin="INVERTING_INPUT_B" pad="6"/>
<connect gate="A" pin="NON_INVERTING_INPUT_A" pad="3"/>
<connect gate="A" pin="NON_INVERTING_INPUT_B" pad="5"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM6172IM"/>
<attribute name="OC_FARNELL" value="1468928"/>
<attribute name="OC_NEWARK" value="07B6862"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM6172IN" prefix="U">
<description>OpAmpIC</description>
<gates>
<gate name="A" symbol="LM6172IN"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-8">
<connects>
<connect gate="A" pin="NEG_A" pad="2"/>
<connect gate="A" pin="NEG_B" pad="6"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="POS_A" pad="3"/>
<connect gate="A" pin="POS_B" pad="5"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM6172IN"/>
<attribute name="OC_FARNELL" value="1468929"/>
<attribute name="OC_NEWARK" value="07B6864"/>
<attribute name="PACKAGE" value="DIP-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM6181IM-8" prefix="U">
<description>Current Feedback Amplifier</description>
<gates>
<gate name="A" symbol="LM6181IM-8"/>
</gates>
<devices>
<device name="" package="SOIC127P620X175-8N">
<connects>
<connect gate="A" pin="NC" pad="8"/>
<connect gate="A" pin="NC_2" pad="1"/>
<connect gate="A" pin="NC_3" pad="5"/>
<connect gate="A" pin="NEG" pad="2"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="POS" pad="3"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM6181IM-8"/>
<attribute name="OC_FARNELL" value="1468930"/>
<attribute name="OC_NEWARK" value="41K6223"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM6181IN" prefix="U">
<description>Feed back Amplifier</description>
<gates>
<gate name="A" symbol="LM6181IN"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-8">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="N/C" pad="8"/>
<connect gate="A" pin="N/C_2" pad="1"/>
<connect gate="A" pin="N/C_3" pad="5"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM6181IN"/>
<attribute name="OC_FARNELL" value="9485953"/>
<attribute name="OC_NEWARK" value="41K6227"/>
<attribute name="PACKAGE" value="8-DIP"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM61BIM3" prefix="U">
<description>Temperature Sensor</description>
<gates>
<gate name="A" symbol="LM61BIM3"/>
</gates>
<devices>
<device name="" package="SOT95P251X112-3N">
<connects>
<connect gate="A" pin="+VS" pad="1"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="VO" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM61BIM3"/>
<attribute name="OC_FARNELL" value="1197387"/>
<attribute name="OC_NEWARK" value="41K6172"/>
<attribute name="PACKAGE" value="SOT-23-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM61CIM3" prefix="U">
<description>Temperature Sensor</description>
<gates>
<gate name="A" symbol="LM61CIM3"/>
</gates>
<devices>
<device name="" package="SOT95P251X112-3N">
<connects>
<connect gate="A" pin="+VS" pad="1"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="VO" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM61CIM3"/>
<attribute name="OC_FARNELL" value="1197388"/>
<attribute name="OC_NEWARK" value="83F4672"/>
<attribute name="PACKAGE" value="SOT-23-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM6211MF" prefix="U">
<description>Operational Amplifier</description>
<gates>
<gate name="A" symbol="LM6211MF"/>
</gates>
<devices>
<device name="" package="SOT95P284X122-5N">
<connects>
<connect gate="A" pin="IN+" pad="3"/>
<connect gate="A" pin="IN-" pad="4"/>
<connect gate="A" pin="V+" pad="5"/>
<connect gate="A" pin="V-" pad="2"/>
<connect gate="A" pin="VOUT" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM6211MF"/>
<attribute name="OC_FARNELL" value="1312794"/>
<attribute name="OC_NEWARK" value="99K2539"/>
<attribute name="PACKAGE" value="SOT23-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM62BIM3" prefix="U">
<description>Temperature Sensor</description>
<gates>
<gate name="A" symbol="LM62BIM3"/>
</gates>
<devices>
<device name="" package="SOT95P251X112-3N">
<connects>
<connect gate="A" pin="+VS" pad="1"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="VO" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM62BIM3"/>
<attribute name="OC_FARNELL" value="1798368"/>
<attribute name="OC_NEWARK" value="73R9751"/>
<attribute name="PACKAGE" value="SOT-23-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM63CIMA" prefix="U">
<description>Digital Temperature Sensor</description>
<gates>
<gate name="A" symbol="LM63CIMA"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="D+" pad="2"/>
<connect gate="A" pin="D-" pad="3"/>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="PWM" pad="4"/>
<connect gate="A" pin="SMBCLK" pad="8"/>
<connect gate="A" pin="SMBDAT" pad="7"/>
<connect gate="A" pin="VDD" pad="1"/>
<connect gate="A" pin="~ALERT/TACH" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM63CIMA"/>
<attribute name="OC_FARNELL" value="1286926"/>
<attribute name="OC_NEWARK" value="41K6239"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM6511IM" prefix="U">
<description>OpAmpIC</description>
<gates>
<gate name="A" symbol="LM6511IM"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="BAL/STRB" pad="6"/>
<connect gate="A" pin="GND" pad="1"/>
<connect gate="A" pin="NEG_A" pad="3"/>
<connect gate="A" pin="OFS" pad="5"/>
<connect gate="A" pin="OUT" pad="7"/>
<connect gate="A" pin="POS_A" pad="2"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM6511IM"/>
<attribute name="OC_FARNELL" value="1685384"/>
<attribute name="OC_NEWARK" value="41K6245"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM6584MT" prefix="U">
<description>Operational Amplifier</description>
<gates>
<gate name="A" symbol="LM6584MT"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-14N">
<connects>
<connect gate="A" pin="+INA" pad="3"/>
<connect gate="A" pin="+INB" pad="5"/>
<connect gate="A" pin="+INC" pad="10"/>
<connect gate="A" pin="+IND" pad="12"/>
<connect gate="A" pin="-INA" pad="2"/>
<connect gate="A" pin="-INB" pad="6"/>
<connect gate="A" pin="-INC" pad="9"/>
<connect gate="A" pin="-IND" pad="13"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="OUTC" pad="8"/>
<connect gate="A" pin="OUTD" pad="14"/>
<connect gate="A" pin="V+" pad="4"/>
<connect gate="A" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM6584MT"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K6249"/>
<attribute name="PACKAGE" value="TSSOP-14"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM6588MA" prefix="U">
<description>Operational Amplifier</description>
<gates>
<gate name="A" symbol="LM6588MA"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-14N">
<connects>
<connect gate="A" pin="+INA" pad="3"/>
<connect gate="A" pin="+INB" pad="5"/>
<connect gate="A" pin="+INC" pad="10"/>
<connect gate="A" pin="+IND" pad="12"/>
<connect gate="A" pin="-INA" pad="2"/>
<connect gate="A" pin="-INB" pad="6"/>
<connect gate="A" pin="-INC" pad="9"/>
<connect gate="A" pin="-IND" pad="13"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="OUTC" pad="8"/>
<connect gate="A" pin="OUTD" pad="14"/>
<connect gate="A" pin="V+" pad="4"/>
<connect gate="A" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM6588MT"/>
<attribute name="OC_FARNELL" value="1685386"/>
<attribute name="OC_NEWARK" value="47T5249"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM70CIMM-3" prefix="U">
<description>10-Bit plus Sign Digital Temperature Sensor</description>
<gates>
<gate name="A" symbol="LM70CIMM-3"/>
</gates>
<devices>
<device name="" package="SOP65P490X110-8N">
<connects>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="NC" pad="8"/>
<connect gate="A" pin="NC_2" pad="3"/>
<connect gate="A" pin="NC_3" pad="6"/>
<connect gate="A" pin="SC" pad="2"/>
<connect gate="A" pin="SI/O" pad="1"/>
<connect gate="A" pin="V+" pad="5"/>
<connect gate="A" pin="~CS" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM70CIMM-3"/>
<attribute name="OC_FARNELL" value="1312795"/>
<attribute name="OC_NEWARK" value="41K6260"/>
<attribute name="PACKAGE" value="8-MSOP"/>
<attribute name="SUPPLIER" value="National  Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM70CIMM-5" prefix="U">
<description>Digital temperature sensor</description>
<gates>
<gate name="A" symbol="LM70CIMM-5"/>
</gates>
<devices>
<device name="" package="SOP65P490X109-8N">
<connects>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="NC" pad="6"/>
<connect gate="A" pin="NC_2" pad="3"/>
<connect gate="A" pin="NC_3" pad="8"/>
<connect gate="A" pin="SC" pad="2"/>
<connect gate="A" pin="SI/O" pad="1"/>
<connect gate="A" pin="V+" pad="5"/>
<connect gate="A" pin="~CS" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM70CIMM-5"/>
<attribute name="OC_FARNELL" value="9779230"/>
<attribute name="OC_NEWARK" value="74C4675"/>
<attribute name="PACKAGE" value="8-MSOP"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM7121IM" prefix="U">
<description>Amp</description>
<gates>
<gate name="A" symbol="LM7121IM"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="IN+" pad="3"/>
<connect gate="A" pin="IN-" pad="2"/>
<connect gate="A" pin="N/C" pad="5"/>
<connect gate="A" pin="N/C_2" pad="1"/>
<connect gate="A" pin="NC" pad="8"/>
<connect gate="A" pin="OUTPUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM7121IM"/>
<attribute name="OC_FARNELL" value="9494120"/>
<attribute name="OC_NEWARK" value="-"/>
<attribute name="PACKAGE" value="8-SOIC"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM7171AIM" prefix="U">
<description>OpAmpIC</description>
<gates>
<gate name="A" symbol="LM7171AIM"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="NC" pad="8"/>
<connect gate="A" pin="NC_2" pad="1"/>
<connect gate="A" pin="NC_3" pad="5"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM7171AIM"/>
<attribute name="OC_FARNELL" value="1286927"/>
<attribute name="OC_NEWARK" value="07B6934"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM7171BIM" prefix="U">
<description>OpAmpIC</description>
<gates>
<gate name="A" symbol="LM7171BIM"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="NC" pad="8"/>
<connect gate="A" pin="NC_2" pad="1"/>
<connect gate="A" pin="NC_3" pad="5"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM7171BIM"/>
<attribute name="OC_FARNELL" value="1468934"/>
<attribute name="OC_NEWARK" value="41K6275"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM7171BIN" prefix="U">
<description>Amplifier</description>
<gates>
<gate name="A" symbol="LM7171BIN"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-8">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="N/C" pad="8"/>
<connect gate="A" pin="N/C_2" pad="1"/>
<connect gate="A" pin="N/C_3" pad="5"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM7171BIN"/>
<attribute name="OC_FARNELL" value="9493727"/>
<attribute name="OC_NEWARK" value="07B6941"/>
<attribute name="PACKAGE" value="8-DIP"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM71CIMF" prefix="U">
<description>Temperature Sensor</description>
<gates>
<gate name="A" symbol="LM71CIMF"/>
</gates>
<devices>
<device name="" package="SOT95P284X119-5N">
<connects>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="SC" pad="4"/>
<connect gate="A" pin="SI/O" pad="3"/>
<connect gate="A" pin="V+" pad="5"/>
<connect gate="A" pin="~CS" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM71CIMF"/>
<attribute name="OC_FARNELL" value="1312796"/>
<attribute name="OC_NEWARK" value="41K6264"/>
<attribute name="PACKAGE" value="SOT23-5"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM7301IM" prefix="U">
<description>Op Amp</description>
<gates>
<gate name="A" symbol="LM7301IM"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="IN+" pad="3"/>
<connect gate="A" pin="IN-" pad="2"/>
<connect gate="A" pin="N/C" pad="5"/>
<connect gate="A" pin="N/C_2" pad="1"/>
<connect gate="A" pin="NC" pad="8"/>
<connect gate="A" pin="OUTPUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM7301IM"/>
<attribute name="OC_FARNELL" value="9494170"/>
<attribute name="OC_NEWARK" value="07B6946"/>
<attribute name="PACKAGE" value="8-SOIC"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM7301IM5" prefix="U">
<description>Operational Amplifier</description>
<gates>
<gate name="A" symbol="LM7301IM5"/>
</gates>
<devices>
<device name="" package="SOT95P300X120-5N">
<connects>
<connect gate="A" pin="NEG" pad="4"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="A" pin="POS" pad="3"/>
<connect gate="A" pin="V+" pad="5"/>
<connect gate="A" pin="V-" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM7301IM5"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="92F324"/>
<attribute name="PACKAGE" value="SOT-5"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM7321MA" prefix="U">
<description>Operational Amplifier</description>
<gates>
<gate name="A" symbol="LM7321MA"/>
</gates>
<devices>
<device name="" package="SOIC127P620X175-8N">
<connects>
<connect gate="A" pin="IN+" pad="3"/>
<connect gate="A" pin="IN-" pad="2"/>
<connect gate="A" pin="NC" pad="8"/>
<connect gate="A" pin="NC_2" pad="5"/>
<connect gate="A" pin="NC_3" pad="1"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM7321MA"/>
<attribute name="OC_FARNELL" value="1663012"/>
<attribute name="OC_NEWARK" value="11N9283"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM7321MF" prefix="U">
<description>Operational Amplifier</description>
<gates>
<gate name="A" symbol="LM7321MF"/>
</gates>
<devices>
<device name="" package="SOT95P300X120-5N">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="4"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="A" pin="V+" pad="5"/>
<connect gate="A" pin="V-" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM7321MF"/>
<attribute name="OC_FARNELL" value="1663013"/>
<attribute name="OC_NEWARK" value="11N9285"/>
<attribute name="PACKAGE" value="SOT-23-5"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM7322MA" prefix="U">
<description>Operational Amplifier</description>
<gates>
<gate name="A" symbol="LM7322MA"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="INA+" pad="3"/>
<connect gate="A" pin="INA-" pad="2"/>
<connect gate="A" pin="INB+" pad="5"/>
<connect gate="A" pin="INB-" pad="6"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM7322MA"/>
<attribute name="OC_FARNELL" value="1663018"/>
<attribute name="OC_NEWARK" value="01P0825"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM7322MM" prefix="U">
<description>Operational Amplifier</description>
<gates>
<gate name="A" symbol="LM7322MM"/>
</gates>
<devices>
<device name="" package="SOP65P490X109-8N">
<connects>
<connect gate="A" pin="INA+" pad="3"/>
<connect gate="A" pin="INA-" pad="2"/>
<connect gate="A" pin="INB+" pad="5"/>
<connect gate="A" pin="INB-" pad="6"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM7322MM"/>
<attribute name="OC_FARNELL" value="1663019"/>
<attribute name="OC_NEWARK" value="07P5471"/>
<attribute name="PACKAGE" value="MSOP-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM7332MA" prefix="U">
<description>Operational Amplifier</description>
<gates>
<gate name="A" symbol="LM7332MA"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="INA+" pad="3"/>
<connect gate="A" pin="INA-" pad="2"/>
<connect gate="A" pin="INB+" pad="5"/>
<connect gate="A" pin="INB-" pad="6"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM7332MA"/>
<attribute name="OC_FARNELL" value="1589522"/>
<attribute name="OC_NEWARK" value="08N3588"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM7341MF" prefix="U">
<description>Operational Amplifier</description>
<gates>
<gate name="A" symbol="LM7341MF"/>
</gates>
<devices>
<device name="" package="SOT95P284X119-5N">
<connects>
<connect gate="A" pin="NEG" pad="4"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="A" pin="POS" pad="3"/>
<connect gate="A" pin="V+" pad="5"/>
<connect gate="A" pin="V-" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM7341MF"/>
<attribute name="OC_FARNELL" value="1663016"/>
<attribute name="OC_NEWARK" value="15P1988"/>
<attribute name="PACKAGE" value="SOT-23-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM7372IMA" prefix="U">
<description>Dual Operational Amplifier</description>
<gates>
<gate name="A" symbol="LM7372IMA"/>
</gates>
<devices>
<device name="" package="SOIC127P620X175-16N">
<connects>
<connect gate="A" pin="+IN" pad="11"/>
<connect gate="A" pin="+IN_2" pad="5"/>
<connect gate="A" pin="-IN" pad="12"/>
<connect gate="A" pin="-IN_2" pad="4"/>
<connect gate="A" pin="NC" pad="10"/>
<connect gate="A" pin="NC_2" pad="8"/>
<connect gate="A" pin="NC_3" pad="1"/>
<connect gate="A" pin="NC_4" pad="15"/>
<connect gate="A" pin="NC_5" pad="2"/>
<connect gate="A" pin="NC_6" pad="9"/>
<connect gate="A" pin="NC_7" pad="7"/>
<connect gate="A" pin="NC_8" pad="16"/>
<connect gate="A" pin="OUTA" pad="3"/>
<connect gate="A" pin="OUTB" pad="13"/>
<connect gate="A" pin="V+" pad="14"/>
<connect gate="A" pin="V-" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM7372IMA"/>
<attribute name="OC_FARNELL" value="1685409"/>
<attribute name="OC_NEWARK" value="41K6286"/>
<attribute name="PACKAGE" value="SOIC-16"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM7372MR" prefix="U">
<description>Dual Operational Amplifier</description>
<gates>
<gate name="A" symbol="LM7372MR"/>
</gates>
<devices>
<device name="" package="SOP127P620X168-9N">
<connects>
<connect gate="A" pin="+INA" pad="3"/>
<connect gate="A" pin="+INB" pad="5"/>
<connect gate="A" pin="-INA" pad="2"/>
<connect gate="A" pin="-INB" pad="6"/>
<connect gate="A" pin="EPAD" pad="9"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM7372MR"/>
<attribute name="OC_FARNELL" value="1286929"/>
<attribute name="OC_NEWARK" value="41K6288"/>
<attribute name="PACKAGE" value="SOP-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM73CIMK-0" prefix="U">
<description>Digital Temperature Sensor</description>
<gates>
<gate name="A" symbol="LM73CIMK-0"/>
</gates>
<devices>
<device name="" package="SOT95P285X100-6N">
<connects>
<connect gate="A" pin="ADDR" pad="1"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="SMBCLK" pad="4"/>
<connect gate="A" pin="SMBDAT" pad="6"/>
<connect gate="A" pin="VDD" pad="3"/>
<connect gate="A" pin="~ALERT" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM73CIMK-0"/>
<attribute name="OC_FARNELL" value="1312598"/>
<attribute name="OC_NEWARK" value="69K2606"/>
<attribute name="PACKAGE" value="SOT-23-6"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM73CIMK-1" prefix="U">
<description>Digital Temperature Sensor</description>
<gates>
<gate name="A" symbol="LM73CIMK-1"/>
</gates>
<devices>
<device name="" package="SOT95P285X100-6N">
<connects>
<connect gate="A" pin="ADDR" pad="1"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="SMBCLK" pad="4"/>
<connect gate="A" pin="SMBDAT" pad="6"/>
<connect gate="A" pin="VDD" pad="3"/>
<connect gate="A" pin="~ALERT" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM73CIMK-1"/>
<attribute name="OC_FARNELL" value="1312599"/>
<attribute name="OC_NEWARK" value="99K2544"/>
<attribute name="PACKAGE" value="SOT-23-6"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM741CH" prefix="U">
<description>IC, OP-AMP, 1MHZ, 0.5V/µS</description>
<gates>
<gate name="A" symbol="LM741CH"/>
</gates>
<devices>
<device name="" package="TO254P914X470-8P">
<connects>
<connect gate="A" pin="+INA" pad="3"/>
<connect gate="A" pin="-INA" pad="2"/>
<connect gate="A" pin="NC" pad="8"/>
<connect gate="A" pin="OFFSET_NULL" pad="1"/>
<connect gate="A" pin="OFFSET_NULL_2" pad="5"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM741CH"/>
<attribute name="OC_FARNELL" value="1216154"/>
<attribute name="OC_NEWARK" value="01M8171"/>
<attribute name="PACKAGE" value="TO-99-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM741CN" prefix="U">
<description>OP AMP</description>
<gates>
<gate name="A" symbol="LM741CN"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-8">
<connects>
<connect gate="A" pin="NC" pad="8"/>
<connect gate="A" pin="NEG" pad="2"/>
<connect gate="A" pin="OFFSET_NULL" pad="5"/>
<connect gate="A" pin="OFFSET_NULL_2" pad="1"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="POS" pad="3"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM741CN"/>
<attribute name="OC_FARNELL" value="9486780"/>
<attribute name="OC_NEWARK" value="97K3586"/>
<attribute name="PACKAGE" value="8-DIP"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM741H" prefix="U">
<description>IC, OP-AMP, 1MHZ, 0.5V/µS</description>
<gates>
<gate name="A" symbol="LM741H"/>
</gates>
<devices>
<device name="" package="TO254P914X470-8P">
<connects>
<connect gate="A" pin="+INA" pad="3"/>
<connect gate="A" pin="-INA" pad="2"/>
<connect gate="A" pin="NC" pad="8"/>
<connect gate="A" pin="OFFSET_NULL" pad="1"/>
<connect gate="A" pin="OFFSET_NULL_2" pad="5"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM741H"/>
<attribute name="OC_FARNELL" value="1216155"/>
<attribute name="OC_NEWARK" value="01M8172"/>
<attribute name="PACKAGE" value="TO-99-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM75AIM" prefix="U">
<description>Digital Temperature Sensor</description>
<gates>
<gate name="A" symbol="LM75AIM"/>
</gates>
<devices>
<device name="" package="SOIC127P620X175-8N">
<connects>
<connect gate="A" pin="+VS" pad="8"/>
<connect gate="A" pin="A0" pad="7"/>
<connect gate="A" pin="A1" pad="6"/>
<connect gate="A" pin="A2" pad="5"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="O.S." pad="3"/>
<connect gate="A" pin="SCL" pad="2"/>
<connect gate="A" pin="SDA" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM75AIM"/>
<attribute name="OC_FARNELL" value="1699380"/>
<attribute name="OC_NEWARK" value="-"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="NATIONAL SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM76CHM-5" prefix="U">
<description>Digital Temperature Sensor</description>
<gates>
<gate name="A" symbol="LM76CHM-5"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="A0" pad="7"/>
<connect gate="A" pin="A1" pad="6"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="INT" pad="5"/>
<connect gate="A" pin="SCL" pad="2"/>
<connect gate="A" pin="SDA" pad="1"/>
<connect gate="A" pin="T_CRIT_A" pad="3"/>
<connect gate="A" pin="VS+" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM76CHM-5"/>
<attribute name="OC_FARNELL" value="9486542"/>
<attribute name="OC_NEWARK" value="41K6311"/>
<attribute name="PACKAGE" value="8-SOIC"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM77CIMM-3" prefix="U">
<description>TempSensors</description>
<gates>
<gate name="A" symbol="LM77CIMM-3"/>
</gates>
<devices>
<device name="" package="SOP65P490X110-8N">
<connects>
<connect gate="A" pin="+VS" pad="8"/>
<connect gate="A" pin="A0" pad="7"/>
<connect gate="A" pin="A1" pad="6"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="INT" pad="5"/>
<connect gate="A" pin="SCL" pad="2"/>
<connect gate="A" pin="SDA" pad="1"/>
<connect gate="A" pin="T_CRIT_A" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM77CIMM-3"/>
<attribute name="OC_FARNELL" value="1564720"/>
<attribute name="OC_NEWARK" value="34C6647"/>
<attribute name="PACKAGE" value="SOP-8"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM78L05ACM" prefix="U">
<description>3-Terminal Positive Regulators</description>
<gates>
<gate name="A" symbol="LM78L05ACM"/>
</gates>
<devices>
<device name="" package="SOIC127P620X175-8N">
<connects>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="GND_2" pad="2"/>
<connect gate="A" pin="GND_3" pad="7"/>
<connect gate="A" pin="GND_4" pad="3"/>
<connect gate="A" pin="NC" pad="5"/>
<connect gate="A" pin="NC_2" pad="4"/>
<connect gate="A" pin="VIN" pad="8"/>
<connect gate="A" pin="VOUT" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM78L05ACM"/>
<attribute name="OC_FARNELL" value="9489436"/>
<attribute name="OC_NEWARK" value="-"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM809M3-2.63" prefix="U">
<description>Microprocessor</description>
<gates>
<gate name="A" symbol="LM809M3-2.63"/>
</gates>
<devices>
<device name="" package="SOT95P250X112-3N">
<connects>
<connect gate="A" pin="GND" pad="1"/>
<connect gate="A" pin="VCC" pad="3"/>
<connect gate="A" pin="~RESET" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM809M3-2.63"/>
<attribute name="OC_FARNELL" value="1652453"/>
<attribute name="OC_NEWARK" value="74C4700"/>
<attribute name="PACKAGE" value="SOT23-3"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM809M3-2.93" prefix="U">
<description>Microprocessor</description>
<gates>
<gate name="A" symbol="LM809M3-2.93"/>
</gates>
<devices>
<device name="" package="SOT95P250X112-3N">
<connects>
<connect gate="A" pin="GND" pad="1"/>
<connect gate="A" pin="VCC" pad="3"/>
<connect gate="A" pin="~RESET" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM809M3-2.93"/>
<attribute name="OC_FARNELL" value="1652454"/>
<attribute name="OC_NEWARK" value="74C4701"/>
<attribute name="PACKAGE" value="SOT23-3"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM809M3-3.08" prefix="U">
<description>Microprocessor</description>
<gates>
<gate name="A" symbol="LM809M3-3.08"/>
</gates>
<devices>
<device name="" package="SOT95P250X112-3N">
<connects>
<connect gate="A" pin="GND" pad="1"/>
<connect gate="A" pin="VCC" pad="3"/>
<connect gate="A" pin="~RESET" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM809M3-3.08"/>
<attribute name="OC_FARNELL" value="1652455"/>
<attribute name="OC_NEWARK" value="74C4702"/>
<attribute name="PACKAGE" value="SOT23-3"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM809M3-4.63" prefix="U">
<description>Microprocessor</description>
<gates>
<gate name="A" symbol="LM809M3-4.63"/>
</gates>
<devices>
<device name="" package="SOT95P250X112-3N">
<connects>
<connect gate="A" pin="GND" pad="1"/>
<connect gate="A" pin="VCC" pad="3"/>
<connect gate="A" pin="~RESET" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM809M3-4.63"/>
<attribute name="OC_FARNELL" value="9778640"/>
<attribute name="OC_NEWARK" value="96K4419"/>
<attribute name="PACKAGE" value="SOT23-3"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM8261M5" prefix="U">
<description>Op Amp</description>
<gates>
<gate name="A" symbol="LM8261M5"/>
</gates>
<devices>
<device name="" package="SOT95P284X119-5N">
<connects>
<connect gate="A" pin="NEG" pad="4"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="A" pin="POS" pad="3"/>
<connect gate="A" pin="V+" pad="5"/>
<connect gate="A" pin="V-" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM8261M5"/>
<attribute name="OC_FARNELL" value="9778853"/>
<attribute name="OC_NEWARK" value="41K6397"/>
<attribute name="PACKAGE" value="SOT23-5"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM8262MM" prefix="U">
<description>Op Amp</description>
<gates>
<gate name="A" symbol="LM8262MM"/>
</gates>
<devices>
<device name="" package="SOP65P490X110-8N">
<connects>
<connect gate="A" pin="+INA" pad="3"/>
<connect gate="A" pin="+INB" pad="5"/>
<connect gate="A" pin="-INA" pad="2"/>
<connect gate="A" pin="-INB" pad="6"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM8262MM"/>
<attribute name="OC_FARNELL" value="1312797"/>
<attribute name="OC_NEWARK" value="74C4733"/>
<attribute name="PACKAGE" value="MSOP-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM8272MM" prefix="U">
<description>Op Amp</description>
<gates>
<gate name="A" symbol="LM8272MM"/>
</gates>
<devices>
<device name="" package="SOP65P490X110-8N">
<connects>
<connect gate="A" pin="+INA" pad="3"/>
<connect gate="A" pin="+INB" pad="5"/>
<connect gate="A" pin="-INA" pad="2"/>
<connect gate="A" pin="-INB" pad="6"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM8272MM"/>
<attribute name="OC_FARNELL" value="9779183"/>
<attribute name="OC_NEWARK" value="41K6401"/>
<attribute name="PACKAGE" value="MSOP-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM833N" prefix="U">
<description>OP AMP</description>
<gates>
<gate name="A" symbol="LM833N"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-8">
<connects>
<connect gate="A" pin="+INA" pad="3"/>
<connect gate="A" pin="+INB" pad="5"/>
<connect gate="A" pin="+VCC" pad="8"/>
<connect gate="A" pin="-INA" pad="2"/>
<connect gate="A" pin="-INB" pad="6"/>
<connect gate="A" pin="-VEE" pad="4"/>
<connect gate="A" pin="OUT_A" pad="1"/>
<connect gate="A" pin="OUT_B" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM833N"/>
<attribute name="OC_FARNELL" value="9488383"/>
<attribute name="OC_NEWARK" value="89K0718"/>
<attribute name="PACKAGE" value="8-DIP"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM8364BALMF20" prefix="U">
<description>Micropower Undervoltage Sensing Circuits</description>
<gates>
<gate name="A" symbol="LM8364BALMF20"/>
</gates>
<devices>
<device name="" package="SOT95P284X122-5N">
<connects>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="IN" pad="2"/>
<connect gate="A" pin="NC" pad="4"/>
<connect gate="A" pin="NC_2" pad="5"/>
<connect gate="A" pin="~RESET" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM8364BALMF20"/>
<attribute name="OC_FARNELL" value="9779485"/>
<attribute name="OC_NEWARK" value="41K6417"/>
<attribute name="PACKAGE" value="SOT23-5"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM8365BALMF27" prefix="U">
<description>Micropower</description>
<gates>
<gate name="A" symbol="LM8365BALMF27"/>
</gates>
<devices>
<device name="" package="SOT95P284X122-5N">
<connects>
<connect gate="A" pin="CD" pad="5"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="IN" pad="2"/>
<connect gate="A" pin="NC" pad="4"/>
<connect gate="A" pin="~RESET" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM8365BALMF27"/>
<attribute name="OC_FARNELL" value="9779523"/>
<attribute name="OC_NEWARK" value="41K6424"/>
<attribute name="PACKAGE" value="SOT23-5"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM86CIMM" prefix="U">
<description>Remote diode</description>
<gates>
<gate name="A" symbol="LM86CIMM"/>
</gates>
<devices>
<device name="" package="SOP65P490X109-8N">
<connects>
<connect gate="A" pin="D+" pad="2"/>
<connect gate="A" pin="D-" pad="3"/>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="SMBCLK" pad="8"/>
<connect gate="A" pin="SMBDATA" pad="7"/>
<connect gate="A" pin="T_CRIT_A" pad="4"/>
<connect gate="A" pin="VDD" pad="1"/>
<connect gate="A" pin="~ALERT" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM86CIMM"/>
<attribute name="OC_FARNELL" value="1652474"/>
<attribute name="OC_NEWARK" value="41K6439"/>
<attribute name="PACKAGE" value="MSOP-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM9036M-5.0" prefix="U">
<description>Ultra-Low Quiescent Current Voltage Regulator</description>
<gates>
<gate name="A" symbol="LM9036M-5.0"/>
</gates>
<devices>
<device name="" package="SOIC127P620X175-8N">
<connects>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="GND_2" pad="6"/>
<connect gate="A" pin="GND_3" pad="7"/>
<connect gate="A" pin="GND_4" pad="2"/>
<connect gate="A" pin="NC" pad="5"/>
<connect gate="A" pin="NC_2" pad="4"/>
<connect gate="A" pin="VIN" pad="8"/>
<connect gate="A" pin="VOUT" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM9036M-50"/>
<attribute name="OC_FARNELL" value="1798369"/>
<attribute name="OC_NEWARK" value="41K6463"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM9036MM-3.3" prefix="U">
<description>Ultra-Low Quiescent Current Voltage Regulator</description>
<gates>
<gate name="A" symbol="LM9036MM-3.3"/>
</gates>
<devices>
<device name="" package="SOP65P490X110-8N">
<connects>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="NC" pad="6"/>
<connect gate="A" pin="NC_2" pad="2"/>
<connect gate="A" pin="NC_3" pad="3"/>
<connect gate="A" pin="NC_4" pad="4"/>
<connect gate="A" pin="NC_5" pad="5"/>
<connect gate="A" pin="VIN" pad="8"/>
<connect gate="A" pin="VOUT" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM9036MM-33"/>
<attribute name="OC_FARNELL" value="1313858"/>
<attribute name="OC_NEWARK" value="31M5491"/>
<attribute name="PACKAGE" value="MSOP-8"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM9076BMA-5.0" prefix="U">
<description>LDO Regulator</description>
<gates>
<gate name="A" symbol="LM9076BMA-5.0"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="CDELAY" pad="2"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="NC" pad="7"/>
<connect gate="A" pin="NC_2" pad="6"/>
<connect gate="A" pin="SD" pad="3"/>
<connect gate="A" pin="VIN" pad="5"/>
<connect gate="A" pin="VOUT" pad="8"/>
<connect gate="A" pin="~RESET" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM9076BMA-50"/>
<attribute name="OC_FARNELL" value="8181578"/>
<attribute name="OC_NEWARK" value="41K6487"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM9076S-3.3" prefix="U">
<description>Ultra-Low Quiescent Current LDO Regulator</description>
<gates>
<gate name="A" symbol="LM9076S-3.3"/>
</gates>
<devices>
<device name="" package="TO170P1435X457-6N">
<connects>
<connect gate="A" pin="CDELAY" pad="5"/>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="GND_2" pad="3"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="VOUT" pad="2"/>
<connect gate="A" pin="~RESET" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM9076S-3.3"/>
<attribute name="OC_FARNELL" value="1286770"/>
<attribute name="OC_NEWARK" value="99K2556"/>
<attribute name="PACKAGE" value="TO-263-5"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM9076S-5.0" prefix="U">
<description>Ultra-Low Quiescent Current LDO Regulator</description>
<gates>
<gate name="A" symbol="LM9076S-5.0"/>
</gates>
<devices>
<device name="" package="TO170P1435X457-6N">
<connects>
<connect gate="A" pin="CDELAY" pad="5"/>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="GND_2" pad="3"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="VOUT" pad="2"/>
<connect gate="A" pin="~RESET" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM9076S-50"/>
<attribute name="OC_FARNELL" value="8181586"/>
<attribute name="OC_NEWARK" value="41K6489"/>
<attribute name="PACKAGE" value="TO-263-5"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM92CIM" prefix="U">
<description>12-Bit + Sign Temperature Sensor</description>
<gates>
<gate name="A" symbol="LM92CIM"/>
</gates>
<devices>
<device name="" package="SOIC127P620X175-8N">
<connects>
<connect gate="A" pin="A0" pad="7"/>
<connect gate="A" pin="A1" pad="6"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="INT" pad="5"/>
<connect gate="A" pin="SCL" pad="2"/>
<connect gate="A" pin="SDA" pad="1"/>
<connect gate="A" pin="T_CRIT_A" pad="3"/>
<connect gate="A" pin="VS+" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM92CIM"/>
<attribute name="OC_FARNELL" value="9489711"/>
<attribute name="OC_NEWARK" value="97K3619"/>
<attribute name="PACKAGE" value="8-SOIC"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM94021BIMG" prefix="U">
<description>Multi-Gain Analog Temperature Sensor</description>
<gates>
<gate name="A" symbol="LM94021BIMG"/>
</gates>
<devices>
<device name="" package="SOT65P210X110-5N">
<connects>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="GS0" pad="1"/>
<connect gate="A" pin="GS1" pad="5"/>
<connect gate="A" pin="OUT" pad="3"/>
<connect gate="A" pin="VDD" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM94021BIMG"/>
<attribute name="OC_FARNELL" value="1047766"/>
<attribute name="OC_NEWARK" value="41K6494"/>
<attribute name="PACKAGE" value="SC-70-5"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM94022BIMG" prefix="U">
<description>Multi-Gain Analog Temperature Sensor</description>
<gates>
<gate name="A" symbol="LM94022BIMG"/>
</gates>
<devices>
<device name="" package="SOT65P210X110-5N">
<connects>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="GS0" pad="1"/>
<connect gate="A" pin="GS1" pad="5"/>
<connect gate="A" pin="OUT" pad="3"/>
<connect gate="A" pin="VDD" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM94022BIMG"/>
<attribute name="OC_FARNELL" value="1312600"/>
<attribute name="OC_NEWARK" value="65K6466"/>
<attribute name="PACKAGE" value="SC70-5"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM94022QBIMG" prefix="U">
<description>IC TEMP SENS 1.5V AB OUT</description>
<gates>
<gate name="A" symbol="LM94022QBIMG"/>
</gates>
<devices>
<device name="" package="SOT65P240X110-5N">
<connects>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="GS1" pad="5"/>
<connect gate="A" pin="GSO" pad="1"/>
<connect gate="A" pin="OUT" pad="3"/>
<connect gate="A" pin="VDD" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM94022QBIMG"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="64M7047"/>
<attribute name="PACKAGE" value="SOT-353"/>
<attribute name="SUPPLIER" value="National semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM95071CIMF" prefix="U">
<description>Temperature Sensor</description>
<gates>
<gate name="A" symbol="LM95071CIMF"/>
</gates>
<devices>
<device name="" package="SOT95P284X122-5N">
<connects>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="SC" pad="4"/>
<connect gate="A" pin="SI/O" pad="3"/>
<connect gate="A" pin="VDD" pad="5"/>
<connect gate="A" pin="~CS" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM95071CIMF"/>
<attribute name="OC_FARNELL" value="1008035"/>
<attribute name="OC_NEWARK" value="41K6498"/>
<attribute name="PACKAGE" value="SOT23-5"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM95214CISD" prefix="U">
<description>Local Temperature Sensor</description>
<gates>
<gate name="A" symbol="LM95214CISD"/>
</gates>
<devices>
<device name="" package="DFN400X400X80-15N">
<connects>
<connect gate="A" pin="A0" pad="9"/>
<connect gate="A" pin="D-" pad="5"/>
<connect gate="A" pin="D1+" pad="7"/>
<connect gate="A" pin="D2+" pad="6"/>
<connect gate="A" pin="D3+" pad="4"/>
<connect gate="A" pin="D4+" pad="3"/>
<connect gate="A" pin="EP" pad="15"/>
<connect gate="A" pin="GND" pad="8"/>
<connect gate="A" pin="NC" pad="1"/>
<connect gate="A" pin="SMBCLK" pad="13"/>
<connect gate="A" pin="SMBDAT" pad="12"/>
<connect gate="A" pin="VDD" pad="2"/>
<connect gate="A" pin="~TCRIT1" pad="10"/>
<connect gate="A" pin="~TCRIT2" pad="11"/>
<connect gate="A" pin="~TCRIT3" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM95214CISD"/>
<attribute name="OC_FARNELL" value="1342335"/>
<attribute name="OC_NEWARK" value="42M2064"/>
<attribute name="PACKAGE" value="LLP-14"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM95231CIMM" prefix="U">
<description>Precision Dual Remote Diode Temperature Sensor</description>
<gates>
<gate name="A" symbol="LM95231CIMM"/>
</gates>
<devices>
<device name="" package="SOP65P490X110-8N">
<connects>
<connect gate="A" pin="D1+" pad="1"/>
<connect gate="A" pin="D1-" pad="2"/>
<connect gate="A" pin="D2+" pad="3"/>
<connect gate="A" pin="D2-" pad="4"/>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="SMBCLK" pad="8"/>
<connect gate="A" pin="SMBDAT" pad="7"/>
<connect gate="A" pin="VDD" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM95231CIMM"/>
<attribute name="OC_FARNELL" value="1312799"/>
<attribute name="OC_NEWARK" value="31M5493"/>
<attribute name="PACKAGE" value="MSOP-8"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM95233CISD" prefix="U">
<description>Temperature Sensor</description>
<gates>
<gate name="A" symbol="LM95233CISD"/>
</gates>
<devices>
<device name="" package="DFN400X400X80-15N">
<connects>
<connect gate="A" pin="A0" pad="9"/>
<connect gate="A" pin="D-" pad="5"/>
<connect gate="A" pin="D1+" pad="7"/>
<connect gate="A" pin="D2+" pad="6"/>
<connect gate="A" pin="EP" pad="15"/>
<connect gate="A" pin="GND" pad="8"/>
<connect gate="A" pin="NC" pad="3"/>
<connect gate="A" pin="NC_2" pad="1"/>
<connect gate="A" pin="NC_3" pad="4"/>
<connect gate="A" pin="SMBCLK" pad="13"/>
<connect gate="A" pin="SMBDAT" pad="12"/>
<connect gate="A" pin="VDD" pad="2"/>
<connect gate="A" pin="~TCRIT1" pad="10"/>
<connect gate="A" pin="~TCRIT2" pad="11"/>
<connect gate="A" pin="~TCRIT3" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM95233CISD"/>
<attribute name="OC_FARNELL" value="1554778"/>
<attribute name="OC_NEWARK" value="99R8560"/>
<attribute name="PACKAGE" value="LLP-14"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM95234CISD" prefix="U">
<description>Local Temperature Sensor</description>
<gates>
<gate name="A" symbol="LM95234CISD"/>
</gates>
<devices>
<device name="" package="DFN400X400X80-15N">
<connects>
<connect gate="A" pin="A0" pad="9"/>
<connect gate="A" pin="D-" pad="5"/>
<connect gate="A" pin="D1+" pad="7"/>
<connect gate="A" pin="D2+" pad="6"/>
<connect gate="A" pin="D3+" pad="4"/>
<connect gate="A" pin="D4+" pad="3"/>
<connect gate="A" pin="EP" pad="15"/>
<connect gate="A" pin="GND" pad="8"/>
<connect gate="A" pin="NC" pad="1"/>
<connect gate="A" pin="SMBCLK" pad="13"/>
<connect gate="A" pin="SMBDAT" pad="12"/>
<connect gate="A" pin="VDD" pad="2"/>
<connect gate="A" pin="~TCRIT1" pad="10"/>
<connect gate="A" pin="~TCRIT2" pad="11"/>
<connect gate="A" pin="~TCRIT3" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM95234CISD"/>
<attribute name="OC_FARNELL" value="1554779"/>
<attribute name="OC_NEWARK" value="32M1293"/>
<attribute name="PACKAGE" value="LLP-14"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM95235CIMM" prefix="U">
<description>TempSensors</description>
<gates>
<gate name="A" symbol="LM95235CIMM"/>
</gates>
<devices>
<device name="" package="SOP65P490X109-8N">
<connects>
<connect gate="A" pin="D+" pad="2"/>
<connect gate="A" pin="D-" pad="3"/>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="SMBCLK" pad="8"/>
<connect gate="A" pin="SMBDAT" pad="7"/>
<connect gate="A" pin="VDD" pad="1"/>
<connect gate="A" pin="~OS/A0" pad="6"/>
<connect gate="A" pin="~T_CRIT" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM95235CIMM"/>
<attribute name="OC_FARNELL" value="1286991"/>
<attribute name="OC_NEWARK" value="99K2561"/>
<attribute name="PACKAGE" value="MSOP-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM95235DIMM" prefix="U">
<description>TempSensors</description>
<gates>
<gate name="A" symbol="LM95235DIMM"/>
</gates>
<devices>
<device name="" package="SOP65P490X109-8N">
<connects>
<connect gate="A" pin="D+" pad="2"/>
<connect gate="A" pin="D-" pad="3"/>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="SMBCLK" pad="8"/>
<connect gate="A" pin="SMBDAT" pad="7"/>
<connect gate="A" pin="VDD" pad="1"/>
<connect gate="A" pin="~OS/A0" pad="6"/>
<connect gate="A" pin="~T_CRIT" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM95235DIMM"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="13M1935"/>
<attribute name="PACKAGE" value="MSOP-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM95235EIMM" prefix="U">
<description>TempSensors</description>
<gates>
<gate name="A" symbol="LM95235EIMM"/>
</gates>
<devices>
<device name="" package="SOP65P490X109-8N">
<connects>
<connect gate="A" pin="D+" pad="2"/>
<connect gate="A" pin="D-" pad="3"/>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="SMBCLK" pad="8"/>
<connect gate="A" pin="SMBDAT" pad="7"/>
<connect gate="A" pin="VDD" pad="1"/>
<connect gate="A" pin="~OS/A0" pad="6"/>
<connect gate="A" pin="~T_CRIT" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM95235EIMM"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="32M1296"/>
<attribute name="PACKAGE" value="MSOP-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM95235QEIMM" prefix="U">
<description>Precision Remote Diode Temperature Sensor</description>
<gates>
<gate name="A" symbol="LM95235QEIMM"/>
</gates>
<devices>
<device name="" package="SOP65P490X109-8N">
<connects>
<connect gate="A" pin="D+" pad="2"/>
<connect gate="A" pin="D-" pad="3"/>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="SMBCLK" pad="8"/>
<connect gate="A" pin="SMBDAT" pad="7"/>
<connect gate="A" pin="VDD" pad="1"/>
<connect gate="A" pin="~OS~/A0" pad="6"/>
<connect gate="A" pin="~T_CRIT" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM95235QEIMM"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="84M8152"/>
<attribute name="PACKAGE" value="SOP-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM95245CIMM" prefix="U">
<description>Precision Remote Diode Digital Temperature Sensor</description>
<gates>
<gate name="A" symbol="LM95245CIMM"/>
</gates>
<devices>
<device name="" package="SOP65P490X110-8N">
<connects>
<connect gate="A" pin="D+" pad="2"/>
<connect gate="A" pin="D-" pad="3"/>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="SMBCLK" pad="8"/>
<connect gate="A" pin="SMBDAT" pad="7"/>
<connect gate="A" pin="VDD" pad="1"/>
<connect gate="A" pin="~OS~/A0" pad="6"/>
<connect gate="A" pin="~T_CRIT" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM95245CIMM"/>
<attribute name="OC_FARNELL" value="1554780"/>
<attribute name="OC_NEWARK" value="-"/>
<attribute name="PACKAGE" value="MSOP-8"/>
<attribute name="SUPPLIER" value="NATIONAL SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM97593VH" prefix="U">
<description>Dual ADC / Digital Tuner / AGC</description>
<gates>
<gate name="A" symbol="LM97593VH_A"/>
<gate name="B" symbol="LM97593VH_B"/>
</gates>
<devices>
<device name="" package="QFP50P1740X2340X340-128N">
<connects>
<connect gate="A" pin="A0" pad="57"/>
<connect gate="A" pin="A1" pad="56"/>
<connect gate="A" pin="A2" pad="55"/>
<connect gate="A" pin="A3" pad="54"/>
<connect gate="A" pin="A4" pad="53"/>
<connect gate="A" pin="A5" pad="52"/>
<connect gate="A" pin="A6" pad="50"/>
<connect gate="A" pin="A7" pad="48"/>
<connect gate="A" pin="AGND" pad="28"/>
<connect gate="A" pin="AGND_2" pad="20"/>
<connect gate="A" pin="AGND_3" pad="9"/>
<connect gate="A" pin="AGND_4" pad="12"/>
<connect gate="A" pin="AGND_5" pad="2"/>
<connect gate="A" pin="AGND_6" pad="18"/>
<connect gate="A" pin="BGAIN0" pad="42"/>
<connect gate="A" pin="BGAIN1" pad="41"/>
<connect gate="A" pin="BGAIN2" pad="40"/>
<connect gate="A" pin="CK" pad="37"/>
<connect gate="A" pin="D18GND" pad="44"/>
<connect gate="A" pin="D18GND_2" pad="51"/>
<connect gate="A" pin="D6" pad="63"/>
<connect gate="A" pin="D7" pad="62"/>
<connect gate="A" pin="DGND" pad="33"/>
<connect gate="A" pin="DGND_2" pad="7"/>
<connect gate="A" pin="DGND_3" pad="5"/>
<connect gate="A" pin="DGND_4" pad="32"/>
<connect gate="A" pin="DRGND" pad="61"/>
<connect gate="A" pin="DRGND_2" pad="1"/>
<connect gate="A" pin="DRGND_3" pad="47"/>
<connect gate="A" pin="NC" pad="36"/>
<connect gate="A" pin="NC_2" pad="3"/>
<connect gate="A" pin="NC_3" pad="35"/>
<connect gate="A" pin="PD" pad="30"/>
<connect gate="A" pin="REFSEL/DCS" pad="8"/>
<connect gate="A" pin="VA" pad="11"/>
<connect gate="A" pin="VA_2" pad="25"/>
<connect gate="A" pin="VA_3" pad="10"/>
<connect gate="A" pin="VA_4" pad="29"/>
<connect gate="A" pin="VA_5" pad="19"/>
<connect gate="A" pin="VCOMA" pad="24"/>
<connect gate="A" pin="VCOMA_2" pad="15"/>
<connect gate="A" pin="VD" pad="6"/>
<connect gate="A" pin="VD18" pad="49"/>
<connect gate="A" pin="VDR" pad="39"/>
<connect gate="A" pin="VDR_2" pad="64"/>
<connect gate="A" pin="VDR_3" pad="38"/>
<connect gate="A" pin="VD_2" pad="34"/>
<connect gate="A" pin="VD_3" pad="31"/>
<connect gate="A" pin="VD_4" pad="4"/>
<connect gate="A" pin="VINA+" pad="14"/>
<connect gate="A" pin="VINA-" pad="13"/>
<connect gate="A" pin="VINB+" pad="26"/>
<connect gate="A" pin="VINB-" pad="27"/>
<connect gate="A" pin="VREF" pad="21"/>
<connect gate="A" pin="VRNA" pad="17"/>
<connect gate="A" pin="VRNB" pad="22"/>
<connect gate="A" pin="VRPA" pad="16"/>
<connect gate="A" pin="VRPB" pad="23"/>
<connect gate="A" pin="~BSTROBE" pad="43"/>
<connect gate="A" pin="~CE" pad="60"/>
<connect gate="A" pin="~MR" pad="45"/>
<connect gate="A" pin="~RD" pad="59"/>
<connect gate="A" pin="~SI" pad="46"/>
<connect gate="A" pin="~WR" pad="58"/>
<connect gate="B" pin="AGAIN0" pad="125"/>
<connect gate="B" pin="AGAIN1" pad="126"/>
<connect gate="B" pin="AGAIN2" pad="127"/>
<connect gate="B" pin="AOUT" pad="82"/>
<connect gate="B" pin="BOUT" pad="78"/>
<connect gate="B" pin="D0" pad="75"/>
<connect gate="B" pin="D1" pad="73"/>
<connect gate="B" pin="D18GND" pad="120"/>
<connect gate="B" pin="D18GND_2" pad="65"/>
<connect gate="B" pin="D18GND_3" pad="103"/>
<connect gate="B" pin="D18GND_4" pad="66"/>
<connect gate="B" pin="D18GND_5" pad="76"/>
<connect gate="B" pin="D2" pad="72"/>
<connect gate="B" pin="D3" pad="71"/>
<connect gate="B" pin="D4" pad="70"/>
<connect gate="B" pin="D5" pad="69"/>
<connect gate="B" pin="DRGND" pad="68"/>
<connect gate="B" pin="DRGND_2" pad="83"/>
<connect gate="B" pin="DRGND_3" pad="110"/>
<connect gate="B" pin="DRGND_4" pad="98"/>
<connect gate="B" pin="DRGND_5" pad="89"/>
<connect gate="B" pin="NC" pad="101"/>
<connect gate="B" pin="NC_2" pad="100"/>
<connect gate="B" pin="NC_3" pad="67"/>
<connect gate="B" pin="POUT0" pad="109"/>
<connect gate="B" pin="POUT1" pad="108"/>
<connect gate="B" pin="POUT10" pad="91"/>
<connect gate="B" pin="POUT11" pad="90"/>
<connect gate="B" pin="POUT12" pad="88"/>
<connect gate="B" pin="POUT13" pad="87"/>
<connect gate="B" pin="POUT14" pad="86"/>
<connect gate="B" pin="POUT15" pad="84"/>
<connect gate="B" pin="POUT2" pad="106"/>
<connect gate="B" pin="POUT3" pad="105"/>
<connect gate="B" pin="POUT4" pad="104"/>
<connect gate="B" pin="POUT5" pad="97"/>
<connect gate="B" pin="POUT6" pad="96"/>
<connect gate="B" pin="POUT7" pad="95"/>
<connect gate="B" pin="POUT8" pad="94"/>
<connect gate="B" pin="POUT9" pad="93"/>
<connect gate="B" pin="POUT_SEL0" pad="114"/>
<connect gate="B" pin="POUT_SEL1" pad="113"/>
<connect gate="B" pin="POUT_SEL2" pad="112"/>
<connect gate="B" pin="RDY" pad="77"/>
<connect gate="B" pin="SCK" pad="80"/>
<connect gate="B" pin="SCK_IN" pad="99"/>
<connect gate="B" pin="SFS" pad="81"/>
<connect gate="B" pin="TCK" pad="119"/>
<connect gate="B" pin="TDI" pad="117"/>
<connect gate="B" pin="TDO" pad="116"/>
<connect gate="B" pin="TMS" pad="118"/>
<connect gate="B" pin="VD18" pad="74"/>
<connect gate="B" pin="VD18_2" pad="115"/>
<connect gate="B" pin="VD18_3" pad="85"/>
<connect gate="B" pin="VD18_4" pad="123"/>
<connect gate="B" pin="VDR" pad="128"/>
<connect gate="B" pin="VDR_2" pad="79"/>
<connect gate="B" pin="VDR_3" pad="102"/>
<connect gate="B" pin="VDR_4" pad="107"/>
<connect gate="B" pin="VDR_5" pad="92"/>
<connect gate="B" pin="~ASTROBE" pad="124"/>
<connect gate="B" pin="~POUT_EN" pad="111"/>
<connect gate="B" pin="~SCAN_EN" pad="122"/>
<connect gate="B" pin="~TRST" pad="121"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM97593VH"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="46M5587"/>
<attribute name="PACKAGE" value="QFP-128"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM98714BCMT" prefix="U">
<description>IC AFE 3CH 16BIT 45MSPS</description>
<gates>
<gate name="A" symbol="LM98714BCMT"/>
</gates>
<devices>
<device name="" package="SOP50P810X110-48N">
<connects>
<connect gate="A" pin="AGND" pad="24"/>
<connect gate="A" pin="AGND_2" pad="10"/>
<connect gate="A" pin="AGND_3" pad="15"/>
<connect gate="A" pin="AGND_4" pad="18"/>
<connect gate="A" pin="AGND_5" pad="20"/>
<connect gate="A" pin="AGND_6" pad="22"/>
<connect gate="A" pin="CLK4" pad="48"/>
<connect gate="A" pin="CLK5" pad="45"/>
<connect gate="A" pin="CLK6" pad="44"/>
<connect gate="A" pin="CLK7" pad="43"/>
<connect gate="A" pin="CLK8" pad="42"/>
<connect gate="A" pin="CLK9" pad="41"/>
<connect gate="A" pin="CLKOUT/CLK10" pad="40"/>
<connect gate="A" pin="CLK_1" pad="3"/>
<connect gate="A" pin="CLK_2" pad="2"/>
<connect gate="A" pin="CLK_3" pad="1"/>
<connect gate="A" pin="DGND" pad="46"/>
<connect gate="A" pin="DGND_2" pad="25"/>
<connect gate="A" pin="DGND_3" pad="38"/>
<connect gate="A" pin="DOUT0/TXOUT0-" pad="37"/>
<connect gate="A" pin="DOUT1/TXOUT0+" pad="36"/>
<connect gate="A" pin="DOUT2/TXOUT1-" pad="35"/>
<connect gate="A" pin="DOUT3/TXOUT1+" pad="34"/>
<connect gate="A" pin="DOUT4/TXOUT2-" pad="33"/>
<connect gate="A" pin="DOUT5/TXOUT2+" pad="32"/>
<connect gate="A" pin="DOUT6/TXCLK-" pad="31"/>
<connect gate="A" pin="DOUT7/TXCLK+" pad="30"/>
<connect gate="A" pin="DVB" pad="27"/>
<connect gate="A" pin="INCLK+" pad="28"/>
<connect gate="A" pin="INCLK-" pad="29"/>
<connect gate="A" pin="OSB" pad="23"/>
<connect gate="A" pin="OSG" pad="21"/>
<connect gate="A" pin="OSR" pad="19"/>
<connect gate="A" pin="SCLK" pad="8"/>
<connect gate="A" pin="SDIO" pad="7"/>
<connect gate="A" pin="SH" pad="4"/>
<connect gate="A" pin="SH_R" pad="6"/>
<connect gate="A" pin="VA" pad="17"/>
<connect gate="A" pin="VA_2" pad="11"/>
<connect gate="A" pin="VA_3" pad="14"/>
<connect gate="A" pin="VC" pad="47"/>
<connect gate="A" pin="VCLP" pad="16"/>
<connect gate="A" pin="VD" pad="39"/>
<connect gate="A" pin="VR" pad="26"/>
<connect gate="A" pin="VREFB" pad="12"/>
<connect gate="A" pin="VREFT" pad="13"/>
<connect gate="A" pin="~RESET" pad="5"/>
<connect gate="A" pin="~SEN" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM98714BCMT"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="95M8828"/>
<attribute name="PACKAGE" value="48-TSSOP"/>
<attribute name="SUPPLIER" value="National semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM98722CCMT">
<description>IC AFE 16BIT 3CH 45MSPS</description>
<gates>
<gate name="A" symbol="LM98722CCMT"/>
</gates>
<devices>
<device name="" package="SOP50P810X110-56N">
<connects>
<connect gate="A" pin="*RESET" pad="6"/>
<connect gate="A" pin="*SEN" pad="11"/>
<connect gate="A" pin="AGND" pad="18"/>
<connect gate="A" pin="AGND_2" pad="13"/>
<connect gate="A" pin="AGND_3" pad="22"/>
<connect gate="A" pin="AGND_4" pad="26"/>
<connect gate="A" pin="AGND_5" pad="24"/>
<connect gate="A" pin="CAL" pad="5"/>
<connect gate="A" pin="CE" pad="4"/>
<connect gate="A" pin="CLKOUT/SH2" pad="45"/>
<connect gate="A" pin="CP" pad="48"/>
<connect gate="A" pin="CPOFILT1" pad="30"/>
<connect gate="A" pin="CPOFILT2" pad="28"/>
<connect gate="A" pin="DGND" pad="29"/>
<connect gate="A" pin="DGND_2" pad="51"/>
<connect gate="A" pin="DGND_3" pad="42"/>
<connect gate="A" pin="DOUT0/TXOUT0-" pad="41"/>
<connect gate="A" pin="DOUT1/TXOUT0+" pad="40"/>
<connect gate="A" pin="DOUT2/TXOUT1-" pad="39"/>
<connect gate="A" pin="DOUT3/TXOUT1+" pad="38"/>
<connect gate="A" pin="DOUT4/TXOUT2-" pad="37"/>
<connect gate="A" pin="DOUT5/TXOUT2+" pad="36"/>
<connect gate="A" pin="DOUT6/TXCLK-" pad="35"/>
<connect gate="A" pin="DOUT7/TXCLK+" pad="34"/>
<connect gate="A" pin="DVB" pad="31"/>
<connect gate="A" pin="IBIAS" pad="21"/>
<connect gate="A" pin="INCLK+" pad="32"/>
<connect gate="A" pin="INCLK-" pad="33"/>
<connect gate="A" pin="OSB" pad="27"/>
<connect gate="A" pin="OSG" pad="25"/>
<connect gate="A" pin="OSR" pad="23"/>
<connect gate="A" pin="PHIA1" pad="49"/>
<connect gate="A" pin="PHIA2" pad="50"/>
<connect gate="A" pin="PHIB1" pad="53"/>
<connect gate="A" pin="PHIB2" pad="54"/>
<connect gate="A" pin="PHIC1" pad="2"/>
<connect gate="A" pin="PHIC2" pad="1"/>
<connect gate="A" pin="RS" pad="47"/>
<connect gate="A" pin="SCLK" pad="10"/>
<connect gate="A" pin="SDI" pad="8"/>
<connect gate="A" pin="SDO" pad="9"/>
<connect gate="A" pin="SH1" pad="3"/>
<connect gate="A" pin="SH3" pad="46"/>
<connect gate="A" pin="SH4" pad="55"/>
<connect gate="A" pin="SH5" pad="56"/>
<connect gate="A" pin="SH_R" pad="7"/>
<connect gate="A" pin="VA" pad="20"/>
<connect gate="A" pin="VA_2" pad="12"/>
<connect gate="A" pin="VA_3" pad="14"/>
<connect gate="A" pin="VA_4" pad="17"/>
<connect gate="A" pin="VC" pad="44"/>
<connect gate="A" pin="VCLP" pad="19"/>
<connect gate="A" pin="VC_2" pad="52"/>
<connect gate="A" pin="VD" pad="43"/>
<connect gate="A" pin="VREFB" pad="15"/>
<connect gate="A" pin="VREFT" pad="16"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM98722CCMT"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="55R4143"/>
<attribute name="PACKAGE" value="56-TSSOP"/>
<attribute name="SUPPLIER" value="National semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM98725CCMT">
<description>IC TIMING GENERATOR/SSCG</description>
<gates>
<gate name="A" symbol="LM98725CCMT"/>
</gates>
<devices>
<device name="" package="SOP50P810X110-56N">
<connects>
<connect gate="A" pin="*RESET" pad="6"/>
<connect gate="A" pin="*SEN" pad="11"/>
<connect gate="A" pin="AGND" pad="18"/>
<connect gate="A" pin="AGND_2" pad="13"/>
<connect gate="A" pin="AGND_3" pad="22"/>
<connect gate="A" pin="AGND_4" pad="26"/>
<connect gate="A" pin="AGND_5" pad="24"/>
<connect gate="A" pin="CAL" pad="5"/>
<connect gate="A" pin="CE" pad="4"/>
<connect gate="A" pin="CLKOUT/SH2" pad="45"/>
<connect gate="A" pin="CP" pad="48"/>
<connect gate="A" pin="CPOFILT1" pad="30"/>
<connect gate="A" pin="CPOFILT2" pad="28"/>
<connect gate="A" pin="DGND" pad="29"/>
<connect gate="A" pin="DGND_2" pad="51"/>
<connect gate="A" pin="DGND_3" pad="42"/>
<connect gate="A" pin="DOUT0/TXOUT0-" pad="41"/>
<connect gate="A" pin="DOUT1/TXOUT0+" pad="40"/>
<connect gate="A" pin="DOUT2/TXOUT1-" pad="39"/>
<connect gate="A" pin="DOUT3/TXOUT1+" pad="38"/>
<connect gate="A" pin="DOUT4/TXOUT2-" pad="37"/>
<connect gate="A" pin="DOUT5/TXOUT2+" pad="36"/>
<connect gate="A" pin="DOUT6/TXCLK-" pad="35"/>
<connect gate="A" pin="DOUT7/TXCLK+" pad="34"/>
<connect gate="A" pin="DVB" pad="31"/>
<connect gate="A" pin="IBIAS" pad="21"/>
<connect gate="A" pin="INCLK+" pad="32"/>
<connect gate="A" pin="INCLK-" pad="33"/>
<connect gate="A" pin="OSB" pad="27"/>
<connect gate="A" pin="OSG" pad="25"/>
<connect gate="A" pin="OSR" pad="23"/>
<connect gate="A" pin="PHIA1" pad="49"/>
<connect gate="A" pin="PHIA2" pad="50"/>
<connect gate="A" pin="PHIB1" pad="53"/>
<connect gate="A" pin="PHIB2" pad="54"/>
<connect gate="A" pin="PHIC1" pad="2"/>
<connect gate="A" pin="PHIC2" pad="1"/>
<connect gate="A" pin="RS" pad="47"/>
<connect gate="A" pin="SCLK" pad="10"/>
<connect gate="A" pin="SDI" pad="8"/>
<connect gate="A" pin="SDO" pad="9"/>
<connect gate="A" pin="SH1" pad="3"/>
<connect gate="A" pin="SH3" pad="46"/>
<connect gate="A" pin="SH4" pad="55"/>
<connect gate="A" pin="SH5" pad="56"/>
<connect gate="A" pin="SH_R" pad="7"/>
<connect gate="A" pin="VA" pad="20"/>
<connect gate="A" pin="VA_2" pad="12"/>
<connect gate="A" pin="VA_3" pad="14"/>
<connect gate="A" pin="VA_4" pad="17"/>
<connect gate="A" pin="VC" pad="44"/>
<connect gate="A" pin="VCLP" pad="19"/>
<connect gate="A" pin="VC_2" pad="52"/>
<connect gate="A" pin="VD" pad="43"/>
<connect gate="A" pin="VREFB" pad="15"/>
<connect gate="A" pin="VREFT" pad="16"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM98725CCMT"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="04R9323"/>
<attribute name="PACKAGE" value="56-TSSOP"/>
<attribute name="SUPPLIER" value="National semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM99CIMM" prefix="U">
<description>Diode Temperature Sensor</description>
<gates>
<gate name="A" symbol="LM99CIMM"/>
</gates>
<devices>
<device name="" package="SOP65P490X109-8N">
<connects>
<connect gate="A" pin="D+" pad="2"/>
<connect gate="A" pin="D-" pad="3"/>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="SMBCLK" pad="8"/>
<connect gate="A" pin="SMBDATA" pad="7"/>
<connect gate="A" pin="VDD" pad="1"/>
<connect gate="A" pin="~ALERT" pad="6"/>
<connect gate="A" pin="~T_CRIT_A" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM99CIMM"/>
<attribute name="OC_FARNELL" value="1312805"/>
<attribute name="OC_NEWARK" value="41K6508"/>
<attribute name="PACKAGE" value="8-MSOP"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMC6001AIN" prefix="U">
<description>OpAmpIC</description>
<gates>
<gate name="A" symbol="LMC6001AIN"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-8">
<connects>
<connect gate="A" pin="NC" pad="8"/>
<connect gate="A" pin="NC_2" pad="1"/>
<connect gate="A" pin="NC_3" pad="5"/>
<connect gate="A" pin="NEG" pad="2"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="POS" pad="3"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMC6001AIN"/>
<attribute name="OC_FARNELL" value="1468879"/>
<attribute name="OC_NEWARK" value="07B5573"/>
<attribute name="PACKAGE" value="DIP-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMC6001BIN" prefix="U">
<description>OpAmpIC</description>
<gates>
<gate name="A" symbol="LMC6001BIN"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-8">
<connects>
<connect gate="A" pin="NC" pad="8"/>
<connect gate="A" pin="NC_2" pad="1"/>
<connect gate="A" pin="NC_3" pad="5"/>
<connect gate="A" pin="NEG" pad="2"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="POS" pad="3"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMC6001BIN"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="07B5574"/>
<attribute name="PACKAGE" value="DIP-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMC6024IM" prefix="U">
<description>OpAmpIC</description>
<gates>
<gate name="A" symbol="LMC6024IM"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="NEG1" pad="2"/>
<connect gate="A" pin="NEG2" pad="6"/>
<connect gate="A" pin="NEG3" pad="9"/>
<connect gate="A" pin="NEG4" pad="13"/>
<connect gate="A" pin="OUT1" pad="1"/>
<connect gate="A" pin="OUT2" pad="7"/>
<connect gate="A" pin="OUT3" pad="8"/>
<connect gate="A" pin="OUT4" pad="14"/>
<connect gate="A" pin="POS1" pad="3"/>
<connect gate="A" pin="POS2" pad="5"/>
<connect gate="A" pin="POS3" pad="10"/>
<connect gate="A" pin="POS4" pad="12"/>
<connect gate="A" pin="V+" pad="4"/>
<connect gate="A" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMC6024IM"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="07B5580"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMC6032IM" prefix="U">
<description>OpAmpIC</description>
<gates>
<gate name="A" symbol="LMC6032IM"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="NEGA" pad="2"/>
<connect gate="A" pin="NEGB" pad="6"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="POSA" pad="3"/>
<connect gate="A" pin="POSB" pad="5"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMC6032IM"/>
<attribute name="OC_FARNELL" value="1468880"/>
<attribute name="OC_NEWARK" value="07B5582"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMC6032IN" prefix="U">
<description>OpAmpIC</description>
<gates>
<gate name="A" symbol="LMC6032IN"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-8">
<connects>
<connect gate="A" pin="NEGA" pad="2"/>
<connect gate="A" pin="NEGB" pad="6"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="POSA" pad="3"/>
<connect gate="A" pin="POSB" pad="5"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMC6032IN"/>
<attribute name="OC_FARNELL" value="1258309"/>
<attribute name="OC_NEWARK" value="92F334"/>
<attribute name="PACKAGE" value="DIP-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMC6034IM" prefix="U">
<description>OpAmpIC</description>
<gates>
<gate name="A" symbol="LMC6034IM"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="NEG1" pad="2"/>
<connect gate="A" pin="NEG2" pad="6"/>
<connect gate="A" pin="NEG3" pad="9"/>
<connect gate="A" pin="NEG4" pad="13"/>
<connect gate="A" pin="OUT1" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="OUTC" pad="8"/>
<connect gate="A" pin="OUTD" pad="14"/>
<connect gate="A" pin="POS1" pad="3"/>
<connect gate="A" pin="POS2" pad="5"/>
<connect gate="A" pin="POS3" pad="10"/>
<connect gate="A" pin="POS4" pad="12"/>
<connect gate="A" pin="V+" pad="4"/>
<connect gate="A" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMC6034IM"/>
<attribute name="OC_FARNELL" value="1564727"/>
<attribute name="OC_NEWARK" value="41K2581"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMC6035IM" prefix="U">
<description>OpAmpIC</description>
<gates>
<gate name="A" symbol="LMC6035IM"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="NEGA" pad="2"/>
<connect gate="A" pin="NEGB" pad="6"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="POSA" pad="3"/>
<connect gate="A" pin="POSB" pad="5"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMC6035IM"/>
<attribute name="OC_FARNELL" value="9494286"/>
<attribute name="OC_NEWARK" value="97K3094"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMC6035IMM" prefix="U">
<description>OpAmpIC</description>
<gates>
<gate name="A" symbol="LMC6035IMM"/>
</gates>
<devices>
<device name="" package="SOP65P490X109-8N">
<connects>
<connect gate="A" pin="NEGA" pad="2"/>
<connect gate="A" pin="NEGB" pad="6"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="POSA" pad="3"/>
<connect gate="A" pin="POSB" pad="5"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMC6035IMM"/>
<attribute name="OC_FARNELL" value="1694505"/>
<attribute name="OC_NEWARK" value="07B5586"/>
<attribute name="PACKAGE" value="MSOP-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMC6036IM" prefix="U">
<description>OpAmpIC</description>
<gates>
<gate name="A" symbol="LMC6036IM"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="+INA" pad="3"/>
<connect gate="A" pin="+INB" pad="5"/>
<connect gate="A" pin="+INC" pad="10"/>
<connect gate="A" pin="+IND" pad="12"/>
<connect gate="A" pin="-INA" pad="2"/>
<connect gate="A" pin="-INB" pad="6"/>
<connect gate="A" pin="-INC" pad="9"/>
<connect gate="A" pin="-IND" pad="13"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="OUTC" pad="8"/>
<connect gate="A" pin="OUTD" pad="14"/>
<connect gate="A" pin="V+" pad="4"/>
<connect gate="A" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMC6036IM"/>
<attribute name="OC_FARNELL" value="9494294"/>
<attribute name="OC_NEWARK" value="92F337"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMC6041AIM" prefix="U">
<description>OpAmpIC</description>
<gates>
<gate name="A" symbol="LMC6041AIM"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="NC" pad="8"/>
<connect gate="A" pin="NC_2" pad="5"/>
<connect gate="A" pin="NC_3" pad="1"/>
<connect gate="A" pin="NEG" pad="2"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="POS" pad="3"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMC6041AIM"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="07B5591"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMC6041IM" prefix="U">
<description>OpAmpIC</description>
<gates>
<gate name="A" symbol="LMC6041IM"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="NC" pad="8"/>
<connect gate="A" pin="NC_2" pad="5"/>
<connect gate="A" pin="NC_3" pad="1"/>
<connect gate="A" pin="NEG" pad="2"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="POS" pad="3"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMC6041IM"/>
<attribute name="OC_FARNELL" value="1798370"/>
<attribute name="OC_NEWARK" value="07B5593"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMC6041IN" prefix="U">
<description>OpAmpIC</description>
<gates>
<gate name="A" symbol="LMC6041IN"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-8">
<connects>
<connect gate="A" pin="NC" pad="8"/>
<connect gate="A" pin="NC_2" pad="5"/>
<connect gate="A" pin="NC_3" pad="1"/>
<connect gate="A" pin="NEG" pad="2"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="POS" pad="3"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMC6041IN"/>
<attribute name="OC_FARNELL" value="1468882"/>
<attribute name="OC_NEWARK" value="07B5595"/>
<attribute name="PACKAGE" value="DIP-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMC6042AIM" prefix="U">
<description>OpAmpIC</description>
<gates>
<gate name="A" symbol="LMC6042AIM"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="NEGA" pad="2"/>
<connect gate="A" pin="NEGB" pad="6"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="POSA" pad="3"/>
<connect gate="A" pin="POSB" pad="5"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMC6042AIM"/>
<attribute name="OC_FARNELL" value="9494596"/>
<attribute name="OC_NEWARK" value="07B5596"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMC6042IM" prefix="U">
<description>OpAmpIC</description>
<gates>
<gate name="A" symbol="LMC6042IM"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="NEGA" pad="2"/>
<connect gate="A" pin="NEGB" pad="6"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="POSA" pad="3"/>
<connect gate="A" pin="POSB" pad="5"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMC6042IM"/>
<attribute name="OC_FARNELL" value="9494600"/>
<attribute name="OC_NEWARK" value="07B5599"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMC6042IN" prefix="U">
<description>OP AMP</description>
<gates>
<gate name="A" symbol="LMC6042IN"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-8">
<connects>
<connect gate="A" pin="NEG_A" pad="2"/>
<connect gate="A" pin="NEG_B" pad="6"/>
<connect gate="A" pin="OUT_A" pad="1"/>
<connect gate="A" pin="OUT_B" pad="7"/>
<connect gate="A" pin="POS_A" pad="3"/>
<connect gate="A" pin="POS_B" pad="5"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMC6042IN"/>
<attribute name="OC_FARNELL" value="9494618"/>
<attribute name="OC_NEWARK" value="97K3098"/>
<attribute name="PACKAGE" value="8-DIP"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMC6044IM" prefix="U">
<description>OpAmpIC</description>
<gates>
<gate name="A" symbol="LMC6044IM"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="NEG1" pad="2"/>
<connect gate="A" pin="NEG2" pad="6"/>
<connect gate="A" pin="NEG3" pad="9"/>
<connect gate="A" pin="NEG4" pad="13"/>
<connect gate="A" pin="OUT1" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="OUTC" pad="8"/>
<connect gate="A" pin="OUTD" pad="14"/>
<connect gate="A" pin="POS1" pad="3"/>
<connect gate="A" pin="POS2" pad="5"/>
<connect gate="A" pin="POS3" pad="10"/>
<connect gate="A" pin="POS4" pad="12"/>
<connect gate="A" pin="V+" pad="4"/>
<connect gate="A" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMC6044IM"/>
<attribute name="OC_FARNELL" value="9494626"/>
<attribute name="OC_NEWARK" value="97K3099"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMC6044IN" prefix="U">
<description>OP AMP</description>
<gates>
<gate name="A" symbol="LMC6044IN"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-14">
<connects>
<connect gate="A" pin="NEG_1" pad="2"/>
<connect gate="A" pin="NEG_2" pad="6"/>
<connect gate="A" pin="NEG_3" pad="9"/>
<connect gate="A" pin="NEG_4" pad="13"/>
<connect gate="A" pin="OUT_1" pad="1"/>
<connect gate="A" pin="OUT_2" pad="7"/>
<connect gate="A" pin="OUT_3" pad="8"/>
<connect gate="A" pin="OUT_4" pad="14"/>
<connect gate="A" pin="POS_1" pad="3"/>
<connect gate="A" pin="POS_2" pad="5"/>
<connect gate="A" pin="POS_3" pad="10"/>
<connect gate="A" pin="POS_4" pad="12"/>
<connect gate="A" pin="V+" pad="4"/>
<connect gate="A" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMC6044IN"/>
<attribute name="OC_FARNELL" value="9494634"/>
<attribute name="OC_NEWARK" value="97K3100"/>
<attribute name="PACKAGE" value="14-DIP"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMC6061AIM" prefix="U">
<description>OpAmpIC</description>
<gates>
<gate name="A" symbol="LMC6061AIM"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="NEGA" pad="2"/>
<connect gate="A" pin="NEGB" pad="6"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="POSA" pad="3"/>
<connect gate="A" pin="POSB" pad="5"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMC6061AIM"/>
<attribute name="OC_FARNELL" value="9494642"/>
<attribute name="OC_NEWARK" value="41K2610"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMC6061IM" prefix="U">
<description>OpAmpIC</description>
<gates>
<gate name="A" symbol="LMC6061IM"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="NEGA" pad="2"/>
<connect gate="A" pin="NEGB" pad="6"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="POSA" pad="3"/>
<connect gate="A" pin="POSB" pad="5"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMC6061IM"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="07B5609"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMC6062AIM" prefix="U">
<description>OpAmpIC</description>
<gates>
<gate name="A" symbol="LMC6062AIM"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="NEGA" pad="2"/>
<connect gate="A" pin="NEGB" pad="6"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="POSA" pad="3"/>
<connect gate="A" pin="POSB" pad="5"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMC6062AIM"/>
<attribute name="OC_FARNELL" value="1685330"/>
<attribute name="OC_NEWARK" value="41K2614"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMC6062IM" prefix="U">
<description>OpAmpIC</description>
<gates>
<gate name="A" symbol="LMC6062IM"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="NEGA" pad="2"/>
<connect gate="A" pin="NEGB" pad="6"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="POSA" pad="3"/>
<connect gate="A" pin="POSB" pad="5"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMC6062IM"/>
<attribute name="OC_FARNELL" value="9494669"/>
<attribute name="OC_NEWARK" value="41K2616"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMC6062IN" prefix="U">
<description>OP AMP</description>
<gates>
<gate name="A" symbol="LMC6062IN"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-8">
<connects>
<connect gate="A" pin="NEG_A" pad="2"/>
<connect gate="A" pin="NEG_B" pad="6"/>
<connect gate="A" pin="OUT_A" pad="1"/>
<connect gate="A" pin="OUT_B" pad="7"/>
<connect gate="A" pin="POS_A" pad="3"/>
<connect gate="A" pin="POS_B" pad="5"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMC6062IN"/>
<attribute name="OC_FARNELL" value="9486003"/>
<attribute name="OC_NEWARK" value="41K2618"/>
<attribute name="PACKAGE" value="8-DIP"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMC6064AIM" prefix="U">
<description>OpAmpIC</description>
<gates>
<gate name="A" symbol="LMC6064AIM"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="NEG1" pad="2"/>
<connect gate="A" pin="NEG2" pad="6"/>
<connect gate="A" pin="NEG3" pad="9"/>
<connect gate="A" pin="NEG4" pad="13"/>
<connect gate="A" pin="OUT1" pad="1"/>
<connect gate="A" pin="OUT2" pad="7"/>
<connect gate="A" pin="OUT3" pad="8"/>
<connect gate="A" pin="OUTD" pad="14"/>
<connect gate="A" pin="POS1" pad="3"/>
<connect gate="A" pin="POS2" pad="5"/>
<connect gate="A" pin="POS3" pad="10"/>
<connect gate="A" pin="POS4" pad="12"/>
<connect gate="A" pin="V+" pad="4"/>
<connect gate="A" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMC6064AIM"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="07B5616"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMC6064IM" prefix="U">
<description>OpAmpIC</description>
<gates>
<gate name="A" symbol="LMC6064IM"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="NEG1" pad="2"/>
<connect gate="A" pin="NEG2" pad="6"/>
<connect gate="A" pin="NEG3" pad="9"/>
<connect gate="A" pin="NEG4" pad="13"/>
<connect gate="A" pin="OUT1" pad="1"/>
<connect gate="A" pin="OUT2" pad="7"/>
<connect gate="A" pin="OUT3" pad="8"/>
<connect gate="A" pin="OUTD" pad="14"/>
<connect gate="A" pin="POS1" pad="3"/>
<connect gate="A" pin="POS2" pad="5"/>
<connect gate="A" pin="POS3" pad="10"/>
<connect gate="A" pin="POS4" pad="12"/>
<connect gate="A" pin="V+" pad="4"/>
<connect gate="A" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMC6064IM"/>
<attribute name="OC_FARNELL" value="1685346"/>
<attribute name="OC_NEWARK" value="47T5167"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMC6064IN" prefix="U">
<description>OP Amps</description>
<gates>
<gate name="A" symbol="LMC6064IN"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-14">
<connects>
<connect gate="A" pin="NEG1" pad="2"/>
<connect gate="A" pin="NEG2" pad="6"/>
<connect gate="A" pin="NEG3" pad="9"/>
<connect gate="A" pin="NEG4" pad="13"/>
<connect gate="A" pin="OUT1" pad="1"/>
<connect gate="A" pin="OUT2" pad="7"/>
<connect gate="A" pin="OUT3" pad="8"/>
<connect gate="A" pin="OUT4" pad="14"/>
<connect gate="A" pin="POS1" pad="3"/>
<connect gate="A" pin="POS2" pad="5"/>
<connect gate="A" pin="POS3" pad="10"/>
<connect gate="A" pin="POS4" pad="12"/>
<connect gate="A" pin="V+" pad="4"/>
<connect gate="A" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMC6064IN"/>
<attribute name="OC_FARNELL" value="9486089"/>
<attribute name="OC_NEWARK" value="92F343"/>
<attribute name="PACKAGE" value="14- DIP"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMC6081AIM" prefix="U">
<description>OpAmpIC</description>
<gates>
<gate name="A" symbol="LMC6081AIM"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="NC" pad="8"/>
<connect gate="A" pin="NC_2" pad="1"/>
<connect gate="A" pin="NC_3" pad="5"/>
<connect gate="A" pin="NEG" pad="2"/>
<connect gate="A" pin="OUTB" pad="6"/>
<connect gate="A" pin="POS" pad="3"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMC6081AIM"/>
<attribute name="OC_FARNELL" value="1215211"/>
<attribute name="OC_NEWARK" value="41K2624"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMC6081IM" prefix="U">
<description>OpAmpIC</description>
<gates>
<gate name="A" symbol="LMC6081IM"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="NC" pad="8"/>
<connect gate="A" pin="NC_2" pad="1"/>
<connect gate="A" pin="NC_3" pad="5"/>
<connect gate="A" pin="NEG" pad="2"/>
<connect gate="A" pin="OUTB" pad="6"/>
<connect gate="A" pin="POS" pad="3"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMC6081IM"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="07B5623"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMC6081IN" prefix="U">
<description>OpAmpIC</description>
<gates>
<gate name="A" symbol="LMC6081IN"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-8">
<connects>
<connect gate="A" pin="NC" pad="8"/>
<connect gate="A" pin="NC_2" pad="1"/>
<connect gate="A" pin="NC_3" pad="5"/>
<connect gate="A" pin="NEG" pad="2"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="POS" pad="3"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMC6081IN"/>
<attribute name="OC_FARNELL" value="1564618"/>
<attribute name="OC_NEWARK" value="41K2628"/>
<attribute name="PACKAGE" value="DIP-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMC6082AIM" prefix="U">
<description>OpAmpIC</description>
<gates>
<gate name="A" symbol="LMC6082AIM"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="NEGA" pad="2"/>
<connect gate="A" pin="NEGB" pad="6"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="POSA" pad="3"/>
<connect gate="A" pin="POSB" pad="5"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMC6082AIM"/>
<attribute name="OC_FARNELL" value="9494677"/>
<attribute name="OC_NEWARK" value="41K2629"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMC6082AIN" prefix="U">
<description>Literature Number</description>
<gates>
<gate name="A" symbol="LMC6082AIN"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-8">
<connects>
<connect gate="A" pin="NEG_A" pad="2"/>
<connect gate="A" pin="NEG_B" pad="6"/>
<connect gate="A" pin="OUT_A" pad="1"/>
<connect gate="A" pin="OUT_B" pad="7"/>
<connect gate="A" pin="POS_A" pad="3"/>
<connect gate="A" pin="POS_B" pad="5"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMC6082AIN"/>
<attribute name="OC_FARNELL" value="9494685"/>
<attribute name="OC_NEWARK" value="41K2631"/>
<attribute name="PACKAGE" value="8-DIP"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMC6082IM" prefix="U">
<description>OpAmpIC</description>
<gates>
<gate name="A" symbol="LMC6082IM"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="NEGA" pad="2"/>
<connect gate="A" pin="NEGB" pad="6"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="POSA" pad="3"/>
<connect gate="A" pin="POSB" pad="5"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMC6082IM"/>
<attribute name="OC_FARNELL" value="9494693"/>
<attribute name="OC_NEWARK" value="07B5628"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMC6082IN" prefix="U">
<description>OpAmpIC</description>
<gates>
<gate name="A" symbol="LMC6082IN"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-8">
<connects>
<connect gate="A" pin="NEGA" pad="2"/>
<connect gate="A" pin="NEGB" pad="6"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="POSA" pad="3"/>
<connect gate="A" pin="POSB" pad="5"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMC6082IN"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K2634"/>
<attribute name="PACKAGE" value="DIP-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMC6084AIM" prefix="U">
<description>Operational Amplifier</description>
<gates>
<gate name="A" symbol="LMC6084AIM"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="NEG1" pad="2"/>
<connect gate="A" pin="NEG2" pad="6"/>
<connect gate="A" pin="NEG3" pad="9"/>
<connect gate="A" pin="NEG4" pad="13"/>
<connect gate="A" pin="OUT1" pad="1"/>
<connect gate="A" pin="OUT2" pad="7"/>
<connect gate="A" pin="OUT3" pad="8"/>
<connect gate="A" pin="OUT4" pad="14"/>
<connect gate="A" pin="POS1" pad="3"/>
<connect gate="A" pin="POS2" pad="5"/>
<connect gate="A" pin="POS3" pad="10"/>
<connect gate="A" pin="POS4" pad="12"/>
<connect gate="A" pin="V+" pad="4"/>
<connect gate="A" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMC6084AIM"/>
<attribute name="OC_FARNELL" value="1215212"/>
<attribute name="OC_NEWARK" value="41K2635"/>
<attribute name="PACKAGE" value="14-SOIC"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMC6084IM" prefix="U">
<description>OpAmpIC</description>
<gates>
<gate name="A" symbol="LMC6084IM"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="NEG1" pad="2"/>
<connect gate="A" pin="NEG2" pad="6"/>
<connect gate="A" pin="NEG3" pad="9"/>
<connect gate="A" pin="NEG4" pad="13"/>
<connect gate="A" pin="OUT1" pad="1"/>
<connect gate="A" pin="OUT2" pad="7"/>
<connect gate="A" pin="OUT3" pad="8"/>
<connect gate="A" pin="OUTD" pad="14"/>
<connect gate="A" pin="POS1" pad="3"/>
<connect gate="A" pin="POS2" pad="5"/>
<connect gate="A" pin="POS3" pad="10"/>
<connect gate="A" pin="POS4" pad="12"/>
<connect gate="A" pin="V+" pad="4"/>
<connect gate="A" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMC6084IM"/>
<attribute name="OC_FARNELL" value="9494707"/>
<attribute name="OC_NEWARK" value="07B5633"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMC6442AIM" prefix="U">
<description>OpAmpIC</description>
<gates>
<gate name="A" symbol="LMC6442AIM"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="+INA" pad="3"/>
<connect gate="A" pin="+INB" pad="5"/>
<connect gate="A" pin="-INA" pad="2"/>
<connect gate="A" pin="-INB" pad="6"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMC6442AIM"/>
<attribute name="OC_FARNELL" value="1468884"/>
<attribute name="OC_NEWARK" value="41K2639"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMC6442IN" prefix="U">
<description>OpAmpIC</description>
<gates>
<gate name="A" symbol="LMC6442IN"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-8">
<connects>
<connect gate="A" pin="+INA" pad="3"/>
<connect gate="A" pin="+INB" pad="5"/>
<connect gate="A" pin="-INA" pad="2"/>
<connect gate="A" pin="-INB" pad="6"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMC6442IN"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="83F3825"/>
<attribute name="PACKAGE" value="DIP-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMC6462AIM" prefix="U">
<description>OpAmpIC</description>
<gates>
<gate name="A" symbol="LMC6462AIM"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="+INA" pad="3"/>
<connect gate="A" pin="+INB" pad="5"/>
<connect gate="A" pin="-INA" pad="2"/>
<connect gate="A" pin="-INB" pad="6"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMC6462AIM"/>
<attribute name="OC_FARNELL" value="9494715"/>
<attribute name="OC_NEWARK" value="97K3111"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMC6462AIN" prefix="U">
<description>OP AMP</description>
<gates>
<gate name="A" symbol="LMC6462AIN"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-8">
<connects>
<connect gate="A" pin="IN_A+" pad="3"/>
<connect gate="A" pin="IN_A-" pad="2"/>
<connect gate="A" pin="IN_B+" pad="5"/>
<connect gate="A" pin="IN_B-" pad="6"/>
<connect gate="A" pin="OUT_A" pad="1"/>
<connect gate="A" pin="OUT_B" pad="7"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMC6462AIN"/>
<attribute name="OC_FARNELL" value="9494588"/>
<attribute name="OC_NEWARK" value="92F347"/>
<attribute name="PACKAGE" value="8-DIP"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMC6462BIM" prefix="U">
<description>OpAmpIC</description>
<gates>
<gate name="A" symbol="LMC6462BIM"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="+INA" pad="3"/>
<connect gate="A" pin="+INB" pad="5"/>
<connect gate="A" pin="-INA" pad="2"/>
<connect gate="A" pin="-INB" pad="6"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMC6462BIM"/>
<attribute name="OC_FARNELL" value="1468886"/>
<attribute name="OC_NEWARK" value="07B5641"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMC6462BIN" prefix="U">
<description>OP Amps</description>
<gates>
<gate name="A" symbol="LMC6462BIN"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-8">
<connects>
<connect gate="A" pin="INA+" pad="3"/>
<connect gate="A" pin="INA-" pad="2"/>
<connect gate="A" pin="INB+" pad="5"/>
<connect gate="A" pin="INB-" pad="6"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMC6462BIN"/>
<attribute name="OC_FARNELL" value="9493808"/>
<attribute name="OC_NEWARK" value="07B5643"/>
<attribute name="PACKAGE" value="8-DIP"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMC6464AIM" prefix="U">
<description>OpAmpIC</description>
<gates>
<gate name="A" symbol="LMC6464AIM"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="+INA" pad="3"/>
<connect gate="A" pin="+INB" pad="5"/>
<connect gate="A" pin="+INC" pad="10"/>
<connect gate="A" pin="+IND" pad="12"/>
<connect gate="A" pin="-INA" pad="2"/>
<connect gate="A" pin="-INB" pad="6"/>
<connect gate="A" pin="-INC" pad="9"/>
<connect gate="A" pin="-IND" pad="13"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="OUTC" pad="8"/>
<connect gate="A" pin="OUTD" pad="14"/>
<connect gate="A" pin="V+" pad="4"/>
<connect gate="A" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMC6464AIM"/>
<attribute name="OC_FARNELL" value="1468887"/>
<attribute name="OC_NEWARK" value="41K2650"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMC6464BIM" prefix="U">
<description>OpAmpIC</description>
<gates>
<gate name="A" symbol="LMC6464BIM"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="+INA" pad="3"/>
<connect gate="A" pin="+INB" pad="5"/>
<connect gate="A" pin="+INC" pad="10"/>
<connect gate="A" pin="+IND" pad="12"/>
<connect gate="A" pin="-INA" pad="2"/>
<connect gate="A" pin="-INB" pad="6"/>
<connect gate="A" pin="-INC" pad="9"/>
<connect gate="A" pin="-IND" pad="13"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="OUTC" pad="8"/>
<connect gate="A" pin="OUTD" pad="14"/>
<connect gate="A" pin="V+" pad="4"/>
<connect gate="A" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMC6464BIM"/>
<attribute name="OC_FARNELL" value="1685334"/>
<attribute name="OC_NEWARK" value="41K2652"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMC6464BIN" prefix="U">
<description>OP AMP</description>
<gates>
<gate name="A" symbol="LMC6464BIN"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-14">
<connects>
<connect gate="A" pin="INA+" pad="3"/>
<connect gate="A" pin="INA-" pad="2"/>
<connect gate="A" pin="INB+" pad="5"/>
<connect gate="A" pin="INB-" pad="6"/>
<connect gate="A" pin="INC+" pad="10"/>
<connect gate="A" pin="INC-" pad="9"/>
<connect gate="A" pin="IND+" pad="12"/>
<connect gate="A" pin="IND-" pad="13"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="OUTC" pad="8"/>
<connect gate="A" pin="OUTD" pad="14"/>
<connect gate="A" pin="V+" pad="4"/>
<connect gate="A" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMC6464BIN"/>
<attribute name="OC_FARNELL" value="1215213"/>
<attribute name="OC_NEWARK" value="41K2654"/>
<attribute name="PACKAGE" value="14-DIP"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMC6482AIM" prefix="U">
<description>OpAmpIC</description>
<gates>
<gate name="A" symbol="LMC6482AIM"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="NEGA" pad="2"/>
<connect gate="A" pin="NEGB" pad="6"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="POSA" pad="3"/>
<connect gate="A" pin="POSB" pad="5"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMC6482AIM"/>
<attribute name="OC_FARNELL" value="9494723"/>
<attribute name="OC_NEWARK" value="07B5649"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMC6482AIN" prefix="U">
<description>OP AMP</description>
<gates>
<gate name="A" symbol="LMC6482AIN"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-8">
<connects>
<connect gate="A" pin="NEG_A" pad="2"/>
<connect gate="A" pin="NEG_B" pad="6"/>
<connect gate="A" pin="OUT_A" pad="1"/>
<connect gate="A" pin="OUT_B" pad="7"/>
<connect gate="A" pin="POS_A" pad="3"/>
<connect gate="A" pin="POS_B" pad="5"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMC6482AIN"/>
<attribute name="OC_FARNELL" value="9494731"/>
<attribute name="OC_NEWARK" value="07B5651"/>
<attribute name="PACKAGE" value="8-DIP"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMC6482IM" prefix="U">
<description>OpAmpIC</description>
<gates>
<gate name="A" symbol="LMC6482IM"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="NEGA" pad="2"/>
<connect gate="A" pin="NEGB" pad="6"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="POSA" pad="3"/>
<connect gate="A" pin="POSB" pad="5"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMC6482IM"/>
<attribute name="OC_FARNELL" value="9494740"/>
<attribute name="OC_NEWARK" value="41K2658"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMC6482IMM" prefix="U">
<description>OpAmpIC</description>
<gates>
<gate name="A" symbol="LMC6482IMM"/>
</gates>
<devices>
<device name="" package="SOP65P490X109-8N">
<connects>
<connect gate="A" pin="NEGA" pad="2"/>
<connect gate="A" pin="NEGB" pad="6"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="POSA" pad="3"/>
<connect gate="A" pin="POSB" pad="5"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMC6482IMM"/>
<attribute name="OC_FARNELL" value="1468890"/>
<attribute name="OC_NEWARK" value="83F3826"/>
<attribute name="PACKAGE" value="MSOP-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMC6482IN" prefix="U">
<description>OP Amps</description>
<gates>
<gate name="A" symbol="LMC6482IN"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-8">
<connects>
<connect gate="A" pin="NEGA" pad="2"/>
<connect gate="A" pin="NEGB" pad="6"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="POSA" pad="3"/>
<connect gate="A" pin="POSB" pad="5"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMC6482IN"/>
<attribute name="OC_FARNELL" value="9486062"/>
<attribute name="OC_NEWARK" value="41K2662"/>
<attribute name="PACKAGE" value="8-DIP"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMC6484AIM" prefix="U">
<description>OpAmpIC</description>
<gates>
<gate name="A" symbol="LMC6484AIM"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="NEG1" pad="2"/>
<connect gate="A" pin="NEG2" pad="6"/>
<connect gate="A" pin="NEG3" pad="9"/>
<connect gate="A" pin="NEG4" pad="13"/>
<connect gate="A" pin="OUT1" pad="1"/>
<connect gate="A" pin="OUT2" pad="7"/>
<connect gate="A" pin="OUT3" pad="8"/>
<connect gate="A" pin="OUTD" pad="14"/>
<connect gate="A" pin="POS1" pad="3"/>
<connect gate="A" pin="POS2" pad="5"/>
<connect gate="A" pin="POS3" pad="10"/>
<connect gate="A" pin="POS4" pad="12"/>
<connect gate="A" pin="V+" pad="4"/>
<connect gate="A" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMC6484AIM"/>
<attribute name="OC_FARNELL" value="9494758"/>
<attribute name="OC_NEWARK" value="41K2663"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMC6484AIN" prefix="U">
<description>OP AMP</description>
<gates>
<gate name="A" symbol="LMC6484AIN"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-14">
<connects>
<connect gate="A" pin="NEG_1" pad="2"/>
<connect gate="A" pin="NEG_2" pad="6"/>
<connect gate="A" pin="NEG_3" pad="9"/>
<connect gate="A" pin="NEG_4" pad="13"/>
<connect gate="A" pin="OUT_1" pad="1"/>
<connect gate="A" pin="OUT_2" pad="7"/>
<connect gate="A" pin="OUT_3" pad="8"/>
<connect gate="A" pin="OUT_4" pad="14"/>
<connect gate="A" pin="POS_1" pad="3"/>
<connect gate="A" pin="POS_2" pad="5"/>
<connect gate="A" pin="POS_3" pad="10"/>
<connect gate="A" pin="POS_4" pad="12"/>
<connect gate="A" pin="V+" pad="4"/>
<connect gate="A" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMC6484AIN"/>
<attribute name="OC_FARNELL" value="9494766"/>
<attribute name="OC_NEWARK" value="07B5657"/>
<attribute name="PACKAGE" value="14-DIP"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMC6484IM" prefix="U">
<description>OpAmpIC</description>
<gates>
<gate name="A" symbol="LMC6484IM"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="NEG1" pad="2"/>
<connect gate="A" pin="NEG2" pad="6"/>
<connect gate="A" pin="NEG3" pad="9"/>
<connect gate="A" pin="NEG4" pad="13"/>
<connect gate="A" pin="OUT1" pad="1"/>
<connect gate="A" pin="OUT2" pad="7"/>
<connect gate="A" pin="OUT3" pad="8"/>
<connect gate="A" pin="OUTD" pad="14"/>
<connect gate="A" pin="POS1" pad="3"/>
<connect gate="A" pin="POS2" pad="5"/>
<connect gate="A" pin="POS3" pad="10"/>
<connect gate="A" pin="POS4" pad="12"/>
<connect gate="A" pin="V+" pad="4"/>
<connect gate="A" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMC6484IM"/>
<attribute name="OC_FARNELL" value="9494774"/>
<attribute name="OC_NEWARK" value="41K2666"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMC6484IN" prefix="U">
<description>OP Amps</description>
<gates>
<gate name="A" symbol="LMC6484IN"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-14">
<connects>
<connect gate="A" pin="NEG1" pad="2"/>
<connect gate="A" pin="NEG2" pad="6"/>
<connect gate="A" pin="NEG3" pad="9"/>
<connect gate="A" pin="NEG4" pad="13"/>
<connect gate="A" pin="OUT1" pad="1"/>
<connect gate="A" pin="OUT2" pad="7"/>
<connect gate="A" pin="OUT3" pad="8"/>
<connect gate="A" pin="OUT4" pad="14"/>
<connect gate="A" pin="POS1" pad="3"/>
<connect gate="A" pin="POS2" pad="5"/>
<connect gate="A" pin="POS3" pad="10"/>
<connect gate="A" pin="POS4" pad="12"/>
<connect gate="A" pin="V+" pad="4"/>
<connect gate="A" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMC6484IN"/>
<attribute name="OC_FARNELL" value="9486070"/>
<attribute name="OC_NEWARK" value="92F350"/>
<attribute name="PACKAGE" value="14- DIP"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMC6492AEM" prefix="U">
<description>OpAmpIC</description>
<gates>
<gate name="A" symbol="LMC6492AEM"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="+INA" pad="3"/>
<connect gate="A" pin="+INB" pad="5"/>
<connect gate="A" pin="-INA" pad="2"/>
<connect gate="A" pin="-INB" pad="6"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMC6492AEM"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="07B5660"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMC6492BEM" prefix="U">
<description>OpAmpIC</description>
<gates>
<gate name="A" symbol="LMC6492BEM"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="+INA" pad="3"/>
<connect gate="A" pin="+INB" pad="5"/>
<connect gate="A" pin="-INA" pad="2"/>
<connect gate="A" pin="-INB" pad="6"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMC6492BEM"/>
<attribute name="OC_FARNELL" value="1685368"/>
<attribute name="OC_NEWARK" value="41K2671"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMC6494AEM" prefix="U">
<description>OpAmpIC</description>
<gates>
<gate name="A" symbol="LMC6494AEM"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="+INA" pad="3"/>
<connect gate="A" pin="+INB" pad="5"/>
<connect gate="A" pin="+INC" pad="10"/>
<connect gate="A" pin="+IND" pad="12"/>
<connect gate="A" pin="-INA" pad="2"/>
<connect gate="A" pin="-INB" pad="6"/>
<connect gate="A" pin="-INC" pad="9"/>
<connect gate="A" pin="-IND" pad="13"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="OUTC" pad="8"/>
<connect gate="A" pin="OUTD" pad="14"/>
<connect gate="A" pin="V+" pad="4"/>
<connect gate="A" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMC6494AEM"/>
<attribute name="OC_FARNELL" value="1685335"/>
<attribute name="OC_NEWARK" value="41K2673"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMC6494BEM" prefix="U">
<description>OpAmpIC</description>
<gates>
<gate name="A" symbol="LMC6494BEM"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="+INA" pad="3"/>
<connect gate="A" pin="+INB" pad="5"/>
<connect gate="A" pin="+INC" pad="10"/>
<connect gate="A" pin="+IND" pad="12"/>
<connect gate="A" pin="-INA" pad="2"/>
<connect gate="A" pin="-INB" pad="6"/>
<connect gate="A" pin="-INC" pad="9"/>
<connect gate="A" pin="-IND" pad="13"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="OUTC" pad="8"/>
<connect gate="A" pin="OUTD" pad="14"/>
<connect gate="A" pin="V+" pad="4"/>
<connect gate="A" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMC6494BEM"/>
<attribute name="OC_FARNELL" value="1215214"/>
<attribute name="OC_NEWARK" value="01M8122"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMC6572AIM" prefix="U">
<description>OpAmpIC</description>
<gates>
<gate name="A" symbol="LMC6572AIM"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="NEGA" pad="2"/>
<connect gate="A" pin="NEGB" pad="6"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="POSA" pad="3"/>
<connect gate="A" pin="POSB" pad="5"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMC6572AIM"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K2677"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMC6572BIM" prefix="U">
<description>OpAmpIC</description>
<gates>
<gate name="A" symbol="LMC6572BIM"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="NEGA" pad="2"/>
<connect gate="A" pin="NEGB" pad="6"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="POSA" pad="3"/>
<connect gate="A" pin="POSB" pad="5"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMC6572BIM"/>
<attribute name="OC_FARNELL" value="1798371"/>
<attribute name="OC_NEWARK" value="75R2088"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMC6574AIM" prefix="U">
<description>OpAmpIC</description>
<gates>
<gate name="A" symbol="LMC6574AIM"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="IN1+" pad="3"/>
<connect gate="A" pin="IN1-" pad="2"/>
<connect gate="A" pin="IN2+" pad="5"/>
<connect gate="A" pin="IN2-" pad="6"/>
<connect gate="A" pin="IN3+" pad="10"/>
<connect gate="A" pin="IN3-" pad="9"/>
<connect gate="A" pin="IN4+" pad="12"/>
<connect gate="A" pin="IN4-" pad="13"/>
<connect gate="A" pin="OUT1" pad="1"/>
<connect gate="A" pin="OUT2" pad="7"/>
<connect gate="A" pin="OUT3" pad="8"/>
<connect gate="A" pin="OUT4" pad="14"/>
<connect gate="A" pin="V+" pad="4"/>
<connect gate="A" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMC6574AIM"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="07B5677"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMC6574BIM" prefix="U">
<description>OpAmpIC</description>
<gates>
<gate name="A" symbol="LMC6574BIM"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="IN1+" pad="3"/>
<connect gate="A" pin="IN1-" pad="2"/>
<connect gate="A" pin="IN2+" pad="5"/>
<connect gate="A" pin="IN2-" pad="6"/>
<connect gate="A" pin="IN3+" pad="10"/>
<connect gate="A" pin="IN3-" pad="9"/>
<connect gate="A" pin="IN4+" pad="12"/>
<connect gate="A" pin="IN4-" pad="13"/>
<connect gate="A" pin="OUT1" pad="1"/>
<connect gate="A" pin="OUT2" pad="7"/>
<connect gate="A" pin="OUT3" pad="8"/>
<connect gate="A" pin="OUT4" pad="14"/>
<connect gate="A" pin="V+" pad="4"/>
<connect gate="A" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMC6574BIM"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K2683"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMC660AIM" prefix="U">
<description>OpAmpIC</description>
<gates>
<gate name="A" symbol="LMC660AIM"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="IN1+" pad="3"/>
<connect gate="A" pin="IN1-" pad="2"/>
<connect gate="A" pin="IN2+" pad="5"/>
<connect gate="A" pin="IN2-" pad="6"/>
<connect gate="A" pin="IN3+" pad="10"/>
<connect gate="A" pin="IN3-" pad="9"/>
<connect gate="A" pin="IN4+" pad="12"/>
<connect gate="A" pin="IN4-" pad="13"/>
<connect gate="A" pin="OUT1" pad="1"/>
<connect gate="A" pin="OUT2" pad="7"/>
<connect gate="A" pin="OUT3" pad="8"/>
<connect gate="A" pin="OUT4" pad="14"/>
<connect gate="A" pin="V+" pad="4"/>
<connect gate="A" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMC660AIM"/>
<attribute name="OC_FARNELL" value="1685336"/>
<attribute name="OC_NEWARK" value="07B5692"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMC660AIN" prefix="U">
<description>OP AMP</description>
<gates>
<gate name="A" symbol="LMC660AIN"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-14">
<connects>
<connect gate="A" pin="NEG_1" pad="2"/>
<connect gate="A" pin="NEG_2" pad="6"/>
<connect gate="A" pin="NEG_3" pad="9"/>
<connect gate="A" pin="NEG_4" pad="13"/>
<connect gate="A" pin="OUT_1" pad="1"/>
<connect gate="A" pin="OUT_2" pad="7"/>
<connect gate="A" pin="OUT_3" pad="8"/>
<connect gate="A" pin="OUT_4" pad="14"/>
<connect gate="A" pin="POS_1" pad="3"/>
<connect gate="A" pin="POS_2" pad="5"/>
<connect gate="A" pin="POS_3" pad="10"/>
<connect gate="A" pin="POS_4" pad="12"/>
<connect gate="A" pin="V+" pad="4"/>
<connect gate="A" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMC660AIN"/>
<attribute name="OC_FARNELL" value="9487107"/>
<attribute name="OC_NEWARK" value="41K2687"/>
<attribute name="PACKAGE" value="14-DIP"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMC660CM" prefix="U">
<description>OpAmpIC</description>
<gates>
<gate name="A" symbol="LMC660CM"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="IN1+" pad="3"/>
<connect gate="A" pin="IN1-" pad="2"/>
<connect gate="A" pin="IN2+" pad="5"/>
<connect gate="A" pin="IN2-" pad="6"/>
<connect gate="A" pin="IN3+" pad="10"/>
<connect gate="A" pin="IN3-" pad="9"/>
<connect gate="A" pin="IN4+" pad="12"/>
<connect gate="A" pin="IN4-" pad="13"/>
<connect gate="A" pin="OUT1" pad="1"/>
<connect gate="A" pin="OUT2" pad="7"/>
<connect gate="A" pin="OUT3" pad="8"/>
<connect gate="A" pin="OUT4" pad="14"/>
<connect gate="A" pin="V+" pad="4"/>
<connect gate="A" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMC660CM"/>
<attribute name="OC_FARNELL" value="9487115"/>
<attribute name="OC_NEWARK" value="97K3123"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMC660CN" prefix="U">
<description>OP AMP</description>
<gates>
<gate name="A" symbol="LMC660CN"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-14">
<connects>
<connect gate="A" pin="NEG_1" pad="2"/>
<connect gate="A" pin="NEG_2" pad="6"/>
<connect gate="A" pin="NEG_3" pad="9"/>
<connect gate="A" pin="NEG_4" pad="13"/>
<connect gate="A" pin="OUT_1" pad="1"/>
<connect gate="A" pin="OUT_2" pad="7"/>
<connect gate="A" pin="OUT_3" pad="8"/>
<connect gate="A" pin="OUT_4" pad="14"/>
<connect gate="A" pin="POS_1" pad="3"/>
<connect gate="A" pin="POS_2" pad="5"/>
<connect gate="A" pin="POS_3" pad="10"/>
<connect gate="A" pin="POS_4" pad="12"/>
<connect gate="A" pin="V+" pad="4"/>
<connect gate="A" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMC660CN"/>
<attribute name="OC_FARNELL" value="9487123"/>
<attribute name="OC_NEWARK" value="92F357"/>
<attribute name="PACKAGE" value="14-DIP"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMC662AIM" prefix="U">
<description>OpAmpIC</description>
<gates>
<gate name="A" symbol="LMC662AIM"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="NEGA" pad="2"/>
<connect gate="A" pin="NEGB" pad="6"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="POSA" pad="3"/>
<connect gate="A" pin="POSB" pad="5"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMC662AIM"/>
<attribute name="OC_FARNELL" value="9494782"/>
<attribute name="OC_NEWARK" value="41K2691"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMC662AIN" prefix="U">
<description>OP AMP</description>
<gates>
<gate name="A" symbol="LMC662AIN"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-8">
<connects>
<connect gate="A" pin="NEG_A" pad="2"/>
<connect gate="A" pin="NEG_B" pad="6"/>
<connect gate="A" pin="OUT_A" pad="1"/>
<connect gate="A" pin="OUT_B" pad="7"/>
<connect gate="A" pin="POS_A" pad="3"/>
<connect gate="A" pin="POS_B" pad="5"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMC662AIN"/>
<attribute name="OC_FARNELL" value="9494790"/>
<attribute name="OC_NEWARK" value="41K2693"/>
<attribute name="PACKAGE" value="8-DIP"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMC662CM" prefix="U">
<description>OpAmpIC</description>
<gates>
<gate name="A" symbol="LMC662CM"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="NEGA" pad="2"/>
<connect gate="A" pin="NEGB" pad="6"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="POSA" pad="3"/>
<connect gate="A" pin="POSB" pad="5"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMC662CM"/>
<attribute name="OC_FARNELL" value="9493395"/>
<attribute name="OC_NEWARK" value="41K2694"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMC662CN" prefix="U">
<description>OP AMP</description>
<gates>
<gate name="A" symbol="LMC662CN"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-8">
<connects>
<connect gate="A" pin="NEG_A" pad="2"/>
<connect gate="A" pin="NEG_B" pad="6"/>
<connect gate="A" pin="OUT_A" pad="1"/>
<connect gate="A" pin="OUT_B" pad="7"/>
<connect gate="A" pin="POS_A" pad="3"/>
<connect gate="A" pin="POS_B" pad="5"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMC662CN"/>
<attribute name="OC_FARNELL" value="9487093"/>
<attribute name="OC_NEWARK" value="41K2696"/>
<attribute name="PACKAGE" value="8-DIP"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMC6762AIM" prefix="U">
<description>CMOS Comparator</description>
<gates>
<gate name="A" symbol="LMC6762AIM"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="+INA" pad="3"/>
<connect gate="A" pin="+INB" pad="5"/>
<connect gate="A" pin="-INA" pad="2"/>
<connect gate="A" pin="-INB" pad="6"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMC6762AIM"/>
<attribute name="OC_FARNELL" value="9494804"/>
<attribute name="OC_NEWARK" value="97K3129"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMC6762BIM" prefix="U">
<description>CMOS Comparator</description>
<gates>
<gate name="A" symbol="LMC6762BIM"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="+INA" pad="3"/>
<connect gate="A" pin="+INB" pad="5"/>
<connect gate="A" pin="-INA" pad="2"/>
<connect gate="A" pin="-INB" pad="6"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMC6762BIM"/>
<attribute name="OC_FARNELL" value="1850237"/>
<attribute name="OC_NEWARK" value="07B5723"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMC6772AIM" prefix="U">
<description>CMOS Comparator</description>
<gates>
<gate name="A" symbol="LMC6772AIM"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="+INA" pad="3"/>
<connect gate="A" pin="+INB" pad="5"/>
<connect gate="A" pin="-INA" pad="2"/>
<connect gate="A" pin="-INB" pad="6"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMC6772AIM"/>
<attribute name="OC_FARNELL" value="9494812"/>
<attribute name="OC_NEWARK" value="92F363"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMC6772AIMM" prefix="U">
<description>CMOS Comparator</description>
<gates>
<gate name="A" symbol="LMC6772AIMM"/>
</gates>
<devices>
<device name="" package="SOP65P490X109-8N">
<connects>
<connect gate="A" pin="IN_A+" pad="3"/>
<connect gate="A" pin="IN_A-" pad="2"/>
<connect gate="A" pin="IN_B+" pad="5"/>
<connect gate="A" pin="IN_B-" pad="6"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMC6772AIMM"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="74C3647"/>
<attribute name="PACKAGE" value="MSOP-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMC6772BIM" prefix="U">
<description>CMOS Comparator</description>
<gates>
<gate name="A" symbol="LMC6772BIM"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="+INA" pad="3"/>
<connect gate="A" pin="+INB" pad="5"/>
<connect gate="A" pin="-INA" pad="2"/>
<connect gate="A" pin="-INB" pad="6"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMC6772BIM"/>
<attribute name="OC_FARNELL" value="1685337"/>
<attribute name="OC_NEWARK" value="41K2705"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMC6772BIN" prefix="U">
<description>CMOS Comparator</description>
<gates>
<gate name="A" symbol="LMC6772BIN"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-8">
<connects>
<connect gate="A" pin="IN_A+" pad="3"/>
<connect gate="A" pin="IN_A-" pad="2"/>
<connect gate="A" pin="IN_B+" pad="5"/>
<connect gate="A" pin="IN_B-" pad="6"/>
<connect gate="A" pin="OUT_A" pad="1"/>
<connect gate="A" pin="OUT_B" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
<connect gate="A" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMC6772BIN"/>
<attribute name="OC_FARNELL" value="9493735"/>
<attribute name="OC_NEWARK" value="41K2707"/>
<attribute name="PACKAGE" value="8-DIP"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMC6772QMM" prefix="U">
<description>CMOS Comparator</description>
<gates>
<gate name="A" symbol="LMC6772QMM"/>
</gates>
<devices>
<device name="" package="SOP65P490X109-8N">
<connects>
<connect gate="A" pin="IN_A+" pad="3"/>
<connect gate="A" pin="IN_A-" pad="2"/>
<connect gate="A" pin="IN_B+" pad="5"/>
<connect gate="A" pin="IN_B-" pad="6"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMC6772QMM"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="55R3684"/>
<attribute name="PACKAGE" value="MSOP-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMC7101AIM5" prefix="U">
<description>Operational Amplifier</description>
<gates>
<gate name="A" symbol="LMC7101AIM5"/>
</gates>
<devices>
<device name="" package="SOT95P280X110-5N">
<connects>
<connect gate="A" pin="NEG" pad="4"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="A" pin="POS" pad="3"/>
<connect gate="A" pin="V+" pad="2"/>
<connect gate="A" pin="V-" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMC7101AIM5"/>
<attribute name="OC_FARNELL" value="9779914"/>
<attribute name="OC_NEWARK" value="83F3867"/>
<attribute name="PACKAGE" value="SOT-23-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMC7101BIM5" prefix="U">
<description>Tiny Low Power Operational Amplifier</description>
<gates>
<gate name="A" symbol="LMC7101BIM5"/>
</gates>
<devices>
<device name="" package="SOT95P285X120-5N">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="4"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="A" pin="V+" pad="2"/>
<connect gate="A" pin="V-" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMC7101BIM5"/>
<attribute name="OC_FARNELL" value="41K2712"/>
<attribute name="OC_NEWARK" value="1212200"/>
<attribute name="PACKAGE" value="SOT-23-5"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMC7101QM5" prefix="U">
<description>Operational Amplifier</description>
<gates>
<gate name="A" symbol="LMC7101QM5"/>
</gates>
<devices>
<device name="" package="SOT95P280X110-5N">
<connects>
<connect gate="A" pin="NEG" pad="4"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="A" pin="POS" pad="3"/>
<connect gate="A" pin="V+" pad="2"/>
<connect gate="A" pin="V-" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMC7101QM5"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="55R3686"/>
<attribute name="PACKAGE" value="SOT-23-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMC7111BIM5" prefix="U">
<description>Operational Amplifier</description>
<gates>
<gate name="A" symbol="LMC7111BIM5"/>
</gates>
<devices>
<device name="" package="SOT95P284X122-5N">
<connects>
<connect gate="A" pin="NEG" pad="4"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="A" pin="POS" pad="3"/>
<connect gate="A" pin="V+" pad="2"/>
<connect gate="A" pin="V-" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMC7111BIM5"/>
<attribute name="OC_FARNELL" value="1468896"/>
<attribute name="OC_NEWARK" value="41K2714"/>
<attribute name="PACKAGE" value="SOT-23-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMC7211AIM" prefix="U">
<description>CMOS Comparator</description>
<gates>
<gate name="A" symbol="LMC7211AIM"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="NC" pad="8"/>
<connect gate="A" pin="NC_2" pad="1"/>
<connect gate="A" pin="NC_3" pad="5"/>
<connect gate="A" pin="NEG" pad="2"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="POS" pad="3"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMC7211AIM"/>
<attribute name="OC_FARNELL" value="1685325"/>
<attribute name="OC_NEWARK" value="47T5172"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMC7211AIM5" prefix="U">
<description>Operational Amplifier</description>
<gates>
<gate name="A" symbol="LMC7211AIM5"/>
</gates>
<devices>
<device name="" package="SOT95P284X110-5N">
<connects>
<connect gate="A" pin="NEG" pad="4"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="A" pin="POS" pad="3"/>
<connect gate="A" pin="V+" pad="2"/>
<connect gate="A" pin="V-" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMC7211AIM5"/>
<attribute name="OC_FARNELL" value="9779922"/>
<attribute name="OC_NEWARK" value="92F366"/>
<attribute name="PACKAGE" value="SOT-23-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMC7211BIM" prefix="U">
<description>CMOS Comparator</description>
<gates>
<gate name="A" symbol="LMC7211BIM"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="NC" pad="8"/>
<connect gate="A" pin="NC_2" pad="1"/>
<connect gate="A" pin="NC_3" pad="5"/>
<connect gate="A" pin="NEG" pad="2"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="POS" pad="3"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMC7211BIM"/>
<attribute name="OC_FARNELL" value="9494820"/>
<attribute name="OC_NEWARK" value="07B5744"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMC7211BIM5" prefix="U">
<description>Tiny CMOS Comparator</description>
<gates>
<gate name="A" symbol="LMC7211BIM5"/>
</gates>
<devices>
<device name="" package="SOT95P285X120-5N">
<connects>
<connect gate="A" pin="NEG" pad="4"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="A" pin="POS" pad="3"/>
<connect gate="A" pin="V+" pad="2"/>
<connect gate="A" pin="V-" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMC7211BIM5"/>
<attribute name="OC_FARNELL" value="9779655"/>
<attribute name="OC_NEWARK" value="41K2722"/>
<attribute name="PACKAGE" value="SOT-23-5"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMC7215IM" prefix="U">
<description>CMOS Comparator</description>
<gates>
<gate name="A" symbol="LMC7215IM"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="NC" pad="8"/>
<connect gate="A" pin="NC_2" pad="1"/>
<connect gate="A" pin="NC_3" pad="5"/>
<connect gate="A" pin="NEG" pad="2"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="POS" pad="3"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMC7215IM"/>
<attribute name="OC_FARNELL" value="9494111"/>
<attribute name="OC_NEWARK" value="07B5749"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMC7215IM5" prefix="U">
<description>CMOS Comparators</description>
<gates>
<gate name="A" symbol="LMC7215IM5"/>
</gates>
<devices>
<device name="" package="SOT95P284X122-5N">
<connects>
<connect gate="A" pin="NEG" pad="4"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="A" pin="POS" pad="3"/>
<connect gate="A" pin="V+" pad="2"/>
<connect gate="A" pin="V-" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMC7215IM5"/>
<attribute name="OC_FARNELL" value="1468940"/>
<attribute name="OC_NEWARK" value="41K2726"/>
<attribute name="PACKAGE" value="SOT-23-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMC7221AIM" prefix="U">
<description>CMOS Comparator</description>
<gates>
<gate name="A" symbol="LMC7221AIM"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="NC" pad="8"/>
<connect gate="A" pin="NC_2" pad="1"/>
<connect gate="A" pin="NC_3" pad="5"/>
<connect gate="A" pin="NEG" pad="2"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="POS" pad="3"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMC7221AIM"/>
<attribute name="OC_FARNELL" value="1685315"/>
<attribute name="OC_NEWARK" value="41K2728"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMC7221AIM5" prefix="U">
<description>Tiny CMOS Comparator</description>
<gates>
<gate name="A" symbol="LMC7221AIM5"/>
</gates>
<devices>
<device name="" package="SOT95P285X120-5N">
<connects>
<connect gate="A" pin="NEG" pad="4"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="A" pin="POS" pad="3"/>
<connect gate="A" pin="V+" pad="2"/>
<connect gate="A" pin="V-" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMC7221AIM5"/>
<attribute name="OC_FARNELL" value="9779930"/>
<attribute name="OC_NEWARK" value="41K2730"/>
<attribute name="PACKAGE" value="SOT-23-5"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMC7221BIM" prefix="U">
<description>CMOS Comparator</description>
<gates>
<gate name="A" symbol="LMC7221BIM"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="NC" pad="8"/>
<connect gate="A" pin="NC_2" pad="1"/>
<connect gate="A" pin="NC_3" pad="5"/>
<connect gate="A" pin="NEG" pad="2"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="POS" pad="3"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMC7221BIM"/>
<attribute name="OC_FARNELL" value="9494839"/>
<attribute name="OC_NEWARK" value="97K3135"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMC7221BIM5" prefix="U">
<description>CMOS Comparator</description>
<gates>
<gate name="A" symbol="LMC7221BIM5"/>
</gates>
<devices>
<device name="" package="SOT95P284X122-5N">
<connects>
<connect gate="A" pin="NEG" pad="4"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="A" pin="POS" pad="3"/>
<connect gate="A" pin="V+" pad="2"/>
<connect gate="A" pin="V-" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMC7221BIM5"/>
<attribute name="OC_FARNELL" value="1468942"/>
<attribute name="OC_NEWARK" value="07B5758"/>
<attribute name="PACKAGE" value="SOT-23-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMC7225IM5" prefix="U">
<description>CMOS Comparator</description>
<gates>
<gate name="A" symbol="LMC7225IM5"/>
</gates>
<devices>
<device name="" package="SOT95P284X122-5N">
<connects>
<connect gate="A" pin="NEG" pad="4"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="A" pin="POS" pad="3"/>
<connect gate="A" pin="V+" pad="2"/>
<connect gate="A" pin="V-" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMC7225IM5"/>
<attribute name="OC_FARNELL" value="1468943"/>
<attribute name="OC_NEWARK" value="41K2736"/>
<attribute name="PACKAGE" value="SOT-23-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMC8101MM" prefix="U">
<description>Op Amp</description>
<gates>
<gate name="A" symbol="LMC8101MM"/>
</gates>
<devices>
<device name="" package="SOP65P490X109-8N">
<connects>
<connect gate="A" pin="NC" pad="8"/>
<connect gate="A" pin="NEG" pad="2"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="POS" pad="3"/>
<connect gate="A" pin="SD" pad="5"/>
<connect gate="A" pin="SL" pad="1"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMC8101MM"/>
<attribute name="OC_FARNELL" value="1685369"/>
<attribute name="OC_NEWARK" value="41K2741"/>
<attribute name="PACKAGE" value="MSOP-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMD18200T" prefix="U">
<description>IC, MOTOR CTRL, HALF BRIDGE 3A</description>
<gates>
<gate name="A" symbol="LMD18200T"/>
</gates>
<devices>
<device name="" package="DIOB_LMD18200T">
<connects>
<connect gate="A" pin="BOOTSTRAP1" pad="1"/>
<connect gate="A" pin="BOOTSTRAP2" pad="11"/>
<connect gate="A" pin="BRAKE_IN" pad="4"/>
<connect gate="A" pin="CURR_SENSE_OUT" pad="8"/>
<connect gate="A" pin="DIRECTION_IN" pad="3"/>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="OUTPUT1" pad="2"/>
<connect gate="A" pin="OUTPUT2" pad="10"/>
<connect gate="A" pin="PWM_IN" pad="5"/>
<connect gate="A" pin="THERM_OUT" pad="9"/>
<connect gate="A" pin="VS_POWER_SUPPLY" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMD18200T"/>
<attribute name="OC_FARNELL" value="9488030"/>
<attribute name="OC_NEWARK" value="41K2745"/>
<attribute name="PACKAGE" value="11-Lead TO-220"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LME49600TS" prefix="U">
<description>IC AMP BUFFER AUD HI FI</description>
<gates>
<gate name="A" symbol="LME49600TS"/>
</gates>
<devices>
<device name="" package="TO127P1435X465-6N">
<connects>
<connect gate="A" pin="BW" pad="1"/>
<connect gate="A" pin="VCC" pad="5"/>
<connect gate="A" pin="VEE" pad="3"/>
<connect gate="A" pin="VIN" pad="2"/>
<connect gate="A" pin="VOUT" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LME49600TS"/>
<attribute name="OC_FARNELL" value="1685402"/>
<attribute name="OC_NEWARK" value="84M8021"/>
<attribute name="PACKAGE" value="TO-263-5"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LME49713HA" prefix="U">
<description>IC AMP AUDIO MONO AB HIFI</description>
<gates>
<gate name="A" symbol="LME49713HA"/>
</gates>
<devices>
<device name="" package="TO254P914X530-8P">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="NC" pad="8"/>
<connect gate="A" pin="NC_2" pad="1"/>
<connect gate="A" pin="NC_3" pad="5"/>
<connect gate="A" pin="OUTPUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LME49713HA"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="34P4693"/>
<attribute name="PACKAGE" value="TO99-8"/>
<attribute name="SUPPLIER" value="National Semicondutors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LME49713MA" prefix="U">
<description>Audio Operational Amplifier</description>
<gates>
<gate name="A" symbol="LME49713MA"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="NC" pad="8"/>
<connect gate="A" pin="NC_2" pad="5"/>
<connect gate="A" pin="NC_3" pad="1"/>
<connect gate="A" pin="OUTPUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LME49713MA"/>
<attribute name="OC_FARNELL" value="1535361"/>
<attribute name="OC_NEWARK" value="64M6873"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LME49721MA" prefix="U">
<description>Audio Operational Amplifier</description>
<gates>
<gate name="A" symbol="LME49721MA"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="+IN_A" pad="3"/>
<connect gate="A" pin="+IN_B" pad="5"/>
<connect gate="A" pin="-IN_A" pad="2"/>
<connect gate="A" pin="-IN_B" pad="6"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="VDD" pad="8"/>
<connect gate="A" pin="VSS" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LME49721MA"/>
<attribute name="OC_FARNELL" value="1506809"/>
<attribute name="OC_NEWARK" value="74M2654"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LME49722MA" prefix="U">
<description>Operational Amplifier</description>
<gates>
<gate name="A" symbol="LME49722MA"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="NEGA" pad="2"/>
<connect gate="A" pin="NEGB" pad="6"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="POSA" pad="3"/>
<connect gate="A" pin="POSB" pad="5"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LME49722MA"/>
<attribute name="OC_FARNELL" value="1685404"/>
<attribute name="OC_NEWARK" value="95M8822"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="National semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LME49723MA" prefix="U">
<description>Operational Amplifier</description>
<gates>
<gate name="A" symbol="LME49723MA"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="NEGA" pad="2"/>
<connect gate="A" pin="NEGB" pad="6"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="POSA" pad="3"/>
<connect gate="A" pin="POSB" pad="5"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LME49723MA"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="84M8023"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="National semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LME49724MR">
<description>Operational Amplifier</description>
<gates>
<gate name="A" symbol="LME49724MR"/>
</gates>
<devices>
<device name="" package="SOIC127P600X168-9N">
<connects>
<connect gate="A" pin="EN" pad="7"/>
<connect gate="A" pin="EP" pad="9"/>
<connect gate="A" pin="VCC" pad="3"/>
<connect gate="A" pin="VEE" pad="6"/>
<connect gate="A" pin="VIN+" pad="8"/>
<connect gate="A" pin="VIN-" pad="1"/>
<connect gate="A" pin="VOCM" pad="2"/>
<connect gate="A" pin="VOUT+" pad="4"/>
<connect gate="A" pin="VOUT-" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LME49724MR"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="04R8947"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="National semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LME49725MA" prefix="U">
<description>Operational Amplifier</description>
<gates>
<gate name="A" symbol="LME49725MA"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="NEGA" pad="2"/>
<connect gate="A" pin="NEGB" pad="6"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="POSA" pad="3"/>
<connect gate="A" pin="POSB" pad="5"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LME49725MA"/>
<attribute name="OC_FARNELL" value="1589526"/>
<attribute name="OC_NEWARK" value="08N3579"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="National semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LME49726MY" prefix="U">
<description>Operational Amplifier</description>
<gates>
<gate name="A" symbol="LME49726MY"/>
</gates>
<devices>
<device name="" package="SOP65P490X110-9N">
<connects>
<connect gate="A" pin="EP" pad="9"/>
<connect gate="A" pin="NEGA" pad="2"/>
<connect gate="A" pin="NEGB" pad="6"/>
<connect gate="A" pin="OUT_A" pad="1"/>
<connect gate="A" pin="OUT_B" pad="7"/>
<connect gate="A" pin="POSA" pad="3"/>
<connect gate="A" pin="POSB" pad="5"/>
<connect gate="A" pin="VDD" pad="8"/>
<connect gate="A" pin="VSS" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LME49726MY"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="04R8951"/>
<attribute name="PACKAGE" value="MSOP-8"/>
<attribute name="SUPPLIER" value="National semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LME49743MT" prefix="U">
<description>Operational Amplifier</description>
<gates>
<gate name="A" symbol="LME49743MT"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-14N">
<connects>
<connect gate="A" pin="+IN1" pad="3"/>
<connect gate="A" pin="+IN2" pad="5"/>
<connect gate="A" pin="+IN3" pad="10"/>
<connect gate="A" pin="+IN4" pad="12"/>
<connect gate="A" pin="-IN1" pad="2"/>
<connect gate="A" pin="-IN2" pad="6"/>
<connect gate="A" pin="-IN3" pad="9"/>
<connect gate="A" pin="-IN4" pad="13"/>
<connect gate="A" pin="OUT1" pad="1"/>
<connect gate="A" pin="OUT2" pad="7"/>
<connect gate="A" pin="OUT3" pad="8"/>
<connect gate="A" pin="OUT4" pad="14"/>
<connect gate="A" pin="V+" pad="4"/>
<connect gate="A" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LME49743MT"/>
<attribute name="OC_FARNELL" value="1685406"/>
<attribute name="OC_NEWARK" value="95M8823"/>
<attribute name="PACKAGE" value="TSSOP-8"/>
<attribute name="SUPPLIER" value="National semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LME49811TB" prefix="U">
<description>IC AMP AUDIO PWR 500W TO247-15</description>
<gates>
<gate name="A" symbol="LME49811TB"/>
</gates>
<devices>
<device name="" package="AMP_LME49811TB">
<connects>
<connect gate="A" pin="COMP" pad="6"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="IN+" pad="4"/>
<connect gate="A" pin="IN-" pad="5"/>
<connect gate="A" pin="NC" pad="12"/>
<connect gate="A" pin="NC_2" pad="8"/>
<connect gate="A" pin="NC_3" pad="9"/>
<connect gate="A" pin="NC_4" pad="7"/>
<connect gate="A" pin="NC_5" pad="1"/>
<connect gate="A" pin="NC_6" pad="11"/>
<connect gate="A" pin="SD" pad="2"/>
<connect gate="A" pin="SINK" pad="13"/>
<connect gate="A" pin="SOURCE" pad="14"/>
<connect gate="A" pin="VCC+" pad="15"/>
<connect gate="A" pin="VEE-" pad="10"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LME49811TB"/>
<attribute name="OC_FARNELL" value="1685355"/>
<attribute name="OC_NEWARK" value="64M6879"/>
<attribute name="PACKAGE" value="TO247-15"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LME49830TB" prefix="U">
<description>IC AMP AUDIO MONO HIFI</description>
<gates>
<gate name="A" symbol="LME49830TB"/>
</gates>
<devices>
<device name="" package="AMP_LME49830TB">
<connects>
<connect gate="A" pin="+VCC" pad="15"/>
<connect gate="A" pin="-VEE" pad="10"/>
<connect gate="A" pin="BASE_M" pad="11"/>
<connect gate="A" pin="BASE_P" pad="12"/>
<connect gate="A" pin="COMP" pad="6"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="IN+" pad="4"/>
<connect gate="A" pin="IN-" pad="5"/>
<connect gate="A" pin="MUTE" pad="2"/>
<connect gate="A" pin="NC" pad="1"/>
<connect gate="A" pin="NC_2" pad="9"/>
<connect gate="A" pin="NC_3" pad="7"/>
<connect gate="A" pin="N_OUT" pad="14"/>
<connect gate="A" pin="OSENSE" pad="8"/>
<connect gate="A" pin="P_OUT" pad="13"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LME49830TB"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="84M8027"/>
<attribute name="PACKAGE" value="TO247-15"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LME49860NA" prefix="U">
<description>OP AMP</description>
<gates>
<gate name="A" symbol="LME49860NA"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-8">
<connects>
<connect gate="A" pin="NEG_A" pad="2"/>
<connect gate="A" pin="NEG_B" pad="6"/>
<connect gate="A" pin="OUT_A" pad="1"/>
<connect gate="A" pin="OUT_B" pad="7"/>
<connect gate="A" pin="POS_A" pad="3"/>
<connect gate="A" pin="POS_B" pad="5"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LME49860NA"/>
<attribute name="OC_FARNELL" value="1433173"/>
<attribute name="OC_NEWARK" value="53M0338"/>
<attribute name="PACKAGE" value="8-DIP"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LME49870MA" prefix="U">
<description>Operational Amplifier</description>
<gates>
<gate name="A" symbol="LME49870MA"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="NC" pad="8"/>
<connect gate="A" pin="NC_2" pad="5"/>
<connect gate="A" pin="NC_3" pad="1"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
<connect gate="A" pin="VOUT" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LME49870MA"/>
<attribute name="OC_FARNELL" value="1685348"/>
<attribute name="OC_NEWARK" value="64M6880"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMH0001SQ" prefix="U">
<description>IC CABLE DVR SERIAL DIGITAL</description>
<gates>
<gate name="A" symbol="LMH0001SQ"/>
</gates>
<devices>
<device name="" package="QFN65P400X400X80-17N">
<connects>
<connect gate="A" pin="DAP" pad="17"/>
<connect gate="A" pin="NC" pad="5"/>
<connect gate="A" pin="NC_2" pad="16"/>
<connect gate="A" pin="NC_3" pad="15"/>
<connect gate="A" pin="NC_4" pad="14"/>
<connect gate="A" pin="NC_5" pad="13"/>
<connect gate="A" pin="NC_6" pad="10"/>
<connect gate="A" pin="NC_7" pad="8"/>
<connect gate="A" pin="NC_8" pad="7"/>
<connect gate="A" pin="NC_9" pad="6"/>
<connect gate="A" pin="RREF" pad="4"/>
<connect gate="A" pin="SDI" pad="1"/>
<connect gate="A" pin="SDO" pad="12"/>
<connect gate="A" pin="VCC" pad="9"/>
<connect gate="A" pin="VEE" pad="3"/>
<connect gate="A" pin="~SDI" pad="2"/>
<connect gate="A" pin="~SDO" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMH0001SQ"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="84M8028"/>
<attribute name="PACKAGE" value="16-WQFN Exposed Pad"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMH0002MA" prefix="U">
<description>Serial Digital Cable Driver</description>
<gates>
<gate name="A" symbol="LMH0002MA"/>
</gates>
<devices>
<device name="" package="SOIC127P620X175-8N">
<connects>
<connect gate="A" pin="RREF" pad="4"/>
<connect gate="A" pin="SD/~HD" pad="6"/>
<connect gate="A" pin="SDI" pad="1"/>
<connect gate="A" pin="SDO" pad="8"/>
<connect gate="A" pin="VCC" pad="5"/>
<connect gate="A" pin="VEE" pad="3"/>
<connect gate="A" pin="~SDI" pad="2"/>
<connect gate="A" pin="~SDO" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMH0002MA"/>
<attribute name="OC_FARNELL" value="1286771"/>
<attribute name="OC_NEWARK" value="79K7683"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMH0002SQ" prefix="U">
<description>IC CABLE DRIVER SDI</description>
<gates>
<gate name="A" symbol="LMH0002SQ"/>
</gates>
<devices>
<device name="" package="QFN65P400X400X80-17N">
<connects>
<connect gate="A" pin="DAP" pad="17"/>
<connect gate="A" pin="NC" pad="5"/>
<connect gate="A" pin="NC_2" pad="16"/>
<connect gate="A" pin="NC_3" pad="15"/>
<connect gate="A" pin="NC_4" pad="14"/>
<connect gate="A" pin="NC_5" pad="13"/>
<connect gate="A" pin="NC_6" pad="8"/>
<connect gate="A" pin="NC_7" pad="7"/>
<connect gate="A" pin="NC_8" pad="6"/>
<connect gate="A" pin="RREF" pad="4"/>
<connect gate="A" pin="SD-HD" pad="10"/>
<connect gate="A" pin="SDI" pad="1"/>
<connect gate="A" pin="SDO" pad="12"/>
<connect gate="A" pin="VCC" pad="9"/>
<connect gate="A" pin="VEE" pad="3"/>
<connect gate="A" pin="~SDI" pad="2"/>
<connect gate="A" pin="~SDO" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMH0002SQ"/>
<attribute name="OC_FARNELL" value="32M0942"/>
<attribute name="OC_NEWARK" value="1345108"/>
<attribute name="PACKAGE" value="16-WQFN Exposed Pad"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMH0024MA" prefix="U">
<description>Cable Equalizer</description>
<gates>
<gate name="A" symbol="LMH0024MA"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-16N">
<connects>
<connect gate="A" pin="AEC+" pad="7"/>
<connect gate="A" pin="AEC-" pad="8"/>
<connect gate="A" pin="BYPASS" pad="9"/>
<connect gate="A" pin="CLI" pad="1"/>
<connect gate="A" pin="MUTE" pad="16"/>
<connect gate="A" pin="NC" pad="10"/>
<connect gate="A" pin="SDI" pad="4"/>
<connect gate="A" pin="SDO" pad="13"/>
<connect gate="A" pin="VCC" pad="15"/>
<connect gate="A" pin="VCC_2" pad="2"/>
<connect gate="A" pin="VEE" pad="14"/>
<connect gate="A" pin="VEE_2" pad="11"/>
<connect gate="A" pin="VEE_3" pad="6"/>
<connect gate="A" pin="VEE_4" pad="3"/>
<connect gate="A" pin="~SDI" pad="5"/>
<connect gate="A" pin="~SDO" pad="12"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMH0024MA"/>
<attribute name="OC_FARNELL" value="1559863"/>
<attribute name="OC_NEWARK" value="99K2250"/>
<attribute name="PACKAGE" value="SOIC-16"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMH0026MH" prefix="U">
<description>SDI Reclocker</description>
<gates>
<gate name="A" symbol="LMH0026MH"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-21N">
<connects>
<connect gate="A" pin="BP/~AUTO-BP" pad="8"/>
<connect gate="A" pin="EPAD" pad="21"/>
<connect gate="A" pin="LF1" pad="1"/>
<connect gate="A" pin="LF2" pad="2"/>
<connect gate="A" pin="LOCKDET" pad="12"/>
<connect gate="A" pin="NC" pad="3"/>
<connect gate="A" pin="RSVD" pad="4"/>
<connect gate="A" pin="SCO/SDO2" pad="14"/>
<connect gate="A" pin="SCO_EN" pad="20"/>
<connect gate="A" pin="SD" pad="19"/>
<connect gate="A" pin="SDI" pad="5"/>
<connect gate="A" pin="SDO" pad="17"/>
<connect gate="A" pin="VCC" pad="7"/>
<connect gate="A" pin="VCCO" pad="18"/>
<connect gate="A" pin="VCCO_2" pad="15"/>
<connect gate="A" pin="XTALIN/EXTCLK" pad="10"/>
<connect gate="A" pin="XTALOUT" pad="11"/>
<connect gate="A" pin="~O/PMUTE" pad="9"/>
<connect gate="A" pin="~SCO/SDO2" pad="13"/>
<connect gate="A" pin="~SDI" pad="6"/>
<connect gate="A" pin="~SDO" pad="16"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMH0026MH"/>
<attribute name="OC_FARNELL" value="1689547"/>
<attribute name="OC_NEWARK" value="45P3498"/>
<attribute name="PACKAGE" value="TSSOP-20"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMH0030VS" prefix="U">
<description>Digital Video Serializer</description>
<gates>
<gate name="A" symbol="LMH0030VS"/>
</gates>
<devices>
<device name="" package="QFP50P1200X1200X120-64N">
<connects>
<connect gate="A" pin="ACLK" pad="36"/>
<connect gate="A" pin="AD0" pad="38"/>
<connect gate="A" pin="AD1" pad="39"/>
<connect gate="A" pin="AD2" pad="40"/>
<connect gate="A" pin="AD3" pad="41"/>
<connect gate="A" pin="AD4" pad="42"/>
<connect gate="A" pin="AD5" pad="44"/>
<connect gate="A" pin="AD6" pad="45"/>
<connect gate="A" pin="AD7" pad="46"/>
<connect gate="A" pin="AD8" pad="47"/>
<connect gate="A" pin="AD9" pad="48"/>
<connect gate="A" pin="ANC/~CTRL" pad="50"/>
<connect gate="A" pin="DV0" pad="5"/>
<connect gate="A" pin="DV1" pad="6"/>
<connect gate="A" pin="DV10" pad="18"/>
<connect gate="A" pin="DV11" pad="19"/>
<connect gate="A" pin="DV12" pad="20"/>
<connect gate="A" pin="DV13" pad="21"/>
<connect gate="A" pin="DV14" pad="22"/>
<connect gate="A" pin="DV15" pad="24"/>
<connect gate="A" pin="DV16" pad="25"/>
<connect gate="A" pin="DV17" pad="26"/>
<connect gate="A" pin="DV18" pad="27"/>
<connect gate="A" pin="DV19" pad="28"/>
<connect gate="A" pin="DV2" pad="7"/>
<connect gate="A" pin="DV3" pad="8"/>
<connect gate="A" pin="DV4" pad="9"/>
<connect gate="A" pin="DV5" pad="11"/>
<connect gate="A" pin="DV6" pad="12"/>
<connect gate="A" pin="DV7" pad="13"/>
<connect gate="A" pin="DV8" pad="14"/>
<connect gate="A" pin="DV9" pad="15"/>
<connect gate="A" pin="IO0" pad="3"/>
<connect gate="A" pin="IO1" pad="4"/>
<connect gate="A" pin="IO2" pad="30"/>
<connect gate="A" pin="IO3" pad="31"/>
<connect gate="A" pin="IO4" pad="32"/>
<connect gate="A" pin="IO5" pad="33"/>
<connect gate="A" pin="IO6" pad="34"/>
<connect gate="A" pin="IO7" pad="35"/>
<connect gate="A" pin="RD/~WR" pad="49"/>
<connect gate="A" pin="RESET" pad="64"/>
<connect gate="A" pin="RREFLVL" pad="53"/>
<connect gate="A" pin="RREFPRE" pad="52"/>
<connect gate="A" pin="SDO" pad="56"/>
<connect gate="A" pin="VCLK" pad="63"/>
<connect gate="A" pin="VDDD" pad="37"/>
<connect gate="A" pin="VDDD_2" pad="16"/>
<connect gate="A" pin="VDDIO" pad="23"/>
<connect gate="A" pin="VDDLS" pad="57"/>
<connect gate="A" pin="VDDPLLA" pad="62"/>
<connect gate="A" pin="VDDPLLD" pad="1"/>
<connect gate="A" pin="VDDSD" pad="51"/>
<connect gate="A" pin="VDDZ" pad="60"/>
<connect gate="A" pin="VSSD" pad="10"/>
<connect gate="A" pin="VSSD_2" pad="17"/>
<connect gate="A" pin="VSSD_3" pad="43"/>
<connect gate="A" pin="VSSIO" pad="29"/>
<connect gate="A" pin="VSSLS" pad="59"/>
<connect gate="A" pin="VSSPLLA" pad="61"/>
<connect gate="A" pin="VSSPLLD" pad="2"/>
<connect gate="A" pin="VSSSD" pad="55"/>
<connect gate="A" pin="VSSSD_2" pad="54"/>
<connect gate="A" pin="~SDO" pad="58"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMH0030VS"/>
<attribute name="OC_FARNELL" value="1495081"/>
<attribute name="OC_NEWARK" value="99K2253"/>
<attribute name="PACKAGE" value="QFP-64"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMH0031VS" prefix="U">
<description>IC DESER/DESCRAM DGTL VID</description>
<gates>
<gate name="A" symbol="LMH0031VS"/>
</gates>
<devices>
<device name="" package="QFP50P1200X1200X120-64N">
<connects>
<connect gate="A" pin="ACLK" pad="13"/>
<connect gate="A" pin="AD0" pad="11"/>
<connect gate="A" pin="AD1" pad="10"/>
<connect gate="A" pin="AD2" pad="9"/>
<connect gate="A" pin="AD3" pad="8"/>
<connect gate="A" pin="AD4" pad="7"/>
<connect gate="A" pin="AD5" pad="5"/>
<connect gate="A" pin="AD6" pad="4"/>
<connect gate="A" pin="AD7" pad="3"/>
<connect gate="A" pin="AD8" pad="2"/>
<connect gate="A" pin="AD9" pad="1"/>
<connect gate="A" pin="ANC/CTRL" pad="63"/>
<connect gate="A" pin="DV0" pad="44"/>
<connect gate="A" pin="DV1" pad="43"/>
<connect gate="A" pin="DV10" pad="31"/>
<connect gate="A" pin="DV11" pad="30"/>
<connect gate="A" pin="DV12" pad="29"/>
<connect gate="A" pin="DV13" pad="28"/>
<connect gate="A" pin="DV14" pad="27"/>
<connect gate="A" pin="DV15" pad="25"/>
<connect gate="A" pin="DV16" pad="24"/>
<connect gate="A" pin="DV17" pad="23"/>
<connect gate="A" pin="DV18" pad="22"/>
<connect gate="A" pin="DV19" pad="21"/>
<connect gate="A" pin="DV2" pad="42"/>
<connect gate="A" pin="DV3" pad="41"/>
<connect gate="A" pin="DV4" pad="40"/>
<connect gate="A" pin="DV5" pad="38"/>
<connect gate="A" pin="DV6" pad="37"/>
<connect gate="A" pin="DV7" pad="36"/>
<connect gate="A" pin="DV8" pad="35"/>
<connect gate="A" pin="DV9" pad="34"/>
<connect gate="A" pin="IO0" pad="46"/>
<connect gate="A" pin="IO1" pad="45"/>
<connect gate="A" pin="IO2" pad="19"/>
<connect gate="A" pin="IO3" pad="18"/>
<connect gate="A" pin="IO4" pad="17"/>
<connect gate="A" pin="IO5" pad="16"/>
<connect gate="A" pin="IO6" pad="15"/>
<connect gate="A" pin="IO7" pad="14"/>
<connect gate="A" pin="RBB" pad="54"/>
<connect gate="A" pin="RD/WR" pad="64"/>
<connect gate="A" pin="RESET" pad="49"/>
<connect gate="A" pin="RREF" pad="53"/>
<connect gate="A" pin="SDI" pad="57"/>
<connect gate="A" pin="SDI_2" pad="56"/>
<connect gate="A" pin="VCLK" pad="50"/>
<connect gate="A" pin="VDDD" pad="62"/>
<connect gate="A" pin="VDDD_2" pad="33"/>
<connect gate="A" pin="VDDD_3" pad="12"/>
<connect gate="A" pin="VDDIO" pad="48"/>
<connect gate="A" pin="VDDIO_2" pad="26"/>
<connect gate="A" pin="VDDPLL" pad="51"/>
<connect gate="A" pin="VDDSI" pad="58"/>
<connect gate="A" pin="VSSD" pad="32"/>
<connect gate="A" pin="VSSD_2" pad="6"/>
<connect gate="A" pin="VSSD_3" pad="39"/>
<connect gate="A" pin="VSSIO" pad="59"/>
<connect gate="A" pin="VSSIO_2" pad="20"/>
<connect gate="A" pin="VSSIO_3" pad="47"/>
<connect gate="A" pin="VSSPLL" pad="52"/>
<connect gate="A" pin="VSSSI" pad="55"/>
<connect gate="A" pin="XTALI/EXT" pad="60"/>
<connect gate="A" pin="XTALO" pad="61"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMH0031VS"/>
<attribute name="OC_FARNELL" value="1495080"/>
<attribute name="OC_NEWARK" value="79K7690"/>
<attribute name="PACKAGE" value="Interface"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMH0034MA" prefix="U">
<description>IC, ADAPTIVE CABLE EQUALIZER</description>
<gates>
<gate name="A" symbol="LMH0034MA"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-16N">
<connects>
<connect gate="A" pin="AEC+" pad="7"/>
<connect gate="A" pin="AEC-" pad="8"/>
<connect gate="A" pin="BYPASS" pad="9"/>
<connect gate="A" pin="CLI" pad="1"/>
<connect gate="A" pin="MUTE/~CD" pad="16"/>
<connect gate="A" pin="MUTEREF" pad="10"/>
<connect gate="A" pin="SDI" pad="4"/>
<connect gate="A" pin="SDO" pad="13"/>
<connect gate="A" pin="VCC" pad="15"/>
<connect gate="A" pin="VCC_2" pad="2"/>
<connect gate="A" pin="VEE" pad="14"/>
<connect gate="A" pin="VEE_2" pad="11"/>
<connect gate="A" pin="VEE_3" pad="6"/>
<connect gate="A" pin="VEE_4" pad="3"/>
<connect gate="A" pin="~SDI" pad="5"/>
<connect gate="A" pin="~SDO" pad="12"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMH0034MA"/>
<attribute name="OC_FARNELL" value="1685558"/>
<attribute name="OC_NEWARK" value="99K2256"/>
<attribute name="PACKAGE" value="SOIC-16"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMH0036SQ" prefix="U">
<description>Multiplexer</description>
<gates>
<gate name="A" symbol="LMH0036SQ"/>
</gates>
<devices>
<device name="" package="QFN50P700X700X80-49N">
<connects>
<connect gate="A" pin="BPASS/~AUTOBYPSS" pad="15"/>
<connect gate="A" pin="EP" pad="49"/>
<connect gate="A" pin="LF1" pad="43"/>
<connect gate="A" pin="LF2" pad="44"/>
<connect gate="A" pin="LOCKDET" pad="24"/>
<connect gate="A" pin="NC" pad="45"/>
<connect gate="A" pin="RSVD" pad="46"/>
<connect gate="A" pin="SCO/SDO2" pad="29"/>
<connect gate="A" pin="SCO_EN" pad="37"/>
<connect gate="A" pin="SD" pad="36"/>
<connect gate="A" pin="SDI0" pad="1"/>
<connect gate="A" pin="SDI1" pad="4"/>
<connect gate="A" pin="SDI2" pad="7"/>
<connect gate="A" pin="SDI3" pad="10"/>
<connect gate="A" pin="SDO" pad="33"/>
<connect gate="A" pin="SEL0" pad="47"/>
<connect gate="A" pin="SEL1" pad="48"/>
<connect gate="A" pin="VCC" pad="35"/>
<connect gate="A" pin="VCC_2" pad="6"/>
<connect gate="A" pin="VCC_3" pad="3"/>
<connect gate="A" pin="VCC_4" pad="30"/>
<connect gate="A" pin="VCC_5" pad="12"/>
<connect gate="A" pin="VCC_6" pad="9"/>
<connect gate="A" pin="VCC_7" pad="31"/>
<connect gate="A" pin="VCC_8" pad="14"/>
<connect gate="A" pin="VCC_9" pad="34"/>
<connect gate="A" pin="VEE" pad="40"/>
<connect gate="A" pin="VEE_10" pad="27"/>
<connect gate="A" pin="VEE_11" pad="26"/>
<connect gate="A" pin="VEE_12" pad="39"/>
<connect gate="A" pin="VEE_13" pad="42"/>
<connect gate="A" pin="VEE_14" pad="41"/>
<connect gate="A" pin="VEE_2" pad="19"/>
<connect gate="A" pin="VEE_3" pad="13"/>
<connect gate="A" pin="VEE_4" pad="17"/>
<connect gate="A" pin="VEE_5" pad="20"/>
<connect gate="A" pin="VEE_6" pad="23"/>
<connect gate="A" pin="VEE_7" pad="21"/>
<connect gate="A" pin="VEE_8" pad="25"/>
<connect gate="A" pin="VEE_9" pad="38"/>
<connect gate="A" pin="XTALIN/EXTCLK" pad="18"/>
<connect gate="A" pin="XTALOUT" pad="22"/>
<connect gate="A" pin="~O/PMUTE" pad="16"/>
<connect gate="A" pin="~SCO/SDO2" pad="28"/>
<connect gate="A" pin="~SDI0" pad="2"/>
<connect gate="A" pin="~SDI1" pad="5"/>
<connect gate="A" pin="~SDI2" pad="8"/>
<connect gate="A" pin="~SDI3" pad="11"/>
<connect gate="A" pin="~SDO" pad="32"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMH0036SQ"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="07P5311"/>
<attribute name="PACKAGE" value="LLP-48"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMH0041SQ" prefix="U">
<description>SDI Deserializer</description>
<gates>
<gate name="A" symbol="LMH0041SQ"/>
</gates>
<devices>
<device name="" package="QFN50P700X700X80-49N">
<connects>
<connect gate="A" pin="DNC" pad="13"/>
<connect gate="A" pin="DVB_ASI" pad="6"/>
<connect gate="A" pin="EP" pad="49"/>
<connect gate="A" pin="GND" pad="29"/>
<connect gate="A" pin="GND_2" pad="8"/>
<connect gate="A" pin="GND_3" pad="9"/>
<connect gate="A" pin="GND_4" pad="10"/>
<connect gate="A" pin="GND_5" pad="23"/>
<connect gate="A" pin="GND_6" pad="24"/>
<connect gate="A" pin="GPIO_0" pad="3"/>
<connect gate="A" pin="GPIO_1" pad="4"/>
<connect gate="A" pin="GPIO_2" pad="11"/>
<connect gate="A" pin="LF_CP" pad="27"/>
<connect gate="A" pin="LF_REF" pad="26"/>
<connect gate="A" pin="LOOPTHRU_EN" pad="2"/>
<connect gate="A" pin="RSET" pad="14"/>
<connect gate="A" pin="RSVD_H" pad="5"/>
<connect gate="A" pin="RX0+" pad="39"/>
<connect gate="A" pin="RX0-" pad="40"/>
<connect gate="A" pin="RX1+" pad="41"/>
<connect gate="A" pin="RX1-" pad="42"/>
<connect gate="A" pin="RX2+" pad="43"/>
<connect gate="A" pin="RX2-" pad="44"/>
<connect gate="A" pin="RX3+" pad="45"/>
<connect gate="A" pin="RX3-" pad="46"/>
<connect gate="A" pin="RX4+" pad="47"/>
<connect gate="A" pin="RX4-" pad="48"/>
<connect gate="A" pin="RXCLK+" pad="37"/>
<connect gate="A" pin="RXCLK-" pad="38"/>
<connect gate="A" pin="RXIN0+" pad="16"/>
<connect gate="A" pin="RXIN0-" pad="17"/>
<connect gate="A" pin="RXIN1+" pad="19"/>
<connect gate="A" pin="RXIN1-" pad="20"/>
<connect gate="A" pin="RX_MUX_SEL" pad="12"/>
<connect gate="A" pin="SCK" pad="33"/>
<connect gate="A" pin="SDA" pad="32"/>
<connect gate="A" pin="SMB_CS" pad="34"/>
<connect gate="A" pin="TXOUT+" pad="21"/>
<connect gate="A" pin="TXOUT-" pad="22"/>
<connect gate="A" pin="VDD2V5" pad="35"/>
<connect gate="A" pin="VDD2V5_2" pad="7"/>
<connect gate="A" pin="VDD2V5_3" pad="25"/>
<connect gate="A" pin="VDD3V3" pad="36"/>
<connect gate="A" pin="VDD3V3_2" pad="1"/>
<connect gate="A" pin="VDD3V3_3" pad="15"/>
<connect gate="A" pin="VDD3V3_4" pad="18"/>
<connect gate="A" pin="VDDPLL" pad="28"/>
<connect gate="A" pin="~LOCK" pad="31"/>
<connect gate="A" pin="~RESET" pad="30"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMH0041SQ"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="07P5314"/>
<attribute name="PACKAGE" value="LLP-48"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMH0044SQ" prefix="U">
<description>Cable Equalizer</description>
<gates>
<gate name="A" symbol="LMH0044SQ"/>
</gates>
<devices>
<device name="" package="QFN65P400X400X80-17N">
<connects>
<connect gate="A" pin="AEC+" pad="5"/>
<connect gate="A" pin="AEC-" pad="6"/>
<connect gate="A" pin="BYPASS" pad="7"/>
<connect gate="A" pin="EP" pad="17"/>
<connect gate="A" pin="MUTE" pad="14"/>
<connect gate="A" pin="MUTEREF" pad="8"/>
<connect gate="A" pin="SDI" pad="2"/>
<connect gate="A" pin="SDO" pad="11"/>
<connect gate="A" pin="VCC" pad="16"/>
<connect gate="A" pin="VCC_2" pad="13"/>
<connect gate="A" pin="VEE" pad="12"/>
<connect gate="A" pin="VEE_2" pad="1"/>
<connect gate="A" pin="VEE_3" pad="4"/>
<connect gate="A" pin="VEE_4" pad="9"/>
<connect gate="A" pin="~CD" pad="15"/>
<connect gate="A" pin="~SDI" pad="3"/>
<connect gate="A" pin="~SDO" pad="10"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMH0044SQ"/>
<attribute name="OC_FARNELL" value="1559246"/>
<attribute name="OC_NEWARK" value="13M1666"/>
<attribute name="PACKAGE" value="LLP-16"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMH0046MH" prefix="U">
<description>SDI Reclocker</description>
<gates>
<gate name="A" symbol="LMH0046MH"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-21N">
<connects>
<connect gate="A" pin="BP/~AUTO-BP" pad="8"/>
<connect gate="A" pin="LF1" pad="1"/>
<connect gate="A" pin="LF2" pad="2"/>
<connect gate="A" pin="LOCK_DET" pad="12"/>
<connect gate="A" pin="RATE0" pad="3"/>
<connect gate="A" pin="RATE1" pad="4"/>
<connect gate="A" pin="SCO/SDO2" pad="14"/>
<connect gate="A" pin="SCO_EN" pad="20"/>
<connect gate="A" pin="SD/~HD" pad="19"/>
<connect gate="A" pin="SDI" pad="5"/>
<connect gate="A" pin="SDO" pad="17"/>
<connect gate="A" pin="VCC" pad="7"/>
<connect gate="A" pin="VCCO" pad="18"/>
<connect gate="A" pin="VCCO_2" pad="15"/>
<connect gate="A" pin="VEE" pad="21"/>
<connect gate="A" pin="XTAL_IN/EXT_CLK" pad="10"/>
<connect gate="A" pin="XTAL_OUT" pad="11"/>
<connect gate="A" pin="~OPMUTE" pad="9"/>
<connect gate="A" pin="~SCO/~SDO2" pad="13"/>
<connect gate="A" pin="~SDI" pad="6"/>
<connect gate="A" pin="~SDO" pad="16"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMH0046MH"/>
<attribute name="OC_FARNELL" value="1559271"/>
<attribute name="OC_NEWARK" value="32M0944"/>
<attribute name="PACKAGE" value="TSSOP-20"/>
<attribute name="SUPPLIER" value="National Semiconducto"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMH0050SQ" prefix="U">
<description>SDI Serializer</description>
<gates>
<gate name="A" symbol="LMH0050SQ"/>
</gates>
<devices>
<device name="" package="QFN50P700X700X80-49N">
<connects>
<connect gate="A" pin="DNC" pad="19"/>
<connect gate="A" pin="DNC_2" pad="20"/>
<connect gate="A" pin="DVB_ASI" pad="6"/>
<connect gate="A" pin="EP" pad="49"/>
<connect gate="A" pin="GND" pad="29"/>
<connect gate="A" pin="GND_10" pad="24"/>
<connect gate="A" pin="GND_2" pad="8"/>
<connect gate="A" pin="GND_3" pad="9"/>
<connect gate="A" pin="GND_4" pad="10"/>
<connect gate="A" pin="GND_5" pad="12"/>
<connect gate="A" pin="GND_6" pad="22"/>
<connect gate="A" pin="GND_7" pad="13"/>
<connect gate="A" pin="GND_8" pad="21"/>
<connect gate="A" pin="GND_9" pad="23"/>
<connect gate="A" pin="GPIO_0" pad="3"/>
<connect gate="A" pin="GPIO_1" pad="4"/>
<connect gate="A" pin="GPIO_2" pad="11"/>
<connect gate="A" pin="LF_CP" pad="27"/>
<connect gate="A" pin="LF_REF" pad="26"/>
<connect gate="A" pin="RSET" pad="14"/>
<connect gate="A" pin="RSVD_H" pad="5"/>
<connect gate="A" pin="RSVD_H_2" pad="2"/>
<connect gate="A" pin="SCK" pad="33"/>
<connect gate="A" pin="SDA" pad="32"/>
<connect gate="A" pin="SMB_CS" pad="34"/>
<connect gate="A" pin="TX0+" pad="39"/>
<connect gate="A" pin="TX0-" pad="40"/>
<connect gate="A" pin="TX1+" pad="41"/>
<connect gate="A" pin="TX1-" pad="42"/>
<connect gate="A" pin="TX2+" pad="43"/>
<connect gate="A" pin="TX2-" pad="44"/>
<connect gate="A" pin="TX3+" pad="45"/>
<connect gate="A" pin="TX3-" pad="46"/>
<connect gate="A" pin="TX4+" pad="47"/>
<connect gate="A" pin="TX4-" pad="48"/>
<connect gate="A" pin="TXCLK+" pad="37"/>
<connect gate="A" pin="TXCLK-" pad="38"/>
<connect gate="A" pin="TXOUT+" pad="16"/>
<connect gate="A" pin="TXOUT-" pad="17"/>
<connect gate="A" pin="VDD2V5" pad="18"/>
<connect gate="A" pin="VDD2V5_2" pad="7"/>
<connect gate="A" pin="VDD2V5_3" pad="25"/>
<connect gate="A" pin="VDD2V5_4" pad="35"/>
<connect gate="A" pin="VDD2V5_5" pad="15"/>
<connect gate="A" pin="VDD3V3" pad="36"/>
<connect gate="A" pin="VDD3V3_2" pad="1"/>
<connect gate="A" pin="VDDPLL" pad="28"/>
<connect gate="A" pin="~LOCK" pad="31"/>
<connect gate="A" pin="~RESET" pad="30"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMH0050SQ"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="07P5318"/>
<attribute name="PACKAGE" value="LLP-48"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMH0051SQ" prefix="U">
<description>SDI Deserializer</description>
<gates>
<gate name="A" symbol="LMH0051SQ"/>
</gates>
<devices>
<device name="" package="QFN50P700X700X80-49N">
<connects>
<connect gate="A" pin="DNC" pad="22"/>
<connect gate="A" pin="DNC_2" pad="21"/>
<connect gate="A" pin="DVB_ASI" pad="6"/>
<connect gate="A" pin="GND" pad="29"/>
<connect gate="A" pin="GND_2" pad="49"/>
<connect gate="A" pin="GND_3" pad="8"/>
<connect gate="A" pin="GND_4" pad="9"/>
<connect gate="A" pin="GND_5" pad="13"/>
<connect gate="A" pin="GND_6" pad="24"/>
<connect gate="A" pin="GND_7" pad="23"/>
<connect gate="A" pin="GND_8" pad="10"/>
<connect gate="A" pin="GPIO_0" pad="3"/>
<connect gate="A" pin="GPIO_1" pad="4"/>
<connect gate="A" pin="GPIO_2" pad="11"/>
<connect gate="A" pin="LF_CP" pad="27"/>
<connect gate="A" pin="LF_REF" pad="26"/>
<connect gate="A" pin="NC" pad="2"/>
<connect gate="A" pin="RSET" pad="14"/>
<connect gate="A" pin="RSVD_H" pad="5"/>
<connect gate="A" pin="RX0+" pad="39"/>
<connect gate="A" pin="RX0-" pad="40"/>
<connect gate="A" pin="RX1+" pad="41"/>
<connect gate="A" pin="RX1-" pad="42"/>
<connect gate="A" pin="RX2+" pad="43"/>
<connect gate="A" pin="RX2-" pad="44"/>
<connect gate="A" pin="RX3+" pad="45"/>
<connect gate="A" pin="RX3-" pad="46"/>
<connect gate="A" pin="RX4+" pad="47"/>
<connect gate="A" pin="RX4-" pad="48"/>
<connect gate="A" pin="RXCLK+" pad="37"/>
<connect gate="A" pin="RXCLK-" pad="38"/>
<connect gate="A" pin="RXIN0+" pad="16"/>
<connect gate="A" pin="RXIN0-" pad="17"/>
<connect gate="A" pin="RXIN1+" pad="19"/>
<connect gate="A" pin="RXIN1-" pad="20"/>
<connect gate="A" pin="RX_MUX_SEL" pad="12"/>
<connect gate="A" pin="SCK" pad="33"/>
<connect gate="A" pin="SDA" pad="32"/>
<connect gate="A" pin="SMB_CS" pad="34"/>
<connect gate="A" pin="VDD2V5" pad="35"/>
<connect gate="A" pin="VDD2V5_2" pad="25"/>
<connect gate="A" pin="VDD2V5_3" pad="7"/>
<connect gate="A" pin="VDD3V3" pad="15"/>
<connect gate="A" pin="VDD3V3_2" pad="18"/>
<connect gate="A" pin="VDD3V3_3" pad="1"/>
<connect gate="A" pin="VDD3V3_4" pad="36"/>
<connect gate="A" pin="VDDPLL" pad="28"/>
<connect gate="A" pin="~LOCK" pad="31"/>
<connect gate="A" pin="~RESET" pad="30"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMH0051SQ"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="01P0818"/>
<attribute name="PACKAGE" value="LLP-48"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMH0070SQE" prefix="U">
<description>SDI Serializer</description>
<gates>
<gate name="A" symbol="LMH0070SQE"/>
</gates>
<devices>
<device name="" package="QFN50P700X700X80-49N">
<connects>
<connect gate="A" pin="DNC" pad="19"/>
<connect gate="A" pin="DNC_2" pad="20"/>
<connect gate="A" pin="DVB_ASI" pad="6"/>
<connect gate="A" pin="EP" pad="49"/>
<connect gate="A" pin="GND" pad="29"/>
<connect gate="A" pin="GND_10" pad="24"/>
<connect gate="A" pin="GND_2" pad="8"/>
<connect gate="A" pin="GND_3" pad="9"/>
<connect gate="A" pin="GND_4" pad="10"/>
<connect gate="A" pin="GND_5" pad="12"/>
<connect gate="A" pin="GND_6" pad="22"/>
<connect gate="A" pin="GND_7" pad="13"/>
<connect gate="A" pin="GND_8" pad="21"/>
<connect gate="A" pin="GND_9" pad="23"/>
<connect gate="A" pin="GPIO_0" pad="3"/>
<connect gate="A" pin="GPIO_1" pad="4"/>
<connect gate="A" pin="GPIO_2" pad="11"/>
<connect gate="A" pin="LF_CP" pad="27"/>
<connect gate="A" pin="LF_REF" pad="26"/>
<connect gate="A" pin="RSET" pad="14"/>
<connect gate="A" pin="RSVD_H" pad="5"/>
<connect gate="A" pin="RSVD_H_2" pad="2"/>
<connect gate="A" pin="SCK" pad="33"/>
<connect gate="A" pin="SDA" pad="32"/>
<connect gate="A" pin="SMB_CS" pad="34"/>
<connect gate="A" pin="TX0+" pad="39"/>
<connect gate="A" pin="TX0-" pad="40"/>
<connect gate="A" pin="TX1+" pad="41"/>
<connect gate="A" pin="TX1-" pad="42"/>
<connect gate="A" pin="TX2+" pad="43"/>
<connect gate="A" pin="TX2-" pad="44"/>
<connect gate="A" pin="TX3+" pad="45"/>
<connect gate="A" pin="TX3-" pad="46"/>
<connect gate="A" pin="TX4+" pad="47"/>
<connect gate="A" pin="TX4-" pad="48"/>
<connect gate="A" pin="TXCLK+" pad="37"/>
<connect gate="A" pin="TXCLK-" pad="38"/>
<connect gate="A" pin="TXOUT+" pad="16"/>
<connect gate="A" pin="TXOUT-" pad="17"/>
<connect gate="A" pin="VDD2V5" pad="18"/>
<connect gate="A" pin="VDD2V5_2" pad="7"/>
<connect gate="A" pin="VDD2V5_3" pad="25"/>
<connect gate="A" pin="VDD2V5_4" pad="35"/>
<connect gate="A" pin="VDD2V5_5" pad="15"/>
<connect gate="A" pin="VDD3V3" pad="36"/>
<connect gate="A" pin="VDD3V3_2" pad="1"/>
<connect gate="A" pin="VDDPLL" pad="28"/>
<connect gate="A" pin="~LOCK" pad="31"/>
<connect gate="A" pin="~RESET" pad="30"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMH0070SQE"/>
<attribute name="OC_FARNELL" value="1609169"/>
<attribute name="OC_NEWARK" value="11N9135"/>
<attribute name="PACKAGE" value="LLP-48"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMH0071SQE" prefix="U">
<description>SDI Serializer</description>
<gates>
<gate name="A" symbol="LMH0071SQE"/>
</gates>
<devices>
<device name="" package="QFN50P700X700X80-49N">
<connects>
<connect gate="A" pin="DNC" pad="13"/>
<connect gate="A" pin="DVB_ASI" pad="6"/>
<connect gate="A" pin="EP" pad="49"/>
<connect gate="A" pin="GND" pad="29"/>
<connect gate="A" pin="GND_2" pad="8"/>
<connect gate="A" pin="GND_3" pad="9"/>
<connect gate="A" pin="GND_4" pad="10"/>
<connect gate="A" pin="GND_5" pad="23"/>
<connect gate="A" pin="GND_6" pad="24"/>
<connect gate="A" pin="GPIO_0" pad="3"/>
<connect gate="A" pin="GPIO_1" pad="4"/>
<connect gate="A" pin="GPIO_2" pad="11"/>
<connect gate="A" pin="LF_CP" pad="27"/>
<connect gate="A" pin="LF_REF" pad="26"/>
<connect gate="A" pin="LOOPTHRU_EN" pad="2"/>
<connect gate="A" pin="RSET" pad="14"/>
<connect gate="A" pin="RSVD_H" pad="5"/>
<connect gate="A" pin="RX0+" pad="39"/>
<connect gate="A" pin="RX0-" pad="40"/>
<connect gate="A" pin="RX1+" pad="41"/>
<connect gate="A" pin="RX1-" pad="42"/>
<connect gate="A" pin="RX2+" pad="43"/>
<connect gate="A" pin="RX2-" pad="44"/>
<connect gate="A" pin="RX3+" pad="45"/>
<connect gate="A" pin="RX3-" pad="46"/>
<connect gate="A" pin="RX4+" pad="47"/>
<connect gate="A" pin="RX4-" pad="48"/>
<connect gate="A" pin="RXCLK+" pad="37"/>
<connect gate="A" pin="RXCLK-" pad="38"/>
<connect gate="A" pin="RXIN0+" pad="16"/>
<connect gate="A" pin="RXIN0-" pad="17"/>
<connect gate="A" pin="RXIN1+" pad="19"/>
<connect gate="A" pin="RXIN1-" pad="20"/>
<connect gate="A" pin="RX_MUX_SEL" pad="12"/>
<connect gate="A" pin="SCK" pad="33"/>
<connect gate="A" pin="SDA" pad="32"/>
<connect gate="A" pin="SMB_CS" pad="34"/>
<connect gate="A" pin="TXOUT+" pad="21"/>
<connect gate="A" pin="TXOUT-" pad="22"/>
<connect gate="A" pin="VDD2V5" pad="35"/>
<connect gate="A" pin="VDD2V5_2" pad="7"/>
<connect gate="A" pin="VDD2V5_3" pad="25"/>
<connect gate="A" pin="VDD3V3" pad="36"/>
<connect gate="A" pin="VDD3V3_2" pad="1"/>
<connect gate="A" pin="VDD3V3_3" pad="15"/>
<connect gate="A" pin="VDD3V3_4" pad="18"/>
<connect gate="A" pin="VDDPLL" pad="28"/>
<connect gate="A" pin="~LOCK" pad="31"/>
<connect gate="A" pin="~RESET" pad="30"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMH0071SQE"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="01P0819"/>
<attribute name="PACKAGE" value="LLP-48"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMH0202MT" prefix="U">
<description>Driver</description>
<gates>
<gate name="A" symbol="LMH0202MT"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-16N">
<connects>
<connect gate="A" pin="RREF1" pad="4"/>
<connect gate="A" pin="RREF2" pad="8"/>
<connect gate="A" pin="SDI1" pad="1"/>
<connect gate="A" pin="SDI2" pad="5"/>
<connect gate="A" pin="SDO1" pad="16"/>
<connect gate="A" pin="SDO2" pad="12"/>
<connect gate="A" pin="SD~/~HD1" pad="14"/>
<connect gate="A" pin="SD~/~HD2" pad="10"/>
<connect gate="A" pin="VCC1" pad="13"/>
<connect gate="A" pin="VCC2" pad="9"/>
<connect gate="A" pin="VEE1" pad="3"/>
<connect gate="A" pin="VEE2" pad="7"/>
<connect gate="A" pin="~SDI1" pad="2"/>
<connect gate="A" pin="~SDI2" pad="6"/>
<connect gate="A" pin="~SDO1" pad="15"/>
<connect gate="A" pin="~SDO2" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMH0202MT"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="99K2259"/>
<attribute name="PACKAGE" value="TSSOP-16"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMH0302SQE" prefix="U">
<description>Cable Driver</description>
<gates>
<gate name="A" symbol="LMH0302SQE"/>
</gates>
<devices>
<device name="" package="QFN65P400X400X80-17N">
<connects>
<connect gate="A" pin="EN" pad="6"/>
<connect gate="A" pin="NC" pad="5"/>
<connect gate="A" pin="NC_2" pad="16"/>
<connect gate="A" pin="NC_3" pad="15"/>
<connect gate="A" pin="NC_4" pad="14"/>
<connect gate="A" pin="NC_5" pad="13"/>
<connect gate="A" pin="NC_6" pad="8"/>
<connect gate="A" pin="NC_7" pad="7"/>
<connect gate="A" pin="RREF" pad="4"/>
<connect gate="A" pin="SD/~HD" pad="10"/>
<connect gate="A" pin="SDI" pad="1"/>
<connect gate="A" pin="SDO" pad="12"/>
<connect gate="A" pin="VCC" pad="9"/>
<connect gate="A" pin="VEE" pad="3"/>
<connect gate="A" pin="VEE_2" pad="17"/>
<connect gate="A" pin="~SDI" pad="2"/>
<connect gate="A" pin="~SDO" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMH0302SQE"/>
<attribute name="OC_FARNELL" value="1685354"/>
<attribute name="OC_NEWARK" value="64M6884"/>
<attribute name="PACKAGE" value="LLP-16"/>
<attribute name="SUPPLIER" value="National semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMH0303SQE" prefix="U">
<description>Cable Driver</description>
<gates>
<gate name="A" symbol="LMH0303SQE"/>
</gates>
<devices>
<device name="" package="QFN65P400X400X80-17N">
<connects>
<connect gate="A" pin="EN" pad="6"/>
<connect gate="A" pin="NC" pad="14"/>
<connect gate="A" pin="NC_2" pad="15"/>
<connect gate="A" pin="RREF" pad="4"/>
<connect gate="A" pin="SCL" pad="8"/>
<connect gate="A" pin="SD/~HD" pad="10"/>
<connect gate="A" pin="SDA" pad="7"/>
<connect gate="A" pin="SDI" pad="1"/>
<connect gate="A" pin="SDO" pad="12"/>
<connect gate="A" pin="VCC" pad="9"/>
<connect gate="A" pin="VEE" pad="3"/>
<connect gate="A" pin="VEE_2" pad="17"/>
<connect gate="A" pin="~FAULT" pad="13"/>
<connect gate="A" pin="~RSTI" pad="5"/>
<connect gate="A" pin="~RSTO" pad="16"/>
<connect gate="A" pin="~SDI" pad="2"/>
<connect gate="A" pin="~SDO" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMH0303SQE"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="34P4703"/>
<attribute name="PACKAGE" value="LLP-16"/>
<attribute name="SUPPLIER" value="National semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMH0307GR" prefix="U">
<description>Cable Driver</description>
<gates>
<gate name="A" symbol="LMH0307GR"/>
</gates>
<devices>
<device name="" package="BGA25C50P5X5_300X300X110">
<connects>
<connect gate="A" pin="EN" pad="E2"/>
<connect gate="A" pin="NC" pad="D3"/>
<connect gate="A" pin="NC_2" pad="E5"/>
<connect gate="A" pin="NC_3" pad="B3"/>
<connect gate="A" pin="RREF" pad="E1"/>
<connect gate="A" pin="RREF_2" pad="D1"/>
<connect gate="A" pin="SCL" pad="E4"/>
<connect gate="A" pin="SD/~HD" pad="D5"/>
<connect gate="A" pin="SDA" pad="E3"/>
<connect gate="A" pin="SDI" pad="A1"/>
<connect gate="A" pin="SDO0" pad="B5"/>
<connect gate="A" pin="SDO1" pad="A4"/>
<connect gate="A" pin="VCC" pad="D4"/>
<connect gate="A" pin="VEE" pad="C4"/>
<connect gate="A" pin="VEE_2" pad="C1"/>
<connect gate="A" pin="VEE_3" pad="B2"/>
<connect gate="A" pin="VEE_4" pad="B4"/>
<connect gate="A" pin="VEE_5" pad="C2"/>
<connect gate="A" pin="VEE_6" pad="C3"/>
<connect gate="A" pin="~FAULT" pad="A5"/>
<connect gate="A" pin="~RSTI" pad="D2"/>
<connect gate="A" pin="~RSTO" pad="A2"/>
<connect gate="A" pin="~SDI" pad="B1"/>
<connect gate="A" pin="~SDO0" pad="C5"/>
<connect gate="A" pin="~SDO1" pad="A3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMH0307GR"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="55R3691"/>
<attribute name="PACKAGE" value="BGA-25"/>
<attribute name="SUPPLIER" value="National semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMH0307SQE" prefix="U">
<description>Cable Driver</description>
<gates>
<gate name="A" symbol="LMH0307SQE"/>
</gates>
<devices>
<device name="" package="QFN65P400X400X80-17N">
<connects>
<connect gate="A" pin="EN" pad="6"/>
<connect gate="A" pin="RREF" pad="4"/>
<connect gate="A" pin="SCL" pad="8"/>
<connect gate="A" pin="SD/~HD" pad="10"/>
<connect gate="A" pin="SDA" pad="7"/>
<connect gate="A" pin="SDI" pad="1"/>
<connect gate="A" pin="SDO" pad="12"/>
<connect gate="A" pin="SDO1" pad="14"/>
<connect gate="A" pin="VCC" pad="9"/>
<connect gate="A" pin="VEE" pad="3"/>
<connect gate="A" pin="VEE_2" pad="17"/>
<connect gate="A" pin="~FAULT" pad="13"/>
<connect gate="A" pin="~RSTI" pad="5"/>
<connect gate="A" pin="~RSTO" pad="16"/>
<connect gate="A" pin="~SDI" pad="2"/>
<connect gate="A" pin="~SDO" pad="11"/>
<connect gate="A" pin="~SDO1" pad="15"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMH0307SQE"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="34P4706"/>
<attribute name="PACKAGE" value="LLP-16"/>
<attribute name="SUPPLIER" value="National semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMH0340SQE" prefix="U">
<description>Serializer and Cable Driver</description>
<gates>
<gate name="A" symbol="LMH0340SQE"/>
</gates>
<devices>
<device name="" package="QFN50P700X700X80-49N">
<connects>
<connect gate="A" pin="DNC" pad="19"/>
<connect gate="A" pin="DNC_2" pad="20"/>
<connect gate="A" pin="DVB_ASI" pad="6"/>
<connect gate="A" pin="EP" pad="49"/>
<connect gate="A" pin="GND" pad="29"/>
<connect gate="A" pin="GND_10" pad="24"/>
<connect gate="A" pin="GND_2" pad="8"/>
<connect gate="A" pin="GND_3" pad="9"/>
<connect gate="A" pin="GND_4" pad="10"/>
<connect gate="A" pin="GND_5" pad="12"/>
<connect gate="A" pin="GND_6" pad="22"/>
<connect gate="A" pin="GND_7" pad="13"/>
<connect gate="A" pin="GND_8" pad="21"/>
<connect gate="A" pin="GND_9" pad="23"/>
<connect gate="A" pin="GPIO_0" pad="3"/>
<connect gate="A" pin="GPIO_1" pad="4"/>
<connect gate="A" pin="GPIO_2" pad="11"/>
<connect gate="A" pin="LF_CP" pad="27"/>
<connect gate="A" pin="LF_REF" pad="26"/>
<connect gate="A" pin="RSET" pad="14"/>
<connect gate="A" pin="RSVD_H" pad="5"/>
<connect gate="A" pin="RSVD_H_2" pad="2"/>
<connect gate="A" pin="SCK" pad="33"/>
<connect gate="A" pin="SDA" pad="32"/>
<connect gate="A" pin="SMB_CS" pad="34"/>
<connect gate="A" pin="TX0+" pad="39"/>
<connect gate="A" pin="TX0-" pad="40"/>
<connect gate="A" pin="TX1+" pad="41"/>
<connect gate="A" pin="TX1-" pad="42"/>
<connect gate="A" pin="TX2+" pad="43"/>
<connect gate="A" pin="TX2-" pad="44"/>
<connect gate="A" pin="TX3+" pad="45"/>
<connect gate="A" pin="TX3-" pad="46"/>
<connect gate="A" pin="TX4+" pad="47"/>
<connect gate="A" pin="TX4-" pad="48"/>
<connect gate="A" pin="TXCLK+" pad="37"/>
<connect gate="A" pin="TXCLK-" pad="38"/>
<connect gate="A" pin="TXOUT+" pad="16"/>
<connect gate="A" pin="TXOUT-" pad="17"/>
<connect gate="A" pin="VDD2V5" pad="18"/>
<connect gate="A" pin="VDD2V5_2" pad="7"/>
<connect gate="A" pin="VDD2V5_3" pad="25"/>
<connect gate="A" pin="VDD2V5_4" pad="35"/>
<connect gate="A" pin="VDD2V5_5" pad="15"/>
<connect gate="A" pin="VDD3V3" pad="36"/>
<connect gate="A" pin="VDD3V3_2" pad="1"/>
<connect gate="A" pin="VDDPLL" pad="28"/>
<connect gate="A" pin="~LOCK" pad="31"/>
<connect gate="A" pin="~RESET" pad="30"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMH0340SQE"/>
<attribute name="OC_FARNELL" value="1609171"/>
<attribute name="OC_NEWARK" value="11N9138"/>
<attribute name="PACKAGE" value="LLP-48"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMH0341SQE" prefix="U">
<description>SDI Serializer</description>
<gates>
<gate name="A" symbol="LMH0341SQE"/>
</gates>
<devices>
<device name="" package="QFN50P700X700X80-49N">
<connects>
<connect gate="A" pin="DNC" pad="13"/>
<connect gate="A" pin="DVB_ASI" pad="6"/>
<connect gate="A" pin="EP" pad="49"/>
<connect gate="A" pin="GND" pad="29"/>
<connect gate="A" pin="GND_2" pad="8"/>
<connect gate="A" pin="GND_3" pad="9"/>
<connect gate="A" pin="GND_4" pad="10"/>
<connect gate="A" pin="GND_5" pad="23"/>
<connect gate="A" pin="GND_6" pad="24"/>
<connect gate="A" pin="GPIO_0" pad="3"/>
<connect gate="A" pin="GPIO_1" pad="4"/>
<connect gate="A" pin="GPIO_2" pad="11"/>
<connect gate="A" pin="LF_CP" pad="27"/>
<connect gate="A" pin="LF_REF" pad="26"/>
<connect gate="A" pin="LOOPTHRU_EN" pad="2"/>
<connect gate="A" pin="RSET" pad="14"/>
<connect gate="A" pin="RSVD_H" pad="5"/>
<connect gate="A" pin="RX0+" pad="39"/>
<connect gate="A" pin="RX0-" pad="40"/>
<connect gate="A" pin="RX1+" pad="41"/>
<connect gate="A" pin="RX1-" pad="42"/>
<connect gate="A" pin="RX2+" pad="43"/>
<connect gate="A" pin="RX2-" pad="44"/>
<connect gate="A" pin="RX3+" pad="45"/>
<connect gate="A" pin="RX3-" pad="46"/>
<connect gate="A" pin="RX4+" pad="47"/>
<connect gate="A" pin="RX4-" pad="48"/>
<connect gate="A" pin="RXCLK+" pad="37"/>
<connect gate="A" pin="RXCLK-" pad="38"/>
<connect gate="A" pin="RXIN0+" pad="16"/>
<connect gate="A" pin="RXIN0-" pad="17"/>
<connect gate="A" pin="RXIN1+" pad="19"/>
<connect gate="A" pin="RXIN1-" pad="20"/>
<connect gate="A" pin="RX_MUX_SEL" pad="12"/>
<connect gate="A" pin="SCK" pad="33"/>
<connect gate="A" pin="SDA" pad="32"/>
<connect gate="A" pin="SMB_CS" pad="34"/>
<connect gate="A" pin="TXOUT+" pad="21"/>
<connect gate="A" pin="TXOUT-" pad="22"/>
<connect gate="A" pin="VDD2V5" pad="35"/>
<connect gate="A" pin="VDD2V5_2" pad="7"/>
<connect gate="A" pin="VDD2V5_3" pad="25"/>
<connect gate="A" pin="VDD3V3" pad="36"/>
<connect gate="A" pin="VDD3V3_2" pad="1"/>
<connect gate="A" pin="VDD3V3_3" pad="15"/>
<connect gate="A" pin="VDD3V3_4" pad="18"/>
<connect gate="A" pin="VDDPLL" pad="28"/>
<connect gate="A" pin="~LOCK" pad="31"/>
<connect gate="A" pin="~RESET" pad="30"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMH0341SQE"/>
<attribute name="OC_FARNELL" value="1853242"/>
<attribute name="OC_NEWARK" value="34P4708"/>
<attribute name="PACKAGE" value="LLP-48"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMH0344GR" prefix="U">
<description>Cable Equalizer</description>
<gates>
<gate name="A" symbol="LMH0344GR"/>
</gates>
<devices>
<device name="" package="BGA25C50P5X5_300X300X110">
<connects>
<connect gate="A" pin="AEC+" pad="E2"/>
<connect gate="A" pin="AEC-" pad="E3"/>
<connect gate="A" pin="BYPASS" pad="D3"/>
<connect gate="A" pin="MUTE" pad="B3"/>
<connect gate="A" pin="MUTEREF" pad="E4"/>
<connect gate="A" pin="NC" pad="C4"/>
<connect gate="A" pin="NC_2" pad="C2"/>
<connect gate="A" pin="NC_3" pad="B5"/>
<connect gate="A" pin="NC_4" pad="C3"/>
<connect gate="A" pin="NC_5" pad="D4"/>
<connect gate="A" pin="NC_6" pad="E1"/>
<connect gate="A" pin="NC_7" pad="A5"/>
<connect gate="A" pin="SDI" pad="C1"/>
<connect gate="A" pin="SDO" pad="C5"/>
<connect gate="A" pin="VCC" pad="A4"/>
<connect gate="A" pin="VCC_2" pad="B2"/>
<connect gate="A" pin="VCC_3" pad="A1"/>
<connect gate="A" pin="VCC_4" pad="A3"/>
<connect gate="A" pin="VEE" pad="E5"/>
<connect gate="A" pin="VEE_2" pad="B4"/>
<connect gate="A" pin="VEE_3" pad="D2"/>
<connect gate="A" pin="VEE_4" pad="B1"/>
<connect gate="A" pin="~CD" pad="A2"/>
<connect gate="A" pin="~SDI" pad="D1"/>
<connect gate="A" pin="~SDO" pad="D5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMH0344GR"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="55R3695"/>
<attribute name="PACKAGE" value="BGA-25"/>
<attribute name="SUPPLIER" value="National semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMH0344SQ" prefix="U">
<description>Cable Equalizer</description>
<gates>
<gate name="A" symbol="LMH0344SQ"/>
</gates>
<devices>
<device name="" package="QFN65P400X400X80-17N">
<connects>
<connect gate="A" pin="AEC+" pad="5"/>
<connect gate="A" pin="AEC-" pad="6"/>
<connect gate="A" pin="BYPASS" pad="7"/>
<connect gate="A" pin="GND" pad="17"/>
<connect gate="A" pin="MUTE" pad="14"/>
<connect gate="A" pin="MUTEREF" pad="8"/>
<connect gate="A" pin="SDI" pad="2"/>
<connect gate="A" pin="SDO" pad="11"/>
<connect gate="A" pin="VCC" pad="16"/>
<connect gate="A" pin="VCC_2" pad="13"/>
<connect gate="A" pin="VEE" pad="12"/>
<connect gate="A" pin="VEE_2" pad="1"/>
<connect gate="A" pin="VEE_3" pad="4"/>
<connect gate="A" pin="VEE_4" pad="9"/>
<connect gate="A" pin="~CD" pad="15"/>
<connect gate="A" pin="~SDI" pad="3"/>
<connect gate="A" pin="~SDO" pad="10"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMH0344SQ"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="84M8032"/>
<attribute name="PACKAGE" value="LLP-16"/>
<attribute name="SUPPLIER" value="National semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMH0346MH" prefix="U">
<description>Differential Outputs</description>
<gates>
<gate name="A" symbol="LMH0346MH"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-21N">
<connects>
<connect gate="A" pin="BP/~AUTO-BP" pad="8"/>
<connect gate="A" pin="LF1" pad="1"/>
<connect gate="A" pin="LF2" pad="2"/>
<connect gate="A" pin="LOCK_DET" pad="12"/>
<connect gate="A" pin="RATE0" pad="3"/>
<connect gate="A" pin="RATE1" pad="4"/>
<connect gate="A" pin="SCO/SDO2" pad="14"/>
<connect gate="A" pin="SCO_EN" pad="20"/>
<connect gate="A" pin="SD/~HD" pad="19"/>
<connect gate="A" pin="SDI" pad="5"/>
<connect gate="A" pin="SDO" pad="17"/>
<connect gate="A" pin="VCC" pad="7"/>
<connect gate="A" pin="VCCO" pad="18"/>
<connect gate="A" pin="VCCO_2" pad="15"/>
<connect gate="A" pin="VEE" pad="21"/>
<connect gate="A" pin="XTAL_IN/EXT_CLK" pad="10"/>
<connect gate="A" pin="XTAL_OUT" pad="11"/>
<connect gate="A" pin="~OP_MUTE" pad="9"/>
<connect gate="A" pin="~SCO/~SDO2" pad="13"/>
<connect gate="A" pin="~SDI" pad="6"/>
<connect gate="A" pin="~SDO" pad="16"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMH0346MH"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="84M8035"/>
<attribute name="PACKAGE" value="TSSOP-20"/>
<attribute name="SUPPLIER" value="National semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMH0356SQ" prefix="U">
<description>4:1  Mux</description>
<gates>
<gate name="A" symbol="LMH0356SQ"/>
</gates>
<devices>
<device name="" package="QFN50P700X700X80-49N">
<connects>
<connect gate="A" pin="BP/~AUTO-BP" pad="15"/>
<connect gate="A" pin="ENABLE" pad="9"/>
<connect gate="A" pin="EP" pad="49"/>
<connect gate="A" pin="LF1" pad="43"/>
<connect gate="A" pin="LF2" pad="44"/>
<connect gate="A" pin="LOCKDET" pad="24"/>
<connect gate="A" pin="RATE0" pad="45"/>
<connect gate="A" pin="RATE1" pad="46"/>
<connect gate="A" pin="SCO/SDO2" pad="29"/>
<connect gate="A" pin="SCO_EN" pad="37"/>
<connect gate="A" pin="SD/~HD" pad="36"/>
<connect gate="A" pin="SDI0" pad="1"/>
<connect gate="A" pin="SDI1" pad="4"/>
<connect gate="A" pin="SDI2" pad="7"/>
<connect gate="A" pin="SDI3" pad="10"/>
<connect gate="A" pin="SDO" pad="33"/>
<connect gate="A" pin="SEL0" pad="47"/>
<connect gate="A" pin="SEL1" pad="48"/>
<connect gate="A" pin="VCC" pad="35"/>
<connect gate="A" pin="VCC_2" pad="6"/>
<connect gate="A" pin="VCC_3" pad="12"/>
<connect gate="A" pin="VCC_4" pad="3"/>
<connect gate="A" pin="VCC_5" pad="14"/>
<connect gate="A" pin="VCC_6" pad="30"/>
<connect gate="A" pin="VCC_7" pad="31"/>
<connect gate="A" pin="VCC_8" pad="34"/>
<connect gate="A" pin="VEE" pad="42"/>
<connect gate="A" pin="VEE_10" pad="26"/>
<connect gate="A" pin="VEE_11" pad="25"/>
<connect gate="A" pin="VEE_12" pad="40"/>
<connect gate="A" pin="VEE_13" pad="27"/>
<connect gate="A" pin="VEE_14" pad="41"/>
<connect gate="A" pin="VEE_2" pad="19"/>
<connect gate="A" pin="VEE_3" pad="23"/>
<connect gate="A" pin="VEE_4" pad="13"/>
<connect gate="A" pin="VEE_5" pad="17"/>
<connect gate="A" pin="VEE_6" pad="38"/>
<connect gate="A" pin="VEE_7" pad="20"/>
<connect gate="A" pin="VEE_8" pad="21"/>
<connect gate="A" pin="VEE_9" pad="39"/>
<connect gate="A" pin="XTALIN/EXTCLK" pad="18"/>
<connect gate="A" pin="XTALOUT" pad="22"/>
<connect gate="A" pin="~O/PMUTE" pad="16"/>
<connect gate="A" pin="~SCO/~SDO2" pad="28"/>
<connect gate="A" pin="~SDI0" pad="2"/>
<connect gate="A" pin="~SDI1" pad="5"/>
<connect gate="A" pin="~SDI2" pad="8"/>
<connect gate="A" pin="~SDI3" pad="11"/>
<connect gate="A" pin="~SDO" pad="32"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMH0356SQ"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="11N9140"/>
<attribute name="PACKAGE" value="LLP-48"/>
<attribute name="SUPPLIER" value="National semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMH1251MT" prefix="U">
<description>Video Switch</description>
<gates>
<gate name="A" symbol="LMH1251MT"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-24N">
<connects>
<connect gate="A" pin="AUTO/MANUAL_DETECT_SELECT" pad="23"/>
<connect gate="A" pin="BIN" pad="5"/>
<connect gate="A" pin="BOUT" pad="18"/>
<connect gate="A" pin="GIN" pad="4"/>
<connect gate="A" pin="GND" pad="16"/>
<connect gate="A" pin="GND_2" pad="6"/>
<connect gate="A" pin="GND_3" pad="12"/>
<connect gate="A" pin="GOUT" pad="19"/>
<connect gate="A" pin="HSYNC_IN" pad="1"/>
<connect gate="A" pin="HSYNC_OUT" pad="14"/>
<connect gate="A" pin="IN_SEL" pad="24"/>
<connect gate="A" pin="PB_IN" pad="9"/>
<connect gate="A" pin="PR_IN" pad="8"/>
<connect gate="A" pin="PWR_SAV" pad="21"/>
<connect gate="A" pin="REXT" pad="15"/>
<connect gate="A" pin="RIN" pad="3"/>
<connect gate="A" pin="ROUT" pad="20"/>
<connect gate="A" pin="SD/HD_SEL" pad="22"/>
<connect gate="A" pin="VCC" pad="7"/>
<connect gate="A" pin="VCC_2" pad="17"/>
<connect gate="A" pin="VSYNC_IN" pad="2"/>
<connect gate="A" pin="VSYNC_OUT" pad="13"/>
<connect gate="A" pin="Y" pad="10"/>
<connect gate="A" pin="~Y" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMH1251MT"/>
<attribute name="OC_FARNELL" value="1286773"/>
<attribute name="OC_NEWARK" value="69K2289"/>
<attribute name="PACKAGE" value="TSSOP-24"/>
<attribute name="SUPPLIER" value="National semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMH1982SQ" prefix="U">
<description>IC, CLOCK GEN, MULTI RATE</description>
<gates>
<gate name="A" symbol="LMH1982SQ"/>
</gates>
<devices>
<device name="" package="QFN50P500X500X80-33N">
<connects>
<connect gate="A" pin="DVDD" pad="9"/>
<connect gate="A" pin="EPAD" pad="33"/>
<connect gate="A" pin="GND" pad="30"/>
<connect gate="A" pin="GND_2" pad="2"/>
<connect gate="A" pin="GND_3" pad="10"/>
<connect gate="A" pin="GND_4" pad="18"/>
<connect gate="A" pin="GND_5" pad="26"/>
<connect gate="A" pin="GND_6" pad="22"/>
<connect gate="A" pin="HD_CLK" pad="20"/>
<connect gate="A" pin="HREF_A" pad="4"/>
<connect gate="A" pin="HREF_B" pad="7"/>
<connect gate="A" pin="LPF" pad="31"/>
<connect gate="A" pin="NO_LOCK" pad="17"/>
<connect gate="A" pin="NO_REF" pad="16"/>
<connect gate="A" pin="REF_SEL" pad="6"/>
<connect gate="A" pin="SCL" pad="12"/>
<connect gate="A" pin="SDA" pad="11"/>
<connect gate="A" pin="SD_CLK" pad="24"/>
<connect gate="A" pin="TOF" pad="25"/>
<connect gate="A" pin="VCXO" pad="29"/>
<connect gate="A" pin="VC_FREERUN" pad="1"/>
<connect gate="A" pin="VDD" pad="21"/>
<connect gate="A" pin="VDD_2" pad="27"/>
<connect gate="A" pin="VDD_3" pad="32"/>
<connect gate="A" pin="VDD_4" pad="28"/>
<connect gate="A" pin="VDD_5" pad="3"/>
<connect gate="A" pin="VREF_A" pad="5"/>
<connect gate="A" pin="VREF_B" pad="8"/>
<connect gate="A" pin="~GENLOCK" pad="14"/>
<connect gate="A" pin="~HD_CLK" pad="19"/>
<connect gate="A" pin="~I2C_EN" pad="13"/>
<connect gate="A" pin="~RESET" pad="15"/>
<connect gate="A" pin="~SD_CLK" pad="23"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMH1982SQ"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="07P5330"/>
<attribute name="PACKAGE" value="QFN-32"/>
<attribute name="SUPPLIER" value="National semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMH2180SD" prefix="U">
<description>Dual Clock Buffer</description>
<gates>
<gate name="A" symbol="LMH2180SD"/>
</gates>
<devices>
<device name="" package="DFN300X300X80-9N">
<connects>
<connect gate="A" pin="EN1" pad="8"/>
<connect gate="A" pin="EN2" pad="4"/>
<connect gate="A" pin="EPAD" pad="9"/>
<connect gate="A" pin="IN1" pad="2"/>
<connect gate="A" pin="IN2" pad="3"/>
<connect gate="A" pin="OUT1" pad="7"/>
<connect gate="A" pin="OUT2" pad="6"/>
<connect gate="A" pin="VDD" pad="1"/>
<connect gate="A" pin="VSS" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMH2180SD"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="84M8041"/>
<attribute name="PACKAGE" value="DFN-8"/>
<attribute name="SUPPLIER" value="National semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMH2180TM" prefix="U">
<description>Dual Clock Buffer</description>
<gates>
<gate name="A" symbol="LMH2180TM"/>
</gates>
<devices>
<device name="" package="BGA8C40P3X3_121X121X67">
<connects>
<connect gate="A" pin="EN1" pad="B3"/>
<connect gate="A" pin="EN2" pad="B1"/>
<connect gate="A" pin="IN1" pad="A2"/>
<connect gate="A" pin="IN2" pad="A1"/>
<connect gate="A" pin="OUT1" pad="C3"/>
<connect gate="A" pin="OUT2" pad="C2"/>
<connect gate="A" pin="VDD" pad="A3"/>
<connect gate="A" pin="VSS" pad="C1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMH2180TM"/>
<attribute name="OC_FARNELL" value=""/>
<attribute name="OC_NEWARK" value="34P4709"/>
<attribute name="PACKAGE" value="BGA-8"/>
<attribute name="SUPPLIER" value="National semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMH2180YD" prefix="U">
<description>75 MHz Dual Clock Buffer</description>
<gates>
<gate name="A" symbol="LMH2180YD"/>
</gates>
<devices>
<device name="" package="DFN300X300X80-9N">
<connects>
<connect gate="A" pin="EN1" pad="8"/>
<connect gate="A" pin="EN2" pad="4"/>
<connect gate="A" pin="EPAD" pad="9"/>
<connect gate="A" pin="IN1" pad="2"/>
<connect gate="A" pin="IN2" pad="3"/>
<connect gate="A" pin="OUT1" pad="7"/>
<connect gate="A" pin="OUT2" pad="6"/>
<connect gate="A" pin="VDD" pad="1"/>
<connect gate="A" pin="VSS" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMH2180YD"/>
<attribute name="OC_FARNELL" value="1552441"/>
<attribute name="OC_NEWARK" value="94M7967"/>
<attribute name="PACKAGE" value="DFN-8"/>
<attribute name="SUPPLIER" value="NATIONAL SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMH2190TM-38" prefix="U">
<description>Quad Channel 27 MHz Clock Tree Driver</description>
<gates>
<gate name="A" symbol="LMH2190TM-38"/>
</gates>
<devices>
<device name="" package="BGA16C4X4X40P_161X161X67">
<connects>
<connect gate="A" pin="CLK1" pad="A3"/>
<connect gate="A" pin="CLK2" pad="A4"/>
<connect gate="A" pin="CLK3" pad="D4"/>
<connect gate="A" pin="CLK4" pad="D3"/>
<connect gate="A" pin="CLK_REQ1" pad="B3"/>
<connect gate="A" pin="CLK_REQ2" pad="B4"/>
<connect gate="A" pin="CLK_REQ3" pad="C4"/>
<connect gate="A" pin="CLK_REQ4" pad="C3"/>
<connect gate="A" pin="ENABLE" pad="A2"/>
<connect gate="A" pin="SCL" pad="D2"/>
<connect gate="A" pin="SCLK_IN" pad="C1"/>
<connect gate="A" pin="SCLK_REQ" pad="C2"/>
<connect gate="A" pin="SDA" pad="D1"/>
<connect gate="A" pin="VBAT" pad="A1"/>
<connect gate="A" pin="VOUT" pad="B1"/>
<connect gate="A" pin="VSS" pad="B2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMH2190TM-38"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="55R3705"/>
<attribute name="PACKAGE" value="BGA-16"/>
<attribute name="SUPPLIER" value="National semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMH6321MR" prefix="U">
<description>300 mA High Speed Buffer</description>
<gates>
<gate name="A" symbol="LMH6321MR"/>
</gates>
<devices>
<device name="" package="SOIC127P620X168-9N">
<connects>
<connect gate="A" pin="CL" pad="2"/>
<connect gate="A" pin="EF" pad="1"/>
<connect gate="A" pin="EPAD" pad="9"/>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="NC" pad="8"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
<connect gate="A" pin="VIN" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMH6321MR"/>
<attribute name="OC_FARNELL" value="1286935"/>
<attribute name="OC_NEWARK" value="24M3430"/>
<attribute name="PACKAGE" value="PSOP-8"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMH6321TS" prefix="U">
<description>300 mA High Speed Buffer</description>
<gates>
<gate name="A" symbol="LMH6321TS"/>
</gates>
<devices>
<device name="" package="TO127P1435X457-8N">
<connects>
<connect gate="A" pin="CL" pad="7"/>
<connect gate="A" pin="EF" pad="6"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="GND_2" pad="8"/>
<connect gate="A" pin="V+" pad="5"/>
<connect gate="A" pin="V-" pad="4"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="VOUT" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMH6321TS"/>
<attribute name="OC_FARNELL" value="1286937"/>
<attribute name="OC_NEWARK" value="99K2268"/>
<attribute name="PACKAGE" value="TO-263-7"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMH6502MA" prefix="U">
<description>Linear-in-dB Variable Gain Amplifier</description>
<gates>
<gate name="A" symbol="LMH6502MA"/>
</gates>
<devices>
<device name="" package="SOIC127P620X175-14N">
<connects>
<connect gate="A" pin="+RG" pad="4"/>
<connect gate="A" pin="+VIN" pad="3"/>
<connect gate="A" pin="-RG" pad="5"/>
<connect gate="A" pin="-VIN" pad="6"/>
<connect gate="A" pin="GND" pad="11"/>
<connect gate="A" pin="I-" pad="12"/>
<connect gate="A" pin="NC" pad="13"/>
<connect gate="A" pin="V+" pad="1"/>
<connect gate="A" pin="V+_2" pad="14"/>
<connect gate="A" pin="V-" pad="8"/>
<connect gate="A" pin="V-_2" pad="7"/>
<connect gate="A" pin="VG" pad="2"/>
<connect gate="A" pin="VOUT" pad="10"/>
<connect gate="A" pin="VREF" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMH6502MA"/>
<attribute name="OC_FARNELL" value="8181047"/>
<attribute name="OC_NEWARK" value="41K2752"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMH6503MA" prefix="U">
<description>Linear Variable Gain Amplifier</description>
<gates>
<gate name="A" symbol="LMH6503MA"/>
</gates>
<devices>
<device name="" package="SOIC127P620X175-14N">
<connects>
<connect gate="A" pin="+RG" pad="4"/>
<connect gate="A" pin="+VIN" pad="3"/>
<connect gate="A" pin="-RG" pad="5"/>
<connect gate="A" pin="-VIN" pad="6"/>
<connect gate="A" pin="GND" pad="11"/>
<connect gate="A" pin="I-" pad="12"/>
<connect gate="A" pin="NC" pad="13"/>
<connect gate="A" pin="V+" pad="1"/>
<connect gate="A" pin="V+_2" pad="14"/>
<connect gate="A" pin="V-" pad="8"/>
<connect gate="A" pin="V-_2" pad="7"/>
<connect gate="A" pin="VG" pad="2"/>
<connect gate="A" pin="VOUT" pad="10"/>
<connect gate="A" pin="VREF" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMH6503MA"/>
<attribute name="OC_FARNELL" value="8181063"/>
<attribute name="OC_NEWARK" value="38K3508"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMH6503MT" prefix="U">
<description>Linear Variable Gain Amplifier</description>
<gates>
<gate name="A" symbol="LMH6503MT"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-14N">
<connects>
<connect gate="A" pin="+RG" pad="4"/>
<connect gate="A" pin="+VIN" pad="3"/>
<connect gate="A" pin="-RG" pad="5"/>
<connect gate="A" pin="-VIN" pad="6"/>
<connect gate="A" pin="GND" pad="11"/>
<connect gate="A" pin="I-" pad="12"/>
<connect gate="A" pin="NC" pad="13"/>
<connect gate="A" pin="V+" pad="1"/>
<connect gate="A" pin="V+_2" pad="14"/>
<connect gate="A" pin="V-" pad="8"/>
<connect gate="A" pin="V-_2" pad="7"/>
<connect gate="A" pin="VG" pad="2"/>
<connect gate="A" pin="VOUT" pad="10"/>
<connect gate="A" pin="VREF" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMH6503MT"/>
<attribute name="OC_FARNELL" value="8181071"/>
<attribute name="OC_NEWARK" value="38K3509"/>
<attribute name="PACKAGE" value="TSSOP-14"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMH6505MA" prefix="U">
<description>Variable Gain Amplifier</description>
<gates>
<gate name="A" symbol="LMH6505MA"/>
</gates>
<devices>
<device name="" package="SOIC127P620X175-8N">
<connects>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="I-" pad="7"/>
<connect gate="A" pin="RG" pad="3"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="5"/>
<connect gate="A" pin="VG" pad="1"/>
<connect gate="A" pin="VIN" pad="2"/>
<connect gate="A" pin="VOUT" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMH6505MA"/>
<attribute name="OC_FARNELL" value="1286774"/>
<attribute name="OC_NEWARK" value="79K7695"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMH6505MM" prefix="U">
<description>Gain Amplifier</description>
<gates>
<gate name="A" symbol="LMH6505MM"/>
</gates>
<devices>
<device name="" package="SOP65P490X109-8N">
<connects>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="I-" pad="7"/>
<connect gate="A" pin="RG" pad="3"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="5"/>
<connect gate="A" pin="VG" pad="1"/>
<connect gate="A" pin="VIN" pad="2"/>
<connect gate="A" pin="VOUT" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMH6505MM"/>
<attribute name="OC_FARNELL" value="1312602"/>
<attribute name="OC_NEWARK" value="79K7699"/>
<attribute name="PACKAGE" value="MSOP-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMH6514SQE" prefix="U">
<description>Gain Amplifier</description>
<gates>
<gate name="A" symbol="LMH6514SQE"/>
</gates>
<devices>
<device name="" package="QFN50P400X400X80-17N">
<connects>
<connect gate="A" pin="GAIN0" pad="11"/>
<connect gate="A" pin="GAIN1" pad="10"/>
<connect gate="A" pin="GAIN2" pad="9"/>
<connect gate="A" pin="GND" pad="17"/>
<connect gate="A" pin="GND_2" pad="5"/>
<connect gate="A" pin="GND_3" pad="8"/>
<connect gate="A" pin="IN+" pad="6"/>
<connect gate="A" pin="IN-" pad="7"/>
<connect gate="A" pin="LATCH" pad="2"/>
<connect gate="A" pin="LOAD+" pad="13"/>
<connect gate="A" pin="LOAD-" pad="16"/>
<connect gate="A" pin="NC" pad="12"/>
<connect gate="A" pin="NC_2" pad="4"/>
<connect gate="A" pin="NC_3" pad="1"/>
<connect gate="A" pin="OUT+" pad="14"/>
<connect gate="A" pin="OUT-" pad="15"/>
<connect gate="A" pin="V+" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMH6514SQE"/>
<attribute name="OC_FARNELL" value="1552443"/>
<attribute name="OC_NEWARK" value="84M8044"/>
<attribute name="PACKAGE" value="LLP-16"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMH6518SQ" prefix="U">
<description>Digitally controlled gain amplifier</description>
<gates>
<gate name="A" symbol="LMH6518SQ"/>
</gates>
<devices>
<device name="" package="QFN50P400X400X80-17N">
<connects>
<connect gate="A" pin="GND" pad="8"/>
<connect gate="A" pin="GND_2" pad="5"/>
<connect gate="A" pin="IN+" pad="6"/>
<connect gate="A" pin="IN-" pad="7"/>
<connect gate="A" pin="OUT+" pad="15"/>
<connect gate="A" pin="OUT-" pad="14"/>
<connect gate="A" pin="OUT_AUX+" pad="1"/>
<connect gate="A" pin="OUT_AUX-" pad="2"/>
<connect gate="A" pin="SCLK" pad="11"/>
<connect gate="A" pin="SDIO" pad="10"/>
<connect gate="A" pin="VCC" pad="3"/>
<connect gate="A" pin="VCC_2" pad="4"/>
<connect gate="A" pin="VCM" pad="13"/>
<connect gate="A" pin="VCM_AUX" pad="16"/>
<connect gate="A" pin="VDD" pad="12"/>
<connect gate="A" pin="~CS" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMH6518SQ"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="34P4711"/>
<attribute name="PACKAGE" value="QFN-16"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMH6550MA" prefix="U">
<description>Differential, High Speed Op Amp</description>
<gates>
<gate name="A" symbol="LMH6550MA"/>
</gates>
<devices>
<device name="" package="SOIC127P620X175-8N">
<connects>
<connect gate="A" pin="+IN" pad="8"/>
<connect gate="A" pin="+OUT" pad="4"/>
<connect gate="A" pin="-IN" pad="1"/>
<connect gate="A" pin="-OUT" pad="5"/>
<connect gate="A" pin="EN" pad="7"/>
<connect gate="A" pin="V+" pad="3"/>
<connect gate="A" pin="V-" pad="6"/>
<connect gate="A" pin="VCM" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMH6550MA"/>
<attribute name="OC_FARNELL" value="1008272"/>
<attribute name="OC_NEWARK" value="41K2766"/>
<attribute name="PACKAGE" value="8-MSOP"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMH6551MA" prefix="U">
<description>Differential, High Speed Op Amp</description>
<gates>
<gate name="A" symbol="LMH6551MA"/>
</gates>
<devices>
<device name="" package="SOIC127P620X175-8N">
<connects>
<connect gate="A" pin="+IN" pad="8"/>
<connect gate="A" pin="+OUT" pad="4"/>
<connect gate="A" pin="-IN" pad="1"/>
<connect gate="A" pin="-OUT" pad="5"/>
<connect gate="A" pin="NC" pad="7"/>
<connect gate="A" pin="V+" pad="3"/>
<connect gate="A" pin="V-" pad="6"/>
<connect gate="A" pin="VCM" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMH6551MA"/>
<attribute name="OC_FARNELL" value="1008273"/>
<attribute name="OC_NEWARK" value="41K2770"/>
<attribute name="PACKAGE" value="8-MSOP"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMH6551MM" prefix="U">
<description>Differential, High Speed Op Amp</description>
<gates>
<gate name="A" symbol="LMH6551MM"/>
</gates>
<devices>
<device name="" package="SOP65P490X110-8N">
<connects>
<connect gate="A" pin="+IN" pad="8"/>
<connect gate="A" pin="+OUT" pad="4"/>
<connect gate="A" pin="-IN" pad="1"/>
<connect gate="A" pin="-OUT" pad="5"/>
<connect gate="A" pin="NC" pad="7"/>
<connect gate="A" pin="V+" pad="3"/>
<connect gate="A" pin="V-" pad="6"/>
<connect gate="A" pin="VCM" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMH6551MM"/>
<attribute name="OC_FARNELL" value="1008037"/>
<attribute name="OC_NEWARK" value="41K2772"/>
<attribute name="PACKAGE" value="8-MSOP"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMH6552SD" prefix="U">
<description>Differential Amplifier</description>
<gates>
<gate name="A" symbol="LMH6552SD"/>
</gates>
<devices>
<device name="" package="DFN250X300X80-9N">
<connects>
<connect gate="A" pin="+IN" pad="8"/>
<connect gate="A" pin="+OUT" pad="4"/>
<connect gate="A" pin="-IN" pad="1"/>
<connect gate="A" pin="-OUT" pad="5"/>
<connect gate="A" pin="EN" pad="7"/>
<connect gate="A" pin="EP" pad="9"/>
<connect gate="A" pin="V+" pad="3"/>
<connect gate="A" pin="V-" pad="6"/>
<connect gate="A" pin="VCM" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMH6552SD"/>
<attribute name="OC_FARNELL" value="1471249"/>
<attribute name="OC_NEWARK" value="64M6887"/>
<attribute name="PACKAGE" value="LLP-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMH6553MR" prefix="U">
<description>Differential Amplifier</description>
<gates>
<gate name="A" symbol="LMH6553MR_1"/>
<gate name="B" symbol="LMH6553MR_2"/>
</gates>
<devices>
<device name="" package="SOIC127P600X168-9N">
<connects>
<connect gate="A" pin="IN+" pad="8"/>
<connect gate="A" pin="IN-" pad="1"/>
<connect gate="A" pin="OUT+" pad="4"/>
<connect gate="A" pin="OUT-" pad="5"/>
<connect gate="A" pin="V+" pad="3"/>
<connect gate="A" pin="V-" pad="6"/>
<connect gate="A" pin="VCLAMP" pad="7"/>
<connect gate="A" pin="VCM" pad="2"/>
<connect gate="B" pin="DAP" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMH6553MR"/>
<attribute name="OC_FARNELL" value="1667414"/>
<attribute name="OC_NEWARK" value="15P1942"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMH6553SD" prefix="U">
<description>Differential Amplifier</description>
<gates>
<gate name="A" symbol="LMH6553SD"/>
</gates>
<devices>
<device name="" package="DFN250X300X80-9N">
<connects>
<connect gate="A" pin="+IN" pad="8"/>
<connect gate="A" pin="+OUT" pad="4"/>
<connect gate="A" pin="-IN" pad="1"/>
<connect gate="A" pin="-OUT" pad="5"/>
<connect gate="A" pin="DAP" pad="9"/>
<connect gate="A" pin="V+" pad="3"/>
<connect gate="A" pin="V-" pad="6"/>
<connect gate="A" pin="VCLAMP" pad="7"/>
<connect gate="A" pin="VCM" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMH6553SD"/>
<attribute name="OC_FARNELL" value="1667417"/>
<attribute name="OC_NEWARK" value="15P1944"/>
<attribute name="PACKAGE" value="LLP-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMH6554LEE" prefix="U">
<description>IC, DIFF AMP, 2.8GHZ, 6200V/µS</description>
<gates>
<gate name="A" symbol="LMH6554LEE"/>
</gates>
<devices>
<device name="" package="QFN40P250X250X80-14N">
<connects>
<connect gate="A" pin="FB+" pad="4"/>
<connect gate="A" pin="FB-" pad="7"/>
<connect gate="A" pin="IN+" pad="6"/>
<connect gate="A" pin="IN-" pad="5"/>
<connect gate="A" pin="NC" pad="14"/>
<connect gate="A" pin="NC_2" pad="11"/>
<connect gate="A" pin="OUT+" pad="13"/>
<connect gate="A" pin="OUT-" pad="12"/>
<connect gate="A" pin="V+" pad="10"/>
<connect gate="A" pin="V+_2" pad="1"/>
<connect gate="A" pin="V-" pad="8"/>
<connect gate="A" pin="V-_2" pad="3"/>
<connect gate="A" pin="VCM" pad="2"/>
<connect gate="A" pin="VEN" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMH6554LEE"/>
<attribute name="OC_FARNELL" value="1793513"/>
<attribute name="OC_NEWARK" value="55R3712"/>
<attribute name="PACKAGE" value="14-UFQFN"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMH6555SQ" prefix="U">
<description>Differential Driver</description>
<gates>
<gate name="A" symbol="LMH6555SQ"/>
</gates>
<devices>
<device name="" package="QFN50P400X400X80-17N">
<connects>
<connect gate="A" pin="DAP" pad="17"/>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="GND_2" pad="14"/>
<connect gate="A" pin="GND_3" pad="15"/>
<connect gate="A" pin="GND_4" pad="1"/>
<connect gate="A" pin="GND_5" pad="2"/>
<connect gate="A" pin="GND_6" pad="3"/>
<connect gate="A" pin="GND_7" pad="4"/>
<connect gate="A" pin="GND_8" pad="6"/>
<connect gate="A" pin="VCC" pad="12"/>
<connect gate="A" pin="VCC_2" pad="9"/>
<connect gate="A" pin="VCC_3" pad="11"/>
<connect gate="A" pin="VCM_REF" pad="10"/>
<connect gate="A" pin="VIN+" pad="16"/>
<connect gate="A" pin="VIN-" pad="5"/>
<connect gate="A" pin="VOUT+" pad="8"/>
<connect gate="A" pin="VOUT-" pad="13"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMH6555SQ"/>
<attribute name="OC_FARNELL" value="1433154"/>
<attribute name="OC_NEWARK" value="46M5438"/>
<attribute name="PACKAGE" value="LLP-16"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMH6559MA" prefix="U">
<description>High-Speed, Closed-Loop Buffer</description>
<gates>
<gate name="A" symbol="LMH6559MA"/>
</gates>
<devices>
<device name="" package="SOIC127P620X175-8N">
<connects>
<connect gate="A" pin="IN" pad="4"/>
<connect gate="A" pin="NC" pad="3"/>
<connect gate="A" pin="NC_2" pad="6"/>
<connect gate="A" pin="NC_3" pad="2"/>
<connect gate="A" pin="NC_4" pad="7"/>
<connect gate="A" pin="V+" pad="1"/>
<connect gate="A" pin="VEE" pad="5"/>
<connect gate="A" pin="VOUT" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMH6559MA"/>
<attribute name="OC_FARNELL" value="8180997"/>
<attribute name="OC_NEWARK" value="41K2774"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="National semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMH6559MF" prefix="U">
<description>IC BUFFER CLOSED-LOOP HS</description>
<gates>
<gate name="A" symbol="LMH6559MF"/>
</gates>
<devices>
<device name="" package="SOT95PX285X122-5N">
<connects>
<connect gate="A" pin="IN" pad="4"/>
<connect gate="A" pin="NC" pad="3"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="A" pin="V+" pad="5"/>
<connect gate="A" pin="V-" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMH6559MF"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="82H3919"/>
<attribute name="PACKAGE" value="SOT23-5"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMH6570MA" prefix="U">
<description>High Speed Video Multiplexer</description>
<gates>
<gate name="A" symbol="LMH6570MA"/>
</gates>
<devices>
<device name="" package="SOIC127P620X175-8N">
<connects>
<connect gate="A" pin="FB" pad="8"/>
<connect gate="A" pin="IN0" pad="1"/>
<connect gate="A" pin="IN1" pad="4"/>
<connect gate="A" pin="OUT" pad="7"/>
<connect gate="A" pin="SD" pad="3"/>
<connect gate="A" pin="SEL" pad="2"/>
<connect gate="A" pin="V+" pad="6"/>
<connect gate="A" pin="V-" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMH6570MA"/>
<attribute name="OC_FARNELL" value="1286775"/>
<attribute name="OC_NEWARK" value="69K2291"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMH6572MQ" prefix="U">
<description>IC VIDEO MULTIPLEXER 2X1</description>
<gates>
<gate name="A" symbol="LMH6572MQ"/>
</gates>
<devices>
<device name="" package="SOP635P600X172-16N">
<connects>
<connect gate="A" pin="B0" pad="3"/>
<connect gate="A" pin="B1" pad="8"/>
<connect gate="A" pin="G0" pad="2"/>
<connect gate="A" pin="G1" pad="7"/>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="GND_2" pad="4"/>
<connect gate="A" pin="OUTB" pad="13"/>
<connect gate="A" pin="OUTG" pad="14"/>
<connect gate="A" pin="OUTR" pad="15"/>
<connect gate="A" pin="R0" pad="1"/>
<connect gate="A" pin="R1" pad="6"/>
<connect gate="A" pin="SEL" pad="10"/>
<connect gate="A" pin="V+" pad="16"/>
<connect gate="A" pin="V-" pad="12"/>
<connect gate="A" pin="V-_2" pad="11"/>
<connect gate="A" pin="~EN" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMH6572MQ"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K2782"/>
<attribute name="PACKAGE" value="16 - SSOP"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMH6574MA" prefix="U">
<description>High Speed Video Multiplexer</description>
<gates>
<gate name="A" symbol="LMH6574MA"/>
</gates>
<devices>
<device name="" package="SOIC127P620X175-14N">
<connects>
<connect gate="A" pin="A0" pad="8"/>
<connect gate="A" pin="A1" pad="9"/>
<connect gate="A" pin="FB" pad="12"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="GND_2" pad="4"/>
<connect gate="A" pin="IN0" pad="1"/>
<connect gate="A" pin="IN1" pad="3"/>
<connect gate="A" pin="IN2" pad="5"/>
<connect gate="A" pin="IN3" pad="7"/>
<connect gate="A" pin="OUT" pad="13"/>
<connect gate="A" pin="SD" pad="11"/>
<connect gate="A" pin="V+" pad="14"/>
<connect gate="A" pin="V-" pad="6"/>
<connect gate="A" pin="~EN" pad="10"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMH6574MA"/>
<attribute name="OC_FARNELL" value="1008275"/>
<attribute name="OC_NEWARK" value="41K2784"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMH6583YA" prefix="U">
<description>Analog Crosspoint Switch</description>
<gates>
<gate name="A" symbol="LMH6583YA"/>
</gates>
<devices>
<device name="" package="QFP50P1000X1000X120-65N">
<connects>
<connect gate="A" pin="BCST" pad="20"/>
<connect gate="A" pin="CFG" pad="19"/>
<connect gate="A" pin="CLK" pad="18"/>
<connect gate="A" pin="DIN" pad="16"/>
<connect gate="A" pin="DOUT" pad="17"/>
<connect gate="A" pin="GND" pad="65"/>
<connect gate="A" pin="GND_2" pad="2"/>
<connect gate="A" pin="GND_3" pad="25"/>
<connect gate="A" pin="GND_4" pad="4"/>
<connect gate="A" pin="GND_5" pad="29"/>
<connect gate="A" pin="GND_6" pad="8"/>
<connect gate="A" pin="GND_7" pad="31"/>
<connect gate="A" pin="GND_8" pad="10"/>
<connect gate="A" pin="GND_9" pad="23"/>
<connect gate="A" pin="IN0" pad="34"/>
<connect gate="A" pin="IN1" pad="36"/>
<connect gate="A" pin="IN10" pad="53"/>
<connect gate="A" pin="IN11" pad="55"/>
<connect gate="A" pin="IN12" pad="57"/>
<connect gate="A" pin="IN13" pad="59"/>
<connect gate="A" pin="IN14" pad="61"/>
<connect gate="A" pin="IN15" pad="63"/>
<connect gate="A" pin="IN2" pad="38"/>
<connect gate="A" pin="IN3" pad="40"/>
<connect gate="A" pin="IN4" pad="42"/>
<connect gate="A" pin="IN5" pad="44"/>
<connect gate="A" pin="IN6" pad="46"/>
<connect gate="A" pin="IN7" pad="48"/>
<connect gate="A" pin="IN8" pad="49"/>
<connect gate="A" pin="IN9" pad="51"/>
<connect gate="A" pin="MODE" pad="14"/>
<connect gate="A" pin="OUT0" pad="1"/>
<connect gate="A" pin="OUT1" pad="5"/>
<connect gate="A" pin="OUT2" pad="7"/>
<connect gate="A" pin="OUT3" pad="11"/>
<connect gate="A" pin="OUT4" pad="22"/>
<connect gate="A" pin="OUT5" pad="26"/>
<connect gate="A" pin="OUT6" pad="28"/>
<connect gate="A" pin="OUT7" pad="32"/>
<connect gate="A" pin="RST" pad="13"/>
<connect gate="A" pin="VCC" pad="60"/>
<connect gate="A" pin="VCC_10" pad="52"/>
<connect gate="A" pin="VCC_11" pad="56"/>
<connect gate="A" pin="VCC_12" pad="64"/>
<connect gate="A" pin="VCC_2" pad="6"/>
<connect gate="A" pin="VCC_3" pad="27"/>
<connect gate="A" pin="VCC_4" pad="12"/>
<connect gate="A" pin="VCC_5" pad="41"/>
<connect gate="A" pin="VCC_6" pad="33"/>
<connect gate="A" pin="VCC_7" pad="37"/>
<connect gate="A" pin="VCC_8" pad="21"/>
<connect gate="A" pin="VCC_9" pad="45"/>
<connect gate="A" pin="VEE" pad="9"/>
<connect gate="A" pin="VEE_10" pad="47"/>
<connect gate="A" pin="VEE_11" pad="50"/>
<connect gate="A" pin="VEE_12" pad="35"/>
<connect gate="A" pin="VEE_2" pad="54"/>
<connect gate="A" pin="VEE_3" pad="3"/>
<connect gate="A" pin="VEE_4" pad="39"/>
<connect gate="A" pin="VEE_5" pad="58"/>
<connect gate="A" pin="VEE_6" pad="24"/>
<connect gate="A" pin="VEE_7" pad="43"/>
<connect gate="A" pin="VEE_8" pad="62"/>
<connect gate="A" pin="VEE_9" pad="30"/>
<connect gate="A" pin="~CS" pad="15"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMH6583YA"/>
<attribute name="OC_FARNELL" value="1554781"/>
<attribute name="OC_NEWARK" value="94M7969"/>
<attribute name="PACKAGE" value="QFP-64"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMH6601MG" prefix="U">
<description>CMOS Operational Amplifier with Shutdown</description>
<gates>
<gate name="A" symbol="LMH6601MG"/>
</gates>
<devices>
<device name="" package="SOT65P240X110-6N">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="4"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="A" pin="V+" pad="6"/>
<connect gate="A" pin="V-" pad="2"/>
<connect gate="A" pin="~SD" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMH6601MG"/>
<attribute name="OC_FARNELL" value="1312603"/>
<attribute name="OC_NEWARK" value="13M1669"/>
<attribute name="PACKAGE" value="SOT-6"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMH6601QMG" prefix="U">
<description>IC AMP VFA 2.4V SHUTDOWN</description>
<gates>
<gate name="A" symbol="LMH6601QMG"/>
</gates>
<devices>
<device name="" package="SOT65P210X110-6N">
<connects>
<connect gate="A" pin="*SD" pad="5"/>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="4"/>
<connect gate="A" pin="OUTPUT" pad="1"/>
<connect gate="A" pin="V+" pad="6"/>
<connect gate="A" pin="V-" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMH6601QMG"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="55R3715"/>
<attribute name="PACKAGE" value="SOT-363"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMH6609MA" prefix="U">
<description>Voltage Feedback Op Amp</description>
<gates>
<gate name="A" symbol="LMH6609MA"/>
</gates>
<devices>
<device name="" package="SOIC127P620X175-8N">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="NC" pad="8"/>
<connect gate="A" pin="NC_2" pad="5"/>
<connect gate="A" pin="NC_3" pad="1"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMH6609MA"/>
<attribute name="OC_FARNELL" value="8180733"/>
<attribute name="OC_NEWARK" value="41K2786"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="National Semicoductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMH6609MF" prefix="U">
<description>Voltage Feedback Op Amp</description>
<gates>
<gate name="A" symbol="LMH6609MF"/>
</gates>
<devices>
<device name="" package="SOT95P285X120-5N">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="4"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="A" pin="V+" pad="5"/>
<connect gate="A" pin="V-" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMH6609MF"/>
<attribute name="OC_FARNELL" value="1685370"/>
<attribute name="OC_NEWARK" value="41K2788"/>
<attribute name="PACKAGE" value="SOT-23-5"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMH6611MK" prefix="U">
<description>Rail-to-Rail Output Amplifiers</description>
<gates>
<gate name="A" symbol="LMH6611MK"/>
</gates>
<devices>
<device name="" package="SOT95P285X100-6N">
<connects>
<connect gate="A" pin="IN+" pad="3"/>
<connect gate="A" pin="IN-" pad="4"/>
<connect gate="A" pin="V+" pad="6"/>
<connect gate="A" pin="V-" pad="2"/>
<connect gate="A" pin="VOUT" pad="1"/>
<connect gate="A" pin="~DIS" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMH6611MK"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="84M8051"/>
<attribute name="PACKAGE" value="SOT-23-6"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMH6612MA" prefix="U">
<description>Output Amplifiers</description>
<gates>
<gate name="A" symbol="LMH6612MA"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="+INA" pad="3"/>
<connect gate="A" pin="+INB" pad="5"/>
<connect gate="A" pin="-INA" pad="2"/>
<connect gate="A" pin="-INB" pad="6"/>
<connect gate="A" pin="OUT_A" pad="1"/>
<connect gate="A" pin="OUT_B" pad="7"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMH6612MA"/>
<attribute name="OC_FARNELL" value="1609184"/>
<attribute name="OC_NEWARK" value="11N9145"/>
<attribute name="PACKAGE" value="8-SOIC"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMH6618MK" prefix="U">
<description>Operational Amplifiers</description>
<gates>
<gate name="A" symbol="LMH6618MK"/>
</gates>
<devices>
<device name="" package="SOT95P285X100-6N">
<connects>
<connect gate="A" pin="IN+" pad="3"/>
<connect gate="A" pin="IN-" pad="4"/>
<connect gate="A" pin="V+" pad="6"/>
<connect gate="A" pin="V-" pad="2"/>
<connect gate="A" pin="VOUT" pad="1"/>
<connect gate="A" pin="~DIS" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMH6618MK"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="54M4604"/>
<attribute name="PACKAGE" value="SOT-23-6"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMH6619MA" prefix="U">
<description>Operational Amplifier</description>
<gates>
<gate name="A" symbol="LMH6619MA"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="+INA" pad="3"/>
<connect gate="A" pin="+INB" pad="5"/>
<connect gate="A" pin="-INA" pad="2"/>
<connect gate="A" pin="-INB" pad="6"/>
<connect gate="A" pin="OUT_A" pad="1"/>
<connect gate="A" pin="OUT_B" pad="7"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMH6619MA"/>
<attribute name="OC_FARNELL" value="1535367"/>
<attribute name="OC_NEWARK" value="74M2655"/>
<attribute name="PACKAGE" value="8-SOIC"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMH6622MA" prefix="U">
<description>OP AMP</description>
<gates>
<gate name="A" symbol="LMH6622MA"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="+INA" pad="3"/>
<connect gate="A" pin="+INB" pad="5"/>
<connect gate="A" pin="-INA" pad="2"/>
<connect gate="A" pin="-INB" pad="6"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMH6622MA"/>
<attribute name="OC_FARNELL" value="1286938"/>
<attribute name="OC_NEWARK" value="41K2790"/>
<attribute name="PACKAGE" value="8-SOIC"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMH6622MM" prefix="U">
<description>Operational Amplifiers</description>
<gates>
<gate name="A" symbol="LMH6622MM"/>
</gates>
<devices>
<device name="" package="SOP65P490X109-8N">
<connects>
<connect gate="A" pin="IN_A+" pad="3"/>
<connect gate="A" pin="IN_A-" pad="2"/>
<connect gate="A" pin="IN_B+" pad="5"/>
<connect gate="A" pin="IN_B-" pad="6"/>
<connect gate="A" pin="OUT_A" pad="1"/>
<connect gate="A" pin="OUT_B" pad="7"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMH6622MM"/>
<attribute name="OC_FARNELL" value="1312809"/>
<attribute name="OC_NEWARK" value="31M5287"/>
<attribute name="PACKAGE" value="8-MSOP"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMH6624MA" prefix="U">
<description>Single/Dual Ultra Low Noise Wideband Op-Amp</description>
<gates>
<gate name="A" symbol="LMH6624MA"/>
</gates>
<devices>
<device name="" package="SOIC127P620X175-8N">
<connects>
<connect gate="A" pin="+INA" pad="3"/>
<connect gate="A" pin="+INB" pad="5"/>
<connect gate="A" pin="-INA" pad="2"/>
<connect gate="A" pin="-INB" pad="6"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMH6624MA"/>
<attribute name="OC_FARNELL" value="8180750"/>
<attribute name="OC_NEWARK" value="41K2794"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="National Semicoductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMH6624MF" prefix="U">
<description>Operational Amplifiers</description>
<gates>
<gate name="A" symbol="LMH6624MF"/>
</gates>
<devices>
<device name="" package="SOT95P285X120-5N">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="4"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="A" pin="V+" pad="5"/>
<connect gate="A" pin="V-" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMH6624MF"/>
<attribute name="OC_FARNELL" value="1468897"/>
<attribute name="OC_NEWARK" value="41K2796"/>
<attribute name="PACKAGE" value="SOT-23-5"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMH6626MA" prefix="U">
<description>Single/Dual Ultra Low Noise Wideband Op-Amp</description>
<gates>
<gate name="A" symbol="LMH6626MA"/>
</gates>
<devices>
<device name="" package="SOIC127P620X175-8N">
<connects>
<connect gate="A" pin="+INA" pad="3"/>
<connect gate="A" pin="+INB" pad="5"/>
<connect gate="A" pin="-INA" pad="2"/>
<connect gate="A" pin="-INB" pad="6"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMH6626MA"/>
<attribute name="OC_FARNELL" value="8180768"/>
<attribute name="OC_NEWARK" value="41K2798"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="National Semicoductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMH6626MM" prefix="U">
<description>Op Amp</description>
<gates>
<gate name="A" symbol="LMH6626MM"/>
</gates>
<devices>
<device name="" package="SOP65P490X109-8N">
<connects>
<connect gate="A" pin="INA+" pad="3"/>
<connect gate="A" pin="INA-" pad="2"/>
<connect gate="A" pin="INB+" pad="5"/>
<connect gate="A" pin="INB-" pad="6"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMH6626MM"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K2800"/>
<attribute name="PACKAGE" value="MSOP-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMH6628MA" prefix="U">
<description>Op Amp</description>
<gates>
<gate name="A" symbol="LMH6628MA"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="+VCC" pad="8"/>
<connect gate="A" pin="-VCC" pad="4"/>
<connect gate="A" pin="VIN1" pad="2"/>
<connect gate="A" pin="VIN2" pad="6"/>
<connect gate="A" pin="VNON-INV1" pad="3"/>
<connect gate="A" pin="VNON-INV2" pad="5"/>
<connect gate="A" pin="VOUT1" pad="1"/>
<connect gate="A" pin="VOUT2" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMH6643MA"/>
<attribute name="OC_FARNELL" value="1286941"/>
<attribute name="OC_NEWARK" value="34C6431"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMH6639MA" prefix="U">
<description>OPAMP</description>
<gates>
<gate name="A" symbol="LMH6639MA"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="IN+" pad="3"/>
<connect gate="A" pin="IN-" pad="2"/>
<connect gate="A" pin="N/C" pad="5"/>
<connect gate="A" pin="N/C_2" pad="1"/>
<connect gate="A" pin="OUTPUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
<connect gate="A" pin="~SD" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMH6639MA"/>
<attribute name="OC_FARNELL" value="41K2804"/>
<attribute name="OC_NEWARK" value="1286940"/>
<attribute name="PACKAGE" value="8SOIC"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMH6639MF" prefix="U">
<description>Output Amplifier</description>
<gates>
<gate name="A" symbol="LMH6639MF"/>
</gates>
<devices>
<device name="" package="SOT95P284X122-6N">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="4"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="A" pin="V+" pad="6"/>
<connect gate="A" pin="V-" pad="2"/>
<connect gate="A" pin="~SD" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMH6639MF"/>
<attribute name="OC_FARNELL" value="1312810"/>
<attribute name="OC_NEWARK" value="41K2806"/>
<attribute name="PACKAGE" value="SOT23-6"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMH6640MF" prefix="U">
<description>Operational Amplifier</description>
<gates>
<gate name="A" symbol="LMH6640MF"/>
</gates>
<devices>
<device name="" package="SOT95P285X120-5N">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="4"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="A" pin="V+" pad="5"/>
<connect gate="A" pin="V-" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMH6654MF"/>
<attribute name="OC_FARNELL" value="1472348"/>
<attribute name="OC_NEWARK" value="41K2836"/>
<attribute name="PACKAGE" value="SOT-23-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMH6642MA" prefix="U">
<description>Output Amplifiers</description>
<gates>
<gate name="A" symbol="LMH6642MA"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="IN+" pad="3"/>
<connect gate="A" pin="IN-" pad="2"/>
<connect gate="A" pin="N/C" pad="8"/>
<connect gate="A" pin="N/C_2" pad="1"/>
<connect gate="A" pin="N/C_3" pad="5"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMH6642MA"/>
<attribute name="OC_FARNELL" value="9490167"/>
<attribute name="OC_NEWARK" value="34C6427"/>
<attribute name="PACKAGE" value="8-SOIC"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMH6642MF" prefix="U">
<description>Rail-to-Rail Output Amplifiers</description>
<gates>
<gate name="A" symbol="LMH6642MF"/>
</gates>
<devices>
<device name="" package="SOT95P285X120-5N">
<connects>
<connect gate="A" pin="IN+" pad="3"/>
<connect gate="A" pin="IN-" pad="4"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="A" pin="V+" pad="5"/>
<connect gate="A" pin="V-" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMH6642MF"/>
<attribute name="OC_FARNELL" value="1312811"/>
<attribute name="OC_NEWARK" value="41K2812"/>
<attribute name="PACKAGE" value="SOT23-5"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMH6643MA" prefix="U">
<description>OpAmpIC</description>
<gates>
<gate name="A" symbol="LMH6643MA"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="+INA" pad="3"/>
<connect gate="A" pin="+INB" pad="5"/>
<connect gate="A" pin="-INA" pad="2"/>
<connect gate="A" pin="-INB" pad="6"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMH6643MA"/>
<attribute name="OC_FARNELL" value="1286941"/>
<attribute name="OC_NEWARK" value="34C6431"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMH6643MM" prefix="U">
<description>Amplifiers</description>
<gates>
<gate name="A" symbol="LMH6643MM"/>
</gates>
<devices>
<device name="" package="SOP65P490X109-8N">
<connects>
<connect gate="A" pin="IN_A+" pad="3"/>
<connect gate="A" pin="IN_A-" pad="2"/>
<connect gate="A" pin="IN_B+" pad="5"/>
<connect gate="A" pin="IN_B-" pad="6"/>
<connect gate="A" pin="OUT_A" pad="1"/>
<connect gate="A" pin="OUT_B" pad="7"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMH6643MM"/>
<attribute name="OC_FARNELL" value="1312812"/>
<attribute name="OC_NEWARK" value="41K2816"/>
<attribute name="PACKAGE" value="8-MSOP"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMH6644MA" prefix="U">
<description>OpAmpIC</description>
<gates>
<gate name="A" symbol="LMH6644MA"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="+INA" pad="3"/>
<connect gate="A" pin="+INB" pad="5"/>
<connect gate="A" pin="+INC" pad="10"/>
<connect gate="A" pin="+IND" pad="12"/>
<connect gate="A" pin="-INA" pad="2"/>
<connect gate="A" pin="-INB" pad="6"/>
<connect gate="A" pin="-INC" pad="9"/>
<connect gate="A" pin="-IND" pad="13"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="OUTC" pad="8"/>
<connect gate="A" pin="OUTD" pad="14"/>
<connect gate="A" pin="V+" pad="4"/>
<connect gate="A" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMH6644MA"/>
<attribute name="OC_FARNELL" value="1286942"/>
<attribute name="OC_NEWARK" value="74C3663"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMH6644MT" prefix="U">
<description>Rail-to-Rail Output Amplifiers</description>
<gates>
<gate name="A" symbol="LMH6644MT"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-14N">
<connects>
<connect gate="A" pin="+INA" pad="3"/>
<connect gate="A" pin="+INB" pad="5"/>
<connect gate="A" pin="+INC" pad="10"/>
<connect gate="A" pin="+IND" pad="12"/>
<connect gate="A" pin="-INA" pad="2"/>
<connect gate="A" pin="-INB" pad="6"/>
<connect gate="A" pin="-INC" pad="9"/>
<connect gate="A" pin="-IND" pad="13"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="OUTC" pad="8"/>
<connect gate="A" pin="OUTD" pad="14"/>
<connect gate="A" pin="V+" pad="4"/>
<connect gate="A" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMH6644MT"/>
<attribute name="OC_FARNELL" value="1286943"/>
<attribute name="OC_NEWARK" value="41K2820"/>
<attribute name="PACKAGE" value="TSSOP--14"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMH6645MA" prefix="U">
<description>OpAmpIC</description>
<gates>
<gate name="A" symbol="LMH6645MA"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="NC" pad="8"/>
<connect gate="A" pin="NC_2" pad="5"/>
<connect gate="A" pin="NC_3" pad="1"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMH6645MA"/>
<attribute name="OC_FARNELL" value="1286944"/>
<attribute name="OC_NEWARK" value="34C6434"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMH6645MF" prefix="U">
<description>Amplifier</description>
<gates>
<gate name="A" symbol="LMH6645MF"/>
</gates>
<devices>
<device name="" package="SOT95P284X122-5N">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="4"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="A" pin="V+" pad="5"/>
<connect gate="A" pin="V-" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMH6645MF"/>
<attribute name="OC_FARNELL" value="1312813"/>
<attribute name="OC_NEWARK" value="31M5292"/>
<attribute name="PACKAGE" value="SOT23-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMH6646MA" prefix="U">
<description>OpAmpIC</description>
<gates>
<gate name="A" symbol="LMH6646MA"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="+INA" pad="3"/>
<connect gate="A" pin="+INB" pad="5"/>
<connect gate="A" pin="-INA" pad="2"/>
<connect gate="A" pin="-INB" pad="6"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMH6646MA"/>
<attribute name="OC_FARNELL" value="1286945"/>
<attribute name="OC_NEWARK" value="34C6436"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMH6646MM" prefix="U">
<description>Amplifiers</description>
<gates>
<gate name="A" symbol="LMH6646MM"/>
</gates>
<devices>
<device name="" package="SOP65P490X109-8N">
<connects>
<connect gate="A" pin="INA+" pad="3"/>
<connect gate="A" pin="INA-" pad="2"/>
<connect gate="A" pin="INB+" pad="5"/>
<connect gate="A" pin="INB-" pad="6"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMH6646MM"/>
<attribute name="OC_FARNELL" value="1496042"/>
<attribute name="OC_NEWARK" value="41K2828"/>
<attribute name="PACKAGE" value="MSOP-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMH6647MA" prefix="U">
<description>OpAmpIC</description>
<gates>
<gate name="A" symbol="LMH6647MA"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="NC" pad="5"/>
<connect gate="A" pin="NC_2" pad="1"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="SD" pad="8"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMH6647MA"/>
<attribute name="OC_FARNELL" value="1286946"/>
<attribute name="OC_NEWARK" value="26M0303"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMH6647MF" prefix="U">
<description>Rail-to-Rail Input and Output Amp</description>
<gates>
<gate name="A" symbol="LMH6647MF"/>
</gates>
<devices>
<device name="" package="SOT95P284X120-6N">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="4"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="A" pin="V+" pad="6"/>
<connect gate="A" pin="V-" pad="2"/>
<connect gate="A" pin="~SD" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMH6647MF"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K2832"/>
<attribute name="PACKAGE" value="SOT23-6"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMH6654MA" prefix="U">
<description>Noise Amplifiers</description>
<gates>
<gate name="A" symbol="LMH6654MA"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="NC" pad="8"/>
<connect gate="A" pin="NC_2" pad="5"/>
<connect gate="A" pin="NC_3" pad="1"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMH6654MA"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="34C6440"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMH6654MF" prefix="U">
<description>Operational Amplifier</description>
<gates>
<gate name="A" symbol="LMH6654MF"/>
</gates>
<devices>
<device name="" package="SOT95P285X120-5N">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="4"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="A" pin="V+" pad="5"/>
<connect gate="A" pin="V-" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMH6654MF"/>
<attribute name="OC_FARNELL" value="1312816"/>
<attribute name="OC_NEWARK" value="41K2836"/>
<attribute name="PACKAGE" value="SOT-23-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMH6655MA" prefix="U">
<description>OP AMP</description>
<gates>
<gate name="A" symbol="LMH6655MA"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="+INA" pad="3"/>
<connect gate="A" pin="+INB" pad="5"/>
<connect gate="A" pin="-INA" pad="2"/>
<connect gate="A" pin="-INB" pad="6"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMH6655MA"/>
<attribute name="OC_FARNELL" value="9490159"/>
<attribute name="OC_NEWARK" value="41K2838"/>
<attribute name="PACKAGE" value="8-SOIC"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMH6655MM" prefix="U">
<description>Noise Amplifiers</description>
<gates>
<gate name="A" symbol="LMH6655MM"/>
</gates>
<devices>
<device name="" package="SOP65P490X109-8N">
<connects>
<connect gate="A" pin="IN_A+" pad="3"/>
<connect gate="A" pin="IN_A-" pad="2"/>
<connect gate="A" pin="IN_B+" pad="5"/>
<connect gate="A" pin="IN_B-" pad="6"/>
<connect gate="A" pin="OUT_A" pad="1"/>
<connect gate="A" pin="OUT_B" pad="7"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMH6655MM"/>
<attribute name="OC_FARNELL" value="1312817"/>
<attribute name="OC_NEWARK" value="41K2840"/>
<attribute name="PACKAGE" value="8-MSOP"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMH6657MF" prefix="U">
<description>Single &amp; Dual Amplifiers</description>
<gates>
<gate name="A" symbol="LMH6657MF"/>
</gates>
<devices>
<device name="" package="SOT95P285X120-5N">
<connects>
<connect gate="A" pin="IN+" pad="3"/>
<connect gate="A" pin="IN-" pad="4"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="A" pin="V+" pad="5"/>
<connect gate="A" pin="V-" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMH6657MF"/>
<attribute name="OC_FARNELL" value="8180784"/>
<attribute name="OC_NEWARK" value="41K2842"/>
<attribute name="PACKAGE" value="SOT23-5"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMH6657MG" prefix="U">
<description>Single &amp; Dual Amplifiers</description>
<gates>
<gate name="A" symbol="LMH6657MG"/>
</gates>
<devices>
<device name="" package="SOT65P240X110-5N">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="4"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="A" pin="V+" pad="5"/>
<connect gate="A" pin="V-" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMH6657MG"/>
<attribute name="OC_FARNELL" value="8180792"/>
<attribute name="OC_NEWARK" value="41K2844"/>
<attribute name="PACKAGE" value="SC-70-5"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMH6658MA" prefix="U">
<description>Single Supply, Single &amp; Dual Amplifiers</description>
<gates>
<gate name="A" symbol="LMH6658MA"/>
</gates>
<devices>
<device name="" package="SOIC127P620X175-8N">
<connects>
<connect gate="A" pin="+INA" pad="3"/>
<connect gate="A" pin="+INB" pad="5"/>
<connect gate="A" pin="-INA" pad="2"/>
<connect gate="A" pin="-INB" pad="6"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMH6658MA"/>
<attribute name="OC_FARNELL" value="8180806"/>
<attribute name="OC_NEWARK" value="41K2846"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="National Semicoductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMH6658MM" prefix="U">
<description>Amplifiers</description>
<gates>
<gate name="A" symbol="LMH6658MM"/>
</gates>
<devices>
<device name="" package="SOP65P490X109-8N">
<connects>
<connect gate="A" pin="INA+" pad="3"/>
<connect gate="A" pin="INA-" pad="2"/>
<connect gate="A" pin="INB+" pad="6"/>
<connect gate="A" pin="INB-" pad="5"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMH6658MM"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K2848"/>
<attribute name="PACKAGE" value="MSOP-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMH6672MA" prefix="U">
<description>High Speed Op Amp</description>
<gates>
<gate name="A" symbol="LMH6672MA"/>
</gates>
<devices>
<device name="" package="SOIC127P620X175-8N">
<connects>
<connect gate="A" pin="+INA" pad="3"/>
<connect gate="A" pin="+INB" pad="5"/>
<connect gate="A" pin="-INA" pad="2"/>
<connect gate="A" pin="-INB" pad="6"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMH6672MA"/>
<attribute name="OC_FARNELL" value="9490140"/>
<attribute name="OC_NEWARK" value="34C6448"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="National Semicoductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMH6672MR" prefix="U">
<description>Dual, High Output Current, High Speed Op Amp</description>
<gates>
<gate name="A" symbol="LMH6672MR"/>
</gates>
<devices>
<device name="" package="SOIC127P620X168-9N">
<connects>
<connect gate="A" pin="+INA" pad="3"/>
<connect gate="A" pin="+INB" pad="5"/>
<connect gate="A" pin="-INA" pad="2"/>
<connect gate="A" pin="-INB" pad="6"/>
<connect gate="A" pin="EPAD" pad="9"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMH6672MR"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="34C6450"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMH6682MA" prefix="U">
<description>OP AMP</description>
<gates>
<gate name="A" symbol="LMH6682MA"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="+INA" pad="3"/>
<connect gate="A" pin="+INB" pad="5"/>
<connect gate="A" pin="-INA" pad="2"/>
<connect gate="A" pin="-INB" pad="6"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="OUT_A" pad="1"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMH6682MA"/>
<attribute name="OC_FARNELL" value="1286951"/>
<attribute name="OC_NEWARK" value="41K2856"/>
<attribute name="PACKAGE" value="8-SOIC"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMH6682MM" prefix="U">
<description>Amplifiers</description>
<gates>
<gate name="A" symbol="LMH6682MM"/>
</gates>
<devices>
<device name="" package="SOP65P490X109-8N">
<connects>
<connect gate="A" pin="INA+" pad="3"/>
<connect gate="A" pin="INA-" pad="2"/>
<connect gate="A" pin="INB+" pad="5"/>
<connect gate="A" pin="INB-" pad="6"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMH6682MM"/>
<attribute name="OC_FARNELL" value="1312818"/>
<attribute name="OC_NEWARK" value="41K2858"/>
<attribute name="PACKAGE" value="MSOP-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMH6683MA" prefix="U">
<description>OpAmpIC</description>
<gates>
<gate name="A" symbol="LMH6683MA"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="+IN1" pad="5"/>
<connect gate="A" pin="+IN2" pad="10"/>
<connect gate="A" pin="+IN3" pad="12"/>
<connect gate="A" pin="-IN1" pad="6"/>
<connect gate="A" pin="-IN2" pad="9"/>
<connect gate="A" pin="-IN3" pad="13"/>
<connect gate="A" pin="NC" pad="3"/>
<connect gate="A" pin="NC_2" pad="1"/>
<connect gate="A" pin="NC_3" pad="2"/>
<connect gate="A" pin="OUT1" pad="7"/>
<connect gate="A" pin="OUT2" pad="8"/>
<connect gate="A" pin="OUT3" pad="14"/>
<connect gate="A" pin="V+" pad="4"/>
<connect gate="A" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMH6683MA"/>
<attribute name="OC_FARNELL" value="1559330"/>
<attribute name="OC_NEWARK" value="41K2860"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMH6702JFQMLV" prefix="U">
<description>Ultra Low Distortion, Wideband Op Amp</description>
<gates>
<gate name="A" symbol="LMH6702JFQMLV"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-8">
<connects>
<connect gate="A" pin="+VCC" pad="7"/>
<connect gate="A" pin="-VCC" pad="4"/>
<connect gate="A" pin="NC" pad="8"/>
<connect gate="A" pin="NC_2" pad="5"/>
<connect gate="A" pin="NC_3" pad="1"/>
<connect gate="A" pin="VINV" pad="2"/>
<connect gate="A" pin="VNON-INV" pad="3"/>
<connect gate="A" pin="VOUT" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMH6702JFQMLV"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="31T9718"/>
<attribute name="PACKAGE" value="DIP-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMH6702MA" prefix="U">
<description>OPAMP</description>
<gates>
<gate name="A" symbol="LMH6702MA"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="IN+" pad="3"/>
<connect gate="A" pin="IN-" pad="2"/>
<connect gate="A" pin="N/C" pad="8"/>
<connect gate="A" pin="N/C_2" pad="1"/>
<connect gate="A" pin="N/C_3" pad="5"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMH6702MA"/>
<attribute name="OC_FARNELL" value="4398490"/>
<attribute name="OC_NEWARK" value="41K2864"/>
<attribute name="PACKAGE" value="8SOIC"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMH6702MF" prefix="U">
<description>Ultra Low Distortion, Wideband Op Amp</description>
<gates>
<gate name="A" symbol="LMH6702MF"/>
</gates>
<devices>
<device name="" package="SOT95P285X120-5N">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="4"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="A" pin="V+" pad="5"/>
<connect gate="A" pin="V-" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMH6702MF"/>
<attribute name="OC_FARNELL" value="1564741"/>
<attribute name="OC_NEWARK" value="41K2866"/>
<attribute name="PACKAGE" value="SOT-23-5"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMH6703MA" prefix="U">
<description>Low Distortion Op Amp</description>
<gates>
<gate name="A" symbol="LMH6703MA"/>
</gates>
<devices>
<device name="" package="SOIC127P620X175-8N">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="N/C" pad="5"/>
<connect gate="A" pin="N/C_2" pad="1"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="VS+" pad="7"/>
<connect gate="A" pin="VS-" pad="4"/>
<connect gate="A" pin="~SD" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMH6703MA"/>
<attribute name="OC_FARNELL" value="1008276"/>
<attribute name="OC_NEWARK" value="41K2868"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="National Semicoductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMH6703MF" prefix="U">
<description>Low Distortion Op Amp</description>
<gates>
<gate name="A" symbol="LMH6703MF"/>
</gates>
<devices>
<device name="" package="SOT95P284X120-6N">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="4"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="A" pin="V+" pad="6"/>
<connect gate="A" pin="V-" pad="2"/>
<connect gate="A" pin="~SD" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMH6703MF"/>
<attribute name="OC_FARNELL" value="1312605"/>
<attribute name="OC_NEWARK" value="65K5777"/>
<attribute name="PACKAGE" value="SOT23-6"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMH6704MA" prefix="U">
<description>650 MHz Selectable Gain Buffer</description>
<gates>
<gate name="A" symbol="LMH6704MA"/>
</gates>
<devices>
<device name="" package="SOIC127P620X175-8N">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="N/C" pad="5"/>
<connect gate="A" pin="N/C_2" pad="1"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="VS+" pad="7"/>
<connect gate="A" pin="VS-" pad="4"/>
<connect gate="A" pin="~DIS" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMH6704MA"/>
<attribute name="OC_FARNELL" value="1008277"/>
<attribute name="OC_NEWARK" value="92K5959"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="National Semicoductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMH6714MA" prefix="U">
<description>OP AMP</description>
<gates>
<gate name="A" symbol="LMH6714MA"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="NC" pad="8"/>
<connect gate="A" pin="NC_2" pad="1"/>
<connect gate="A" pin="NC_3" pad="5"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMH6714MA"/>
<attribute name="OC_FARNELL" value="8180857"/>
<attribute name="OC_NEWARK" value="41K2874"/>
<attribute name="PACKAGE" value="8-SOIC"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMH6714MF" prefix="U">
<description>Wideband Video Op Amp</description>
<gates>
<gate name="A" symbol="LMH6714MF"/>
</gates>
<devices>
<device name="" package="SOT95P285X120-5N">
<connects>
<connect gate="A" pin="IN+" pad="3"/>
<connect gate="A" pin="IN-" pad="4"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="A" pin="V+" pad="5"/>
<connect gate="A" pin="V-" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMH6714MF"/>
<attribute name="OC_FARNELL" value="8180865"/>
<attribute name="OC_NEWARK" value="41K2876"/>
<attribute name="PACKAGE" value="SOT23-5"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMH6715MA" prefix="U">
<description>OpAmpIC</description>
<gates>
<gate name="A" symbol="LMH6715MA"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="+VCC" pad="8"/>
<connect gate="A" pin="-VCC" pad="4"/>
<connect gate="A" pin="VIN1" pad="2"/>
<connect gate="A" pin="VIN2" pad="6"/>
<connect gate="A" pin="VNON-INV1" pad="3"/>
<connect gate="A" pin="VNON-INV2" pad="5"/>
<connect gate="A" pin="VOUT1" pad="1"/>
<connect gate="A" pin="VOUT2" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMH6715MA"/>
<attribute name="OC_FARNELL" value="1564715"/>
<attribute name="OC_NEWARK" value="41K2878"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMH6720MA" prefix="U">
<description>OP AMP</description>
<gates>
<gate name="A" symbol="LMH6720MA"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="NC" pad="1"/>
<connect gate="A" pin="NC_2" pad="5"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
<connect gate="A" pin="~SD" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMH6720MA"/>
<attribute name="OC_FARNELL" value="8180873"/>
<attribute name="OC_NEWARK" value="41K2882"/>
<attribute name="PACKAGE" value="8-SOIC"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMH6720MF" prefix="U">
<description>Wideband Video Op Amp</description>
<gates>
<gate name="A" symbol="LMH6720MF"/>
</gates>
<devices>
<device name="" package="SOT95P285X120-6N">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="4"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="A" pin="V+" pad="6"/>
<connect gate="A" pin="V-" pad="2"/>
<connect gate="A" pin="~SD" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMH6720MF"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K2884"/>
<attribute name="PACKAGE" value="SOT-6"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMH6722MA" prefix="U">
<description>Wideband Video Op Amp</description>
<gates>
<gate name="A" symbol="LMH6722MA"/>
</gates>
<devices>
<device name="" package="SOIC127P620X175-14N">
<connects>
<connect gate="A" pin="+INA" pad="3"/>
<connect gate="A" pin="+INB" pad="5"/>
<connect gate="A" pin="+INC" pad="10"/>
<connect gate="A" pin="+IND" pad="12"/>
<connect gate="A" pin="-INA" pad="2"/>
<connect gate="A" pin="-INB" pad="6"/>
<connect gate="A" pin="-INC" pad="9"/>
<connect gate="A" pin="-IND" pad="13"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="OUTC" pad="8"/>
<connect gate="A" pin="OUTD" pad="14"/>
<connect gate="A" pin="V+" pad="4"/>
<connect gate="A" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMH6722MA"/>
<attribute name="OC_FARNELL" value="8180890"/>
<attribute name="OC_NEWARK" value="41K2886"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMH6722QSD" prefix="U">
<description>Wideband Video Op Amp</description>
<gates>
<gate name="A" symbol="LMH6722QSD"/>
</gates>
<devices>
<device name="" package="DFN400X300X80-15N">
<connects>
<connect gate="A" pin="+INA" pad="3"/>
<connect gate="A" pin="+INB" pad="5"/>
<connect gate="A" pin="+INC" pad="10"/>
<connect gate="A" pin="+IND" pad="12"/>
<connect gate="A" pin="-INA" pad="2"/>
<connect gate="A" pin="-INB" pad="6"/>
<connect gate="A" pin="-INC" pad="9"/>
<connect gate="A" pin="-IND" pad="13"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="OUTC" pad="8"/>
<connect gate="A" pin="OUTD" pad="14"/>
<connect gate="A" pin="THER_PAD" pad="15"/>
<connect gate="A" pin="V+" pad="4"/>
<connect gate="A" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMH6722QSD"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="55R3717"/>
<attribute name="PACKAGE" value="DFN-14"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMH6722SD" prefix="U">
<description>Wideband Video Op Amp</description>
<gates>
<gate name="A" symbol="LMH6722SD"/>
</gates>
<devices>
<device name="" package="DFN400X300X80-15N">
<connects>
<connect gate="A" pin="+INA" pad="3"/>
<connect gate="A" pin="+INB" pad="5"/>
<connect gate="A" pin="+INC" pad="10"/>
<connect gate="A" pin="+IND" pad="12"/>
<connect gate="A" pin="-INA" pad="2"/>
<connect gate="A" pin="-INB" pad="6"/>
<connect gate="A" pin="-INC" pad="9"/>
<connect gate="A" pin="-IND" pad="13"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="OUTC" pad="8"/>
<connect gate="A" pin="OUTD" pad="14"/>
<connect gate="A" pin="THER_PAD" pad="15"/>
<connect gate="A" pin="V+" pad="4"/>
<connect gate="A" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMH6722SD"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="55R3719"/>
<attribute name="PACKAGE" value="DFN-14"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMH6723MA" prefix="U">
<description>OpAmpIC</description>
<gates>
<gate name="A" symbol="LMH6723MA"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="NC" pad="8"/>
<connect gate="A" pin="NC_2" pad="5"/>
<connect gate="A" pin="NC_3" pad="1"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMH6723MA"/>
<attribute name="OC_FARNELL" value="1693965"/>
<attribute name="OC_NEWARK" value="41K2888"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMH6723MF" prefix="U">
<description>Current Feedback Op-Amp</description>
<gates>
<gate name="A" symbol="LMH6723MF"/>
</gates>
<devices>
<device name="" package="SOT95P285X120-5N">
<connects>
<connect gate="A" pin="IN+" pad="3"/>
<connect gate="A" pin="IN-" pad="4"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="A" pin="V+" pad="5"/>
<connect gate="A" pin="V-" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMH6723MF"/>
<attribute name="OC_FARNELL" value="8180911"/>
<attribute name="OC_NEWARK" value="38K3537"/>
<attribute name="PACKAGE" value="SOT23-5"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMH6724MA" prefix="U">
<description>Current Feedback Op-Amp</description>
<gates>
<gate name="A" symbol="LMH6724MA"/>
</gates>
<devices>
<device name="" package="SOIC127P620X175-8N">
<connects>
<connect gate="A" pin="+INA" pad="3"/>
<connect gate="A" pin="+INB" pad="5"/>
<connect gate="A" pin="-INA" pad="2"/>
<connect gate="A" pin="-INB" pad="6"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMH6724MA"/>
<attribute name="OC_FARNELL" value="8180920"/>
<attribute name="OC_NEWARK" value="38K3538"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="National Semicoductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMH6732MF" prefix="U">
<description>High Speed Op Amp</description>
<gates>
<gate name="A" symbol="LMH6732MF"/>
</gates>
<devices>
<device name="" package="SOT95P285X120-6N">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="4"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="A" pin="RP" pad="5"/>
<connect gate="A" pin="V+" pad="6"/>
<connect gate="A" pin="V-" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMH6732MF"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K2898"/>
<attribute name="PACKAGE" value="SOT-23-6"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMH6733MQ" prefix="U">
<description>Triple Operational Amplifier</description>
<gates>
<gate name="A" symbol="LMH6733MQ"/>
</gates>
<devices>
<device name="" package="SOP63P640X170-16N">
<connects>
<connect gate="A" pin="+INA" pad="2"/>
<connect gate="A" pin="+INB" pad="5"/>
<connect gate="A" pin="+INC" pad="8"/>
<connect gate="A" pin="-INA" pad="1"/>
<connect gate="A" pin="-INB" pad="4"/>
<connect gate="A" pin="-INC" pad="7"/>
<connect gate="A" pin="OUTA" pad="14"/>
<connect gate="A" pin="OUTB" pad="12"/>
<connect gate="A" pin="OUTC" pad="10"/>
<connect gate="A" pin="VS+" pad="15"/>
<connect gate="A" pin="VS+_2" pad="11"/>
<connect gate="A" pin="VS-" pad="13"/>
<connect gate="A" pin="VS-_2" pad="9"/>
<connect gate="A" pin="~DIS_A" pad="16"/>
<connect gate="A" pin="~DIS_B" pad="3"/>
<connect gate="A" pin="~DIS_C" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMH6733MQ"/>
<attribute name="OC_FARNELL" value="1333959"/>
<attribute name="OC_NEWARK" value="32M0950"/>
<attribute name="PACKAGE" value="SSOP-16"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMH6738MQ" prefix="U">
<description>Very Wideband, Low Distortion Triple Op Amp</description>
<gates>
<gate name="A" symbol="LMH6738MQ"/>
</gates>
<devices>
<device name="" package="SOP63P640X170-16N">
<connects>
<connect gate="A" pin="+INA" pad="2"/>
<connect gate="A" pin="+INB" pad="5"/>
<connect gate="A" pin="+INC" pad="8"/>
<connect gate="A" pin="-INA" pad="1"/>
<connect gate="A" pin="-INB" pad="4"/>
<connect gate="A" pin="-INC" pad="7"/>
<connect gate="A" pin="OUTA" pad="14"/>
<connect gate="A" pin="OUTB" pad="12"/>
<connect gate="A" pin="OUTC" pad="10"/>
<connect gate="A" pin="VS+" pad="15"/>
<connect gate="A" pin="VS+_2" pad="11"/>
<connect gate="A" pin="VS-" pad="9"/>
<connect gate="A" pin="VS-_2" pad="13"/>
<connect gate="A" pin="~DIS_A" pad="16"/>
<connect gate="A" pin="~DIS_B" pad="3"/>
<connect gate="A" pin="~DIS_C" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMH6738MQ"/>
<attribute name="OC_FARNELL" value="8180970"/>
<attribute name="OC_NEWARK" value="38K3542"/>
<attribute name="PACKAGE" value="SSOP-16"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMH6739MQ" prefix="U">
<description>Low Distortion Triple Video Buffer</description>
<gates>
<gate name="A" symbol="LMH6739MQ"/>
</gates>
<devices>
<device name="" package="SOP65P640X170-16N">
<connects>
<connect gate="A" pin="+INA" pad="2"/>
<connect gate="A" pin="+INB" pad="5"/>
<connect gate="A" pin="+INC" pad="8"/>
<connect gate="A" pin="-INA" pad="1"/>
<connect gate="A" pin="-INB" pad="4"/>
<connect gate="A" pin="-INC" pad="7"/>
<connect gate="A" pin="OUTA" pad="14"/>
<connect gate="A" pin="OUTB" pad="12"/>
<connect gate="A" pin="OUTC" pad="10"/>
<connect gate="A" pin="VS+" pad="11"/>
<connect gate="A" pin="VS+_2" pad="15"/>
<connect gate="A" pin="VS-" pad="13"/>
<connect gate="A" pin="VS-_2" pad="9"/>
<connect gate="A" pin="~DISA" pad="16"/>
<connect gate="A" pin="~DISB" pad="3"/>
<connect gate="A" pin="~DISC" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMH6739MQ"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K2902"/>
<attribute name="PACKAGE" value="SSOP-16"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMH7220MG" prefix="U">
<description>Speed Comparator</description>
<gates>
<gate name="A" symbol="LMH7220MG"/>
</gates>
<devices>
<device name="" package="SOT65P210X110-6N">
<connects>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="IN+" pad="6"/>
<connect gate="A" pin="IN-" pad="1"/>
<connect gate="A" pin="OUT_Q" pad="4"/>
<connect gate="A" pin="OUT_~Q" pad="3"/>
<connect gate="A" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMH7220MG"/>
<attribute name="OC_FARNELL" value="1609190"/>
<attribute name="OC_NEWARK" value="11N9148"/>
<attribute name="PACKAGE" value="SC-70-6"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMH7220MK" prefix="U">
<description>High Speed Comparator</description>
<gates>
<gate name="A" symbol="LMH7220MK"/>
</gates>
<devices>
<device name="" package="SOT95P285X100-6N">
<connects>
<connect gate="A" pin="+IN" pad="6"/>
<connect gate="A" pin="-IN" pad="1"/>
<connect gate="A" pin="OUT_Q" pad="4"/>
<connect gate="A" pin="OUT_~Q" pad="3"/>
<connect gate="A" pin="V-" pad="2"/>
<connect gate="A" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMH7220MK"/>
<attribute name="OC_FARNELL" value="1685408"/>
<attribute name="OC_NEWARK" value="13M1673"/>
<attribute name="PACKAGE" value="SOT-23-9"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMH7322SQ" prefix="U">
<description>High Speed Comparator</description>
<gates>
<gate name="A" symbol="LMH7322SQ"/>
</gates>
<devices>
<device name="" package="QFN50P400X400X80-25N">
<connects>
<connect gate="A" pin="+INA" pad="8"/>
<connect gate="A" pin="+INB" pad="11"/>
<connect gate="A" pin="-INA" pad="7"/>
<connect gate="A" pin="-INB" pad="12"/>
<connect gate="A" pin="EPAD" pad="25"/>
<connect gate="A" pin="LEA" pad="2"/>
<connect gate="A" pin="LEB" pad="17"/>
<connect gate="A" pin="QA" pad="23"/>
<connect gate="A" pin="QB" pad="20"/>
<connect gate="A" pin="RFREFA" pad="9"/>
<connect gate="A" pin="RFREFB" pad="10"/>
<connect gate="A" pin="RHYSA" pad="6"/>
<connect gate="A" pin="RHYSB" pad="13"/>
<connect gate="A" pin="VCCIA" pad="5"/>
<connect gate="A" pin="VCCIB" pad="14"/>
<connect gate="A" pin="VCCO" pad="1"/>
<connect gate="A" pin="VCCOA" pad="22"/>
<connect gate="A" pin="VCCOB" pad="21"/>
<connect gate="A" pin="VCCOB_2" pad="18"/>
<connect gate="A" pin="VEEA" pad="4"/>
<connect gate="A" pin="VEEB" pad="15"/>
<connect gate="A" pin="~LEA" pad="3"/>
<connect gate="A" pin="~LEB" pad="16"/>
<connect gate="A" pin="~QA" pad="24"/>
<connect gate="A" pin="~QB" pad="19"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMH7322SQ"/>
<attribute name="OC_FARNELL" value="1359428"/>
<attribute name="OC_NEWARK" value="39M4947"/>
<attribute name="PACKAGE" value="QFN-24"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMH7324SQ" prefix="U">
<description>Speed Comparator</description>
<gates>
<gate name="A" symbol="LMH7324SQ"/>
</gates>
<devices>
<device name="" package="QFN50P500X500X80-33N">
<connects>
<connect gate="A" pin="DAP" pad="33"/>
<connect gate="A" pin="INA+" pad="30"/>
<connect gate="A" pin="INA-" pad="31"/>
<connect gate="A" pin="INB+" pad="11"/>
<connect gate="A" pin="INB-" pad="10"/>
<connect gate="A" pin="INC+" pad="14"/>
<connect gate="A" pin="INC-" pad="15"/>
<connect gate="A" pin="IND+" pad="27"/>
<connect gate="A" pin="IND-" pad="26"/>
<connect gate="A" pin="QA" pad="3"/>
<connect gate="A" pin="QB" pad="6"/>
<connect gate="A" pin="QC" pad="19"/>
<connect gate="A" pin="QD" pad="22"/>
<connect gate="A" pin="VCCIA" pad="32"/>
<connect gate="A" pin="VCCIB" pad="9"/>
<connect gate="A" pin="VCCIC" pad="16"/>
<connect gate="A" pin="VCCID" pad="25"/>
<connect gate="A" pin="VCCOA" pad="1"/>
<connect gate="A" pin="VCCOB" pad="8"/>
<connect gate="A" pin="VCCOC" pad="17"/>
<connect gate="A" pin="VCCOD" pad="24"/>
<connect gate="A" pin="VEEA" pad="29"/>
<connect gate="A" pin="VEEA_2" pad="4"/>
<connect gate="A" pin="VEEB" pad="12"/>
<connect gate="A" pin="VEEB_2" pad="5"/>
<connect gate="A" pin="VEEC" pad="20"/>
<connect gate="A" pin="VEEC_2" pad="13"/>
<connect gate="A" pin="VEED" pad="28"/>
<connect gate="A" pin="VEED_2" pad="21"/>
<connect gate="A" pin="~QA" pad="2"/>
<connect gate="A" pin="~QB" pad="7"/>
<connect gate="A" pin="~QC" pad="18"/>
<connect gate="A" pin="~QD" pad="23"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMH7324SQ"/>
<attribute name="OC_FARNELL" value="1506815"/>
<attribute name="OC_NEWARK" value="74M2656"/>
<attribute name="PACKAGE" value="LLP-32"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMK01000ISQ" prefix="U">
<description>High Performance Clock Buffer Divider</description>
<gates>
<gate name="A" symbol="LMK01000ISQ"/>
</gates>
<devices>
<device name="" package="QFN50P700X700X80-49N">
<connects>
<connect gate="A" pin="BIAS" pad="36"/>
<connect gate="A" pin="CLKIN0" pad="28"/>
<connect gate="A" pin="CLKIN1" pad="34"/>
<connect gate="A" pin="CLKOUT0" pad="14"/>
<connect gate="A" pin="CLKOUT1" pad="17"/>
<connect gate="A" pin="CLKOUT2" pad="20"/>
<connect gate="A" pin="CLKOUT3" pad="23"/>
<connect gate="A" pin="CLKOUT4" pad="38"/>
<connect gate="A" pin="CLKOUT5" pad="41"/>
<connect gate="A" pin="CLKOUT6" pad="44"/>
<connect gate="A" pin="CLKOUT7" pad="47"/>
<connect gate="A" pin="CLKUWIRE" pad="4"/>
<connect gate="A" pin="DATAUWIRE" pad="5"/>
<connect gate="A" pin="EPAD" pad="49"/>
<connect gate="A" pin="GND" pad="25"/>
<connect gate="A" pin="GND_2" pad="1"/>
<connect gate="A" pin="GOE" pad="11"/>
<connect gate="A" pin="LEUWIRE" pad="6"/>
<connect gate="A" pin="NC" pad="32"/>
<connect gate="A" pin="NC_2" pad="7"/>
<connect gate="A" pin="NC_3" pad="2"/>
<connect gate="A" pin="NC_4" pad="9"/>
<connect gate="A" pin="NC_5" pad="10"/>
<connect gate="A" pin="TEST" pad="12"/>
<connect gate="A" pin="VCC1" pad="3"/>
<connect gate="A" pin="VCC10" pad="33"/>
<connect gate="A" pin="VCC11" pad="37"/>
<connect gate="A" pin="VCC12" pad="40"/>
<connect gate="A" pin="VCC13" pad="43"/>
<connect gate="A" pin="VCC14" pad="46"/>
<connect gate="A" pin="VCC2" pad="8"/>
<connect gate="A" pin="VCC3" pad="13"/>
<connect gate="A" pin="VCC4" pad="16"/>
<connect gate="A" pin="VCC5" pad="19"/>
<connect gate="A" pin="VCC6" pad="22"/>
<connect gate="A" pin="VCC7" pad="26"/>
<connect gate="A" pin="VCC8" pad="30"/>
<connect gate="A" pin="VCC9" pad="31"/>
<connect gate="A" pin="~CLKIN0" pad="29"/>
<connect gate="A" pin="~CLKIN1" pad="35"/>
<connect gate="A" pin="~CLKOUT0" pad="15"/>
<connect gate="A" pin="~CLKOUT1" pad="18"/>
<connect gate="A" pin="~CLKOUT2" pad="21"/>
<connect gate="A" pin="~CLKOUT3" pad="24"/>
<connect gate="A" pin="~CLKOUT4" pad="39"/>
<connect gate="A" pin="~CLKOUT5" pad="42"/>
<connect gate="A" pin="~CLKOUT6" pad="45"/>
<connect gate="A" pin="~CLKOUT7" pad="48"/>
<connect gate="A" pin="~SYNC" pad="27"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMK01000ISQ"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="84M8055"/>
<attribute name="PACKAGE" value="QFN-48"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMK01010ISQ" prefix="U">
<description>High Performance Clock Buffer Divider</description>
<gates>
<gate name="A" symbol="LMK01010ISQ"/>
</gates>
<devices>
<device name="" package="QFN50P700X700X80-49N">
<connects>
<connect gate="A" pin="BIAS" pad="36"/>
<connect gate="A" pin="CLKIN0" pad="28"/>
<connect gate="A" pin="CLKIN1" pad="34"/>
<connect gate="A" pin="CLKOUT0" pad="14"/>
<connect gate="A" pin="CLKOUT1" pad="17"/>
<connect gate="A" pin="CLKOUT2" pad="20"/>
<connect gate="A" pin="CLKOUT3" pad="23"/>
<connect gate="A" pin="CLKOUT4" pad="38"/>
<connect gate="A" pin="CLKOUT5" pad="41"/>
<connect gate="A" pin="CLKOUT6" pad="44"/>
<connect gate="A" pin="CLKOUT7" pad="47"/>
<connect gate="A" pin="CLKUWIRE" pad="4"/>
<connect gate="A" pin="DATAUWIRE" pad="5"/>
<connect gate="A" pin="EPAD" pad="49"/>
<connect gate="A" pin="GND" pad="25"/>
<connect gate="A" pin="GND_2" pad="1"/>
<connect gate="A" pin="GOE" pad="11"/>
<connect gate="A" pin="LEUWIRE" pad="6"/>
<connect gate="A" pin="NC" pad="32"/>
<connect gate="A" pin="NC_2" pad="7"/>
<connect gate="A" pin="NC_3" pad="2"/>
<connect gate="A" pin="NC_4" pad="9"/>
<connect gate="A" pin="NC_5" pad="10"/>
<connect gate="A" pin="TEST" pad="12"/>
<connect gate="A" pin="VCC1" pad="3"/>
<connect gate="A" pin="VCC10" pad="33"/>
<connect gate="A" pin="VCC11" pad="37"/>
<connect gate="A" pin="VCC12" pad="40"/>
<connect gate="A" pin="VCC13" pad="43"/>
<connect gate="A" pin="VCC14" pad="46"/>
<connect gate="A" pin="VCC2" pad="8"/>
<connect gate="A" pin="VCC3" pad="13"/>
<connect gate="A" pin="VCC4" pad="16"/>
<connect gate="A" pin="VCC5" pad="19"/>
<connect gate="A" pin="VCC6" pad="22"/>
<connect gate="A" pin="VCC7" pad="26"/>
<connect gate="A" pin="VCC8" pad="30"/>
<connect gate="A" pin="VCC9" pad="31"/>
<connect gate="A" pin="~CLKIN0" pad="29"/>
<connect gate="A" pin="~CLKIN1" pad="35"/>
<connect gate="A" pin="~CLKOUT0" pad="15"/>
<connect gate="A" pin="~CLKOUT1" pad="18"/>
<connect gate="A" pin="~CLKOUT2" pad="21"/>
<connect gate="A" pin="~CLKOUT3" pad="24"/>
<connect gate="A" pin="~CLKOUT4" pad="39"/>
<connect gate="A" pin="~CLKOUT5" pad="42"/>
<connect gate="A" pin="~CLKOUT6" pad="45"/>
<connect gate="A" pin="~CLKOUT7" pad="48"/>
<connect gate="A" pin="~SYNC" pad="27"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMK01010ISQ"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="84M8058"/>
<attribute name="PACKAGE" value="QFN-48"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMK02000ISQ" prefix="U">
<description>Precision Clock Conditioner</description>
<gates>
<gate name="A" symbol="LMK02000ISQ"/>
</gates>
<devices>
<device name="" package="QFN50P700X700X80-49N">
<connects>
<connect gate="A" pin="BIAS" pad="36"/>
<connect gate="A" pin="CLKIN" pad="28"/>
<connect gate="A" pin="CLKOUT0" pad="14"/>
<connect gate="A" pin="CLKOUT1" pad="17"/>
<connect gate="A" pin="CLKOUT2" pad="20"/>
<connect gate="A" pin="CLKOUT3" pad="23"/>
<connect gate="A" pin="CLKOUT4" pad="38"/>
<connect gate="A" pin="CLKOUT5" pad="41"/>
<connect gate="A" pin="CLKOUT6" pad="44"/>
<connect gate="A" pin="CLKOUT7" pad="47"/>
<connect gate="A" pin="CLKUWIRE" pad="4"/>
<connect gate="A" pin="CPOUT" pad="32"/>
<connect gate="A" pin="DATAUWIRE" pad="5"/>
<connect gate="A" pin="EPAD" pad="49"/>
<connect gate="A" pin="FIN" pad="34"/>
<connect gate="A" pin="GND" pad="25"/>
<connect gate="A" pin="GND_2" pad="1"/>
<connect gate="A" pin="GOE" pad="11"/>
<connect gate="A" pin="LD" pad="12"/>
<connect gate="A" pin="LDOBYP1" pad="9"/>
<connect gate="A" pin="LDOBYP2" pad="10"/>
<connect gate="A" pin="LEUWIRE" pad="6"/>
<connect gate="A" pin="NC" pad="2"/>
<connect gate="A" pin="NC_2" pad="7"/>
<connect gate="A" pin="VCC1" pad="3"/>
<connect gate="A" pin="VCC10" pad="33"/>
<connect gate="A" pin="VCC11" pad="37"/>
<connect gate="A" pin="VCC12" pad="40"/>
<connect gate="A" pin="VCC13" pad="43"/>
<connect gate="A" pin="VCC14" pad="46"/>
<connect gate="A" pin="VCC2" pad="8"/>
<connect gate="A" pin="VCC3" pad="13"/>
<connect gate="A" pin="VCC4" pad="16"/>
<connect gate="A" pin="VCC5" pad="19"/>
<connect gate="A" pin="VCC6" pad="22"/>
<connect gate="A" pin="VCC7" pad="26"/>
<connect gate="A" pin="VCC8" pad="30"/>
<connect gate="A" pin="VCC9" pad="31"/>
<connect gate="A" pin="~CLKIN" pad="29"/>
<connect gate="A" pin="~CLKOUT0" pad="15"/>
<connect gate="A" pin="~CLKOUT1" pad="18"/>
<connect gate="A" pin="~CLKOUT2" pad="21"/>
<connect gate="A" pin="~CLKOUT3" pad="24"/>
<connect gate="A" pin="~CLKOUT4" pad="39"/>
<connect gate="A" pin="~CLKOUT5" pad="42"/>
<connect gate="A" pin="~CLKOUT6" pad="45"/>
<connect gate="A" pin="~CLKOUT7" pad="48"/>
<connect gate="A" pin="~FIN" pad="35"/>
<connect gate="A" pin="~SYNC" pad="27"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMK02000ISQ"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="39M4948"/>
<attribute name="PACKAGE" value="QFN-48"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMK02002ISQ" prefix="U">
<description>Precision Clock Conditioner</description>
<gates>
<gate name="A" symbol="LMK02002ISQ"/>
</gates>
<devices>
<device name="" package="QFN50P700X700X80-49N">
<connects>
<connect gate="A" pin="BIAS" pad="36"/>
<connect gate="A" pin="CLKIN" pad="28"/>
<connect gate="A" pin="CLKOUT0" pad="38"/>
<connect gate="A" pin="CLKOUT1" pad="41"/>
<connect gate="A" pin="CLKOUT2" pad="44"/>
<connect gate="A" pin="CLKOUT3" pad="47"/>
<connect gate="A" pin="CLKUWIRE" pad="4"/>
<connect gate="A" pin="CPOUT" pad="32"/>
<connect gate="A" pin="DATAUWIRE" pad="5"/>
<connect gate="A" pin="EPAD" pad="49"/>
<connect gate="A" pin="FIN" pad="34"/>
<connect gate="A" pin="GND" pad="25"/>
<connect gate="A" pin="GND_2" pad="1"/>
<connect gate="A" pin="GOE" pad="11"/>
<connect gate="A" pin="LD" pad="12"/>
<connect gate="A" pin="LDOBYP1" pad="9"/>
<connect gate="A" pin="LDOBYP2" pad="10"/>
<connect gate="A" pin="LEUWIRE" pad="6"/>
<connect gate="A" pin="NC" pad="2"/>
<connect gate="A" pin="NC_10" pad="24"/>
<connect gate="A" pin="NC_2" pad="7"/>
<connect gate="A" pin="NC_3" pad="17"/>
<connect gate="A" pin="NC_4" pad="15"/>
<connect gate="A" pin="NC_5" pad="14"/>
<connect gate="A" pin="NC_6" pad="20"/>
<connect gate="A" pin="NC_7" pad="23"/>
<connect gate="A" pin="NC_8" pad="21"/>
<connect gate="A" pin="NC_9" pad="18"/>
<connect gate="A" pin="VCC1" pad="3"/>
<connect gate="A" pin="VCC10" pad="33"/>
<connect gate="A" pin="VCC11" pad="37"/>
<connect gate="A" pin="VCC12" pad="40"/>
<connect gate="A" pin="VCC13" pad="43"/>
<connect gate="A" pin="VCC14" pad="46"/>
<connect gate="A" pin="VCC2" pad="8"/>
<connect gate="A" pin="VCC3" pad="13"/>
<connect gate="A" pin="VCC4" pad="16"/>
<connect gate="A" pin="VCC5" pad="19"/>
<connect gate="A" pin="VCC6" pad="22"/>
<connect gate="A" pin="VCC7" pad="26"/>
<connect gate="A" pin="VCC8" pad="30"/>
<connect gate="A" pin="VCC9" pad="31"/>
<connect gate="A" pin="~CLKIN" pad="29"/>
<connect gate="A" pin="~CLKOUT0" pad="39"/>
<connect gate="A" pin="~CLKOUT1" pad="42"/>
<connect gate="A" pin="~CLKOUT2" pad="45"/>
<connect gate="A" pin="~CLKOUT3" pad="48"/>
<connect gate="A" pin="~FIN" pad="35"/>
<connect gate="A" pin="~SYNC" pad="27"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMK02000ISQ"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="54M4611"/>
<attribute name="PACKAGE" value="QFN-48"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMK03000CISQ" prefix="U">
<description>Precision Clock Conditioner</description>
<gates>
<gate name="A" symbol="LMK03000CISQ"/>
</gates>
<devices>
<device name="" package="QFN50P700X700X80-49N">
<connects>
<connect gate="A" pin="BIAS" pad="36"/>
<connect gate="A" pin="CLKOUT0" pad="14"/>
<connect gate="A" pin="CLKOUT1" pad="17"/>
<connect gate="A" pin="CLKOUT2" pad="20"/>
<connect gate="A" pin="CLKOUT3" pad="23"/>
<connect gate="A" pin="CLKOUT4" pad="38"/>
<connect gate="A" pin="CLKOUT5" pad="41"/>
<connect gate="A" pin="CLKOUT6" pad="44"/>
<connect gate="A" pin="CLKOUT7" pad="47"/>
<connect gate="A" pin="CLKUWIRE" pad="4"/>
<connect gate="A" pin="CPOUT" pad="32"/>
<connect gate="A" pin="DATAUWIRE" pad="5"/>
<connect gate="A" pin="EPAD" pad="49"/>
<connect gate="A" pin="FOUT" pad="2"/>
<connect gate="A" pin="GND" pad="25"/>
<connect gate="A" pin="GND_2" pad="1"/>
<connect gate="A" pin="GOE" pad="11"/>
<connect gate="A" pin="LD" pad="12"/>
<connect gate="A" pin="LDOBYP1" pad="9"/>
<connect gate="A" pin="LDOBYP2" pad="10"/>
<connect gate="A" pin="LEUWIRE" pad="6"/>
<connect gate="A" pin="NC" pad="35"/>
<connect gate="A" pin="NC_2" pad="7"/>
<connect gate="A" pin="NC_3" pad="34"/>
<connect gate="A" pin="OSCIN" pad="29"/>
<connect gate="A" pin="OSCIN_2" pad="28"/>
<connect gate="A" pin="VCC1" pad="3"/>
<connect gate="A" pin="VCC10" pad="33"/>
<connect gate="A" pin="VCC11" pad="37"/>
<connect gate="A" pin="VCC12" pad="40"/>
<connect gate="A" pin="VCC13" pad="43"/>
<connect gate="A" pin="VCC14" pad="46"/>
<connect gate="A" pin="VCC2" pad="8"/>
<connect gate="A" pin="VCC3" pad="13"/>
<connect gate="A" pin="VCC4" pad="16"/>
<connect gate="A" pin="VCC5" pad="19"/>
<connect gate="A" pin="VCC6" pad="22"/>
<connect gate="A" pin="VCC7" pad="26"/>
<connect gate="A" pin="VCC8" pad="30"/>
<connect gate="A" pin="VCC9" pad="31"/>
<connect gate="A" pin="~CLKOUT0" pad="15"/>
<connect gate="A" pin="~CLKOUT1" pad="18"/>
<connect gate="A" pin="~CLKOUT2" pad="21"/>
<connect gate="A" pin="~CLKOUT3" pad="24"/>
<connect gate="A" pin="~CLKOUT4" pad="39"/>
<connect gate="A" pin="~CLKOUT5" pad="42"/>
<connect gate="A" pin="~CLKOUT6" pad="45"/>
<connect gate="A" pin="~CLKOUT7" pad="48"/>
<connect gate="A" pin="~SYNC" pad="27"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMK03000CISQ"/>
<attribute name="OC_FARNELL" value="1364442"/>
<attribute name="OC_NEWARK" value="39M4949"/>
<attribute name="PACKAGE" value="QFN-48"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMK03000DISQ" prefix="U">
<description>Precision Clock Conditioner</description>
<gates>
<gate name="A" symbol="LMK03000DISQ"/>
</gates>
<devices>
<device name="" package="QFN50P700X700X80-49N">
<connects>
<connect gate="A" pin="BIAS" pad="36"/>
<connect gate="A" pin="CLKOUT0" pad="14"/>
<connect gate="A" pin="CLKOUT1" pad="17"/>
<connect gate="A" pin="CLKOUT2" pad="20"/>
<connect gate="A" pin="CLKOUT3" pad="23"/>
<connect gate="A" pin="CLKOUT4" pad="38"/>
<connect gate="A" pin="CLKOUT5" pad="41"/>
<connect gate="A" pin="CLKOUT6" pad="44"/>
<connect gate="A" pin="CLKOUT7" pad="47"/>
<connect gate="A" pin="CLKUWIRE" pad="4"/>
<connect gate="A" pin="CPOUT" pad="32"/>
<connect gate="A" pin="DATAUWIRE" pad="5"/>
<connect gate="A" pin="EPAD" pad="49"/>
<connect gate="A" pin="FOUT" pad="2"/>
<connect gate="A" pin="GND" pad="25"/>
<connect gate="A" pin="GND_2" pad="1"/>
<connect gate="A" pin="GOE" pad="11"/>
<connect gate="A" pin="LD" pad="12"/>
<connect gate="A" pin="LDOBYP1" pad="9"/>
<connect gate="A" pin="LDOBYP2" pad="10"/>
<connect gate="A" pin="LEUWIRE" pad="6"/>
<connect gate="A" pin="NC" pad="35"/>
<connect gate="A" pin="NC_2" pad="7"/>
<connect gate="A" pin="NC_3" pad="34"/>
<connect gate="A" pin="OSCIN" pad="28"/>
<connect gate="A" pin="VCC1" pad="3"/>
<connect gate="A" pin="VCC10" pad="33"/>
<connect gate="A" pin="VCC11" pad="37"/>
<connect gate="A" pin="VCC12" pad="40"/>
<connect gate="A" pin="VCC13" pad="43"/>
<connect gate="A" pin="VCC14" pad="46"/>
<connect gate="A" pin="VCC2" pad="8"/>
<connect gate="A" pin="VCC3" pad="13"/>
<connect gate="A" pin="VCC4" pad="16"/>
<connect gate="A" pin="VCC5" pad="19"/>
<connect gate="A" pin="VCC6" pad="22"/>
<connect gate="A" pin="VCC7" pad="26"/>
<connect gate="A" pin="VCC8" pad="30"/>
<connect gate="A" pin="VCC9" pad="31"/>
<connect gate="A" pin="~CLKOUT0+" pad="15"/>
<connect gate="A" pin="~CLKOUT1" pad="18"/>
<connect gate="A" pin="~CLKOUT2" pad="21"/>
<connect gate="A" pin="~CLKOUT3" pad="24"/>
<connect gate="A" pin="~CLKOUT4" pad="39"/>
<connect gate="A" pin="~CLKOUT5" pad="42"/>
<connect gate="A" pin="~CLKOUT6" pad="45"/>
<connect gate="A" pin="~CLKOUT7" pad="48"/>
<connect gate="A" pin="~OSCIN" pad="29"/>
<connect gate="A" pin="~SYNC" pad="27"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMK03000DISQ"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="95M8824"/>
<attribute name="PACKAGE" value="QFN-48"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMK03000ISQ" prefix="U">
<description>Precision Clock Conditioner</description>
<gates>
<gate name="A" symbol="LMK03000ISQ"/>
</gates>
<devices>
<device name="" package="QFN50P700X700X80-49N">
<connects>
<connect gate="A" pin="BIAS" pad="36"/>
<connect gate="A" pin="CLKOUT0" pad="14"/>
<connect gate="A" pin="CLKOUT1" pad="17"/>
<connect gate="A" pin="CLKOUT2" pad="20"/>
<connect gate="A" pin="CLKOUT3" pad="23"/>
<connect gate="A" pin="CLKOUT4" pad="38"/>
<connect gate="A" pin="CLKOUT5" pad="41"/>
<connect gate="A" pin="CLKOUT6" pad="44"/>
<connect gate="A" pin="CLKOUT7" pad="47"/>
<connect gate="A" pin="CLKUWIRE" pad="4"/>
<connect gate="A" pin="CPOUT" pad="32"/>
<connect gate="A" pin="DATAUWIRE" pad="5"/>
<connect gate="A" pin="EPAD" pad="49"/>
<connect gate="A" pin="FOUT" pad="2"/>
<connect gate="A" pin="GND" pad="25"/>
<connect gate="A" pin="GND_2" pad="1"/>
<connect gate="A" pin="GOE" pad="11"/>
<connect gate="A" pin="LD" pad="12"/>
<connect gate="A" pin="LDOBYP1" pad="9"/>
<connect gate="A" pin="LDOBYP2" pad="10"/>
<connect gate="A" pin="LEUWIRE" pad="6"/>
<connect gate="A" pin="NC" pad="35"/>
<connect gate="A" pin="NC_2" pad="7"/>
<connect gate="A" pin="NC_3" pad="34"/>
<connect gate="A" pin="OSCIN" pad="28"/>
<connect gate="A" pin="VCC1" pad="3"/>
<connect gate="A" pin="VCC10" pad="33"/>
<connect gate="A" pin="VCC11" pad="37"/>
<connect gate="A" pin="VCC12" pad="40"/>
<connect gate="A" pin="VCC13" pad="43"/>
<connect gate="A" pin="VCC14" pad="46"/>
<connect gate="A" pin="VCC2" pad="8"/>
<connect gate="A" pin="VCC3" pad="13"/>
<connect gate="A" pin="VCC4" pad="16"/>
<connect gate="A" pin="VCC5" pad="19"/>
<connect gate="A" pin="VCC6" pad="22"/>
<connect gate="A" pin="VCC7" pad="26"/>
<connect gate="A" pin="VCC8" pad="30"/>
<connect gate="A" pin="VCC9" pad="31"/>
<connect gate="A" pin="~CLKOUT0+" pad="15"/>
<connect gate="A" pin="~CLKOUT1" pad="18"/>
<connect gate="A" pin="~CLKOUT2" pad="21"/>
<connect gate="A" pin="~CLKOUT3" pad="24"/>
<connect gate="A" pin="~CLKOUT4" pad="39"/>
<connect gate="A" pin="~CLKOUT5" pad="42"/>
<connect gate="A" pin="~CLKOUT6" pad="45"/>
<connect gate="A" pin="~CLKOUT7" pad="48"/>
<connect gate="A" pin="~OSCIN" pad="29"/>
<connect gate="A" pin="~SYNC" pad="27"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMK03000ISQ"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="39M4950"/>
<attribute name="PACKAGE" value="QFN-48"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMK03001CISQ" prefix="U">
<description>Precision Clock Conditioner</description>
<gates>
<gate name="A" symbol="LMK03001CISQ"/>
</gates>
<devices>
<device name="" package="QFN50P700X700X80-49N">
<connects>
<connect gate="A" pin="BIAS" pad="36"/>
<connect gate="A" pin="CLKOUT0" pad="14"/>
<connect gate="A" pin="CLKOUT1" pad="17"/>
<connect gate="A" pin="CLKOUT2" pad="20"/>
<connect gate="A" pin="CLKOUT3" pad="23"/>
<connect gate="A" pin="CLKOUT4" pad="38"/>
<connect gate="A" pin="CLKOUT5" pad="41"/>
<connect gate="A" pin="CLKOUT6" pad="44"/>
<connect gate="A" pin="CLKOUT7" pad="47"/>
<connect gate="A" pin="CLKUWIRE" pad="4"/>
<connect gate="A" pin="CPOUT" pad="32"/>
<connect gate="A" pin="DATAUWIRE" pad="5"/>
<connect gate="A" pin="EPAD" pad="49"/>
<connect gate="A" pin="FOUT" pad="2"/>
<connect gate="A" pin="GND" pad="25"/>
<connect gate="A" pin="GND_2" pad="1"/>
<connect gate="A" pin="GOE" pad="11"/>
<connect gate="A" pin="LD" pad="12"/>
<connect gate="A" pin="LDOBYP1" pad="9"/>
<connect gate="A" pin="LDOBYP2" pad="10"/>
<connect gate="A" pin="LEUWIRE" pad="6"/>
<connect gate="A" pin="NC" pad="35"/>
<connect gate="A" pin="NC_2" pad="7"/>
<connect gate="A" pin="NC_3" pad="34"/>
<connect gate="A" pin="OSCIN" pad="28"/>
<connect gate="A" pin="VCC1" pad="3"/>
<connect gate="A" pin="VCC10" pad="33"/>
<connect gate="A" pin="VCC11" pad="37"/>
<connect gate="A" pin="VCC12" pad="40"/>
<connect gate="A" pin="VCC13" pad="43"/>
<connect gate="A" pin="VCC14" pad="46"/>
<connect gate="A" pin="VCC2" pad="8"/>
<connect gate="A" pin="VCC3" pad="13"/>
<connect gate="A" pin="VCC4" pad="16"/>
<connect gate="A" pin="VCC5" pad="19"/>
<connect gate="A" pin="VCC6" pad="22"/>
<connect gate="A" pin="VCC7" pad="26"/>
<connect gate="A" pin="VCC8" pad="30"/>
<connect gate="A" pin="VCC9" pad="31"/>
<connect gate="A" pin="~CLKOUT0+" pad="15"/>
<connect gate="A" pin="~CLKOUT1" pad="18"/>
<connect gate="A" pin="~CLKOUT2" pad="21"/>
<connect gate="A" pin="~CLKOUT3" pad="24"/>
<connect gate="A" pin="~CLKOUT4" pad="39"/>
<connect gate="A" pin="~CLKOUT5" pad="42"/>
<connect gate="A" pin="~CLKOUT6" pad="45"/>
<connect gate="A" pin="~CLKOUT7" pad="48"/>
<connect gate="A" pin="~OSCIN" pad="29"/>
<connect gate="A" pin="~SYNC" pad="27"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMK03001CISQ"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="39M4951"/>
<attribute name="PACKAGE" value="QFN-48"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMK03001DISQ" prefix="U">
<description>Precision Clock Conditioner</description>
<gates>
<gate name="A" symbol="LMK03001DISQ"/>
</gates>
<devices>
<device name="" package="QFN50P700X700X80-49N">
<connects>
<connect gate="A" pin="BIAS" pad="36"/>
<connect gate="A" pin="CLKOUT0" pad="14"/>
<connect gate="A" pin="CLKOUT1" pad="17"/>
<connect gate="A" pin="CLKOUT2" pad="20"/>
<connect gate="A" pin="CLKOUT3" pad="23"/>
<connect gate="A" pin="CLKOUT4" pad="38"/>
<connect gate="A" pin="CLKOUT5" pad="41"/>
<connect gate="A" pin="CLKOUT6" pad="44"/>
<connect gate="A" pin="CLKOUT7" pad="47"/>
<connect gate="A" pin="CLKUWIRE" pad="4"/>
<connect gate="A" pin="CPOUT" pad="32"/>
<connect gate="A" pin="DATAUWIRE" pad="5"/>
<connect gate="A" pin="EPAD" pad="49"/>
<connect gate="A" pin="FOUT" pad="2"/>
<connect gate="A" pin="GND" pad="25"/>
<connect gate="A" pin="GND_2" pad="1"/>
<connect gate="A" pin="GOE" pad="11"/>
<connect gate="A" pin="LD" pad="12"/>
<connect gate="A" pin="LDOBYP1" pad="9"/>
<connect gate="A" pin="LDOBYP2" pad="10"/>
<connect gate="A" pin="LEUWIRE" pad="6"/>
<connect gate="A" pin="NC" pad="35"/>
<connect gate="A" pin="NC_2" pad="7"/>
<connect gate="A" pin="NC_3" pad="34"/>
<connect gate="A" pin="OSCIN" pad="28"/>
<connect gate="A" pin="VCC1" pad="3"/>
<connect gate="A" pin="VCC10" pad="33"/>
<connect gate="A" pin="VCC11" pad="37"/>
<connect gate="A" pin="VCC12" pad="40"/>
<connect gate="A" pin="VCC13" pad="43"/>
<connect gate="A" pin="VCC14" pad="46"/>
<connect gate="A" pin="VCC2" pad="8"/>
<connect gate="A" pin="VCC3" pad="13"/>
<connect gate="A" pin="VCC4" pad="16"/>
<connect gate="A" pin="VCC5" pad="19"/>
<connect gate="A" pin="VCC6" pad="22"/>
<connect gate="A" pin="VCC7" pad="26"/>
<connect gate="A" pin="VCC8" pad="30"/>
<connect gate="A" pin="VCC9" pad="31"/>
<connect gate="A" pin="~CLKOUT0+" pad="15"/>
<connect gate="A" pin="~CLKOUT1" pad="18"/>
<connect gate="A" pin="~CLKOUT2" pad="21"/>
<connect gate="A" pin="~CLKOUT3" pad="24"/>
<connect gate="A" pin="~CLKOUT4" pad="39"/>
<connect gate="A" pin="~CLKOUT5" pad="42"/>
<connect gate="A" pin="~CLKOUT6" pad="45"/>
<connect gate="A" pin="~CLKOUT7" pad="48"/>
<connect gate="A" pin="~OSCIN" pad="29"/>
<connect gate="A" pin="~SYNC" pad="27"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMK03001DISQ"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="95M8825"/>
<attribute name="PACKAGE" value="QFN-48"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMK03001ISQ" prefix="U">
<description>Precision Clock Conditioner</description>
<gates>
<gate name="A" symbol="LMK03001ISQ"/>
</gates>
<devices>
<device name="" package="QFN50P700X700X80-49N">
<connects>
<connect gate="A" pin="BIAS" pad="36"/>
<connect gate="A" pin="CLKOUT0" pad="14"/>
<connect gate="A" pin="CLKOUT1" pad="17"/>
<connect gate="A" pin="CLKOUT2" pad="20"/>
<connect gate="A" pin="CLKOUT3" pad="23"/>
<connect gate="A" pin="CLKOUT4" pad="38"/>
<connect gate="A" pin="CLKOUT5" pad="41"/>
<connect gate="A" pin="CLKOUT6" pad="44"/>
<connect gate="A" pin="CLKOUT7" pad="47"/>
<connect gate="A" pin="CLKUWIRE" pad="4"/>
<connect gate="A" pin="CPOUT" pad="32"/>
<connect gate="A" pin="DATAUWIRE" pad="5"/>
<connect gate="A" pin="EPAD" pad="49"/>
<connect gate="A" pin="FOUT" pad="2"/>
<connect gate="A" pin="GND" pad="25"/>
<connect gate="A" pin="GND_2" pad="1"/>
<connect gate="A" pin="GOE" pad="11"/>
<connect gate="A" pin="LD" pad="12"/>
<connect gate="A" pin="LDOBYP1" pad="9"/>
<connect gate="A" pin="LDOBYP2" pad="10"/>
<connect gate="A" pin="LEUWIRE" pad="6"/>
<connect gate="A" pin="NC" pad="35"/>
<connect gate="A" pin="NC_2" pad="7"/>
<connect gate="A" pin="NC_3" pad="34"/>
<connect gate="A" pin="OSCIN" pad="28"/>
<connect gate="A" pin="VCC1" pad="3"/>
<connect gate="A" pin="VCC10" pad="33"/>
<connect gate="A" pin="VCC11" pad="37"/>
<connect gate="A" pin="VCC12" pad="40"/>
<connect gate="A" pin="VCC13" pad="43"/>
<connect gate="A" pin="VCC14" pad="46"/>
<connect gate="A" pin="VCC2" pad="8"/>
<connect gate="A" pin="VCC3" pad="13"/>
<connect gate="A" pin="VCC4" pad="16"/>
<connect gate="A" pin="VCC5" pad="19"/>
<connect gate="A" pin="VCC6" pad="22"/>
<connect gate="A" pin="VCC7" pad="26"/>
<connect gate="A" pin="VCC8" pad="30"/>
<connect gate="A" pin="VCC9" pad="31"/>
<connect gate="A" pin="~CLKOUT0+" pad="15"/>
<connect gate="A" pin="~CLKOUT1" pad="18"/>
<connect gate="A" pin="~CLKOUT2" pad="21"/>
<connect gate="A" pin="~CLKOUT3" pad="24"/>
<connect gate="A" pin="~CLKOUT4" pad="39"/>
<connect gate="A" pin="~CLKOUT5" pad="42"/>
<connect gate="A" pin="~CLKOUT6" pad="45"/>
<connect gate="A" pin="~CLKOUT7" pad="48"/>
<connect gate="A" pin="~OSCIN" pad="29"/>
<connect gate="A" pin="~SYNC" pad="27"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMK03001ISQ"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="39M4952"/>
<attribute name="PACKAGE" value="QFN-48"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMK03033CISQ" prefix="U">
<description>Precision Clock Conditioner</description>
<gates>
<gate name="A" symbol="LMK03033CISQ"/>
</gates>
<devices>
<device name="" package="QFN50P700X700X80-49N">
<connects>
<connect gate="A" pin="BIAS" pad="36"/>
<connect gate="A" pin="CLKOUT0" pad="14"/>
<connect gate="A" pin="CLKOUT1" pad="17"/>
<connect gate="A" pin="CLKOUT2" pad="20"/>
<connect gate="A" pin="CLKOUT3" pad="23"/>
<connect gate="A" pin="CLKOUT4" pad="38"/>
<connect gate="A" pin="CLKOUT5" pad="41"/>
<connect gate="A" pin="CLKOUT6" pad="44"/>
<connect gate="A" pin="CLKOUT7" pad="47"/>
<connect gate="A" pin="CLKUWIRE" pad="4"/>
<connect gate="A" pin="CPOUT" pad="32"/>
<connect gate="A" pin="DAP" pad="49"/>
<connect gate="A" pin="DATAUWIRE" pad="5"/>
<connect gate="A" pin="FOUT" pad="2"/>
<connect gate="A" pin="GND" pad="1"/>
<connect gate="A" pin="GND_2" pad="25"/>
<connect gate="A" pin="GOE" pad="11"/>
<connect gate="A" pin="LD" pad="12"/>
<connect gate="A" pin="LDOBYP1" pad="9"/>
<connect gate="A" pin="LDOBYP2" pad="10"/>
<connect gate="A" pin="LEUWIRE" pad="6"/>
<connect gate="A" pin="NC" pad="7"/>
<connect gate="A" pin="NC_2" pad="34"/>
<connect gate="A" pin="NC_3" pad="35"/>
<connect gate="A" pin="OSCIN" pad="28"/>
<connect gate="A" pin="VCC1" pad="3"/>
<connect gate="A" pin="VCC10" pad="33"/>
<connect gate="A" pin="VCC11" pad="37"/>
<connect gate="A" pin="VCC12" pad="40"/>
<connect gate="A" pin="VCC13" pad="43"/>
<connect gate="A" pin="VCC14" pad="46"/>
<connect gate="A" pin="VCC2" pad="8"/>
<connect gate="A" pin="VCC3" pad="13"/>
<connect gate="A" pin="VCC4" pad="16"/>
<connect gate="A" pin="VCC5" pad="19"/>
<connect gate="A" pin="VCC6" pad="22"/>
<connect gate="A" pin="VCC7" pad="26"/>
<connect gate="A" pin="VCC8" pad="30"/>
<connect gate="A" pin="VCC9" pad="31"/>
<connect gate="A" pin="~CLKOUT0" pad="15"/>
<connect gate="A" pin="~CLKOUT1" pad="18"/>
<connect gate="A" pin="~CLKOUT2" pad="21"/>
<connect gate="A" pin="~CLKOUT3" pad="24"/>
<connect gate="A" pin="~CLKOUT4" pad="39"/>
<connect gate="A" pin="~CLKOUT5" pad="42"/>
<connect gate="A" pin="~CLKOUT6" pad="45"/>
<connect gate="A" pin="~CLKOUT7" pad="48"/>
<connect gate="A" pin="~OSCIN" pad="29"/>
<connect gate="A" pin="~SYNC" pad="27"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMK03033CISQ"/>
<attribute name="OC_FARNELL" value="1667424"/>
<attribute name="OC_NEWARK" value="-"/>
<attribute name="PACKAGE" value="LLP-48"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMK04000BISQE">
<description>IC, CLOCK CONDITIONER</description>
<gates>
<gate name="A" symbol="LMK04000BISQE"/>
</gates>
<devices>
<device name="" package="QFN50P700X700X80-49N">
<connects>
<connect gate="A" pin="BIAS" pad="36"/>
<connect gate="A" pin="CLKIN0" pad="20"/>
<connect gate="A" pin="CLKIN0_LOS" pad="34"/>
<connect gate="A" pin="CLKIN1" pad="25"/>
<connect gate="A" pin="CLKIN1_LOS" pad="35"/>
<connect gate="A" pin="CLKOUT0" pad="14"/>
<connect gate="A" pin="CLKOUT1" pad="38"/>
<connect gate="A" pin="CLKOUT2" pad="41"/>
<connect gate="A" pin="CLKOUT3" pad="44"/>
<connect gate="A" pin="CLKOUT4" pad="47"/>
<connect gate="A" pin="CLKUWIRE" pad="4"/>
<connect gate="A" pin="CPOUT1" pad="23"/>
<connect gate="A" pin="CPOUT2" pad="32"/>
<connect gate="A" pin="DATAUWIRE" pad="5"/>
<connect gate="A" pin="DLD_BYP" pad="16"/>
<connect gate="A" pin="FOUT" pad="2"/>
<connect gate="A" pin="GND" pad="17"/>
<connect gate="A" pin="GND_2" pad="1"/>
<connect gate="A" pin="GOE" pad="11"/>
<connect gate="A" pin="HEAT_TAB" pad="49"/>
<connect gate="A" pin="LD" pad="12"/>
<connect gate="A" pin="LDOBYP1" pad="9"/>
<connect gate="A" pin="LDOBYP2" pad="10"/>
<connect gate="A" pin="LEUWIRE" pad="6"/>
<connect gate="A" pin="NC" pad="7"/>
<connect gate="A" pin="OSCIN" pad="28"/>
<connect gate="A" pin="VCC1" pad="3"/>
<connect gate="A" pin="VCC10" pad="33"/>
<connect gate="A" pin="VCC11" pad="37"/>
<connect gate="A" pin="VCC12" pad="40"/>
<connect gate="A" pin="VCC13" pad="43"/>
<connect gate="A" pin="VCC14" pad="46"/>
<connect gate="A" pin="VCC2" pad="8"/>
<connect gate="A" pin="VCC3" pad="13"/>
<connect gate="A" pin="VCC4" pad="18"/>
<connect gate="A" pin="VCC5" pad="19"/>
<connect gate="A" pin="VCC6" pad="22"/>
<connect gate="A" pin="VCC7" pad="24"/>
<connect gate="A" pin="VCC8" pad="30"/>
<connect gate="A" pin="VCC9" pad="31"/>
<connect gate="A" pin="~CLKIN0" pad="21"/>
<connect gate="A" pin="~CLKIN1" pad="26"/>
<connect gate="A" pin="~CLKOUT0" pad="15"/>
<connect gate="A" pin="~CLKOUT1" pad="39"/>
<connect gate="A" pin="~CLKOUT2" pad="42"/>
<connect gate="A" pin="~CLKOUT3" pad="45"/>
<connect gate="A" pin="~CLKOUT4" pad="48"/>
<connect gate="A" pin="~OSCIN" pad="29"/>
<connect gate="A" pin="~SYNC" pad="27"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMK04000BISQE"/>
<attribute name="OC_FARNELL" value="1791113"/>
<attribute name="OC_NEWARK" value="57R6018"/>
<attribute name="PACKAGE" value="QFN-48"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMK04001BISQE">
<description>IC, CLOCK CONDITIONER</description>
<gates>
<gate name="A" symbol="LMK04001BISQE"/>
</gates>
<devices>
<device name="" package="QFN50P700X700X80-49N">
<connects>
<connect gate="A" pin="BIAS" pad="36"/>
<connect gate="A" pin="CLKIN0" pad="20"/>
<connect gate="A" pin="CLKIN0_LOS" pad="34"/>
<connect gate="A" pin="CLKIN1" pad="25"/>
<connect gate="A" pin="CLKIN1_LOS" pad="35"/>
<connect gate="A" pin="CLKOUT0" pad="14"/>
<connect gate="A" pin="CLKOUT1" pad="38"/>
<connect gate="A" pin="CLKOUT2" pad="41"/>
<connect gate="A" pin="CLKOUT3" pad="44"/>
<connect gate="A" pin="CLKOUT4" pad="47"/>
<connect gate="A" pin="CLKUWIRE" pad="4"/>
<connect gate="A" pin="CPOUT1" pad="23"/>
<connect gate="A" pin="CPOUT2" pad="32"/>
<connect gate="A" pin="DATAUWIRE" pad="5"/>
<connect gate="A" pin="DLD_BYP" pad="16"/>
<connect gate="A" pin="FOUT" pad="2"/>
<connect gate="A" pin="GND" pad="17"/>
<connect gate="A" pin="GND_2" pad="1"/>
<connect gate="A" pin="GOE" pad="11"/>
<connect gate="A" pin="HEAT_TAB" pad="49"/>
<connect gate="A" pin="LD" pad="12"/>
<connect gate="A" pin="LDOBYP1" pad="9"/>
<connect gate="A" pin="LDOBYP2" pad="10"/>
<connect gate="A" pin="LEUWIRE" pad="6"/>
<connect gate="A" pin="NC" pad="7"/>
<connect gate="A" pin="OSCIN" pad="28"/>
<connect gate="A" pin="VCC1" pad="3"/>
<connect gate="A" pin="VCC10" pad="33"/>
<connect gate="A" pin="VCC11" pad="37"/>
<connect gate="A" pin="VCC12" pad="40"/>
<connect gate="A" pin="VCC13" pad="43"/>
<connect gate="A" pin="VCC14" pad="46"/>
<connect gate="A" pin="VCC2" pad="8"/>
<connect gate="A" pin="VCC3" pad="13"/>
<connect gate="A" pin="VCC4" pad="18"/>
<connect gate="A" pin="VCC5" pad="19"/>
<connect gate="A" pin="VCC6" pad="22"/>
<connect gate="A" pin="VCC7" pad="24"/>
<connect gate="A" pin="VCC8" pad="30"/>
<connect gate="A" pin="VCC9" pad="31"/>
<connect gate="A" pin="~CLKIN0" pad="21"/>
<connect gate="A" pin="~CLKIN1" pad="26"/>
<connect gate="A" pin="~CLKOUT0" pad="15"/>
<connect gate="A" pin="~CLKOUT1" pad="39"/>
<connect gate="A" pin="~CLKOUT2" pad="42"/>
<connect gate="A" pin="~CLKOUT3" pad="45"/>
<connect gate="A" pin="~CLKOUT4" pad="48"/>
<connect gate="A" pin="~OSCIN" pad="29"/>
<connect gate="A" pin="~SYNC" pad="27"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMK04001BISQE"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="57R6021"/>
<attribute name="PACKAGE" value="QFN-48"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMK04002BISQE">
<description>IC, CLOCK CONDITIONER</description>
<gates>
<gate name="A" symbol="LMK04002BISQE"/>
</gates>
<devices>
<device name="" package="QFN50P700X700X80-49N">
<connects>
<connect gate="A" pin="BIAS" pad="36"/>
<connect gate="A" pin="CLKIN0" pad="20"/>
<connect gate="A" pin="CLKIN0_LOS" pad="34"/>
<connect gate="A" pin="CLKIN1" pad="25"/>
<connect gate="A" pin="CLKIN1_LOS" pad="35"/>
<connect gate="A" pin="CLKOUT0" pad="14"/>
<connect gate="A" pin="CLKOUT1" pad="38"/>
<connect gate="A" pin="CLKOUT2" pad="41"/>
<connect gate="A" pin="CLKOUT3" pad="44"/>
<connect gate="A" pin="CLKOUT4" pad="47"/>
<connect gate="A" pin="CLKUWIRE" pad="4"/>
<connect gate="A" pin="CPOUT1" pad="23"/>
<connect gate="A" pin="CPOUT2" pad="32"/>
<connect gate="A" pin="DATAUWIRE" pad="5"/>
<connect gate="A" pin="DLD_BYP" pad="16"/>
<connect gate="A" pin="FOUT" pad="2"/>
<connect gate="A" pin="GND" pad="17"/>
<connect gate="A" pin="GND_2" pad="1"/>
<connect gate="A" pin="GOE" pad="11"/>
<connect gate="A" pin="HEAT_TAB" pad="49"/>
<connect gate="A" pin="LD" pad="12"/>
<connect gate="A" pin="LDOBYP1" pad="9"/>
<connect gate="A" pin="LDOBYP2" pad="10"/>
<connect gate="A" pin="LEUWIRE" pad="6"/>
<connect gate="A" pin="NC" pad="7"/>
<connect gate="A" pin="OSCIN" pad="28"/>
<connect gate="A" pin="VCC1" pad="3"/>
<connect gate="A" pin="VCC10" pad="33"/>
<connect gate="A" pin="VCC11" pad="37"/>
<connect gate="A" pin="VCC12" pad="40"/>
<connect gate="A" pin="VCC13" pad="43"/>
<connect gate="A" pin="VCC14" pad="46"/>
<connect gate="A" pin="VCC2" pad="8"/>
<connect gate="A" pin="VCC3" pad="13"/>
<connect gate="A" pin="VCC4" pad="18"/>
<connect gate="A" pin="VCC5" pad="19"/>
<connect gate="A" pin="VCC6" pad="22"/>
<connect gate="A" pin="VCC7" pad="24"/>
<connect gate="A" pin="VCC8" pad="30"/>
<connect gate="A" pin="VCC9" pad="31"/>
<connect gate="A" pin="~CLKIN0" pad="21"/>
<connect gate="A" pin="~CLKIN1" pad="26"/>
<connect gate="A" pin="~CLKOUT0" pad="15"/>
<connect gate="A" pin="~CLKOUT1" pad="39"/>
<connect gate="A" pin="~CLKOUT2" pad="42"/>
<connect gate="A" pin="~CLKOUT3" pad="45"/>
<connect gate="A" pin="~CLKOUT4" pad="48"/>
<connect gate="A" pin="~OSCIN" pad="29"/>
<connect gate="A" pin="~SYNC" pad="27"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMK04002BISQE"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="57R6023"/>
<attribute name="PACKAGE" value="QFN-48"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMK04010BISQE">
<description>NSC-LMK04010BISQE@E</description>
<gates>
<gate name="A" symbol="LMK04010BISQE"/>
</gates>
<devices>
<device name="" package="QFN50P700X700X80-49N">
<connects>
<connect gate="A" pin="BIAS" pad="36"/>
<connect gate="A" pin="CLKIN0" pad="20"/>
<connect gate="A" pin="CLKIN0_LOS" pad="34"/>
<connect gate="A" pin="CLKIN1" pad="25"/>
<connect gate="A" pin="CLKIN1_LOS" pad="35"/>
<connect gate="A" pin="CLKOUT0" pad="14"/>
<connect gate="A" pin="CLKOUT1" pad="38"/>
<connect gate="A" pin="CLKOUT2" pad="41"/>
<connect gate="A" pin="CLKOUT3" pad="44"/>
<connect gate="A" pin="CLKOUT4" pad="47"/>
<connect gate="A" pin="CLKUWIRE" pad="4"/>
<connect gate="A" pin="CPOUT1" pad="23"/>
<connect gate="A" pin="CPOUT2" pad="32"/>
<connect gate="A" pin="DATAUWIRE" pad="5"/>
<connect gate="A" pin="DLD_BYP" pad="16"/>
<connect gate="A" pin="FOUT" pad="2"/>
<connect gate="A" pin="GND" pad="17"/>
<connect gate="A" pin="GND_2" pad="1"/>
<connect gate="A" pin="GOE" pad="11"/>
<connect gate="A" pin="HEAT_TAB" pad="49"/>
<connect gate="A" pin="LD" pad="12"/>
<connect gate="A" pin="LDOBYP1" pad="9"/>
<connect gate="A" pin="LDOBYP2" pad="10"/>
<connect gate="A" pin="LEUWIRE" pad="6"/>
<connect gate="A" pin="NC" pad="7"/>
<connect gate="A" pin="OSCIN" pad="28"/>
<connect gate="A" pin="VCC1" pad="3"/>
<connect gate="A" pin="VCC10" pad="33"/>
<connect gate="A" pin="VCC11" pad="37"/>
<connect gate="A" pin="VCC12" pad="40"/>
<connect gate="A" pin="VCC13" pad="43"/>
<connect gate="A" pin="VCC14" pad="46"/>
<connect gate="A" pin="VCC2" pad="8"/>
<connect gate="A" pin="VCC3" pad="13"/>
<connect gate="A" pin="VCC4" pad="18"/>
<connect gate="A" pin="VCC5" pad="19"/>
<connect gate="A" pin="VCC6" pad="22"/>
<connect gate="A" pin="VCC7" pad="24"/>
<connect gate="A" pin="VCC8" pad="30"/>
<connect gate="A" pin="VCC9" pad="31"/>
<connect gate="A" pin="~CLKIN0" pad="21"/>
<connect gate="A" pin="~CLKIN1" pad="26"/>
<connect gate="A" pin="~CLKOUT0" pad="15"/>
<connect gate="A" pin="~CLKOUT1" pad="39"/>
<connect gate="A" pin="~CLKOUT2" pad="42"/>
<connect gate="A" pin="~CLKOUT3" pad="45"/>
<connect gate="A" pin="~CLKOUT4" pad="48"/>
<connect gate="A" pin="~OSCIN" pad="29"/>
<connect gate="A" pin="~SYNC" pad="27"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMK04010BISQE"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="57R6026"/>
<attribute name="PACKAGE" value="QFN-48"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMK04011BISQE">
<description>IC, CLOCK CONDITIONER</description>
<gates>
<gate name="A" symbol="LMK04011BISQE"/>
</gates>
<devices>
<device name="" package="QFN50P700X700X80-49N">
<connects>
<connect gate="A" pin="BIAS" pad="36"/>
<connect gate="A" pin="CLKIN0" pad="20"/>
<connect gate="A" pin="CLKIN0_LOS" pad="34"/>
<connect gate="A" pin="CLKIN1" pad="25"/>
<connect gate="A" pin="CLKIN1_LOS" pad="35"/>
<connect gate="A" pin="CLKOUT0" pad="14"/>
<connect gate="A" pin="CLKOUT1" pad="38"/>
<connect gate="A" pin="CLKOUT2" pad="41"/>
<connect gate="A" pin="CLKOUT3" pad="44"/>
<connect gate="A" pin="CLKOUT4" pad="47"/>
<connect gate="A" pin="CLKUWIRE" pad="4"/>
<connect gate="A" pin="CPOUT1" pad="23"/>
<connect gate="A" pin="CPOUT2" pad="32"/>
<connect gate="A" pin="DATAUWIRE" pad="5"/>
<connect gate="A" pin="DLD_BYP" pad="16"/>
<connect gate="A" pin="FOUT" pad="2"/>
<connect gate="A" pin="GND" pad="17"/>
<connect gate="A" pin="GND_2" pad="1"/>
<connect gate="A" pin="GOE" pad="11"/>
<connect gate="A" pin="HEAT_TAB" pad="49"/>
<connect gate="A" pin="LD" pad="12"/>
<connect gate="A" pin="LDOBYP1" pad="9"/>
<connect gate="A" pin="LDOBYP2" pad="10"/>
<connect gate="A" pin="LEUWIRE" pad="6"/>
<connect gate="A" pin="NC" pad="7"/>
<connect gate="A" pin="OSCIN" pad="28"/>
<connect gate="A" pin="VCC1" pad="3"/>
<connect gate="A" pin="VCC10" pad="33"/>
<connect gate="A" pin="VCC11" pad="37"/>
<connect gate="A" pin="VCC12" pad="40"/>
<connect gate="A" pin="VCC13" pad="43"/>
<connect gate="A" pin="VCC14" pad="46"/>
<connect gate="A" pin="VCC2" pad="8"/>
<connect gate="A" pin="VCC3" pad="13"/>
<connect gate="A" pin="VCC4" pad="18"/>
<connect gate="A" pin="VCC5" pad="19"/>
<connect gate="A" pin="VCC6" pad="22"/>
<connect gate="A" pin="VCC7" pad="24"/>
<connect gate="A" pin="VCC8" pad="30"/>
<connect gate="A" pin="VCC9" pad="31"/>
<connect gate="A" pin="~CLKIN0" pad="21"/>
<connect gate="A" pin="~CLKIN1" pad="26"/>
<connect gate="A" pin="~CLKOUT0" pad="15"/>
<connect gate="A" pin="~CLKOUT1" pad="39"/>
<connect gate="A" pin="~CLKOUT2" pad="42"/>
<connect gate="A" pin="~CLKOUT3" pad="45"/>
<connect gate="A" pin="~CLKOUT4" pad="48"/>
<connect gate="A" pin="~OSCIN" pad="29"/>
<connect gate="A" pin="~SYNC" pad="27"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMK04011BISQE"/>
<attribute name="OC_FARNELL" value="1679687"/>
<attribute name="OC_NEWARK" value="33P7273"/>
<attribute name="PACKAGE" value="QFN-48"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMK04031BISQE">
<description>IC, CLOCK CONDITIONER</description>
<gates>
<gate name="A" symbol="LMK04031BISQE"/>
</gates>
<devices>
<device name="" package="QFN50P700X700X80-49N">
<connects>
<connect gate="A" pin="BIAS" pad="36"/>
<connect gate="A" pin="CLKIN0" pad="20"/>
<connect gate="A" pin="CLKIN0_LOS" pad="34"/>
<connect gate="A" pin="CLKIN1" pad="25"/>
<connect gate="A" pin="CLKIN1_LOS" pad="35"/>
<connect gate="A" pin="CLKOUT0" pad="14"/>
<connect gate="A" pin="CLKOUT1" pad="38"/>
<connect gate="A" pin="CLKOUT2" pad="41"/>
<connect gate="A" pin="CLKOUT3" pad="44"/>
<connect gate="A" pin="CLKOUT4" pad="47"/>
<connect gate="A" pin="CLKUWIRE" pad="4"/>
<connect gate="A" pin="CPOUT1" pad="23"/>
<connect gate="A" pin="CPOUT2" pad="32"/>
<connect gate="A" pin="DATAUWIRE" pad="5"/>
<connect gate="A" pin="DLD_BYP" pad="16"/>
<connect gate="A" pin="FOUT" pad="2"/>
<connect gate="A" pin="GND" pad="17"/>
<connect gate="A" pin="GND_2" pad="1"/>
<connect gate="A" pin="GOE" pad="11"/>
<connect gate="A" pin="HEAT_TAB" pad="49"/>
<connect gate="A" pin="LD" pad="12"/>
<connect gate="A" pin="LDOBYP1" pad="9"/>
<connect gate="A" pin="LDOBYP2" pad="10"/>
<connect gate="A" pin="LEUWIRE" pad="6"/>
<connect gate="A" pin="NC" pad="7"/>
<connect gate="A" pin="OSCIN" pad="28"/>
<connect gate="A" pin="VCC1" pad="3"/>
<connect gate="A" pin="VCC10" pad="33"/>
<connect gate="A" pin="VCC11" pad="37"/>
<connect gate="A" pin="VCC12" pad="40"/>
<connect gate="A" pin="VCC13" pad="43"/>
<connect gate="A" pin="VCC14" pad="46"/>
<connect gate="A" pin="VCC2" pad="8"/>
<connect gate="A" pin="VCC3" pad="13"/>
<connect gate="A" pin="VCC4" pad="18"/>
<connect gate="A" pin="VCC5" pad="19"/>
<connect gate="A" pin="VCC6" pad="22"/>
<connect gate="A" pin="VCC7" pad="24"/>
<connect gate="A" pin="VCC8" pad="30"/>
<connect gate="A" pin="VCC9" pad="31"/>
<connect gate="A" pin="~CLKIN0" pad="21"/>
<connect gate="A" pin="~CLKIN1" pad="26"/>
<connect gate="A" pin="~CLKOUT0" pad="15"/>
<connect gate="A" pin="~CLKOUT1" pad="39"/>
<connect gate="A" pin="~CLKOUT2" pad="42"/>
<connect gate="A" pin="~CLKOUT3" pad="45"/>
<connect gate="A" pin="~CLKOUT4" pad="48"/>
<connect gate="A" pin="~OSCIN" pad="29"/>
<connect gate="A" pin="~SYNC" pad="27"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMK04031BISQE"/>
<attribute name="OC_FARNELL" value="1679688"/>
<attribute name="OC_NEWARK" value="19P7823"/>
<attribute name="PACKAGE" value="QFN-48"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMK04033BISQE">
<description>IC, CLOCK CONDITIONER</description>
<gates>
<gate name="A" symbol="LMK04033BISQE"/>
</gates>
<devices>
<device name="" package="QFN50P700X700X80-49N">
<connects>
<connect gate="A" pin="BIAS" pad="36"/>
<connect gate="A" pin="CLKIN0" pad="20"/>
<connect gate="A" pin="CLKIN0_LOS" pad="34"/>
<connect gate="A" pin="CLKIN1" pad="25"/>
<connect gate="A" pin="CLKIN1_LOS" pad="35"/>
<connect gate="A" pin="CLKOUT0" pad="14"/>
<connect gate="A" pin="CLKOUT1" pad="38"/>
<connect gate="A" pin="CLKOUT2" pad="41"/>
<connect gate="A" pin="CLKOUT3" pad="44"/>
<connect gate="A" pin="CLKOUT4" pad="47"/>
<connect gate="A" pin="CLKUWIRE" pad="4"/>
<connect gate="A" pin="CPOUT1" pad="23"/>
<connect gate="A" pin="CPOUT2" pad="32"/>
<connect gate="A" pin="DATAUWIRE" pad="5"/>
<connect gate="A" pin="DLD_BYP" pad="16"/>
<connect gate="A" pin="FOUT" pad="2"/>
<connect gate="A" pin="GND" pad="17"/>
<connect gate="A" pin="GND_2" pad="1"/>
<connect gate="A" pin="GOE" pad="11"/>
<connect gate="A" pin="HEAT_TAB" pad="49"/>
<connect gate="A" pin="LD" pad="12"/>
<connect gate="A" pin="LDOBYP1" pad="9"/>
<connect gate="A" pin="LDOBYP2" pad="10"/>
<connect gate="A" pin="LEUWIRE" pad="6"/>
<connect gate="A" pin="NC" pad="7"/>
<connect gate="A" pin="OSCIN" pad="28"/>
<connect gate="A" pin="VCC1" pad="3"/>
<connect gate="A" pin="VCC10" pad="33"/>
<connect gate="A" pin="VCC11" pad="37"/>
<connect gate="A" pin="VCC12" pad="40"/>
<connect gate="A" pin="VCC13" pad="43"/>
<connect gate="A" pin="VCC14" pad="46"/>
<connect gate="A" pin="VCC2" pad="8"/>
<connect gate="A" pin="VCC3" pad="13"/>
<connect gate="A" pin="VCC4" pad="18"/>
<connect gate="A" pin="VCC5" pad="19"/>
<connect gate="A" pin="VCC6" pad="22"/>
<connect gate="A" pin="VCC7" pad="24"/>
<connect gate="A" pin="VCC8" pad="30"/>
<connect gate="A" pin="VCC9" pad="31"/>
<connect gate="A" pin="~CLKIN0" pad="21"/>
<connect gate="A" pin="~CLKIN1" pad="26"/>
<connect gate="A" pin="~CLKOUT0" pad="15"/>
<connect gate="A" pin="~CLKOUT1" pad="39"/>
<connect gate="A" pin="~CLKOUT2" pad="42"/>
<connect gate="A" pin="~CLKOUT3" pad="45"/>
<connect gate="A" pin="~CLKOUT4" pad="48"/>
<connect gate="A" pin="~OSCIN" pad="29"/>
<connect gate="A" pin="~SYNC" pad="27"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMK04033BISQE"/>
<attribute name="OC_FARNELL" value="1684976"/>
<attribute name="OC_NEWARK" value="19P7824"/>
<attribute name="PACKAGE" value="QFN-48"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMP2011MA" prefix="U">
<description>Rail-to-Rail Output Operational Amplifier</description>
<gates>
<gate name="A" symbol="LMP2011MA"/>
</gates>
<devices>
<device name="" package="SOIC127P620X175-8N">
<connects>
<connect gate="A" pin="+VIN" pad="3"/>
<connect gate="A" pin="-VIN" pad="2"/>
<connect gate="A" pin="N/C" pad="8"/>
<connect gate="A" pin="N/C_2" pad="1"/>
<connect gate="A" pin="N/C_3" pad="5"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
<connect gate="A" pin="VOUT" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMP2011MA"/>
<attribute name="OC_FARNELL" value="1008279"/>
<attribute name="OC_NEWARK" value="41K2904"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMP2011MF" prefix="U">
<description>Rail-to-Rail Output Operational Amplifier</description>
<gates>
<gate name="A" symbol="LMP2011MF"/>
</gates>
<devices>
<device name="" package="SOT95P285X120-5N">
<connects>
<connect gate="A" pin="V+" pad="5"/>
<connect gate="A" pin="V-" pad="2"/>
<connect gate="A" pin="VIN+" pad="3"/>
<connect gate="A" pin="VIN-" pad="4"/>
<connect gate="A" pin="VOUT" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMP2011MF"/>
<attribute name="OC_FARNELL" value="1008280"/>
<attribute name="OC_NEWARK" value="41K2906"/>
<attribute name="PACKAGE" value="SOT23-5"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMP2012MA" prefix="U">
<description>Rail-to-Rail Output Operational Amplifier</description>
<gates>
<gate name="A" symbol="LMP2012MA"/>
</gates>
<devices>
<device name="" package="SOIC127P620X175-8N">
<connects>
<connect gate="A" pin="+VIN" pad="3"/>
<connect gate="A" pin="-VIN" pad="2"/>
<connect gate="A" pin="N/C" pad="8"/>
<connect gate="A" pin="N/C_2" pad="1"/>
<connect gate="A" pin="N/C_3" pad="5"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
<connect gate="A" pin="VOUT" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMP2012MA"/>
<attribute name="OC_FARNELL" value="1286777"/>
<attribute name="OC_NEWARK" value="79K7706"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMP2012MM" prefix="U">
<description>Op Amp</description>
<gates>
<gate name="A" symbol="LMP2012MM"/>
</gates>
<devices>
<device name="" package="SOP65P490X109-8N">
<connects>
<connect gate="A" pin="INA+" pad="3"/>
<connect gate="A" pin="INA-" pad="2"/>
<connect gate="A" pin="INB+" pad="5"/>
<connect gate="A" pin="INB-" pad="6"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMP2012MM"/>
<attribute name="OC_FARNELL" value="1008038"/>
<attribute name="OC_NEWARK" value="41K2908"/>
<attribute name="PACKAGE" value="MSOP-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMP2014MT" prefix="U">
<description>Rail-to-Rail Output Operational</description>
<gates>
<gate name="A" symbol="LMP2014MT"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-14N">
<connects>
<connect gate="A" pin="+INA" pad="3"/>
<connect gate="A" pin="+INB" pad="5"/>
<connect gate="A" pin="+INC" pad="10"/>
<connect gate="A" pin="+IND" pad="12"/>
<connect gate="A" pin="-INA" pad="2"/>
<connect gate="A" pin="-INB" pad="6"/>
<connect gate="A" pin="-INC" pad="9"/>
<connect gate="A" pin="-IND" pad="13"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="OUTC" pad="8"/>
<connect gate="A" pin="OUTD" pad="14"/>
<connect gate="A" pin="V+" pad="4"/>
<connect gate="A" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMP2014MT"/>
<attribute name="OC_FARNELL" value="1559339"/>
<attribute name="OC_NEWARK" value="41K2910"/>
<attribute name="PACKAGE" value="TSSOP-14"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMP2015MA" prefix="U">
<description>Operational Amplifier</description>
<gates>
<gate name="A" symbol="LMP2015MA"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="NC" pad="8"/>
<connect gate="A" pin="NC_2" pad="1"/>
<connect gate="A" pin="NC_3" pad="5"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
<connect gate="A" pin="VIN+" pad="3"/>
<connect gate="A" pin="VIN-" pad="2"/>
<connect gate="A" pin="VOUT" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMP2015MA"/>
<attribute name="OC_FARNELL" value="1542530"/>
<attribute name="OC_NEWARK" value="75M6030"/>
<attribute name="PACKAGE" value="8-SOIC"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMP2015MF" prefix="U">
<description>Rail-to-Rail Output Operational Amplifier</description>
<gates>
<gate name="A" symbol="LMP2015MF"/>
</gates>
<devices>
<device name="" package="SOT95P285X120-5N">
<connects>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="A" pin="V+" pad="5"/>
<connect gate="A" pin="V-" pad="2"/>
<connect gate="A" pin="VIN+" pad="3"/>
<connect gate="A" pin="VIN-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMP2015MF"/>
<attribute name="OC_FARNELL" value="1542531"/>
<attribute name="OC_NEWARK" value="75M6031"/>
<attribute name="PACKAGE" value="SOT-23-5"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMP2016MA" prefix="U">
<description>OpAmpIC</description>
<gates>
<gate name="A" symbol="LMP2016MA"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="NC" pad="8"/>
<connect gate="A" pin="NC_2" pad="1"/>
<connect gate="A" pin="NC_3" pad="5"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
<connect gate="A" pin="VIN+" pad="3"/>
<connect gate="A" pin="VIN-" pad="2"/>
<connect gate="A" pin="VOUT" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMP2016MA"/>
<attribute name="OC_FARNELL" value=""/>
<attribute name="OC_NEWARK" value="84M8066"/>
<attribute name="PACKAGE" value="SOIC"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMP2016MM" prefix="U">
<description>Op Amp</description>
<gates>
<gate name="A" symbol="LMP2016MM"/>
</gates>
<devices>
<device name="" package="SOP65P490X109-8N">
<connects>
<connect gate="A" pin="INA+" pad="3"/>
<connect gate="A" pin="INA-" pad="2"/>
<connect gate="A" pin="INB+" pad="5"/>
<connect gate="A" pin="INB-" pad="6"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMP2016MM"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="84M8068"/>
<attribute name="PACKAGE" value="MSOP-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMP2021MA" prefix="U">
<description>Amplifiers</description>
<gates>
<gate name="A" symbol="LMP2021MA"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="IN+" pad="3"/>
<connect gate="A" pin="IN-" pad="2"/>
<connect gate="A" pin="NC" pad="8"/>
<connect gate="A" pin="NC_2" pad="5"/>
<connect gate="A" pin="NC_3" pad="1"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMP2021MA"/>
<attribute name="OC_FARNELL" value="1684977"/>
<attribute name="OC_NEWARK" value="19P7825"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMP2021MF" prefix="U">
<description>EMI Hardened Amplifiers</description>
<gates>
<gate name="A" symbol="LMP2021MF"/>
</gates>
<devices>
<device name="" package="SOT95P285X120-5N">
<connects>
<connect gate="A" pin="IN+" pad="3"/>
<connect gate="A" pin="IN-" pad="4"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="A" pin="V+" pad="5"/>
<connect gate="A" pin="V-" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMP2021MF"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="34P4733"/>
<attribute name="PACKAGE" value="SOT-23-5"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMP2022MA" prefix="U">
<description>Hardened Amplifiers</description>
<gates>
<gate name="A" symbol="LMP2022MA"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="IN+" pad="3"/>
<connect gate="A" pin="IN-" pad="2"/>
<connect gate="A" pin="NC" pad="8"/>
<connect gate="A" pin="NC_2" pad="1"/>
<connect gate="A" pin="NC_3" pad="5"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMP2022MA"/>
<attribute name="OC_FARNELL" value="1689556"/>
<attribute name="OC_NEWARK" value="19P7827"/>
<attribute name="PACKAGE" value="8-SOIC"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMP2231AMA" prefix="U">
<description>Precision Operational Amplifier</description>
<gates>
<gate name="A" symbol="LMP2231AMA"/>
</gates>
<devices>
<device name="" package="SOIC127P620X175-8N">
<connects>
<connect gate="A" pin="N/C" pad="8"/>
<connect gate="A" pin="N/C_2" pad="1"/>
<connect gate="A" pin="NC" pad="5"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
<connect gate="A" pin="VIN+" pad="3"/>
<connect gate="A" pin="VIN-" pad="2"/>
<connect gate="A" pin="VOUT" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMP2231AMA"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="84M8070"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMP2231AMF" prefix="U">
<description>Precision Operational Amplifier</description>
<gates>
<gate name="A" symbol="LMP2231AMF"/>
</gates>
<devices>
<device name="" package="SOT95P285X110-5N">
<connects>
<connect gate="A" pin="IN+" pad="3"/>
<connect gate="A" pin="IN-" pad="4"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="A" pin="V+" pad="5"/>
<connect gate="A" pin="V-" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMP2231AMF"/>
<attribute name="OC_FARNELL" value="1694642"/>
<attribute name="OC_NEWARK" value="84M8072"/>
<attribute name="PACKAGE" value="SOT-5"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMP2232AMA" prefix="U">
<description>Precision Operational Amplifier</description>
<gates>
<gate name="A" symbol="LMP2232AMA"/>
</gates>
<devices>
<device name="" package="SOIC127P620X175-8N">
<connects>
<connect gate="A" pin="INA+" pad="3"/>
<connect gate="A" pin="INA-" pad="2"/>
<connect gate="A" pin="INB+" pad="5"/>
<connect gate="A" pin="INB-" pad="6"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMP2232AMA"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="64M6896"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMP2234AMA" prefix="U">
<description>Precision Operational Amplifier</description>
<gates>
<gate name="A" symbol="LMP2234AMA"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-14N">
<connects>
<connect gate="A" pin="INA+" pad="3"/>
<connect gate="A" pin="INA-" pad="2"/>
<connect gate="A" pin="INB+" pad="5"/>
<connect gate="A" pin="INB-" pad="6"/>
<connect gate="A" pin="INC+" pad="10"/>
<connect gate="A" pin="INC-" pad="9"/>
<connect gate="A" pin="IND+" pad="12"/>
<connect gate="A" pin="IND-" pad="13"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="OUTC" pad="8"/>
<connect gate="A" pin="OUTD" pad="14"/>
<connect gate="A" pin="V+" pad="4"/>
<connect gate="A" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMP2234AMT"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="55M4618"/>
<attribute name="PACKAGE" value="TSSOP-14"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMP2234AMT" prefix="U">
<description>Precision Operational Amplifier</description>
<gates>
<gate name="A" symbol="LMP2234AMT"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-14N">
<connects>
<connect gate="A" pin="INA+" pad="3"/>
<connect gate="A" pin="INA-" pad="2"/>
<connect gate="A" pin="INB+" pad="5"/>
<connect gate="A" pin="INB-" pad="6"/>
<connect gate="A" pin="INC+" pad="10"/>
<connect gate="A" pin="INC-" pad="9"/>
<connect gate="A" pin="IND+" pad="12"/>
<connect gate="A" pin="IND-" pad="13"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="OUTC" pad="8"/>
<connect gate="A" pin="OUTD" pad="14"/>
<connect gate="A" pin="V+" pad="4"/>
<connect gate="A" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMP2234AMT"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="55M4618"/>
<attribute name="PACKAGE" value="TSSOP-14"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMP7300MA" prefix="U">
<description>Precision Comparator</description>
<gates>
<gate name="A" symbol="LMP7300MA"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="+IN" pad="1"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="HYSP" pad="6"/>
<connect gate="A" pin="HYST" pad="5"/>
<connect gate="A" pin="OUT" pad="4"/>
<connect gate="A" pin="REF" pad="7"/>
<connect gate="A" pin="V+" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMP7300MA"/>
<attribute name="OC_FARNELL" value="1495062"/>
<attribute name="OC_NEWARK" value="46M5449"/>
<attribute name="PACKAGE" value="8-SOIC"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMP7701MF" prefix="U">
<description>Wide Supply Range Amplifiers</description>
<gates>
<gate name="A" symbol="LMP7701MF"/>
</gates>
<devices>
<device name="" package="SOT95P285X120-5N">
<connects>
<connect gate="A" pin="IN+" pad="3"/>
<connect gate="A" pin="IN-" pad="4"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="A" pin="V+" pad="5"/>
<connect gate="A" pin="V-" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMP7701MF"/>
<attribute name="OC_FARNELL" value="1312606"/>
<attribute name="OC_NEWARK" value="69K2293"/>
<attribute name="PACKAGE" value="SOT23-5"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMP7702MA" prefix="U">
<description>Amplifiers</description>
<gates>
<gate name="A" symbol="LMP7702MA"/>
</gates>
<devices>
<device name="" package="SOIC127P620X175-8N">
<connects>
<connect gate="A" pin="INA+" pad="3"/>
<connect gate="A" pin="INA-" pad="2"/>
<connect gate="A" pin="INB+" pad="5"/>
<connect gate="A" pin="INB-" pad="6"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMP7702MA"/>
<attribute name="OC_FARNELL" value="1651867"/>
<attribute name="OC_NEWARK" value="55M4624"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMP7702MM" prefix="U">
<description>Op Amp</description>
<gates>
<gate name="A" symbol="LMP7702MM"/>
</gates>
<devices>
<device name="" package="SOP65P490X109-8N">
<connects>
<connect gate="A" pin="INA+" pad="3"/>
<connect gate="A" pin="INA-" pad="2"/>
<connect gate="A" pin="INB+" pad="5"/>
<connect gate="A" pin="INB-" pad="6"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMP7702MM"/>
<attribute name="OC_FARNELL" value="1559864"/>
<attribute name="OC_NEWARK" value="99K2273"/>
<attribute name="PACKAGE" value="MSOP-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMP7704MA" prefix="U">
<description>Precision Amplifier</description>
<gates>
<gate name="A" symbol="LMP7704MA"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="INA+" pad="3"/>
<connect gate="A" pin="INA-" pad="2"/>
<connect gate="A" pin="INB+" pad="5"/>
<connect gate="A" pin="INB-" pad="6"/>
<connect gate="A" pin="INC+" pad="10"/>
<connect gate="A" pin="INC-" pad="9"/>
<connect gate="A" pin="IND+" pad="12"/>
<connect gate="A" pin="IND-" pad="13"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="OUTC" pad="8"/>
<connect gate="A" pin="OUTD" pad="14"/>
<connect gate="A" pin="V+" pad="4"/>
<connect gate="A" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMP7704MA"/>
<attribute name="OC_FARNELL" value="1663020"/>
<attribute name="OC_NEWARK" value="11N9157"/>
<attribute name="PACKAGE" value="14-SOIC"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMP7704MT" prefix="U">
<description>Wide Supply Range Amplifiers</description>
<gates>
<gate name="A" symbol="LMP7704MT"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-14N">
<connects>
<connect gate="A" pin="+INA" pad="3"/>
<connect gate="A" pin="+INB" pad="5"/>
<connect gate="A" pin="+INC" pad="10"/>
<connect gate="A" pin="+IND" pad="12"/>
<connect gate="A" pin="-INA" pad="2"/>
<connect gate="A" pin="-INB" pad="6"/>
<connect gate="A" pin="-INC" pad="9"/>
<connect gate="A" pin="-IND" pad="13"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="OUTC" pad="8"/>
<connect gate="A" pin="OUTD" pad="14"/>
<connect gate="A" pin="V+" pad="4"/>
<connect gate="A" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMP7704MT"/>
<attribute name="OC_FARNELL" value="1286779"/>
<attribute name="OC_NEWARK" value="79K7710"/>
<attribute name="PACKAGE" value="TSSOP-14"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMP7707MA" prefix="U">
<description>Decompensated Amplifiers</description>
<gates>
<gate name="A" symbol="LMP7707MA"/>
</gates>
<devices>
<device name="" package="SOIC127P620X175-8N">
<connects>
<connect gate="A" pin="IN+" pad="3"/>
<connect gate="A" pin="IN-" pad="2"/>
<connect gate="A" pin="NC" pad="8"/>
<connect gate="A" pin="NC_2" pad="5"/>
<connect gate="A" pin="NC_3" pad="1"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMP7707MA"/>
<attribute name="OC_FARNELL" value="1663000"/>
<attribute name="OC_NEWARK" value="02P9785"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMP7708MA" prefix="U">
<description>Decompensated Amplifiers</description>
<gates>
<gate name="A" symbol="LMP7708MA"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="+INA" pad="3"/>
<connect gate="A" pin="+INB" pad="5"/>
<connect gate="A" pin="-INA" pad="2"/>
<connect gate="A" pin="-INB" pad="6"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMP7708MA"/>
<attribute name="OC_FARNELL" value="1663001"/>
<attribute name="OC_NEWARK" value="02P9786"/>
<attribute name="PACKAGE" value="8-SOIC"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMP7708MM" prefix="U">
<description>Decompensated Amplifiers</description>
<gates>
<gate name="A" symbol="LMP7708MM"/>
</gates>
<devices>
<device name="" package="SOP65P490X110-8N">
<connects>
<connect gate="A" pin="+INA" pad="3"/>
<connect gate="A" pin="+INB" pad="5"/>
<connect gate="A" pin="-INA" pad="2"/>
<connect gate="A" pin="-INB" pad="6"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMP7708MM"/>
<attribute name="OC_FARNELL" value="58M7986"/>
<attribute name="OC_NEWARK" value="1433151"/>
<attribute name="PACKAGE" value="MSOP-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMP7709MA" prefix="U">
<description>Decompensated Amplifiers</description>
<gates>
<gate name="A" symbol="LMP7709MA"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="INA+" pad="3"/>
<connect gate="A" pin="INA-" pad="2"/>
<connect gate="A" pin="INB+" pad="5"/>
<connect gate="A" pin="INB-" pad="6"/>
<connect gate="A" pin="INC+" pad="10"/>
<connect gate="A" pin="INC-" pad="9"/>
<connect gate="A" pin="IND+" pad="12"/>
<connect gate="A" pin="IND-" pad="13"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="OUTC" pad="8"/>
<connect gate="A" pin="OUTD" pad="14"/>
<connect gate="A" pin="V+" pad="4"/>
<connect gate="A" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMP7709MA"/>
<attribute name="OC_FARNELL" value="1663002"/>
<attribute name="OC_NEWARK" value="02P9787"/>
<attribute name="PACKAGE" value="14-SOIC"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMP7709MT" prefix="U">
<description>Decompensated Amplifiers</description>
<gates>
<gate name="A" symbol="LMP7709MT"/>
</gates>
<devices>
<device name="" package="SOP65P620X110-14N">
<connects>
<connect gate="A" pin="INA+" pad="3"/>
<connect gate="A" pin="INA-" pad="2"/>
<connect gate="A" pin="INB+" pad="5"/>
<connect gate="A" pin="INB-" pad="6"/>
<connect gate="A" pin="INC+" pad="10"/>
<connect gate="A" pin="INC-" pad="9"/>
<connect gate="A" pin="IND+" pad="12"/>
<connect gate="A" pin="IND-" pad="13"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="OUTC" pad="8"/>
<connect gate="A" pin="OUTD" pad="14"/>
<connect gate="A" pin="V+" pad="4"/>
<connect gate="A" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMP7709MT"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="54M4621"/>
<attribute name="PACKAGE" value="TSSOP-14"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMP7711MK" prefix="U">
<description>CMOS Input Amplifiers</description>
<gates>
<gate name="A" symbol="LMP7711MK"/>
</gates>
<devices>
<device name="" package="SOT95P285X100-6N">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="4"/>
<connect gate="A" pin="EN" pad="5"/>
<connect gate="A" pin="OUT_" pad="1"/>
<connect gate="A" pin="V+" pad="6"/>
<connect gate="A" pin="V-" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMP7711MK"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="79K7713"/>
<attribute name="PACKAGE" value="SOT-23-6"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMP7712MM" prefix="U">
<description>CMOS Input Amplifiers</description>
<gates>
<gate name="A" symbol="LMP7712MM"/>
</gates>
<devices>
<device name="" package="SOP50P490X110-10N">
<connects>
<connect gate="A" pin="+INA" pad="3"/>
<connect gate="A" pin="+INB" pad="7"/>
<connect gate="A" pin="-INA" pad="2"/>
<connect gate="A" pin="-INB" pad="8"/>
<connect gate="A" pin="ENA" pad="5"/>
<connect gate="A" pin="ENB" pad="6"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="9"/>
<connect gate="A" pin="V+" pad="10"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMP7712MM"/>
<attribute name="OC_FARNELL" value="1312609"/>
<attribute name="OC_NEWARK" value="31M5302"/>
<attribute name="PACKAGE" value="MSOP-10"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMP7715MF" prefix="U">
<description>CMOS Input Amplifiers</description>
<gates>
<gate name="A" symbol="LMP7715MF"/>
</gates>
<devices>
<device name="" package="SOT95P285X120-5N">
<connects>
<connect gate="A" pin="IN+" pad="3"/>
<connect gate="A" pin="IN-" pad="4"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="A" pin="V+" pad="5"/>
<connect gate="A" pin="V-" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMP7715MF"/>
<attribute name="OC_FARNELL" value="1312821"/>
<attribute name="OC_NEWARK" value="99K2277"/>
<attribute name="PACKAGE" value="SOT23-5"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMP7716MM" prefix="U">
<description>Amplifiers</description>
<gates>
<gate name="A" symbol="LMP7716MM"/>
</gates>
<devices>
<device name="" package="SOP65P490X109-8N">
<connects>
<connect gate="A" pin="INA+" pad="3"/>
<connect gate="A" pin="INA-" pad="2"/>
<connect gate="A" pin="INB+" pad="5"/>
<connect gate="A" pin="INB-" pad="6"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMP7716MM"/>
<attribute name="OC_FARNELL" value="1312822"/>
<attribute name="OC_NEWARK" value="99K2281"/>
<attribute name="PACKAGE" value="MSOP-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMP7716QMM" prefix="U">
<description>Amplifiers</description>
<gates>
<gate name="A" symbol="LMP7716QMM"/>
</gates>
<devices>
<device name="" package="SOP65P490X109-8N">
<connects>
<connect gate="A" pin="INA+" pad="3"/>
<connect gate="A" pin="INA-" pad="2"/>
<connect gate="A" pin="INB+" pad="5"/>
<connect gate="A" pin="INB-" pad="6"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMP7716QMM"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="34P4740"/>
<attribute name="PACKAGE" value="MSOP-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMP7717MA" prefix="U">
<description>Decompensated Operational Amplifier</description>
<gates>
<gate name="A" symbol="LMP7717MA"/>
</gates>
<devices>
<device name="" package="SOIC127P620X175-8N">
<connects>
<connect gate="A" pin="+INA" pad="3"/>
<connect gate="A" pin="+INB" pad="5"/>
<connect gate="A" pin="-INA" pad="2"/>
<connect gate="A" pin="-INB" pad="6"/>
<connect gate="A" pin="OUT_A" pad="1"/>
<connect gate="A" pin="OUT_B" pad="7"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMP7717MA"/>
<attribute name="OC_FARNELL" value="1342336"/>
<attribute name="OC_NEWARK" value="42M2044"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMP7717MF" prefix="U">
<description>Decompensated Operational Amplifier</description>
<gates>
<gate name="A" symbol="LMP7717MF"/>
</gates>
<devices>
<device name="" package="SOT95P285X120-5N">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="4"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="A" pin="V+" pad="5"/>
<connect gate="A" pin="V-" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMP7717MF"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="46M5453"/>
<attribute name="PACKAGE" value="SOT-23-5"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMP7718MA" prefix="U">
<description>Decompensated Operational Amplifier</description>
<gates>
<gate name="A" symbol="LMP7718MA"/>
</gates>
<devices>
<device name="" package="SOIC127P620X175-8N">
<connects>
<connect gate="A" pin="INA+" pad="3"/>
<connect gate="A" pin="INA-" pad="2"/>
<connect gate="A" pin="INB+" pad="5"/>
<connect gate="A" pin="INB-" pad="6"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMP7718MA"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="53M0340"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMP7718MM" prefix="U">
<description>OP AMP</description>
<gates>
<gate name="A" symbol="LMP7718MM"/>
</gates>
<devices>
<device name="" package="SOP65P490X110-8N">
<connects>
<connect gate="A" pin="+INA" pad="3"/>
<connect gate="A" pin="+INB" pad="5"/>
<connect gate="A" pin="-INA" pad="2"/>
<connect gate="A" pin="-INB" pad="6"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMP7718MM"/>
<attribute name="OC_FARNELL" value="1433174"/>
<attribute name="OC_NEWARK" value="58M7988"/>
<attribute name="PACKAGE" value="MSOP-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMP7721MA" prefix="U">
<description>Precision Amplifier</description>
<gates>
<gate name="A" symbol="LMP7721MA"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="IN+" pad="1"/>
<connect gate="A" pin="IN-" pad="8"/>
<connect gate="A" pin="NC" pad="7"/>
<connect gate="A" pin="NC_2" pad="2"/>
<connect gate="A" pin="NC_3" pad="5"/>
<connect gate="A" pin="V+" pad="6"/>
<connect gate="A" pin="V-" pad="3"/>
<connect gate="A" pin="VOUT" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMP7721MA"/>
<attribute name="OC_FARNELL" value="1552453"/>
<attribute name="OC_NEWARK" value="94M7981"/>
<attribute name="PACKAGE" value="8-SOIC"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMP7731MA" prefix="U">
<description>Low Noise, Precision, RRIO Amplifier</description>
<gates>
<gate name="A" symbol="LMP7731MA"/>
</gates>
<devices>
<device name="" package="SOIC127P620X175-8N">
<connects>
<connect gate="A" pin="IN+" pad="3"/>
<connect gate="A" pin="IN-" pad="2"/>
<connect gate="A" pin="N/C" pad="8"/>
<connect gate="A" pin="N/C_2" pad="5"/>
<connect gate="A" pin="N/C_3" pad="1"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMP7731MA"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="01P0821"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMP7731MF" prefix="U">
<description>Amplifier</description>
<gates>
<gate name="A" symbol="LMP7731MF"/>
</gates>
<devices>
<device name="" package="SOT95P284X119-5N">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="4"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="A" pin="V+" pad="5"/>
<connect gate="A" pin="V-" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMP7731MF"/>
<attribute name="OC_FARNELL" value="1433181"/>
<attribute name="OC_NEWARK" value="50M8797"/>
<attribute name="PACKAGE" value="SOT23-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMP7732MA" prefix="U">
<description>RRIO Amplifier</description>
<gates>
<gate name="A" symbol="LMP7732MA"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="+INA" pad="3"/>
<connect gate="A" pin="+INB" pad="5"/>
<connect gate="A" pin="-INA" pad="2"/>
<connect gate="A" pin="-INB" pad="6"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMP7732MA"/>
<attribute name="OC_FARNELL" value="1495065"/>
<attribute name="OC_NEWARK" value="54M4627"/>
<attribute name="PACKAGE" value="8-SOIC"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMP7732MM" prefix="U">
<description>RRIO Amplifier</description>
<gates>
<gate name="A" symbol="LMP7732MM"/>
</gates>
<devices>
<device name="" package="SOP65P490X110-8N">
<connects>
<connect gate="A" pin="+INA" pad="3"/>
<connect gate="A" pin="+INB" pad="5"/>
<connect gate="A" pin="-INA" pad="2"/>
<connect gate="A" pin="-INB" pad="6"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMP7732MM"/>
<attribute name="OC_FARNELL" value="1663023"/>
<attribute name="OC_NEWARK" value="15P1952"/>
<attribute name="PACKAGE" value="MSOP-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMP8100MA" prefix="U">
<description>Amplifier</description>
<gates>
<gate name="A" symbol="LMP8100MA"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="DGND" pad="2"/>
<connect gate="A" pin="GRT1" pad="11"/>
<connect gate="A" pin="GRT2" pad="10"/>
<connect gate="A" pin="IN+" pad="12"/>
<connect gate="A" pin="NC" pad="14"/>
<connect gate="A" pin="NC_2" pad="9"/>
<connect gate="A" pin="NC_3" pad="1"/>
<connect gate="A" pin="SCK" pad="3"/>
<connect gate="A" pin="SDI" pad="5"/>
<connect gate="A" pin="SDO" pad="6"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="7"/>
<connect gate="A" pin="VOUT" pad="13"/>
<connect gate="A" pin="~CS" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMP8100MA"/>
<attribute name="OC_FARNELL" value="1433175"/>
<attribute name="OC_NEWARK" value="53M0341"/>
<attribute name="PACKAGE" value="14-SOIC"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMP8601MA" prefix="U">
<description>Bidirectional Precision Current Sensing Amplifier</description>
<gates>
<gate name="A" symbol="LMP8601MA"/>
</gates>
<devices>
<device name="" package="SOIC127P620X175-8N">
<connects>
<connect gate="A" pin="+IN" pad="8"/>
<connect gate="A" pin="-IN" pad="1"/>
<connect gate="A" pin="A1" pad="3"/>
<connect gate="A" pin="A2" pad="4"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="OFFSET" pad="7"/>
<connect gate="A" pin="OUT" pad="5"/>
<connect gate="A" pin="VS" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMP8601MA"/>
<attribute name="OC_FARNELL" value="1684983"/>
<attribute name="OC_NEWARK" value="19P7829"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMP8601QMA" prefix="U">
<description>Bidirectional Precision Current Sensing Amplifier</description>
<gates>
<gate name="A" symbol="LMP8601QMA"/>
</gates>
<devices>
<device name="" package="SOIC127P620X175-8N">
<connects>
<connect gate="A" pin="+IN" pad="8"/>
<connect gate="A" pin="-IN" pad="1"/>
<connect gate="A" pin="A1" pad="3"/>
<connect gate="A" pin="A2" pad="4"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="OFFSET" pad="7"/>
<connect gate="A" pin="OUT" pad="5"/>
<connect gate="A" pin="VS" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMP8601QMA"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="34P4743"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMP8602MA" prefix="U">
<description>Bidirectional Precision Current Sensing Amplifier</description>
<gates>
<gate name="A" symbol="LMP8602MA"/>
</gates>
<devices>
<device name="" package="SOIC127P620X175-8N">
<connects>
<connect gate="A" pin="+IN" pad="8"/>
<connect gate="A" pin="-IN" pad="1"/>
<connect gate="A" pin="A1" pad="3"/>
<connect gate="A" pin="A2" pad="4"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="OFFSET" pad="7"/>
<connect gate="A" pin="OUT" pad="5"/>
<connect gate="A" pin="VS" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMP8602MA"/>
<attribute name="OC_FARNELL" value="1736508"/>
<attribute name="OC_NEWARK" value="16R1307"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMP8602MM" prefix="U">
<description>Sensing Amplifier</description>
<gates>
<gate name="A" symbol="LMP8602MM"/>
</gates>
<devices>
<device name="" package="SOP65P490X109-8N">
<connects>
<connect gate="A" pin="+IN" pad="8"/>
<connect gate="A" pin="-IN" pad="1"/>
<connect gate="A" pin="A1" pad="3"/>
<connect gate="A" pin="A2" pad="4"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="OFFSET" pad="7"/>
<connect gate="A" pin="OUT" pad="5"/>
<connect gate="A" pin="VS" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMP8602MM"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="55R3741"/>
<attribute name="PACKAGE" value="MSOP-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMP8603MA" prefix="U">
<description>Bidirectional Precision Current Sensing Amplifier</description>
<gates>
<gate name="A" symbol="LMP8603MA"/>
</gates>
<devices>
<device name="" package="SOIC127P620X175-8N">
<connects>
<connect gate="A" pin="+IN" pad="8"/>
<connect gate="A" pin="-IN" pad="1"/>
<connect gate="A" pin="A1" pad="3"/>
<connect gate="A" pin="A2" pad="4"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="OFFSET" pad="7"/>
<connect gate="A" pin="OUT" pad="5"/>
<connect gate="A" pin="VS" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMP8603MA"/>
<attribute name="OC_FARNELL" value="1736509"/>
<attribute name="OC_NEWARK" value="16R1308"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMP8603MM" prefix="U">
<description>Sensing Amplifier</description>
<gates>
<gate name="A" symbol="LMP8603MM"/>
</gates>
<devices>
<device name="" package="SOP65P490X109-8N">
<connects>
<connect gate="A" pin="+IN" pad="8"/>
<connect gate="A" pin="-IN" pad="1"/>
<connect gate="A" pin="A1" pad="3"/>
<connect gate="A" pin="A2" pad="4"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="OFFSET" pad="7"/>
<connect gate="A" pin="OUT" pad="5"/>
<connect gate="A" pin="VS" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMP8603MM"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="55R3745"/>
<attribute name="PACKAGE" value="MSOP-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMP8645MK">
<description>Precision High Voltage Current Sense Amplifier</description>
<gates>
<gate name="A" symbol="LMP8645MK"/>
</gates>
<devices>
<device name="" package="SOT95P285X100-6N">
<connects>
<connect gate="A" pin="IN+" pad="3"/>
<connect gate="A" pin="IN-" pad="4"/>
<connect gate="A" pin="RG" pad="5"/>
<connect gate="A" pin="V+" pad="6"/>
<connect gate="A" pin="V-" pad="2"/>
<connect gate="A" pin="VOUT" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMP8645MK"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="55R3751"/>
<attribute name="PACKAGE" value="SOT-23-6"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMS1487ECM" prefix="U">
<description>RS-485 / RS-422 Differential Bus Transceiver</description>
<gates>
<gate name="A" symbol="LMS1487ECM"/>
</gates>
<devices>
<device name="" package="SOIC127P620X175-8N">
<connects>
<connect gate="A" pin="A" pad="6"/>
<connect gate="A" pin="B" pad="7"/>
<connect gate="A" pin="DE" pad="3"/>
<connect gate="A" pin="DI" pad="4"/>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="RO" pad="1"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="~RE" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMS1487ECM"/>
<attribute name="OC_FARNELL" value="8181497"/>
<attribute name="OC_NEWARK" value="38K3547"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMS1487ECNA" prefix="U">
<description>Transceiver</description>
<gates>
<gate name="A" symbol="LMS1487ECNA"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-8">
<connects>
<connect gate="A" pin="A" pad="6"/>
<connect gate="A" pin="B" pad="7"/>
<connect gate="A" pin="DE" pad="3"/>
<connect gate="A" pin="DI" pad="4"/>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="RO" pad="1"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="~RE" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMS1487ECNA"/>
<attribute name="OC_FARNELL" value="8181500"/>
<attribute name="OC_NEWARK" value="38K3548"/>
<attribute name="PACKAGE" value="DIP-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMS1587CS-1.5" prefix="U">
<description>Low Dropout Fast Response Regulators</description>
<gates>
<gate name="A" symbol="LMS1587CS-1.5"/>
</gates>
<devices>
<device name="" package="TO254P1435X464-4N">
<connects>
<connect gate="A" pin="GND" pad="1"/>
<connect gate="A" pin="IN" pad="3"/>
<connect gate="A" pin="OUT" pad="2"/>
<connect gate="A" pin="VOUT" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMS1587CS-1.5"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K2946"/>
<attribute name="PACKAGE" value="TO-263-3"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMS1587CS-3.3" prefix="U">
<description>Low Dropout Fast Response Regulators</description>
<gates>
<gate name="A" symbol="LMS1587CS-3.3"/>
</gates>
<devices>
<device name="" package="TO254P1435X464-4N">
<connects>
<connect gate="A" pin="GND" pad="1"/>
<connect gate="A" pin="IN" pad="3"/>
<connect gate="A" pin="OUT" pad="2"/>
<connect gate="A" pin="VOUT" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMS1587CS-3.3"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K2947"/>
<attribute name="PACKAGE" value="TO-263-3"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMS1587CT-3.3" prefix="U">
<description>IC REG LDO 3.3V 3A</description>
<gates>
<gate name="A" symbol="LMS1587CT-3.3"/>
</gates>
<devices>
<device name="" package="TO254P470X1016X2222-3P">
<connects>
<connect gate="A" pin="ADJ/GND" pad="1"/>
<connect gate="A" pin="VIN" pad="3"/>
<connect gate="A" pin="VOUT" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMS1587CT-3.3"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K2952"/>
<attribute name="PACKAGE" value="TO-220"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMS1587CT-ADJ" prefix="U">
<description>ADJ/NOPB IC REG LDO ADJ 3A</description>
<gates>
<gate name="A" symbol="LMS1587CT-ADJ"/>
</gates>
<devices>
<device name="" package="TO254P470X1016X2222-3P">
<connects>
<connect gate="A" pin="ADJ/GND" pad="1"/>
<connect gate="A" pin="VIN" pad="3"/>
<connect gate="A" pin="VOUT" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMS1587CT-ADJ"/>
<attribute name="OC_FARNELL" value="7613842"/>
<attribute name="OC_NEWARK" value="74C3703"/>
<attribute name="PACKAGE" value="TO-220"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMS1587IS-1.5" prefix="U">
<description>Low Dropout Fast Response Regulators</description>
<gates>
<gate name="A" symbol="LMS1587IS-1.5"/>
</gates>
<devices>
<device name="" package="TO254P1435X464-4N">
<connects>
<connect gate="A" pin="GND" pad="1"/>
<connect gate="A" pin="IN" pad="3"/>
<connect gate="A" pin="OUT" pad="2"/>
<connect gate="A" pin="VOUT" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMS1587IS-1.5"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K2954"/>
<attribute name="PACKAGE" value="TO-263-3"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMS1587IS-3.3" prefix="U">
<description>Low Dropout Fast Response Regulators</description>
<gates>
<gate name="A" symbol="LMS1587IS-3.3"/>
</gates>
<devices>
<device name="" package="TO254P1435X464-4N">
<connects>
<connect gate="A" pin="ADJ/GND" pad="1"/>
<connect gate="A" pin="IN" pad="3"/>
<connect gate="A" pin="OUT" pad="2"/>
<connect gate="A" pin="VOUT" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMS1587IS-3.3"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K2955"/>
<attribute name="PACKAGE" value="TO-263-3"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMS1587IS-ADJ" prefix="U">
<description>Low Dropout Fast Response Regulators</description>
<gates>
<gate name="A" symbol="LMS1587IS-ADJ"/>
</gates>
<devices>
<device name="" package="TO254P1435X464-4N">
<connects>
<connect gate="A" pin="ADJ" pad="1"/>
<connect gate="A" pin="IN" pad="3"/>
<connect gate="A" pin="OUT" pad="2"/>
<connect gate="A" pin="VOUT" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMS1587IS-ADJ"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K2953"/>
<attribute name="PACKAGE" value="TO-263-3"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMS33460MG" prefix="U">
<description>Detector</description>
<gates>
<gate name="A" symbol="LMS33460MG"/>
</gates>
<devices>
<device name="" package="SOT65P210X110-5N">
<connects>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="GND_2" pad="2"/>
<connect gate="A" pin="NC" pad="1"/>
<connect gate="A" pin="VIN" pad="5"/>
<connect gate="A" pin="~VOUT" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMS33460MG"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K2970"/>
<attribute name="PACKAGE" value="SC70-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMS8117ADT-3.3" prefix="U">
<description>Low-Dropout Linear Regulator</description>
<gates>
<gate name="A" symbol="LMS8117ADT-3.3"/>
</gates>
<devices>
<device name="" package="TO457P970X238-3N">
<connects>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="VIN" pad="3"/>
<connect gate="A" pin="VOUT" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMS8117ADT-3.3"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K3014"/>
<attribute name="PACKAGE" value="TO-252-3"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMS8117AMP-1.8" prefix="U">
<description>Low-Dropout Linear Regulator</description>
<gates>
<gate name="A" symbol="LMS8117AMP-1.8"/>
</gates>
<devices>
<device name="" package="SOT230P696X180-4N">
<connects>
<connect gate="A" pin="GND" pad="1"/>
<connect gate="A" pin="IN" pad="3"/>
<connect gate="A" pin="OUT" pad="2"/>
<connect gate="A" pin="VOUT" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMS8117AMP-1.8"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K3019"/>
<attribute name="PACKAGE" value="SOT-223-3"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMS8117AMP-3.3" prefix="U">
<description>Low-Dropout Linear Regulator</description>
<gates>
<gate name="A" symbol="LMS8117AMP-3.3"/>
</gates>
<devices>
<device name="" package="SOT230P696X180-4N">
<connects>
<connect gate="A" pin="GND" pad="1"/>
<connect gate="A" pin="IN" pad="3"/>
<connect gate="A" pin="OUT" pad="2"/>
<connect gate="A" pin="VOUT" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMS8117AMP-3.3"/>
<attribute name="OC_FARNELL" value="1469032"/>
<attribute name="OC_NEWARK" value="41K3020"/>
<attribute name="PACKAGE" value="SOT-223-3"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMS8117AMP-ADJ" prefix="U">
<description>Low-Dropout Linear Regulator</description>
<gates>
<gate name="A" symbol="LMS8117AMP-ADJ"/>
</gates>
<devices>
<device name="" package="SOT230P696X180-4N">
<connects>
<connect gate="A" pin="ADJ" pad="1"/>
<connect gate="A" pin="IN" pad="3"/>
<connect gate="A" pin="OUT" pad="2"/>
<connect gate="A" pin="VOUT" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMS8117AMP-ADJ"/>
<attribute name="OC_FARNELL" value="1685597"/>
<attribute name="OC_NEWARK" value="41K3018"/>
<attribute name="PACKAGE" value="SOT-223-3"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMV1032URX-25" prefix="U">
<description>Amplifiers for 3-Wire Analog Electret Microphones</description>
<gates>
<gate name="A" symbol="LMV1032URX-25"/>
</gates>
<devices>
<device name="" package="BGA4C2X2X50P_117X117X42">
<connects>
<connect gate="A" pin="GND" pad="A1"/>
<connect gate="A" pin="INPUT" pad="B1"/>
<connect gate="A" pin="OUTPUT" pad="A2"/>
<connect gate="A" pin="VCC" pad="B2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMV1032URX-25"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="69K2316"/>
<attribute name="PACKAGE" value="BGA-4"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMV1088RL" prefix="U">
<description>AUDIO POWER AMP, CLASS AB</description>
<gates>
<gate name="A" symbol="LMV1088RL"/>
</gates>
<devices>
<device name="" package="BGA36C6X6X50P_345X345X67">
<connects>
<connect gate="A" pin="ADR" pad="D1"/>
<connect gate="A" pin="CAL" pad="F6"/>
<connect gate="A" pin="GND" pad="B4"/>
<connect gate="A" pin="GND_2" pad="C5"/>
<connect gate="A" pin="GND_3" pad="D3"/>
<connect gate="A" pin="I2CVDD" pad="F2"/>
<connect gate="A" pin="LPF" pad="F5"/>
<connect gate="A" pin="MIC1+" pad="B6"/>
<connect gate="A" pin="MIC1-" pad="C6"/>
<connect gate="A" pin="MIC2+" pad="A5"/>
<connect gate="A" pin="MIC2-" pad="A4"/>
<connect gate="A" pin="MICBIAS" pad="A6"/>
<connect gate="A" pin="NC" pad="E6"/>
<connect gate="A" pin="NC_10" pad="C2"/>
<connect gate="A" pin="NC_2" pad="B1"/>
<connect gate="A" pin="NC_3" pad="E3"/>
<connect gate="A" pin="NC_4" pad="A1"/>
<connect gate="A" pin="NC_5" pad="E4"/>
<connect gate="A" pin="NC_6" pad="C1"/>
<connect gate="A" pin="NC_7" pad="E5"/>
<connect gate="A" pin="NC_8" pad="B2"/>
<connect gate="A" pin="NC_9" pad="D2"/>
<connect gate="A" pin="OUT" pad="F4"/>
<connect gate="A" pin="PE" pad="A3"/>
<connect gate="A" pin="REF" pad="D6"/>
<connect gate="A" pin="SCL" pad="E1"/>
<connect gate="A" pin="SDA" pad="F1"/>
<connect gate="A" pin="T1" pad="B5"/>
<connect gate="A" pin="T2" pad="D5"/>
<connect gate="A" pin="T3" pad="C4"/>
<connect gate="A" pin="T4" pad="D4"/>
<connect gate="A" pin="T5" pad="B3"/>
<connect gate="A" pin="T6" pad="C3"/>
<connect gate="A" pin="T7" pad="A2"/>
<connect gate="A" pin="T8" pad="E2"/>
<connect gate="A" pin="VDD" pad="F3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMV1088RL"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="64M6914"/>
<attribute name="PACKAGE" value="BGA-36"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMV1089RL" prefix="U">
<description>Audio Amplifier</description>
<gates>
<gate name="A" symbol="LMV1089RL"/>
</gates>
<devices>
<device name="" package="BGA36C6X6X50P_345X345X67">
<connects>
<connect gate="A" pin="ADR" pad="D1"/>
<connect gate="A" pin="CAL" pad="F6"/>
<connect gate="A" pin="EN" pad="E6"/>
<connect gate="A" pin="GA0" pad="C4"/>
<connect gate="A" pin="GA1" pad="D4"/>
<connect gate="A" pin="GB0" pad="C3"/>
<connect gate="A" pin="GB1" pad="E2"/>
<connect gate="A" pin="GND" pad="B4"/>
<connect gate="A" pin="GND_2" pad="C5"/>
<connect gate="A" pin="GND_3" pad="D3"/>
<connect gate="A" pin="I2CVDD" pad="F2"/>
<connect gate="A" pin="LPF+" pad="E5"/>
<connect gate="A" pin="LPF-" pad="F5"/>
<connect gate="A" pin="M1_UNP" pad="B5"/>
<connect gate="A" pin="M2_UNP" pad="D5"/>
<connect gate="A" pin="MIC1+" pad="B6"/>
<connect gate="A" pin="MIC1-" pad="C6"/>
<connect gate="A" pin="MIC2+" pad="A5"/>
<connect gate="A" pin="MIC2-" pad="A4"/>
<connect gate="A" pin="MICBIAS" pad="A6"/>
<connect gate="A" pin="NC" pad="C2"/>
<connect gate="A" pin="NC_2" pad="B1"/>
<connect gate="A" pin="NC_3" pad="E3"/>
<connect gate="A" pin="NC_4" pad="A1"/>
<connect gate="A" pin="NC_5" pad="C1"/>
<connect gate="A" pin="NC_6" pad="B2"/>
<connect gate="A" pin="NC_7" pad="D2"/>
<connect gate="A" pin="OUT+" pad="E4"/>
<connect gate="A" pin="OUT-" pad="F4"/>
<connect gate="A" pin="PE" pad="A3"/>
<connect gate="A" pin="REF" pad="D6"/>
<connect gate="A" pin="SCL" pad="E1"/>
<connect gate="A" pin="SDA" pad="F1"/>
<connect gate="A" pin="T5" pad="B3"/>
<connect gate="A" pin="T7" pad="A2"/>
<connect gate="A" pin="VDD" pad="F3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMV1089RL"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="19P2244"/>
<attribute name="PACKAGE" value="BGA-36"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMV1089VY" prefix="U">
<description>Far Field Noise Suppression Microphone Amplifier</description>
<gates>
<gate name="A" symbol="LMV1089VY"/>
</gates>
<devices>
<device name="" package="QFP80P900X900X160-32N">
<connects>
<connect gate="A" pin="12CVDD" pad="8"/>
<connect gate="A" pin="ADR" pad="13"/>
<connect gate="A" pin="CAL" pad="10"/>
<connect gate="A" pin="EN" pad="32"/>
<connect gate="A" pin="GA0" pad="14"/>
<connect gate="A" pin="GA1" pad="4"/>
<connect gate="A" pin="GB0" pad="19"/>
<connect gate="A" pin="GB1" pad="11"/>
<connect gate="A" pin="GND" pad="15"/>
<connect gate="A" pin="GND_2" pad="3"/>
<connect gate="A" pin="GND_3" pad="22"/>
<connect gate="A" pin="LPF+" pad="1"/>
<connect gate="A" pin="LPF-" pad="2"/>
<connect gate="A" pin="M1_UNP" pad="30"/>
<connect gate="A" pin="M2_UNP" pad="31"/>
<connect gate="A" pin="MIC1+" pad="27"/>
<connect gate="A" pin="MIC1-" pad="28"/>
<connect gate="A" pin="MIC2+" pad="25"/>
<connect gate="A" pin="MIC2-" pad="26"/>
<connect gate="A" pin="MIC_BIAS" pad="23"/>
<connect gate="A" pin="NC" pad="24"/>
<connect gate="A" pin="NC_2" pad="16"/>
<connect gate="A" pin="NC_3" pad="17"/>
<connect gate="A" pin="OUT+" pad="6"/>
<connect gate="A" pin="OUT-" pad="5"/>
<connect gate="A" pin="PE" pad="20"/>
<connect gate="A" pin="REF" pad="29"/>
<connect gate="A" pin="SCL" pad="12"/>
<connect gate="A" pin="SDA" pad="9"/>
<connect gate="A" pin="T5" pad="21"/>
<connect gate="A" pin="T7" pad="18"/>
<connect gate="A" pin="VDD" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMV1089VY"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="04R9105"/>
<attribute name="PACKAGE" value="QFP-32"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMV1090TL" prefix="U">
<description>Far Field Noise Suppression Microphone Amplifier</description>
<gates>
<gate name="A" symbol="LMV1090TL"/>
</gates>
<devices>
<device name="" package="BGA16C4X450P_197X197X60">
<connects>
<connect gate="A" pin="EN" pad="D1"/>
<connect gate="A" pin="GND" pad="B1"/>
<connect gate="A" pin="I2CVDD" pad="D4"/>
<connect gate="A" pin="LPF+" pad="B2"/>
<connect gate="A" pin="LPF-" pad="C2"/>
<connect gate="A" pin="MIC1+" pad="A2"/>
<connect gate="A" pin="MIC1-" pad="A1"/>
<connect gate="A" pin="MIC2+" pad="A4"/>
<connect gate="A" pin="MIC2-" pad="A3"/>
<connect gate="A" pin="MICBIAS" pad="C4"/>
<connect gate="A" pin="OUT+" pad="B3"/>
<connect gate="A" pin="OUT-" pad="C3"/>
<connect gate="A" pin="REF" pad="B4"/>
<connect gate="A" pin="SCL" pad="D3"/>
<connect gate="A" pin="SDA" pad="D2"/>
<connect gate="A" pin="VDD" pad="C1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMV1090TL"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="55R3755"/>
<attribute name="PACKAGE" value="BGA-16"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMV1091TM">
<description>Amplifier</description>
<gates>
<gate name="A" symbol="LMV1091TM"/>
</gates>
<devices>
<device name="" package="BGA25C40P5X5_201X201X60">
<connects>
<connect gate="A" pin="GA0" pad="B3"/>
<connect gate="A" pin="GA1" pad="B4"/>
<connect gate="A" pin="GA2" pad="C4"/>
<connect gate="A" pin="GA3" pad="D4"/>
<connect gate="A" pin="GB0" pad="C2"/>
<connect gate="A" pin="GB1" pad="D2"/>
<connect gate="A" pin="GB2" pad="D3"/>
<connect gate="A" pin="GND" pad="B5"/>
<connect gate="A" pin="LPF+" pad="E1"/>
<connect gate="A" pin="LPF-" pad="E4"/>
<connect gate="A" pin="MIC1+" pad="A4"/>
<connect gate="A" pin="MIC1-" pad="A5"/>
<connect gate="A" pin="MIC2+" pad="A2"/>
<connect gate="A" pin="MIC2-" pad="A3"/>
<connect gate="A" pin="MIC_BIAS" pad="A1"/>
<connect gate="A" pin="MODE0" pad="B1"/>
<connect gate="A" pin="MODE1" pad="B2"/>
<connect gate="A" pin="MUTE1" pad="D1"/>
<connect gate="A" pin="MUTE2" pad="C1"/>
<connect gate="A" pin="NC" pad="C3"/>
<connect gate="A" pin="OUT+" pad="E2"/>
<connect gate="A" pin="OUT-" pad="E3"/>
<connect gate="A" pin="REF" pad="C5"/>
<connect gate="A" pin="VDD" pad="D5"/>
<connect gate="A" pin="~SD" pad="E5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMV1091TM"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="77R5160"/>
<attribute name="PACKAGE" value="BGA-25"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMV112SD" prefix="U">
<description>Dual Clock Buffer</description>
<gates>
<gate name="A" symbol="LMV112SD"/>
</gates>
<devices>
<device name="" package="DFN300X300X80-9N">
<connects>
<connect gate="A" pin="EN1" pad="8"/>
<connect gate="A" pin="EN2" pad="4"/>
<connect gate="A" pin="EPAD" pad="9"/>
<connect gate="A" pin="IN1" pad="2"/>
<connect gate="A" pin="IN2" pad="3"/>
<connect gate="A" pin="OUT1" pad="7"/>
<connect gate="A" pin="OUT2" pad="6"/>
<connect gate="A" pin="VDD" pad="1"/>
<connect gate="A" pin="VSS" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMV112SD"/>
<attribute name="OC_FARNELL" value="1685395"/>
<attribute name="OC_NEWARK" value="65K5780"/>
<attribute name="PACKAGE" value="DFN-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMV116MF" prefix="U">
<description>Operational Amplifier</description>
<gates>
<gate name="A" symbol="LMV116MF"/>
</gates>
<devices>
<device name="" package="SOT95P285X120-5N">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="4"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="A" pin="V+" pad="5"/>
<connect gate="A" pin="V-" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMV116MF"/>
<attribute name="OC_FARNELL" value="8187622"/>
<attribute name="OC_NEWARK" value="41K3058"/>
<attribute name="PACKAGE" value="SOT-23-5"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMV118MF" prefix="U">
<description>Rail-to-Rail Output Operational Amplifiers</description>
<gates>
<gate name="A" symbol="LMV118MF"/>
</gates>
<devices>
<device name="" package="SOT95P285X120-6N">
<connects>
<connect gate="A" pin="+IN_" pad="3"/>
<connect gate="A" pin="-IN" pad="4"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="A" pin="SD" pad="5"/>
<connect gate="A" pin="V+" pad="6"/>
<connect gate="A" pin="V-" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMV118MF"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K3060"/>
<attribute name="PACKAGE" value="SOT-23-6"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMV2011MA" prefix="U">
<description>High Precision, Rail-to-Rail Output OP-AMP</description>
<gates>
<gate name="A" symbol="LMV2011MA"/>
</gates>
<devices>
<device name="" package="SOIC127P620X175-8N">
<connects>
<connect gate="A" pin="+VIN" pad="3"/>
<connect gate="A" pin="-VIN" pad="2"/>
<connect gate="A" pin="NC" pad="8"/>
<connect gate="A" pin="NC_2" pad="1"/>
<connect gate="A" pin="NC_3" pad="5"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMV2011MA"/>
<attribute name="OC_FARNELL" value="1286953"/>
<attribute name="OC_NEWARK" value="41K3062"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMV2011MF" prefix="U">
<description>High Precision, Rail-to-Rail Output OP-AMP</description>
<gates>
<gate name="A" symbol="LMV2011MF"/>
</gates>
<devices>
<device name="" package="SOT95P285X120-5N">
<connects>
<connect gate="A" pin="V+" pad="5"/>
<connect gate="A" pin="V-" pad="2"/>
<connect gate="A" pin="VIN+" pad="3"/>
<connect gate="A" pin="VIN-" pad="4"/>
<connect gate="A" pin="VOUT" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMV2011MF"/>
<attribute name="OC_FARNELL" value="1312824"/>
<attribute name="OC_NEWARK" value="41K3064"/>
<attribute name="PACKAGE" value="SOT23-5"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMV301MG" prefix="U">
<description>Op Amp w/ Rail-to-Rail output</description>
<gates>
<gate name="A" symbol="LMV301MG"/>
</gates>
<devices>
<device name="" package="SOT65P240X110-5N">
<connects>
<connect gate="A" pin="+IN" pad="1"/>
<connect gate="A" pin="-IN" pad="3"/>
<connect gate="A" pin="OUT" pad="4"/>
<connect gate="A" pin="V+" pad="5"/>
<connect gate="A" pin="V-" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMV301MG"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K3078"/>
<attribute name="PACKAGE" value="SC-70-5"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMV321M5" prefix="U">
<description>Operational Amplifiers</description>
<gates>
<gate name="A" symbol="LMV321M5"/>
</gates>
<devices>
<device name="" package="SOT95P284X119-5N">
<connects>
<connect gate="A" pin="+IN" pad="1"/>
<connect gate="A" pin="-IN" pad="3"/>
<connect gate="A" pin="OUT" pad="4"/>
<connect gate="A" pin="V+" pad="5"/>
<connect gate="A" pin="V-" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMV321M5"/>
<attribute name="OC_FARNELL" value="1197385"/>
<attribute name="OC_NEWARK" value="83F4296"/>
<attribute name="PACKAGE" value="SOT23-5"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMV321M7" prefix="U">
<description>Operational Amplifiers</description>
<gates>
<gate name="A" symbol="LMV321M7"/>
</gates>
<devices>
<device name="" package="SOT65P210X110-5N">
<connects>
<connect gate="A" pin="+IN" pad="1"/>
<connect gate="A" pin="-IN" pad="3"/>
<connect gate="A" pin="OUT" pad="4"/>
<connect gate="A" pin="V+" pad="5"/>
<connect gate="A" pin="V-" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMV321M7"/>
<attribute name="OC_FARNELL" value="1468902"/>
<attribute name="OC_NEWARK" value="41K3082"/>
<attribute name="PACKAGE" value="SC70-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMV324M" prefix="U">
<description>Op Amp</description>
<gates>
<gate name="A" symbol="LMV324M"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="INA+" pad="3"/>
<connect gate="A" pin="INA-" pad="2"/>
<connect gate="A" pin="INB+" pad="5"/>
<connect gate="A" pin="INB-" pad="6"/>
<connect gate="A" pin="INC+" pad="10"/>
<connect gate="A" pin="INC-" pad="9"/>
<connect gate="A" pin="IND+" pad="12"/>
<connect gate="A" pin="IND-" pad="13"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="OUTC" pad="8"/>
<connect gate="A" pin="OUTD" pad="14"/>
<connect gate="A" pin="V+" pad="4"/>
<connect gate="A" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMV324M"/>
<attribute name="OC_FARNELL" value="9306765"/>
<attribute name="OC_NEWARK" value="41K3084"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMV324MT" prefix="U">
<description>OpAmpIC</description>
<gates>
<gate name="A" symbol="LMV324MT"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-14N">
<connects>
<connect gate="A" pin="+INA" pad="3"/>
<connect gate="A" pin="+INB" pad="5"/>
<connect gate="A" pin="+INC" pad="10"/>
<connect gate="A" pin="+IND" pad="12"/>
<connect gate="A" pin="-INA" pad="2"/>
<connect gate="A" pin="-INB" pad="6"/>
<connect gate="A" pin="-INC" pad="9"/>
<connect gate="A" pin="-IND" pad="13"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="OUTC" pad="8"/>
<connect gate="A" pin="OUTD" pad="14"/>
<connect gate="A" pin="V+" pad="4"/>
<connect gate="A" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMV324MT"/>
<attribute name="OC_FARNELL" value="1468903"/>
<attribute name="OC_NEWARK" value="41K3085"/>
<attribute name="PACKAGE" value="TSSOP-14"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMV331M5" prefix="U">
<description>Pack Comparators</description>
<gates>
<gate name="A" symbol="LMV331M5"/>
</gates>
<devices>
<device name="" package="SOT95P284X122-5N">
<connects>
<connect gate="A" pin="+IN" pad="1"/>
<connect gate="A" pin="-IN" pad="3"/>
<connect gate="A" pin="OUT" pad="4"/>
<connect gate="A" pin="V+" pad="5"/>
<connect gate="A" pin="V-" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMV331M5"/>
<attribute name="OC_FARNELL" value="1197386"/>
<attribute name="OC_NEWARK" value="41K3088"/>
<attribute name="PACKAGE" value="SOT23-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMV331M7" prefix="U">
<description>Pack Comparators</description>
<gates>
<gate name="A" symbol="LMV331M7"/>
</gates>
<devices>
<device name="" package="SOT65P210X110-5N">
<connects>
<connect gate="A" pin="+IN" pad="1"/>
<connect gate="A" pin="-IN" pad="3"/>
<connect gate="A" pin="OUT" pad="4"/>
<connect gate="A" pin="V+" pad="5"/>
<connect gate="A" pin="V-" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMV331M7"/>
<attribute name="OC_FARNELL" value="1468945"/>
<attribute name="OC_NEWARK" value="41K3090"/>
<attribute name="PACKAGE" value="SC70-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMV339M" prefix="U">
<description>Tiny Pack Comparators</description>
<gates>
<gate name="A" symbol="LMV339M"/>
</gates>
<devices>
<device name="" package="SOIC127P620X175-14N">
<connects>
<connect gate="A" pin="INA+" pad="5"/>
<connect gate="A" pin="INA-" pad="4"/>
<connect gate="A" pin="INB+" pad="7"/>
<connect gate="A" pin="INB-" pad="6"/>
<connect gate="A" pin="INC+" pad="9"/>
<connect gate="A" pin="INC-" pad="8"/>
<connect gate="A" pin="IND+" pad="11"/>
<connect gate="A" pin="IND-" pad="10"/>
<connect gate="A" pin="OUTA" pad="2"/>
<connect gate="A" pin="OUTB" pad="1"/>
<connect gate="A" pin="OUTC" pad="14"/>
<connect gate="A" pin="OUTD" pad="13"/>
<connect gate="A" pin="V+" pad="3"/>
<connect gate="A" pin="V-" pad="12"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMV339M"/>
<attribute name="OC_FARNELL" value="9306790"/>
<attribute name="OC_NEWARK" value="41K3092"/>
<attribute name="PACKAGE" value="14-SOIC"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMV339MT" prefix="U">
<description>Pack Comparators</description>
<gates>
<gate name="A" symbol="LMV339MT"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-14N">
<connects>
<connect gate="A" pin="+INA" pad="5"/>
<connect gate="A" pin="+INB" pad="7"/>
<connect gate="A" pin="+INC" pad="9"/>
<connect gate="A" pin="+IND" pad="11"/>
<connect gate="A" pin="-INA" pad="4"/>
<connect gate="A" pin="-INB" pad="6"/>
<connect gate="A" pin="-INC" pad="8"/>
<connect gate="A" pin="-IND" pad="10"/>
<connect gate="A" pin="OUTA" pad="2"/>
<connect gate="A" pin="OUTB" pad="1"/>
<connect gate="A" pin="OUTC" pad="14"/>
<connect gate="A" pin="OUTD" pad="13"/>
<connect gate="A" pin="V+" pad="3"/>
<connect gate="A" pin="V-" pad="12"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMV339MT"/>
<attribute name="OC_FARNELL" value="1564706"/>
<attribute name="OC_NEWARK" value="07B5784"/>
<attribute name="PACKAGE" value="TSSOP-14"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMV341MG" prefix="U">
<description>Operational Amplifiers</description>
<gates>
<gate name="A" symbol="LMV341MG"/>
</gates>
<devices>
<device name="" package="SOT65P210X110-6N">
<connects>
<connect gate="A" pin="+IN" pad="1"/>
<connect gate="A" pin="-IN" pad="3"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="OUT" pad="4"/>
<connect gate="A" pin="V+" pad="6"/>
<connect gate="A" pin="~SHDN" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMV341MG"/>
<attribute name="OC_FARNELL" value="1496054"/>
<attribute name="OC_NEWARK" value="41K3096"/>
<attribute name="PACKAGE" value="SC70-6"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMV342MA" prefix="U">
<description>OpAmpIC</description>
<gates>
<gate name="A" symbol="LMV342MA"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="+INA" pad="3"/>
<connect gate="A" pin="+INB" pad="5"/>
<connect gate="A" pin="-INA" pad="2"/>
<connect gate="A" pin="-INB" pad="6"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMV342MA"/>
<attribute name="OC_FARNELL" value="5796398"/>
<attribute name="OC_NEWARK" value="41K3098"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMV342MM" prefix="U">
<description>Operational Amplifiers</description>
<gates>
<gate name="A" symbol="LMV342MM"/>
</gates>
<devices>
<device name="" package="SOP65P490X110-8N">
<connects>
<connect gate="A" pin="+INA" pad="3"/>
<connect gate="A" pin="+INB" pad="5"/>
<connect gate="A" pin="-INA" pad="2"/>
<connect gate="A" pin="-INB" pad="6"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMV342MM"/>
<attribute name="OC_FARNELL" value="9779396"/>
<attribute name="OC_NEWARK" value="41K3100"/>
<attribute name="PACKAGE" value="MSOP-8"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMV344MA" prefix="U">
<description>OpAmpIC</description>
<gates>
<gate name="A" symbol="LMV344MA"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="+INA" pad="3"/>
<connect gate="A" pin="+INB" pad="5"/>
<connect gate="A" pin="+INC" pad="10"/>
<connect gate="A" pin="+IND" pad="12"/>
<connect gate="A" pin="-INA" pad="2"/>
<connect gate="A" pin="-INB" pad="6"/>
<connect gate="A" pin="-INC" pad="9"/>
<connect gate="A" pin="-IND" pad="13"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="OUTC" pad="8"/>
<connect gate="A" pin="OUTD" pad="14"/>
<connect gate="A" pin="V+" pad="4"/>
<connect gate="A" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMV344MA"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K3102"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMV344MT" prefix="U">
<description>Operational Amplifiers</description>
<gates>
<gate name="A" symbol="LMV344MT"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-14N">
<connects>
<connect gate="A" pin="+INA" pad="3"/>
<connect gate="A" pin="+INB" pad="5"/>
<connect gate="A" pin="+INC" pad="10"/>
<connect gate="A" pin="+IND" pad="12"/>
<connect gate="A" pin="-INA" pad="2"/>
<connect gate="A" pin="-INB" pad="6"/>
<connect gate="A" pin="-INC" pad="9"/>
<connect gate="A" pin="-IND" pad="13"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="OUTC" pad="8"/>
<connect gate="A" pin="OUTD" pad="14"/>
<connect gate="A" pin="V+" pad="4"/>
<connect gate="A" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMV344MT"/>
<attribute name="OC_FARNELL" value="1286954"/>
<attribute name="OC_NEWARK" value="41K3104"/>
<attribute name="PACKAGE" value="TSSOP-14"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMV358M" prefix="U">
<description>Operational Amplifiers</description>
<gates>
<gate name="A" symbol="LMV358M"/>
</gates>
<devices>
<device name="" package="SOIC127P620X175-8N">
<connects>
<connect gate="A" pin="INA+" pad="3"/>
<connect gate="A" pin="INA-" pad="2"/>
<connect gate="A" pin="INB+" pad="5"/>
<connect gate="A" pin="INB-" pad="6"/>
<connect gate="A" pin="OUT_A" pad="1"/>
<connect gate="A" pin="OUT_B" pad="7"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMV358M"/>
<attribute name="OC_FARNELL" value="9306730"/>
<attribute name="OC_NEWARK" value="41K3106"/>
<attribute name="PACKAGE" value="8-SOIC"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMV358MM" prefix="U">
<description>Op Amp</description>
<gates>
<gate name="A" symbol="LMV358MM"/>
</gates>
<devices>
<device name="" package="SOP65P490X109-8N">
<connects>
<connect gate="A" pin="INA+" pad="3"/>
<connect gate="A" pin="INA-" pad="2"/>
<connect gate="A" pin="INB+" pad="5"/>
<connect gate="A" pin="INB-" pad="6"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMV358MM"/>
<attribute name="OC_FARNELL" value="1468904"/>
<attribute name="OC_NEWARK" value="83F4304"/>
<attribute name="PACKAGE" value="MSOP-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMV393M" prefix="U">
<description>Pack Comparators</description>
<gates>
<gate name="A" symbol="LMV393M"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="IN_A+" pad="3"/>
<connect gate="A" pin="IN_A-" pad="2"/>
<connect gate="A" pin="IN_B+" pad="5"/>
<connect gate="A" pin="IN_B-" pad="6"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMV393M"/>
<attribute name="OC_FARNELL" value="9306773"/>
<attribute name="OC_NEWARK" value="83F4305"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMV393MM" prefix="U">
<description>Pack Comparators</description>
<gates>
<gate name="A" symbol="LMV393MM"/>
</gates>
<devices>
<device name="" package="SOP65P490X109-8N">
<connects>
<connect gate="A" pin="INA+" pad="3"/>
<connect gate="A" pin="INA-" pad="2"/>
<connect gate="A" pin="INB+" pad="5"/>
<connect gate="A" pin="INB-" pad="6"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMV393MM"/>
<attribute name="OC_FARNELL" value="1474210"/>
<attribute name="OC_NEWARK" value="83F4306"/>
<attribute name="PACKAGE" value="MSOP-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMV431ACM5" prefix="U">
<description>Regulator</description>
<gates>
<gate name="A" symbol="LMV431ACM5"/>
</gates>
<devices>
<device name="" package="SOT95P284X122-5N">
<connects>
<connect gate="A" pin="ANODE" pad="5"/>
<connect gate="A" pin="CATHODE" pad="3"/>
<connect gate="A" pin="NC" pad="2"/>
<connect gate="A" pin="NC_2" pad="1"/>
<connect gate="A" pin="REF" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMV431ACM5"/>
<attribute name="OC_FARNELL" value="9778373"/>
<attribute name="OC_NEWARK" value="41K3116"/>
<attribute name="PACKAGE" value="SOT23-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMV431BIMF" prefix="U">
<description>Regulators</description>
<gates>
<gate name="A" symbol="LMV431BIMF"/>
</gates>
<devices>
<device name="" package="SOT95P251X112-3N">
<connects>
<connect gate="A" pin="ANODE" pad="3"/>
<connect gate="A" pin="CATHODE" pad="2"/>
<connect gate="A" pin="REF" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMV431BIMF"/>
<attribute name="OC_FARNELL" value="1798372"/>
<attribute name="OC_NEWARK" value="73R9725"/>
<attribute name="PACKAGE" value="SOT23-3"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMV431CM5" prefix="U">
<description>Regulators</description>
<gates>
<gate name="A" symbol="LMV431CM5"/>
</gates>
<devices>
<device name="" package="SOT95P284X122-5N">
<connects>
<connect gate="A" pin="ANODE" pad="5"/>
<connect gate="A" pin="CATHODE" pad="3"/>
<connect gate="A" pin="NC" pad="2"/>
<connect gate="A" pin="NC_2" pad="1"/>
<connect gate="A" pin="REF" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMV431CM5"/>
<attribute name="OC_FARNELL" value="9778381"/>
<attribute name="OC_NEWARK" value="74C3745"/>
<attribute name="PACKAGE" value="SOT23-5"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMV431IM5" prefix="U">
<description>Regulator</description>
<gates>
<gate name="A" symbol="LMV431IM5"/>
</gates>
<devices>
<device name="" package="SOT95P284X122-5N">
<connects>
<connect gate="A" pin="ANODE" pad="5"/>
<connect gate="A" pin="CATHODE" pad="3"/>
<connect gate="A" pin="NC" pad="2"/>
<connect gate="A" pin="NC_2" pad="1"/>
<connect gate="A" pin="REF" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMV431IM5"/>
<attribute name="OC_FARNELL" value="9778390"/>
<attribute name="OC_NEWARK" value="90B2086"/>
<attribute name="PACKAGE" value="SOT23-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMV551MF" prefix="U">
<description>Amplifiers</description>
<gates>
<gate name="A" symbol="LMV551MF"/>
</gates>
<devices>
<device name="" package="SOT95P284X119-5N">
<connects>
<connect gate="A" pin="+IN" pad="1"/>
<connect gate="A" pin="-IN" pad="3"/>
<connect gate="A" pin="OUT" pad="4"/>
<connect gate="A" pin="V+" pad="5"/>
<connect gate="A" pin="V-" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMV551MF"/>
<attribute name="OC_FARNELL" value="1663004"/>
<attribute name="OC_NEWARK" value="34P4747"/>
<attribute name="PACKAGE" value="SOT23-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMV551MG" prefix="U">
<description>Amplifiers</description>
<gates>
<gate name="A" symbol="LMV551MG"/>
</gates>
<devices>
<device name="" package="SOT65P210X110-5N">
<connects>
<connect gate="A" pin="+IN" pad="1"/>
<connect gate="A" pin="-IN" pad="3"/>
<connect gate="A" pin="OUT" pad="4"/>
<connect gate="A" pin="V+" pad="5"/>
<connect gate="A" pin="V-" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMV551MG"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="64M6916"/>
<attribute name="PACKAGE" value="SC70-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMV552MM" prefix="U">
<description>Micropower RRO Amplifiers</description>
<gates>
<gate name="A" symbol="LMV552MM"/>
</gates>
<devices>
<device name="" package="SOP65P490X110-8N">
<connects>
<connect gate="A" pin="+INA" pad="3"/>
<connect gate="A" pin="+INB" pad="5"/>
<connect gate="A" pin="-INA" pad="2"/>
<connect gate="A" pin="-INB" pad="6"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMV552MM"/>
<attribute name="OC_FARNELL" value="1342346"/>
<attribute name="OC_NEWARK" value="42M2046"/>
<attribute name="PACKAGE" value="MSOP-8"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMV554MT" prefix="U">
<description>Amplifiers</description>
<gates>
<gate name="A" symbol="LMV554MT"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-14N">
<connects>
<connect gate="A" pin="INA+" pad="3"/>
<connect gate="A" pin="INA-" pad="2"/>
<connect gate="A" pin="INB+" pad="5"/>
<connect gate="A" pin="INB-" pad="6"/>
<connect gate="A" pin="INC+" pad="10"/>
<connect gate="A" pin="INC-" pad="9"/>
<connect gate="A" pin="IND+" pad="12"/>
<connect gate="A" pin="IND-" pad="13"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="OUTC" pad="8"/>
<connect gate="A" pin="OUTD" pad="14"/>
<connect gate="A" pin="V+" pad="4"/>
<connect gate="A" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMV554MT"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="54M4634"/>
<attribute name="PACKAGE" value="TSSOP-14"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMV651MF" prefix="U">
<description>Low Power Amplifiers</description>
<gates>
<gate name="A" symbol="LMV651MF"/>
</gates>
<devices>
<device name="" package="SOT95P285X120-5N">
<connects>
<connect gate="A" pin="IN+" pad="1"/>
<connect gate="A" pin="IN-" pad="3"/>
<connect gate="A" pin="OUT" pad="4"/>
<connect gate="A" pin="V+" pad="5"/>
<connect gate="A" pin="V-" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMV651MF"/>
<attribute name="OC_FARNELL" value="1663006"/>
<attribute name="OC_NEWARK" value="11N9165"/>
<attribute name="PACKAGE" value="SOT-23-5"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMV651MG" prefix="U">
<description>Low Power Amplifiers</description>
<gates>
<gate name="A" symbol="LMV651MG"/>
</gates>
<devices>
<device name="" package="SOT65P240X110-5N">
<connects>
<connect gate="A" pin="+IN" pad="1"/>
<connect gate="A" pin="-IN" pad="3"/>
<connect gate="A" pin="OUT" pad="4"/>
<connect gate="A" pin="V+" pad="5"/>
<connect gate="A" pin="V-" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMV651MG"/>
<attribute name="OC_FARNELL" value="1312610"/>
<attribute name="OC_NEWARK" value="99K2287"/>
<attribute name="PACKAGE" value="SC70-5"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMV652MM" prefix="U">
<description>Low Power Amplifiers</description>
<gates>
<gate name="A" symbol="LMV652MM"/>
</gates>
<devices>
<device name="" package="SOP65P490X110-8N">
<connects>
<connect gate="A" pin="INA+" pad="3"/>
<connect gate="A" pin="INA-" pad="2"/>
<connect gate="A" pin="INB+" pad="5"/>
<connect gate="A" pin="INB-" pad="6"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMV652MM"/>
<attribute name="OC_FARNELL" value="1342331"/>
<attribute name="OC_NEWARK" value="32M0962"/>
<attribute name="PACKAGE" value="MSOP-8"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMV654MT" prefix="U">
<description>Low Power Amplifiers</description>
<gates>
<gate name="A" symbol="LMV654MT"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-14N">
<connects>
<connect gate="A" pin="+INA" pad="3"/>
<connect gate="A" pin="+INB" pad="5"/>
<connect gate="A" pin="+INC" pad="10"/>
<connect gate="A" pin="+IND" pad="12"/>
<connect gate="A" pin="-INA" pad="2"/>
<connect gate="A" pin="-INB" pad="6"/>
<connect gate="A" pin="-INC" pad="9"/>
<connect gate="A" pin="-IND" pad="13"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="OUTC" pad="8"/>
<connect gate="A" pin="OUTD" pad="14"/>
<connect gate="A" pin="V+" pad="4"/>
<connect gate="A" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMV654MT"/>
<attribute name="OC_FARNELL" value="1320979"/>
<attribute name="OC_NEWARK" value="13M1680"/>
<attribute name="PACKAGE" value="TSSOP-14"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMV710M5" prefix="U">
<description>Low Power, RRIO Operational Amplifiers</description>
<gates>
<gate name="A" symbol="LMV710M5"/>
</gates>
<devices>
<device name="" package="SOT95P285X120-5N">
<connects>
<connect gate="A" pin="IN+" pad="3"/>
<connect gate="A" pin="IN-" pad="4"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="A" pin="V+" pad="5"/>
<connect gate="A" pin="V-" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMV710M5"/>
<attribute name="OC_FARNELL" value="9778861"/>
<attribute name="OC_NEWARK" value="41K3135"/>
<attribute name="PACKAGE" value="SOT23-5"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMV712MM" prefix="U">
<description>Operational Amplifier</description>
<gates>
<gate name="A" symbol="LMV712MM"/>
</gates>
<devices>
<device name="" package="SOP50P490X110-10N">
<connects>
<connect gate="A" pin="INA+" pad="3"/>
<connect gate="A" pin="INA-" pad="2"/>
<connect gate="A" pin="INB+" pad="7"/>
<connect gate="A" pin="INB-" pad="8"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="9"/>
<connect gate="A" pin="SDA" pad="5"/>
<connect gate="A" pin="SDB" pad="6"/>
<connect gate="A" pin="V+" pad="10"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMV712MM"/>
<attribute name="OC_FARNELL" value="1312827"/>
<attribute name="OC_NEWARK" value="34C6458"/>
<attribute name="PACKAGE" value="10-MSOP"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMV716MM" prefix="U">
<description>Op Amp</description>
<gates>
<gate name="A" symbol="LMV716MM"/>
</gates>
<devices>
<device name="" package="SOP65P490X109-8N">
<connects>
<connect gate="A" pin="INA+" pad="3"/>
<connect gate="A" pin="INA-" pad="2"/>
<connect gate="A" pin="INB+" pad="5"/>
<connect gate="A" pin="INB-" pad="6"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMV716MM"/>
<attribute name="OC_FARNELL" value="99K2291"/>
<attribute name="OC_NEWARK" value="1312829"/>
<attribute name="PACKAGE" value="MSOP-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMV7219M5" prefix="U">
<description>Comparator</description>
<gates>
<gate name="A" symbol="LMV7219M5"/>
</gates>
<devices>
<device name="" package="SOT95P284X122-5N">
<connects>
<connect gate="A" pin="NEG" pad="4"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="A" pin="POS" pad="3"/>
<connect gate="A" pin="V+" pad="5"/>
<connect gate="A" pin="V-" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMV7219M5"/>
<attribute name="OC_FARNELL" value="9778764"/>
<attribute name="OC_NEWARK" value="35K4600"/>
<attribute name="PACKAGE" value="SOT23-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMV7219M7" prefix="U">
<description>2.7V to 5V Comparator</description>
<gates>
<gate name="A" symbol="LMV7219M7"/>
</gates>
<devices>
<device name="" package="SOT65P240X110-5N">
<connects>
<connect gate="A" pin="NEG" pad="4"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="A" pin="POS" pad="3"/>
<connect gate="A" pin="V+" pad="5"/>
<connect gate="A" pin="V-" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMV7219M7"/>
<attribute name="OC_FARNELL" value="1312830"/>
<attribute name="OC_NEWARK" value="41K3151"/>
<attribute name="PACKAGE" value="SC-70-5"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMV721M5" prefix="U">
<description>Operational Amplifier</description>
<gates>
<gate name="A" symbol="LMV721M5"/>
</gates>
<devices>
<device name="" package="SOT95P284X122-5N">
<connects>
<connect gate="A" pin="V+" pad="5"/>
<connect gate="A" pin="V-" pad="2"/>
<connect gate="A" pin="VIN+" pad="3"/>
<connect gate="A" pin="VIN-" pad="4"/>
<connect gate="A" pin="VOUT" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMV721M5"/>
<attribute name="OC_FARNELL" value="9778497"/>
<attribute name="OC_NEWARK" value="41K3145"/>
<attribute name="PACKAGE" value="SOT23-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMV721M7" prefix="U">
<description>Operational Amplifier</description>
<gates>
<gate name="A" symbol="LMV721M7"/>
</gates>
<devices>
<device name="" package="SOT65P210X110-5N">
<connects>
<connect gate="A" pin="V+" pad="5"/>
<connect gate="A" pin="V-" pad="2"/>
<connect gate="A" pin="VIN+" pad="3"/>
<connect gate="A" pin="VIN-" pad="4"/>
<connect gate="A" pin="VOUT" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMV721M7"/>
<attribute name="OC_FARNELL" value="9778500"/>
<attribute name="OC_NEWARK" value="74C3758"/>
<attribute name="PACKAGE" value="SC70-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMV722M" prefix="U">
<description>Operational Amplifiers</description>
<gates>
<gate name="A" symbol="LMV722M"/>
</gates>
<devices>
<device name="" package="SOIC127P620X175-8N">
<connects>
<connect gate="A" pin="+INA" pad="3"/>
<connect gate="A" pin="+INB" pad="5"/>
<connect gate="A" pin="-INA" pad="2"/>
<connect gate="A" pin="-INB" pad="6"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMV722M"/>
<attribute name="OC_FARNELL" value="9486321"/>
<attribute name="OC_NEWARK" value="41K3156"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMV722MM" prefix="U">
<description>Op Amp</description>
<gates>
<gate name="A" symbol="LMV722MM"/>
</gates>
<devices>
<device name="" package="SOP65P490X109-8N">
<connects>
<connect gate="A" pin="+INA" pad="3"/>
<connect gate="A" pin="+INB" pad="5"/>
<connect gate="A" pin="-INA" pad="2"/>
<connect gate="A" pin="-INB" pad="6"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMV722MM"/>
<attribute name="OC_FARNELL" value="1276328"/>
<attribute name="OC_NEWARK" value="74C3767"/>
<attribute name="PACKAGE" value="MSOP-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMV7235M5" prefix="U">
<description>Ultra Low Power, Low Voltage, Rail-to-Rail Input Comparator</description>
<gates>
<gate name="A" symbol="LMV7235M5"/>
</gates>
<devices>
<device name="" package="SOT95P285X120-5N">
<connects>
<connect gate="A" pin="NEG" pad="4"/>
<connect gate="A" pin="POS" pad="3"/>
<connect gate="A" pin="V+" pad="5"/>
<connect gate="A" pin="V-" pad="2"/>
<connect gate="A" pin="VOUT" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMV7235M5"/>
<attribute name="OC_FARNELL" value="9778918"/>
<attribute name="OC_NEWARK" value="41K3159"/>
<attribute name="PACKAGE" value="SOT23-5"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMV7235M7" prefix="U">
<description>Comparator</description>
<gates>
<gate name="A" symbol="LMV7235M7"/>
</gates>
<devices>
<device name="" package="SOT65P210X110-5N">
<connects>
<connect gate="A" pin="NEG" pad="4"/>
<connect gate="A" pin="POS" pad="3"/>
<connect gate="A" pin="V+" pad="5"/>
<connect gate="A" pin="V-" pad="2"/>
<connect gate="A" pin="VOUT" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMV7235M7"/>
<attribute name="OC_FARNELL" value="1312831"/>
<attribute name="OC_NEWARK" value="41K3161"/>
<attribute name="PACKAGE" value="SC70-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMV7239M5" prefix="U">
<description>Comparator</description>
<gates>
<gate name="A" symbol="LMV7239M5"/>
</gates>
<devices>
<device name="" package="SOT95P284X119-5N">
<connects>
<connect gate="A" pin="NEG" pad="4"/>
<connect gate="A" pin="POS" pad="3"/>
<connect gate="A" pin="V+" pad="5"/>
<connect gate="A" pin="V-" pad="2"/>
<connect gate="A" pin="VOUT" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMV7239M5"/>
<attribute name="OC_FARNELL" value="9778926"/>
<attribute name="OC_NEWARK" value="24C8926"/>
<attribute name="PACKAGE" value="SOT23-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMV7239M7" prefix="U">
<description>Ultra Low Power, Low Voltage, Rail-to-Rail Input Comparator</description>
<gates>
<gate name="A" symbol="LMV7239M7"/>
</gates>
<devices>
<device name="" package="SOT65P240X110-5N">
<connects>
<connect gate="A" pin="NEG" pad="4"/>
<connect gate="A" pin="POS" pad="3"/>
<connect gate="A" pin="V+" pad="5"/>
<connect gate="A" pin="V-" pad="2"/>
<connect gate="A" pin="VOUT" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMV7239M7"/>
<attribute name="OC_FARNELL" value="1312833"/>
<attribute name="OC_NEWARK" value="41K3165"/>
<attribute name="PACKAGE" value="SC-70-5"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMV7271MF" prefix="U">
<description>Low Power Comparators</description>
<gates>
<gate name="A" symbol="LMV7271MF"/>
</gates>
<devices>
<device name="" package="SOT95P285X120-5N">
<connects>
<connect gate="A" pin="+IN" pad="1"/>
<connect gate="A" pin="-IN" pad="3"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="OUT" pad="4"/>
<connect gate="A" pin="V+" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMV7271MF"/>
<attribute name="OC_FARNELL" value="9779795"/>
<attribute name="OC_NEWARK" value="41K3167"/>
<attribute name="PACKAGE" value="SOT-23-5"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMV7271MG" prefix="U">
<description>Comparators</description>
<gates>
<gate name="A" symbol="LMV7271MG"/>
</gates>
<devices>
<device name="" package="SOT65P210X110-5N">
<connects>
<connect gate="A" pin="+IN" pad="1"/>
<connect gate="A" pin="-IN" pad="3"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="V+" pad="5"/>
<connect gate="A" pin="VOUT" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMV7271MG"/>
<attribute name="OC_FARNELL" value="1312834"/>
<attribute name="OC_NEWARK" value="41K3169"/>
<attribute name="PACKAGE" value="SC70-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMV7275MF" prefix="U">
<description>Comparators</description>
<gates>
<gate name="A" symbol="LMV7275MF"/>
</gates>
<devices>
<device name="" package="SOT95P284X119-5N">
<connects>
<connect gate="A" pin="+IN" pad="1"/>
<connect gate="A" pin="-IN" pad="3"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="V+" pad="5"/>
<connect gate="A" pin="VOUT" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMV7275MF"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K3173"/>
<attribute name="PACKAGE" value="SOT23-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMV7275MG" prefix="U">
<description>Comparators</description>
<gates>
<gate name="A" symbol="LMV7275MG"/>
</gates>
<devices>
<device name="" package="SOT65P210X110-5N">
<connects>
<connect gate="A" pin="+IN" pad="1"/>
<connect gate="A" pin="-IN" pad="3"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="V+" pad="5"/>
<connect gate="A" pin="VOUT" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMV7275MG"/>
<attribute name="OC_FARNELL" value="1559359"/>
<attribute name="OC_NEWARK" value="41K3175"/>
<attribute name="PACKAGE" value="SC70-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMV7291MG" prefix="U">
<description>Low Power Comparator</description>
<gates>
<gate name="A" symbol="LMV7291MG"/>
</gates>
<devices>
<device name="" package="SOT65P240X110-5N">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="4"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="V+" pad="5"/>
<connect gate="A" pin="VOUT" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMV7291MG"/>
<attribute name="OC_FARNELL" value="8187649"/>
<attribute name="OC_NEWARK" value="41K3177"/>
<attribute name="PACKAGE" value="SC-70-5"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMV751M5" prefix="U">
<description>Op Amp</description>
<gates>
<gate name="A" symbol="LMV751M5"/>
</gates>
<devices>
<device name="" package="SOT95P284X122-5N">
<connects>
<connect gate="A" pin="V+" pad="5"/>
<connect gate="A" pin="V-" pad="2"/>
<connect gate="A" pin="VIN+" pad="3"/>
<connect gate="A" pin="VIN-" pad="4"/>
<connect gate="A" pin="VOUT" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMV751M5"/>
<attribute name="OC_FARNELL" value="1312611"/>
<attribute name="OC_NEWARK" value="41K3179"/>
<attribute name="PACKAGE" value="SOT23-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMV761MA" prefix="U">
<description>Low Voltage, Precision Comparator</description>
<gates>
<gate name="A" symbol="LMV761MA"/>
</gates>
<devices>
<device name="" package="SOIC127P620X175-8N">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="NC" pad="8"/>
<connect gate="A" pin="NC_2" pad="1"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
<connect gate="A" pin="~SD" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMV761MA"/>
<attribute name="OC_FARNELL" value="9490590"/>
<attribute name="OC_NEWARK" value="41K3181"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMV761MF" prefix="U">
<description>Low Voltage, Precision Comparator</description>
<gates>
<gate name="A" symbol="LMV761MF"/>
</gates>
<devices>
<device name="" package="SOT95P284X120-6N">
<connects>
<connect gate="A" pin="IN+" pad="1"/>
<connect gate="A" pin="IN-" pad="3"/>
<connect gate="A" pin="OUT" pad="4"/>
<connect gate="A" pin="V+" pad="6"/>
<connect gate="A" pin="V-" pad="2"/>
<connect gate="A" pin="~SD" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMV761MF"/>
<attribute name="OC_FARNELL" value="9779388"/>
<attribute name="OC_NEWARK" value="74C3787"/>
<attribute name="PACKAGE" value="SOT23-6"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMV762MA" prefix="U">
<description>Precision Comparator</description>
<gates>
<gate name="A" symbol="LMV762MA"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="IN_A+" pad="3"/>
<connect gate="A" pin="IN_A-" pad="2"/>
<connect gate="A" pin="IN_B+" pad="5"/>
<connect gate="A" pin="IN_B-" pad="6"/>
<connect gate="A" pin="OUT_A" pad="1"/>
<connect gate="A" pin="OUT_B" pad="7"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMV762MA"/>
<attribute name="OC_FARNELL" value="9490582"/>
<attribute name="OC_NEWARK" value="41K3185"/>
<attribute name="PACKAGE" value="8-SOIC"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMV762MM" prefix="U">
<description>Low Voltage, Precision Comparator</description>
<gates>
<gate name="A" symbol="LMV762MM"/>
</gates>
<devices>
<device name="" package="SOP65P490X110-8N">
<connects>
<connect gate="A" pin="INA+" pad="3"/>
<connect gate="A" pin="INA-" pad="2"/>
<connect gate="A" pin="INB+" pad="5"/>
<connect gate="A" pin="INB-" pad="6"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMV762MM"/>
<attribute name="OC_FARNELL" value="9779370"/>
<attribute name="OC_NEWARK" value="41K3187"/>
<attribute name="PACKAGE" value="MSOP-8"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMV771MG" prefix="U">
<description>Operational Amplifiers</description>
<gates>
<gate name="A" symbol="LMV771MG"/>
</gates>
<devices>
<device name="" package="SOT65P210X110-5N">
<connects>
<connect gate="A" pin="+IN" pad="1"/>
<connect gate="A" pin="-IN" pad="3"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="V+" pad="5"/>
<connect gate="A" pin="VOUT" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMV771MG"/>
<attribute name="OC_FARNELL" value="1312612"/>
<attribute name="OC_NEWARK" value="41K3189"/>
<attribute name="PACKAGE" value="SC70-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMV772MA" prefix="U">
<description>Operational Amplifiers</description>
<gates>
<gate name="A" symbol="LMV772MA"/>
</gates>
<devices>
<device name="" package="SOIC127P620X175-8N">
<connects>
<connect gate="A" pin="+INA" pad="3"/>
<connect gate="A" pin="+INB" pad="5"/>
<connect gate="A" pin="-INA" pad="2"/>
<connect gate="A" pin="-INB" pad="6"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMV772MA"/>
<attribute name="OC_FARNELL" value="8187657"/>
<attribute name="OC_NEWARK" value="41K3191"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMV772MM" prefix="U">
<description>Operational Amplifiers</description>
<gates>
<gate name="A" symbol="LMV772MM"/>
</gates>
<devices>
<device name="" package="SOP65P490X110-8N">
<connects>
<connect gate="A" pin="INA+" pad="3"/>
<connect gate="A" pin="INA-" pad="2"/>
<connect gate="A" pin="INB+" pad="5"/>
<connect gate="A" pin="INB-" pad="6"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMV772MM"/>
<attribute name="OC_FARNELL" value="8187665"/>
<attribute name="OC_NEWARK" value="41K3193"/>
<attribute name="PACKAGE" value="MSOP-8"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMV774MT" prefix="U">
<description>Operational Amplifiers</description>
<gates>
<gate name="A" symbol="LMV774MT"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-14N">
<connects>
<connect gate="A" pin="+INA" pad="3"/>
<connect gate="A" pin="+INB" pad="5"/>
<connect gate="A" pin="+INC" pad="10"/>
<connect gate="A" pin="+IND" pad="12"/>
<connect gate="A" pin="-INA" pad="2"/>
<connect gate="A" pin="-INB" pad="6"/>
<connect gate="A" pin="-INC" pad="9"/>
<connect gate="A" pin="-IND" pad="13"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="OUTC" pad="8"/>
<connect gate="A" pin="OUTD" pad="14"/>
<connect gate="A" pin="V+" pad="4"/>
<connect gate="A" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMV774MT"/>
<attribute name="OC_FARNELL" value="8187673"/>
<attribute name="OC_NEWARK" value="41K3195"/>
<attribute name="PACKAGE" value="TSSOP-14"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMV791MK" prefix="U">
<description>Op Amp</description>
<gates>
<gate name="A" symbol="LMV791MK"/>
</gates>
<devices>
<device name="" package="SOT95P284X100-6N">
<connects>
<connect gate="A" pin="EN" pad="5"/>
<connect gate="A" pin="IN+" pad="3"/>
<connect gate="A" pin="IN-" pad="4"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="A" pin="V+" pad="6"/>
<connect gate="A" pin="V-" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMV791MK"/>
<attribute name="OC_FARNELL" value="1312614"/>
<attribute name="OC_NEWARK" value="69K2319"/>
<attribute name="PACKAGE" value="SOT23-6"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMV792MM" prefix="U">
<description>OpAmpIC</description>
<gates>
<gate name="A" symbol="LMV792MM"/>
</gates>
<devices>
<device name="" package="SOP50P490X109-10N">
<connects>
<connect gate="A" pin="ENA" pad="5"/>
<connect gate="A" pin="ENB" pad="6"/>
<connect gate="A" pin="INA+" pad="3"/>
<connect gate="A" pin="INA-" pad="2"/>
<connect gate="A" pin="INB+" pad="7"/>
<connect gate="A" pin="INB-" pad="8"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="9"/>
<connect gate="A" pin="V+" pad="10"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMV792MM"/>
<attribute name="OC_FARNELL" value="1312615"/>
<attribute name="OC_NEWARK" value="79K7735"/>
<attribute name="PACKAGE" value="MSOP-10"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMV793MA" prefix="U">
<description>OpAmpIC</description>
<gates>
<gate name="A" symbol="LMV793MA"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="NC" pad="8"/>
<connect gate="A" pin="NC_2" pad="5"/>
<connect gate="A" pin="NC_3" pad="1"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMV793MA"/>
<attribute name="OC_FARNELL" value="1342339"/>
<attribute name="OC_NEWARK" value="46M5457"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMV793MF" prefix="U">
<description>Decompensated Operational Amplifier</description>
<gates>
<gate name="A" symbol="LMV793MF"/>
</gates>
<devices>
<device name="" package="SOT95P285X120-5N">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="4"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="A" pin="V+" pad="5"/>
<connect gate="A" pin="V-" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMV793MF"/>
<attribute name="OC_FARNELL" value="1342338"/>
<attribute name="OC_NEWARK" value="46M5459"/>
<attribute name="PACKAGE" value="SOT-23-5"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMV794MA" prefix="U">
<description>OpAmpIC</description>
<gates>
<gate name="A" symbol="LMV794MA"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="NC" pad="8"/>
<connect gate="A" pin="NC_2" pad="5"/>
<connect gate="A" pin="NC_3" pad="1"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMV794MA"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="53M0342"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMV794MM" prefix="U">
<description>OpAmpIC</description>
<gates>
<gate name="A" symbol="LMV794MM"/>
</gates>
<devices>
<device name="" package="SOP65P490X109-8N">
<connects>
<connect gate="A" pin="INA+" pad="3"/>
<connect gate="A" pin="INA-" pad="2"/>
<connect gate="A" pin="INB+" pad="5"/>
<connect gate="A" pin="INB-" pad="6"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMV794MM"/>
<attribute name="OC_FARNELL" value="1433176"/>
<attribute name="OC_NEWARK" value="54M4637"/>
<attribute name="PACKAGE" value="MSOP-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMV796MF" prefix="U">
<description>OP AMP</description>
<gates>
<gate name="A" symbol="LMV796MF"/>
</gates>
<devices>
<device name="" package="SOT95P285X120-5N">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="4"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="A" pin="V+" pad="5"/>
<connect gate="A" pin="V-" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMV796MF"/>
<attribute name="OC_FARNELL" value="1312616"/>
<attribute name="OC_NEWARK" value="99K2296"/>
<attribute name="PACKAGE" value="SOT-23-5"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMV797MM" prefix="U">
<description>OpAmpIC</description>
<gates>
<gate name="A" symbol="LMV797MM"/>
</gates>
<devices>
<device name="" package="SOP65P490X109-8N">
<connects>
<connect gate="A" pin="INA+" pad="3"/>
<connect gate="A" pin="INA-" pad="2"/>
<connect gate="A" pin="INB+" pad="5"/>
<connect gate="A" pin="INB-" pad="6"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMV797MM"/>
<attribute name="OC_FARNELL" value="1312617"/>
<attribute name="OC_NEWARK" value="99K2300"/>
<attribute name="PACKAGE" value="MSOP-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMV821M5" prefix="U">
<description>Op Amps</description>
<gates>
<gate name="A" symbol="LMV821M5"/>
</gates>
<devices>
<device name="" package="SOT95P284X122-5N">
<connects>
<connect gate="A" pin="+IN" pad="1"/>
<connect gate="A" pin="-IN" pad="3"/>
<connect gate="A" pin="OUT" pad="4"/>
<connect gate="A" pin="V+" pad="5"/>
<connect gate="A" pin="V-" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMV821M5"/>
<attribute name="OC_FARNELL" value="1468906"/>
<attribute name="OC_NEWARK" value="41K3197"/>
<attribute name="PACKAGE" value="SOT23-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMV821M7" prefix="U">
<description>Op Amps</description>
<gates>
<gate name="A" symbol="LMV821M7"/>
</gates>
<devices>
<device name="" package="SOT65P210X110-5N">
<connects>
<connect gate="A" pin="+IN" pad="1"/>
<connect gate="A" pin="-IN" pad="3"/>
<connect gate="A" pin="OUT" pad="4"/>
<connect gate="A" pin="V+" pad="5"/>
<connect gate="A" pin="V-" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMV821M7"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K3199"/>
<attribute name="PACKAGE" value="SC70-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMV822M" prefix="U">
<description>Op Amps</description>
<gates>
<gate name="A" symbol="LMV822M"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="+IN_A" pad="3"/>
<connect gate="A" pin="+IN_B" pad="5"/>
<connect gate="A" pin="-IN_A" pad="2"/>
<connect gate="A" pin="-IN_B" pad="6"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMV822M"/>
<attribute name="OC_FARNELL" value="1685318"/>
<attribute name="OC_NEWARK" value="41K3201"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMV822MM" prefix="U">
<description>Op Amps</description>
<gates>
<gate name="A" symbol="LMV822MM"/>
</gates>
<devices>
<device name="" package="SOP65P490X109-8N">
<connects>
<connect gate="A" pin="INA+" pad="3"/>
<connect gate="A" pin="INA-" pad="2"/>
<connect gate="A" pin="INB+" pad="5"/>
<connect gate="A" pin="INB-" pad="6"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMV822MM"/>
<attribute name="OC_FARNELL" value="1685319"/>
<attribute name="OC_NEWARK" value="41K3202"/>
<attribute name="PACKAGE" value="MSOP-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMV824M" prefix="U">
<description>Op Amps</description>
<gates>
<gate name="A" symbol="LMV824M"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="+INA" pad="3"/>
<connect gate="A" pin="+INB" pad="5"/>
<connect gate="A" pin="+INC" pad="10"/>
<connect gate="A" pin="+IND" pad="12"/>
<connect gate="A" pin="-INA" pad="2"/>
<connect gate="A" pin="-INB" pad="6"/>
<connect gate="A" pin="-INC" pad="9"/>
<connect gate="A" pin="-IND" pad="13"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="OUTC" pad="8"/>
<connect gate="A" pin="OUTD" pad="14"/>
<connect gate="A" pin="V+" pad="4"/>
<connect gate="A" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMV824M"/>
<attribute name="OC_FARNELL" value="1564623"/>
<attribute name="OC_NEWARK" value="41K3205"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMV824MT" prefix="U">
<description>Op Amps</description>
<gates>
<gate name="A" symbol="LMV824MT"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-14N">
<connects>
<connect gate="A" pin="INA+" pad="3"/>
<connect gate="A" pin="INA-" pad="2"/>
<connect gate="A" pin="INB+" pad="5"/>
<connect gate="A" pin="INB-" pad="6"/>
<connect gate="A" pin="INC+" pad="10"/>
<connect gate="A" pin="INC-" pad="9"/>
<connect gate="A" pin="IND+" pad="12"/>
<connect gate="A" pin="IND-" pad="13"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="OUTC" pad="8"/>
<connect gate="A" pin="OUTD" pad="14"/>
<connect gate="A" pin="V+" pad="4"/>
<connect gate="A" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMV824MT"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K3206"/>
<attribute name="PACKAGE" value="TSSOP-14"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMV831MG" prefix="U">
<description>EMI Hardened Operational amplifier</description>
<gates>
<gate name="A" symbol="LMV831MG"/>
</gates>
<devices>
<device name="" package="SOT65P240X110-5N">
<connects>
<connect gate="A" pin="IN+" pad="1"/>
<connect gate="A" pin="IN-" pad="3"/>
<connect gate="A" pin="OUT" pad="4"/>
<connect gate="A" pin="V+" pad="5"/>
<connect gate="A" pin="V-" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMV831MG"/>
<attribute name="OC_FARNELL" value="1667426"/>
<attribute name="OC_NEWARK" value="15P1957"/>
<attribute name="PACKAGE" value="SC-70-5"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMV832MM" prefix="U">
<description>EMI Hardened Operational amplifier</description>
<gates>
<gate name="A" symbol="LMV832MM"/>
</gates>
<devices>
<device name="" package="SOP65P490X110-8N">
<connects>
<connect gate="A" pin="INA+" pad="3"/>
<connect gate="A" pin="INA-" pad="2"/>
<connect gate="A" pin="INB+" pad="5"/>
<connect gate="A" pin="INB-" pad="6"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMV832MM"/>
<attribute name="OC_FARNELL" value="1667429"/>
<attribute name="OC_NEWARK" value="15P1959"/>
<attribute name="PACKAGE" value="MSOP-8"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMV834MT" prefix="U">
<description>EMI Hardened Operational amplifier</description>
<gates>
<gate name="A" symbol="LMV834MT"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-14N">
<connects>
<connect gate="A" pin="INA+" pad="3"/>
<connect gate="A" pin="INA-" pad="2"/>
<connect gate="A" pin="INB+" pad="5"/>
<connect gate="A" pin="INB-" pad="6"/>
<connect gate="A" pin="INC+" pad="10"/>
<connect gate="A" pin="INC-" pad="9"/>
<connect gate="A" pin="IND+" pad="12"/>
<connect gate="A" pin="IND-" pad="13"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="OUTC" pad="8"/>
<connect gate="A" pin="OUTD" pad="14"/>
<connect gate="A" pin="V+" pad="4"/>
<connect gate="A" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMV834MT"/>
<attribute name="OC_FARNELL" value="1679690"/>
<attribute name="OC_NEWARK" value="56P4148"/>
<attribute name="PACKAGE" value="TSSOP-14"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMV841MG" prefix="U">
<description>Wide Supply Range Operational amp</description>
<gates>
<gate name="A" symbol="LMV841MG"/>
</gates>
<devices>
<device name="" package="SOT65P240X110-5N">
<connects>
<connect gate="A" pin="+IN" pad="1"/>
<connect gate="A" pin="-IN" pad="3"/>
<connect gate="A" pin="OUT" pad="4"/>
<connect gate="A" pin="V+" pad="5"/>
<connect gate="A" pin="V-" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMV841MG"/>
<attribute name="OC_FARNELL" value="1320980"/>
<attribute name="OC_NEWARK" value="32M0965"/>
<attribute name="PACKAGE" value="SC70-5"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMV842MA" prefix="U">
<description>Op Amps</description>
<gates>
<gate name="A" symbol="LMV842MA"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="INB+" pad="5"/>
<connect gate="A" pin="INB-" pad="6"/>
<connect gate="A" pin="IN_A+" pad="3"/>
<connect gate="A" pin="IN_A-" pad="2"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMV842MA"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="84M8080"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMV842MM" prefix="U">
<description>Op Amps</description>
<gates>
<gate name="A" symbol="LMV842MM"/>
</gates>
<devices>
<device name="" package="SOP65P490X109-8N">
<connects>
<connect gate="A" pin="INA+" pad="3"/>
<connect gate="A" pin="INA-" pad="2"/>
<connect gate="A" pin="INB+" pad="5"/>
<connect gate="A" pin="INB-" pad="6"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMV842MM"/>
<attribute name="OC_FARNELL" value="1685352"/>
<attribute name="OC_NEWARK" value="47T5191"/>
<attribute name="PACKAGE" value="MSOP-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMV842QMA" prefix="U">
<description>Op Amps</description>
<gates>
<gate name="A" symbol="LMV842QMA"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="INB+" pad="5"/>
<connect gate="A" pin="INB-" pad="6"/>
<connect gate="A" pin="IN_A+" pad="3"/>
<connect gate="A" pin="IN_A-" pad="2"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMV842QMA"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="55R3762"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMV842QMM" prefix="U">
<description>Op Amps</description>
<gates>
<gate name="A" symbol="LMV842QMM"/>
</gates>
<devices>
<device name="" package="SOP65P490X109-8N">
<connects>
<connect gate="A" pin="INA+" pad="3"/>
<connect gate="A" pin="INA-" pad="2"/>
<connect gate="A" pin="INB+" pad="5"/>
<connect gate="A" pin="INB-" pad="6"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMV842QMM"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="55R3764"/>
<attribute name="PACKAGE" value="MSOP-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMV844MA" prefix="U">
<description>Op Amps</description>
<gates>
<gate name="A" symbol="LMV844MA"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="+INA" pad="3"/>
<connect gate="A" pin="+INB" pad="5"/>
<connect gate="A" pin="+INC" pad="10"/>
<connect gate="A" pin="+IND" pad="12"/>
<connect gate="A" pin="-INA" pad="2"/>
<connect gate="A" pin="-INB" pad="6"/>
<connect gate="A" pin="-INC" pad="9"/>
<connect gate="A" pin="-IND" pad="13"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="OUTC" pad="8"/>
<connect gate="A" pin="OUTD" pad="14"/>
<connect gate="A" pin="V+" pad="4"/>
<connect gate="A" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMV844MA"/>
<attribute name="OC_FARNELL" value="1694608"/>
<attribute name="OC_NEWARK" value="64M6921"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMV844MT" prefix="U">
<description>Wide Supply Range Operational amp</description>
<gates>
<gate name="A" symbol="LMV844MT"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-14N">
<connects>
<connect gate="A" pin="+INA" pad="3"/>
<connect gate="A" pin="+INB" pad="5"/>
<connect gate="A" pin="+INC" pad="10"/>
<connect gate="A" pin="+IND" pad="12"/>
<connect gate="A" pin="-INA" pad="2"/>
<connect gate="A" pin="-INB" pad="6"/>
<connect gate="A" pin="-INC" pad="9"/>
<connect gate="A" pin="-IND" pad="13"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="OUTC" pad="8"/>
<connect gate="A" pin="OUTD" pad="14"/>
<connect gate="A" pin="V+" pad="4"/>
<connect gate="A" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMV844MT"/>
<attribute name="OC_FARNELL" value="1342340"/>
<attribute name="OC_NEWARK" value="46M5463"/>
<attribute name="PACKAGE" value="TSSOP-14"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMV844QMA" prefix="U">
<description>Op Amps</description>
<gates>
<gate name="A" symbol="LMV844QMA"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="+INA" pad="3"/>
<connect gate="A" pin="+INB" pad="5"/>
<connect gate="A" pin="+INC" pad="10"/>
<connect gate="A" pin="+IND" pad="12"/>
<connect gate="A" pin="-INA" pad="2"/>
<connect gate="A" pin="-INB" pad="6"/>
<connect gate="A" pin="-INC" pad="9"/>
<connect gate="A" pin="-IND" pad="13"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="OUTC" pad="8"/>
<connect gate="A" pin="OUTD" pad="14"/>
<connect gate="A" pin="V+" pad="4"/>
<connect gate="A" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMV844QMA"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="27R1772"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMV851MG" prefix="U">
<description>Op Amps</description>
<gates>
<gate name="A" symbol="LMV851MG"/>
</gates>
<devices>
<device name="" package="SOT65P210X110-5N">
<connects>
<connect gate="A" pin="+IN" pad="1"/>
<connect gate="A" pin="-IN" pad="3"/>
<connect gate="A" pin="OUT" pad="4"/>
<connect gate="A" pin="V+" pad="5"/>
<connect gate="A" pin="V-" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMV851MG"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="64M6923"/>
<attribute name="PACKAGE" value="SC70-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMV852MM" prefix="U">
<description>Op Amps</description>
<gates>
<gate name="A" symbol="LMV852MM"/>
</gates>
<devices>
<device name="" package="SOP65P490X109-8N">
<connects>
<connect gate="A" pin="INA+" pad="3"/>
<connect gate="A" pin="INA-" pad="2"/>
<connect gate="A" pin="INB+" pad="5"/>
<connect gate="A" pin="INB-" pad="6"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMV852MM"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="64M6925"/>
<attribute name="PACKAGE" value="MSOP-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMV854MT" prefix="U">
<description>Op Amps</description>
<gates>
<gate name="A" symbol="LMV854MT"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-14N">
<connects>
<connect gate="A" pin="INA+" pad="3"/>
<connect gate="A" pin="INA-" pad="2"/>
<connect gate="A" pin="INB+" pad="5"/>
<connect gate="A" pin="INB-" pad="6"/>
<connect gate="A" pin="INC+" pad="10"/>
<connect gate="A" pin="INC-" pad="9"/>
<connect gate="A" pin="IND+" pad="12"/>
<connect gate="A" pin="IND-" pad="13"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="OUTC" pad="8"/>
<connect gate="A" pin="OUTD" pad="14"/>
<connect gate="A" pin="V+" pad="4"/>
<connect gate="A" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMV854MT"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="64M6927"/>
<attribute name="PACKAGE" value="TSSOP-14"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMV861MG" prefix="U">
<description>OpAmpIC</description>
<gates>
<gate name="A" symbol="LMV861MG"/>
</gates>
<devices>
<device name="" package="SOT65P240X110-5N">
<connects>
<connect gate="A" pin="IN+" pad="1"/>
<connect gate="A" pin="IN-" pad="3"/>
<connect gate="A" pin="OUT" pad="4"/>
<connect gate="A" pin="V+" pad="5"/>
<connect gate="A" pin="V-" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMV861MG"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="84M8085"/>
<attribute name="PACKAGE" value="SC70-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMV862MM" prefix="U">
<description>Op Amps</description>
<gates>
<gate name="A" symbol="LMV862MM"/>
</gates>
<devices>
<device name="" package="SOP65P490X109-8N">
<connects>
<connect gate="A" pin="INA+" pad="3"/>
<connect gate="A" pin="INA-" pad="2"/>
<connect gate="A" pin="INB+" pad="5"/>
<connect gate="A" pin="INB-" pad="6"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMV862MM"/>
<attribute name="OC_FARNELL" value="1663005"/>
<attribute name="OC_NEWARK" value="07P5346"/>
<attribute name="PACKAGE" value="MSOP-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMV931MF" prefix="U">
<description>Operational Amplifiers</description>
<gates>
<gate name="A" symbol="LMV931MF"/>
</gates>
<devices>
<device name="" package="SOT95P284X119-5N">
<connects>
<connect gate="A" pin="+IN" pad="1"/>
<connect gate="A" pin="-IN" pad="3"/>
<connect gate="A" pin="OUT" pad="4"/>
<connect gate="A" pin="V+" pad="5"/>
<connect gate="A" pin="V-" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMV931MF"/>
<attribute name="OC_FARNELL" value="1312837"/>
<attribute name="OC_NEWARK" value="41K3209"/>
<attribute name="PACKAGE" value="SOT23-5"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMV931MG" prefix="U">
<description>Operational Amplifiers</description>
<gates>
<gate name="A" symbol="LMV931MG"/>
</gates>
<devices>
<device name="" package="SOT65P210X110-5N">
<connects>
<connect gate="A" pin="IN+" pad="1"/>
<connect gate="A" pin="IN-" pad="3"/>
<connect gate="A" pin="OUT" pad="4"/>
<connect gate="A" pin="V+" pad="5"/>
<connect gate="A" pin="V-" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMV931MG"/>
<attribute name="OC_FARNELL" value="1312838"/>
<attribute name="OC_NEWARK" value="74C3793"/>
<attribute name="PACKAGE" value="SC-70-5"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMV932MA" prefix="U">
<description>OpAmpIC</description>
<gates>
<gate name="A" symbol="LMV932MA"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="+INA" pad="3"/>
<connect gate="A" pin="+INB" pad="5"/>
<connect gate="A" pin="-INA" pad="2"/>
<connect gate="A" pin="-INB" pad="6"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMV932MA"/>
<attribute name="OC_FARNELL" value="1286955"/>
<attribute name="OC_NEWARK" value="29H6237"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMV932MM" prefix="U">
<description>Operational Amplifiers</description>
<gates>
<gate name="A" symbol="LMV932MM"/>
</gates>
<devices>
<device name="" package="SOP65P490X109-8N">
<connects>
<connect gate="A" pin="IN_A+" pad="3"/>
<connect gate="A" pin="IN_A-" pad="2"/>
<connect gate="A" pin="IN_B+" pad="5"/>
<connect gate="A" pin="IN_B-" pad="6"/>
<connect gate="A" pin="OUT_A" pad="1"/>
<connect gate="A" pin="OUT_B" pad="7"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMV932MM"/>
<attribute name="OC_FARNELL" value="1312839"/>
<attribute name="OC_NEWARK" value="41K3215"/>
<attribute name="PACKAGE" value="8-MSOP"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMV934MA" prefix="U">
<description>OpAmpIC</description>
<gates>
<gate name="A" symbol="LMV934MA"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="+INA" pad="3"/>
<connect gate="A" pin="+INB" pad="5"/>
<connect gate="A" pin="+INC" pad="10"/>
<connect gate="A" pin="+IND" pad="12"/>
<connect gate="A" pin="-INA" pad="2"/>
<connect gate="A" pin="-INB" pad="6"/>
<connect gate="A" pin="-INC" pad="9"/>
<connect gate="A" pin="-IND" pad="13"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="OUTC" pad="8"/>
<connect gate="A" pin="OUTD" pad="14"/>
<connect gate="A" pin="V+" pad="4"/>
<connect gate="A" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMV934MA"/>
<attribute name="OC_FARNELL" value="1286956"/>
<attribute name="OC_NEWARK" value="29H6239"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMV934MT" prefix="U">
<description>OpAmpIC</description>
<gates>
<gate name="A" symbol="LMV934MT"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-14N">
<connects>
<connect gate="A" pin="INA+" pad="3"/>
<connect gate="A" pin="INA-" pad="2"/>
<connect gate="A" pin="INB+" pad="5"/>
<connect gate="A" pin="INB-" pad="6"/>
<connect gate="A" pin="INC+" pad="10"/>
<connect gate="A" pin="INC-" pad="9"/>
<connect gate="A" pin="IND+" pad="12"/>
<connect gate="A" pin="IND-" pad="13"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="OUTC" pad="8"/>
<connect gate="A" pin="OUTD" pad="14"/>
<connect gate="A" pin="V+" pad="4"/>
<connect gate="A" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMV934MT"/>
<attribute name="OC_FARNELL" value="1286957"/>
<attribute name="OC_NEWARK" value="41K3219"/>
<attribute name="PACKAGE" value="TSSOP-14"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMV951MK" prefix="U">
<description>Rail-to-Rail Input and Output Amplifier</description>
<gates>
<gate name="A" symbol="LMV951MK"/>
</gates>
<devices>
<device name="" package="SOT95P285X100-6N">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="4"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="A" pin="SD" pad="5"/>
<connect gate="A" pin="V+" pad="6"/>
<connect gate="A" pin="V-" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMV951MK"/>
<attribute name="OC_FARNELL" value="1313864"/>
<attribute name="OC_NEWARK" value="32M0967"/>
<attribute name="PACKAGE" value="SOT-23-6"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMV981MF" prefix="U">
<description>Operational Amplifiers</description>
<gates>
<gate name="A" symbol="LMV981MF"/>
</gates>
<devices>
<device name="" package="SOT95P284X122-6N">
<connects>
<connect gate="A" pin="+IN" pad="1"/>
<connect gate="A" pin="-IN" pad="3"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="OUT" pad="4"/>
<connect gate="A" pin="VDD" pad="6"/>
<connect gate="A" pin="~SHDN" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMV981MF"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K3221"/>
<attribute name="PACKAGE" value="SOT23-6"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMV981MG" prefix="U">
<description>Operational Amplifiers</description>
<gates>
<gate name="A" symbol="LMV981MG"/>
</gates>
<devices>
<device name="" package="SOT65P240X110-6N">
<connects>
<connect gate="A" pin="+IN" pad="1"/>
<connect gate="A" pin="-IN" pad="3"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="OUT" pad="4"/>
<connect gate="A" pin="VDD" pad="6"/>
<connect gate="A" pin="~SHDN" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMV981MG"/>
<attribute name="OC_FARNELL" value="1685374"/>
<attribute name="OC_NEWARK" value="41K3223"/>
<attribute name="PACKAGE" value="SC70-6"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMV982MM" prefix="U">
<description>OpAmpIC</description>
<gates>
<gate name="A" symbol="LMV982MM"/>
</gates>
<devices>
<device name="" package="SOP50P490X109-10N">
<connects>
<connect gate="A" pin="+INA" pad="3"/>
<connect gate="A" pin="+INB" pad="7"/>
<connect gate="A" pin="-INA" pad="2"/>
<connect gate="A" pin="-INB" pad="8"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="9"/>
<connect gate="A" pin="V+" pad="10"/>
<connect gate="A" pin="V-" pad="4"/>
<connect gate="A" pin="~SHDN_A" pad="5"/>
<connect gate="A" pin="~SHDN_B" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LMV982MM"/>
<attribute name="OC_FARNELL" value="1312842"/>
<attribute name="OC_NEWARK" value="74C3805"/>
<attribute name="PACKAGE" value="MSOP-10"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP2902M" prefix="U">
<description>OpAmpIC</description>
<gates>
<gate name="A" symbol="LP2902M"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="+INA" pad="3"/>
<connect gate="A" pin="+INB" pad="5"/>
<connect gate="A" pin="+INC" pad="10"/>
<connect gate="A" pin="+IND" pad="12"/>
<connect gate="A" pin="-INA" pad="2"/>
<connect gate="A" pin="-INB" pad="6"/>
<connect gate="A" pin="-INC" pad="9"/>
<connect gate="A" pin="-IND" pad="13"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="OUTC" pad="8"/>
<connect gate="A" pin="OUTD" pad="14"/>
<connect gate="A" pin="V+" pad="4"/>
<connect gate="A" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP2902M"/>
<attribute name="OC_FARNELL" value="1798373"/>
<attribute name="OC_NEWARK" value="73R9754"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP2951ACM" prefix="U">
<description>Micropower Voltage Regulators</description>
<gates>
<gate name="A" symbol="LP2951ACM"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="FB" pad="7"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="IN" pad="8"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="A" pin="SD" pad="3"/>
<connect gate="A" pin="SEN" pad="2"/>
<connect gate="A" pin="VTAP" pad="6"/>
<connect gate="A" pin="~ERR" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP2951ACM"/>
<attribute name="OC_FARNELL" value="9493425"/>
<attribute name="OC_NEWARK" value="17M0417"/>
<attribute name="PACKAGE" value="8-SOIC"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP2951ACN" prefix="U">
<description>Micropower Voltage Regulators</description>
<gates>
<gate name="A" symbol="LP2951ACN"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-8">
<connects>
<connect gate="A" pin="FB" pad="7"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="IN" pad="8"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="A" pin="SD" pad="3"/>
<connect gate="A" pin="SEN" pad="2"/>
<connect gate="A" pin="VTAP" pad="6"/>
<connect gate="A" pin="~ERROR" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP2951ACN"/>
<attribute name="OC_FARNELL" value="9488553"/>
<attribute name="OC_NEWARK" value="-"/>
<attribute name="PACKAGE" value="DIP-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP2951ACSD-3.3" prefix="U">
<description>Voltage Regulators</description>
<gates>
<gate name="A" symbol="LP2951ACSD-3.3"/>
</gates>
<devices>
<device name="" package="DFN400X400X80-9N">
<connects>
<connect gate="A" pin="DAP" pad="9"/>
<connect gate="A" pin="FB" pad="7"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="IN" pad="8"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="A" pin="SD" pad="3"/>
<connect gate="A" pin="SEN" pad="2"/>
<connect gate="A" pin="VTAP" pad="6"/>
<connect gate="A" pin="~ERR" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP2951ACSD-33"/>
<attribute name="OC_FARNELL" value="1008041"/>
<attribute name="OC_NEWARK" value="97K3648"/>
<attribute name="PACKAGE" value="LLP-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP2951CMM" prefix="U">
<description>Voltage Regulators</description>
<gates>
<gate name="A" symbol="LP2951CMM"/>
</gates>
<devices>
<device name="" package="SOP65P490X110-8N">
<connects>
<connect gate="A" pin="FB" pad="7"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="IN" pad="8"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="A" pin="SENSE" pad="2"/>
<connect gate="A" pin="SHDN" pad="3"/>
<connect gate="A" pin="VTAP" pad="6"/>
<connect gate="A" pin="~ERROR" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP2951CMM"/>
<attribute name="OC_FARNELL" value="1652320"/>
<attribute name="OC_NEWARK" value="07B7051"/>
<attribute name="PACKAGE" value="8-MSOP"/>
<attribute name="SUPPLIER" value="NATIONAL SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP2951CSD-3.3" prefix="U">
<description>Voltage Regulators</description>
<gates>
<gate name="A" symbol="LP2951CSD-3.3"/>
</gates>
<devices>
<device name="" package="DFN400X400X80-9N">
<connects>
<connect gate="A" pin="FB" pad="7"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="GND_2" pad="9"/>
<connect gate="A" pin="IN" pad="8"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="A" pin="SD" pad="3"/>
<connect gate="A" pin="SEN" pad="2"/>
<connect gate="A" pin="VTAP" pad="6"/>
<connect gate="A" pin="~ERR" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP2951CSD-3.3"/>
<attribute name="OC_FARNELL" value="1008044"/>
<attribute name="OC_NEWARK" value="97K3651"/>
<attribute name="PACKAGE" value="LLP-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP2951CSD" prefix="U">
<description>Voltage Regulators</description>
<gates>
<gate name="A" symbol="LP2951CSD"/>
</gates>
<devices>
<device name="" package="DFN400X400X80-9N">
<connects>
<connect gate="A" pin="FB" pad="7"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="GND_2" pad="9"/>
<connect gate="A" pin="IN" pad="8"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="A" pin="SD" pad="3"/>
<connect gate="A" pin="SEN" pad="2"/>
<connect gate="A" pin="VTAP" pad="6"/>
<connect gate="A" pin="~ERR" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP2951CSD"/>
<attribute name="OC_FARNELL" value="1008042"/>
<attribute name="OC_NEWARK" value="97K3650"/>
<attribute name="PACKAGE" value="LLP-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP2952IM" prefix="U">
<description>Voltage Regulators</description>
<gates>
<gate name="A" symbol="LP2952IM"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-16N">
<connects>
<connect gate="A" pin="FB" pad="14"/>
<connect gate="A" pin="GND" pad="9"/>
<connect gate="A" pin="GND_2" pad="8"/>
<connect gate="A" pin="GND_3" pad="1"/>
<connect gate="A" pin="GND_4" pad="16"/>
<connect gate="A" pin="IN" pad="15"/>
<connect gate="A" pin="NC" pad="11"/>
<connect gate="A" pin="NC_2" pad="10"/>
<connect gate="A" pin="NC_3" pad="2"/>
<connect gate="A" pin="NC_4" pad="7"/>
<connect gate="A" pin="OUT" pad="3"/>
<connect gate="A" pin="REF" pad="12"/>
<connect gate="A" pin="SEN" pad="4"/>
<connect gate="A" pin="V_TAP" pad="13"/>
<connect gate="A" pin="~ERR" pad="6"/>
<connect gate="A" pin="~SD" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP2952IM"/>
<attribute name="OC_FARNELL" value="1215215"/>
<attribute name="OC_NEWARK" value="07B7069"/>
<attribute name="PACKAGE" value="16-SOIC"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP2980AIM5-3.0" prefix="U">
<description>Low-Dropout Regulator</description>
<gates>
<gate name="A" symbol="LP2980AIM5-3.0"/>
</gates>
<devices>
<device name="" package="SOT95P284X119-5N">
<connects>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="NC" pad="4"/>
<connect gate="A" pin="ON/OFF" pad="3"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="VOUT" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP2980AIM5-3.0"/>
<attribute name="OC_FARNELL" value="9779949"/>
<attribute name="OC_NEWARK" value="41K6697"/>
<attribute name="PACKAGE" value="SOT23-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP2980AIM5-3.3" prefix="U">
<description>Low-Dropout Regulator</description>
<gates>
<gate name="A" symbol="LP2980AIM5-3.3"/>
</gates>
<devices>
<device name="" package="SOT95P284X119-5N">
<connects>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="NC" pad="4"/>
<connect gate="A" pin="ON/OFF" pad="3"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="VOUT" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP2980AIM5-3.3"/>
<attribute name="OC_FARNELL" value="1212201"/>
<attribute name="OC_NEWARK" value="41K6700"/>
<attribute name="PACKAGE" value="SOT23-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP2980AIM5-5.0" prefix="U">
<description>Low-Dropout Regulator</description>
<gates>
<gate name="A" symbol="LP2980AIM5-5.0"/>
</gates>
<devices>
<device name="" package="SOT95P285X110-5N">
<connects>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="N/C" pad="4"/>
<connect gate="A" pin="ON/OFF" pad="3"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="VOUT" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP2980AIM5-5.0"/>
<attribute name="OC_FARNELL" value="9779647"/>
<attribute name="OC_NEWARK" value="41K6707"/>
<attribute name="PACKAGE" value="SOT23-5"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP2980IM5-3.0" prefix="U">
<description>Dropout Regulator</description>
<gates>
<gate name="A" symbol="LP2980IM5-3.0"/>
</gates>
<devices>
<device name="" package="SOT95P284X119-5N">
<connects>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="N/C" pad="4"/>
<connect gate="A" pin="ON/OFF" pad="3"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="VOUT" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP2980IM5-3.0"/>
<attribute name="OC_FARNELL" value="9779612"/>
<attribute name="OC_NEWARK" value="41K6734"/>
<attribute name="PACKAGE" value="SOT23-5"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP2980IM5-3.3" prefix="U">
<description>Dropout Regulator</description>
<gates>
<gate name="A" symbol="LP2980IM5-3.3"/>
</gates>
<devices>
<device name="" package="SOT95P284X119-5N">
<connects>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="N/C" pad="4"/>
<connect gate="A" pin="ON/OFF" pad="3"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="VOUT" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP2980IM5-3.3"/>
<attribute name="OC_FARNELL" value="9778977"/>
<attribute name="OC_NEWARK" value="41K6737"/>
<attribute name="PACKAGE" value="SOT23-5"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP2980IM5-5.0" prefix="U">
<description>Literature Number</description>
<gates>
<gate name="A" symbol="LP2980IM5-5.0"/>
</gates>
<devices>
<device name="" package="SOT95P284X119-5N">
<connects>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="N/C" pad="4"/>
<connect gate="A" pin="ON/OFF" pad="3"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="VOUT" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP2980IM5-5.0"/>
<attribute name="OC_FARNELL" value="9779329"/>
<attribute name="OC_NEWARK" value="41K6744"/>
<attribute name="PACKAGE" value="SOT23-5"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP2982AIM5-3.0" prefix="U">
<description>Low-Dropout Regulator</description>
<gates>
<gate name="A" symbol="LP2982AIM5-3.0"/>
</gates>
<devices>
<device name="" package="SOT95P284X122-5N">
<connects>
<connect gate="A" pin="BYPASS" pad="4"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="ON/~OFF" pad="3"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="VOUT" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP2982AIM5-3.0"/>
<attribute name="OC_FARNELL" value="1685496"/>
<attribute name="OC_NEWARK" value="41K6819"/>
<attribute name="PACKAGE" value="SOT-5"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP2982AIM5-3.3" prefix="U">
<description>Low-Dropout Regulator</description>
<gates>
<gate name="A" symbol="LP2982AIM5-3.3"/>
</gates>
<devices>
<device name="" package="SOT95P284X122-5N">
<connects>
<connect gate="A" pin="BYPASS" pad="4"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="ON/~OFF" pad="3"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="VOUT" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP2982AIM5-3.3"/>
<attribute name="OC_FARNELL" value="1652322"/>
<attribute name="OC_NEWARK" value="41K6820"/>
<attribute name="PACKAGE" value="SOT-5"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP2982AIM5-5.0" prefix="U">
<description>Low-Dropout Regulator</description>
<gates>
<gate name="A" symbol="LP2982AIM5-5.0"/>
</gates>
<devices>
<device name="" package="SOT95P284X122-5N">
<connects>
<connect gate="A" pin="BYPASS" pad="4"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="ON/~OFF" pad="3"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="VOUT" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP2982AIM5-5.0"/>
<attribute name="OC_FARNELL" value="1685676"/>
<attribute name="OC_NEWARK" value="41K6826"/>
<attribute name="PACKAGE" value="SOT-5"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP2982IM5-3.3" prefix="U">
<description>Low-Dropout Regulator</description>
<gates>
<gate name="A" symbol="LP2982IM5-3.3"/>
</gates>
<devices>
<device name="" package="SOT95P284X122-5N">
<connects>
<connect gate="A" pin="BYPASS" pad="4"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="ON/~OFF" pad="3"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="VOUT" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP2982IM5-3.3"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K6844"/>
<attribute name="PACKAGE" value="SOT-5"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP2982IM5-5.0" prefix="U">
<description>Low-Dropout Regulator</description>
<gates>
<gate name="A" symbol="LP2982IM5-5.0"/>
</gates>
<devices>
<device name="" package="SOT95P284X119-5N">
<connects>
<connect gate="A" pin="BYPASS" pad="4"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="ON/OFF" pad="3"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="VOUT" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP2982IM5-5.0"/>
<attribute name="OC_FARNELL" value="9779825"/>
<attribute name="OC_NEWARK" value="41K6850"/>
<attribute name="PACKAGE" value="SOT23-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP2985AIM5-2.5" prefix="U">
<description>Low-Noise Ultra Low-Dropout Regulator</description>
<gates>
<gate name="A" symbol="LP2985AIM5-2.5"/>
</gates>
<devices>
<device name="" package="SOT95P285X120-5N">
<connects>
<connect gate="A" pin="BYPASS" pad="4"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="ON/OFF" pad="3"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="VOUT" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP2985AIM5-2.5"/>
<attribute name="OC_FARNELL" value="9778543"/>
<attribute name="OC_NEWARK" value="41K6881"/>
<attribute name="PACKAGE" value="SOT23-5"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP2985AIM5-2.7" prefix="U">
<description>Low-Dropout Regulator</description>
<gates>
<gate name="A" symbol="LP2985AIM5-2.7"/>
</gates>
<devices>
<device name="" package="SOT95P284X120-5N">
<connects>
<connect gate="A" pin="BP" pad="4"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="ON/OFF" pad="3"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="VOUT" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP2985AIM5-2.7"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K6883"/>
<attribute name="PACKAGE" value="SOT23-5"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP2985AIM5-2.8" prefix="U">
<description>Low-Dropout Regulator</description>
<gates>
<gate name="A" symbol="LP2985AIM5-2.8"/>
</gates>
<devices>
<device name="" package="SOT95P284X120-5N">
<connects>
<connect gate="A" pin="BP" pad="4"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="ON/OFF" pad="3"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="VOUT" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP2985AIM5-2.8"/>
<attribute name="OC_FARNELL" value="1469132"/>
<attribute name="OC_NEWARK" value="41K6884"/>
<attribute name="PACKAGE" value="SOT23-5"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP2985AIM5-3.0" prefix="U">
<description>Low-Noise Ultra Low-Dropout Regulator</description>
<gates>
<gate name="A" symbol="LP2985AIM5-3.0"/>
</gates>
<devices>
<device name="" package="SOT95P285X120-5N">
<connects>
<connect gate="A" pin="BYPASS" pad="4"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="ON/OFF" pad="3"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="VOUT" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP2985AIM5-3.0"/>
<attribute name="OC_FARNELL" value="9778250"/>
<attribute name="OC_NEWARK" value="41K6886"/>
<attribute name="PACKAGE" value="SOT23-5"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP2985AIM5-3.3" prefix="U">
<description>Low-Dropout Regulator</description>
<gates>
<gate name="A" symbol="LP2985AIM5-3.3"/>
</gates>
<devices>
<device name="" package="SOT95P284X119-5N">
<connects>
<connect gate="A" pin="BYPASS" pad="4"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="ON/OFF" pad="3"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="VOUT" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP2985AIM5-3.3"/>
<attribute name="OC_FARNELL" value="9778276"/>
<attribute name="OC_NEWARK" value="97K3686"/>
<attribute name="PACKAGE" value="SOT23-5"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP2985AIM5-3.6" prefix="U">
<description>Low-Dropout Regulator</description>
<gates>
<gate name="A" symbol="LP2985AIM5-3.6"/>
</gates>
<devices>
<device name="" package="SOT95P284X120-5N">
<connects>
<connect gate="A" pin="BP" pad="4"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="ON/OFF" pad="3"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="VOUT" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP2985AIM5-3.6"/>
<attribute name="OC_FARNELL" value="1685681"/>
<attribute name="OC_NEWARK" value="41K6891"/>
<attribute name="PACKAGE" value="SOT23-5"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP2985AIM5-3.8" prefix="U">
<description>Low-Dropout Regulator</description>
<gates>
<gate name="A" symbol="LP2985AIM5-3.8"/>
</gates>
<devices>
<device name="" package="SOT95P284X120-5N">
<connects>
<connect gate="A" pin="BP" pad="4"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="ON/OFF" pad="3"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="VOUT" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP2985AIM5-3.8"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K6892"/>
<attribute name="PACKAGE" value="SOT23-5"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP2985AIM5-4.0" prefix="U">
<description>Low-Dropout Regulator</description>
<gates>
<gate name="A" symbol="LP2985AIM5-4.0"/>
</gates>
<devices>
<device name="" package="SOT95P284X120-5N">
<connects>
<connect gate="A" pin="BP" pad="4"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="ON/OFF" pad="3"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="VOUT" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP2985AIM5-4.0"/>
<attribute name="OC_FARNELL" value="1685682"/>
<attribute name="OC_NEWARK" value="41K6893"/>
<attribute name="PACKAGE" value="SOT23-5"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP2985AIM5-4.5" prefix="U">
<description>Low-Dropout Regulator</description>
<gates>
<gate name="A" symbol="LP2985AIM5-4.5"/>
</gates>
<devices>
<device name="" package="SOT95P284X120-5N">
<connects>
<connect gate="A" pin="BP" pad="4"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="ON/OFF" pad="3"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="VOUT" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP2985AIM5-4.5"/>
<attribute name="OC_FARNELL" value="1685756"/>
<attribute name="OC_NEWARK" value="55K6862"/>
<attribute name="PACKAGE" value="SOT23-5"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP2985AIM5-5.0" prefix="U">
<description>Drop out Regulator</description>
<gates>
<gate name="A" symbol="LP2985AIM5-5.0"/>
</gates>
<devices>
<device name="" package="SOT95P284X119-5N">
<connects>
<connect gate="A" pin="BY_PASS" pad="4"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="ON/OFF" pad="3"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="VOUT" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP2985AIM5-5.0"/>
<attribute name="OC_FARNELL" value="9778292"/>
<attribute name="OC_NEWARK" value="97K3687"/>
<attribute name="PACKAGE" value="SOT23-5"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP2985AIM5-6.1" prefix="U">
<description>Low-Dropout Regulator</description>
<gates>
<gate name="A" symbol="LP2985AIM5-6.1"/>
</gates>
<devices>
<device name="" package="SOT95P284X120-5N">
<connects>
<connect gate="A" pin="BP" pad="4"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="ON/OFF" pad="3"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="VOUT" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP2985AIM5-6.1"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K6898"/>
<attribute name="PACKAGE" value="SOT23-5"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP2985AITP-2.8" prefix="U">
<description>IC REG LDO 150MA 2.8V</description>
<gates>
<gate name="A" symbol="LP2985AITP-2.8"/>
</gates>
<devices>
<device name="" package="BGA05C25PX433P3X3_93X110X50">
<connects>
<connect gate="A" pin="BP" pad="B2"/>
<connect gate="A" pin="GND" pad="A1"/>
<connect gate="A" pin="ON-OFF" pad="A3"/>
<connect gate="A" pin="VIN" pad="C3"/>
<connect gate="A" pin="VOUT" pad="C1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP2985AITP-28"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K6926"/>
<attribute name="PACKAGE" value="5-UFBGA"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP2985AITP-3.3" prefix="U">
<description>IC REG LDO 150MA 3.3V</description>
<gates>
<gate name="A" symbol="LP2985AITP-3.3"/>
</gates>
<devices>
<device name="" package="BGA05C25PX433P3X3_93X110X50">
<connects>
<connect gate="A" pin="BP" pad="B2"/>
<connect gate="A" pin="GND" pad="A1"/>
<connect gate="A" pin="ON-OFF" pad="A3"/>
<connect gate="A" pin="VIN" pad="C3"/>
<connect gate="A" pin="VOUT" pad="C1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP2985AITP-3.3"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K6928"/>
<attribute name="PACKAGE" value="5-UFBGA"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP2985AITP-5.0" prefix="U">
<description>Ultra Low-Dropout Regulator</description>
<gates>
<gate name="A" symbol="LP2985AITP-5.0"/>
</gates>
<devices>
<device name="" package="BGA5C50P2X3_110X93X57">
<connects>
<connect gate="A" pin="BYPASS" pad="B2"/>
<connect gate="A" pin="GND" pad="A1"/>
<connect gate="A" pin="ON/OFF" pad="A3"/>
<connect gate="A" pin="VIN" pad="C3"/>
<connect gate="A" pin="VOUT" pad="C1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP2985AITP-5.0"/>
<attribute name="OC_FARNELL" value="1008045"/>
<attribute name="OC_NEWARK" value=" 97K3688"/>
<attribute name="PACKAGE" value="BGA-5"/>
<attribute name="SUPPLIER" value="NSC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP2985IM5-2.5" prefix="U">
<description>Low-Noise Ultra Low-Dropout Regulator</description>
<gates>
<gate name="A" symbol="LP2985IM5-2.5"/>
</gates>
<devices>
<device name="" package="SOT95P285X120-5N">
<connects>
<connect gate="A" pin="BYPASS" pad="4"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="ON/OFF" pad="3"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="VOUT" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP2985IM5-2.5"/>
<attribute name="OC_FARNELL" value="9778535"/>
<attribute name="OC_NEWARK" value="41K6944"/>
<attribute name="PACKAGE" value="SOT23-5"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP2985IM5-2.8" prefix="U">
<description>Low-Dropout Regulator</description>
<gates>
<gate name="A" symbol="LP2985IM5-2.8"/>
</gates>
<devices>
<device name="" package="SOT95P284X120-5N">
<connects>
<connect gate="A" pin="BP" pad="4"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="ON/OFF" pad="3"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="VOUT" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP2985IM5-2.8"/>
<attribute name="OC_FARNELL" value="1685560"/>
<attribute name="OC_NEWARK" value="41K6947"/>
<attribute name="PACKAGE" value="SOT23-5"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP2985IM5-3.0" prefix="U">
<description>Low-Dropout Regulator</description>
<gates>
<gate name="A" symbol="LP2985IM5-3.0"/>
</gates>
<devices>
<device name="" package="SOT95P284X119-5N">
<connects>
<connect gate="A" pin="BYPASS" pad="4"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="ON/OFF" pad="3"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="VOUT" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP2985IM5-3.0"/>
<attribute name="OC_FARNELL" value="9778268"/>
<attribute name="OC_NEWARK" value="97K3690"/>
<attribute name="PACKAGE" value="SOT23-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP2985IM5-3.1" prefix="U">
<description>Low-Dropout Regulator</description>
<gates>
<gate name="A" symbol="LP2985IM5-3.1"/>
</gates>
<devices>
<device name="" package="SOT95P284X120-5N">
<connects>
<connect gate="A" pin="BP" pad="4"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="ON/OFF" pad="3"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="VOUT" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP2985IM5-3.1"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K6950"/>
<attribute name="PACKAGE" value="SOT23-5"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP2985IM5-3.2" prefix="U">
<description>Low-Dropout Regulator</description>
<gates>
<gate name="A" symbol="LP2985IM5-3.2"/>
</gates>
<devices>
<device name="" package="SOT95P284X120-5N">
<connects>
<connect gate="A" pin="BP" pad="4"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="ON/OFF" pad="3"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="VOUT" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP2985IM5-3.2"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K6951"/>
<attribute name="PACKAGE" value="SOT23-5"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP2985IM5-3.3" prefix="U">
<description>Low-Noise Ultra Low-Dropout Regulator</description>
<gates>
<gate name="A" symbol="LP2985IM5-3.3"/>
</gates>
<devices>
<device name="" package="SOT95P285X120-5N">
<connects>
<connect gate="A" pin="BYPASS" pad="4"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="ON/OFF" pad="3"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="VOUT" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP2985IM5-3.3"/>
<attribute name="OC_FARNELL" value="9778284"/>
<attribute name="OC_NEWARK" value="41K6952"/>
<attribute name="PACKAGE" value="SOT23-5"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP2985IM5-3.6" prefix="U">
<description>Low-Dropout Regulator</description>
<gates>
<gate name="A" symbol="LP2985IM5-3.6"/>
</gates>
<devices>
<device name="" package="SOT95P284X120-5N">
<connects>
<connect gate="A" pin="BP" pad="4"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="ON/OFF" pad="3"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="VOUT" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP2985IM5-3.6"/>
<attribute name="OC_FARNELL" value="1652323"/>
<attribute name="OC_NEWARK" value="41K6954"/>
<attribute name="PACKAGE" value="SOT23-5"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP2985IM5-3.8" prefix="U">
<description>Low-Dropout Regulator</description>
<gates>
<gate name="A" symbol="LP2985IM5-3.8"/>
</gates>
<devices>
<device name="" package="SOT95P284X120-5N">
<connects>
<connect gate="A" pin="BP" pad="4"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="ON/OFF" pad="3"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="VOUT" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP2985IM5-3.8"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K6955"/>
<attribute name="PACKAGE" value="SOT23-5"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP2985IM5-4.0" prefix="U">
<description>Low-Dropout Regulator</description>
<gates>
<gate name="A" symbol="LP2985IM5-4.0"/>
</gates>
<devices>
<device name="" package="SOT95P284X120-5N">
<connects>
<connect gate="A" pin="BP" pad="4"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="ON/OFF" pad="3"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="VOUT" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP2985IM5-4.0"/>
<attribute name="OC_FARNELL" value="1685683"/>
<attribute name="OC_NEWARK" value="41K6956"/>
<attribute name="PACKAGE" value="SOT23-5"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP2985IM5-4.5" prefix="U">
<description>Low-Dropout Regulator</description>
<gates>
<gate name="A" symbol="LP2985IM5-4.5"/>
</gates>
<devices>
<device name="" package="SOT95P284X120-5N">
<connects>
<connect gate="A" pin="BP" pad="4"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="ON/OFF" pad="3"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="VOUT" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP2985IM5-4.5"/>
<attribute name="OC_FARNELL" value="1685684"/>
<attribute name="OC_NEWARK" value="41K6957"/>
<attribute name="PACKAGE" value="SOT23-5"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP2985IM5-5.0" prefix="U">
<description>Dropout Regulator</description>
<gates>
<gate name="A" symbol="LP2985IM5-5.0"/>
</gates>
<devices>
<device name="" package="SOT95P284X119-5N">
<connects>
<connect gate="A" pin="BYPASS" pad="4"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="ON/OFF" pad="3"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="VOUT" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP2985IM5-5.0"/>
<attribute name="OC_FARNELL" value="9778306"/>
<attribute name="OC_NEWARK" value="83F4676"/>
<attribute name="PACKAGE" value="SOT23-5"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP2985IM5-6.1" prefix="U">
<description>Low-Dropout Regulator</description>
<gates>
<gate name="A" symbol="LP2985IM5-6.1"/>
</gates>
<devices>
<device name="" package="SOT95P284X120-5N">
<connects>
<connect gate="A" pin="BP" pad="4"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="ON/OFF" pad="3"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="VOUT" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP2985IM5-6.1"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K6962"/>
<attribute name="PACKAGE" value="SOT23-5"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP2986AILD-3.3" prefix="U">
<description>Voltage Regulator</description>
<gates>
<gate name="A" symbol="LP2986AILD-3.3"/>
</gates>
<devices>
<device name="" package="DFN400X400X80-9N">
<connects>
<connect gate="A" pin="FB" pad="2"/>
<connect gate="A" pin="GND" pad="1"/>
<connect gate="A" pin="HEAT_PAD" pad="9"/>
<connect gate="A" pin="IN" pad="4"/>
<connect gate="A" pin="OUT" pad="5"/>
<connect gate="A" pin="SENSE" pad="6"/>
<connect gate="A" pin="TAP" pad="3"/>
<connect gate="A" pin="~ERROR" pad="7"/>
<connect gate="A" pin="~SD" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP2986AILD-3.3"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K7004"/>
<attribute name="PACKAGE" value="DFN-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP2986AIM-3.0" prefix="U">
<description>Voltage Regulator</description>
<gates>
<gate name="A" symbol="LP2986AIM-3.0"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="FB" pad="2"/>
<connect gate="A" pin="GND" pad="1"/>
<connect gate="A" pin="IN" pad="4"/>
<connect gate="A" pin="OUT" pad="5"/>
<connect gate="A" pin="SENSE" pad="6"/>
<connect gate="A" pin="TAP" pad="3"/>
<connect gate="A" pin="~ERROR" pad="7"/>
<connect gate="A" pin="~SD" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP2986AIM-3.0"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K7009"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP2986AIM-3.3" prefix="U">
<description>Voltage Regulator</description>
<gates>
<gate name="A" symbol="LP2986AIM-3.3"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="FB" pad="2"/>
<connect gate="A" pin="GND" pad="1"/>
<connect gate="A" pin="IN" pad="4"/>
<connect gate="A" pin="OUT" pad="5"/>
<connect gate="A" pin="SENSE" pad="6"/>
<connect gate="A" pin="TAP" pad="3"/>
<connect gate="A" pin="~ERROR" pad="7"/>
<connect gate="A" pin="~SD" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP2986AIM-3.3"/>
<attribute name="OC_FARNELL" value="1694038"/>
<attribute name="OC_NEWARK" value="41K7010"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP2986AIM-5.0" prefix="U">
<description>Voltage Regulator</description>
<gates>
<gate name="A" symbol="LP2986AIM-5.0"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="FDBK" pad="2"/>
<connect gate="A" pin="GND" pad="1"/>
<connect gate="A" pin="IN" pad="4"/>
<connect gate="A" pin="OUT" pad="5"/>
<connect gate="A" pin="SEN" pad="6"/>
<connect gate="A" pin="TAP" pad="3"/>
<connect gate="A" pin="~ERR" pad="7"/>
<connect gate="A" pin="~SD" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP2986AIM-5.0"/>
<attribute name="OC_FARNELL" value="9494880"/>
<attribute name="OC_NEWARK" value="41K7011"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP2986AIMM-3.0" prefix="U">
<description>Voltage Regulator</description>
<gates>
<gate name="A" symbol="LP2986AIMM-3.0"/>
</gates>
<devices>
<device name="" package="SOIC65P490X109-8N">
<connects>
<connect gate="A" pin="FB" pad="2"/>
<connect gate="A" pin="GND" pad="1"/>
<connect gate="A" pin="IN" pad="4"/>
<connect gate="A" pin="OUT" pad="5"/>
<connect gate="A" pin="SENSE" pad="6"/>
<connect gate="A" pin="TAP" pad="3"/>
<connect gate="A" pin="~ERROR" pad="7"/>
<connect gate="A" pin="~SD" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP2986AIMM-3.0"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K7012"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="National Smiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP2986AIMM-3.3" prefix="U">
<description>Voltage Regulator</description>
<gates>
<gate name="A" symbol="LP2986AIMM-3.3"/>
</gates>
<devices>
<device name="" package="SOP65P490X109-8N">
<connects>
<connect gate="A" pin="FEEDBACK" pad="2"/>
<connect gate="A" pin="GND" pad="1"/>
<connect gate="A" pin="IN" pad="4"/>
<connect gate="A" pin="OUT" pad="5"/>
<connect gate="A" pin="SEN" pad="6"/>
<connect gate="A" pin="TAP" pad="3"/>
<connect gate="A" pin="~ERR" pad="7"/>
<connect gate="A" pin="~SD" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP2986AIMM-3.3"/>
<attribute name="OC_FARNELL" value="9779981"/>
<attribute name="OC_NEWARK" value="07B7172"/>
<attribute name="PACKAGE" value="8-MSOP"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP2986AIMM-5.0" prefix="U">
<description>Voltage Regulator</description>
<gates>
<gate name="A" symbol="LP2986AIMM-5.0"/>
</gates>
<devices>
<device name="" package="SOP65P490X109-8N">
<connects>
<connect gate="A" pin="FEEDBACK" pad="2"/>
<connect gate="A" pin="GND" pad="1"/>
<connect gate="A" pin="IN" pad="4"/>
<connect gate="A" pin="OUT" pad="5"/>
<connect gate="A" pin="SEN" pad="6"/>
<connect gate="A" pin="TAP" pad="3"/>
<connect gate="A" pin="~ERR" pad="7"/>
<connect gate="A" pin="~SD" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP2986AIMM-5.0"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="07B7173"/>
<attribute name="PACKAGE" value="8-MSOP"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP2986ILD-3.3" prefix="U">
<description>Voltage Regulator</description>
<gates>
<gate name="A" symbol="LP2986ILD-3.3"/>
</gates>
<devices>
<device name="" package="DFN400X400X80-9N">
<connects>
<connect gate="A" pin="FB" pad="2"/>
<connect gate="A" pin="GND" pad="1"/>
<connect gate="A" pin="HEAT_PAD" pad="9"/>
<connect gate="A" pin="IN" pad="4"/>
<connect gate="A" pin="OUT" pad="5"/>
<connect gate="A" pin="SENSE" pad="6"/>
<connect gate="A" pin="TAP" pad="3"/>
<connect gate="A" pin="~ERROR" pad="7"/>
<connect gate="A" pin="~SD" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP2986ILD-3.3"/>
<attribute name="OC_FARNELL" value="4801155"/>
<attribute name="OC_NEWARK" value="34C6686"/>
<attribute name="PACKAGE" value="DFN-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP2986IM-3.0" prefix="U">
<description>Voltage Regulator</description>
<gates>
<gate name="A" symbol="LP2986IM-3.0"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="FB" pad="2"/>
<connect gate="A" pin="GND" pad="1"/>
<connect gate="A" pin="IN" pad="4"/>
<connect gate="A" pin="OUT" pad="5"/>
<connect gate="A" pin="SENSE" pad="6"/>
<connect gate="A" pin="TAP" pad="3"/>
<connect gate="A" pin="~ERROR" pad="7"/>
<connect gate="A" pin="~SD" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP2986IM-3.0"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K7026"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP2986IM-3.3" prefix="U">
<description>Voltage Regulator</description>
<gates>
<gate name="A" symbol="LP2986IM-3.3"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="FB" pad="2"/>
<connect gate="A" pin="GND" pad="1"/>
<connect gate="A" pin="IN" pad="4"/>
<connect gate="A" pin="OUT" pad="5"/>
<connect gate="A" pin="SENSE" pad="6"/>
<connect gate="A" pin="TAP" pad="3"/>
<connect gate="A" pin="~ERROR" pad="7"/>
<connect gate="A" pin="~SD" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP2986IM-3.3"/>
<attribute name="OC_FARNELL" value="1798336"/>
<attribute name="OC_NEWARK" value="73R9755"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP2986IM-5.0" prefix="U">
<description>Voltage Regulator</description>
<gates>
<gate name="A" symbol="LP2986IM-5.0"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="FB" pad="2"/>
<connect gate="A" pin="GND" pad="1"/>
<connect gate="A" pin="IN" pad="4"/>
<connect gate="A" pin="OUT" pad="5"/>
<connect gate="A" pin="SENSE" pad="6"/>
<connect gate="A" pin="TAP" pad="3"/>
<connect gate="A" pin="~ERROR" pad="7"/>
<connect gate="A" pin="~SD" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP2986IM-5.0"/>
<attribute name="OC_FARNELL" value="1694044"/>
<attribute name="OC_NEWARK" value="41K7011"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP2986IMM-3.0" prefix="U">
<description>Voltage Regulator</description>
<gates>
<gate name="A" symbol="LP2986IMM-3.0"/>
</gates>
<devices>
<device name="" package="SOIC65P490X109-8N">
<connects>
<connect gate="A" pin="FB" pad="2"/>
<connect gate="A" pin="GND" pad="1"/>
<connect gate="A" pin="IN" pad="4"/>
<connect gate="A" pin="OUT" pad="5"/>
<connect gate="A" pin="SENSE" pad="6"/>
<connect gate="A" pin="TAP" pad="3"/>
<connect gate="A" pin="~ERROR" pad="7"/>
<connect gate="A" pin="~SD" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP2986IMM-3.0"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="07B7183"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="National Smiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP2986IMM-3.3" prefix="U">
<description>Voltage Regulator</description>
<gates>
<gate name="A" symbol="LP2986IMM-3.3"/>
</gates>
<devices>
<device name="" package="SOIC65P490X109-8N">
<connects>
<connect gate="A" pin="FB" pad="2"/>
<connect gate="A" pin="GND" pad="1"/>
<connect gate="A" pin="IN" pad="4"/>
<connect gate="A" pin="OUT" pad="5"/>
<connect gate="A" pin="SENSE" pad="6"/>
<connect gate="A" pin="TAP" pad="3"/>
<connect gate="A" pin="~ERROR" pad="7"/>
<connect gate="A" pin="~SD" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP2986IMM-3.3"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K7030"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="National Smiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP2986IMM-5.0" prefix="U">
<description>Voltage Regulator</description>
<gates>
<gate name="A" symbol="LP2986IMM-5.0"/>
</gates>
<devices>
<device name="" package="SOIC65P490X109-8N">
<connects>
<connect gate="A" pin="FB" pad="2"/>
<connect gate="A" pin="GND" pad="1"/>
<connect gate="A" pin="IN" pad="4"/>
<connect gate="A" pin="OUT" pad="5"/>
<connect gate="A" pin="SENSE" pad="6"/>
<connect gate="A" pin="TAP" pad="3"/>
<connect gate="A" pin="~ERROR" pad="7"/>
<connect gate="A" pin="~SD" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP2986IMM-5.0"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K7031"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="National Smiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP2987AILD-5.0" prefix="U">
<description>Voltage Regulator</description>
<gates>
<gate name="A" symbol="LP2987AILD-5.0"/>
</gates>
<devices>
<device name="" package="DFN400X400X80-9N">
<connects>
<connect gate="A" pin="DELAY" pad="2"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="HEATPAD" pad="9"/>
<connect gate="A" pin="INPUT" pad="4"/>
<connect gate="A" pin="NC" pad="1"/>
<connect gate="A" pin="OUTPUT" pad="5"/>
<connect gate="A" pin="SENSE" pad="6"/>
<connect gate="A" pin="~ERROR" pad="7"/>
<connect gate="A" pin="~SHUTDOWN" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP2987AILD-5.0"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="34C6693"/>
<attribute name="PACKAGE" value="DFN-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP2988AIM-5.0" prefix="U">
<description>Voltage Regulator</description>
<gates>
<gate name="A" symbol="LP2988AIM-5.0"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="BYPASS" pad="1"/>
<connect gate="A" pin="DELAY" pad="2"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="INPUT" pad="4"/>
<connect gate="A" pin="OUTPUT" pad="5"/>
<connect gate="A" pin="SENSE" pad="6"/>
<connect gate="A" pin="~ERROR" pad="7"/>
<connect gate="A" pin="~SHUTDOWN" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP2988AIM-5.0"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K7122"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP2988AIMM-3.0" prefix="U">
<description>Voltage Regulator</description>
<gates>
<gate name="A" symbol="LP2988AIMM-3.0"/>
</gates>
<devices>
<device name="" package="SOP65P490X109-8N">
<connects>
<connect gate="A" pin="BYPASS" pad="1"/>
<connect gate="A" pin="DELAY" pad="2"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="INPUT" pad="4"/>
<connect gate="A" pin="OUTPUT" pad="5"/>
<connect gate="A" pin="SENSE" pad="6"/>
<connect gate="A" pin="~ERROR" pad="7"/>
<connect gate="A" pin="~SHUTDOWN" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP2988AIMM-3.0"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K7125"/>
<attribute name="PACKAGE" value="SOP-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP2988AIMM-3.3" prefix="U">
<description>Voltage Regulator</description>
<gates>
<gate name="A" symbol="LP2988AIMM-3.3"/>
</gates>
<devices>
<device name="" package="SOP65P490X109-8N">
<connects>
<connect gate="A" pin="BYPASS" pad="1"/>
<connect gate="A" pin="DELAY" pad="2"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="INPUT" pad="4"/>
<connect gate="A" pin="OUTPUT" pad="5"/>
<connect gate="A" pin="SENSE" pad="6"/>
<connect gate="A" pin="~ERROR" pad="7"/>
<connect gate="A" pin="~SHUTDOWN" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP2988AIMM-3.3"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K7127"/>
<attribute name="PACKAGE" value="SOP-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP2988AIMM-5.0" prefix="U">
<description>Voltage Regulator</description>
<gates>
<gate name="A" symbol="LP2988AIMM-5.0"/>
</gates>
<devices>
<device name="" package="SOP65P490X109-8N">
<connects>
<connect gate="A" pin="BYPASS" pad="1"/>
<connect gate="A" pin="DELAY" pad="2"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="INPUT" pad="4"/>
<connect gate="A" pin="OUTPUT" pad="5"/>
<connect gate="A" pin="SENSE" pad="6"/>
<connect gate="A" pin="~ERROR" pad="7"/>
<connect gate="A" pin="~SHUTDOWN" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP2988AIMM-5.0"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="07B7216"/>
<attribute name="PACKAGE" value="SOP-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP2988ILD-3.0" prefix="U">
<description>Voltage Regulator</description>
<gates>
<gate name="A" symbol="LP2988ILD-3.0"/>
</gates>
<devices>
<device name="" package="DFN400X400X80-9N">
<connects>
<connect gate="A" pin="BYPASS" pad="1"/>
<connect gate="A" pin="DELAY" pad="2"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="HEATPAD" pad="9"/>
<connect gate="A" pin="INPUT" pad="4"/>
<connect gate="A" pin="OUTPUT" pad="5"/>
<connect gate="A" pin="SENSE" pad="6"/>
<connect gate="A" pin="~ERROR" pad="7"/>
<connect gate="A" pin="~SHUTDOWN" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP2988ILD-3.0"/>
<attribute name="OC_FARNELL" value="4801416"/>
<attribute name="OC_NEWARK" value="-"/>
<attribute name="PACKAGE" value="DFN-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP2988ILD-3.3" prefix="U">
<description>Voltage Regulator</description>
<gates>
<gate name="A" symbol="LP2988ILD-3.3"/>
</gates>
<devices>
<device name="" package="DFN400X400X80-9N">
<connects>
<connect gate="A" pin="BYPASS" pad="1"/>
<connect gate="A" pin="DELAY" pad="2"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="HEATPAD" pad="9"/>
<connect gate="A" pin="INPUT" pad="4"/>
<connect gate="A" pin="OUTPUT" pad="5"/>
<connect gate="A" pin="SENSE" pad="6"/>
<connect gate="A" pin="~ERROR" pad="7"/>
<connect gate="A" pin="~SHUTDOWN" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP2988ILD-3.3"/>
<attribute name="OC_FARNELL" value="4801428"/>
<attribute name="OC_NEWARK" value="-"/>
<attribute name="PACKAGE" value="DFN-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP2988ILD-5.0" prefix="U">
<description>Voltage Regulator</description>
<gates>
<gate name="A" symbol="LP2988ILD-5.0"/>
</gates>
<devices>
<device name="" package="DFN400X400X80-9N">
<connects>
<connect gate="A" pin="BYPASS" pad="1"/>
<connect gate="A" pin="DELAY" pad="2"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="HEATPAD" pad="9"/>
<connect gate="A" pin="INPUT" pad="4"/>
<connect gate="A" pin="OUTPUT" pad="5"/>
<connect gate="A" pin="SENSE" pad="6"/>
<connect gate="A" pin="~ERROR" pad="7"/>
<connect gate="A" pin="~SHUTDOWN" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP2988ILD-5.0"/>
<attribute name="OC_FARNELL" value="4801430"/>
<attribute name="OC_NEWARK" value="-"/>
<attribute name="PACKAGE" value="DFN-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP2988IM-5.0" prefix="U">
<description>Voltage Regulator</description>
<gates>
<gate name="A" symbol="LP2988IM-5.0"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="BYPASS" pad="1"/>
<connect gate="A" pin="DELAY" pad="2"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="INPUT" pad="4"/>
<connect gate="A" pin="OUTPUT" pad="5"/>
<connect gate="A" pin="SENSE" pad="6"/>
<connect gate="A" pin="~ERROR" pad="7"/>
<connect gate="A" pin="~SHUTDOWN" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP2988IM-5.0"/>
<attribute name="OC_FARNELL" value="1179763"/>
<attribute name="OC_NEWARK" value="83F4641"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP2988IMM-3.0" prefix="U">
<description>Voltage Regulator</description>
<gates>
<gate name="A" symbol="LP2988IMM-3.0"/>
</gates>
<devices>
<device name="" package="SOP65P490X109-8N">
<connects>
<connect gate="A" pin="BYPASS" pad="1"/>
<connect gate="A" pin="DELAY" pad="2"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="INPUT" pad="4"/>
<connect gate="A" pin="OUTPUT" pad="5"/>
<connect gate="A" pin="SENSE" pad="6"/>
<connect gate="A" pin="~ERROR" pad="7"/>
<connect gate="A" pin="~SHUTDOWN" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP2988IMM-3.0"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K7165"/>
<attribute name="PACKAGE" value="SOP-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP2988IMM-3.3" prefix="U">
<description>Voltage Regulator</description>
<gates>
<gate name="A" symbol="LP2988IMM-3.3"/>
</gates>
<devices>
<device name="" package="SOP65P490X109-8N">
<connects>
<connect gate="A" pin="BYPASS" pad="1"/>
<connect gate="A" pin="DELAY" pad="2"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="INPUT" pad="4"/>
<connect gate="A" pin="OUTPUT" pad="5"/>
<connect gate="A" pin="SENSE" pad="6"/>
<connect gate="A" pin="~ERROR" pad="7"/>
<connect gate="A" pin="~SHUTDOWN" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP2988IMM-3.3"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K7167"/>
<attribute name="PACKAGE" value="SOP-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP2988IMM-5.0" prefix="U">
<description>Voltage Regulator</description>
<gates>
<gate name="A" symbol="LP2988IMM-5.0"/>
</gates>
<devices>
<device name="" package="SOP65P490X109-8N">
<connects>
<connect gate="A" pin="BYPASS" pad="1"/>
<connect gate="A" pin="DELAY" pad="2"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="INPUT" pad="4"/>
<connect gate="A" pin="OUTPUT" pad="5"/>
<connect gate="A" pin="SENSE" pad="6"/>
<connect gate="A" pin="~ERROR" pad="7"/>
<connect gate="A" pin="~SHUTDOWN" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP2988IMM-5.0"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K7169"/>
<attribute name="PACKAGE" value="SOP-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP2989AILD-3.0" prefix="U">
<description>Low Dropout Regulator</description>
<gates>
<gate name="A" symbol="LP2989AILD-3.0"/>
</gates>
<devices>
<device name="" package="DFN400X400X80-9N">
<connects>
<connect gate="A" pin="BYPASS" pad="1"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="HEATPAD" pad="9"/>
<connect gate="A" pin="INPUT" pad="4"/>
<connect gate="A" pin="NC" pad="2"/>
<connect gate="A" pin="OUTPUT" pad="5"/>
<connect gate="A" pin="SENSE" pad="6"/>
<connect gate="A" pin="~ERROR" pad="7"/>
<connect gate="A" pin="~SHUTDOWN" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP2989AILD-3.0"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="34C6721"/>
<attribute name="PACKAGE" value="DFN-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP2989AILD-3.3" prefix="U">
<description>Low Dropout Regulator</description>
<gates>
<gate name="A" symbol="LP2989AILD-3.3"/>
</gates>
<devices>
<device name="" package="DFN400X400X80-9N">
<connects>
<connect gate="A" pin="BYPASS" pad="1"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="HEATPAD" pad="9"/>
<connect gate="A" pin="INPUT" pad="4"/>
<connect gate="A" pin="NC" pad="2"/>
<connect gate="A" pin="OUTPUT" pad="5"/>
<connect gate="A" pin="SENSE" pad="6"/>
<connect gate="A" pin="~ERROR" pad="7"/>
<connect gate="A" pin="~SHUTDOWN" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP2989AILD-3.3"/>
<attribute name="OC_FARNELL" value="1685519"/>
<attribute name="OC_NEWARK" value="41K7190"/>
<attribute name="PACKAGE" value="DFN-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP2989AILD-5.0" prefix="U">
<description>Low Dropout Regulator</description>
<gates>
<gate name="A" symbol="LP2989AILD-5.0"/>
</gates>
<devices>
<device name="" package="DFN400X400X80-9N">
<connects>
<connect gate="A" pin="BYPASS" pad="1"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="HEATPAD" pad="9"/>
<connect gate="A" pin="INPUT" pad="4"/>
<connect gate="A" pin="NC" pad="2"/>
<connect gate="A" pin="OUTPUT" pad="5"/>
<connect gate="A" pin="SENSE" pad="6"/>
<connect gate="A" pin="~ERROR" pad="7"/>
<connect gate="A" pin="~SHUTDOWN" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP2989AILD-5.0"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K7193"/>
<attribute name="PACKAGE" value="DFN-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP2989AIM-1.8" prefix="U">
<description>Low Dropout Regulator</description>
<gates>
<gate name="A" symbol="LP2989AIM-1.8"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="BYPASS" pad="1"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="INPUT" pad="4"/>
<connect gate="A" pin="NC" pad="2"/>
<connect gate="A" pin="OUTPUT" pad="5"/>
<connect gate="A" pin="SENSE" pad="6"/>
<connect gate="A" pin="~ERROR" pad="7"/>
<connect gate="A" pin="~SHUTDOWN" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP2989AIM-1.8"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K7203"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP2989AIM-2.5" prefix="U">
<description>Low Dropout Regulator</description>
<gates>
<gate name="A" symbol="LP2989AIM-2.5"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="BYPASS" pad="1"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="INPUT" pad="4"/>
<connect gate="A" pin="NC" pad="2"/>
<connect gate="A" pin="OUTPUT" pad="5"/>
<connect gate="A" pin="SENSE" pad="6"/>
<connect gate="A" pin="~ERROR" pad="7"/>
<connect gate="A" pin="~SHUTDOWN" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP2989AIM-2.5"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="74C5261"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP2989AIM-3.3" prefix="U">
<description>Low Dropout Regulator</description>
<gates>
<gate name="A" symbol="LP2989AIM-3.3"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="BYPASS" pad="1"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="INPUT" pad="4"/>
<connect gate="A" pin="NC" pad="2"/>
<connect gate="A" pin="OUTPUT" pad="5"/>
<connect gate="A" pin="SENSE" pad="6"/>
<connect gate="A" pin="~ERROR" pad="7"/>
<connect gate="A" pin="~SHUTDOWN" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP2989AIM-3.3"/>
<attribute name="OC_FARNELL" value="1685686"/>
<attribute name="OC_NEWARK" value="41K7206"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP2989AIM-5.0" prefix="U">
<description>Ultra Low-Dropout Regulator</description>
<gates>
<gate name="A" symbol="LP2989AIM-5.0"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="BYPASS" pad="1"/>
<connect gate="A" pin="GROUND" pad="3"/>
<connect gate="A" pin="INPUT" pad="4"/>
<connect gate="A" pin="N/C" pad="2"/>
<connect gate="A" pin="OUTPUT" pad="5"/>
<connect gate="A" pin="SENSE" pad="6"/>
<connect gate="A" pin="~ERROR" pad="7"/>
<connect gate="A" pin="~SHUTDOWN" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP2989AIM-5.0"/>
<attribute name="OC_FARNELL" value="7614664"/>
<attribute name="OC_NEWARK" value="74C5263"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP2989AIMM-3.3" prefix="U">
<description>Low Dropout Regulator</description>
<gates>
<gate name="A" symbol="LP2989AIMM-3.3"/>
</gates>
<devices>
<device name="" package="SOP65P490X109-8N">
<connects>
<connect gate="A" pin="BYPASS" pad="1"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="INPUT" pad="4"/>
<connect gate="A" pin="NC" pad="2"/>
<connect gate="A" pin="OUTPUT" pad="5"/>
<connect gate="A" pin="SENSE" pad="6"/>
<connect gate="A" pin="~ERROR" pad="7"/>
<connect gate="A" pin="~SHUTDOWN" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP2989AIMM-3.3"/>
<attribute name="OC_FARNELL" value="1685687"/>
<attribute name="OC_NEWARK" value="41K7212"/>
<attribute name="PACKAGE" value="SOP-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP2989AIMM-5.0" prefix="U">
<description>Low Dropout Regulator</description>
<gates>
<gate name="A" symbol="LP2989AIMM-5.0"/>
</gates>
<devices>
<device name="" package="SOP65P490X109-8N">
<connects>
<connect gate="A" pin="BYPASS" pad="1"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="INPUT" pad="4"/>
<connect gate="A" pin="NC" pad="2"/>
<connect gate="A" pin="OUTPUT" pad="5"/>
<connect gate="A" pin="SENSE" pad="6"/>
<connect gate="A" pin="~ERROR" pad="7"/>
<connect gate="A" pin="~SHUTDOWN" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP2989AIMM-5.0"/>
<attribute name="OC_FARNELL" value="1685688"/>
<attribute name="OC_NEWARK" value="41K7213"/>
<attribute name="PACKAGE" value="SOP-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP2989ILD-3.0" prefix="U">
<description>Low Dropout Regulator</description>
<gates>
<gate name="A" symbol="LP2989ILD-3.0"/>
</gates>
<devices>
<device name="" package="DFN400X400X80-9N">
<connects>
<connect gate="A" pin="BYPASS" pad="1"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="HEATPAD" pad="9"/>
<connect gate="A" pin="INPUT" pad="4"/>
<connect gate="A" pin="NC" pad="2"/>
<connect gate="A" pin="OUTPUT" pad="5"/>
<connect gate="A" pin="SENSE" pad="6"/>
<connect gate="A" pin="~ERROR" pad="7"/>
<connect gate="A" pin="~SHUTDOWN" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP2989ILD-3.0"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="34C6733"/>
<attribute name="PACKAGE" value="DFN-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP2989ILD-3.3" prefix="U">
<description>Low Dropout Regulator</description>
<gates>
<gate name="A" symbol="LP2989ILD-3.3"/>
</gates>
<devices>
<device name="" package="DFN400X400X80-9N">
<connects>
<connect gate="A" pin="BYPASS" pad="1"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="HEATPAD" pad="9"/>
<connect gate="A" pin="INPUT" pad="4"/>
<connect gate="A" pin="NC" pad="2"/>
<connect gate="A" pin="OUTPUT" pad="5"/>
<connect gate="A" pin="SENSE" pad="6"/>
<connect gate="A" pin="~ERROR" pad="7"/>
<connect gate="A" pin="~SHUTDOWN" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP2989ILD-3.3"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="34C6734"/>
<attribute name="PACKAGE" value="DFN-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP2989IM-1.8" prefix="U">
<description>Low Dropout Regulator</description>
<gates>
<gate name="A" symbol="LP2989IM-1.8"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="BYPASS" pad="1"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="INPUT" pad="4"/>
<connect gate="A" pin="NC" pad="2"/>
<connect gate="A" pin="OUTPUT" pad="5"/>
<connect gate="A" pin="SENSE" pad="6"/>
<connect gate="A" pin="~ERROR" pad="7"/>
<connect gate="A" pin="~SHUTDOWN" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP2989IM-1.8"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="74C5284"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP2989IM-2.5" prefix="U">
<description>Low-Dropout Regulator</description>
<gates>
<gate name="A" symbol="LP2989IM-2.5"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="BYPASS" pad="1"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="NC" pad="2"/>
<connect gate="A" pin="SENSE" pad="6"/>
<connect gate="A" pin="VIN" pad="4"/>
<connect gate="A" pin="VOUT" pad="5"/>
<connect gate="A" pin="~ERROR" pad="7"/>
<connect gate="A" pin="~SD" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP2989IM-2.5"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K7244"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP2989IM-3.3" prefix="U">
<description>Low-Dropout Regulator</description>
<gates>
<gate name="A" symbol="LP2989IM-3.3"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="BYPASS" pad="1"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="NC" pad="2"/>
<connect gate="A" pin="SENSE" pad="6"/>
<connect gate="A" pin="VIN" pad="4"/>
<connect gate="A" pin="VOUT" pad="5"/>
<connect gate="A" pin="~ERROR" pad="7"/>
<connect gate="A" pin="~SD" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP2989IM-3.3"/>
<attribute name="OC_FARNELL" value="1652324"/>
<attribute name="OC_NEWARK" value="41K7246"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP2989IM-5.0" prefix="U">
<description>Low-Dropout Regulator</description>
<gates>
<gate name="A" symbol="LP2989IM-5.0"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="BYPASS" pad="1"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="NC" pad="2"/>
<connect gate="A" pin="SENSE" pad="6"/>
<connect gate="A" pin="VIN" pad="4"/>
<connect gate="A" pin="VOUT" pad="5"/>
<connect gate="A" pin="~ERROR" pad="7"/>
<connect gate="A" pin="~SD" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP2989IM-5.0"/>
<attribute name="OC_FARNELL" value="1685689"/>
<attribute name="OC_NEWARK" value="41K7247"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP2989IMM-3.0" prefix="U">
<description>Low Dropout Regulator</description>
<gates>
<gate name="A" symbol="LP2989IMM-3.0"/>
</gates>
<devices>
<device name="" package="SOP65P490X109-8N">
<connects>
<connect gate="A" pin="BYPASS" pad="1"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="INPUT" pad="4"/>
<connect gate="A" pin="NC" pad="2"/>
<connect gate="A" pin="OUTPUT" pad="5"/>
<connect gate="A" pin="SENSE" pad="6"/>
<connect gate="A" pin="~ERROR" pad="7"/>
<connect gate="A" pin="~SHUTDOWN" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP2989IMM-3.0"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K7251"/>
<attribute name="PACKAGE" value="SOP-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP2989IMM-3.3" prefix="U">
<description>Low Dropout Regulator</description>
<gates>
<gate name="A" symbol="LP2989IMM-3.3"/>
</gates>
<devices>
<device name="" package="SOP65P490X109-8N">
<connects>
<connect gate="A" pin="BYPASS" pad="1"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="INPUT" pad="4"/>
<connect gate="A" pin="NC" pad="2"/>
<connect gate="A" pin="OUTPUT" pad="5"/>
<connect gate="A" pin="SENSE" pad="6"/>
<connect gate="A" pin="~ERROR" pad="7"/>
<connect gate="A" pin="~SHUTDOWN" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP2989IMM-3.3"/>
<attribute name="OC_FARNELL" value="1685549"/>
<attribute name="OC_NEWARK" value="41K7252"/>
<attribute name="PACKAGE" value="SOP-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP2989IMM-5.0" prefix="U">
<description>Low Dropout Regulator</description>
<gates>
<gate name="A" symbol="LP2989IMM-5.0"/>
</gates>
<devices>
<device name="" package="SOP65P490X109-8N">
<connects>
<connect gate="A" pin="BYPASS" pad="1"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="INPUT" pad="4"/>
<connect gate="A" pin="NC" pad="2"/>
<connect gate="A" pin="OUTPUT" pad="5"/>
<connect gate="A" pin="SENSE" pad="6"/>
<connect gate="A" pin="~ERROR" pad="7"/>
<connect gate="A" pin="~SHUTDOWN" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP2989IMM-5.0"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K7253"/>
<attribute name="PACKAGE" value="SOP-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP2992AILD-3.3" prefix="U">
<description>IC, LDO VOLT REG</description>
<gates>
<gate name="A" symbol="LP2992AILD-3.3"/>
</gates>
<devices>
<device name="" package="DFN329X292X80-7N">
<connects>
<connect gate="A" pin="BYP" pad="1"/>
<connect gate="A" pin="EPAD" pad="7"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="NC" pad="5"/>
<connect gate="A" pin="ON/~OFF" pad="3"/>
<connect gate="A" pin="VIN" pad="4"/>
<connect gate="A" pin="VOUT" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP2992AILD-33"/>
<attribute name="OC_FARNELL" value="1685690"/>
<attribute name="OC_NEWARK" value="41K7268"/>
<attribute name="PACKAGE" value="DFN-6"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP2992AILD-5.0" prefix="U">
<description>IC, LDO VOLT REG</description>
<gates>
<gate name="A" symbol="LP2992AILD-5.0"/>
</gates>
<devices>
<device name="" package="DFN329X292X80-7N">
<connects>
<connect gate="A" pin="BYP" pad="1"/>
<connect gate="A" pin="EPAD" pad="7"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="NC" pad="5"/>
<connect gate="A" pin="ON/~OFF" pad="3"/>
<connect gate="A" pin="VIN" pad="4"/>
<connect gate="A" pin="VOUT" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP2992AILD-5.0"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K7269"/>
<attribute name="PACKAGE" value="DFN-6"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP2992AIM5-1.5" prefix="U">
<description>Low-Dropout Regulator</description>
<gates>
<gate name="A" symbol="LP2992AIM5-1.5"/>
</gates>
<devices>
<device name="" package="SOT95P284X122-5N">
<connects>
<connect gate="A" pin="BYPASS" pad="4"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="ON/~OFF" pad="3"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="VOUT" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP2992AIM5-1.5"/>
<attribute name="OC_FARNELL" value="1469138"/>
<attribute name="OC_NEWARK" value="41K7275"/>
<attribute name="PACKAGE" value="SOT23-5"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP2992AIM5-1.8" prefix="U">
<description>Low-Dropout Regulator</description>
<gates>
<gate name="A" symbol="LP2992AIM5-1.8"/>
</gates>
<devices>
<device name="" package="SOT95P284X122-5N">
<connects>
<connect gate="A" pin="BYPASS" pad="4"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="ON/~OFF" pad="3"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="VOUT" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP2992AIM5-1.8"/>
<attribute name="OC_FARNELL" value="1685691"/>
<attribute name="OC_NEWARK" value="41K7276"/>
<attribute name="PACKAGE" value="SOT23-5"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP2992AIM5-2.5" prefix="U">
<description>Low-Dropout Regulator</description>
<gates>
<gate name="A" symbol="LP2992AIM5-2.5"/>
</gates>
<devices>
<device name="" package="SOT95P284X122-5N">
<connects>
<connect gate="A" pin="BYPASS" pad="4"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="ON/~OFF" pad="3"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="VOUT" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP2992AIM5-2.5"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K7277"/>
<attribute name="PACKAGE" value="SOT23-5"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP2992AIM5-3.3" prefix="U">
<description>Low-Dropout Regulator</description>
<gates>
<gate name="A" symbol="LP2992AIM5-3.3"/>
</gates>
<devices>
<device name="" package="SOT95P284X122-5N">
<connects>
<connect gate="A" pin="BYPASS" pad="4"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="ON/~OFF" pad="3"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="VOUT" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP2992AIM5-3.3"/>
<attribute name="OC_FARNELL" value="1469139"/>
<attribute name="OC_NEWARK" value="74C5317"/>
<attribute name="PACKAGE" value="SOT23-5"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP2992AIM5-5.0" prefix="U">
<description>Low-Dropout Regulator</description>
<gates>
<gate name="A" symbol="LP2992AIM5-5.0"/>
</gates>
<devices>
<device name="" package="SOT95P284X122-5N">
<connects>
<connect gate="A" pin="BYPASS" pad="4"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="ON/~OFF" pad="3"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="VOUT" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP2992AIM5-5.0"/>
<attribute name="OC_FARNELL" value="1685561"/>
<attribute name="OC_NEWARK" value="41K7280"/>
<attribute name="PACKAGE" value="SOT23-5"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP2992ILD-3.3" prefix="U">
<description>Low-Dropout Regulator</description>
<gates>
<gate name="A" symbol="LP2992ILD-3.3"/>
</gates>
<devices>
<device name="" package="DFN292X329X80-7N">
<connects>
<connect gate="A" pin="BYPASS" pad="1"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="HEATPAD" pad="7"/>
<connect gate="A" pin="NC" pad="5"/>
<connect gate="A" pin="ON/~OFF" pad="3"/>
<connect gate="A" pin="VIN" pad="4"/>
<connect gate="A" pin="VOUT" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP2992ILD-3.3"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K7290"/>
<attribute name="PACKAGE" value="DFN-6"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP2992ILD-5.0" prefix="U">
<description>Low-Dropout Regulator</description>
<gates>
<gate name="A" symbol="LP2992ILD-5.0"/>
</gates>
<devices>
<device name="" package="DFN292X329X80-7N">
<connects>
<connect gate="A" pin="BYPASS" pad="1"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="HEATPAD" pad="7"/>
<connect gate="A" pin="NC" pad="5"/>
<connect gate="A" pin="ON/~OFF" pad="3"/>
<connect gate="A" pin="VIN" pad="4"/>
<connect gate="A" pin="VOUT" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP2992ILD-5.0"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K7291"/>
<attribute name="PACKAGE" value="DFN-6"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP2992IM5-1.5" prefix="U">
<description>Low-Dropout Regulator</description>
<gates>
<gate name="A" symbol="LP2992IM5-1.5"/>
</gates>
<devices>
<device name="" package="SOT95P284X122-5N">
<connects>
<connect gate="A" pin="BYPASS" pad="4"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="ON/~OFF" pad="3"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="VOUT" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP2992IM5-1.5"/>
<attribute name="OC_FARNELL" value="1685694"/>
<attribute name="OC_NEWARK" value="41K7297"/>
<attribute name="PACKAGE" value="SOT23-5"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP2992IM5-1.8" prefix="U">
<description>Low-Dropout Regulator</description>
<gates>
<gate name="A" symbol="LP2992IM5-1.8"/>
</gates>
<devices>
<device name="" package="SOT95P284X122-5N">
<connects>
<connect gate="A" pin="BYPASS" pad="4"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="ON/~OFF" pad="3"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="VOUT" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP2992IM5-1.8"/>
<attribute name="OC_FARNELL" value="1469140"/>
<attribute name="OC_NEWARK" value="41K7298"/>
<attribute name="PACKAGE" value="SOT23-5"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP2992IM5-2.5" prefix="U">
<description>Low-Dropout Regulator</description>
<gates>
<gate name="A" symbol="LP2992IM5-2.5"/>
</gates>
<devices>
<device name="" package="SOT95P284X122-5N">
<connects>
<connect gate="A" pin="BYPASS" pad="4"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="ON/~OFF" pad="3"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="VOUT" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP2992IM5-2.5"/>
<attribute name="OC_FARNELL" value="1685695"/>
<attribute name="OC_NEWARK" value="41K7299"/>
<attribute name="PACKAGE" value="SOT23-5"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP2992IM5-3.0" prefix="U">
<description>Low-Dropout Regulator</description>
<gates>
<gate name="A" symbol="LP2992IM5-3.0"/>
</gates>
<devices>
<device name="" package="SOT95P284X122-5N">
<connects>
<connect gate="A" pin="BYPASS" pad="4"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="ON/~OFF" pad="3"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="VOUT" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP2992IM5-3.0"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K7300"/>
<attribute name="PACKAGE" value="SOT23-5"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP2992IM5-3.3" prefix="U">
<description>Low-Dropout Regulator</description>
<gates>
<gate name="A" symbol="LP2992IM5-3.3"/>
</gates>
<devices>
<device name="" package="SOT95P284X122-5N">
<connects>
<connect gate="A" pin="BYPASS" pad="4"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="ON/~OFF" pad="3"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="VOUT" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP2992IM5-3.3"/>
<attribute name="OC_FARNELL" value="1469141"/>
<attribute name="OC_NEWARK" value="41K7301"/>
<attribute name="PACKAGE" value="SOT23-5"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP2992IM5-5.0" prefix="U">
<description>Low-Dropout Regulator</description>
<gates>
<gate name="A" symbol="LP2992IM5-5.0"/>
</gates>
<devices>
<device name="" package="SOT95P284X122-5N">
<connects>
<connect gate="A" pin="BYPASS" pad="4"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="ON/~OFF" pad="3"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="VOUT" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP2992IM5-5.0"/>
<attribute name="OC_FARNELL" value="1469142"/>
<attribute name="OC_NEWARK" value="41K7302"/>
<attribute name="PACKAGE" value="SOT23-5"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP2995M" prefix="U">
<description>LDO</description>
<gates>
<gate name="A" symbol="LP2995M"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="AVIN" pad="6"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="NC" pad="1"/>
<connect gate="A" pin="PVIN" pad="7"/>
<connect gate="A" pin="VDDQ" pad="5"/>
<connect gate="A" pin="VREF" pad="4"/>
<connect gate="A" pin="VSENSE" pad="3"/>
<connect gate="A" pin="VTT" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP2995M"/>
<attribute name="OC_FARNELL" value="41K7313"/>
<attribute name="OC_NEWARK" value="1286958"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP2995MR" prefix="U">
<description>Termination Regulator</description>
<gates>
<gate name="A" symbol="LP2995MR"/>
</gates>
<devices>
<device name="" package="SOIC127P620X168-9N">
<connects>
<connect gate="A" pin="AVIN" pad="6"/>
<connect gate="A" pin="EPAD" pad="9"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="NC" pad="1"/>
<connect gate="A" pin="PVIN" pad="7"/>
<connect gate="A" pin="VDDQ" pad="5"/>
<connect gate="A" pin="VREF" pad="4"/>
<connect gate="A" pin="VSENSE" pad="3"/>
<connect gate="A" pin="VTT" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP2995MR"/>
<attribute name="OC_FARNELL" value="1654324"/>
<attribute name="OC_NEWARK" value="41K7314"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP2996LQ" prefix="U">
<description>Termination Regulator</description>
<gates>
<gate name="A" symbol="LP2996LQ"/>
</gates>
<devices>
<device name="" package="QFN50P400X400X80-17N">
<connects>
<connect gate="A" pin="AVIN" pad="10"/>
<connect gate="A" pin="EPAD" pad="17"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="NC" pad="16"/>
<connect gate="A" pin="NC_2" pad="3"/>
<connect gate="A" pin="NC_3" pad="6"/>
<connect gate="A" pin="NC_4" pad="1"/>
<connect gate="A" pin="NC_5" pad="9"/>
<connect gate="A" pin="NC_6" pad="13"/>
<connect gate="A" pin="PVIN" pad="12"/>
<connect gate="A" pin="PVIN_2" pad="11"/>
<connect gate="A" pin="VDDQ" pad="8"/>
<connect gate="A" pin="VREF" pad="7"/>
<connect gate="A" pin="VSENSE" pad="5"/>
<connect gate="A" pin="VTT" pad="15"/>
<connect gate="A" pin="VTT_2" pad="14"/>
<connect gate="A" pin="~SD" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP2996LQ"/>
<attribute name="OC_FARNELL" value="41K7317"/>
<attribute name="OC_NEWARK" value="1559602"/>
<attribute name="PACKAGE" value="QFN-16"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP2996M" prefix="U">
<description>DDR Termination Regulator</description>
<gates>
<gate name="A" symbol="LP2996M"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="AVIN" pad="6"/>
<connect gate="A" pin="GND" pad="1"/>
<connect gate="A" pin="PVIN" pad="7"/>
<connect gate="A" pin="VDDQ" pad="5"/>
<connect gate="A" pin="VREF" pad="4"/>
<connect gate="A" pin="VSEN" pad="3"/>
<connect gate="A" pin="VTT" pad="8"/>
<connect gate="A" pin="~SD" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP2996M"/>
<attribute name="OC_FARNELL" value="1286960"/>
<attribute name="OC_NEWARK" value="26M0447"/>
<attribute name="PACKAGE" value="8-SOIC"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP2996MR" prefix="U">
<description>DDR Termination Regulator</description>
<gates>
<gate name="A" symbol="LP2996MR"/>
</gates>
<devices>
<device name="" package="SOIC127P620X168-9N">
<connects>
<connect gate="A" pin="AVIN" pad="6"/>
<connect gate="A" pin="EPAD" pad="9"/>
<connect gate="A" pin="GND" pad="1"/>
<connect gate="A" pin="PVIN" pad="7"/>
<connect gate="A" pin="VDDQ" pad="5"/>
<connect gate="A" pin="VREF" pad="4"/>
<connect gate="A" pin="VSENSE" pad="3"/>
<connect gate="A" pin="VTT" pad="8"/>
<connect gate="A" pin="~SD" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP2996MR"/>
<attribute name="OC_FARNELL" value="1286962"/>
<attribute name="OC_NEWARK" value="26M0448"/>
<attribute name="PACKAGE" value="PSOP-8"/>
<attribute name="SUPPLIER" value="NATIONAL SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP2997M" prefix="U">
<description>Terminator Regulator</description>
<gates>
<gate name="A" symbol="LP2997M"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="AVIN" pad="6"/>
<connect gate="A" pin="GND" pad="1"/>
<connect gate="A" pin="PVIN" pad="7"/>
<connect gate="A" pin="VDDQ" pad="5"/>
<connect gate="A" pin="VREF" pad="4"/>
<connect gate="A" pin="VSEN" pad="3"/>
<connect gate="A" pin="VTT" pad="8"/>
<connect gate="A" pin="~SD" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP2997M"/>
<attribute name="OC_FARNELL" value="1008283"/>
<attribute name="OC_NEWARK" value="41K7323"/>
<attribute name="PACKAGE" value="8-SOIC"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP2997MR" prefix="U">
<description>Termination Regulator</description>
<gates>
<gate name="A" symbol="LP2997MR"/>
</gates>
<devices>
<device name="" package="SOIC127P600X168-9N">
<connects>
<connect gate="A" pin="AVIN" pad="6"/>
<connect gate="A" pin="GND" pad="1"/>
<connect gate="A" pin="GND_2" pad="9"/>
<connect gate="A" pin="PVIN" pad="7"/>
<connect gate="A" pin="VDDQ" pad="5"/>
<connect gate="A" pin="VREF" pad="4"/>
<connect gate="A" pin="VSEN" pad="3"/>
<connect gate="A" pin="VTT" pad="8"/>
<connect gate="A" pin="~SD" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP2997MR"/>
<attribute name="OC_FARNELL" value="1286963"/>
<attribute name="OC_NEWARK" value="24M3586"/>
<attribute name="PACKAGE" value="SOP-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP2998MA" prefix="U">
<description>Termination Regulator</description>
<gates>
<gate name="A" symbol="LP2998MA"/>
</gates>
<devices>
<device name="" package="SOIC127P620X175-8N">
<connects>
<connect gate="A" pin="AVIN" pad="6"/>
<connect gate="A" pin="GND" pad="1"/>
<connect gate="A" pin="PVIN" pad="7"/>
<connect gate="A" pin="VDDQ" pad="5"/>
<connect gate="A" pin="VREF" pad="4"/>
<connect gate="A" pin="VSEN" pad="3"/>
<connect gate="A" pin="VTT" pad="8"/>
<connect gate="A" pin="~SD" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP2998MA"/>
<attribute name="OC_FARNELL" value="1542532"/>
<attribute name="OC_NEWARK" value="75M6036"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP2998MR" prefix="U">
<description>Termination Regulator</description>
<gates>
<gate name="A" symbol="LP2998MR"/>
</gates>
<devices>
<device name="" package="SOIC127P620X168-9N">
<connects>
<connect gate="A" pin="AVIN" pad="6"/>
<connect gate="A" pin="EP" pad="9"/>
<connect gate="A" pin="GND" pad="1"/>
<connect gate="A" pin="PVIN" pad="7"/>
<connect gate="A" pin="VDDQ" pad="5"/>
<connect gate="A" pin="VREF" pad="4"/>
<connect gate="A" pin="VSEN" pad="3"/>
<connect gate="A" pin="VTT" pad="8"/>
<connect gate="A" pin="~SD" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP2998MR"/>
<attribute name="OC_FARNELL" value="1542533"/>
<attribute name="OC_NEWARK" value="84M8159"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP324M" prefix="U">
<description>OpAmpIC</description>
<gates>
<gate name="A" symbol="LP324M"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="+IN1" pad="3"/>
<connect gate="A" pin="+IN2" pad="5"/>
<connect gate="A" pin="+IN3" pad="10"/>
<connect gate="A" pin="+IN4" pad="12"/>
<connect gate="A" pin="-IN1" pad="2"/>
<connect gate="A" pin="-IN2" pad="6"/>
<connect gate="A" pin="-IN3" pad="9"/>
<connect gate="A" pin="-IN4" pad="13"/>
<connect gate="A" pin="GND" pad="11"/>
<connect gate="A" pin="OUT1" pad="1"/>
<connect gate="A" pin="OUT2" pad="7"/>
<connect gate="A" pin="OUT3" pad="8"/>
<connect gate="A" pin="OUT4" pad="14"/>
<connect gate="A" pin="V+" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP324M"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K7327"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP324MT" prefix="U">
<description>LP324MT</description>
<gates>
<gate name="A" symbol="LP324MT"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-14N">
<connects>
<connect gate="A" pin="+INA" pad="3"/>
<connect gate="A" pin="+INB" pad="5"/>
<connect gate="A" pin="+INC" pad="10"/>
<connect gate="A" pin="+IND" pad="12"/>
<connect gate="A" pin="-INA" pad="2"/>
<connect gate="A" pin="-INB" pad="6"/>
<connect gate="A" pin="-INC" pad="9"/>
<connect gate="A" pin="-IND" pad="13"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="OUTC" pad="8"/>
<connect gate="A" pin="OUTD" pad="14"/>
<connect gate="A" pin="V+" pad="4"/>
<connect gate="A" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP324MT"/>
<attribute name="OC_FARNELL" value="41K7328"/>
<attribute name="OC_NEWARK" value="-"/>
<attribute name="PACKAGE" value="TSSOP-14"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP324N" prefix="U">
<description>Micropower Quad Operational Amplifier</description>
<gates>
<gate name="A" symbol="LP324N"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-14">
<connects>
<connect gate="A" pin="+IN1" pad="3"/>
<connect gate="A" pin="+IN2" pad="5"/>
<connect gate="A" pin="+IN3" pad="10"/>
<connect gate="A" pin="+IN4" pad="12"/>
<connect gate="A" pin="-IN1" pad="2"/>
<connect gate="A" pin="-IN2" pad="6"/>
<connect gate="A" pin="-IN3" pad="9"/>
<connect gate="A" pin="-IN4" pad="13"/>
<connect gate="A" pin="GND" pad="11"/>
<connect gate="A" pin="OUT1" pad="1"/>
<connect gate="A" pin="OUT2" pad="7"/>
<connect gate="A" pin="OUT3" pad="8"/>
<connect gate="A" pin="OUT4" pad="14"/>
<connect gate="A" pin="V+" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP324N"/>
<attribute name="OC_FARNELL" value="9486950"/>
<attribute name="OC_NEWARK" value="41K7331"/>
<attribute name="PACKAGE" value="DIP-14"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP339M" prefix="U">
<description>Quad Comparator</description>
<gates>
<gate name="A" symbol="LP339M"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="GND" pad="12"/>
<connect gate="A" pin="IN1+" pad="5"/>
<connect gate="A" pin="IN1-" pad="4"/>
<connect gate="A" pin="IN2+" pad="7"/>
<connect gate="A" pin="IN2-" pad="6"/>
<connect gate="A" pin="IN3+" pad="9"/>
<connect gate="A" pin="IN3-" pad="8"/>
<connect gate="A" pin="IN4+" pad="11"/>
<connect gate="A" pin="IN4-" pad="10"/>
<connect gate="A" pin="OUT1" pad="2"/>
<connect gate="A" pin="OUT2" pad="1"/>
<connect gate="A" pin="OUT3" pad="14"/>
<connect gate="A" pin="OUT4" pad="13"/>
<connect gate="A" pin="V+" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP339M"/>
<attribute name="OC_FARNELL" value="9487662"/>
<attribute name="OC_NEWARK" value="41K7332"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP339N" prefix="U">
<description>LP339N</description>
<gates>
<gate name="A" symbol="LP339N"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-14">
<connects>
<connect gate="A" pin="+IN1" pad="5"/>
<connect gate="A" pin="+IN2" pad="7"/>
<connect gate="A" pin="+IN3" pad="9"/>
<connect gate="A" pin="+IN4" pad="11"/>
<connect gate="A" pin="-IN1" pad="4"/>
<connect gate="A" pin="-IN2" pad="6"/>
<connect gate="A" pin="-IN3" pad="8"/>
<connect gate="A" pin="-IN4" pad="10"/>
<connect gate="A" pin="GND" pad="12"/>
<connect gate="A" pin="OUT1" pad="2"/>
<connect gate="A" pin="OUT2" pad="1"/>
<connect gate="A" pin="OUT3" pad="14"/>
<connect gate="A" pin="OUT4" pad="13"/>
<connect gate="A" pin="V+" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP339N"/>
<attribute name="OC_FARNELL" value="9490477"/>
<attribute name="OC_NEWARK" value="-"/>
<attribute name="PACKAGE" value="DIP-14"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3470M5-2.63" prefix="U">
<description>Tiny Power On Reset Circuit</description>
<gates>
<gate name="A" symbol="LP3470M5-2.63"/>
</gates>
<devices>
<device name="" package="SOT95P285X120-5N">
<connects>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="SRT" pad="1"/>
<connect gate="A" pin="VCC" pad="4"/>
<connect gate="A" pin="VCC1" pad="3"/>
<connect gate="A" pin="~RESET" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3470M5-2.63"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K7351"/>
<attribute name="PACKAGE" value="SOT23-5"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3470M5-2.93" prefix="U">
<description>Tiny Power On Reset Circuit</description>
<gates>
<gate name="A" symbol="LP3470M5-2.93"/>
</gates>
<devices>
<device name="" package="SOT95P285X120-5N">
<connects>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="SRT" pad="1"/>
<connect gate="A" pin="VCC" pad="4"/>
<connect gate="A" pin="VCC1" pad="3"/>
<connect gate="A" pin="~RESET" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3470M5-2.93"/>
<attribute name="OC_FARNELL" value="7593340"/>
<attribute name="OC_NEWARK" value="07B7252"/>
<attribute name="PACKAGE" value="SOT-23-5"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3470M5-3.08" prefix="U">
<description>CIRCUIT RESET PWR</description>
<gates>
<gate name="A" symbol="LP3470M5-3.08"/>
</gates>
<devices>
<device name="" package="SOT95P284X119-5N">
<connects>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="SRT" pad="1"/>
<connect gate="A" pin="VCC" pad="4"/>
<connect gate="A" pin="VCC1" pad="3"/>
<connect gate="A" pin="~RESET" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3470M5-3.08"/>
<attribute name="OC_FARNELL" value="1652458"/>
<attribute name="OC_NEWARK" value="07B7253"/>
<attribute name="PACKAGE" value="SOT23-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3470M5-4.63" prefix="U">
<description>CIRCUIT RESET PWR</description>
<gates>
<gate name="A" symbol="LP3470M5-4.63"/>
</gates>
<devices>
<device name="" package="SOT95P284X119-5N">
<connects>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="SRT" pad="1"/>
<connect gate="A" pin="VCC" pad="4"/>
<connect gate="A" pin="VCC1" pad="3"/>
<connect gate="A" pin="~RESET" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3470M5-4.63"/>
<attribute name="OC_FARNELL" value="1652459"/>
<attribute name="OC_NEWARK" value="07B7256"/>
<attribute name="PACKAGE" value="SOT23-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP38511MR-ADJ" prefix="U">
<description>Linear Voltage Regulator</description>
<gates>
<gate name="A" symbol="LP38511MR-ADJ"/>
</gates>
<devices>
<device name="" package="SOIC127P600X168-8N">
<connects>
<connect gate="A" pin="ADJ" pad="3"/>
<connect gate="A" pin="EN" pad="6"/>
<connect gate="A" pin="EP" pad="9"/>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="IN" pad="8"/>
<connect gate="A" pin="IN_2" pad="7"/>
<connect gate="A" pin="NC" pad="4"/>
<connect gate="A" pin="OUT" pad="2"/>
<connect gate="A" pin="OUT_2" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP38511MR-ADJ"/>
<attribute name="OC_FARNELL" value="1714824"/>
<attribute name="OC_NEWARK" value="10R2193"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP38511TJ-ADJ" prefix="U">
<description>IC REG LDO 800MA ADJ</description>
<gates>
<gate name="A" symbol="LP38511TJ-ADJ"/>
</gates>
<devices>
<device name="" package="TO170P1436X210-6N">
<connects>
<connect gate="A" pin="ADJ" pad="5"/>
<connect gate="A" pin="DAP" pad="6"/>
<connect gate="A" pin="EN" pad="1"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="IN" pad="2"/>
<connect gate="A" pin="OUT" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP38511TJ-ADJ"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="04R9329"/>
<attribute name="PACKAGE" value="TO263-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP38512MR-ADJ" prefix="U">
<description>Linear Voltage Regulator</description>
<gates>
<gate name="A" symbol="LP38512MR-ADJ"/>
</gates>
<devices>
<device name="" package="SOIC127P600X168-8N">
<connects>
<connect gate="A" pin="ADJ" pad="3"/>
<connect gate="A" pin="EN" pad="6"/>
<connect gate="A" pin="EP" pad="9"/>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="IN" pad="8"/>
<connect gate="A" pin="IN_2" pad="7"/>
<connect gate="A" pin="NC" pad="4"/>
<connect gate="A" pin="OUT" pad="2"/>
<connect gate="A" pin="OUT_2" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP38512MR-ADJ"/>
<attribute name="OC_FARNELL" value="1714825"/>
<attribute name="OC_NEWARK" value="10R2194"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP38512TJ-ADJ" prefix="U">
<description>IC REG LDO 1.5A ADJ</description>
<gates>
<gate name="A" symbol="LP38512TJ-ADJ"/>
</gates>
<devices>
<device name="" package="TO170P1436X210-6N">
<connects>
<connect gate="A" pin="ADJ" pad="5"/>
<connect gate="A" pin="DAP" pad="6"/>
<connect gate="A" pin="EN" pad="1"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="IN" pad="2"/>
<connect gate="A" pin="OUT" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP38512TJ-ADJ"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="04R9331"/>
<attribute name="PACKAGE" value="TO263-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP38512TS-1.8" prefix="U">
<description>Linear Voltage Regulator</description>
<gates>
<gate name="A" symbol="LP38512TS-1.8"/>
</gates>
<devices>
<device name="" package="TO170P1435X465-6N">
<connects>
<connect gate="A" pin="EN" pad="1"/>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="GND_2" pad="3"/>
<connect gate="A" pin="IN" pad="2"/>
<connect gate="A" pin="OUT" pad="4"/>
<connect gate="A" pin="~ERR" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP38512TS-1.8"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="64M7072"/>
<attribute name="PACKAGE" value="TO-263-5"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP38513S-1.8" prefix="U">
<description>Linear Regulator</description>
<gates>
<gate name="A" symbol="LP38513S-1.8"/>
</gates>
<devices>
<device name="" package="TO17P1435X465-6N">
<connects>
<connect gate="A" pin="EN" pad="1"/>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="GND_2" pad="3"/>
<connect gate="A" pin="IN" pad="2"/>
<connect gate="A" pin="OUT" pad="4"/>
<connect gate="A" pin="~ERROR" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP38513S-1.8"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="55M4625"/>
<attribute name="PACKAGE" value="TO-263-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP38513T-1.8" prefix="U">
<description>IC REG ULTRA LDO 3A 1.8V</description>
<gates>
<gate name="A" symbol="LP38513T-1.8"/>
</gates>
<devices>
<device name="" package="TO170P470X1016X2092-5P">
<connects>
<connect gate="A" pin="*ERROR" pad="5"/>
<connect gate="A" pin="EN" pad="1"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="VIN" pad="2"/>
<connect gate="A" pin="VOUT" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP38513T-1.8"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="64M7076"/>
<attribute name="PACKAGE" value="TO220-5"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3852EMP-2.5" prefix="U">
<description>Linear Regulators</description>
<gates>
<gate name="A" symbol="LP3852EMP-2.5"/>
</gates>
<devices>
<device name="" package="SOT150P696X180-5N">
<connects>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="VIN" pad="2"/>
<connect gate="A" pin="VOUT" pad="3"/>
<connect gate="A" pin="~ERROR" pad="4"/>
<connect gate="A" pin="~SD" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3852EMP-2.5"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K7366"/>
<attribute name="PACKAGE" value="SOT-223-5"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3852EMP-3.3" prefix="U">
<description>Linear Regulators</description>
<gates>
<gate name="A" symbol="LP3852EMP-3.3"/>
</gates>
<devices>
<device name="" package="SOT150P696X180-5N">
<connects>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="VIN" pad="2"/>
<connect gate="A" pin="VOUT" pad="3"/>
<connect gate="A" pin="~ERROR" pad="4"/>
<connect gate="A" pin="~SD" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3852EMP-3.3"/>
<attribute name="OC_FARNELL" value="1685701"/>
<attribute name="OC_NEWARK" value="41K7367"/>
<attribute name="PACKAGE" value="SOT-223-5"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3853ES-1.8" prefix="U">
<description>Low Dropout Linear Regulators</description>
<gates>
<gate name="A" symbol="LP3853ES-1.8"/>
</gates>
<devices>
<device name="" package="TO170P1435X457-6N">
<connects>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="GND_2" pad="3"/>
<connect gate="A" pin="VIN" pad="2"/>
<connect gate="A" pin="VOUT" pad="4"/>
<connect gate="A" pin="~ERROR~/SENSE" pad="5"/>
<connect gate="A" pin="~SD" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3853ES-1.8"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K7385"/>
<attribute name="PACKAGE" value="TO263-5"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3853ES-2.5" prefix="U">
<description>Low Dropout Linear Regulators</description>
<gates>
<gate name="A" symbol="LP3853ES-2.5"/>
</gates>
<devices>
<device name="" package="TO170P1435X457-6N">
<connects>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="GND_2" pad="3"/>
<connect gate="A" pin="VIN" pad="2"/>
<connect gate="A" pin="VOUT" pad="4"/>
<connect gate="A" pin="~ERROR~/SENSE" pad="5"/>
<connect gate="A" pin="~SD" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3853ES-2.5"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K7386"/>
<attribute name="PACKAGE" value="TO263-5"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3853ES-3.3" prefix="U">
<description>Low Dropout Linear Regulators</description>
<gates>
<gate name="A" symbol="LP3853ES-3.3"/>
</gates>
<devices>
<device name="" package="TO170P1435X457-6N">
<connects>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="GND_2" pad="3"/>
<connect gate="A" pin="VIN" pad="2"/>
<connect gate="A" pin="VOUT" pad="4"/>
<connect gate="A" pin="~ERROR~/SENSE" pad="5"/>
<connect gate="A" pin="~SD" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3853ES-3.3"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K7387"/>
<attribute name="PACKAGE" value="TO263-5"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3853ES-5.0" prefix="U">
<description>Low Dropout Linear Regulators</description>
<gates>
<gate name="A" symbol="LP3853ES-5.0"/>
</gates>
<devices>
<device name="" package="TO170P1435X457-6N">
<connects>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="GND_2" pad="3"/>
<connect gate="A" pin="VIN" pad="2"/>
<connect gate="A" pin="VOUT" pad="4"/>
<connect gate="A" pin="~ERROR~/SENSE" pad="5"/>
<connect gate="A" pin="~SD" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3853ES-5.0"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K7388"/>
<attribute name="PACKAGE" value="TO263-5"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3855EMP-2.5" prefix="U">
<description>Linear Regulators</description>
<gates>
<gate name="A" symbol="LP3855EMP-2.5"/>
</gates>
<devices>
<device name="" package="SOT150P696X180-5N">
<connects>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="VIN" pad="2"/>
<connect gate="A" pin="VOUT" pad="3"/>
<connect gate="A" pin="~ERROR" pad="4"/>
<connect gate="A" pin="~SD" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3855EMP-2.5"/>
<attribute name="OC_FARNELL" value="1685705"/>
<attribute name="OC_NEWARK" value="41K7399"/>
<attribute name="PACKAGE" value="SOT-223-5"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3855EMP-3.3" prefix="U">
<description>Linear Regulators</description>
<gates>
<gate name="A" symbol="LP3855EMP-3.3"/>
</gates>
<devices>
<device name="" package="SOT150P696X180-5N">
<connects>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="VIN" pad="2"/>
<connect gate="A" pin="VOUT" pad="3"/>
<connect gate="A" pin="~ERROR" pad="4"/>
<connect gate="A" pin="~SD" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3855EMP-3.3"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K7400"/>
<attribute name="PACKAGE" value="SOT-223-5"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3855EMP-ADJ" prefix="U">
<description>Linear Regulators</description>
<gates>
<gate name="A" symbol="LP3855EMP-ADJ"/>
</gates>
<devices>
<device name="" package="SOT150P696X180-5N">
<connects>
<connect gate="A" pin="ADJ" pad="4"/>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="VIN" pad="2"/>
<connect gate="A" pin="VOUT" pad="3"/>
<connect gate="A" pin="~SD" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3855EMP-ADJ"/>
<attribute name="OC_FARNELL" value="8188769"/>
<attribute name="OC_NEWARK" value="41K7397"/>
<attribute name="PACKAGE" value="SOT223-5"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3855ES-3.3" prefix="U">
<description>Linear Regulators</description>
<gates>
<gate name="A" symbol="LP3855ES-3.3"/>
</gates>
<devices>
<device name="" package="TO170P1435X457-6N">
<connects>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="GND_2" pad="6"/>
<connect gate="A" pin="VIN" pad="2"/>
<connect gate="A" pin="VOUT" pad="4"/>
<connect gate="A" pin="~ERROR" pad="5"/>
<connect gate="A" pin="~SD" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3855ES-3.3"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K7410"/>
<attribute name="PACKAGE" value="TO-263-5"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3855ES-ADJ" prefix="U">
<description>Linear Regulators</description>
<gates>
<gate name="A" symbol="LP3855ES-ADJ"/>
</gates>
<devices>
<device name="" package="TO170P1435X457-6N">
<connects>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="GND_2" pad="6"/>
<connect gate="A" pin="VIN" pad="2"/>
<connect gate="A" pin="VOUT" pad="4"/>
<connect gate="A" pin="~ERROR" pad="5"/>
<connect gate="A" pin="~SD" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3855ES-ADJ"/>
<attribute name="OC_FARNELL" value="8188750"/>
<attribute name="OC_NEWARK" value="41K7407"/>
<attribute name="PACKAGE" value="TO-263-5"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3856ES-1.8" prefix="U">
<description>Linear regulators</description>
<gates>
<gate name="A" symbol="LP3856ES-1.8"/>
</gates>
<devices>
<device name="" package="TO170P1435X465-6N">
<connects>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="GND_2" pad="6"/>
<connect gate="A" pin="SENSE" pad="5"/>
<connect gate="A" pin="VIN" pad="2"/>
<connect gate="A" pin="VOUT" pad="4"/>
<connect gate="A" pin="~SD" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3856ES-1.8"/>
<attribute name="OC_FARNELL" value="8188149"/>
<attribute name="OC_NEWARK" value="41K7423"/>
<attribute name="PACKAGE" value="TO-263-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3856ES-2.5" prefix="U">
<description>Low Dropout Linear Regulators</description>
<gates>
<gate name="A" symbol="LP3856ES-2.5"/>
</gates>
<devices>
<device name="" package="TO170P1435X457-6N">
<connects>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="GND_2" pad="3"/>
<connect gate="A" pin="VIN" pad="2"/>
<connect gate="A" pin="VOUT" pad="4"/>
<connect gate="A" pin="~ERROR~/SENSE" pad="5"/>
<connect gate="A" pin="~SD" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3856ES-2.5"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K7424"/>
<attribute name="PACKAGE" value="TO263-5"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3856ES-3.3" prefix="U">
<description>Linear regulators</description>
<gates>
<gate name="A" symbol="LP3856ES-3.3"/>
</gates>
<devices>
<device name="" package="TO170P1435X465-6N">
<connects>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="GND_2" pad="6"/>
<connect gate="A" pin="SENSE" pad="5"/>
<connect gate="A" pin="VIN" pad="2"/>
<connect gate="A" pin="VOUT" pad="4"/>
<connect gate="A" pin="~SD" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3856ES-3.3"/>
<attribute name="OC_FARNELL" value="8188165"/>
<attribute name="OC_NEWARK" value="41K7425"/>
<attribute name="PACKAGE" value="TO-263-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3856ES-ADJ" prefix="U">
<description>Linear regulators</description>
<gates>
<gate name="A" symbol="LP3856ES-ADJ"/>
</gates>
<devices>
<device name="" package="TO170P1435X465-6N">
<connects>
<connect gate="A" pin="ADJ" pad="5"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="GND_2" pad="6"/>
<connect gate="A" pin="VIN" pad="2"/>
<connect gate="A" pin="VOUT" pad="4"/>
<connect gate="A" pin="~SD" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3856ES-ADJ"/>
<attribute name="OC_FARNELL" value="8188734"/>
<attribute name="OC_NEWARK" value="41K7422"/>
<attribute name="PACKAGE" value="TO-263-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3856ET-ADJ" prefix="U">
<description>IC REG LDO 3A ADJ VOLT</description>
<gates>
<gate name="A" symbol="LP3856ET-ADJ"/>
</gates>
<devices>
<device name="" package="TO170P470X1016X2092-5P">
<connects>
<connect gate="A" pin="*SD" pad="1"/>
<connect gate="A" pin="ADJ" pad="5"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="VIN" pad="2"/>
<connect gate="A" pin="VOUT" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3856ET-ADJ"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K7432"/>
<attribute name="PACKAGE" value="TO220-5"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP38690DT-1.8" prefix="U">
<description>IC REG LDO 1A 1.8V</description>
<gates>
<gate name="A" symbol="LP38690DT-1.8"/>
</gates>
<devices>
<device name="" package="TO228P1042X238-3N">
<connects>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="VIN" pad="3"/>
<connect gate="A" pin="VOUT" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP38690DT-1.8"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K7437"/>
<attribute name="PACKAGE" value="TO-252"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP38690DT-2.5" prefix="U">
<description>IC REG LDO 1A 2.5V</description>
<gates>
<gate name="A" symbol="LP38690DT-2.5"/>
</gates>
<devices>
<device name="" package="TO228P1042X238-3N">
<connects>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="VIN" pad="3"/>
<connect gate="A" pin="VOUT" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP38690DT-2.5"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K7438"/>
<attribute name="PACKAGE" value="TO-252"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP38690DT-3.3" prefix="U">
<description>IC, LDO VOLT REG, 3.3V, 1A, TO-252</description>
<gates>
<gate name="A" symbol="LP38690DT-3.3"/>
</gates>
<devices>
<device name="" package="TO228P1042X238-3N">
<connects>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="VIN" pad="3"/>
<connect gate="A" pin="VOUT" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP38690DT-3.3"/>
<attribute name="OC_FARNELL" value="1008048"/>
<attribute name="OC_NEWARK" value="41K7439"/>
<attribute name="PACKAGE" value="TO-252"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP38690DT-5.0" prefix="U">
<description>IC REG LDO 1A 5.0V</description>
<gates>
<gate name="A" symbol="LP38690DT-5.0"/>
</gates>
<devices>
<device name="" package="TO228P1042X238-3N">
<connects>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="VIN" pad="3"/>
<connect gate="A" pin="VOUT" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP38690DT-5.0"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K7440"/>
<attribute name="PACKAGE" value="TO-252"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP38690SD-2.5" prefix="U">
<description>IC REG LDO 1A 2.5V</description>
<gates>
<gate name="A" symbol="LP38690SD-2.5"/>
</gates>
<devices>
<device name="" package="DFN300X300X80-7N">
<connects>
<connect gate="A" pin="EP" pad="7"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="NC" pad="3"/>
<connect gate="A" pin="SNS" pad="5"/>
<connect gate="A" pin="VIN" pad="6"/>
<connect gate="A" pin="VIN_2" pad="1"/>
<connect gate="A" pin="VOUT" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP38690SD-2.5"/>
<attribute name="OC_FARNELL" value="1685710"/>
<attribute name="OC_NEWARK" value="41K7447"/>
<attribute name="PACKAGE" value="6-WDFN Exposed Pad"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP38690SD-3.3" prefix="U">
<description>IC REG LDO 1A 3.3V</description>
<gates>
<gate name="A" symbol="LP38690SD-3.3"/>
</gates>
<devices>
<device name="" package="DFN300X300X80-7N">
<connects>
<connect gate="A" pin="EP" pad="7"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="NC" pad="3"/>
<connect gate="A" pin="SNS" pad="5"/>
<connect gate="A" pin="VIN" pad="6"/>
<connect gate="A" pin="VIN_2" pad="1"/>
<connect gate="A" pin="VOUT" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP38690SD-3.3"/>
<attribute name="OC_FARNELL" value="1685711"/>
<attribute name="OC_NEWARK" value="41K7448"/>
<attribute name="PACKAGE" value="6-WDFN Exposed Pad"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP38690SD-5.0" prefix="U">
<description>IC REG LDO 1A 5.0V</description>
<gates>
<gate name="A" symbol="LP38690SD-5.0"/>
</gates>
<devices>
<device name="" package="DFN300X300X80-7N">
<connects>
<connect gate="A" pin="EP" pad="7"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="NC" pad="3"/>
<connect gate="A" pin="SNS" pad="5"/>
<connect gate="A" pin="VIN" pad="6"/>
<connect gate="A" pin="VIN_2" pad="1"/>
<connect gate="A" pin="VOUT" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP38690SD-5.0"/>
<attribute name="OC_FARNELL" value="1685712"/>
<attribute name="OC_NEWARK" value="41K7449"/>
<attribute name="PACKAGE" value="6-WDFN Exposed Pad"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP38690SD-ADJ" prefix="U">
<description>Regulator</description>
<gates>
<gate name="A" symbol="LP38690SD-ADJ"/>
</gates>
<devices>
<device name="" package="DFN300X300X80-7N">
<connects>
<connect gate="A" pin="ADJ" pad="4"/>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="GND_2" pad="2"/>
<connect gate="A" pin="NC" pad="3"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="VIN_2" pad="6"/>
<connect gate="A" pin="VOUT" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP38690SD-ADJ"/>
<attribute name="OC_FARNELL" value="1559628"/>
<attribute name="OC_NEWARK" value="41K7445"/>
<attribute name="PACKAGE" value="DFN-6"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP38691DT-1.8" prefix="U">
<description>IC REG LDO 500MA 1.8V</description>
<gates>
<gate name="A" symbol="LP38691DT-1.8"/>
</gates>
<devices>
<device name="" package="TO228P1042X238-3N">
<connects>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="VIN" pad="3"/>
<connect gate="A" pin="VOUT" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP38691DT-1.8"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K7455"/>
<attribute name="PACKAGE" value="TO-252"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP38691DT-3.3" prefix="U">
<description>IC REG LDO 500MA 3.3V</description>
<gates>
<gate name="A" symbol="LP38691DT-3.3"/>
</gates>
<devices>
<device name="" package="TO228P1042X238-3N">
<connects>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="VIN" pad="3"/>
<connect gate="A" pin="VOUT" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP38691DT-3.3"/>
<attribute name="OC_FARNELL" value="1685713"/>
<attribute name="OC_NEWARK" value="41K7457"/>
<attribute name="PACKAGE" value="TO-252"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP38691DT-5.0" prefix="U">
<description>IC REG LDO 500MA 5.0V</description>
<gates>
<gate name="A" symbol="LP38691DT-5.0"/>
</gates>
<devices>
<device name="" package="TO228P1042X238-3N">
<connects>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="VIN" pad="3"/>
<connect gate="A" pin="VOUT" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP38691DT-5.0"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K7458"/>
<attribute name="PACKAGE" value="TO-252"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP38691SD-1.8" prefix="U">
<description>IC REG LDO 500MA 1.8V</description>
<gates>
<gate name="A" symbol="LP38691SD-1.8"/>
</gates>
<devices>
<device name="" package="DFN300X300X80-7N">
<connects>
<connect gate="A" pin="EP" pad="7"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="NC" pad="3"/>
<connect gate="A" pin="SNS" pad="5"/>
<connect gate="A" pin="VIN" pad="6"/>
<connect gate="A" pin="VIN_2" pad="1"/>
<connect gate="A" pin="VOUT" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP38691SD-1.8"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K7464"/>
<attribute name="PACKAGE" value="6-WDFN Exposed Pad"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP38691SD-2.5" prefix="U">
<description>IC REG LDO 500MA 2.5V</description>
<gates>
<gate name="A" symbol="LP38691SD-2.5"/>
</gates>
<devices>
<device name="" package="DFN300X300X80-7N">
<connects>
<connect gate="A" pin="EP" pad="7"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="NC" pad="3"/>
<connect gate="A" pin="SNS" pad="5"/>
<connect gate="A" pin="VIN" pad="6"/>
<connect gate="A" pin="VIN_2" pad="1"/>
<connect gate="A" pin="VOUT" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP38691SD-2.5"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K7465"/>
<attribute name="PACKAGE" value="6-WDFN Exposed Pad"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP38691SD-3.3" prefix="U">
<description>IC REG LDO 500MA 3.3V</description>
<gates>
<gate name="A" symbol="LP38691SD-3.3"/>
</gates>
<devices>
<device name="" package="DFN300X300X80-7N">
<connects>
<connect gate="A" pin="EP" pad="7"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="NC" pad="3"/>
<connect gate="A" pin="SNS" pad="5"/>
<connect gate="A" pin="VIN" pad="6"/>
<connect gate="A" pin="VIN_2" pad="1"/>
<connect gate="A" pin="VOUT" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP38691SD-3.3"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K7466"/>
<attribute name="PACKAGE" value="6-WDFN Exposed Pad"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP38691SD-5.0" prefix="U">
<description>IC REG LDO 500MA 5.0V</description>
<gates>
<gate name="A" symbol="LP38691SD-5.0"/>
</gates>
<devices>
<device name="" package="DFN300X300X80-7N">
<connects>
<connect gate="A" pin="EP" pad="7"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="NC" pad="3"/>
<connect gate="A" pin="SNS" pad="5"/>
<connect gate="A" pin="VIN" pad="6"/>
<connect gate="A" pin="VIN_2" pad="1"/>
<connect gate="A" pin="VOUT" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP38691SD-5.0"/>
<attribute name="OC_FARNELL" value="1685716"/>
<attribute name="OC_NEWARK" value="41K7467"/>
<attribute name="PACKAGE" value="6-WDFN Exposed Pad"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP38691SD-ADJ" prefix="U">
<description>Linear Regulator</description>
<gates>
<gate name="A" symbol="LP38691SD-ADJ"/>
</gates>
<devices>
<device name="" package="DFN300X300X80-7N">
<connects>
<connect gate="A" pin="ADJ" pad="4"/>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="GND_2" pad="2"/>
<connect gate="A" pin="NC" pad="3"/>
<connect gate="A" pin="VIN" pad="6"/>
<connect gate="A" pin="VIN_2" pad="1"/>
<connect gate="A" pin="VOUT" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP38691SD-ADJ"/>
<attribute name="OC_FARNELL" value="1312620"/>
<attribute name="OC_NEWARK" value="41K7463"/>
<attribute name="PACKAGE" value="LLP-6"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP38692MP-1.8" prefix="U">
<description>IC REG LDO 1A 1.8V</description>
<gates>
<gate name="A" symbol="LP38692MP-1.8"/>
</gates>
<devices>
<device name="" package="SOT150P696X180-5N">
<connects>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="N/C" pad="2"/>
<connect gate="A" pin="VEN" pad="1"/>
<connect gate="A" pin="VIN" pad="4"/>
<connect gate="A" pin="VOUT" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP38692MP-1.8"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K7474"/>
<attribute name="PACKAGE" value="SOT-223-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP38692MP-2.5" prefix="U">
<description>2.5/NOPB IC REG LDO 1A 2.5V</description>
<gates>
<gate name="A" symbol="LP38692MP-2.5"/>
</gates>
<devices>
<device name="" package="SOT150P696X180-5N">
<connects>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="N/C" pad="2"/>
<connect gate="A" pin="VEN" pad="1"/>
<connect gate="A" pin="VIN" pad="4"/>
<connect gate="A" pin="VOUT" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP38692MP-2.5"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K7475"/>
<attribute name="PACKAGE" value="SOT-223-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP38692MP-3.3" prefix="U">
<description>Linear  Regulator</description>
<gates>
<gate name="A" symbol="LP38692MP-3.3"/>
</gates>
<devices>
<device name="" package="SOT150P696X180-5N">
<connects>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="N/C" pad="2"/>
<connect gate="A" pin="VEN" pad="1"/>
<connect gate="A" pin="VIN" pad="4"/>
<connect gate="A" pin="VOUT" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP38692MP-3.3"/>
<attribute name="OC_FARNELL" value="1008056"/>
<attribute name="OC_NEWARK" value="41K7476"/>
<attribute name="PACKAGE" value="SOT-223-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP38692MP-5.0" prefix="U">
<description>Linear  Regulator</description>
<gates>
<gate name="A" symbol="LP38692MP-5.0"/>
</gates>
<devices>
<device name="" package="SOT150P696X180-5N">
<connects>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="N/C" pad="2"/>
<connect gate="A" pin="VEN" pad="1"/>
<connect gate="A" pin="VIN" pad="4"/>
<connect gate="A" pin="VOUT" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP38692MP-5.0"/>
<attribute name="OC_FARNELL" value="1008057"/>
<attribute name="OC_NEWARK" value="41K7477"/>
<attribute name="PACKAGE" value="SOT-223-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP38692MP-ADJ" prefix="U">
<description>Linear  Regulator</description>
<gates>
<gate name="A" symbol="LP38692MP-ADJ"/>
</gates>
<devices>
<device name="" package="SOT150P696X180-5N">
<connects>
<connect gate="A" pin="ADJ" pad="2"/>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="VEN" pad="1"/>
<connect gate="A" pin="VIN" pad="4"/>
<connect gate="A" pin="VOUT" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP38692MP-ADJ"/>
<attribute name="OC_FARNELL" value="1008058"/>
<attribute name="OC_NEWARK" value="41K7473"/>
<attribute name="PACKAGE" value="SOT-223-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP38692SD-2.5" prefix="U">
<description>IC REG LDO 1A 2.5V</description>
<gates>
<gate name="A" symbol="LP38692SD-2.5"/>
</gates>
<devices>
<device name="" package="DFN300X300X80-7N">
<connects>
<connect gate="A" pin="EP" pad="7"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="SNS" pad="5"/>
<connect gate="A" pin="VEN" pad="3"/>
<connect gate="A" pin="VIN" pad="6"/>
<connect gate="A" pin="VIN_2" pad="1"/>
<connect gate="A" pin="VOUT" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP38692SD-2.5"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K7485"/>
<attribute name="PACKAGE" value="6-WDFN Exposed Pad"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP38692SD-3.3" prefix="U">
<description>IC REG LDO 1A 3.3V</description>
<gates>
<gate name="A" symbol="LP38692SD-3.3"/>
</gates>
<devices>
<device name="" package="DFN300X300X80-7N">
<connects>
<connect gate="A" pin="EP" pad="7"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="SNS" pad="5"/>
<connect gate="A" pin="VEN" pad="3"/>
<connect gate="A" pin="VIN" pad="6"/>
<connect gate="A" pin="VIN_2" pad="1"/>
<connect gate="A" pin="VOUT" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP38692SD-3.3"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K7486"/>
<attribute name="PACKAGE" value="6-WDFN Exposed Pad"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP38692SD-5.0" prefix="U">
<description>IC REG LDO 1A 5.0V</description>
<gates>
<gate name="A" symbol="LP38692SD-5.0"/>
</gates>
<devices>
<device name="" package="DFN300X300X80-7N">
<connects>
<connect gate="A" pin="EP" pad="7"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="SNS" pad="5"/>
<connect gate="A" pin="VEN" pad="3"/>
<connect gate="A" pin="VIN" pad="6"/>
<connect gate="A" pin="VIN_2" pad="1"/>
<connect gate="A" pin="VOUT" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP38692SD-5.0"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K7487"/>
<attribute name="PACKAGE" value="6-WDFN Exposed Pad"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP38692SD-ADJ" prefix="U">
<description>Regulator</description>
<gates>
<gate name="A" symbol="LP38692SD-ADJ"/>
</gates>
<devices>
<device name="" package="DFN300X300X80-7N">
<connects>
<connect gate="A" pin="ADJ" pad="4"/>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="GND_2" pad="2"/>
<connect gate="A" pin="VEN" pad="3"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="VIN_2" pad="6"/>
<connect gate="A" pin="VOUT" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP38692SD-ADJ"/>
<attribute name="OC_FARNELL" value="1685717"/>
<attribute name="OC_NEWARK" value="41K7483"/>
<attribute name="PACKAGE" value="DFN-6"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP38693MP-1.8" prefix="U">
<description>IC REG LDO 500MA 1.8V</description>
<gates>
<gate name="A" symbol="LP38693MP-1.8"/>
</gates>
<devices>
<device name="" package="SOT150P696X180-5N">
<connects>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="N/C" pad="2"/>
<connect gate="A" pin="VEN" pad="1"/>
<connect gate="A" pin="VIN" pad="4"/>
<connect gate="A" pin="VOUT" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP38693MP-1.8"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K7494"/>
<attribute name="PACKAGE" value="SOT-223-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP38693MP-2.5" prefix="U">
<description>IC REG LDO 500MA 2.5V</description>
<gates>
<gate name="A" symbol="LP38693MP-2.5"/>
</gates>
<devices>
<device name="" package="SOT150P696X180-5N">
<connects>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="N/C" pad="2"/>
<connect gate="A" pin="VEN" pad="1"/>
<connect gate="A" pin="VIN" pad="4"/>
<connect gate="A" pin="VOUT" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP38693MP-2.5"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K7495"/>
<attribute name="PACKAGE" value="SOT-223-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP38693MP-3.3" prefix="U">
<description>Linear Regulators</description>
<gates>
<gate name="A" symbol="LP38693MP-3.3"/>
</gates>
<devices>
<device name="" package="SOT150P696X180-5N">
<connects>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="NC" pad="2"/>
<connect gate="A" pin="VEN" pad="1"/>
<connect gate="A" pin="VIN" pad="4"/>
<connect gate="A" pin="VOUT" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP38693MP-3.3"/>
<attribute name="OC_FARNELL" value="1008061"/>
<attribute name="OC_NEWARK" value="41K7496"/>
<attribute name="PACKAGE" value="SOT-223-5"/>
<attribute name="SUPPLIER" value="National"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP38693MP-5.0" prefix="U">
<description>Linear Regulators</description>
<gates>
<gate name="A" symbol="LP38693MP-5.0"/>
</gates>
<devices>
<device name="" package="SOT150P696X180-5N">
<connects>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="NC" pad="2"/>
<connect gate="A" pin="VEN" pad="1"/>
<connect gate="A" pin="VIN" pad="4"/>
<connect gate="A" pin="VOUT" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP38693MP-5.0"/>
<attribute name="OC_FARNELL" value="1008062"/>
<attribute name="OC_NEWARK" value="41K7497"/>
<attribute name="PACKAGE" value="SOT-223-5"/>
<attribute name="SUPPLIER" value="National"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP38693MP-ADJ" prefix="U">
<description>IC, ADJ LDO REG, 1.25V TO 9V</description>
<gates>
<gate name="A" symbol="LP38693MP-ADJ"/>
</gates>
<devices>
<device name="" package="SOT150P696X180-5N">
<connects>
<connect gate="A" pin="ADJ" pad="2"/>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="VEN" pad="1"/>
<connect gate="A" pin="VIN" pad="4"/>
<connect gate="A" pin="VOUT" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP38693MP-ADJ"/>
<attribute name="OC_FARNELL" value="1685718"/>
<attribute name="OC_NEWARK" value="41K7493"/>
<attribute name="PACKAGE" value="SOT-223-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP38693SD-3.3" prefix="U">
<description>IC REG LDO 500MA 3.3V</description>
<gates>
<gate name="A" symbol="LP38693SD-3.3"/>
</gates>
<devices>
<device name="" package="DFN300X300X80-7N">
<connects>
<connect gate="A" pin="EP" pad="7"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="SNS" pad="5"/>
<connect gate="A" pin="VEN" pad="3"/>
<connect gate="A" pin="VIN" pad="6"/>
<connect gate="A" pin="VIN_2" pad="1"/>
<connect gate="A" pin="VOUT" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP38693SD-3.3"/>
<attribute name="OC_FARNELL" value="1685720"/>
<attribute name="OC_NEWARK" value="41K7506"/>
<attribute name="PACKAGE" value="6-WDFN Exposed Pad"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP38693SD-5.0" prefix="U">
<description>IC, LDO VOLT REG, 5V, 0.5A,</description>
<gates>
<gate name="A" symbol="LP38693SD-5.0"/>
</gates>
<devices>
<device name="" package="DFN300X300X80-7N">
<connects>
<connect gate="A" pin="EP" pad="7"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="SNS" pad="5"/>
<connect gate="A" pin="VEN" pad="3"/>
<connect gate="A" pin="VIN" pad="6"/>
<connect gate="A" pin="VIN_2" pad="1"/>
<connect gate="A" pin="VOUT" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP38693SD-5.0"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K7507"/>
<attribute name="PACKAGE" value="6-WDFN Exposed Pad"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP38693SD-ADJ" prefix="U">
<description>Regulator</description>
<gates>
<gate name="A" symbol="LP38693SD-ADJ"/>
</gates>
<devices>
<device name="" package="DFN300X300X80-7N">
<connects>
<connect gate="A" pin="ADJ" pad="4"/>
<connect gate="A" pin="EP" pad="7"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="VEN" pad="3"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="VIN_2" pad="6"/>
<connect gate="A" pin="VOUT" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP38693SD-ADJ"/>
<attribute name="OC_FARNELL" value="1685719"/>
<attribute name="OC_NEWARK" value="41K7503"/>
<attribute name="PACKAGE" value="DFN-6"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3871EMP-1.8" prefix="U">
<description>Linear Regulator</description>
<gates>
<gate name="A" symbol="LP3871EMP-1.8"/>
</gates>
<devices>
<device name="" package="SOT15P696X180-5N">
<connects>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="VIN" pad="2"/>
<connect gate="A" pin="VOUT" pad="3"/>
<connect gate="A" pin="~ERROR" pad="4"/>
<connect gate="A" pin="~SD" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3871EMP-1.8"/>
<attribute name="OC_FARNELL" value="1685721"/>
<attribute name="OC_NEWARK" value="41K7513"/>
<attribute name="PACKAGE" value="SOT223-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3871EMP-2.5" prefix="U">
<description>Linear Regulator</description>
<gates>
<gate name="A" symbol="LP3871EMP-2.5"/>
</gates>
<devices>
<device name="" package="SOT15P696X180-5N">
<connects>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="VIN" pad="2"/>
<connect gate="A" pin="VOUT" pad="3"/>
<connect gate="A" pin="~ERROR" pad="4"/>
<connect gate="A" pin="~SD" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3871EMP-2.5"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K7514"/>
<attribute name="PACKAGE" value="SOT223-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3871EMP-3.3" prefix="U">
<description>Linear Regulators</description>
<gates>
<gate name="A" symbol="LP3871EMP-3.3"/>
</gates>
<devices>
<device name="" package="SOT150P696X180-5N">
<connects>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="VIN" pad="2"/>
<connect gate="A" pin="VOUT" pad="3"/>
<connect gate="A" pin="~ERR" pad="4"/>
<connect gate="A" pin="~SD" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3871EMP-3.3"/>
<attribute name="OC_FARNELL" value="8188246"/>
<attribute name="OC_NEWARK" value="41K7515"/>
<attribute name="PACKAGE" value="SOT-223-5"/>
<attribute name="SUPPLIER" value="National"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3871ES-3.3" prefix="U">
<description>Linear Regulator</description>
<gates>
<gate name="A" symbol="LP3871ES-3.3"/>
</gates>
<devices>
<device name="" package="TO17P1435X465-6N">
<connects>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="GND_2" pad="3"/>
<connect gate="A" pin="VIN" pad="2"/>
<connect gate="A" pin="VOUT" pad="4"/>
<connect gate="A" pin="~ERROR" pad="5"/>
<connect gate="A" pin="~SD" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3871ES-3.3"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K7523"/>
<attribute name="PACKAGE" value="TO-263-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3872EMP-3.3" prefix="U">
<description>Linear Regulator</description>
<gates>
<gate name="A" symbol="LP3872EMP-3.3"/>
</gates>
<devices>
<device name="" package="SOT15P696X180-5N">
<connects>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="VIN" pad="2"/>
<connect gate="A" pin="VOUT" pad="3"/>
<connect gate="A" pin="~ERROR" pad="4"/>
<connect gate="A" pin="~SD" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3872EMP-3.3"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K7535"/>
<attribute name="PACKAGE" value="SOT223-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3872ES-1.8" prefix="U">
<description>Linear Regulator</description>
<gates>
<gate name="A" symbol="LP3872ES-1.8"/>
</gates>
<devices>
<device name="" package="TO17P1435X465-6N">
<connects>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="GND_2" pad="3"/>
<connect gate="A" pin="VIN" pad="2"/>
<connect gate="A" pin="VOUT" pad="4"/>
<connect gate="A" pin="~ERROR" pad="5"/>
<connect gate="A" pin="~SD" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3872ES-1.8"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K7541"/>
<attribute name="PACKAGE" value="TO-263-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3872ES-3.3" prefix="U">
<description>Linear Regulator</description>
<gates>
<gate name="A" symbol="LP3872ES-3.3"/>
</gates>
<devices>
<device name="" package="TO17P1435X465-6N">
<connects>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="GND_2" pad="3"/>
<connect gate="A" pin="VIN" pad="2"/>
<connect gate="A" pin="VOUT" pad="4"/>
<connect gate="A" pin="~ERROR" pad="5"/>
<connect gate="A" pin="~SD" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3872ES-3.3"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K7543"/>
<attribute name="PACKAGE" value="TO-263-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3872ET-1.8" prefix="U">
<description>IC REG LDO 1.5A 1.8V</description>
<gates>
<gate name="A" symbol="LP3872ET-1.8"/>
</gates>
<devices>
<device name="" package="TO170P470X1016X2092-5P">
<connects>
<connect gate="A" pin="*SD" pad="1"/>
<connect gate="A" pin="ERROR-SENSE" pad="5"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="VIN" pad="2"/>
<connect gate="A" pin="VOUT" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3872ET-1.8"/>
<attribute name="OC_FARNELL" value="8188408"/>
<attribute name="OC_NEWARK" value="-"/>
<attribute name="PACKAGE" value="TO220-5"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3873ES-1.8" prefix="U">
<description>Linear Regulator</description>
<gates>
<gate name="A" symbol="LP3873ES-1.8"/>
</gates>
<devices>
<device name="" package="TO17P1435X465-6N">
<connects>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="GND_2" pad="3"/>
<connect gate="A" pin="VIN" pad="2"/>
<connect gate="A" pin="VOUT" pad="4"/>
<connect gate="A" pin="~ERROR" pad="5"/>
<connect gate="A" pin="~SD" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3873ES-1.8"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K7553"/>
<attribute name="PACKAGE" value="TO-263-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3873ES-2.5" prefix="U">
<description>Linear Regulator</description>
<gates>
<gate name="A" symbol="LP3873ES-2.5"/>
</gates>
<devices>
<device name="" package="TO17P1435X465-6N">
<connects>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="GND_2" pad="3"/>
<connect gate="A" pin="VIN" pad="2"/>
<connect gate="A" pin="VOUT" pad="4"/>
<connect gate="A" pin="~ERROR" pad="5"/>
<connect gate="A" pin="~SD" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3873ES-2.5"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K7554"/>
<attribute name="PACKAGE" value="TO-263-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3873ES-3.3" prefix="U">
<description>Linear Regulator</description>
<gates>
<gate name="A" symbol="LP3873ES-3.3"/>
</gates>
<devices>
<device name="" package="TO17P1435X465-6N">
<connects>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="GND_2" pad="3"/>
<connect gate="A" pin="VIN" pad="2"/>
<connect gate="A" pin="VOUT" pad="4"/>
<connect gate="A" pin="~ERROR" pad="5"/>
<connect gate="A" pin="~SD" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3873ES-3.3"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K7555"/>
<attribute name="PACKAGE" value="TO-263-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3874EMP-1.8" prefix="U">
<description>Linear Regulator</description>
<gates>
<gate name="A" symbol="LP3874EMP-1.8"/>
</gates>
<devices>
<device name="" package="SOT15P696X180-5N">
<connects>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="VIN" pad="2"/>
<connect gate="A" pin="VOUT" pad="3"/>
<connect gate="A" pin="~ERROR" pad="4"/>
<connect gate="A" pin="~SD" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3874EMP-1.8"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K7566"/>
<attribute name="PACKAGE" value="SOT223-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3874EMP-2.5" prefix="U">
<description>Linear Regulator</description>
<gates>
<gate name="A" symbol="LP3874EMP-2.5"/>
</gates>
<devices>
<device name="" package="SOT15P696X180-5N">
<connects>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="VIN" pad="2"/>
<connect gate="A" pin="VOUT" pad="3"/>
<connect gate="A" pin="~ERROR" pad="4"/>
<connect gate="A" pin="~SD" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3874EMP-2.5"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K7567"/>
<attribute name="PACKAGE" value="SOT223-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3874EMP-3.3" prefix="U">
<description>Linear Regulators</description>
<gates>
<gate name="A" symbol="LP3874EMP-3.3"/>
</gates>
<devices>
<device name="" package="SOT150P696X180-5N">
<connects>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="SEN" pad="4"/>
<connect gate="A" pin="VIN" pad="2"/>
<connect gate="A" pin="VOUT" pad="3"/>
<connect gate="A" pin="~SD" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3874EMP-3.3"/>
<attribute name="OC_FARNELL" value="8188548"/>
<attribute name="OC_NEWARK" value="41K7568"/>
<attribute name="PACKAGE" value="SOT-223-5"/>
<attribute name="SUPPLIER" value="National"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3874EMP-5.0" prefix="U">
<description>Linear Regulators</description>
<gates>
<gate name="A" symbol="LP3874EMP-5.0"/>
</gates>
<devices>
<device name="" package="SOT150P696X180-5N">
<connects>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="SEN" pad="4"/>
<connect gate="A" pin="VIN" pad="2"/>
<connect gate="A" pin="VOUT" pad="3"/>
<connect gate="A" pin="~SD" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3874EMP-5.0"/>
<attribute name="OC_FARNELL" value="8188556"/>
<attribute name="OC_NEWARK" value="38K3883"/>
<attribute name="PACKAGE" value="SOT-223-5"/>
<attribute name="SUPPLIER" value="National"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3874EMP-ADJ" prefix="U">
<description>Linear Regulator</description>
<gates>
<gate name="A" symbol="LP3874EMP-ADJ"/>
</gates>
<devices>
<device name="" package="SOT15P696X180-5N">
<connects>
<connect gate="A" pin="ADJ" pad="5"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="VIN" pad="2"/>
<connect gate="A" pin="VOUT" pad="4"/>
<connect gate="A" pin="~SD" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3874EMP-ADJ"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K7565"/>
<attribute name="PACKAGE" value="SOT223-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3874ES-3.3" prefix="U">
<description>Linear Regulator</description>
<gates>
<gate name="A" symbol="LP3874ES-3.3"/>
</gates>
<devices>
<device name="" package="TO17P1435X465-6N">
<connects>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="GND_2" pad="3"/>
<connect gate="A" pin="SENSE" pad="5"/>
<connect gate="A" pin="VIN" pad="2"/>
<connect gate="A" pin="VOUT" pad="4"/>
<connect gate="A" pin="~SD" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3874ES-3.3"/>
<attribute name="OC_FARNELL" value="1559668"/>
<attribute name="OC_NEWARK" value="41K7578"/>
<attribute name="PACKAGE" value="TO-263-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3874ES-ADJ" prefix="U">
<description>Linear regulators</description>
<gates>
<gate name="A" symbol="LP3874ES-ADJ"/>
</gates>
<devices>
<device name="" package="TO170P1435X465-6N">
<connects>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="GND_2" pad="6"/>
<connect gate="A" pin="SENSE" pad="5"/>
<connect gate="A" pin="VIN" pad="2"/>
<connect gate="A" pin="VOUT" pad="4"/>
<connect gate="A" pin="~SD" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3874ES-ADJ"/>
<attribute name="OC_FARNELL" value="8188700"/>
<attribute name="OC_NEWARK" value="41K7575"/>
<attribute name="PACKAGE" value="TO-263-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3875EMP-1.8" prefix="U">
<description>Linear Regulator</description>
<gates>
<gate name="A" symbol="LP3875EMP-1.8"/>
</gates>
<devices>
<device name="" package="SOT15P696X180-5N">
<connects>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="SENSE" pad="4"/>
<connect gate="A" pin="VIN" pad="2"/>
<connect gate="A" pin="VOUT" pad="3"/>
<connect gate="A" pin="~SD" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3875EMP-1.8"/>
<attribute name="OC_FARNELL" value="1685726"/>
<attribute name="OC_NEWARK" value="41K7591"/>
<attribute name="PACKAGE" value="SOT223-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3875EMP-3.3" prefix="U">
<description>Linear Regulator</description>
<gates>
<gate name="A" symbol="LP3875EMP-3.3"/>
</gates>
<devices>
<device name="" package="SOT15P696X180-5N">
<connects>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="SENSE" pad="4"/>
<connect gate="A" pin="VIN" pad="2"/>
<connect gate="A" pin="VOUT" pad="3"/>
<connect gate="A" pin="~SD" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3875EMP-3.3"/>
<attribute name="OC_FARNELL" value="1685728"/>
<attribute name="OC_NEWARK" value="41K7593"/>
<attribute name="PACKAGE" value="SOT223-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3875EMP-ADJ" prefix="U">
<description>Linear Regulators</description>
<gates>
<gate name="A" symbol="LP3875EMP-ADJ"/>
</gates>
<devices>
<device name="" package="SOT150P696X180-5N">
<connects>
<connect gate="A" pin="ADJ" pad="4"/>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="VIN" pad="2"/>
<connect gate="A" pin="VOUT" pad="3"/>
<connect gate="A" pin="~SD" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3875EMP-ADJ"/>
<attribute name="OC_FARNELL" value="8188688"/>
<attribute name="OC_NEWARK" value="41K7590"/>
<attribute name="PACKAGE" value="SOT-223-5"/>
<attribute name="SUPPLIER" value="National"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3875ES-1.8" prefix="U">
<description>Linear Regulator</description>
<gates>
<gate name="A" symbol="LP3875ES-1.8"/>
</gates>
<devices>
<device name="" package="TO17P1435X465-6N">
<connects>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="GND_2" pad="3"/>
<connect gate="A" pin="SENSE" pad="5"/>
<connect gate="A" pin="VIN" pad="2"/>
<connect gate="A" pin="VOUT" pad="4"/>
<connect gate="A" pin="~SD" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3875ES-1.8"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K7601"/>
<attribute name="PACKAGE" value="TO-263-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3875ES-2.5" prefix="U">
<description>Linear Regulator</description>
<gates>
<gate name="A" symbol="LP3875ES-2.5"/>
</gates>
<devices>
<device name="" package="TO17P1435X465-6N">
<connects>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="GND_2" pad="3"/>
<connect gate="A" pin="SENSE" pad="5"/>
<connect gate="A" pin="VIN" pad="2"/>
<connect gate="A" pin="VOUT" pad="4"/>
<connect gate="A" pin="~SD" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3875ES-2.5"/>
<attribute name="OC_FARNELL" value="1685729"/>
<attribute name="OC_NEWARK" value="41K7602"/>
<attribute name="PACKAGE" value="TO-263-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3875ES-3.3" prefix="U">
<description>Linear Regulator</description>
<gates>
<gate name="A" symbol="LP3875ES-3.3"/>
</gates>
<devices>
<device name="" package="TO17P1435X465-6N">
<connects>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="GND_2" pad="3"/>
<connect gate="A" pin="SENSE" pad="5"/>
<connect gate="A" pin="VIN" pad="2"/>
<connect gate="A" pin="VOUT" pad="4"/>
<connect gate="A" pin="~SD" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3875ES-3.3"/>
<attribute name="OC_FARNELL" value="1685730"/>
<attribute name="OC_NEWARK" value="41K7603"/>
<attribute name="PACKAGE" value="TO-263-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3875ES-ADJ" prefix="U">
<description>Linear regulators</description>
<gates>
<gate name="A" symbol="LP3875ES-ADJ"/>
</gates>
<devices>
<device name="" package="TO170P1435X465-6N">
<connects>
<connect gate="A" pin="ADJ" pad="5"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="GND_2" pad="6"/>
<connect gate="A" pin="VIN" pad="2"/>
<connect gate="A" pin="VOUT" pad="4"/>
<connect gate="A" pin="~SD" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3875ES-ADJ"/>
<attribute name="OC_FARNELL" value="8207321"/>
<attribute name="OC_NEWARK" value="41K7600"/>
<attribute name="PACKAGE" value="TO-263-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3875ET-3.3" prefix="U">
<description>V REG LDO 1.5A 3.3V, 3875</description>
<gates>
<gate name="A" symbol="LP3875ET-3.3"/>
</gates>
<devices>
<device name="" package="TO170P470X1016X2092-5P">
<connects>
<connect gate="A" pin="*SD" pad="1"/>
<connect gate="A" pin="ERROR-SENSE" pad="5"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="VIN" pad="2"/>
<connect gate="A" pin="VOUT" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3875ET-3.3"/>
<attribute name="OC_FARNELL" value="8206953"/>
<attribute name="OC_NEWARK" value="-"/>
<attribute name="PACKAGE" value="TO220-5"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3876ES-1.8" prefix="U">
<description>Linear Regulator</description>
<gates>
<gate name="A" symbol="LP3876ES-1.8"/>
</gates>
<devices>
<device name="" package="TO17P1435X465-6N">
<connects>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="GND_2" pad="3"/>
<connect gate="A" pin="SENSE" pad="5"/>
<connect gate="A" pin="VIN" pad="2"/>
<connect gate="A" pin="VOUT" pad="4"/>
<connect gate="A" pin="~SD" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3876ES-1.8"/>
<attribute name="OC_FARNELL" value="1685731"/>
<attribute name="OC_NEWARK" value="41K7616"/>
<attribute name="PACKAGE" value="TO-263-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3876ES-2.5" prefix="U">
<description>Linear Regulator</description>
<gates>
<gate name="A" symbol="LP3876ES-2.5"/>
</gates>
<devices>
<device name="" package="TO17P1435X465-6N">
<connects>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="GND_2" pad="3"/>
<connect gate="A" pin="SENSE" pad="5"/>
<connect gate="A" pin="VIN" pad="2"/>
<connect gate="A" pin="VOUT" pad="4"/>
<connect gate="A" pin="~SD" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3876ES-2.5"/>
<attribute name="OC_FARNELL" value="1685732"/>
<attribute name="OC_NEWARK" value="41K7617"/>
<attribute name="PACKAGE" value="TO-263-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3876ES-3.3" prefix="U">
<description>Linear Regulator</description>
<gates>
<gate name="A" symbol="LP3876ES-3.3"/>
</gates>
<devices>
<device name="" package="TO17P1435X465-6N">
<connects>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="GND_2" pad="3"/>
<connect gate="A" pin="SENSE" pad="5"/>
<connect gate="A" pin="VIN" pad="2"/>
<connect gate="A" pin="VOUT" pad="4"/>
<connect gate="A" pin="~SD" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3876ES-3.3"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K7618"/>
<attribute name="PACKAGE" value="TO-263-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3876ES-ADJ" prefix="U">
<description>Linear regulators</description>
<gates>
<gate name="A" symbol="LP3876ES-ADJ"/>
</gates>
<devices>
<device name="" package="TO170P1435X465-6N">
<connects>
<connect gate="A" pin="ADJ" pad="5"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="GND_2" pad="6"/>
<connect gate="A" pin="VIN" pad="2"/>
<connect gate="A" pin="VOUT" pad="4"/>
<connect gate="A" pin="~SD" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3876ES-ADJ"/>
<attribute name="OC_FARNELL" value="8207348"/>
<attribute name="OC_NEWARK" value="41K7615"/>
<attribute name="PACKAGE" value="TO-263-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3878MR-ADJ" prefix="U">
<description>Voltage Regulator</description>
<gates>
<gate name="A" symbol="LP3878MR-ADJ"/>
</gates>
<devices>
<device name="" package="SOIC127P600X168-8N">
<connects>
<connect gate="A" pin="ADJ" pad="6"/>
<connect gate="A" pin="BYPASS" pad="1"/>
<connect gate="A" pin="GND" pad="9"/>
<connect gate="A" pin="GND_2" pad="3"/>
<connect gate="A" pin="IN" pad="4"/>
<connect gate="A" pin="NC" pad="7"/>
<connect gate="A" pin="NC_2" pad="2"/>
<connect gate="A" pin="OUT" pad="5"/>
<connect gate="A" pin="~SD" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3878MR-ADJ"/>
<attribute name="OC_FARNELL" value="1286784"/>
<attribute name="OC_NEWARK" value="65K6513"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3879MR-1.0" prefix="U">
<description>Voltage Regulator</description>
<gates>
<gate name="A" symbol="LP3879MR-1.0"/>
</gates>
<devices>
<device name="" package="SOIC127P600X168-9N">
<connects>
<connect gate="A" pin="BYPASS" pad="1"/>
<connect gate="A" pin="GND" pad="9"/>
<connect gate="A" pin="GND_2" pad="3"/>
<connect gate="A" pin="IN" pad="4"/>
<connect gate="A" pin="NC" pad="7"/>
<connect gate="A" pin="NC_2" pad="2"/>
<connect gate="A" pin="OUT" pad="5"/>
<connect gate="A" pin="SEN" pad="6"/>
<connect gate="A" pin="~SD" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3879MR-1.0"/>
<attribute name="OC_FARNELL" value="1554782"/>
<attribute name="OC_NEWARK" value="79K7982"/>
<attribute name="PACKAGE" value="SOP-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3879MR-1.2" prefix="U">
<description>Voltage Regulator</description>
<gates>
<gate name="A" symbol="LP3879MR-1.2"/>
</gates>
<devices>
<device name="" package="SOIC127P600X168-9N">
<connects>
<connect gate="A" pin="BYPASS" pad="1"/>
<connect gate="A" pin="GND" pad="9"/>
<connect gate="A" pin="GND_2" pad="3"/>
<connect gate="A" pin="IN" pad="4"/>
<connect gate="A" pin="NC" pad="7"/>
<connect gate="A" pin="NC_2" pad="2"/>
<connect gate="A" pin="OUT" pad="5"/>
<connect gate="A" pin="SEN" pad="6"/>
<connect gate="A" pin="~SD" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3879MR-1.2"/>
<attribute name="OC_FARNELL" value="1554783"/>
<attribute name="OC_NEWARK" value="99K2577"/>
<attribute name="PACKAGE" value="SOP-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3879SD-1.0">
<description>Voltage Regulator</description>
<gates>
<gate name="A" symbol="LP3879SD-1.0"/>
</gates>
<devices>
<device name="" package="DFN400X400X80-9N">
<connects>
<connect gate="A" pin="BYPASS" pad="1"/>
<connect gate="A" pin="EP" pad="9"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="IN" pad="4"/>
<connect gate="A" pin="N/C" pad="2"/>
<connect gate="A" pin="N/C_2" pad="7"/>
<connect gate="A" pin="OUT" pad="5"/>
<connect gate="A" pin="SENSE" pad="6"/>
<connect gate="A" pin="~SHUTDOWN" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3879SD-1.0"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="99K2580"/>
<attribute name="PACKAGE" value="LLP-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3879SD-1.2">
<description>Voltage Regulator</description>
<gates>
<gate name="A" symbol="LP3879SD-1.2"/>
</gates>
<devices>
<device name="" package="DFN400X400X80-9N">
<connects>
<connect gate="A" pin="BYPASS" pad="1"/>
<connect gate="A" pin="EP" pad="9"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="IN" pad="4"/>
<connect gate="A" pin="N/C" pad="2"/>
<connect gate="A" pin="N/C_2" pad="7"/>
<connect gate="A" pin="OUT" pad="5"/>
<connect gate="A" pin="SENSE" pad="6"/>
<connect gate="A" pin="~SHUTDOWN" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3879SD-1.2"/>
<attribute name="OC_FARNELL" value="1685772"/>
<attribute name="OC_NEWARK" value="99K2583"/>
<attribute name="PACKAGE" value="LLP-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3881EMR-1.8" prefix="U">
<description>LDO</description>
<gates>
<gate name="A" symbol="LP3881EMR-1.8"/>
</gates>
<devices>
<device name="" package="SOP127P600X168-9N">
<connects>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="GND_2" pad="4"/>
<connect gate="A" pin="GND_3" pad="9"/>
<connect gate="A" pin="NC" pad="8"/>
<connect gate="A" pin="S/D" pad="6"/>
<connect gate="A" pin="VBIAS" pad="3"/>
<connect gate="A" pin="VIN" pad="7"/>
<connect gate="A" pin="VOUT" pad="2"/>
<connect gate="A" pin="VOUT_2" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3881EMR-1.8"/>
<attribute name="OC_FARNELL" value="1286786"/>
<attribute name="OC_NEWARK" value="-"/>
<attribute name="PACKAGE" value="SOP-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3881ES-1.2" prefix="U">
<description>Linear Regulator</description>
<gates>
<gate name="A" symbol="LP3881ES-1.2"/>
</gates>
<devices>
<device name="" package="TO17P1435X465-6N">
<connects>
<connect gate="A" pin="BIAS" pad="5"/>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="GND_2" pad="3"/>
<connect gate="A" pin="IN" pad="2"/>
<connect gate="A" pin="OUT" pad="4"/>
<connect gate="A" pin="~SD" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3881ES-1.2"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K7636"/>
<attribute name="PACKAGE" value="TO-263-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3881ES-1.5" prefix="U">
<description>Linear Regulator</description>
<gates>
<gate name="A" symbol="LP3881ES-1.5"/>
</gates>
<devices>
<device name="" package="TO17P1435X465-6N">
<connects>
<connect gate="A" pin="BIAS" pad="5"/>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="GND_2" pad="3"/>
<connect gate="A" pin="IN" pad="2"/>
<connect gate="A" pin="OUT" pad="4"/>
<connect gate="A" pin="~SD" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3881ES-1.5"/>
<attribute name="OC_FARNELL" value="8207062"/>
<attribute name="OC_NEWARK" value="41K7637"/>
<attribute name="PACKAGE" value="TO-263-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3881ET-1.5" prefix="U">
<description>IC REG LDO 0.8A 1.5V</description>
<gates>
<gate name="A" symbol="LP3881ET-1.5"/>
</gates>
<devices>
<device name="" package="TO170P470X1016X2092-5P">
<connects>
<connect gate="A" pin="*SHUTDOWN" pad="1"/>
<connect gate="A" pin="BIAS" pad="5"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="VIN" pad="2"/>
<connect gate="A" pin="VOUT" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3881ET-1.5"/>
<attribute name="OC_FARNELL" value="8207097"/>
<attribute name="OC_NEWARK" value="-"/>
<attribute name="PACKAGE" value="TO220-5"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3882EMR-1.2" prefix="U">
<description>LDO</description>
<gates>
<gate name="A" symbol="LP3882EMR-1.2"/>
</gates>
<devices>
<device name="" package="SOP127P600X168-9N">
<connects>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="GND_2" pad="4"/>
<connect gate="A" pin="GND_3" pad="9"/>
<connect gate="A" pin="NC" pad="8"/>
<connect gate="A" pin="VBIAS" pad="3"/>
<connect gate="A" pin="VIN" pad="7"/>
<connect gate="A" pin="VOUT" pad="2"/>
<connect gate="A" pin="VOUT_2" pad="1"/>
<connect gate="A" pin="~SD" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3882EMR-1.2"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K7645"/>
<attribute name="PACKAGE" value="SOP-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3882ES-1.2" prefix="U">
<description>Linear regulators</description>
<gates>
<gate name="A" symbol="LP3882ES-1.2"/>
</gates>
<devices>
<device name="" package="TO170P1435X465-6N">
<connects>
<connect gate="A" pin="BIAS" pad="5"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="GND_2" pad="6"/>
<connect gate="A" pin="IN" pad="2"/>
<connect gate="A" pin="OUT" pad="4"/>
<connect gate="A" pin="~SD" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3882ES-1.2"/>
<attribute name="OC_FARNELL" value="8207119"/>
<attribute name="OC_NEWARK" value="41K7651"/>
<attribute name="PACKAGE" value="TO-263-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3882ET-1.2" prefix="U">
<description>V REG LDO 1.5A +1.2V, 3882</description>
<gates>
<gate name="A" symbol="LP3882ET-1.2"/>
</gates>
<devices>
<device name="" package="TO170P470X1016X2092-5P">
<connects>
<connect gate="A" pin="*SHUTDOWN" pad="1"/>
<connect gate="A" pin="BIAS" pad="5"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="VIN" pad="2"/>
<connect gate="A" pin="VOUT" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3882ET-1.2"/>
<attribute name="OC_FARNELL" value="8207143"/>
<attribute name="OC_NEWARK" value="-"/>
<attribute name="PACKAGE" value="TO220-5"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3883ES-1.2" prefix="U">
<description>Linear regulators</description>
<gates>
<gate name="A" symbol="LP3883ES-1.2"/>
</gates>
<devices>
<device name="" package="TO170P1435X465-6N">
<connects>
<connect gate="A" pin="BIAS" pad="5"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="GND_2" pad="6"/>
<connect gate="A" pin="IN" pad="2"/>
<connect gate="A" pin="OUT" pad="4"/>
<connect gate="A" pin="~SD" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3883ES-1.2"/>
<attribute name="OC_FARNELL" value="8207178"/>
<attribute name="OC_NEWARK" value="38K3931"/>
<attribute name="PACKAGE" value="TO-263-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP38841MR-ADJ" prefix="U">
<description>Linear Regulators</description>
<gates>
<gate name="A" symbol="LP38841MR-ADJ"/>
</gates>
<devices>
<device name="" package="SOIC127P600X168-9N">
<connects>
<connect gate="A" pin="ADJ" pad="1"/>
<connect gate="A" pin="BIAS" pad="3"/>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="GND_2" pad="9"/>
<connect gate="A" pin="GND_3" pad="4"/>
<connect gate="A" pin="IN" pad="7"/>
<connect gate="A" pin="NC" pad="8"/>
<connect gate="A" pin="OUT" pad="2"/>
<connect gate="A" pin="~SD" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP38841MR-ADJ"/>
<attribute name="OC_FARNELL" value="1286789"/>
<attribute name="OC_NEWARK" value="41K7669"/>
<attribute name="PACKAGE" value="SOP-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP38841T-0.8" prefix="U">
<description>V REG LDO 0.8A 0.8V</description>
<gates>
<gate name="A" symbol="LP38841T-0.8"/>
</gates>
<devices>
<device name="" package="TO170P470X1016X2222-5P">
<connects>
<connect gate="A" pin="*SHUTDOWN" pad="1"/>
<connect gate="A" pin="BIAS" pad="5"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="INPUT" pad="2"/>
<connect gate="A" pin="OUTPUT" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP38841T-0.8"/>
<attribute name="OC_FARNELL" value="1008290"/>
<attribute name="OC_NEWARK" value="-"/>
<attribute name="PACKAGE" value="TO-220-5"/>
<attribute name="SUPPLIER" value="NATIONAL SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP38841T-1.5" prefix="U">
<description>V REG LDO 0.8A 1.5V</description>
<gates>
<gate name="A" symbol="LP38841T-1.5"/>
</gates>
<devices>
<device name="" package="TO170P470X1016X2222-5P">
<connects>
<connect gate="A" pin="*SHUTDOWN" pad="1"/>
<connect gate="A" pin="BIAS" pad="5"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="INPUT" pad="2"/>
<connect gate="A" pin="OUTPUT" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP38841T-1.5"/>
<attribute name="OC_FARNELL" value="1008292"/>
<attribute name="OC_NEWARK" value="-"/>
<attribute name="PACKAGE" value="TO-220-5"/>
<attribute name="SUPPLIER" value="NATIONAL SEMICONDUCTOR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP38842MR-ADJ" prefix="U">
<description>Linear Regulators</description>
<gates>
<gate name="A" symbol="LP38842MR-ADJ"/>
</gates>
<devices>
<device name="" package="SOIC127P600X168-9N">
<connects>
<connect gate="A" pin="ADJ" pad="1"/>
<connect gate="A" pin="BIAS" pad="3"/>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="GND_2" pad="9"/>
<connect gate="A" pin="GND_3" pad="4"/>
<connect gate="A" pin="IN" pad="7"/>
<connect gate="A" pin="NC" pad="8"/>
<connect gate="A" pin="OUT" pad="2"/>
<connect gate="A" pin="~SD" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP38842MR-ADJ"/>
<attribute name="OC_FARNELL" value="1286792"/>
<attribute name="OC_NEWARK" value="41K7680"/>
<attribute name="PACKAGE" value="SOP-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP38842S-1.2" prefix="U">
<description>Dropout Linear Regulator</description>
<gates>
<gate name="A" symbol="LP38842S-1.2"/>
</gates>
<devices>
<device name="" package="TO170P1435X465-6N">
<connects>
<connect gate="A" pin="BIAS" pad="5"/>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="GND_2" pad="3"/>
<connect gate="A" pin="IN" pad="2"/>
<connect gate="A" pin="OUT" pad="4"/>
<connect gate="A" pin="~SD" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP38842S-1.2"/>
<attribute name="OC_FARNELL" value="1008294"/>
<attribute name="OC_NEWARK" value="41K7683"/>
<attribute name="PACKAGE" value="TO-263-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP38843S-1.2" prefix="U">
<description>Ultra Low Dropout Linear Regulators</description>
<gates>
<gate name="A" symbol="LP38843S-1.2"/>
</gates>
<devices>
<device name="" package="TO170P1435X457-5N">
<connects>
<connect gate="A" pin="BIAS" pad="5"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="GND_2" pad="6"/>
<connect gate="A" pin="IN" pad="2"/>
<connect gate="A" pin="OUT" pad="4"/>
<connect gate="A" pin="~SHUTDOWN" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP38843S-1.2"/>
<attribute name="OC_FARNELL" value="1008300"/>
<attribute name="OC_NEWARK" value="41K7692"/>
<attribute name="PACKAGE" value="TO-263-5"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP38843T-1.5" prefix="U">
<description>V REG LDO 3A 1.5V</description>
<gates>
<gate name="A" symbol="LP38843T-1.5"/>
</gates>
<devices>
<device name="" package="TO170P470X1016X2092-5P">
<connects>
<connect gate="A" pin="*SHUTDOWN" pad="1"/>
<connect gate="A" pin="BIAS" pad="5"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="VIN" pad="2"/>
<connect gate="A" pin="VOUT" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP38843T-1.5"/>
<attribute name="OC_FARNELL" value="1008305"/>
<attribute name="OC_NEWARK" value="-"/>
<attribute name="PACKAGE" value="TO220-5"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP38851MR-ADJ" prefix="U">
<description>LDO Linear Regulator</description>
<gates>
<gate name="A" symbol="LP38851MR-ADJ"/>
</gates>
<devices>
<device name="" package="SOIC127P600X168-9N">
<connects>
<connect gate="A" pin="ADJ" pad="1"/>
<connect gate="A" pin="BIAS" pad="3"/>
<connect gate="A" pin="EN" pad="6"/>
<connect gate="A" pin="GND" pad="9"/>
<connect gate="A" pin="GND_2" pad="4"/>
<connect gate="A" pin="IN" pad="7"/>
<connect gate="A" pin="N/C" pad="8"/>
<connect gate="A" pin="OUT" pad="2"/>
<connect gate="A" pin="SS" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP38851MR-ADJ"/>
<attribute name="OC_FARNELL" value="1798337"/>
<attribute name="OC_NEWARK" value="73R9756"/>
<attribute name="PACKAGE" value="SOP-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP38851S-ADJ" prefix="U">
<description>LP38851S-ADJ</description>
<gates>
<gate name="A" symbol="LP38851S-ADJ"/>
</gates>
<devices>
<device name="" package="TO127P1435X457-7N">
<connects>
<connect gate="A" pin="ADJ" pad="5"/>
<connect gate="A" pin="BIAS" pad="7"/>
<connect gate="A" pin="EN" pad="2"/>
<connect gate="A" pin="EPAD" pad="8"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="IN" pad="3"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="SS" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP38851S-ADJ"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="54M4714"/>
<attribute name="PACKAGE" value="TO-263-7"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP38851T-ADJ" prefix="U">
<description>LP38851T-ADJ</description>
<gates>
<gate name="A" symbol="LP38851T-ADJ"/>
</gates>
<devices>
<device name="" package="TO127P469X1016X2102-7P">
<connects>
<connect gate="A" pin="ADJ" pad="5"/>
<connect gate="A" pin="BIAS" pad="7"/>
<connect gate="A" pin="EN" pad="2"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="IN" pad="3"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="SS" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP38851T-ADJ"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="46M5590"/>
<attribute name="PACKAGE" value="TO220-7"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP38852S-ADJ" prefix="U">
<description>LP38852S-ADJ</description>
<gates>
<gate name="A" symbol="LP38852S-ADJ"/>
</gates>
<devices>
<device name="" package="TO127P1435X457-7N">
<connects>
<connect gate="A" pin="ADJ" pad="5"/>
<connect gate="A" pin="BIAS" pad="7"/>
<connect gate="A" pin="EN" pad="2"/>
<connect gate="A" pin="EPAD" pad="8"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="IN" pad="3"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="SS" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP38852S-ADJ"/>
<attribute name="OC_FARNELL" value="1694494"/>
<attribute name="OC_NEWARK" value="32M1316"/>
<attribute name="PACKAGE" value="TO-263-7"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP38853MR-ADJ" prefix="U">
<description>REG LDO</description>
<gates>
<gate name="A" symbol="LP38853MR-ADJ"/>
</gates>
<devices>
<device name="" package="SOIC127P600X168-9N">
<connects>
<connect gate="A" pin="ADJ" pad="1"/>
<connect gate="A" pin="BIAS" pad="3"/>
<connect gate="A" pin="EN" pad="6"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="GND_2" pad="9"/>
<connect gate="A" pin="IN" pad="7"/>
<connect gate="A" pin="NC" pad="8"/>
<connect gate="A" pin="OUT" pad="2"/>
<connect gate="A" pin="SS" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP38853MR-ADJ"/>
<attribute name="OC_FARNELL" value="1320982"/>
<attribute name="OC_NEWARK" value="31M5516"/>
<attribute name="PACKAGE" value="SOP-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP38853S-ADJ" prefix="U">
<description>Linear Regulator</description>
<gates>
<gate name="A" symbol="LP38853S-ADJ"/>
</gates>
<devices>
<device name="" package="TO127P1435X464-8N">
<connects>
<connect gate="A" pin="ADJ" pad="5"/>
<connect gate="A" pin="BIAS" pad="7"/>
<connect gate="A" pin="EN" pad="2"/>
<connect gate="A" pin="GND" pad="8"/>
<connect gate="A" pin="GND_2" pad="4"/>
<connect gate="A" pin="IN" pad="3"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="SS" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP38853S-ADJ"/>
<attribute name="OC_FARNELL" value="1320983"/>
<attribute name="OC_NEWARK" value="32M1324"/>
<attribute name="PACKAGE" value="TO-263-7"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP38853T-ADJ" prefix="U">
<description>LP38853T-ADJ</description>
<gates>
<gate name="A" symbol="LP38853T-ADJ"/>
</gates>
<devices>
<device name="" package="TO127P469X1016X2102-7P">
<connects>
<connect gate="A" pin="ADJ" pad="5"/>
<connect gate="A" pin="BIAS" pad="7"/>
<connect gate="A" pin="EN" pad="2"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="IN" pad="3"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="SS" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP38853T-ADJ"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="32M1326"/>
<attribute name="PACKAGE" value="TO220-7"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP38855T-0.8" prefix="U">
<description>LP38855T-0.8</description>
<gates>
<gate name="A" symbol="LP38855T-0.8"/>
</gates>
<devices>
<device name="" package="TO170P470X1016X2092-5P">
<connects>
<connect gate="A" pin="BIAS" pad="5"/>
<connect gate="A" pin="EN" pad="1"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="IN" pad="2"/>
<connect gate="A" pin="VOUT" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP38855T-0.8"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="32M1331"/>
<attribute name="PACKAGE" value="TO220-5"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP38855T-1.2" prefix="U">
<description>IC, LDO VOLT REG, 1.2V, 1.5A,</description>
<gates>
<gate name="A" symbol="LP38855T-1.2"/>
</gates>
<devices>
<device name="" package="TO170P470X1016X2092-5P">
<connects>
<connect gate="A" pin="BIAS" pad="5"/>
<connect gate="A" pin="EN" pad="1"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="IN" pad="2"/>
<connect gate="A" pin="VOUT" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP38855T-1.2"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="32M1332"/>
<attribute name="PACKAGE" value="TO220-5"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP38856S-0.8" prefix="U">
<description>Fast-Response High-Accuracy LDO Linear Regulator</description>
<gates>
<gate name="A" symbol="LP38856S-0.8"/>
</gates>
<devices>
<device name="" package="TO170P1435X457-5N">
<connects>
<connect gate="A" pin="BIAS" pad="5"/>
<connect gate="A" pin="EN" pad="1"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="GND_2" pad="6"/>
<connect gate="A" pin="IN" pad="2"/>
<connect gate="A" pin="OUT" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP38856S-0.8"/>
<attribute name="OC_FARNELL" value="1286793"/>
<attribute name="OC_NEWARK" value="-"/>
<attribute name="PACKAGE" value="TO-263-5"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP38856S-1.2" prefix="U">
<description>Linear Regulator</description>
<gates>
<gate name="A" symbol="LP38856S-1.2"/>
</gates>
<devices>
<device name="" package="TO170P1435X465-6N">
<connects>
<connect gate="A" pin="BIAS" pad="5"/>
<connect gate="A" pin="EN" pad="1"/>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="GND_2" pad="3"/>
<connect gate="A" pin="IN" pad="2"/>
<connect gate="A" pin="OUT" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP38856S-1.2"/>
<attribute name="OC_FARNELL" value="1286794"/>
<attribute name="OC_NEWARK" value="13M1968"/>
<attribute name="PACKAGE" value="TO-263-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP38856T-0.8" prefix="U">
<description>V REG LDO DR 3.0A 0.8V</description>
<gates>
<gate name="A" symbol="LP38856T-0.8"/>
</gates>
<devices>
<device name="" package="TO170P470X1016X2092-5P">
<connects>
<connect gate="A" pin="BIAS" pad="5"/>
<connect gate="A" pin="EN" pad="1"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="IN" pad="2"/>
<connect gate="A" pin="VOUT" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP38856T-0.8"/>
<attribute name="OC_FARNELL" value="1286795"/>
<attribute name="OC_NEWARK" value="-"/>
<attribute name="PACKAGE" value="TO220-5"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP38856T-1.2" prefix="U">
<description>V REG LDO DR 3.0A 1.2V</description>
<gates>
<gate name="A" symbol="LP38856T-1.2"/>
</gates>
<devices>
<device name="" package="TO170P470X1016X2092-5P">
<connects>
<connect gate="A" pin="BIAS" pad="5"/>
<connect gate="A" pin="EN" pad="1"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="IN" pad="2"/>
<connect gate="A" pin="VOUT" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP38856T-1.2"/>
<attribute name="OC_FARNELL" value="1286796"/>
<attribute name="OC_NEWARK" value="-"/>
<attribute name="PACKAGE" value="TO220-5"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP38858T-0.8" prefix="U">
<description>IC, LDO VOLT REG, 800mV</description>
<gates>
<gate name="A" symbol="LP38858T-0.8"/>
</gates>
<devices>
<device name="" package="TO170P470X1016X2092-5P">
<connects>
<connect gate="A" pin="*SS" pad="1"/>
<connect gate="A" pin="BIAS" pad="5"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="IN" pad="2"/>
<connect gate="A" pin="VOUT" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP38858T-0.8"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="32M1337"/>
<attribute name="PACKAGE" value="TO220-5"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP38858T-1.2" prefix="U">
<description>IC, LDO VOLT REG, 1.2V, 1.5A</description>
<gates>
<gate name="A" symbol="LP38858T-1.2"/>
</gates>
<devices>
<device name="" package="TO170P470X1016X2092-5P">
<connects>
<connect gate="A" pin="*SS" pad="1"/>
<connect gate="A" pin="BIAS" pad="5"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="IN" pad="2"/>
<connect gate="A" pin="VOUT" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP38858T-1.2"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="32M1338"/>
<attribute name="PACKAGE" value="TO220-5"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP38859S-1.2" prefix="U">
<description>Linear Regulator</description>
<gates>
<gate name="A" symbol="LP38859S-1.2"/>
</gates>
<devices>
<device name="" package="TO170P1435X465-6N">
<connects>
<connect gate="A" pin="BIAS" pad="5"/>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="GND_2" pad="3"/>
<connect gate="A" pin="IN" pad="2"/>
<connect gate="A" pin="OUT" pad="4"/>
<connect gate="A" pin="SS" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP38859S-12"/>
<attribute name="OC_FARNELL" value="1286798"/>
<attribute name="OC_NEWARK" value="13M1980"/>
<attribute name="PACKAGE" value="TO-263-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP38859T-0.8" prefix="U">
<description>V REG LDO DR 3.0A 0.8V</description>
<gates>
<gate name="A" symbol="LP38859T-0.8"/>
</gates>
<devices>
<device name="" package="TO170P470X1016X2092-5P">
<connects>
<connect gate="A" pin="*SS" pad="1"/>
<connect gate="A" pin="BIAS" pad="5"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="IN" pad="2"/>
<connect gate="A" pin="VOUT" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP38859T-0.8"/>
<attribute name="OC_FARNELL" value="1286799"/>
<attribute name="OC_NEWARK" value="-"/>
<attribute name="PACKAGE" value="TO220-5"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP38859T-1.2" prefix="U">
<description>Fast-Response High-Accuracy LDO Linear Regulator</description>
<gates>
<gate name="A" symbol="LP38859T-1.2"/>
</gates>
<devices>
<device name="" package="TO170P1435X457-5N">
<connects>
<connect gate="A" pin="BIAS" pad="5"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="GND_2" pad="6"/>
<connect gate="A" pin="IN" pad="2"/>
<connect gate="A" pin="OUT" pad="4"/>
<connect gate="A" pin="SS" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP38859T-1.2"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="13M1987"/>
<attribute name="PACKAGE" value="TO-263-5"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3891EMR-1.2" prefix="U">
<description>Fast-Response Ultra Low Dropout Linear Regulators</description>
<gates>
<gate name="A" symbol="LP3891EMR-1.2"/>
</gates>
<devices>
<device name="" package="SOIC127P600X168-9N">
<connects>
<connect gate="A" pin="BIAS" pad="3"/>
<connect gate="A" pin="EPAD" pad="9"/>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="GND_2" pad="4"/>
<connect gate="A" pin="NC" pad="8"/>
<connect gate="A" pin="S/D" pad="6"/>
<connect gate="A" pin="VIN" pad="7"/>
<connect gate="A" pin="VOUT" pad="2"/>
<connect gate="A" pin="VOUT_2" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3891EMR-12"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K7700"/>
<attribute name="PACKAGE" value="SOP-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3891ES-1.2" prefix="U">
<description>Linear regulators</description>
<gates>
<gate name="A" symbol="LP3891ES-1.2"/>
</gates>
<devices>
<device name="" package="TO170P1435X465-6N">
<connects>
<connect gate="A" pin="BIAS" pad="5"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="GND_2" pad="6"/>
<connect gate="A" pin="IN" pad="2"/>
<connect gate="A" pin="OUT" pad="4"/>
<connect gate="A" pin="~SD" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3891ES-1.2"/>
<attribute name="OC_FARNELL" value="1286968"/>
<attribute name="OC_NEWARK" value="24M3600"/>
<attribute name="PACKAGE" value="TO-263-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3891ET-1.5" prefix="U">
<description>V REG LDO DR 0.8A 1.5V</description>
<gates>
<gate name="A" symbol="LP3891ET-1.5"/>
</gates>
<devices>
<device name="" package="TO170P470X1016X2092-5P">
<connects>
<connect gate="A" pin="*SHUTDOWN" pad="1"/>
<connect gate="A" pin="BIAS" pad="5"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="VIN" pad="2"/>
<connect gate="A" pin="VOUT" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3891ET-1.5"/>
<attribute name="OC_FARNELL" value="1286972"/>
<attribute name="OC_NEWARK" value="-"/>
<attribute name="PACKAGE" value="TO220-5"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3892ES-1.2" prefix="U">
<description>Linear regulators</description>
<gates>
<gate name="A" symbol="LP3892ES-1.2"/>
</gates>
<devices>
<device name="" package="TO170P1435X465-6N">
<connects>
<connect gate="A" pin="BIAS" pad="5"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="GND_2" pad="6"/>
<connect gate="A" pin="IN" pad="2"/>
<connect gate="A" pin="OUT" pad="4"/>
<connect gate="A" pin="~SD" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3892ES-1.2"/>
<attribute name="OC_FARNELL" value="1286978"/>
<attribute name="OC_NEWARK" value="41K7721"/>
<attribute name="PACKAGE" value="TO-263-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3892ES-1.5" prefix="U">
<description>Fast-Response High-Accuracy LDO Linear Regulator</description>
<gates>
<gate name="A" symbol="LP3892ES-1.5"/>
</gates>
<devices>
<device name="" package="TO170P1435X457-5N">
<connects>
<connect gate="A" pin="BIAS" pad="5"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="GND_2" pad="6"/>
<connect gate="A" pin="IN" pad="2"/>
<connect gate="A" pin="OUT" pad="4"/>
<connect gate="A" pin="~SHUTDOWN" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3892ES-1.5"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K7722"/>
<attribute name="PACKAGE" value="TO-263-5"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3892ET-1.2" prefix="U">
<description>V REG LDO DR 1.5A 1.2V</description>
<gates>
<gate name="A" symbol="LP3892ET-1.2"/>
</gates>
<devices>
<device name="" package="TO170P470X1016X2092-5P">
<connects>
<connect gate="A" pin="*SHUTDOWN" pad="1"/>
<connect gate="A" pin="BIAS" pad="5"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="VIN" pad="2"/>
<connect gate="A" pin="VOUT" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3892ET-1.2"/>
<attribute name="OC_FARNELL" value="1286980"/>
<attribute name="OC_NEWARK" value="-"/>
<attribute name="PACKAGE" value="TO220-5"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3893ES-1.2" prefix="U">
<description>Fast-Response High-Accuracy LDO Linear Regulator</description>
<gates>
<gate name="A" symbol="LP3893ES-1.2"/>
</gates>
<devices>
<device name="" package="TO170P1435X457-5N">
<connects>
<connect gate="A" pin="BIAS" pad="5"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="GND_2" pad="6"/>
<connect gate="A" pin="IN" pad="2"/>
<connect gate="A" pin="OUT" pad="4"/>
<connect gate="A" pin="~SHUTDOWN" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3893ES-1.2"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K7730"/>
<attribute name="PACKAGE" value="TO-263-5"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3893ET-1.5" prefix="U">
<description>V REG LDO DR 3A 1.5V, SMD,</description>
<gates>
<gate name="A" symbol="LP3893ET-1.5"/>
</gates>
<devices>
<device name="" package="TO170P470X1016X2092-5P">
<connects>
<connect gate="A" pin="*SHUTDOWN" pad="1"/>
<connect gate="A" pin="BIAS" pad="5"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="VIN" pad="2"/>
<connect gate="A" pin="VOUT" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3893ET-1.5"/>
<attribute name="OC_FARNELL" value="1286988"/>
<attribute name="OC_NEWARK" value="-"/>
<attribute name="PACKAGE" value="TO220-5"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3918TL-A" prefix="U">
<description>Battery Charge Management and Regulator Unit</description>
<gates>
<gate name="A" symbol="LP3918TL-A"/>
</gates>
<devices>
<device name="" package="BGA25C5X5X50P_246X246X67">
<connects>
<connect gate="A" pin="ACOK_N" pad="A5"/>
<connect gate="A" pin="BATT" pad="C1"/>
<connect gate="A" pin="CHGIN" pad="B1"/>
<connect gate="A" pin="GNDA" pad="D3"/>
<connect gate="A" pin="HF_PWR" pad="C2"/>
<connect gate="A" pin="IMON" pad="A1"/>
<connect gate="A" pin="LDO1" pad="E1"/>
<connect gate="A" pin="LDO2" pad="E2"/>
<connect gate="A" pin="LDO3" pad="E3"/>
<connect gate="A" pin="LDO4" pad="E4"/>
<connect gate="A" pin="LDO5" pad="D5"/>
<connect gate="A" pin="LDO6" pad="C5"/>
<connect gate="A" pin="LDO7" pad="B5"/>
<connect gate="A" pin="PON_N" pad="B4"/>
<connect gate="A" pin="PS_HOLD" pad="A2"/>
<connect gate="A" pin="PWR_ON" pad="B2"/>
<connect gate="A" pin="RESET_N" pad="A4"/>
<connect gate="A" pin="RX_EN" pad="D4"/>
<connect gate="A" pin="SCL" pad="B3"/>
<connect gate="A" pin="SDA" pad="C3"/>
<connect gate="A" pin="TCXO_EN" pad="D2"/>
<connect gate="A" pin="TX_EN" pad="C4"/>
<connect gate="A" pin="VIN1" pad="D1"/>
<connect gate="A" pin="VIN2" pad="E5"/>
<connect gate="A" pin="VSS" pad="A3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DESCRIPTION" value="Battery Charge Management and Regulator Unit"/>
<attribute name="MPN" value="LP3918TL-A"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="38P0394"/>
<attribute name="PACKAGE" value="BGA-25"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3918TL" prefix="U">
<description>Battery Charge Management and Regulator Unit</description>
<gates>
<gate name="A" symbol="LP3918TL"/>
</gates>
<devices>
<device name="" package="BGA25C5X5X50P_246X246X67">
<connects>
<connect gate="A" pin="ACOK_N" pad="A5"/>
<connect gate="A" pin="BATT" pad="C1"/>
<connect gate="A" pin="CHGIN" pad="B1"/>
<connect gate="A" pin="GNDA" pad="D3"/>
<connect gate="A" pin="HF_PWR" pad="C2"/>
<connect gate="A" pin="IMON" pad="A1"/>
<connect gate="A" pin="LDO1" pad="E1"/>
<connect gate="A" pin="LDO2" pad="E2"/>
<connect gate="A" pin="LDO3" pad="E3"/>
<connect gate="A" pin="LDO4" pad="E4"/>
<connect gate="A" pin="LDO5" pad="D5"/>
<connect gate="A" pin="LDO6" pad="C5"/>
<connect gate="A" pin="LDO7" pad="B5"/>
<connect gate="A" pin="PON_N" pad="B4"/>
<connect gate="A" pin="PS_HOLD" pad="A2"/>
<connect gate="A" pin="PWR_ON" pad="B2"/>
<connect gate="A" pin="RESET_N" pad="A4"/>
<connect gate="A" pin="RX_EN" pad="D4"/>
<connect gate="A" pin="SCL" pad="B3"/>
<connect gate="A" pin="SDA" pad="C3"/>
<connect gate="A" pin="TCXO_EN" pad="D2"/>
<connect gate="A" pin="TX_EN" pad="C4"/>
<connect gate="A" pin="VIN1" pad="D1"/>
<connect gate="A" pin="VIN2" pad="E5"/>
<connect gate="A" pin="VSS" pad="A3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DESCRIPTION" value="Battery Charge Management and Regulator Unit"/>
<attribute name="MPN" value="LP3918TL"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="66M8448"/>
<attribute name="PACKAGE" value="BGA-25"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3921SQ" prefix="U">
<description>Battery Charger Management and Regulator Unit</description>
<gates>
<gate name="A" symbol="LP3921SQ"/>
</gates>
<devices>
<device name="" package="QFN50P500X500X80-33N">
<connects>
<connect gate="A" pin="ACOK_N" pad="31"/>
<connect gate="A" pin="BATT" pad="21"/>
<connect gate="A" pin="BYPASS" pad="12"/>
<connect gate="A" pin="CHG_IN" pad="22"/>
<connect gate="A" pin="EPAD" pad="33"/>
<connect gate="A" pin="GND" pad="11"/>
<connect gate="A" pin="GNDA" pad="18"/>
<connect gate="A" pin="HF_PWR" pad="27"/>
<connect gate="A" pin="IMON" pad="24"/>
<connect gate="A" pin="IN+" pad="9"/>
<connect gate="A" pin="IN-" pad="10"/>
<connect gate="A" pin="LDO1" pad="16"/>
<connect gate="A" pin="LDO2" pad="15"/>
<connect gate="A" pin="LDO3" pad="14"/>
<connect gate="A" pin="LDO4" pad="13"/>
<connect gate="A" pin="LDO5" pad="3"/>
<connect gate="A" pin="LDO6" pad="1"/>
<connect gate="A" pin="LDO7" pad="5"/>
<connect gate="A" pin="OUT+" pad="6"/>
<connect gate="A" pin="OUT-" pad="8"/>
<connect gate="A" pin="PON_N" pad="29"/>
<connect gate="A" pin="PS_HOLD" pad="25"/>
<connect gate="A" pin="PWR_ON" pad="23"/>
<connect gate="A" pin="RESET_N" pad="30"/>
<connect gate="A" pin="RX_EN" pad="32"/>
<connect gate="A" pin="SCL" pad="20"/>
<connect gate="A" pin="SDA" pad="19"/>
<connect gate="A" pin="TCXO_EN" pad="26"/>
<connect gate="A" pin="TX_EN" pad="2"/>
<connect gate="A" pin="VDD" pad="7"/>
<connect gate="A" pin="VIN1" pad="17"/>
<connect gate="A" pin="VIN2" pad="4"/>
<connect gate="A" pin="VSS" pad="28"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3921SQ"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="04R9353"/>
<attribute name="PACKAGE" value="QFN-32"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3943ISQ" prefix="U">
<description>16-LED Fun Light Driver</description>
<gates>
<gate name="A" symbol="LP3943ISQ"/>
</gates>
<devices>
<device name="" package="QFN50P400X400X80-26N">
<connects>
<connect gate="A" pin="A0" pad="22"/>
<connect gate="A" pin="A1" pad="23"/>
<connect gate="A" pin="A2" pad="24"/>
<connect gate="A" pin="EPAD" pad="25"/>
<connect gate="A" pin="GND" pad="9"/>
<connect gate="A" pin="LED0" pad="1"/>
<connect gate="A" pin="LED1" pad="2"/>
<connect gate="A" pin="LED10" pad="12"/>
<connect gate="A" pin="LED11" pad="13"/>
<connect gate="A" pin="LED12" pad="14"/>
<connect gate="A" pin="LED13" pad="15"/>
<connect gate="A" pin="LED14" pad="16"/>
<connect gate="A" pin="LED15" pad="17"/>
<connect gate="A" pin="LED2" pad="3"/>
<connect gate="A" pin="LED3" pad="4"/>
<connect gate="A" pin="LED4" pad="5"/>
<connect gate="A" pin="LED5" pad="6"/>
<connect gate="A" pin="LED6" pad="7"/>
<connect gate="A" pin="LED7" pad="8"/>
<connect gate="A" pin="LED8" pad="10"/>
<connect gate="A" pin="LED9" pad="11"/>
<connect gate="A" pin="SCL" pad="19"/>
<connect gate="A" pin="SDA" pad="20"/>
<connect gate="A" pin="VDD" pad="21"/>
<connect gate="A" pin="~RST" pad="18"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3943ISQ"/>
<attribute name="OC_FARNELL" value="8206872"/>
<attribute name="OC_NEWARK" value="41K7750"/>
<attribute name="PACKAGE" value="QFN-24"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3947ISD-51" prefix="U">
<description>USB/AC Adaptor</description>
<gates>
<gate name="A" symbol="LP3947ISD-51"/>
</gates>
<devices>
<device name="" package="DFN400X400X80-15N">
<connects>
<connect gate="A" pin="BATT" pad="4"/>
<connect gate="A" pin="CHG" pad="12"/>
<connect gate="A" pin="CHG-IN" pad="14"/>
<connect gate="A" pin="DIFF-AMP" pad="8"/>
<connect gate="A" pin="EN" pad="1"/>
<connect gate="A" pin="EOC" pad="10"/>
<connect gate="A" pin="EP" pad="15"/>
<connect gate="A" pin="GND" pad="11"/>
<connect gate="A" pin="ISEL" pad="13"/>
<connect gate="A" pin="MODE" pad="7"/>
<connect gate="A" pin="SCL" pad="2"/>
<connect gate="A" pin="SDA" pad="3"/>
<connect gate="A" pin="TS" pad="9"/>
<connect gate="A" pin="VBSENSE" pad="6"/>
<connect gate="A" pin="VT" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3947ISD-51"/>
<attribute name="OC_FARNELL" value="1312623"/>
<attribute name="OC_NEWARK" value="31M5520"/>
<attribute name="PACKAGE" value="LLP-14"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3952RL" prefix="U">
<description>6-Channel Color LED Driver</description>
<gates>
<gate name="A" symbol="LP3952RL"/>
</gates>
<devices>
<device name="" package="BGA36C5X5X50P_300X300X72">
<connects>
<connect gate="A" pin="ADDR_SEL" pad="C4"/>
<connect gate="A" pin="ASE" pad="D2"/>
<connect gate="A" pin="B1" pad="A6"/>
<connect gate="A" pin="B2" pad="A2"/>
<connect gate="A" pin="FB" pad="E6"/>
<connect gate="A" pin="G1" pad="B6"/>
<connect gate="A" pin="G2" pad="A3"/>
<connect gate="A" pin="GND" pad="E5"/>
<connect gate="A" pin="GNDA" pad="D1"/>
<connect gate="A" pin="GNDT" pad="B2"/>
<connect gate="A" pin="GND_10" pad="D6"/>
<connect gate="A" pin="GND_11" pad="C3"/>
<connect gate="A" pin="GND_2" pad="F1"/>
<connect gate="A" pin="GND_3" pad="F2"/>
<connect gate="A" pin="GND_4" pad="F3"/>
<connect gate="A" pin="GND_5" pad="F4"/>
<connect gate="A" pin="GND_6" pad="E1"/>
<connect gate="A" pin="GND_7" pad="E2"/>
<connect gate="A" pin="GND_8" pad="E3"/>
<connect gate="A" pin="GND_9" pad="E4"/>
<connect gate="A" pin="GND_RGB" pad="A5"/>
<connect gate="A" pin="GND_SW" pad="F5"/>
<connect gate="A" pin="IRGB" pad="B5"/>
<connect gate="A" pin="IRT" pad="C2"/>
<connect gate="A" pin="NRST" pad="B4"/>
<connect gate="A" pin="PWM" pad="D4"/>
<connect gate="A" pin="R1" pad="C6"/>
<connect gate="A" pin="R2" pad="A4"/>
<connect gate="A" pin="SCL" pad="B3"/>
<connect gate="A" pin="SDA" pad="C5"/>
<connect gate="A" pin="SW" pad="F6"/>
<connect gate="A" pin="VDD1" pad="D3"/>
<connect gate="A" pin="VDD2" pad="A1"/>
<connect gate="A" pin="VDDA" pad="B1"/>
<connect gate="A" pin="VDDIO" pad="D5"/>
<connect gate="A" pin="VREF" pad="C1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3952RL"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="54M4742"/>
<attribute name="PACKAGE" value="BGA-36"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP39542RL" prefix="U">
<description>Lighting Management Unit</description>
<gates>
<gate name="A" symbol="LP39542RL"/>
</gates>
<devices>
<device name="" package="BGA36C50P6X6_300X300X67">
<connects>
<connect gate="A" pin="ADDR_SEL" pad="C4"/>
<connect gate="A" pin="ASE" pad="D2"/>
<connect gate="A" pin="B1" pad="A6"/>
<connect gate="A" pin="B2" pad="A2"/>
<connect gate="A" pin="FB" pad="E6"/>
<connect gate="A" pin="FLASH" pad="D6"/>
<connect gate="A" pin="FLASH_EN" pad="C3"/>
<connect gate="A" pin="G1" pad="B6"/>
<connect gate="A" pin="G2" pad="A3"/>
<connect gate="A" pin="GND" pad="E5"/>
<connect gate="A" pin="GNDA" pad="D1"/>
<connect gate="A" pin="GNDT" pad="B2"/>
<connect gate="A" pin="GND_RGB" pad="A5"/>
<connect gate="A" pin="GND_SW" pad="F5"/>
<connect gate="A" pin="GND_WLED" pad="F4"/>
<connect gate="A" pin="IFLASH" pad="E4"/>
<connect gate="A" pin="IRGB" pad="B5"/>
<connect gate="A" pin="IRT" pad="C2"/>
<connect gate="A" pin="NRST" pad="B4"/>
<connect gate="A" pin="R1" pad="C6"/>
<connect gate="A" pin="R2" pad="A4"/>
<connect gate="A" pin="SCL" pad="B3"/>
<connect gate="A" pin="SDA" pad="C5"/>
<connect gate="A" pin="SW" pad="F6"/>
<connect gate="A" pin="SYNC_PWM" pad="D4"/>
<connect gate="A" pin="VDD1" pad="D3"/>
<connect gate="A" pin="VDD2" pad="A1"/>
<connect gate="A" pin="VDDA" pad="B1"/>
<connect gate="A" pin="VDDIO" pad="D5"/>
<connect gate="A" pin="VREF" pad="C1"/>
<connect gate="A" pin="WLED1" pad="F1"/>
<connect gate="A" pin="WLED2" pad="E1"/>
<connect gate="A" pin="WLED3" pad="F2"/>
<connect gate="A" pin="WLED4" pad="E2"/>
<connect gate="A" pin="WLED5" pad="F3"/>
<connect gate="A" pin="WLED6" pad="E3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP39542RL"/>
<attribute name="OC_FARNELL" value="1506814"/>
<attribute name="OC_NEWARK" value="64M7081"/>
<attribute name="PACKAGE" value="BGA-36"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3961EMP-1.8" prefix="U">
<description>Dropout Linear  Regulator</description>
<gates>
<gate name="A" symbol="LP3961EMP-1.8"/>
</gates>
<devices>
<device name="" package="SOT150P696X180-5N">
<connects>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="VIN" pad="2"/>
<connect gate="A" pin="VOUT" pad="3"/>
<connect gate="A" pin="~ERR" pad="4"/>
<connect gate="A" pin="~SD" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3961EMP-1.8"/>
<attribute name="OC_FARNELL" value="9778705"/>
<attribute name="OC_NEWARK" value="41K7765"/>
<attribute name="PACKAGE" value="SOT-223-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3961EMP-2.5" prefix="U">
<description>Dropout Linear  Regulator</description>
<gates>
<gate name="A" symbol="LP3961EMP-2.5"/>
</gates>
<devices>
<device name="" package="SOT150P696X180-5N">
<connects>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="VIN" pad="2"/>
<connect gate="A" pin="VOUT" pad="3"/>
<connect gate="A" pin="~ERR" pad="4"/>
<connect gate="A" pin="~SD" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3961EMP-2.5"/>
<attribute name="OC_FARNELL" value="9778713"/>
<attribute name="OC_NEWARK" value="74C5357"/>
<attribute name="PACKAGE" value="SOT-223-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3961EMP-3.3" prefix="U">
<description>Dropout Linear  Regulator</description>
<gates>
<gate name="A" symbol="LP3961EMP-3.3"/>
</gates>
<devices>
<device name="" package="SOT150P696X180-5N">
<connects>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="VIN" pad="2"/>
<connect gate="A" pin="VOUT" pad="3"/>
<connect gate="A" pin="~ERR" pad="4"/>
<connect gate="A" pin="~SD" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3961EMP-3.3"/>
<attribute name="OC_FARNELL" value="9778721"/>
<attribute name="OC_NEWARK" value="41K7767"/>
<attribute name="PACKAGE" value="SOT-223-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3961EMP-5.0" prefix="U">
<description>Fast Ultra Low Dropout Linear Regulators</description>
<gates>
<gate name="A" symbol="LP3961EMP-5.0"/>
</gates>
<devices>
<device name="" package="SOT150P696X180-5N">
<connects>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="VIN" pad="2"/>
<connect gate="A" pin="VOUT" pad="3"/>
<connect gate="A" pin="~ERROR" pad="4"/>
<connect gate="A" pin="~SD" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3961EMP-50"/>
<attribute name="OC_FARNELL" value="1685735"/>
<attribute name="OC_NEWARK" value="41K7768"/>
<attribute name="PACKAGE" value="TO-223-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3961ES-1.8" prefix="U">
<description>Fast Ultra Low Dropout Linear Regulators</description>
<gates>
<gate name="A" symbol="LP3961ES-1.8"/>
</gates>
<devices>
<device name="" package="TO170P1435X457-5N">
<connects>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="GND_2" pad="6"/>
<connect gate="A" pin="VIN" pad="2"/>
<connect gate="A" pin="VOUT" pad="4"/>
<connect gate="A" pin="~ERROR/SENSE/ADJ" pad="5"/>
<connect gate="A" pin="~SD" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3961ES-1.8"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K7773"/>
<attribute name="PACKAGE" value="TO-263-5"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3961ES-2.5" prefix="U">
<description>Linear regulators</description>
<gates>
<gate name="A" symbol="LP3961ES-2.5"/>
</gates>
<devices>
<device name="" package="TO170P1435X465-6N">
<connects>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="GND_2" pad="6"/>
<connect gate="A" pin="VIN" pad="2"/>
<connect gate="A" pin="VOUT" pad="4"/>
<connect gate="A" pin="~ERROR" pad="5"/>
<connect gate="A" pin="~SD" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3961ES-2.5"/>
<attribute name="OC_FARNELL" value="9486437"/>
<attribute name="OC_NEWARK" value="41K7774"/>
<attribute name="PACKAGE" value="TO-263-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3961ES-3.3" prefix="U">
<description>Linear regulators</description>
<gates>
<gate name="A" symbol="LP3961ES-3.3"/>
</gates>
<devices>
<device name="" package="TO170P1435X465-6N">
<connects>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="GND_2" pad="6"/>
<connect gate="A" pin="VIN" pad="2"/>
<connect gate="A" pin="VOUT" pad="4"/>
<connect gate="A" pin="~ERROR" pad="5"/>
<connect gate="A" pin="~SD" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3961ES-3.3"/>
<attribute name="OC_FARNELL" value="9486445"/>
<attribute name="OC_NEWARK" value="41K7775"/>
<attribute name="PACKAGE" value="TO-263-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3962EMP-2.5" prefix="U">
<description>Fast Ultra Low Dropout Linear Regulators</description>
<gates>
<gate name="A" symbol="LP3962EMP-2.5"/>
</gates>
<devices>
<device name="" package="SOT150P696X180-5N">
<connects>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="VIN" pad="2"/>
<connect gate="A" pin="VOUT" pad="3"/>
<connect gate="A" pin="~ERROR" pad="4"/>
<connect gate="A" pin="~SD" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3962EMP-2.5"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="01C7562"/>
<attribute name="PACKAGE" value="TO-223-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3962EMP-3.3" prefix="U">
<description>Fast Ultra Low Dropout Linear Regulators</description>
<gates>
<gate name="A" symbol="LP3962EMP-3.3"/>
</gates>
<devices>
<device name="" package="SOT150P696X180-5N">
<connects>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="VIN" pad="2"/>
<connect gate="A" pin="VOUT" pad="3"/>
<connect gate="A" pin="~ERROR" pad="4"/>
<connect gate="A" pin="~SD" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3962EMP-3.3"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K7787"/>
<attribute name="PACKAGE" value="TO-223-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3962ES-1.8" prefix="U">
<description>Fast Ultra Low Dropout Linear Regulators</description>
<gates>
<gate name="A" symbol="LP3962ES-1.8"/>
</gates>
<devices>
<device name="" package="TO170P1435X457-5N">
<connects>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="GND_2" pad="6"/>
<connect gate="A" pin="VIN" pad="2"/>
<connect gate="A" pin="VOUT" pad="4"/>
<connect gate="A" pin="~ERROR/SENSE/ADJ" pad="5"/>
<connect gate="A" pin="~SD" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3962ES-1.8"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="74C5383"/>
<attribute name="PACKAGE" value="TO-263-5"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3962ES-2.5" prefix="U">
<description>Fast Ultra Low Dropout Linear Regulators</description>
<gates>
<gate name="A" symbol="LP3962ES-2.5"/>
</gates>
<devices>
<device name="" package="TO170P1435X457-5N">
<connects>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="GND_2" pad="6"/>
<connect gate="A" pin="VIN" pad="2"/>
<connect gate="A" pin="VOUT" pad="4"/>
<connect gate="A" pin="~ERROR/SENSE/ADJ" pad="5"/>
<connect gate="A" pin="~SD" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3962ES-2.5"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K7794"/>
<attribute name="PACKAGE" value="TO-263-5"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3962ES-3.3" prefix="U">
<description>Fast Ultra Low Dropout Linear Regulators</description>
<gates>
<gate name="A" symbol="LP3962ES-3.3"/>
</gates>
<devices>
<device name="" package="TO170P1435X457-5N">
<connects>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="GND_2" pad="6"/>
<connect gate="A" pin="VIN" pad="2"/>
<connect gate="A" pin="VOUT" pad="4"/>
<connect gate="A" pin="~ERROR/SENSE/ADJ" pad="5"/>
<connect gate="A" pin="~SD" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3962ES-3.3"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K7795"/>
<attribute name="PACKAGE" value="TO-263-5"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3963ES-2.5" prefix="U">
<description>Fast Ultra Low Dropout Linear Regulators</description>
<gates>
<gate name="A" symbol="LP3963ES-2.5"/>
</gates>
<devices>
<device name="" package="TO170P1435X457-5N">
<connects>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="GND_2" pad="6"/>
<connect gate="A" pin="VIN" pad="2"/>
<connect gate="A" pin="VOUT" pad="4"/>
<connect gate="A" pin="~ERROR/SENSE/ADJ" pad="5"/>
<connect gate="A" pin="~SD" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3963ES-2.5"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K7806"/>
<attribute name="PACKAGE" value="TO-263-5"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3963ES-3.3" prefix="U">
<description>Fast Ultra Low Dropout Linear Regulators</description>
<gates>
<gate name="A" symbol="LP3963ES-3.3"/>
</gates>
<devices>
<device name="" package="TO170P1435X457-5N">
<connects>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="GND_2" pad="6"/>
<connect gate="A" pin="VIN" pad="2"/>
<connect gate="A" pin="VOUT" pad="4"/>
<connect gate="A" pin="~ERROR/SENSE/ADJ" pad="5"/>
<connect gate="A" pin="~SD" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3963ES-3.3"/>
<attribute name="OC_FARNELL" value="1564755"/>
<attribute name="OC_NEWARK" value="41K7807"/>
<attribute name="PACKAGE" value="TO-263-5"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3964EMP-1.8" prefix="U">
<description>Fast Ultra Low Dropout Linear Regulators</description>
<gates>
<gate name="A" symbol="LP3964EMP-1.8"/>
</gates>
<devices>
<device name="" package="SOT150P696X180-5N">
<connects>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="SENSE/ADJ" pad="4"/>
<connect gate="A" pin="VIN" pad="2"/>
<connect gate="A" pin="VOUT" pad="3"/>
<connect gate="A" pin="~SD" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3964EMP-1.8"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K7818"/>
<attribute name="PACKAGE" value="TO-223-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3964EMP-2.5" prefix="U">
<description>Dropout Linear  Regulator</description>
<gates>
<gate name="A" symbol="LP3964EMP-2.5"/>
</gates>
<devices>
<device name="" package="SOT150P696X180-5N">
<connects>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="SEN/ADJ" pad="4"/>
<connect gate="A" pin="VIN" pad="2"/>
<connect gate="A" pin="VOUT" pad="3"/>
<connect gate="A" pin="~SD" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3964EMP-2.5"/>
<attribute name="OC_FARNELL" value="9778748"/>
<attribute name="OC_NEWARK" value="74C5410"/>
<attribute name="PACKAGE" value="SOT-223-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3964EMP-3.3" prefix="U">
<description>Fast Ultra Low Dropout Linear Regulators</description>
<gates>
<gate name="A" symbol="LP3964EMP-3.3"/>
</gates>
<devices>
<device name="" package="SOT150P696X180-5N">
<connects>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="VIN" pad="2"/>
<connect gate="A" pin="VOUT" pad="3"/>
<connect gate="A" pin="~ERROR" pad="4"/>
<connect gate="A" pin="~SD" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3964EMP-3.3"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K7820"/>
<attribute name="PACKAGE" value="TO-223-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3964EMP-ADJ" prefix="U">
<description>Dropout Linear  Regulator</description>
<gates>
<gate name="A" symbol="LP3964EMP-ADJ"/>
</gates>
<devices>
<device name="" package="SOT150P696X180-5N">
<connects>
<connect gate="A" pin="ADJ" pad="4"/>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="VIN" pad="2"/>
<connect gate="A" pin="VOUT" pad="3"/>
<connect gate="A" pin="~SD" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3964EMP-ADJ"/>
<attribute name="OC_FARNELL" value="9778896"/>
<attribute name="OC_NEWARK" value="41K7817"/>
<attribute name="PACKAGE" value="SOT-223-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3964ES-2.5" prefix="U">
<description>Fast Ultra Low Dropout Linear Regulators</description>
<gates>
<gate name="A" symbol="LP3964ES-2.5"/>
</gates>
<devices>
<device name="" package="TO170P1435X457-5N">
<connects>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="GND_2" pad="6"/>
<connect gate="A" pin="VIN" pad="2"/>
<connect gate="A" pin="VOUT" pad="4"/>
<connect gate="A" pin="~ERROR/SENSE/ADJ" pad="5"/>
<connect gate="A" pin="~SD" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3964ES-2.5"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K7829"/>
<attribute name="PACKAGE" value="TO-263-5"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3964ES-3.3" prefix="U">
<description>Linear regulators</description>
<gates>
<gate name="A" symbol="LP3964ES-3.3"/>
</gates>
<devices>
<device name="" package="TO170P1435X465-6N">
<connects>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="GND_2" pad="6"/>
<connect gate="A" pin="SENSE/ADJ" pad="5"/>
<connect gate="A" pin="VIN" pad="2"/>
<connect gate="A" pin="VOUT" pad="4"/>
<connect gate="A" pin="~SD" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3964ES-3.3"/>
<attribute name="OC_FARNELL" value="9486380"/>
<attribute name="OC_NEWARK" value="9486380"/>
<attribute name="PACKAGE" value="TO-263-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3964ES-ADJ" prefix="U">
<description>Low Dropout Regulator</description>
<gates>
<gate name="A" symbol="LP3964ES-ADJ"/>
</gates>
<devices>
<device name="" package="TO170P1435X457-6N">
<connects>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="GND_2" pad="6"/>
<connect gate="A" pin="SENSE/ADJ" pad="5"/>
<connect gate="A" pin="VIN" pad="2"/>
<connect gate="A" pin="VOUT" pad="4"/>
<connect gate="A" pin="~SD" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3964ES-ADJ"/>
<attribute name="OC_FARNELL" value="9486534"/>
<attribute name="OC_NEWARK" value="97K3755"/>
<attribute name="PACKAGE" value="TO-263-5"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3964ET-ADJ" prefix="U">
<description>IC REGULATOR ULTR LDO</description>
<gates>
<gate name="A" symbol="LP3964ET-ADJ"/>
</gates>
<devices>
<device name="" package="TO170P470X1016X2092-5P">
<connects>
<connect gate="A" pin="*ERROR-SENS-ADJ" pad="5"/>
<connect gate="A" pin="*SHUTDOWN" pad="1"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="VIN" pad="2"/>
<connect gate="A" pin="VOUT" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3964ET-ADJ"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K7837"/>
<attribute name="PACKAGE" value="TO220-5"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3965EMP-1.8" prefix="U">
<description>Fast Ultra Low Dropout Linear Regulators</description>
<gates>
<gate name="A" symbol="LP3965EMP-1.8"/>
</gates>
<devices>
<device name="" package="SOT150P696X180-5N">
<connects>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="SENSE/ADJ" pad="4"/>
<connect gate="A" pin="VIN" pad="2"/>
<connect gate="A" pin="VOUT" pad="3"/>
<connect gate="A" pin="~SD" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3965EMP-1.8"/>
<attribute name="OC_FARNELL" value="1564764"/>
<attribute name="OC_NEWARK" value="41K7843"/>
<attribute name="PACKAGE" value="TO-223-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3965EMP-2.5" prefix="U">
<description>Fast Ultra Low Dropout Linear Regulators</description>
<gates>
<gate name="A" symbol="LP3965EMP-2.5"/>
</gates>
<devices>
<device name="" package="SOT150P696X180-5N">
<connects>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="SENSE/ADJ" pad="4"/>
<connect gate="A" pin="VIN" pad="2"/>
<connect gate="A" pin="VOUT" pad="3"/>
<connect gate="A" pin="~SD" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3965EMP-2.5"/>
<attribute name="OC_FARNELL" value="1564739"/>
<attribute name="OC_NEWARK" value="41K7844"/>
<attribute name="PACKAGE" value="TO-223-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3965EMP-3.3" prefix="U">
<description>Fast Ultra Low Dropout Linear Regulators</description>
<gates>
<gate name="A" symbol="LP3965EMP-3.3"/>
</gates>
<devices>
<device name="" package="SOT150P696X180-5N">
<connects>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="SENSE/ADJ" pad="4"/>
<connect gate="A" pin="VIN" pad="2"/>
<connect gate="A" pin="VOUT" pad="3"/>
<connect gate="A" pin="~SD" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3965EMP-3.3"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K7845"/>
<attribute name="PACKAGE" value="TO-223-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3965EMP-ADJ" prefix="U">
<description>Fast Ultra Low Dropout Linear Regulators</description>
<gates>
<gate name="A" symbol="LP3965EMP-ADJ"/>
</gates>
<devices>
<device name="" package="SOT150P696X180-5N">
<connects>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="SENSE/ADJ" pad="4"/>
<connect gate="A" pin="VIN" pad="2"/>
<connect gate="A" pin="VOUT" pad="3"/>
<connect gate="A" pin="~SD" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3965EMP-ADJ"/>
<attribute name="OC_FARNELL" value="1469145"/>
<attribute name="OC_NEWARK" value="41K7842"/>
<attribute name="PACKAGE" value="TO-223-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3965ES-1.8" prefix="U">
<description>Fast Ultra Low Dropout Linear Regulators</description>
<gates>
<gate name="A" symbol="LP3965ES-1.8"/>
</gates>
<devices>
<device name="" package="TO170P1435X457-5N">
<connects>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="GND_2" pad="6"/>
<connect gate="A" pin="VIN" pad="2"/>
<connect gate="A" pin="VOUT" pad="4"/>
<connect gate="A" pin="~ERROR/SENSE/ADJ" pad="5"/>
<connect gate="A" pin="~SD" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3965ES-1.8"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="74C5445"/>
<attribute name="PACKAGE" value="TO-263-5"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3965ES-2.5" prefix="U">
<description>Fast Ultra Low Dropout Linear Regulators</description>
<gates>
<gate name="A" symbol="LP3965ES-2.5"/>
</gates>
<devices>
<device name="" package="TO170P1435X457-5N">
<connects>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="GND_2" pad="6"/>
<connect gate="A" pin="VIN" pad="2"/>
<connect gate="A" pin="VOUT" pad="4"/>
<connect gate="A" pin="~ERROR/SENSE/ADJ" pad="5"/>
<connect gate="A" pin="~SD" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3965ES-2.5"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K7854"/>
<attribute name="PACKAGE" value="TO-263-5"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3965ES-3.3" prefix="U">
<description>Fast Ultra Low Dropout Linear Regulators</description>
<gates>
<gate name="A" symbol="LP3965ES-3.3"/>
</gates>
<devices>
<device name="" package="TO170P1435X457-5N">
<connects>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="GND_2" pad="6"/>
<connect gate="A" pin="VIN" pad="2"/>
<connect gate="A" pin="VOUT" pad="4"/>
<connect gate="A" pin="~ERROR/SENSE/ADJ" pad="5"/>
<connect gate="A" pin="~SD" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3965ES-3.3"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="74C5447"/>
<attribute name="PACKAGE" value="TO-263-5"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3965ES-ADJ" prefix="U">
<description>Fast Ultra Low Dropout Linear Regulators</description>
<gates>
<gate name="A" symbol="LP3965ES-ADJ"/>
</gates>
<devices>
<device name="" package="TO170P1435X457-5N">
<connects>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="GND_2" pad="6"/>
<connect gate="A" pin="VIN" pad="2"/>
<connect gate="A" pin="VOUT" pad="4"/>
<connect gate="A" pin="~ERROR/SENSE/ADJ" pad="5"/>
<connect gate="A" pin="~SD" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3965ES-ADJ"/>
<attribute name="OC_FARNELL" value="1469147"/>
<attribute name="OC_NEWARK" value="41K7852"/>
<attribute name="PACKAGE" value="TO-263-5"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3966ES-1.8" prefix="U">
<description>Fast Ultra Low Dropout Linear Regulators</description>
<gates>
<gate name="A" symbol="LP3966ES-1.8"/>
</gates>
<devices>
<device name="" package="TO170P1435X457-5N">
<connects>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="GND_2" pad="6"/>
<connect gate="A" pin="VIN" pad="2"/>
<connect gate="A" pin="VOUT" pad="4"/>
<connect gate="A" pin="~ERROR/SENSE/ADJ" pad="5"/>
<connect gate="A" pin="~SD" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3966ES-1.8"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="74C5460"/>
<attribute name="PACKAGE" value="TO-263-5"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3966ES-2.5" prefix="U">
<description>Fast Ultra Low Dropout Linear Regulators</description>
<gates>
<gate name="A" symbol="LP3966ES-2.5"/>
</gates>
<devices>
<device name="" package="TO170P1435X457-5N">
<connects>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="GND_2" pad="6"/>
<connect gate="A" pin="VIN" pad="2"/>
<connect gate="A" pin="VOUT" pad="4"/>
<connect gate="A" pin="~ERROR/SENSE/ADJ" pad="5"/>
<connect gate="A" pin="~SD" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3966ES-2.5"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="74C5461"/>
<attribute name="PACKAGE" value="TO-263-5"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3966ES-3.3" prefix="U">
<description>Fast Ultra Low Dropout Linear Regulators</description>
<gates>
<gate name="A" symbol="LP3966ES-3.3"/>
</gates>
<devices>
<device name="" package="TO170P1435X457-5N">
<connects>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="GND_2" pad="6"/>
<connect gate="A" pin="VIN" pad="2"/>
<connect gate="A" pin="VOUT" pad="4"/>
<connect gate="A" pin="~ERROR/SENSE/ADJ" pad="5"/>
<connect gate="A" pin="~SD" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3966ES-3.3"/>
<attribute name="OC_FARNELL" value="1564694"/>
<attribute name="OC_NEWARK" value="41K7870"/>
<attribute name="PACKAGE" value="TO-263-5"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3966ES-ADJ" prefix="U">
<description>Fast Ultra Low Dropout Linear Regulators</description>
<gates>
<gate name="A" symbol="LP3966ES-ADJ"/>
</gates>
<devices>
<device name="" package="TO170P1435X457-5N">
<connects>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="GND_2" pad="6"/>
<connect gate="A" pin="VIN" pad="2"/>
<connect gate="A" pin="VOUT" pad="4"/>
<connect gate="A" pin="~ERROR/SENSE/ADJ" pad="5"/>
<connect gate="A" pin="~SD" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3966ES-ADJ"/>
<attribute name="OC_FARNELL" value="1469148"/>
<attribute name="OC_NEWARK" value="41K7867"/>
<attribute name="PACKAGE" value="TO-263-5"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3966ET-ADJ" prefix="U">
<description>IC, ADJ LDO REG, 1.2V TO 5V, 3A</description>
<gates>
<gate name="A" symbol="LP3966ET-ADJ"/>
</gates>
<devices>
<device name="" package="TO170P470X1016X2092-5P">
<connects>
<connect gate="A" pin="*ERROR-SENS-ADJ" pad="5"/>
<connect gate="A" pin="*SHUTDOWN" pad="1"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="VIN" pad="2"/>
<connect gate="A" pin="VOUT" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3966ET-ADJ"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K7877"/>
<attribute name="PACKAGE" value="TO220-5"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3981ILD-2.5" prefix="U">
<description>Ultra Low-Dropout CMOS Voltage Regulator</description>
<gates>
<gate name="A" symbol="LP3981ILD-2.5"/>
</gates>
<devices>
<device name="" package="DFN300X400X80-7N">
<connects>
<connect gate="A" pin="BYPASS" pad="5"/>
<connect gate="A" pin="EPAD" pad="7"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="VEN" pad="6"/>
<connect gate="A" pin="VIN" pad="2"/>
<connect gate="A" pin="VOUT" pad="1"/>
<connect gate="A" pin="VOUT-SENSE" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3981ILD-25"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K7882"/>
<attribute name="PACKAGE" value="DFN-6"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3981ILD-3.3" prefix="U">
<description>Ultra Low-Dropout CMOS Voltage Regulator</description>
<gates>
<gate name="A" symbol="LP3981ILD-3.3"/>
</gates>
<devices>
<device name="" package="DFN300X400X80-7N">
<connects>
<connect gate="A" pin="BYPASS" pad="5"/>
<connect gate="A" pin="EPAD" pad="7"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="VEN" pad="6"/>
<connect gate="A" pin="VIN" pad="2"/>
<connect gate="A" pin="VOUT" pad="1"/>
<connect gate="A" pin="VOUT-SENSE" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3981ILD-3.3"/>
<attribute name="OC_FARNELL" value="1685551"/>
<attribute name="OC_NEWARK" value="41K7886"/>
<attribute name="PACKAGE" value="DFN-6"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3981IMM-2.5" prefix="U">
<description>Ultra Low-Dropout CMOS Voltage Regulator</description>
<gates>
<gate name="A" symbol="LP3981IMM-2.5"/>
</gates>
<devices>
<device name="" package="SOP65P490X110-8N">
<connects>
<connect gate="A" pin="BYPASS" pad="6"/>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="NC" pad="8"/>
<connect gate="A" pin="NC_2" pad="3"/>
<connect gate="A" pin="VEN" pad="7"/>
<connect gate="A" pin="VIN" pad="2"/>
<connect gate="A" pin="VOUT" pad="1"/>
<connect gate="A" pin="VOUT-SENSE" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3981IMM-25"/>
<attribute name="OC_FARNELL" value="1685562"/>
<attribute name="OC_NEWARK" value="41K7893"/>
<attribute name="PACKAGE" value="MSOP-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3981IMM-2.8" prefix="U">
<description>Ultra Low-Dropout CMOS Voltage Regulator</description>
<gates>
<gate name="A" symbol="LP3981IMM-2.8"/>
</gates>
<devices>
<device name="" package="SOP65P490X110-8N">
<connects>
<connect gate="A" pin="BYPASS" pad="6"/>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="NC" pad="8"/>
<connect gate="A" pin="NC_2" pad="3"/>
<connect gate="A" pin="VEN" pad="7"/>
<connect gate="A" pin="VIN" pad="2"/>
<connect gate="A" pin="VOUT" pad="1"/>
<connect gate="A" pin="VOUT-SENSE" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3981IMM-2.8"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K7895"/>
<attribute name="PACKAGE" value="MSOP-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3981IMM-3.0" prefix="U">
<description>Ultra Low-Dropout CMOS Voltage Regulator</description>
<gates>
<gate name="A" symbol="LP3981IMM-3.0"/>
</gates>
<devices>
<device name="" package="SOP65P490X110-8N">
<connects>
<connect gate="A" pin="BYPASS" pad="6"/>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="NC" pad="8"/>
<connect gate="A" pin="NC_2" pad="3"/>
<connect gate="A" pin="VEN" pad="7"/>
<connect gate="A" pin="VIN" pad="2"/>
<connect gate="A" pin="VOUT" pad="1"/>
<connect gate="A" pin="VOUT-SENSE" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3981IMM-3.0"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K7897"/>
<attribute name="PACKAGE" value="MSOP-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3981IMM-3.3" prefix="U">
<description>Ultra Low-Dropout CMOS Voltage Regulator</description>
<gates>
<gate name="A" symbol="LP3981IMM-3.3"/>
</gates>
<devices>
<device name="" package="SOP65P490X110-8N">
<connects>
<connect gate="A" pin="BYPASS" pad="6"/>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="NC" pad="8"/>
<connect gate="A" pin="NC_2" pad="3"/>
<connect gate="A" pin="VEN" pad="7"/>
<connect gate="A" pin="VIN" pad="2"/>
<connect gate="A" pin="VOUT" pad="1"/>
<connect gate="A" pin="VOUT-SENSE" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3981IMM-3.3"/>
<attribute name="OC_FARNELL" value="1685563"/>
<attribute name="OC_NEWARK" value="41K7899"/>
<attribute name="PACKAGE" value="MSOP-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3982ILD-1.8" prefix="U">
<description>Micropower, Ultra Low-Dropout</description>
<gates>
<gate name="A" symbol="LP3982ILD-1.8"/>
</gates>
<devices>
<device name="" package="DFN300X200X80-9N">
<connects>
<connect gate="A" pin="CC" pad="6"/>
<connect gate="A" pin="EPAD" pad="9"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="SET" pad="5"/>
<connect gate="A" pin="VIN" pad="2"/>
<connect gate="A" pin="VOUT" pad="4"/>
<connect gate="A" pin="VOUT_2" pad="1"/>
<connect gate="A" pin="~FAULT" pad="8"/>
<connect gate="A" pin="~SHDN" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3982ILD-18"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K7908"/>
<attribute name="PACKAGE" value="DFN-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3982ILD-3.3" prefix="U">
<description>Micropower, Ultra Low-Dropout</description>
<gates>
<gate name="A" symbol="LP3982ILD-3.3"/>
</gates>
<devices>
<device name="" package="DFN300X200X80-9N">
<connects>
<connect gate="A" pin="CC" pad="6"/>
<connect gate="A" pin="EPAD" pad="9"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="SET" pad="5"/>
<connect gate="A" pin="VIN" pad="2"/>
<connect gate="A" pin="VOUT" pad="4"/>
<connect gate="A" pin="VOUT_2" pad="1"/>
<connect gate="A" pin="~FAULT" pad="8"/>
<connect gate="A" pin="~SHDN" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3982ILD-3.3"/>
<attribute name="OC_FARNELL" value="1685737"/>
<attribute name="OC_NEWARK" value="41K7913"/>
<attribute name="PACKAGE" value="DFN-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3982ILD-ADJ" prefix="U">
<description>Micropower, Ultra Low-Dropout</description>
<gates>
<gate name="A" symbol="LP3982ILD-ADJ"/>
</gates>
<devices>
<device name="" package="DFN300X200X80-9N">
<connects>
<connect gate="A" pin="CC" pad="6"/>
<connect gate="A" pin="EPAD" pad="9"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="SET" pad="5"/>
<connect gate="A" pin="VIN" pad="2"/>
<connect gate="A" pin="VOUT" pad="4"/>
<connect gate="A" pin="VOUT_2" pad="1"/>
<connect gate="A" pin="~FAULT" pad="8"/>
<connect gate="A" pin="~SHDN" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3982ILD-ADJ"/>
<attribute name="OC_FARNELL" value="1685559"/>
<attribute name="OC_NEWARK" value="41K7907"/>
<attribute name="PACKAGE" value="DFN-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3982IMM-1.8" prefix="U">
<description>CMOS Regulator</description>
<gates>
<gate name="A" symbol="LP3982IMM-1.8"/>
</gates>
<devices>
<device name="" package="SOP65P490X109-8N">
<connects>
<connect gate="A" pin="CC" pad="6"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="IN" pad="2"/>
<connect gate="A" pin="OUT" pad="4"/>
<connect gate="A" pin="OUT_2" pad="1"/>
<connect gate="A" pin="~FAULT" pad="8"/>
<connect gate="A" pin="~SET" pad="5"/>
<connect gate="A" pin="~SHDN" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3982IMM-1.8"/>
<attribute name="OC_FARNELL" value="1197406"/>
<attribute name="OC_NEWARK" value="41K7922"/>
<attribute name="PACKAGE" value="8-MSOP"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3982IMM-2.5" prefix="U">
<description>CMOS Regulator</description>
<gates>
<gate name="A" symbol="LP3982IMM-2.5"/>
</gates>
<devices>
<device name="" package="SOP65P490X109-8N">
<connects>
<connect gate="A" pin="CC" pad="6"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="IN" pad="2"/>
<connect gate="A" pin="OUT" pad="4"/>
<connect gate="A" pin="OUT_2" pad="1"/>
<connect gate="A" pin="~FAULT" pad="8"/>
<connect gate="A" pin="~SD" pad="7"/>
<connect gate="A" pin="~SET" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3982IMM-2.5"/>
<attribute name="OC_FARNELL" value="9779574"/>
<attribute name="OC_NEWARK" value="41K7923"/>
<attribute name="PACKAGE" value="MSOP-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3982IMM-3.0" prefix="U">
<description>CMOS Regulator</description>
<gates>
<gate name="A" symbol="LP3982IMM-3.0"/>
</gates>
<devices>
<device name="" package="SOP65P490X110-8N">
<connects>
<connect gate="A" pin="CC" pad="6"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="IN" pad="2"/>
<connect gate="A" pin="OUT" pad="4"/>
<connect gate="A" pin="OUT_2" pad="1"/>
<connect gate="A" pin="SET" pad="5"/>
<connect gate="A" pin="~FAULT" pad="8"/>
<connect gate="A" pin="~SHDN" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3982IMM-3.0"/>
<attribute name="OC_FARNELL" value="9779582"/>
<attribute name="OC_NEWARK" value="41K7926"/>
<attribute name="PACKAGE" value="MSOP-8"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3982IMM-3.3" prefix="U">
<description>CMOS Regulator</description>
<gates>
<gate name="A" symbol="LP3982IMM-3.3"/>
</gates>
<devices>
<device name="" package="SOP65P490X110-8N">
<connects>
<connect gate="A" pin="CC" pad="6"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="IN" pad="2"/>
<connect gate="A" pin="OUT" pad="4"/>
<connect gate="A" pin="OUT_2" pad="1"/>
<connect gate="A" pin="SET" pad="5"/>
<connect gate="A" pin="~FAULT" pad="8"/>
<connect gate="A" pin="~SHDN" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3982IMM-3.3"/>
<attribute name="OC_FARNELL" value="9779590"/>
<attribute name="OC_NEWARK" value="41K7927"/>
<attribute name="PACKAGE" value="MSOP-8"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3982IMM-ADJ" prefix="U">
<description>CMOS Regulator</description>
<gates>
<gate name="A" symbol="LP3982IMM-ADJ"/>
</gates>
<devices>
<device name="" package="SOP65P490X110-8N">
<connects>
<connect gate="A" pin="CC" pad="6"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="IN" pad="2"/>
<connect gate="A" pin="OUT" pad="4"/>
<connect gate="A" pin="OUT_2" pad="1"/>
<connect gate="A" pin="SET" pad="5"/>
<connect gate="A" pin="~FAULT" pad="8"/>
<connect gate="A" pin="~SHDN" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3982IMM-ADJ"/>
<attribute name="OC_FARNELL" value="1469151"/>
<attribute name="OC_NEWARK" value="41K7921"/>
<attribute name="PACKAGE" value="MSOP-8"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3985IM5-2.5" prefix="U">
<description>Low-Dropout CMOS Voltage Regulator</description>
<gates>
<gate name="A" symbol="LP3985IM5-2.5"/>
</gates>
<devices>
<device name="" package="SOT95P300X120-5N">
<connects>
<connect gate="A" pin="BYPASS" pad="4"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="VEN" pad="3"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="VOUT" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3985IM5-2.5"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="23K8220"/>
<attribute name="PACKAGE" value="SOT-5"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3985IM5-2.8" prefix="U">
<description>Low-Dropout CMOS Voltage Regulator</description>
<gates>
<gate name="A" symbol="LP3985IM5-2.8"/>
</gates>
<devices>
<device name="" package="SOT95P300X120-5N">
<connects>
<connect gate="A" pin="BYPASS" pad="4"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="VEN" pad="3"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="VOUT" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3985IM5-2.8"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K7955"/>
<attribute name="PACKAGE" value="SOT-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3985IM5-3.0" prefix="U">
<description>Low-Dropout CMOS Voltage Regulator</description>
<gates>
<gate name="A" symbol="LP3985IM5-3.0"/>
</gates>
<devices>
<device name="" package="SOT95P300X120-5N">
<connects>
<connect gate="A" pin="BYPASS" pad="4"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="VEN" pad="3"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="VOUT" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3985IM5-3.0"/>
<attribute name="OC_FARNELL" value="1469153"/>
<attribute name="OC_NEWARK" value="41K7958"/>
<attribute name="PACKAGE" value="SOT-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3985IM5-3.3" prefix="U">
<description>Low-Dropout CMOS Voltage Regulator</description>
<gates>
<gate name="A" symbol="LP3985IM5-3.3"/>
</gates>
<devices>
<device name="" package="SOT95P300X120-5N">
<connects>
<connect gate="A" pin="BYPASS" pad="4"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="VEN" pad="3"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="VOUT" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3985IM5-3.3"/>
<attribute name="OC_FARNELL" value="1469025"/>
<attribute name="OC_NEWARK" value="23K8224"/>
<attribute name="PACKAGE" value="SOT-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3985IM5-4.7" prefix="U">
<description>Low-Dropout CMOS Voltage Regulator</description>
<gates>
<gate name="A" symbol="LP3985IM5-4.7"/>
</gates>
<devices>
<device name="" package="SOT95P300X120-5N">
<connects>
<connect gate="A" pin="BYPASS" pad="4"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="VEN" pad="3"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="VOUT" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3985IM5-4.7"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K7961"/>
<attribute name="PACKAGE" value="SOT-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3985IM5-5.0" prefix="U">
<description>Low-Dropout CMOS Voltage Regulator</description>
<gates>
<gate name="A" symbol="LP3985IM5-5.0"/>
</gates>
<devices>
<device name="" package="SOT95P300X120-5N">
<connects>
<connect gate="A" pin="BYPASS" pad="4"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="VEN" pad="3"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="VOUT" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3985IM5-5.0"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K7962"/>
<attribute name="PACKAGE" value="SOT-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3985ITL-2.7" prefix="U">
<description>Low-Dropout CMOS Voltage Regulator</description>
<gates>
<gate name="A" symbol="LP3985ITL-2.7"/>
</gates>
<devices>
<device name="" package="BGA5C3X350P_146X100X675">
<connects>
<connect gate="A" pin="BYPASS" pad="A3"/>
<connect gate="A" pin="GND" pad="B2"/>
<connect gate="A" pin="VEN" pad="A1"/>
<connect gate="A" pin="VIN" pad="C3"/>
<connect gate="A" pin="VOUT" pad="C1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3985ITL-27"/>
<attribute name="OC_FARNELL" value="1008070"/>
<attribute name="OC_NEWARK" value="97K3767"/>
<attribute name="PACKAGE" value="BGA-5"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3985ITL-285" prefix="U">
<description>Low-Dropout CMOS Voltage Regulator</description>
<gates>
<gate name="A" symbol="LP3985ITL-285"/>
</gates>
<devices>
<device name="" package="BGA5C3X350P_146X100X675">
<connects>
<connect gate="A" pin="BYPASS" pad="A3"/>
<connect gate="A" pin="GND" pad="B2"/>
<connect gate="A" pin="VEN" pad="A1"/>
<connect gate="A" pin="VIN" pad="C3"/>
<connect gate="A" pin="VOUT" pad="C1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3985ITL-285"/>
<attribute name="OC_FARNELL" value="1798338"/>
<attribute name="OC_NEWARK" value="21K5555"/>
<attribute name="PACKAGE" value="BGA-5"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3985ITL-3.3" prefix="U">
<description>Low-Dropout CMOS Voltage Regulator</description>
<gates>
<gate name="A" symbol="LP3985ITL-3.3"/>
</gates>
<devices>
<device name="" package="BGA5C3X3X50P_100X146X67">
<connects>
<connect gate="A" pin="BYPASS" pad="A3"/>
<connect gate="A" pin="GND" pad="B2"/>
<connect gate="A" pin="VEN" pad="A1"/>
<connect gate="A" pin="VIN" pad="C3"/>
<connect gate="A" pin="VOUT" pad="C1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3985ITL-3.3"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K7983"/>
<attribute name="PACKAGE" value="BGA-5"/>
<attribute name="SUPPLIER" value="National semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3985ITL-4.75" prefix="U">
<description>Low-Dropout CMOS Voltage Regulator</description>
<gates>
<gate name="A" symbol="LP3985ITL-4.75"/>
</gates>
<devices>
<device name="" package="BGA5C3X3X50P_100X146X67">
<connects>
<connect gate="A" pin="BYPASS" pad="A3"/>
<connect gate="A" pin="GND" pad="B2"/>
<connect gate="A" pin="VEN" pad="A1"/>
<connect gate="A" pin="VIN" pad="C3"/>
<connect gate="A" pin="VOUT" pad="C1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3985ITL-4.75"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="99K2592"/>
<attribute name="PACKAGE" value="BGA-5"/>
<attribute name="SUPPLIER" value="National semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3985ITL-5.0" prefix="U">
<description>Low-Dropout CMOS Voltage Regulator</description>
<gates>
<gate name="A" symbol="LP3985ITL-5.0"/>
</gates>
<devices>
<device name="" package="BGA5C3X3X50P_100X146X67">
<connects>
<connect gate="A" pin="BYPASS" pad="A3"/>
<connect gate="A" pin="GND" pad="B2"/>
<connect gate="A" pin="VEN" pad="A1"/>
<connect gate="A" pin="VIN" pad="C3"/>
<connect gate="A" pin="VOUT" pad="C1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3985ITL-5.0"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K7985"/>
<attribute name="PACKAGE" value="BGA-5"/>
<attribute name="SUPPLIER" value="National semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3990MF-1.5" prefix="U">
<description>Linear Voltage Regulator</description>
<gates>
<gate name="A" symbol="LP3990MF-1.5"/>
</gates>
<devices>
<device name="" package="SOT95P285X120-5N">
<connects>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="NC" pad="4"/>
<connect gate="A" pin="VEN" pad="3"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="VOUT" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3990MF-1.5"/>
<attribute name="OC_FARNELL" value="1312627"/>
<attribute name="OC_NEWARK" value="-"/>
<attribute name="PACKAGE" value="SOT-23-5"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3990MF-1.8" prefix="U">
<description>Linear Voltage Regulator</description>
<gates>
<gate name="A" symbol="LP3990MF-1.8"/>
</gates>
<devices>
<device name="" package="SOT95P285X120-5N">
<connects>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="NC" pad="4"/>
<connect gate="A" pin="VEN" pad="3"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="VOUT" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3990MF-18"/>
<attribute name="OC_FARNELL" value="1312628"/>
<attribute name="OC_NEWARK" value="69K2651"/>
<attribute name="PACKAGE" value="SOT-23-5"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3990TL-1.2" prefix="U">
<description>Linear Voltage Regulator</description>
<gates>
<gate name="A" symbol="LP3990TL-1.2"/>
</gates>
<devices>
<device name="" package="BGA4C2X2X50P_129X101X60">
<connects>
<connect gate="A" pin="GND" pad="A1"/>
<connect gate="A" pin="VEN" pad="A2"/>
<connect gate="A" pin="VIN" pad="B2"/>
<connect gate="A" pin="VOUT" pad="B1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3990TL-1.2"/>
<attribute name="OC_FARNELL" value="1008077"/>
<attribute name="OC_NEWARK" value="97K3774"/>
<attribute name="PACKAGE" value="BGA-4"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3990TL-1.5" prefix="U">
<description>Linear Voltage Regulator</description>
<gates>
<gate name="A" symbol="LP3990TL-1.5"/>
</gates>
<devices>
<device name="" package="BGA4C2X2X50P_129X101X60">
<connects>
<connect gate="A" pin="GND" pad="A1"/>
<connect gate="A" pin="VEN" pad="A2"/>
<connect gate="A" pin="VIN" pad="B2"/>
<connect gate="A" pin="VOUT" pad="B1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3990TL-15"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K8064"/>
<attribute name="PACKAGE" value="BGA-4"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3991TL-1.2" prefix="U">
<description>Linear Voltage Regulator</description>
<gates>
<gate name="A" symbol="LP3991TL-1.2"/>
</gates>
<devices>
<device name="" package="BGA4C2X2X50P_963X144X67">
<connects>
<connect gate="A" pin="GND" pad="A1"/>
<connect gate="A" pin="VEN" pad="A2"/>
<connect gate="A" pin="VIN" pad="B2"/>
<connect gate="A" pin="VOUT" pad="B1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3991TL-12"/>
<attribute name="OC_FARNELL" value="1320985"/>
<attribute name="OC_NEWARK" value="31M5529"/>
<attribute name="PACKAGE" value="BGA-4"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3991TL-1.3" prefix="U">
<description>Linear Voltage Regulator</description>
<gates>
<gate name="A" symbol="LP3991TL-1.3"/>
</gates>
<devices>
<device name="" package="BGA4C2X2X50P_96X144X67">
<connects>
<connect gate="A" pin="GND" pad="A1"/>
<connect gate="A" pin="VEN" pad="A2"/>
<connect gate="A" pin="VIN" pad="B2"/>
<connect gate="A" pin="VOUT" pad="B1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3991TL-1.3"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="32M1362"/>
<attribute name="PACKAGE" value="BGA-4"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3991TL-1.5" prefix="U">
<description>Linear Voltage Regulator</description>
<gates>
<gate name="A" symbol="LP3991TL-1.5"/>
</gates>
<devices>
<device name="" package="BGA4C2X2X50P_96X144X67">
<connects>
<connect gate="A" pin="GND" pad="A1"/>
<connect gate="A" pin="VEN" pad="A2"/>
<connect gate="A" pin="VIN" pad="B2"/>
<connect gate="A" pin="VOUT" pad="B1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3991TL-1.5"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="32M1363"/>
<attribute name="PACKAGE" value="BGA-4"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3991TL-2.8" prefix="U">
<description>Linear Voltage Regulator</description>
<gates>
<gate name="A" symbol="LP3991TL-2.8"/>
</gates>
<devices>
<device name="" package="BGA4C2X2X50P_96X144X67">
<connects>
<connect gate="A" pin="GND" pad="A1"/>
<connect gate="A" pin="VEN" pad="A2"/>
<connect gate="A" pin="VIN" pad="B2"/>
<connect gate="A" pin="VOUT" pad="B1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3991TL-2.8"/>
<attribute name="OC_FARNELL" value="1320987"/>
<attribute name="OC_NEWARK" value="32M1364"/>
<attribute name="PACKAGE" value="BGA-4"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3992IMF-1.5" prefix="U">
<description>Voltage Regulator</description>
<gates>
<gate name="A" symbol="LP3992IMF-1.5"/>
</gates>
<devices>
<device name="" package="SOT95P284X122-5N">
<connects>
<connect gate="A" pin="COUT" pad="4"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="VOUT" pad="5"/>
<connect gate="A" pin="~SD" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3992IMF-1.5"/>
<attribute name="OC_FARNELL" value="8207240"/>
<attribute name="OC_NEWARK" value="41K8073"/>
<attribute name="PACKAGE" value="SOT23-5"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3995ILD-1.8" prefix="U">
<description>CMOS Voltage Regulator</description>
<gates>
<gate name="A" symbol="LP3995ILD-1.8"/>
</gates>
<devices>
<device name="" package="DFN329X292X80-7N">
<connects>
<connect gate="A" pin="C_BYPASS" pad="4"/>
<connect gate="A" pin="EPAD" pad="7"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="NC" pad="5"/>
<connect gate="A" pin="VEN" pad="3"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="VOUT" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3995ILD-18"/>
<attribute name="OC_FARNELL" value="8207275"/>
<attribute name="OC_NEWARK" value="-"/>
<attribute name="PACKAGE" value="DFN-6"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3995ITL-1.8" prefix="U">
<description>CMOS Voltage Regulator</description>
<gates>
<gate name="A" symbol="LP3995ITL-1.8"/>
</gates>
<devices>
<device name="" package="BGA5C3X3X50P_100X143X67">
<connects>
<connect gate="A" pin="CYPASS" pad="A3"/>
<connect gate="A" pin="GND" pad="B2"/>
<connect gate="A" pin="VEN" pad="A1"/>
<connect gate="A" pin="VIN" pad="C3"/>
<connect gate="A" pin="VOUT" pad="C1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3995ITL-1.8"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K8087"/>
<attribute name="PACKAGE" value="BGA-5"/>
<attribute name="SUPPLIER" value="National semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3995ITL-1.9" prefix="U">
<description>CMOS Voltage Regulator</description>
<gates>
<gate name="A" symbol="LP3995ITL-1.9"/>
</gates>
<devices>
<device name="" package="BGA5C3X3X50P_100X143X67">
<connects>
<connect gate="A" pin="CYPASS" pad="A3"/>
<connect gate="A" pin="GND" pad="B2"/>
<connect gate="A" pin="VEN" pad="A1"/>
<connect gate="A" pin="VIN" pad="C3"/>
<connect gate="A" pin="VOUT" pad="C1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3995ITL-1.9"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K8088"/>
<attribute name="PACKAGE" value="BGA-5"/>
<attribute name="SUPPLIER" value="National semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3995ITL-2.1" prefix="U">
<description>CMOS Voltage Regulator</description>
<gates>
<gate name="A" symbol="LP3995ITL-2.1"/>
</gates>
<devices>
<device name="" package="BGA5C3X3X50P_100X143X67">
<connects>
<connect gate="A" pin="CYPASS" pad="A3"/>
<connect gate="A" pin="GND" pad="B2"/>
<connect gate="A" pin="VEN" pad="A1"/>
<connect gate="A" pin="VIN" pad="C3"/>
<connect gate="A" pin="VOUT" pad="C1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3995ITL-2.1"/>
<attribute name="OC_FARNELL" value="8238472"/>
<attribute name="OC_NEWARK" value="-"/>
<attribute name="PACKAGE" value="BGA-5"/>
<attribute name="SUPPLIER" value="National semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3995ITL-2.5" prefix="U">
<description>CMOS Voltage Regulator</description>
<gates>
<gate name="A" symbol="LP3995ITL-2.5"/>
</gates>
<devices>
<device name="" package="BGA5C3X3X50P_100X143X67">
<connects>
<connect gate="A" pin="CYPASS" pad="A3"/>
<connect gate="A" pin="GND" pad="B2"/>
<connect gate="A" pin="VEN" pad="A1"/>
<connect gate="A" pin="VIN" pad="C3"/>
<connect gate="A" pin="VOUT" pad="C1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3995ITL-2.5"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K8090"/>
<attribute name="PACKAGE" value="BGA-5"/>
<attribute name="SUPPLIER" value="National semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3995ITL-2.85" prefix="U">
<description>CMOS Voltage Regulator</description>
<gates>
<gate name="A" symbol="LP3995ITL-2.85"/>
</gates>
<devices>
<device name="" package="BGA5C3X3X50P_100X143X67">
<connects>
<connect gate="A" pin="CYPASS" pad="A3"/>
<connect gate="A" pin="GND" pad="B2"/>
<connect gate="A" pin="VEN" pad="A1"/>
<connect gate="A" pin="VIN" pad="C3"/>
<connect gate="A" pin="VOUT" pad="C1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3995ITL-2.85"/>
<attribute name="OC_FARNELL" value="1008084"/>
<attribute name="OC_NEWARK" value="41K8092"/>
<attribute name="PACKAGE" value="BGA-5"/>
<attribute name="SUPPLIER" value="National semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3997MM-3.3" prefix="U">
<description>CMOS LDO Regulator</description>
<gates>
<gate name="A" symbol="LP3997MM-3.3"/>
</gates>
<devices>
<device name="" package="SOP65P490X110-8N">
<connects>
<connect gate="A" pin="CBYP" pad="1"/>
<connect gate="A" pin="DELAY" pad="2"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="SENSE" pad="6"/>
<connect gate="A" pin="VIN" pad="4"/>
<connect gate="A" pin="VOUT" pad="5"/>
<connect gate="A" pin="~ERROR" pad="7"/>
<connect gate="A" pin="~SD" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3997MM-33"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="79K8005"/>
<attribute name="PACKAGE" value="MSOP-8"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3999ITL-1.8" prefix="U">
<description>Low Noise 150mA Voltage Regulator</description>
<gates>
<gate name="A" symbol="LP3999ITL-1.8"/>
</gates>
<devices>
<device name="" package="BGA5C3X3X50P_100X438X67">
<connects>
<connect gate="A" pin="CBYPASS" pad="A3"/>
<connect gate="A" pin="GND" pad="B2"/>
<connect gate="A" pin="VEN" pad="A1"/>
<connect gate="A" pin="VIN" pad="C3"/>
<connect gate="A" pin="VOUT" pad="C1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3999ITL-1.8"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K8104"/>
<attribute name="PACKAGE" value="BGA-5"/>
<attribute name="SUPPLIER" value="National semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3999ITL-2.4" prefix="U">
<description>Low Noise 150mA Voltage Regulator</description>
<gates>
<gate name="A" symbol="LP3999ITL-2.4"/>
</gates>
<devices>
<device name="" package="BGA5C3X3X50P_100X438X67">
<connects>
<connect gate="A" pin="CBYPASS" pad="A3"/>
<connect gate="A" pin="GND" pad="B2"/>
<connect gate="A" pin="VEN" pad="A1"/>
<connect gate="A" pin="VIN" pad="C3"/>
<connect gate="A" pin="VOUT" pad="C1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP3999ITL-2.4"/>
<attribute name="OC_FARNELL" value="8238545"/>
<attribute name="OC_NEWARK" value="-"/>
<attribute name="PACKAGE" value="BGA-5"/>
<attribute name="SUPPLIER" value="National semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP5524TM-5" prefix="U">
<description>Parallel LED Driver</description>
<gates>
<gate name="A" symbol="LP5524TM-5"/>
</gates>
<devices>
<device name="" package="BGA9C3X340P_121X121X67">
<connects>
<connect gate="A" pin="D1A" pad="B3"/>
<connect gate="A" pin="D1B" pad="B1"/>
<connect gate="A" pin="D2A" pad="C3"/>
<connect gate="A" pin="D2B" pad="C1"/>
<connect gate="A" pin="ENA" pad="A3"/>
<connect gate="A" pin="ENB" pad="A2"/>
<connect gate="A" pin="GND" pad="C2"/>
<connect gate="A" pin="ISET" pad="A1"/>
<connect gate="A" pin="VIN" pad="B2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP5524TM-5"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="54M4758"/>
<attribute name="PACKAGE" value="BGA-9"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP55281RL" prefix="U">
<description>Quad RGB Driver</description>
<gates>
<gate name="A" symbol="LP55281RL"/>
</gates>
<devices>
<device name="" package="BGA36C6X6X50P_300X300X65">
<connects>
<connect gate="A" pin="ALED" pad="F2"/>
<connect gate="A" pin="ASE1" pad="D2"/>
<connect gate="A" pin="ASE2" pad="D4"/>
<connect gate="A" pin="B1" pad="A6"/>
<connect gate="A" pin="B2" pad="A2"/>
<connect gate="A" pin="B3" pad="D6"/>
<connect gate="A" pin="B4" pad="E1"/>
<connect gate="A" pin="FB" pad="E6"/>
<connect gate="A" pin="G1" pad="B6"/>
<connect gate="A" pin="G2" pad="A3"/>
<connect gate="A" pin="G3" pad="D5"/>
<connect gate="A" pin="G4" pad="E2"/>
<connect gate="A" pin="GND" pad="E4"/>
<connect gate="A" pin="GNDA" pad="D1"/>
<connect gate="A" pin="GND_2" pad="F1"/>
<connect gate="A" pin="GND_RGB1" pad="A5"/>
<connect gate="A" pin="GND_RGB2" pad="F4"/>
<connect gate="A" pin="GND_SW" pad="F5"/>
<connect gate="A" pin="IF_SEL" pad="B2"/>
<connect gate="A" pin="IRGB" pad="B5"/>
<connect gate="A" pin="IRT" pad="C2"/>
<connect gate="A" pin="NRST" pad="F3"/>
<connect gate="A" pin="R1" pad="C6"/>
<connect gate="A" pin="R2" pad="A4"/>
<connect gate="A" pin="R3" pad="E5"/>
<connect gate="A" pin="R4" pad="E3"/>
<connect gate="A" pin="SCK/SCL" pad="B3"/>
<connect gate="A" pin="SI/A0" pad="C4"/>
<connect gate="A" pin="SO" pad="B4"/>
<connect gate="A" pin="SS/SDA" pad="C5"/>
<connect gate="A" pin="SW" pad="F6"/>
<connect gate="A" pin="VDD1" pad="D3"/>
<connect gate="A" pin="VDD2" pad="A1"/>
<connect gate="A" pin="VDDA" pad="B1"/>
<connect gate="A" pin="VDDIO" pad="C3"/>
<connect gate="A" pin="VREF" pad="C1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP55281RL"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="84M8168"/>
<attribute name="PACKAGE" value="BGA-36"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP55281TL" prefix="U">
<description>Quad RGB Driver</description>
<gates>
<gate name="A" symbol="LP55281TL"/>
</gates>
<devices>
<device name="" package="BGA36C6X6X50P_300X300X65">
<connects>
<connect gate="A" pin="ALED" pad="F2"/>
<connect gate="A" pin="ASE1" pad="D2"/>
<connect gate="A" pin="ASE2" pad="D4"/>
<connect gate="A" pin="B1" pad="A6"/>
<connect gate="A" pin="B2" pad="A2"/>
<connect gate="A" pin="B3" pad="D6"/>
<connect gate="A" pin="B4" pad="E1"/>
<connect gate="A" pin="FB" pad="E6"/>
<connect gate="A" pin="G1" pad="B6"/>
<connect gate="A" pin="G2" pad="A3"/>
<connect gate="A" pin="G3" pad="D5"/>
<connect gate="A" pin="G4" pad="E2"/>
<connect gate="A" pin="GND" pad="E4"/>
<connect gate="A" pin="GNDA" pad="D1"/>
<connect gate="A" pin="GND_2" pad="F1"/>
<connect gate="A" pin="GND_RGB1" pad="A5"/>
<connect gate="A" pin="GND_RGB2" pad="F4"/>
<connect gate="A" pin="GND_SW" pad="F5"/>
<connect gate="A" pin="IF_SEL" pad="B2"/>
<connect gate="A" pin="IRGB" pad="B5"/>
<connect gate="A" pin="IRT" pad="C2"/>
<connect gate="A" pin="NRST" pad="F3"/>
<connect gate="A" pin="R1" pad="C6"/>
<connect gate="A" pin="R2" pad="A4"/>
<connect gate="A" pin="R3" pad="E5"/>
<connect gate="A" pin="R4" pad="E3"/>
<connect gate="A" pin="SCK/SCL" pad="B3"/>
<connect gate="A" pin="SI/A0" pad="C4"/>
<connect gate="A" pin="SO" pad="B4"/>
<connect gate="A" pin="SS/SDA" pad="C5"/>
<connect gate="A" pin="SW" pad="F6"/>
<connect gate="A" pin="VDD1" pad="D3"/>
<connect gate="A" pin="VDD2" pad="A1"/>
<connect gate="A" pin="VDDA" pad="B1"/>
<connect gate="A" pin="VDDIO" pad="C3"/>
<connect gate="A" pin="VREF" pad="C1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP55281TL"/>
<attribute name="OC_FARNELL" value="1675300"/>
<attribute name="OC_NEWARK" value="54M4760"/>
<attribute name="PACKAGE" value="BGA-36"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP5900SD-1.5" prefix="U">
<description>Linear Regulator</description>
<gates>
<gate name="A" symbol="LP5900SD-1.5"/>
</gates>
<devices>
<device name="" package="DFN220X250X80-7N">
<connects>
<connect gate="A" pin="EPAD" pad="7"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="NC" pad="5"/>
<connect gate="A" pin="NC_2" pad="2"/>
<connect gate="A" pin="VEN" pad="4"/>
<connect gate="A" pin="VIN" pad="6"/>
<connect gate="A" pin="VOUT" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP5900SD-15"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="13M2039"/>
<attribute name="PACKAGE" value="DFN-6"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP5900SD-1.8" prefix="U">
<description>Linear Regulator</description>
<gates>
<gate name="A" symbol="LP5900SD-1.8"/>
</gates>
<devices>
<device name="" package="DFN220X250X80-7N">
<connects>
<connect gate="A" pin="EPAD" pad="7"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="NC" pad="5"/>
<connect gate="A" pin="NC_2" pad="2"/>
<connect gate="A" pin="VEN" pad="4"/>
<connect gate="A" pin="VIN" pad="6"/>
<connect gate="A" pin="VOUT" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP5900SD-1.8"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="13M2041"/>
<attribute name="PACKAGE" value="DFN-6"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP5900SD-2.2" prefix="U">
<description>Linear Regulator for RF/Analog Circuits</description>
<gates>
<gate name="A" symbol="LP5900SD-2.2"/>
</gates>
<devices>
<device name="" package="DFN220X250X80-7N">
<connects>
<connect gate="A" pin="EPAD" pad="7"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="NC" pad="5"/>
<connect gate="A" pin="NC_2" pad="2"/>
<connect gate="A" pin="VEN" pad="4"/>
<connect gate="A" pin="VIN" pad="6"/>
<connect gate="A" pin="VOUT" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP5900SD-2.2"/>
<attribute name="OC_FARNELL" value="1312644"/>
<attribute name="OC_NEWARK" value="31M5541"/>
<attribute name="PACKAGE" value="DFN-6"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP5900SD-2.5" prefix="U">
<description>Linear Regulator</description>
<gates>
<gate name="A" symbol="LP5900SD-2.5"/>
</gates>
<devices>
<device name="" package="DFN220X250X80-7N">
<connects>
<connect gate="A" pin="EPAD" pad="7"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="NC" pad="5"/>
<connect gate="A" pin="NC_2" pad="2"/>
<connect gate="A" pin="VEN" pad="4"/>
<connect gate="A" pin="VIN" pad="6"/>
<connect gate="A" pin="VOUT" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP5900SD-2.5"/>
<attribute name="OC_FARNELL" value="1693897"/>
<attribute name="OC_NEWARK" value="13M2047"/>
<attribute name="PACKAGE" value="DFN-6"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP5900SD-2.7" prefix="U">
<description>Linear Regulator</description>
<gates>
<gate name="A" symbol="LP5900SD-2.7"/>
</gates>
<devices>
<device name="" package="DFN220X250X80-7N">
<connects>
<connect gate="A" pin="EPAD" pad="7"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="NC" pad="5"/>
<connect gate="A" pin="NC_2" pad="2"/>
<connect gate="A" pin="VEN" pad="4"/>
<connect gate="A" pin="VIN" pad="6"/>
<connect gate="A" pin="VOUT" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP5900SD-2.7"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="32M1379"/>
<attribute name="PACKAGE" value="DFN-6"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP5900SD-2.8" prefix="U">
<description>Linear Regulator for RF/Analog Circuits</description>
<gates>
<gate name="A" symbol="LP5900SD-2.8"/>
</gates>
<devices>
<device name="" package="DFN220X250X80-7N">
<connects>
<connect gate="A" pin="EPAD" pad="7"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="NC" pad="5"/>
<connect gate="A" pin="NC_2" pad="2"/>
<connect gate="A" pin="VEN" pad="4"/>
<connect gate="A" pin="VIN" pad="6"/>
<connect gate="A" pin="VOUT" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP5900SD-2.8"/>
<attribute name="OC_FARNELL" value="1312646"/>
<attribute name="OC_NEWARK" value="13M2049"/>
<attribute name="PACKAGE" value="DFN-6"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP5900SD-3.0" prefix="U">
<description>Linear Regulator for RF/Analog Circuits</description>
<gates>
<gate name="A" symbol="LP5900SD-3.0"/>
</gates>
<devices>
<device name="" package="DFN220X250X80-7N">
<connects>
<connect gate="A" pin="EPAD" pad="7"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="NC" pad="5"/>
<connect gate="A" pin="NC_2" pad="2"/>
<connect gate="A" pin="VEN" pad="4"/>
<connect gate="A" pin="VIN" pad="6"/>
<connect gate="A" pin="VOUT" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP5900SD-3.0"/>
<attribute name="OC_FARNELL" value="1312647"/>
<attribute name="OC_NEWARK" value="13M2051"/>
<attribute name="PACKAGE" value="DFN-6"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP5900SD-3.3" prefix="U">
<description>Linear Regulator for RF/Analog Circuits</description>
<gates>
<gate name="A" symbol="LP5900SD-3.3"/>
</gates>
<devices>
<device name="" package="DFN220X250X80-7N">
<connects>
<connect gate="A" pin="EPAD" pad="7"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="NC" pad="5"/>
<connect gate="A" pin="NC_2" pad="2"/>
<connect gate="A" pin="VEN" pad="4"/>
<connect gate="A" pin="VIN" pad="6"/>
<connect gate="A" pin="VOUT" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP5900SD-33"/>
<attribute name="OC_FARNELL" value="1312648"/>
<attribute name="OC_NEWARK" value="13M2053"/>
<attribute name="PACKAGE" value="DFN-6"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP5900TL-1.5" prefix="U">
<description>Linear Regulator</description>
<gates>
<gate name="A" symbol="LP5900TL-1.5"/>
</gates>
<devices>
<device name="" package="BGA4C2X2X50P_106X109X67">
<connects>
<connect gate="A" pin="GND" pad="B1"/>
<connect gate="A" pin="VEN" pad="A1"/>
<connect gate="A" pin="VIN" pad="A2"/>
<connect gate="A" pin="VOUT" pad="B2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP5900TL-1.5"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="69K2658"/>
<attribute name="PACKAGE" value="BGA-4"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP5900TL-1.8" prefix="U">
<description>Linear Regulator</description>
<gates>
<gate name="A" symbol="LP5900TL-1.8"/>
</gates>
<devices>
<device name="" package="BGA4C2X2X50P_109X106X67">
<connects>
<connect gate="A" pin="GND" pad="B1"/>
<connect gate="A" pin="VEN" pad="A1"/>
<connect gate="A" pin="VIN" pad="A2"/>
<connect gate="A" pin="VOUT" pad="B2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP5900TL-18"/>
<attribute name="OC_FARNELL" value="1495079"/>
<attribute name="OC_NEWARK" value="79K8013"/>
<attribute name="PACKAGE" value="BGA-4"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP5900TL-2.2" prefix="U">
<description>Linear Regulator</description>
<gates>
<gate name="A" symbol="LP5900TL-2.2"/>
</gates>
<devices>
<device name="" package="BGA4C2X2X50P_106X109X67">
<connects>
<connect gate="A" pin="GND" pad="B1"/>
<connect gate="A" pin="VEN" pad="A1"/>
<connect gate="A" pin="VIN" pad="A2"/>
<connect gate="A" pin="VOUT" pad="B2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP5900TL-2.2"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="79K8017"/>
<attribute name="PACKAGE" value="BGA-4"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP5900TL-2.5" prefix="U">
<description>Linear Regulator</description>
<gates>
<gate name="A" symbol="LP5900TL-2.5"/>
</gates>
<devices>
<device name="" package="BGA4C2X2X50P_106X109X67">
<connects>
<connect gate="A" pin="GND" pad="B1"/>
<connect gate="A" pin="VEN" pad="A1"/>
<connect gate="A" pin="VIN" pad="A2"/>
<connect gate="A" pin="VOUT" pad="B2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP5900TL-2.5"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="79K8019"/>
<attribute name="PACKAGE" value="BGA-4"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP5900TL-2.6" prefix="U">
<description>Linear Regulator</description>
<gates>
<gate name="A" symbol="LP5900TL-2.6"/>
</gates>
<devices>
<device name="" package="BGA4C2X2X50P_106X109X67">
<connects>
<connect gate="A" pin="GND" pad="B1"/>
<connect gate="A" pin="VEN" pad="A1"/>
<connect gate="A" pin="VIN" pad="A2"/>
<connect gate="A" pin="VOUT" pad="B2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP5900TL-2.6"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="13M2070"/>
<attribute name="PACKAGE" value="BGA-4"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP5900TL-2.7" prefix="U">
<description>Linear Regulator</description>
<gates>
<gate name="A" symbol="LP5900TL-2.7"/>
</gates>
<devices>
<device name="" package="BGA4C2X2X50P_106X109X67">
<connects>
<connect gate="A" pin="GND" pad="B1"/>
<connect gate="A" pin="VEN" pad="A1"/>
<connect gate="A" pin="VIN" pad="A2"/>
<connect gate="A" pin="VOUT" pad="B2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP5900TL-2.7"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="32M1382"/>
<attribute name="PACKAGE" value="BGA-4"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP5900TL-3.0" prefix="U">
<description>Linear Regulator</description>
<gates>
<gate name="A" symbol="LP5900TL-3.0"/>
</gates>
<devices>
<device name="" package="BGA4C2X2X50P_106X109X67">
<connects>
<connect gate="A" pin="GND" pad="B1"/>
<connect gate="A" pin="VEN" pad="A1"/>
<connect gate="A" pin="VIN" pad="A2"/>
<connect gate="A" pin="VOUT" pad="B2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP5900TL-3.0"/>
<attribute name="OC_FARNELL" value="1685763"/>
<attribute name="OC_NEWARK" value="69K2661"/>
<attribute name="PACKAGE" value="BGA-4"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP5900TL-3.3" prefix="U">
<description>Linear Regulator</description>
<gates>
<gate name="A" symbol="LP5900TL-3.3"/>
</gates>
<devices>
<device name="" package="BGA4C2X2X50P_106X109X67">
<connects>
<connect gate="A" pin="GND" pad="B1"/>
<connect gate="A" pin="VEN" pad="A1"/>
<connect gate="A" pin="VIN" pad="A2"/>
<connect gate="A" pin="VOUT" pad="B2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP5900TL-3.3"/>
<attribute name="OC_FARNELL" value="1685765"/>
<attribute name="OC_NEWARK" value="69K2662"/>
<attribute name="PACKAGE" value="BGA-4"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP5951MF-1.3" prefix="U">
<description>Low-Dropout CMOS Voltage Regulator</description>
<gates>
<gate name="A" symbol="LP5951MF-1.3"/>
</gates>
<devices>
<device name="" package="SOT95P285X120-5N">
<connects>
<connect gate="A" pin="EN" pad="3"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="NC" pad="4"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="VOUT" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP5951MF-1.3"/>
<attribute name="OC_FARNELL" value="1312651"/>
<attribute name="OC_NEWARK" value="99K2605"/>
<attribute name="PACKAGE" value="SOT-23-5"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP5951MF-1.5" prefix="U">
<description>Low-Dropout CMOS Voltage Regulator</description>
<gates>
<gate name="A" symbol="LP5951MF-1.5"/>
</gates>
<devices>
<device name="" package="SOT95P285X120-5N">
<connects>
<connect gate="A" pin="EN" pad="3"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="NC" pad="4"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="VOUT" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP5951MF-1.5"/>
<attribute name="OC_FARNELL" value="1312652"/>
<attribute name="OC_NEWARK" value="13M2073"/>
<attribute name="PACKAGE" value="SOT-23-5"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP5951MF-1.8" prefix="U">
<description>Low-Dropout CMOS Voltage Regulator</description>
<gates>
<gate name="A" symbol="LP5951MF-1.8"/>
</gates>
<devices>
<device name="" package="SOT95P285X120-5N">
<connects>
<connect gate="A" pin="EN" pad="3"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="NC" pad="4"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="VOUT" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP5951MF-1.8"/>
<attribute name="OC_FARNELL" value="1312653"/>
<attribute name="OC_NEWARK" value="13M2075"/>
<attribute name="PACKAGE" value="SOT-23-5"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP5951MF-2.0" prefix="U">
<description>Low-Dropout CMOS Voltage Regulator</description>
<gates>
<gate name="A" symbol="LP5951MF-2.0"/>
</gates>
<devices>
<device name="" package="SOT95P285X120-5N">
<connects>
<connect gate="A" pin="EN" pad="3"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="NC" pad="4"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="VOUT" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP5951MF-2.0"/>
<attribute name="OC_FARNELL" value="1312654"/>
<attribute name="OC_NEWARK" value="31M5546"/>
<attribute name="PACKAGE" value="SOT-23-5"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP5951MF-2.5" prefix="U">
<description>Low-Dropout CMOS Voltage Regulator</description>
<gates>
<gate name="A" symbol="LP5951MF-2.5"/>
</gates>
<devices>
<device name="" package="SOT95P285X120-5N">
<connects>
<connect gate="A" pin="EN" pad="3"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="NC" pad="4"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="VOUT" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP5951MF-2.5"/>
<attribute name="OC_FARNELL" value="1312655"/>
<attribute name="OC_NEWARK" value="13M2079"/>
<attribute name="PACKAGE" value="SOT-23-5"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP5951MF-2.8" prefix="U">
<description>Low-Dropout CMOS Voltage Regulator</description>
<gates>
<gate name="A" symbol="LP5951MF-2.8"/>
</gates>
<devices>
<device name="" package="SOT95P285X120-5N">
<connects>
<connect gate="A" pin="EN" pad="3"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="NC" pad="4"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="VOUT" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP5951MF-2.8"/>
<attribute name="OC_FARNELL" value="1312656"/>
<attribute name="OC_NEWARK" value="13M2081"/>
<attribute name="PACKAGE" value="SOT-23-5"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP5951MF-3.0" prefix="U">
<description>Low-Dropout CMOS Voltage Regulator</description>
<gates>
<gate name="A" symbol="LP5951MF-3.0"/>
</gates>
<devices>
<device name="" package="SOT95P285X120-5N">
<connects>
<connect gate="A" pin="EN" pad="3"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="NC" pad="4"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="VOUT" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP5951MF-3.0"/>
<attribute name="OC_FARNELL" value="1312657"/>
<attribute name="OC_NEWARK" value="13M2083"/>
<attribute name="PACKAGE" value="SOT-23-5"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP5951MF-3.3" prefix="U">
<description>Low-Dropout CMOS Voltage Regulator</description>
<gates>
<gate name="A" symbol="LP5951MF-3.3"/>
</gates>
<devices>
<device name="" package="SOT95P285X120-5N">
<connects>
<connect gate="A" pin="EN" pad="3"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="NC" pad="4"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="VOUT" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP5951MF-33"/>
<attribute name="OC_FARNELL" value="1312658"/>
<attribute name="OC_NEWARK" value="13M2085"/>
<attribute name="PACKAGE" value="SOT-23-5"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP5951MG-1.3" prefix="U">
<description>CMOS Voltage Regulator</description>
<gates>
<gate name="A" symbol="LP5951MG-1.3"/>
</gates>
<devices>
<device name="" package="SOT65P240X110-5N">
<connects>
<connect gate="A" pin="EN" pad="3"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="NC" pad="4"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="VOUT" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP5951MG-13"/>
<attribute name="OC_FARNELL" value="1286707"/>
<attribute name="OC_NEWARK" value="13M2102"/>
<attribute name="PACKAGE" value="SOT-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP5951MG-1.5" prefix="U">
<description>CMOS Voltage Regulator</description>
<gates>
<gate name="A" symbol="LP5951MG-1.5"/>
</gates>
<devices>
<device name="" package="SOT65P240X110-5N">
<connects>
<connect gate="A" pin="EN" pad="3"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="NC" pad="4"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="VOUT" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP5951MG-1.5"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="13M2105"/>
<attribute name="PACKAGE" value="SOT-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP5951MG-1.8" prefix="U">
<description>CMOS Voltage Regulator</description>
<gates>
<gate name="A" symbol="LP5951MG-1.8"/>
</gates>
<devices>
<device name="" package="SOT65P240X110-5N">
<connects>
<connect gate="A" pin="EN" pad="3"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="NC" pad="4"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="VOUT" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP5951MG-1.8"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="32M1385"/>
<attribute name="PACKAGE" value="SOT-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP5951MG-2.0" prefix="U">
<description>CMOS Voltage Regulator</description>
<gates>
<gate name="A" symbol="LP5951MG-2.0"/>
</gates>
<devices>
<device name="" package="SOT65P240X110-5N">
<connects>
<connect gate="A" pin="EN" pad="3"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="NC" pad="4"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="VOUT" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP5951MG-2.0"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="32M1386"/>
<attribute name="PACKAGE" value="SOT-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP5951MG-2.5" prefix="U">
<description>CMOS Voltage Regulator</description>
<gates>
<gate name="A" symbol="LP5951MG-2.5"/>
</gates>
<devices>
<device name="" package="SOT65P240X110-5N">
<connects>
<connect gate="A" pin="EN" pad="3"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="NC" pad="4"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="VOUT" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP5951MG-2.5"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="32M1388"/>
<attribute name="PACKAGE" value="SOT-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP5951MG-2.8" prefix="U">
<description>CMOS Voltage Regulator</description>
<gates>
<gate name="A" symbol="LP5951MG-2.8"/>
</gates>
<devices>
<device name="" package="SOT65P240X110-5N">
<connects>
<connect gate="A" pin="EN" pad="3"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="NC" pad="4"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="VOUT" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP5951MG-28"/>
<attribute name="OC_FARNELL" value="1320990"/>
<attribute name="OC_NEWARK" value="31M5553"/>
<attribute name="PACKAGE" value="SC-70-5"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP5951MG-3.0" prefix="U">
<description>CMOS Voltage Regulator</description>
<gates>
<gate name="A" symbol="LP5951MG-3.0"/>
</gates>
<devices>
<device name="" package="SOT65P240X110-5N">
<connects>
<connect gate="A" pin="EN" pad="3"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="NC" pad="4"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="VOUT" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP5951MG-3.0"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="32M1390"/>
<attribute name="PACKAGE" value="SOT-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP5951MG-3.3" prefix="U">
<description>CMOS Voltage Regulator</description>
<gates>
<gate name="A" symbol="LP5951MG-3.3"/>
</gates>
<devices>
<device name="" package="SOT65P240X110-5N">
<connects>
<connect gate="A" pin="EN" pad="3"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="NC" pad="4"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="VOUT" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP5951MG-3.3"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="32M1393"/>
<attribute name="PACKAGE" value="SOT-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP5952TL-0.7" prefix="U">
<description>Dual Rail Linear Regulator</description>
<gates>
<gate name="A" symbol="LP5952TL-0.7"/>
</gates>
<devices>
<device name="" package="BGA5C3X3X50P_95X133X67">
<connects>
<connect gate="A" pin="EN" pad="C3"/>
<connect gate="A" pin="GND" pad="B2"/>
<connect gate="A" pin="VBATT" pad="C1"/>
<connect gate="A" pin="VIN" pad="A1"/>
<connect gate="A" pin="VOUT" pad="A3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP5952TL-0.7"/>
<attribute name="OC_FARNELL" value="1313874"/>
<attribute name="OC_NEWARK" value="32M1403"/>
<attribute name="PACKAGE" value="BGA-5"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP5952TL-1.2" prefix="U">
<description>Dual Rail Linear Regulator</description>
<gates>
<gate name="A" symbol="LP5952TL-1.2"/>
</gates>
<devices>
<device name="" package="BGA5C3X3X50P_95X133X67">
<connects>
<connect gate="A" pin="EN" pad="C3"/>
<connect gate="A" pin="GND" pad="B2"/>
<connect gate="A" pin="VBATT" pad="C1"/>
<connect gate="A" pin="VIN" pad="A1"/>
<connect gate="A" pin="VOUT" pad="A3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP5952TL-1.2"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="32M1404"/>
<attribute name="PACKAGE" value="BGA-5"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP5952TL-1.3" prefix="U">
<description>Dual Rail Linear Regulator</description>
<gates>
<gate name="A" symbol="LP5952TL-1.3"/>
</gates>
<devices>
<device name="" package="BGA5C3X3X50P_95X133X67">
<connects>
<connect gate="A" pin="EN" pad="C3"/>
<connect gate="A" pin="GND" pad="B2"/>
<connect gate="A" pin="VBATT" pad="C1"/>
<connect gate="A" pin="VIN" pad="A1"/>
<connect gate="A" pin="VOUT" pad="A3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP5952TL-1.3"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="32M1405"/>
<attribute name="PACKAGE" value="BGA-5"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP5952TL-1.4" prefix="U">
<description>Dual Rail Linear Regulator</description>
<gates>
<gate name="A" symbol="LP5952TL-1.4"/>
</gates>
<devices>
<device name="" package="BGA5C3X3X50P_133X95X67">
<connects>
<connect gate="A" pin="EN" pad="C3"/>
<connect gate="A" pin="GND" pad="B2"/>
<connect gate="A" pin="VBATT" pad="C1"/>
<connect gate="A" pin="VIN" pad="A1"/>
<connect gate="A" pin="VOUT" pad="A3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP5952TL-14"/>
<attribute name="OC_FARNELL" value="32M1407"/>
<attribute name="OC_NEWARK" value="1325427"/>
<attribute name="PACKAGE" value="BGA-5"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP5952TL-1.5" prefix="U">
<description>Dual Rail Linear Regulator</description>
<gates>
<gate name="A" symbol="LP5952TL-1.5"/>
</gates>
<devices>
<device name="" package="BGA5C3X3X50P_95X133X67">
<connects>
<connect gate="A" pin="EN" pad="C3"/>
<connect gate="A" pin="GND" pad="B2"/>
<connect gate="A" pin="VBATT" pad="C1"/>
<connect gate="A" pin="VIN" pad="A1"/>
<connect gate="A" pin="VOUT" pad="A3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP5952TL-1.5"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="32M1408"/>
<attribute name="PACKAGE" value="BGA-5"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP5952TL-1.6" prefix="U">
<description>Dual Rail Linear Regulator</description>
<gates>
<gate name="A" symbol="LP5952TL-1.6"/>
</gates>
<devices>
<device name="" package="BGA5C3X3X50P_95X133X67">
<connects>
<connect gate="A" pin="EN" pad="C3"/>
<connect gate="A" pin="GND" pad="B2"/>
<connect gate="A" pin="VBATT" pad="C1"/>
<connect gate="A" pin="VIN" pad="A1"/>
<connect gate="A" pin="VOUT" pad="A3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP5952TL-1.6"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="32M1410"/>
<attribute name="PACKAGE" value="BGA-5"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP5952TL-1.8" prefix="U">
<description>Dual Rail Linear Regulator</description>
<gates>
<gate name="A" symbol="LP5952TL-1.8"/>
</gates>
<devices>
<device name="" package="BGA5C3X3X50P_95X133X67">
<connects>
<connect gate="A" pin="EN" pad="C3"/>
<connect gate="A" pin="GND" pad="B2"/>
<connect gate="A" pin="VBATT" pad="C1"/>
<connect gate="A" pin="VIN" pad="A1"/>
<connect gate="A" pin="VOUT" pad="A3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP5952TL-1.8"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="32M1411"/>
<attribute name="PACKAGE" value="BGA-5"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP5952TL-2.0" prefix="U">
<description>Dual Rail Linear Regulator</description>
<gates>
<gate name="A" symbol="LP5952TL-2.0"/>
</gates>
<devices>
<device name="" package="BGA5C3X3X50P_95X133X67">
<connects>
<connect gate="A" pin="EN" pad="C3"/>
<connect gate="A" pin="GND" pad="B2"/>
<connect gate="A" pin="VBATT" pad="C1"/>
<connect gate="A" pin="VIN" pad="A1"/>
<connect gate="A" pin="VOUT" pad="A3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP5952TL-2.0"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="32M1412"/>
<attribute name="PACKAGE" value="BGA-5"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP5996SD-3333" prefix="U">
<description>Dual Linear Regulator</description>
<gates>
<gate name="A" symbol="LP5996SD-3333"/>
</gates>
<devices>
<device name="" package="DFN300X300X80-11N">
<connects>
<connect gate="A" pin="CBYP" pad="4"/>
<connect gate="A" pin="EN1" pad="2"/>
<connect gate="A" pin="EN2" pad="3"/>
<connect gate="A" pin="EPAD" pad="11"/>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="NC" pad="8"/>
<connect gate="A" pin="NC_2" pad="5"/>
<connect gate="A" pin="NC_3" pad="7"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="VOUT1" pad="10"/>
<connect gate="A" pin="VOUT2" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP5996SD-3333"/>
<attribute name="OC_FARNELL" value="1312666"/>
<attribute name="OC_NEWARK" value="31M5562"/>
<attribute name="PACKAGE" value="DFN-10"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP8358MF-1.2" prefix="U">
<description>Low Dropout Regulator</description>
<gates>
<gate name="A" symbol="LP8358MF-1.2"/>
</gates>
<devices>
<device name="" package="SOT95P285X120-5N">
<connects>
<connect gate="A" pin="EN" pad="3"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="PG" pad="4"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="VOUT" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LP8358MF-12"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K8192"/>
<attribute name="PACKAGE" value="SOT-23-5"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LPC660AIM" prefix="U">
<description>CMOS Quad Operational Amplifier</description>
<gates>
<gate name="A" symbol="LPC660AIM"/>
</gates>
<devices>
<device name="" package="SOIC127P620X175-14N">
<connects>
<connect gate="A" pin="+IN1" pad="3"/>
<connect gate="A" pin="+IN2" pad="5"/>
<connect gate="A" pin="+IN3" pad="10"/>
<connect gate="A" pin="+IN4" pad="12"/>
<connect gate="A" pin="-IN1" pad="2"/>
<connect gate="A" pin="-IN2" pad="6"/>
<connect gate="A" pin="-IN3" pad="9"/>
<connect gate="A" pin="-IN4" pad="13"/>
<connect gate="A" pin="OUT1" pad="1"/>
<connect gate="A" pin="OUT2" pad="7"/>
<connect gate="A" pin="OUT3" pad="8"/>
<connect gate="A" pin="OUT4" pad="14"/>
<connect gate="A" pin="V+" pad="4"/>
<connect gate="A" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LPC660AIM"/>
<attribute name="OC_FARNELL" value="1685388"/>
<attribute name="OC_NEWARK" value="41K6509"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LPC661IM" prefix="U">
<description>CMOS Operational Amplifier</description>
<gates>
<gate name="A" symbol="LPC661IM"/>
</gates>
<devices>
<device name="" package="SOIC127P620X175-8N">
<connects>
<connect gate="A" pin="NC" pad="8"/>
<connect gate="A" pin="NC_2" pad="5"/>
<connect gate="A" pin="NC_3" pad="1"/>
<connect gate="A" pin="NEG" pad="2"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="POS" pad="3"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LPC661IM"/>
<attribute name="OC_FARNELL" value="1215216"/>
<attribute name="OC_NEWARK" value="41K6513"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LPC662AIM" prefix="U">
<description>CMOS Dual Operational Amplifier</description>
<gates>
<gate name="A" symbol="LPC662AIM"/>
</gates>
<devices>
<device name="" package="SOIC127P620X175-8N">
<connects>
<connect gate="A" pin="NEGA" pad="2"/>
<connect gate="A" pin="NEGB" pad="6"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="POSA" pad="3"/>
<connect gate="A" pin="POSB" pad="5"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LPC662AIM"/>
<attribute name="OC_FARNELL" value="1685389"/>
<attribute name="OC_NEWARK" value="41K6515"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LPC662IM" prefix="U">
<description>CMOS Dual Operational Amplifier</description>
<gates>
<gate name="A" symbol="LPC662IM"/>
</gates>
<devices>
<device name="" package="SOIC127P620X175-8N">
<connects>
<connect gate="A" pin="NEGA" pad="2"/>
<connect gate="A" pin="NEGB" pad="6"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="POSA" pad="3"/>
<connect gate="A" pin="POSB" pad="5"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LPC662IM"/>
<attribute name="OC_FARNELL" value="9493875"/>
<attribute name="OC_NEWARK" value="97K3624"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LPV321M5" prefix="U">
<description>Operational Amplifier</description>
<gates>
<gate name="A" symbol="LPV321M5"/>
</gates>
<devices>
<device name="" package="SOT95P280X120-5N">
<connects>
<connect gate="A" pin="+IN" pad="1"/>
<connect gate="A" pin="-IN" pad="3"/>
<connect gate="A" pin="OUT" pad="4"/>
<connect gate="A" pin="V+" pad="5"/>
<connect gate="A" pin="V-" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LPV321M5"/>
<attribute name="OC_FARNELL" value="1468938"/>
<attribute name="OC_NEWARK" value="41K6519"/>
<attribute name="PACKAGE" value="SOT-5"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LPV321M7" prefix="U">
<description>Operational Amplifier</description>
<gates>
<gate name="A" symbol="LPV321M7"/>
</gates>
<devices>
<device name="" package="SOT65P240X110-5N">
<connects>
<connect gate="A" pin="+IN" pad="1"/>
<connect gate="A" pin="-IN" pad="3"/>
<connect gate="A" pin="OUT" pad="4"/>
<connect gate="A" pin="V+" pad="5"/>
<connect gate="A" pin="V-" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LPV321M7"/>
<attribute name="OC_FARNELL" value="74C4805"/>
<attribute name="OC_NEWARK" value="-"/>
<attribute name="PACKAGE" value="SOT-5"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LPV324M" prefix="U">
<description>Operational Amplifiers</description>
<gates>
<gate name="A" symbol="LPV324M"/>
</gates>
<devices>
<device name="" package="SOIC127P620X175-14N">
<connects>
<connect gate="A" pin="+INA" pad="3"/>
<connect gate="A" pin="+INB" pad="5"/>
<connect gate="A" pin="+INC" pad="10"/>
<connect gate="A" pin="+IND" pad="12"/>
<connect gate="A" pin="-INA" pad="2"/>
<connect gate="A" pin="-INB" pad="6"/>
<connect gate="A" pin="-INC" pad="9"/>
<connect gate="A" pin="-IND" pad="13"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="OUTC" pad="8"/>
<connect gate="A" pin="OUTD" pad="14"/>
<connect gate="A" pin="V+" pad="4"/>
<connect gate="A" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LPV324M"/>
<attribute name="OC_FARNELL" value="1685329"/>
<attribute name="OC_NEWARK" value="41K6523"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LPV324MT" prefix="U">
<description>Operational Amplifiers</description>
<gates>
<gate name="A" symbol="LPV324MT"/>
</gates>
<devices>
<device name="" package="SOP65P640X110-14N">
<connects>
<connect gate="A" pin="+INA" pad="3"/>
<connect gate="A" pin="+INB" pad="5"/>
<connect gate="A" pin="+INC" pad="10"/>
<connect gate="A" pin="+IND" pad="12"/>
<connect gate="A" pin="-INA" pad="2"/>
<connect gate="A" pin="-INB" pad="6"/>
<connect gate="A" pin="-INC" pad="9"/>
<connect gate="A" pin="-IND" pad="13"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="OUTC" pad="8"/>
<connect gate="A" pin="OUTD" pad="14"/>
<connect gate="A" pin="V+" pad="4"/>
<connect gate="A" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LPV324MT"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K6524"/>
<attribute name="PACKAGE" value="TSSOP-14"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LPV358MM" prefix="U">
<description>Output Operational Amplifiers</description>
<gates>
<gate name="A" symbol="LPV358MM"/>
</gates>
<devices>
<device name="" package="SOP65P490X110-8N">
<connects>
<connect gate="A" pin="+INA" pad="3"/>
<connect gate="A" pin="+INB" pad="5"/>
<connect gate="A" pin="-INA" pad="2"/>
<connect gate="A" pin="-INB" pad="6"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LPV358MM"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="74C4812"/>
<attribute name="PACKAGE" value="MSOP-8"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LPV511MG" prefix="U">
<description>Op Amp</description>
<gates>
<gate name="A" symbol="LPV511MG"/>
</gates>
<devices>
<device name="" package="SOT65P210X110-5N">
<connects>
<connect gate="A" pin="V+" pad="5"/>
<connect gate="A" pin="V-" pad="2"/>
<connect gate="A" pin="VIN+" pad="3"/>
<connect gate="A" pin="VIN-" pad="4"/>
<connect gate="A" pin="VOUT" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LPV511MG"/>
<attribute name="OC_FARNELL" value="1312667"/>
<attribute name="OC_NEWARK" value="79K7967"/>
<attribute name="PACKAGE" value="SC-70-5"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LPV531MK" prefix="U">
<description>LPV531MK</description>
<gates>
<gate name="A" symbol="LPV531MK"/>
</gates>
<devices>
<device name="" package="SOT95P285X100-6N">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="4"/>
<connect gate="A" pin="ISEL" pad="5"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="A" pin="V+" pad="6"/>
<connect gate="A" pin="V-" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LPV531MK"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="99K2566"/>
<attribute name="PACKAGE" value="SOT-6"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LPV7215MF" prefix="U">
<description>Comparator</description>
<gates>
<gate name="A" symbol="LPV7215MF"/>
</gates>
<devices>
<device name="" package="SOT95P285X120-5N">
<connects>
<connect gate="A" pin="+VIN" pad="3"/>
<connect gate="A" pin="-VIN" pad="4"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="A" pin="V+" pad="5"/>
<connect gate="A" pin="V-" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LPV7215MF"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="32M1312"/>
<attribute name="PACKAGE" value="SOT-5"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LPV7215MG" prefix="U">
<description>Output Comparator</description>
<gates>
<gate name="A" symbol="LPV7215MG"/>
</gates>
<devices>
<device name="" package="SOT65P210X110-5N">
<connects>
<connect gate="A" pin="V+" pad="5"/>
<connect gate="A" pin="V-" pad="2"/>
<connect gate="A" pin="VIN+" pad="3"/>
<connect gate="A" pin="VIN-" pad="4"/>
<connect gate="A" pin="VOUT" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LPV7215MG"/>
<attribute name="OC_FARNELL" value="1202775"/>
<attribute name="OC_NEWARK" value="99K2571"/>
<attribute name="PACKAGE" value="SC-70-5"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PC16550DN">
<description>Receiver/Transmitter</description>
<gates>
<gate name="A" symbol="PC16550DN"/>
</gates>
<devices>
<device name="" package="DIP254P1524X533-40">
<connects>
<connect gate="A" pin="A0" pad="28"/>
<connect gate="A" pin="A1" pad="27"/>
<connect gate="A" pin="A2" pad="26"/>
<connect gate="A" pin="CS0" pad="12"/>
<connect gate="A" pin="CS1" pad="13"/>
<connect gate="A" pin="D0" pad="1"/>
<connect gate="A" pin="D1" pad="2"/>
<connect gate="A" pin="D2" pad="3"/>
<connect gate="A" pin="D3" pad="4"/>
<connect gate="A" pin="D4" pad="5"/>
<connect gate="A" pin="D5" pad="6"/>
<connect gate="A" pin="D6" pad="7"/>
<connect gate="A" pin="D7" pad="8"/>
<connect gate="A" pin="DDIS" pad="23"/>
<connect gate="A" pin="INTR" pad="30"/>
<connect gate="A" pin="MR" pad="35"/>
<connect gate="A" pin="RCLK" pad="9"/>
<connect gate="A" pin="RD" pad="22"/>
<connect gate="A" pin="SIN" pad="10"/>
<connect gate="A" pin="SOUT" pad="11"/>
<connect gate="A" pin="VDD" pad="40"/>
<connect gate="A" pin="VSS" pad="20"/>
<connect gate="A" pin="WR" pad="19"/>
<connect gate="A" pin="XIN" pad="16"/>
<connect gate="A" pin="XOUT" pad="17"/>
<connect gate="A" pin="~ADS" pad="25"/>
<connect gate="A" pin="~BAUDOUT" pad="15"/>
<connect gate="A" pin="~CS2" pad="14"/>
<connect gate="A" pin="~CTS" pad="36"/>
<connect gate="A" pin="~DCD" pad="38"/>
<connect gate="A" pin="~DSR" pad="37"/>
<connect gate="A" pin="~DTR" pad="33"/>
<connect gate="A" pin="~OUT1" pad="34"/>
<connect gate="A" pin="~OUT2" pad="31"/>
<connect gate="A" pin="~RD" pad="21"/>
<connect gate="A" pin="~RI" pad="39"/>
<connect gate="A" pin="~RTS" pad="32"/>
<connect gate="A" pin="~RXRDY" pad="29"/>
<connect gate="A" pin="~TXRDY" pad="24"/>
<connect gate="A" pin="~WR" pad="18"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="PC16550DN"/>
<attribute name="OC_FARNELL" value="9490507"/>
<attribute name="OC_NEWARK" value="41K8300"/>
<attribute name="PACKAGE" value="40-DIP"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SCAN12100TYA" prefix="U">
<description>SCAN12100TYA</description>
<gates>
<gate name="A" symbol="SCAN12100TYA"/>
</gates>
<devices>
<device name="" package="QFP50P1600X1600X120-101N">
<connects>
<connect gate="A" pin="ADD0" pad="37"/>
<connect gate="A" pin="ADD1" pad="36"/>
<connect gate="A" pin="ADD2" pad="35"/>
<connect gate="A" pin="ADD3" pad="34"/>
<connect gate="A" pin="ADD4" pad="33"/>
<connect gate="A" pin="AVDD18" pad="47"/>
<connect gate="A" pin="AVDD18_2" pad="20"/>
<connect gate="A" pin="AVDD18_3" pad="15"/>
<connect gate="A" pin="AVDD18_4" pad="32"/>
<connect gate="A" pin="AVDD18_5" pad="9"/>
<connect gate="A" pin="AVDD18_6" pad="38"/>
<connect gate="A" pin="AVDD18_7" pad="85"/>
<connect gate="A" pin="AVDD33" pad="21"/>
<connect gate="A" pin="AVDD33_2" pad="8"/>
<connect gate="A" pin="AVDD33_3" pad="14"/>
<connect gate="A" pin="AVDD33_4" pad="42"/>
<connect gate="A" pin="CALIGN_EN" pad="92"/>
<connect gate="A" pin="CDET" pad="79"/>
<connect gate="A" pin="DIN_[0]" pad="65"/>
<connect gate="A" pin="DIN_[1]" pad="66"/>
<connect gate="A" pin="DIN_[2]" pad="67"/>
<connect gate="A" pin="DIN_[3]" pad="68"/>
<connect gate="A" pin="DIN_[4]" pad="69"/>
<connect gate="A" pin="DIN_[5]" pad="70"/>
<connect gate="A" pin="DIN_[6]" pad="71"/>
<connect gate="A" pin="DIN_[7]" pad="72"/>
<connect gate="A" pin="DIN_[8]" pad="73"/>
<connect gate="A" pin="DIN_[9]" pad="74"/>
<connect gate="A" pin="DOUTN" pad="11"/>
<connect gate="A" pin="DOUTP" pad="12"/>
<connect gate="A" pin="EPAD" pad="101"/>
<connect gate="A" pin="EQ_[0]" pad="88"/>
<connect gate="A" pin="EQ_[1]" pad="89"/>
<connect gate="A" pin="GND" pad="39"/>
<connect gate="A" pin="GND_10" pad="48"/>
<connect gate="A" pin="GND_11" pad="19"/>
<connect gate="A" pin="GND_12" pad="27"/>
<connect gate="A" pin="GND_13" pad="10"/>
<connect gate="A" pin="GND_14" pad="49"/>
<connect gate="A" pin="GND_15" pad="16"/>
<connect gate="A" pin="GND_16" pad="75"/>
<connect gate="A" pin="GND_17" pad="13"/>
<connect gate="A" pin="GND_18" pad="63"/>
<connect gate="A" pin="GND_2" pad="86"/>
<connect gate="A" pin="GND_3" pad="3"/>
<connect gate="A" pin="GND_4" pad="25"/>
<connect gate="A" pin="GND_5" pad="4"/>
<connect gate="A" pin="GND_6" pad="40"/>
<connect gate="A" pin="GND_7" pad="5"/>
<connect gate="A" pin="GND_8" pad="26"/>
<connect gate="A" pin="GND_9" pad="24"/>
<connect gate="A" pin="IOVDD" pad="76"/>
<connect gate="A" pin="IOVDD_2" pad="50"/>
<connect gate="A" pin="IOVDD_3" pad="51"/>
<connect gate="A" pin="IOVDD_4" pad="87"/>
<connect gate="A" pin="LOCKB" pad="77"/>
<connect gate="A" pin="LOOP_[0]" pad="99"/>
<connect gate="A" pin="LOOP_[1]" pad="100"/>
<connect gate="A" pin="LOS" pad="78"/>
<connect gate="A" pin="MDC" pad="30"/>
<connect gate="A" pin="MDIO" pad="31"/>
<connect gate="A" pin="OPMODE" pad="94"/>
<connect gate="A" pin="PE[0]" pad="82"/>
<connect gate="A" pin="PE[1]" pad="81"/>
<connect gate="A" pin="PVDD33" pad="2"/>
<connect gate="A" pin="PVDD33_2" pad="28"/>
<connect gate="A" pin="PVDD33_3" pad="1"/>
<connect gate="A" pin="PVDD33_4" pad="29"/>
<connect gate="A" pin="REFCLKN" pad="7"/>
<connect gate="A" pin="REFCLKP" pad="6"/>
<connect gate="A" pin="RES1" pad="83"/>
<connect gate="A" pin="RES2" pad="84"/>
<connect gate="A" pin="RESETB" pad="95"/>
<connect gate="A" pin="RINN" pad="17"/>
<connect gate="A" pin="RINP" pad="18"/>
<connect gate="A" pin="ROUT_[0]" pad="53"/>
<connect gate="A" pin="ROUT_[1]" pad="54"/>
<connect gate="A" pin="ROUT_[2]" pad="55"/>
<connect gate="A" pin="ROUT_[3]" pad="56"/>
<connect gate="A" pin="ROUT_[4]" pad="57"/>
<connect gate="A" pin="ROUT_[5]" pad="58"/>
<connect gate="A" pin="ROUT_[6]" pad="59"/>
<connect gate="A" pin="ROUT_[7]" pad="60"/>
<connect gate="A" pin="ROUT_[8]" pad="61"/>
<connect gate="A" pin="ROUT_[9]" pad="62"/>
<connect gate="A" pin="RXCLK" pad="52"/>
<connect gate="A" pin="RXCLKMODE" pad="93"/>
<connect gate="A" pin="RXPWDNB" pad="91"/>
<connect gate="A" pin="SPMODE[0]" pad="96"/>
<connect gate="A" pin="SPMODE[1]" pad="97"/>
<connect gate="A" pin="SYSCLKN" pad="23"/>
<connect gate="A" pin="SYSCLKP" pad="22"/>
<connect gate="A" pin="TCK" pad="43"/>
<connect gate="A" pin="TDI" pad="45"/>
<connect gate="A" pin="TDO" pad="41"/>
<connect gate="A" pin="TENBMODE" pad="98"/>
<connect gate="A" pin="TMS" pad="44"/>
<connect gate="A" pin="TRSTB" pad="46"/>
<connect gate="A" pin="TXCLK" pad="64"/>
<connect gate="A" pin="TXPWDNB" pad="90"/>
<connect gate="A" pin="VSEL" pad="80"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="SCAN12100TYA"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="46M5620"/>
<attribute name="PACKAGE" value="TQFP-100"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SCAN25100TYA" prefix="U">
<description>IC,Serial-to-Parallel Converter</description>
<gates>
<gate name="A" symbol="SCAN25100TYA"/>
</gates>
<devices>
<device name="" package="QFP50P1600X1600X120-101N">
<connects>
<connect gate="A" pin="ADD0" pad="37"/>
<connect gate="A" pin="ADD1" pad="36"/>
<connect gate="A" pin="ADD2" pad="35"/>
<connect gate="A" pin="ADD3" pad="34"/>
<connect gate="A" pin="ADD4" pad="33"/>
<connect gate="A" pin="AVDD18" pad="47"/>
<connect gate="A" pin="AVDD18_2" pad="20"/>
<connect gate="A" pin="AVDD18_3" pad="15"/>
<connect gate="A" pin="AVDD18_4" pad="32"/>
<connect gate="A" pin="AVDD18_5" pad="9"/>
<connect gate="A" pin="AVDD18_6" pad="38"/>
<connect gate="A" pin="AVDD18_7" pad="85"/>
<connect gate="A" pin="AVDD33" pad="21"/>
<connect gate="A" pin="AVDD33_2" pad="8"/>
<connect gate="A" pin="AVDD33_3" pad="14"/>
<connect gate="A" pin="AVDD33_4" pad="42"/>
<connect gate="A" pin="CALIGN_EN" pad="92"/>
<connect gate="A" pin="CDET" pad="79"/>
<connect gate="A" pin="DIN_[0]" pad="65"/>
<connect gate="A" pin="DIN_[1]" pad="66"/>
<connect gate="A" pin="DIN_[2]" pad="67"/>
<connect gate="A" pin="DIN_[3]" pad="68"/>
<connect gate="A" pin="DIN_[4]" pad="69"/>
<connect gate="A" pin="DIN_[5]" pad="70"/>
<connect gate="A" pin="DIN_[6]" pad="71"/>
<connect gate="A" pin="DIN_[7]" pad="72"/>
<connect gate="A" pin="DIN_[8]" pad="73"/>
<connect gate="A" pin="DIN_[9]" pad="74"/>
<connect gate="A" pin="DOUTN" pad="11"/>
<connect gate="A" pin="DOUTP" pad="12"/>
<connect gate="A" pin="EPAD" pad="101"/>
<connect gate="A" pin="EQ_[0]" pad="88"/>
<connect gate="A" pin="EQ_[1]" pad="89"/>
<connect gate="A" pin="GND" pad="39"/>
<connect gate="A" pin="GND_10" pad="48"/>
<connect gate="A" pin="GND_11" pad="19"/>
<connect gate="A" pin="GND_12" pad="27"/>
<connect gate="A" pin="GND_13" pad="10"/>
<connect gate="A" pin="GND_14" pad="49"/>
<connect gate="A" pin="GND_15" pad="16"/>
<connect gate="A" pin="GND_16" pad="75"/>
<connect gate="A" pin="GND_17" pad="13"/>
<connect gate="A" pin="GND_18" pad="63"/>
<connect gate="A" pin="GND_2" pad="86"/>
<connect gate="A" pin="GND_3" pad="3"/>
<connect gate="A" pin="GND_4" pad="25"/>
<connect gate="A" pin="GND_5" pad="4"/>
<connect gate="A" pin="GND_6" pad="40"/>
<connect gate="A" pin="GND_7" pad="5"/>
<connect gate="A" pin="GND_8" pad="26"/>
<connect gate="A" pin="GND_9" pad="24"/>
<connect gate="A" pin="IOVDD" pad="76"/>
<connect gate="A" pin="IOVDD_2" pad="50"/>
<connect gate="A" pin="IOVDD_3" pad="51"/>
<connect gate="A" pin="IOVDD_4" pad="87"/>
<connect gate="A" pin="LOCKB" pad="77"/>
<connect gate="A" pin="LOOP_[0]" pad="99"/>
<connect gate="A" pin="LOOP_[1]" pad="100"/>
<connect gate="A" pin="LOS" pad="78"/>
<connect gate="A" pin="MDC" pad="30"/>
<connect gate="A" pin="MDIO" pad="31"/>
<connect gate="A" pin="OPMODE" pad="94"/>
<connect gate="A" pin="PE[0]" pad="82"/>
<connect gate="A" pin="PE[1]" pad="81"/>
<connect gate="A" pin="PVDD33" pad="2"/>
<connect gate="A" pin="PVDD33_2" pad="28"/>
<connect gate="A" pin="PVDD33_3" pad="1"/>
<connect gate="A" pin="PVDD33_4" pad="29"/>
<connect gate="A" pin="REFCLKN" pad="7"/>
<connect gate="A" pin="REFCLKP" pad="6"/>
<connect gate="A" pin="RES1" pad="83"/>
<connect gate="A" pin="RES2" pad="84"/>
<connect gate="A" pin="RESETB" pad="95"/>
<connect gate="A" pin="RINN" pad="17"/>
<connect gate="A" pin="RINP" pad="18"/>
<connect gate="A" pin="ROUT_[0]" pad="53"/>
<connect gate="A" pin="ROUT_[1]" pad="54"/>
<connect gate="A" pin="ROUT_[2]" pad="55"/>
<connect gate="A" pin="ROUT_[3]" pad="56"/>
<connect gate="A" pin="ROUT_[4]" pad="57"/>
<connect gate="A" pin="ROUT_[5]" pad="58"/>
<connect gate="A" pin="ROUT_[6]" pad="59"/>
<connect gate="A" pin="ROUT_[7]" pad="60"/>
<connect gate="A" pin="ROUT_[8]" pad="61"/>
<connect gate="A" pin="ROUT_[9]" pad="62"/>
<connect gate="A" pin="RXCLK" pad="52"/>
<connect gate="A" pin="RXCLKMODE" pad="93"/>
<connect gate="A" pin="RXPWDNB" pad="91"/>
<connect gate="A" pin="SPMODE[0]" pad="96"/>
<connect gate="A" pin="SPMODE[1]" pad="97"/>
<connect gate="A" pin="SYSCLKN" pad="23"/>
<connect gate="A" pin="SYSCLKP" pad="22"/>
<connect gate="A" pin="TCK" pad="43"/>
<connect gate="A" pin="TDI" pad="45"/>
<connect gate="A" pin="TDO" pad="41"/>
<connect gate="A" pin="TENBMODE" pad="98"/>
<connect gate="A" pin="TMS" pad="44"/>
<connect gate="A" pin="TRSTB" pad="46"/>
<connect gate="A" pin="TXCLK" pad="64"/>
<connect gate="A" pin="TXPWDNB" pad="90"/>
<connect gate="A" pin="VSEL" pad="80"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="SCAN25100TYA"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="22M1774"/>
<attribute name="PACKAGE" value="TQFP-100"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SCAN90CP02VY" prefix="U">
<description>SCAN90CP02VY</description>
<gates>
<gate name="A" symbol="SCAN90CP02VY"/>
</gates>
<devices>
<device name="" package="QFP80P900X900X145-32N">
<connects>
<connect gate="A" pin="GND" pad="26"/>
<connect gate="A" pin="GND_2" pad="30"/>
<connect gate="A" pin="GND_3" pad="5"/>
<connect gate="A" pin="GND_4" pad="11"/>
<connect gate="A" pin="GND_5" pad="15"/>
<connect gate="A" pin="GND_6" pad="20"/>
<connect gate="A" pin="IN0+" pad="9"/>
<connect gate="A" pin="IN0-" pad="10"/>
<connect gate="A" pin="IN1+" pad="13"/>
<connect gate="A" pin="IN1-" pad="14"/>
<connect gate="A" pin="OUT0+" pad="32"/>
<connect gate="A" pin="OUT0-" pad="31"/>
<connect gate="A" pin="OUT1+" pad="28"/>
<connect gate="A" pin="OUT1-" pad="27"/>
<connect gate="A" pin="PEM00" pad="4"/>
<connect gate="A" pin="PEM01" pad="3"/>
<connect gate="A" pin="PEM10" pad="2"/>
<connect gate="A" pin="PEM11" pad="1"/>
<connect gate="A" pin="SEL0" pad="7"/>
<connect gate="A" pin="SEL1" pad="6"/>
<connect gate="A" pin="TCK" pad="19"/>
<connect gate="A" pin="TDI" pad="22"/>
<connect gate="A" pin="TDO" pad="23"/>
<connect gate="A" pin="TMS" pad="21"/>
<connect gate="A" pin="VDD1" pad="18"/>
<connect gate="A" pin="VDD2" pad="25"/>
<connect gate="A" pin="VDD2_2" pad="16"/>
<connect gate="A" pin="VDDA" pad="29"/>
<connect gate="A" pin="VDDA_2" pad="12"/>
<connect gate="A" pin="~EN0" pad="8"/>
<connect gate="A" pin="~EN1" pad="17"/>
<connect gate="A" pin="~TRST" pad="24"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="SCAN90CP02VY"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K8421"/>
<attribute name="PACKAGE" value="QFP-32"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SCAN921025HSM" prefix="U">
<description>Parallel-to-Serial Converter</description>
<gates>
<gate name="A" symbol="SCAN921025HSM"/>
</gates>
<devices>
<device name="" package="BGA49C7X780P_700X700X150">
<connects>
<connect gate="A" pin="AGND" pad="B5"/>
<connect gate="A" pin="AGND_2" pad="B6"/>
<connect gate="A" pin="AGND_3" pad="C6"/>
<connect gate="A" pin="AGND_4" pad="E7"/>
<connect gate="A" pin="AGND_5" pad="F7"/>
<connect gate="A" pin="AVCC" pad="G5"/>
<connect gate="A" pin="AVCC_2" pad="A5"/>
<connect gate="A" pin="AVCC_3" pad="A6"/>
<connect gate="A" pin="AVCC_4" pad="B4"/>
<connect gate="A" pin="AVCC_5" pad="B7"/>
<connect gate="A" pin="DEN" pad="D6"/>
<connect gate="A" pin="DGND" pad="G4"/>
<connect gate="A" pin="DGND_2" pad="C2"/>
<connect gate="A" pin="DGND_3" pad="A1"/>
<connect gate="A" pin="DGND_4" pad="F5"/>
<connect gate="A" pin="DGND_5" pad="E6"/>
<connect gate="A" pin="DIN0" pad="A3"/>
<connect gate="A" pin="DIN1" pad="B1"/>
<connect gate="A" pin="DIN2" pad="D2"/>
<connect gate="A" pin="DIN3" pad="C1"/>
<connect gate="A" pin="DIN4" pad="D3"/>
<connect gate="A" pin="DIN5" pad="D1"/>
<connect gate="A" pin="DIN6" pad="E2"/>
<connect gate="A" pin="DIN7" pad="E1"/>
<connect gate="A" pin="DIN8" pad="F2"/>
<connect gate="A" pin="DIN9" pad="F4"/>
<connect gate="A" pin="DO+" pad="D7"/>
<connect gate="A" pin="DO-" pad="D5"/>
<connect gate="A" pin="DVCC" pad="C4"/>
<connect gate="A" pin="DVCC_2" pad="C3"/>
<connect gate="A" pin="DVCC_3" pad="E5"/>
<connect gate="A" pin="NC" pad="G7"/>
<connect gate="A" pin="NC_2" pad="B2"/>
<connect gate="A" pin="NC_3" pad="A7"/>
<connect gate="A" pin="NC_4" pad="C5"/>
<connect gate="A" pin="NC_5" pad="D4"/>
<connect gate="A" pin="NC_6" pad="A2"/>
<connect gate="A" pin="NC_7" pad="F6"/>
<connect gate="A" pin="NC_8" pad="G6"/>
<connect gate="A" pin="SYNC1" pad="A4"/>
<connect gate="A" pin="SYNC2" pad="B3"/>
<connect gate="A" pin="TCK" pad="F3"/>
<connect gate="A" pin="TCLK" pad="E4"/>
<connect gate="A" pin="TCLKR/~F" pad="G3"/>
<connect gate="A" pin="TDI" pad="F1"/>
<connect gate="A" pin="TDO" pad="G1"/>
<connect gate="A" pin="TMS" pad="E3"/>
<connect gate="A" pin="~PWRDN" pad="C7"/>
<connect gate="A" pin="~TRST" pad="G2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="SCAN921025HSM"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="41K8430"/>
<attribute name="PACKAGE" value="BGA-49"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SCAN921260UJB" prefix="U">
<description>X6 1:10 Deserializer</description>
<gates>
<gate name="A" symbol="SCAN921260UJB_A"/>
<gate name="B" symbol="SCAN921260UJB_B"/>
</gates>
<devices>
<device name="" package="BGA196C14X14X100P_1500X1500X14">
<connects>
<connect gate="A" pin="AGND" pad="B11"/>
<connect gate="A" pin="AGND_2" pad="A8"/>
<connect gate="A" pin="AGND_3" pad="A5"/>
<connect gate="A" pin="AGND_4" pad="B7"/>
<connect gate="A" pin="AGND_5" pad="B8"/>
<connect gate="A" pin="AVDD" pad="C7"/>
<connect gate="A" pin="AVDD_2" pad="A11"/>
<connect gate="A" pin="AVDD_3" pad="B6"/>
<connect gate="A" pin="AVDD_4" pad="B9"/>
<connect gate="A" pin="BISTMODE_REQ" pad="B10"/>
<connect gate="A" pin="BIST_SEL0" pad="D8"/>
<connect gate="A" pin="BIST_SEL1" pad="D14"/>
<connect gate="A" pin="BIST_SEL2" pad="C14"/>
<connect gate="A" pin="CHTST" pad="C3"/>
<connect gate="A" pin="CHTST_EN" pad="E3"/>
<connect gate="A" pin="DGND" pad="G9"/>
<connect gate="A" pin="DGND_10" pad="D11"/>
<connect gate="A" pin="DGND_11" pad="F5"/>
<connect gate="A" pin="DGND_12" pad="F6"/>
<connect gate="A" pin="DGND_13" pad="G7"/>
<connect gate="A" pin="DGND_14" pad="F9"/>
<connect gate="A" pin="DGND_15" pad="G5"/>
<connect gate="A" pin="DGND_16" pad="G8"/>
<connect gate="A" pin="DGND_2" pad="B14"/>
<connect gate="A" pin="DGND_3" pad="A1"/>
<connect gate="A" pin="DGND_4" pad="E8"/>
<connect gate="A" pin="DGND_5" pad="D9"/>
<connect gate="A" pin="DGND_6" pad="E5"/>
<connect gate="A" pin="DGND_7" pad="D4"/>
<connect gate="A" pin="DGND_8" pad="D7"/>
<connect gate="A" pin="DGND_9" pad="D5"/>
<connect gate="A" pin="DVDD" pad="G10"/>
<connect gate="A" pin="DVDD_10" pad="D6"/>
<connect gate="A" pin="DVDD_11" pad="E10"/>
<connect gate="A" pin="DVDD_12" pad="F10"/>
<connect gate="A" pin="DVDD_13" pad="F12"/>
<connect gate="A" pin="DVDD_14" pad="G6"/>
<connect gate="A" pin="DVDD_2" pad="C4"/>
<connect gate="A" pin="DVDD_3" pad="E9"/>
<connect gate="A" pin="DVDD_4" pad="B1"/>
<connect gate="A" pin="DVDD_5" pad="E6"/>
<connect gate="A" pin="DVDD_6" pad="D12"/>
<connect gate="A" pin="DVDD_7" pad="F7"/>
<connect gate="A" pin="DVDD_8" pad="E7"/>
<connect gate="A" pin="DVDD_9" pad="B3"/>
<connect gate="A" pin="GND" pad="B2"/>
<connect gate="A" pin="NC" pad="F11"/>
<connect gate="A" pin="NC_2" pad="E11"/>
<connect gate="A" pin="PGND" pad="G2"/>
<connect gate="A" pin="PGND_2" pad="A14"/>
<connect gate="A" pin="PGND_3" pad="B12"/>
<connect gate="A" pin="PGND_4" pad="G1"/>
<connect gate="A" pin="PGND_5" pad="D10"/>
<connect gate="A" pin="PGND_6" pad="F8"/>
<connect gate="A" pin="PGND_7" pad="G13"/>
<connect gate="A" pin="PVDD" pad="G14"/>
<connect gate="A" pin="PVDD_2" pad="F1"/>
<connect gate="A" pin="PVDD_3" pad="F14"/>
<connect gate="A" pin="PVDD_4" pad="E1"/>
<connect gate="A" pin="RCLK0" pad="F2"/>
<connect gate="A" pin="RCLK5" pad="F13"/>
<connect gate="A" pin="REN" pad="A2"/>
<connect gate="A" pin="RFCLK" pad="B4"/>
<connect gate="A" pin="RIN0+" pad="A4"/>
<connect gate="A" pin="RIN0-" pad="A3"/>
<connect gate="A" pin="RIN1+" pad="C6"/>
<connect gate="A" pin="RIN1-" pad="C5"/>
<connect gate="A" pin="RIN2+" pad="A7"/>
<connect gate="A" pin="RIN2-" pad="A6"/>
<connect gate="A" pin="RIN3+" pad="C9"/>
<connect gate="A" pin="RIN3-" pad="C8"/>
<connect gate="A" pin="RIN4+" pad="A10"/>
<connect gate="A" pin="RIN4-" pad="A9"/>
<connect gate="A" pin="RIN5+" pad="C11"/>
<connect gate="A" pin="RIN5-" pad="C10"/>
<connect gate="A" pin="RIN6+" pad="A13"/>
<connect gate="A" pin="RIN6-" pad="A12"/>
<connect gate="A" pin="ROUT05" pad="G4"/>
<connect gate="A" pin="ROUT06" pad="G3"/>
<connect gate="A" pin="ROUT07" pad="F4"/>
<connect gate="A" pin="ROUT08" pad="E4"/>
<connect gate="A" pin="ROUT09" pad="E2"/>
<connect gate="A" pin="ROUT55" pad="G11"/>
<connect gate="A" pin="ROUT56" pad="G12"/>
<connect gate="A" pin="ROUT57" pad="E12"/>
<connect gate="A" pin="ROUT58" pad="E13"/>
<connect gate="A" pin="ROUT59" pad="E14"/>
<connect gate="A" pin="SEL0" pad="C12"/>
<connect gate="A" pin="SEL1" pad="C13"/>
<connect gate="A" pin="SEL2" pad="B13"/>
<connect gate="A" pin="TCK" pad="D2"/>
<connect gate="A" pin="TDI" pad="D1"/>
<connect gate="A" pin="TDO" pad="D3"/>
<connect gate="A" pin="TMS" pad="C1"/>
<connect gate="A" pin="~LOCK0" pad="F3"/>
<connect gate="A" pin="~LOCK5" pad="D13"/>
<connect gate="A" pin="~PWRDN" pad="B5"/>
<connect gate="A" pin="~TRST" pad="C2"/>
<connect gate="B" pin="BIST_ACT" pad="K11"/>
<connect gate="B" pin="DGND" pad="H9"/>
<connect gate="B" pin="DGND_2" pad="L7"/>
<connect gate="B" pin="DGND_3" pad="J6"/>
<connect gate="B" pin="DGND_4" pad="J7"/>
<connect gate="B" pin="DGND_5" pad="K8"/>
<connect gate="B" pin="DGND_6" pad="K9"/>
<connect gate="B" pin="DGND_7" pad="H7"/>
<connect gate="B" pin="DGND_8" pad="H5"/>
<connect gate="B" pin="DGND_9" pad="H8"/>
<connect gate="B" pin="DVDD" pad="L10"/>
<connect gate="B" pin="DVDD_10" pad="K7"/>
<connect gate="B" pin="DVDD_11" pad="K10"/>
<connect gate="B" pin="DVDD_2" pad="H6"/>
<connect gate="B" pin="DVDD_3" pad="J5"/>
<connect gate="B" pin="DVDD_4" pad="H10"/>
<connect gate="B" pin="DVDD_5" pad="J8"/>
<connect gate="B" pin="DVDD_6" pad="J9"/>
<connect gate="B" pin="DVDD_7" pad="J10"/>
<connect gate="B" pin="DVDD_8" pad="K5"/>
<connect gate="B" pin="DVDD_9" pad="K6"/>
<connect gate="B" pin="NC" pad="L5"/>
<connect gate="B" pin="NC_2" pad="L4"/>
<connect gate="B" pin="PGND" pad="H1"/>
<connect gate="B" pin="PGND_2" pad="H13"/>
<connect gate="B" pin="PGND_3" pad="J13"/>
<connect gate="B" pin="PGND_4" pad="J4"/>
<connect gate="B" pin="PGND_5" pad="N8"/>
<connect gate="B" pin="PGND_6" pad="N7"/>
<connect gate="B" pin="PGND_7" pad="H14"/>
<connect gate="B" pin="PGND_8" pad="P7"/>
<connect gate="B" pin="PGND_9" pad="P8"/>
<connect gate="B" pin="PVDD" pad="P10"/>
<connect gate="B" pin="PVDD_2" pad="P5"/>
<connect gate="B" pin="PVDD_3" pad="J14"/>
<connect gate="B" pin="PVDD_4" pad="K14"/>
<connect gate="B" pin="PVDD_5" pad="P9"/>
<connect gate="B" pin="PVDD_6" pad="J1"/>
<connect gate="B" pin="PVDD_7" pad="K1"/>
<connect gate="B" pin="PVDD_8" pad="P6"/>
<connect gate="B" pin="RCLK1" pad="L2"/>
<connect gate="B" pin="RCLK2" pad="N5"/>
<connect gate="B" pin="RCLK3" pad="N10"/>
<connect gate="B" pin="RCLK4" pad="M13"/>
<connect gate="B" pin="ROUT00" pad="K3"/>
<connect gate="B" pin="ROUT01" pad="K4"/>
<connect gate="B" pin="ROUT02" pad="H3"/>
<connect gate="B" pin="ROUT03" pad="H4"/>
<connect gate="B" pin="ROUT04" pad="H2"/>
<connect gate="B" pin="ROUT10" pad="J3"/>
<connect gate="B" pin="ROUT11" pad="L3"/>
<connect gate="B" pin="ROUT12" pad="J2"/>
<connect gate="B" pin="ROUT13" pad="L1"/>
<connect gate="B" pin="ROUT14" pad="K2"/>
<connect gate="B" pin="ROUT15" pad="M1"/>
<connect gate="B" pin="ROUT16" pad="N1"/>
<connect gate="B" pin="ROUT17" pad="N2"/>
<connect gate="B" pin="ROUT18" pad="M2"/>
<connect gate="B" pin="ROUT19" pad="M3"/>
<connect gate="B" pin="ROUT20" pad="M7"/>
<connect gate="B" pin="ROUT21" pad="L6"/>
<connect gate="B" pin="ROUT22" pad="N6"/>
<connect gate="B" pin="ROUT23" pad="M6"/>
<connect gate="B" pin="ROUT24" pad="P4"/>
<connect gate="B" pin="ROUT25" pad="M5"/>
<connect gate="B" pin="ROUT26" pad="P3"/>
<connect gate="B" pin="ROUT27" pad="N4"/>
<connect gate="B" pin="ROUT28" pad="P2"/>
<connect gate="B" pin="ROUT29" pad="M4"/>
<connect gate="B" pin="ROUT30" pad="M8"/>
<connect gate="B" pin="ROUT31" pad="L8"/>
<connect gate="B" pin="ROUT32" pad="N9"/>
<connect gate="B" pin="ROUT33" pad="M9"/>
<connect gate="B" pin="ROUT34" pad="L9"/>
<connect gate="B" pin="ROUT35" pad="M10"/>
<connect gate="B" pin="ROUT36" pad="M11"/>
<connect gate="B" pin="ROUT37" pad="N11"/>
<connect gate="B" pin="ROUT38" pad="P11"/>
<connect gate="B" pin="ROUT39" pad="N12"/>
<connect gate="B" pin="ROUT40" pad="K13"/>
<connect gate="B" pin="ROUT41" pad="L12"/>
<connect gate="B" pin="ROUT42" pad="L14"/>
<connect gate="B" pin="ROUT43" pad="M14"/>
<connect gate="B" pin="ROUT44" pad="L13"/>
<connect gate="B" pin="ROUT45" pad="L11"/>
<connect gate="B" pin="ROUT46" pad="M12"/>
<connect gate="B" pin="ROUT47" pad="N13"/>
<connect gate="B" pin="ROUT48" pad="N14"/>
<connect gate="B" pin="ROUT49" pad="P14"/>
<connect gate="B" pin="ROUT50" pad="K12"/>
<connect gate="B" pin="ROUT51" pad="J12"/>
<connect gate="B" pin="ROUT52" pad="J11"/>
<connect gate="B" pin="ROUT53" pad="H12"/>
<connect gate="B" pin="ROUT54" pad="H11"/>
<connect gate="B" pin="~LOCK1" pad="P1"/>
<connect gate="B" pin="~LOCK2" pad="N3"/>
<connect gate="B" pin="~LOCK3" pad="P12"/>
<connect gate="B" pin="~LOCK4" pad="P13"/>
</connects>
<technologies>
<technology name="">
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="65K7801"/>
<attribute name="PACKAGE" value="BGA-196"/>
<attribute name="PARTNUMBER" value="SCAN921260UJB"/>
<attribute name="SUPPLIER" value="National Semiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SCANSTA101SM" prefix="U">
<description>STA Master</description>
<gates>
<gate name="A" symbol="SCANSTA101SM"/>
</gates>
<devices>
<device name="" package="BGA49C80P7X7_700X700X150">
<connects>
<connect gate="A" pin="A0" pad="B5"/>
<connect gate="A" pin="A1" pad="C5"/>
<connect gate="A" pin="A2" pad="A7"/>
<connect gate="A" pin="A3" pad="B7"/>
<connect gate="A" pin="A4" pad="B6"/>
<connect gate="A" pin="D0" pad="G6"/>
<connect gate="A" pin="D1" pad="F6"/>
<connect gate="A" pin="D10" pad="F2"/>
<connect gate="A" pin="D11" pad="E1"/>
<connect gate="A" pin="D12" pad="D3"/>
<connect gate="A" pin="D13" pad="C1"/>
<connect gate="A" pin="D14" pad="D2"/>
<connect gate="A" pin="D15" pad="B1"/>
<connect gate="A" pin="D2" pad="G5"/>
<connect gate="A" pin="D3" pad="F5"/>
<connect gate="A" pin="D4" pad="G3"/>
<connect gate="A" pin="D5" pad="F4"/>
<connect gate="A" pin="D6" pad="G2"/>
<connect gate="A" pin="D7" pad="F3"/>
<connect gate="A" pin="D8" pad="G1"/>
<connect gate="A" pin="D9" pad="F1"/>
<connect gate="A" pin="GND" pad="E4"/>
<connect gate="A" pin="GND_2" pad="C4"/>
<connect gate="A" pin="GND_3" pad="E7"/>
<connect gate="A" pin="GND_4" pad="D1"/>
<connect gate="A" pin="INT" pad="C6"/>
<connect gate="A" pin="NC" pad="D4"/>
<connect gate="A" pin="R/~W" pad="C3"/>
<connect gate="A" pin="SCK" pad="E3"/>
<connect gate="A" pin="TCK" pad="B4"/>
<connect gate="A" pin="TCK_SM" pad="F7"/>
<connect gate="A" pin="TDI" pad="A5"/>
<connect gate="A" pin="TDI_SM" pad="G7"/>
<connect gate="A" pin="TDO" pad="B3"/>
<connect gate="A" pin="TDO_SM" pad="E5"/>
<connect gate="A" pin="TMS" pad="A6"/>
<connect gate="A" pin="TMS_SM" pad="E6"/>
<connect gate="A" pin="TRSIT_SM" pad="D7"/>
<connect gate="A" pin="VDD" pad="G4"/>
<connect gate="A" pin="VDD_2" pad="A4"/>
<connect gate="A" pin="VDD_3" pad="D5"/>
<connect gate="A" pin="VDD_4" pad="E2"/>
<connect gate="A" pin="~CE" pad="A1"/>
<connect gate="A" pin="~DTACK" pad="C7"/>
<connect gate="A" pin="~OE" pad="B2"/>
<connect gate="A" pin="~RST" pad="A2"/>
<connect gate="A" pin="~STB" pad="C2"/>
<connect gate="A" pin="~TRST" pad="A3"/>
<connect gate="A" pin="~TRST0_SM" pad="D6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="SCANSTA101SM"/>
<attribute name="OC_FARNELL" value="1685748"/>
<attribute name="OC_NEWARK" value="41K8400"/>
<attribute name="PACKAGE" value="BGA-49"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SCANSTA111MT" prefix="U">
<description>SCAN Bridge</description>
<gates>
<gate name="A" symbol="SCANSTA111MT"/>
</gates>
<devices>
<device name="" package="SOP50P810X110-48N">
<connects>
<connect gate="A" pin="A0" pad="40"/>
<connect gate="A" pin="A1" pad="29"/>
<connect gate="A" pin="AB" pad="9"/>
<connect gate="A" pin="GND" pad="48"/>
<connect gate="A" pin="GND_2" pad="36"/>
<connect gate="A" pin="GND_3" pad="25"/>
<connect gate="A" pin="LSP_ACTIVE1" pad="28"/>
<connect gate="A" pin="LSP_ACTIVE2" pad="22"/>
<connect gate="A" pin="LSP_ACTIVE_0" pad="39"/>
<connect gate="A" pin="S0" pad="12"/>
<connect gate="A" pin="S1" pad="13"/>
<connect gate="A" pin="S2" pad="14"/>
<connect gate="A" pin="S3" pad="15"/>
<connect gate="A" pin="S4" pad="16"/>
<connect gate="A" pin="S5" pad="17"/>
<connect gate="A" pin="S6" pad="18"/>
<connect gate="A" pin="TCK0" pad="46"/>
<connect gate="A" pin="TCK1" pad="37"/>
<connect gate="A" pin="TCK2" pad="26"/>
<connect gate="A" pin="TCKB" pad="3"/>
<connect gate="A" pin="TDI0" pad="44"/>
<connect gate="A" pin="TDI1" pad="33"/>
<connect gate="A" pin="TDI2" pad="19"/>
<connect gate="A" pin="TDIB" pad="5"/>
<connect gate="A" pin="TDO0" pad="43"/>
<connect gate="A" pin="TDO1" pad="32"/>
<connect gate="A" pin="TDO2" pad="20"/>
<connect gate="A" pin="TDOB" pad="6"/>
<connect gate="A" pin="TMS0" pad="45"/>
<connect gate="A" pin="TMS1" pad="34"/>
<connect gate="A" pin="TMS2" pad="23"/>
<connect gate="A" pin="TMSB" pad="4"/>
<connect gate="A" pin="TRIST0" pad="42"/>
<connect gate="A" pin="TRIST1" pad="31"/>
<connect gate="A" pin="TRIST2" pad="21"/>
<connect gate="A" pin="TRISTB" pad="7"/>
<connect gate="A" pin="VCC" pad="35"/>
<connect gate="A" pin="VCC_2" pad="1"/>
<connect gate="A" pin="VCC_3" pad="24"/>
<connect gate="A" pin="Y0" pad="41"/>
<connect gate="A" pin="Y1" pad="30"/>
<connect gate="A" pin="YB" pad="8"/>
<connect gate="A" pin="~OE" pad="10"/>
<connect gate="A" pin="~TEST-~ENABLE" pad="11"/>
<connect gate="A" pin="~TRST0" pad="47"/>
<connect gate="A" pin="~TRST1" pad="38"/>
<connect gate="A" pin="~TRST2" pad="27"/>
<connect gate="A" pin="~TRST~B" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="SCANSTA111MT"/>
<attribute name="OC_FARNELL" value=""/>
<attribute name="OC_NEWARK" value="41J7921"/>
<attribute name="PACKAGE" value="SSOP-48"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SCANSTA112SM" prefix="U">
<description>Multiplexer</description>
<gates>
<gate name="A" symbol="SCANSTA112SM"/>
</gates>
<devices>
<device name="" package="BGA100C80P10X10_1000X1000X150">
<connects>
<connect gate="A" pin="A001" pad="F6"/>
<connect gate="A" pin="A0B0" pad="G5"/>
<connect gate="A" pin="A0B1" pad="F5"/>
<connect gate="A" pin="A101" pad="E10"/>
<connect gate="A" pin="A1B0" pad="H5"/>
<connect gate="A" pin="A1B1" pad="G6"/>
<connect gate="A" pin="ADDMASK" pad="D1"/>
<connect gate="A" pin="GND" pad="J8"/>
<connect gate="A" pin="GND_10" pad="J10"/>
<connect gate="A" pin="GND_2" pad="A6"/>
<connect gate="A" pin="GND_3" pad="G1"/>
<connect gate="A" pin="GND_4" pad="C8"/>
<connect gate="A" pin="GND_5" pad="B3"/>
<connect gate="A" pin="GND_6" pad="B1"/>
<connect gate="A" pin="GND_7" pad="K5"/>
<connect gate="A" pin="GND_8" pad="H3"/>
<connect gate="A" pin="GND_9" pad="D10"/>
<connect gate="A" pin="LSPSEL0" pad="E2"/>
<connect gate="A" pin="LSPSEL1" pad="E5"/>
<connect gate="A" pin="LSPSEL2" pad="F2"/>
<connect gate="A" pin="LSPSEL3" pad="F3"/>
<connect gate="A" pin="LSPSEL4" pad="G2"/>
<connect gate="A" pin="LSPSEL5" pad="H1"/>
<connect gate="A" pin="LSPSEL6" pad="G3"/>
<connect gate="A" pin="MPSELB1/~B0" pad="J1"/>
<connect gate="A" pin="S0" pad="A1"/>
<connect gate="A" pin="S1" pad="B2"/>
<connect gate="A" pin="S2" pad="E4"/>
<connect gate="A" pin="S3" pad="C2"/>
<connect gate="A" pin="S4" pad="D4"/>
<connect gate="A" pin="S5" pad="D3"/>
<connect gate="A" pin="S6" pad="E3"/>
<connect gate="A" pin="S7" pad="C1"/>
<connect gate="A" pin="SB/~S" pad="F4"/>
<connect gate="A" pin="TCK01" pad="F8"/>
<connect gate="A" pin="TCK02" pad="C10"/>
<connect gate="A" pin="TCK03" pad="B8"/>
<connect gate="A" pin="TCK04" pad="A7"/>
<connect gate="A" pin="TCK05" pad="B5"/>
<connect gate="A" pin="TCK06" pad="A2"/>
<connect gate="A" pin="TCKB0" pad="J3"/>
<connect gate="A" pin="TCKB1" pad="J6"/>
<connect gate="A" pin="TDI01" pad="H9"/>
<connect gate="A" pin="TDI02" pad="E9"/>
<connect gate="A" pin="TDI03" pad="E7"/>
<connect gate="A" pin="TDI04" pad="C7"/>
<connect gate="A" pin="TDI05" pad="E6"/>
<connect gate="A" pin="TDI06" pad="B4"/>
<connect gate="A" pin="TDIB0" pad="K1"/>
<connect gate="A" pin="TDIB1" pad="K6"/>
<connect gate="A" pin="TDO01" pad="G7"/>
<connect gate="A" pin="TDO02" pad="E8"/>
<connect gate="A" pin="TDO03" pad="A10"/>
<connect gate="A" pin="TDO04" pad="C6"/>
<connect gate="A" pin="TDO05" pad="B6"/>
<connect gate="A" pin="TDO06" pad="A3"/>
<connect gate="A" pin="TDOB0" pad="J2"/>
<connect gate="A" pin="TDOB1" pad="J5"/>
<connect gate="A" pin="TLRTRST" pad="K10"/>
<connect gate="A" pin="TLRTRST6" pad="J9"/>
<connect gate="A" pin="TMS01" pad="G8"/>
<connect gate="A" pin="TMS02" pad="D9"/>
<connect gate="A" pin="TMS03" pad="B9"/>
<connect gate="A" pin="TMS04" pad="A8"/>
<connect gate="A" pin="TMS05" pad="A5"/>
<connect gate="A" pin="TMS06" pad="C4"/>
<connect gate="A" pin="TMSB0" pad="H4"/>
<connect gate="A" pin="TMSB1" pad="J7"/>
<connect gate="A" pin="TRANS" pad="D2"/>
<connect gate="A" pin="TRIST01" pad="G10"/>
<connect gate="A" pin="TRIST02" pad="B10"/>
<connect gate="A" pin="TRIST03" pad="D7"/>
<connect gate="A" pin="TRISTB0" pad="K3"/>
<connect gate="A" pin="TRISTB1" pad="H7"/>
<connect gate="A" pin="VCC" pad="F10"/>
<connect gate="A" pin="VCC_10" pad="K2"/>
<connect gate="A" pin="VCC_2" pad="A4"/>
<connect gate="A" pin="VCC_3" pad="C9"/>
<connect gate="A" pin="VCC_4" pad="A9"/>
<connect gate="A" pin="VCC_5" pad="E1"/>
<connect gate="A" pin="VCC_6" pad="H8"/>
<connect gate="A" pin="VCC_7" pad="C3"/>
<connect gate="A" pin="VCC_8" pad="K7"/>
<connect gate="A" pin="VCC_9" pad="H2"/>
<connect gate="A" pin="Y001" pad="F9"/>
<connect gate="A" pin="Y0B0" pad="K4"/>
<connect gate="A" pin="Y0B1" pad="K9"/>
<connect gate="A" pin="Y101" pad="G9"/>
<connect gate="A" pin="Y1B0" pad="J4"/>
<connect gate="A" pin="Y1B1" pad="K8"/>
<connect gate="A" pin="~OE" pad="F1"/>
<connect gate="A" pin="~RESET" pad="F7"/>
<connect gate="A" pin="~TRST01" pad="H10"/>
<connect gate="A" pin="~TRST02" pad="D8"/>
<connect gate="A" pin="~TRST03" pad="D6"/>
<connect gate="A" pin="~TRST04" pad="B7"/>
<connect gate="A" pin="~TRST05" pad="C5"/>
<connect gate="A" pin="~TRST06" pad="D5"/>
<connect gate="A" pin="~TRSTB0" pad="G4"/>
<connect gate="A" pin="~TRSTB1" pad="H6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="SCANSTA112SM"/>
<attribute name="OC_FARNELL" value="1685750"/>
<attribute name="OC_NEWARK" value="41K8406"/>
<attribute name="PACKAGE" value="BGA-100"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SCANSTA112VS" prefix="U">
<description>Multiplexer</description>
<gates>
<gate name="A" symbol="SCANSTA112VS"/>
</gates>
<devices>
<device name="" package="QFP50P1600X1600X120-100N">
<connects>
<connect gate="A" pin="A001" pad="66"/>
<connect gate="A" pin="A0B0" pad="29"/>
<connect gate="A" pin="A0B1" pad="41"/>
<connect gate="A" pin="A101" pad="64"/>
<connect gate="A" pin="A1B0" pad="34"/>
<connect gate="A" pin="A1B1" pad="50"/>
<connect gate="A" pin="ADDMASK" pad="11"/>
<connect gate="A" pin="GND" pad="88"/>
<connect gate="A" pin="GND_10" pad="78"/>
<connect gate="A" pin="GND_2" pad="38"/>
<connect gate="A" pin="GND_3" pad="48"/>
<connect gate="A" pin="GND_4" pad="18"/>
<connect gate="A" pin="GND_5" pad="28"/>
<connect gate="A" pin="GND_6" pad="58"/>
<connect gate="A" pin="GND_7" pad="98"/>
<connect gate="A" pin="GND_8" pad="8"/>
<connect gate="A" pin="GND_9" pad="68"/>
<connect gate="A" pin="LSPSEL0" pad="15"/>
<connect gate="A" pin="LSPSEL1" pad="16"/>
<connect gate="A" pin="LSPSEL2" pad="17"/>
<connect gate="A" pin="LSPSEL3" pad="19"/>
<connect gate="A" pin="LSPSEL4" pad="20"/>
<connect gate="A" pin="LSPSEL5" pad="21"/>
<connect gate="A" pin="LSPSEL6" pad="22"/>
<connect gate="A" pin="MPSELB1/~B0" pad="24"/>
<connect gate="A" pin="S0" pad="1"/>
<connect gate="A" pin="S1" pad="2"/>
<connect gate="A" pin="S2" pad="4"/>
<connect gate="A" pin="S3" pad="5"/>
<connect gate="A" pin="S4" pad="6"/>
<connect gate="A" pin="S5" pad="7"/>
<connect gate="A" pin="S6" pad="9"/>
<connect gate="A" pin="S7" pad="10"/>
<connect gate="A" pin="SB/~S" pad="25"/>
<connect gate="A" pin="TCK01" pad="59"/>
<connect gate="A" pin="TCK02" pad="71"/>
<connect gate="A" pin="TCK03" pad="80"/>
<connect gate="A" pin="TCK04" pad="86"/>
<connect gate="A" pin="TCK05" pad="92"/>
<connect gate="A" pin="TCK06" pad="99"/>
<connect gate="A" pin="TCKB0" pad="30"/>
<connect gate="A" pin="TCKB1" pad="42"/>
<connect gate="A" pin="TD005" pad="90"/>
<connect gate="A" pin="TDI01" pad="55"/>
<connect gate="A" pin="TDI02" pad="67"/>
<connect gate="A" pin="TDI03" pad="75"/>
<connect gate="A" pin="TDI04" pad="82"/>
<connect gate="A" pin="TDI05" pad="91"/>
<connect gate="A" pin="TDI06" pad="95"/>
<connect gate="A" pin="TDIB0" pad="26"/>
<connect gate="A" pin="TDIB1" pad="39"/>
<connect gate="A" pin="TDO01" pad="56"/>
<connect gate="A" pin="TDO02" pad="69"/>
<connect gate="A" pin="TDO03" pad="76"/>
<connect gate="A" pin="TDO04" pad="84"/>
<connect gate="A" pin="TDO06" pad="96"/>
<connect gate="A" pin="TDOB0" pad="27"/>
<connect gate="A" pin="TDOB1" pad="40"/>
<connect gate="A" pin="TLR_TRST" pad="51"/>
<connect gate="A" pin="TLR_TRST6" pad="52"/>
<connect gate="A" pin="TMS01" pad="57"/>
<connect gate="A" pin="TMS02" pad="70"/>
<connect gate="A" pin="TMS03" pad="77"/>
<connect gate="A" pin="TMS04" pad="85"/>
<connect gate="A" pin="TMS05" pad="89"/>
<connect gate="A" pin="TMS06" pad="97"/>
<connect gate="A" pin="TMSB0" pad="32"/>
<connect gate="A" pin="TMSB1" pad="45"/>
<connect gate="A" pin="TRANS" pad="12"/>
<connect gate="A" pin="TRIST01" pad="61"/>
<connect gate="A" pin="TRIST02" pad="74"/>
<connect gate="A" pin="TRIST03" pad="81"/>
<connect gate="A" pin="TRISTB0" pad="35"/>
<connect gate="A" pin="TRSITB1" pad="47"/>
<connect gate="A" pin="VCC" pad="13"/>
<connect gate="A" pin="VCC_10" pad="93"/>
<connect gate="A" pin="VCC_2" pad="3"/>
<connect gate="A" pin="VCC_3" pad="83"/>
<connect gate="A" pin="VCC_4" pad="53"/>
<connect gate="A" pin="VCC_5" pad="43"/>
<connect gate="A" pin="VCC_6" pad="23"/>
<connect gate="A" pin="VCC_7" pad="33"/>
<connect gate="A" pin="VCC_8" pad="63"/>
<connect gate="A" pin="VCC_9" pad="73"/>
<connect gate="A" pin="Y001" pad="65"/>
<connect gate="A" pin="Y0B0" pad="36"/>
<connect gate="A" pin="Y0B1" pad="49"/>
<connect gate="A" pin="Y101" pad="62"/>
<connect gate="A" pin="Y1B0" pad="37"/>
<connect gate="A" pin="Y1B1" pad="46"/>
<connect gate="A" pin="~OE" pad="14"/>
<connect gate="A" pin="~RESET" pad="54"/>
<connect gate="A" pin="~TRST02" pad="72"/>
<connect gate="A" pin="~TRST03" pad="79"/>
<connect gate="A" pin="~TRST04" pad="87"/>
<connect gate="A" pin="~TRST05" pad="94"/>
<connect gate="A" pin="~TRST06" pad="100"/>
<connect gate="A" pin="~TRSTB0" pad="31"/>
<connect gate="A" pin="~TRSTB1" pad="44"/>
<connect gate="A" pin="~TRST~01" pad="60"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="SCANSTA112VS"/>
<attribute name="OC_FARNELL" value="1685751"/>
<attribute name="OC_NEWARK" value="41K8408"/>
<attribute name="PACKAGE" value="QFP-100"/>
<attribute name="SUPPLIER" value="TEXAS INSTRUMENTS"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SCANSTA476TSD" prefix="U">
<description>Analog voltage monitor</description>
<gates>
<gate name="A" symbol="SCANSTA476TSD"/>
</gates>
<devices>
<device name="" package="DFN500X500X80-17N">
<connects>
<connect gate="A" pin="A0" pad="16"/>
<connect gate="A" pin="A1" pad="15"/>
<connect gate="A" pin="A2" pad="14"/>
<connect gate="A" pin="A3" pad="13"/>
<connect gate="A" pin="A4" pad="12"/>
<connect gate="A" pin="A5" pad="11"/>
<connect gate="A" pin="A6" pad="10"/>
<connect gate="A" pin="A7" pad="9"/>
<connect gate="A" pin="GND" pad="17"/>
<connect gate="A" pin="TCK" pad="8"/>
<connect gate="A" pin="TDI" pad="6"/>
<connect gate="A" pin="TDO" pad="5"/>
<connect gate="A" pin="TMS" pad="7"/>
<connect gate="A" pin="VDD" pad="1"/>
<connect gate="A" pin="VDD_2" pad="3"/>
<connect gate="A" pin="VREF" pad="2"/>
<connect gate="A" pin="~TRST" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="SCANSTA476TSD"/>
<attribute name="OC_FARNELL" value="1554784"/>
<attribute name="OC_NEWARK" value="94M8821"/>
<attribute name="PACKAGE" value="DFN-16"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TL082CM" prefix="U">
<description>IC OP AMP WIDEBAND JFET</description>
<gates>
<gate name="A" symbol="TL082CM"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="+INA" pad="3"/>
<connect gate="A" pin="+INB" pad="5"/>
<connect gate="A" pin="-INA" pad="2"/>
<connect gate="A" pin="-INB" pad="6"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="TL082CM"/>
<attribute name="OC_FARNELL" value="1564710"/>
<attribute name="OC_NEWARK" value="41K8445"/>
<attribute name="PACKAGE" value="8-SOIC"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TL082CP" prefix="U">
<description>IC OP AMP WIDEBAND JFET</description>
<gates>
<gate name="A" symbol="TL082CP"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-8">
<connects>
<connect gate="A" pin="+INA" pad="3"/>
<connect gate="A" pin="+INB" pad="5"/>
<connect gate="A" pin="-INA" pad="2"/>
<connect gate="A" pin="-INB" pad="6"/>
<connect gate="A" pin="OUTA" pad="1"/>
<connect gate="A" pin="OUTB" pad="7"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="TL082CP"/>
<attribute name="OC_FARNELL" value="1685320"/>
<attribute name="OC_NEWARK" value="41K8447"/>
<attribute name="PACKAGE" value="8-DIP"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM1086IS-3.3" prefix="U">
<description>Low Dropout Positive Regulators</description>
<gates>
<gate name="A" symbol="LM1086IS-3.3"/>
</gates>
<devices>
<device name="" package="TO254P1435X457-4N">
<connects>
<connect gate="A" pin="ADJ/GND" pad="1"/>
<connect gate="A" pin="IN" pad="3"/>
<connect gate="A" pin="OUT" pad="2"/>
<connect gate="A" pin="VOUT" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM1086IS-3.3"/>
<attribute name="OC_FARNELL" value="9490647"/>
<attribute name="OC_NEWARK" value="41K3412"/>
<attribute name="PACKAGE" value="TO-263-3"/>
<attribute name="SUPPLIER" value="TEXAS INSTRUMENTS "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM1086IS-1.8" prefix="U">
<description>Low Dropout Positive Regulators</description>
<gates>
<gate name="A" symbol="LM1086IS-1.8"/>
</gates>
<devices>
<device name="" package="TO254P1435X457-4N">
<connects>
<connect gate="A" pin="ADJ/GND" pad="1"/>
<connect gate="A" pin="IN" pad="3"/>
<connect gate="A" pin="OUT" pad="2"/>
<connect gate="A" pin="VOUT" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM1086IS-1.8"/>
<attribute name="OC_FARNELL" value="9490639"/>
<attribute name="OC_NEWARK" value="38K3613"/>
<attribute name="PACKAGE" value="TO-263-3"/>
<attribute name="SUPPLIER" value="TEXAS INSTRUMENTS "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM1086CS-ADJ" prefix="U">
<description>Low Dropout Positive Regulators</description>
<gates>
<gate name="A" symbol="LM1086CS-ADJ"/>
</gates>
<devices>
<device name="" package="TO254P1435X457-4N">
<connects>
<connect gate="A" pin="ADJ/GND" pad="1"/>
<connect gate="A" pin="IN" pad="3"/>
<connect gate="A" pin="OUT" pad="2"/>
<connect gate="A" pin="VOUT" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM1086CS-ADJ"/>
<attribute name="OC_FARNELL" value="9489975"/>
<attribute name="OC_NEWARK" value="41K3383 "/>
<attribute name="PACKAGE" value="TO-263-3"/>
<attribute name="SUPPLIER" value="TEXAS INSTRUMENTS "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM1086IS-5.0" prefix="U">
<description>Low Dropout Positive Regulators</description>
<gates>
<gate name="A" symbol="LM1086IS-5.0"/>
</gates>
<devices>
<device name="" package="TO254P1435X457-4N">
<connects>
<connect gate="A" pin="ADJ/GND" pad="1"/>
<connect gate="A" pin="IN" pad="3"/>
<connect gate="A" pin="OUT" pad="2"/>
<connect gate="A" pin="VOUT" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM1086IS-5.0"/>
<attribute name="OC_FARNELL" value="9490655"/>
<attribute name="OC_NEWARK" value="41K3414"/>
<attribute name="PACKAGE" value="TO-263-3"/>
<attribute name="SUPPLIER" value="TEXAS INSTRUMENTS "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM1086CS-3.3" prefix="U">
<description>Low Dropout Positive Regulators</description>
<gates>
<gate name="A" symbol="LM1086CS-3.3"/>
</gates>
<devices>
<device name="" package="TO254P1435X457-4N">
<connects>
<connect gate="A" pin="ADJ/GND" pad="1"/>
<connect gate="A" pin="IN" pad="3"/>
<connect gate="A" pin="OUT" pad="2"/>
<connect gate="A" pin="VOUT" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM1086CS-3.3"/>
<attribute name="OC_FARNELL" value="9489959 "/>
<attribute name="OC_NEWARK" value="41K3386"/>
<attribute name="PACKAGE" value="TO-263-3"/>
<attribute name="SUPPLIER" value="TEXAS INSTRUMENTS "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
