<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.2.0">
<drawing>
<library>
<description>&lt;h3&gt;GeekAmmo  Library&lt;/h3&gt;

These are parts used by the GeekAmmo company (now part of SparkFun Electronics)!

 If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt;Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SOT23-3">
</package>
<package name="06X1-PTH">
<description>6x 0.1in Pin Header Octagon Shape</description>
</package>
<package name="FIDUCIAL">
</package>
<package name="7914G">
<description>&lt;b&gt;Bourns 7914G 4 mm SMD Sealed Key Switch&lt;/b&gt;
&lt;br/&gt;
&lt;br/&gt;
http://www.bourns.com/data/global/pdfs/7914.pdf</description>
</package>
<package name="USB-MALE-A-PCB">
<description>&lt;b&gt;USB Male A for direct PCB&lt;/b&gt;</description>
</package>
<package name="MC331XX">
<description>MC331XX Footprint for MULTICOMP PTC
&lt;br&gt;
&lt;br&gt;
WARNING: Not compatible with other 1812 PTC footprint.</description>
</package>
<package name="S0-28W">
<description>&lt;B&gt;28-Lead Plastic Small Outline (SO) &lt;/B&gt; Wide, 300 mil Body (SOIC)&lt;/B&gt;
&lt;p&gt;Source: &lt;a href="http://ww1.microchip.com/downloads/en/PackagingSpec/00049BF.pdf"&gt;http://ww1.microchip.com/downloads/en/PackagingSpec/00049BF.pdf&lt;/a&gt;&lt;/p&gt;</description>
</package>
<package name="13X2-PTH">
<description>13x2 Pin Header Male or Female</description>
</package>
<package name="20X1-PTH">
</package>
<package name="LCD16X2-RGB">
<description>GeekAmmo LCD 16x2 RGB / MONO</description>
</package>
<package name="TAC-SWITCH-PTH">
</package>
<package name="RTRIM3362P">
<description>Bourns 3362P</description>
</package>
<package name="SOT23-5">
<description>&lt;b&gt;SOT23-5&lt;/b&gt;</description>
</package>
<package name="SOT23-8">
<description>&lt;b&gt;SOT23-8&lt;/b&gt;</description>
</package>
<package name="SOT23-6">
<description>&lt;b&gt;SOT23-6&lt;/b&gt;</description>
</package>
<package name="SSOP-28">
<description>&lt;b&gt;SSOP 28&lt;/b&gt;</description>
</package>
<package name="USB-MICRO-MOLEX-105017-0001">
<description>&lt;b&gt; Molex Micro USB 105017-0001&lt;/b&gt;</description>
</package>
<package name="RFD22301">
<description>&lt;b&gt;RFD22301 Core of RFDuino&lt;/b&gt;</description>
</package>
</packages>
<symbols>
<symbol name="N-CHANNEL-MOSFET">
<pin name="D" direction="pas"/>
<pin name="S" direction="pas"/>
<pin name="G" direction="pas"/>
</symbol>
<symbol name="FRAME1-A4">
</symbol>
<symbol name="DOCFIELD1">
</symbol>
<symbol name="06X1">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="FIDUCIAL">
</symbol>
<symbol name="TACTILE-SWITCH">
<pin name="1" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="FRAME2-A4">
</symbol>
<symbol name="DOCFIELD2">
</symbol>
<symbol name="USB-4PIN">
<pin name="VBUS" direction="pwr"/>
<pin name="D-"/>
<pin name="D+"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="P-CHANNEL-MOSFET">
<pin name="D" direction="pas"/>
<pin name="S" direction="pas"/>
<pin name="G" direction="pas"/>
</symbol>
<symbol name="PTC">
<pin name="1"/>
<pin name="2"/>
</symbol>
<symbol name="PIC18F2550_28">
<pin name="RC7/RX/DT/SDO"/>
<pin name="VSS" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="RB0/AN12/INT0/LFT0/SDI/SDA"/>
<pin name="RB1/AN10/INT1/SCK/SCL"/>
<pin name="RB2/AN8/INT2/VMO"/>
<pin name="RB3/AN9/CCP2/VPO"/>
<pin name="RB4/AN11/KBI0/CSSPP"/>
<pin name="RB5/KBI1/PGM"/>
<pin name="RB6/KBI2/PGC"/>
<pin name="RB7/BKI3/PGD"/>
<pin name="!MCLR!/VPP/RE3" direction="in"/>
<pin name="RA0/AN0"/>
<pin name="RA1/AN1"/>
<pin name="RA2/AN2/VREF-/CVREF"/>
<pin name="RA3/AN3/VREF+"/>
<pin name="RA4/T0CKI/CIOUT/RCV"/>
<pin name="RA5/AN4/!SS!/HLVDIN/C2OUT"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="OSC1/CLKI" direction="in"/>
<pin name="RA6/OSC2/CLKO" direction="out"/>
<pin name="RC0/TIOSO/T13CKI"/>
<pin name="RC1/T1OSI/ICCP2/!UOE"/>
<pin name="RC2/CCP1/P1A"/>
<pin name="VUSB"/>
<pin name="RC4/D-/VM"/>
<pin name="RC5/D+/VP"/>
<pin name="RC6/TX/CK"/>
</symbol>
<symbol name="PI-IO">
<pin name="3.3V@1" direction="pwr"/>
<pin name="5V@1" direction="pwr"/>
<pin name="GPIO0/2/SDA"/>
<pin name="5V@2" direction="pwr"/>
<pin name="GPIO1/3/SCL"/>
<pin name="GND@3"/>
<pin name="GPIO4"/>
<pin name="GPIO14/TXD"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GPIO15/RXD"/>
<pin name="GPIO17"/>
<pin name="GPIO18"/>
<pin name="GPIO21/27"/>
<pin name="GND@4" direction="pwr"/>
<pin name="GPIO22"/>
<pin name="GPIO23"/>
<pin name="3.3V@2" direction="pwr"/>
<pin name="GPIO24"/>
<pin name="GPIO10/MOSI"/>
<pin name="GND@5" direction="pwr"/>
<pin name="GPIO9/MISO"/>
<pin name="GPIO25"/>
<pin name="GPIO11/SCLK"/>
<pin name="GPIO8/CE0"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GPIO7/CE1"/>
</symbol>
<symbol name="LCD16X2-RGB">
<pin name="VSS"/>
<pin name="VDD"/>
<pin name="VO"/>
<pin name="RS"/>
<pin name="R/W"/>
<pin name="!E!"/>
<pin name="DB0"/>
<pin name="DB1"/>
<pin name="DB2"/>
<pin name="DB3"/>
<pin name="DB4"/>
<pin name="DB5"/>
<pin name="DB6"/>
<pin name="DB7"/>
<pin name="ANODE"/>
<pin name="RED"/>
<pin name="GREEN"/>
<pin name="BLUE"/>
</symbol>
<symbol name="RTRIM">
<pin name="1" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="MCP73831">
<pin name="VDD" direction="pwr"/>
<pin name="STAT" direction="out"/>
<pin name="VBAT" direction="pwr"/>
<pin name="PROG" direction="in"/>
<pin name="VSS" direction="pwr"/>
</symbol>
<symbol name="LTC2954">
<pin name="VIN" direction="pwr"/>
<pin name="!PB!" direction="pas"/>
<pin name="GND" direction="pwr"/>
<pin name="ONT" direction="pas"/>
<pin name="PDT" direction="pas"/>
<pin name="!KILL!" direction="in"/>
<pin name="!INT!" direction="out"/>
<pin name="EN/!EN!" direction="out"/>
</symbol>
<symbol name="MCP1640">
<pin name="VIN" direction="pwr"/>
<pin name="EN" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="VFB" direction="in"/>
<pin name="VOUT" direction="pwr"/>
<pin name="SW" direction="pas"/>
</symbol>
<symbol name="FT232R">
<pin name="RESET" direction="in"/>
<pin name="OSCI" direction="in"/>
<pin name="OSCO" direction="out"/>
<pin name="DSR" direction="in"/>
<pin name="DCD" direction="in"/>
<pin name="RI" direction="in"/>
<pin name="3V3OUT" direction="out"/>
<pin name="USBDM"/>
<pin name="USBDP"/>
<pin name="GND@7" direction="pwr"/>
<pin name="GND@18" direction="pwr"/>
<pin name="GND@21" direction="pwr"/>
<pin name="TXD" direction="out"/>
<pin name="RXD" direction="in"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="AGND" direction="pwr"/>
<pin name="TEST" direction="in"/>
<pin name="VCC" direction="pwr"/>
<pin name="CBUS0" direction="in"/>
<pin name="CBUS1" direction="in"/>
<pin name="RTS" direction="out"/>
<pin name="CTS" direction="in"/>
<pin name="DTR" direction="out"/>
<pin name="CBUS3" direction="in"/>
<pin name="CBUS2" direction="in"/>
<pin name="CBUS4" direction="in"/>
</symbol>
<symbol name="USB-5PIN">
<pin name="VBUS" direction="pwr"/>
<pin name="D-"/>
<pin name="D+"/>
<pin name="GND" direction="pwr"/>
<pin name="ID"/>
</symbol>
<symbol name="RFD22301">
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GPIO2"/>
<pin name="GPIO3"/>
<pin name="GPIO4"/>
<pin name="GPIO5"/>
<pin name="GPIO6"/>
<pin name="GND@8" direction="pwr"/>
<pin name="GND@9" direction="pwr"/>
<pin name="GND@10" direction="pwr"/>
<pin name="EXTANT"/>
<pin name="GND@12" direction="pwr"/>
<pin name="3V"/>
<pin name="RESET"/>
<pin name="FACT"/>
<pin name="GPIO0/AREF"/>
<pin name="GPIO1"/>
<pin name="GND@18" direction="pwr"/>
<pin name="GND@19" direction="pwr"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="N-CHANNEL-MOSFET">
<description>N-Channel MOSFET Mode Field Effect Transistor</description>
<gates>
<gate name="G$1" symbol="N-CHANNEL-MOSFET"/>
</gates>
<devices>
<device name="-BSS138" package="SOT23-3">
<connects>
<connect gate="G$1" pin="D" pad="3"/>
<connect gate="G$1" pin="G" pad="1"/>
<connect gate="G$1" pin="S" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET" value="http://www.fairchildsemi.com/ds/BS/BSS138.pdf"/>
<attribute name="DIGIKEY" value="BSS138TR-ND"/>
<attribute name="ELEMENT14" value="2323154"/>
<attribute name="OTHER" value=""/>
<attribute name="URL" value="http://au.element14.com/fairchild-semiconductor/bss138/mosfet-n-ch-50v-220ma-sot-23/dp/2323154"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FRAME1-A4">
<description>&lt;b&gt;FRAME TYPE 1 - A4&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="FRAME1-A4"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DOCFIELD1">
<description>&lt;b&gt;DOCUMENT FIELDS TYPE 1&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="DOCFIELD1"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HEADER-06X1?">
<description>&lt;b&gt;6 x 0.1 inch Header&lt;/b&gt;
&lt;p&gt;40x1 0.1inch Male Breakaway header can be used.&lt;br&gt;
- &lt;a href="http://www.4uconnector.com/online/SearchPro.asp?FormName=ProSearch&amp;FormAction=search&amp;s_GroupNo=&amp;s_keyword=00834"&gt;4UCON 00834&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;For female part, if possible use 6 x 1 without breaking.&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="06X1"/>
</gates>
<devices>
<device name="-MALE" package="06X1-PTH">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DIGIKEY" value=""/>
<attribute name="ELEMENT14" value=""/>
<attribute name="OTHER" value="4UCON 00834"/>
<attribute name="URL" value="http://www.4uconnector.com/online/SearchPro.asp?FormName=ProSearch&amp;FormAction=search&amp;s_GroupNo=&amp;s_keyword=00834"/>
</technology>
</technologies>
</device>
<device name="-FEMALE" package="06X1-PTH">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FIDUCIAL">
<gates>
<gate name="G$1" symbol="FIDUCIAL"/>
</gates>
<devices>
<device name="" package="FIDUCIAL">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TACTILE-SWITCH">
<description>&lt;B&gt;Tactile Switch 4 Pins, SPST NO&lt;/B&gt;</description>
<gates>
<gate name="G$1" symbol="TACTILE-SWITCH"/>
</gates>
<devices>
<device name="-7914G" package="7914G">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-PTH" package="TAC-SWITCH-PTH">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FRAME2-A4">
<description>&lt;b&gt;FRAME TYPE 2 - A4&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="FRAME2-A4"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DOCFIELD2">
<description>&lt;b&gt;DOCUMENT FIELDS TYPE 2&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="DOCFIELD2"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="USB-CON-4PIN">
<description>&lt;b&gt;USB Connector 4 Pin - No SHIELD&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="USB-4PIN"/>
</gates>
<devices>
<device name="" package="USB-MALE-A-PCB">
<connects>
<connect gate="G$1" pin="D+" pad="3"/>
<connect gate="G$1" pin="D-" pad="2"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="VBUS" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="P-CHANNEL-MOSFET">
<description>P-Channel MOSFET Mode Field Effect Transistor</description>
<gates>
<gate name="G$1" symbol="P-CHANNEL-MOSFET"/>
</gates>
<devices>
<device name="" package="SOT23-3">
<connects>
<connect gate="G$1" pin="D" pad="3"/>
<connect gate="G$1" pin="G" pad="1"/>
<connect gate="G$1" pin="S" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PTC">
<description>PTC Resettable Fuse</description>
<gates>
<gate name="G$1" symbol="PTC"/>
</gates>
<devices>
<device name="" package="MC331XX">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC18F2*_28">
<description>&lt;b&gt;USB Microcontrollers with nanoWatt Technology&lt;/b&gt; High-Performance, Enhanced Flash, 28/40/44-Pin, &lt;p&gt;
Source: http://ww1.microchip.com/downloads/en/devicedoc/39632c.pdf</description>
<gates>
<gate name="G$1" symbol="PIC18F2550_28"/>
</gates>
<devices>
<device name="" package="S0-28W">
<connects>
<connect gate="G$1" pin="!MCLR!/VPP/RE3" pad="1"/>
<connect gate="G$1" pin="OSC1/CLKI" pad="9"/>
<connect gate="G$1" pin="RA0/AN0" pad="2"/>
<connect gate="G$1" pin="RA1/AN1" pad="3"/>
<connect gate="G$1" pin="RA2/AN2/VREF-/CVREF" pad="4"/>
<connect gate="G$1" pin="RA3/AN3/VREF+" pad="5"/>
<connect gate="G$1" pin="RA4/T0CKI/CIOUT/RCV" pad="6"/>
<connect gate="G$1" pin="RA5/AN4/!SS!/HLVDIN/C2OUT" pad="7"/>
<connect gate="G$1" pin="RA6/OSC2/CLKO" pad="10"/>
<connect gate="G$1" pin="RB0/AN12/INT0/LFT0/SDI/SDA" pad="21"/>
<connect gate="G$1" pin="RB1/AN10/INT1/SCK/SCL" pad="22"/>
<connect gate="G$1" pin="RB2/AN8/INT2/VMO" pad="23"/>
<connect gate="G$1" pin="RB3/AN9/CCP2/VPO" pad="24"/>
<connect gate="G$1" pin="RB4/AN11/KBI0/CSSPP" pad="25"/>
<connect gate="G$1" pin="RB5/KBI1/PGM" pad="26"/>
<connect gate="G$1" pin="RB6/KBI2/PGC" pad="27"/>
<connect gate="G$1" pin="RB7/BKI3/PGD" pad="28"/>
<connect gate="G$1" pin="RC0/TIOSO/T13CKI" pad="11"/>
<connect gate="G$1" pin="RC1/T1OSI/ICCP2/!UOE" pad="12"/>
<connect gate="G$1" pin="RC2/CCP1/P1A" pad="13"/>
<connect gate="G$1" pin="RC4/D-/VM" pad="15"/>
<connect gate="G$1" pin="RC5/D+/VP" pad="16"/>
<connect gate="G$1" pin="RC6/TX/CK" pad="17"/>
<connect gate="G$1" pin="RC7/RX/DT/SDO" pad="18"/>
<connect gate="G$1" pin="VDD" pad="20"/>
<connect gate="G$1" pin="VSS" pad="8"/>
<connect gate="G$1" pin="VSS@1" pad="19"/>
<connect gate="G$1" pin="VUSB" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PI-IO">
<description>Raspberry Pi IO connector</description>
<gates>
<gate name="G$1" symbol="PI-IO"/>
</gates>
<devices>
<device name="" package="13X2-PTH">
<connects>
<connect gate="G$1" pin="3.3V@1" pad="1"/>
<connect gate="G$1" pin="3.3V@2" pad="17"/>
<connect gate="G$1" pin="5V@1" pad="2"/>
<connect gate="G$1" pin="5V@2" pad="4"/>
<connect gate="G$1" pin="GND@1" pad="9"/>
<connect gate="G$1" pin="GND@2" pad="25"/>
<connect gate="G$1" pin="GND@3" pad="6"/>
<connect gate="G$1" pin="GND@4" pad="14"/>
<connect gate="G$1" pin="GND@5" pad="20"/>
<connect gate="G$1" pin="GPIO0/2/SDA" pad="3"/>
<connect gate="G$1" pin="GPIO1/3/SCL" pad="5"/>
<connect gate="G$1" pin="GPIO10/MOSI" pad="19"/>
<connect gate="G$1" pin="GPIO11/SCLK" pad="23"/>
<connect gate="G$1" pin="GPIO14/TXD" pad="8"/>
<connect gate="G$1" pin="GPIO15/RXD" pad="10"/>
<connect gate="G$1" pin="GPIO17" pad="11"/>
<connect gate="G$1" pin="GPIO18" pad="12"/>
<connect gate="G$1" pin="GPIO21/27" pad="13"/>
<connect gate="G$1" pin="GPIO22" pad="15"/>
<connect gate="G$1" pin="GPIO23" pad="16"/>
<connect gate="G$1" pin="GPIO24" pad="18"/>
<connect gate="G$1" pin="GPIO25" pad="22"/>
<connect gate="G$1" pin="GPIO4" pad="7"/>
<connect gate="G$1" pin="GPIO7/CE1" pad="26"/>
<connect gate="G$1" pin="GPIO8/CE0" pad="24"/>
<connect gate="G$1" pin="GPIO9/MISO" pad="21"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LCD16X2-RGB">
<description>&lt;b&gt;GeekAmmo LCD 16x2 RGB&lt;/b&gt;&lt;br/&gt;
GMO-00056 Negative&lt;br/&gt;
GMO-00057 Positive&lt;br/&gt;</description>
<gates>
<gate name="G$1" symbol="LCD16X2-RGB"/>
</gates>
<devices>
<device name="" package="LCD16X2-RGB">
<connects>
<connect gate="G$1" pin="!E!" pad="6"/>
<connect gate="G$1" pin="ANODE" pad="15"/>
<connect gate="G$1" pin="BLUE" pad="18"/>
<connect gate="G$1" pin="DB0" pad="7"/>
<connect gate="G$1" pin="DB1" pad="8"/>
<connect gate="G$1" pin="DB2" pad="9"/>
<connect gate="G$1" pin="DB3" pad="10"/>
<connect gate="G$1" pin="DB4" pad="11"/>
<connect gate="G$1" pin="DB5" pad="12"/>
<connect gate="G$1" pin="DB6" pad="13"/>
<connect gate="G$1" pin="DB7" pad="14"/>
<connect gate="G$1" pin="GREEN" pad="17"/>
<connect gate="G$1" pin="R/W" pad="5"/>
<connect gate="G$1" pin="RED" pad="16"/>
<connect gate="G$1" pin="RS" pad="4"/>
<connect gate="G$1" pin="VDD" pad="2"/>
<connect gate="G$1" pin="VO" pad="3"/>
<connect gate="G$1" pin="VSS" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RTRIM">
<description>&lt;b&gt;BOURNS 3362 - 1/4" Square Trimpot® Trimming Potentiometer&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="RTRIM"/>
</gates>
<devices>
<device name="-3362P" package="RTRIM3362P">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MCP73831">
<description>&lt;b&gt;MCP73831 Miniature Single-Cell, Fully Integrated Li-Ion, Li-Polymer Charge Management Controllers&lt;/b&gt;
&lt;p&gt;The MCP73831/2 devices are highly advanced linear charge management controllers for use in spacelimited, cost-sensitive applications.&lt;/p&gt;
&lt;p&gt;&lt;a href="http://ww1.microchip.com/downloads/en/DeviceDoc/20001984F.pdf"&gt;http://ww1.microchip.com/downloads/en/DeviceDoc/20001984F.pdf&lt;/a&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="MCP73831"/>
</gates>
<devices>
<device name="" package="SOT23-5">
<connects>
<connect gate="G$1" pin="PROG" pad="5"/>
<connect gate="G$1" pin="STAT" pad="1"/>
<connect gate="G$1" pin="VBAT" pad="3"/>
<connect gate="G$1" pin="VDD" pad="4"/>
<connect gate="G$1" pin="VSS" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LTC2954">
<description>&lt;b&gt;LTC2954 Push Button On/Off Controller with uP Interrupt&lt;/b&gt;
&lt;p&gt;
The LTC®2954 is a pushbutton on/off controller that manages system power via a pushbutton interface. &lt;/p&gt;
&lt;p&gt;&lt;a href="http://www.linear.com/docs/16598"&gt;http://www.linear.com/docs/16598&lt;/a&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="LTC2954"/>
</gates>
<devices>
<device name="" package="SOT23-8">
<connects>
<connect gate="G$1" pin="!INT!" pad="5"/>
<connect gate="G$1" pin="!KILL!" pad="8"/>
<connect gate="G$1" pin="!PB!" pad="2"/>
<connect gate="G$1" pin="EN/!EN!" pad="6"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="ONT" pad="3"/>
<connect gate="G$1" pin="PDT" pad="7"/>
<connect gate="G$1" pin="VIN" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MCP1640">
<description>&lt;b&gt;MCP1640 0.65V Start-up Synchronous Boost Regulator with True Output Disconnect or Input/Output Bypass Option&lt;/b&gt;
&lt;p&gt;The MCP1640/B/C/D is a compact, high-efficiency, fixed frequency, synchronous step-up DC-DC converter.&lt;/p&gt;
&lt;p&gt;&lt;a href="http://ww1.microchip.com/downloads/en/DeviceDoc/22234B.pdf"&gt;http://ww1.microchip.com/downloads/en/DeviceDoc/22234B.pdf&lt;/a&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="MCP1640"/>
</gates>
<devices>
<device name="" package="SOT23-6">
<connects>
<connect gate="G$1" pin="EN" pad="3"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="SW" pad="1"/>
<connect gate="G$1" pin="VFB" pad="4"/>
<connect gate="G$1" pin="VIN" pad="6"/>
<connect gate="G$1" pin="VOUT" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FT232R">
<description>&lt;b&gt;FT232R USB UART IC&lt;/b&gt;
&lt;p&gt;The  FT232R  is  a  USB  to  serial  UART interface  with advanced features.&lt;/p&gt;
&lt;p&gt;&lt;a href="http://www.ftdichip.com/Support/Documents/DataSheets/ICs/DS_FT232R.pdf"&gt;http://www.ftdichip.com/Support/Documents/DataSheets/ICs/DS_FT232R.pdf&lt;/a&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="FT232R"/>
</gates>
<devices>
<device name="" package="SSOP-28">
<connects>
<connect gate="G$1" pin="3V3OUT" pad="17"/>
<connect gate="G$1" pin="AGND" pad="25"/>
<connect gate="G$1" pin="CBUS0" pad="23"/>
<connect gate="G$1" pin="CBUS1" pad="22"/>
<connect gate="G$1" pin="CBUS2" pad="13"/>
<connect gate="G$1" pin="CBUS3" pad="14"/>
<connect gate="G$1" pin="CBUS4" pad="12"/>
<connect gate="G$1" pin="CTS" pad="11"/>
<connect gate="G$1" pin="DCD" pad="10"/>
<connect gate="G$1" pin="DSR" pad="9"/>
<connect gate="G$1" pin="DTR" pad="2"/>
<connect gate="G$1" pin="GND@18" pad="18"/>
<connect gate="G$1" pin="GND@21" pad="21"/>
<connect gate="G$1" pin="GND@7" pad="7"/>
<connect gate="G$1" pin="OSCI" pad="27"/>
<connect gate="G$1" pin="OSCO" pad="28"/>
<connect gate="G$1" pin="RESET" pad="19"/>
<connect gate="G$1" pin="RI" pad="6"/>
<connect gate="G$1" pin="RTS" pad="3"/>
<connect gate="G$1" pin="RXD" pad="5"/>
<connect gate="G$1" pin="TEST" pad="26"/>
<connect gate="G$1" pin="TXD" pad="1"/>
<connect gate="G$1" pin="USBDM" pad="16"/>
<connect gate="G$1" pin="USBDP" pad="15"/>
<connect gate="G$1" pin="VCC" pad="20"/>
<connect gate="G$1" pin="VCCIO" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="USB-CON-5PIN">
<description>&lt;b&gt; Molex Micro USB 105017-0001&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="USB-5PIN"/>
</gates>
<devices>
<device name="-105017-0001" package="USB-MICRO-MOLEX-105017-0001">
<connects>
<connect gate="G$1" pin="D+" pad="3"/>
<connect gate="G$1" pin="D-" pad="2"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="ID" pad="4"/>
<connect gate="G$1" pin="VBUS" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RF22301">
<description>&lt;b&gt;RFD22301 RFDuino Bluetooth 4.0 Low Energy BLE RF Module
With Built-In ARM Cortex M0 Microconroller&lt;/b&gt;
&lt;p&gt;Hi performance, professional grade Bluetooth 4.0 
Low Energy radio transceiver with built-in ARM 
Cortex M0 microcontroller that can be 
programmed using the simple-to-use
Arduino IDE using RFduino extensions.
Built-in user application microcontroller with 
ADC, I2C, SPI, UART and GPIO.&lt;/p&gt;
&lt;p&gt;&lt;a href="http://www.rfduino.com/"&gt;http://www.rfduino.com/&lt;/a&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="RFD22301"/>
</gates>
<devices>
<device name="" package="RFD22301">
<connects>
<connect gate="G$1" pin="3V" pad="13"/>
<connect gate="G$1" pin="EXTANT" pad="11"/>
<connect gate="G$1" pin="FACT" pad="15"/>
<connect gate="G$1" pin="GND@1" pad="1"/>
<connect gate="G$1" pin="GND@10" pad="10"/>
<connect gate="G$1" pin="GND@12" pad="12"/>
<connect gate="G$1" pin="GND@18" pad="18"/>
<connect gate="G$1" pin="GND@19" pad="19"/>
<connect gate="G$1" pin="GND@2" pad="2"/>
<connect gate="G$1" pin="GND@8" pad="8"/>
<connect gate="G$1" pin="GND@9" pad="9"/>
<connect gate="G$1" pin="GPIO0/AREF" pad="16"/>
<connect gate="G$1" pin="GPIO1" pad="17"/>
<connect gate="G$1" pin="GPIO2" pad="3"/>
<connect gate="G$1" pin="GPIO3" pad="4"/>
<connect gate="G$1" pin="GPIO4" pad="5"/>
<connect gate="G$1" pin="GPIO5" pad="6"/>
<connect gate="G$1" pin="GPIO6" pad="7"/>
<connect gate="G$1" pin="RESET" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
