<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.6.0">
<drawing>
<library>
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find all manner of analog ICs- DACs, ADCs, video chips, op-amps, and others.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt;Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SO08">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt; Fits JEDEC packages (narrow SOIC-8)</description>
</package>
<package name="SO16L">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt; .300 SIOC&lt;p&gt;
Source: http://www.maxim-ic.com/cgi-bin/packages?pkg=16%2FSOIC%2E300&amp;Type=Max</description>
</package>
<package name="TSSOP20">
</package>
<package name="TSSOP16">
<description>&lt;b&gt;TSOP16&lt;/b&gt;&lt;p&gt;
thin small outline package</description>
</package>
<package name="SOIC-14">
</package>
<package name="TSSOP-16">
</package>
<package name="SO08-EPAD">
</package>
<package name="ALM-1412">
</package>
<package name="QFN-24_ALT2">
<description>&lt;h3&gt;24-pin QFN with Exposed Thermal pad&lt;/h3&gt;
Parts that use this package:
&lt;ul&gt;
&lt;li&gt;A6282&lt;/li&gt;
&lt;/ul&gt;
Last modified: 8/20/10&lt;br&gt;
&lt;br&gt;
&lt;b&gt;***UNPROVEN***&lt;/b&gt;&lt;BR&gt;</description>
</package>
<package name="SOT23-6">
</package>
<package name="DIL18">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="DIP08">
<description>&lt;b&gt;Dual In Line&lt;/b&gt;</description>
</package>
<package name="SO014">
</package>
<package name="MSOP8">
<description>&lt;b&gt;8M, 8-Lead, 0.118" Wide, Miniature Small Outline Package&lt;/b&gt;&lt;p&gt;
MSOP&lt;br&gt;
8M-Package doc1097.pdf</description>
</package>
<package name="SO08-MAX6675">
<description>&lt;b&gt;SMALL OUTLINE INTEGRATED CIRCUIT&lt;/b&gt;&lt;p&gt;
body 3.9 mm/JEDEC MS-012AA</description>
</package>
<package name="SOIC8">
</package>
<package name="SSOP24">
</package>
<package name="SO16">
<description>&lt;b&gt;Small Outline package&lt;/b&gt; 150 mil</description>
</package>
<package name="DIL-08">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="SOT23-5">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;</description>
</package>
<package name="SSOP20">
<description>&lt;b&gt;Shrink Small Outline Package&lt;/b&gt;&lt;p&gt;
package type SS</description>
</package>
<package name="TVSOP-16">
</package>
<package name="TQFP32-5MM">
</package>
<package name="DIL16">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="DIL14">
</package>
<package name="TSSOP-14">
</package>
<package name="POWER-SOP8">
<description>&lt;b&gt;8M, 8-Lead, 0.118" Wide, Miniature Small Outline Package&lt;/b&gt;&lt;p&gt;
MSOP&lt;br&gt;
8M-Package doc1097.pdf</description>
</package>
<package name="QFN-8_PAD">
</package>
<package name="DIP08-KIT">
</package>
<package name="AD9837">
</package>
<package name="SO08-TIGHT">
</package>
<package name="DIL14-KIT">
</package>
<package name="QFN-10-RSE">
</package>
<package name="LFCSP_20">
</package>
<package name="MSOP10">
<description>&lt;b&gt;10 Lead Platic MSOP&lt;/b&gt;&lt;p&gt;
Source: http://www.linear.com .. LT1996</description>
</package>
<package name="SSOP16">
</package>
<package name="SO08-UNIVERSAL">
<description>SOIC-08 footprint wth long lands.&lt;br&gt;

To fit both narrow and wide SOICs - for SOIC-to-DIP adapter board.
&lt;br&gt;&lt;br&gt;
Not recommended if you're trying to fit a specific chip.</description>
</package>
<package name="TO-92">
</package>
</packages>
<symbols>
<symbol name="ACS712">
<pin name="IP+@1"/>
<pin name="IP+@2"/>
<pin name="IP-@3"/>
<pin name="IP-@4"/>
<pin name="GND"/>
<pin name="FILT"/>
<pin name="VOUT"/>
<pin name="VCC"/>
</symbol>
<symbol name="AD725">
<pin name="STND"/>
<pin name="AGND"/>
<pin name="4FSC"/>
<pin name="APOS"/>
<pin name="CE"/>
<pin name="RIN"/>
<pin name="GIN"/>
<pin name="BIN"/>
<pin name="HSYNC"/>
<pin name="VSYNC"/>
<pin name="DPOS"/>
<pin name="DGND"/>
<pin name="YTRAP"/>
<pin name="LUMA"/>
<pin name="COMP"/>
<pin name="CRMA"/>
</symbol>
<symbol name="AD5330">
<pin name="VDD"/>
<pin name="VREF"/>
<pin name="CS"/>
<pin name="DB0"/>
<pin name="DB1"/>
<pin name="DB2"/>
<pin name="DB3"/>
<pin name="DB4"/>
<pin name="DB5"/>
<pin name="DB6"/>
<pin name="DB7"/>
<pin name="WR"/>
<pin name="CLR"/>
<pin name="PD"/>
<pin name="GND"/>
<pin name="VOUT"/>
<pin name="LDAC"/>
<pin name="GAIN"/>
<pin name="BUF"/>
</symbol>
<symbol name="AD7302">
<pin name="DB7"/>
<pin name="DB6"/>
<pin name="DB5"/>
<pin name="DB4"/>
<pin name="DB3"/>
<pin name="DB2"/>
<pin name="DB1"/>
<pin name="DB0"/>
<pin name="CS"/>
<pin name="WR"/>
<pin name="DGND"/>
<pin name="VOUTA"/>
<pin name="VOUTB"/>
<pin name="AGND"/>
<pin name="REFIN"/>
<pin name="VDD"/>
<pin name="CLR"/>
<pin name="LDAC"/>
<pin name="PD"/>
<pin name="AB"/>
</symbol>
<symbol name="AD7745">
<pin name="/RDY"/>
<pin name="CIN1+"/>
<pin name="CIN1-"/>
<pin name="CIN2+"/>
<pin name="CIN2-"/>
<pin name="EXCA"/>
<pin name="EXCB"/>
<pin name="GND"/>
<pin name="NC"/>
<pin name="REFIN+"/>
<pin name="REFIN-"/>
<pin name="SCL"/>
<pin name="SDA"/>
<pin name="VDD"/>
<pin name="VIN+"/>
<pin name="VIN-"/>
</symbol>
<symbol name="AD7781">
<pin name="SCLK"/>
<pin name="DOUT"/>
<pin name="GAIN"/>
<pin name="AIN+"/>
<pin name="AIN-"/>
<pin name="REFIN+"/>
<pin name="REFIN-"/>
<pin name="BPDSW"/>
<pin name="GND"/>
<pin name="AVDD"/>
<pin name="DVDD"/>
<pin name="*PDRST"/>
<pin name="FILTER"/>
</symbol>
<symbol name="OP-AMP+--1">
<pin name="-IN" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
<pin name="EPAD"/>
</symbol>
<symbol name="OP-AMP-1">
<pin name="-IN" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="AD9835">
<pin name="FS_ADJ"/>
<pin name="REFIN"/>
<pin name="REFOUT"/>
<pin name="DVDD"/>
<pin name="DGND"/>
<pin name="MCLK"/>
<pin name="SCLK"/>
<pin name="SDATA"/>
<pin name="FSYNC"/>
<pin name="FSEL"/>
<pin name="PSEL1"/>
<pin name="PSEL0"/>
<pin name="AGND"/>
<pin name="IOUT"/>
<pin name="AVDD"/>
<pin name="COMP"/>
</symbol>
<symbol name="ALM-1412">
<pin name="RF_IN"/>
<pin name="GND"/>
<pin name="SD"/>
<pin name="RF_OUT"/>
<pin name="VDD"/>
<pin name="GND@6"/>
<pin name="GND@7"/>
<pin name="GND@8"/>
<pin name="GND@9"/>
</symbol>
<symbol name="AS3400">
<pin name="AGND"/>
<pin name="LINL"/>
<pin name="LINR"/>
<pin name="VOL_CSDA"/>
<pin name="MODE_CSCL"/>
<pin name="MICL"/>
<pin name="MICS"/>
<pin name="MICR"/>
<pin name="QMICR"/>
<pin name="QLINR"/>
<pin name="IOP1R"/>
<pin name="QOP1R"/>
<pin name="IOP2R"/>
<pin name="QOP2R"/>
<pin name="VSS"/>
<pin name="HPL"/>
<pin name="HPR"/>
<pin name="HPVDD"/>
<pin name="VBAT"/>
<pin name="CPP"/>
<pin name="GND"/>
<pin name="CPN"/>
<pin name="VNEG"/>
<pin name="QMICL"/>
<pin name="PAD"/>
</symbol>
<symbol name="MCP4725">
<pin name="VOUT"/>
<pin name="VSS"/>
<pin name="VDD"/>
<pin name="AO"/>
<pin name="SCL"/>
<pin name="SDA"/>
</symbol>
<symbol name="HT8950">
<pin name="SW0"/>
<pin name="SW1"/>
<pin name="SW2"/>
<pin name="VSS"/>
<pin name="AO"/>
<pin name="AIN"/>
<pin name="VDD"/>
<pin name="LAMP"/>
<pin name="AUDIO"/>
<pin name="VREF"/>
<pin name="TS"/>
<pin name="FVIB"/>
<pin name="OSC2"/>
<pin name="OSC1"/>
<pin name="VIB"/>
<pin name="TGU"/>
<pin name="TGD"/>
<pin name="ROB"/>
</symbol>
<symbol name="OP-AMP+-">
<pin name="+IN" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
</symbol>
<symbol name="OP-AMP">
<pin name="+IN" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LMV324">
<pin name="-IN" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="-V" direction="pwr"/>
<pin name="OUT" direction="out"/>
<pin name="+V" direction="pwr"/>
</symbol>
<symbol name="LMV324_2">
<pin name="-IN" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="OPAMP_2">
<pin name="-IN1" direction="in"/>
<pin name="+IN1" direction="in"/>
<pin name="OUT1" direction="out"/>
<pin name="+V" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="OPAMP_2_1">
<pin name="OUT2" direction="out"/>
<pin name="-IN2" direction="in"/>
<pin name="+IN2" direction="in"/>
</symbol>
<symbol name="LT1014">
<pin name="-IN" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="-V" direction="pwr"/>
<pin name="OUT" direction="out"/>
<pin name="+V" direction="pwr"/>
</symbol>
<symbol name="LT1014_2">
<pin name="-IN" direction="pwr"/>
<pin name="+IN" direction="pwr"/>
<pin name="OUT" direction="pwr"/>
</symbol>
<symbol name="LTC6244">
<pin name="-IN"/>
<pin name="+IN"/>
<pin name="-V"/>
<pin name="+V"/>
<pin name="OUT"/>
</symbol>
<symbol name="LTC6244_2">
<pin name="-IN"/>
<pin name="+IN"/>
<pin name="OUT"/>
</symbol>
<symbol name="MAX323">
<pin name="NO1"/>
<pin name="COM1"/>
<pin name="IN2"/>
<pin name="V-"/>
<pin name="NO2"/>
<pin name="COM2"/>
<pin name="IN1"/>
<pin name="V+"/>
</symbol>
<symbol name="MCP41XXX">
<pin name="VCC"/>
<pin name="CS"/>
<pin name="SCK"/>
<pin name="DI"/>
<pin name="A"/>
<pin name="W"/>
<pin name="B"/>
<pin name="GND"/>
</symbol>
<symbol name="MCP42XXX">
<pin name="A0"/>
<pin name="W0"/>
<pin name="B0"/>
<pin name="A1"/>
<pin name="W1"/>
<pin name="B1"/>
<pin name="SCK"/>
<pin name="DI"/>
<pin name="DO"/>
<pin name="SHTDWN"/>
<pin name="RST"/>
<pin name="GND"/>
<pin name="VCC"/>
<pin name="CS"/>
</symbol>
<symbol name="MSGEQ7">
<pin name="DCOUT"/>
<pin name="CG"/>
<pin name="CKIN"/>
<pin name="GND"/>
<pin name="RESET" direction="in"/>
<pin name="STROBE" direction="in"/>
<pin name="AUDIO_IN" direction="in"/>
<pin name="VDD" direction="in"/>
</symbol>
<symbol name="CD74HC4067">
<pin name="COM"/>
<pin name="CHAN7"/>
<pin name="CHAN6"/>
<pin name="CHAN5"/>
<pin name="CHAN4"/>
<pin name="CHAN3"/>
<pin name="CHAN2"/>
<pin name="CHAN1"/>
<pin name="CHAN0"/>
<pin name="S0" direction="in"/>
<pin name="S1" direction="in"/>
<pin name="GND"/>
<pin name="S3" direction="in"/>
<pin name="S2" direction="in"/>
<pin name="EN" direction="in" function="dot"/>
<pin name="CHAN15"/>
<pin name="CHAN14"/>
<pin name="CHAN13"/>
<pin name="CHAN12"/>
<pin name="CHAN11"/>
<pin name="CHAN10"/>
<pin name="CHAN9"/>
<pin name="CHAN8"/>
<pin name="VCC"/>
</symbol>
<symbol name="TS3A5017">
<pin name="IN2"/>
<pin name="1S4"/>
<pin name="1S3"/>
<pin name="1S2"/>
<pin name="1S1"/>
<pin name="1D"/>
<pin name="GND"/>
<pin name="2D"/>
<pin name="2S1"/>
<pin name="2S2"/>
<pin name="2S3"/>
<pin name="2S4"/>
<pin name="IN1"/>
<pin name="VCC"/>
<pin name="1EN" function="dot"/>
<pin name="2EN" function="dot"/>
</symbol>
<symbol name="NE555">
<pin name="TRE" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="DIS" direction="in"/>
<pin name="TRI" direction="in"/>
<pin name="VCC+" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="CON" direction="in"/>
<pin name="/RES" direction="in"/>
</symbol>
<symbol name="PCM1803A">
<pin name="VINL"/>
<pin name="VINR"/>
<pin name="VREF1"/>
<pin name="VREF2"/>
<pin name="VCCA"/>
<pin name="GNDA"/>
<pin name="PDWN"/>
<pin name="BPAS"/>
<pin name="TEST"/>
<pin name="LRCK"/>
<pin name="BCK"/>
<pin name="DOUT"/>
<pin name="GNDD"/>
<pin name="VDD"/>
<pin name="SCK"/>
<pin name="OSR"/>
<pin name="FMT0"/>
<pin name="FMT1"/>
<pin name="MD0"/>
<pin name="MD1"/>
</symbol>
<symbol name="SN74LV4052APWR">
<pin name="2Y0"/>
<pin name="2Y2"/>
<pin name="2-COM"/>
<pin name="2Y3"/>
<pin name="2Y1"/>
<pin name="INH"/>
<pin name="GNG@7"/>
<pin name="GND@8"/>
<pin name="B"/>
<pin name="A"/>
<pin name="1Y3"/>
<pin name="1Y0"/>
<pin name="1-COM"/>
<pin name="1Y1"/>
<pin name="1Y2"/>
<pin name="VCC"/>
</symbol>
<symbol name="TVP5150-NTSC_DECODER-1">
<pin name="AGND"/>
<pin name="AIP1A"/>
<pin name="AIP1B"/>
<pin name="AVID"/>
<pin name="CH_AGND"/>
<pin name="CH_AVDD"/>
<pin name="DGND"/>
<pin name="DVDD"/>
<pin name="FID/GLCO"/>
<pin name="HSYNC"/>
<pin name="INT_REQ"/>
<pin name="IO_DVDD"/>
<pin name="PCLK/SCLK"/>
<pin name="PDN"/>
<pin name="PLL_AGND"/>
<pin name="PLL_AVDD"/>
<pin name="REFM"/>
<pin name="REFP"/>
<pin name="RESET/"/>
<pin name="SCL"/>
<pin name="SDA"/>
<pin name="VSYNC"/>
<pin name="XTAL1"/>
<pin name="XTAL2"/>
<pin name="YOUT_0"/>
<pin name="YOUT_1"/>
<pin name="YOUT_2"/>
<pin name="YOUT_3"/>
<pin name="YOUT_4"/>
<pin name="YOUT_5"/>
<pin name="YOUT_6"/>
<pin name="YOUT_7"/>
</symbol>
<symbol name="X9015_DIGI_POT">
<pin name="VSS" direction="pwr"/>
<pin name="RW/VW"/>
<pin name="VCC" direction="pwr"/>
<pin name="CS'"/>
<pin name="INC'"/>
<pin name="U/D'"/>
<pin name="RH/VH"/>
<pin name="RL/VL"/>
</symbol>
<symbol name="74HC4051_MUX">
<pin name="VSS"/>
<pin name="VEE"/>
<pin name="INH"/>
<pin name="IO7"/>
<pin name="IO5"/>
<pin name="IO6"/>
<pin name="IO"/>
<pin name="IO4"/>
<pin name="VDD"/>
<pin name="IO2"/>
<pin name="IO1"/>
<pin name="IO0"/>
<pin name="IO3"/>
<pin name="A"/>
<pin name="B"/>
<pin name="C"/>
</symbol>
<symbol name="74HC4052">
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="INH" direction="in"/>
<pin name="VCC" direction="pwr"/>
<pin name="VEE" direction="pwr"/>
<pin name="X"/>
<pin name="X0"/>
<pin name="X1"/>
<pin name="X2"/>
<pin name="X3"/>
<pin name="Y"/>
<pin name="Y0"/>
<pin name="Y1"/>
<pin name="Y2"/>
<pin name="Y3"/>
</symbol>
<symbol name="74VHC4052_ANALOG_MUX">
<pin name="VCC"/>
<pin name="GND"/>
<pin name="X3"/>
<pin name="IN/OUT_X"/>
<pin name="X2"/>
<pin name="X1"/>
<pin name="Y1"/>
<pin name="Y2"/>
<pin name="X0"/>
<pin name="Y0"/>
<pin name="Y3"/>
<pin name="IN/OUT_Y"/>
<pin name="A"/>
<pin name="B"/>
<pin name="VEE"/>
<pin name="INH"/>
</symbol>
<symbol name="556_TIMER_DUAL">
<pin name="GND"/>
<pin name="TRIG"/>
<pin name="OUT"/>
<pin name="CV"/>
<pin name="RST"/>
<pin name="THR"/>
<pin name="DIS"/>
<pin name="TRIG2"/>
<pin name="OUT2"/>
<pin name="RST2"/>
<pin name="CV2"/>
<pin name="THR2"/>
<pin name="DIS2"/>
<pin name="VCC"/>
</symbol>
<symbol name="INA139">
<pin name="VIN+"/>
<pin name="VIN-"/>
<pin name="V+"/>
<pin name="GND"/>
<pin name="OUT"/>
</symbol>
<symbol name="OP-AMP+-FULL">
<pin name="+IN" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
<pin name="GAIN@8"/>
<pin name="GAIN@1"/>
<pin name="BP"/>
</symbol>
<symbol name="TPA6138A2">
<pin name="CN"/>
<pin name="VSS"/>
<pin name="!MUTE"/>
<pin name="GND"/>
<pin name="OUTR"/>
<pin name="INR-"/>
<pin name="INR+"/>
<pin name="INL+"/>
<pin name="INL-"/>
<pin name="OUTL"/>
<pin name="UVP"/>
<pin name="VDD"/>
<pin name="CP"/>
</symbol>
<symbol name="TPA2005D1">
<pin name="VDD" direction="pwr"/>
<pin name="IN+"/>
<pin name="IN-"/>
<pin name="GND@1" direction="pwr"/>
<pin name="OUT+"/>
<pin name="OUT-"/>
<pin name="SHUTDOWN" direction="in" function="dot"/>
<pin name="GND@2" direction="pwr"/>
</symbol>
<symbol name="HIH6131">
<pin name="SCL"/>
<pin name="SDA"/>
<pin name="AL_L"/>
<pin name="AL_H"/>
<pin name="VDD"/>
<pin name="VCORE"/>
<pin name="GND"/>
<pin name="NC"/>
</symbol>
<symbol name="INA169">
<pin name="VIN+"/>
<pin name="VIN-"/>
<pin name="V+"/>
<pin name="GND"/>
<pin name="OUT"/>
</symbol>
<symbol name="TPA6111">
<pin name="BYP"/>
<pin name="GND"/>
<pin name="IN1"/>
<pin name="IN2"/>
<pin name="SHT"/>
<pin name="VDD"/>
<pin name="VO1"/>
<pin name="VO2"/>
</symbol>
<symbol name="ADC8045">
<pin name="IN-"/>
<pin name="IN+"/>
<pin name="OUT"/>
<pin name="FB"/>
<pin name="VSS"/>
<pin name="VDD"/>
</symbol>
<symbol name="AD9837">
<pin name="SCLK"/>
<pin name="SDATA"/>
<pin name="FSYNC"/>
<pin name="MCLK"/>
<pin name="DGND"/>
<pin name="AGND"/>
<pin name="VOUT"/>
<pin name="COMP"/>
<pin name="VDD"/>
<pin name="CAP/2.5V"/>
</symbol>
<symbol name="TS3USB221A">
<pin name="D-"/>
<pin name="D+"/>
<pin name="2D+"/>
<pin name="1D+"/>
<pin name="1D-"/>
<pin name="2D-"/>
<pin name="!OE"/>
<pin name="S"/>
<pin name="VCC"/>
<pin name="VSS"/>
</symbol>
<symbol name="LM339">
<pin name="-IN" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="PWRN">
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="AD8232">
<pin name="OUT"/>
<pin name="OPAMP-"/>
<pin name="REFOUT"/>
<pin name="OPAMP+"/>
<pin name="SW"/>
<pin name="RLD"/>
<pin name="RLDFB"/>
<pin name="-IN"/>
<pin name="+IN"/>
<pin name="HPDRIVE"/>
<pin name="HPSENSE"/>
<pin name="IAOUT"/>
<pin name="REFIN"/>
<pin name="+VS"/>
<pin name="GND"/>
<pin name="FR"/>
<pin name="AC/!DC"/>
<pin name="!SDN"/>
<pin name="LO+"/>
<pin name="LO-"/>
<pin name="GND_PAD"/>
</symbol>
<symbol name="ADS1015">
<pin name="AIN0"/>
<pin name="AIN1"/>
<pin name="AIN2"/>
<pin name="AIN3"/>
<pin name="ALERT/RDY"/>
<pin name="ADDR"/>
<pin name="SCL"/>
<pin name="SDA"/>
<pin name="VSS"/>
<pin name="VDD"/>
</symbol>
<symbol name="AD5262">
<pin name="A1" direction="pas"/>
<pin name="A2" direction="pas"/>
<pin name="B1" direction="pas"/>
<pin name="B2" direction="pas"/>
<pin name="CLK" direction="in"/>
<pin name="CS_N" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="PR_N" direction="in"/>
<pin name="SDI" direction="in"/>
<pin name="SDO" direction="out"/>
<pin name="SHDN_N" direction="in"/>
<pin name="VDD" direction="pwr"/>
<pin name="VL" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="W1" direction="pas"/>
<pin name="W2" direction="pas"/>
</symbol>
<symbol name="MAX6675">
<pin name="GND"/>
<pin name="T-"/>
<pin name="T+"/>
<pin name="VCC"/>
<pin name="(MI)SO"/>
<pin name="!CS"/>
<pin name="SCK"/>
</symbol>
<symbol name="GENERIC-8PIN">
<pin name="1"/>
<pin name="2"/>
<pin name="3"/>
<pin name="4"/>
<pin name="5"/>
<pin name="6"/>
<pin name="7"/>
<pin name="8"/>
</symbol>
<symbol name="TL431">
<pin name="C"/>
<pin name="R"/>
<pin name="A"/>
</symbol>
<symbol name="AD627">
<pin name="IN+"/>
<pin name="IN-"/>
<pin name="OUTPUT"/>
<pin name="REF"/>
<pin name="RG@1"/>
<pin name="RG@8"/>
<pin name="VS+"/>
<pin name="VS-"/>
</symbol>
<symbol name="OP-AMP+--2">
<pin name="+IN" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
</symbol>
<symbol name="OP-AMP-1-1">
<pin name="+IN" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="SN74LVC1G66_SPST_AMUX">
<pin name="A_IN"/>
<pin name="CTRL_IN"/>
<pin name="A_OUT"/>
<pin name="VSS"/>
<pin name="VCC"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="ACS712">
<description>Hall-effect-based isolated linear current sensor</description>
<gates>
<gate name="G$1" symbol="ACS712"/>
</gates>
<devices>
<device name="" package="SO08">
<connects>
<connect gate="G$1" pin="FILT" pad="6"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="IP+@1" pad="1"/>
<connect gate="G$1" pin="IP+@2" pad="2"/>
<connect gate="G$1" pin="IP-@3" pad="3"/>
<connect gate="G$1" pin="IP-@4" pad="4"/>
<connect gate="G$1" pin="VCC" pad="8"/>
<connect gate="G$1" pin="VOUT" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-08964"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD725">
<description>RGB component to NTSC/PAL Encoder</description>
<gates>
<gate name="G$1" symbol="AD725"/>
</gates>
<devices>
<device name="" package="SO16L">
<connects>
<connect gate="G$1" pin="4FSC" pad="3"/>
<connect gate="G$1" pin="AGND" pad="2"/>
<connect gate="G$1" pin="APOS" pad="4"/>
<connect gate="G$1" pin="BIN" pad="8"/>
<connect gate="G$1" pin="CE" pad="5"/>
<connect gate="G$1" pin="COMP" pad="10"/>
<connect gate="G$1" pin="CRMA" pad="9"/>
<connect gate="G$1" pin="DGND" pad="13"/>
<connect gate="G$1" pin="DPOS" pad="14"/>
<connect gate="G$1" pin="GIN" pad="7"/>
<connect gate="G$1" pin="HSYNC" pad="16"/>
<connect gate="G$1" pin="LUMA" pad="11"/>
<connect gate="G$1" pin="RIN" pad="6"/>
<connect gate="G$1" pin="STND" pad="1"/>
<connect gate="G$1" pin="VSYNC" pad="15"/>
<connect gate="G$1" pin="YTRAP" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD5330" prefix="U">
<description>8-bit parallel input DAC</description>
<gates>
<gate name="G$1" symbol="AD5330"/>
</gates>
<devices>
<device name="" package="TSSOP20">
<connects>
<connect gate="G$1" pin="BUF" pad="1"/>
<connect gate="G$1" pin="CLR" pad="9"/>
<connect gate="G$1" pin="CS" pad="6"/>
<connect gate="G$1" pin="DB0" pad="13"/>
<connect gate="G$1" pin="DB1" pad="14"/>
<connect gate="G$1" pin="DB2" pad="15"/>
<connect gate="G$1" pin="DB3" pad="16"/>
<connect gate="G$1" pin="DB4" pad="17"/>
<connect gate="G$1" pin="DB5" pad="18"/>
<connect gate="G$1" pin="DB6" pad="19"/>
<connect gate="G$1" pin="DB7" pad="20"/>
<connect gate="G$1" pin="GAIN" pad="8"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="LDAC" pad="10"/>
<connect gate="G$1" pin="PD" pad="11"/>
<connect gate="G$1" pin="VDD" pad="12"/>
<connect gate="G$1" pin="VOUT" pad="4"/>
<connect gate="G$1" pin="VREF" pad="3"/>
<connect gate="G$1" pin="WR" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD7302">
<description>8-bit parallel input 2-output DAC</description>
<gates>
<gate name="G$1" symbol="AD7302"/>
</gates>
<devices>
<device name="SMD" package="TSSOP20">
<connects>
<connect gate="G$1" pin="AB" pad="11"/>
<connect gate="G$1" pin="AGND" pad="17"/>
<connect gate="G$1" pin="CLR" pad="14"/>
<connect gate="G$1" pin="CS" pad="9"/>
<connect gate="G$1" pin="DB0" pad="8"/>
<connect gate="G$1" pin="DB1" pad="7"/>
<connect gate="G$1" pin="DB2" pad="6"/>
<connect gate="G$1" pin="DB3" pad="5"/>
<connect gate="G$1" pin="DB4" pad="4"/>
<connect gate="G$1" pin="DB5" pad="3"/>
<connect gate="G$1" pin="DB6" pad="2"/>
<connect gate="G$1" pin="DB7" pad="1"/>
<connect gate="G$1" pin="DGND" pad="20"/>
<connect gate="G$1" pin="LDAC" pad="13"/>
<connect gate="G$1" pin="PD" pad="12"/>
<connect gate="G$1" pin="REFIN" pad="16"/>
<connect gate="G$1" pin="VDD" pad="15"/>
<connect gate="G$1" pin="VOUTA" pad="19"/>
<connect gate="G$1" pin="VOUTB" pad="18"/>
<connect gate="G$1" pin="WR" pad="10"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD7745">
<description>24-bit capacitance to digital converter</description>
<gates>
<gate name="G$1" symbol="AD7745"/>
</gates>
<devices>
<device name="" package="TSSOP16">
<connects>
<connect gate="G$1" pin="/RDY" pad="2"/>
<connect gate="G$1" pin="CIN1+" pad="8"/>
<connect gate="G$1" pin="CIN1-" pad="7"/>
<connect gate="G$1" pin="CIN2+" pad="9"/>
<connect gate="G$1" pin="CIN2-" pad="10"/>
<connect gate="G$1" pin="EXCA" pad="3"/>
<connect gate="G$1" pin="EXCB" pad="4"/>
<connect gate="G$1" pin="GND" pad="13"/>
<connect gate="G$1" pin="NC" pad="15"/>
<connect gate="G$1" pin="REFIN+" pad="5"/>
<connect gate="G$1" pin="REFIN-" pad="6"/>
<connect gate="G$1" pin="SCL" pad="1"/>
<connect gate="G$1" pin="SDA" pad="16"/>
<connect gate="G$1" pin="VDD" pad="14"/>
<connect gate="G$1" pin="VIN+" pad="11"/>
<connect gate="G$1" pin="VIN-" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD7781" prefix="U">
<description>20-Bit, Pin-Programmable, Ultralow Power Sigma-Delta ADC</description>
<gates>
<gate name="G$1" symbol="AD7781"/>
</gates>
<devices>
<device name="CRZ" package="SOIC-14">
<connects>
<connect gate="G$1" pin="*PDRST" pad="13"/>
<connect gate="G$1" pin="AIN+" pad="5"/>
<connect gate="G$1" pin="AIN-" pad="6"/>
<connect gate="G$1" pin="AVDD" pad="11"/>
<connect gate="G$1" pin="BPDSW" pad="9"/>
<connect gate="G$1" pin="DOUT" pad="2"/>
<connect gate="G$1" pin="DVDD" pad="12"/>
<connect gate="G$1" pin="FILTER" pad="14"/>
<connect gate="G$1" pin="GAIN" pad="4"/>
<connect gate="G$1" pin="GND" pad="10"/>
<connect gate="G$1" pin="REFIN+" pad="7"/>
<connect gate="G$1" pin="REFIN-" pad="8"/>
<connect gate="G$1" pin="SCLK" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CRUZ" package="TSSOP-16">
<connects>
<connect gate="G$1" pin="*PDRST" pad="14"/>
<connect gate="G$1" pin="AIN+" pad="6"/>
<connect gate="G$1" pin="AIN-" pad="7"/>
<connect gate="G$1" pin="AVDD" pad="12"/>
<connect gate="G$1" pin="BPDSW" pad="10"/>
<connect gate="G$1" pin="DOUT" pad="3"/>
<connect gate="G$1" pin="DVDD" pad="13"/>
<connect gate="G$1" pin="FILTER" pad="15"/>
<connect gate="G$1" pin="GAIN" pad="5"/>
<connect gate="G$1" pin="GND" pad="11"/>
<connect gate="G$1" pin="REFIN+" pad="8"/>
<connect gate="G$1" pin="REFIN-" pad="9"/>
<connect gate="G$1" pin="SCLK" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD8397-EPAD" prefix="IC">
<description>Rail-to-rail high current output op-amp</description>
<gates>
<gate name="A" symbol="OP-AMP+--1"/>
<gate name="B" symbol="OP-AMP-1"/>
</gates>
<devices>
<device name="EPAD" package="SO08-EPAD">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="EPAD" pad="EPAD"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD9835">
<description>50MHz DDS waveform generator</description>
<gates>
<gate name="G$1" symbol="AD9835"/>
</gates>
<devices>
<device name="" package="TSSOP16">
<connects>
<connect gate="G$1" pin="AGND" pad="13"/>
<connect gate="G$1" pin="AVDD" pad="15"/>
<connect gate="G$1" pin="COMP" pad="16"/>
<connect gate="G$1" pin="DGND" pad="5"/>
<connect gate="G$1" pin="DVDD" pad="4"/>
<connect gate="G$1" pin="FSEL" pad="10"/>
<connect gate="G$1" pin="FSYNC" pad="9"/>
<connect gate="G$1" pin="FS_ADJ" pad="1"/>
<connect gate="G$1" pin="IOUT" pad="14"/>
<connect gate="G$1" pin="MCLK" pad="6"/>
<connect gate="G$1" pin="PSEL0" pad="12"/>
<connect gate="G$1" pin="PSEL1" pad="11"/>
<connect gate="G$1" pin="REFIN" pad="2"/>
<connect gate="G$1" pin="REFOUT" pad="3"/>
<connect gate="G$1" pin="SCLK" pad="7"/>
<connect gate="G$1" pin="SDATA" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AS3400" prefix="U">
<description>Active noise cancellation chip.&lt;br&gt;
Stereo in, stereo out, two microphones.&lt;br&gt;
Single alkaline cell power.&lt;br&gt;
QFN-24 w/exposed pad.</description>
<gates>
<gate name="G$1" symbol="AS3400"/>
</gates>
<devices>
<device name="" package="QFN-24_ALT2">
<connects>
<connect gate="G$1" pin="AGND" pad="1"/>
<connect gate="G$1" pin="CPN" pad="22"/>
<connect gate="G$1" pin="CPP" pad="20"/>
<connect gate="G$1" pin="GND" pad="21"/>
<connect gate="G$1" pin="HPL" pad="16"/>
<connect gate="G$1" pin="HPR" pad="17"/>
<connect gate="G$1" pin="HPVDD" pad="18"/>
<connect gate="G$1" pin="IOP1R" pad="11"/>
<connect gate="G$1" pin="IOP2R" pad="13"/>
<connect gate="G$1" pin="LINL" pad="2"/>
<connect gate="G$1" pin="LINR" pad="3"/>
<connect gate="G$1" pin="MICL" pad="6"/>
<connect gate="G$1" pin="MICR" pad="8"/>
<connect gate="G$1" pin="MICS" pad="7"/>
<connect gate="G$1" pin="MODE_CSCL" pad="5"/>
<connect gate="G$1" pin="PAD" pad="EP"/>
<connect gate="G$1" pin="QLINR" pad="10"/>
<connect gate="G$1" pin="QMICL" pad="24"/>
<connect gate="G$1" pin="QMICR" pad="9"/>
<connect gate="G$1" pin="QOP1R" pad="12"/>
<connect gate="G$1" pin="QOP2R" pad="14"/>
<connect gate="G$1" pin="VBAT" pad="19"/>
<connect gate="G$1" pin="VNEG" pad="23"/>
<connect gate="G$1" pin="VOL_CSDA" pad="4"/>
<connect gate="G$1" pin="VSS" pad="15"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MCP4725" prefix="U">
<description>Microchip 12-bit I2C DAC, SOT23-6</description>
<gates>
<gate name="U1" symbol="MCP4725"/>
</gates>
<devices>
<device name="SOT-23" package="SOT23-6">
<connects>
<connect gate="U1" pin="AO" pad="6"/>
<connect gate="U1" pin="SCL" pad="5"/>
<connect gate="U1" pin="SDA" pad="4"/>
<connect gate="U1" pin="VDD" pad="3"/>
<connect gate="U1" pin="VOUT" pad="1"/>
<connect gate="U1" pin="VSS" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-08886"/>
<attribute name="VALUE" value="MCP4725"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HT8950">
<description>Holtek voice modulator IC, COM-10574</description>
<gates>
<gate name="G$1" symbol="HT8950"/>
</gates>
<devices>
<device name="" package="DIL18">
<connects>
<connect gate="G$1" pin="AIN" pad="6"/>
<connect gate="G$1" pin="AO" pad="5"/>
<connect gate="G$1" pin="AUDIO" pad="9"/>
<connect gate="G$1" pin="FVIB" pad="12"/>
<connect gate="G$1" pin="LAMP" pad="8"/>
<connect gate="G$1" pin="OSC1" pad="14"/>
<connect gate="G$1" pin="OSC2" pad="13"/>
<connect gate="G$1" pin="ROB" pad="18"/>
<connect gate="G$1" pin="SW0" pad="1"/>
<connect gate="G$1" pin="SW1" pad="2"/>
<connect gate="G$1" pin="SW2" pad="3"/>
<connect gate="G$1" pin="TGD" pad="17"/>
<connect gate="G$1" pin="TGU" pad="16"/>
<connect gate="G$1" pin="TS" pad="11"/>
<connect gate="G$1" pin="VDD" pad="7"/>
<connect gate="G$1" pin="VIB" pad="15"/>
<connect gate="G$1" pin="VREF" pad="10"/>
<connect gate="G$1" pin="VSS" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM358" prefix="IC">
<description>Jellybean op-amp</description>
<gates>
<gate name="G1" symbol="OP-AMP+-"/>
<gate name="G2" symbol="OP-AMP"/>
</gates>
<devices>
<device name="" package="DIP08">
<connects>
<connect gate="G1" pin="+IN" pad="3"/>
<connect gate="G1" pin="-IN" pad="2"/>
<connect gate="G1" pin="OUT" pad="1"/>
<connect gate="G1" pin="V+" pad="8"/>
<connect gate="G1" pin="V-" pad="4"/>
<connect gate="G2" pin="+IN" pad="5"/>
<connect gate="G2" pin="-IN" pad="6"/>
<connect gate="G2" pin="OUT" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-09172"/>
</technology>
</technologies>
</device>
<device name="KIT" package="DIP08-KIT">
<connects>
<connect gate="G1" pin="+IN" pad="3"/>
<connect gate="G1" pin="-IN" pad="2"/>
<connect gate="G1" pin="OUT" pad="1"/>
<connect gate="G1" pin="V+" pad="8"/>
<connect gate="G1" pin="V-" pad="4"/>
<connect gate="G2" pin="+IN" pad="5"/>
<connect gate="G2" pin="-IN" pad="6"/>
<connect gate="G2" pin="OUT" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-09172"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM393">
<description>Low-voltage comparator</description>
<gates>
<gate name="G1" symbol="OP-AMP+-"/>
<gate name="G2" symbol="OP-AMP"/>
</gates>
<devices>
<device name="" package="SO08">
<connects>
<connect gate="G1" pin="+IN" pad="3"/>
<connect gate="G1" pin="-IN" pad="2"/>
<connect gate="G1" pin="OUT" pad="1"/>
<connect gate="G1" pin="V+" pad="8"/>
<connect gate="G1" pin="V-" pad="4"/>
<connect gate="G2" pin="+IN" pad="5"/>
<connect gate="G2" pin="-IN" pad="6"/>
<connect gate="G2" pin="OUT" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMV324" prefix="IC">
<description>Jellybean quad op-amp</description>
<gates>
<gate name="G1" symbol="LMV324"/>
<gate name="G3" symbol="LMV324_2"/>
<gate name="G2" symbol="LMV324_2"/>
<gate name="G4" symbol="LMV324_2"/>
</gates>
<devices>
<device name="" package="SO014">
<connects>
<connect gate="G1" pin="+IN" pad="3"/>
<connect gate="G1" pin="+V" pad="4"/>
<connect gate="G1" pin="-IN" pad="2"/>
<connect gate="G1" pin="-V" pad="11"/>
<connect gate="G1" pin="OUT" pad="1"/>
<connect gate="G2" pin="+IN" pad="10"/>
<connect gate="G2" pin="-IN" pad="9"/>
<connect gate="G2" pin="OUT" pad="8"/>
<connect gate="G3" pin="+IN" pad="5"/>
<connect gate="G3" pin="-IN" pad="6"/>
<connect gate="G3" pin="OUT" pad="7"/>
<connect gate="G4" pin="+IN" pad="12"/>
<connect gate="G4" pin="-IN" pad="13"/>
<connect gate="G4" pin="OUT" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-08227"/>
<attribute name="VALUE" value="LMV324"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMV358" prefix="IC">
<description>Jellybean rail-to-rail output op-amp</description>
<gates>
<gate name="G1" symbol="OPAMP_2"/>
<gate name="G2" symbol="OPAMP_2_1"/>
</gates>
<devices>
<device name="SOIC" package="SO08">
<connects>
<connect gate="G1" pin="+IN1" pad="3"/>
<connect gate="G1" pin="+V" pad="8"/>
<connect gate="G1" pin="-IN1" pad="2"/>
<connect gate="G1" pin="GND" pad="4"/>
<connect gate="G1" pin="OUT1" pad="1"/>
<connect gate="G2" pin="+IN2" pad="5"/>
<connect gate="G2" pin="-IN2" pad="6"/>
<connect gate="G2" pin="OUT2" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-09657"/>
</technology>
</technologies>
</device>
<device name="SOICT" package="SO08-TIGHT">
<connects>
<connect gate="G1" pin="+IN1" pad="3"/>
<connect gate="G1" pin="+V" pad="8"/>
<connect gate="G1" pin="-IN1" pad="2"/>
<connect gate="G1" pin="GND" pad="4"/>
<connect gate="G1" pin="OUT1" pad="1"/>
<connect gate="G2" pin="+IN2" pad="5"/>
<connect gate="G2" pin="-IN2" pad="6"/>
<connect gate="G2" pin="OUT2" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-09657"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LT1014">
<description>Precision quad op-amp. I/O range includes negative rail.</description>
<gates>
<gate name="G1" symbol="LT1014"/>
<gate name="G2" symbol="LT1014_2"/>
<gate name="G3" symbol="LT1014_2"/>
<gate name="G4" symbol="LT1014_2"/>
</gates>
<devices>
<device name="" package="SO16L">
<connects>
<connect gate="G1" pin="+IN" pad="3"/>
<connect gate="G1" pin="+V" pad="4"/>
<connect gate="G1" pin="-IN" pad="2"/>
<connect gate="G1" pin="-V" pad="13"/>
<connect gate="G1" pin="OUT" pad="1"/>
<connect gate="G2" pin="+IN" pad="5"/>
<connect gate="G2" pin="-IN" pad="6"/>
<connect gate="G2" pin="OUT" pad="7"/>
<connect gate="G3" pin="+IN" pad="12"/>
<connect gate="G3" pin="-IN" pad="11"/>
<connect gate="G3" pin="OUT" pad="10"/>
<connect gate="G4" pin="+IN" pad="14"/>
<connect gate="G4" pin="-IN" pad="15"/>
<connect gate="G4" pin="OUT" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX323" prefix="U">
<description>Dual low-voltage SPST analog switch</description>
<gates>
<gate name="G$1" symbol="MAX323"/>
</gates>
<devices>
<device name="" package="SO08">
<connects>
<connect gate="G$1" pin="COM1" pad="2"/>
<connect gate="G$1" pin="COM2" pad="6"/>
<connect gate="G$1" pin="IN1" pad="7"/>
<connect gate="G$1" pin="IN2" pad="3"/>
<connect gate="G$1" pin="NO1" pad="1"/>
<connect gate="G$1" pin="NO2" pad="5"/>
<connect gate="G$1" pin="V+" pad="8"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MCP41XXX" prefix="U">
<description>SPI controlled single digital potentiometer by Microchip&lt;br /&gt;
&lt;br /&gt;
PID: COM-10613</description>
<gates>
<gate name="G$1" symbol="MCP41XXX"/>
</gates>
<devices>
<device name="" package="SO08">
<connects>
<connect gate="G$1" pin="A" pad="5"/>
<connect gate="G$1" pin="B" pad="7"/>
<connect gate="G$1" pin="CS" pad="1"/>
<connect gate="G$1" pin="DI" pad="3"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="SCK" pad="2"/>
<connect gate="G$1" pin="VCC" pad="8"/>
<connect gate="G$1" pin="W" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="DIL" package="DIL-08">
<connects>
<connect gate="G$1" pin="A" pad="5"/>
<connect gate="G$1" pin="B" pad="7"/>
<connect gate="G$1" pin="CS" pad="1"/>
<connect gate="G$1" pin="DI" pad="3"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="SCK" pad="2"/>
<connect gate="G$1" pin="VCC" pad="8"/>
<connect gate="G$1" pin="W" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MCP42XXX" prefix="U">
<description>SPI controlled dual digital potentiometer by Microchip</description>
<gates>
<gate name="G$1" symbol="MCP42XXX"/>
</gates>
<devices>
<device name="" package="SO014">
<connects>
<connect gate="G$1" pin="A0" pad="8"/>
<connect gate="G$1" pin="A1" pad="7"/>
<connect gate="G$1" pin="B0" pad="10"/>
<connect gate="G$1" pin="B1" pad="5"/>
<connect gate="G$1" pin="CS" pad="1"/>
<connect gate="G$1" pin="DI" pad="3"/>
<connect gate="G$1" pin="DO" pad="13"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="RST" pad="11"/>
<connect gate="G$1" pin="SCK" pad="2"/>
<connect gate="G$1" pin="SHTDWN" pad="12"/>
<connect gate="G$1" pin="VCC" pad="14"/>
<connect gate="G$1" pin="W0" pad="9"/>
<connect gate="G$1" pin="W1" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MSGEQ7" prefix="IC">
<description>7-band graphic equalizer</description>
<gates>
<gate name="G$1" symbol="MSGEQ7"/>
</gates>
<devices>
<device name="SOIC" package="SOIC8">
<connects>
<connect gate="G$1" pin="AUDIO_IN" pad="5"/>
<connect gate="G$1" pin="CG" pad="6"/>
<connect gate="G$1" pin="CKIN" pad="8"/>
<connect gate="G$1" pin="DCOUT" pad="3"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="RESET" pad="7"/>
<connect gate="G$1" pin="STROBE" pad="4"/>
<connect gate="G$1" pin="VDD" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-10141"/>
</technology>
</technologies>
</device>
<device name="DIL" package="DIL-08">
<connects>
<connect gate="G$1" pin="AUDIO_IN" pad="5"/>
<connect gate="G$1" pin="CG" pad="6"/>
<connect gate="G$1" pin="CKIN" pad="8"/>
<connect gate="G$1" pin="DCOUT" pad="3"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="RESET" pad="7"/>
<connect gate="G$1" pin="STROBE" pad="4"/>
<connect gate="G$1" pin="VDD" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MUX-74HC4067">
<description>16-channel analog MUX</description>
<gates>
<gate name="G$1" symbol="CD74HC4067"/>
</gates>
<devices>
<device name="SMD" package="SSOP24">
<connects>
<connect gate="G$1" pin="CHAN0" pad="9"/>
<connect gate="G$1" pin="CHAN1" pad="8"/>
<connect gate="G$1" pin="CHAN10" pad="21"/>
<connect gate="G$1" pin="CHAN11" pad="20"/>
<connect gate="G$1" pin="CHAN12" pad="19"/>
<connect gate="G$1" pin="CHAN13" pad="18"/>
<connect gate="G$1" pin="CHAN14" pad="17"/>
<connect gate="G$1" pin="CHAN15" pad="16"/>
<connect gate="G$1" pin="CHAN2" pad="7"/>
<connect gate="G$1" pin="CHAN3" pad="6"/>
<connect gate="G$1" pin="CHAN4" pad="5"/>
<connect gate="G$1" pin="CHAN5" pad="4"/>
<connect gate="G$1" pin="CHAN6" pad="3"/>
<connect gate="G$1" pin="CHAN7" pad="2"/>
<connect gate="G$1" pin="CHAN8" pad="23"/>
<connect gate="G$1" pin="CHAN9" pad="22"/>
<connect gate="G$1" pin="COM" pad="1"/>
<connect gate="G$1" pin="EN" pad="15"/>
<connect gate="G$1" pin="GND" pad="12"/>
<connect gate="G$1" pin="S0" pad="10"/>
<connect gate="G$1" pin="S1" pad="11"/>
<connect gate="G$1" pin="S2" pad="14"/>
<connect gate="G$1" pin="S3" pad="13"/>
<connect gate="G$1" pin="VCC" pad="24"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-08252"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MUX-TS3A5017">
<description>Dual-channel 4:1 analog mux</description>
<gates>
<gate name="G$1" symbol="TS3A5017"/>
</gates>
<devices>
<device name="" package="SO16">
<connects>
<connect gate="G$1" pin="1D" pad="7"/>
<connect gate="G$1" pin="1EN" pad="1"/>
<connect gate="G$1" pin="1S1" pad="6"/>
<connect gate="G$1" pin="1S2" pad="5"/>
<connect gate="G$1" pin="1S3" pad="4"/>
<connect gate="G$1" pin="1S4" pad="3"/>
<connect gate="G$1" pin="2D" pad="9"/>
<connect gate="G$1" pin="2EN" pad="15"/>
<connect gate="G$1" pin="2S1" pad="10"/>
<connect gate="G$1" pin="2S2" pad="11"/>
<connect gate="G$1" pin="2S3" pad="12"/>
<connect gate="G$1" pin="2S4" pad="13"/>
<connect gate="G$1" pin="GND" pad="8"/>
<connect gate="G$1" pin="IN1" pad="14"/>
<connect gate="G$1" pin="IN2" pad="2"/>
<connect gate="G$1" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NE555" prefix="IC" uservalue="yes">
<description>&lt;b&gt;General purpose bipolar Timer&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="NE555"/>
</gates>
<devices>
<device name="P" package="DIL-08">
<connects>
<connect gate="G$1" pin="/RES" pad="4"/>
<connect gate="G$1" pin="CON" pad="5"/>
<connect gate="G$1" pin="DIS" pad="7"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="OUT" pad="3"/>
<connect gate="G$1" pin="TRE" pad="6"/>
<connect gate="G$1" pin="TRI" pad="2"/>
<connect gate="G$1" pin="VCC+" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="Arrow Electronics"/>
<attribute name="MPN" value="NE555N"/>
<attribute name="OC_FARNELL" value="1467742"/>
<attribute name="OC_NEWARK" value="89K1486"/>
</technology>
</technologies>
</device>
<device name="D" package="SO08">
<connects>
<connect gate="G$1" pin="/RES" pad="4"/>
<connect gate="G$1" pin="CON" pad="5"/>
<connect gate="G$1" pin="DIS" pad="7"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="OUT" pad="3"/>
<connect gate="G$1" pin="TRE" pad="6"/>
<connect gate="G$1" pin="TRI" pad="2"/>
<connect gate="G$1" pin="VCC+" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="KIT" package="DIP08-KIT">
<connects>
<connect gate="G$1" pin="/RES" pad="4"/>
<connect gate="G$1" pin="CON" pad="5"/>
<connect gate="G$1" pin="DIS" pad="7"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="OUT" pad="3"/>
<connect gate="G$1" pin="TRE" pad="6"/>
<connect gate="G$1" pin="TRI" pad="2"/>
<connect gate="G$1" pin="VCC+" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-11930"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OPA344">
<description>Single gate rail-to-rail output op-amp. Inputs extend 300mV past rails.</description>
<gates>
<gate name="G$1" symbol="OP-AMP+-"/>
</gates>
<devices>
<device name="" package="SOT23-5">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="4"/>
<connect gate="G$1" pin="OUT" pad="1"/>
<connect gate="G$1" pin="V+" pad="5"/>
<connect gate="G$1" pin="V-" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-08251"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OPAMP-DUAL" prefix="IC">
<description>Generic op-amp footprint</description>
<gates>
<gate name="A" symbol="OP-AMP+-"/>
<gate name="B" symbol="OP-AMP"/>
</gates>
<devices>
<device name="U" package="SO08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="" package="DIP08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
</connects>
<technologies>
<technology name="DIP"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PCM1803" prefix="U">
<description>24-bit ADC</description>
<gates>
<gate name="G$1" symbol="PCM1803A"/>
</gates>
<devices>
<device name="SMD" package="SSOP20">
<connects>
<connect gate="G$1" pin="BCK" pad="11"/>
<connect gate="G$1" pin="BPAS" pad="8"/>
<connect gate="G$1" pin="DOUT" pad="12"/>
<connect gate="G$1" pin="FMT0" pad="17"/>
<connect gate="G$1" pin="FMT1" pad="18"/>
<connect gate="G$1" pin="GNDA" pad="6"/>
<connect gate="G$1" pin="GNDD" pad="13"/>
<connect gate="G$1" pin="LRCK" pad="10"/>
<connect gate="G$1" pin="MD0" pad="19"/>
<connect gate="G$1" pin="MD1" pad="20"/>
<connect gate="G$1" pin="OSR" pad="16"/>
<connect gate="G$1" pin="PDWN" pad="7"/>
<connect gate="G$1" pin="SCK" pad="15"/>
<connect gate="G$1" pin="TEST" pad="9"/>
<connect gate="G$1" pin="VCCA" pad="5"/>
<connect gate="G$1" pin="VDD" pad="14"/>
<connect gate="G$1" pin="VINL" pad="1"/>
<connect gate="G$1" pin="VINR" pad="2"/>
<connect gate="G$1" pin="VREF1" pad="3"/>
<connect gate="G$1" pin="VREF2" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SV74LV4052APWR">
<description>Dual 4:1 analog mux</description>
<gates>
<gate name="G$1" symbol="SN74LV4052APWR"/>
</gates>
<devices>
<device name="" package="TSSOP16">
<connects>
<connect gate="G$1" pin="1-COM" pad="13"/>
<connect gate="G$1" pin="1Y0" pad="12"/>
<connect gate="G$1" pin="1Y1" pad="14"/>
<connect gate="G$1" pin="1Y2" pad="15"/>
<connect gate="G$1" pin="1Y3" pad="11"/>
<connect gate="G$1" pin="2-COM" pad="3"/>
<connect gate="G$1" pin="2Y0" pad="1"/>
<connect gate="G$1" pin="2Y1" pad="5"/>
<connect gate="G$1" pin="2Y2" pad="2"/>
<connect gate="G$1" pin="2Y3" pad="4"/>
<connect gate="G$1" pin="A" pad="10"/>
<connect gate="G$1" pin="B" pad="9"/>
<connect gate="G$1" pin="GND@8" pad="8"/>
<connect gate="G$1" pin="GNG@7" pad="7"/>
<connect gate="G$1" pin="INH" pad="6"/>
<connect gate="G$1" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="2" package="TVSOP-16">
<connects>
<connect gate="G$1" pin="1-COM" pad="P$13"/>
<connect gate="G$1" pin="1Y0" pad="P$12"/>
<connect gate="G$1" pin="1Y1" pad="P$14"/>
<connect gate="G$1" pin="1Y2" pad="P$15"/>
<connect gate="G$1" pin="1Y3" pad="P$11"/>
<connect gate="G$1" pin="2-COM" pad="P$3"/>
<connect gate="G$1" pin="2Y0" pad="P$1"/>
<connect gate="G$1" pin="2Y1" pad="P$5"/>
<connect gate="G$1" pin="2Y2" pad="P$2"/>
<connect gate="G$1" pin="2Y3" pad="P$4"/>
<connect gate="G$1" pin="A" pad="P$10"/>
<connect gate="G$1" pin="B" pad="P$9"/>
<connect gate="G$1" pin="GND@8" pad="P$8"/>
<connect gate="G$1" pin="GNG@7" pad="P$7"/>
<connect gate="G$1" pin="INH" pad="P$6"/>
<connect gate="G$1" pin="VCC" pad="P$16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TVP5150-NTSC_DECODER">
<description>Texas Instrument NTSC/PAL Decoder
TI Part #TVP5150AM1
*** UNPROVEN FOOTPRINT ***

Decodes NTSC video signal to YCbCr 4:2:2 signal</description>
<gates>
<gate name="G$1" symbol="TVP5150-NTSC_DECODER-1"/>
</gates>
<devices>
<device name="" package="TQFP32-5MM">
<connects>
<connect gate="G$1" pin="AGND" pad="7"/>
<connect gate="G$1" pin="AIP1A" pad="1"/>
<connect gate="G$1" pin="AIP1B" pad="2"/>
<connect gate="G$1" pin="AVID" pad="26"/>
<connect gate="G$1" pin="CH_AGND" pad="31"/>
<connect gate="G$1" pin="CH_AVDD" pad="32"/>
<connect gate="G$1" pin="DGND" pad="19"/>
<connect gate="G$1" pin="DVDD" pad="20"/>
<connect gate="G$1" pin="FID/GLCO" pad="23"/>
<connect gate="G$1" pin="HSYNC" pad="25"/>
<connect gate="G$1" pin="INT_REQ" pad="27"/>
<connect gate="G$1" pin="IO_DVDD" pad="10"/>
<connect gate="G$1" pin="PCLK/SCLK" pad="9"/>
<connect gate="G$1" pin="PDN" pad="28"/>
<connect gate="G$1" pin="PLL_AGND" pad="3"/>
<connect gate="G$1" pin="PLL_AVDD" pad="4"/>
<connect gate="G$1" pin="REFM" pad="30"/>
<connect gate="G$1" pin="REFP" pad="29"/>
<connect gate="G$1" pin="RESET/" pad="8"/>
<connect gate="G$1" pin="SCL" pad="21"/>
<connect gate="G$1" pin="SDA" pad="22"/>
<connect gate="G$1" pin="VSYNC" pad="24"/>
<connect gate="G$1" pin="XTAL1" pad="5"/>
<connect gate="G$1" pin="XTAL2" pad="6"/>
<connect gate="G$1" pin="YOUT_0" pad="18"/>
<connect gate="G$1" pin="YOUT_1" pad="17"/>
<connect gate="G$1" pin="YOUT_2" pad="16"/>
<connect gate="G$1" pin="YOUT_3" pad="15"/>
<connect gate="G$1" pin="YOUT_4" pad="14"/>
<connect gate="G$1" pin="YOUT_5" pad="13"/>
<connect gate="G$1" pin="YOUT_6" pad="12"/>
<connect gate="G$1" pin="YOUT_7" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="X9015_DIGI_POT">
<description>Digital pot- up/down/increment control only</description>
<gates>
<gate name="G$1" symbol="X9015_DIGI_POT"/>
</gates>
<devices>
<device name="S" package="SO08">
<connects>
<connect gate="G$1" pin="CS'" pad="7"/>
<connect gate="G$1" pin="INC'" pad="1"/>
<connect gate="G$1" pin="RH/VH" pad="3"/>
<connect gate="G$1" pin="RL/VL" pad="6"/>
<connect gate="G$1" pin="RW/VW" pad="5"/>
<connect gate="G$1" pin="U/D'" pad="2"/>
<connect gate="G$1" pin="VCC" pad="8"/>
<connect gate="G$1" pin="VSS" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74HC4051_MUX">
<description>8:1 analog mux</description>
<gates>
<gate name="G$1" symbol="74HC4051_MUX"/>
</gates>
<devices>
<device name="" package="SO16">
<connects>
<connect gate="G$1" pin="A" pad="11"/>
<connect gate="G$1" pin="B" pad="10"/>
<connect gate="G$1" pin="C" pad="9"/>
<connect gate="G$1" pin="INH" pad="6"/>
<connect gate="G$1" pin="IO" pad="3"/>
<connect gate="G$1" pin="IO0" pad="13"/>
<connect gate="G$1" pin="IO1" pad="14"/>
<connect gate="G$1" pin="IO2" pad="15"/>
<connect gate="G$1" pin="IO3" pad="12"/>
<connect gate="G$1" pin="IO4" pad="1"/>
<connect gate="G$1" pin="IO5" pad="5"/>
<connect gate="G$1" pin="IO6" pad="2"/>
<connect gate="G$1" pin="IO7" pad="4"/>
<connect gate="G$1" pin="VDD" pad="16"/>
<connect gate="G$1" pin="VEE" pad="7"/>
<connect gate="G$1" pin="VSS" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74HC4052" prefix="U">
<description>Dual 4:1 analog mux</description>
<gates>
<gate name="G$1" symbol="74HC4052"/>
</gates>
<devices>
<device name="SO" package="SO16">
<connects>
<connect gate="G$1" pin="A" pad="10"/>
<connect gate="G$1" pin="B" pad="9"/>
<connect gate="G$1" pin="GND" pad="8"/>
<connect gate="G$1" pin="INH" pad="6"/>
<connect gate="G$1" pin="VCC" pad="16"/>
<connect gate="G$1" pin="VEE" pad="7"/>
<connect gate="G$1" pin="X" pad="13"/>
<connect gate="G$1" pin="X0" pad="12"/>
<connect gate="G$1" pin="X1" pad="14"/>
<connect gate="G$1" pin="X2" pad="15"/>
<connect gate="G$1" pin="X3" pad="11"/>
<connect gate="G$1" pin="Y" pad="3"/>
<connect gate="G$1" pin="Y0" pad="1"/>
<connect gate="G$1" pin="Y1" pad="5"/>
<connect gate="G$1" pin="Y2" pad="2"/>
<connect gate="G$1" pin="Y3" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-09813"/>
<attribute name="VALUE" value="74HC4052"/>
</technology>
</technologies>
</device>
<device name="DIP" package="DIL16">
<connects>
<connect gate="G$1" pin="A" pad="10"/>
<connect gate="G$1" pin="B" pad="9"/>
<connect gate="G$1" pin="GND" pad="8"/>
<connect gate="G$1" pin="INH" pad="6"/>
<connect gate="G$1" pin="VCC" pad="16"/>
<connect gate="G$1" pin="VEE" pad="7"/>
<connect gate="G$1" pin="X" pad="13"/>
<connect gate="G$1" pin="X0" pad="12"/>
<connect gate="G$1" pin="X1" pad="14"/>
<connect gate="G$1" pin="X2" pad="15"/>
<connect gate="G$1" pin="X3" pad="11"/>
<connect gate="G$1" pin="Y" pad="3"/>
<connect gate="G$1" pin="Y0" pad="1"/>
<connect gate="G$1" pin="Y1" pad="5"/>
<connect gate="G$1" pin="Y2" pad="2"/>
<connect gate="G$1" pin="Y3" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74VHC4052_ANALOG_MUX" prefix="U">
<description>Dual 4:1 analog mux</description>
<gates>
<gate name="G$1" symbol="74VHC4052_ANALOG_MUX"/>
</gates>
<devices>
<device name="" package="TSSOP16">
<connects>
<connect gate="G$1" pin="A" pad="10"/>
<connect gate="G$1" pin="B" pad="9"/>
<connect gate="G$1" pin="GND" pad="8"/>
<connect gate="G$1" pin="IN/OUT_X" pad="13"/>
<connect gate="G$1" pin="IN/OUT_Y" pad="3"/>
<connect gate="G$1" pin="INH" pad="6"/>
<connect gate="G$1" pin="VCC" pad="16"/>
<connect gate="G$1" pin="VEE" pad="7"/>
<connect gate="G$1" pin="X0" pad="12"/>
<connect gate="G$1" pin="X1" pad="14"/>
<connect gate="G$1" pin="X2" pad="15"/>
<connect gate="G$1" pin="X3" pad="11"/>
<connect gate="G$1" pin="Y0" pad="1"/>
<connect gate="G$1" pin="Y1" pad="5"/>
<connect gate="G$1" pin="Y2" pad="2"/>
<connect gate="G$1" pin="Y3" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="556" prefix="IC" uservalue="yes">
<description>Dual timer circuit (2 555 timers in one package)</description>
<gates>
<gate name="G$1" symbol="556_TIMER_DUAL"/>
</gates>
<devices>
<device name="" package="DIL14">
<connects>
<connect gate="G$1" pin="CV" pad="3"/>
<connect gate="G$1" pin="CV2" pad="11"/>
<connect gate="G$1" pin="DIS" pad="1"/>
<connect gate="G$1" pin="DIS2" pad="13"/>
<connect gate="G$1" pin="GND" pad="7"/>
<connect gate="G$1" pin="OUT" pad="5"/>
<connect gate="G$1" pin="OUT2" pad="9"/>
<connect gate="G$1" pin="RST" pad="4"/>
<connect gate="G$1" pin="RST2" pad="10"/>
<connect gate="G$1" pin="THR" pad="2"/>
<connect gate="G$1" pin="THR2" pad="12"/>
<connect gate="G$1" pin="TRIG" pad="6"/>
<connect gate="G$1" pin="TRIG2" pad="8"/>
<connect gate="G$1" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="KIT" package="DIL14-KIT">
<connects>
<connect gate="G$1" pin="CV" pad="3"/>
<connect gate="G$1" pin="CV2" pad="11"/>
<connect gate="G$1" pin="DIS" pad="1"/>
<connect gate="G$1" pin="DIS2" pad="13"/>
<connect gate="G$1" pin="GND" pad="7"/>
<connect gate="G$1" pin="OUT" pad="5"/>
<connect gate="G$1" pin="OUT2" pad="9"/>
<connect gate="G$1" pin="RST" pad="4"/>
<connect gate="G$1" pin="RST2" pad="10"/>
<connect gate="G$1" pin="THR" pad="2"/>
<connect gate="G$1" pin="THR2" pad="12"/>
<connect gate="G$1" pin="TRIG" pad="6"/>
<connect gate="G$1" pin="TRIG2" pad="8"/>
<connect gate="G$1" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="VALUE" value="556"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM386" prefix="U">
<description>low voltage audio power amplifier</description>
<gates>
<gate name="G$1" symbol="OP-AMP+-FULL"/>
</gates>
<devices>
<device name="" package="DIP08">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="BP" pad="7"/>
<connect gate="G$1" pin="GAIN@1" pad="1"/>
<connect gate="G$1" pin="GAIN@8" pad="8"/>
<connect gate="G$1" pin="OUT" pad="5"/>
<connect gate="G$1" pin="V+" pad="6"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LTC6244">
<description>Low-noise, high-speed rail-to-rail CMOS op-amp</description>
<gates>
<gate name="G1" symbol="LTC6244"/>
<gate name="G2" symbol="LTC6244_2"/>
</gates>
<devices>
<device name="" package="MSOP8">
<connects>
<connect gate="G1" pin="+IN" pad="3"/>
<connect gate="G1" pin="+V" pad="8"/>
<connect gate="G1" pin="-IN" pad="2"/>
<connect gate="G1" pin="-V" pad="4"/>
<connect gate="G1" pin="OUT" pad="1"/>
<connect gate="G2" pin="+IN" pad="5"/>
<connect gate="G2" pin="-IN" pad="6"/>
<connect gate="G2" pin="OUT" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="INA139" prefix="U" uservalue="yes">
<description>High-side shunt current sense&lt;BR&gt;
2.7V-40V, 1%</description>
<gates>
<gate name="G$1" symbol="INA139"/>
</gates>
<devices>
<device name="" package="SOT23-5">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="OUT" pad="1"/>
<connect gate="G$1" pin="V+" pad="5"/>
<connect gate="G$1" pin="VIN+" pad="3"/>
<connect gate="G$1" pin="VIN-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TPA6138A2">
<description>&lt;H3&gt;Headphone driver amp&lt;/h3&gt;&lt;p&gt;
Differential to single-ended audio amplifier.</description>
<gates>
<gate name="G$1" symbol="TPA6138A2"/>
</gates>
<devices>
<device name="" package="TSSOP-14">
<connects>
<connect gate="G$1" pin="!MUTE" pad="5"/>
<connect gate="G$1" pin="CN" pad="7"/>
<connect gate="G$1" pin="CP" pad="8"/>
<connect gate="G$1" pin="GND" pad="4 10"/>
<connect gate="G$1" pin="INL+" pad="14"/>
<connect gate="G$1" pin="INL-" pad="13"/>
<connect gate="G$1" pin="INR+" pad="1"/>
<connect gate="G$1" pin="INR-" pad="2"/>
<connect gate="G$1" pin="OUTL" pad="12"/>
<connect gate="G$1" pin="OUTR" pad="3"/>
<connect gate="G$1" pin="UVP" pad="11"/>
<connect gate="G$1" pin="VDD" pad="9"/>
<connect gate="G$1" pin="VSS" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TPA2005D1" prefix="U">
<description>&lt;b&gt;1.4W MONO CLASS-D AUDIO POWER AMPLIFIER&lt;/b&gt;&lt;p&gt;

The TPA2005D1 is a 1.4-W high efficiency filter-free class-D audio power amplifier in a BGA, QFN, or MSOP package that requires only three external components.&lt;p&gt;
Datasheet: &lt;href="http://focus.ti.com/lit/ds/symlink/tpa2005d1.pdf"&gt;http://focus.ti.com/lit/ds/symlink/tpa2005d1.pdf&lt;/a&gt;
&lt;ul&gt;
&lt;li&gt;1.4 W Into 8 ? From a 5V Supply at THD = 10% (Typ)&lt;/li&gt;
&lt;li&gt;Maximum Battery Life and Minimum Heat&lt;/li&gt;
&lt;li&gt;Efficiency With an 8-? Speaker: 84% at 400 mW, 79% at 100 mW&lt;/li&gt;
&lt;li&gt;2.8-mA Quiescent Current&lt;/li&gt;
&lt;li&gt;0.5-mA Shutdown Current&lt;/li&gt;
&lt;li&gt;Ideal for Wireless or Cellular Handsets and PDAs&lt;/li&gt;
&lt;li&gt;Capable of Driving an 8-? Speaker (2.5 V ? VDD ? 5.5 V) and a 4-? Speaker (2.5 V ? VDD ? 4.2 V)&lt;/li&gt;
&lt;li&gt;Only Three External Components&lt;/li&gt;
&lt;li&gt;Optimized PWM Output Stage Eliminates LC Output Filter&lt;/li&gt;
&lt;li&gt;Internally Generated 250-kHz Switching Frequency Eliminates Capacitor and Resistor&lt;/li&gt;
&lt;li&gt;Improved PSRR (-71 dB at 217 Hz) and Wide Supply Voltage (2.5 V to 5.5 V) Eliminates Need for a Voltage Regulator&lt;/li&gt;
&lt;li&gt;Fully Differential Design Reduces RF Rectification and Eliminates Bypass Capacitor&lt;/li&gt;
&lt;li&gt;Improved CMRR Eliminates Two Input Coupling Capacitors&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="TPA2005D1"/>
</gates>
<devices>
<device name="DGN" package="POWER-SOP8">
<connects>
<connect gate="G$1" pin="GND@1" pad="7"/>
<connect gate="G$1" pin="GND@2" pad="9"/>
<connect gate="G$1" pin="IN+" pad="3"/>
<connect gate="G$1" pin="IN-" pad="4"/>
<connect gate="G$1" pin="OUT+" pad="5"/>
<connect gate="G$1" pin="OUT-" pad="8"/>
<connect gate="G$1" pin="SHUTDOWN" pad="1"/>
<connect gate="G$1" pin="VDD" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="DRB" package="QFN-8_PAD">
<connects>
<connect gate="G$1" pin="GND@1" pad="7"/>
<connect gate="G$1" pin="GND@2" pad="9 10 11 12 13"/>
<connect gate="G$1" pin="IN+" pad="3"/>
<connect gate="G$1" pin="IN-" pad="4"/>
<connect gate="G$1" pin="OUT+" pad="5"/>
<connect gate="G$1" pin="OUT-" pad="8"/>
<connect gate="G$1" pin="SHUTDOWN" pad="1"/>
<connect gate="G$1" pin="VDD" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HIH6131">
<gates>
<gate name="G$1" symbol="HIH6131"/>
</gates>
<devices>
<device name="" package="SOIC8">
<connects>
<connect gate="G$1" pin="AL_H" pad="5"/>
<connect gate="G$1" pin="AL_L" pad="6"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="NC" pad="7"/>
<connect gate="G$1" pin="SCL" pad="3"/>
<connect gate="G$1" pin="SDA" pad="4"/>
<connect gate="G$1" pin="VCORE" pad="1"/>
<connect gate="G$1" pin="VDD" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="INA169" prefix="U">
<gates>
<gate name="G$1" symbol="INA169"/>
</gates>
<devices>
<device name="" package="SOT23-5">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="OUT" pad="1"/>
<connect gate="G$1" pin="V+" pad="5"/>
<connect gate="G$1" pin="VIN+" pad="3"/>
<connect gate="G$1" pin="VIN-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TPA6111" prefix="U">
<description>TPA6111A2: Basic 150mW stereo headphone amplifier.</description>
<gates>
<gate name="G$1" symbol="TPA6111"/>
</gates>
<devices>
<device name="SMD-T" package="SO08-TIGHT">
<connects>
<connect gate="G$1" pin="BYP" pad="3"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="IN1" pad="2"/>
<connect gate="G$1" pin="IN2" pad="6"/>
<connect gate="G$1" pin="SHT" pad="5"/>
<connect gate="G$1" pin="VDD" pad="8"/>
<connect gate="G$1" pin="VO1" pad="1"/>
<connect gate="G$1" pin="VO2" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-10149"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADC8045" prefix="U" uservalue="yes">
<description>Unity-gain stable feedback amplifier.&lt;br&gt;
Low noise, low distortion, 1GHz BW.</description>
<gates>
<gate name="G$1" symbol="ADC8045"/>
</gates>
<devices>
<device name="" package="SO08">
<connects>
<connect gate="G$1" pin="FB" pad="1"/>
<connect gate="G$1" pin="IN+" pad="3"/>
<connect gate="G$1" pin="IN-" pad="2"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="VDD" pad="7"/>
<connect gate="G$1" pin="VSS" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-11224"/>
<attribute name="VALUE" value="ADC8045"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD9837">
<description>Programmable waveform generator, sine, triangular, and square wave outputs.</description>
<gates>
<gate name="G1" symbol="AD9837"/>
</gates>
<devices>
<device name="" package="AD9837">
<connects>
<connect gate="G1" pin="AGND" pad="P$9"/>
<connect gate="G1" pin="CAP/2.5V" pad="P$3"/>
<connect gate="G1" pin="COMP" pad="P$1"/>
<connect gate="G1" pin="DGND" pad="P$0 P$4"/>
<connect gate="G1" pin="FSYNC" pad="P$8"/>
<connect gate="G1" pin="MCLK" pad="P$5"/>
<connect gate="G1" pin="SCLK" pad="P$7"/>
<connect gate="G1" pin="SDATA" pad="P$6"/>
<connect gate="G1" pin="VDD" pad="P$2"/>
<connect gate="G1" pin="VOUT" pad="P$10"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-11223"/>
<attribute name="VALUE" value="AD9837BCPZ"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MCP6291" prefix="U">
<description>Rail to rail OpAmp with 10MHz GBP</description>
<gates>
<gate name="G$1" symbol="OP-AMP+-"/>
</gates>
<devices>
<device name="T-E/OT" package="SOT23-5">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="4"/>
<connect gate="G$1" pin="OUT" pad="1"/>
<connect gate="G$1" pin="V+" pad="5"/>
<connect gate="G$1" pin="V-" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-11991"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TS3USB221A" prefix="U" uservalue="yes">
<description>DPDT Analog Mux&lt;br&gt;
Vcc 2.5 to 3.3V&lt;br&gt;
Passes up to 5.5V at 3.3V supply&lt;br&gt;
900MHz BW, 6&amp;#8486; switch resistance</description>
<gates>
<gate name="G$1" symbol="TS3USB221A"/>
</gates>
<devices>
<device name="" package="QFN-10-RSE">
<connects>
<connect gate="G$1" pin="!OE" pad="6"/>
<connect gate="G$1" pin="1D+" pad="1"/>
<connect gate="G$1" pin="1D-" pad="2"/>
<connect gate="G$1" pin="2D+" pad="3"/>
<connect gate="G$1" pin="2D-" pad="4"/>
<connect gate="G$1" pin="D+" pad="8"/>
<connect gate="G$1" pin="D-" pad="7"/>
<connect gate="G$1" pin="S" pad="9"/>
<connect gate="G$1" pin="VCC" pad="10"/>
<connect gate="G$1" pin="VSS" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-12115"/>
<attribute name="VALUE" value="TS3USB221A"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM339" prefix="U">
<description>
&lt;p&gt;Based on information from the SLCS006N datasheet from TI (www.ti.com).&lt;/p&gt;
&lt;table align=center&gt;
  &lt;tr&gt;&lt;td&gt;&lt;h2&gt;Change Log&lt;/h2&gt;&lt;/td&gt;&lt;/tr&gt;
  &lt;tr&gt;
    &lt;th&gt;Date&lt;/th&gt;&lt;th&gt;Author&lt;/th&gt;&lt;th&gt;Change&lt;/th&gt;
  &lt;/tr&gt;
  &lt;tr&gt;
    &lt;td&gt;July 16, 2008&lt;/td&gt;&lt;td&gt;nick@scantool.net&lt;/td&gt;&lt;td&gt;Device created.&lt;/td&gt;
  &lt;/tr&gt;
&lt;/table&gt;</description>
<gates>
<gate name="B" symbol="LM339"/>
<gate name="A" symbol="LM339"/>
<gate name="C" symbol="LM339"/>
<gate name="D" symbol="LM339"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="" package="TSSOP-14">
<connects>
<connect gate="A" pin="+IN" pad="7"/>
<connect gate="A" pin="-IN" pad="6"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="4"/>
<connect gate="B" pin="OUT" pad="2"/>
<connect gate="C" pin="+IN" pad="9"/>
<connect gate="C" pin="-IN" pad="8"/>
<connect gate="C" pin="OUT" pad="14"/>
<connect gate="D" pin="+IN" pad="11"/>
<connect gate="D" pin="-IN" pad="10"/>
<connect gate="D" pin="OUT" pad="13"/>
<connect gate="P" pin="GND" pad="12"/>
<connect gate="P" pin="VCC" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DESC" value="IC, Quad Comparator"/>
<attribute name="MANUF" value="Texas Instruments"/>
<attribute name="PARTNUM" value="LM339PWR"/>
<attribute name="SUPPLIER" value="Digikey:296-6607-1-ND"/>
<attribute name="VALSTAT" value="PARTNUM"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD8232">
<gates>
<gate name="U$1" symbol="AD8232"/>
</gates>
<devices>
<device name="" package="LFCSP_20">
<connects>
<connect gate="U$1" pin="!SDN" pad="13"/>
<connect gate="U$1" pin="+IN" pad="2"/>
<connect gate="U$1" pin="+VS" pad="17"/>
<connect gate="U$1" pin="-IN" pad="3"/>
<connect gate="U$1" pin="AC/!DC" pad="14"/>
<connect gate="U$1" pin="FR" pad="15"/>
<connect gate="U$1" pin="GND" pad="16"/>
<connect gate="U$1" pin="GND_PAD" pad="PAD"/>
<connect gate="U$1" pin="HPDRIVE" pad="1"/>
<connect gate="U$1" pin="HPSENSE" pad="20"/>
<connect gate="U$1" pin="IAOUT" pad="19"/>
<connect gate="U$1" pin="LO+" pad="12"/>
<connect gate="U$1" pin="LO-" pad="11"/>
<connect gate="U$1" pin="OPAMP+" pad="7"/>
<connect gate="U$1" pin="OPAMP-" pad="9"/>
<connect gate="U$1" pin="OUT" pad="10"/>
<connect gate="U$1" pin="REFIN" pad="18"/>
<connect gate="U$1" pin="REFOUT" pad="8"/>
<connect gate="U$1" pin="RLD" pad="5"/>
<connect gate="U$1" pin="RLDFB" pad="4"/>
<connect gate="U$1" pin="SW" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-11886"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADS1015" prefix="U" uservalue="yes">
<description>12-Bit Del-Sig ADC&lt;br&gt;
Four single-ended inputs or two differential inputs&lt;br&gt;
Internal PGA&lt;br&gt;
I&lt;sup&gt;2&lt;/sup&gt;C interface&lt;br&gt;
2.0-5.5V</description>
<gates>
<gate name="G$1" symbol="ADS1015"/>
</gates>
<devices>
<device name="" package="MSOP10">
<connects>
<connect gate="G$1" pin="ADDR" pad="1"/>
<connect gate="G$1" pin="AIN0" pad="4"/>
<connect gate="G$1" pin="AIN1" pad="5"/>
<connect gate="G$1" pin="AIN2" pad="6"/>
<connect gate="G$1" pin="AIN3" pad="7"/>
<connect gate="G$1" pin="ALERT/RDY" pad="2"/>
<connect gate="G$1" pin="SCL" pad="10"/>
<connect gate="G$1" pin="SDA" pad="9"/>
<connect gate="G$1" pin="VDD" pad="8"/>
<connect gate="G$1" pin="VSS" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-12239"/>
<attribute name="VALUE" value="ADS1015"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD5262">
<gates>
<gate name="1" symbol="AD5262"/>
</gates>
<devices>
<device name="" package="SSOP16">
<connects>
<connect gate="1" pin="A1" pad="2"/>
<connect gate="1" pin="A2" pad="16"/>
<connect gate="1" pin="B1" pad="4"/>
<connect gate="1" pin="B2" pad="14"/>
<connect gate="1" pin="CLK" pad="7"/>
<connect gate="1" pin="CS_N" pad="9"/>
<connect gate="1" pin="GND" pad="11"/>
<connect gate="1" pin="PR_N" pad="10"/>
<connect gate="1" pin="SDI" pad="8"/>
<connect gate="1" pin="SDO" pad="1"/>
<connect gate="1" pin="SHDN_N" pad="6"/>
<connect gate="1" pin="VDD" pad="5"/>
<connect gate="1" pin="VL" pad="13"/>
<connect gate="1" pin="VSS" pad="12"/>
<connect gate="1" pin="W1" pad="3"/>
<connect gate="1" pin="W2" pad="15"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-12358"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MCP6021">
<description>Rail-to-rail input/output op-amp with 10 MHz bandwidth.</description>
<gates>
<gate name="G$1" symbol="OP-AMP+-"/>
</gates>
<devices>
<device name="T-E/OT" package="SOT23-5">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="4"/>
<connect gate="G$1" pin="OUT" pad="1"/>
<connect gate="G$1" pin="V+" pad="5"/>
<connect gate="G$1" pin="V-" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-12504"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX6675" prefix="U">
<description>&lt;b&gt;Cold-Junction-Compensated K-Thermocoupleto-Digital
Converter (0°C to +1024°C)&lt;br/&gt;&lt;/b&gt;
The MAX6675 performs cold-junction compensation
and digitizes the signal from a type-K thermocouple.&lt;br/&gt;
The data is output in a 12-bit resolution, SPI™-compatible,
read-only format.&lt;br/&gt;
This converter resolves temperatures to 0.25°C, allows readings as high as +1024°C, and exhibits thermocouple accuracy of 8LSBs for temperatures ranging from 0°C to +700°C.</description>
<gates>
<gate name="G$1" symbol="MAX6675"/>
</gates>
<devices>
<device name="" package="SOIC8">
<connects>
<connect gate="G$1" pin="!CS" pad="6"/>
<connect gate="G$1" pin="(MI)SO" pad="7"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="SCK" pad="5"/>
<connect gate="G$1" pin="T+" pad="3"/>
<connect gate="G$1" pin="T-" pad="2"/>
<connect gate="G$1" pin="VCC" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-12512"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX31855K" prefix="U">
<description>&lt;b&gt;Cold-Junction-Compensated K-Thermocoupleto-Digital
Converter (-270°C to +1800°C)&lt;br/&gt;&lt;/b&gt;
The MAX31855K performs cold-junction compensation
and digitizes the signal from a type-K thermocouple.&lt;br/&gt;
The data is output in a 14-bit resolution, SPI™-compatible,
read-only format.&lt;br/&gt;
This converter resolves temperatures to 0.25°C, allows readings as high as +1800°C and as low as -270°C, and exhibits thermocouple accuracy of ±2°C for temperatures ranging from -200°C to +700°C for K-type thermocouples.</description>
<gates>
<gate name="G$1" symbol="MAX6675"/>
</gates>
<devices>
<device name="" package="SOIC8">
<connects>
<connect gate="G$1" pin="!CS" pad="6"/>
<connect gate="G$1" pin="(MI)SO" pad="7"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="SCK" pad="5"/>
<connect gate="G$1" pin="T+" pad="3"/>
<connect gate="G$1" pin="T-" pad="2"/>
<connect gate="G$1" pin="VCC" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="GENERIC-SOIC8" prefix="U">
<description>A placeholder for generic narrow &amp; wide SOIC8 foorptints - used on the DIP adapter board.</description>
<gates>
<gate name="G$1" symbol="GENERIC-8PIN"/>
</gates>
<devices>
<device name="" package="SO08-UNIVERSAL">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="MSGEQ7N-FILTER" package="SO08">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-10141"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TL431" prefix="U">
<description>Precision Programmable Reference</description>
<gates>
<gate name="G$1" symbol="TL431"/>
</gates>
<devices>
<device name="PTH" package="TO-92">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="C" pad="3"/>
<connect gate="G$1" pin="R" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD627" prefix="U">
<description>Hall-effect-based isolated linear current sensor</description>
<gates>
<gate name="U1" symbol="AD627"/>
</gates>
<devices>
<device name="SOIC" package="SO08-TIGHT">
<connects>
<connect gate="U1" pin="IN+" pad="3"/>
<connect gate="U1" pin="IN-" pad="2"/>
<connect gate="U1" pin="OUTPUT" pad="6"/>
<connect gate="U1" pin="REF" pad="5"/>
<connect gate="U1" pin="RG@1" pad="1"/>
<connect gate="U1" pin="RG@8" pad="8"/>
<connect gate="U1" pin="VS+" pad="7"/>
<connect gate="U1" pin="VS-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-13132"/>
<attribute name="VALUE" value="AD627"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD8607" prefix="U">
<gates>
<gate name="A" symbol="OP-AMP+--2"/>
<gate name="B" symbol="OP-AMP-1-1"/>
</gates>
<devices>
<device name="" package="SO08-TIGHT">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-13133"/>
<attribute name="VALUE" value="AD8607"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SN74LVC1G66_SPST_AMUX" prefix="U" uservalue="yes">
<description>SPST NO Analog Switch &lt;br&gt;
10-Ohm on resistance &lt;br&gt;
1.65-5.5V</description>
<gates>
<gate name="G$1" symbol="SN74LVC1G66_SPST_AMUX"/>
</gates>
<devices>
<device name="" package="SOT23-5">
<connects>
<connect gate="G$1" pin="A_IN" pad="1"/>
<connect gate="G$1" pin="A_OUT" pad="2"/>
<connect gate="G$1" pin="CTRL_IN" pad="4"/>
<connect gate="G$1" pin="VCC" pad="5"/>
<connect gate="G$1" pin="VSS" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-13549"/>
<attribute name="VALUE" value="SN74LVC1G66"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
