<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.3.0">
<drawing>
<library>
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find crystals and oscillators and other things that go "tick".&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="HC49U-V">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
<package name="TC38H">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
<package name="TC26H_KIT">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
<package name="TC26H">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
<package name="HC49UP">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
<package name="HC49US">
<description>&lt;B&gt;CRYSTAL&lt;/B&gt;</description>
</package>
<package name="CRYSTAL-32KHZ-SMD-MELF">
</package>
<package name="CRYSTAL-SMD-5X3">
</package>
<package name="TC26HEZ">
<description>32kHz crystal package&lt;br&gt;
This is the "EZ" version, which has limited top masking for improved ease of assembly.</description>
</package>
<package name="CRYSTAL-32KHZ-SMD_EPSON_MC146">
</package>
<package name="CRYSTAL-SMD-10.5X4.8-2PIN">
</package>
<package name="SO08">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt; Fits JEDEC packages (narrow SOIC-8)</description>
</package>
<package name="DS3234">
</package>
<package name="CRYSTAL-SMD-7X5">
</package>
<package name="CRYSTAL-SMD-7.5X5.2-6PIN">
<description>FXO-HC73 Series Oscillator. 7.5x5.2mm 6-pin package</description>
</package>
<package name="CRYSTAL-OSC-SMD-5X3">
</package>
<package name="RESONATOR-PTH">
</package>
<package name="RESONATOR-WIDE-SMD">
</package>
<package name="RESONATOR_NOCAP">
</package>
<package name="SIT8002">
</package>
<package name="CRYSTAL-TXC-7A">
</package>
<package name="SO08-TIGHT">
</package>
<package name="RESONATOR-SMD">
</package>
<package name="RESONATOR-SMD_MED">
</package>
<package name="CRYSTAL-OSC-SMD-5X3.2">
</package>
<package name="CRYSTAL-SMD-3.2X1.5MM">
<description>&lt;h3&gt;3.2 x 1.5mm Crystal Package&lt;/h3&gt;
&lt;p&gt;e.g: &lt;a href="http://www.sii.co.jp/en/quartz/files/2013/03/file_PRODUCT_MASTER_50812_GRAPHIC03.pdf"&gt;SX-32S&lt;/a&gt;&lt;/p&gt;</description>
</package>
</packages>
<symbols>
<symbol name="Q">
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="DS1077">
<pin name="OUT1"/>
<pin name="OUT0"/>
<pin name="VCC"/>
<pin name="GND"/>
<pin name="CTRL0"/>
<pin name="CTRL1"/>
<pin name="SDA"/>
<pin name="SCL"/>
</symbol>
<symbol name="DS1307">
<pin name="X1"/>
<pin name="X2"/>
<pin name="VBATT"/>
<pin name="GND"/>
<pin name="SDA"/>
<pin name="SCL"/>
<pin name="SQW"/>
<pin name="VCC"/>
</symbol>
<symbol name="DS3234">
<pin name="GND"/>
<pin name="VCC"/>
<pin name="SCLK@20"/>
<pin name="DOUT"/>
<pin name="DIN"/>
<pin name="CS"/>
<pin name="INT/SQW"/>
<pin name="RST"/>
<pin name="32KHZ"/>
<pin name="GND@2"/>
<pin name="VBAT"/>
<pin name="SCLK@18"/>
<pin name="GND@14"/>
<pin name="GND@9"/>
<pin name="GND@13"/>
<pin name="GND@12"/>
<pin name="GND@11"/>
<pin name="GND@10"/>
<pin name="GND@8"/>
<pin name="GND@7"/>
</symbol>
<symbol name="OSCILLATOR">
<pin name="EN"/>
<pin name="GND"/>
<pin name="OUT"/>
<pin name="VCC"/>
</symbol>
<symbol name="RESONATOR">
<pin name="3" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="RESONATOR_NOCAP">
<pin name="3" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="SIT8002">
<pin name="/ST-OE"/>
<pin name="GND"/>
<pin name="OUT"/>
<pin name="VDD"/>
</symbol>
<symbol name="CRYSTAL-GND">
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
<symbol name="OSCILLATOR-1">
<pin name="EN"/>
<pin name="GND"/>
<pin name="OUT"/>
<pin name="VCC"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="CRYSTAL" prefix="Y" uservalue="yes">
<description>Various standard crystals. Proven footprints.</description>
<gates>
<gate name="G$1" symbol="Q"/>
</gates>
<devices>
<device name="HC49UV" package="HC49U-V">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TC38H" package="TC38H">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TC26H" package="TC26H">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="XTAL-10112"/>
<attribute name="VALUE" value="32.768kHz"/>
</technology>
</technologies>
</device>
<device name="SMD" package="HC49UP">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="HC49US" package="HC49US">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="32-SMD-MELF" package="CRYSTAL-32KHZ-SMD-MELF">
<connects>
<connect gate="G$1" pin="1" pad="X1"/>
<connect gate="G$1" pin="2" pad="X2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="XTAL-07894"/>
</technology>
</technologies>
</device>
<device name="CRYSTAL-SMD-5X3-16MHZ" package="CRYSTAL-SMD-5X3">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="XTAL-08218"/>
</technology>
</technologies>
</device>
<device name="EPSONMC146" package="CRYSTAL-32KHZ-SMD_EPSON_MC146">
<connects>
<connect gate="G$1" pin="1" pad="P$2"/>
<connect gate="G$1" pin="2" pad="P$1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="10.5X4.8" package="CRYSTAL-SMD-10.5X4.8-2PIN">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TC26H_EZ" package="TC26HEZ">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TXC-7A" package="CRYSTAL-TXC-7A">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CRYSTAL-SMD-5X3-12.288MHZ" package="CRYSTAL-SMD-5X3">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="XTAL-09653"/>
<attribute name="VALUE" value="12.288MHz"/>
</technology>
</technologies>
</device>
<device name="3.2X1.5MM" package="CRYSTAL-SMD-3.2X1.5MM">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="XTAL-13062"/>
<attribute name="VALUE" value="32.768kHz"/>
</technology>
</technologies>
</device>
<device name="CRYSTAL-SMD-5X3-12MHZ" package="CRYSTAL-SMD-5X3">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="XTAL-08297"/>
<attribute name="VALUE" value="12MHz"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS1077">
<description>I2C non-volatile programmable oscillator, 16kHz to 133MHz</description>
<gates>
<gate name="G$1" symbol="DS1077"/>
</gates>
<devices>
<device name="" package="SO08">
<connects>
<connect gate="G$1" pin="CTRL0" pad="5"/>
<connect gate="G$1" pin="CTRL1" pad="6"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="OUT0" pad="2"/>
<connect gate="G$1" pin="OUT1" pad="1"/>
<connect gate="G$1" pin="SCL" pad="8"/>
<connect gate="G$1" pin="SDA" pad="7"/>
<connect gate="G$1" pin="VCC" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS1307">
<description>I2C real-time clock with battery backup.</description>
<gates>
<gate name="G$1" symbol="DS1307"/>
</gates>
<devices>
<device name="SO8" package="SO08">
<connects>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="SCL" pad="6"/>
<connect gate="G$1" pin="SDA" pad="5"/>
<connect gate="G$1" pin="SQW" pad="7"/>
<connect gate="G$1" pin="VBATT" pad="3"/>
<connect gate="G$1" pin="VCC" pad="8"/>
<connect gate="G$1" pin="X1" pad="1"/>
<connect gate="G$1" pin="X2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SO8-TIGHT" package="SO08-TIGHT">
<connects>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="SCL" pad="6"/>
<connect gate="G$1" pin="SDA" pad="5"/>
<connect gate="G$1" pin="SQW" pad="7"/>
<connect gate="G$1" pin="VBATT" pad="3"/>
<connect gate="G$1" pin="VCC" pad="8"/>
<connect gate="G$1" pin="X1" pad="1"/>
<connect gate="G$1" pin="X2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-08138"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS3234">
<description>SPI RTC module with battery backup and internal clock.</description>
<gates>
<gate name="G$1" symbol="DS3234"/>
</gates>
<devices>
<device name="" package="DS3234">
<connects>
<connect gate="G$1" pin="32KHZ" pad="3"/>
<connect gate="G$1" pin="CS" pad="1"/>
<connect gate="G$1" pin="DIN" pad="17"/>
<connect gate="G$1" pin="DOUT" pad="19"/>
<connect gate="G$1" pin="GND" pad="15"/>
<connect gate="G$1" pin="GND@10" pad="10"/>
<connect gate="G$1" pin="GND@11" pad="11"/>
<connect gate="G$1" pin="GND@12" pad="12"/>
<connect gate="G$1" pin="GND@13" pad="13"/>
<connect gate="G$1" pin="GND@14" pad="14"/>
<connect gate="G$1" pin="GND@2" pad="2"/>
<connect gate="G$1" pin="GND@7" pad="7"/>
<connect gate="G$1" pin="GND@8" pad="8"/>
<connect gate="G$1" pin="GND@9" pad="9"/>
<connect gate="G$1" pin="INT/SQW" pad="5"/>
<connect gate="G$1" pin="RST" pad="6"/>
<connect gate="G$1" pin="SCLK@18" pad="18"/>
<connect gate="G$1" pin="SCLK@20" pad="20"/>
<connect gate="G$1" pin="VBAT" pad="16"/>
<connect gate="G$1" pin="VCC" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OSCILLATOR" prefix="U">
<description>Generic 5x3 and 7x5 oscillators</description>
<gates>
<gate name="G$1" symbol="OSCILLATOR"/>
</gates>
<devices>
<device name="SMD" package="CRYSTAL-SMD-7X5">
<connects>
<connect gate="G$1" pin="EN" pad="P$1"/>
<connect gate="G$1" pin="GND" pad="P$2"/>
<connect gate="G$1" pin="OUT" pad="P$3"/>
<connect gate="G$1" pin="VCC" pad="P$4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD6" package="CRYSTAL-SMD-7.5X5.2-6PIN">
<connects>
<connect gate="G$1" pin="EN" pad="1"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="OUT" pad="3"/>
<connect gate="G$1" pin="VCC" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="5X3" package="CRYSTAL-SMD-5X3">
<connects>
<connect gate="G$1" pin="EN" pad="1"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="OUT" pad="3"/>
<connect gate="G$1" pin="VCC" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="5X3-PIN1-INDICATED" package="CRYSTAL-OSC-SMD-5X3">
<connects>
<connect gate="G$1" pin="EN" pad="1"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="OUT" pad="3"/>
<connect gate="G$1" pin="VCC" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="XTAL-11225" package="CRYSTAL-SMD-7X5">
<connects>
<connect gate="G$1" pin="EN" pad="P$1"/>
<connect gate="G$1" pin="GND" pad="P$2"/>
<connect gate="G$1" pin="OUT" pad="P$3"/>
<connect gate="G$1" pin="VCC" pad="P$4"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="XTAL-11225"/>
<attribute name="VALUE" value="16MHz"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RESONATOR" prefix="Y" uservalue="yes">
<description>&lt;b&gt;Resonator&lt;/b&gt;&lt;br&gt;
Small SMD resonator.&lt;br&gt;
Used, eg, on the Arduino Pro/ Pro Mini boards.&lt;br&gt;
8MHz- XTAL-08895&lt;br&gt;
16MHz- XTAL-08900</description>
<gates>
<gate name="G$1" symbol="RESONATOR"/>
</gates>
<devices>
<device name="PTH" package="RESONATOR-PTH">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="8MHZ" package="RESONATOR-SMD">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="XTAL-08895"/>
<attribute name="VALUE" value="8MHZ"/>
</technology>
</technologies>
</device>
<device name="16MHZ" package="RESONATOR-SMD">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="XTAL-08900"/>
<attribute name="VALUE" value="16MHZ"/>
</technology>
</technologies>
</device>
<device name="4MHZ" package="RESONATOR-SMD_MED">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="XTAL-12492"/>
<attribute name="VALUE" value="4MHz"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RESONATOR-WIDE">
<gates>
<gate name="G$1" symbol="RESONATOR"/>
</gates>
<devices>
<device name="" package="RESONATOR-WIDE-SMD">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RESONATOR_NOCAP">
<gates>
<gate name="G$1" symbol="RESONATOR_NOCAP"/>
</gates>
<devices>
<device name="" package="RESONATOR_NOCAP">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="3" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SIT8002">
<description>Silicon Oscillator- not field programmable</description>
<gates>
<gate name="G$1" symbol="SIT8002"/>
</gates>
<devices>
<device name="" package="SIT8002">
<connects>
<connect gate="G$1" pin="/ST-OE" pad="1"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="OUT" pad="3"/>
<connect gate="G$1" pin="VDD" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CRYSTAL-GROUNDED">
<gates>
<gate name="G$1" symbol="CRYSTAL-GND"/>
</gates>
<devices>
<device name="" package="CRYSTAL-SMD-5X3">
<connects>
<connect gate="G$1" pin="1" pad="3"/>
<connect gate="G$1" pin="2" pad="1"/>
<connect gate="G$1" pin="3" pad="2 4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="33MHZ-OSCILLATOR" prefix="U">
<description>Generic 5x3.2 Oscillator</description>
<gates>
<gate name="G$1" symbol="OSCILLATOR-1"/>
</gates>
<devices>
<device name="" package="CRYSTAL-OSC-SMD-5X3.2">
<connects>
<connect gate="G$1" pin="EN" pad="1"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="OUT" pad="3"/>
<connect gate="G$1" pin="VCC" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="XTAL-11986"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
