<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.6.0">
<drawing>
<library>
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete LEDs for illumination or indication, but no displays.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="APA3010SF4C">
</package>
<package name="LED5MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
5 mm, round</description>
</package>
<package name="LED3MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
3 mm, round</description>
</package>
<package name="LED-1206">
</package>
<package name="LED-0603">
</package>
<package name="LED10MM">
</package>
<package name="FKIT-LED-1206">
</package>
<package name="LED3MM-NS">
<description>&lt;h3&gt;LED 3MM - No Silk&lt;/h3&gt;
3 mm, round</description>
</package>
<package name="LED5MM-KIT">
<description>&lt;h3&gt;LED5MM-KIT&lt;/h3&gt;
5MM Through-hole LED&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Warning:&lt;/b&gt; This is the KIT version of this package. This package has a smaller diameter top stop mask, which doesn't cover the diameter of the pad. This means only the bottom side of the pads' copper will be exposed. You'll only be able to solder to the bottom side.</description>
</package>
<package name="LED-TRICOLOR-SMD">
</package>
<package name="LED_BARGAPH_10">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="LED_PIRANHA_5MM">
</package>
<package name="LED_RING">
<description>&lt;h3&gt;LED Ring&lt;/h3&gt;
http://dlnmh9ip6v2uc.cloudfront.net/datasheets/Components/LED/Top-Up%20LED%20Ring%20LED-CCL-A.pdf&lt;br&gt;</description>
</package>
<package name="LIGHTPIPE-7511">
</package>
<package name="LTE-302">
</package>
<package name="LUXEON">
</package>
<package name="LUXEON-REBEL">
</package>
<package name="LED-RGB-THRU">
</package>
<package name="LED-TRICOLOR-5050">
<description>&lt;H3&gt;5050 SMD RGB LED&lt;/h3&gt;
5.0mm x 5.0mm, 2.6mm thickness</description>
</package>
<package name="LED-TRICOLOR-5050-IC">
</package>
<package name="LED-1206-BOTTOM">
</package>
<package name="SFH4641">
</package>
<package name="SFH4641-NARROW">
</package>
<package name="SFH4641-SHORT">
</package>
<package name="SFH4641-OVERSIZE">
</package>
<package name="WS2812B">
<description>&lt;b&gt;Intelligent control LED with integrated light source&lt;/b&gt;&lt;p&gt;
WS2812B&lt;br&gt;
source: http://www.world-semi.com/uploads/soft/130904/1_1500205981.pdf</description>
</package>
<package name="PLCC-6-LED">
</package>
<package name="LTST-C195KGJRKT">
</package>
<package name="SFH4641-SHORT2">
</package>
<package name="P-LCC-4-3">
<description>&lt;h3&gt;Everlight Red/Green/Blue LED&lt;/h3&gt;
67-23/R6GHBHC-B01/2T &lt;b&gt;||&lt;/b&gt; 67-23/R6GHBH-B01</description>
</package>
<package name="RGB_BAR_GRAPH">
</package>
</packages>
<symbols>
<symbol name="APA3010SF4C">
<pin name="1"/>
<pin name="2"/>
</symbol>
<symbol name="LED">
<pin name="C" direction="pas"/>
<pin name="A" direction="pas"/>
</symbol>
<symbol name="LED-TRICOLORSMD">
<pin name="GRN"/>
<pin name="BLU"/>
<pin name="A"/>
<pin name="RED"/>
</symbol>
<symbol name="LED_BARGRAPH_10">
<pin name="C" direction="pas"/>
<pin name="A" direction="pas"/>
</symbol>
<symbol name="LED-TRICOLOR-THROUGHHOLE">
<pin name="GRN"/>
<pin name="BLU"/>
<pin name="C"/>
<pin name="RED"/>
</symbol>
<symbol name="LED_RING">
<pin name="COM1" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="COM2" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="COM3" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="COM0" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="9" direction="pas"/>
</symbol>
<symbol name="LIGHTPIPE-7511">
</symbol>
<symbol name="LTE-302">
<pin name="A"/>
<pin name="C"/>
</symbol>
<symbol name="LUXEON">
<pin name="C" direction="pas"/>
<pin name="A" direction="pas"/>
<pin name="S"/>
</symbol>
<symbol name="LED-RGB-CA">
<pin name="RED_CATHODE"/>
<pin name="GREEN_CATHODE"/>
<pin name="BLUE_CATHODE"/>
<pin name="ANODE"/>
</symbol>
<symbol name="LED-RGB-CC">
<pin name="RED_CATHODE"/>
<pin name="GREEN_CATHODE"/>
<pin name="BLUE_CATHODE"/>
<pin name="CATHODE"/>
</symbol>
<symbol name="LED-TRICOLOR-INDV">
<pin name="BLU-A"/>
<pin name="BLU-C"/>
<pin name="GRN-A"/>
<pin name="GRN-C"/>
<pin name="RED-A"/>
<pin name="RED-C"/>
</symbol>
<symbol name="LED-TRICOLOR-WS28X1">
<pin name="VDD"/>
<pin name="VSS"/>
<pin name="DI"/>
<pin name="DO"/>
</symbol>
<symbol name="WS2812B">
<description>&lt;b&gt;Intelligent control LED with integrated light source&lt;/b&gt;&lt;p&gt;
WS2812B&lt;br&gt;
source: http://www.world-semi.com/uploads/soft/130904/1_1500205981.pdf</description>
<pin name="VDD" direction="pwr"/>
<pin name="DOUT" direction="out"/>
<pin name="VSS" direction="pwr"/>
<pin name="DIN" direction="in"/>
</symbol>
<symbol name="LED-TRICOLOR-SMD">
<pin name="GRN"/>
<pin name="BLU"/>
<pin name="BC"/>
<pin name="RED"/>
<pin name="RC"/>
<pin name="GC"/>
</symbol>
<symbol name="LED-RG">
<pin name="GC" direction="pas"/>
<pin name="GA" direction="pas"/>
<pin name="RC" direction="pas"/>
<pin name="RA" direction="pas"/>
</symbol>
<symbol name="LED-RGB">
<description>67-23/R6GHBHC-B01/2T</description>
<pin name="RED" direction="pas"/>
<pin name="GREEN" direction="pas"/>
<pin name="BLUE" direction="pas"/>
<pin name="ANODE" direction="pas"/>
</symbol>
<symbol name="RGB_BAR_GRAPH">
<description>48 Segment RGB Bar Graph - Common Anode</description>
<pin name="R1"/>
<pin name="G1"/>
<pin name="B1"/>
<pin name="R2"/>
<pin name="G2"/>
<pin name="B2"/>
<pin name="R3"/>
<pin name="G3"/>
<pin name="B3"/>
<pin name="C1"/>
<pin name="C2"/>
<pin name="C3"/>
<pin name="C4"/>
<pin name="C5"/>
<pin name="C6"/>
<pin name="C7"/>
<pin name="C8"/>
<pin name="C9"/>
<pin name="C10"/>
<pin name="C11"/>
<pin name="C12"/>
<pin name="C13"/>
<pin name="C14"/>
<pin name="C15"/>
<pin name="C16"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="APA3010SF4C" prefix="D">
<description>DIO-10854 &lt;BR&gt;&lt;br&gt;
Right-angle 880nm SMT infrared LED</description>
<gates>
<gate name="G$1" symbol="APA3010SF4C"/>
</gates>
<devices>
<device name="" package="APA3010SF4C">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="DIO-10854"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LED" prefix="D" uservalue="yes">
<description>&lt;b&gt;LEDs&lt;/b&gt;
Standard schematic elements and footprints for 5mm, 3mm, 1206, and 0603 sized LEDs. 5mm - Spark Fun Electronics SKU : COM-00529 (and others)</description>
<gates>
<gate name="G$1" symbol="LED"/>
</gates>
<devices>
<device name="5MM" package="LED5MM">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="3MM" package="LED3MM">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="DIO-08794"/>
</technology>
</technologies>
</device>
<device name="1206" package="LED-1206">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0603" package="LED-0603">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="10MM" package="LED10MM">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-FKIT-1206" package="FKIT-LED-1206">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-3MM-NO_SILK" package="LED3MM-NS">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="5MM-KIT" package="LED5MM-KIT">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1206-BOTTOM" package="LED-1206-BOTTOM">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LED-TRICOLOR">
<description>&lt;b&gt;Tri-Color LED SMD&lt;/b&gt;
Proven layout and schematic for triple color LED in SMD package - common anode. Spark Fun Electronics SKU : COM-07844</description>
<gates>
<gate name="G$1" symbol="LED-TRICOLORSMD"/>
</gates>
<devices>
<device name="" package="LED-TRICOLOR-SMD">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="BLU" pad="B"/>
<connect gate="G$1" pin="GRN" pad="G"/>
<connect gate="G$1" pin="RED" pad="R"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LED_BARGRAPH_10" prefix="D" uservalue="yes">
<description>10-Segment LED Bar Graph&lt;p&gt;
&lt;p&gt;
SFE part numbers:&lt;p&gt;
COM-09935 (red, Vf = 2.1V, Ifmax = 20mA)&lt;br&gt;
COM-09936 (yellow, Vf = 2.1V, Ifmax = 20mA)&lt;br&gt;
COM-09937 (blue, Vf = 3.4V, Ifmax = 20mA)&lt;br&gt;
COM-09938 (green, Vf = 3.4V, Ifmax = 20mA)&lt;br&gt;</description>
<gates>
<gate name="A" symbol="LED_BARGRAPH_10"/>
<gate name="B" symbol="LED_BARGRAPH_10"/>
<gate name="C" symbol="LED_BARGRAPH_10"/>
<gate name="D" symbol="LED_BARGRAPH_10"/>
<gate name="E" symbol="LED_BARGRAPH_10"/>
<gate name="F" symbol="LED_BARGRAPH_10"/>
<gate name="G" symbol="LED_BARGRAPH_10"/>
<gate name="H" symbol="LED_BARGRAPH_10"/>
<gate name="I" symbol="LED_BARGRAPH_10"/>
<gate name="J" symbol="LED_BARGRAPH_10"/>
</gates>
<devices>
<device name="" package="LED_BARGAPH_10">
<connects>
<connect gate="A" pin="A" pad="1"/>
<connect gate="A" pin="C" pad="20"/>
<connect gate="B" pin="A" pad="2"/>
<connect gate="B" pin="C" pad="19"/>
<connect gate="C" pin="A" pad="3"/>
<connect gate="C" pin="C" pad="18"/>
<connect gate="D" pin="A" pad="4"/>
<connect gate="D" pin="C" pad="17"/>
<connect gate="E" pin="A" pad="5"/>
<connect gate="E" pin="C" pad="16"/>
<connect gate="F" pin="A" pad="6"/>
<connect gate="F" pin="C" pad="15"/>
<connect gate="G" pin="A" pad="7"/>
<connect gate="G" pin="C" pad="14"/>
<connect gate="H" pin="A" pad="8"/>
<connect gate="H" pin="C" pad="13"/>
<connect gate="I" pin="A" pad="9"/>
<connect gate="I" pin="C" pad="12"/>
<connect gate="J" pin="A" pad="10"/>
<connect gate="J" pin="C" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LED_PIRANHA_5MM">
<description>High-brightness RGB through-hole LED, similar to that used in the Shiftbrite</description>
<gates>
<gate name="G$1" symbol="LED-TRICOLOR-THROUGHHOLE"/>
</gates>
<devices>
<device name="" package="LED_PIRANHA_5MM">
<connects>
<connect gate="G$1" pin="BLU" pad="B"/>
<connect gate="G$1" pin="C" pad="-"/>
<connect gate="G$1" pin="GRN" pad="G"/>
<connect gate="G$1" pin="RED" pad="R"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LED_RING" prefix="LED">
<description>&lt;h3&gt;16 LED Ring&lt;/h3&gt;
COM-10595&lt;br&gt;
http://dlnmh9ip6v2uc.cloudfront.net/datasheets/Components/LED/Top-Up%20LED%20Ring%20LED-CCL-A.pdf</description>
<gates>
<gate name="G$1" symbol="LED_RING"/>
</gates>
<devices>
<device name="" package="LED_RING">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="COM0" pad="COM0"/>
<connect gate="G$1" pin="COM1" pad="COM1"/>
<connect gate="G$1" pin="COM2" pad="COM2"/>
<connect gate="G$1" pin="COM3" pad="COM3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LIGHTPIPE-7511">
<gates>
<gate name="G$1" symbol="LIGHTPIPE-7511"/>
</gates>
<devices>
<device name="" package="LIGHTPIPE-7511">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LTE-302" prefix="D" uservalue="yes">
<description>Through-hole side-firing 940nm IR LED</description>
<gates>
<gate name="G$1" symbol="LTE-302"/>
</gates>
<devices>
<device name="" package="LTE-302">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LUXEON">
<description>&lt;b&gt;Luxeon LED&lt;/b&gt;
This footprint works with the current 1 Watt, 3 Watt, and 5 Watt LEDs. These blindingly bright LEDs generate a lot of heat so the footprint has a large pad under the LED for thermal transfer. Schematic and footprint are proven. Spark Fun Electronics SKU : COM-00603</description>
<gates>
<gate name="G$1" symbol="LUXEON"/>
</gates>
<devices>
<device name="SMD" package="LUXEON">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
<connect gate="G$1" pin="S" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LUXEON-REBEL">
<description>Luxeon Rebel single-color high output LED</description>
<gates>
<gate name="G$1" symbol="LUXEON"/>
</gates>
<devices>
<device name="" package="LUXEON-REBEL">
<connects>
<connect gate="G$1" pin="A" pad="ANODE"/>
<connect gate="G$1" pin="C" pad="CATHODE"/>
<connect gate="G$1" pin="S" pad="P$3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LED-GREEN" prefix="D" uservalue="yes">
<description>&lt;B&gt;Various green LEDs&lt;br&gt;&lt;br&gt;&lt;/B&gt;
Green LEDs used in SFE Production&lt;br&gt;&lt;br&gt;
0603- DIO-00821&lt;br&gt;
LARGE- DIO-00862&lt;br&gt;
LILYPAD- DIO-09910&lt;br&gt;</description>
<gates>
<gate name="G$1" symbol="LED"/>
</gates>
<devices>
<device name="0603" package="LED-0603">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="DIO-00821"/>
<attribute name="VALUE" value="GREEN"/>
</technology>
</technologies>
</device>
<device name="LILYPAD" package="LED-1206">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="DIO-09910"/>
<attribute name="VALUE" value="GREEN"/>
</technology>
</technologies>
</device>
<device name="1206" package="LED-1206">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="DIO-00862"/>
<attribute name="VALUE" value="GREEN"/>
</technology>
</technologies>
</device>
<device name="1206-BOTTOM" package="LED-1206-BOTTOM">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="DIO-11076"/>
<attribute name="VALUE" value="Green"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LED-RED" prefix="D" uservalue="yes">
<description>Assorted Red LEDs&lt;br&gt;
LilyPad 1206- DIO-09912&lt;br&gt;
1206- DIO-00809&lt;br&gt;
0603- DIO-00819&lt;br&gt;
"SMART" means more efficient and expensive</description>
<gates>
<gate name="G$1" symbol="LED"/>
</gates>
<devices>
<device name="0603" package="LED-0603">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="DIO-00819"/>
<attribute name="VALUE" value="RED"/>
</technology>
</technologies>
</device>
<device name="1206" package="LED-1206">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="DIO-09912"/>
<attribute name="VALUE" value="RED"/>
</technology>
</technologies>
</device>
<device name="LILYPAD" package="LED-1206">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="DIO-09912"/>
<attribute name="VALUE" value="RED"/>
</technology>
</technologies>
</device>
<device name="0603-SMART" package="LED-0603">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="DIO-11154"/>
<attribute name="VALUE" value="Red"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LED-WHITE" prefix="D" uservalue="yes">
<description>White SMD LEDs&lt;br&gt;
LilyPad 1206- DIO-09955</description>
<gates>
<gate name="G$1" symbol="LED"/>
</gates>
<devices>
<device name="1206" package="LED-1206">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="DIO-09955"/>
<attribute name="VALUE" value="WHITE"/>
</technology>
</technologies>
</device>
<device name="0603" package="LED-0603">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="DIO-09004"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LED-YELLOW" prefix="D" uservalue="yes">
<description>Yellow SMD LEDs&lt;br&gt;
LilyPad 1206- DIO-09909&lt;br&gt;
0603- DIO-09003&lt;br&gt;
"SMART" means more efficient and expensive</description>
<gates>
<gate name="G$1" symbol="LED"/>
</gates>
<devices>
<device name="LILYPAD" package="LED-1206">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="DIO-09909"/>
<attribute name="VALUE" value="Yellow"/>
</technology>
</technologies>
</device>
<device name="0603" package="LED-0603">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="DIO-09003"/>
<attribute name="VALUE" value="Yellow"/>
</technology>
</technologies>
</device>
<device name="1206" package="LED-1206">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="DIO-00820"/>
<attribute name="VALUE" value="YELLOW"/>
</technology>
</technologies>
</device>
<device name="0603-SMART" package="LED-0603">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="DIO-11230"/>
<attribute name="VALUE" value="Yellow"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LED-RGB-CA-THRU" prefix="D">
<description>RGB Through-hole common anode&lt;br&gt;
SparkFun store front&lt;br&gt;
COM-10821 (diffuse)&lt;br&gt;
COM-10820 (clear)&lt;br&gt;</description>
<gates>
<gate name="G$1" symbol="LED-RGB-CA"/>
</gates>
<devices>
<device name="DIFFUSE" package="LED-RGB-THRU">
<connects>
<connect gate="G$1" pin="ANODE" pad="2"/>
<connect gate="G$1" pin="BLUE_CATHODE" pad="4"/>
<connect gate="G$1" pin="GREEN_CATHODE" pad="3"/>
<connect gate="G$1" pin="RED_CATHODE" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="DIO-10632"/>
</technology>
</technologies>
</device>
<device name="CLEAR" package="LED-RGB-THRU">
<connects>
<connect gate="G$1" pin="ANODE" pad="2"/>
<connect gate="G$1" pin="BLUE_CATHODE" pad="4"/>
<connect gate="G$1" pin="GREEN_CATHODE" pad="3"/>
<connect gate="G$1" pin="RED_CATHODE" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="DIO-10631"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LED-RGB-CC-THRU" prefix="D">
<description>RGB Through-hole common cathode LED&lt;br&gt;
SparkFun Storefront:&lt;br&gt;
COM-00105 (Clear)&lt;br&gt;
COM-09264 (Diffuse)</description>
<gates>
<gate name="G$1" symbol="LED-RGB-CC"/>
</gates>
<devices>
<device name="DIFFUSE" package="LED-RGB-THRU">
<connects>
<connect gate="G$1" pin="BLUE_CATHODE" pad="4"/>
<connect gate="G$1" pin="CATHODE" pad="2"/>
<connect gate="G$1" pin="GREEN_CATHODE" pad="3"/>
<connect gate="G$1" pin="RED_CATHODE" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="DIO-09434"/>
</technology>
</technologies>
</device>
<device name="CLEAR" package="LED-RGB-THRU">
<connects>
<connect gate="G$1" pin="BLUE_CATHODE" pad="4"/>
<connect gate="G$1" pin="CATHODE" pad="2"/>
<connect gate="G$1" pin="GREEN_CATHODE" pad="3"/>
<connect gate="G$1" pin="RED_CATHODE" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="DIO-08418"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LED-TRICOLOR-5050" prefix="LED">
<gates>
<gate name="D1" symbol="LED-TRICOLOR-INDV"/>
</gates>
<devices>
<device name="NO_IC" package="LED-TRICOLOR-5050">
<connects>
<connect gate="D1" pin="BLU-A" pad="3"/>
<connect gate="D1" pin="BLU-C" pad="4"/>
<connect gate="D1" pin="GRN-A" pad="1"/>
<connect gate="D1" pin="GRN-C" pad="6"/>
<connect gate="D1" pin="RED-A" pad="2"/>
<connect gate="D1" pin="RED-C" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="DIO-10298"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LED-TRICOLOR-5050-IC" prefix="U">
<description>&lt;h3&gt; WS2812 RGB LED w/ WS2811 driver&lt;/h3&gt;&lt;p&gt;
5x5mm SMD LED with built-in controller IC.&lt;br&gt;
DIO-11598</description>
<gates>
<gate name="U1" symbol="LED-TRICOLOR-WS28X1"/>
</gates>
<devices>
<device name="WS2811" package="LED-TRICOLOR-5050-IC">
<connects>
<connect gate="U1" pin="DI" pad="2" route="any"/>
<connect gate="U1" pin="DO" pad="1"/>
<connect gate="U1" pin="VDD" pad="3 5"/>
<connect gate="U1" pin="VSS" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="DIO-11598"/>
<attribute name="VALUE" value="WS2811"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LED-BLUE" prefix="D" uservalue="yes">
<description>&lt;H3&gt;Blue LEDs for production use&lt;/H3&gt;&lt;p&gt;
Various blue LEDs stocked by SparkFun production&lt;br&gt;
0603 - DIO-08575&lt;br&gt;
Rebel - DIO-09553&lt;br&gt;
1206 - DIO-09911</description>
<gates>
<gate name="G$1" symbol="LED"/>
</gates>
<devices>
<device name="0603" package="LED-0603">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="DIO-08575"/>
<attribute name="VALUE" value="BLUE"/>
</technology>
</technologies>
</device>
<device name="1206" package="LED-1206">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="DIO-09911"/>
<attribute name="VALUE" value="BLUE"/>
</technology>
</technologies>
</device>
<device name="REBEL" package="LUXEON-REBEL">
<connects>
<connect gate="G$1" pin="A" pad="ANODE"/>
<connect gate="G$1" pin="C" pad="CATHODE"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="DIO-09553"/>
<attribute name="VALUE" value="BLUE"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LED-PINK" prefix="D" uservalue="yes">
<description>&lt;b&gt;Various Pink LEDs&lt;br&gt;&lt;br&gt;&lt;/b&gt;
Pink LEDs used in SFE Production&lt;br&gt;&lt;br&gt;
LILYPAD- DIO-10415&lt;br&gt;</description>
<gates>
<gate name="G$1" symbol="LED"/>
</gates>
<devices>
<device name="1206" package="LED-1206">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="DIO-10415"/>
<attribute name="VALUE" value="PINK"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LED-PURPLE" prefix="D" uservalue="yes">
<description>Various green LEDs&lt;br&gt;
0603- DIO-00821&lt;br&gt;
LARGE- DIO-00862&lt;br&gt;
LILYPAD- DIO-09910&lt;br&gt;</description>
<gates>
<gate name="G$1" symbol="LED"/>
</gates>
<devices>
<device name="1206" package="LED-1206">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="DIO-11140"/>
<attribute name="VALUE" value="PURPLE"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SFH4641" prefix="D">
<gates>
<gate name="G$1" symbol="LED"/>
</gates>
<devices>
<device name="LARGE" package="SFH4641">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="DIO-11994"/>
</technology>
</technologies>
</device>
<device name="NARROW" package="SFH4641-NARROW">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="DIO-11994"/>
</technology>
</technologies>
</device>
<device name="SHORT" package="SFH4641-SHORT">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="DIO-11994"/>
</technology>
</technologies>
</device>
<device name="OVERSIZE" package="SFH4641-OVERSIZE">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="DIO-11994"/>
</technology>
</technologies>
</device>
<device name="SHORT2" package="SFH4641-SHORT2">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="DIO-11994"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WS2812B" prefix="D" uservalue="yes">
<description>&lt;b&gt;WS2812B&lt;/b&gt; - Intelligent control LED integrated light source

&lt;p&gt;Technical Specifications:
&lt;ul&gt;
&lt;li&gt;Power Supply Voltage (VDD): 3.5 to 5.3 V&lt;/li&gt;
&lt;li&gt;Input Voltage (VI): -0.5 to VDD+0.5 V&lt;/li&gt;
&lt;li&gt;Operating Junction Temperature (Topt): -25°C to +80°C&lt;/li&gt;
&lt;li&gt;Storage Temperature Range (Tstg): -55°C to +150°C&lt;/li&gt;
&lt;/ul&gt;
&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="WS2812B"/>
</gates>
<devices>
<device name="" package="WS2812B">
<connects>
<connect gate="G$1" pin="DIN" pad="4"/>
<connect gate="G$1" pin="DOUT" pad="2"/>
<connect gate="G$1" pin="VDD" pad="1"/>
<connect gate="G$1" pin="VSS" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="DIO-12503"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LED-IR-THRU" prefix="D">
<gates>
<gate name="G$1" symbol="LED"/>
</gates>
<devices>
<device name="TSAL6100" package="LED5MM">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="DIO-12058"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LED-TRICOLOR-NO-COM" prefix="LED">
<gates>
<gate name="G$1" symbol="LED-TRICOLOR-SMD"/>
</gates>
<devices>
<device name="PLCC-6-SMD" package="PLCC-6-LED">
<connects>
<connect gate="G$1" pin="BC" pad="CB"/>
<connect gate="G$1" pin="BLU" pad="AB"/>
<connect gate="G$1" pin="GC" pad="CG"/>
<connect gate="G$1" pin="GRN" pad="AG"/>
<connect gate="G$1" pin="RC" pad="CR"/>
<connect gate="G$1" pin="RED" pad="AR"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="DIO-12113"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LED-RG" prefix="D">
<gates>
<gate name="G$1" symbol="LED-RG"/>
</gates>
<devices>
<device name="LTST-C195KGJRKT" package="LTST-C195KGJRKT">
<connects>
<connect gate="G$1" pin="GA" pad="P$1"/>
<connect gate="G$1" pin="GC" pad="P$3"/>
<connect gate="G$1" pin="RA" pad="P$2"/>
<connect gate="G$1" pin="RC" pad="P$4"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="DIO-12140"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="0.13_RGB_LED" prefix="D" uservalue="yes">
<description>&lt;h3&gt;Everlight Red/Green/Blue LED&lt;/h3&gt;
67-23/R6GHBHC-B01/2T &lt;b&gt;||&lt;/b&gt; 67-23/R6GHBH-B01&lt;br /&gt;
&lt;table width="100%"&gt;
				&lt;tbody&gt;
					&lt;tr&gt;
						&lt;td width="50%"&gt;&lt;strong&gt;Size&lt;/strong&gt;&lt;/td&gt;
						&lt;td&gt;3.2*2.8*1.9mm&lt;/td&gt;
					&lt;/tr&gt;
                                        &lt;tr&gt;
                                                &lt;td width="50%"&gt;&lt;strong&gt;Mounting Type&lt;/strong&gt;&lt;/td&gt;
                                                &lt;td&gt;SMD Full-Color LED PLCC4&lt;/td&gt;
                                        &lt;/tr&gt;
                                        &lt;tr&gt;
                                                &lt;td width="50%"&gt;&lt;strong&gt;Emitting Color&lt;/strong&gt;&lt;/td&gt;
                                                &lt;td&gt;Red/Green/Blue (620-625/530-535/470-475 nm)&lt;/td&gt;
                                        &lt;/tr&gt;
                                        &lt;tr&gt;
                                                &lt;td width="50%"&gt;&lt;strong&gt;Chip Material&lt;/strong&gt;&lt;/td&gt;
                                                &lt;td&gt;AlGaInP/InGaN/InGaN&lt;/td&gt;
                                        &lt;/tr&gt;
                                        &lt;tr&gt;
                                                &lt;td width="50%"&gt;&lt;strong&gt;Luminous Intensity&lt;/strong&gt;&lt;/td&gt;
                                                &lt;td&gt;57-112/225-450/36-72 mcd&lt;/td&gt;
                                        &lt;/tr&gt;
                                        &lt;tr&gt;
                                                &lt;td width="50%"&gt;&lt;strong&gt;Viewing Angle&lt;/strong&gt;&lt;/td&gt;
                                                &lt;td&gt;120 deg&lt;/td&gt;
                                        &lt;/tr&gt;
                                        &lt;tr&gt;
                                                &lt;td width="50%"&gt;&lt;strong&gt;Lens Type-Color&lt;/strong&gt;&lt;/td&gt;
                                                &lt;td&gt;Water Clear&lt;/td&gt;
                                        &lt;/tr&gt;
                                        &lt;tr&gt;
                                                &lt;td width="50%"&gt;&lt;strong&gt;Forward Voltage&lt;/strong&gt;&lt;/td&gt;
                                                &lt;td&gt;2.0/3.5/3.5 V&lt;/td&gt;
                                        &lt;/tr&gt;
                                        &lt;tr&gt;
                                                &lt;td width="50%"&gt;&lt;strong&gt;Forward Current&lt;/strong&gt;&lt;/td&gt;
                                                &lt;td&gt;10 mA&lt;/td&gt;
                                        &lt;/tr&gt;
                                        &lt;tr&gt;
                                                &lt;td width="50%"&gt;&lt;strong&gt;Maximum Forward Voltage&lt;/strong&gt;&lt;/td&gt;
                                                &lt;td&gt;2.4/3.9/3.9 V&lt;/td&gt;
                                        &lt;/tr&gt;
                                        &lt;tr&gt;
                                                &lt;td width="50%"&gt;&lt;strong&gt;Maximum Forward Current&lt;/strong&gt;&lt;/td&gt;
                                                &lt;td&gt;25/25/25 mA&lt;/td&gt;
                                        &lt;/tr&gt;
                                        &lt;tr&gt;
                                                &lt;td width="50%"&gt;&lt;strong&gt;Min-Max Operating Temperature&lt;/strong&gt;&lt;/td&gt;
                                                &lt;td&gt; -40C to +85C&lt;/td&gt;
                                        &lt;/tr&gt;
                                        &lt;tr&gt;
                                                &lt;td width="50%"&gt;&lt;strong&gt;Factory Pack&lt;/strong&gt;&lt;/td&gt;
                                                &lt;td&gt;2000 pcs-Reel&lt;/td&gt;
                                        &lt;/tr&gt;
					&lt;tr&gt;
						&lt;td&gt;&lt;strong&gt;RoHS&lt;/strong&gt;&lt;/td&gt;
						&lt;td&gt;✓&lt;/td&gt;
					&lt;/tr&gt;
				&lt;/tbody&gt;
				&lt;/table&gt;</description>
<gates>
<gate name="G$1" symbol="LED-RGB"/>
</gates>
<devices>
<device name="PLCC" package="P-LCC-4-3">
<connects>
<connect gate="G$1" pin="ANODE" pad="4"/>
<connect gate="G$1" pin="BLUE" pad="3"/>
<connect gate="G$1" pin="GREEN" pad="2"/>
<connect gate="G$1" pin="RED" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="DIO-12986"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RGB_BAR_GRAPH" prefix="D">
<description>SparkFun 48 Segment RGB Bar Graph - Common Anode</description>
<gates>
<gate name="D1" symbol="RGB_BAR_GRAPH"/>
</gates>
<devices>
<device name="CA" package="RGB_BAR_GRAPH">
<connects>
<connect gate="D1" pin="B1" pad="24"/>
<connect gate="D1" pin="B2" pad="6"/>
<connect gate="D1" pin="B3" pad="14"/>
<connect gate="D1" pin="C1" pad="1"/>
<connect gate="D1" pin="C10" pad="8"/>
<connect gate="D1" pin="C11" pad="19"/>
<connect gate="D1" pin="C12" pad="18"/>
<connect gate="D1" pin="C13" pad="10"/>
<connect gate="D1" pin="C14" pad="11"/>
<connect gate="D1" pin="C15" pad="15"/>
<connect gate="D1" pin="C16" pad="12"/>
<connect gate="D1" pin="C2" pad="25"/>
<connect gate="D1" pin="C3" pad="3"/>
<connect gate="D1" pin="C4" pad="4"/>
<connect gate="D1" pin="C5" pad="23"/>
<connect gate="D1" pin="C6" pad="5"/>
<connect gate="D1" pin="C7" pad="22"/>
<connect gate="D1" pin="C8" pad="21"/>
<connect gate="D1" pin="C9" pad="20"/>
<connect gate="D1" pin="G1" pad="7"/>
<connect gate="D1" pin="G2" pad="16"/>
<connect gate="D1" pin="G3" pad="2"/>
<connect gate="D1" pin="R1" pad="9"/>
<connect gate="D1" pin="R2" pad="17"/>
<connect gate="D1" pin="R3" pad="13"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="COM-13520"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
