<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.2.0">
<drawing>
<library>
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find all manner of retired footprints for resistors, capacitors, board names, ICs, etc., that are no longer used in our catalog.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt;Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="ANDROID-ELECTRIC_SHEEP_LOGO">
</package>
<package name="ANDROID-ELECTRIC_SHEEP_LOGO_SMALL">
</package>
<package name="CREATIVE_COMMONS">
</package>
<package name="SFE-LOGO">
</package>
<package name="SFE-NEW-WEBLOGO">
</package>
<package name="SFE-LOGO-FLAME-COPPER">
</package>
<package name="SFE-LOGO-FLAME">
</package>
<package name="SFE-NEW-WEB">
</package>
<package name="SFE-NEW-WEB-SOLDERMASK">
</package>
<package name="STARBOARD_LOGO">
</package>
<package name="STARBOARD_LOGO_TEXT">
</package>
<package name="FIDUCIAL-1.5X3">
</package>
<package name="FIDUCIAL-1X2.5">
</package>
<package name="TESTING">
</package>
<package name="FRIST_LOGO">
</package>
<package name="0402-CAP">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="1206">
</package>
<package name="EIA3216">
</package>
<package name="HSMC-C265">
</package>
<package name="SO014">
</package>
<package name="SPARKFUN-DIGITALIC_QFN-44">
</package>
<package name="SPARKFUN-DIGITALIC_QFN-44-NOPAD">
</package>
<package name="SPARKFUN-DIGITALIC_TQFP44">
</package>
<package name="QFN-44-NOPAD_1:1">
</package>
<package name="1X02">
</package>
<package name="SJ_2S">
<description>Small solder jumper with big paste layer so it will short during reflow.</description>
</package>
<package name="1X02_LOCK">
</package>
<package name="SJ_2S-NO">
<description>Small solder jumper with no paste layer so it will open after reflow.</description>
</package>
<package name="SJ_2S-NO-NS">
</package>
<package name="SJ_3">
</package>
<package name="1X03">
</package>
<package name="SJ_3_PASTE1&amp;2">
</package>
<package name="SJ_3_PASTE2&amp;3">
</package>
<package name="SJ_2S-TRACE">
<description>Solder jumper, small, shorted with trace. No paste layer. Trace is cuttable.</description>
</package>
<package name="SJ_2S-NOTRACE">
</package>
<package name="SJ_2S-TRACE-PTH">
</package>
<package name="SJ_2S-PTH">
</package>
<package name="SJ_ROUND">
</package>
<package name="SJ_2W">
<description>&lt;b&gt;Solder jumper&lt;/b&gt;</description>
</package>
<package name="SJ_2">
<description>&lt;b&gt;Solder jumper&lt;/b&gt;</description>
</package>
<package name="SJ_3_PASTE1&amp;2&amp;3">
</package>
<package name="TACTILE-PTH">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
</package>
<package name="KSA_SEALED_TAC_SWITCH">
</package>
<package name="TACTILE-SWITCH-SMD">
</package>
<package name="PIC24FXXX_TQFP64">
<description>64-Lead TQFP Plastic Thin Quad Flatpack - 10x10x1mm Body, 2mmFP</description>
</package>
</packages>
<symbols>
<symbol name="ANDROID-ELECTRIC_SHEEP_LOGO">
</symbol>
<symbol name="CREATIVE_COMMONS">
</symbol>
<symbol name="A3L-LOC">
</symbol>
<symbol name="LOGO1">
</symbol>
<symbol name="STARBOARD_LOGO">
</symbol>
<symbol name="FIDUCIAL">
</symbol>
<symbol name="SPARKFUN-EAGLE-RULES">
</symbol>
<symbol name="FIRST">
</symbol>
<symbol name="CAP">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="CAP_POL">
<pin name="+" direction="pas"/>
<pin name="-" direction="pas"/>
</symbol>
<symbol name="LED">
<pin name="C" direction="pas"/>
<pin name="A" direction="pas"/>
</symbol>
<symbol name="74ACT125D">
<pin name="VCC"/>
<pin name="A0"/>
<pin name="B0"/>
<pin name="A1"/>
<pin name="B1"/>
<pin name="A2"/>
<pin name="B2"/>
<pin name="GND"/>
<pin name="B3"/>
<pin name="A3"/>
<pin name="O3"/>
<pin name="O2"/>
<pin name="O1"/>
<pin name="O0"/>
</symbol>
<symbol name="SPARKFUN-DIGITALIC_ATMEGA32U4">
<pin name="!RESET"/>
<pin name="AREF"/>
<pin name="AVCC@24"/>
<pin name="AVCC@44"/>
<pin name="D+"/>
<pin name="D-"/>
<pin name="GND@15"/>
<pin name="GND@23"/>
<pin name="GND@35"/>
<pin name="GND@43"/>
<pin name="PB0(SS)"/>
<pin name="PB1(SCK)"/>
<pin name="PB2(MOSI)"/>
<pin name="PB3(MISO)"/>
<pin name="PB4(ADC11)"/>
<pin name="PB5(ADC12)"/>
<pin name="PB6(ADC13)"/>
<pin name="PB7"/>
<pin name="PC6"/>
<pin name="PC7"/>
<pin name="PD0(SCL)"/>
<pin name="PD1(SDA)"/>
<pin name="PD2(RX)"/>
<pin name="PD3(TX)"/>
<pin name="PD4(ADC8)"/>
<pin name="PD5"/>
<pin name="PD6(ADC9)"/>
<pin name="PD7(ADC10)"/>
<pin name="PE2/!HWB"/>
<pin name="PE6"/>
<pin name="PF0(ADC0)"/>
<pin name="PF1(ADC1)"/>
<pin name="PF4(ADC4)"/>
<pin name="PF5(ADC5)"/>
<pin name="PF6(ADC6)"/>
<pin name="PF7(ADC7)"/>
<pin name="UCAP"/>
<pin name="UGND"/>
<pin name="UVCC"/>
<pin name="VBUS"/>
<pin name="VCC@14"/>
<pin name="VCC@34"/>
<pin name="XTAL1"/>
<pin name="XTAL2"/>
</symbol>
<symbol name="JUMPER-2">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="JUMPER-3">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
<symbol name="SJ">
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="SJ_2">
<pin name="3" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="LETTER_L">
</symbol>
<symbol name="DOCFIELD">
</symbol>
<symbol name="SWITCH-MOMENTARY">
<pin name="1" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="PIC24FJXXXDAX06">
<pin name="!MCLR" direction="in"/>
<pin name="AN2/C2INB/VMIO/RP13/CN4/RB2"/>
<pin name="AN3/C2INA/VPIO/CN5/RB3"/>
<pin name="AN8/RP8/CN26/RB8"/>
<pin name="AN9/RP9/CN27/RB9"/>
<pin name="AN14/CTPLS/RP14/CN32/RB14"/>
<pin name="AN15/RP29/REFO/CN12/RB15"/>
<pin name="AVDD" direction="pwr"/>
<pin name="AVSS" direction="pwr"/>
<pin name="C1INC/RP26/CN9/RG7"/>
<pin name="C1IND/RP21/CN8/RG6"/>
<pin name="C2INC/RP27/GD15/CN11/RG9"/>
<pin name="C2IND/RP19/GD14/CN10/RG8"/>
<pin name="C3INA/SESSEND/CN16/RD7"/>
<pin name="C3INB/CN15/RD6"/>
<pin name="D+/CN83/RG2"/>
<pin name="D-/CN84/RG3"/>
<pin name="DMH/RP11/INT0/CN49/RD0"/>
<pin name="DPH/RP23/CN51/RD2"/>
<pin name="DPLN/SDA1/RP4/GD8/CN54/RD9"/>
<pin name="ENVREG" direction="in"/>
<pin name="GD0/CN58/RE0"/>
<pin name="GD1/CN59/RE1"/>
<pin name="GD2/CN60/RE2"/>
<pin name="GD3/CN61/RE3"/>
<pin name="GD10/VBUSST/VCMPST1/VBUSVLD/CN68/RF0"/>
<pin name="GD11/VCMPST2/SESSVLD/CN69/RF1"/>
<pin name="GD12/SCL3/CN64/RE6"/>
<pin name="GD13/SDA3/CN65/RE7"/>
<pin name="HSYNC/CN62/RE4"/>
<pin name="OSCI/CLKI/CN23/RC12"/>
<pin name="OSCO/CLKO/CN22/RC15"/>
<pin name="PGEC1/AN1/VREF-/RP1/CN3/RB1"/>
<pin name="PGEC2/AN6/RP6/CN24/RB6"/>
<pin name="PGEC3/AN5/C1INA/VBUSON/RP18/CN7/RB5"/>
<pin name="PGED1/AN0/VREF+/RP0/CN2/RB0"/>
<pin name="PGED2/AN7/RP7/RCV/CN25/RB7"/>
<pin name="PGED3/AN4/C1INB/USBOEN/RP28/CN6/RB4"/>
<pin name="RP12/GD7/CN56/RD11"/>
<pin name="RP16/USBID/CN71/RF3"/>
<pin name="RP20/GPWR/CN14/RD5"/>
<pin name="RP22/GEN/CN52/RD3"/>
<pin name="RP25/GCLK/CN13/RD4"/>
<pin name="RTCC/DMLN/RP2/CN53/RD8"/>
<pin name="SCL1/RP3/GD6/CN55/RD10"/>
<pin name="SCL2/RP17/GD5/CN18/RF5"/>
<pin name="SDA2/RP10/GD4/CN17/RF4"/>
<pin name="SOSCI/C3IND/CN1/RC13"/>
<pin name="SOSCO/SCLKI/T1CK/C3INC/RPI37/CN0/RC14"/>
<pin name="TCK/AN12/CTEDG2/CN30/RB12"/>
<pin name="TDI/AN13/CTEDG1/CN31/RB13"/>
<pin name="TDO/AN11/CN29/RB11"/>
<pin name="TMS/CVREF/AN10/CN28/RB10"/>
<pin name="VBUS/RF7" direction="in"/>
<pin name="VCAP" direction="pwr"/>
<pin name="VCPCON/RP24/GD9/VBUSCHG/CN50/RD1"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="VDD@3" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VSS@3" direction="pwr"/>
<pin name="VSYNC/CN63/RE5"/>
<pin name="VUSB" direction="pwr"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="ANDROID-ELECTRIC_SHEEP_LOGO" prefix="LOGO">
<description>Logos used for the Electric  Sheep</description>
<gates>
<gate name="G$1" symbol="ANDROID-ELECTRIC_SHEEP_LOGO"/>
</gates>
<devices>
<device name="_" package="ANDROID-ELECTRIC_SHEEP_LOGO">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="" package="ANDROID-ELECTRIC_SHEEP_LOGO_SMALL">
<technologies>
<technology name="">
<attribute name="SF_ID" value="DEV-10745"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CREATIVE_COMMONS" prefix="CC_TEXT">
<description>Creative Commons License summary- RETIRED.

Please use parts FRAME-LETTER/FRAME-LEDGER to add this to both schematic and board file.</description>
<gates>
<gate name="G$1" symbol="CREATIVE_COMMONS"/>
</gates>
<devices>
<device name="" package="CREATIVE_COMMONS">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FRAME-A3" prefix="FRAME">
<description>&lt;b&gt;Schematic Frame&lt;/b&gt;&lt;p&gt;
A3 Larger Frame-RETIRED

Please use FRAME-LEDGER/FRAME-LETTER for schematics now.</description>
<gates>
<gate name="G$1" symbol="A3L-LOC"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LOGO-SFE" prefix="LOGO">
<description>&lt;b&gt;Spark Fun Electronics PCB Logo&lt;/b&gt;
This is the standard Spark Fun Electronics PCB logo.</description>
<gates>
<gate name="G$1" symbol="LOGO1"/>
</gates>
<devices>
<device name="M" package="SFE-LOGO">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="NEW" package="SFE-NEW-WEBLOGO">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CP" package="SFE-LOGO-FLAME-COPPER">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SK" package="SFE-LOGO-FLAME">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="NW2" package="SFE-NEW-WEB">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SM" package="SFE-NEW-WEB-SOLDERMASK">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STARBOARD_LOGO" prefix="LOGO">
<description>Starboard - RETIRED
PRT-10961
PRT-10640
PRT-10639
PRT-10638
PRT-10637
PRT-10572</description>
<gates>
<gate name="G$1" symbol="STARBOARD_LOGO"/>
</gates>
<devices>
<device name="" package="STARBOARD_LOGO">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-TEXT" package="STARBOARD_LOGO_TEXT">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FIDUCIAL" prefix="FID">
<description>&lt;b&gt;Fiducial Alignment Points&lt;/b&gt;
Various fiducial points for machine vision alignment.</description>
<gates>
<gate name="G$1" symbol="FIDUCIAL"/>
</gates>
<devices>
<device name="1.5X3" package="FIDUCIAL-1.5X3">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1X2.5" package="FIDUCIAL-1X2.5">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SPARKFUN-EAGLE-RULES" prefix="RULES">
<description>&lt;b&gt;Description:&lt;/b&gt; These are the default rules that SparkFun engineers must follow. We highly recommend following these rules as well.</description>
<gates>
<gate name="G$1" symbol="SPARKFUN-EAGLE-RULES"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LOGO-FIRST" prefix="LOGO">
<gates>
<gate name="G$1" symbol="FIRST"/>
</gates>
<devices>
<device name="" package="FRIST_LOGO">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750KOHM1/10W1%(0603)" prefix="R" uservalue="yes">
<description>RES-07852</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name="71.5OHM-1/4W-1%(PTH)" prefix="R" uservalue="yes">
<description>RES-10463</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name="0.33OHM1/10W1%(0603)" prefix="R" uservalue="yes">
<description>RES-08412</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name="1.0OHM1/4W5%PTH" prefix="R" uservalue="yes">
<description>RES-09453</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name="1.4KOHM-1/10W-1%(0603)" prefix="R" uservalue="yes">
<description>RES-11114</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name="3.6KOHM1/10W1%(0603)" prefix="R" uservalue="yes">
<description>RES-08417</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name="1.2KOHM1/4W5%(PTH)" prefix="R" uservalue="yes">
<description>RES-09452</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name="0.15OHM1/5W1%(0603)" prefix="R" uservalue="yes">
<description>RES-09738</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name="3.0MOHM-1/10W-1%(0603)" prefix="R" uservalue="yes">
<description>RES-10937</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name=".47UF-16V(-20/+80%)(0805)" prefix="C" uservalue="yes">
<description>CAP-08139 - Retired</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name=".68UF-16V-20%,+80%(0603)" prefix="C" uservalue="yes">
<description>CAP-08708 - Retired</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name="0.2F-3.3V--20%,+80%(COIN)" prefix="C" uservalue="yes">
<description>CAP-10408 - Retired</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name="0.018UF-50V-10%(0603)" prefix="C" uservalue="yes">
<description>CAP-08494 - Retired</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name="0.22UF-50V-?20%(ELECT)(PTH)" prefix="C" uservalue="yes">
<description>CAP-09998 - Retired</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name="0.68UF-16V--20%,+80%(0603)" prefix="C" uservalue="yes">
<description>CAP-08723 - Retired</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name="2.2UF-25V-10%(TANT)" prefix="C" uservalue="yes">
<description>CAP-08706 - Retired</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name="3.3UF-80V-20%(ELECT)" prefix="C" uservalue="yes">
<description>CAP-08365 - Retired</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name="6.7PF" prefix="C" uservalue="yes">
<description>CAP-08429 - Retired</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name="6.8PF-50V-+/-.25PF(0603)" prefix="C" uservalue="yes">
<description>CAP-08620 - Retired</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name="10UF-16V-20%(ELECT)" prefix="C" uservalue="yes">
<description>CAP-09575 - Retired</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name="12NF-200V-10%(0805)" prefix="C" uservalue="yes">
<description>CAP-11056 - Retired</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name=".1UF-CER" prefix="C">
<description>.1uF ceramic SMT&lt;br&gt;
CAP-00810- 25V +80%/-20% (0603)&lt;br&gt;
CAP-08390- 100V 10% (0603)&lt;br&gt;
CAP-08604- 25V 5% (0603)&lt;br&gt;</description>
<gates>
<gate name="G$1" symbol="CAP"/>
</gates>
<devices>
<device name="" package="0402-CAP">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CAP-00810"/>
<attribute name="VALUE" value="0.1uF"/>
</technology>
</technologies>
</device>
<device name="CAP-08604" package="0402-CAP">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CAP-08604"/>
<attribute name="VALUE" value="0.1uF"/>
</technology>
</technologies>
</device>
<device name="CAP-08390" package="0402-CAP">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CAP-08390"/>
<attribute name="VALUE" value="0.1uF"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name=".22UF-CER" prefix="C" uservalue="yes">
<description>.22uF ceramic SMT&lt;br&gt;
CAP-09885- 50V +80%/-20% (0603)</description>
<gates>
<gate name="G$1" symbol="CAP"/>
</gates>
<devices>
<device name="" package="0402-CAP">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CAP-09885"/>
<attribute name="VALUE" value=".22uF"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="2.2UF-CER" prefix="C">
<description>2.2uF Ceramic SMT&lt;BR&gt;
CAP-07888- 10V, 20% (0603)&lt;br&gt;
CAP-10009- 50V, 10% (1206)</description>
<gates>
<gate name="G$1" symbol="CAP"/>
</gates>
<devices>
<device name="CAP-07888" package="0402-CAP">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CAP-07888"/>
<attribute name="VALUE" value="2.2uF"/>
</technology>
</technologies>
</device>
<device name="CAP-10009" package="1206">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CAP-10009"/>
<attribute name="VALUE" value="2.2uF"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="10NF-CER" prefix="C" uservalue="yes">
<description>10nF/.01uF/10000pF ceramic SMT&lt;br&gt;
CAP-00867- 50V 10% (0603)</description>
<gates>
<gate name="G$1" symbol="CAP"/>
</gates>
<devices>
<device name="" package="0402-CAP">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CAP-00867"/>
<attribute name="VALUE" value="10nF"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="10UF-TANT" prefix="C" uservalue="yes">
<description>10uF Tantalum SMT&lt;br&gt;
CAP-00811- 16V 10% (EIA-3216)</description>
<gates>
<gate name="G$1" symbol="CAP_POL"/>
</gates>
<devices>
<device name="" package="EIA3216">
<connects>
<connect gate="G$1" pin="+" pad="A"/>
<connect gate="G$1" pin="-" pad="C"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CAP-00811"/>
<attribute name="VALUE" value="10uF"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HSMC-C265">
<description>RETIRED &lt;BR&gt;
&lt;BR&gt;

Avago HSMC-C265 reverse-mounted red LED

This is a SMD LED that is mounted to one side of a PCB and shines through a hole to the other side of the PCB. Useful for making boards with no components on one side for mounting and having LED indicator lights shine through the board, panel, etc.</description>
<gates>
<gate name="G$1" symbol="LED"/>
</gates>
<devices>
<device name="" package="HSMC-C265">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74ACT125D">
<description>Quad Buffer with 3-State Outputs-
ON Semi Conductor:

Digikey P/N 74ACT125SC-ND</description>
<gates>
<gate name="G$1" symbol="74ACT125D"/>
</gates>
<devices>
<device name="" package="SO014">
<connects>
<connect gate="G$1" pin="A0" pad="1"/>
<connect gate="G$1" pin="A1" pad="4"/>
<connect gate="G$1" pin="A2" pad="13"/>
<connect gate="G$1" pin="A3" pad="10"/>
<connect gate="G$1" pin="B0" pad="2"/>
<connect gate="G$1" pin="B1" pad="5"/>
<connect gate="G$1" pin="B2" pad="12"/>
<connect gate="G$1" pin="B3" pad="9"/>
<connect gate="G$1" pin="GND" pad="7"/>
<connect gate="G$1" pin="O0" pad="3"/>
<connect gate="G$1" pin="O1" pad="6"/>
<connect gate="G$1" pin="O2" pad="11"/>
<connect gate="G$1" pin="O3" pad="8"/>
<connect gate="G$1" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATMEGA32U4">
<description>Atmel 44-pin 8-bit Microcontroller with 32KBytes of ISP Flash and USB Controller ----- 

Please use the QFN-44-NOPAD_1:1 package for the footprint of all boards using a 32U4. Route traces directly away from the pads as much as possible.</description>
<gates>
<gate name="G$1" symbol="SPARKFUN-DIGITALIC_ATMEGA32U4"/>
</gates>
<devices>
<device name="QFN" package="SPARKFUN-DIGITALIC_QFN-44">
<connects>
<connect gate="G$1" pin="!RESET" pad="13"/>
<connect gate="G$1" pin="AREF" pad="42"/>
<connect gate="G$1" pin="AVCC@24" pad="24"/>
<connect gate="G$1" pin="AVCC@44" pad="44"/>
<connect gate="G$1" pin="D+" pad="4"/>
<connect gate="G$1" pin="D-" pad="3"/>
<connect gate="G$1" pin="GND@15" pad="15"/>
<connect gate="G$1" pin="GND@23" pad="23"/>
<connect gate="G$1" pin="GND@35" pad="35"/>
<connect gate="G$1" pin="GND@43" pad="43"/>
<connect gate="G$1" pin="PB0(SS)" pad="8"/>
<connect gate="G$1" pin="PB1(SCK)" pad="9"/>
<connect gate="G$1" pin="PB2(MOSI)" pad="10"/>
<connect gate="G$1" pin="PB3(MISO)" pad="11"/>
<connect gate="G$1" pin="PB4(ADC11)" pad="28"/>
<connect gate="G$1" pin="PB5(ADC12)" pad="29"/>
<connect gate="G$1" pin="PB6(ADC13)" pad="30"/>
<connect gate="G$1" pin="PB7" pad="12"/>
<connect gate="G$1" pin="PC6" pad="31"/>
<connect gate="G$1" pin="PC7" pad="32"/>
<connect gate="G$1" pin="PD0(SCL)" pad="18"/>
<connect gate="G$1" pin="PD1(SDA)" pad="19"/>
<connect gate="G$1" pin="PD2(RX)" pad="20"/>
<connect gate="G$1" pin="PD3(TX)" pad="21"/>
<connect gate="G$1" pin="PD4(ADC8)" pad="25"/>
<connect gate="G$1" pin="PD5" pad="22"/>
<connect gate="G$1" pin="PD6(ADC9)" pad="26"/>
<connect gate="G$1" pin="PD7(ADC10)" pad="27"/>
<connect gate="G$1" pin="PE2/!HWB" pad="33"/>
<connect gate="G$1" pin="PE6" pad="1"/>
<connect gate="G$1" pin="PF0(ADC0)" pad="41"/>
<connect gate="G$1" pin="PF1(ADC1)" pad="40"/>
<connect gate="G$1" pin="PF4(ADC4)" pad="39"/>
<connect gate="G$1" pin="PF5(ADC5)" pad="38"/>
<connect gate="G$1" pin="PF6(ADC6)" pad="37"/>
<connect gate="G$1" pin="PF7(ADC7)" pad="36"/>
<connect gate="G$1" pin="UCAP" pad="6"/>
<connect gate="G$1" pin="UGND" pad="5"/>
<connect gate="G$1" pin="UVCC" pad="2"/>
<connect gate="G$1" pin="VBUS" pad="7"/>
<connect gate="G$1" pin="VCC@14" pad="14"/>
<connect gate="G$1" pin="VCC@34" pad="34"/>
<connect gate="G$1" pin="XTAL1" pad="17"/>
<connect gate="G$1" pin="XTAL2" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="QFN2" package="SPARKFUN-DIGITALIC_QFN-44-NOPAD">
<connects>
<connect gate="G$1" pin="!RESET" pad="13"/>
<connect gate="G$1" pin="AREF" pad="42"/>
<connect gate="G$1" pin="AVCC@24" pad="24"/>
<connect gate="G$1" pin="AVCC@44" pad="44"/>
<connect gate="G$1" pin="D+" pad="4"/>
<connect gate="G$1" pin="D-" pad="3"/>
<connect gate="G$1" pin="GND@15" pad="15"/>
<connect gate="G$1" pin="GND@23" pad="23"/>
<connect gate="G$1" pin="GND@35" pad="35"/>
<connect gate="G$1" pin="GND@43" pad="43"/>
<connect gate="G$1" pin="PB0(SS)" pad="8"/>
<connect gate="G$1" pin="PB1(SCK)" pad="9"/>
<connect gate="G$1" pin="PB2(MOSI)" pad="10"/>
<connect gate="G$1" pin="PB3(MISO)" pad="11"/>
<connect gate="G$1" pin="PB4(ADC11)" pad="28"/>
<connect gate="G$1" pin="PB5(ADC12)" pad="29"/>
<connect gate="G$1" pin="PB6(ADC13)" pad="30"/>
<connect gate="G$1" pin="PB7" pad="12"/>
<connect gate="G$1" pin="PC6" pad="31"/>
<connect gate="G$1" pin="PC7" pad="32"/>
<connect gate="G$1" pin="PD0(SCL)" pad="18"/>
<connect gate="G$1" pin="PD1(SDA)" pad="19"/>
<connect gate="G$1" pin="PD2(RX)" pad="20"/>
<connect gate="G$1" pin="PD3(TX)" pad="21"/>
<connect gate="G$1" pin="PD4(ADC8)" pad="25"/>
<connect gate="G$1" pin="PD5" pad="22"/>
<connect gate="G$1" pin="PD6(ADC9)" pad="26"/>
<connect gate="G$1" pin="PD7(ADC10)" pad="27"/>
<connect gate="G$1" pin="PE2/!HWB" pad="33"/>
<connect gate="G$1" pin="PE6" pad="1"/>
<connect gate="G$1" pin="PF0(ADC0)" pad="41"/>
<connect gate="G$1" pin="PF1(ADC1)" pad="40"/>
<connect gate="G$1" pin="PF4(ADC4)" pad="39"/>
<connect gate="G$1" pin="PF5(ADC5)" pad="38"/>
<connect gate="G$1" pin="PF6(ADC6)" pad="37"/>
<connect gate="G$1" pin="PF7(ADC7)" pad="36"/>
<connect gate="G$1" pin="UCAP" pad="6"/>
<connect gate="G$1" pin="UGND" pad="5"/>
<connect gate="G$1" pin="UVCC" pad="2"/>
<connect gate="G$1" pin="VBUS" pad="7"/>
<connect gate="G$1" pin="VCC@14" pad="14"/>
<connect gate="G$1" pin="VCC@34" pad="34"/>
<connect gate="G$1" pin="XTAL1" pad="17"/>
<connect gate="G$1" pin="XTAL2" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TQFP" package="SPARKFUN-DIGITALIC_TQFP44">
<connects>
<connect gate="G$1" pin="!RESET" pad="13"/>
<connect gate="G$1" pin="AREF" pad="42"/>
<connect gate="G$1" pin="AVCC@24" pad="24"/>
<connect gate="G$1" pin="AVCC@44" pad="44"/>
<connect gate="G$1" pin="D+" pad="4"/>
<connect gate="G$1" pin="D-" pad="3"/>
<connect gate="G$1" pin="GND@15" pad="15"/>
<connect gate="G$1" pin="GND@23" pad="23"/>
<connect gate="G$1" pin="GND@35" pad="35"/>
<connect gate="G$1" pin="GND@43" pad="43"/>
<connect gate="G$1" pin="PB0(SS)" pad="8"/>
<connect gate="G$1" pin="PB1(SCK)" pad="9"/>
<connect gate="G$1" pin="PB2(MOSI)" pad="10"/>
<connect gate="G$1" pin="PB3(MISO)" pad="11"/>
<connect gate="G$1" pin="PB4(ADC11)" pad="28"/>
<connect gate="G$1" pin="PB5(ADC12)" pad="29"/>
<connect gate="G$1" pin="PB6(ADC13)" pad="30"/>
<connect gate="G$1" pin="PB7" pad="12"/>
<connect gate="G$1" pin="PC6" pad="31"/>
<connect gate="G$1" pin="PC7" pad="32"/>
<connect gate="G$1" pin="PD0(SCL)" pad="18"/>
<connect gate="G$1" pin="PD1(SDA)" pad="19"/>
<connect gate="G$1" pin="PD2(RX)" pad="20"/>
<connect gate="G$1" pin="PD3(TX)" pad="21"/>
<connect gate="G$1" pin="PD4(ADC8)" pad="25"/>
<connect gate="G$1" pin="PD5" pad="22"/>
<connect gate="G$1" pin="PD6(ADC9)" pad="26"/>
<connect gate="G$1" pin="PD7(ADC10)" pad="27"/>
<connect gate="G$1" pin="PE2/!HWB" pad="33"/>
<connect gate="G$1" pin="PE6" pad="1"/>
<connect gate="G$1" pin="PF0(ADC0)" pad="41"/>
<connect gate="G$1" pin="PF1(ADC1)" pad="40"/>
<connect gate="G$1" pin="PF4(ADC4)" pad="39"/>
<connect gate="G$1" pin="PF5(ADC5)" pad="38"/>
<connect gate="G$1" pin="PF6(ADC6)" pad="37"/>
<connect gate="G$1" pin="PF7(ADC7)" pad="36"/>
<connect gate="G$1" pin="UCAP" pad="6"/>
<connect gate="G$1" pin="UGND" pad="5"/>
<connect gate="G$1" pin="UVCC" pad="2"/>
<connect gate="G$1" pin="VBUS" pad="7"/>
<connect gate="G$1" pin="VCC@14" pad="14"/>
<connect gate="G$1" pin="VCC@34" pad="34"/>
<connect gate="G$1" pin="XTAL1" pad="17"/>
<connect gate="G$1" pin="XTAL2" pad="16"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-11161"/>
</technology>
</technologies>
</device>
<device name="QFN_1:1" package="QFN-44-NOPAD_1:1">
<connects>
<connect gate="G$1" pin="!RESET" pad="13"/>
<connect gate="G$1" pin="AREF" pad="42"/>
<connect gate="G$1" pin="AVCC@24" pad="24"/>
<connect gate="G$1" pin="AVCC@44" pad="44"/>
<connect gate="G$1" pin="D+" pad="4"/>
<connect gate="G$1" pin="D-" pad="3"/>
<connect gate="G$1" pin="GND@15" pad="15"/>
<connect gate="G$1" pin="GND@23" pad="23"/>
<connect gate="G$1" pin="GND@35" pad="35"/>
<connect gate="G$1" pin="GND@43" pad="43"/>
<connect gate="G$1" pin="PB0(SS)" pad="8"/>
<connect gate="G$1" pin="PB1(SCK)" pad="9"/>
<connect gate="G$1" pin="PB2(MOSI)" pad="10"/>
<connect gate="G$1" pin="PB3(MISO)" pad="11"/>
<connect gate="G$1" pin="PB4(ADC11)" pad="28"/>
<connect gate="G$1" pin="PB5(ADC12)" pad="29"/>
<connect gate="G$1" pin="PB6(ADC13)" pad="30"/>
<connect gate="G$1" pin="PB7" pad="12"/>
<connect gate="G$1" pin="PC6" pad="31"/>
<connect gate="G$1" pin="PC7" pad="32"/>
<connect gate="G$1" pin="PD0(SCL)" pad="18"/>
<connect gate="G$1" pin="PD1(SDA)" pad="19"/>
<connect gate="G$1" pin="PD2(RX)" pad="20"/>
<connect gate="G$1" pin="PD3(TX)" pad="21"/>
<connect gate="G$1" pin="PD4(ADC8)" pad="25"/>
<connect gate="G$1" pin="PD5" pad="22"/>
<connect gate="G$1" pin="PD6(ADC9)" pad="26"/>
<connect gate="G$1" pin="PD7(ADC10)" pad="27"/>
<connect gate="G$1" pin="PE2/!HWB" pad="33"/>
<connect gate="G$1" pin="PE6" pad="1"/>
<connect gate="G$1" pin="PF0(ADC0)" pad="41"/>
<connect gate="G$1" pin="PF1(ADC1)" pad="40"/>
<connect gate="G$1" pin="PF4(ADC4)" pad="39"/>
<connect gate="G$1" pin="PF5(ADC5)" pad="38"/>
<connect gate="G$1" pin="PF6(ADC6)" pad="37"/>
<connect gate="G$1" pin="PF7(ADC7)" pad="36"/>
<connect gate="G$1" pin="UCAP" pad="6"/>
<connect gate="G$1" pin="UGND" pad="5"/>
<connect gate="G$1" pin="UVCC" pad="2"/>
<connect gate="G$1" pin="VBUS" pad="7"/>
<connect gate="G$1" pin="VCC@14" pad="14"/>
<connect gate="G$1" pin="VCC@34" pad="34"/>
<connect gate="G$1" pin="XTAL1" pad="17"/>
<connect gate="G$1" pin="XTAL2" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="JUMPER-2" prefix="JP" uservalue="yes">
<description>&lt;b&gt;Jumper&lt;/b&gt;
Basic 0.1" spaced jumper. Use with breakaway headers.</description>
<gates>
<gate name="A" symbol="JUMPER-2"/>
</gates>
<devices>
<device name="PTH" package="1X02">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD-NC" package="SJ_2S">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH_LOCK" package="1X02_LOCK">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD-NO" package="SJ_2S-NO">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD-NO-NS" package="SJ_2S-NO-NS">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="JUMPER-2-OLD" prefix="JP" uservalue="yes">
<description>&lt;b&gt;Jumper&lt;/b&gt;
Basic 0.1" spaced jumper. Use with breakaway headers.</description>
<gates>
<gate name="A" symbol="JUMPER-2"/>
</gates>
<devices>
<device name="PTH" package="1X02">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD-NC" package="SJ_2S">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH_LOCK" package="1X02_LOCK">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD-NO" package="SJ_2S-NO">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="JUMPER-3" prefix="JP">
<gates>
<gate name="G$1" symbol="JUMPER-3"/>
</gates>
<devices>
<device name="SMD" package="SJ_3">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH" package="1X03">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1-2" package="SJ_3_PASTE1&amp;2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="2-3" package="SJ_3_PASTE2&amp;3">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="JUMPER-3-OLD" prefix="JP">
<gates>
<gate name="G$1" symbol="JUMPER-3"/>
</gates>
<devices>
<device name="SMD" package="SJ_3">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH" package="1X03">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1-2" package="SJ_3_PASTE1&amp;2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="2-3" package="SJ_3_PASTE2&amp;3">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SOLDERJUMPER" prefix="SJ">
<description>&lt;b&gt;Solder Jumper&lt;/b&gt;
Standard SMD solder jumper. Used to automate production. Two varients : Normally Open and Normally Closed are the same, but have different paste layers. NC will have a large amount of paste and should jumper during reflow.</description>
<gates>
<gate name="1" symbol="SJ"/>
</gates>
<devices>
<device name="NC" package="SJ_2S">
<connects>
<connect gate="1" pin="1" pad="1"/>
<connect gate="1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TRACE" package="SJ_2S-TRACE">
<connects>
<connect gate="1" pin="1" pad="1"/>
<connect gate="1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="NC2" package="SJ_2S-NOTRACE">
<connects>
<connect gate="1" pin="1" pad="1"/>
<connect gate="1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="NO" package="SJ_2S-NO">
<connects>
<connect gate="1" pin="1" pad="1"/>
<connect gate="1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TRACE-PTH" package="SJ_2S-TRACE-PTH">
<connects>
<connect gate="1" pin="1" pad="1"/>
<connect gate="1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH" package="SJ_2S-PTH">
<connects>
<connect gate="1" pin="1" pad="1"/>
<connect gate="1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="ROUND" package="SJ_ROUND">
<connects>
<connect gate="1" pin="1" pad="1"/>
<connect gate="1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SOLDERJUMPER-OLD" prefix="SJ">
<description>&lt;b&gt;Solder Jumper&lt;/b&gt;
Standard SMD solder jumper. Used to automate production. Two varients : Normally Open and Normally Closed are the same, but have different paste layers. NC will have a large amount of paste and should jumper during reflow.</description>
<gates>
<gate name="1" symbol="SJ"/>
</gates>
<devices>
<device name="NC" package="SJ_2S">
<connects>
<connect gate="1" pin="1" pad="1"/>
<connect gate="1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TRACE" package="SJ_2S-TRACE">
<connects>
<connect gate="1" pin="1" pad="1"/>
<connect gate="1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="NC2" package="SJ_2S-NOTRACE">
<connects>
<connect gate="1" pin="1" pad="1"/>
<connect gate="1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="NO" package="SJ_2S-NO">
<connects>
<connect gate="1" pin="1" pad="1"/>
<connect gate="1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SOLDERJUMPER_2WAY" prefix="SJ" uservalue="yes">
<description>&lt;b&gt;Solder Jumper&lt;/b&gt;
2 way solder jumper</description>
<gates>
<gate name="G$1" symbol="SJ_2"/>
</gates>
<devices>
<device name="W" package="SJ_2W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="T" package="SJ_2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="S" package="SJ_3">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PASTE1&amp;2" package="SJ_3_PASTE1&amp;2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PASTE2&amp;3" package="SJ_3_PASTE2&amp;3">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PASTE1&amp;2&amp;3" package="SJ_3_PASTE1&amp;2&amp;3">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SOLDERJUMPER_2WAY-OLD" prefix="SJ" uservalue="yes">
<description>&lt;b&gt;Solder Jumper&lt;/b&gt;
2 way solder jumper</description>
<gates>
<gate name="G$1" symbol="SJ_2"/>
</gates>
<devices>
<device name="W" package="SJ_2W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="T" package="SJ_2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="S" package="SJ_3">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PASTE1&amp;2" package="SJ_3_PASTE1&amp;2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PASTE2&amp;3" package="SJ_3_PASTE2&amp;3">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FRAME-LETTER" prefix="FRAME">
<description>&lt;b&gt;Schematic Frame&lt;/b&gt;&lt;p&gt;
Standard 8.5x11 US Letter frame</description>
<gates>
<gate name="G$1" symbol="LETTER_L"/>
<gate name="G$2" symbol="DOCFIELD"/>
</gates>
<devices>
<device name="" package="CREATIVE_COMMONS">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TAC_SWITCH" prefix="S" uservalue="yes">
<description>&lt;b&gt;Momentary Switch&lt;/b&gt;&lt;br&gt;
Button commonly used for reset or general input.&lt;br&gt;
Spark Fun Electronics SKU : COM-00097&lt;br&gt;
SMT- SWCH-08247</description>
<gates>
<gate name="S" symbol="SWITCH-MOMENTARY"/>
</gates>
<devices>
<device name="PTH" package="TACTILE-PTH">
<connects>
<connect gate="S" pin="1" pad="1"/>
<connect gate="S" pin="2" pad="2"/>
<connect gate="S" pin="3" pad="3"/>
<connect gate="S" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="KSA_SEALED" package="KSA_SEALED_TAC_SWITCH">
<connects>
<connect gate="S" pin="1" pad="P$1"/>
<connect gate="S" pin="2" pad="P$2"/>
<connect gate="S" pin="3" pad="P$3"/>
<connect gate="S" pin="4" pad="P$4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD" package="TACTILE-SWITCH-SMD">
<connects>
<connect gate="S" pin="1" pad="1"/>
<connect gate="S" pin="2" pad="2"/>
<connect gate="S" pin="3" pad="3"/>
<connect gate="S" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="SWCH-08247"/>
<attribute name="VALUE" value="TAC_SWITCHSMD"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC24FXXXDAX06" prefix="U">
<description>&lt;b&gt;PIC24FXXXDAX06&lt;/b&gt;&lt;br&gt;
PIC24FXXXDA106 / PIC24FXXXDA206&lt;br&gt;
PIC24FJ256DA206-I/PT for IOIO&lt;br&gt;
IC-10386</description>
<gates>
<gate name="G$1" symbol="PIC24FJXXXDAX06"/>
</gates>
<devices>
<device name="" package="PIC24FXXX_TQFP64">
<connects>
<connect gate="G$1" pin="!MCLR" pad="7"/>
<connect gate="G$1" pin="AN14/CTPLS/RP14/CN32/RB14" pad="29"/>
<connect gate="G$1" pin="AN15/RP29/REFO/CN12/RB15" pad="30"/>
<connect gate="G$1" pin="AN2/C2INB/VMIO/RP13/CN4/RB2" pad="14"/>
<connect gate="G$1" pin="AN3/C2INA/VPIO/CN5/RB3" pad="13"/>
<connect gate="G$1" pin="AN8/RP8/CN26/RB8" pad="21"/>
<connect gate="G$1" pin="AN9/RP9/CN27/RB9" pad="22"/>
<connect gate="G$1" pin="AVDD" pad="19"/>
<connect gate="G$1" pin="AVSS" pad="20"/>
<connect gate="G$1" pin="C1INC/RP26/CN9/RG7" pad="5"/>
<connect gate="G$1" pin="C1IND/RP21/CN8/RG6" pad="4"/>
<connect gate="G$1" pin="C2INC/RP27/GD15/CN11/RG9" pad="8"/>
<connect gate="G$1" pin="C2IND/RP19/GD14/CN10/RG8" pad="6"/>
<connect gate="G$1" pin="C3INA/SESSEND/CN16/RD7" pad="55"/>
<connect gate="G$1" pin="C3INB/CN15/RD6" pad="54"/>
<connect gate="G$1" pin="D+/CN83/RG2" pad="37"/>
<connect gate="G$1" pin="D-/CN84/RG3" pad="36"/>
<connect gate="G$1" pin="DMH/RP11/INT0/CN49/RD0" pad="46"/>
<connect gate="G$1" pin="DPH/RP23/CN51/RD2" pad="50"/>
<connect gate="G$1" pin="DPLN/SDA1/RP4/GD8/CN54/RD9" pad="43"/>
<connect gate="G$1" pin="ENVREG" pad="57"/>
<connect gate="G$1" pin="GD0/CN58/RE0" pad="60"/>
<connect gate="G$1" pin="GD1/CN59/RE1" pad="61"/>
<connect gate="G$1" pin="GD10/VBUSST/VCMPST1/VBUSVLD/CN68/RF0" pad="58"/>
<connect gate="G$1" pin="GD11/VCMPST2/SESSVLD/CN69/RF1" pad="59"/>
<connect gate="G$1" pin="GD12/SCL3/CN64/RE6" pad="2"/>
<connect gate="G$1" pin="GD13/SDA3/CN65/RE7" pad="3"/>
<connect gate="G$1" pin="GD2/CN60/RE2" pad="62"/>
<connect gate="G$1" pin="GD3/CN61/RE3" pad="63"/>
<connect gate="G$1" pin="HSYNC/CN62/RE4" pad="64"/>
<connect gate="G$1" pin="OSCI/CLKI/CN23/RC12" pad="39"/>
<connect gate="G$1" pin="OSCO/CLKO/CN22/RC15" pad="40"/>
<connect gate="G$1" pin="PGEC1/AN1/VREF-/RP1/CN3/RB1" pad="15"/>
<connect gate="G$1" pin="PGEC2/AN6/RP6/CN24/RB6" pad="17"/>
<connect gate="G$1" pin="PGEC3/AN5/C1INA/VBUSON/RP18/CN7/RB5" pad="11"/>
<connect gate="G$1" pin="PGED1/AN0/VREF+/RP0/CN2/RB0" pad="16"/>
<connect gate="G$1" pin="PGED2/AN7/RP7/RCV/CN25/RB7" pad="18"/>
<connect gate="G$1" pin="PGED3/AN4/C1INB/USBOEN/RP28/CN6/RB4" pad="12"/>
<connect gate="G$1" pin="RP12/GD7/CN56/RD11" pad="45"/>
<connect gate="G$1" pin="RP16/USBID/CN71/RF3" pad="33"/>
<connect gate="G$1" pin="RP20/GPWR/CN14/RD5" pad="53"/>
<connect gate="G$1" pin="RP22/GEN/CN52/RD3" pad="51"/>
<connect gate="G$1" pin="RP25/GCLK/CN13/RD4" pad="52"/>
<connect gate="G$1" pin="RTCC/DMLN/RP2/CN53/RD8" pad="42"/>
<connect gate="G$1" pin="SCL1/RP3/GD6/CN55/RD10" pad="44"/>
<connect gate="G$1" pin="SCL2/RP17/GD5/CN18/RF5" pad="32"/>
<connect gate="G$1" pin="SDA2/RP10/GD4/CN17/RF4" pad="31"/>
<connect gate="G$1" pin="SOSCI/C3IND/CN1/RC13" pad="47"/>
<connect gate="G$1" pin="SOSCO/SCLKI/T1CK/C3INC/RPI37/CN0/RC14" pad="48"/>
<connect gate="G$1" pin="TCK/AN12/CTEDG2/CN30/RB12" pad="27"/>
<connect gate="G$1" pin="TDI/AN13/CTEDG1/CN31/RB13" pad="28"/>
<connect gate="G$1" pin="TDO/AN11/CN29/RB11" pad="24"/>
<connect gate="G$1" pin="TMS/CVREF/AN10/CN28/RB10" pad="23"/>
<connect gate="G$1" pin="VBUS/RF7" pad="34"/>
<connect gate="G$1" pin="VCAP" pad="56"/>
<connect gate="G$1" pin="VCPCON/RP24/GD9/VBUSCHG/CN50/RD1" pad="49"/>
<connect gate="G$1" pin="VDD@1" pad="10"/>
<connect gate="G$1" pin="VDD@2" pad="26"/>
<connect gate="G$1" pin="VDD@3" pad="38"/>
<connect gate="G$1" pin="VSS@1" pad="9"/>
<connect gate="G$1" pin="VSS@2" pad="25"/>
<connect gate="G$1" pin="VSS@3" pad="41"/>
<connect gate="G$1" pin="VSYNC/CN63/RE5" pad="1"/>
<connect gate="G$1" pin="VUSB" pad="35"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-10386"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
