<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<library>
<packages>
<package name="PDIP">
</package>
<package name="SOIC127P600X175-8N">
</package>
</packages>
<symbols>
<symbol name="AT24MAC402">
<pin name="VCC" direction="pwr"/>
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="WP" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="SDA"/>
<pin name="SCL" direction="in"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="24MAC402-SSHM-T" prefix="U">
<description>EEPROM, SERIAL, 2KB, 48-BIT MAC, 8SOIC</description>
<gates>
<gate name="A" symbol="AT24MAC402"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="A0" pad="1"/>
<connect gate="A" pin="A1" pad="2"/>
<connect gate="A" pin="A2" pad="3"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="SCL" pad="6"/>
<connect gate="A" pin="SDA" pad="5"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="WP" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="24MAC402-SSHM-T"/>
<attribute name="OC_FARNELL" value="2134868"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="PACKAGE" value="8SOIC"/>
<attribute name="SUPPLIER" value="ATMEL"/>
</technology>
</technologies>
</device>
<device name="PDIP" package="PDIP">
<connects>
<connect gate="A" pin="A0" pad="1"/>
<connect gate="A" pin="A1" pad="2"/>
<connect gate="A" pin="A2" pad="3"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="SCL" pad="6"/>
<connect gate="A" pin="SDA" pad="5"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="WP" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
