<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.3.0">
<drawing>
<library>
<description>&lt;b&gt;USB-Controller from Future Technology Devices International Ltd.&lt;/b&gt; 
&lt;br&gt;&lt;br&gt;
Based on the source of the libraries ftdichip-4.lbr and ftdichip-2.lbr.&lt;br&gt;
With new Vinculum-II Chips.&lt;br&gt;

Includes the following controller:&lt;br&gt;
&lt;ul&gt;
&lt;li&gt;FT232BL , FT245BL (2nd generation)
&lt;li&gt;FT2232L (3rd generation)
&lt;li&gt;FT232RL , FT245RL (4th generation)
&lt;li&gt;FT4232HL (5th generation)
&lt;li&gt;VNC1L
&lt;li&gt;VNC2-32
&lt;li&gt;VNC2-48 (symbol compatible&lt;sup&gt;*&lt;/sup&gt; with VNC1L)
&lt;li&gt;VNC2-64
&lt;/ul&gt;
http://www.ftdichip.com

&lt;br&gt;&lt;br&gt;

Originally by:
&lt;ul&gt;
&lt;li&gt;B.Redemann, 4232 by R.Pearce (ftdichip-4.lbr)
&lt;li&gt;Paul Carpenter, PC Services www.pcserviceselectronics.co.uk (ftdichip-2.lbr)
&lt;/ul&gt;
Updated with Vinculum-II by Marcin Zakaszewski.</description>
<packages>
<package name="LQFP32">
<description>&lt;b&gt;LQFP-32 package&lt;/b&gt;&lt;p&gt;
7x7 mm case, 0.8 mm lead pitch</description>
</package>
<package name="SSOP28DB">
<description>&lt;b&gt;Small Shrink Outline Package&lt;/b&gt;</description>
</package>
<package name="LQFP64">
<description>&lt;b&gt;LQFP-64 package&lt;/b&gt;&lt;p&gt;
10x10 mm case, 0.5 mm lead pitch</description>
</package>
<package name="LQFP48">
<description>&lt;b&gt;LQFP-48 package&lt;/b&gt;&lt;p&gt;
7x7 mm case, 0.5 mm lead pitch</description>
</package>
</packages>
<symbols>
<symbol name="FT232BL">
<pin name="3V3OUT" direction="out"/>
<pin name="USBDM"/>
<pin name="USBDP"/>
<pin name="RSTOUT#" direction="out" function="dot"/>
<pin name="RESET#" direction="in" function="dot"/>
<pin name="XTIN" direction="in"/>
<pin name="XTOUT" direction="out"/>
<pin name="EECS"/>
<pin name="EESK" direction="out"/>
<pin name="EEDATA"/>
<pin name="TXD" direction="out"/>
<pin name="RXD" direction="in"/>
<pin name="RTS#" direction="out" function="dot"/>
<pin name="CTS#" direction="in" function="dot"/>
<pin name="DTR#" direction="out" function="dot"/>
<pin name="DSR#" direction="in" function="dot"/>
<pin name="DCD#" direction="in" function="dot"/>
<pin name="RI#" direction="in" function="dot"/>
<pin name="TXDEN" direction="out"/>
<pin name="TXLED#" direction="oc" function="dot"/>
<pin name="RXLED#" direction="oc" function="dot"/>
<pin name="PWRCTL" direction="in"/>
<pin name="PWREN#" direction="out" function="dot"/>
<pin name="SLEEP#" direction="out" function="dot"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="AVCC" direction="pwr"/>
<pin name="AGND" direction="pwr"/>
<pin name="TEST" direction="in"/>
<pin name="VCC1" direction="pwr"/>
<pin name="VCC2" direction="pwr"/>
<pin name="GND1" direction="pwr"/>
<pin name="GND2" direction="pwr"/>
</symbol>
<symbol name="FT245BL">
<pin name="AVCC" direction="pwr"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="3V3OUT" direction="out"/>
<pin name="USBDM"/>
<pin name="USBDP"/>
<pin name="RSTOUT#" direction="out" function="dot"/>
<pin name="RESET#" direction="in" function="dot"/>
<pin name="XTIN" direction="in"/>
<pin name="XTOUT" direction="out"/>
<pin name="EECS"/>
<pin name="EEDATA"/>
<pin name="EESK" direction="out"/>
<pin name="TEST" direction="in"/>
<pin name="AGND" direction="pwr"/>
<pin name="D0"/>
<pin name="D1"/>
<pin name="D2"/>
<pin name="D3"/>
<pin name="D4"/>
<pin name="D5"/>
<pin name="D6"/>
<pin name="D7"/>
<pin name="RD#" direction="in" function="dot"/>
<pin name="WR" direction="in"/>
<pin name="TXE#" direction="out" function="dot"/>
<pin name="RXF#" direction="out" function="dot"/>
<pin name="PWREN#" direction="out" function="dot"/>
<pin name="SI/WU" direction="in"/>
<pin name="GND1" direction="pwr"/>
<pin name="GND2" direction="pwr"/>
<pin name="VCC1" direction="pwr"/>
<pin name="VCC2" direction="pwr"/>
</symbol>
<symbol name="FT2232C">
<pin name="ADBUS0"/>
<pin name="ADBUS1"/>
<pin name="ADBUS2"/>
<pin name="ADBUS3"/>
<pin name="ADBUS4"/>
<pin name="ADBUS5"/>
<pin name="ADBUS6"/>
<pin name="ADBUS7"/>
<pin name="ACBUS0"/>
<pin name="ACBUS1"/>
<pin name="ACBUS2"/>
<pin name="ACBUS3"/>
<pin name="SI/WUA"/>
<pin name="BDBUS0"/>
<pin name="BDBUS1"/>
<pin name="BDBUS2"/>
<pin name="BDBUS3"/>
<pin name="BDBUS4"/>
<pin name="BDBUS5"/>
<pin name="BDBUS6"/>
<pin name="BDBUS7"/>
<pin name="BCBUS0"/>
<pin name="BCBUS1"/>
<pin name="BCBUS2"/>
<pin name="BCBUS3"/>
<pin name="SI/WUB"/>
<pin name="PWREN#" function="dot"/>
<pin name="GND0"/>
<pin name="GND1"/>
<pin name="GND2"/>
<pin name="GND3"/>
<pin name="AGND"/>
<pin name="VCCIOB"/>
<pin name="VCCIOA"/>
<pin name="VCC1"/>
<pin name="VCC0"/>
<pin name="AVVC"/>
<pin name="3V3OUT"/>
<pin name="USBDM"/>
<pin name="USBDP"/>
<pin name="RSTOUT#" function="dot"/>
<pin name="RESET#" function="dot"/>
<pin name="XTIN"/>
<pin name="XTOUT"/>
<pin name="EECS"/>
<pin name="EESK"/>
<pin name="EEDATA"/>
<pin name="TEST"/>
</symbol>
<symbol name="FT232R">
<pin name="3V3OUT" direction="out"/>
<pin name="USBDM"/>
<pin name="USBDP"/>
<pin name="RESET#" direction="in" function="dot"/>
<pin name="OSCI" direction="in"/>
<pin name="OSCO" direction="out"/>
<pin name="GND1" direction="pwr"/>
<pin name="GND2" direction="pwr"/>
<pin name="GND3" direction="pwr"/>
<pin name="TXD" direction="out"/>
<pin name="RXD" direction="in"/>
<pin name="RTS#" direction="out" function="dot"/>
<pin name="CTS#" direction="in" function="dot"/>
<pin name="DTR#" direction="out" function="dot"/>
<pin name="DSR#" direction="in" function="dot"/>
<pin name="DCD#" direction="in" function="dot"/>
<pin name="RI#" direction="in" function="dot"/>
<pin name="CBUS0"/>
<pin name="CBUS1"/>
<pin name="CBUS2"/>
<pin name="CBUS3"/>
<pin name="CBUS4"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="AGND" direction="pwr"/>
<pin name="TEST" direction="in"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="FT245R">
<pin name="3V3OUT" direction="out"/>
<pin name="USBDM"/>
<pin name="USBDP"/>
<pin name="RESET#" direction="in" function="dot"/>
<pin name="OSCI" direction="in"/>
<pin name="OSCO" direction="out"/>
<pin name="GND1" direction="pwr"/>
<pin name="GND2" direction="pwr"/>
<pin name="GND3" direction="pwr"/>
<pin name="D0" direction="out"/>
<pin name="D1" direction="in"/>
<pin name="D2" direction="out"/>
<pin name="D3" direction="in"/>
<pin name="D4" direction="out"/>
<pin name="D5" direction="in"/>
<pin name="D6" direction="in"/>
<pin name="D7" direction="in"/>
<pin name="RXF#" function="dot"/>
<pin name="TXE#" function="dot"/>
<pin name="RD#" function="dot"/>
<pin name="WR"/>
<pin name="PWREN#"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="AGND" direction="pwr"/>
<pin name="TEST" direction="in"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="4232CORE">
<pin name="SUSPEND#" direction="out" function="dot"/>
<pin name="PWREN#" direction="out" function="dot"/>
<pin name="GND@6" direction="pwr"/>
<pin name="GND@5" direction="pwr"/>
<pin name="GND@4" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
<pin name="AGND" direction="pwr"/>
<pin name="VCCIO@2" direction="pwr"/>
<pin name="VCCIO@1" direction="pwr"/>
<pin name="VCORE@3" direction="pwr"/>
<pin name="VCORE@2" direction="pwr"/>
<pin name="VPLL" direction="pwr"/>
<pin name="VREGIN"/>
<pin name="USBDM" direction="in"/>
<pin name="USBDP" direction="in"/>
<pin name="REF" direction="in"/>
<pin name="RESET#" direction="in" function="dot"/>
<pin name="XTIN" direction="in"/>
<pin name="XTOUT" direction="out"/>
<pin name="EECS"/>
<pin name="EECLK" direction="out"/>
<pin name="EEDATA"/>
<pin name="TEST" direction="in"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@7" direction="pwr"/>
<pin name="GND@8" direction="pwr"/>
<pin name="VCCIO@3" direction="pwr"/>
<pin name="VCCIO@4" direction="pwr"/>
<pin name="VCORE@1" direction="pwr"/>
<pin name="VPHY" direction="pwr"/>
<pin name="VREGOUT" direction="out"/>
</symbol>
<symbol name="4232PORT">
<pin name="DB0/TXD"/>
<pin name="DB1/RXD"/>
<pin name="DB2/RTS"/>
<pin name="DB3/CTS"/>
<pin name="DB4/DTR"/>
<pin name="DB5/DSR"/>
<pin name="DB6/DCD"/>
<pin name="DB7/RI"/>
</symbol>
<symbol name="VNC1L">
<pin name="VCCIO@1" direction="pwr"/>
<pin name="VCCIO@2" direction="pwr"/>
<pin name="VCCIO@3" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="AVCC" direction="pwr"/>
<pin name="ADBUS0"/>
<pin name="ADBUS1"/>
<pin name="ADBUS2"/>
<pin name="ADBUS3"/>
<pin name="ADBUS4"/>
<pin name="ADBUS5"/>
<pin name="ADBUS6"/>
<pin name="ADBUS7"/>
<pin name="ACBUS0"/>
<pin name="ACBUS1"/>
<pin name="ACBUS2"/>
<pin name="ACBUS3"/>
<pin name="ACBUS4"/>
<pin name="ACBUS5"/>
<pin name="ACBUS6"/>
<pin name="ACBUS7"/>
<pin name="BDBUS0"/>
<pin name="BDBUS1"/>
<pin name="BDBUS2"/>
<pin name="BDBUS3"/>
<pin name="BDBUS4"/>
<pin name="BDBUS5"/>
<pin name="BDBUS6"/>
<pin name="BDBUS7"/>
<pin name="BCBUS0"/>
<pin name="BCBUS1"/>
<pin name="BCBUS2"/>
<pin name="BCBUS3"/>
<pin name="USB1DM"/>
<pin name="USB1DP"/>
<pin name="USB2DM"/>
<pin name="USB2DP"/>
<pin name="XTIN" direction="in"/>
<pin name="XTOUT" direction="out"/>
<pin name="RESET#" direction="in" function="dot"/>
<pin name="PROG#" direction="in" function="dot"/>
<pin name="PLLFLTR" direction="in"/>
<pin name="TEST" direction="in"/>
<pin name="AGND" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
<pin name="GND@4" direction="pwr"/>
</symbol>
<symbol name="VNC2-32">
<pin name="VCCIO@1" direction="pwr"/>
<pin name="VCCIO@2" direction="pwr"/>
<pin name="VCCIO@3" direction="pwr"/>
<pin name="VREG_IN" direction="pwr"/>
<pin name="VCCPLL_IN" direction="pwr"/>
<pin name="IOBUS0"/>
<pin name="IOBUS1"/>
<pin name="IOBUS2"/>
<pin name="IOBUS3"/>
<pin name="IOBUS4"/>
<pin name="IOBUS5"/>
<pin name="IOBUS6"/>
<pin name="IOBUS7"/>
<pin name="IOBUS8"/>
<pin name="IOBUS9"/>
<pin name="IOBUS10"/>
<pin name="IOBUS11"/>
<pin name="USB1DM"/>
<pin name="USB1DP"/>
<pin name="USB2DM"/>
<pin name="USB2DP"/>
<pin name="XTIN" direction="in"/>
<pin name="XTOUT" direction="out"/>
<pin name="RESET#" direction="in" function="dot"/>
<pin name="PROG#" direction="in" function="dot"/>
<pin name="VREG_OUT" direction="out"/>
<pin name="TEST" direction="in"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GNDPLL" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
<pin name="GND@4" direction="pwr"/>
</symbol>
<symbol name="VNC2-48">
<pin name="VCCIO@1" direction="pwr"/>
<pin name="VCCIO@2" direction="pwr"/>
<pin name="VCCIO@3" direction="pwr"/>
<pin name="VREG_IN" direction="pwr"/>
<pin name="VCCPLL_IN" direction="pwr"/>
<pin name="IOBUS12"/>
<pin name="IOBUS13"/>
<pin name="IOBUS14"/>
<pin name="IOBUS15"/>
<pin name="IOBUS16"/>
<pin name="IOBUS17"/>
<pin name="IOBUS18"/>
<pin name="IOBUS19"/>
<pin name="IOBUS20"/>
<pin name="IOBUS21"/>
<pin name="IOBUS22"/>
<pin name="IOBUS23"/>
<pin name="IOBUS24"/>
<pin name="IOBUS25"/>
<pin name="IOBUS26"/>
<pin name="IOBUS27"/>
<pin name="IOBUS0"/>
<pin name="IOBUS1"/>
<pin name="IOBUS2"/>
<pin name="IOBUS3"/>
<pin name="IOBUS4"/>
<pin name="IOBUS5"/>
<pin name="IOBUS6"/>
<pin name="IOBUS7"/>
<pin name="IOBUS8"/>
<pin name="IOBUS9"/>
<pin name="IOBUS10"/>
<pin name="IOBUS11"/>
<pin name="USB1DM"/>
<pin name="USB1DP"/>
<pin name="USB2DM"/>
<pin name="USB2DP"/>
<pin name="XTIN" direction="in"/>
<pin name="XTOUT" direction="out"/>
<pin name="RESET#" direction="in" function="dot"/>
<pin name="PROG#" direction="in" function="dot"/>
<pin name="VREG_OUT" direction="out"/>
<pin name="TEST" direction="in"/>
<pin name="GNDPLL" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
<pin name="GND@4" direction="pwr"/>
</symbol>
<symbol name="VNC2-64CORE">
<pin name="VCCIO@1" direction="pwr"/>
<pin name="VCCIO@2" direction="pwr"/>
<pin name="VCCIO@3" direction="pwr"/>
<pin name="VREG_IN" direction="pwr"/>
<pin name="VCCPLL_IN" direction="pwr"/>
<pin name="USB1DM"/>
<pin name="USB1DP"/>
<pin name="USB2DM"/>
<pin name="USB2DP"/>
<pin name="XTIN" direction="in"/>
<pin name="XTOUT" direction="out"/>
<pin name="RESET#" direction="in" function="dot"/>
<pin name="PROG#" direction="in" function="dot"/>
<pin name="VREG_OUT" direction="out"/>
<pin name="TEST" direction="in"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GNDPLL" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
<pin name="GND@4" direction="pwr"/>
</symbol>
<symbol name="VNC2-64PORT1">
<pin name="IOBUS0"/>
<pin name="IOBUS1"/>
<pin name="IOBUS2"/>
<pin name="IOBUS3"/>
<pin name="IOBUS4"/>
<pin name="IOBUS5"/>
<pin name="IOBUS6"/>
<pin name="IOBUS7"/>
</symbol>
<symbol name="VNC2-64PORT2">
<pin name="IOBUS8"/>
<pin name="IOBUS9"/>
<pin name="IOBUS10"/>
<pin name="IOBUS11"/>
<pin name="IOBUS12"/>
<pin name="IOBUS13"/>
<pin name="IOBUS14"/>
<pin name="IOBUS15"/>
</symbol>
<symbol name="VNC2-64PORT3">
<pin name="IOBUS16"/>
<pin name="IOBUS17"/>
<pin name="IOBUS18"/>
<pin name="IOBUS19"/>
<pin name="IOBUS20"/>
<pin name="IOBUS21"/>
<pin name="IOBUS22"/>
<pin name="IOBUS23"/>
</symbol>
<symbol name="VNC2-64PORT4">
<pin name="IOBUS24"/>
<pin name="IOBUS25"/>
<pin name="IOBUS26"/>
<pin name="IOBUS27"/>
<pin name="IOBUS28"/>
<pin name="IOBUS29"/>
<pin name="IOBUS30"/>
<pin name="IOBUS31"/>
</symbol>
<symbol name="VNC2-64PORT5">
<pin name="IOBUS32"/>
<pin name="IOBUS33"/>
<pin name="IOBUS34"/>
<pin name="IOBUS35"/>
<pin name="IOBUS36"/>
<pin name="IOBUS37"/>
<pin name="IOBUS38"/>
<pin name="IOBUS39"/>
</symbol>
<symbol name="VNC2-64PORT6">
<pin name="IOBUS40"/>
<pin name="IOBUS41"/>
<pin name="IOBUS42"/>
<pin name="IOBUS43"/>
</symbol>
<symbol name="FT232H">
<description>FTDI FT232H High Speed USB 2.0 Slave Controller</description>
<pin name="VREGIN" direction="pwr"/>
<pin name="VCCD" direction="pwr"/>
<pin name="VCCCORE" direction="pwr"/>
<pin name="VCCA" direction="pwr"/>
<pin name="VPHY" direction="pwr"/>
<pin name="VPLL" direction="pwr"/>
<pin name="VCCIO1" direction="pwr"/>
<pin name="VCCIO2" direction="pwr"/>
<pin name="VCCIO3" direction="pwr"/>
<pin name="AGND1" direction="pwr"/>
<pin name="AGND2" direction="pwr"/>
<pin name="AGND3" direction="pwr"/>
<pin name="GND1" direction="pwr"/>
<pin name="GND2" direction="pwr"/>
<pin name="GND3" direction="pwr"/>
<pin name="GND4" direction="pwr"/>
<pin name="GND5" direction="pwr"/>
<pin name="GND6" direction="pwr"/>
<pin name="GND7" direction="pwr"/>
<pin name="GND8" direction="pwr"/>
<pin name="DP"/>
<pin name="DM" function="dot"/>
<pin name="RESET#"/>
<pin name="REF"/>
<pin name="EECS"/>
<pin name="EECLK"/>
<pin name="EEDATA"/>
<pin name="TEST"/>
<pin name="XCSI"/>
<pin name="XCSO"/>
<pin name="ADBUS0"/>
<pin name="ADBUS1"/>
<pin name="ADBUS2"/>
<pin name="ADBUS3"/>
<pin name="ADBUS4"/>
<pin name="ADBUS5"/>
<pin name="ADBUS6"/>
<pin name="ADBUS7"/>
<pin name="ACBUS0"/>
<pin name="ACBUS1"/>
<pin name="ACBUS2"/>
<pin name="ACBUS3"/>
<pin name="ACBUS4"/>
<pin name="ACBUS5"/>
<pin name="ACBUS6"/>
<pin name="ACBUS7"/>
<pin name="ACBUS8"/>
<pin name="ACBUS9"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="FT232BL" prefix="U">
<description>&lt;b&gt;USB UART&lt;/b&gt;
&lt;p&gt;
2&lt;sup&gt;nd&lt;/sup&gt; Generation USB UART (USB &amp;lt;-&amp;gt; Serial) Controller
&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="FT232BL"/>
</gates>
<devices>
<device name="" package="LQFP32">
<connects>
<connect gate="G$1" pin="3V3OUT" pad="6"/>
<connect gate="G$1" pin="AGND" pad="29"/>
<connect gate="G$1" pin="AVCC" pad="30"/>
<connect gate="G$1" pin="CTS#" pad="22"/>
<connect gate="G$1" pin="DCD#" pad="19"/>
<connect gate="G$1" pin="DSR#" pad="20"/>
<connect gate="G$1" pin="DTR#" pad="21"/>
<connect gate="G$1" pin="EECS" pad="32"/>
<connect gate="G$1" pin="EEDATA" pad="2"/>
<connect gate="G$1" pin="EESK" pad="1"/>
<connect gate="G$1" pin="GND1" pad="9"/>
<connect gate="G$1" pin="GND2" pad="17"/>
<connect gate="G$1" pin="PWRCTL" pad="14"/>
<connect gate="G$1" pin="PWREN#" pad="15"/>
<connect gate="G$1" pin="RESET#" pad="4"/>
<connect gate="G$1" pin="RI#" pad="18"/>
<connect gate="G$1" pin="RSTOUT#" pad="5"/>
<connect gate="G$1" pin="RTS#" pad="23"/>
<connect gate="G$1" pin="RXD" pad="24"/>
<connect gate="G$1" pin="RXLED#" pad="11"/>
<connect gate="G$1" pin="SLEEP#" pad="10"/>
<connect gate="G$1" pin="TEST" pad="31"/>
<connect gate="G$1" pin="TXD" pad="25"/>
<connect gate="G$1" pin="TXDEN" pad="16"/>
<connect gate="G$1" pin="TXLED#" pad="12"/>
<connect gate="G$1" pin="USBDM" pad="8"/>
<connect gate="G$1" pin="USBDP" pad="7"/>
<connect gate="G$1" pin="VCC1" pad="3"/>
<connect gate="G$1" pin="VCC2" pad="26"/>
<connect gate="G$1" pin="VCCIO" pad="13"/>
<connect gate="G$1" pin="XTIN" pad="27"/>
<connect gate="G$1" pin="XTOUT" pad="28"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FT245BL" prefix="U" uservalue="yes">
<description>&lt;b&gt;USB FIFO&lt;/b&gt;
&lt;p&gt;
2&lt;sup&gt;nd&lt;/sup&gt; Generation USB FIFO (USB &amp;lt;-&amp;gt; Parallel) Controller
&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="FT232BL"/>
</gates>
<devices>
<device name="" package="LQFP32">
<connects>
<connect gate="G$1" pin="3V3OUT" pad="6"/>
<connect gate="G$1" pin="AGND" pad="29"/>
<connect gate="G$1" pin="AVCC" pad="30"/>
<connect gate="G$1" pin="CTS#" pad="22"/>
<connect gate="G$1" pin="DCD#" pad="19"/>
<connect gate="G$1" pin="DSR#" pad="20"/>
<connect gate="G$1" pin="DTR#" pad="21"/>
<connect gate="G$1" pin="EECS" pad="32"/>
<connect gate="G$1" pin="EEDATA" pad="2"/>
<connect gate="G$1" pin="EESK" pad="1"/>
<connect gate="G$1" pin="GND1" pad="9"/>
<connect gate="G$1" pin="GND2" pad="17"/>
<connect gate="G$1" pin="PWRCTL" pad="14"/>
<connect gate="G$1" pin="PWREN#" pad="15"/>
<connect gate="G$1" pin="RESET#" pad="4"/>
<connect gate="G$1" pin="RI#" pad="18"/>
<connect gate="G$1" pin="RSTOUT#" pad="5"/>
<connect gate="G$1" pin="RTS#" pad="23"/>
<connect gate="G$1" pin="RXD" pad="24"/>
<connect gate="G$1" pin="RXLED#" pad="11"/>
<connect gate="G$1" pin="SLEEP#" pad="10"/>
<connect gate="G$1" pin="TEST" pad="31"/>
<connect gate="G$1" pin="TXD" pad="25"/>
<connect gate="G$1" pin="TXDEN" pad="16"/>
<connect gate="G$1" pin="TXLED#" pad="12"/>
<connect gate="G$1" pin="USBDM" pad="8"/>
<connect gate="G$1" pin="USBDP" pad="7"/>
<connect gate="G$1" pin="VCC1" pad="3"/>
<connect gate="G$1" pin="VCC2" pad="26"/>
<connect gate="G$1" pin="VCCIO" pad="13"/>
<connect gate="G$1" pin="XTIN" pad="27"/>
<connect gate="G$1" pin="XTOUT" pad="28"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FT2232L" prefix="U" uservalue="yes">
<description>&lt;b&gt;USB UART / FIFO Controller&lt;/b&gt;
&lt;p&gt;
3&lt;sup&gt;nd&lt;/sup&gt; Generation USB Double-UART (USB &amp;lt;-&amp;gt; Serial) - FIFO Controller
&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="FT2232C"/>
</gates>
<devices>
<device name="" package="LQFP48">
<connects>
<connect gate="G$1" pin="3V3OUT" pad="6"/>
<connect gate="G$1" pin="ACBUS0" pad="15"/>
<connect gate="G$1" pin="ACBUS1" pad="13"/>
<connect gate="G$1" pin="ACBUS2" pad="12"/>
<connect gate="G$1" pin="ACBUS3" pad="11"/>
<connect gate="G$1" pin="ADBUS0" pad="24"/>
<connect gate="G$1" pin="ADBUS1" pad="23"/>
<connect gate="G$1" pin="ADBUS2" pad="22"/>
<connect gate="G$1" pin="ADBUS3" pad="21"/>
<connect gate="G$1" pin="ADBUS4" pad="20"/>
<connect gate="G$1" pin="ADBUS5" pad="19"/>
<connect gate="G$1" pin="ADBUS6" pad="17"/>
<connect gate="G$1" pin="ADBUS7" pad="16"/>
<connect gate="G$1" pin="AGND" pad="45"/>
<connect gate="G$1" pin="AVVC" pad="46"/>
<connect gate="G$1" pin="BCBUS0" pad="30"/>
<connect gate="G$1" pin="BCBUS1" pad="29"/>
<connect gate="G$1" pin="BCBUS2" pad="28"/>
<connect gate="G$1" pin="BCBUS3" pad="27"/>
<connect gate="G$1" pin="BDBUS0" pad="40"/>
<connect gate="G$1" pin="BDBUS1" pad="39"/>
<connect gate="G$1" pin="BDBUS2" pad="38"/>
<connect gate="G$1" pin="BDBUS3" pad="37"/>
<connect gate="G$1" pin="BDBUS4" pad="36"/>
<connect gate="G$1" pin="BDBUS5" pad="35"/>
<connect gate="G$1" pin="BDBUS6" pad="33"/>
<connect gate="G$1" pin="BDBUS7" pad="32"/>
<connect gate="G$1" pin="EECS" pad="48"/>
<connect gate="G$1" pin="EEDATA" pad="2"/>
<connect gate="G$1" pin="EESK" pad="1"/>
<connect gate="G$1" pin="GND0" pad="9"/>
<connect gate="G$1" pin="GND1" pad="18"/>
<connect gate="G$1" pin="GND2" pad="25"/>
<connect gate="G$1" pin="GND3" pad="34"/>
<connect gate="G$1" pin="PWREN#" pad="41"/>
<connect gate="G$1" pin="RESET#" pad="4"/>
<connect gate="G$1" pin="RSTOUT#" pad="5"/>
<connect gate="G$1" pin="SI/WUA" pad="10"/>
<connect gate="G$1" pin="SI/WUB" pad="26"/>
<connect gate="G$1" pin="TEST" pad="47"/>
<connect gate="G$1" pin="USBDM" pad="8"/>
<connect gate="G$1" pin="USBDP" pad="7"/>
<connect gate="G$1" pin="VCC0" pad="3"/>
<connect gate="G$1" pin="VCC1" pad="42"/>
<connect gate="G$1" pin="VCCIOA" pad="14"/>
<connect gate="G$1" pin="VCCIOB" pad="31"/>
<connect gate="G$1" pin="XTIN" pad="43"/>
<connect gate="G$1" pin="XTOUT" pad="44"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FT232RL" prefix="U" uservalue="yes">
<description>&lt;b&gt;USB UART&lt;/b&gt;
&lt;p&gt;
4&lt;sup&gt;th&lt;/sup&gt; Generation USB UART (USB &amp;lt;-&amp;gt; Serial) Controller
&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="FT232R"/>
</gates>
<devices>
<device name="" package="SSOP28DB">
<connects>
<connect gate="G$1" pin="3V3OUT" pad="17"/>
<connect gate="G$1" pin="AGND" pad="25"/>
<connect gate="G$1" pin="CBUS0" pad="23"/>
<connect gate="G$1" pin="CBUS1" pad="22"/>
<connect gate="G$1" pin="CBUS2" pad="13"/>
<connect gate="G$1" pin="CBUS3" pad="14"/>
<connect gate="G$1" pin="CBUS4" pad="12"/>
<connect gate="G$1" pin="CTS#" pad="11"/>
<connect gate="G$1" pin="DCD#" pad="10"/>
<connect gate="G$1" pin="DSR#" pad="9"/>
<connect gate="G$1" pin="DTR#" pad="2"/>
<connect gate="G$1" pin="GND1" pad="7"/>
<connect gate="G$1" pin="GND2" pad="18"/>
<connect gate="G$1" pin="GND3" pad="21"/>
<connect gate="G$1" pin="OSCI" pad="27"/>
<connect gate="G$1" pin="OSCO" pad="28"/>
<connect gate="G$1" pin="RESET#" pad="19"/>
<connect gate="G$1" pin="RI#" pad="6"/>
<connect gate="G$1" pin="RTS#" pad="3"/>
<connect gate="G$1" pin="RXD" pad="5"/>
<connect gate="G$1" pin="TEST" pad="26"/>
<connect gate="G$1" pin="TXD" pad="1"/>
<connect gate="G$1" pin="USBDM" pad="16"/>
<connect gate="G$1" pin="USBDP" pad="15"/>
<connect gate="G$1" pin="VCC" pad="20"/>
<connect gate="G$1" pin="VCCIO" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FT232RQ" prefix="U" uservalue="yes">
<description>&lt;b&gt;USB UART&lt;/b&gt;
&lt;p&gt;
4&lt;sup&gt;th&lt;/sup&gt; Generation USB UART (USB &amp;lt;-&amp;gt; Serial) Controller
&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="FT232R"/>
</gates>
<devices>
<device name="" package="LQFP32">
<connects>
<connect gate="G$1" pin="3V3OUT" pad="16"/>
<connect gate="G$1" pin="AGND" pad="24"/>
<connect gate="G$1" pin="CBUS0" pad="22"/>
<connect gate="G$1" pin="CBUS1" pad="21"/>
<connect gate="G$1" pin="CBUS2" pad="10"/>
<connect gate="G$1" pin="CBUS3" pad="11"/>
<connect gate="G$1" pin="CBUS4" pad="9"/>
<connect gate="G$1" pin="CTS#" pad="8"/>
<connect gate="G$1" pin="DCD#" pad="7"/>
<connect gate="G$1" pin="DSR#" pad="6"/>
<connect gate="G$1" pin="DTR#" pad="31"/>
<connect gate="G$1" pin="GND1" pad="4"/>
<connect gate="G$1" pin="GND2" pad="17"/>
<connect gate="G$1" pin="GND3" pad="20"/>
<connect gate="G$1" pin="OSCI" pad="27"/>
<connect gate="G$1" pin="OSCO" pad="28"/>
<connect gate="G$1" pin="RESET#" pad="18"/>
<connect gate="G$1" pin="RI#" pad="3"/>
<connect gate="G$1" pin="RTS#" pad="32"/>
<connect gate="G$1" pin="RXD" pad="2"/>
<connect gate="G$1" pin="TEST" pad="26"/>
<connect gate="G$1" pin="TXD" pad="30"/>
<connect gate="G$1" pin="USBDM" pad="15"/>
<connect gate="G$1" pin="USBDP" pad="14"/>
<connect gate="G$1" pin="VCC" pad="19"/>
<connect gate="G$1" pin="VCCIO" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FT245RL">
<description>&lt;b&gt;USB FIFO Controller&lt;/b&gt;
&lt;p&gt;
4&lt;sup&gt;th&lt;/sup&gt; Generation USB Controller (USB &amp;lt;-&amp;gt; Parallel) - FIFO &lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="FT245R"/>
</gates>
<devices>
<device name="" package="SSOP28DB">
<connects>
<connect gate="G$1" pin="3V3OUT" pad="17"/>
<connect gate="G$1" pin="AGND" pad="25"/>
<connect gate="G$1" pin="D0" pad="1"/>
<connect gate="G$1" pin="D1" pad="5"/>
<connect gate="G$1" pin="D2" pad="3"/>
<connect gate="G$1" pin="D3" pad="11"/>
<connect gate="G$1" pin="D4" pad="2"/>
<connect gate="G$1" pin="D5" pad="9"/>
<connect gate="G$1" pin="D6" pad="10"/>
<connect gate="G$1" pin="D7" pad="6"/>
<connect gate="G$1" pin="GND1" pad="7"/>
<connect gate="G$1" pin="GND2" pad="18"/>
<connect gate="G$1" pin="GND3" pad="21"/>
<connect gate="G$1" pin="OSCI" pad="27"/>
<connect gate="G$1" pin="OSCO" pad="28"/>
<connect gate="G$1" pin="PWREN#" pad="12"/>
<connect gate="G$1" pin="RD#" pad="13"/>
<connect gate="G$1" pin="RESET#" pad="19"/>
<connect gate="G$1" pin="RXF#" pad="23"/>
<connect gate="G$1" pin="TEST" pad="26"/>
<connect gate="G$1" pin="TXE#" pad="22"/>
<connect gate="G$1" pin="USBDM" pad="16"/>
<connect gate="G$1" pin="USBDP" pad="15"/>
<connect gate="G$1" pin="VCC" pad="20"/>
<connect gate="G$1" pin="VCCIO" pad="4"/>
<connect gate="G$1" pin="WR" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FT245RQ" prefix="U" uservalue="yes">
<description>&lt;b&gt;USB FIFO Controller&lt;/b&gt;
&lt;p&gt;
4&lt;sup&gt;th&lt;/sup&gt; Generation USB Controller (USB &amp;lt;-&amp;gt; Parallel) - FIFO &lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="FT245R"/>
</gates>
<devices>
<device name="" package="LQFP32">
<connects>
<connect gate="G$1" pin="3V3OUT" pad="16"/>
<connect gate="G$1" pin="AGND" pad="24"/>
<connect gate="G$1" pin="D0" pad="30"/>
<connect gate="G$1" pin="D1" pad="2"/>
<connect gate="G$1" pin="D2" pad="32"/>
<connect gate="G$1" pin="D3" pad="8"/>
<connect gate="G$1" pin="D4" pad="31"/>
<connect gate="G$1" pin="D5" pad="6"/>
<connect gate="G$1" pin="D6" pad="7"/>
<connect gate="G$1" pin="D7" pad="3"/>
<connect gate="G$1" pin="GND1" pad="4"/>
<connect gate="G$1" pin="GND2" pad="17"/>
<connect gate="G$1" pin="GND3" pad="20"/>
<connect gate="G$1" pin="OSCI" pad="27"/>
<connect gate="G$1" pin="OSCO" pad="28"/>
<connect gate="G$1" pin="PWREN#" pad="9"/>
<connect gate="G$1" pin="RD#" pad="10"/>
<connect gate="G$1" pin="RESET#" pad="18"/>
<connect gate="G$1" pin="RXF#" pad="22"/>
<connect gate="G$1" pin="TEST" pad="26"/>
<connect gate="G$1" pin="TXE#" pad="21"/>
<connect gate="G$1" pin="USBDM" pad="15"/>
<connect gate="G$1" pin="USBDP" pad="14"/>
<connect gate="G$1" pin="VCC" pad="19"/>
<connect gate="G$1" pin="VCCIO" pad="1"/>
<connect gate="G$1" pin="WR" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FT4232H" prefix="IC">
<description>&lt;b&gt;Quad USB UART&lt;/b&gt;&lt;br&gt;
5&lt;sup&gt;th&lt;/sup&gt; generation USB to 4-port serial controller</description>
<gates>
<gate name="CORE" symbol="4232CORE"/>
<gate name="A" symbol="4232PORT"/>
<gate name="B" symbol="4232PORT"/>
<gate name="C" symbol="4232PORT"/>
<gate name="D" symbol="4232PORT"/>
</gates>
<devices>
<device name="L" package="LQFP64">
<connects>
<connect gate="A" pin="DB0/TXD" pad="16"/>
<connect gate="A" pin="DB1/RXD" pad="17"/>
<connect gate="A" pin="DB2/RTS" pad="18"/>
<connect gate="A" pin="DB3/CTS" pad="19"/>
<connect gate="A" pin="DB4/DTR" pad="21"/>
<connect gate="A" pin="DB5/DSR" pad="22"/>
<connect gate="A" pin="DB6/DCD" pad="23"/>
<connect gate="A" pin="DB7/RI" pad="24"/>
<connect gate="B" pin="DB0/TXD" pad="26"/>
<connect gate="B" pin="DB1/RXD" pad="27"/>
<connect gate="B" pin="DB2/RTS" pad="28"/>
<connect gate="B" pin="DB3/CTS" pad="29"/>
<connect gate="B" pin="DB4/DTR" pad="30"/>
<connect gate="B" pin="DB5/DSR" pad="32"/>
<connect gate="B" pin="DB6/DCD" pad="33"/>
<connect gate="B" pin="DB7/RI" pad="34"/>
<connect gate="C" pin="DB0/TXD" pad="38"/>
<connect gate="C" pin="DB1/RXD" pad="39"/>
<connect gate="C" pin="DB2/RTS" pad="40"/>
<connect gate="C" pin="DB3/CTS" pad="41"/>
<connect gate="C" pin="DB4/DTR" pad="43"/>
<connect gate="C" pin="DB5/DSR" pad="44"/>
<connect gate="C" pin="DB6/DCD" pad="45"/>
<connect gate="C" pin="DB7/RI" pad="46"/>
<connect gate="CORE" pin="AGND" pad="10"/>
<connect gate="CORE" pin="EECLK" pad="62"/>
<connect gate="CORE" pin="EECS" pad="63"/>
<connect gate="CORE" pin="EEDATA" pad="61"/>
<connect gate="CORE" pin="GND@1" pad="1"/>
<connect gate="CORE" pin="GND@2" pad="5"/>
<connect gate="CORE" pin="GND@3" pad="11"/>
<connect gate="CORE" pin="GND@4" pad="15"/>
<connect gate="CORE" pin="GND@5" pad="25"/>
<connect gate="CORE" pin="GND@6" pad="35"/>
<connect gate="CORE" pin="GND@7" pad="47"/>
<connect gate="CORE" pin="GND@8" pad="51"/>
<connect gate="CORE" pin="PWREN#" pad="60"/>
<connect gate="CORE" pin="REF" pad="6"/>
<connect gate="CORE" pin="RESET#" pad="14"/>
<connect gate="CORE" pin="SUSPEND#" pad="36"/>
<connect gate="CORE" pin="TEST" pad="13"/>
<connect gate="CORE" pin="USBDM" pad="7"/>
<connect gate="CORE" pin="USBDP" pad="8"/>
<connect gate="CORE" pin="VCCIO@1" pad="20"/>
<connect gate="CORE" pin="VCCIO@2" pad="31"/>
<connect gate="CORE" pin="VCCIO@3" pad="42"/>
<connect gate="CORE" pin="VCCIO@4" pad="56"/>
<connect gate="CORE" pin="VCORE@1" pad="12"/>
<connect gate="CORE" pin="VCORE@2" pad="37"/>
<connect gate="CORE" pin="VCORE@3" pad="64"/>
<connect gate="CORE" pin="VPHY" pad="4"/>
<connect gate="CORE" pin="VPLL" pad="9"/>
<connect gate="CORE" pin="VREGIN" pad="50"/>
<connect gate="CORE" pin="VREGOUT" pad="49"/>
<connect gate="CORE" pin="XTIN" pad="2"/>
<connect gate="CORE" pin="XTOUT" pad="3"/>
<connect gate="D" pin="DB0/TXD" pad="48"/>
<connect gate="D" pin="DB1/RXD" pad="52"/>
<connect gate="D" pin="DB2/RTS" pad="53"/>
<connect gate="D" pin="DB3/CTS" pad="54"/>
<connect gate="D" pin="DB4/DTR" pad="55"/>
<connect gate="D" pin="DB5/DSR" pad="57"/>
<connect gate="D" pin="DB6/DCD" pad="58"/>
<connect gate="D" pin="DB7/RI" pad="59"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="VNC1L" prefix="IC">
<description>Dual USB Host Controller Vinculum</description>
<gates>
<gate name="G$1" symbol="VNC1L"/>
</gates>
<devices>
<device name="-1A" package="LQFP48">
<connects>
<connect gate="G$1" pin="ACBUS0" pad="41"/>
<connect gate="G$1" pin="ACBUS1" pad="42"/>
<connect gate="G$1" pin="ACBUS2" pad="43"/>
<connect gate="G$1" pin="ACBUS3" pad="44"/>
<connect gate="G$1" pin="ACBUS4" pad="45"/>
<connect gate="G$1" pin="ACBUS5" pad="46"/>
<connect gate="G$1" pin="ACBUS6" pad="47"/>
<connect gate="G$1" pin="ACBUS7" pad="48"/>
<connect gate="G$1" pin="ADBUS0" pad="31"/>
<connect gate="G$1" pin="ADBUS1" pad="32"/>
<connect gate="G$1" pin="ADBUS2" pad="33"/>
<connect gate="G$1" pin="ADBUS3" pad="34"/>
<connect gate="G$1" pin="ADBUS4" pad="35"/>
<connect gate="G$1" pin="ADBUS5" pad="36"/>
<connect gate="G$1" pin="ADBUS6" pad="37"/>
<connect gate="G$1" pin="ADBUS7" pad="38"/>
<connect gate="G$1" pin="AGND" pad="6"/>
<connect gate="G$1" pin="AVCC" pad="3"/>
<connect gate="G$1" pin="BCBUS0" pad="20"/>
<connect gate="G$1" pin="BCBUS1" pad="21"/>
<connect gate="G$1" pin="BCBUS2" pad="22"/>
<connect gate="G$1" pin="BCBUS3" pad="23"/>
<connect gate="G$1" pin="BDBUS0" pad="11"/>
<connect gate="G$1" pin="BDBUS1" pad="12"/>
<connect gate="G$1" pin="BDBUS2" pad="13"/>
<connect gate="G$1" pin="BDBUS3" pad="14"/>
<connect gate="G$1" pin="BDBUS4" pad="15"/>
<connect gate="G$1" pin="BDBUS5" pad="16"/>
<connect gate="G$1" pin="BDBUS6" pad="18"/>
<connect gate="G$1" pin="BDBUS7" pad="19"/>
<connect gate="G$1" pin="GND@1" pad="1"/>
<connect gate="G$1" pin="GND@2" pad="24"/>
<connect gate="G$1" pin="GND@3" pad="27"/>
<connect gate="G$1" pin="GND@4" pad="39"/>
<connect gate="G$1" pin="PLLFLTR" pad="7"/>
<connect gate="G$1" pin="PROG#" pad="10"/>
<connect gate="G$1" pin="RESET#" pad="9"/>
<connect gate="G$1" pin="TEST" pad="8"/>
<connect gate="G$1" pin="USB1DM" pad="26"/>
<connect gate="G$1" pin="USB1DP" pad="25"/>
<connect gate="G$1" pin="USB2DM" pad="29"/>
<connect gate="G$1" pin="USB2DP" pad="28"/>
<connect gate="G$1" pin="VCC" pad="2"/>
<connect gate="G$1" pin="VCCIO@1" pad="40"/>
<connect gate="G$1" pin="VCCIO@2" pad="30"/>
<connect gate="G$1" pin="VCCIO@3" pad="17"/>
<connect gate="G$1" pin="XTIN" pad="4"/>
<connect gate="G$1" pin="XTOUT" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="VNC2-32" prefix="IC">
<description>&lt;b&gt;Vinculum-II&lt;/b&gt;
&lt;p&gt;
2&lt;sup&gt;nd&lt;/sup&gt; Generation Dual USB Host Controller
&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="VNC2-32"/>
</gates>
<devices>
<device name="L1B" package="LQFP32">
<connects>
<connect gate="G$1" pin="GND@1" pad="1"/>
<connect gate="G$1" pin="GND@2" pad="16"/>
<connect gate="G$1" pin="GND@3" pad="19"/>
<connect gate="G$1" pin="GND@4" pad="27"/>
<connect gate="G$1" pin="GNDPLL" pad="6"/>
<connect gate="G$1" pin="IOBUS0" pad="11"/>
<connect gate="G$1" pin="IOBUS1" pad="12"/>
<connect gate="G$1" pin="IOBUS10" pad="31"/>
<connect gate="G$1" pin="IOBUS11" pad="32"/>
<connect gate="G$1" pin="IOBUS2" pad="14"/>
<connect gate="G$1" pin="IOBUS3" pad="15"/>
<connect gate="G$1" pin="IOBUS4" pad="23"/>
<connect gate="G$1" pin="IOBUS5" pad="24"/>
<connect gate="G$1" pin="IOBUS6" pad="25"/>
<connect gate="G$1" pin="IOBUS7" pad="26"/>
<connect gate="G$1" pin="IOBUS8" pad="29"/>
<connect gate="G$1" pin="IOBUS9" pad="30"/>
<connect gate="G$1" pin="PROG#" pad="9"/>
<connect gate="G$1" pin="RESET#" pad="10"/>
<connect gate="G$1" pin="TEST" pad="8"/>
<connect gate="G$1" pin="USB1DM" pad="18"/>
<connect gate="G$1" pin="USB1DP" pad="17"/>
<connect gate="G$1" pin="USB2DM" pad="21"/>
<connect gate="G$1" pin="USB2DP" pad="20"/>
<connect gate="G$1" pin="VCCIO@1" pad="28"/>
<connect gate="G$1" pin="VCCIO@2" pad="22"/>
<connect gate="G$1" pin="VCCIO@3" pad="13"/>
<connect gate="G$1" pin="VCCPLL_IN" pad="3"/>
<connect gate="G$1" pin="VREG_IN" pad="2"/>
<connect gate="G$1" pin="VREG_OUT" pad="7"/>
<connect gate="G$1" pin="XTIN" pad="4"/>
<connect gate="G$1" pin="XTOUT" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="VNC2-48" prefix="IC">
<description>&lt;b&gt;Vinculum-II&lt;/b&gt;
&lt;p&gt;
2&lt;sup&gt;nd&lt;/sup&gt; Generation Dual USB Host Controller
&lt;/p&gt;
&lt;p&gt;
48-pin device symbol is compatible&lt;sup&gt;*&lt;/sup&gt; with VNC1L symbol to allow easy replacement on schematic.
&lt;/p&gt;
&lt;p&gt;
&lt;sup&gt;*&lt;/sup&gt;please be noticed that VREG_OUT pin in VNC2 &lt;u&gt;has different&lt;/u&gt; functionality than PLLFLTR pin in VNC1L.
&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="VNC2-48"/>
</gates>
<devices>
<device name="L1B" package="LQFP48">
<connects>
<connect gate="G$1" pin="GND@1" pad="1"/>
<connect gate="G$1" pin="GND@2" pad="24"/>
<connect gate="G$1" pin="GND@3" pad="27"/>
<connect gate="G$1" pin="GND@4" pad="39"/>
<connect gate="G$1" pin="GNDPLL" pad="6"/>
<connect gate="G$1" pin="IOBUS0" pad="11"/>
<connect gate="G$1" pin="IOBUS1" pad="12"/>
<connect gate="G$1" pin="IOBUS10" pad="22"/>
<connect gate="G$1" pin="IOBUS11" pad="23"/>
<connect gate="G$1" pin="IOBUS12" pad="31"/>
<connect gate="G$1" pin="IOBUS13" pad="32"/>
<connect gate="G$1" pin="IOBUS14" pad="33"/>
<connect gate="G$1" pin="IOBUS15" pad="34"/>
<connect gate="G$1" pin="IOBUS16" pad="35"/>
<connect gate="G$1" pin="IOBUS17" pad="36"/>
<connect gate="G$1" pin="IOBUS18" pad="37"/>
<connect gate="G$1" pin="IOBUS19" pad="38"/>
<connect gate="G$1" pin="IOBUS2" pad="13"/>
<connect gate="G$1" pin="IOBUS20" pad="41"/>
<connect gate="G$1" pin="IOBUS21" pad="42"/>
<connect gate="G$1" pin="IOBUS22" pad="43"/>
<connect gate="G$1" pin="IOBUS23" pad="44"/>
<connect gate="G$1" pin="IOBUS24" pad="45"/>
<connect gate="G$1" pin="IOBUS25" pad="46"/>
<connect gate="G$1" pin="IOBUS26" pad="47"/>
<connect gate="G$1" pin="IOBUS27" pad="48"/>
<connect gate="G$1" pin="IOBUS3" pad="14"/>
<connect gate="G$1" pin="IOBUS4" pad="15"/>
<connect gate="G$1" pin="IOBUS5" pad="16"/>
<connect gate="G$1" pin="IOBUS6" pad="18"/>
<connect gate="G$1" pin="IOBUS7" pad="19"/>
<connect gate="G$1" pin="IOBUS8" pad="20"/>
<connect gate="G$1" pin="IOBUS9" pad="21"/>
<connect gate="G$1" pin="PROG#" pad="10"/>
<connect gate="G$1" pin="RESET#" pad="9"/>
<connect gate="G$1" pin="TEST" pad="8"/>
<connect gate="G$1" pin="USB1DM" pad="26"/>
<connect gate="G$1" pin="USB1DP" pad="25"/>
<connect gate="G$1" pin="USB2DM" pad="29"/>
<connect gate="G$1" pin="USB2DP" pad="28"/>
<connect gate="G$1" pin="VCCIO@1" pad="40"/>
<connect gate="G$1" pin="VCCIO@2" pad="30"/>
<connect gate="G$1" pin="VCCIO@3" pad="17"/>
<connect gate="G$1" pin="VCCPLL_IN" pad="3"/>
<connect gate="G$1" pin="VREG_IN" pad="2"/>
<connect gate="G$1" pin="VREG_OUT" pad="7"/>
<connect gate="G$1" pin="XTIN" pad="4"/>
<connect gate="G$1" pin="XTOUT" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="VNC2-64" prefix="IC">
<description>&lt;b&gt;Vinculum-II&lt;/b&gt;
&lt;p&gt;
2&lt;sup&gt;nd&lt;/sup&gt; Generation Dual USB Host Controller
&lt;/p&gt;</description>
<gates>
<gate name="CORE" symbol="VNC2-64CORE"/>
<gate name="A" symbol="VNC2-64PORT1"/>
<gate name="B" symbol="VNC2-64PORT2"/>
<gate name="C" symbol="VNC2-64PORT3"/>
<gate name="D" symbol="VNC2-64PORT4"/>
<gate name="E" symbol="VNC2-64PORT5"/>
<gate name="F" symbol="VNC2-64PORT6"/>
</gates>
<devices>
<device name="L1B" package="LQFP64">
<connects>
<connect gate="A" pin="IOBUS0" pad="11"/>
<connect gate="A" pin="IOBUS1" pad="12"/>
<connect gate="A" pin="IOBUS2" pad="13"/>
<connect gate="A" pin="IOBUS3" pad="14"/>
<connect gate="A" pin="IOBUS4" pad="15"/>
<connect gate="A" pin="IOBUS5" pad="16"/>
<connect gate="A" pin="IOBUS6" pad="17"/>
<connect gate="A" pin="IOBUS7" pad="18"/>
<connect gate="B" pin="IOBUS10" pad="22"/>
<connect gate="B" pin="IOBUS11" pad="23"/>
<connect gate="B" pin="IOBUS12" pad="24"/>
<connect gate="B" pin="IOBUS13" pad="25"/>
<connect gate="B" pin="IOBUS14" pad="26"/>
<connect gate="B" pin="IOBUS15" pad="27"/>
<connect gate="B" pin="IOBUS8" pad="19"/>
<connect gate="B" pin="IOBUS9" pad="20"/>
<connect gate="C" pin="IOBUS16" pad="28"/>
<connect gate="C" pin="IOBUS17" pad="29"/>
<connect gate="C" pin="IOBUS18" pad="31"/>
<connect gate="C" pin="IOBUS19" pad="32"/>
<connect gate="C" pin="IOBUS20" pad="39"/>
<connect gate="C" pin="IOBUS21" pad="40"/>
<connect gate="C" pin="IOBUS22" pad="41"/>
<connect gate="C" pin="IOBUS23" pad="42"/>
<connect gate="CORE" pin="GND@1" pad="1"/>
<connect gate="CORE" pin="GND@2" pad="30"/>
<connect gate="CORE" pin="GND@3" pad="35"/>
<connect gate="CORE" pin="GND@4" pad="53"/>
<connect gate="CORE" pin="GNDPLL" pad="6"/>
<connect gate="CORE" pin="PROG#" pad="10"/>
<connect gate="CORE" pin="RESET#" pad="9"/>
<connect gate="CORE" pin="TEST" pad="8"/>
<connect gate="CORE" pin="USB1DM" pad="34"/>
<connect gate="CORE" pin="USB1DP" pad="33"/>
<connect gate="CORE" pin="USB2DM" pad="37"/>
<connect gate="CORE" pin="USB2DP" pad="36"/>
<connect gate="CORE" pin="VCCIO@1" pad="54"/>
<connect gate="CORE" pin="VCCIO@2" pad="38"/>
<connect gate="CORE" pin="VCCIO@3" pad="21"/>
<connect gate="CORE" pin="VCCPLL_IN" pad="3"/>
<connect gate="CORE" pin="VREG_IN" pad="2"/>
<connect gate="CORE" pin="VREG_OUT" pad="7"/>
<connect gate="CORE" pin="XTIN" pad="4"/>
<connect gate="CORE" pin="XTOUT" pad="5"/>
<connect gate="D" pin="IOBUS24" pad="43"/>
<connect gate="D" pin="IOBUS25" pad="44"/>
<connect gate="D" pin="IOBUS26" pad="45"/>
<connect gate="D" pin="IOBUS27" pad="46"/>
<connect gate="D" pin="IOBUS28" pad="47"/>
<connect gate="D" pin="IOBUS29" pad="48"/>
<connect gate="D" pin="IOBUS30" pad="49"/>
<connect gate="D" pin="IOBUS31" pad="50"/>
<connect gate="E" pin="IOBUS32" pad="51"/>
<connect gate="E" pin="IOBUS33" pad="52"/>
<connect gate="E" pin="IOBUS34" pad="55"/>
<connect gate="E" pin="IOBUS35" pad="56"/>
<connect gate="E" pin="IOBUS36" pad="57"/>
<connect gate="E" pin="IOBUS37" pad="58"/>
<connect gate="E" pin="IOBUS38" pad="59"/>
<connect gate="E" pin="IOBUS39" pad="60"/>
<connect gate="F" pin="IOBUS40" pad="61"/>
<connect gate="F" pin="IOBUS41" pad="62"/>
<connect gate="F" pin="IOBUS42" pad="63"/>
<connect gate="F" pin="IOBUS43" pad="64"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FT232H" prefix="IC">
<description>&lt;b&gt;FTDI FT232H&lt;/b&gt;
&lt;p&gt;
High Speed USB 2.0 Slave Controller
&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="FT232H"/>
</gates>
<devices>
<device name="" package="LQFP48">
<connects>
<connect gate="G$1" pin="ACBUS0" pad="21"/>
<connect gate="G$1" pin="ACBUS1" pad="25"/>
<connect gate="G$1" pin="ACBUS2" pad="26"/>
<connect gate="G$1" pin="ACBUS3" pad="27"/>
<connect gate="G$1" pin="ACBUS4" pad="28"/>
<connect gate="G$1" pin="ACBUS5" pad="29"/>
<connect gate="G$1" pin="ACBUS6" pad="30"/>
<connect gate="G$1" pin="ACBUS7" pad="31"/>
<connect gate="G$1" pin="ACBUS8" pad="32"/>
<connect gate="G$1" pin="ACBUS9" pad="33"/>
<connect gate="G$1" pin="ADBUS0" pad="13"/>
<connect gate="G$1" pin="ADBUS1" pad="14"/>
<connect gate="G$1" pin="ADBUS2" pad="15"/>
<connect gate="G$1" pin="ADBUS3" pad="16"/>
<connect gate="G$1" pin="ADBUS4" pad="17"/>
<connect gate="G$1" pin="ADBUS5" pad="18"/>
<connect gate="G$1" pin="ADBUS6" pad="19"/>
<connect gate="G$1" pin="ADBUS7" pad="20"/>
<connect gate="G$1" pin="AGND1" pad="4"/>
<connect gate="G$1" pin="AGND2" pad="9"/>
<connect gate="G$1" pin="AGND3" pad="41"/>
<connect gate="G$1" pin="DM" pad="6"/>
<connect gate="G$1" pin="DP" pad="7"/>
<connect gate="G$1" pin="EECLK" pad="44"/>
<connect gate="G$1" pin="EECS" pad="45"/>
<connect gate="G$1" pin="EEDATA" pad="43"/>
<connect gate="G$1" pin="GND1" pad="10"/>
<connect gate="G$1" pin="GND2" pad="11"/>
<connect gate="G$1" pin="GND3" pad="22"/>
<connect gate="G$1" pin="GND4" pad="23"/>
<connect gate="G$1" pin="GND5" pad="35"/>
<connect gate="G$1" pin="GND6" pad="36"/>
<connect gate="G$1" pin="GND7" pad="47"/>
<connect gate="G$1" pin="GND8" pad="48"/>
<connect gate="G$1" pin="REF" pad="5"/>
<connect gate="G$1" pin="RESET#" pad="34"/>
<connect gate="G$1" pin="TEST" pad="42"/>
<connect gate="G$1" pin="VCCA" pad="37"/>
<connect gate="G$1" pin="VCCCORE" pad="38"/>
<connect gate="G$1" pin="VCCD" pad="39"/>
<connect gate="G$1" pin="VCCIO1" pad="12"/>
<connect gate="G$1" pin="VCCIO2" pad="24"/>
<connect gate="G$1" pin="VCCIO3" pad="46"/>
<connect gate="G$1" pin="VPHY" pad="3"/>
<connect gate="G$1" pin="VPLL" pad="8"/>
<connect gate="G$1" pin="VREGIN" pad="40"/>
<connect gate="G$1" pin="XCSI" pad="1"/>
<connect gate="G$1" pin="XCSO" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
