<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.3.2">
<drawing>
<library>
<packages>
<package name="DIL28-6">
</package>
<package name="DIL40-6">
</package>
</packages>
<symbols>
<symbol name="SP0256AL2">
<pin name="VSS" direction="pwr"/>
<pin name="!RESET" direction="in"/>
<pin name="ROMDIS"/>
<pin name="C1"/>
<pin name="C2"/>
<pin name="C3"/>
<pin name="VDD" direction="pwr"/>
<pin name="SBY" direction="out"/>
<pin name="!LRQ" direction="out"/>
<pin name="A8"/>
<pin name="A7" direction="in"/>
<pin name="SEROUT" direction="out"/>
<pin name="A6" direction="in"/>
<pin name="A5" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="SE"/>
<pin name="!ALD" direction="in"/>
<pin name="SERIN" direction="in"/>
<pin name="TEST"/>
<pin name="VD1" direction="pwr"/>
<pin name="DIGITALOUT" direction="out"/>
<pin name="!SBYRESET" direction="in"/>
<pin name="ROMCLK" direction="out"/>
<pin name="OSC1"/>
<pin name="OSC2"/>
</symbol>
<symbol name="CTS256AL2">
<pin name="B5/R/W"/>
<pin name="B7/CLOCKOUT"/>
<pin name="BO"/>
<pin name="B1"/>
<pin name="B2"/>
<pin name="A0"/>
<pin name="A1"/>
<pin name="A2"/>
<pin name="A3"/>
<pin name="A4"/>
<pin name="A7"/>
<pin name="INT3"/>
<pin name="INT1"/>
<pin name="RESET"/>
<pin name="A6/SCLK"/>
<pin name="A5/RXD"/>
<pin name="XTAL2/CLOCKIN"/>
<pin name="XTAL1"/>
<pin name="D7"/>
<pin name="D6"/>
<pin name="D5"/>
<pin name="D4"/>
<pin name="D3"/>
<pin name="D2"/>
<pin name="VCC"/>
<pin name="D1"/>
<pin name="DO"/>
<pin name="C0"/>
<pin name="C1"/>
<pin name="C2"/>
<pin name="C3"/>
<pin name="C4"/>
<pin name="C5"/>
<pin name="C6"/>
<pin name="C7"/>
<pin name="MC"/>
<pin name="B3/TXD"/>
<pin name="B4/ALATCH"/>
<pin name="B6/ENABLE"/>
<pin name="VSS"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="SP0256-AL2" prefix="U">
<description>General Instruments SP0256-AL2 vintage speech synthesizer IC</description>
<gates>
<gate name="G$1" symbol="SP0256AL2"/>
</gates>
<devices>
<device name="" package="DIL28-6">
<connects>
<connect gate="G$1" pin="!ALD" pad="P$20"/>
<connect gate="G$1" pin="!LRQ" pad="P$9"/>
<connect gate="G$1" pin="!RESET" pad="P$2"/>
<connect gate="G$1" pin="!SBYRESET" pad="P$25"/>
<connect gate="G$1" pin="A1" pad="P$18"/>
<connect gate="G$1" pin="A2" pad="P$17"/>
<connect gate="G$1" pin="A3" pad="P$16"/>
<connect gate="G$1" pin="A4" pad="P$15"/>
<connect gate="G$1" pin="A5" pad="P$14"/>
<connect gate="G$1" pin="A6" pad="P$13"/>
<connect gate="G$1" pin="A7" pad="P$11"/>
<connect gate="G$1" pin="A8" pad="P$10"/>
<connect gate="G$1" pin="C1" pad="P$4"/>
<connect gate="G$1" pin="C2" pad="P$5"/>
<connect gate="G$1" pin="C3" pad="P$6"/>
<connect gate="G$1" pin="DIGITALOUT" pad="P$24"/>
<connect gate="G$1" pin="OSC1" pad="P$27"/>
<connect gate="G$1" pin="OSC2" pad="P$28"/>
<connect gate="G$1" pin="ROMCLK" pad="P$26"/>
<connect gate="G$1" pin="ROMDIS" pad="P$3"/>
<connect gate="G$1" pin="SBY" pad="P$8"/>
<connect gate="G$1" pin="SE" pad="P$19"/>
<connect gate="G$1" pin="SERIN" pad="P$21"/>
<connect gate="G$1" pin="SEROUT" pad="P$12"/>
<connect gate="G$1" pin="TEST" pad="P$22"/>
<connect gate="G$1" pin="VD1" pad="P$23"/>
<connect gate="G$1" pin="VDD" pad="P$7"/>
<connect gate="G$1" pin="VSS" pad="P$1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CTS256A-AL2" prefix="U">
<gates>
<gate name="G$1" symbol="CTS256AL2"/>
</gates>
<devices>
<device name="" package="DIL40-6">
<connects>
<connect gate="G$1" pin="A0" pad="P$6"/>
<connect gate="G$1" pin="A1" pad="P$7"/>
<connect gate="G$1" pin="A2" pad="P$8"/>
<connect gate="G$1" pin="A3" pad="P$9"/>
<connect gate="G$1" pin="A4" pad="P$10"/>
<connect gate="G$1" pin="A5/RXD" pad="P$16"/>
<connect gate="G$1" pin="A6/SCLK" pad="P$15"/>
<connect gate="G$1" pin="A7" pad="P$11"/>
<connect gate="G$1" pin="B1" pad="P$4"/>
<connect gate="G$1" pin="B2" pad="P$5"/>
<connect gate="G$1" pin="B3/TXD" pad="P$37"/>
<connect gate="G$1" pin="B4/ALATCH" pad="P$38"/>
<connect gate="G$1" pin="B5/R/W" pad="P$1"/>
<connect gate="G$1" pin="B6/ENABLE" pad="P$39"/>
<connect gate="G$1" pin="B7/CLOCKOUT" pad="P$2"/>
<connect gate="G$1" pin="BO" pad="P$3"/>
<connect gate="G$1" pin="C0" pad="P$28"/>
<connect gate="G$1" pin="C1" pad="P$29"/>
<connect gate="G$1" pin="C2" pad="P$30"/>
<connect gate="G$1" pin="C3" pad="P$31"/>
<connect gate="G$1" pin="C4" pad="P$32"/>
<connect gate="G$1" pin="C5" pad="P$33"/>
<connect gate="G$1" pin="C6" pad="P$34"/>
<connect gate="G$1" pin="C7" pad="P$35"/>
<connect gate="G$1" pin="D1" pad="P$26"/>
<connect gate="G$1" pin="D2" pad="P$24"/>
<connect gate="G$1" pin="D3" pad="P$23"/>
<connect gate="G$1" pin="D4" pad="P$22"/>
<connect gate="G$1" pin="D5" pad="P$21"/>
<connect gate="G$1" pin="D6" pad="P$20"/>
<connect gate="G$1" pin="D7" pad="P$19"/>
<connect gate="G$1" pin="DO" pad="P$27"/>
<connect gate="G$1" pin="INT1" pad="P$13"/>
<connect gate="G$1" pin="INT3" pad="P$12"/>
<connect gate="G$1" pin="MC" pad="P$36"/>
<connect gate="G$1" pin="RESET" pad="P$14"/>
<connect gate="G$1" pin="VCC" pad="P$25"/>
<connect gate="G$1" pin="VSS" pad="P$40"/>
<connect gate="G$1" pin="XTAL1" pad="P$18"/>
<connect gate="G$1" pin="XTAL2/CLOCKIN" pad="P$17"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
