<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.0.1">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="152.324" y2="0" width="0" layer="20"/>
<wire x1="152.324" y1="0" x2="152.324" y2="101.59" width="0" layer="20"/>
<wire x1="152.324" y1="101.59" x2="0" y2="101.59" width="0" layer="20"/>
<wire x1="0" y1="101.59" x2="0" y2="0" width="0" layer="20"/>
<text>5VDC TIP+</text>
<text>WILLIAM HARRINGTON
ORATOR REV 1</text>
<text>FEMALE - DCE</text>
<text>OPTS</text>
<text>UART</text>
<text>RESET</text>
<text>VOLUME</text>
<text>AUDIO_OUT</text>
<text>LM386</text>
<text>MAX202CPE</text>
<text>74HCT138N</text>
<text>74HCT373N</text>
<text>74HCT373N</text>
<text>SPEECH ROM</text>
<text>74HCT14N</text>
<text>USR/EXCP ROM</text>
<text>ROM_CS</text>
<text>PIN    6 7 8  MODE

         0 0 0  PARALLEL INPUT
         0 0 1  SERIAL     50 BAUD
         0 1 0  SERIAL   110 BAUD
         0 1 1  SERIAL   300 BAUD
         1 0 0  SERIAL 1200 BAUD
         1 0 1  SERIAL 2400 BAUD
         1 1 0  SERIAL 4800 BAUD
         1 1 1  SERIAL 9600 BAUD

PIN    9 

         0  7 BITS, 2 STOP BITS, NO PARITY*
         1  SELECTABLE **

PIN   10  RAM BUFFER

          0  INTERNAL (20 BYTE IN / 26 BYTE OUT)
          1  EXTERNAL (1972 BYTE IN / 256 BYTE OUT)

PIN   11  DELIMETER

          0  CARRIAGE RETURN ONLY
          1  ANY

PIN     3  INPUT BUFFER (OUTPUT ONLY)

          0  BUSY
          1  NOT BUSY

* DEFAULT</text>
<text>PIN   3 4

        0 1  6 BITS/CHAR
        1 0  7 BITS/CHAR
        1 1  8 BITS/CHAR

PIN    8    PARITY

         0  ENABLED
         1  DISABLED

PIN    7  PARITY

         0  ODD
         1  EVEN

PIN    3  STOP BITS

         0  ONE
         1  TWO</text>
<text>OPTS MODE SELECTION</text>
<text>UART CONFIGURATION **</text>
<polygon width="0.002540625" layer="46">
<vertex x="4.2291" y="90.3986"/>
<vertex x="5.0165" y="90.3986"/>
<vertex x="5.0165" y="87.4014"/>
<vertex x="4.2164" y="87.4014"/>
<vertex x="4.2164" y="90.3986"/>
</polygon>
<polygon width="0.002540625" layer="46">
<vertex x="6.1214" y="83.7057"/>
<vertex x="6.1214" y="84.4931"/>
<vertex x="9.1186" y="84.4931"/>
<vertex x="9.1186" y="83.693"/>
<vertex x="6.1214" y="83.693"/>
</polygon>
<polygon width="0.002540625" layer="46">
<vertex x="10.1219" y="90.6526"/>
<vertex x="11.1252" y="90.6526"/>
<vertex x="11.1252" y="87.1474"/>
<vertex x="10.1219" y="87.1474"/>
</polygon>
<polygon width="0.002540625" layer="46">
<vertex x="142.7988" y="69.088"/>
<vertex x="144.907" y="69.088"/>
<vertex x="144.907" y="67.4878"/>
<vertex x="142.7988" y="67.4878"/>
</polygon>
<polygon width="0.002540625" layer="46">
<vertex x="142.7988" y="77.2922"/>
<vertex x="144.907" y="77.2922"/>
<vertex x="144.907" y="75.692"/>
<vertex x="142.7988" y="75.692"/>
</polygon>
</plain>
<libraries>
<library name="rcl">
<description>&lt;b&gt;Resistors, Capacitors, Inductors&lt;/b&gt;&lt;p&gt;
Based on the previous libraries:
&lt;ul&gt;
&lt;li&gt;r.lbr
&lt;li&gt;cap.lbr 
&lt;li&gt;cap-fe.lbr
&lt;li&gt;captant.lbr
&lt;li&gt;polcap.lbr
&lt;li&gt;ipc-smd.lbr
&lt;/ul&gt;
All SMD packages are defined according to the IPC specifications and  CECC&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;p&gt;
&lt;p&gt;
for Electrolyt Capacitors see also :&lt;p&gt;
www.bccomponents.com &lt;p&gt;
www.panasonic.com&lt;p&gt;
www.kemet.com&lt;p&gt;
http://www.secc.co.jp/pdf/os_e/2004/e_os_all.pdf &lt;b&gt;(SANYO)&lt;/b&gt;
&lt;p&gt;
for trimmer refence see : &lt;u&gt;www.electrospec-inc.com/cross_references/trimpotcrossref.asp&lt;/u&gt;&lt;p&gt;

&lt;table border=0 cellspacing=0 cellpadding=0 width="100%" cellpaddding=0&gt;
&lt;tr valign="top"&gt;

&lt;! &lt;td width="10"&gt;&amp;nbsp;&lt;/td&gt;
&lt;td width="90%"&gt;

&lt;b&gt;&lt;font color="#0000FF" size="4"&gt;TRIM-POT CROSS REFERENCE&lt;/font&gt;&lt;/b&gt;
&lt;P&gt;
&lt;TABLE BORDER=0 CELLSPACING=1 CELLPADDING=2&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;RECTANGULAR MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;BOURNS&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;BI&amp;nbsp;TECH&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;DALE-VISHAY&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;PHILIPS/MEPCO&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;MURATA&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;PANASONIC&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;SPECTROL&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;MILSPEC&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;&lt;TD&gt;&amp;nbsp;&lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3 &gt;
      3005P&lt;BR&gt;
      3006P&lt;BR&gt;
      3006W&lt;BR&gt;
      3006Y&lt;BR&gt;
      3009P&lt;BR&gt;
      3009W&lt;BR&gt;
      3009Y&lt;BR&gt;
      3057J&lt;BR&gt;
      3057L&lt;BR&gt;
      3057P&lt;BR&gt;
      3057Y&lt;BR&gt;
      3059J&lt;BR&gt;
      3059L&lt;BR&gt;
      3059P&lt;BR&gt;
      3059Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      89P&lt;BR&gt;
      89W&lt;BR&gt;
      89X&lt;BR&gt;
      89PH&lt;BR&gt;
      76P&lt;BR&gt;
      89XH&lt;BR&gt;
      78SLT&lt;BR&gt;
      78L&amp;nbsp;ALT&lt;BR&gt;
      56P&amp;nbsp;ALT&lt;BR&gt;
      78P&amp;nbsp;ALT&lt;BR&gt;
      T8S&lt;BR&gt;
      78L&lt;BR&gt;
      56P&lt;BR&gt;
      78P&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      T18/784&lt;BR&gt;
      783&lt;BR&gt;
      781&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      2199&lt;BR&gt;
      1697/1897&lt;BR&gt;
      1680/1880&lt;BR&gt;
      2187&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      8035EKP/CT20/RJ-20P&lt;BR&gt;
      -&lt;BR&gt;
      RJ-20X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      1211L&lt;BR&gt;
      8012EKQ&amp;nbsp;ALT&lt;BR&gt;
      8012EKR&amp;nbsp;ALT&lt;BR&gt;
      1211P&lt;BR&gt;
      8012EKJ&lt;BR&gt;
      8012EKL&lt;BR&gt;
      8012EKQ&lt;BR&gt;
      8012EKR&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      2101P&lt;BR&gt;
      2101W&lt;BR&gt;
      2101Y&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      2102L&lt;BR&gt;
      2102S&lt;BR&gt;
      2102Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      EVMCOG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      43P&lt;BR&gt;
      43W&lt;BR&gt;
      43Y&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      40L&lt;BR&gt;
      40P&lt;BR&gt;
      40Y&lt;BR&gt;
      70Y-T602&lt;BR&gt;
      70L&lt;BR&gt;
      70P&lt;BR&gt;
      70Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      -&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SQUARE MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
   &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MURATA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;SPECTROL&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MILSPEC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3250L&lt;BR&gt;
      3250P&lt;BR&gt;
      3250W&lt;BR&gt;
      3250X&lt;BR&gt;
      3252P&lt;BR&gt;
      3252W&lt;BR&gt;
      3252X&lt;BR&gt;
      3260P&lt;BR&gt;
      3260W&lt;BR&gt;
      3260X&lt;BR&gt;
      3262P&lt;BR&gt;
      3262W&lt;BR&gt;
      3262X&lt;BR&gt;
      3266P&lt;BR&gt;
      3266W&lt;BR&gt;
      3266X&lt;BR&gt;
      3290H&lt;BR&gt;
      3290P&lt;BR&gt;
      3290W&lt;BR&gt;
      3292P&lt;BR&gt;
      3292W&lt;BR&gt;
      3292X&lt;BR&gt;
      3296P&lt;BR&gt;
      3296W&lt;BR&gt;
      3296X&lt;BR&gt;
      3296Y&lt;BR&gt;
      3296Z&lt;BR&gt;
      3299P&lt;BR&gt;
      3299W&lt;BR&gt;
      3299X&lt;BR&gt;
      3299Y&lt;BR&gt;
      3299Z&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      -&lt;BR&gt;
      64W&amp;nbsp;ALT&lt;BR&gt;
      -&lt;BR&gt;
      64P&amp;nbsp;ALT&lt;BR&gt;
      64W&amp;nbsp;ALT&lt;BR&gt;
      64X&amp;nbsp;ALT&lt;BR&gt;
      64P&lt;BR&gt;
      64W&lt;BR&gt;
      64X&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66P&lt;BR&gt;
      66W&lt;BR&gt;
      66X&lt;BR&gt;
      67P&lt;BR&gt;
      67W&lt;BR&gt;
      67X&lt;BR&gt;
      67Y&lt;BR&gt;
      67Z&lt;BR&gt;
      68P&lt;BR&gt;
      68W&lt;BR&gt;
      68X&lt;BR&gt;
      67Y&amp;nbsp;ALT&lt;BR&gt;
      67Z&amp;nbsp;ALT&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      5050&lt;BR&gt;
      5091&lt;BR&gt;
      5080&lt;BR&gt;
      5087&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T63YB&lt;BR&gt;
      T63XB&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      5887&lt;BR&gt;
      5891&lt;BR&gt;
      5880&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T93Z&lt;BR&gt;
      T93YA&lt;BR&gt;
      T93XA&lt;BR&gt;
      T93YB&lt;BR&gt;
      T93XB&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8026EKP&lt;BR&gt;
      8026EKW&lt;BR&gt;
      8026EKM&lt;BR&gt;
      8026EKP&lt;BR&gt;
      8026EKB&lt;BR&gt;
      8026EKM&lt;BR&gt;
      1309X&lt;BR&gt;
      1309P&lt;BR&gt;
      1309W&lt;BR&gt;
      8024EKP&lt;BR&gt;
      8024EKW&lt;BR&gt;
      8024EKN&lt;BR&gt;
      RJ-9P/CT9P&lt;BR&gt;
      RJ-9W&lt;BR&gt;
      RJ-9X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3103P&lt;BR&gt;
      3103Y&lt;BR&gt;
      3103Z&lt;BR&gt;
      3103P&lt;BR&gt;
      3103Y&lt;BR&gt;
      3103Z&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3105P/3106P&lt;BR&gt;
      3105W/3106W&lt;BR&gt;
      3105X/3106X&lt;BR&gt;
      3105Y/3106Y&lt;BR&gt;
      3105Z/3105Z&lt;BR&gt;
      3102P&lt;BR&gt;
      3102W&lt;BR&gt;
      3102X&lt;BR&gt;
      3102Y&lt;BR&gt;
      3102Z&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMCBG&lt;BR&gt;
      EVMCCG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      55-1-X&lt;BR&gt;
      55-4-X&lt;BR&gt;
      55-3-X&lt;BR&gt;
      55-2-X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      50-2-X&lt;BR&gt;
      50-4-X&lt;BR&gt;
      50-3-X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      64P&lt;BR&gt;
      64W&lt;BR&gt;
      64X&lt;BR&gt;
      64Y&lt;BR&gt;
      64Z&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SINGLE TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MURATA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;SPECTROL&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MILSPEC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3323P&lt;BR&gt;
      3323S&lt;BR&gt;
      3323W&lt;BR&gt;
      3329H&lt;BR&gt;
      3329P&lt;BR&gt;
      3329W&lt;BR&gt;
      3339H&lt;BR&gt;
      3339P&lt;BR&gt;
      3339W&lt;BR&gt;
      3352E&lt;BR&gt;
      3352H&lt;BR&gt;
      3352K&lt;BR&gt;
      3352P&lt;BR&gt;
      3352T&lt;BR&gt;
      3352V&lt;BR&gt;
      3352W&lt;BR&gt;
      3362H&lt;BR&gt;
      3362M&lt;BR&gt;
      3362P&lt;BR&gt;
      3362R&lt;BR&gt;
      3362S&lt;BR&gt;
      3362U&lt;BR&gt;
      3362W&lt;BR&gt;
      3362X&lt;BR&gt;
      3386B&lt;BR&gt;
      3386C&lt;BR&gt;
      3386F&lt;BR&gt;
      3386H&lt;BR&gt;
      3386K&lt;BR&gt;
      3386M&lt;BR&gt;
      3386P&lt;BR&gt;
      3386S&lt;BR&gt;
      3386W&lt;BR&gt;
      3386X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      25P&lt;BR&gt;
      25S&lt;BR&gt;
      25RX&lt;BR&gt;
      82P&lt;BR&gt;
      82M&lt;BR&gt;
      82PA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      91E&lt;BR&gt;
      91X&lt;BR&gt;
      91T&lt;BR&gt;
      91B&lt;BR&gt;
      91A&lt;BR&gt;
      91V&lt;BR&gt;
      91W&lt;BR&gt;
      25W&lt;BR&gt;
      25V&lt;BR&gt;
      25P&lt;BR&gt;
      -&lt;BR&gt;
      25S&lt;BR&gt;
      25U&lt;BR&gt;
      25RX&lt;BR&gt;
      25X&lt;BR&gt;
      72XW&lt;BR&gt;
      72XL&lt;BR&gt;
      72PM&lt;BR&gt;
      72RX&lt;BR&gt;
      -&lt;BR&gt;
      72PX&lt;BR&gt;
      72P&lt;BR&gt;
      72RXW&lt;BR&gt;
      72RXL&lt;BR&gt;
      72X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T7YB&lt;BR&gt;
      T7YA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      TXD&lt;BR&gt;
      TYA&lt;BR&gt;
      TYP&lt;BR&gt;
      -&lt;BR&gt;
      TYD&lt;BR&gt;
      TX&lt;BR&gt;
      -&lt;BR&gt;
      150SX&lt;BR&gt;
      100SX&lt;BR&gt;
      102T&lt;BR&gt;
      101S&lt;BR&gt;
      190T&lt;BR&gt;
      150TX&lt;BR&gt;
      101&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      101SX&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ET6P&lt;BR&gt;
      ET6S&lt;BR&gt;
      ET6X&lt;BR&gt;
      RJ-6W/8014EMW&lt;BR&gt;
      RJ-6P/8014EMP&lt;BR&gt;
      RJ-6X/8014EMX&lt;BR&gt;
      TM7W&lt;BR&gt;
      TM7P&lt;BR&gt;
      TM7X&lt;BR&gt;
      -&lt;BR&gt;
      8017SMS&lt;BR&gt;
      -&lt;BR&gt;
      8017SMB&lt;BR&gt;
      8017SMA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      CT-6W&lt;BR&gt;
      CT-6H&lt;BR&gt;
      CT-6P&lt;BR&gt;
      CT-6R&lt;BR&gt;
      -&lt;BR&gt;
      CT-6V&lt;BR&gt;
      CT-6X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8038EKV&lt;BR&gt;
      -&lt;BR&gt;
      8038EKX&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8038EKP&lt;BR&gt;
      8038EKZ&lt;BR&gt;
      8038EKW&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3321H&lt;BR&gt;
      3321P&lt;BR&gt;
      3321N&lt;BR&gt;
      1102H&lt;BR&gt;
      1102P&lt;BR&gt;
      1102T&lt;BR&gt;
      RVA0911V304A&lt;BR&gt;
      -&lt;BR&gt;
      RVA0911H413A&lt;BR&gt;
      RVG0707V100A&lt;BR&gt;
      RVA0607V(H)306A&lt;BR&gt;
      RVA1214H213A&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3104B&lt;BR&gt;
      3104C&lt;BR&gt;
      3104F&lt;BR&gt;
      3104H&lt;BR&gt;
      -&lt;BR&gt;
      3104M&lt;BR&gt;
      3104P&lt;BR&gt;
      3104S&lt;BR&gt;
      3104W&lt;BR&gt;
      3104X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      EVMQ0G&lt;BR&gt;
      EVMQIG&lt;BR&gt;
      EVMQ3G&lt;BR&gt;
      EVMS0G&lt;BR&gt;
      EVMQ0G&lt;BR&gt;
      EVMG0G&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMK4GA00B&lt;BR&gt;
      EVM30GA00B&lt;BR&gt;
      EVMK0GA00B&lt;BR&gt;
      EVM38GA00B&lt;BR&gt;
      EVMB6&lt;BR&gt;
      EVLQ0&lt;BR&gt;
      -&lt;BR&gt;
      EVMMSG&lt;BR&gt;
      EVMMBG&lt;BR&gt;
      EVMMAG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMMCS&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM1&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM0&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM3&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      62-3-1&lt;BR&gt;
      62-1-2&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      67R&lt;BR&gt;
      -&lt;BR&gt;
      67P&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      67X&lt;BR&gt;
      63V&lt;BR&gt;
      63S&lt;BR&gt;
      63M&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      63H&lt;BR&gt;
      63P&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      63X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
&lt;/TABLE&gt;
&lt;P&gt;&amp;nbsp;&lt;P&gt;
&lt;TABLE BORDER=0 CELLSPACING=1 CELLPADDING=3&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;
      &lt;FONT color="#0000FF" SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SMD TRIM-POT CROSS REFERENCE&lt;/B&gt;&lt;/FONT&gt;
      &lt;P&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURNS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;TOCOS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;AUX/KYOCERA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3224G&lt;BR&gt;
      3224J&lt;BR&gt;
      3224W&lt;BR&gt;
      3269P&lt;BR&gt;
      3269W&lt;BR&gt;
      3269X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      44G&lt;BR&gt;
      44J&lt;BR&gt;
      44W&lt;BR&gt;
      84P&lt;BR&gt;
      84W&lt;BR&gt;
      84X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST63Z&lt;BR&gt;
      ST63Y&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST5P&lt;BR&gt;
      ST5W&lt;BR&gt;
      ST5X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SINGLE TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURNS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;TOCOS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;AUX/KYOCERA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3314G&lt;BR&gt;
      3314J&lt;BR&gt;
      3364A/B&lt;BR&gt;
      3364C/D&lt;BR&gt;
      3364W/X&lt;BR&gt;
      3313G&lt;BR&gt;
      3313J&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      23B&lt;BR&gt;
      23A&lt;BR&gt;
      21X&lt;BR&gt;
      21W&lt;BR&gt;
      -&lt;BR&gt;
      22B&lt;BR&gt;
      22A&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ST5YL/ST53YL&lt;BR&gt;
      ST5YJ/5T53YJ&lt;BR&gt;
      ST-23A&lt;BR&gt;
      ST-22B&lt;BR&gt;
      ST-22&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ST-4B&lt;BR&gt;
      ST-4A&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST-3B&lt;BR&gt;
      ST-3A&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      EVM-6YS&lt;BR&gt;
      EVM-1E&lt;BR&gt;
      EVM-1G&lt;BR&gt;
      EVM-1D&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      G4B&lt;BR&gt;
      G4A&lt;BR&gt;
      TR04-3S1&lt;BR&gt;
      TRG04-2S1&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      DVR-43A&lt;BR&gt;
      CVR-42C&lt;BR&gt;
      CVR-42A/C&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
&lt;/TABLE&gt;
&lt;P&gt;
&lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;ALT =&amp;nbsp;ALTERNATE&lt;/B&gt;&lt;/FONT&gt;
&lt;P&gt;

&amp;nbsp;
&lt;P&gt;
&lt;/td&gt;
&lt;/tr&gt;
&lt;/table&gt;</description>
<packages>
<package name="C025-024X044">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.5 mm, outline 2.4 x 4.4 mm</description>
</package>
<package name="E2,5-7">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.54 mm, diameter 7 mm</description>
</package>
<package name="0204/7">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0204, grid 7.5 mm</description>
</package>
<package name="E3,5-8">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 3.5 mm, diameter 8 mm</description>
</package>
<package name="E3,5-10">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 3.5 mm, diameter 10 mm</description>
</package>
<package name="0207/10">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0207, grid 10 mm</description>
</package>
</packages>
</library>
<library name="74xx-eu">
<description>&lt;b&gt;TTL Devices, 74xx Series with European Symbols&lt;/b&gt;&lt;p&gt;
Based on the following sources:
&lt;ul&gt;
&lt;li&gt;Texas Instruments &lt;i&gt;TTL Data Book&lt;/i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;Volume 1, 1996.
&lt;li&gt;TTL Data Book, Volume 2 , 1993
&lt;li&gt;National Seminconductor Databook 1990, ALS/LS Logic
&lt;li&gt;ttl 74er digital data dictionary, ECA Electronic + Acustic GmbH, ISBN 3-88109-032-0
&lt;li&gt;http://icmaster.com/ViewCompare.asp
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DIL14">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="DIL20">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="DIL16">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="linear">
<description>&lt;b&gt;Linear Devices&lt;/b&gt;&lt;p&gt;
Operational amplifiers,  comparators, voltage regulators, ADCs, DACs, etc.&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DIL08">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="maxim">
<description>&lt;b&gt;Maxim Components&lt;/b&gt;&lt;p&gt;

&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DIL16">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="ic-package">
<description>&lt;b&gt;IC Packages an Sockets&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DIL24-6">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt; 0.6 inch</description>
</package>
<package name="DIL16">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="con-jack">
<description>&lt;b&gt;Jacks&lt;/b&gt;&lt;p&gt;
Power Connectors&lt;br&gt;
Phone Connectors&lt;br&gt;
Cinch Connectors&lt;br&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SPC4077">
<description>&lt;b&gt;DC POWER JACK 2mm&lt;/b&gt;&lt;br&gt; Right Angle, Through Hole, Rated 5A at 16VDC, PC Terminals&lt;p&gt;
Source: www.spctechnology.com .. 84N1161.pdf&lt;br&gt;
Distributor: &lt;b&gt;Farnell (www.Farnell.de)&lt;/b&gt;&lt;br&gt;
Created by Robert Siegler</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="DB9">
<description>&lt;h3&gt;9 Pin Serial Connector - Female PCB Mount Right Angle&lt;/h3&gt;
0.318" style. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:11&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/Connectors/DB9-PCB.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;DB9&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="jumper">
<description>&lt;b&gt;Jumpers&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="JP4Q">
<description>&lt;b&gt;JUMPER&lt;/b&gt;</description>
</package>
<package name="JP1">
<description>&lt;b&gt;JUMPER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="led">
<description>&lt;b&gt;LEDs&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;br&gt;
Extended by Federico Battaglin &lt;author&gt;&amp;lt;federico.rd@fdpinternational.com&amp;gt;&lt;/author&gt; with DUOLED</description>
<packages>
<package name="LED5MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
5 mm, round</description>
</package>
</packages>
</library>
<library name="crystal">
<description>&lt;b&gt;Crystals and Crystal Resonators&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="HC49U70">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="pot">
<description>&lt;b&gt;Potentiometers&lt;/b&gt;&lt;p&gt;
Beckman, Copal, Piher, Spectrol, Schukat&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="EVUEXXJ">
<description>&lt;b&gt;9 mm Square Rotary Potentiometers&lt;/b&gt; Single Type with Bushing, Horizontal, Snap-in&lt;p&gt;
Source: Panasonic</description>
</package>
</packages>
</library>
<library name="SparkFun-Switches">
<description>&lt;h3&gt;SparkFun Switches, Buttons, Encoders&lt;/h3&gt;
In this library you'll find switches, buttons, joysticks, and anything that moves to create or disrupt an electrical connection.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TACTILE_SWITCH_PTH_RIGHT_ANGLE_KIT">
<description>&lt;h3&gt;Momentary Switch (Pushbutton) - SPST - PTH, Right-angle&lt;/h3&gt;
&lt;p&gt;Normally-open (NO) SPST momentary switches (buttons, pushbuttons).&lt;/p&gt;
&lt;p&gt;&lt;a href="http://cdn.sparkfun.com/datasheets/Components/Switches/SW016.JPG"&gt;Dimensional Drawing&lt;/a&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="resistor-sil">
<description>&lt;b&gt;Resistors in Single Inline Packages&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SIL6">
<description>&lt;b&gt;Single In Line&lt;/b&gt;</description>
</package>
<package name="SIL7">
<description>&lt;b&gt;Single In Line&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="special">
<description>&lt;b&gt;Special Devices&lt;/b&gt;&lt;p&gt;
7-segment displays, switches, heatsinks, crystals, transformers, etc.&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="EDG-05">
<description>&lt;b&gt;DIP SWITCH&lt;/b&gt;</description>
</package>
<package name="EDG-06">
<description>&lt;b&gt;DIP SWITCH&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="testpad">
<description>&lt;b&gt;Test Pins/Pads&lt;/b&gt;&lt;p&gt;
Cream on SMD OFF.&lt;br&gt;
new: Attribute TP_SIGNAL_NAME&lt;br&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="P1-13">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="speech">
<packages>
<package name="DIL40-6">
</package>
<package name="DIL28-6">
</package>
</packages>
</library>
<library name="tms4016">
<packages>
<package name="DIL24-6">
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="STX3100">
<description>&lt;b&gt;MIC/HEADPHONE JACK&lt;/b&gt;&lt;p&gt;
KS-S stereo microphone/headphone jack&lt;p&gt;
 PG203JN (Schukat)</description>
</package>
</packages>
</library>
<library name="lm2575">
<packages>
<package name="DIL16">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="diode">
<description>&lt;b&gt;Diodes&lt;/b&gt;&lt;p&gt;
Based on the following sources:
&lt;ul&gt;
&lt;li&gt;Motorola : www.onsemi.com
&lt;li&gt;Fairchild : www.fairchildsemi.com
&lt;li&gt;Philips : www.semiconductors.com
&lt;li&gt;Vishay : www.vishay.de
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DO41-7.6">
<description>&lt;b&gt;DO41&lt;/b&gt; 7.6mm x 2mm&lt;p&gt;
Source: http://www.diodes.com/datasheets/ds23001.pdf</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C8" library="rcl" package="C025-024X044" value="22pF">
<attribute name="NAME"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="rcl" package="C025-024X044" value="0.1uF">
<attribute name="NAME"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="rcl" package="C025-024X044" value="0.1uF">
<attribute name="NAME"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C18" library="rcl" package="C025-024X044" value="22nF">
<attribute name="NAME"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C19" library="rcl" package="C025-024X044" value="22nF">
<attribute name="NAME"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C20" library="rcl" package="C025-024X044" value="1uF">
<attribute name="NAME"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C23" library="rcl" package="C025-024X044" value="0.1uF">
<attribute name="NAME"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="rcl" package="C025-024X044" value="0.1uF">
<attribute name="NAME"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C10" library="rcl" package="C025-024X044" value="22pF">
<attribute name="NAME"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="rcl" package="C025-024X044" value="0.1uF">
<attribute name="NAME"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C9" library="rcl" package="C025-024X044" value="0.1uF">
<attribute name="NAME"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C11" library="rcl" package="C025-024X044" value="0.1uF">
<attribute name="NAME"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C24" library="rcl" package="C025-024X044" value="10uF">
<attribute name="NAME"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C25" library="rcl" package="C025-024X044" value="0.1uF">
<attribute name="NAME"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C26" library="rcl" package="C025-024X044" value="0.1uF">
<attribute name="NAME"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C27" library="rcl" package="E2,5-7" value="100uF">
<attribute name="NAME"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="rcl" package="C025-024X044" value="0.1uF">
<attribute name="NAME"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C14" library="rcl" package="C025-024X044" value="0.1uF">
<attribute name="NAME"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C15" library="rcl" package="C025-024X044" value="0.1uF">
<attribute name="NAME"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C16" library="rcl" package="C025-024X044" value="0.1uF">
<attribute name="NAME"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C17" library="rcl" package="C025-024X044" value="0.1uF">
<attribute name="NAME"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C21" library="rcl" package="C025-024X044" value="22pF">
<attribute name="NAME"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C22" library="rcl" package="C025-024X044" value="22pF">
<attribute name="NAME"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="IC1" library="74xx-eu" package="DIL14" value="74HCT14N">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC2" library="74xx-eu" package="DIL20" value="74HCT373N">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC3" library="74xx-eu" package="DIL20" value="74HCT373N">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC4" library="74xx-eu" package="DIL16" value="74HCT138N">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC5" library="linear" package="DIL08" value="LM386N-4">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC6" library="maxim" package="DIL16" value="MAX202CPE">
<attribute name="MF" value="MAXIM"/>
<attribute name="MPN" value="MAX202CPE+"/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="9723803"/>
<attribute name="OC_NEWARK" value="68K4531"/>
<attribute name="VALUE"/>
</element>
<element name="IC7" library="ic-package" package="DIL24-6" value="ROM">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="con-jack" package="SPC4077" value="5V DC">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="VALUE"/>
</element>
<element name="J2" library="SparkFun-Connectors" package="DB9" value="DB9-F">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CONN-08194"/>
<attribute name="VALUE"/>
</element>
<element name="JP1" library="jumper" package="JP4Q" value="OPT BLK">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP2" library="jumper" package="JP1" value="AMP_OUT">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED1" library="led" package="LED5MM" value="SBY">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q1" library="crystal" package="HC49U70" value="10MHz">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="VALUE"/>
</element>
<element name="Q2" library="crystal" package="HC49U70" value="3.12MHz">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="rcl" package="0204/7" value="100K">
<attribute name="NAME"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="rcl" package="0204/7" value="330">
<attribute name="NAME"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="rcl" package="0204/7" value="33K">
<attribute name="NAME"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="rcl" package="0204/7" value="33K">
<attribute name="NAME"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="rcl" package="0204/7" value="10">
<attribute name="NAME"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="pot" package="EVUEXXJ" value="EVUE3J">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="S1" library="SparkFun-Switches" package="TACTILE_SWITCH_PTH_RIGHT_ANGLE_KIT" value="MOMENTARY-SWITCH-SPST-PTH-RIGHT-ANGLE-KIT">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CONN-10672"/>
<attribute name="SF_SKU" value="COM-10791"/>
<attribute name="VALUE"/>
</element>
<element name="RN1" library="resistor-sil" package="SIL6" value="10K">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="VALUE"/>
</element>
<element name="RN2" library="resistor-sil" package="SIL7" value="10K">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="VALUE"/>
</element>
<element name="SW1" library="special" package="EDG-05" value="UART_OPT">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SW2" library="special" package="EDG-06" value="OPTIONS">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP1" library="testpad" package="P1-13" value="PTR1PAD1-13">
<attribute name="NAME"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="TP7" library="testpad" package="P1-13" value="PTR1PAD1-13">
<attribute name="NAME"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="TP8" library="testpad" package="P1-13" value="PTR1PAD1-13">
<attribute name="NAME"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="speech" package="DIL40-6" value="CTS256A-AL2">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U2" library="speech" package="DIL28-6" value="SPO256-AL2">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U3" library="tms4016" package="DIL24-6" value="TMS4016">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="X1" library="adafruit" package="STX3100" value="STEREOJACK">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="rcl" package="C025-024X044" value="0.1uF">
<attribute name="NAME"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="IC8" library="ic-package" package="DIL16" value="SPR">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="rcl" package="C025-024X044" value="0.1uF">
<attribute name="NAME"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="TP6" library="testpad" package="P1-13" value="PTR1PAD1-13">
<attribute name="NAME"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="TP3" library="testpad" package="P1-13" value="PTR1PAD1-13">
<attribute name="NAME"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="TP2" library="testpad" package="P1-13" value="PTR1PAD1-13">
<attribute name="NAME"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="TP5" library="testpad" package="P1-13" value="PTR1PAD1-13">
<attribute name="NAME"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="TP4" library="testpad" package="P1-13" value="PTR1PAD1-13">
<attribute name="NAME"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="LED2" library="led" package="LED5MM" value="SBY">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R9" library="rcl" package="0204/7" value="330">
<attribute name="NAME"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="U4" library="lm2575" package="DIL16" value="LM2575-5.0N"/>
<element name="C13" library="rcl" package="E3,5-8" value="100uF">
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="C12" library="rcl" package="E3,5-10" value="330uF">
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="D1" library="diode" package="DO41-7.6" value="1N5818-B"/>
<element name="L1" library="rcl" package="0207/10" value="330uH">
<attribute name="SPICEPREFIX" value="L"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="IC2" pad="10"/>
<contactref element="IC3" pad="10"/>
<contactref element="IC4" pad="8"/>
<contactref element="IC1" pad="7"/>
<contactref element="C8" pad="2"/>
<contactref element="C10" pad="2"/>
<contactref element="U1" pad="P$40"/>
<contactref element="U1" pad="P$36"/>
<contactref element="C2" pad="2"/>
<contactref element="S1" pad="1"/>
<contactref element="IC1" pad="9"/>
<contactref element="IC1" pad="13"/>
<contactref element="R2" pad="1"/>
<contactref element="J1" pad="1"/>
<contactref element="RN2" pad="1"/>
<contactref element="C16" pad="1"/>
<contactref element="C17" pad="2"/>
<contactref element="IC6" pad="15"/>
<contactref element="J2" pad="5"/>
<contactref element="IC2" pad="1"/>
<contactref element="IC4" pad="5"/>
<contactref element="U2" pad="P$1"/>
<contactref element="C21" pad="2"/>
<contactref element="C22" pad="2"/>
<contactref element="U3" pad="P$12"/>
<contactref element="U3" pad="P$20"/>
<contactref element="U2" pad="P$22"/>
<contactref element="RN1" pad="1"/>
<contactref element="IC3" pad="18"/>
<contactref element="IC7" pad="20"/>
<contactref element="IC7" pad="12"/>
<contactref element="C18" pad="2"/>
<contactref element="C19" pad="2"/>
<contactref element="R6" pad="1"/>
<contactref element="IC5" pad="2"/>
<contactref element="IC5" pad="4"/>
<contactref element="C25" pad="2"/>
<contactref element="C23" pad="2"/>
<contactref element="C26" pad="2"/>
<contactref element="X1" pad="1"/>
<contactref element="C4" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="C7" pad="2"/>
<contactref element="C9" pad="2"/>
<contactref element="C11" pad="2"/>
<contactref element="JP2" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="IC8" pad="1"/>
<contactref element="IC8" pad="8"/>
<contactref element="C3" pad="2"/>
<contactref element="TP3" pad="TP"/>
<contactref element="R9" pad="1"/>
<contactref element="U4" pad="5"/>
<contactref element="J1" pad="2"/>
<contactref element="U4" pad="14"/>
<contactref element="U4" pad="13"/>
<contactref element="U4" pad="12"/>
<contactref element="U4" pad="11"/>
<contactref element="U4" pad="9"/>
<contactref element="C13" pad="-"/>
<contactref element="C12" pad="-"/>
<contactref element="D1" pad="A"/>
</signal>
<signal name="VCC">
<contactref element="IC2" pad="20"/>
<contactref element="IC3" pad="20"/>
<contactref element="IC4" pad="16"/>
<contactref element="IC1" pad="14"/>
<contactref element="SW2" pad="6"/>
<contactref element="SW2" pad="5"/>
<contactref element="SW2" pad="4"/>
<contactref element="SW2" pad="3"/>
<contactref element="SW2" pad="2"/>
<contactref element="SW2" pad="1"/>
<contactref element="U1" pad="P$25"/>
<contactref element="R1" pad="2"/>
<contactref element="IC6" pad="16"/>
<contactref element="U2" pad="P$19"/>
<contactref element="U2" pad="P$23"/>
<contactref element="U2" pad="P$7"/>
<contactref element="U3" pad="P$24"/>
<contactref element="SW1" pad="5"/>
<contactref element="SW1" pad="1"/>
<contactref element="SW1" pad="2"/>
<contactref element="SW1" pad="3"/>
<contactref element="SW1" pad="4"/>
<contactref element="IC3" pad="17"/>
<contactref element="IC3" pad="4"/>
<contactref element="IC7" pad="24"/>
<contactref element="IC5" pad="6"/>
<contactref element="C23" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="C5" pad="1"/>
<contactref element="C6" pad="1"/>
<contactref element="C7" pad="1"/>
<contactref element="C9" pad="1"/>
<contactref element="C11" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="IC8" pad="11"/>
<contactref element="IC8" pad="7"/>
<contactref element="C3" pad="1"/>
<contactref element="TP6" pad="TP"/>
<contactref element="LED2" pad="A"/>
<contactref element="L1" pad="1"/>
<contactref element="C12" pad="+"/>
</signal>
<signal name="N$1">
<contactref element="SW2" pad="12"/>
<contactref element="U1" pad="P$6"/>
<contactref element="RN2" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="SW2" pad="11"/>
<contactref element="U1" pad="P$7"/>
<contactref element="RN2" pad="3"/>
</signal>
<signal name="N$3">
<contactref element="SW2" pad="10"/>
<contactref element="U1" pad="P$8"/>
<contactref element="RN2" pad="4"/>
</signal>
<signal name="N$4">
<contactref element="SW2" pad="9"/>
<contactref element="U1" pad="P$9"/>
<contactref element="RN2" pad="5"/>
</signal>
<signal name="N$5">
<contactref element="SW2" pad="8"/>
<contactref element="U1" pad="P$10"/>
<contactref element="RN2" pad="6"/>
</signal>
<signal name="N$6">
<contactref element="SW2" pad="7"/>
<contactref element="U1" pad="P$11"/>
<contactref element="RN2" pad="7"/>
</signal>
<signal name="N$7">
<contactref element="Q1" pad="2"/>
<contactref element="U1" pad="P$17"/>
<contactref element="C8" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="Q1" pad="1"/>
<contactref element="U1" pad="P$18"/>
<contactref element="C10" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="U1" pad="P$12"/>
<contactref element="TP1" pad="TP"/>
</signal>
<signal name="RX">
<contactref element="U1" pad="P$16"/>
<contactref element="IC6" pad="9"/>
</signal>
<signal name="TX">
<contactref element="U1" pad="P$37"/>
<contactref element="IC6" pad="10"/>
</signal>
<signal name="BSY">
<contactref element="U1" pad="P$3"/>
<contactref element="IC6" pad="11"/>
</signal>
<signal name="RW">
<contactref element="U1" pad="P$1"/>
<contactref element="U3" pad="P$21"/>
</signal>
<signal name="A8">
<contactref element="U1" pad="P$27"/>
<contactref element="U3" pad="P$23"/>
<contactref element="IC7" pad="23"/>
</signal>
<signal name="A9">
<contactref element="U1" pad="P$26"/>
<contactref element="U3" pad="P$22"/>
<contactref element="IC7" pad="22"/>
</signal>
<signal name="A10">
<contactref element="U1" pad="P$24"/>
<contactref element="U3" pad="P$19"/>
<contactref element="IC7" pad="19"/>
</signal>
<signal name="RST">
<contactref element="U1" pad="P$14"/>
<contactref element="IC1" pad="4"/>
<contactref element="U2" pad="P$25"/>
<contactref element="U2" pad="P$2"/>
</signal>
<signal name="N$10">
<contactref element="IC1" pad="2"/>
<contactref element="IC1" pad="3"/>
</signal>
<signal name="N$11">
<contactref element="IC1" pad="1"/>
<contactref element="R1" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="S1" pad="2"/>
</signal>
<signal name="SBY">
<contactref element="IC1" pad="11"/>
<contactref element="U2" pad="P$8"/>
</signal>
<signal name="N$12">
<contactref element="IC1" pad="10"/>
<contactref element="LED1" pad="A"/>
</signal>
<signal name="N$13">
<contactref element="LED1" pad="K"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="N$14">
<contactref element="IC6" pad="1"/>
<contactref element="C14" pad="1"/>
</signal>
<signal name="N$15">
<contactref element="C14" pad="2"/>
<contactref element="IC6" pad="3"/>
</signal>
<signal name="N$16">
<contactref element="IC6" pad="4"/>
<contactref element="C15" pad="1"/>
</signal>
<signal name="N$17">
<contactref element="C15" pad="2"/>
<contactref element="IC6" pad="5"/>
</signal>
<signal name="V+">
<contactref element="IC6" pad="2"/>
<contactref element="C17" pad="1"/>
</signal>
<signal name="V-">
<contactref element="IC6" pad="6"/>
<contactref element="C16" pad="2"/>
</signal>
<signal name="N$20">
<contactref element="IC6" pad="8"/>
<contactref element="J2" pad="3"/>
</signal>
<signal name="N$21">
<contactref element="IC6" pad="13"/>
<contactref element="J2" pad="7"/>
</signal>
<signal name="N$22">
<contactref element="IC6" pad="14"/>
<contactref element="J2" pad="8"/>
</signal>
<signal name="N$23">
<contactref element="IC6" pad="7"/>
<contactref element="J2" pad="2"/>
</signal>
<signal name="D0">
<contactref element="U1" pad="P$28"/>
<contactref element="IC2" pad="3"/>
<contactref element="U3" pad="P$9"/>
<contactref element="IC3" pad="19"/>
<contactref element="IC7" pad="9"/>
</signal>
<signal name="D1">
<contactref element="U1" pad="P$29"/>
<contactref element="IC2" pad="4"/>
<contactref element="U3" pad="P$10"/>
<contactref element="IC3" pad="16"/>
<contactref element="IC7" pad="10"/>
</signal>
<signal name="D2">
<contactref element="U1" pad="P$30"/>
<contactref element="IC2" pad="7"/>
<contactref element="U3" pad="P$11"/>
<contactref element="IC3" pad="15"/>
<contactref element="IC7" pad="11"/>
</signal>
<signal name="D3">
<contactref element="U1" pad="P$31"/>
<contactref element="IC2" pad="8"/>
<contactref element="U3" pad="P$13"/>
<contactref element="IC3" pad="12"/>
<contactref element="IC7" pad="13"/>
</signal>
<signal name="D4">
<contactref element="U1" pad="P$32"/>
<contactref element="IC2" pad="13"/>
<contactref element="U3" pad="P$14"/>
<contactref element="IC3" pad="9"/>
<contactref element="IC7" pad="14"/>
</signal>
<signal name="D5">
<contactref element="U1" pad="P$33"/>
<contactref element="IC2" pad="14"/>
<contactref element="U3" pad="P$15"/>
<contactref element="IC3" pad="6"/>
<contactref element="IC7" pad="15"/>
</signal>
<signal name="D6">
<contactref element="U1" pad="P$34"/>
<contactref element="IC2" pad="17"/>
<contactref element="U3" pad="P$16"/>
<contactref element="IC3" pad="5"/>
<contactref element="IC7" pad="16"/>
</signal>
<signal name="D7">
<contactref element="U1" pad="P$35"/>
<contactref element="IC2" pad="18"/>
<contactref element="U3" pad="P$17"/>
<contactref element="IC3" pad="2"/>
<contactref element="IC7" pad="17"/>
</signal>
<signal name="N$18">
<contactref element="U1" pad="P$38"/>
<contactref element="IC2" pad="11"/>
</signal>
<signal name="N$19">
<contactref element="U1" pad="P$39"/>
<contactref element="IC4" pad="4"/>
</signal>
<signal name="N$24">
<contactref element="U1" pad="P$19"/>
<contactref element="IC1" pad="5"/>
</signal>
<signal name="N$25">
<contactref element="IC1" pad="6"/>
<contactref element="IC4" pad="6"/>
</signal>
<signal name="A0">
<contactref element="IC2" pad="2"/>
<contactref element="U2" pad="P$18"/>
<contactref element="U3" pad="P$8"/>
<contactref element="IC7" pad="8"/>
</signal>
<signal name="A1">
<contactref element="IC2" pad="5"/>
<contactref element="U2" pad="P$17"/>
<contactref element="U3" pad="P$7"/>
<contactref element="IC7" pad="7"/>
</signal>
<signal name="A2">
<contactref element="IC2" pad="6"/>
<contactref element="U2" pad="P$16"/>
<contactref element="U3" pad="P$6"/>
<contactref element="IC7" pad="6"/>
</signal>
<signal name="A3">
<contactref element="IC2" pad="9"/>
<contactref element="U2" pad="P$15"/>
<contactref element="U3" pad="P$5"/>
<contactref element="IC7" pad="5"/>
</signal>
<signal name="A4">
<contactref element="IC2" pad="12"/>
<contactref element="U2" pad="P$14"/>
<contactref element="U3" pad="P$4"/>
<contactref element="IC7" pad="4"/>
</signal>
<signal name="A5">
<contactref element="IC2" pad="15"/>
<contactref element="U2" pad="P$13"/>
<contactref element="U3" pad="P$3"/>
<contactref element="IC7" pad="3"/>
</signal>
<signal name="A6">
<contactref element="IC2" pad="16"/>
<contactref element="U2" pad="P$11"/>
<contactref element="U3" pad="P$2"/>
<contactref element="IC7" pad="2"/>
</signal>
<signal name="A7">
<contactref element="IC2" pad="19"/>
<contactref element="U2" pad="P$10"/>
<contactref element="U3" pad="P$1"/>
<contactref element="IC7" pad="1"/>
</signal>
<signal name="N$26">
<contactref element="U1" pad="P$22"/>
<contactref element="IC4" pad="1"/>
</signal>
<signal name="N$27">
<contactref element="U1" pad="P$21"/>
<contactref element="IC4" pad="2"/>
</signal>
<signal name="N$28">
<contactref element="U1" pad="P$20"/>
<contactref element="IC4" pad="3"/>
</signal>
<signal name="N$29">
<contactref element="U2" pad="P$28"/>
<contactref element="C22" pad="1"/>
<contactref element="Q2" pad="2"/>
</signal>
<signal name="N$30">
<contactref element="U2" pad="P$27"/>
<contactref element="C21" pad="1"/>
<contactref element="Q2" pad="1"/>
</signal>
<signal name="AUDIO">
<contactref element="U2" pad="P$24"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="SER_CS">
<contactref element="IC4" pad="14"/>
<contactref element="IC3" pad="1"/>
</signal>
<signal name="RAM_CS">
<contactref element="IC4" pad="12"/>
<contactref element="U3" pad="P$18"/>
</signal>
<signal name="N$31">
<contactref element="IC4" pad="11"/>
<contactref element="JP1" pad="8"/>
</signal>
<signal name="N$32">
<contactref element="IC4" pad="10"/>
<contactref element="JP1" pad="6"/>
</signal>
<signal name="N$33">
<contactref element="IC4" pad="9"/>
<contactref element="JP1" pad="4"/>
</signal>
<signal name="N$34">
<contactref element="IC4" pad="7"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="N$35">
<contactref element="IC4" pad="13"/>
<contactref element="U2" pad="P$20"/>
</signal>
<signal name="N$36">
<contactref element="IC4" pad="15"/>
<contactref element="TP7" pad="TP"/>
</signal>
<signal name="A11">
<contactref element="U1" pad="P$23"/>
<contactref element="IC7" pad="21"/>
</signal>
<signal name="N$37">
<contactref element="U1" pad="P$13"/>
<contactref element="U2" pad="P$9"/>
</signal>
<signal name="ROM_CS">
<contactref element="JP1" pad="7"/>
<contactref element="JP1" pad="1"/>
<contactref element="JP1" pad="3"/>
<contactref element="JP1" pad="5"/>
<contactref element="IC7" pad="18"/>
</signal>
<signal name="N$38">
<contactref element="IC3" pad="3"/>
<contactref element="RN1" pad="2"/>
<contactref element="SW1" pad="10"/>
</signal>
<signal name="N$39">
<contactref element="IC3" pad="7"/>
<contactref element="RN1" pad="3"/>
<contactref element="SW1" pad="9"/>
</signal>
<signal name="N$40">
<contactref element="IC3" pad="8"/>
<contactref element="RN1" pad="4"/>
<contactref element="SW1" pad="8"/>
</signal>
<signal name="N$41">
<contactref element="IC3" pad="13"/>
<contactref element="RN1" pad="5"/>
<contactref element="SW1" pad="7"/>
</signal>
<signal name="N$42">
<contactref element="IC3" pad="14"/>
<contactref element="RN1" pad="6"/>
<contactref element="SW1" pad="6"/>
</signal>
<signal name="N$43">
<contactref element="TP8" pad="TP"/>
<contactref element="IC3" pad="11"/>
</signal>
<signal name="N$44">
<contactref element="R3" pad="2"/>
<contactref element="R4" pad="1"/>
<contactref element="C18" pad="1"/>
</signal>
<signal name="N$45">
<contactref element="R4" pad="2"/>
<contactref element="C20" pad="2"/>
<contactref element="C19" pad="1"/>
</signal>
<signal name="N$46">
<contactref element="C20" pad="1"/>
<contactref element="R6" pad="3"/>
</signal>
<signal name="N$47">
<contactref element="R6" pad="2"/>
<contactref element="IC5" pad="3"/>
</signal>
<signal name="N$48">
<contactref element="IC5" pad="7"/>
<contactref element="C25" pad="1"/>
</signal>
<signal name="N$49">
<contactref element="IC5" pad="8"/>
<contactref element="C24" pad="1"/>
</signal>
<signal name="N$50">
<contactref element="C24" pad="2"/>
<contactref element="IC5" pad="1"/>
</signal>
<signal name="N$51">
<contactref element="IC5" pad="5"/>
<contactref element="C27" pad="-"/>
<contactref element="R5" pad="2"/>
</signal>
<signal name="N$52">
<contactref element="R5" pad="1"/>
<contactref element="C26" pad="1"/>
</signal>
<signal name="N$53">
<contactref element="C27" pad="+"/>
<contactref element="X1" pad="3"/>
<contactref element="X1" pad="5"/>
<contactref element="JP2" pad="1"/>
</signal>
<signal name="SPR_SERIN">
<contactref element="U2" pad="P$12"/>
<contactref element="IC8" pad="14"/>
</signal>
<signal name="SPR_SEROUT">
<contactref element="U2" pad="P$21"/>
<contactref element="IC8" pad="10"/>
</signal>
<signal name="SPR_ROMENB">
<contactref element="U2" pad="P$3"/>
<contactref element="IC8" pad="9"/>
</signal>
<signal name="SPR_CLK">
<contactref element="U2" pad="P$26"/>
<contactref element="IC8" pad="4"/>
</signal>
<signal name="C1">
<contactref element="U2" pad="P$4"/>
<contactref element="IC8" pad="15"/>
</signal>
<signal name="C2">
<contactref element="U2" pad="P$5"/>
<contactref element="IC8" pad="16"/>
</signal>
<signal name="C3">
<contactref element="U2" pad="P$6"/>
<contactref element="IC8" pad="2"/>
</signal>
<signal name="N$54">
<contactref element="U1" pad="P$15"/>
<contactref element="TP2" pad="TP"/>
</signal>
<signal name="N$58">
<contactref element="IC1" pad="8"/>
<contactref element="TP4" pad="TP"/>
</signal>
<signal name="N$59">
<contactref element="IC1" pad="12"/>
<contactref element="TP5" pad="TP"/>
</signal>
<signal name="N$60">
<contactref element="R9" pad="2"/>
<contactref element="LED2" pad="K"/>
</signal>
<signal name="VIN">
<contactref element="J1" pad="3"/>
<contactref element="U4" pad="16"/>
<contactref element="C13" pad="+"/>
</signal>
<signal name="N$55">
<contactref element="L1" pad="2"/>
<contactref element="D1" pad="C"/>
<contactref element="U4" pad="3"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
