<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.0.1">
<drawing>
<library>
<description>MAXIM LED Display Drivers</description>
<packages>
<package name="DIL40">
<description>&lt;b&gt;PDIP 40 PINS&lt;/b&gt; - PDIP .600"&lt;br&gt;
&lt;p&gt;
Supporting Materials:
&lt;ul&gt;
&lt;li&gt;&lt;a href=https://pdfserv.maximintegrated.com/package_dwgs/21-0044.PDF&gt;Document 21-0044&lt;/a&gt;&lt;/li&gt;
&lt;/p&gt;</description>
</package>
<package name="SSOP36">
<description>&lt;b&gt;36L SSOP, 0.80 MM PITCH&lt;/b&gt; - 40 Pin Thin QFN 6x6x0.75 mm&lt;br&gt;
&lt;p&gt;
Supporting Materials:
&lt;ul&gt;
&lt;li&gt;&lt;a href=https://pdfserv.maximintegrated.com/land_patterns/90-0098.PDF&gt;Land Patern No 90-0098&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href=https://pdfserv.maximintegrated.com/package_dwgs/21-0040.PDF&gt;Document 21-0040&lt;/a&gt;&lt;/li&gt;
&lt;/p&gt;</description>
</package>
<package name="TQFN40-EP">
<description>&lt;b&gt;40 TQFN-EP Package Type&lt;/b&gt; - 40 Pin Thin QFN 6x6x0.75 mm&lt;br&gt;
&lt;p&gt;
Supporting Materials:
&lt;ul&gt;
&lt;li&gt;&lt;a href=https://pdfserv.maximintegrated.com/land_patterns/90-0055.PDF&gt;Land Patern No 90-0055&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href=https://pdfserv.maximintegrated.com/package_dwgs/21-0141.PDF&gt;Document 21-0141&lt;/a&gt;&lt;/li&gt;
&lt;/p&gt;</description>
</package>
<package name="SSOP28">
<description>&lt;b&gt;0.209" SSOP, 28 LEADS&lt;/b&gt; - SSOP 5.3mm BODY&lt;br&gt;
&lt;p&gt;
Supporting Materials:
&lt;ul&gt;
&lt;li&gt;&lt;a href=https://pdfserv.maximintegrated.com/land_patterns/90-0095.PDF&gt;Land Patern No 90-0095&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href=https://pdfserv.maximintegrated.com/package_dwgs/21-0056.PDF&gt;Document 21-0056&lt;/a&gt;&lt;/li&gt;
&lt;/p&gt;</description>
</package>
<package name="DIL28-6">
<description>&lt;b&gt;PDIP 28 LEADS&lt;/b&gt; - PDIP .300"&lt;br&gt;
&lt;p&gt;
Supporting Materials:
&lt;ul&gt;
&lt;li&gt;&lt;a href=https://pdfserv.maximintegrated.com/package_dwgs/21-0043.PDF&gt;Document 21-0043&lt;/a&gt;&lt;/li&gt;
&lt;/p&gt;</description>
</package>
<package name="DIL16">
<description>&lt;b&gt;PDIP 16 PIN&lt;/b&gt; - PDIP 0.300"
&lt;p&gt;
Supporting Materials:
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://pdfserv.maximintegrated.com/package_dwgs/21-0043.PDF"&gt;Document 21-0043&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;
&lt;/p&gt;</description>
</package>
<package name="QSOP16">
<description>&lt;b&gt;QSOP 16 PIN&lt;/b&gt; - QSOP .150", 0.25" LEAD PITCH
&lt;p&gt;
Supporting Materials:
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://pdfserv.maximintegrated.com/package_dwgs/21-0055.PDF"&gt;Document 21-0055&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;
&lt;/p&gt;</description>
</package>
</packages>
<symbols>
<symbol name="MAX6953-DIL40">
<pin name="O0"/>
<pin name="O1"/>
<pin name="O2"/>
<pin name="GND@4" direction="pwr"/>
<pin name="GND@5" direction="pwr"/>
<pin name="GND@6" direction="pwr"/>
<pin name="O3"/>
<pin name="O4"/>
<pin name="O5"/>
<pin name="O6"/>
<pin name="O7"/>
<pin name="O8"/>
<pin name="O9"/>
<pin name="O10"/>
<pin name="O11"/>
<pin name="NC@16" direction="nc"/>
<pin name="ISET"/>
<pin name="AD1" direction="in"/>
<pin name="GND@19" direction="pwr"/>
<pin name="BLINK" direction="out"/>
<pin name="OSC"/>
<pin name="AD0" direction="in"/>
<pin name="SDA"/>
<pin name="SCL" direction="in"/>
<pin name="NC@25" direction="nc"/>
<pin name="O12"/>
<pin name="O13"/>
<pin name="O14"/>
<pin name="O15"/>
<pin name="O16"/>
<pin name="O17"/>
<pin name="O18"/>
<pin name="O19"/>
<pin name="O20"/>
<pin name="V+@35" direction="pwr"/>
<pin name="V+@36" direction="pwr"/>
<pin name="V+@37" direction="pwr"/>
<pin name="O21"/>
<pin name="O22"/>
<pin name="O23"/>
</symbol>
<symbol name="MAX6952-DIL40">
<pin name="O0"/>
<pin name="O1"/>
<pin name="O2"/>
<pin name="GND@4" direction="pwr"/>
<pin name="GND@5" direction="pwr"/>
<pin name="GND@6" direction="pwr"/>
<pin name="O3"/>
<pin name="O4"/>
<pin name="O5"/>
<pin name="O6"/>
<pin name="O7"/>
<pin name="O8"/>
<pin name="O9"/>
<pin name="O10"/>
<pin name="O11"/>
<pin name="NC@16" direction="nc"/>
<pin name="ISET"/>
<pin name="DOUT" direction="out"/>
<pin name="GND@18" direction="pwr"/>
<pin name="!CS"/>
<pin name="OSC" direction="in"/>
<pin name="BLINK" direction="out"/>
<pin name="DIN" direction="in"/>
<pin name="CLK" direction="in"/>
<pin name="NC@25" direction="nc"/>
<pin name="O12"/>
<pin name="O13"/>
<pin name="O14"/>
<pin name="O15"/>
<pin name="O16"/>
<pin name="O17"/>
<pin name="O18"/>
<pin name="O19"/>
<pin name="O20"/>
<pin name="V+@35" direction="pwr"/>
<pin name="V+@36" direction="pwr"/>
<pin name="V+@37" direction="pwr"/>
<pin name="O21"/>
<pin name="O22"/>
<pin name="O23"/>
</symbol>
<symbol name="MAX6952-SSOP36">
<pin name="O0"/>
<pin name="O1"/>
<pin name="O2"/>
<pin name="GND@4" direction="pwr"/>
<pin name="GND@5" direction="pwr"/>
<pin name="O3"/>
<pin name="O4"/>
<pin name="O5"/>
<pin name="O6"/>
<pin name="O7"/>
<pin name="O8"/>
<pin name="O9"/>
<pin name="O10"/>
<pin name="O11"/>
<pin name="ISET"/>
<pin name="DOUT" direction="out"/>
<pin name="GND@16" direction="pwr"/>
<pin name="!CS"/>
<pin name="OSC" direction="in"/>
<pin name="BLINK" direction="out"/>
<pin name="DIN" direction="in"/>
<pin name="CLK" direction="in"/>
<pin name="O12"/>
<pin name="O13"/>
<pin name="O14"/>
<pin name="O15"/>
<pin name="O16"/>
<pin name="O17"/>
<pin name="O18"/>
<pin name="O19"/>
<pin name="O20"/>
<pin name="V+@33" direction="pwr"/>
<pin name="V+@32" direction="pwr"/>
<pin name="O21"/>
<pin name="O22"/>
<pin name="O23"/>
</symbol>
<symbol name="MAX6953-SSOP36">
<pin name="O0"/>
<pin name="O1"/>
<pin name="O2"/>
<pin name="GND@4" direction="pwr"/>
<pin name="GND@5" direction="pwr"/>
<pin name="O3"/>
<pin name="O4"/>
<pin name="O5"/>
<pin name="O6"/>
<pin name="O7"/>
<pin name="O8"/>
<pin name="O9"/>
<pin name="O10"/>
<pin name="O11"/>
<pin name="ISET"/>
<pin name="AD1" direction="in"/>
<pin name="BLINK" direction="out"/>
<pin name="OSC"/>
<pin name="AD0" direction="in"/>
<pin name="SDA"/>
<pin name="SCL" direction="in"/>
<pin name="O12"/>
<pin name="O13"/>
<pin name="O14"/>
<pin name="O15"/>
<pin name="O16"/>
<pin name="O17"/>
<pin name="O18"/>
<pin name="O19"/>
<pin name="O20"/>
<pin name="V+@33" direction="pwr"/>
<pin name="V+@32" direction="pwr"/>
<pin name="O21"/>
<pin name="O22"/>
<pin name="O23"/>
<pin name="GND@17"/>
</symbol>
<symbol name="MAX6954-SSOP36">
<pin name="O0"/>
<pin name="O1"/>
<pin name="O2"/>
<pin name="GND@16" direction="pwr"/>
<pin name="GND@18" direction="pwr"/>
<pin name="O3"/>
<pin name="O4"/>
<pin name="O5"/>
<pin name="O6"/>
<pin name="O7"/>
<pin name="O8"/>
<pin name="O9"/>
<pin name="O10"/>
<pin name="O11"/>
<pin name="ISET"/>
<pin name="!CS" direction="in"/>
<pin name="DOUT" direction="out"/>
<pin name="OSC" direction="in"/>
<pin name="BLINK" direction="out"/>
<pin name="DIN" direction="in"/>
<pin name="CLK" direction="in"/>
<pin name="O12"/>
<pin name="O13"/>
<pin name="O14"/>
<pin name="O15"/>
<pin name="O16"/>
<pin name="O17"/>
<pin name="O18"/>
<pin name="P0"/>
<pin name="P1"/>
<pin name="V+@21" direction="pwr"/>
<pin name="V+@19" direction="pwr"/>
<pin name="P2"/>
<pin name="P3"/>
<pin name="P4"/>
<pin name="OSC_OUT" direction="out"/>
</symbol>
<symbol name="MAX6954-DIL40">
<pin name="O0"/>
<pin name="O1"/>
<pin name="O2"/>
<pin name="GND@17" direction="pwr"/>
<pin name="GND@18" direction="pwr"/>
<pin name="GND@20" direction="pwr"/>
<pin name="O3"/>
<pin name="O4"/>
<pin name="O5"/>
<pin name="O6"/>
<pin name="O7"/>
<pin name="O8"/>
<pin name="O9"/>
<pin name="O10"/>
<pin name="O11"/>
<pin name="NC@16" direction="nc"/>
<pin name="ISET"/>
<pin name="!CS" direction="in"/>
<pin name="DOUT" direction="out"/>
<pin name="OSC" direction="in"/>
<pin name="BLINK" direction="out"/>
<pin name="DIN" direction="in"/>
<pin name="CLK" direction="in"/>
<pin name="NC@25" direction="nc"/>
<pin name="O12"/>
<pin name="O13"/>
<pin name="O14"/>
<pin name="O15"/>
<pin name="O16"/>
<pin name="O17"/>
<pin name="O18"/>
<pin name="P0"/>
<pin name="P1"/>
<pin name="V+@24" direction="pwr"/>
<pin name="V+@23" direction="pwr"/>
<pin name="V+@21" direction="pwr"/>
<pin name="P2"/>
<pin name="P3"/>
<pin name="P4"/>
<pin name="OSC_OUT" direction="out"/>
</symbol>
<symbol name="MAX6954-TQFN">
<pin name="O0"/>
<pin name="O1"/>
<pin name="O2"/>
<pin name="GND@12" direction="pwr"/>
<pin name="GND@13" direction="pwr"/>
<pin name="GND@15" direction="pwr"/>
<pin name="O3"/>
<pin name="O4"/>
<pin name="O5"/>
<pin name="O6"/>
<pin name="O7"/>
<pin name="O8"/>
<pin name="O9"/>
<pin name="O10"/>
<pin name="O11"/>
<pin name="NC@11" direction="nc"/>
<pin name="ISET"/>
<pin name="!CS" direction="in"/>
<pin name="DOUT" direction="out"/>
<pin name="OSC" direction="in"/>
<pin name="BLINK" direction="out"/>
<pin name="DIN" direction="in"/>
<pin name="CLK" direction="in"/>
<pin name="NC@20" direction="nc"/>
<pin name="O12"/>
<pin name="O13"/>
<pin name="O14"/>
<pin name="O15"/>
<pin name="O16"/>
<pin name="O17"/>
<pin name="O18"/>
<pin name="P0"/>
<pin name="P1"/>
<pin name="V+@19" direction="pwr"/>
<pin name="V+@18" direction="pwr"/>
<pin name="V+@16" direction="pwr"/>
<pin name="P2"/>
<pin name="P3"/>
<pin name="P4"/>
<pin name="OSC_OUT" direction="out"/>
</symbol>
<symbol name="MAX6955-SSOP36">
<pin name="O0"/>
<pin name="O1"/>
<pin name="O2"/>
<pin name="GND@16" direction="pwr"/>
<pin name="GND@18" direction="pwr"/>
<pin name="O3"/>
<pin name="O4"/>
<pin name="O5"/>
<pin name="O6"/>
<pin name="O7"/>
<pin name="O8"/>
<pin name="O9"/>
<pin name="O10"/>
<pin name="O11"/>
<pin name="ISET"/>
<pin name="AD1" direction="in"/>
<pin name="SDA"/>
<pin name="OSC" direction="in"/>
<pin name="BLINK" direction="out"/>
<pin name="AD0" direction="in"/>
<pin name="SCL" direction="in"/>
<pin name="O12"/>
<pin name="O13"/>
<pin name="O14"/>
<pin name="O15"/>
<pin name="O16"/>
<pin name="O17"/>
<pin name="O18"/>
<pin name="P0"/>
<pin name="P1"/>
<pin name="V+@21" direction="pwr"/>
<pin name="V+@19" direction="pwr"/>
<pin name="P2"/>
<pin name="P3"/>
<pin name="P4"/>
<pin name="OSC_OUT" direction="out"/>
</symbol>
<symbol name="MAX6955-TQFN">
<pin name="O0"/>
<pin name="O1"/>
<pin name="O2"/>
<pin name="GND@12" direction="pwr"/>
<pin name="GND@13" direction="pwr"/>
<pin name="GND@15" direction="pwr"/>
<pin name="O3"/>
<pin name="O4"/>
<pin name="O5"/>
<pin name="O6"/>
<pin name="O7"/>
<pin name="O8"/>
<pin name="O9"/>
<pin name="O10"/>
<pin name="O11"/>
<pin name="NC@11" direction="nc"/>
<pin name="ISET"/>
<pin name="SDA"/>
<pin name="AD1" direction="in"/>
<pin name="OSC" direction="in"/>
<pin name="BLINK" direction="out"/>
<pin name="AD0" direction="in"/>
<pin name="SCL" direction="in"/>
<pin name="NC@20" direction="nc"/>
<pin name="O12"/>
<pin name="O13"/>
<pin name="O14"/>
<pin name="O15"/>
<pin name="O16"/>
<pin name="O17"/>
<pin name="O18"/>
<pin name="P0"/>
<pin name="P1"/>
<pin name="V+@19" direction="pwr"/>
<pin name="V+@18" direction="pwr"/>
<pin name="V+@16" direction="pwr"/>
<pin name="P2"/>
<pin name="P3"/>
<pin name="P4"/>
<pin name="OSC_OUT" direction="out"/>
</symbol>
<symbol name="MAX6956-DIL28">
<pin name="P12"/>
<pin name="P13"/>
<pin name="P14"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
<pin name="P15"/>
<pin name="P16"/>
<pin name="P17"/>
<pin name="P18"/>
<pin name="P19"/>
<pin name="P20"/>
<pin name="P21"/>
<pin name="P22"/>
<pin name="P23"/>
<pin name="ISET"/>
<pin name="AD1" direction="in"/>
<pin name="AD0" direction="in"/>
<pin name="SDA"/>
<pin name="SCL" direction="in"/>
<pin name="P24"/>
<pin name="P25"/>
<pin name="P26"/>
<pin name="P27"/>
<pin name="P28"/>
<pin name="P29"/>
<pin name="P30"/>
<pin name="P31"/>
<pin name="V+@28" direction="pwr"/>
</symbol>
<symbol name="MAX6956-SSOP28">
<pin name="P12"/>
<pin name="P13"/>
<pin name="P14"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
<pin name="P15"/>
<pin name="P16"/>
<pin name="P17"/>
<pin name="P18"/>
<pin name="P19"/>
<pin name="P20"/>
<pin name="P21"/>
<pin name="P22"/>
<pin name="P23"/>
<pin name="ISET"/>
<pin name="AD1" direction="in"/>
<pin name="AD0" direction="in"/>
<pin name="SDA"/>
<pin name="SCL" direction="in"/>
<pin name="P24"/>
<pin name="P25"/>
<pin name="P26"/>
<pin name="P27"/>
<pin name="P28"/>
<pin name="P29"/>
<pin name="P30"/>
<pin name="P31"/>
<pin name="V+@28" direction="pwr"/>
</symbol>
<symbol name="MAX6956-SSOP36">
<pin name="P12"/>
<pin name="P13"/>
<pin name="P14"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
<pin name="P15"/>
<pin name="P16"/>
<pin name="P17"/>
<pin name="P18"/>
<pin name="P19"/>
<pin name="P20"/>
<pin name="P21"/>
<pin name="P22"/>
<pin name="P23"/>
<pin name="ISET"/>
<pin name="AD1" direction="in"/>
<pin name="AD0" direction="in"/>
<pin name="SDA"/>
<pin name="SCL" direction="in"/>
<pin name="P24"/>
<pin name="P25"/>
<pin name="P26"/>
<pin name="P27"/>
<pin name="P28"/>
<pin name="P29"/>
<pin name="P30"/>
<pin name="P31"/>
<pin name="V+@36" direction="pwr"/>
<pin name="P4"/>
<pin name="P5"/>
<pin name="P6"/>
<pin name="P7"/>
<pin name="P8"/>
<pin name="P9"/>
<pin name="P10"/>
<pin name="P11"/>
</symbol>
<symbol name="MAX6956-TQFN">
<pin name="P12"/>
<pin name="P13"/>
<pin name="P14"/>
<pin name="GND@38" direction="pwr"/>
<pin name="GND@39" direction="pwr"/>
<pin name="P15"/>
<pin name="P16"/>
<pin name="P17"/>
<pin name="P18"/>
<pin name="P19"/>
<pin name="P20"/>
<pin name="P21"/>
<pin name="P22"/>
<pin name="P23"/>
<pin name="ISET"/>
<pin name="AD1" direction="in"/>
<pin name="AD0" direction="in"/>
<pin name="SDA"/>
<pin name="SCL" direction="in"/>
<pin name="P24"/>
<pin name="P25"/>
<pin name="P26"/>
<pin name="P27"/>
<pin name="P28"/>
<pin name="P29"/>
<pin name="P30"/>
<pin name="P31"/>
<pin name="V+@35" direction="pwr"/>
<pin name="P4"/>
<pin name="P5"/>
<pin name="P6"/>
<pin name="P7"/>
<pin name="P8"/>
<pin name="P9"/>
<pin name="P10"/>
<pin name="P11"/>
<pin name="GND@37" direction="pwr"/>
<pin name="NC@11" direction="nc"/>
<pin name="NC@20" direction="nc"/>
<pin name="NC@31" direction="nc"/>
</symbol>
<symbol name="MAX6957-DIL28">
<pin name="P12"/>
<pin name="P13"/>
<pin name="P14"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
<pin name="P15"/>
<pin name="P16"/>
<pin name="P17"/>
<pin name="P18"/>
<pin name="P19"/>
<pin name="P20"/>
<pin name="P21"/>
<pin name="P22"/>
<pin name="P23"/>
<pin name="ISET"/>
<pin name="DIN" direction="in"/>
<pin name="SCLK" direction="in"/>
<pin name="!CS" direction="in"/>
<pin name="DOUT" direction="out"/>
<pin name="P24"/>
<pin name="P25"/>
<pin name="P26"/>
<pin name="P27"/>
<pin name="P28"/>
<pin name="P29"/>
<pin name="P30"/>
<pin name="P31"/>
<pin name="V+@28" direction="pwr"/>
</symbol>
<symbol name="MAX6957-SSOP28">
<pin name="P12"/>
<pin name="P13"/>
<pin name="P14"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
<pin name="P15"/>
<pin name="P16"/>
<pin name="P17"/>
<pin name="P18"/>
<pin name="P19"/>
<pin name="P20"/>
<pin name="P21"/>
<pin name="P22"/>
<pin name="P23"/>
<pin name="ISET"/>
<pin name="DIN" direction="in"/>
<pin name="SCLK" direction="in"/>
<pin name="!CS" direction="in"/>
<pin name="DOUT" direction="out"/>
<pin name="P24"/>
<pin name="P25"/>
<pin name="P26"/>
<pin name="P27"/>
<pin name="P28"/>
<pin name="P29"/>
<pin name="P30"/>
<pin name="P31"/>
<pin name="V+@28" direction="pwr"/>
</symbol>
<symbol name="MAX6957-SSOP36">
<pin name="P12"/>
<pin name="P13"/>
<pin name="P14"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
<pin name="P15"/>
<pin name="P16"/>
<pin name="P17"/>
<pin name="P18"/>
<pin name="P19"/>
<pin name="P20"/>
<pin name="P21"/>
<pin name="P22"/>
<pin name="P23"/>
<pin name="ISET"/>
<pin name="DIN" direction="in"/>
<pin name="SCLK" direction="in"/>
<pin name="!CS"/>
<pin name="DOUT" direction="out"/>
<pin name="P24"/>
<pin name="P25"/>
<pin name="P26"/>
<pin name="P27"/>
<pin name="P28"/>
<pin name="P29"/>
<pin name="P30"/>
<pin name="P31"/>
<pin name="V+@36" direction="pwr"/>
<pin name="P4"/>
<pin name="P5"/>
<pin name="P6"/>
<pin name="P7"/>
<pin name="P8"/>
<pin name="P9"/>
<pin name="P10"/>
<pin name="P11"/>
</symbol>
<symbol name="MAX6957-TQFN">
<pin name="P12"/>
<pin name="P13"/>
<pin name="P14"/>
<pin name="GND@38" direction="pwr"/>
<pin name="GND@39" direction="pwr"/>
<pin name="P15"/>
<pin name="P16"/>
<pin name="P17"/>
<pin name="P18"/>
<pin name="P19"/>
<pin name="P20"/>
<pin name="P21"/>
<pin name="P22"/>
<pin name="P23"/>
<pin name="ISET"/>
<pin name="DIN" direction="in"/>
<pin name="SCLK" direction="in"/>
<pin name="!CS"/>
<pin name="DOUT" direction="in"/>
<pin name="P24"/>
<pin name="P25"/>
<pin name="P26"/>
<pin name="P27"/>
<pin name="P28"/>
<pin name="P29"/>
<pin name="P30"/>
<pin name="P31"/>
<pin name="V+@35" direction="pwr"/>
<pin name="P4"/>
<pin name="P5"/>
<pin name="P6"/>
<pin name="P7"/>
<pin name="P8"/>
<pin name="P9"/>
<pin name="P10"/>
<pin name="P11"/>
<pin name="GND@37" direction="pwr"/>
<pin name="NC@11" direction="nc"/>
<pin name="NC@20" direction="nc"/>
<pin name="NC@31" direction="nc"/>
</symbol>
<symbol name="MAX6958-59-QSOP16">
<pin name="SDA"/>
<pin name="SCL" direction="in"/>
<pin name="INPUT1" direction="in"/>
<pin name="INPUT2" direction="in"/>
<pin name="V+@16" direction="pwr"/>
<pin name="GND@8" direction="pwr"/>
<pin name="SEG9"/>
<pin name="SEG8"/>
<pin name="SEG7"/>
<pin name="SEG6"/>
<pin name="SEG5"/>
<pin name="SEG4"/>
<pin name="DIG3/SEG3"/>
<pin name="DIG2/SEG2"/>
<pin name="DIG1/SEG1"/>
<pin name="DIG0/SEG0"/>
</symbol>
<symbol name="MAX6958-59-DIL16">
<pin name="SDA"/>
<pin name="SCL" direction="in"/>
<pin name="INPUT1" direction="in"/>
<pin name="INPUT2" direction="in"/>
<pin name="V+@16" direction="pwr"/>
<pin name="GND@8" direction="pwr"/>
<pin name="SEG9"/>
<pin name="SEG8"/>
<pin name="SEG7"/>
<pin name="SEG6"/>
<pin name="SEG5"/>
<pin name="SEG4"/>
<pin name="DIG3/SEG3"/>
<pin name="DIG2/SEG2"/>
<pin name="DIG1/SEG1"/>
<pin name="DIG0/SEG0"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="MAX6953EPL" prefix="U">
<description>&lt;b&gt;MAX6953&lt;/b&gt; - 2-Wire Interfaced, 2.7V to 5.5V, 4-Digit 5 x 7 Matrix LED Display Driver&lt;br&gt;
&lt;p&gt;
Supporting Materials:
&lt;a href=https://datasheets.maximintegrated.com/en/ds/MAX6953.pdf&gt;Datasheet&lt;/a&gt;
&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="MAX6953-DIL40"/>
</gates>
<devices>
<device name="" package="DIL40">
<connects>
<connect gate="G$1" pin="AD0" pad="22"/>
<connect gate="G$1" pin="AD1" pad="18"/>
<connect gate="G$1" pin="BLINK" pad="20"/>
<connect gate="G$1" pin="GND@19" pad="19"/>
<connect gate="G$1" pin="GND@4" pad="4"/>
<connect gate="G$1" pin="GND@5" pad="5"/>
<connect gate="G$1" pin="GND@6" pad="6"/>
<connect gate="G$1" pin="ISET" pad="17"/>
<connect gate="G$1" pin="NC@16" pad="16"/>
<connect gate="G$1" pin="NC@25" pad="25"/>
<connect gate="G$1" pin="O0" pad="1"/>
<connect gate="G$1" pin="O1" pad="2"/>
<connect gate="G$1" pin="O10" pad="14"/>
<connect gate="G$1" pin="O11" pad="15"/>
<connect gate="G$1" pin="O12" pad="26"/>
<connect gate="G$1" pin="O13" pad="27"/>
<connect gate="G$1" pin="O14" pad="28"/>
<connect gate="G$1" pin="O15" pad="29"/>
<connect gate="G$1" pin="O16" pad="30"/>
<connect gate="G$1" pin="O17" pad="31"/>
<connect gate="G$1" pin="O18" pad="32"/>
<connect gate="G$1" pin="O19" pad="33"/>
<connect gate="G$1" pin="O2" pad="3"/>
<connect gate="G$1" pin="O20" pad="34"/>
<connect gate="G$1" pin="O21" pad="38"/>
<connect gate="G$1" pin="O22" pad="39"/>
<connect gate="G$1" pin="O23" pad="40"/>
<connect gate="G$1" pin="O3" pad="7"/>
<connect gate="G$1" pin="O4" pad="8"/>
<connect gate="G$1" pin="O5" pad="9"/>
<connect gate="G$1" pin="O6" pad="10"/>
<connect gate="G$1" pin="O7" pad="11"/>
<connect gate="G$1" pin="O8" pad="12"/>
<connect gate="G$1" pin="O9" pad="13"/>
<connect gate="G$1" pin="OSC" pad="21"/>
<connect gate="G$1" pin="SCL" pad="24"/>
<connect gate="G$1" pin="SDA" pad="23"/>
<connect gate="G$1" pin="V+@35" pad="35"/>
<connect gate="G$1" pin="V+@36" pad="36"/>
<connect gate="G$1" pin="V+@37" pad="37"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX6952EPL" prefix="U">
<description>&lt;b&gt;MAX6952&lt;/b&gt; - 4-Wire Interfaced, 2.7V to 5.5V, 4-Digit 5 x 7 Matrix LED Display Driver&lt;br&gt;
&lt;p&gt;
Supporting Materials:
&lt;a href=https://datasheets.maximintegrated.com/en/ds/MAX6952.pdf&gt;Datasheet&lt;/a&gt;
&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="MAX6952-DIL40"/>
</gates>
<devices>
<device name="" package="DIL40">
<connects>
<connect gate="G$1" pin="!CS" pad="23"/>
<connect gate="G$1" pin="BLINK" pad="19"/>
<connect gate="G$1" pin="CLK" pad="21"/>
<connect gate="G$1" pin="DIN" pad="20"/>
<connect gate="G$1" pin="DOUT" pad="22"/>
<connect gate="G$1" pin="GND@18" pad="18"/>
<connect gate="G$1" pin="GND@4" pad="4"/>
<connect gate="G$1" pin="GND@5" pad="5"/>
<connect gate="G$1" pin="GND@6" pad="6"/>
<connect gate="G$1" pin="ISET" pad="17"/>
<connect gate="G$1" pin="NC@16" pad="16"/>
<connect gate="G$1" pin="NC@25" pad="25"/>
<connect gate="G$1" pin="O0" pad="1"/>
<connect gate="G$1" pin="O1" pad="2"/>
<connect gate="G$1" pin="O10" pad="14"/>
<connect gate="G$1" pin="O11" pad="15"/>
<connect gate="G$1" pin="O12" pad="26"/>
<connect gate="G$1" pin="O13" pad="27"/>
<connect gate="G$1" pin="O14" pad="28"/>
<connect gate="G$1" pin="O15" pad="29"/>
<connect gate="G$1" pin="O16" pad="30"/>
<connect gate="G$1" pin="O17" pad="31"/>
<connect gate="G$1" pin="O18" pad="32"/>
<connect gate="G$1" pin="O19" pad="33"/>
<connect gate="G$1" pin="O2" pad="3"/>
<connect gate="G$1" pin="O20" pad="34"/>
<connect gate="G$1" pin="O21" pad="38"/>
<connect gate="G$1" pin="O22" pad="39"/>
<connect gate="G$1" pin="O23" pad="40"/>
<connect gate="G$1" pin="O3" pad="7"/>
<connect gate="G$1" pin="O4" pad="8"/>
<connect gate="G$1" pin="O5" pad="9"/>
<connect gate="G$1" pin="O6" pad="10"/>
<connect gate="G$1" pin="O7" pad="11"/>
<connect gate="G$1" pin="O8" pad="12"/>
<connect gate="G$1" pin="O9" pad="13"/>
<connect gate="G$1" pin="OSC" pad="24"/>
<connect gate="G$1" pin="V+@35" pad="35"/>
<connect gate="G$1" pin="V+@36" pad="36"/>
<connect gate="G$1" pin="V+@37" pad="37"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX6952EAX" prefix="U">
<description>&lt;b&gt;MAX6952&lt;/b&gt; - 4-Wire Interfaced, 2.7V to 5.5V, 4-Digit 5 x 7 Matrix LED Display Driver&lt;br&gt;
&lt;p&gt;
Supporting Materials:
&lt;a href=https://datasheets.maximintegrated.com/en/ds/MAX6952.pdf&gt;Datasheet&lt;/a&gt;
&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="MAX6952-SSOP36"/>
</gates>
<devices>
<device name="" package="SSOP36">
<connects>
<connect gate="G$1" pin="!CS" pad="21"/>
<connect gate="G$1" pin="BLINK" pad="17"/>
<connect gate="G$1" pin="CLK" pad="19"/>
<connect gate="G$1" pin="DIN" pad="18"/>
<connect gate="G$1" pin="DOUT" pad="20"/>
<connect gate="G$1" pin="GND@16" pad="16"/>
<connect gate="G$1" pin="GND@4" pad="4"/>
<connect gate="G$1" pin="GND@5" pad="5"/>
<connect gate="G$1" pin="ISET" pad="15"/>
<connect gate="G$1" pin="O0" pad="1"/>
<connect gate="G$1" pin="O1" pad="2"/>
<connect gate="G$1" pin="O10" pad="13"/>
<connect gate="G$1" pin="O11" pad="14"/>
<connect gate="G$1" pin="O12" pad="23"/>
<connect gate="G$1" pin="O13" pad="24"/>
<connect gate="G$1" pin="O14" pad="25"/>
<connect gate="G$1" pin="O15" pad="26"/>
<connect gate="G$1" pin="O16" pad="27"/>
<connect gate="G$1" pin="O17" pad="28"/>
<connect gate="G$1" pin="O18" pad="29"/>
<connect gate="G$1" pin="O19" pad="30"/>
<connect gate="G$1" pin="O2" pad="3"/>
<connect gate="G$1" pin="O20" pad="31"/>
<connect gate="G$1" pin="O21" pad="34"/>
<connect gate="G$1" pin="O22" pad="35"/>
<connect gate="G$1" pin="O23" pad="36"/>
<connect gate="G$1" pin="O3" pad="6"/>
<connect gate="G$1" pin="O4" pad="7"/>
<connect gate="G$1" pin="O5" pad="8"/>
<connect gate="G$1" pin="O6" pad="9"/>
<connect gate="G$1" pin="O7" pad="10"/>
<connect gate="G$1" pin="O8" pad="11"/>
<connect gate="G$1" pin="O9" pad="12"/>
<connect gate="G$1" pin="OSC" pad="22"/>
<connect gate="G$1" pin="V+@32" pad="32"/>
<connect gate="G$1" pin="V+@33" pad="33"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX6953EAX" prefix="U">
<description>&lt;b&gt;MAX6953&lt;/b&gt; - 2-Wire Interfaced, 2.7V to 5.5V, 4-Digit 5 x 7 Matrix LED Display Driver&lt;br&gt;
&lt;p&gt;
Supporting Materials:
&lt;a href=https://datasheets.maximintegrated.com/en/ds/MAX6953.pdf&gt;Datasheet&lt;/a&gt;
&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="MAX6953-SSOP36"/>
</gates>
<devices>
<device name="" package="SSOP36">
<connects>
<connect gate="G$1" pin="AD0" pad="20"/>
<connect gate="G$1" pin="AD1" pad="16"/>
<connect gate="G$1" pin="BLINK" pad="18"/>
<connect gate="G$1" pin="GND@17" pad="17"/>
<connect gate="G$1" pin="GND@4" pad="4"/>
<connect gate="G$1" pin="GND@5" pad="5"/>
<connect gate="G$1" pin="ISET" pad="15"/>
<connect gate="G$1" pin="O0" pad="1"/>
<connect gate="G$1" pin="O1" pad="2"/>
<connect gate="G$1" pin="O10" pad="13"/>
<connect gate="G$1" pin="O11" pad="14"/>
<connect gate="G$1" pin="O12" pad="23"/>
<connect gate="G$1" pin="O13" pad="24"/>
<connect gate="G$1" pin="O14" pad="25"/>
<connect gate="G$1" pin="O15" pad="26"/>
<connect gate="G$1" pin="O16" pad="27"/>
<connect gate="G$1" pin="O17" pad="28"/>
<connect gate="G$1" pin="O18" pad="29"/>
<connect gate="G$1" pin="O19" pad="30"/>
<connect gate="G$1" pin="O2" pad="3"/>
<connect gate="G$1" pin="O20" pad="31"/>
<connect gate="G$1" pin="O21" pad="34"/>
<connect gate="G$1" pin="O22" pad="35"/>
<connect gate="G$1" pin="O23" pad="36"/>
<connect gate="G$1" pin="O3" pad="6"/>
<connect gate="G$1" pin="O4" pad="7"/>
<connect gate="G$1" pin="O5" pad="8"/>
<connect gate="G$1" pin="O6" pad="9"/>
<connect gate="G$1" pin="O7" pad="10"/>
<connect gate="G$1" pin="O8" pad="11"/>
<connect gate="G$1" pin="O9" pad="12"/>
<connect gate="G$1" pin="OSC" pad="19"/>
<connect gate="G$1" pin="SCL" pad="22"/>
<connect gate="G$1" pin="SDA" pad="21"/>
<connect gate="G$1" pin="V+@32" pad="32"/>
<connect gate="G$1" pin="V+@33" pad="33"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX6954APL" prefix="U">
<description>&lt;b&gt;MAX6954&lt;/b&gt; - 4-Wire Interfaced, 2.7V to 5.5V LED Display Driver with I/O Expander and Key Scan&lt;br&gt;
&lt;p&gt;
Supporting Materials:
&lt;a href=https://datasheets.maximintegrated.com/en/ds/MAX6954.pdf&gt;Datasheet&lt;/a&gt;
&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="MAX6954-DIL40"/>
</gates>
<devices>
<device name="" package="DIL40">
<connects>
<connect gate="G$1" pin="!CS" pad="3"/>
<connect gate="G$1" pin="BLINK" pad="36"/>
<connect gate="G$1" pin="CLK" pad="5"/>
<connect gate="G$1" pin="DIN" pad="6"/>
<connect gate="G$1" pin="DOUT" pad="4"/>
<connect gate="G$1" pin="GND@17" pad="17"/>
<connect gate="G$1" pin="GND@18" pad="18"/>
<connect gate="G$1" pin="GND@20" pad="20"/>
<connect gate="G$1" pin="ISET" pad="19"/>
<connect gate="G$1" pin="NC@16" pad="16"/>
<connect gate="G$1" pin="NC@25" pad="25"/>
<connect gate="G$1" pin="O0" pad="7"/>
<connect gate="G$1" pin="O1" pad="8"/>
<connect gate="G$1" pin="O10" pad="27"/>
<connect gate="G$1" pin="O11" pad="28"/>
<connect gate="G$1" pin="O12" pad="29"/>
<connect gate="G$1" pin="O13" pad="30"/>
<connect gate="G$1" pin="O14" pad="31"/>
<connect gate="G$1" pin="O15" pad="32"/>
<connect gate="G$1" pin="O16" pad="33"/>
<connect gate="G$1" pin="O17" pad="34"/>
<connect gate="G$1" pin="O18" pad="35"/>
<connect gate="G$1" pin="O2" pad="9"/>
<connect gate="G$1" pin="O3" pad="10"/>
<connect gate="G$1" pin="O4" pad="11"/>
<connect gate="G$1" pin="O5" pad="12"/>
<connect gate="G$1" pin="O6" pad="13"/>
<connect gate="G$1" pin="O7" pad="14"/>
<connect gate="G$1" pin="O8" pad="15"/>
<connect gate="G$1" pin="O9" pad="26"/>
<connect gate="G$1" pin="OSC" pad="22"/>
<connect gate="G$1" pin="OSC_OUT" pad="37"/>
<connect gate="G$1" pin="P0" pad="1"/>
<connect gate="G$1" pin="P1" pad="2"/>
<connect gate="G$1" pin="P2" pad="38"/>
<connect gate="G$1" pin="P3" pad="39"/>
<connect gate="G$1" pin="P4" pad="40"/>
<connect gate="G$1" pin="V+@21" pad="21"/>
<connect gate="G$1" pin="V+@23" pad="23"/>
<connect gate="G$1" pin="V+@24" pad="24"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX6954AAX" prefix="U">
<description>&lt;b&gt;MAX6954&lt;/b&gt; - 4-Wire Interfaced, 2.7V to 5.5V LED Display Driver with I/O Expander and Key Scan&lt;br&gt;
&lt;p&gt;
Supporting Materials:
&lt;a href=https://datasheets.maximintegrated.com/en/ds/MAX6954.pdf&gt;Datasheet&lt;/a&gt;
&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="MAX6954-SSOP36"/>
</gates>
<devices>
<device name="" package="SSOP36">
<connects>
<connect gate="G$1" pin="!CS" pad="3"/>
<connect gate="G$1" pin="BLINK" pad="32"/>
<connect gate="G$1" pin="CLK" pad="5"/>
<connect gate="G$1" pin="DIN" pad="6"/>
<connect gate="G$1" pin="DOUT" pad="4"/>
<connect gate="G$1" pin="GND@16" pad="16"/>
<connect gate="G$1" pin="GND@18" pad="18"/>
<connect gate="G$1" pin="ISET" pad="17"/>
<connect gate="G$1" pin="O0" pad="7"/>
<connect gate="G$1" pin="O1" pad="8"/>
<connect gate="G$1" pin="O10" pad="23"/>
<connect gate="G$1" pin="O11" pad="24"/>
<connect gate="G$1" pin="O12" pad="25"/>
<connect gate="G$1" pin="O13" pad="26"/>
<connect gate="G$1" pin="O14" pad="27"/>
<connect gate="G$1" pin="O15" pad="28"/>
<connect gate="G$1" pin="O16" pad="29"/>
<connect gate="G$1" pin="O17" pad="30"/>
<connect gate="G$1" pin="O18" pad="31"/>
<connect gate="G$1" pin="O2" pad="9"/>
<connect gate="G$1" pin="O3" pad="10"/>
<connect gate="G$1" pin="O4" pad="11"/>
<connect gate="G$1" pin="O5" pad="12"/>
<connect gate="G$1" pin="O6" pad="13"/>
<connect gate="G$1" pin="O7" pad="14"/>
<connect gate="G$1" pin="O8" pad="15"/>
<connect gate="G$1" pin="O9" pad="22"/>
<connect gate="G$1" pin="OSC" pad="20"/>
<connect gate="G$1" pin="OSC_OUT" pad="33"/>
<connect gate="G$1" pin="P0" pad="1"/>
<connect gate="G$1" pin="P1" pad="2"/>
<connect gate="G$1" pin="P2" pad="34"/>
<connect gate="G$1" pin="P3" pad="35"/>
<connect gate="G$1" pin="P4" pad="36"/>
<connect gate="G$1" pin="V+@19" pad="19"/>
<connect gate="G$1" pin="V+@21" pad="21"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX6954ATL">
<description>&lt;b&gt;MAX6954&lt;/b&gt; - 4-Wire Interfaced, 2.7V to 5.5V LED Display Driver with I/O Expander and Key Scan&lt;br&gt;
&lt;p&gt;
Supporting Materials:
&lt;a href=https://datasheets.maximintegrated.com/en/ds/MAX6954.pdf&gt;Datasheet&lt;/a&gt;
&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="MAX6954-TQFN"/>
</gates>
<devices>
<device name="" package="TQFN40-EP">
<connects>
<connect gate="G$1" pin="!CS" pad="38"/>
<connect gate="G$1" pin="BLINK" pad="31"/>
<connect gate="G$1" pin="CLK" pad="40"/>
<connect gate="G$1" pin="DIN" pad="1"/>
<connect gate="G$1" pin="DOUT" pad="39"/>
<connect gate="G$1" pin="GND@12" pad="12"/>
<connect gate="G$1" pin="GND@13" pad="13"/>
<connect gate="G$1" pin="GND@15" pad="15"/>
<connect gate="G$1" pin="ISET" pad="14"/>
<connect gate="G$1" pin="NC@11" pad="11"/>
<connect gate="G$1" pin="NC@20" pad="20"/>
<connect gate="G$1" pin="O0" pad="2"/>
<connect gate="G$1" pin="O1" pad="3"/>
<connect gate="G$1" pin="O10" pad="22"/>
<connect gate="G$1" pin="O11" pad="23"/>
<connect gate="G$1" pin="O12" pad="24"/>
<connect gate="G$1" pin="O13" pad="25"/>
<connect gate="G$1" pin="O14" pad="26"/>
<connect gate="G$1" pin="O15" pad="27"/>
<connect gate="G$1" pin="O16" pad="28"/>
<connect gate="G$1" pin="O17" pad="29"/>
<connect gate="G$1" pin="O18" pad="30"/>
<connect gate="G$1" pin="O2" pad="4"/>
<connect gate="G$1" pin="O3" pad="5"/>
<connect gate="G$1" pin="O4" pad="6"/>
<connect gate="G$1" pin="O5" pad="7"/>
<connect gate="G$1" pin="O6" pad="8"/>
<connect gate="G$1" pin="O7" pad="9"/>
<connect gate="G$1" pin="O8" pad="10"/>
<connect gate="G$1" pin="O9" pad="21"/>
<connect gate="G$1" pin="OSC" pad="17"/>
<connect gate="G$1" pin="OSC_OUT" pad="32"/>
<connect gate="G$1" pin="P0" pad="36"/>
<connect gate="G$1" pin="P1" pad="37"/>
<connect gate="G$1" pin="P2" pad="33"/>
<connect gate="G$1" pin="P3" pad="34"/>
<connect gate="G$1" pin="P4" pad="35"/>
<connect gate="G$1" pin="V+@16" pad="16"/>
<connect gate="G$1" pin="V+@18" pad="18"/>
<connect gate="G$1" pin="V+@19" pad="19"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX6955AAX" prefix="U">
<description>&lt;b&gt;MAX6955&lt;/b&gt; - 2-Wire Interfaced, 2.7V to 5.5V LED Display Driver with I/O Expander and Key Scan&lt;br&gt;
&lt;p&gt;
Supporting Materials:
&lt;a href=https://datasheets.maximintegrated.com/en/ds/MAX6955.pdf&gt;Datasheet&lt;/a&gt;
&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="MAX6955-SSOP36"/>
</gates>
<devices>
<device name="" package="SSOP36">
<connects>
<connect gate="G$1" pin="AD0" pad="3"/>
<connect gate="G$1" pin="AD1" pad="6"/>
<connect gate="G$1" pin="BLINK" pad="32"/>
<connect gate="G$1" pin="GND@16" pad="16"/>
<connect gate="G$1" pin="GND@18" pad="18"/>
<connect gate="G$1" pin="ISET" pad="17"/>
<connect gate="G$1" pin="O0" pad="7"/>
<connect gate="G$1" pin="O1" pad="8"/>
<connect gate="G$1" pin="O10" pad="23"/>
<connect gate="G$1" pin="O11" pad="24"/>
<connect gate="G$1" pin="O12" pad="25"/>
<connect gate="G$1" pin="O13" pad="26"/>
<connect gate="G$1" pin="O14" pad="27"/>
<connect gate="G$1" pin="O15" pad="28"/>
<connect gate="G$1" pin="O16" pad="29"/>
<connect gate="G$1" pin="O17" pad="30"/>
<connect gate="G$1" pin="O18" pad="31"/>
<connect gate="G$1" pin="O2" pad="9"/>
<connect gate="G$1" pin="O3" pad="10"/>
<connect gate="G$1" pin="O4" pad="11"/>
<connect gate="G$1" pin="O5" pad="12"/>
<connect gate="G$1" pin="O6" pad="13"/>
<connect gate="G$1" pin="O7" pad="14"/>
<connect gate="G$1" pin="O8" pad="15"/>
<connect gate="G$1" pin="O9" pad="22"/>
<connect gate="G$1" pin="OSC" pad="20"/>
<connect gate="G$1" pin="OSC_OUT" pad="33"/>
<connect gate="G$1" pin="P0" pad="1"/>
<connect gate="G$1" pin="P1" pad="2"/>
<connect gate="G$1" pin="P2" pad="34"/>
<connect gate="G$1" pin="P3" pad="35"/>
<connect gate="G$1" pin="P4" pad="36"/>
<connect gate="G$1" pin="SCL" pad="5"/>
<connect gate="G$1" pin="SDA" pad="4"/>
<connect gate="G$1" pin="V+@19" pad="19"/>
<connect gate="G$1" pin="V+@21" pad="21"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX6955ATL" prefix="U">
<description>&lt;b&gt;MAX6955&lt;/b&gt; - 2-Wire Interfaced, 2.7V to 5.5V LED Display Driver with I/O Expander and Key Scan&lt;br&gt;
&lt;p&gt;
Supporting Materials:
&lt;a href=https://datasheets.maximintegrated.com/en/ds/MAX6955.pdf&gt;Datasheet&lt;/a&gt;
&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="MAX6955-TQFN"/>
</gates>
<devices>
<device name="" package="TQFN40-EP">
<connects>
<connect gate="G$1" pin="AD0" pad="38"/>
<connect gate="G$1" pin="AD1" pad="1"/>
<connect gate="G$1" pin="BLINK" pad="31"/>
<connect gate="G$1" pin="GND@12" pad="12"/>
<connect gate="G$1" pin="GND@13" pad="13"/>
<connect gate="G$1" pin="GND@15" pad="15"/>
<connect gate="G$1" pin="ISET" pad="14"/>
<connect gate="G$1" pin="NC@11" pad="11"/>
<connect gate="G$1" pin="NC@20" pad="20"/>
<connect gate="G$1" pin="O0" pad="2"/>
<connect gate="G$1" pin="O1" pad="3"/>
<connect gate="G$1" pin="O10" pad="22"/>
<connect gate="G$1" pin="O11" pad="23"/>
<connect gate="G$1" pin="O12" pad="24"/>
<connect gate="G$1" pin="O13" pad="25"/>
<connect gate="G$1" pin="O14" pad="26"/>
<connect gate="G$1" pin="O15" pad="27"/>
<connect gate="G$1" pin="O16" pad="28"/>
<connect gate="G$1" pin="O17" pad="29"/>
<connect gate="G$1" pin="O18" pad="30"/>
<connect gate="G$1" pin="O2" pad="4"/>
<connect gate="G$1" pin="O3" pad="5"/>
<connect gate="G$1" pin="O4" pad="6"/>
<connect gate="G$1" pin="O5" pad="7"/>
<connect gate="G$1" pin="O6" pad="8"/>
<connect gate="G$1" pin="O7" pad="9"/>
<connect gate="G$1" pin="O8" pad="10"/>
<connect gate="G$1" pin="O9" pad="21"/>
<connect gate="G$1" pin="OSC" pad="17"/>
<connect gate="G$1" pin="OSC_OUT" pad="32"/>
<connect gate="G$1" pin="P0" pad="36"/>
<connect gate="G$1" pin="P1" pad="37"/>
<connect gate="G$1" pin="P2" pad="33"/>
<connect gate="G$1" pin="P3" pad="34"/>
<connect gate="G$1" pin="P4" pad="35"/>
<connect gate="G$1" pin="SCL" pad="40"/>
<connect gate="G$1" pin="SDA" pad="39"/>
<connect gate="G$1" pin="V+@16" pad="16"/>
<connect gate="G$1" pin="V+@18" pad="18"/>
<connect gate="G$1" pin="V+@19" pad="19"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX6956ANI" prefix="U">
<description>&lt;b&gt;MAX6956&lt;/b&gt; - 2-Wire Interfaced, 2.7V to 5.5V, 20-Port or 28-Port LED Display Driver and I/O Expander&lt;br&gt;
&lt;p&gt;
Supporting Materials:
&lt;a href=https://datasheets.maximintegrated.com/en/ds/MAX6956.pdf&gt;Datasheet&lt;/a&gt;
&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="MAX6956-DIL28"/>
</gates>
<devices>
<device name="" package="DIL28-6">
<connects>
<connect gate="G$1" pin="AD0" pad="4"/>
<connect gate="G$1" pin="AD1" pad="27"/>
<connect gate="G$1" pin="GND@2" pad="2"/>
<connect gate="G$1" pin="GND@3" pad="3"/>
<connect gate="G$1" pin="ISET" pad="1"/>
<connect gate="G$1" pin="P12" pad="5"/>
<connect gate="G$1" pin="P13" pad="6"/>
<connect gate="G$1" pin="P14" pad="7"/>
<connect gate="G$1" pin="P15" pad="8"/>
<connect gate="G$1" pin="P16" pad="9"/>
<connect gate="G$1" pin="P17" pad="10"/>
<connect gate="G$1" pin="P18" pad="11"/>
<connect gate="G$1" pin="P19" pad="12"/>
<connect gate="G$1" pin="P20" pad="13"/>
<connect gate="G$1" pin="P21" pad="14"/>
<connect gate="G$1" pin="P22" pad="15"/>
<connect gate="G$1" pin="P23" pad="16"/>
<connect gate="G$1" pin="P24" pad="17"/>
<connect gate="G$1" pin="P25" pad="18"/>
<connect gate="G$1" pin="P26" pad="19"/>
<connect gate="G$1" pin="P27" pad="20"/>
<connect gate="G$1" pin="P28" pad="21"/>
<connect gate="G$1" pin="P29" pad="22"/>
<connect gate="G$1" pin="P30" pad="23"/>
<connect gate="G$1" pin="P31" pad="24"/>
<connect gate="G$1" pin="SCL" pad="26"/>
<connect gate="G$1" pin="SDA" pad="25"/>
<connect gate="G$1" pin="V+@28" pad="28"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX6956AAI" prefix="U">
<description>&lt;b&gt;MAX6956&lt;/b&gt; - 2-Wire Interfaced, 2.7V to 5.5V, 20-Port or 28-Port LED Display Driver and I/O Expander&lt;br&gt;
&lt;p&gt;
Supporting Materials:
&lt;a href=https://datasheets.maximintegrated.com/en/ds/MAX6956.pdf&gt;Datasheet&lt;/a&gt;
&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="MAX6956-SSOP28"/>
</gates>
<devices>
<device name="" package="SSOP28">
<connects>
<connect gate="G$1" pin="AD0" pad="4"/>
<connect gate="G$1" pin="AD1" pad="27"/>
<connect gate="G$1" pin="GND@2" pad="2"/>
<connect gate="G$1" pin="GND@3" pad="3"/>
<connect gate="G$1" pin="ISET" pad="1"/>
<connect gate="G$1" pin="P12" pad="5"/>
<connect gate="G$1" pin="P13" pad="6"/>
<connect gate="G$1" pin="P14" pad="7"/>
<connect gate="G$1" pin="P15" pad="8"/>
<connect gate="G$1" pin="P16" pad="9"/>
<connect gate="G$1" pin="P17" pad="10"/>
<connect gate="G$1" pin="P18" pad="11"/>
<connect gate="G$1" pin="P19" pad="12"/>
<connect gate="G$1" pin="P20" pad="13"/>
<connect gate="G$1" pin="P21" pad="14"/>
<connect gate="G$1" pin="P22" pad="15"/>
<connect gate="G$1" pin="P23" pad="16"/>
<connect gate="G$1" pin="P24" pad="17"/>
<connect gate="G$1" pin="P25" pad="18"/>
<connect gate="G$1" pin="P26" pad="19"/>
<connect gate="G$1" pin="P27" pad="20"/>
<connect gate="G$1" pin="P28" pad="21"/>
<connect gate="G$1" pin="P29" pad="22"/>
<connect gate="G$1" pin="P30" pad="23"/>
<connect gate="G$1" pin="P31" pad="24"/>
<connect gate="G$1" pin="SCL" pad="26"/>
<connect gate="G$1" pin="SDA" pad="25"/>
<connect gate="G$1" pin="V+@28" pad="28"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX6956AAX" prefix="U">
<description>&lt;b&gt;MAX6956&lt;/b&gt; - 2-Wire Interfaced, 2.7V to 5.5V, 20-Port or 28-Port LED Display Driver and I/O Expander&lt;br&gt;
&lt;p&gt;
Supporting Materials:
&lt;a href=https://datasheets.maximintegrated.com/en/ds/MAX6956.pdf&gt;Datasheet&lt;/a&gt;
&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="MAX6956-SSOP36"/>
</gates>
<devices>
<device name="" package="SSOP36">
<connects>
<connect gate="G$1" pin="AD0" pad="4"/>
<connect gate="G$1" pin="AD1" pad="35"/>
<connect gate="G$1" pin="GND@2" pad="2"/>
<connect gate="G$1" pin="GND@3" pad="3"/>
<connect gate="G$1" pin="ISET" pad="1"/>
<connect gate="G$1" pin="P10" pad="9"/>
<connect gate="G$1" pin="P11" pad="11"/>
<connect gate="G$1" pin="P12" pad="6"/>
<connect gate="G$1" pin="P13" pad="8"/>
<connect gate="G$1" pin="P14" pad="10"/>
<connect gate="G$1" pin="P15" pad="12"/>
<connect gate="G$1" pin="P16" pad="13"/>
<connect gate="G$1" pin="P17" pad="14"/>
<connect gate="G$1" pin="P18" pad="15"/>
<connect gate="G$1" pin="P19" pad="16"/>
<connect gate="G$1" pin="P20" pad="17"/>
<connect gate="G$1" pin="P21" pad="18"/>
<connect gate="G$1" pin="P22" pad="19"/>
<connect gate="G$1" pin="P23" pad="20"/>
<connect gate="G$1" pin="P24" pad="21"/>
<connect gate="G$1" pin="P25" pad="22"/>
<connect gate="G$1" pin="P26" pad="23"/>
<connect gate="G$1" pin="P27" pad="24"/>
<connect gate="G$1" pin="P28" pad="25"/>
<connect gate="G$1" pin="P29" pad="27"/>
<connect gate="G$1" pin="P30" pad="29"/>
<connect gate="G$1" pin="P31" pad="31"/>
<connect gate="G$1" pin="P4" pad="32"/>
<connect gate="G$1" pin="P5" pad="30"/>
<connect gate="G$1" pin="P6" pad="28"/>
<connect gate="G$1" pin="P7" pad="26"/>
<connect gate="G$1" pin="P8" pad="5"/>
<connect gate="G$1" pin="P9" pad="7"/>
<connect gate="G$1" pin="SCL" pad="34"/>
<connect gate="G$1" pin="SDA" pad="33"/>
<connect gate="G$1" pin="V+@36" pad="36"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX6956ATL" prefix="U">
<description>&lt;b&gt;MAX6956&lt;/b&gt; - 2-Wire Interfaced, 2.7V to 5.5V, 20-Port or 28-Port LED Display Driver and I/O Expander&lt;br&gt;
&lt;p&gt;
Supporting Materials:
&lt;a href=https://datasheets.maximintegrated.com/en/ds/MAX6956.pdf&gt;Datasheet&lt;/a&gt;
&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="MAX6956-TQFN"/>
</gates>
<devices>
<device name="" package="TQFN40-EP">
<connects>
<connect gate="G$1" pin="AD0" pad="40"/>
<connect gate="G$1" pin="AD1" pad="34"/>
<connect gate="G$1" pin="GND@37" pad="37"/>
<connect gate="G$1" pin="GND@38" pad="38"/>
<connect gate="G$1" pin="GND@39" pad="39"/>
<connect gate="G$1" pin="ISET" pad="36"/>
<connect gate="G$1" pin="NC@11" pad="11"/>
<connect gate="G$1" pin="NC@20" pad="20"/>
<connect gate="G$1" pin="NC@31" pad="31"/>
<connect gate="G$1" pin="P10" pad="5"/>
<connect gate="G$1" pin="P11" pad="7"/>
<connect gate="G$1" pin="P12" pad="2"/>
<connect gate="G$1" pin="P13" pad="4"/>
<connect gate="G$1" pin="P14" pad="6"/>
<connect gate="G$1" pin="P15" pad="8"/>
<connect gate="G$1" pin="P16" pad="9"/>
<connect gate="G$1" pin="P17" pad="10"/>
<connect gate="G$1" pin="P18" pad="12"/>
<connect gate="G$1" pin="P19" pad="13"/>
<connect gate="G$1" pin="P20" pad="14"/>
<connect gate="G$1" pin="P21" pad="15"/>
<connect gate="G$1" pin="P22" pad="16"/>
<connect gate="G$1" pin="P23" pad="17"/>
<connect gate="G$1" pin="P24" pad="18"/>
<connect gate="G$1" pin="P25" pad="19"/>
<connect gate="G$1" pin="P26" pad="21"/>
<connect gate="G$1" pin="P27" pad="22"/>
<connect gate="G$1" pin="P28" pad="23"/>
<connect gate="G$1" pin="P29" pad="25"/>
<connect gate="G$1" pin="P30" pad="27"/>
<connect gate="G$1" pin="P31" pad="29"/>
<connect gate="G$1" pin="P4" pad="30"/>
<connect gate="G$1" pin="P5" pad="28"/>
<connect gate="G$1" pin="P6" pad="26"/>
<connect gate="G$1" pin="P7" pad="24"/>
<connect gate="G$1" pin="P8" pad="1"/>
<connect gate="G$1" pin="P9" pad="3"/>
<connect gate="G$1" pin="SCL" pad="33"/>
<connect gate="G$1" pin="SDA" pad="32"/>
<connect gate="G$1" pin="V+@35" pad="35"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX6957ANI" prefix="U">
<description>&lt;b&gt;MAX6957&lt;/b&gt; - 4-Wire Interfaced, 2.7V to 5.5V, 20-Port and 28-Port LED Display Driver and I/O Expander&lt;br&gt;
&lt;p&gt;
Supporting Materials:
&lt;a href=https://datasheets.maximintegrated.com/en/ds/MAX6957.pdf&gt;Datasheet&lt;/a&gt;
&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="MAX6957-DIL28"/>
</gates>
<devices>
<device name="" package="DIL28-6">
<connects>
<connect gate="G$1" pin="!CS" pad="27"/>
<connect gate="G$1" pin="DIN" pad="26"/>
<connect gate="G$1" pin="DOUT" pad="4"/>
<connect gate="G$1" pin="GND@2" pad="2"/>
<connect gate="G$1" pin="GND@3" pad="3"/>
<connect gate="G$1" pin="ISET" pad="1"/>
<connect gate="G$1" pin="P12" pad="5"/>
<connect gate="G$1" pin="P13" pad="6"/>
<connect gate="G$1" pin="P14" pad="7"/>
<connect gate="G$1" pin="P15" pad="8"/>
<connect gate="G$1" pin="P16" pad="9"/>
<connect gate="G$1" pin="P17" pad="10"/>
<connect gate="G$1" pin="P18" pad="11"/>
<connect gate="G$1" pin="P19" pad="12"/>
<connect gate="G$1" pin="P20" pad="13"/>
<connect gate="G$1" pin="P21" pad="14"/>
<connect gate="G$1" pin="P22" pad="15"/>
<connect gate="G$1" pin="P23" pad="16"/>
<connect gate="G$1" pin="P24" pad="17"/>
<connect gate="G$1" pin="P25" pad="18"/>
<connect gate="G$1" pin="P26" pad="19"/>
<connect gate="G$1" pin="P27" pad="20"/>
<connect gate="G$1" pin="P28" pad="21"/>
<connect gate="G$1" pin="P29" pad="22"/>
<connect gate="G$1" pin="P30" pad="23"/>
<connect gate="G$1" pin="P31" pad="24"/>
<connect gate="G$1" pin="SCLK" pad="25"/>
<connect gate="G$1" pin="V+@28" pad="28"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX6957AAI" prefix="U">
<description>&lt;b&gt;MAX6957&lt;/b&gt; - 4-Wire Interfaced, 2.7V to 5.5V, 20-Port and 28-Port LED Display Driver and I/O Expander&lt;br&gt;
&lt;p&gt;
Supporting Materials:
&lt;a href=https://datasheets.maximintegrated.com/en/ds/MAX6957.pdf&gt;Datasheet&lt;/a&gt;
&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="MAX6957-SSOP28"/>
</gates>
<devices>
<device name="" package="SSOP28">
<connects>
<connect gate="G$1" pin="!CS" pad="27"/>
<connect gate="G$1" pin="DIN" pad="26"/>
<connect gate="G$1" pin="DOUT" pad="4"/>
<connect gate="G$1" pin="GND@2" pad="2"/>
<connect gate="G$1" pin="GND@3" pad="3"/>
<connect gate="G$1" pin="ISET" pad="1"/>
<connect gate="G$1" pin="P12" pad="5"/>
<connect gate="G$1" pin="P13" pad="6"/>
<connect gate="G$1" pin="P14" pad="7"/>
<connect gate="G$1" pin="P15" pad="8"/>
<connect gate="G$1" pin="P16" pad="9"/>
<connect gate="G$1" pin="P17" pad="10"/>
<connect gate="G$1" pin="P18" pad="11"/>
<connect gate="G$1" pin="P19" pad="12"/>
<connect gate="G$1" pin="P20" pad="13"/>
<connect gate="G$1" pin="P21" pad="14"/>
<connect gate="G$1" pin="P22" pad="15"/>
<connect gate="G$1" pin="P23" pad="16"/>
<connect gate="G$1" pin="P24" pad="17"/>
<connect gate="G$1" pin="P25" pad="18"/>
<connect gate="G$1" pin="P26" pad="19"/>
<connect gate="G$1" pin="P27" pad="20"/>
<connect gate="G$1" pin="P28" pad="21"/>
<connect gate="G$1" pin="P29" pad="22"/>
<connect gate="G$1" pin="P30" pad="23"/>
<connect gate="G$1" pin="P31" pad="24"/>
<connect gate="G$1" pin="SCLK" pad="25"/>
<connect gate="G$1" pin="V+@28" pad="28"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX6957AAX" prefix="U">
<description>&lt;b&gt;MAX6957&lt;/b&gt; - 4-Wire Interfaced, 2.7V to 5.5V, 20-Port and 28-Port LED Display Driver and I/O Expander&lt;br&gt;
&lt;p&gt;
Supporting Materials:
&lt;a href=https://datasheets.maximintegrated.com/en/ds/MAX6957.pdf&gt;Datasheet&lt;/a&gt;
&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="MAX6957-SSOP36"/>
</gates>
<devices>
<device name="" package="SSOP36">
<connects>
<connect gate="G$1" pin="!CS" pad="35"/>
<connect gate="G$1" pin="DIN" pad="34"/>
<connect gate="G$1" pin="DOUT" pad="4"/>
<connect gate="G$1" pin="GND@2" pad="2"/>
<connect gate="G$1" pin="GND@3" pad="3"/>
<connect gate="G$1" pin="ISET" pad="1"/>
<connect gate="G$1" pin="P10" pad="9"/>
<connect gate="G$1" pin="P11" pad="11"/>
<connect gate="G$1" pin="P12" pad="6"/>
<connect gate="G$1" pin="P13" pad="8"/>
<connect gate="G$1" pin="P14" pad="10"/>
<connect gate="G$1" pin="P15" pad="12"/>
<connect gate="G$1" pin="P16" pad="13"/>
<connect gate="G$1" pin="P17" pad="14"/>
<connect gate="G$1" pin="P18" pad="15"/>
<connect gate="G$1" pin="P19" pad="16"/>
<connect gate="G$1" pin="P20" pad="17"/>
<connect gate="G$1" pin="P21" pad="18"/>
<connect gate="G$1" pin="P22" pad="19"/>
<connect gate="G$1" pin="P23" pad="20"/>
<connect gate="G$1" pin="P24" pad="21"/>
<connect gate="G$1" pin="P25" pad="22"/>
<connect gate="G$1" pin="P26" pad="23"/>
<connect gate="G$1" pin="P27" pad="24"/>
<connect gate="G$1" pin="P28" pad="25"/>
<connect gate="G$1" pin="P29" pad="27"/>
<connect gate="G$1" pin="P30" pad="29"/>
<connect gate="G$1" pin="P31" pad="31"/>
<connect gate="G$1" pin="P4" pad="32"/>
<connect gate="G$1" pin="P5" pad="30"/>
<connect gate="G$1" pin="P6" pad="28"/>
<connect gate="G$1" pin="P7" pad="26"/>
<connect gate="G$1" pin="P8" pad="5"/>
<connect gate="G$1" pin="P9" pad="7"/>
<connect gate="G$1" pin="SCLK" pad="33"/>
<connect gate="G$1" pin="V+@36" pad="36"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX6957ATL" prefix="U">
<description>&lt;b&gt;MAX6957&lt;/b&gt; - 4-Wire Interfaced, 2.7V to 5.5V, 20-Port and 28-Port LED Display Driver and I/O Expander&lt;br&gt;
&lt;p&gt;
Supporting Materials:
&lt;a href=https://datasheets.maximintegrated.com/en/ds/MAX6957.pdf&gt;Datasheet&lt;/a&gt;
&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="MAX6957-TQFN"/>
</gates>
<devices>
<device name="" package="TQFN40-EP">
<connects>
<connect gate="G$1" pin="!CS" pad="34"/>
<connect gate="G$1" pin="DIN" pad="33"/>
<connect gate="G$1" pin="DOUT" pad="40"/>
<connect gate="G$1" pin="GND@37" pad="37"/>
<connect gate="G$1" pin="GND@38" pad="38"/>
<connect gate="G$1" pin="GND@39" pad="39"/>
<connect gate="G$1" pin="ISET" pad="36"/>
<connect gate="G$1" pin="NC@11" pad="11"/>
<connect gate="G$1" pin="NC@20" pad="20"/>
<connect gate="G$1" pin="NC@31" pad="31"/>
<connect gate="G$1" pin="P10" pad="5"/>
<connect gate="G$1" pin="P11" pad="7"/>
<connect gate="G$1" pin="P12" pad="2"/>
<connect gate="G$1" pin="P13" pad="4"/>
<connect gate="G$1" pin="P14" pad="6"/>
<connect gate="G$1" pin="P15" pad="8"/>
<connect gate="G$1" pin="P16" pad="9"/>
<connect gate="G$1" pin="P17" pad="10"/>
<connect gate="G$1" pin="P18" pad="12"/>
<connect gate="G$1" pin="P19" pad="13"/>
<connect gate="G$1" pin="P20" pad="14"/>
<connect gate="G$1" pin="P21" pad="15"/>
<connect gate="G$1" pin="P22" pad="16"/>
<connect gate="G$1" pin="P23" pad="17"/>
<connect gate="G$1" pin="P24" pad="18"/>
<connect gate="G$1" pin="P25" pad="19"/>
<connect gate="G$1" pin="P26" pad="21"/>
<connect gate="G$1" pin="P27" pad="22"/>
<connect gate="G$1" pin="P28" pad="23"/>
<connect gate="G$1" pin="P29" pad="25"/>
<connect gate="G$1" pin="P30" pad="27"/>
<connect gate="G$1" pin="P31" pad="29"/>
<connect gate="G$1" pin="P4" pad="30"/>
<connect gate="G$1" pin="P5" pad="28"/>
<connect gate="G$1" pin="P6" pad="26"/>
<connect gate="G$1" pin="P7" pad="24"/>
<connect gate="G$1" pin="P8" pad="1"/>
<connect gate="G$1" pin="P9" pad="3"/>
<connect gate="G$1" pin="SCLK" pad="32"/>
<connect gate="G$1" pin="V+@35" pad="35"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX6958-59AAE" prefix="U">
<description>&lt;b&gt;MAX6958-59&lt;/b&gt; - 2-Wire Interfaced, 3V to 5.5V, 4-Digit, 9-Segment LED Display Drivers with Keyscan&lt;br&gt;
&lt;p&gt;
Supporting Materials:
&lt;a href=https://datasheets.maximintegrated.com/en/ds/MAX6958-MAX6959.pdf&gt;Datasheet&lt;/a&gt;
&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="MAX6958-59-QSOP16"/>
</gates>
<devices>
<device name="" package="QSOP16">
<connects>
<connect gate="G$1" pin="DIG0/SEG0" pad="4"/>
<connect gate="G$1" pin="DIG1/SEG1" pad="5"/>
<connect gate="G$1" pin="DIG2/SEG2" pad="6"/>
<connect gate="G$1" pin="DIG3/SEG3" pad="7"/>
<connect gate="G$1" pin="GND@8" pad="8"/>
<connect gate="G$1" pin="INPUT1" pad="9"/>
<connect gate="G$1" pin="INPUT2" pad="10"/>
<connect gate="G$1" pin="SCL" pad="2"/>
<connect gate="G$1" pin="SDA" pad="1"/>
<connect gate="G$1" pin="SEG4" pad="11"/>
<connect gate="G$1" pin="SEG5" pad="12"/>
<connect gate="G$1" pin="SEG6" pad="13"/>
<connect gate="G$1" pin="SEG7" pad="14"/>
<connect gate="G$1" pin="SEG8" pad="15"/>
<connect gate="G$1" pin="SEG9" pad="3"/>
<connect gate="G$1" pin="V+@16" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX6958-59AAP" prefix="U">
<description>&lt;b&gt;MAX6958-59&lt;/b&gt; - 2-Wire Interfaced, 3V to 5.5V, 4-Digit, 9-Segment LED Display Drivers with Keyscan&lt;br&gt;
&lt;p&gt;
Supporting Materials:
&lt;a href=https://datasheets.maximintegrated.com/en/ds/MAX6958-MAX6959.pdf&gt;Datasheet&lt;/a&gt;
&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="MAX6958-59-DIL16"/>
</gates>
<devices>
<device name="" package="DIL16">
<connects>
<connect gate="G$1" pin="DIG0/SEG0" pad="4"/>
<connect gate="G$1" pin="DIG1/SEG1" pad="5"/>
<connect gate="G$1" pin="DIG2/SEG2" pad="6"/>
<connect gate="G$1" pin="DIG3/SEG3" pad="7"/>
<connect gate="G$1" pin="GND@8" pad="8"/>
<connect gate="G$1" pin="INPUT1" pad="9"/>
<connect gate="G$1" pin="INPUT2" pad="10"/>
<connect gate="G$1" pin="SCL" pad="2"/>
<connect gate="G$1" pin="SDA" pad="1"/>
<connect gate="G$1" pin="SEG4" pad="11"/>
<connect gate="G$1" pin="SEG5" pad="12"/>
<connect gate="G$1" pin="SEG6" pad="13"/>
<connect gate="G$1" pin="SEG7" pad="14"/>
<connect gate="G$1" pin="SEG8" pad="15"/>
<connect gate="G$1" pin="SEG9" pad="3"/>
<connect gate="G$1" pin="V+@16" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
