<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.0.1">
<drawing>
<library>
<description>&lt;b&gt;Pulse Engineering&lt;/b&gt; - v1.00 (01/12/2006)&lt;p&gt;
source http://www.pulseeng.com/&lt;p&gt;
&lt;author&gt;Created by Bob Starr (rtzaudio@mindspring.com)&lt;/author&gt;</description>
<packages>
<package name="PE-65612">
<description>DIGITAL AUDIO DATA TX TRANSFORMER</description>
</package>
<package name="PE-65812">
<description>DIGITAL AUDIO DATA TX TRANSFORMER</description>
</package>
<package name="PJ-J0">
<description>RJ45 with Ethernet Balun and LED's</description>
</package>
<package name="JY0-0016">
<description>RJ45/Dual USB Combo</description>
</package>
<package name="DO3316P">
<description>&lt;b&gt;COILCRAFT&lt;/b&gt;</description>
</package>
<package name="P0751/2">
</package>
<package name="EE020">
<description>TYPE EE20 LAMINATED TRANSFORMER</description>
</package>
<package name="PE-5262XXLP">
</package>
</packages>
<symbols>
<symbol name="PE-65612">
<pin name="4" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="J0026">
<pin name="RD-"/>
<pin name="RD+"/>
<pin name="CTR"/>
<pin name="TD-"/>
<pin name="TD+"/>
<pin name="CTT"/>
<pin name="LA" direction="pas"/>
<pin name="LC" direction="pas"/>
<pin name="RA" direction="pas"/>
<pin name="RC" direction="pas"/>
<pin name="CG1" direction="pas"/>
<pin name="CG2" direction="pas"/>
<pin name="S1" direction="pas"/>
<pin name="S2" direction="pas"/>
</symbol>
<symbol name="PE-65812">
<pin name="5" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="JY0-0016">
<pin name="RD-"/>
<pin name="RD+"/>
<pin name="CTR"/>
<pin name="TD-"/>
<pin name="TD+"/>
<pin name="CTT"/>
<pin name="LA" direction="pas"/>
<pin name="LC" direction="pas"/>
<pin name="RA" direction="pas"/>
<pin name="RC" direction="pas"/>
<pin name="S3" direction="pas"/>
<pin name="S4" direction="pas"/>
<pin name="S1" direction="pas"/>
<pin name="S2" direction="pas"/>
</symbol>
<symbol name="USB-4">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="L-US">
<pin name="P$1" direction="pas"/>
<pin name="P$2" direction="pas"/>
</symbol>
<symbol name="EE020-1">
<pin name="4" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="EE020-2">
<pin name="4" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="PE-526XXNL">
<pin name="1" direction="pwr"/>
<pin name="2" direction="pwr"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="J0026" prefix="J">
<description>RJ45 PulseJack w/LEDs</description>
<gates>
<gate name="G$1" symbol="J0026"/>
</gates>
<devices>
<device name="" package="PJ-J0">
<connects>
<connect gate="G$1" pin="CG1" pad="4"/>
<connect gate="G$1" pin="CG2" pad="5"/>
<connect gate="G$1" pin="CTR" pad="6"/>
<connect gate="G$1" pin="CTT" pad="3"/>
<connect gate="G$1" pin="LA" pad="9"/>
<connect gate="G$1" pin="LC" pad="10"/>
<connect gate="G$1" pin="RA" pad="12"/>
<connect gate="G$1" pin="RC" pad="11"/>
<connect gate="G$1" pin="RD+" pad="7"/>
<connect gate="G$1" pin="RD-" pad="8"/>
<connect gate="G$1" pin="S1" pad="S1"/>
<connect gate="G$1" pin="S2" pad="S2"/>
<connect gate="G$1" pin="TD+" pad="1"/>
<connect gate="G$1" pin="TD-" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PE-65612" prefix="T">
<description>DIGITAL AUDIO DATA TX TRANSFORMER&lt;p&gt;AES 3-199X or IEC 958</description>
<gates>
<gate name="G$1" symbol="PE-65612"/>
</gates>
<devices>
<device name="" package="PE-65612">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PE-65812" prefix="T">
<description>DIGITAL AUDIO DATA TX TRANSFORMER&lt;p&gt;AES 3-199X or IEC 958</description>
<gates>
<gate name="G$1" symbol="PE-65812"/>
</gates>
<devices>
<device name="" package="PE-65812">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="JY0-0016" prefix="J">
<description>RJ45/Dual USB Combo</description>
<gates>
<gate name="-RJ45" symbol="JY0-0016"/>
<gate name="-USB-A" symbol="USB-4"/>
<gate name="-USB-B" symbol="USB-4"/>
</gates>
<devices>
<device name="" package="JY0-0016">
<connects>
<connect gate="-RJ45" pin="CTR" pad="6"/>
<connect gate="-RJ45" pin="CTT" pad="1"/>
<connect gate="-RJ45" pin="LA" pad="10"/>
<connect gate="-RJ45" pin="LC" pad="9"/>
<connect gate="-RJ45" pin="RA" pad="8"/>
<connect gate="-RJ45" pin="RC" pad="7"/>
<connect gate="-RJ45" pin="RD+" pad="4"/>
<connect gate="-RJ45" pin="RD-" pad="5"/>
<connect gate="-RJ45" pin="S1" pad="S1"/>
<connect gate="-RJ45" pin="S2" pad="S2"/>
<connect gate="-RJ45" pin="S3" pad="S3"/>
<connect gate="-RJ45" pin="S4" pad="S4"/>
<connect gate="-RJ45" pin="TD+" pad="2"/>
<connect gate="-RJ45" pin="TD-" pad="3"/>
<connect gate="-USB-A" pin="1" pad="A1"/>
<connect gate="-USB-A" pin="2" pad="A2"/>
<connect gate="-USB-A" pin="3" pad="A3"/>
<connect gate="-USB-A" pin="4" pad="A4"/>
<connect gate="-USB-B" pin="1" pad="B1"/>
<connect gate="-USB-B" pin="2" pad="B2"/>
<connect gate="-USB-B" pin="3" pad="B3"/>
<connect gate="-USB-B" pin="4" pad="B4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="P0751/2" prefix="L">
<description>&lt;b&gt;SMT POWER INDUCTOR&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="L-US"/>
</gates>
<devices>
<device name="" package="P0751/2">
<connects>
<connect gate="G$1" pin="P$1" pad="1"/>
<connect gate="G$1" pin="P$2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EE020-TYPE-1" prefix="T">
<description>POWER TRANSFORMER</description>
<gates>
<gate name="G$1" symbol="EE020-1"/>
</gates>
<devices>
<device name="" package="EE020">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EE020-TYPE-2" prefix="T">
<description>POWER TRANSFORMER</description>
<gates>
<gate name="G$1" symbol="EE020-2"/>
</gates>
<devices>
<device name="" package="EE020">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PE-526XXNL">
<gates>
<gate name="G$1" symbol="PE-526XXNL"/>
</gates>
<devices>
<device name="" package="PE-5262XXLP">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
